(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "4P2C"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 8.89 0)
		)
		(property "Value" "4P2C"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 0 1.27 90)
		)
		(property "Datasheet" "~"
			(at 0 1.27 90)
		)
		(property "Description" "RJ connector, 4P2C (4 positions 2 connected)"
			(at 0 0 0)
		)
		(property "ki_keywords" "4P2C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "4P2C*"
			(at 0 0 0)
		)
		(symbol "4P2C_0_1")
		(symbol "4P2C_1_1"
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4P2C_Shielded"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 8.89 0)
		)
		(property "Value" "4P2C_Shielded"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 0 1.27 90)
		)
		(property "Datasheet" "~"
			(at 0 1.27 90)
		)
		(property "Description" "RJ connector, 4P2C (4 positions 2 connected), Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "4P2C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "4P2C*"
			(at 0 0 0)
		)
		(symbol "4P2C_Shielded_0_1")
		(symbol "4P2C_Shielded_1_1"
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "SH")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4P4C"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 8.89 0)
		)
		(property "Value" "4P4C"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 0 1.27 90)
		)
		(property "Datasheet" "~"
			(at 0 1.27 90)
		)
		(property "Description" "RJ connector, 4P4C (4 positions 4 connected), RJ9/RJ10/RJ22"
			(at 0 0 0)
		)
		(property "ki_keywords" "4P4C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "4P4C* RJ9* RJ10* RJ22*"
			(at 0 0 0)
		)
		(symbol "4P4C_0_1")
		(symbol "4P4C_1_1"
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4P4C_Shielded"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 8.89 0)
		)
		(property "Value" "4P4C_Shielded"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 0 1.27 90)
		)
		(property "Datasheet" "~"
			(at 0 1.27 90)
		)
		(property "Description" "RJ connector, 4P4C (4 positions 4 connected), RJ9/RJ10/RJ22, Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "4P4C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "4P4C* RJ9* RJ10* RJ22*"
			(at 0 0 0)
		)
		(symbol "4P4C_Shielded_0_1")
		(symbol "4P4C_Shielded_1_1"
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "SH")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "6P2C"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "6P2C"
			(at 2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 6P2C (6 positions 2 connected), RJ11"
			(at 0 0 0)
		)
		(property "ki_keywords" "6P2C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "6P2C* RJ11*"
			(at 0 0 0)
		)
		(symbol "6P2C_0_1")
		(symbol "6P2C_1_1"
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "6P2C_Shielded"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "6P2C_Shielded"
			(at 2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 6P2C (6 positions 2 connected), RJ11, Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "6P2C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "6P2C* RJ11*"
			(at 0 0 0)
		)
		(symbol "6P2C_Shielded_0_1")
		(symbol "6P2C_Shielded_1_1"
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "~")
				(number "SH")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "6P4C"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "6P4C"
			(at 2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 6P4C (6 positions 4 connected), RJ13/RJ14"
			(at 0 0 0)
		)
		(property "ki_keywords" "6P4C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "6P4C* RJ13* RJ14*"
			(at 0 0 0)
		)
		(symbol "6P4C_0_1")
		(symbol "6P4C_1_1"
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "6P4C_Shielded"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "6P4C_Shielded"
			(at 2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 6P4C (6 positions 4 connected), RJ13/RJ14, Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "6P4C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "6P4C* RJ13* RJ14*"
			(at 0 0 0)
		)
		(symbol "6P4C_Shielded_0_1")
		(symbol "6P4C_Shielded_1_1"
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "~")
				(number "SH")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "6P6C"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "6P6C"
			(at 2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 6P6C (6 positions 6 connected), RJ12/RJ18/RJ25"
			(at 0 0 0)
		)
		(property "ki_keywords" "6P6C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "6P6C* RJ12* RJ18* RJ25*"
			(at 0 0 0)
		)
		(symbol "6P6C_0_1")
		(symbol "6P6C_1_1"
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "6P6C_Shielded"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "6P6C_Shielded"
			(at 2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 6P6C (6 positions 6 connected), RJ12/RJ18/RJ25, Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "6P6C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "6P6C* RJ12* RJ18* RJ25*"
			(at 0 0 0)
		)
		(symbol "6P6C_Shielded_0_1")
		(symbol "6P6C_Shielded_1_1"
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "~")
				(number "SH")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8P4C"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "8P4C"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P4C (8 positions 4 connected), RJ38/RJ48"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P4C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P4C* RJ38* RJ48*"
			(at 0 0 0)
		)
		(symbol "8P4C_0_1")
		(symbol "8P4C_1_1"
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8P4C_Shielded"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "8P4C_Shielded"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P4C (8 positions 4 connected), RJ38/RJ48, Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P4C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P4C* RJ38* RJ48*"
			(at 0 0 0)
		)
		(symbol "8P4C_Shielded_0_1")
		(symbol "8P4C_Shielded_1_1"
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(name "~")
				(number "SH")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8P8C"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "8P8C"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected), RJ31/RJ32/RJ33/RJ34/RJ35/RJ41/RJ45/RJ49/RJ61"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ31* RJ32* RJ33* RJ34* RJ35* RJ41* RJ45* RJ49* RJ61*"
			(at 0 0 0)
		)
		(symbol "8P8C_0_1")
		(symbol "8P8C_1_1"
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8P8C_LED"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "8P8C_LED"
			(at 1.27 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected), two LEDs, RJ45"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector led"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ45*"
			(at 0 0 0)
		)
		(symbol "8P8C_LED_0_1")
		(symbol "8P8C_LED_1_1"
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8P8C_LED_Shielded"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "8P8C_LED_Shielded"
			(at 1.27 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected), two LEDs, RJ45, Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector led"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ45*"
			(at 0 0 0)
		)
		(symbol "8P8C_LED_Shielded_0_1")
		(symbol "8P8C_LED_Shielded_1_1"
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(name "~")
				(number "SH")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8P8C_LED_Shielded_x2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "8P8C_LED_Shielded_x2"
			(at 1.27 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected), two LEDs, RJ45, Shielded, two ports"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector led dual"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C*02* RJ45*02*"
			(at 0 0 0)
		)
		(symbol "8P8C_LED_Shielded_x2_0_1")
		(symbol "8P8C_LED_Shielded_x2_1_1"
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(name "~")
				(number "SH")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(symbol "8P8C_LED_Shielded_x2_2_1"
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "~")
				(number "21")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~")
				(number "22")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~")
				(number "23")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~")
				(number "24")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(name "~")
				(number "SH")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "~")
				(number "20")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~")
				(number "19")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~")
				(number "18")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "17")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "15")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8P8C_Shielded"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "8P8C_Shielded"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected), RJ31/RJ32/RJ33/RJ34/RJ35/RJ41/RJ45/RJ49/RJ61, Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ31* RJ32* RJ33* RJ34* RJ35* RJ41* RJ45* RJ49* RJ61*"
			(at 0 0 0)
		)
		(symbol "8P8C_Shielded_0_1")
		(symbol "8P8C_Shielded_1_1"
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(name "~")
				(number "SH")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATX-20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -8.89 13.97 0)
		)
		(property "Value" "ATX-20"
			(at 6.35 13.97 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://web.aub.edu.lb/pub/docs/atx_201.pdf#page=20"
			(at 27.94 -13.97 0)
		)
		(property "Description" "ATX Power supply 20pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "ATX PSU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Mini?Fit*2x10*Vertical* *Mini?Fit*2x10*Horizontal*"
			(at 0 0 0)
		)
		(symbol "ATX-20_0_1")
		(symbol "ATX-20_1_1"
			(pin open_collector line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PS_ON#")
				(number "14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_out line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PWR_OK")
				(number "8")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "+12V")
				(number "10")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "+5V")
				(number "19")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "+5V")
				(number "20")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "+5V")
				(number "4")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "+5V")
				(number "6")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "+5VSB")
				(number "9")
			)
			(pin power_out line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "+3.3V")
				(number "1")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "+3.3V")
				(number "11")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "+3.3V")
				(number "2")
			)
			(pin power_out line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "-5V/NC")
				(number "18")
			)
			(pin power_out line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "-12V")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATX-24"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -8.89 13.97 0)
		)
		(property "Value" "ATX-24"
			(at 6.35 13.97 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.intel.com/content/dam/www/public/us/en/documents/guides/power-supply-design-guide-june.pdf#page=33"
			(at 60.96 -13.97 0)
		)
		(property "Description" "ATX Power supply 24pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "ATX PSU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Mini?Fit*2x12*Vertical* *Mini?Fit*2x12*Horizontal*"
			(at 0 0 0)
		)
		(symbol "ATX-24_0_1")
		(symbol "ATX-24_1_1"
			(pin open_collector line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PS_ON#")
				(number "16")
			)
			(pin no_connect line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin power_out line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PWR_OK")
				(number "8")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "+12V")
				(number "10")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(hide yes)
				(name "+12V")
				(number "11")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "+5V")
				(number "21")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "+5V")
				(number "22")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "+5V")
				(number "23")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "+5V")
				(number "4")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "+5V")
				(number "6")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "+5VSB")
				(number "9")
			)
			(pin power_out line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "+3.3V")
				(number "1")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "+3.3V")
				(number "12")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "+3.3V")
				(number "13")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "+3.3V")
				(number "2")
			)
			(pin power_out line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "-12V")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AVR-ISP-10"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -6.35 11.43 0)
		)
		(property "Value" "AVR-ISP-10"
			(at 0 11.43 0)
		)
		(property "Footprint" ""
			(at -6.35 1.27 90)
		)
		(property "Datasheet" "~"
			(at -32.385 -13.97 0)
		)
		(property "Description" "Atmel 10-pin ISP connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR ISP Connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "IDC?Header*2x05* Pin?Header*2x05*"
			(at 0 0 0)
		)
		(symbol "AVR-ISP-10_0_1")
		(symbol "AVR-ISP-10_1_1"
			(pin passive line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "MISO")
				(number "9")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "MOSI")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCK")
				(number "7")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{RST}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AVR-ISP-6"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -6.35 11.43 0)
		)
		(property "Value" "AVR-ISP-6"
			(at 0 11.43 0)
		)
		(property "Footprint" ""
			(at -6.35 1.27 90)
		)
		(property "Datasheet" "~"
			(at -32.385 -13.97 0)
		)
		(property "Description" "Atmel 6-pin ISP connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR ISP Connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "IDC?Header*2x03* Pin?Header*2x03*"
			(at 0 0 0)
		)
		(symbol "AVR-ISP-6_0_1")
		(symbol "AVR-ISP-6_1_1"
			(pin passive line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "MISO")
				(number "1")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "MOSI")
				(number "4")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCK")
				(number "3")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{RST}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AVR-JTAG-10"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -8.89 13.97 0)
		)
		(property "Value" "AVR-JTAG-10"
			(at 1.27 13.97 0)
		)
		(property "Footprint" ""
			(at -3.81 3.81 90)
		)
		(property "Datasheet" "~"
			(at -32.385 -13.97 0)
		)
		(property "Description" "Atmel 10-pin JTAG connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR JTAG Connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "IDC?Header*2x05* Pin?Header*2x05*"
			(at 0 0 0)
		)
		(symbol "AVR-JTAG-10_0_1")
		(symbol "AVR-JTAG-10_1_1"
			(pin passive line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VREF")
				(number "4")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{SRST}")
				(number "6")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{TRST}")
				(number "8")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "TCK")
				(number "1")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "TMS")
				(number "5")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "TDO")
				(number "3")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "TDI")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AVR-PDI-6"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -6.35 8.89 0)
		)
		(property "Value" "AVR-PDI-6"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at -6.35 -1.27 90)
		)
		(property "Datasheet" "~"
			(at -32.385 -13.97 0)
		)
		(property "Description" "Atmel 6-pin PDI connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR PDI Connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "IDC?Header*2x03* Pin?Header*2x03*"
			(at 0 0 0)
		)
		(symbol "AVR-PDI-6_0_1")
		(symbol "AVR-PDI-6_1_1"
			(pin passive line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "DATA")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "CLOCK")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AVR-TPI-6"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -6.35 8.89 0)
		)
		(property "Value" "AVR-TPI-6"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at -6.35 -1.27 90)
		)
		(property "Datasheet" "~"
			(at -32.385 -13.97 0)
		)
		(property "Description" "Atmel 6-pin TPI connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR TPI Connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "IDC?Header*2x03* Pin?Header*2x03*"
			(at 0 0 0)
		)
		(symbol "AVR-TPI-6_0_1")
		(symbol "AVR-TPI-6_1_1"
			(pin passive line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "DATA")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "CLOCK")
				(number "3")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{RST}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AVR-UPDI-6"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -6.35 8.89 0)
		)
		(property "Value" "AVR-UPDI-6"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at -6.35 -1.27 90)
		)
		(property "Datasheet" "https://www.microchip.com/webdoc/GUID-9D10622A-5C16-4405-B092-1BDD437B4976/index.html?GUID-9B349315-2842-4189-B88C-49F4E1055D7F"
			(at -32.385 -13.97 0)
		)
		(property "Description" "Atmel 6-pin UPDI connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR UPDI Connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "IDC?Header*2x03* Pin?Header*2x03*"
			(at 0 0 0)
		)
		(symbol "AVR-UPDI-6_0_1")
		(symbol "AVR-UPDI-6_1_1"
			(pin passive line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "DATA")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Barrel_Jack"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 5.334 0)
		)
		(property "Value" "Barrel_Jack"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 1.27 -1.016 0)
		)
		(property "Datasheet" "~"
			(at 1.27 -1.016 0)
		)
		(property "Description" "DC Barrel Jack"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC power barrel jack connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BarrelJack*"
			(at 0 0 0)
		)
		(symbol "Barrel_Jack_0_1")
		(symbol "Barrel_Jack_1_1"
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Barrel_Jack_MountingPin"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 5.334 0)
		)
		(property "Value" "Barrel_Jack_MountingPin"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" ""
			(at 1.27 -1.016 0)
		)
		(property "Datasheet" "~"
			(at 1.27 -1.016 0)
		)
		(property "Description" "DC Barrel Jack with a mounting pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC power barrel jack connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BarrelJack*"
			(at 0 0 0)
		)
		(symbol "Barrel_Jack_MountingPin_0_1")
		(symbol "Barrel_Jack_MountingPin_1_1"
			(text "Mounting"
				(at 0 -4.191 0)
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 3.048)
				(name "MountPin")
				(number "MP")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Barrel_Jack_Switch"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 5.334 0)
		)
		(property "Value" "Barrel_Jack_Switch"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 1.27 -1.016 0)
		)
		(property "Datasheet" "~"
			(at 1.27 -1.016 0)
		)
		(property "Description" "DC Barrel Jack with an internal switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC power barrel jack connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BarrelJack*"
			(at 0 0 0)
		)
		(symbol "Barrel_Jack_Switch_0_1")
		(symbol "Barrel_Jack_Switch_1_1"
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Barrel_Jack_Switch_MountingPin"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 5.334 0)
		)
		(property "Value" "Barrel_Jack_Switch_MountingPin"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" ""
			(at 1.27 -1.016 0)
		)
		(property "Datasheet" "~"
			(at 1.27 -1.016 0)
		)
		(property "Description" "DC Barrel Jack with an internal switch and a mounting pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC power barrel jack connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BarrelJack*"
			(at 0 0 0)
		)
		(symbol "Barrel_Jack_Switch_MountingPin_0_1")
		(symbol "Barrel_Jack_Switch_MountingPin_1_1"
			(text "Mounting"
				(at 0 -4.191 0)
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 3.048)
				(name "MountPin")
				(number "MP")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Barrel_Jack_Switch_Pin3Ring"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 5.334 0)
		)
		(property "Value" "Barrel_Jack_Switch_Pin3Ring"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 1.27 -1.016 0)
		)
		(property "Datasheet" "~"
			(at 1.27 -1.016 0)
		)
		(property "Description" "DC Barrel Jack with an internal switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC power barrel jack connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BarrelJack*"
			(at 0 0 0)
		)
		(symbol "Barrel_Jack_Switch_Pin3Ring_0_1")
		(symbol "Barrel_Jack_Switch_Pin3Ring_1_1"
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Bus_ISA_16bit"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 67.945 0)
		)
		(property "Value" "Bus_ISA_16bit"
			(at 0 -65.405 0)
		)
		(property "Footprint" ""
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://en.wikipedia.org/wiki/Industry_Standard_Architecture"
			(at 0 1.27 0)
		)
		(property "Description" "16-bit ISA-AT bus connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "ISA"
			(at 0 0 0)
		)
		(symbol "Bus_ISA_16bit_0_1")
		(symbol "Bus_ISA_16bit_1_1"
			(pin power_in line
				(at -17.78 63.5 0)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at -17.78 60.96 0)
				(length 2.54)
				(name "RESET")
				(number "2")
			)
			(pin power_in line
				(at -17.78 58.42 0)
				(length 2.54)
				(name "+5V")
				(number "3")
			)
			(pin passive line
				(at -17.78 55.88 0)
				(length 2.54)
				(name "IRQ2")
				(number "4")
			)
			(pin power_in line
				(at -17.78 53.34 0)
				(length 2.54)
				(name "-5V")
				(number "5")
			)
			(pin passive line
				(at -17.78 50.8 0)
				(length 2.54)
				(name "DRQ2")
				(number "6")
			)
			(pin power_in line
				(at -17.78 48.26 0)
				(length 2.54)
				(name "-12V")
				(number "7")
			)
			(pin passive line
				(at -17.78 45.72 0)
				(length 2.54)
				(name "UNUSED")
				(number "8")
			)
			(pin power_in line
				(at -17.78 43.18 0)
				(length 2.54)
				(name "+12V")
				(number "9")
			)
			(pin power_in line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin output line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "~{SMEMW}")
				(number "11")
			)
			(pin output line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "~{SMEMR}")
				(number "12")
			)
			(pin output line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "~{IOW}")
				(number "13")
			)
			(pin output line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "~{IOR}")
				(number "14")
			)
			(pin passive line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "~{DACK3}")
				(number "15")
			)
			(pin passive line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "DRQ3")
				(number "16")
			)
			(pin passive line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "~{DACK1}")
				(number "17")
			)
			(pin passive line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "DRQ1")
				(number "18")
			)
			(pin passive line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "~{REFRESH}")
				(number "19")
			)
			(pin output line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "CLK")
				(number "20")
			)
			(pin passive line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "IRQ7")
				(number "21")
			)
			(pin passive line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "IRQ6")
				(number "22")
			)
			(pin passive line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "IRQ5")
				(number "23")
			)
			(pin passive line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "IRQ4")
				(number "24")
			)
			(pin passive line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "IRQ3")
				(number "25")
			)
			(pin passive line
				(at -17.78 0 0)
				(length 2.54)
				(name "~{DACK2}")
				(number "26")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "TC")
				(number "27")
			)
			(pin output line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "ALE")
				(number "28")
			)
			(pin power_in line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "VCC")
				(number "29")
			)
			(pin output line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "OSC")
				(number "30")
			)
			(pin power_in line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "~{MEMCS16}")
				(number "63")
			)
			(pin passive line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "~{IOCS16}")
				(number "64")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "IRQ10")
				(number "65")
			)
			(pin passive line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "IRQ11")
				(number "66")
			)
			(pin passive line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "IRQ12")
				(number "67")
			)
			(pin passive line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "IRQ15")
				(number "68")
			)
			(pin passive line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "IRQ14")
				(number "69")
			)
			(pin output line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "~{DACK0}")
				(number "70")
			)
			(pin passive line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "DRQ0")
				(number "71")
			)
			(pin output line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "~{DACK5}")
				(number "72")
			)
			(pin passive line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "DRQ5")
				(number "73")
			)
			(pin output line
				(at -17.78 -45.72 0)
				(length 2.54)
				(name "~{DACK6}")
				(number "74")
			)
			(pin passive line
				(at -17.78 -48.26 0)
				(length 2.54)
				(name "DRQ6")
				(number "75")
			)
			(pin output line
				(at -17.78 -50.8 0)
				(length 2.54)
				(name "~{DACK7}")
				(number "76")
			)
			(pin passive line
				(at -17.78 -53.34 0)
				(length 2.54)
				(name "DRQ7")
				(number "77")
			)
			(pin power_in line
				(at -17.78 -55.88 0)
				(length 2.54)
				(name "+5V")
				(number "78")
			)
			(pin passive line
				(at -17.78 -58.42 0)
				(length 2.54)
				(name "MASTER")
				(number "79")
			)
			(pin power_in line
				(at -17.78 -60.96 0)
				(length 2.54)
				(name "GND")
				(number "80")
			)
			(pin passive line
				(at 17.78 63.5 180)
				(length 2.54)
				(name "IO")
				(number "32")
			)
			(pin tri_state line
				(at 17.78 60.96 180)
				(length 2.54)
				(name "DB7")
				(number "33")
			)
			(pin tri_state line
				(at 17.78 58.42 180)
				(length 2.54)
				(name "DB6")
				(number "34")
			)
			(pin tri_state line
				(at 17.78 55.88 180)
				(length 2.54)
				(name "DB5")
				(number "35")
			)
			(pin tri_state line
				(at 17.78 53.34 180)
				(length 2.54)
				(name "DB4")
				(number "36")
			)
			(pin tri_state line
				(at 17.78 50.8 180)
				(length 2.54)
				(name "DB3")
				(number "37")
			)
			(pin tri_state line
				(at 17.78 48.26 180)
				(length 2.54)
				(name "DB2")
				(number "38")
			)
			(pin tri_state line
				(at 17.78 45.72 180)
				(length 2.54)
				(name "DB1")
				(number "39")
			)
			(pin tri_state line
				(at 17.78 43.18 180)
				(length 2.54)
				(name "DB0")
				(number "40")
			)
			(pin passive line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "IO_READY")
				(number "41")
			)
			(pin output line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "AEN")
				(number "42")
			)
			(pin tri_state line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "BA19")
				(number "43")
			)
			(pin tri_state line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "BA18")
				(number "44")
			)
			(pin tri_state line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "BA17")
				(number "45")
			)
			(pin tri_state line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "BA16")
				(number "46")
			)
			(pin tri_state line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "BA15")
				(number "47")
			)
			(pin tri_state line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "BA14")
				(number "48")
			)
			(pin tri_state line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "BA13")
				(number "49")
			)
			(pin tri_state line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "BA12")
				(number "50")
			)
			(pin tri_state line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "BA11")
				(number "51")
			)
			(pin tri_state line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "BA10")
				(number "52")
			)
			(pin tri_state line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "BA09")
				(number "53")
			)
			(pin tri_state line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "BA08")
				(number "54")
			)
			(pin tri_state line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "BA07")
				(number "55")
			)
			(pin tri_state line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "BA06")
				(number "56")
			)
			(pin tri_state line
				(at 17.78 0 180)
				(length 2.54)
				(name "BA05")
				(number "57")
			)
			(pin tri_state line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "BA04")
				(number "58")
			)
			(pin tri_state line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "BA03")
				(number "59")
			)
			(pin tri_state line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "BA02")
				(number "60")
			)
			(pin tri_state line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "BA01")
				(number "61")
			)
			(pin tri_state line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "BA00")
				(number "62")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "SBHE")
				(number "81")
			)
			(pin passive line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "LA23")
				(number "82")
			)
			(pin passive line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "LA22")
				(number "83")
			)
			(pin passive line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "LA21")
				(number "84")
			)
			(pin passive line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "LA20")
				(number "85")
			)
			(pin passive line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "LA19")
				(number "86")
			)
			(pin passive line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "LA18")
				(number "87")
			)
			(pin passive line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "LA17")
				(number "88")
			)
			(pin output line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "~{MEMR}")
				(number "89")
			)
			(pin output line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "~{MEMW}")
				(number "90")
			)
			(pin tri_state line
				(at 17.78 -43.18 180)
				(length 2.54)
				(name "D8")
				(number "91")
			)
			(pin tri_state line
				(at 17.78 -45.72 180)
				(length 2.54)
				(name "D9")
				(number "92")
			)
			(pin tri_state line
				(at 17.78 -48.26 180)
				(length 2.54)
				(name "D10")
				(number "93")
			)
			(pin tri_state line
				(at 17.78 -50.8 180)
				(length 2.54)
				(name "D11")
				(number "94")
			)
			(pin tri_state line
				(at 17.78 -53.34 180)
				(length 2.54)
				(name "D12")
				(number "95")
			)
			(pin tri_state line
				(at 17.78 -55.88 180)
				(length 2.54)
				(name "D13")
				(number "96")
			)
			(pin tri_state line
				(at 17.78 -58.42 180)
				(length 2.54)
				(name "D14")
				(number "97")
			)
			(pin tri_state line
				(at 17.78 -60.96 180)
				(length 2.54)
				(name "D15")
				(number "98")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Bus_ISA_8bit"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 42.545 0)
		)
		(property "Value" "Bus_ISA_8bit"
			(at 0 -42.545 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://en.wikipedia.org/wiki/Industry_Standard_Architecture"
			(at 0 0 0)
		)
		(property "Description" "8-bit ISA-PC bus connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "ISA"
			(at 0 0 0)
		)
		(symbol "Bus_ISA_8bit_0_1")
		(symbol "Bus_ISA_8bit_1_1"
			(pin power_in line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "RESET")
				(number "2")
			)
			(pin power_in line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin passive line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "IRQ2")
				(number "4")
			)
			(pin power_in line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "-5V")
				(number "5")
			)
			(pin passive line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "DRQ2")
				(number "6")
			)
			(pin power_in line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "-12V")
				(number "7")
			)
			(pin passive line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "UNUSED")
				(number "8")
			)
			(pin power_in line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "+12V")
				(number "9")
			)
			(pin power_in line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "~{SMEMW}")
				(number "11")
			)
			(pin output line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "~{SMEMR}")
				(number "12")
			)
			(pin output line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "~{IOW}")
				(number "13")
			)
			(pin output line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "~{IOR}")
				(number "14")
			)
			(pin passive line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "~{DACK3}")
				(number "15")
			)
			(pin passive line
				(at -17.78 0 0)
				(length 2.54)
				(name "DRQ3")
				(number "16")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "~{DACK1}")
				(number "17")
			)
			(pin passive line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "DRQ1")
				(number "18")
			)
			(pin passive line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "~{DACK0}")
				(number "19")
			)
			(pin output line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "CLK")
				(number "20")
			)
			(pin passive line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "IRQ7")
				(number "21")
			)
			(pin passive line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "IRQ6")
				(number "22")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "IRQ5")
				(number "23")
			)
			(pin passive line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "IRQ4")
				(number "24")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "IRQ3")
				(number "25")
			)
			(pin passive line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "~{DACK2}")
				(number "26")
			)
			(pin passive line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "TC")
				(number "27")
			)
			(pin output line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "ALE")
				(number "28")
			)
			(pin power_in line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "VCC")
				(number "29")
			)
			(pin output line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "OSC")
				(number "30")
			)
			(pin power_in line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "IO")
				(number "32")
			)
			(pin tri_state line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "DB7")
				(number "33")
			)
			(pin tri_state line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "DB6")
				(number "34")
			)
			(pin tri_state line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "DB5")
				(number "35")
			)
			(pin tri_state line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "DB4")
				(number "36")
			)
			(pin tri_state line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "DB3")
				(number "37")
			)
			(pin tri_state line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "DB2")
				(number "38")
			)
			(pin tri_state line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "DB1")
				(number "39")
			)
			(pin tri_state line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "DB0")
				(number "40")
			)
			(pin passive line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "IO_READY")
				(number "41")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "AEN")
				(number "42")
			)
			(pin tri_state line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "BA19")
				(number "43")
			)
			(pin tri_state line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "BA18")
				(number "44")
			)
			(pin tri_state line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "BA17")
				(number "45")
			)
			(pin tri_state line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "BA16")
				(number "46")
			)
			(pin tri_state line
				(at 17.78 0 180)
				(length 2.54)
				(name "BA15")
				(number "47")
			)
			(pin tri_state line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "BA14")
				(number "48")
			)
			(pin tri_state line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "BA13")
				(number "49")
			)
			(pin tri_state line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "BA12")
				(number "50")
			)
			(pin tri_state line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "BA11")
				(number "51")
			)
			(pin tri_state line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "BA10")
				(number "52")
			)
			(pin tri_state line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "BA09")
				(number "53")
			)
			(pin tri_state line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "BA08")
				(number "54")
			)
			(pin tri_state line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "BA07")
				(number "55")
			)
			(pin tri_state line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "BA06")
				(number "56")
			)
			(pin tri_state line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "BA05")
				(number "57")
			)
			(pin tri_state line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "BA04")
				(number "58")
			)
			(pin tri_state line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "BA03")
				(number "59")
			)
			(pin tri_state line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "BA02")
				(number "60")
			)
			(pin tri_state line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "BA01")
				(number "61")
			)
			(pin tri_state line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "BA00")
				(number "62")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Bus_M.2_Socket_A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -22.86 46.99 0)
		)
		(property "Value" "Bus_M.2_Socket_A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" ""
			(at 0 26.67 0)
		)
		(property "Datasheet" "https://web.archive.org/web/20200613074028/http://read.pudn.com/downloads794/doc/project/3133918/PCIe_M.2_Electromechanical_Spec_Rev1.0_Final_11012013_RS_Clean.pdf#page=148"
			(at 0 12.7 0)
		)
		(property "Description" "M.2 Socket 1-DP Mechanical Key A"
			(at 0 0 0)
		)
		(property "ki_keywords" "M2 NGNF PCI-E"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*M*2*A*"
			(at 0 0 0)
		)
		(symbol "Bus_M.2_Socket_A_0_1")
		(symbol "Bus_M.2_Socket_A_1_1"
			(pin output line
				(at -25.4 43.18 0)
				(length 2.54)
				(name "~{PERST0}")
				(number "52")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "~{CLKREQ0}")
				(number "53")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 2.54)
				(name "~{PEWAKE0}")
				(number "55")
			)
			(pin output line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "PETp0")
				(number "35")
			)
			(pin output line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "PETn0")
				(number "37")
			)
			(pin input line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "PERp0")
				(number "41")
			)
			(pin input line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PERn0")
				(number "43")
			)
			(pin output line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PETp1")
				(number "59")
			)
			(pin output line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "PETn1")
				(number "61")
			)
			(pin input line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PERp1")
				(number "65")
			)
			(pin input line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PERn1")
				(number "67")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "USB_D+")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "USB_D-")
				(number "5")
			)
			(pin output line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "~{PERST1}")
				(number "66")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "~{CLKREQ1}")
				(number "68")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "~{PEWAKE1}")
				(number "70")
			)
			(pin input line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "MLDIR_Sense")
				(number "17")
			)
			(pin output line
				(at -25.4 -35.56 0)
				(length 2.54)
				(name "REFCLKp0")
				(number "47")
			)
			(pin output line
				(at -25.4 -38.1 0)
				(length 2.54)
				(name "REFCLKn0")
				(number "49")
			)
			(pin output line
				(at -25.4 -40.64 0)
				(length 2.54)
				(name "REFCLKp1")
				(number "71")
			)
			(pin output line
				(at -25.4 -43.18 0)
				(length 2.54)
				(name "REFCLKn1")
				(number "73")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "3.3V")
				(number "2")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "3.3V")
				(number "4")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "3.3V")
				(number "72")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "3.3V")
				(number "74")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "36")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "51")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "57")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "69")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "75")
			)
			(pin passive line
				(at 25.4 43.18 180)
				(length 2.54)
				(name "RESERVED")
				(number "64")
			)
			(pin passive line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "VENDOR_DEFINED")
				(number "38")
			)
			(pin passive line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "VENDOR_DEFINED")
				(number "40")
			)
			(pin passive line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "VENDOR_DEFINED")
				(number "42")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "I2C_DATA")
				(number "58")
			)
			(pin output line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "I2C_CLK")
				(number "60")
			)
			(pin input line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "~{ALERT}")
				(number "62")
			)
			(pin output line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "~{W_DISABLE1}")
				(number "56")
			)
			(pin output line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "~{W_DISABLE2}")
				(number "54")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "DP_AUXn")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "DP_AUXp")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "DP_ML0n")
				(number "32")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "DP_ML0p")
				(number "34")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "DP_ML1n")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "DP_ML1p")
				(number "28")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "DP_ML2n")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "DP_ML2p")
				(number "27")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "DP_ML3n")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "DP_ML3p")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "DP_HPD")
				(number "31")
			)
			(pin open_collector line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "~{LED_1}")
				(number "6")
			)
			(pin open_collector line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "~{LED_2}")
				(number "16")
			)
			(pin output line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "SUSCLK")
				(number "50")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "COEX1")
				(number "48")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "COEX2")
				(number "46")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "COEX3")
				(number "44")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Bus_M.2_Socket_B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -22.86 46.99 0)
		)
		(property "Value" "Bus_M.2_Socket_B"
			(at 16.51 46.99 0)
		)
		(property "Footprint" ""
			(at 0 26.67 0)
		)
		(property "Datasheet" "https://web.archive.org/web/20200613074028/http://read.pudn.com/downloads794/doc/project/3133918/PCIe_M.2_Electromechanical_Spec_Rev1.0_Final_11012013_RS_Clean.pdf#page=154"
			(at 0 -25.4 0)
		)
		(property "Description" "M.2 Socket 2 Mechanical Key B"
			(at 0 0 0)
		)
		(property "ki_keywords" "M2 NGNF PCI-E"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*M*2*B*"
			(at 0 0 0)
		)
		(symbol "Bus_M.2_Socket_B_0_1")
		(symbol "Bus_M.2_Socket_B_1_1"
			(pin output line
				(at -25.4 43.18 0)
				(length 2.54)
				(name "~{PERST}")
				(number "50")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "~{CLKREQ}")
				(number "52")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 2.54)
				(name "~{PEWAKE}")
				(number "54")
			)
			(pin output line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "PETp0/SATA-A+")
				(number "49")
			)
			(pin output line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "PETn0/SATA-A-")
				(number "47")
			)
			(pin input line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "PERp0/SATA-B-")
				(number "43")
			)
			(pin input line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PERn0/SATA-B+")
				(number "41")
			)
			(pin output line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PETp1/USB3.0-Tx+/SSIC-TxP")
				(number "37")
			)
			(pin output line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "PETn1/USB3.0-Tx-/SSIC-TxN")
				(number "35")
			)
			(pin input line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PERp1/USB3.0-Rx+/SSIC-RxP")
				(number "31")
			)
			(pin input line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PERn1/USB3.0-Rx-/SSIC-RxN")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "USB_D+")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "USB_D-")
				(number "9")
			)
			(pin output line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "SIM_DETECT")
				(number "66")
			)
			(pin input line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "UIM-PWR")
				(number "36")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "UIM-DATA")
				(number "34")
			)
			(pin input line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "UIM-CLK")
				(number "32")
			)
			(pin input line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "UIM-RESET")
				(number "30")
			)
			(pin output line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "DEVSLP")
				(number "38")
			)
			(pin output line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "~{FULL_CARD_POWER_OFF}")
				(number "6")
			)
			(pin output line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "~{RESET}")
				(number "67")
			)
			(pin output line
				(at -25.4 -35.56 0)
				(length 2.54)
				(name "REFCLKp")
				(number "55")
			)
			(pin output line
				(at -25.4 -38.1 0)
				(length 2.54)
				(name "REFCLKn")
				(number "53")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "3.3V")
				(number "2")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "3.3V")
				(number "4")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "3.3V")
				(number "70")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "3.3V")
				(number "72")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "3.3V")
				(number "74")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "27")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "51")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "57")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "71")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "73")
			)
			(pin no_connect line
				(at 22.86 -40.64 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "58")
			)
			(pin no_connect line
				(at 22.86 -43.18 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "56")
			)
			(pin input line
				(at 25.4 43.18 180)
				(length 2.54)
				(name "CONFIG_0")
				(number "21")
			)
			(pin input line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "CONFIG_1")
				(number "69")
			)
			(pin input line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "CONFIG_2")
				(number "75")
			)
			(pin input line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "CONFIG_3")
				(number "1")
			)
			(pin input line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "ANTCTL0")
				(number "59")
			)
			(pin input line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "ANTCTL1")
				(number "61")
			)
			(pin input line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "ANTCTL2")
				(number "63")
			)
			(pin input line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "ANTCTL3")
				(number "65")
			)
			(pin output line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "~{W_DISABLE1}")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "GPIO_0")
				(number "40")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "GPIO_1")
				(number "42")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "GPIO_2")
				(number "44")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "GPIO_3")
				(number "46")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "GPIO_4")
				(number "48")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "GPIO_5")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "GPIO_6")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "GPIO_7")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "GPIO_8")
				(number "28")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "GPIO_9/DAS/~{DSS}/~{LED1}")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "GPIO_10")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "GPIO_11")
				(number "23")
			)
			(pin output line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "DPR")
				(number "25")
			)
			(pin output line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "SUSCLK")
				(number "68")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "COEX1")
				(number "64")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "COEX2")
				(number "62")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "COEX3")
				(number "60")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Bus_M.2_Socket_E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -22.86 46.99 0)
		)
		(property "Value" "Bus_M.2_Socket_E"
			(at 16.51 46.99 0)
		)
		(property "Footprint" ""
			(at 0 26.67 0)
		)
		(property "Datasheet" "https://web.archive.org/web/20200613074028/http://read.pudn.com/downloads794/doc/project/3133918/PCIe_M.2_Electromechanical_Spec_Rev1.0_Final_11012013_RS_Clean.pdf#page=150"
			(at 0 12.7 0)
		)
		(property "Description" "M.2 Socket 1-SD Mechanical Key E"
			(at 0 0 0)
		)
		(property "ki_keywords" "M2 NGNF PCI-E"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*M*2*E*"
			(at 0 0 0)
		)
		(symbol "Bus_M.2_Socket_E_0_1")
		(symbol "Bus_M.2_Socket_E_1_1"
			(pin output line
				(at -25.4 43.18 0)
				(length 2.54)
				(name "~{PERST0}")
				(number "52")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "~{CLKREQ0}")
				(number "53")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 2.54)
				(name "~{PEWAKE0}")
				(number "55")
			)
			(pin output line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "PETp0")
				(number "35")
			)
			(pin output line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "PETn0")
				(number "37")
			)
			(pin input line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "PERp0")
				(number "41")
			)
			(pin input line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PERn0")
				(number "43")
			)
			(pin output line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "RESERVED/PETp1")
				(number "59")
			)
			(pin output line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "RESERVED/PETn1")
				(number "61")
			)
			(pin input line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "RESERVED/PERp1")
				(number "65")
			)
			(pin input line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "RESERVED/PERn1")
				(number "67")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "USB_D+")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "USB_D-")
				(number "5")
			)
			(pin output line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "UIM_SWP/~{PERST1}")
				(number "66")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "UIM_POWER_SNK/~{CLKREQ1}")
				(number "68")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "UIM_POWER_SRC/GPIO1/~{PEWAKE1}")
				(number "70")
			)
			(pin output line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "SDIO_CLK")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "SDIO_CMD")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "SDIO_DATA0")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "SDIO_DATA1")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "SDIO_DATA2")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "SDIO_DATA3")
				(number "19")
			)
			(pin input line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "~{SDIO_WAKE}")
				(number "21")
			)
			(pin output line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "~{SDIO_RESET}")
				(number "23")
			)
			(pin output line
				(at -25.4 -35.56 0)
				(length 2.54)
				(name "REFCLKp0")
				(number "47")
			)
			(pin output line
				(at -25.4 -38.1 0)
				(length 2.54)
				(name "REFCLKn0")
				(number "49")
			)
			(pin output line
				(at -25.4 -40.64 0)
				(length 2.54)
				(name "RESERVED/REFCLKp1")
				(number "71")
			)
			(pin output line
				(at -25.4 -43.18 0)
				(length 2.54)
				(name "RESERVED/REFCLKn1")
				(number "73")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "3.3V")
				(number "2")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "3.3V")
				(number "4")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "3.3V")
				(number "72")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "3.3V")
				(number "74")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "51")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "57")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "69")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "75")
			)
			(pin passive line
				(at 25.4 43.18 180)
				(length 2.54)
				(name "RESERVED")
				(number "64")
			)
			(pin passive line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "VENDOR_DEFINED")
				(number "38")
			)
			(pin passive line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "VENDOR_DEFINED")
				(number "40")
			)
			(pin passive line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "VENDOR_DEFINED")
				(number "42")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "I2C_DATA")
				(number "58")
			)
			(pin output line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "I2C_CLK")
				(number "60")
			)
			(pin input line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "~{ALERT}")
				(number "62")
			)
			(pin output line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "~{W_DISABLE1}")
				(number "56")
			)
			(pin output line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "~{W_DISABLE2}")
				(number "54")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PCM_CLK/I2S_SCK")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PCM_SYNC/I2S_WS")
				(number "10")
			)
			(pin input line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PCM_IN/I2S_SD_IN")
				(number "12")
			)
			(pin output line
				(at 25.4 0 180)
				(length 2.54)
				(name "PCM_OUT/I2S_SD_OUT")
				(number "14")
			)
			(pin input line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "~{UART_WAKE}")
				(number "20")
			)
			(pin input line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "UART_RXD")
				(number "22")
			)
			(pin output line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "UART_TXD")
				(number "32")
			)
			(pin input line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "UART_CTS")
				(number "34")
			)
			(pin output line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "UART_RTS")
				(number "36")
			)
			(pin open_collector line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "~{LED_1}")
				(number "6")
			)
			(pin open_collector line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "~{LED_2}")
				(number "16")
			)
			(pin output line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "SUSCLK")
				(number "50")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "COEX1")
				(number "48")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "COEX2")
				(number "46")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "COEX3")
				(number "44")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Bus_M.2_Socket_M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -22.86 46.99 0)
		)
		(property "Value" "Bus_M.2_Socket_M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" ""
			(at 0 26.67 0)
		)
		(property "Datasheet" "https://web.archive.org/web/20200613074028/http://read.pudn.com/downloads794/doc/project/3133918/PCIe_M.2_Electromechanical_Spec_Rev1.0_Final_11012013_RS_Clean.pdf#page=155"
			(at 0 35.56 0)
		)
		(property "Description" "M.2 Socket 3 Mechanical Key M"
			(at 0 0 0)
		)
		(property "ki_keywords" "M2 NGNF PCI-E"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*M*2*M*"
			(at 0 0 0)
		)
		(symbol "Bus_M.2_Socket_M_0_1")
		(symbol "Bus_M.2_Socket_M_1_1"
			(pin output line
				(at -25.4 43.18 0)
				(length 2.54)
				(name "~{PERST}")
				(number "50")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "~{CLKREQ}")
				(number "52")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 2.54)
				(name "~{PEWAKE}")
				(number "54")
			)
			(pin output line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "PETp0/SATA-A+")
				(number "49")
			)
			(pin output line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "PETn0/SATA-A-")
				(number "47")
			)
			(pin input line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "PERp0/SATA-B-")
				(number "43")
			)
			(pin input line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PERn0/SATA-B+")
				(number "41")
			)
			(pin output line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PETp1")
				(number "37")
			)
			(pin output line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "PETn1")
				(number "35")
			)
			(pin input line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PERp1")
				(number "31")
			)
			(pin input line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PERn1")
				(number "29")
			)
			(pin output line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PETp2")
				(number "25")
			)
			(pin output line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PETn2")
				(number "23")
			)
			(pin input line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PERp2")
				(number "19")
			)
			(pin input line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PERn2")
				(number "17")
			)
			(pin output line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PETp3")
				(number "13")
			)
			(pin output line
				(at -25.4 0 0)
				(length 2.54)
				(name "PETn3")
				(number "11")
			)
			(pin input line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PERp3")
				(number "7")
			)
			(pin input line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PERn3")
				(number "5")
			)
			(pin output line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "DEVSLP")
				(number "38")
			)
			(pin output line
				(at -25.4 -35.56 0)
				(length 2.54)
				(name "REFCLKp")
				(number "55")
			)
			(pin output line
				(at -25.4 -38.1 0)
				(length 2.54)
				(name "REFCLKn")
				(number "53")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "3.3V")
				(number "12")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "3.3V")
				(number "14")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "3.3V")
				(number "16")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "3.3V")
				(number "18")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "3.3V")
				(number "2")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "3.3V")
				(number "4")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "3.3V")
				(number "70")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "3.3V")
				(number "72")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "3.3V")
				(number "74")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "27")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "51")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "57")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "71")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "73")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "75")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin no_connect line
				(at 22.86 40.64 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "58")
			)
			(pin no_connect line
				(at 22.86 38.1 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "56")
			)
			(pin no_connect line
				(at 22.86 35.56 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "48")
			)
			(pin no_connect line
				(at 22.86 33.02 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "46")
			)
			(pin no_connect line
				(at 22.86 30.48 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "44")
			)
			(pin no_connect line
				(at 22.86 27.94 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "42")
			)
			(pin no_connect line
				(at 22.86 25.4 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "40")
			)
			(pin no_connect line
				(at 22.86 22.86 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "36")
			)
			(pin no_connect line
				(at 22.86 20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin no_connect line
				(at 22.86 17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "32")
			)
			(pin no_connect line
				(at 22.86 15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "30")
			)
			(pin no_connect line
				(at 22.86 12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin no_connect line
				(at 22.86 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "26")
			)
			(pin no_connect line
				(at 22.86 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin no_connect line
				(at 22.86 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin no_connect line
				(at 22.86 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at 22.86 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 22.86 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 22.86 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "67")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "DAS/~{DSS}/~{LED1}")
				(number "10")
			)
			(pin passive line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PEDET")
				(number "69")
			)
			(pin output line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "SUSCLK")
				(number "68")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Bus_PCI_32bit_5V"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 80.01 0)
		)
		(property "Value" "Bus_PCI_32bit_5V"
			(at 0 -82.55 0)
		)
		(property "Footprint" ""
			(at 0 -1.27 0)
		)
		(property "Datasheet" "http://pinouts.ru/Slots/PCI_pinout.shtml"
			(at 0 -1.27 0)
		)
		(property "Description" "PCI bus connector for 5V cards"
			(at 0 0 0)
		)
		(property "ki_keywords" "PCI 5V"
			(at 0 0 0)
		)
		(symbol "Bus_PCI_32bit_5V_0_1")
		(symbol "Bus_PCI_32bit_5V_1_1"
			(pin power_in line
				(at -22.86 76.2 0)
				(length 3.81)
				(name "-12V")
				(number "B1")
			)
			(pin output line
				(at -22.86 73.66 0)
				(length 3.81)
				(name "TCK")
				(number "B2")
			)
			(pin power_in line
				(at -22.86 71.12 0)
				(length 3.81)
				(name "GND")
				(number "B3")
			)
			(pin input line
				(at -22.86 68.58 0)
				(length 3.81)
				(name "TDO")
				(number "B4")
			)
			(pin power_in line
				(at -22.86 66.04 0)
				(length 3.81)
				(name "+5V")
				(number "B5")
			)
			(pin power_in line
				(at -22.86 63.5 0)
				(length 3.81)
				(name "+5V")
				(number "B6")
			)
			(pin input line
				(at -22.86 60.96 0)
				(length 3.81)
				(name "INTB#")
				(number "B7")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 3.81)
				(name "INTD#")
				(number "B8")
			)
			(pin input line
				(at -22.86 55.88 0)
				(length 3.81)
				(name "PRSNT1#")
				(number "B9")
			)
			(pin passive line
				(at -22.86 53.34 0)
				(length 3.81)
				(name "RESERVED")
				(number "B10")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 3.81)
				(name "PRSNT2#")
				(number "B11")
			)
			(pin power_in line
				(at -22.86 48.26 0)
				(length 3.81)
				(name "GND")
				(number "B12")
			)
			(pin power_in line
				(at -22.86 45.72 0)
				(length 3.81)
				(name "GND")
				(number "B13")
			)
			(pin passive line
				(at -22.86 43.18 0)
				(length 3.81)
				(name "RESERVED")
				(number "B14")
			)
			(pin power_in line
				(at -22.86 40.64 0)
				(length 3.81)
				(name "GND")
				(number "B15")
			)
			(pin output line
				(at -22.86 38.1 0)
				(length 3.81)
				(name "CLK")
				(number "B16")
			)
			(pin power_in line
				(at -22.86 35.56 0)
				(length 3.81)
				(name "GND")
				(number "B17")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 3.81)
				(name "REQ#")
				(number "B18")
			)
			(pin power_in line
				(at -22.86 30.48 0)
				(length 3.81)
				(name "+5V")
				(number "B19")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 3.81)
				(name "AD[31]")
				(number "B20")
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 3.81)
				(name "AD[29]")
				(number "B21")
			)
			(pin power_in line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "GND")
				(number "B22")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "AD[27]")
				(number "B23")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "AD[25]")
				(number "B24")
			)
			(pin power_in line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "+3.3V")
				(number "B25")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "C/BE#[3]")
				(number "B26")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "AD[23]")
				(number "B27")
			)
			(pin power_in line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "GND")
				(number "B28")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "AD[21]")
				(number "B29")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "AD[19]")
				(number "B30")
			)
			(pin power_in line
				(at -22.86 0 0)
				(length 3.81)
				(name "+3.3V")
				(number "B31")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "AD[17]")
				(number "B32")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "C/BE#[2]")
				(number "B33")
			)
			(pin power_in line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "GND")
				(number "B34")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "IRDY#")
				(number "B35")
			)
			(pin power_in line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "+3.3V")
				(number "B36")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "DEVSEL#")
				(number "B37")
			)
			(pin power_in line
				(at -22.86 -17.78 0)
				(length 3.81)
				(name "GND")
				(number "B38")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "LOCK#")
				(number "B39")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 3.81)
				(name "PERR#")
				(number "B40")
			)
			(pin power_in line
				(at -22.86 -25.4 0)
				(length 3.81)
				(name "+3.3V")
				(number "B41")
			)
			(pin input line
				(at -22.86 -27.94 0)
				(length 3.81)
				(name "SERR#")
				(number "B42")
			)
			(pin power_in line
				(at -22.86 -30.48 0)
				(length 3.81)
				(name "+3.3V")
				(number "B43")
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 3.81)
				(name "C/BE#[1]")
				(number "B44")
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 3.81)
				(name "AD[14]")
				(number "B45")
			)
			(pin power_in line
				(at -22.86 -38.1 0)
				(length 3.81)
				(name "GND")
				(number "B46")
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 3.81)
				(name "AD[12]")
				(number "B47")
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 3.81)
				(name "AD[10]")
				(number "B48")
			)
			(pin power_in line
				(at -22.86 -45.72 0)
				(length 3.81)
				(name "GND")
				(number "B49")
			)
			(pin bidirectional line
				(at -22.86 -53.34 0)
				(length 3.81)
				(name "AD[08]")
				(number "B52")
			)
			(pin bidirectional line
				(at -22.86 -55.88 0)
				(length 3.81)
				(name "AD[07]")
				(number "B53")
			)
			(pin input line
				(at -22.86 -58.42 0)
				(length 3.81)
				(name "+3.3V")
				(number "B54")
			)
			(pin bidirectional line
				(at -22.86 -60.96 0)
				(length 3.81)
				(name "AD[05]")
				(number "B55")
			)
			(pin bidirectional line
				(at -22.86 -63.5 0)
				(length 3.81)
				(name "AD[03]")
				(number "B56")
			)
			(pin power_in line
				(at -22.86 -66.04 0)
				(length 3.81)
				(name "GND")
				(number "B57")
			)
			(pin bidirectional line
				(at -22.86 -68.58 0)
				(length 3.81)
				(name "AD[01]")
				(number "B58")
			)
			(pin power_in line
				(at -22.86 -71.12 0)
				(length 3.81)
				(name "+5V")
				(number "B59")
			)
			(pin bidirectional line
				(at -22.86 -73.66 0)
				(length 3.81)
				(name "ACK64#")
				(number "B60")
			)
			(pin power_in line
				(at -22.86 -76.2 0)
				(length 3.81)
				(name "+5V")
				(number "B61")
			)
			(pin power_in line
				(at -22.86 -78.74 0)
				(length 3.81)
				(name "+5V")
				(number "B62")
			)
			(pin output line
				(at 22.86 76.2 180)
				(length 3.81)
				(name "TRST#")
				(number "A1")
			)
			(pin power_in line
				(at 22.86 73.66 180)
				(length 3.81)
				(name "+12V")
				(number "A2")
			)
			(pin output line
				(at 22.86 71.12 180)
				(length 3.81)
				(name "TMS")
				(number "A3")
			)
			(pin output line
				(at 22.86 68.58 180)
				(length 3.81)
				(name "TDI")
				(number "A4")
			)
			(pin power_in line
				(at 22.86 66.04 180)
				(length 3.81)
				(name "+5V")
				(number "A5")
			)
			(pin input line
				(at 22.86 63.5 180)
				(length 3.81)
				(name "INTA#")
				(number "A6")
			)
			(pin input line
				(at 22.86 60.96 180)
				(length 3.81)
				(name "INTC#")
				(number "A7")
			)
			(pin power_in line
				(at 22.86 58.42 180)
				(length 3.81)
				(name "+5V")
				(number "A8")
			)
			(pin passive line
				(at 22.86 55.88 180)
				(length 3.81)
				(name "RESERVED")
				(number "A9")
			)
			(pin power_in line
				(at 22.86 53.34 180)
				(length 3.81)
				(name "+5V")
				(number "A10")
			)
			(pin passive line
				(at 22.86 50.8 180)
				(length 3.81)
				(name "RESERVED")
				(number "A11")
			)
			(pin power_in line
				(at 22.86 48.26 180)
				(length 3.81)
				(name "GND")
				(number "A12")
			)
			(pin power_in line
				(at 22.86 45.72 180)
				(length 3.81)
				(name "GND")
				(number "A13")
			)
			(pin passive line
				(at 22.86 43.18 180)
				(length 3.81)
				(name "RESERVED")
				(number "A14")
			)
			(pin output line
				(at 22.86 40.64 180)
				(length 3.81)
				(name "RST#")
				(number "A15")
			)
			(pin power_in line
				(at 22.86 38.1 180)
				(length 3.81)
				(name "+5V")
				(number "A16")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 3.81)
				(name "GNT#")
				(number "A17")
			)
			(pin power_in line
				(at 22.86 33.02 180)
				(length 3.81)
				(name "GND")
				(number "A18")
			)
			(pin passive line
				(at 22.86 30.48 180)
				(length 3.81)
				(name "RESERVED")
				(number "A19")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 3.81)
				(name "AD[30]")
				(number "A20")
			)
			(pin power_in line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "+3.3V")
				(number "A21")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 3.81)
				(name "AD[28]")
				(number "A22")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "AD[26]")
				(number "A23")
			)
			(pin power_in line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "GND")
				(number "A24")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "AD[24]")
				(number "A25")
			)
			(pin output line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "IDSEL")
				(number "A26")
			)
			(pin power_in line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "+3.3V")
				(number "A27")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "AD[22]")
				(number "A28")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "AD[20]")
				(number "A29")
			)
			(pin power_in line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "GND")
				(number "A30")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "AD[18]")
				(number "A31")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "AD[16]")
				(number "A32")
			)
			(pin power_in line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "+3.3V")
				(number "A33")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "FRAME#")
				(number "A34")
			)
			(pin power_in line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "GND")
				(number "A35")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "TRDY#")
				(number "A36")
			)
			(pin power_in line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "GND")
				(number "A37")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "STOP#")
				(number "A38")
			)
			(pin power_in line
				(at 22.86 -20.32 180)
				(length 3.81)
				(name "+3.3V")
				(number "A39")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "SDONE")
				(number "A40")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 3.81)
				(name "SBO#")
				(number "A41")
			)
			(pin power_in line
				(at 22.86 -27.94 180)
				(length 3.81)
				(name "GND")
				(number "A42")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 3.81)
				(name "PAR")
				(number "A43")
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 3.81)
				(name "AD[15]")
				(number "A44")
			)
			(pin power_in line
				(at 22.86 -35.56 180)
				(length 3.81)
				(name "+3.3V")
				(number "A45")
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 3.81)
				(name "AD[13]")
				(number "A46")
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 3.81)
				(name "AD[11]")
				(number "A47")
			)
			(pin power_in line
				(at 22.86 -43.18 180)
				(length 3.81)
				(name "GND")
				(number "A48")
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 3.81)
				(name "AD[09]")
				(number "A49")
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 3.81)
				(name "C/BE#[0]")
				(number "A52")
			)
			(pin power_in line
				(at 22.86 -55.88 180)
				(length 3.81)
				(name "+3.3V")
				(number "A53")
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 3.81)
				(name "AD[06]")
				(number "A54")
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 3.81)
				(name "AD[04]")
				(number "A55")
			)
			(pin power_in line
				(at 22.86 -63.5 180)
				(length 3.81)
				(name "GND")
				(number "A56")
			)
			(pin bidirectional line
				(at 22.86 -66.04 180)
				(length 3.81)
				(name "AD[02]")
				(number "A57")
			)
			(pin bidirectional line
				(at 22.86 -68.58 180)
				(length 3.81)
				(name "AD[00]")
				(number "A58")
			)
			(pin power_in line
				(at 22.86 -71.12 180)
				(length 3.81)
				(name "+5V")
				(number "A59")
			)
			(pin bidirectional line
				(at 22.86 -73.66 180)
				(length 3.81)
				(name "REQ64#")
				(number "A60")
			)
			(pin power_in line
				(at 22.86 -76.2 180)
				(length 3.81)
				(name "+5V")
				(number "A61")
			)
			(pin power_in line
				(at 22.86 -78.74 180)
				(length 3.81)
				(name "+5V")
				(number "A62")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Bus_PCI_32bit_Universal"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 80.01 0)
		)
		(property "Value" "Bus_PCI_32bit_Universal"
			(at 0 -82.55 0)
		)
		(property "Footprint" ""
			(at 0 -1.27 0)
		)
		(property "Datasheet" "http://pinouts.ru/Slots/PCI_pinout.shtml"
			(at 0 -1.27 0)
		)
		(property "Description" "PCI bus connector for universal 5V/3.3V cards"
			(at 0 0 0)
		)
		(property "ki_keywords" "PCI 5V 3.3V 3V3"
			(at 0 0 0)
		)
		(symbol "Bus_PCI_32bit_Universal_0_1")
		(symbol "Bus_PCI_32bit_Universal_1_1"
			(pin power_in line
				(at -22.86 76.2 0)
				(length 3.81)
				(name "-12V")
				(number "B1")
			)
			(pin output line
				(at -22.86 73.66 0)
				(length 3.81)
				(name "TCK")
				(number "B2")
			)
			(pin power_in line
				(at -22.86 71.12 0)
				(length 3.81)
				(name "GND")
				(number "B3")
			)
			(pin input line
				(at -22.86 68.58 0)
				(length 3.81)
				(name "TDO")
				(number "B4")
			)
			(pin power_in line
				(at -22.86 66.04 0)
				(length 3.81)
				(name "+5V")
				(number "B5")
			)
			(pin power_in line
				(at -22.86 63.5 0)
				(length 3.81)
				(name "+5V")
				(number "B6")
			)
			(pin input line
				(at -22.86 60.96 0)
				(length 3.81)
				(name "~{INTB#}")
				(number "B7")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 3.81)
				(name "~{INTD#}")
				(number "B8")
			)
			(pin input line
				(at -22.86 55.88 0)
				(length 3.81)
				(name "~{PRSNT1#}")
				(number "B9")
			)
			(pin passive line
				(at -22.86 53.34 0)
				(length 3.81)
				(name "RESERVED")
				(number "B10")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 3.81)
				(name "~{PRSNT2#}")
				(number "B11")
			)
			(pin passive line
				(at -22.86 43.18 0)
				(length 3.81)
				(name "RESERVED")
				(number "B14")
			)
			(pin power_in line
				(at -22.86 40.64 0)
				(length 3.81)
				(name "GND")
				(number "B15")
			)
			(pin output line
				(at -22.86 38.1 0)
				(length 3.81)
				(name "CLK")
				(number "B16")
			)
			(pin power_in line
				(at -22.86 35.56 0)
				(length 3.81)
				(name "GND")
				(number "B17")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 3.81)
				(name "~{REQ#}")
				(number "B18")
			)
			(pin power_in line
				(at -22.86 30.48 0)
				(length 3.81)
				(name "VIO")
				(number "B19")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 3.81)
				(name "AD[31]")
				(number "B20")
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 3.81)
				(name "AD[29]")
				(number "B21")
			)
			(pin power_in line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "GND")
				(number "B22")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "AD[27]")
				(number "B23")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "AD[25]")
				(number "B24")
			)
			(pin power_in line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "+3.3V")
				(number "B25")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "C/BE#[3]")
				(number "B26")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "AD[23]")
				(number "B27")
			)
			(pin power_in line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "GND")
				(number "B28")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "AD[21]")
				(number "B29")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "AD[19]")
				(number "B30")
			)
			(pin power_in line
				(at -22.86 0 0)
				(length 3.81)
				(name "+3.3V")
				(number "B31")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "AD[17]")
				(number "B32")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "~{C/BE#[2]}")
				(number "B33")
			)
			(pin power_in line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "GND")
				(number "B34")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "~{IRDY#}")
				(number "B35")
			)
			(pin power_in line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "+3.3V")
				(number "B36")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "~{DEVSEL#}")
				(number "B37")
			)
			(pin power_in line
				(at -22.86 -17.78 0)
				(length 3.81)
				(name "GND")
				(number "B38")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "~{LOCK#}")
				(number "B39")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 3.81)
				(name "~{PERR#}")
				(number "B40")
			)
			(pin power_in line
				(at -22.86 -25.4 0)
				(length 3.81)
				(name "+3.3V")
				(number "B41")
			)
			(pin input line
				(at -22.86 -27.94 0)
				(length 3.81)
				(name "~{SERR#}")
				(number "B42")
			)
			(pin power_in line
				(at -22.86 -30.48 0)
				(length 3.81)
				(name "+3.3V")
				(number "B43")
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 3.81)
				(name "~{C/BE#[1]}")
				(number "B44")
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 3.81)
				(name "AD[14]")
				(number "B45")
			)
			(pin power_in line
				(at -22.86 -38.1 0)
				(length 3.81)
				(name "GND")
				(number "B46")
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 3.81)
				(name "AD[12]")
				(number "B47")
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 3.81)
				(name "AD[10]")
				(number "B48")
			)
			(pin power_in line
				(at -22.86 -45.72 0)
				(length 3.81)
				(name "M66EN")
				(number "B49")
			)
			(pin bidirectional line
				(at -22.86 -53.34 0)
				(length 3.81)
				(name "AD[08]")
				(number "B52")
			)
			(pin bidirectional line
				(at -22.86 -55.88 0)
				(length 3.81)
				(name "AD[07]")
				(number "B53")
			)
			(pin input line
				(at -22.86 -58.42 0)
				(length 3.81)
				(name "+3.3V")
				(number "B54")
			)
			(pin bidirectional line
				(at -22.86 -60.96 0)
				(length 3.81)
				(name "AD[05]")
				(number "B55")
			)
			(pin bidirectional line
				(at -22.86 -63.5 0)
				(length 3.81)
				(name "AD[03]")
				(number "B56")
			)
			(pin power_in line
				(at -22.86 -66.04 0)
				(length 3.81)
				(name "GND")
				(number "B57")
			)
			(pin bidirectional line
				(at -22.86 -68.58 0)
				(length 3.81)
				(name "AD[01]")
				(number "B58")
			)
			(pin power_in line
				(at -22.86 -71.12 0)
				(length 3.81)
				(name "VIO")
				(number "B59")
			)
			(pin bidirectional line
				(at -22.86 -73.66 0)
				(length 3.81)
				(name "~{ACK64#}")
				(number "B60")
			)
			(pin power_in line
				(at -22.86 -76.2 0)
				(length 3.81)
				(name "+5V")
				(number "B61")
			)
			(pin power_in line
				(at -22.86 -78.74 0)
				(length 3.81)
				(name "+5V")
				(number "B62")
			)
			(pin output line
				(at 22.86 76.2 180)
				(length 3.81)
				(name "~{TRST#}")
				(number "A1")
			)
			(pin power_in line
				(at 22.86 73.66 180)
				(length 3.81)
				(name "+12V")
				(number "A2")
			)
			(pin output line
				(at 22.86 71.12 180)
				(length 3.81)
				(name "TMS")
				(number "A3")
			)
			(pin output line
				(at 22.86 68.58 180)
				(length 3.81)
				(name "TDI")
				(number "A4")
			)
			(pin power_in line
				(at 22.86 66.04 180)
				(length 3.81)
				(name "+5V")
				(number "A5")
			)
			(pin input line
				(at 22.86 63.5 180)
				(length 3.81)
				(name "~{INTA#}")
				(number "A6")
			)
			(pin input line
				(at 22.86 60.96 180)
				(length 3.81)
				(name "~{INTC#}")
				(number "A7")
			)
			(pin power_in line
				(at 22.86 58.42 180)
				(length 3.81)
				(name "+5V")
				(number "A8")
			)
			(pin passive line
				(at 22.86 55.88 180)
				(length 3.81)
				(name "RESERVED")
				(number "A9")
			)
			(pin power_in line
				(at 22.86 53.34 180)
				(length 3.81)
				(name "VIO")
				(number "A10")
			)
			(pin passive line
				(at 22.86 50.8 180)
				(length 3.81)
				(name "RESERVED")
				(number "A11")
			)
			(pin passive line
				(at 22.86 43.18 180)
				(length 3.81)
				(name "3.3VAUX")
				(number "A14")
			)
			(pin output line
				(at 22.86 40.64 180)
				(length 3.81)
				(name "~{RST#}")
				(number "A15")
			)
			(pin power_in line
				(at 22.86 38.1 180)
				(length 3.81)
				(name "VIO")
				(number "A16")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 3.81)
				(name "~{GNT#}")
				(number "A17")
			)
			(pin power_in line
				(at 22.86 33.02 180)
				(length 3.81)
				(name "GND")
				(number "A18")
			)
			(pin passive line
				(at 22.86 30.48 180)
				(length 3.81)
				(name "PME#")
				(number "A19")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 3.81)
				(name "AD[30]")
				(number "A20")
			)
			(pin power_in line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "+3.3V")
				(number "A21")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 3.81)
				(name "AD[28]")
				(number "A22")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "AD[26]")
				(number "A23")
			)
			(pin power_in line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "GND")
				(number "A24")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "AD[24]")
				(number "A25")
			)
			(pin output line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "IDSEL")
				(number "A26")
			)
			(pin power_in line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "+3.3V")
				(number "A27")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "AD[22]")
				(number "A28")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "AD[20]")
				(number "A29")
			)
			(pin power_in line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "GND")
				(number "A30")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "AD[18]")
				(number "A31")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "AD[16]")
				(number "A32")
			)
			(pin power_in line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "+3.3V")
				(number "A33")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "~{FRAME#}")
				(number "A34")
			)
			(pin power_in line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "GND")
				(number "A35")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "~{TRDY#}")
				(number "A36")
			)
			(pin power_in line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "GND")
				(number "A37")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "~{STOP#}")
				(number "A38")
			)
			(pin power_in line
				(at 22.86 -20.32 180)
				(length 3.81)
				(name "+3.3V")
				(number "A39")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "RESERVED")
				(number "A40")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 3.81)
				(name "RESERVED")
				(number "A41")
			)
			(pin power_in line
				(at 22.86 -27.94 180)
				(length 3.81)
				(name "GND")
				(number "A42")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 3.81)
				(name "PAR")
				(number "A43")
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 3.81)
				(name "AD[15]")
				(number "A44")
			)
			(pin power_in line
				(at 22.86 -35.56 180)
				(length 3.81)
				(name "+3.3V")
				(number "A45")
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 3.81)
				(name "AD[13]")
				(number "A46")
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 3.81)
				(name "AD[11]")
				(number "A47")
			)
			(pin power_in line
				(at 22.86 -43.18 180)
				(length 3.81)
				(name "GND")
				(number "A48")
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 3.81)
				(name "AD[09]")
				(number "A49")
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 3.81)
				(name "~{C/BE#[0]}")
				(number "A52")
			)
			(pin power_in line
				(at 22.86 -55.88 180)
				(length 3.81)
				(name "+3.3V")
				(number "A53")
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 3.81)
				(name "AD[06]")
				(number "A54")
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 3.81)
				(name "AD[04]")
				(number "A55")
			)
			(pin power_in line
				(at 22.86 -63.5 180)
				(length 3.81)
				(name "GND")
				(number "A56")
			)
			(pin bidirectional line
				(at 22.86 -66.04 180)
				(length 3.81)
				(name "AD[02]")
				(number "A57")
			)
			(pin bidirectional line
				(at 22.86 -68.58 180)
				(length 3.81)
				(name "AD[00]")
				(number "A58")
			)
			(pin power_in line
				(at 22.86 -71.12 180)
				(length 3.81)
				(name "VIO")
				(number "A59")
			)
			(pin bidirectional line
				(at 22.86 -73.66 180)
				(length 3.81)
				(name "~{REQ64#}")
				(number "A60")
			)
			(pin power_in line
				(at 22.86 -76.2 180)
				(length 3.81)
				(name "+5V")
				(number "A61")
			)
			(pin power_in line
				(at 22.86 -78.74 180)
				(length 3.81)
				(name "+5V")
				(number "A62")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Bus_PCI_Express_Mini"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -16.51 31.75 0)
		)
		(property "Value" "Bus_PCI_Express_Mini"
			(at 22.86 31.75 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at -3.81 -29.21 0)
		)
		(property "Description" "Mini-PCI Express bus connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "mini pcie"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PCI*Express*Mini*"
			(at 0 0 0)
		)
		(symbol "Bus_PCI_Express_Mini_0_1")
		(symbol "Bus_PCI_Express_Mini_1_1"
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "USB_D+")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "USB_D-")
				(number "36")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PETp0")
				(number "33")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PETn0")
				(number "31")
			)
			(pin output line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PERp0")
				(number "25")
			)
			(pin output line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PERn0")
				(number "23")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "REFCLK+")
				(number "13")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "REFCLK-")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "SMB_DATA")
				(number "32")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "SMB_CLK")
				(number "30")
			)
			(pin open_collector line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "~{WAKE}")
				(number "1")
			)
			(pin open_collector line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "~{CLKREQ}")
				(number "7")
			)
			(pin input line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "~{W_DISABLE}")
				(number "20")
			)
			(pin input line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "~{PERST}")
				(number "22")
			)
			(pin power_in line
				(at -10.16 33.02 270)
				(length 2.54)
				(name "+3V3AUX")
				(number "2")
			)
			(pin power_in line
				(at -7.62 33.02 270)
				(length 2.54)
				(name "+3V3AUX")
				(number "24")
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 2.54)
				(name "+3V3AUX")
				(number "39")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "+3V3AUX")
				(number "41")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "+3V3AUX")
				(number "52")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "27")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "37")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "40")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "50")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 2.54 -30.48 90)
				(length 2.54)
				(name "MP")
				(number "MP")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 2.54)
				(name "+1V5")
				(number "6")
			)
			(pin power_in line
				(at 7.62 33.02 270)
				(length 2.54)
				(name "+1V5")
				(number "28")
			)
			(pin power_in line
				(at 10.16 33.02 270)
				(length 2.54)
				(name "+1V5")
				(number "48")
			)
			(pin open_collector line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "~{LED_WPAN}")
				(number "46")
			)
			(pin open_collector line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "~{LED_WLAN}")
				(number "44")
			)
			(pin open_collector line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "~{LED_WWAN}")
				(number "42")
			)
			(pin passive line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "COEX1")
				(number "3")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "COEX2")
				(number "5")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "Reserved")
				(number "45")
			)
			(pin passive line
				(at 17.78 0 180)
				(length 2.54)
				(name "Reserved")
				(number "47")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "Reserved")
				(number "49")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "Reserved")
				(number "51")
			)
			(pin power_out line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "UIM_VPP")
				(number "16")
			)
			(pin power_out line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "UIM_PWR")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "UIM_DATA")
				(number "10")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "UIM_CLK")
				(number "12")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "~{UIM_RESET}")
				(number "14")
			)
			(pin passive line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "UIM_C4")
				(number "19")
			)
			(pin passive line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "UIM_C8")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Bus_PCI_Express_x1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -8.89 22.86 0)
		)
		(property "Value" "Bus_PCI_Express_x1"
			(at 12.7 22.86 0)
		)
		(property "Footprint" "Connector_PCBEdge:BUS_PCIexpress_x1"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.ritrontek.com/uploadfile/2016/1026/20161026105231124.pdf#page=63"
			(at -6.35 -19.05 0)
		)
		(property "Description" "PCI Express bus connector x1"
			(at 0 0 0)
		)
		(property "ki_keywords" "pcie"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PCIexpress*"
			(at 0 0 0)
		)
		(symbol "Bus_PCI_Express_x1_0_1")
		(symbol "Bus_PCI_Express_x1_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 3.81)
				(name "SMCLK")
				(number "B5")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 3.81)
				(name "SMDAT")
				(number "B6")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "REFCLK+")
				(number "A13")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "REFCLK-")
				(number "A14")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "~{PRSNT1}")
				(number "A1")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 3.81)
				(name "~{PRSNT2}")
				(number "B17")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "PETp0")
				(number "B14")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 3.81)
				(name "PETn0")
				(number "B15")
			)
			(pin passive line
				(at -2.54 25.4 270)
				(length 3.81)
				(hide yes)
				(name "+12V")
				(number "A2")
			)
			(pin passive line
				(at -2.54 25.4 270)
				(length 3.81)
				(hide yes)
				(name "+12V")
				(number "A3")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 3.81)
				(name "+12V")
				(number "B1")
			)
			(pin passive line
				(at -2.54 25.4 270)
				(length 3.81)
				(hide yes)
				(name "+12V")
				(number "B2")
			)
			(pin passive line
				(at -2.54 25.4 270)
				(length 3.81)
				(hide yes)
				(name "+12V")
				(number "B3")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "3.3Vaux")
				(number "B10")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A12")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A15")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A18")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A4")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B13")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B16")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B18")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "GND")
				(number "B4")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B7")
			)
			(pin passive line
				(at 2.54 25.4 270)
				(length 3.81)
				(hide yes)
				(name "+3.3V")
				(number "A10")
			)
			(pin passive line
				(at 2.54 25.4 270)
				(length 3.81)
				(hide yes)
				(name "+3.3V")
				(number "A9")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 3.81)
				(name "+3.3V")
				(number "B8")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 3.81)
				(name "RSVD")
				(number "B12")
			)
			(pin open_collector line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "~{WAKE}")
				(number "B11")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "~{PERST}")
				(number "A11")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "JTAG1")
				(number "B9")
			)
			(pin input line
				(at 15.24 0 180)
				(length 3.81)
				(name "JTAG2")
				(number "A5")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "JTAG3")
				(number "A6")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "JTAG4")
				(number "A7")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "JTAG5")
				(number "A8")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "PERp0")
				(number "A16")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 3.81)
				(name "PERn0")
				(number "A17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Bus_PCI_Express_x16"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -8.89 66.04 0)
		)
		(property "Value" "Bus_PCI_Express_x16"
			(at 13.97 66.04 0)
		)
		(property "Footprint" "Connector_PCBEdge:BUS_PCIexpress_x16"
			(at 0 22.86 0)
		)
		(property "Datasheet" "http://www.ritrontek.com/uploadfile/2016/1026/20161026105231124.pdf#page=63"
			(at -1.27 -6.35 0)
		)
		(property "Description" "PCI Express bus connector x16"
			(at 0 0 0)
		)
		(property "ki_keywords" "pcie"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PCIexpress*"
			(at 0 0 0)
		)
		(symbol "Bus_PCI_Express_x16_0_1")
		(symbol "Bus_PCI_Express_x16_1_1"
			(pin input line
				(at -15.24 48.26 0)
				(length 3.81)
				(name "SMCLK")
				(number "B5")
			)
			(pin bidirectional line
				(at -15.24 45.72 0)
				(length 3.81)
				(name "SMDAT")
				(number "B6")
			)
			(pin input line
				(at -15.24 40.64 0)
				(length 3.81)
				(name "REFCLK+")
				(number "A13")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 3.81)
				(name "REFCLK-")
				(number "A14")
			)
			(pin passive line
				(at -15.24 33.02 0)
				(length 3.81)
				(name "~{PRSNT1}")
				(number "A1")
			)
			(pin passive line
				(at -15.24 30.48 0)
				(length 3.81)
				(name "~{PRSNT2}")
				(number "B17")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 3.81)
				(name "~{PRSNT2}")
				(number "B31")
			)
			(pin passive line
				(at -15.24 25.4 0)
				(length 3.81)
				(name "~{PRSNT2}")
				(number "B48")
			)
			(pin passive line
				(at -15.24 22.86 0)
				(length 3.81)
				(name "~{PRSNT2}")
				(number "B81")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 3.81)
				(name "PETp0")
				(number "B14")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 3.81)
				(name "PETn0")
				(number "B15")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "PETp1")
				(number "B19")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "PETn1")
				(number "B20")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "PETp2")
				(number "B23")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "PETn2")
				(number "B24")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "PETp3")
				(number "B27")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "PETn3")
				(number "B28")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "PETp4")
				(number "B33")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "PETn4")
				(number "B34")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "PETp5")
				(number "B37")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "PETn5")
				(number "B38")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "PETp6")
				(number "B41")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 3.81)
				(name "PETn6")
				(number "B42")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 3.81)
				(name "PETp7")
				(number "B45")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 3.81)
				(name "PETn7")
				(number "B46")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 3.81)
				(name "PETp8")
				(number "B50")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 3.81)
				(name "PETn8")
				(number "B51")
			)
			(pin input line
				(at -15.24 -27.94 0)
				(length 3.81)
				(name "PETp9")
				(number "B54")
			)
			(pin input line
				(at -15.24 -30.48 0)
				(length 3.81)
				(name "PETn9")
				(number "B55")
			)
			(pin input line
				(at -15.24 -33.02 0)
				(length 3.81)
				(name "PETp10")
				(number "B58")
			)
			(pin input line
				(at -15.24 -35.56 0)
				(length 3.81)
				(name "PETn10")
				(number "B59")
			)
			(pin input line
				(at -15.24 -38.1 0)
				(length 3.81)
				(name "PETp11")
				(number "B62")
			)
			(pin input line
				(at -15.24 -40.64 0)
				(length 3.81)
				(name "PETn11")
				(number "B63")
			)
			(pin input line
				(at -15.24 -43.18 0)
				(length 3.81)
				(name "PETp12")
				(number "B66")
			)
			(pin input line
				(at -15.24 -45.72 0)
				(length 3.81)
				(name "PETn12")
				(number "B67")
			)
			(pin input line
				(at -15.24 -48.26 0)
				(length 3.81)
				(name "PETp13")
				(number "B70")
			)
			(pin input line
				(at -15.24 -50.8 0)
				(length 3.81)
				(name "PETn13")
				(number "B71")
			)
			(pin input line
				(at -15.24 -53.34 0)
				(length 3.81)
				(name "PETp14")
				(number "B74")
			)
			(pin input line
				(at -15.24 -55.88 0)
				(length 3.81)
				(name "PETn14")
				(number "B75")
			)
			(pin input line
				(at -15.24 -58.42 0)
				(length 3.81)
				(name "PETp15")
				(number "B78")
			)
			(pin input line
				(at -15.24 -60.96 0)
				(length 3.81)
				(name "PETn15")
				(number "B79")
			)
			(pin passive line
				(at -2.54 68.58 270)
				(length 3.81)
				(hide yes)
				(name "+12V")
				(number "A2")
			)
			(pin passive line
				(at -2.54 68.58 270)
				(length 3.81)
				(hide yes)
				(name "+12V")
				(number "A3")
			)
			(pin power_in line
				(at -2.54 68.58 270)
				(length 3.81)
				(name "+12V")
				(number "B1")
			)
			(pin passive line
				(at -2.54 68.58 270)
				(length 3.81)
				(hide yes)
				(name "+12V")
				(number "B2")
			)
			(pin passive line
				(at -2.54 68.58 270)
				(length 3.81)
				(hide yes)
				(name "+12V")
				(number "B3")
			)
			(pin power_in line
				(at 0 68.58 270)
				(length 3.81)
				(name "3.3Vaux")
				(number "B10")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A12")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A15")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A18")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A20")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A23")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A24")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A27")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A28")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A31")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A34")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A37")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A38")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A4")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A41")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A42")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A45")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A46")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A49")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A51")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A54")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A55")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A58")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A59")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A62")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A63")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A66")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A67")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A70")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A71")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A74")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A75")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A78")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A79")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A82")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B13")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B16")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B18")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B21")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B22")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B25")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B26")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B29")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B32")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B35")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B36")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B39")
			)
			(pin power_in line
				(at 0 -68.58 90)
				(length 3.81)
				(name "GND")
				(number "B4")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B40")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B43")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B44")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B47")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B49")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B52")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B53")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B56")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B57")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B60")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B61")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B64")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B65")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B68")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B69")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B7")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B72")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B73")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B76")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B77")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B80")
			)
			(pin passive line
				(at 2.54 68.58 270)
				(length 3.81)
				(hide yes)
				(name "+3.3V")
				(number "A10")
			)
			(pin passive line
				(at 2.54 68.58 270)
				(length 3.81)
				(hide yes)
				(name "+3.3V")
				(number "A9")
			)
			(pin power_in line
				(at 2.54 68.58 270)
				(length 3.81)
				(name "+3.3V")
				(number "B8")
			)
			(pin passive line
				(at 15.24 60.96 180)
				(length 3.81)
				(name "RSVD")
				(number "B82")
			)
			(pin passive line
				(at 15.24 58.42 180)
				(length 3.81)
				(name "RSVD")
				(number "A50")
			)
			(pin passive line
				(at 15.24 55.88 180)
				(length 3.81)
				(name "RSVD")
				(number "A33")
			)
			(pin passive line
				(at 15.24 53.34 180)
				(length 3.81)
				(name "RSVD")
				(number "B30")
			)
			(pin passive line
				(at 15.24 50.8 180)
				(length 3.81)
				(name "RSVD")
				(number "A32")
			)
			(pin passive line
				(at 15.24 48.26 180)
				(length 3.81)
				(name "RSVD")
				(number "A19")
			)
			(pin passive line
				(at 15.24 45.72 180)
				(length 3.81)
				(name "RSVD")
				(number "B12")
			)
			(pin open_collector line
				(at 15.24 40.64 180)
				(length 3.81)
				(name "~{WAKE}")
				(number "B11")
			)
			(pin input line
				(at 15.24 38.1 180)
				(length 3.81)
				(name "~{PERST}")
				(number "A11")
			)
			(pin input line
				(at 15.24 33.02 180)
				(length 3.81)
				(name "JTAG1")
				(number "B9")
			)
			(pin input line
				(at 15.24 30.48 180)
				(length 3.81)
				(name "JTAG2")
				(number "A5")
			)
			(pin input line
				(at 15.24 27.94 180)
				(length 3.81)
				(name "JTAG3")
				(number "A6")
			)
			(pin output line
				(at 15.24 25.4 180)
				(length 3.81)
				(name "JTAG4")
				(number "A7")
			)
			(pin input line
				(at 15.24 22.86 180)
				(length 3.81)
				(name "JTAG5")
				(number "A8")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 3.81)
				(name "PERp0")
				(number "A16")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 3.81)
				(name "PERn0")
				(number "A17")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "PERp1")
				(number "A21")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "PERn1")
				(number "A22")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "PERp2")
				(number "A25")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "PERn2")
				(number "A26")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "PERp3")
				(number "A29")
			)
			(pin output line
				(at 15.24 0 180)
				(length 3.81)
				(name "PERn3")
				(number "A30")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "PERp4")
				(number "A35")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "PERn4")
				(number "A36")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "PERp5")
				(number "A39")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "PERn5")
				(number "A40")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "PERp6")
				(number "A43")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 3.81)
				(name "PERn6")
				(number "A44")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 3.81)
				(name "PERp7")
				(number "A47")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 3.81)
				(name "PERn7")
				(number "A48")
			)
			(pin output line
				(at 15.24 -22.86 180)
				(length 3.81)
				(name "PERp8")
				(number "A52")
			)
			(pin output line
				(at 15.24 -25.4 180)
				(length 3.81)
				(name "PERn8")
				(number "A53")
			)
			(pin output line
				(at 15.24 -27.94 180)
				(length 3.81)
				(name "PERp9")
				(number "A56")
			)
			(pin output line
				(at 15.24 -30.48 180)
				(length 3.81)
				(name "PERn9")
				(number "A57")
			)
			(pin output line
				(at 15.24 -33.02 180)
				(length 3.81)
				(name "PERp10")
				(number "A60")
			)
			(pin output line
				(at 15.24 -35.56 180)
				(length 3.81)
				(name "PERn10")
				(number "A61")
			)
			(pin output line
				(at 15.24 -38.1 180)
				(length 3.81)
				(name "PERp11")
				(number "A64")
			)
			(pin output line
				(at 15.24 -40.64 180)
				(length 3.81)
				(name "PERn11")
				(number "A65")
			)
			(pin output line
				(at 15.24 -43.18 180)
				(length 3.81)
				(name "PERp12")
				(number "A68")
			)
			(pin output line
				(at 15.24 -45.72 180)
				(length 3.81)
				(name "PERn12")
				(number "A69")
			)
			(pin output line
				(at 15.24 -48.26 180)
				(length 3.81)
				(name "PERp13")
				(number "A72")
			)
			(pin output line
				(at 15.24 -50.8 180)
				(length 3.81)
				(name "PERn13")
				(number "A73")
			)
			(pin output line
				(at 15.24 -53.34 180)
				(length 3.81)
				(name "PERp14")
				(number "A76")
			)
			(pin output line
				(at 15.24 -55.88 180)
				(length 3.81)
				(name "PERn14")
				(number "A77")
			)
			(pin output line
				(at 15.24 -58.42 180)
				(length 3.81)
				(name "PERp15")
				(number "A80")
			)
			(pin output line
				(at 15.24 -60.96 180)
				(length 3.81)
				(name "PERn15")
				(number "A81")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Bus_PCI_Express_x4"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -8.89 33.02 0)
		)
		(property "Value" "Bus_PCI_Express_x4"
			(at 12.7 33.02 0)
		)
		(property "Footprint" "Connector_PCBEdge:BUS_PCIexpress_x4"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://www.ritrontek.com/uploadfile/2016/1026/20161026105231124.pdf#page=63"
			(at -6.35 -31.75 0)
		)
		(property "Description" "PCI Express bus connector x4"
			(at 0 0 0)
		)
		(property "ki_keywords" "pcie"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PCIexpress*"
			(at 0 0 0)
		)
		(symbol "Bus_PCI_Express_x4_0_1")
		(symbol "Bus_PCI_Express_x4_1_1"
			(pin input line
				(at -15.24 22.86 0)
				(length 3.81)
				(name "SMCLK")
				(number "B5")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 3.81)
				(name "SMDAT")
				(number "B6")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 3.81)
				(name "REFCLK+")
				(number "A13")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "REFCLK-")
				(number "A14")
			)
			(pin passive line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "~{PRSNT1}")
				(number "A1")
			)
			(pin passive line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "~{PRSNT2}")
				(number "B17")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "~{PRSNT2}")
				(number "B31")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "PETp0")
				(number "B14")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "PETn0")
				(number "B15")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "PETp1")
				(number "B19")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 3.81)
				(name "PETn1")
				(number "B20")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 3.81)
				(name "PETp2")
				(number "B23")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 3.81)
				(name "PETn2")
				(number "B24")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 3.81)
				(name "PETp3")
				(number "B27")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 3.81)
				(name "PETn3")
				(number "B28")
			)
			(pin passive line
				(at -2.54 35.56 270)
				(length 3.81)
				(hide yes)
				(name "+12V")
				(number "A2")
			)
			(pin passive line
				(at -2.54 35.56 270)
				(length 3.81)
				(hide yes)
				(name "+12V")
				(number "A3")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "+12V")
				(number "B1")
			)
			(pin passive line
				(at -2.54 35.56 270)
				(length 3.81)
				(hide yes)
				(name "+12V")
				(number "B2")
			)
			(pin passive line
				(at -2.54 35.56 270)
				(length 3.81)
				(hide yes)
				(name "+12V")
				(number "B3")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "3.3Vaux")
				(number "B10")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A12")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A15")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A18")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A20")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A23")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A24")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A27")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A28")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A31")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A4")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B13")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B16")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B18")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B21")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B22")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B25")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B26")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B29")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B32")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 3.81)
				(name "GND")
				(number "B4")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B7")
			)
			(pin passive line
				(at 2.54 35.56 270)
				(length 3.81)
				(hide yes)
				(name "+3.3V")
				(number "A10")
			)
			(pin passive line
				(at 2.54 35.56 270)
				(length 3.81)
				(hide yes)
				(name "+3.3V")
				(number "A9")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 3.81)
				(name "+3.3V")
				(number "B8")
			)
			(pin passive line
				(at 15.24 27.94 180)
				(length 3.81)
				(name "RSVD")
				(number "B30")
			)
			(pin passive line
				(at 15.24 25.4 180)
				(length 3.81)
				(name "RSVD")
				(number "A32")
			)
			(pin passive line
				(at 15.24 22.86 180)
				(length 3.81)
				(name "RSVD")
				(number "A19")
			)
			(pin passive line
				(at 15.24 20.32 180)
				(length 3.81)
				(name "RSVD")
				(number "B12")
			)
			(pin open_collector line
				(at 15.24 15.24 180)
				(length 3.81)
				(name "~{WAKE}")
				(number "B11")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "~{PERST}")
				(number "A11")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "JTAG1")
				(number "B9")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "JTAG2")
				(number "A5")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "JTAG3")
				(number "A6")
			)
			(pin output line
				(at 15.24 0 180)
				(length 3.81)
				(name "JTAG4")
				(number "A7")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "JTAG5")
				(number "A8")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "PERp0")
				(number "A16")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "PERn0")
				(number "A17")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "PERp1")
				(number "A21")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 3.81)
				(name "PERn1")
				(number "A22")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 3.81)
				(name "PERp2")
				(number "A25")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 3.81)
				(name "PERn2")
				(number "A26")
			)
			(pin output line
				(at 15.24 -22.86 180)
				(length 3.81)
				(name "PERp3")
				(number "A29")
			)
			(pin output line
				(at 15.24 -25.4 180)
				(length 3.81)
				(name "PERn3")
				(number "A30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Bus_PCI_Express_x8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -8.89 43.18 0)
		)
		(property "Value" "Bus_PCI_Express_x8"
			(at 12.7 43.18 0)
		)
		(property "Footprint" "Connector_PCBEdge:BUS_PCIexpress_x8"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.ritrontek.com/uploadfile/2016/1026/20161026105231124.pdf#page=63"
			(at -1.27 -24.13 0)
		)
		(property "Description" "PCI Express bus connector x8"
			(at 0 0 0)
		)
		(property "ki_keywords" "pcie"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PCIexpress*"
			(at 0 0 0)
		)
		(symbol "Bus_PCI_Express_x8_0_1")
		(symbol "Bus_PCI_Express_x8_1_1"
			(pin input line
				(at -15.24 30.48 0)
				(length 3.81)
				(name "SMCLK")
				(number "B5")
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 3.81)
				(name "SMDAT")
				(number "B6")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 3.81)
				(name "REFCLK+")
				(number "A13")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 3.81)
				(name "REFCLK-")
				(number "A14")
			)
			(pin passive line
				(at -15.24 15.24 0)
				(length 3.81)
				(name "~{PRSNT1}")
				(number "A1")
			)
			(pin passive line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "~{PRSNT2}")
				(number "B17")
			)
			(pin passive line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "~{PRSNT2}")
				(number "B31")
			)
			(pin passive line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "~{PRSNT2}")
				(number "B48")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "PETp0")
				(number "B14")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "PETn0")
				(number "B15")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "PETp1")
				(number "B19")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "PETn1")
				(number "B20")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "PETp2")
				(number "B23")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "PETn2")
				(number "B24")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 3.81)
				(name "PETp3")
				(number "B27")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 3.81)
				(name "PETn3")
				(number "B28")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 3.81)
				(name "PETp4")
				(number "B33")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 3.81)
				(name "PETn4")
				(number "B34")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 3.81)
				(name "PETp5")
				(number "B37")
			)
			(pin input line
				(at -15.24 -27.94 0)
				(length 3.81)
				(name "PETn5")
				(number "B38")
			)
			(pin input line
				(at -15.24 -30.48 0)
				(length 3.81)
				(name "PETp6")
				(number "B41")
			)
			(pin input line
				(at -15.24 -33.02 0)
				(length 3.81)
				(name "PETn6")
				(number "B42")
			)
			(pin input line
				(at -15.24 -35.56 0)
				(length 3.81)
				(name "PETp7")
				(number "B45")
			)
			(pin input line
				(at -15.24 -38.1 0)
				(length 3.81)
				(name "PETn7")
				(number "B46")
			)
			(pin passive line
				(at -2.54 45.72 270)
				(length 3.81)
				(hide yes)
				(name "+12V")
				(number "A2")
			)
			(pin passive line
				(at -2.54 45.72 270)
				(length 3.81)
				(hide yes)
				(name "+12V")
				(number "A3")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 3.81)
				(name "+12V")
				(number "B1")
			)
			(pin passive line
				(at -2.54 45.72 270)
				(length 3.81)
				(hide yes)
				(name "+12V")
				(number "B2")
			)
			(pin passive line
				(at -2.54 45.72 270)
				(length 3.81)
				(hide yes)
				(name "+12V")
				(number "B3")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 3.81)
				(name "3.3Vaux")
				(number "B10")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A12")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A15")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A18")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A20")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A23")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A24")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A27")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A28")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A31")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A34")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A37")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A38")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A4")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A41")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A42")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A45")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A46")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A49")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B13")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B16")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B18")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B21")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B22")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B25")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B26")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B29")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B32")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B35")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B36")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B39")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "B4")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B40")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B43")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B44")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B47")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B49")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B7")
			)
			(pin passive line
				(at 2.54 45.72 270)
				(length 3.81)
				(hide yes)
				(name "+3.3V")
				(number "A10")
			)
			(pin passive line
				(at 2.54 45.72 270)
				(length 3.81)
				(hide yes)
				(name "+3.3V")
				(number "A9")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 3.81)
				(name "+3.3V")
				(number "B8")
			)
			(pin passive line
				(at 15.24 38.1 180)
				(length 3.81)
				(name "RSVD")
				(number "A33")
			)
			(pin passive line
				(at 15.24 35.56 180)
				(length 3.81)
				(name "RSVD")
				(number "B30")
			)
			(pin passive line
				(at 15.24 33.02 180)
				(length 3.81)
				(name "RSVD")
				(number "A32")
			)
			(pin passive line
				(at 15.24 30.48 180)
				(length 3.81)
				(name "RSVD")
				(number "A19")
			)
			(pin passive line
				(at 15.24 27.94 180)
				(length 3.81)
				(name "RSVD")
				(number "B12")
			)
			(pin open_collector line
				(at 15.24 22.86 180)
				(length 3.81)
				(name "~{WAKE}")
				(number "B11")
			)
			(pin input line
				(at 15.24 20.32 180)
				(length 3.81)
				(name "~{PERST}")
				(number "A11")
			)
			(pin input line
				(at 15.24 15.24 180)
				(length 3.81)
				(name "JTAG1")
				(number "B9")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "JTAG2")
				(number "A5")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "JTAG3")
				(number "A6")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "JTAG4")
				(number "A7")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "JTAG5")
				(number "A8")
			)
			(pin output line
				(at 15.24 0 180)
				(length 3.81)
				(name "PERp0")
				(number "A16")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "PERn0")
				(number "A17")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "PERp1")
				(number "A21")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "PERn1")
				(number "A22")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "PERp2")
				(number "A25")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "PERn2")
				(number "A26")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 3.81)
				(name "PERp3")
				(number "A29")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 3.81)
				(name "PERn3")
				(number "A30")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 3.81)
				(name "PERp4")
				(number "A35")
			)
			(pin output line
				(at 15.24 -22.86 180)
				(length 3.81)
				(name "PERn4")
				(number "A36")
			)
			(pin output line
				(at 15.24 -25.4 180)
				(length 3.81)
				(name "PERp5")
				(number "A39")
			)
			(pin output line
				(at 15.24 -27.94 180)
				(length 3.81)
				(name "PERn5")
				(number "A40")
			)
			(pin output line
				(at 15.24 -30.48 180)
				(length 3.81)
				(name "PERp6")
				(number "A43")
			)
			(pin output line
				(at 15.24 -33.02 180)
				(length 3.81)
				(name "PERn6")
				(number "A44")
			)
			(pin output line
				(at 15.24 -35.56 180)
				(length 3.81)
				(name "PERp7")
				(number "A47")
			)
			(pin output line
				(at 15.24 -38.1 180)
				(length 3.81)
				(name "PERn7")
				(number "A48")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CUI_PD-30"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 -8.89 0)
		)
		(property "Value" "CUI_PD-30"
			(at 0 -10.795 0)
		)
		(property "Footprint" "Connector:CUI_PD-30"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.cui.com/product/resource/pd-30.pdf"
			(at 0 0 0)
		)
		(property "Description" "3 pin connector, PD-30"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector 3-pin PD-30 power DIN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CUI*PD*30*"
			(at 0 0 0)
		)
		(symbol "CUI_PD-30_0_1"
			(text "1"
				(at -2.1336 1.2192 0)
			)
			(text "2"
				(at 2.1336 -1.2446 0)
			)
			(text "3"
				(at 3.048 2.54 0)
			)
		)
		(symbol "CUI_PD-30_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "Shield")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CUI_PD-30S"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 -8.89 0)
		)
		(property "Value" "CUI_PD-30S"
			(at 0 -10.795 0)
		)
		(property "Footprint" "Connector:CUI_PD-30S"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.cui.com/product/resource/pd-30.pdf"
			(at 0 0 0)
		)
		(property "Description" "3 pin connector, PD-30S"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector 3-pin PD-30S power DIN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CUI*PD*30S*"
			(at 0 0 0)
		)
		(symbol "CUI_PD-30S_0_1"
			(text "1"
				(at -2.1336 1.2192 0)
			)
			(text "2"
				(at 2.1336 -1.2192 0)
			)
			(text "3"
				(at 3.048 2.54 0)
			)
		)
		(symbol "CUI_PD-30S_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "Shield")
				(number "4")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CoaxialSwitch_Testpoint"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TP"
			(at 0 -3.81 0)
		)
		(property "Value" "CoaxialSwitch_Testpoint"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 1.27 0)
		)
		(property "Datasheet" "~"
			(at 0 1.27 0)
		)
		(property "Description" "Subminiature Coaxial Switch testpoint"
			(at 0 0 0)
		)
		(property "ki_keywords" "Coaxial Switch RF testpoint"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CoaxialSwitch*"
			(at 0 0 0)
		)
		(symbol "CoaxialSwitch_Testpoint_0_1")
		(symbol "CoaxialSwitch_Testpoint_1_1"
			(pin passive line
				(at -5.08 1.27 0)
				(length 2.54)
				(name "C")
				(number "C")
			)
			(pin passive line
				(at 5.08 1.27 180)
				(length 2.54)
				(name "A")
				(number "A")
			)
			(pin passive line
				(at 5.08 -1.27 180)
				(length 2.54)
				(name "G")
				(number "G")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x01_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 2.54 0)
		)
		(property "Value" "Conn_01x01_Pin"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x01_Pin_1_1"
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x01_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 2.54 0)
		)
		(property "Value" "Conn_01x01_Socket"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x01_Socket_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x02_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 2.54 0)
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x02_Pin_1_1"
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x02_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 2.54 0)
		)
		(property "Value" "Conn_01x02_Socket"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x02_Socket_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x03_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 5.08 0)
		)
		(property "Value" "Conn_01x03_Pin"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x03_Pin_1_1"
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x03_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 5.08 0)
		)
		(property "Value" "Conn_01x03_Socket"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x03_Socket_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x04_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 5.08 0)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x04_Pin_1_1"
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x04_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 5.08 0)
		)
		(property "Value" "Conn_01x04_Socket"
			(at 0 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x04_Socket_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x05_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 7.62 0)
		)
		(property "Value" "Conn_01x05_Pin"
			(at 0 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x05_Pin_1_1"
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x05_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 7.62 0)
		)
		(property "Value" "Conn_01x05_Socket"
			(at 0 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x05_Socket_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x06_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 7.62 0)
		)
		(property "Value" "Conn_01x06_Pin"
			(at 0 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x06_Pin_1_1"
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x06_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 7.62 0)
		)
		(property "Value" "Conn_01x06_Socket"
			(at 0 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x06_Socket_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x07_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "Conn_01x07_Pin"
			(at 0 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x07, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x07_Pin_1_1"
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x07_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "Conn_01x07_Socket"
			(at 0 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x07, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x07_Socket_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x08_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "Conn_01x08_Pin"
			(at 0 -12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x08_Pin_1_1"
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x08_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "Conn_01x08_Socket"
			(at 0 -12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x08_Socket_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x09_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 12.7 0)
		)
		(property "Value" "Conn_01x09_Pin"
			(at 0 -12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x09, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x09_Pin_1_1"
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x09_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 12.7 0)
		)
		(property "Value" "Conn_01x09_Socket"
			(at 0 -12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x09, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x09_Socket_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x10_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 12.7 0)
		)
		(property "Value" "Conn_01x10_Pin"
			(at 0 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x10, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x10_Pin_1_1"
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x10_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 12.7 0)
		)
		(property "Value" "Conn_01x10_Socket"
			(at 0 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x10, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x10_Socket_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x11_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 15.24 0)
		)
		(property "Value" "Conn_01x11_Pin"
			(at 0 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x11, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x11_Pin_1_1"
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x11_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 15.24 0)
		)
		(property "Value" "Conn_01x11_Socket"
			(at 0 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x11, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x11_Socket_1_1"
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x12_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 15.24 0)
		)
		(property "Value" "Conn_01x12_Pin"
			(at 0 -17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x12, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x12_Pin_1_1"
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x12_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 15.24 0)
		)
		(property "Value" "Conn_01x12_Socket"
			(at 0 -17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x12, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x12_Socket_1_1"
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x13_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 17.78 0)
		)
		(property "Value" "Conn_01x13_Pin"
			(at 0 -17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x13, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x13_Pin_1_1"
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x13_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 17.78 0)
		)
		(property "Value" "Conn_01x13_Socket"
			(at 0 -17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x13, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x13_Socket_1_1"
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x14_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 17.78 0)
		)
		(property "Value" "Conn_01x14_Pin"
			(at 0 -20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x14, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x14_Pin_1_1"
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x14_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 17.78 0)
		)
		(property "Value" "Conn_01x14_Socket"
			(at 0 -20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x14, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x14_Socket_1_1"
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x15_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 20.32 0)
		)
		(property "Value" "Conn_01x15_Pin"
			(at 0 -20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x15, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x15_Pin_1_1"
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x15_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 20.32 0)
		)
		(property "Value" "Conn_01x15_Socket"
			(at 0 -20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x15, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x15_Socket_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x16_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 20.32 0)
		)
		(property "Value" "Conn_01x16_Pin"
			(at 0 -22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x16, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x16_Pin_1_1"
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x16_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 20.32 0)
		)
		(property "Value" "Conn_01x16_Socket"
			(at 0 -22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x16, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x16_Socket_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x17_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 22.86 0)
		)
		(property "Value" "Conn_01x17_Pin"
			(at 0 -22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x17, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x17_Pin_1_1"
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x17_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 22.86 0)
		)
		(property "Value" "Conn_01x17_Socket"
			(at 0 -22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x17, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x17_Socket_1_1"
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x18_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 22.86 0)
		)
		(property "Value" "Conn_01x18_Pin"
			(at 0 -25.4 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x18, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x18_Pin_1_1"
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x18_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 22.86 0)
		)
		(property "Value" "Conn_01x18_Socket"
			(at 0 -25.4 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x18, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x18_Socket_1_1"
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x19_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 25.4 0)
		)
		(property "Value" "Conn_01x19_Pin"
			(at 0 -25.4 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x19, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x19_Pin_1_1"
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x19_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 25.4 0)
		)
		(property "Value" "Conn_01x19_Socket"
			(at 0 -25.4 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x19, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x19_Socket_1_1"
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x20_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 25.4 0)
		)
		(property "Value" "Conn_01x20_Pin"
			(at 0 -27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x20, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x20_Pin_1_1"
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x20_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 25.4 0)
		)
		(property "Value" "Conn_01x20_Socket"
			(at 0 -27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x20, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x20_Socket_1_1"
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x21_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 27.94 0)
		)
		(property "Value" "Conn_01x21_Pin"
			(at 0 -27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x21, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x21_Pin_1_1"
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x21_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 27.94 0)
		)
		(property "Value" "Conn_01x21_Socket"
			(at 0 -27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x21, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x21_Socket_1_1"
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x22_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 27.94 0)
		)
		(property "Value" "Conn_01x22_Pin"
			(at 0 -30.48 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x22, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x22_Pin_1_1"
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x22_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 27.94 0)
		)
		(property "Value" "Conn_01x22_Socket"
			(at 0 -30.48 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x22, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x22_Socket_1_1"
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x23_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 30.48 0)
		)
		(property "Value" "Conn_01x23_Pin"
			(at 0 -30.48 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x23, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x23_Pin_1_1"
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x23_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 30.48 0)
		)
		(property "Value" "Conn_01x23_Socket"
			(at 0 -30.48 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x23, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x23_Socket_1_1"
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x24_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 30.48 0)
		)
		(property "Value" "Conn_01x24_Pin"
			(at 0 -33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x24, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x24_Pin_1_1"
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x24_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 30.48 0)
		)
		(property "Value" "Conn_01x24_Socket"
			(at 0 -33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x24, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x24_Socket_1_1"
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x25_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 33.02 0)
		)
		(property "Value" "Conn_01x25_Pin"
			(at 0 -33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x25, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x25_Pin_1_1"
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x25_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 33.02 0)
		)
		(property "Value" "Conn_01x25_Socket"
			(at 0 -33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x25, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x25_Socket_1_1"
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x26_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 33.02 0)
		)
		(property "Value" "Conn_01x26_Pin"
			(at 0 -35.56 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x26, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x26_Pin_1_1"
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x26_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 33.02 0)
		)
		(property "Value" "Conn_01x26_Socket"
			(at 0 -35.56 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x26, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x26_Socket_1_1"
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x27_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 35.56 0)
		)
		(property "Value" "Conn_01x27_Pin"
			(at 0 -35.56 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x27, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x27_Pin_1_1"
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x27_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 35.56 0)
		)
		(property "Value" "Conn_01x27_Socket"
			(at 0 -35.56 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x27, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x27_Socket_1_1"
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x28_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 35.56 0)
		)
		(property "Value" "Conn_01x28_Pin"
			(at 0 -38.1 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x28, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x28_Pin_1_1"
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x28_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 35.56 0)
		)
		(property "Value" "Conn_01x28_Socket"
			(at 0 -38.1 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x28, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x28_Socket_1_1"
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x29_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 38.1 0)
		)
		(property "Value" "Conn_01x29_Pin"
			(at 0 -38.1 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x29, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x29_Pin_1_1"
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x29_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 38.1 0)
		)
		(property "Value" "Conn_01x29_Socket"
			(at 0 -38.1 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x29, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x29_Socket_1_1"
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x30_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 38.1 0)
		)
		(property "Value" "Conn_01x30_Pin"
			(at 0 -40.64 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x30, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x30_Pin_1_1"
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x30_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 38.1 0)
		)
		(property "Value" "Conn_01x30_Socket"
			(at 0 -40.64 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x30, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x30_Socket_1_1"
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x31_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 40.64 0)
		)
		(property "Value" "Conn_01x31_Pin"
			(at 0 -40.64 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x31, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x31_Pin_1_1"
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x31_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 40.64 0)
		)
		(property "Value" "Conn_01x31_Socket"
			(at 0 -40.64 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x31, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x31_Socket_1_1"
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x32_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 40.64 0)
		)
		(property "Value" "Conn_01x32_Pin"
			(at 0 -43.18 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x32, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x32_Pin_1_1"
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x32_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 40.64 0)
		)
		(property "Value" "Conn_01x32_Socket"
			(at 0 -43.18 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x32, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x32_Socket_1_1"
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x33_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 43.18 0)
		)
		(property "Value" "Conn_01x33_Pin"
			(at 0 -43.18 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x33, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x33_Pin_1_1"
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x33_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 43.18 0)
		)
		(property "Value" "Conn_01x33_Socket"
			(at 0 -43.18 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x33, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x33_Socket_1_1"
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x34_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 43.18 0)
		)
		(property "Value" "Conn_01x34_Pin"
			(at 0 -45.72 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x34, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x34_Pin_1_1"
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x34_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 43.18 0)
		)
		(property "Value" "Conn_01x34_Socket"
			(at 0 -45.72 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x34, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x34_Socket_1_1"
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x35_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 45.72 0)
		)
		(property "Value" "Conn_01x35_Pin"
			(at 0 -45.72 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x35, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x35_Pin_1_1"
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x35_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 45.72 0)
		)
		(property "Value" "Conn_01x35_Socket"
			(at 0 -45.72 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x35, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x35_Socket_1_1"
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x36_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 45.72 0)
		)
		(property "Value" "Conn_01x36_Pin"
			(at 0 -48.26 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x36, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x36_Pin_1_1"
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x36_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 45.72 0)
		)
		(property "Value" "Conn_01x36_Socket"
			(at 0 -48.26 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x36, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x36_Socket_1_1"
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x37_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 48.26 0)
		)
		(property "Value" "Conn_01x37_Pin"
			(at 0 -48.26 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x37, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x37_Pin_1_1"
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x37_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 48.26 0)
		)
		(property "Value" "Conn_01x37_Socket"
			(at 0 -48.26 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x37, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x37_Socket_1_1"
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x38_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 48.26 0)
		)
		(property "Value" "Conn_01x38_Pin"
			(at 0 -50.8 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x38, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x38_Pin_1_1"
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x38_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 48.26 0)
		)
		(property "Value" "Conn_01x38_Socket"
			(at 0 -50.8 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x38, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x38_Socket_1_1"
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x39_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 50.8 0)
		)
		(property "Value" "Conn_01x39_Pin"
			(at 0 -50.8 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x39, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x39_Pin_1_1"
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x39_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 50.8 0)
		)
		(property "Value" "Conn_01x39_Socket"
			(at 0 -50.8 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x39, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x39_Socket_1_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x40_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 50.8 0)
		)
		(property "Value" "Conn_01x40_Pin"
			(at 0 -53.34 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x40, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x40_Pin_1_1"
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 5.08 -50.8 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x40_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 50.8 0)
		)
		(property "Value" "Conn_01x40_Socket"
			(at 0 -53.34 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic connector, single row, 01x40, script generated"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x40_Socket_1_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x41_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 53.34 0)
		)
		(property "Value" "Conn_01x41_Pin"
			(at 0 -53.34 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x41, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x41_Pin_1_1"
			(pin passive line
				(at 5.08 50.8 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 5.08 -50.8 180)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x41_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 53.34 0)
		)
		(property "Value" "Conn_01x41_Socket"
			(at 0 -53.34 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x41, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x41_Socket_1_1"
			(pin passive line
				(at -5.08 50.8 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x42_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 53.34 0)
		)
		(property "Value" "Conn_01x42_Pin"
			(at 0 -55.88 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x42, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x42_Pin_1_1"
			(pin passive line
				(at 5.08 50.8 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 5.08 -50.8 180)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 5.08 -53.34 180)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x42_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 53.34 0)
		)
		(property "Value" "Conn_01x42_Socket"
			(at 0 -55.88 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x42, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x42_Socket_1_1"
			(pin passive line
				(at -5.08 50.8 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x43_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 55.88 0)
		)
		(property "Value" "Conn_01x43_Pin"
			(at 0 -55.88 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x43, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x43_Pin_1_1"
			(pin passive line
				(at 5.08 53.34 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 50.8 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 5.08 -50.8 180)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 5.08 -53.34 180)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x43_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 55.88 0)
		)
		(property "Value" "Conn_01x43_Socket"
			(at 0 -55.88 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x43, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x43_Socket_1_1"
			(pin passive line
				(at -5.08 53.34 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x44_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 55.88 0)
		)
		(property "Value" "Conn_01x44_Pin"
			(at 0 -58.42 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x44, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x44_Pin_1_1"
			(pin passive line
				(at 5.08 53.34 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 50.8 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 5.08 -50.8 180)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 5.08 -53.34 180)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 5.08 -55.88 180)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x44_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 55.88 0)
		)
		(property "Value" "Conn_01x44_Socket"
			(at 0 -58.42 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x44, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x44_Socket_1_1"
			(pin passive line
				(at -5.08 53.34 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x45_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 58.42 0)
		)
		(property "Value" "Conn_01x45_Pin"
			(at 0 -58.42 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x45, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x45_Pin_1_1"
			(pin passive line
				(at 5.08 55.88 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 53.34 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 50.8 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 5.08 -50.8 180)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 5.08 -53.34 180)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 5.08 -55.88 180)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x45_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 58.42 0)
		)
		(property "Value" "Conn_01x45_Socket"
			(at 0 -58.42 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x45, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x45_Socket_1_1"
			(pin passive line
				(at -5.08 55.88 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x46_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 58.42 0)
		)
		(property "Value" "Conn_01x46_Pin"
			(at 0 -60.96 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x46, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x46_Pin_1_1"
			(pin passive line
				(at 5.08 55.88 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 53.34 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 50.8 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 5.08 -50.8 180)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 5.08 -53.34 180)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 5.08 -55.88 180)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 5.08 -58.42 180)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x46_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 58.42 0)
		)
		(property "Value" "Conn_01x46_Socket"
			(at 0 -60.96 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x46, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x46_Socket_1_1"
			(pin passive line
				(at -5.08 55.88 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x47_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 60.96 0)
		)
		(property "Value" "Conn_01x47_Pin"
			(at 0 -60.96 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x47, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x47_Pin_1_1"
			(pin passive line
				(at 5.08 58.42 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 55.88 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 53.34 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 50.8 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 5.08 -50.8 180)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 5.08 -53.34 180)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 5.08 -55.88 180)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 5.08 -58.42 180)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x47_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 60.96 0)
		)
		(property "Value" "Conn_01x47_Socket"
			(at 0 -60.96 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x47, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x47_Socket_1_1"
			(pin passive line
				(at -5.08 58.42 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x48_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 60.96 0)
		)
		(property "Value" "Conn_01x48_Pin"
			(at 0 -63.5 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x48, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x48_Pin_1_1"
			(pin passive line
				(at 5.08 58.42 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 55.88 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 53.34 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 50.8 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 5.08 -50.8 180)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 5.08 -53.34 180)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 5.08 -55.88 180)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 5.08 -58.42 180)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 5.08 -60.96 180)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x48_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 60.96 0)
		)
		(property "Value" "Conn_01x48_Socket"
			(at 0 -63.5 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x48, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x48_Socket_1_1"
			(pin passive line
				(at -5.08 58.42 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x49_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 63.5 0)
		)
		(property "Value" "Conn_01x49_Pin"
			(at 0 -63.5 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x49, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x49_Pin_1_1"
			(pin passive line
				(at 5.08 60.96 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 58.42 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 55.88 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 53.34 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 50.8 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 5.08 -50.8 180)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 5.08 -53.34 180)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 5.08 -55.88 180)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 5.08 -58.42 180)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 5.08 -60.96 180)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x49_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 63.5 0)
		)
		(property "Value" "Conn_01x49_Socket"
			(at 0 -63.5 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x49, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x49_Socket_1_1"
			(pin passive line
				(at -5.08 60.96 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x50_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 63.5 0)
		)
		(property "Value" "Conn_01x50_Pin"
			(at 0 -66.04 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x50, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x50_Pin_1_1"
			(pin passive line
				(at 5.08 60.96 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 58.42 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 55.88 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 53.34 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 50.8 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 5.08 -50.8 180)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 5.08 -53.34 180)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 5.08 -55.88 180)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 5.08 -58.42 180)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 5.08 -60.96 180)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 5.08 -63.5 180)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x50_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 63.5 0)
		)
		(property "Value" "Conn_01x50_Socket"
			(at 0 -66.04 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x50, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x50_Socket_1_1"
			(pin passive line
				(at -5.08 60.96 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x51_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 66.04 0)
		)
		(property "Value" "Conn_01x51_Pin"
			(at 0 -66.04 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x51, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x51_Pin_1_1"
			(pin passive line
				(at 5.08 63.5 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 60.96 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 58.42 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 55.88 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 53.34 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 50.8 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 5.08 -50.8 180)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 5.08 -53.34 180)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 5.08 -55.88 180)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 5.08 -58.42 180)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 5.08 -60.96 180)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 5.08 -63.5 180)
				(length 3.81)
				(name "Pin_51")
				(number "51")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x51_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 66.04 0)
		)
		(property "Value" "Conn_01x51_Socket"
			(at 0 -66.04 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x51, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x51_Socket_1_1"
			(pin passive line
				(at -5.08 63.5 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 3.81)
				(name "Pin_51")
				(number "51")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x52_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 66.04 0)
		)
		(property "Value" "Conn_01x52_Pin"
			(at 0 -68.58 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x52, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x52_Pin_1_1"
			(pin passive line
				(at 5.08 63.5 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 60.96 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 58.42 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 55.88 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 53.34 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 50.8 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 5.08 -50.8 180)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 5.08 -53.34 180)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 5.08 -55.88 180)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 5.08 -58.42 180)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 5.08 -60.96 180)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 5.08 -63.5 180)
				(length 3.81)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 5.08 -66.04 180)
				(length 3.81)
				(name "Pin_52")
				(number "52")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x52_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 66.04 0)
		)
		(property "Value" "Conn_01x52_Socket"
			(at 0 -68.58 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x52, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x52_Socket_1_1"
			(pin passive line
				(at -5.08 63.5 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 3.81)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 3.81)
				(name "Pin_52")
				(number "52")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x53_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 68.58 0)
		)
		(property "Value" "Conn_01x53_Pin"
			(at 0 -68.58 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x53, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x53_Pin_1_1"
			(pin passive line
				(at 5.08 66.04 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 63.5 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 60.96 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 58.42 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 55.88 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 53.34 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 50.8 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 5.08 -50.8 180)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 5.08 -53.34 180)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 5.08 -55.88 180)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 5.08 -58.42 180)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 5.08 -60.96 180)
				(length 3.81)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 5.08 -63.5 180)
				(length 3.81)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 5.08 -66.04 180)
				(length 3.81)
				(name "Pin_53")
				(number "53")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x53_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 68.58 0)
		)
		(property "Value" "Conn_01x53_Socket"
			(at 0 -68.58 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x53, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x53_Socket_1_1"
			(pin passive line
				(at -5.08 66.04 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 3.81)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 3.81)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 3.81)
				(name "Pin_53")
				(number "53")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x54_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 68.58 0)
		)
		(property "Value" "Conn_01x54_Pin"
			(at 0 -71.12 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x54, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x54_Pin_1_1"
			(pin passive line
				(at 5.08 66.04 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 63.5 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 60.96 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 58.42 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 55.88 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 53.34 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 50.8 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 5.08 -50.8 180)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 5.08 -53.34 180)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 5.08 -55.88 180)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 5.08 -58.42 180)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 5.08 -60.96 180)
				(length 3.81)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 5.08 -63.5 180)
				(length 3.81)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 5.08 -66.04 180)
				(length 3.81)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 5.08 -68.58 180)
				(length 3.81)
				(name "Pin_54")
				(number "54")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x54_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 68.58 0)
		)
		(property "Value" "Conn_01x54_Socket"
			(at 0 -71.12 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x54, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x54_Socket_1_1"
			(pin passive line
				(at -5.08 66.04 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 3.81)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 3.81)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 3.81)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 3.81)
				(name "Pin_54")
				(number "54")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x55_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 71.12 0)
		)
		(property "Value" "Conn_01x55_Pin"
			(at 0 -71.12 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x55, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x55_Pin_1_1"
			(pin passive line
				(at 5.08 68.58 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 66.04 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 63.5 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 60.96 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 58.42 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 55.88 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 53.34 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 50.8 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 5.08 -50.8 180)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 5.08 -53.34 180)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 5.08 -55.88 180)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 5.08 -58.42 180)
				(length 3.81)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 5.08 -60.96 180)
				(length 3.81)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 5.08 -63.5 180)
				(length 3.81)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 5.08 -66.04 180)
				(length 3.81)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 5.08 -68.58 180)
				(length 3.81)
				(name "Pin_55")
				(number "55")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x55_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 71.12 0)
		)
		(property "Value" "Conn_01x55_Socket"
			(at 0 -71.12 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x55, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x55_Socket_1_1"
			(pin passive line
				(at -5.08 68.58 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 3.81)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 3.81)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 3.81)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 3.81)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 3.81)
				(name "Pin_55")
				(number "55")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x56_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 71.12 0)
		)
		(property "Value" "Conn_01x56_Pin"
			(at 0 -73.66 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x56, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x56_Pin_1_1"
			(pin passive line
				(at 5.08 68.58 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 66.04 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 63.5 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 60.96 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 58.42 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 55.88 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 53.34 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 50.8 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 5.08 -50.8 180)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 5.08 -53.34 180)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 5.08 -55.88 180)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 5.08 -58.42 180)
				(length 3.81)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 5.08 -60.96 180)
				(length 3.81)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 5.08 -63.5 180)
				(length 3.81)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 5.08 -66.04 180)
				(length 3.81)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 5.08 -68.58 180)
				(length 3.81)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 5.08 -71.12 180)
				(length 3.81)
				(name "Pin_56")
				(number "56")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x56_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 71.12 0)
		)
		(property "Value" "Conn_01x56_Socket"
			(at 0 -73.66 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x56, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x56_Socket_1_1"
			(pin passive line
				(at -5.08 68.58 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 3.81)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 3.81)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 3.81)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 3.81)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 3.81)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 3.81)
				(name "Pin_56")
				(number "56")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x57_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 73.66 0)
		)
		(property "Value" "Conn_01x57_Pin"
			(at 0 -73.66 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x57, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x57_Pin_1_1"
			(pin passive line
				(at 5.08 71.12 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 68.58 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 66.04 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 63.5 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 60.96 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 58.42 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 55.88 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 53.34 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 50.8 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 5.08 -50.8 180)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 5.08 -53.34 180)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 5.08 -55.88 180)
				(length 3.81)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 5.08 -58.42 180)
				(length 3.81)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 5.08 -60.96 180)
				(length 3.81)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 5.08 -63.5 180)
				(length 3.81)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 5.08 -66.04 180)
				(length 3.81)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 5.08 -68.58 180)
				(length 3.81)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 5.08 -71.12 180)
				(length 3.81)
				(name "Pin_57")
				(number "57")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x57_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 73.66 0)
		)
		(property "Value" "Conn_01x57_Socket"
			(at 0 -73.66 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x57, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x57_Socket_1_1"
			(pin passive line
				(at -5.08 71.12 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 68.58 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 3.81)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 3.81)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 3.81)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 3.81)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 3.81)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 3.81)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 3.81)
				(name "Pin_57")
				(number "57")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x58_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 73.66 0)
		)
		(property "Value" "Conn_01x58_Pin"
			(at 0 -76.2 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x58, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x58_Pin_1_1"
			(pin passive line
				(at 5.08 71.12 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 68.58 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 66.04 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 63.5 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 60.96 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 58.42 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 55.88 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 53.34 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 50.8 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 5.08 -50.8 180)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 5.08 -53.34 180)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 5.08 -55.88 180)
				(length 3.81)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 5.08 -58.42 180)
				(length 3.81)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 5.08 -60.96 180)
				(length 3.81)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 5.08 -63.5 180)
				(length 3.81)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 5.08 -66.04 180)
				(length 3.81)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 5.08 -68.58 180)
				(length 3.81)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 5.08 -71.12 180)
				(length 3.81)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 5.08 -73.66 180)
				(length 3.81)
				(name "Pin_58")
				(number "58")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x58_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 73.66 0)
		)
		(property "Value" "Conn_01x58_Socket"
			(at 0 -76.2 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x58, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x58_Socket_1_1"
			(pin passive line
				(at -5.08 71.12 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 68.58 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 3.81)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 3.81)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 3.81)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 3.81)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 3.81)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 3.81)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 3.81)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -73.66 0)
				(length 3.81)
				(name "Pin_58")
				(number "58")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x59_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 76.2 0)
		)
		(property "Value" "Conn_01x59_Pin"
			(at 0 -76.2 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x59, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x59_Pin_1_1"
			(pin passive line
				(at 5.08 73.66 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 71.12 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 68.58 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 66.04 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 63.5 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 60.96 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 58.42 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 55.88 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 53.34 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 50.8 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 5.08 -50.8 180)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 5.08 -53.34 180)
				(length 3.81)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 5.08 -55.88 180)
				(length 3.81)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 5.08 -58.42 180)
				(length 3.81)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 5.08 -60.96 180)
				(length 3.81)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 5.08 -63.5 180)
				(length 3.81)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 5.08 -66.04 180)
				(length 3.81)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 5.08 -68.58 180)
				(length 3.81)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 5.08 -71.12 180)
				(length 3.81)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 5.08 -73.66 180)
				(length 3.81)
				(name "Pin_59")
				(number "59")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x59_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 76.2 0)
		)
		(property "Value" "Conn_01x59_Socket"
			(at 0 -76.2 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x59, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x59_Socket_1_1"
			(pin passive line
				(at -5.08 73.66 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 71.12 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 68.58 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 3.81)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 3.81)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 3.81)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 3.81)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 3.81)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 3.81)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 3.81)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 3.81)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at -5.08 -73.66 0)
				(length 3.81)
				(name "Pin_59")
				(number "59")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x60_Pin"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 76.2 0)
		)
		(property "Value" "Conn_01x60_Pin"
			(at 0 -78.74 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x60, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x60_Pin_1_1"
			(pin passive line
				(at 5.08 73.66 180)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 5.08 71.12 180)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 5.08 68.58 180)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 5.08 66.04 180)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 5.08 63.5 180)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 5.08 60.96 180)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 5.08 58.42 180)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 5.08 55.88 180)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 5.08 53.34 180)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 5.08 50.8 180)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 5.08 48.26 180)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 5.08 45.72 180)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 5.08 43.18 180)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 5.08 -40.64 180)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 5.08 -43.18 180)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 5.08 -45.72 180)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 5.08 -48.26 180)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 5.08 -50.8 180)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 5.08 -53.34 180)
				(length 3.81)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 5.08 -55.88 180)
				(length 3.81)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 5.08 -58.42 180)
				(length 3.81)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 5.08 -60.96 180)
				(length 3.81)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 5.08 -63.5 180)
				(length 3.81)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 5.08 -66.04 180)
				(length 3.81)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 5.08 -68.58 180)
				(length 3.81)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 5.08 -71.12 180)
				(length 3.81)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 5.08 -73.66 180)
				(length 3.81)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 5.08 -76.2 180)
				(length 3.81)
				(name "Pin_60")
				(number "60")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x60_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 76.2 0)
		)
		(property "Value" "Conn_01x60_Socket"
			(at 0 -78.74 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic connector, single row, 01x60, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??_*"
			(at 0 0 0)
		)
		(symbol "Conn_01x60_Socket_1_1"
			(pin passive line
				(at -5.08 73.66 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 71.12 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 68.58 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 3.81)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 3.81)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 3.81)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 3.81)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 3.81)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 3.81)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 3.81)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 3.81)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at -5.08 -73.66 0)
				(length 3.81)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at -5.08 -76.2 0)
				(length 3.81)
				(name "Pin_60")
				(number "60")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_15X4"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 80.01 0)
		)
		(property "Value" "Conn_15X4"
			(at 6.35 2.54 90)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 2.54 0)
		)
		(property "Description" "Connector Europe, 60 contacts, ranges A,B,C,D"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(symbol "Conn_15X4_0_1")
		(symbol "Conn_15X4_1_1"
			(pin passive line
				(at -7.62 76.2 0)
				(length 3.81)
				(name "1A")
				(number "A1")
			)
			(pin passive line
				(at -7.62 73.66 0)
				(length 3.81)
				(name "1B")
				(number "B1")
			)
			(pin passive line
				(at -7.62 71.12 0)
				(length 3.81)
				(name "1C")
				(number "C1")
			)
			(pin passive line
				(at -7.62 68.58 0)
				(length 3.81)
				(name "1D")
				(number "D1")
			)
			(pin passive line
				(at -7.62 66.04 0)
				(length 3.81)
				(name "2A")
				(number "A2")
			)
			(pin passive line
				(at -7.62 63.5 0)
				(length 3.81)
				(name "2B")
				(number "B2")
			)
			(pin passive line
				(at -7.62 60.96 0)
				(length 3.81)
				(name "2C")
				(number "C2")
			)
			(pin passive line
				(at -7.62 58.42 0)
				(length 3.81)
				(name "2D")
				(number "D2")
			)
			(pin passive line
				(at -7.62 55.88 0)
				(length 3.81)
				(name "3A")
				(number "A3")
			)
			(pin passive line
				(at -7.62 53.34 0)
				(length 3.81)
				(name "3B")
				(number "B3")
			)
			(pin passive line
				(at -7.62 50.8 0)
				(length 3.81)
				(name "3C")
				(number "C3")
			)
			(pin passive line
				(at -7.62 48.26 0)
				(length 3.81)
				(name "3D")
				(number "D3")
			)
			(pin passive line
				(at -7.62 45.72 0)
				(length 3.81)
				(name "4A")
				(number "A4")
			)
			(pin passive line
				(at -7.62 43.18 0)
				(length 3.81)
				(name "4B")
				(number "B4")
			)
			(pin passive line
				(at -7.62 40.64 0)
				(length 3.81)
				(name "4C")
				(number "C4")
			)
			(pin passive line
				(at -7.62 38.1 0)
				(length 3.81)
				(name "4D")
				(number "D4")
			)
			(pin passive line
				(at -7.62 35.56 0)
				(length 3.81)
				(name "5A")
				(number "A5")
			)
			(pin passive line
				(at -7.62 33.02 0)
				(length 3.81)
				(name "5B")
				(number "B5")
			)
			(pin passive line
				(at -7.62 30.48 0)
				(length 3.81)
				(name "5C")
				(number "C5")
			)
			(pin passive line
				(at -7.62 27.94 0)
				(length 3.81)
				(name "5D")
				(number "D5")
			)
			(pin passive line
				(at -7.62 25.4 0)
				(length 3.81)
				(name "6A")
				(number "A6")
			)
			(pin passive line
				(at -7.62 22.86 0)
				(length 3.81)
				(name "6B")
				(number "B6")
			)
			(pin passive line
				(at -7.62 20.32 0)
				(length 3.81)
				(name "6C")
				(number "C6")
			)
			(pin passive line
				(at -7.62 17.78 0)
				(length 3.81)
				(name "6D")
				(number "D6")
			)
			(pin passive line
				(at -7.62 15.24 0)
				(length 3.81)
				(name "7A")
				(number "A7")
			)
			(pin passive line
				(at -7.62 12.7 0)
				(length 3.81)
				(name "7B")
				(number "B7")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "7C")
				(number "C7")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "7D")
				(number "D7")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "8A")
				(number "A8")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "8B")
				(number "B8")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "8C")
				(number "C8")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "8D")
				(number "D8")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "9A")
				(number "A9")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "9B")
				(number "B9")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "9C")
				(number "C9")
			)
			(pin passive line
				(at -7.62 -12.7 0)
				(length 3.81)
				(name "9D")
				(number "D9")
			)
			(pin passive line
				(at -7.62 -15.24 0)
				(length 3.81)
				(name "10A")
				(number "A10")
			)
			(pin passive line
				(at -7.62 -17.78 0)
				(length 3.81)
				(name "10B")
				(number "B10")
			)
			(pin passive line
				(at -7.62 -20.32 0)
				(length 3.81)
				(name "10C")
				(number "C10")
			)
			(pin passive line
				(at -7.62 -22.86 0)
				(length 3.81)
				(name "10D")
				(number "D10")
			)
			(pin passive line
				(at -7.62 -25.4 0)
				(length 3.81)
				(name "11A")
				(number "A11")
			)
			(pin passive line
				(at -7.62 -27.94 0)
				(length 3.81)
				(name "11B")
				(number "B11")
			)
			(pin passive line
				(at -7.62 -30.48 0)
				(length 3.81)
				(name "11C")
				(number "C11")
			)
			(pin passive line
				(at -7.62 -33.02 0)
				(length 3.81)
				(name "11D")
				(number "D11")
			)
			(pin passive line
				(at -7.62 -35.56 0)
				(length 3.81)
				(name "12A")
				(number "A12")
			)
			(pin passive line
				(at -7.62 -38.1 0)
				(length 3.81)
				(name "12B")
				(number "B12")
			)
			(pin passive line
				(at -7.62 -40.64 0)
				(length 3.81)
				(name "12C")
				(number "C12")
			)
			(pin passive line
				(at -7.62 -43.18 0)
				(length 3.81)
				(name "12D")
				(number "D12")
			)
			(pin passive line
				(at -7.62 -45.72 0)
				(length 3.81)
				(name "13A")
				(number "A13")
			)
			(pin passive line
				(at -7.62 -48.26 0)
				(length 3.81)
				(name "13B")
				(number "B13")
			)
			(pin passive line
				(at -7.62 -50.8 0)
				(length 3.81)
				(name "13C")
				(number "C13")
			)
			(pin passive line
				(at -7.62 -53.34 0)
				(length 3.81)
				(name "13D")
				(number "D13")
			)
			(pin passive line
				(at -7.62 -55.88 0)
				(length 3.81)
				(name "14A")
				(number "A14")
			)
			(pin passive line
				(at -7.62 -58.42 0)
				(length 3.81)
				(name "14B")
				(number "B14")
			)
			(pin passive line
				(at -7.62 -60.96 0)
				(length 3.81)
				(name "14C")
				(number "C14")
			)
			(pin passive line
				(at -7.62 -63.5 0)
				(length 3.81)
				(name "14D")
				(number "D14")
			)
			(pin passive line
				(at -7.62 -66.04 0)
				(length 3.81)
				(name "15A")
				(number "A15")
			)
			(pin passive line
				(at -7.62 -68.58 0)
				(length 3.81)
				(name "15B")
				(number "B15")
			)
			(pin passive line
				(at -7.62 -71.12 0)
				(length 3.81)
				(name "15C")
				(number "C15")
			)
			(pin passive line
				(at -7.62 -73.66 0)
				(length 3.81)
				(name "15D")
				(number "D15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_ARM_Cortex_Debug_ETM_20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -0.508 0 0)
		)
		(property "Value" "Conn_ARM_Cortex_Debug_ETM_20"
			(at 0 25.4 0)
		)
		(property "Footprint" ""
			(at -2.54 7.62 0)
		)
		(property "Datasheet" "http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf"
			(at 0 0 0)
		)
		(property "Description" "Arm Cortex Debug+ETM Connector"
			(at -0.508 -25.4 0)
		)
		(property "ki_keywords" "Trace"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader?2x10?P1.27mm*"
			(at 0 0 0)
		)
		(symbol "Conn_ARM_Cortex_Debug_ETM_20_0_0"
			(pin passive line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "GNDDetect")
				(number "9")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin open_collector line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "~{RESET}")
				(number "10")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "SWDCLK/TCK")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "SWDIO/TMS")
				(number "2")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "SWO/TDO")
				(number "6")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "NC/TDI")
				(number "8")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "TRACECLK")
				(number "12")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "TRACEDATA0")
				(number "14")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "TRACEDATA1")
				(number "16")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "TRACEDATA2")
				(number "18")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "TRACEDATA3")
				(number "20")
			)
		)
		(symbol "Conn_ARM_Cortex_Debug_ETM_20_1_0"
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VTref")
				(number "1")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "KEY")
				(number "7")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "GND")
				(number "11")
				(alternate "TgtPwr+Cap" power_out line)
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "GND")
				(number "13")
				(alternate "TgtPwr+Cap" power_out line)
			)
		)
		(symbol "Conn_ARM_Cortex_Debug_ETM_20_1_1")
		(embedded_fonts no)
	)
	(symbol "Conn_ARM_JTAG_SWD_10"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -2.54 16.51 0)
		)
		(property "Value" "Conn_ARM_JTAG_SWD_10"
			(at -2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf"
			(at -8.89 -31.75 90)
		)
		(property "Description" "Cortex Debug Connector, standard ARM Cortex-M SWD and JTAG interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cortex Debug Connector ARM SWD JTAG"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader?2x05?P1.27mm*"
			(at 0 0 0)
		)
		(symbol "Conn_ARM_JTAG_SWD_10_0_1")
		(symbol "Conn_ARM_JTAG_SWD_10_1_1"
			(pin no_connect line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "KEY")
				(number "7")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GNDDetect")
				(number "9")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VTref")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{RESET}")
				(number "10")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SWCLK/TCK")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "SWDIO/TMS")
				(number "2")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SWO/TDO")
				(number "6")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "NC/TDI")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_ARM_JTAG_SWD_20"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 21.59 0)
		)
		(property "Value" "Conn_ARM_JTAG_SWD_20"
			(at -5.08 19.05 0)
		)
		(property "Footprint" ""
			(at 11.43 -26.67 0)
		)
		(property "Datasheet" "http://infocenter.arm.com/help/topic/com.arm.doc.dui0499b/DUI0499B_system_design_reference.pdf"
			(at -8.89 -31.75 90)
		)
		(property "Description" "Standard IDC20 Pinheader Connector, ARM legacy JTAG and SWD interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "IDC20 Pinheader Pins Connector ARM JTAG SWD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "IDC*Header*P2.54mm* PinHeader*2x10*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "Conn_ARM_JTAG_SWD_20_0_1")
		(symbol "Conn_ARM_JTAG_SWD_20_1_1"
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VTREF")
				(number "1")
			)
			(pin passive line
				(at -2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at -2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at -2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at -2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at -2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at -2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at -2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at -2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC/NC")
				(number "2")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "~{TRST}")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "~{SRST}")
				(number "15")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RTCK")
				(number "11")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "TCK/SWCLK")
				(number "9")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "TMS/SWDIO")
				(number "7")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "TDO/SWO")
				(number "13")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "TDI")
				(number "5")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "DBGACK/NC")
				(number "19")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "DBGRQ/NC")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_ARM_SWD_TagConnect_TC2030"
		(exclude_from_sim no)
		(in_bom no)
		(on_board yes)
		(property "Reference" "J"
			(at 2.54 11.43 0)
		)
		(property "Value" "Conn_ARM_SWD_TagConnect_TC2030"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Connector:Tag-Connect_TC2030-IDC-FP_2x03_P1.27mm_Vertical"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.tag-connect.com/wp-content/uploads/bsk-pdf-manager/TC2030-CTX_1.pdf"
			(at 0 -15.24 0)
		)
		(property "Description" "Tag-Connect ARM Cortex SWD JTAG connector, 6 pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cortex Debug Connector ARM SWD JTAG"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TC2030*"
			(at 0 0 0)
		)
		(symbol "Conn_ARM_SWD_TagConnect_TC2030_0_0"
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin open_collector line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "~{RESET}")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "SWCLK")
				(number "4")
				(alternate "TCK" output line)
			)
			(pin bidirectional line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "SWDIO")
				(number "2")
				(alternate "TMS" bidirectional line)
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "SWO")
				(number "6")
				(alternate "TDO" input line)
			)
		)
		(symbol "Conn_ARM_SWD_TagConnect_TC2030_0_1")
		(embedded_fonts no)
	)
	(symbol "Conn_Coaxial"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 3.048 0)
		)
		(property "Value" "Conn_Coaxial"
			(at 2.921 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
		)
		(property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*"
			(at 0 0 0)
		)
		(symbol "Conn_Coaxial_0_1")
		(symbol "Conn_Coaxial_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "In")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "Ext")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_Coaxial_Power"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 -1.27 90)
		)
		(property "Value" "Conn_Coaxial_Power"
			(at -3.175 -1.27 90)
		)
		(property "Footprint" ""
			(at 0 -1.27 0)
		)
		(property "Datasheet" "~"
			(at 0 -1.27 0)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
		)
		(property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO*"
			(at 0 0 0)
		)
		(symbol "Conn_Coaxial_Power_0_1")
		(symbol "Conn_Coaxial_Power_1_1"
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "In")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "Ext")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_Coaxial_Small"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 3.048 0)
		)
		(property "Value" "Conn_Coaxial_Small"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "small coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
		)
		(property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*"
			(at 0 0 0)
		)
		(symbol "Conn_Coaxial_Small_0_1")
		(symbol "Conn_Coaxial_Small_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 1.27)
				(name "In")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 1.27)
				(name "Ext")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_Coaxial_x2"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 5.715 0)
		)
		(property "Value" "Conn_Coaxial_x2"
			(at 2.921 0 90)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 -2.54 0)
		)
		(property "Description" "double coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
		)
		(property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO*"
			(at 0 0 0)
		)
		(symbol "Conn_Coaxial_x2_0_1")
		(symbol "Conn_Coaxial_x2_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "IN1")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "IN2")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "EXT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_Coaxial_x2_Isolated"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 3.048 0)
		)
		(property "Value" "Conn_Coaxial_x2_Isolated"
			(at 2.921 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
		)
		(property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO*"
			(at 0 0 0)
		)
		(symbol "Conn_Coaxial_x2_Isolated_0_1")
		(symbol "Conn_Coaxial_x2_Isolated_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "In1")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "Ext1")
				(number "2")
			)
		)
		(symbol "Conn_Coaxial_x2_Isolated_2_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "In2")
				(number "3")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "Ext2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_PIC_ICSP_ICD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 6.35 8.89 0)
		)
		(property "Value" "Conn_PIC_ICSP_ICD"
			(at -8.89 -1.27 90)
		)
		(property "Footprint" ""
			(at 1.27 3.81 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/30277d.pdf"
			(at -7.62 -3.81 90)
		)
		(property "Description" "Microchip PIC In-Circuit Serial Programming/Debugging (ICSP/ICD) connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "icsp icd pic microchip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader*1x06*P2.54mm* PinSocket*1x06*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "Conn_PIC_ICSP_ICD_0_1")
		(symbol "Conn_PIC_ICSP_ICD_1_1"
			(pin passive line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{MCLR}/VPP")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PGD/ICSPDAT")
				(number "4")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PGC/ICSPCLK")
				(number "5")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PGM/LVP")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_Plug_2P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at -7.112 8.636 0)
		)
		(property "Value" "Conn_Plug_2P"
			(at 0.254 -8.89 0)
		)
		(property "Footprint" ""
			(at -4.572 -0.254 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "2 Pins non-protected generic plug"
			(at 0 0 0)
		)
		(property "ki_keywords" "2P mains plug wall"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CEE*7/2* CEE*7/16* CEE*7/17* NEMA*1?15* SN?441011*Type?11*"
			(at 0 0 0)
		)
		(symbol "Conn_Plug_2P_0_1")
		(symbol "Conn_Plug_2P_1_1"
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "L")
				(number "1")
			)
			(pin power_out line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "N")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_Plug_3P_Protected"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at -9.652 11.176 0)
		)
		(property "Value" "Conn_Plug_3P_Protected"
			(at 0.254 -11.43 0)
		)
		(property "Footprint" ""
			(at -23.114 22.86 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "3 Pins protected generic plug"
			(at 0.508 0 0)
		)
		(property "ki_keywords" "3P mains plug protected wall"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CEE*7/2* CEE*7/16* CEE*7/17* NEMA*1?15* SN?441011?Type*11*"
			(at 0 0 0)
		)
		(symbol "Conn_Plug_3P_Protected_0_1")
		(symbol "Conn_Plug_3P_Protected_1_1"
			(pin power_in line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "L")
				(number "1")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "PE")
				(number "3")
			)
			(pin power_out line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "N")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_Receptacle_2P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -7.112 8.636 0)
		)
		(property "Value" "Conn_Receptacle_2P"
			(at 0.254 -8.89 0)
		)
		(property "Footprint" ""
			(at -4.572 -0.254 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "2 Pins non-protected generic plug"
			(at 0.254 0 0)
		)
		(property "ki_keywords" "2P mains receptacle wall"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CEE*7/2* CEE*7/16* CEE*7/17* NEMA*1?15* SN?441011*Type?11*"
			(at 0 0 0)
		)
		(symbol "Conn_Receptacle_2P_0_1")
		(symbol "Conn_Receptacle_2P_1_1"
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "L")
				(number "1")
			)
			(pin power_out line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "N")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_Receptacle_3P_Protected"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -9.652 11.176 0)
		)
		(property "Value" "Conn_Receptacle_3P_Protected"
			(at 0.254 -11.43 0)
		)
		(property "Footprint" ""
			(at -23.114 22.86 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "3 Pins protected generic receptacle"
			(at 0.508 0 0)
		)
		(property "ki_keywords" "3P mains receptacle protected wall"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CEE*7/2* CEE*7/16* CEE*7/17* NEMA*1?15* SN?441011?Type*11*"
			(at 0 0 0)
		)
		(symbol "Conn_Receptacle_3P_Protected_0_1")
		(symbol "Conn_Receptacle_3P_Protected_1_1"
			(pin power_in line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "L")
				(number "2")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "PE")
				(number "3")
			)
			(pin power_out line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "N")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_ST_STDC14"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -8.89 16.51 0)
		)
		(property "Value" "Conn_ST_STDC14"
			(at 17.78 16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/content/ccc/resource/technical/document/user_manual/group1/99/49/91/b6/b2/3a/46/e5/DM00526767/files/DM00526767.pdf/jcr:content/translations/en.DM00526767.pdf"
			(at -8.89 -31.75 90)
		)
		(property "Description" "ST Debug Connector, standard ARM Cortex-M SWD and JTAG interface plus UART"
			(at 0 0 0)
		)
		(property "ki_keywords" "ST STM32 Cortex Debug Connector ARM SWD JTAG"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader?2x07?P1.27mm*"
			(at 0 0 0)
		)
		(symbol "Conn_ST_STDC14_0_1")
		(symbol "Conn_ST_STDC14_1_1"
			(pin no_connect line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "GNDDetect")
				(number "11")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin open_collector line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "~{RST}")
				(number "12")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "JCLK/SWCLK")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "JTMS/SWDIO")
				(number "4")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "JTDO/SWO")
				(number "8")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "JTDI/NC")
				(number "10")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "JRCLK/NC")
				(number "9")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "VCP_RX")
				(number "13")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "VCP_TX")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_Shielded_Pair"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 5.588 0)
		)
		(property "Value" "Conn_Shielded_Pair"
			(at 0 7.62 0)
		)
		(property "Footprint" ""
			(at -0.635 2.54 0)
		)
		(property "Datasheet" "~"
			(at -0.635 2.54 0)
		)
		(property "Description" "triaxial connector (LEMO 00.302, ...)"
			(at 0 0 0)
		)
		(property "ki_keywords" "LEMO triaxial connector differential LVDS Conn_Triaxial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LEMO*"
			(at 0 0 0)
		)
		(symbol "Conn_Shielded_Pair_0_1")
		(symbol "Conn_Shielded_Pair_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "In1")
				(number "1")
			)
			(pin passive line
				(at 0 -2.54 90)
				(length 2.54)
				(name "Ext")
				(number "3")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "In2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_Triaxial"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 5.588 0)
		)
		(property "Value" "Conn_Triaxial"
			(at 0 7.62 0)
		)
		(property "Footprint" ""
			(at -0.635 2.54 0)
		)
		(property "Datasheet" "~"
			(at -0.635 2.54 0)
		)
		(property "Description" "triaxial connector (LEMO 00.302, ...)"
			(at 0 0 0)
		)
		(property "ki_keywords" "LEMO triaxial connector differential LVDS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LEMO*"
			(at 0 0 0)
		)
		(symbol "Conn_Triaxial_0_1")
		(symbol "Conn_Triaxial_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "In1")
				(number "1")
			)
			(pin passive line
				(at 0 -2.54 90)
				(length 2.54)
				(name "Ext")
				(number "3")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "In2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_Triaxial_Same_Side"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 5.588 0)
		)
		(property "Value" "Conn_Triaxial_Same_Side"
			(at 0 7.62 0)
		)
		(property "Footprint" ""
			(at -0.635 2.54 0)
		)
		(property "Datasheet" "~"
			(at -0.635 2.54 0)
		)
		(property "Description" "triaxial connector (LEMO 00.302, ...)"
			(at 0 -7.112 0)
		)
		(property "ki_keywords" "LEMO triaxial connector differential LVDS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LEMO*"
			(at 0 0 0)
		)
		(symbol "Conn_Triaxial_Same_Side_0_1")
		(symbol "Conn_Triaxial_Same_Side_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "In1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "In2")
				(number "2")
			)
			(pin passive line
				(at 0 -2.54 90)
				(length 2.54)
				(name "Ext")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DA15_Pins"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.508 21.59 0)
		)
		(property "Value" "DA15_Pins"
			(at 0 -22.225 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "15-pin D-SUB connector, pins (male) (low-density/2 columns)"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSUB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Pins*"
			(at 0 0 0)
		)
		(symbol "DA15_Pins_0_1")
		(symbol "DA15_Pins_1_1"
			(pin passive line
				(at -7.62 17.78 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at -7.62 15.24 0)
				(length 3.81)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -7.62 12.7 0)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "P13")
				(number "13")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "P12")
				(number "12")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "P111")
				(number "11")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "P10")
				(number "10")
			)
			(pin passive line
				(at -7.62 -12.7 0)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -7.62 -15.24 0)
				(length 3.81)
				(name "P9")
				(number "9")
			)
			(pin passive line
				(at -7.62 -17.78 0)
				(length 3.81)
				(name "1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DA15_Pins_MountingHoles"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 24.13 0)
		)
		(property "Value" "DA15_Pins_MountingHoles"
			(at 0 22.225 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "15-pin D-SUB connector, pins (male) (low-density/2 columns), Mounting Hole"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSUB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Pins*"
			(at 0 0 0)
		)
		(symbol "DA15_Pins_MountingHoles_0_1")
		(symbol "DA15_Pins_MountingHoles_1_1"
			(pin passive line
				(at -7.62 17.78 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at -7.62 15.24 0)
				(length 3.81)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -7.62 12.7 0)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "P13")
				(number "13")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "P12")
				(number "12")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "P111")
				(number "11")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "P10")
				(number "10")
			)
			(pin passive line
				(at -7.62 -12.7 0)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -7.62 -15.24 0)
				(length 3.81)
				(name "P9")
				(number "9")
			)
			(pin passive line
				(at -7.62 -17.78 0)
				(length 3.81)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(name "PAD")
				(number "0")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DA15_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.508 21.59 0)
		)
		(property "Value" "DA15_Socket"
			(at 0 -22.225 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "15-pin D-SUB connector, socket (female) (low-density/2 columns)"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSUB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Socket*"
			(at 0 0 0)
		)
		(symbol "DA15_Socket_0_1")
		(symbol "DA15_Socket_1_1"
			(pin passive line
				(at -7.62 17.78 0)
				(length 3.81)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -7.62 15.24 0)
				(length 3.81)
				(name "P9")
				(number "9")
			)
			(pin passive line
				(at -7.62 12.7 0)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "P10")
				(number "10")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "P111")
				(number "11")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "P12")
				(number "12")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "P13")
				(number "13")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -7.62 -12.7 0)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -7.62 -15.24 0)
				(length 3.81)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -7.62 -17.78 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DA15_Socket_MountingHoles"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 24.13 0)
		)
		(property "Value" "DA15_Socket_MountingHoles"
			(at 0 22.225 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "15-pin D-SUB connector, socket (female) (low-density/2 columns), Mounting Hole"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSUB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Socket*"
			(at 0 0 0)
		)
		(symbol "DA15_Socket_MountingHoles_0_1")
		(symbol "DA15_Socket_MountingHoles_1_1"
			(pin passive line
				(at -7.62 17.78 0)
				(length 3.81)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -7.62 15.24 0)
				(length 3.81)
				(name "P9")
				(number "9")
			)
			(pin passive line
				(at -7.62 12.7 0)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "P10")
				(number "10")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "P111")
				(number "11")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "P12")
				(number "12")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "P13")
				(number "13")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -7.62 -12.7 0)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -7.62 -15.24 0)
				(length 3.81)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -7.62 -17.78 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(name "PAD")
				(number "0")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DB25_Pins"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 34.29 0)
		)
		(property "Value" "DB25_Pins"
			(at 0 -34.925 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "25-pin D-SUB connector, pins (male)"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSUB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Pins*"
			(at 0 0 0)
		)
		(symbol "DB25_Pins_0_1")
		(symbol "DB25_Pins_1_1"
			(pin passive line
				(at -7.62 30.48 0)
				(length 3.81)
				(name "13")
				(number "13")
			)
			(pin passive line
				(at -7.62 27.94 0)
				(length 3.81)
				(name "P25")
				(number "25")
			)
			(pin passive line
				(at -7.62 25.4 0)
				(length 3.81)
				(name "12")
				(number "12")
			)
			(pin passive line
				(at -7.62 22.86 0)
				(length 3.81)
				(name "P24")
				(number "24")
			)
			(pin passive line
				(at -7.62 20.32 0)
				(length 3.81)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at -7.62 17.78 0)
				(length 3.81)
				(name "P23")
				(number "23")
			)
			(pin passive line
				(at -7.62 15.24 0)
				(length 3.81)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at -7.62 12.7 0)
				(length 3.81)
				(name "P22")
				(number "22")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "P21")
				(number "21")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "P20")
				(number "20")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "P19")
				(number "19")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "P18")
				(number "18")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -7.62 -12.7 0)
				(length 3.81)
				(name "P17")
				(number "17")
			)
			(pin passive line
				(at -7.62 -15.24 0)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -7.62 -17.78 0)
				(length 3.81)
				(name "P16")
				(number "16")
			)
			(pin passive line
				(at -7.62 -20.32 0)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -7.62 -22.86 0)
				(length 3.81)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -7.62 -25.4 0)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -7.62 -27.94 0)
				(length 3.81)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -7.62 -30.48 0)
				(length 3.81)
				(name "1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DB25_Pins_MountingHoles"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 36.83 0)
		)
		(property "Value" "DB25_Pins_MountingHoles"
			(at 0 34.925 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "25-pin D-SUB connector, pins (male), Mounting Hole"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSUB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Pins*"
			(at 0 0 0)
		)
		(symbol "DB25_Pins_MountingHoles_0_1")
		(symbol "DB25_Pins_MountingHoles_1_1"
			(pin passive line
				(at -7.62 30.48 0)
				(length 3.81)
				(name "13")
				(number "13")
			)
			(pin passive line
				(at -7.62 27.94 0)
				(length 3.81)
				(name "P25")
				(number "25")
			)
			(pin passive line
				(at -7.62 25.4 0)
				(length 3.81)
				(name "12")
				(number "12")
			)
			(pin passive line
				(at -7.62 22.86 0)
				(length 3.81)
				(name "P24")
				(number "24")
			)
			(pin passive line
				(at -7.62 20.32 0)
				(length 3.81)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at -7.62 17.78 0)
				(length 3.81)
				(name "P23")
				(number "23")
			)
			(pin passive line
				(at -7.62 15.24 0)
				(length 3.81)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at -7.62 12.7 0)
				(length 3.81)
				(name "P22")
				(number "22")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "P21")
				(number "21")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "P20")
				(number "20")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "P19")
				(number "19")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "P18")
				(number "18")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -7.62 -12.7 0)
				(length 3.81)
				(name "P17")
				(number "17")
			)
			(pin passive line
				(at -7.62 -15.24 0)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -7.62 -17.78 0)
				(length 3.81)
				(name "P16")
				(number "16")
			)
			(pin passive line
				(at -7.62 -20.32 0)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -7.62 -22.86 0)
				(length 3.81)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -7.62 -25.4 0)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -7.62 -27.94 0)
				(length 3.81)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -7.62 -30.48 0)
				(length 3.81)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(name "PAD")
				(number "0")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DB25_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 34.29 0)
		)
		(property "Value" "DB25_Socket"
			(at 0 -34.925 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "25-pin D-SUB connector, socket (female)"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSUB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Socket*"
			(at 0 0 0)
		)
		(symbol "DB25_Socket_0_1")
		(symbol "DB25_Socket_1_1"
			(pin passive line
				(at -7.62 30.48 0)
				(length 3.81)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -7.62 27.94 0)
				(length 3.81)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -7.62 25.4 0)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -7.62 22.86 0)
				(length 3.81)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -7.62 20.32 0)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -7.62 17.78 0)
				(length 3.81)
				(name "P16")
				(number "16")
			)
			(pin passive line
				(at -7.62 15.24 0)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -7.62 12.7 0)
				(length 3.81)
				(name "P17")
				(number "17")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "P18")
				(number "18")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "P19")
				(number "19")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "P20")
				(number "20")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "P21")
				(number "21")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at -7.62 -12.7 0)
				(length 3.81)
				(name "P22")
				(number "22")
			)
			(pin passive line
				(at -7.62 -15.24 0)
				(length 3.81)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at -7.62 -17.78 0)
				(length 3.81)
				(name "P23")
				(number "23")
			)
			(pin passive line
				(at -7.62 -20.32 0)
				(length 3.81)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at -7.62 -22.86 0)
				(length 3.81)
				(name "P24")
				(number "24")
			)
			(pin passive line
				(at -7.62 -25.4 0)
				(length 3.81)
				(name "12")
				(number "12")
			)
			(pin passive line
				(at -7.62 -27.94 0)
				(length 3.81)
				(name "P25")
				(number "25")
			)
			(pin passive line
				(at -7.62 -30.48 0)
				(length 3.81)
				(name "13")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DB25_Socket_MountingHoles"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 36.83 0)
		)
		(property "Value" "DB25_Socket_MountingHoles"
			(at 0 34.925 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "25-pin D-SUB connector, socket (female), Mounting Hole"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSUB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Socket*"
			(at 0 0 0)
		)
		(symbol "DB25_Socket_MountingHoles_0_1")
		(symbol "DB25_Socket_MountingHoles_1_1"
			(pin passive line
				(at -7.62 30.48 0)
				(length 3.81)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -7.62 27.94 0)
				(length 3.81)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -7.62 25.4 0)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -7.62 22.86 0)
				(length 3.81)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -7.62 20.32 0)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -7.62 17.78 0)
				(length 3.81)
				(name "P16")
				(number "16")
			)
			(pin passive line
				(at -7.62 15.24 0)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -7.62 12.7 0)
				(length 3.81)
				(name "P17")
				(number "17")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "P18")
				(number "18")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "P19")
				(number "19")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "P20")
				(number "20")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "P21")
				(number "21")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at -7.62 -12.7 0)
				(length 3.81)
				(name "P22")
				(number "22")
			)
			(pin passive line
				(at -7.62 -15.24 0)
				(length 3.81)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at -7.62 -17.78 0)
				(length 3.81)
				(name "P23")
				(number "23")
			)
			(pin passive line
				(at -7.62 -20.32 0)
				(length 3.81)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at -7.62 -22.86 0)
				(length 3.81)
				(name "P24")
				(number "24")
			)
			(pin passive line
				(at -7.62 -25.4 0)
				(length 3.81)
				(name "12")
				(number "12")
			)
			(pin passive line
				(at -7.62 -27.94 0)
				(length 3.81)
				(name "P25")
				(number "25")
			)
			(pin passive line
				(at -7.62 -30.48 0)
				(length 3.81)
				(name "13")
				(number "13")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(name "PAD")
				(number "0")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DC37_Pins"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 50.8 0)
		)
		(property "Value" "DC37_Pins"
			(at 0 -50.8 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "37-pin D-SUB connector, pins (male)"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSUB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Pins*"
			(at 0 0 0)
		)
		(symbol "DC37_Pins_0_1")
		(symbol "DC37_Pins_1_1"
			(pin passive line
				(at -7.62 45.72 0)
				(length 3.81)
				(name "19")
				(number "19")
			)
			(pin passive line
				(at -7.62 43.18 0)
				(length 3.81)
				(name "37")
				(number "37")
			)
			(pin passive line
				(at -7.62 40.64 0)
				(length 3.81)
				(name "18")
				(number "18")
			)
			(pin passive line
				(at -7.62 38.1 0)
				(length 3.81)
				(name "36")
				(number "36")
			)
			(pin passive line
				(at -7.62 35.56 0)
				(length 3.81)
				(name "17")
				(number "17")
			)
			(pin passive line
				(at -7.62 33.02 0)
				(length 3.81)
				(name "35")
				(number "35")
			)
			(pin passive line
				(at -7.62 30.48 0)
				(length 3.81)
				(name "16")
				(number "16")
			)
			(pin passive line
				(at -7.62 27.94 0)
				(length 3.81)
				(name "34")
				(number "34")
			)
			(pin passive line
				(at -7.62 25.4 0)
				(length 3.81)
				(name "15")
				(number "15")
			)
			(pin passive line
				(at -7.62 22.86 0)
				(length 3.81)
				(name "33")
				(number "33")
			)
			(pin passive line
				(at -7.62 20.32 0)
				(length 3.81)
				(name "14")
				(number "14")
			)
			(pin passive line
				(at -7.62 17.78 0)
				(length 3.81)
				(name "32")
				(number "32")
			)
			(pin passive line
				(at -7.62 15.24 0)
				(length 3.81)
				(name "13")
				(number "13")
			)
			(pin passive line
				(at -7.62 12.7 0)
				(length 3.81)
				(name "31")
				(number "31")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "12")
				(number "12")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "30")
				(number "30")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "29")
				(number "29")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "28")
				(number "28")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "27")
				(number "27")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at -7.62 -12.7 0)
				(length 3.81)
				(name "26")
				(number "26")
			)
			(pin passive line
				(at -7.62 -15.24 0)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -7.62 -17.78 0)
				(length 3.81)
				(name "25")
				(number "25")
			)
			(pin passive line
				(at -7.62 -20.32 0)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -7.62 -22.86 0)
				(length 3.81)
				(name "24")
				(number "24")
			)
			(pin passive line
				(at -7.62 -25.4 0)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -7.62 -27.94 0)
				(length 3.81)
				(name "23")
				(number "23")
			)
			(pin passive line
				(at -7.62 -30.48 0)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -7.62 -33.02 0)
				(length 3.81)
				(name "22")
				(number "22")
			)
			(pin passive line
				(at -7.62 -35.56 0)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -7.62 -38.1 0)
				(length 3.81)
				(name "21")
				(number "21")
			)
			(pin passive line
				(at -7.62 -40.64 0)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -7.62 -43.18 0)
				(length 3.81)
				(name "20")
				(number "20")
			)
			(pin passive line
				(at -7.62 -45.72 0)
				(length 3.81)
				(name "1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DC37_Pins_MountingHoles"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 52.705 0)
		)
		(property "Value" "DC37_Pins_MountingHoles"
			(at 0 50.8 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "37-pin D-SUB connector, pins (male), Mounting Hole"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSUB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Pins*"
			(at 0 0 0)
		)
		(symbol "DC37_Pins_MountingHoles_0_1")
		(symbol "DC37_Pins_MountingHoles_1_1"
			(pin passive line
				(at -7.62 45.72 0)
				(length 3.81)
				(name "19")
				(number "19")
			)
			(pin passive line
				(at -7.62 43.18 0)
				(length 3.81)
				(name "37")
				(number "37")
			)
			(pin passive line
				(at -7.62 40.64 0)
				(length 3.81)
				(name "18")
				(number "18")
			)
			(pin passive line
				(at -7.62 38.1 0)
				(length 3.81)
				(name "36")
				(number "36")
			)
			(pin passive line
				(at -7.62 35.56 0)
				(length 3.81)
				(name "17")
				(number "17")
			)
			(pin passive line
				(at -7.62 33.02 0)
				(length 3.81)
				(name "35")
				(number "35")
			)
			(pin passive line
				(at -7.62 30.48 0)
				(length 3.81)
				(name "16")
				(number "16")
			)
			(pin passive line
				(at -7.62 27.94 0)
				(length 3.81)
				(name "34")
				(number "34")
			)
			(pin passive line
				(at -7.62 25.4 0)
				(length 3.81)
				(name "15")
				(number "15")
			)
			(pin passive line
				(at -7.62 22.86 0)
				(length 3.81)
				(name "33")
				(number "33")
			)
			(pin passive line
				(at -7.62 20.32 0)
				(length 3.81)
				(name "14")
				(number "14")
			)
			(pin passive line
				(at -7.62 17.78 0)
				(length 3.81)
				(name "32")
				(number "32")
			)
			(pin passive line
				(at -7.62 15.24 0)
				(length 3.81)
				(name "13")
				(number "13")
			)
			(pin passive line
				(at -7.62 12.7 0)
				(length 3.81)
				(name "31")
				(number "31")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "12")
				(number "12")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "30")
				(number "30")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "29")
				(number "29")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "28")
				(number "28")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "27")
				(number "27")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at -7.62 -12.7 0)
				(length 3.81)
				(name "26")
				(number "26")
			)
			(pin passive line
				(at -7.62 -15.24 0)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -7.62 -17.78 0)
				(length 3.81)
				(name "25")
				(number "25")
			)
			(pin passive line
				(at -7.62 -20.32 0)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -7.62 -22.86 0)
				(length 3.81)
				(name "24")
				(number "24")
			)
			(pin passive line
				(at -7.62 -25.4 0)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -7.62 -27.94 0)
				(length 3.81)
				(name "23")
				(number "23")
			)
			(pin passive line
				(at -7.62 -30.48 0)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -7.62 -33.02 0)
				(length 3.81)
				(name "22")
				(number "22")
			)
			(pin passive line
				(at -7.62 -35.56 0)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -7.62 -38.1 0)
				(length 3.81)
				(name "21")
				(number "21")
			)
			(pin passive line
				(at -7.62 -40.64 0)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -7.62 -43.18 0)
				(length 3.81)
				(name "20")
				(number "20")
			)
			(pin passive line
				(at -7.62 -45.72 0)
				(length 3.81)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(name "PAD")
				(number "0")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DC37_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 50.165 0)
		)
		(property "Value" "DC37_Socket"
			(at 0 -50.8 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "37-pin D-SUB connector, socket (female)"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSUB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Socket*"
			(at 0 0 0)
		)
		(symbol "DC37_Socket_0_1")
		(symbol "DC37_Socket_1_1"
			(pin passive line
				(at -7.62 45.72 0)
				(length 3.81)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -7.62 43.18 0)
				(length 3.81)
				(name "20")
				(number "20")
			)
			(pin passive line
				(at -7.62 40.64 0)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -7.62 38.1 0)
				(length 3.81)
				(name "21")
				(number "21")
			)
			(pin passive line
				(at -7.62 35.56 0)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -7.62 33.02 0)
				(length 3.81)
				(name "22")
				(number "22")
			)
			(pin passive line
				(at -7.62 30.48 0)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -7.62 27.94 0)
				(length 3.81)
				(name "23")
				(number "23")
			)
			(pin passive line
				(at -7.62 25.4 0)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -7.62 22.86 0)
				(length 3.81)
				(name "24")
				(number "24")
			)
			(pin passive line
				(at -7.62 20.32 0)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -7.62 17.78 0)
				(length 3.81)
				(name "25")
				(number "25")
			)
			(pin passive line
				(at -7.62 15.24 0)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -7.62 12.7 0)
				(length 3.81)
				(name "26")
				(number "26")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "27")
				(number "27")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "28")
				(number "28")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "29")
				(number "29")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "30")
				(number "30")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "12")
				(number "12")
			)
			(pin passive line
				(at -7.62 -12.7 0)
				(length 3.81)
				(name "31")
				(number "31")
			)
			(pin passive line
				(at -7.62 -15.24 0)
				(length 3.81)
				(name "13")
				(number "13")
			)
			(pin passive line
				(at -7.62 -17.78 0)
				(length 3.81)
				(name "32")
				(number "32")
			)
			(pin passive line
				(at -7.62 -20.32 0)
				(length 3.81)
				(name "14")
				(number "14")
			)
			(pin passive line
				(at -7.62 -22.86 0)
				(length 3.81)
				(name "33")
				(number "33")
			)
			(pin passive line
				(at -7.62 -25.4 0)
				(length 3.81)
				(name "15")
				(number "15")
			)
			(pin passive line
				(at -7.62 -27.94 0)
				(length 3.81)
				(name "34")
				(number "34")
			)
			(pin passive line
				(at -7.62 -30.48 0)
				(length 3.81)
				(name "16")
				(number "16")
			)
			(pin passive line
				(at -7.62 -33.02 0)
				(length 3.81)
				(name "35")
				(number "35")
			)
			(pin passive line
				(at -7.62 -35.56 0)
				(length 3.81)
				(name "17")
				(number "17")
			)
			(pin passive line
				(at -7.62 -38.1 0)
				(length 3.81)
				(name "36")
				(number "36")
			)
			(pin passive line
				(at -7.62 -40.64 0)
				(length 3.81)
				(name "18")
				(number "18")
			)
			(pin passive line
				(at -7.62 -43.18 0)
				(length 3.81)
				(name "37")
				(number "37")
			)
			(pin passive line
				(at -7.62 -45.72 0)
				(length 3.81)
				(name "19")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DC37_Socket_MountingHoles"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 52.07 0)
		)
		(property "Value" "DC37_Socket_MountingHoles"
			(at 0 50.165 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "37-pin D-SUB connector, socket (female), Mounting Hole"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSUB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Socket*"
			(at 0 0 0)
		)
		(symbol "DC37_Socket_MountingHoles_0_1")
		(symbol "DC37_Socket_MountingHoles_1_1"
			(pin passive line
				(at -7.62 45.72 0)
				(length 3.81)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -7.62 43.18 0)
				(length 3.81)
				(name "20")
				(number "20")
			)
			(pin passive line
				(at -7.62 40.64 0)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -7.62 38.1 0)
				(length 3.81)
				(name "21")
				(number "21")
			)
			(pin passive line
				(at -7.62 35.56 0)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -7.62 33.02 0)
				(length 3.81)
				(name "22")
				(number "22")
			)
			(pin passive line
				(at -7.62 30.48 0)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -7.62 27.94 0)
				(length 3.81)
				(name "23")
				(number "23")
			)
			(pin passive line
				(at -7.62 25.4 0)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -7.62 22.86 0)
				(length 3.81)
				(name "24")
				(number "24")
			)
			(pin passive line
				(at -7.62 20.32 0)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -7.62 17.78 0)
				(length 3.81)
				(name "25")
				(number "25")
			)
			(pin passive line
				(at -7.62 15.24 0)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -7.62 12.7 0)
				(length 3.81)
				(name "26")
				(number "26")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "27")
				(number "27")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "28")
				(number "28")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "29")
				(number "29")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "30")
				(number "30")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "12")
				(number "12")
			)
			(pin passive line
				(at -7.62 -12.7 0)
				(length 3.81)
				(name "31")
				(number "31")
			)
			(pin passive line
				(at -7.62 -15.24 0)
				(length 3.81)
				(name "13")
				(number "13")
			)
			(pin passive line
				(at -7.62 -17.78 0)
				(length 3.81)
				(name "32")
				(number "32")
			)
			(pin passive line
				(at -7.62 -20.32 0)
				(length 3.81)
				(name "14")
				(number "14")
			)
			(pin passive line
				(at -7.62 -22.86 0)
				(length 3.81)
				(name "33")
				(number "33")
			)
			(pin passive line
				(at -7.62 -25.4 0)
				(length 3.81)
				(name "15")
				(number "15")
			)
			(pin passive line
				(at -7.62 -27.94 0)
				(length 3.81)
				(name "34")
				(number "34")
			)
			(pin passive line
				(at -7.62 -30.48 0)
				(length 3.81)
				(name "16")
				(number "16")
			)
			(pin passive line
				(at -7.62 -33.02 0)
				(length 3.81)
				(name "35")
				(number "35")
			)
			(pin passive line
				(at -7.62 -35.56 0)
				(length 3.81)
				(name "17")
				(number "17")
			)
			(pin passive line
				(at -7.62 -38.1 0)
				(length 3.81)
				(name "36")
				(number "36")
			)
			(pin passive line
				(at -7.62 -40.64 0)
				(length 3.81)
				(name "18")
				(number "18")
			)
			(pin passive line
				(at -7.62 -43.18 0)
				(length 3.81)
				(name "37")
				(number "37")
			)
			(pin passive line
				(at -7.62 -45.72 0)
				(length 3.81)
				(name "19")
				(number "19")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(name "PAD")
				(number "0")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DE15_Pins_HighDensity"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 21.59 0)
		)
		(property "Value" "DE15_Pins_HighDensity"
			(at 0 19.05 0)
		)
		(property "Footprint" ""
			(at -24.13 10.16 0)
		)
		(property "Datasheet" "~"
			(at -24.13 10.16 0)
		)
		(property "Description" "15-pin male plug socket D-SUB connector, High density (3 columns), Triple Row, Generic, VGA-connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSUB VGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Pins*"
			(at 0 0 0)
		)
		(symbol "DE15_Pins_HighDensity_0_1")
		(symbol "DE15_Pins_HighDensity_1_1"
			(pin passive line
				(at -7.62 12.7 0)
				(length 5.08)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 5.08)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 5.08)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 5.08)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 5.08)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 5.08)
				(name "~")
				(number "15")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 5.08)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 5.08)
				(name "~")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DE15_Pins_HighDensity_MountingHoles"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 21.59 0)
		)
		(property "Value" "DE15_Pins_HighDensity_MountingHoles"
			(at 0 19.05 0)
		)
		(property "Footprint" ""
			(at -24.13 10.16 0)
		)
		(property "Datasheet" "~"
			(at -24.13 10.16 0)
		)
		(property "Description" "15-pin male plug socket D-SUB connector, High density (3 columns), Triple Row, Generic, VGA-connector, Mounting Hole"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSUB VGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Pins*"
			(at 0 0 0)
		)
		(symbol "DE15_Pins_HighDensity_MountingHoles_0_1")
		(symbol "DE15_Pins_HighDensity_MountingHoles_1_1"
			(pin passive line
				(at -7.62 12.7 0)
				(length 5.08)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 5.08)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 5.08)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 5.08)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 5.08)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(name "~")
				(number "0")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 5.08)
				(name "~")
				(number "15")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 5.08)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 5.08)
				(name "~")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DE15_Socket_HighDensity"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 21.59 0)
		)
		(property "Value" "DE15_Socket_HighDensity"
			(at 0 19.05 0)
		)
		(property "Footprint" ""
			(at -24.13 10.16 0)
		)
		(property "Datasheet" "~"
			(at -24.13 10.16 0)
		)
		(property "Description" "15-pin D-SUB connector, socket (female), High density (3 columns), Triple Row, Generic, VGA-connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSUB VGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Socket*"
			(at 0 0 0)
		)
		(symbol "DE15_Socket_HighDensity_0_1")
		(symbol "DE15_Socket_HighDensity_1_1"
			(pin passive line
				(at -7.62 12.7 0)
				(length 5.08)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 5.08)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 5.08)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 5.08)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 5.08)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 5.08)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 5.08)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 5.08)
				(name "~")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DE15_Socket_HighDensity_MountingHoles"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 21.59 0)
		)
		(property "Value" "DE15_Socket_HighDensity_MountingHoles"
			(at 0 19.05 0)
		)
		(property "Footprint" ""
			(at -24.13 10.16 0)
		)
		(property "Datasheet" "~"
			(at -24.13 10.16 0)
		)
		(property "Description" "15-pin D-SUB connector, socket (female), High density (3 columns), Triple Row, Generic, VGA-connector, Mounting Hole"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSUB VGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Socket*"
			(at 0 0 0)
		)
		(symbol "DE15_Socket_HighDensity_MountingHoles_0_1")
		(symbol "DE15_Socket_HighDensity_MountingHoles_1_1"
			(pin passive line
				(at -7.62 12.7 0)
				(length 5.08)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 5.08)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 5.08)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 5.08)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(name "~")
				(number "0")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 5.08)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 5.08)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 5.08)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 5.08)
				(name "~")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DE9_Pins"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 13.97 0)
		)
		(property "Value" "DE9_Pins"
			(at 0 -14.605 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "9-pin D-SUB connector, pins (male)"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSUB DB9"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Pins*"
			(at 0 0 0)
		)
		(symbol "DE9_Pins_0_1")
		(symbol "DE9_Pins_1_1"
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DE9_Pins_MountingHoles"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 16.51 0)
		)
		(property "Value" "DE9_Pins_MountingHoles"
			(at 0 14.605 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "9-pin D-SUB connector, pins (male), Mounting Hole"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSUB DB9"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Pins*"
			(at 0 0 0)
		)
		(symbol "DE9_Pins_MountingHoles_0_1")
		(symbol "DE9_Pins_MountingHoles_1_1"
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(name "PAD")
				(number "0")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DE9_Socket"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 13.97 0)
		)
		(property "Value" "DE9_Socket"
			(at 0 -14.605 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "9-pin D-SUB connector, socket (female)"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSUB DB9"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Socket*"
			(at 0 0 0)
		)
		(symbol "DE9_Socket_0_1")
		(symbol "DE9_Socket_1_1"
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "5")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DE9_Socket_MountingHoles"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 16.51 0)
		)
		(property "Value" "DE9_Socket_MountingHoles"
			(at 0 14.605 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "9-pin D-SUB connector, socket (female), Mounting Hole"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSUB DB9"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DSUB*Socket*"
			(at 0 0 0)
		)
		(symbol "DE9_Socket_MountingHoles_0_1")
		(symbol "DE9_Socket_MountingHoles_1_1"
			(pin passive line
				(at -7.62 10.16 0)
				(length 3.81)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 3.81)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(name "PAD")
				(number "0")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN-3"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 3.302 6.35 0)
		)
		(property "Value" "DIN-3"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf"
			(at 0 0 0)
		)
		(property "Description" "3-pin DIN connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "circular DIN connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN*"
			(at 0 0 0)
		)
		(symbol "DIN-3_0_1")
		(symbol "DIN-3_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN-4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 5.334 5.08 0)
		)
		(property "Value" "DIN-4"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf"
			(at 0 0 0)
		)
		(property "Description" "4-pin DIN connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "circular DIN connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN*"
			(at 0 0 0)
		)
		(symbol "DIN-4_0_1")
		(symbol "DIN-4_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN-5"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 3.175 5.715 0)
		)
		(property "Value" "DIN-5"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf"
			(at 0 0 0)
		)
		(property "Description" "5-pin DIN connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "circular DIN connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN*"
			(at 0 0 0)
		)
		(symbol "DIN-5_0_1")
		(symbol "DIN-5_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN-5_180degree"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 3.175 5.715 0)
		)
		(property "Value" "DIN-5_180degree"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf"
			(at 0 0 0)
		)
		(property "Description" "5-pin DIN connector (5-pin DIN-5 stereo)"
			(at 0 0 0)
		)
		(property "ki_keywords" "circular DIN connector stereo audio"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN*"
			(at 0 0 0)
		)
		(symbol "DIN-5_180degree_0_1")
		(symbol "DIN-5_180degree_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN-6"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 3.175 5.715 0)
		)
		(property "Value" "DIN-6"
			(at 4.445 -4.445 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf"
			(at 0 0 0)
		)
		(property "Description" "6-pin DIN connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "circular DIN connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN*"
			(at 0 0 0)
		)
		(symbol "DIN-6_0_1")
		(symbol "DIN-6_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN-7"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 3.175 5.715 0)
		)
		(property "Value" "DIN-7"
			(at 0 -6.604 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf"
			(at 0 0 0)
		)
		(property "Description" "7-pin DIN connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "circular DIN connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN*"
			(at 0 0 0)
		)
		(symbol "DIN-7_0_1")
		(symbol "DIN-7_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN-7_CenterPin7"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 6.35 0)
		)
		(property "Value" "DIN-7_CenterPin7"
			(at 3.048 -5.334 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf"
			(at 0 0 0)
		)
		(property "Description" "7-pin DIN connector with pin 7 in center"
			(at 0 0 0)
		)
		(property "ki_keywords" "circular DIN connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN*"
			(at 0 0 0)
		)
		(symbol "DIN-7_CenterPin7_0_1")
		(symbol "DIN-7_CenterPin7_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN-8"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 3.175 5.715 0)
		)
		(property "Value" "DIN-8"
			(at 2.032 -5.842 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-pin DIN connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "circular DIN connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN*"
			(at 0 0 0)
		)
		(symbol "DIN-8_0_1")
		(symbol "DIN-8_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_01x32_A"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 40.64 0)
		)
		(property "Value" "DIN41612_01x32_A"
			(at 0 -43.18 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, single row (A), 01x32, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*1x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_01x32_A_1_1"
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_a32")
				(number "a32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x05_AB_EvenPins"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 7.62 0)
		)
		(property "Value" "DIN41612_02x05_AB_EvenPins"
			(at 1.27 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (AB) even pins only, 02x05, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x05_AB_EvenPins_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_b10")
				(number "b10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x05_AC_EvenPins"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 7.62 0)
		)
		(property "Value" "DIN41612_02x05_AC_EvenPins"
			(at 1.27 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (AC) even pins only, 02x05, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x05_AC_EvenPins_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_c2")
				(number "c2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_c4")
				(number "c4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_c6")
				(number "c6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_c8")
				(number "c8")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_c10")
				(number "c10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x05_AE_EvenPins"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 7.62 0)
		)
		(property "Value" "DIN41612_02x05_AE_EvenPins"
			(at 1.27 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (AE) even pins only, 02x05, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x05_AE_EvenPins_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_e2")
				(number "e2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_e4")
				(number "e4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_e6")
				(number "e6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_e8")
				(number "e8")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_e10")
				(number "e10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x05_ZB_EvenPins"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 7.62 0)
		)
		(property "Value" "DIN41612_02x05_ZB_EvenPins"
			(at 1.27 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (ZB) even pins only, 02x05, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x05_ZB_EvenPins_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_z2")
				(number "z2")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_z4")
				(number "z4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_z6")
				(number "z6")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_z8")
				(number "z8")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_z10")
				(number "z10")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_b10")
				(number "b10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x08_AB_EvenPins"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 10.16 0)
		)
		(property "Value" "DIN41612_02x08_AB_EvenPins"
			(at 1.27 -12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (AB) even pins only, 02x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x08_AB_EvenPins_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_b16")
				(number "b16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x08_AC_EvenPins"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 10.16 0)
		)
		(property "Value" "DIN41612_02x08_AC_EvenPins"
			(at 1.27 -12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (AC) even pins only, 02x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x08_AC_EvenPins_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_c2")
				(number "c2")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_c4")
				(number "c4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_c6")
				(number "c6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_c8")
				(number "c8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_c10")
				(number "c10")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_c12")
				(number "c12")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_c14")
				(number "c14")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_c16")
				(number "c16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x08_AE_EvenPins"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 10.16 0)
		)
		(property "Value" "DIN41612_02x08_AE_EvenPins"
			(at 1.27 -12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (AE) even pins only, 02x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x08_AE_EvenPins_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_e2")
				(number "e2")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_e4")
				(number "e4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_e6")
				(number "e6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_e8")
				(number "e8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_e10")
				(number "e10")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_e12")
				(number "e12")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_e14")
				(number "e14")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_e16")
				(number "e16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x08_ZB_EvenPins"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 10.16 0)
		)
		(property "Value" "DIN41612_02x08_ZB_EvenPins"
			(at 1.27 -12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (ZB) even pins only, 02x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x08_ZB_EvenPins_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_z2")
				(number "z2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_z4")
				(number "z4")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_z6")
				(number "z6")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_z8")
				(number "z8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_z10")
				(number "z10")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_z12")
				(number "z12")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_z14")
				(number "z14")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_z16")
				(number "z16")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_b16")
				(number "b16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x10_AB"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 12.7 0)
		)
		(property "Value" "DIN41612_02x10_AB"
			(at 1.27 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (AB), 02x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x10_AB_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 3.81)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 3.81)
				(name "Pin_b10")
				(number "b10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x10_AC"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 12.7 0)
		)
		(property "Value" "DIN41612_02x10_AC"
			(at 1.27 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (AC), 02x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x10_AC_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 3.81)
				(name "Pin_c1")
				(number "c1")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_c2")
				(number "c2")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_c3")
				(number "c3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_c4")
				(number "c4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_c5")
				(number "c5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_c6")
				(number "c6")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_c7")
				(number "c7")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_c8")
				(number "c8")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_c9")
				(number "c9")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 3.81)
				(name "Pin_c10")
				(number "c10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x10_AE"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 12.7 0)
		)
		(property "Value" "DIN41612_02x10_AE"
			(at 1.27 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (AE), 02x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x10_AE_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 3.81)
				(name "Pin_e1")
				(number "e1")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_e2")
				(number "e2")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_e3")
				(number "e3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_e4")
				(number "e4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_e5")
				(number "e5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_e6")
				(number "e6")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_e7")
				(number "e7")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_e8")
				(number "e8")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_e9")
				(number "e9")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 3.81)
				(name "Pin_e10")
				(number "e10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x10_ZB"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 12.7 0)
		)
		(property "Value" "DIN41612_02x10_ZB"
			(at 1.27 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (ZB), 02x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x10_ZB_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_z1")
				(number "z1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_z2")
				(number "z2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_z3")
				(number "z3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_z4")
				(number "z4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_z5")
				(number "z5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_z6")
				(number "z6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_z7")
				(number "z7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_z8")
				(number "z8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_z9")
				(number "z9")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_z10")
				(number "z10")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 3.81)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 3.81)
				(name "Pin_b10")
				(number "b10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x16_AB"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 20.32 0)
		)
		(property "Value" "DIN41612_02x16_AB"
			(at 1.27 -22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (AB), 02x16, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x16_AB_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 3.81)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 3.81)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 3.81)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 3.81)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 3.81)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 3.81)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 3.81)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 3.81)
				(name "Pin_b16")
				(number "b16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x16_AB_EvenPins"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 20.32 0)
		)
		(property "Value" "DIN41612_02x16_AB_EvenPins"
			(at 1.27 -22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (AB) even pins only, 02x16, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x16_AB_EvenPins_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 3.81)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 3.81)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 3.81)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 3.81)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 3.81)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 3.81)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 3.81)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 3.81)
				(name "Pin_b32")
				(number "b32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x16_AC"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 20.32 0)
		)
		(property "Value" "DIN41612_02x16_AC"
			(at 1.27 -22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (AC), 02x16, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x16_AC_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 3.81)
				(name "Pin_c1")
				(number "c1")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 3.81)
				(name "Pin_c2")
				(number "c2")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 3.81)
				(name "Pin_c3")
				(number "c3")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 3.81)
				(name "Pin_c4")
				(number "c4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_c5")
				(number "c5")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_c6")
				(number "c6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_c7")
				(number "c7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_c8")
				(number "c8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_c9")
				(number "c9")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_c10")
				(number "c10")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_c11")
				(number "c11")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_c12")
				(number "c12")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 3.81)
				(name "Pin_c13")
				(number "c13")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 3.81)
				(name "Pin_c14")
				(number "c14")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 3.81)
				(name "Pin_c15")
				(number "c15")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 3.81)
				(name "Pin_c16")
				(number "c16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x16_AC_EvenPins"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 20.32 0)
		)
		(property "Value" "DIN41612_02x16_AC_EvenPins"
			(at 1.27 -22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (AC) even pins only, 02x16, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x16_AC_EvenPins_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 3.81)
				(name "Pin_c2")
				(number "c2")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 3.81)
				(name "Pin_c4")
				(number "c4")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 3.81)
				(name "Pin_c6")
				(number "c6")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 3.81)
				(name "Pin_c8")
				(number "c8")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_c10")
				(number "c10")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_c12")
				(number "c12")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_c14")
				(number "c14")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_c16")
				(number "c16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_c18")
				(number "c18")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_c20")
				(number "c20")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_c22")
				(number "c22")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_c24")
				(number "c24")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 3.81)
				(name "Pin_c26")
				(number "c26")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 3.81)
				(name "Pin_c28")
				(number "c28")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 3.81)
				(name "Pin_c30")
				(number "c30")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 3.81)
				(name "Pin_c32")
				(number "c32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x16_AE"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 20.32 0)
		)
		(property "Value" "DIN41612_02x16_AE"
			(at 1.27 -22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (AE), 02x16, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x16_AE_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 3.81)
				(name "Pin_e1")
				(number "e1")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 3.81)
				(name "Pin_e2")
				(number "e2")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 3.81)
				(name "Pin_e3")
				(number "e3")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 3.81)
				(name "Pin_e4")
				(number "e4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_e5")
				(number "e5")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_e6")
				(number "e6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_e7")
				(number "e7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_e8")
				(number "e8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_e9")
				(number "e9")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_e10")
				(number "e10")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_e11")
				(number "e11")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_e12")
				(number "e12")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 3.81)
				(name "Pin_e13")
				(number "e13")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 3.81)
				(name "Pin_e14")
				(number "e14")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 3.81)
				(name "Pin_e15")
				(number "e15")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 3.81)
				(name "Pin_e16")
				(number "e16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x16_AE_EvenPins"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 20.32 0)
		)
		(property "Value" "DIN41612_02x16_AE_EvenPins"
			(at 1.27 -22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (AE) even pins only, 02x16, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x16_AE_EvenPins_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 3.81)
				(name "Pin_e2")
				(number "e2")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 3.81)
				(name "Pin_e4")
				(number "e4")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 3.81)
				(name "Pin_e6")
				(number "e6")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 3.81)
				(name "Pin_e8")
				(number "e8")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_e10")
				(number "e10")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_e12")
				(number "e12")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_e14")
				(number "e14")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_e16")
				(number "e16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_e18")
				(number "e18")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_e20")
				(number "e20")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_e22")
				(number "e22")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_e24")
				(number "e24")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 3.81)
				(name "Pin_e26")
				(number "e26")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 3.81)
				(name "Pin_e28")
				(number "e28")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 3.81)
				(name "Pin_e30")
				(number "e30")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 3.81)
				(name "Pin_e32")
				(number "e32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x16_ZB"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 20.32 0)
		)
		(property "Value" "DIN41612_02x16_ZB"
			(at 1.27 -22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (ZB), 02x16, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x16_ZB_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_z1")
				(number "z1")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_z2")
				(number "z2")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_z3")
				(number "z3")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_z4")
				(number "z4")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_z5")
				(number "z5")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_z6")
				(number "z6")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_z7")
				(number "z7")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_z8")
				(number "z8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_z9")
				(number "z9")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_z10")
				(number "z10")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_z11")
				(number "z11")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_z12")
				(number "z12")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_z13")
				(number "z13")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_z14")
				(number "z14")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_z15")
				(number "z15")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_z16")
				(number "z16")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 3.81)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 3.81)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 3.81)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 3.81)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 3.81)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 3.81)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 3.81)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 3.81)
				(name "Pin_b16")
				(number "b16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x16_ZB_EvenPins"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 20.32 0)
		)
		(property "Value" "DIN41612_02x16_ZB_EvenPins"
			(at 1.27 -22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (ZB) even pins only, 02x16, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x16_ZB_EvenPins_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_z2")
				(number "z2")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_z4")
				(number "z4")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_z6")
				(number "z6")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_z8")
				(number "z8")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_z10")
				(number "z10")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_z12")
				(number "z12")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_z14")
				(number "z14")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_z16")
				(number "z16")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_z18")
				(number "z18")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_z20")
				(number "z20")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_z22")
				(number "z22")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_z24")
				(number "z24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_z26")
				(number "z26")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_z28")
				(number "z28")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_z30")
				(number "z30")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_z32")
				(number "z32")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 3.81)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 3.81)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 3.81)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 3.81)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 3.81)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 3.81)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 3.81)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 3.81)
				(name "Pin_b32")
				(number "b32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x32_AB"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 40.64 0)
		)
		(property "Value" "DIN41612_02x32_AB"
			(at 1.27 -43.18 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (AB), 02x32, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x32_AB_1_1"
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 3.81)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 3.81)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 3.81)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 3.81)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 3.81)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 3.81)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 3.81)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 3.81)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 3.81)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 3.81)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 3.81)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 3.81)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 3.81)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 3.81)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 3.81)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 3.81)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 3.81)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 3.81)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 3.81)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 3.81)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 3.81)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 3.81)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 3.81)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 3.81)
				(name "Pin_b32")
				(number "b32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x32_AC"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 40.64 0)
		)
		(property "Value" "DIN41612_02x32_AC"
			(at 1.27 -43.18 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (AC), 02x32, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x32_AC_1_1"
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 3.81)
				(name "Pin_c1")
				(number "c1")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 3.81)
				(name "Pin_c2")
				(number "c2")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 3.81)
				(name "Pin_c3")
				(number "c3")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 3.81)
				(name "Pin_c4")
				(number "c4")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 3.81)
				(name "Pin_c5")
				(number "c5")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 3.81)
				(name "Pin_c6")
				(number "c6")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 3.81)
				(name "Pin_c7")
				(number "c7")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 3.81)
				(name "Pin_c8")
				(number "c8")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 3.81)
				(name "Pin_c9")
				(number "c9")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 3.81)
				(name "Pin_c10")
				(number "c10")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 3.81)
				(name "Pin_c11")
				(number "c11")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 3.81)
				(name "Pin_c12")
				(number "c12")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_c13")
				(number "c13")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_c14")
				(number "c14")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_c15")
				(number "c15")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_c16")
				(number "c16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_c17")
				(number "c17")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_c18")
				(number "c18")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_c19")
				(number "c19")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_c20")
				(number "c20")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 3.81)
				(name "Pin_c21")
				(number "c21")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 3.81)
				(name "Pin_c22")
				(number "c22")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 3.81)
				(name "Pin_c23")
				(number "c23")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 3.81)
				(name "Pin_c24")
				(number "c24")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 3.81)
				(name "Pin_c25")
				(number "c25")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 3.81)
				(name "Pin_c26")
				(number "c26")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 3.81)
				(name "Pin_c27")
				(number "c27")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 3.81)
				(name "Pin_c28")
				(number "c28")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 3.81)
				(name "Pin_c29")
				(number "c29")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 3.81)
				(name "Pin_c30")
				(number "c30")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 3.81)
				(name "Pin_c31")
				(number "c31")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 3.81)
				(name "Pin_c32")
				(number "c32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x32_AE"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 40.64 0)
		)
		(property "Value" "DIN41612_02x32_AE"
			(at 1.27 -43.18 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (AE), 02x32, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x32_AE_1_1"
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 3.81)
				(name "Pin_e1")
				(number "e1")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 3.81)
				(name "Pin_e2")
				(number "e2")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 3.81)
				(name "Pin_e3")
				(number "e3")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 3.81)
				(name "Pin_e4")
				(number "e4")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 3.81)
				(name "Pin_e5")
				(number "e5")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 3.81)
				(name "Pin_e6")
				(number "e6")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 3.81)
				(name "Pin_e7")
				(number "e7")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 3.81)
				(name "Pin_e8")
				(number "e8")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 3.81)
				(name "Pin_e9")
				(number "e9")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 3.81)
				(name "Pin_e10")
				(number "e10")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 3.81)
				(name "Pin_e11")
				(number "e11")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 3.81)
				(name "Pin_e12")
				(number "e12")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_e13")
				(number "e13")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_e14")
				(number "e14")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_e15")
				(number "e15")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_e16")
				(number "e16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_e17")
				(number "e17")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_e18")
				(number "e18")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_e19")
				(number "e19")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_e20")
				(number "e20")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 3.81)
				(name "Pin_e21")
				(number "e21")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 3.81)
				(name "Pin_e22")
				(number "e22")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 3.81)
				(name "Pin_e23")
				(number "e23")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 3.81)
				(name "Pin_e24")
				(number "e24")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 3.81)
				(name "Pin_e25")
				(number "e25")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 3.81)
				(name "Pin_e26")
				(number "e26")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 3.81)
				(name "Pin_e27")
				(number "e27")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 3.81)
				(name "Pin_e28")
				(number "e28")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 3.81)
				(name "Pin_e29")
				(number "e29")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 3.81)
				(name "Pin_e30")
				(number "e30")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 3.81)
				(name "Pin_e31")
				(number "e31")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 3.81)
				(name "Pin_e32")
				(number "e32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIN41612_02x32_ZB"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 40.64 0)
		)
		(property "Value" "DIN41612_02x32_ZB"
			(at 1.27 -43.18 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "DIN41612 connector, double row (ZB), 02x32, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIN41612*2x*"
			(at 0 0 0)
		)
		(symbol "DIN41612_02x32_ZB_1_1"
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_z1")
				(number "z1")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_z2")
				(number "z2")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_z3")
				(number "z3")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_z4")
				(number "z4")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_z5")
				(number "z5")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_z6")
				(number "z6")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_z7")
				(number "z7")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_z8")
				(number "z8")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_z9")
				(number "z9")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_z10")
				(number "z10")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_z11")
				(number "z11")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_z12")
				(number "z12")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_z13")
				(number "z13")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_z14")
				(number "z14")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_z15")
				(number "z15")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_z16")
				(number "z16")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_z17")
				(number "z17")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_z18")
				(number "z18")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_z19")
				(number "z19")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_z20")
				(number "z20")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_z21")
				(number "z21")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_z22")
				(number "z22")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_z23")
				(number "z23")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_z24")
				(number "z24")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_z25")
				(number "z25")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_z26")
				(number "z26")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_z27")
				(number "z27")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_z28")
				(number "z28")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_z29")
				(number "z29")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_z30")
				(number "z30")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_z31")
				(number "z31")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_z32")
				(number "z32")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 3.81)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 3.81)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 3.81)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 3.81)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 3.81)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 3.81)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 3.81)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 3.81)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 3.81)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 3.81)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 3.81)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 3.81)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 3.81)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 3.81)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 3.81)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 3.81)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 3.81)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 3.81)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 3.81)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 3.81)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 3.81)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 3.81)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 3.81)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 3.81)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 3.81)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 3.81)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 3.81)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 3.81)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 3.81)
				(name "Pin_b32")
				(number "b32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DVI-D_Dual_Link"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -6.35 29.21 0)
		)
		(property "Value" "DVI-D_Dual_Link"
			(at 10.16 29.21 0)
		)
		(property "Footprint" ""
			(at 0.635 2.54 0)
		)
		(property "Datasheet" "https://www.molex.com/content/dam/molex/molex-dot-com/products/automated/en-us/salesdrawingpdf/743/74320/743204004_sd.pdf?inline"
			(at 0 0 0)
		)
		(property "Description" "DVI-D dual link connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "dvi digital visual interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DVI-D*"
			(at 0 0 0)
		)
		(symbol "DVI-D_Dual_Link_0_0"
			(text "DVI-D"
				(at 2.54 20.32 0)
			)
			(text "Dual Link"
				(at 2.54 17.78 0)
			)
		)
		(symbol "DVI-D_Dual_Link_1_1"
			(text "8"
				(at -2.032 7.62 900)
			)
			(text "1"
				(at -2.032 -6.604 900)
			)
			(text "24"
				(at 7.62 7.62 900)
			)
			(text "17"
				(at 7.62 -6.604 900)
			)
			(pin passive line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "D2+")
				(number "2")
			)
			(pin passive line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "D2-")
				(number "1")
			)
			(pin passive line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "D1+")
				(number "10")
			)
			(pin passive line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "D1-")
				(number "9")
			)
			(pin passive line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D0+")
				(number "18")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D0-")
				(number "17")
			)
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D4+")
				(number "5")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D4-")
				(number "4")
			)
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D3+")
				(number "13")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "D3-")
				(number "12")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "D5+")
				(number "21")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "D5-")
				(number "20")
			)
			(pin passive clock
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CK+")
				(number "23")
			)
			(pin passive clock
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "CK-")
				(number "24")
			)
			(pin passive clock
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "DDCCL")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "DDCIO")
				(number "7")
			)
			(pin passive line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "HPD")
				(number "16")
			)
			(pin no_connect line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 2.54)
				(name "D2/4S")
				(number "3")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "D1/3S")
				(number "11")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "+5V")
				(number "14")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(name "D0/5S")
				(number "19")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "CKS")
				(number "22")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 7.62 -27.94 90)
				(length 2.54)
				(name "SH")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DVI-I_Dual_Link"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -7.62 36.83 0)
		)
		(property "Value" "DVI-I_Dual_Link"
			(at 7.62 36.83 0)
		)
		(property "Footprint" ""
			(at 0.635 10.16 0)
		)
		(property "Datasheet" "https://www.molex.com/content/dam/molex/molex-dot-com/products/automated/en-us/salesdrawingpdf/743/74320/743201004_sd.pdf?inline"
			(at 0 0 0)
		)
		(property "Description" "DVI-I dual link connector"
			(at 0 -2.54 0)
		)
		(property "ki_keywords" "dvi digital visual interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DVI-I*"
			(at 0 0 0)
		)
		(symbol "DVI-I_Dual_Link_0_0"
			(text "DVI-I"
				(at 2.54 27.94 0)
			)
			(text "Dual Link"
				(at 2.54 25.4 0)
			)
		)
		(symbol "DVI-I_Dual_Link_0_1")
		(symbol "DVI-I_Dual_Link_1_1"
			(text "C2"
				(at -2.032 20.32 900)
			)
			(text "C1"
				(at -2.032 18.288 900)
			)
			(text "8"
				(at -2.032 15.24 900)
			)
			(text "1"
				(at -2.032 1.016 900)
			)
			(text "C4"
				(at 7.62 20.32 900)
			)
			(text "C3"
				(at 7.62 18.288 900)
			)
			(text "24"
				(at 7.62 15.24 900)
			)
			(text "17"
				(at 7.62 1.016 900)
			)
			(pin passive line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "D2+")
				(number "2")
			)
			(pin passive line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "D2-")
				(number "1")
			)
			(pin passive line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "D1+")
				(number "10")
			)
			(pin passive line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "D1-")
				(number "9")
			)
			(pin passive line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "D0+")
				(number "18")
			)
			(pin passive line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "D0-")
				(number "17")
			)
			(pin passive line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "D4+")
				(number "5")
			)
			(pin passive line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D4-")
				(number "4")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D3+")
				(number "13")
			)
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D3-")
				(number "12")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D5+")
				(number "21")
			)
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D5-")
				(number "20")
			)
			(pin passive clock
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CK+")
				(number "23")
			)
			(pin passive clock
				(at -12.7 0 0)
				(length 2.54)
				(name "CK-")
				(number "24")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "Red")
				(number "C1")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "Green")
				(number "C2")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "Blue")
				(number "C3")
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "HSYNC")
				(number "C4")
			)
			(pin passive line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "VSYNC")
				(number "8")
			)
			(pin passive clock
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "DDCCL")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "DDCIO")
				(number "7")
			)
			(pin passive line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "HPD")
				(number "16")
			)
			(pin passive line
				(at -7.62 -38.1 90)
				(length 2.54)
				(name "D2/4S")
				(number "3")
			)
			(pin passive line
				(at -5.08 -38.1 90)
				(length 2.54)
				(name "D1/3S")
				(number "11")
			)
			(pin passive line
				(at -2.54 -38.1 90)
				(length 2.54)
				(name "D0/5S")
				(number "19")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "+5V")
				(number "14")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(name "CKS")
				(number "22")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at 5.08 -38.1 90)
				(length 2.54)
				(name "GNDA")
				(number "C5")
			)
			(pin passive line
				(at 7.62 -38.1 90)
				(length 2.54)
				(name "SH")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ExpressCard"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 11.43 36.83 0)
		)
		(property "Value" "ExpressCard"
			(at 7.62 -36.83 0)
		)
		(property "Footprint" ""
			(at 5.08 -53.34 0)
		)
		(property "Datasheet" "https://web.archive.org/web/20180809060653/http://www.usb.org/developers/expresscard/EC_specifications/ExpressCard_2_0_FINAL.pdf"
			(at 5.08 -53.34 0)
		)
		(property "Description" "ExpressCard connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "expresscard pci express"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ExpressCard*"
			(at 0 0 0)
		)
		(symbol "ExpressCard_0_0"
			(text "ExpressCard"
				(at -7.62 0 900)
			)
		)
		(symbol "ExpressCard_0_1")
		(symbol "ExpressCard_1_1"
			(pin power_out line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "3V3")
				(number "15")
			)
			(pin power_out line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "3V3")
				(number "14")
			)
			(pin power_out line
				(at 0 38.1 270)
				(length 2.54)
				(name "3V3_AUX")
				(number "12")
			)
			(pin power_out line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin power_out line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "1V5")
				(number "10")
			)
			(pin power_out line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "1V5")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "USBD+")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "USBD-")
				(number "2")
			)
			(pin output line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PETp0/SSTX+")
				(number "25")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PETn0/SSTX-")
				(number "24")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PERp0/SSRX+")
				(number "22")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PERn0/SSRX-")
				(number "21")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "REFCLK+")
				(number "19")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "REFCLK-")
				(number "18")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{CPPE}")
				(number "17")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{CLKREQ}")
				(number "16")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "~{PERST}")
				(number "13")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "~{WAKE}")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "~{USB3}")
				(number "5")
			)
			(pin input line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "~{CPUSB}")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "SMDDATA")
				(number "8")
			)
			(pin output line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "SMBCLK")
				(number "7")
			)
			(pin passive line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "RESERVED")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDMI_A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -6.35 26.67 0)
		)
		(property "Value" "HDMI_A"
			(at 10.16 26.67 0)
		)
		(property "Footprint" ""
			(at 0.635 0 0)
		)
		(property "Datasheet" "https://en.wikipedia.org/wiki/HDMI"
			(at 0.635 0 0)
		)
		(property "Description" "HDMI type A connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "hdmi conn"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDMI*A*"
			(at 0 0 0)
		)
		(symbol "HDMI_A_0_0")
		(symbol "HDMI_A_0_1")
		(symbol "HDMI_A_1_1"
			(pin passive line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "D2+")
				(number "1")
			)
			(pin passive line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "D2-")
				(number "3")
			)
			(pin passive line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "D1+")
				(number "4")
			)
			(pin passive line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "D1-")
				(number "6")
			)
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "D0+")
				(number "7")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "D0-")
				(number "9")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CK+")
				(number "10")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CK-")
				(number "12")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CEC")
				(number "13")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SCL")
				(number "15")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "SDA")
				(number "16")
			)
			(pin passive line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "UTILITY")
				(number "14")
			)
			(pin passive line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "HPD")
				(number "19")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 2.54)
				(name "D2S")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "D1S")
				(number "5")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "+5V")
				(number "18")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "D0S")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "CKS")
				(number "11")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 7.62 -27.94 90)
				(length 2.54)
				(name "SH")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDMI_A_1.4"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -6.35 26.67 0)
		)
		(property "Value" "HDMI_A_1.4"
			(at 10.16 26.67 0)
		)
		(property "Footprint" ""
			(at 0.635 0 0)
		)
		(property "Datasheet" "https://en.wikipedia.org/wiki/HDMI"
			(at 0.635 0 0)
		)
		(property "Description" "HDMI 1.4+ type A connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "hdmi conn"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDMI*A*"
			(at 0 0 0)
		)
		(symbol "HDMI_A_1.4_0_0")
		(symbol "HDMI_A_1.4_0_1")
		(symbol "HDMI_A_1.4_1_1"
			(pin passive line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "D2+")
				(number "1")
			)
			(pin passive line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "D2-")
				(number "3")
			)
			(pin passive line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "D1+")
				(number "4")
			)
			(pin passive line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "D1-")
				(number "6")
			)
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "D0+")
				(number "7")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "D0-")
				(number "9")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CK+")
				(number "10")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CK-")
				(number "12")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CEC")
				(number "13")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SCL")
				(number "15")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "SDA")
				(number "16")
			)
			(pin passive line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "UTILITY/HEAC+")
				(number "14")
			)
			(pin passive line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "HPD/HEAC-")
				(number "19")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 2.54)
				(name "D2S")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "D1S")
				(number "5")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "+5V")
				(number "18")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "D0S")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "CKS")
				(number "11")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 7.62 -27.94 90)
				(length 2.54)
				(name "SH")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDMI_B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -7.62 31.75 0)
		)
		(property "Value" "HDMI_B"
			(at 7.62 31.75 0)
		)
		(property "Footprint" ""
			(at 0.635 0 0)
		)
		(property "Datasheet" "http://pinouts.ru/Video/hdmi_pinout.shtml"
			(at 0.635 0 0)
		)
		(property "Description" "HDMI type B connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "hdmi conn"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDMI*B*"
			(at 0 0 0)
		)
		(symbol "HDMI_B_0_0")
		(symbol "HDMI_B_0_1")
		(symbol "HDMI_B_1_1"
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "D2+")
				(number "1")
			)
			(pin passive line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "D2-")
				(number "3")
			)
			(pin passive line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "D1+")
				(number "4")
			)
			(pin passive line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "D1-")
				(number "6")
			)
			(pin passive line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "D0+")
				(number "7")
			)
			(pin passive line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "D0-")
				(number "9")
			)
			(pin passive line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "CK+")
				(number "10")
			)
			(pin passive line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "CK-")
				(number "12")
			)
			(pin passive line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "D5+")
				(number "13")
			)
			(pin passive line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "D5-")
				(number "15")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "D4+")
				(number "16")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 2.54)
				(name "D4-")
				(number "18")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "D3+")
				(number "19")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "D3-")
				(number "21")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "CEC")
				(number "22")
			)
			(pin passive line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "SCL")
				(number "25")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "SDA")
				(number "26")
			)
			(pin passive line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "HPD")
				(number "29")
			)
			(pin no_connect line
				(at -12.7 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at -12.7 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin power_in line
				(at -10.16 -33.02 90)
				(length 2.54)
				(name "D2S")
				(number "2")
			)
			(pin power_in line
				(at -7.62 -33.02 90)
				(length 2.54)
				(name "D1S")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -33.02 90)
				(length 2.54)
				(name "D0S")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 2.54)
				(name "CKS")
				(number "11")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "+5V")
				(number "28")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "D5S")
				(number "14")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 2.54)
				(name "D4S")
				(number "17")
			)
			(pin power_in line
				(at 5.08 -33.02 90)
				(length 2.54)
				(name "D3S")
				(number "20")
			)
			(pin power_in line
				(at 7.62 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "27")
			)
			(pin passive line
				(at 10.16 -33.02 90)
				(length 2.54)
				(name "SH")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDMI_C_1.3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -6.35 26.67 0)
		)
		(property "Value" "HDMI_C_1.3"
			(at 10.16 26.67 0)
		)
		(property "Footprint" ""
			(at 0.635 0 0)
		)
		(property "Datasheet" "http://pinoutguide.com/PortableDevices/mini_hdmi_pinout.shtml"
			(at 0.635 0 0)
		)
		(property "Description" "HDMI 1.3+ type C connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "hdmi conn"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDMI*C*"
			(at 0 0 0)
		)
		(symbol "HDMI_C_1.3_0_0")
		(symbol "HDMI_C_1.3_0_1")
		(symbol "HDMI_C_1.3_1_1"
			(pin passive line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "D2+")
				(number "2")
			)
			(pin passive line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "D2-")
				(number "3")
			)
			(pin passive line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "D1+")
				(number "5")
			)
			(pin passive line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "D1-")
				(number "6")
			)
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "D0+")
				(number "8")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "D0-")
				(number "9")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CK+")
				(number "11")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CK-")
				(number "12")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CEC")
				(number "14")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SCL")
				(number "15")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "SDA")
				(number "16")
			)
			(pin passive line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "UTILITY")
				(number "17")
			)
			(pin passive line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "HPD")
				(number "19")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 2.54)
				(name "D2S")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "D1S")
				(number "4")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "+5V")
				(number "18")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "D0S")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "CKS")
				(number "10")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 7.62 -27.94 90)
				(length 2.54)
				(name "SH")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDMI_C_1.4"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -6.35 26.67 0)
		)
		(property "Value" "HDMI_C_1.4"
			(at 10.16 26.67 0)
		)
		(property "Footprint" ""
			(at 0.635 0 0)
		)
		(property "Datasheet" "http://pinoutguide.com/PortableDevices/mini_hdmi_pinout.shtml"
			(at 0.635 0 0)
		)
		(property "Description" "HDMI 1.4+ type C connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "hdmi conn"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDMI*C*"
			(at 0 0 0)
		)
		(symbol "HDMI_C_1.4_0_0")
		(symbol "HDMI_C_1.4_0_1")
		(symbol "HDMI_C_1.4_1_1"
			(pin passive line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "D2+")
				(number "2")
			)
			(pin passive line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "D2-")
				(number "3")
			)
			(pin passive line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "D1+")
				(number "5")
			)
			(pin passive line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "D1-")
				(number "6")
			)
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "D0+")
				(number "8")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "D0-")
				(number "9")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CK+")
				(number "11")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CK-")
				(number "12")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CEC")
				(number "14")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SCL")
				(number "15")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "SDA")
				(number "16")
			)
			(pin passive line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "UTILITY/HEAC+")
				(number "17")
			)
			(pin passive line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "HPD/HEAC-")
				(number "19")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 2.54)
				(name "D2S")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "D1S")
				(number "4")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "+5V")
				(number "18")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "D0S")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "CKS")
				(number "10")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 7.62 -27.94 90)
				(length 2.54)
				(name "SH")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDMI_D_1.4"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -6.35 26.67 0)
		)
		(property "Value" "HDMI_D_1.4"
			(at 10.16 26.67 0)
		)
		(property "Footprint" ""
			(at 0.635 0 0)
		)
		(property "Datasheet" "http://pinoutguide.com/PortableDevices/micro_hdmi_type_d_pinout.shtml"
			(at 0.635 0 0)
		)
		(property "Description" "HDMI 1.4+ type D connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "hdmi conn"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDMI*D*"
			(at 0 0 0)
		)
		(symbol "HDMI_D_1.4_0_0")
		(symbol "HDMI_D_1.4_0_1")
		(symbol "HDMI_D_1.4_1_1"
			(pin passive line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "D2+")
				(number "3")
			)
			(pin passive line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "D2-")
				(number "5")
			)
			(pin passive line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "D1+")
				(number "6")
			)
			(pin passive line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "D1-")
				(number "8")
			)
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "D0+")
				(number "9")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "D0-")
				(number "11")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CK+")
				(number "12")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CK-")
				(number "14")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CEC")
				(number "15")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SCL")
				(number "17")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "SDA")
				(number "18")
			)
			(pin passive line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "UTILITY/HEAC+")
				(number "2")
			)
			(pin passive line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "HPD/HEAC-")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 2.54)
				(name "D2S")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "D1S")
				(number "7")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "+5V")
				(number "19")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "D0S")
				(number "10")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "CKS")
				(number "13")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 7.62 -27.94 90)
				(length 2.54)
				(name "SH")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDMI_E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -6.35 26.67 0)
		)
		(property "Value" "HDMI_E"
			(at 10.16 26.67 0)
		)
		(property "Footprint" ""
			(at 0.635 0 0)
		)
		(property "Datasheet" "https://www.hdmi.org/manufacturer/specification.aspx"
			(at 0.635 0 0)
		)
		(property "Description" "HDMI type E connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "hdmi conn"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDMI*E*"
			(at 0 0 0)
		)
		(symbol "HDMI_E_0_0")
		(symbol "HDMI_E_0_1")
		(symbol "HDMI_E_1_1"
			(pin passive line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "D2+")
				(number "1")
			)
			(pin passive line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "D2-")
				(number "3")
			)
			(pin passive line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "D1+")
				(number "4")
			)
			(pin passive line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "D1-")
				(number "6")
			)
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "D0+")
				(number "7")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "D0-")
				(number "9")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CK+")
				(number "10")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CK-")
				(number "12")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CEC")
				(number "13")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SCL")
				(number "15")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "SDA")
				(number "16")
			)
			(pin passive line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "UTILITY")
				(number "14")
			)
			(pin passive line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "HPD")
				(number "19")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 2.54)
				(name "D2S")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "D1S")
				(number "5")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "+5V")
				(number "18")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "D0S")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "CKS")
				(number "11")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 7.62 -27.94 90)
				(length 2.54)
				(name "SH")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IEC61076-2_M8_A-coding_01x03_Plug_Shielded"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 7.62 0)
		)
		(property "Value" "IEC61076-2_M8_A-coding_01x03_Plug_Shielded"
			(at 0 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "IEC 61076-2 3 ways shielded M8 A-coding plug connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "M8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*M8*03*"
			(at 0 0 0)
		)
		(symbol "IEC61076-2_M8_A-coding_01x03_Plug_Shielded_0_1")
		(symbol "IEC61076-2_M8_A-coding_01x03_Plug_Shielded_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 3.81)
				(name "~")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IEC61076-2_M8_A-coding_01x03_Receptacle_Shielded"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 7.62 0)
		)
		(property "Value" "IEC61076-2_M8_A-coding_01x03_Receptacle_Shielded"
			(at 0 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "IEC 61076-2 3 ways shielded M8 A-coding receptacle connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "M8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*M8*03*"
			(at 0 0 0)
		)
		(symbol "IEC61076-2_M8_A-coding_01x03_Receptacle_Shielded_0_1")
		(symbol "IEC61076-2_M8_A-coding_01x03_Receptacle_Shielded_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 3.81)
				(name "~")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IEC61076-2_M8_A-coding_01x04_Plug_Shielded"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 7.62 0)
		)
		(property "Value" "IEC61076-2_M8_A-coding_01x04_Plug_Shielded"
			(at 0 -7.62 0)
		)
		(property "Footprint" ""
			(at -0.762 0 0)
		)
		(property "Datasheet" ""
			(at -0.762 0 0)
		)
		(property "Description" "IEC 61076-2 4 ways shielded M8 A-coding plug connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "M8 connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*M8*04*"
			(at 0 0 0)
		)
		(symbol "IEC61076-2_M8_A-coding_01x04_Plug_Shielded_0_1")
		(symbol "IEC61076-2_M8_A-coding_01x04_Plug_Shielded_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 3.81)
				(name "~")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IEC61076-2_M8_A-coding_01x04_Receptacle_Shielded"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 7.62 0)
		)
		(property "Value" "IEC61076-2_M8_A-coding_01x04_Receptacle_Shielded"
			(at 0 -7.874 0)
		)
		(property "Footprint" ""
			(at -0.762 0 0)
		)
		(property "Datasheet" ""
			(at -0.762 0 0)
		)
		(property "Description" "IEC 61076-2 4 ways shielded M8 A-coding receptacle connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "M8 connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*M8*04*"
			(at 0 0 0)
		)
		(symbol "IEC61076-2_M8_A-coding_01x04_Receptacle_Shielded_0_1")
		(symbol "IEC61076-2_M8_A-coding_01x04_Receptacle_Shielded_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 3.81)
				(name "~")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IEC_60320_C13_Plug"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at -5.842 8.636 0)
		)
		(property "Value" "IEC_60320_C13_Plug"
			(at 0.508 -9.144 0)
		)
		(property "Footprint" ""
			(at -4.064 -1.016 0)
		)
		(property "Datasheet" "~"
			(at -4.064 -1.016 0)
		)
		(property "Description" "C13 Plug, 10A max"
			(at -2.159 -1.016 0)
		)
		(property "ki_keywords" "Receptacle C13 IEC320"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "C*13*Plug*"
			(at 0 0 0)
		)
		(symbol "IEC_60320_C13_Plug_1_1"
			(pin power_in line
				(at 8.89 5.08 180)
				(length 2.54)
				(name "L")
				(number "2")
			)
			(pin bidirectional line
				(at 8.89 0 180)
				(length 2.54)
				(name "PE")
				(number "3")
			)
			(pin power_in line
				(at 8.89 -5.08 180)
				(length 2.54)
				(name "N")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IEC_60320_C14_Receptacle"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.842 8.636 0)
		)
		(property "Value" "IEC_60320_C14_Receptacle"
			(at 0 -9.144 0)
		)
		(property "Footprint" ""
			(at -2.286 0 0)
		)
		(property "Datasheet" "~"
			(at -2.286 0 0)
		)
		(property "Description" "C14 Plug, 10A max"
			(at -0.635 0 0)
		)
		(property "ki_keywords" "Plug C14 IEC320"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "C*14*Receptacle*"
			(at 0 0 0)
		)
		(symbol "IEC_60320_C14_Receptacle_1_1"
			(pin power_in line
				(at 8.89 5.08 180)
				(length 2.54)
				(name "L")
				(number "1")
			)
			(pin bidirectional line
				(at 8.89 0 180)
				(length 2.54)
				(name "PE")
				(number "3")
			)
			(pin power_in line
				(at 8.89 -5.08 180)
				(length 2.54)
				(name "N")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IEC_60320_C5_Plug"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at -5.842 8.636 0)
		)
		(property "Value" "IEC_60320_C5_Plug"
			(at 0.254 -9.144 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "C5 Receptacle, 2,5 A max"
			(at 0 0 0)
		)
		(property "ki_keywords" "C5 IEC 60320"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "C*5*Plug*"
			(at 0 0 0)
		)
		(symbol "IEC_60320_C5_Plug_0_1")
		(symbol "IEC_60320_C5_Plug_1_1"
			(pin power_in line
				(at 8.89 5.08 180)
				(length 2.54)
				(name "L")
				(number "2")
			)
			(pin bidirectional line
				(at 8.89 0 180)
				(length 2.54)
				(name "PE")
				(number "3")
			)
			(pin power_in line
				(at 8.89 -5.08 180)
				(length 2.54)
				(name "N")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IEC_60320_C6_Receptacle"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.842 8.636 0)
		)
		(property "Value" "IEC_60320_C6_Receptacle"
			(at 0.508 -9.144 0)
		)
		(property "Footprint" ""
			(at -1.8538 -0.0376 0)
		)
		(property "Datasheet" "~"
			(at -1.8538 -0.0376 0)
		)
		(property "Description" "C6 plug, 2,5A max"
			(at 0 0 0)
		)
		(property "ki_keywords" "IEC 60320 C6"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "C*6*Receptacle*"
			(at 0 0 0)
		)
		(symbol "IEC_60320_C6_Receptacle_0_1")
		(symbol "IEC_60320_C6_Receptacle_1_1"
			(pin power_in line
				(at 8.89 5.08 180)
				(length 2.54)
				(name "L")
				(number "1")
			)
			(pin bidirectional line
				(at 8.89 0 180)
				(length 2.54)
				(name "PE")
				(number "3")
			)
			(pin power_in line
				(at 8.89 -5.08 180)
				(length 2.54)
				(name "N")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IEC_60320_C7_Plug"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at -5.842 8.636 0)
		)
		(property "Value" "IEC_60320_C7_Plug"
			(at 0 -9.144 0)
		)
		(property "Footprint" ""
			(at -15.748 5.334 0)
		)
		(property "Datasheet" "~"
			(at -15.748 5.334 0)
		)
		(property "Description" "C7 coupler, 2,5 A max"
			(at -15.748 5.334 0)
		)
		(property "ki_keywords" "C7 Plug  IEC 60320"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "C*7*Plug*"
			(at 0 0 0)
		)
		(symbol "IEC_60320_C7_Plug_0_1")
		(symbol "IEC_60320_C7_Plug_1_1"
			(pin power_in line
				(at 8.89 5.08 180)
				(length 2.54)
				(name "L")
				(number "2")
			)
			(pin power_in line
				(at 8.89 -5.08 180)
				(length 2.54)
				(name "N")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IEC_60320_C8_Receptacle"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.842 8.636 0)
		)
		(property "Value" "IEC_60320_C8_Receptacle"
			(at 0.254 -9.144 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "C8 coupler, 2,5 A max"
			(at 0 0 0)
		)
		(property "ki_keywords" "C8 Receptacle  IEC 60320"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "C*8*Receptacle*"
			(at 0 0 0)
		)
		(symbol "IEC_60320_C8_Receptacle_0_1")
		(symbol "IEC_60320_C8_Receptacle_1_1"
			(pin power_in line
				(at 8.89 5.08 180)
				(length 2.54)
				(name "L")
				(number "1")
			)
			(pin power_in line
				(at 8.89 -5.08 180)
				(length 2.54)
				(name "N")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IEEE1394a"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 12.7 0)
		)
		(property "Value" "IEEE1394a"
			(at 0 10.16 0)
		)
		(property "Footprint" ""
			(at 0 1.27 0)
		)
		(property "Datasheet" "~"
			(at 0 1.27 0)
		)
		(property "Description" "FireWire/IEEE1394a 6-pin connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector IEEE1394a FireWire"
			(at 0 0 0)
		)
		(symbol "IEEE1394a_0_1")
		(symbol "IEEE1394a_1_1"
			(pin power_in line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "PWR")
				(number "1")
			)
			(pin bidirectional line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "TPA+")
				(number "6")
			)
			(pin bidirectional line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "TPA-")
				(number "5")
			)
			(pin bidirectional line
				(at -7.62 0 0)
				(length 2.54)
				(name "TPB+")
				(number "4")
			)
			(pin bidirectional line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "TPB-")
				(number "3")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "SH")
				(number "7")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "SH")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "JAE_SIM_Card_SF72S006"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 5.08 12.7 0)
		)
		(property "Value" "JAE_SIM_Card_SF72S006"
			(at 30.48 12.7 0)
		)
		(property "Footprint" "Connector_JAE:JAE_SIM_Card_SF72S006"
			(at 11.43 -13.97 0)
		)
		(property "Datasheet" "https://www.jae.com/direct/topics/topics_file_download/topics_id=68892&ext_no=06&index=0&_lang=en&v=202003111511468456809"
			(at 13.97 0 0)
		)
		(property "Description" "Nano-SIM Card (4FF) connector with Detect Switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "SIM card UICC 4FF"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "JAE*SIM*Card*SF72S006*"
			(at 0 0 0)
		)
		(symbol "JAE_SIM_Card_SF72S006_0_1")
		(symbol "JAE_SIM_Card_SF72S006_1_1"
			(pin power_in line
				(at 0 10.16 0)
				(length 3.81)
				(name "VCC")
				(number "C1")
			)
			(pin input line
				(at 0 7.62 0)
				(length 3.81)
				(name "RST")
				(number "C2")
			)
			(pin input line
				(at 0 5.08 0)
				(length 3.81)
				(name "CLK")
				(number "C3")
			)
			(pin power_in line
				(at 0 2.54 0)
				(length 3.81)
				(name "GND")
				(number "C5")
			)
			(pin bidirectional line
				(at 0 0 0)
				(length 3.81)
				(name "VPP/SWP")
				(number "C6")
			)
			(pin bidirectional line
				(at 0 -2.54 0)
				(length 3.81)
				(name "I/O")
				(number "C7")
			)
			(pin passive line
				(at 0 -5.08 0)
				(length 3.81)
				(name "DSW")
				(number "DSW")
			)
			(pin passive line
				(at 0 -7.62 0)
				(length 3.81)
				(name "CSW")
				(number "CSW")
			)
			(pin passive line
				(at 0 -10.16 0)
				(length 3.81)
				(name "SH")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LEMO2"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 6.35 0)
		)
		(property "Value" "LEMO2"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 1.27 0)
		)
		(property "Datasheet" "~"
			(at 0 1.27 0)
		)
		(property "Description" "2-pin LEMO connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "LEMO connector"
			(at 0 0 0)
		)
		(symbol "LEMO2_0_1")
		(symbol "LEMO2_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LEMO4"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 7.62 0)
		)
		(property "Value" "LEMO4"
			(at 0 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "4-pin LEMO connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "LEMO connector"
			(at 0 0 0)
		)
		(symbol "LEMO4_0_1")
		(symbol "LEMO4_1_1"
			(pin passive line
				(at -7.62 3.81 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 -3.81 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 3.81 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 -3.81 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LEMO5"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 5.08 7.62 0)
		)
		(property "Value" "LEMO5"
			(at 7.62 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "5-pin LEMO connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "LEMO connector"
			(at 0 0 0)
		)
		(symbol "LEMO5_0_1")
		(symbol "LEMO5_1_1"
			(pin passive line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LEMO6"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 8.255 9.525 0)
		)
		(property "Value" "LEMO6"
			(at 8.255 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "6-pin LEMO connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "LEMO connector"
			(at 0 0 0)
		)
		(symbol "LEMO6_0_1")
		(symbol "LEMO6_1_1"
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MXM3.0"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 2.54 0)
		)
		(property "Value" "MXM3.0"
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at 1.27 135.89 0)
		)
		(property "Datasheet" "~"
			(at 1.27 135.89 0)
		)
		(property "Description" "MXM3.0 connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "MXM connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MM70*"
			(at 0 0 0)
		)
		(symbol "MXM3.0_1_1"
			(pin output line
				(at -17.78 129.54 0)
				(length 3.81)
				(name "PEX_RX0#")
				(number "147")
			)
			(pin output line
				(at -17.78 127 0)
				(length 3.81)
				(name "PEX_RX0")
				(number "149")
			)
			(pin output line
				(at -17.78 124.46 0)
				(length 3.81)
				(name "PEX_RX1#")
				(number "141")
			)
			(pin output line
				(at -17.78 121.92 0)
				(length 3.81)
				(name "PEX_RX1")
				(number "143")
			)
			(pin output line
				(at -17.78 119.38 0)
				(length 3.81)
				(name "PEX_RX2#")
				(number "135")
			)
			(pin output line
				(at -17.78 116.84 0)
				(length 3.81)
				(name "PEX_RX2")
				(number "137")
			)
			(pin output line
				(at -17.78 114.3 0)
				(length 3.81)
				(name "PEX_RX3#")
				(number "121")
			)
			(pin output line
				(at -17.78 111.76 0)
				(length 3.81)
				(name "PEX_RX3")
				(number "123")
			)
			(pin output line
				(at -17.78 109.22 0)
				(length 3.81)
				(name "PEX_RX4#")
				(number "115")
			)
			(pin output line
				(at -17.78 106.68 0)
				(length 3.81)
				(name "PEX_RX4")
				(number "117")
			)
			(pin output line
				(at -17.78 104.14 0)
				(length 3.81)
				(name "PEX_RX5#")
				(number "109")
			)
			(pin output line
				(at -17.78 101.6 0)
				(length 3.81)
				(name "PEX_RX5")
				(number "111")
			)
			(pin output line
				(at -17.78 99.06 0)
				(length 3.81)
				(name "PEX_RX6#")
				(number "103")
			)
			(pin output line
				(at -17.78 96.52 0)
				(length 3.81)
				(name "PEX_RX6")
				(number "105")
			)
			(pin output line
				(at -17.78 93.98 0)
				(length 3.81)
				(name "PEX_RX7#")
				(number "97")
			)
			(pin output line
				(at -17.78 91.44 0)
				(length 3.81)
				(name "PEX_RX7")
				(number "99")
			)
			(pin output line
				(at -17.78 88.9 0)
				(length 3.81)
				(name "PEX_RX8#")
				(number "91")
			)
			(pin output line
				(at -17.78 86.36 0)
				(length 3.81)
				(name "PEX_RX8")
				(number "93")
			)
			(pin output line
				(at -17.78 83.82 0)
				(length 3.81)
				(name "PEX_RX9#")
				(number "85")
			)
			(pin output line
				(at -17.78 81.28 0)
				(length 3.81)
				(name "PEX_RX9")
				(number "87")
			)
			(pin output line
				(at -17.78 78.74 0)
				(length 3.81)
				(name "PEX_RX10#")
				(number "79")
			)
			(pin output line
				(at -17.78 76.2 0)
				(length 3.81)
				(name "PEX_RX10")
				(number "81")
			)
			(pin output line
				(at -17.78 73.66 0)
				(length 3.81)
				(name "PEX_RX11#")
				(number "73")
			)
			(pin output line
				(at -17.78 71.12 0)
				(length 3.81)
				(name "PEX_RX11")
				(number "75")
			)
			(pin output line
				(at -17.78 68.58 0)
				(length 3.81)
				(name "PEX_RX12#")
				(number "67")
			)
			(pin output line
				(at -17.78 66.04 0)
				(length 3.81)
				(name "PEX_RX12")
				(number "69")
			)
			(pin output line
				(at -17.78 63.5 0)
				(length 3.81)
				(name "PEX_RX13#")
				(number "61")
			)
			(pin output line
				(at -17.78 60.96 0)
				(length 3.81)
				(name "PEX_RX13")
				(number "63")
			)
			(pin output line
				(at -17.78 58.42 0)
				(length 3.81)
				(name "PEX_RX14#")
				(number "55")
			)
			(pin output line
				(at -17.78 55.88 0)
				(length 3.81)
				(name "PEX_RX14")
				(number "57")
			)
			(pin output line
				(at -17.78 53.34 0)
				(length 3.81)
				(name "PEX_RX15#")
				(number "49")
			)
			(pin output line
				(at -17.78 50.8 0)
				(length 3.81)
				(name "PEX_RX15")
				(number "51")
			)
			(pin input line
				(at -17.78 48.26 0)
				(length 3.81)
				(name "PEX_TX0#")
				(number "148")
			)
			(pin input line
				(at -17.78 45.72 0)
				(length 3.81)
				(name "PEX_TX0")
				(number "150")
			)
			(pin input line
				(at -17.78 43.18 0)
				(length 3.81)
				(name "PEX_TX1#")
				(number "142")
			)
			(pin input line
				(at -17.78 40.64 0)
				(length 3.81)
				(name "PEX_TX1")
				(number "144")
			)
			(pin input line
				(at -17.78 38.1 0)
				(length 3.81)
				(name "PEX_TX2#")
				(number "136")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 3.81)
				(name "PEX_TX2")
				(number "138")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 3.81)
				(name "PEX_TX3#")
				(number "120")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 3.81)
				(name "PEX_TX3")
				(number "122")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 3.81)
				(name "PEX_TX4#")
				(number "114")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 3.81)
				(name "PEX_TX4")
				(number "116")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 3.81)
				(name "PEX_TX5#")
				(number "108")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "PEX_TX5")
				(number "110")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "PEX_TX6#")
				(number "102")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "PEX_TX6")
				(number "104")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "PEX_TX7#")
				(number "96")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "PEX_TX7")
				(number "98")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "PEX_TX8#")
				(number "90")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "PEX_TX8")
				(number "92")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "PEX_TX9#")
				(number "84")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "PEX_TX9")
				(number "86")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "PEX_TX10#")
				(number "78")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "PEX_TX10")
				(number "80")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "PEX_TX11#")
				(number "72")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "PEX_TX11")
				(number "74")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "PEX_TX12#")
				(number "66")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "PEX_TX12")
				(number "68")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "PEX_TX13#")
				(number "60")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "PEX_TX13")
				(number "62")
			)
			(pin input line
				(at -17.78 -22.86 0)
				(length 3.81)
				(name "PEX_TX14#")
				(number "54")
			)
			(pin input line
				(at -17.78 -25.4 0)
				(length 3.81)
				(name "PEX_TX14")
				(number "56")
			)
			(pin input line
				(at -17.78 -27.94 0)
				(length 3.81)
				(name "PEX_TX15#")
				(number "48")
			)
			(pin input line
				(at -17.78 -30.48 0)
				(length 3.81)
				(name "PEX_TX15")
				(number "50")
			)
			(pin input line
				(at -17.78 -33.02 0)
				(length 3.81)
				(name "PEX_REFCLK#")
				(number "153")
			)
			(pin input line
				(at -17.78 -35.56 0)
				(length 3.81)
				(name "PEX_REFCLK")
				(number "155")
			)
			(pin input line
				(at -17.78 -38.1 0)
				(length 3.81)
				(name "PEX_STD_SW#")
				(number "19")
			)
			(pin output line
				(at -17.78 -40.64 0)
				(length 3.81)
				(name "PEX_CLK_REQ#")
				(number "154")
			)
			(pin input line
				(at -17.78 -43.18 0)
				(length 3.81)
				(name "PEX_RST#")
				(number "156")
			)
			(pin input line
				(at -17.78 -48.26 0)
				(length 3.81)
				(name "DVI_HPD")
				(number "31")
			)
			(pin output line
				(at -17.78 -50.8 0)
				(length 3.81)
				(name "LVDS_UCLK#")
				(number "169")
			)
			(pin output line
				(at -17.78 -53.34 0)
				(length 3.81)
				(name "LVDS_UCLK")
				(number "171")
			)
			(pin output line
				(at -17.78 -55.88 0)
				(length 3.81)
				(name "LVDS_UTX3#")
				(number "175")
			)
			(pin output line
				(at -17.78 -58.42 0)
				(length 3.81)
				(name "LVDS_UTX3")
				(number "177")
			)
			(pin output line
				(at -17.78 -60.96 0)
				(length 3.81)
				(name "LVDS_UTX2#")
				(number "181")
			)
			(pin output line
				(at -17.78 -63.5 0)
				(length 3.81)
				(name "LVDS_UTX2")
				(number "183")
			)
			(pin output line
				(at -17.78 -66.04 0)
				(length 3.81)
				(name "LVDS_UTX1#")
				(number "187")
			)
			(pin output line
				(at -17.78 -68.58 0)
				(length 3.81)
				(name "LVDS_UTX1")
				(number "189")
			)
			(pin output line
				(at -17.78 -71.12 0)
				(length 3.81)
				(name "LVDS_UTX0#")
				(number "193")
			)
			(pin output line
				(at -17.78 -73.66 0)
				(length 3.81)
				(name "LVDS_UTX0")
				(number "195")
			)
			(pin bidirectional line
				(at -17.78 -76.2 0)
				(length 3.81)
				(name "LVDS_DDC_DAT")
				(number "33")
			)
			(pin output line
				(at -17.78 -78.74 0)
				(length 3.81)
				(name "LVDS_DDC_CLK")
				(number "35")
			)
			(pin output line
				(at -17.78 -81.28 0)
				(length 3.81)
				(name "LVDS_LCLK#")
				(number "176")
			)
			(pin output line
				(at -17.78 -83.82 0)
				(length 3.81)
				(name "LVDS_LCLK")
				(number "178")
			)
			(pin output line
				(at -17.78 -86.36 0)
				(length 3.81)
				(name "LVDS_LTX3#")
				(number "182")
			)
			(pin output line
				(at -17.78 -88.9 0)
				(length 3.81)
				(name "LVDS_LTX3")
				(number "184")
			)
			(pin output line
				(at -17.78 -91.44 0)
				(length 3.81)
				(name "LVDS_LTX2#")
				(number "188")
			)
			(pin output line
				(at -17.78 -93.98 0)
				(length 3.81)
				(name "LVDS_LTX2")
				(number "190")
			)
			(pin output line
				(at -17.78 -96.52 0)
				(length 3.81)
				(name "LVDS_LTX1#")
				(number "194")
			)
			(pin output line
				(at -17.78 -99.06 0)
				(length 3.81)
				(name "LVDS_LTX1")
				(number "196")
			)
			(pin output line
				(at -17.78 -101.6 0)
				(length 3.81)
				(name "LVDS_LTX0#")
				(number "200")
			)
			(pin output line
				(at -17.78 -104.14 0)
				(length 3.81)
				(name "LVDS_LTX0")
				(number "202")
			)
			(pin bidirectional line
				(at -17.78 -109.22 0)
				(length 3.81)
				(name "SMB_DAT")
				(number "32")
			)
			(pin input line
				(at -17.78 -111.76 0)
				(length 3.81)
				(name "SMB_CLK")
				(number "34")
			)
			(pin output line
				(at -17.78 -114.3 0)
				(length 3.81)
				(name "TH_OVERT#")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -116.84 0)
				(length 3.81)
				(name "TH_ALERT#")
				(number "22")
			)
			(pin output line
				(at -17.78 -119.38 0)
				(length 3.81)
				(name "TH_PWM")
				(number "24")
			)
			(pin input line
				(at -17.78 -121.92 0)
				(length 3.81)
				(name "PWR_LEVEL")
				(number "18")
			)
			(pin output line
				(at -17.78 -124.46 0)
				(length 3.81)
				(name "PWR_GOOD")
				(number "6")
			)
			(pin input line
				(at -17.78 -127 0)
				(length 3.81)
				(name "PWR_EN")
				(number "8")
			)
			(pin power_in line
				(at -2.54 137.16 270)
				(length 3.81)
				(name "5V")
				(number "1")
			)
			(pin passive line
				(at -2.54 137.16 270)
				(length 3.81)
				(hide yes)
				(name "5V")
				(number "3")
			)
			(pin passive line
				(at -2.54 137.16 270)
				(length 3.81)
				(hide yes)
				(name "5V")
				(number "5")
			)
			(pin passive line
				(at -2.54 137.16 270)
				(length 3.81)
				(hide yes)
				(name "5V")
				(number "7")
			)
			(pin passive line
				(at -2.54 137.16 270)
				(length 3.81)
				(hide yes)
				(name "5V")
				(number "9")
			)
			(pin power_in line
				(at 0 137.16 270)
				(length 3.81)
				(name "PWR_SRC")
				(number "E1")
			)
			(pin passive line
				(at 0 137.16 270)
				(length 3.81)
				(hide yes)
				(name "PWR_SRC")
				(number "E2")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "100")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "101")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "106")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "107")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "112")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "113")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "118")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "119")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "124")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "125")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "133")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "134")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "139")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "140")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "145")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "146")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "151")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "152")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "157")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "166")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "173")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "174")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "179")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "180")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "185")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "186")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "191")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "192")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "197")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "198")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "203")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "204")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "209")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "210")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "215")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "216")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "221")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "222")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "228")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "244")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "250")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "251")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "256")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "257")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "262")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "263")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "268")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "269")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "275")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "36")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "37")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "46")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "47")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "52")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "58")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "59")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "64")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "70")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "71")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "76")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "77")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "82")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "83")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "88")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "89")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "94")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "95")
			)
			(pin power_in line
				(at 0 -137.16 90)
				(length 3.81)
				(name "GND")
				(number "E3")
			)
			(pin passive line
				(at 0 -137.16 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E4")
			)
			(pin power_in line
				(at 2.54 137.16 270)
				(length 3.81)
				(name "3V3")
				(number "278")
			)
			(pin passive line
				(at 2.54 137.16 270)
				(length 3.81)
				(hide yes)
				(name "3V3")
				(number "280")
			)
			(pin output line
				(at 17.78 129.54 180)
				(length 3.81)
				(name "VGA_RED")
				(number "168")
			)
			(pin output line
				(at 17.78 127 180)
				(length 3.81)
				(name "VGA_GREEN")
				(number "170")
			)
			(pin output line
				(at 17.78 124.46 180)
				(length 3.81)
				(name "VGA_BLUE")
				(number "172")
			)
			(pin output line
				(at 17.78 121.92 180)
				(length 3.81)
				(name "VGA_VSYNC")
				(number "162")
			)
			(pin output line
				(at 17.78 119.38 180)
				(length 3.81)
				(name "VGA_HSYNC")
				(number "164")
			)
			(pin output line
				(at 17.78 116.84 180)
				(length 3.81)
				(name "VGA_DDC_CLK")
				(number "160")
			)
			(pin bidirectional line
				(at 17.78 114.3 180)
				(length 3.81)
				(name "VGA_DDC_DAT")
				(number "158")
			)
			(pin input line
				(at 17.78 109.22 180)
				(length 3.81)
				(name "VGA_DISABLE#")
				(number "21")
			)
			(pin output line
				(at 17.78 106.68 180)
				(length 3.81)
				(name "PNL_PWR_EN")
				(number "23")
			)
			(pin output line
				(at 17.78 104.14 180)
				(length 3.81)
				(name "PNL_BL_EN")
				(number "25")
			)
			(pin output line
				(at 17.78 101.6 180)
				(length 3.81)
				(name "PNL_BL_PWM")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 99.06 180)
				(length 3.81)
				(name "HDMI_CEC")
				(number "29")
			)
			(pin output line
				(at 17.78 96.52 180)
				(length 3.81)
				(name "WAKE#")
				(number "4")
			)
			(pin output line
				(at 17.78 93.98 180)
				(length 3.81)
				(name "PRSNT_L#")
				(number "281")
			)
			(pin output line
				(at 17.78 91.44 180)
				(length 3.81)
				(name "PRSNT_R#")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 88.9 180)
				(length 3.81)
				(name "GPIO0")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 86.36 180)
				(length 3.81)
				(name "GPIO1")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 83.82 180)
				(length 3.81)
				(name "GPIO2")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 81.28 180)
				(length 3.81)
				(name "RSVD")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 78.74 180)
				(length 3.81)
				(name "RSVD")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 76.2 180)
				(length 3.81)
				(name "RSVD")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 73.66 180)
				(length 3.81)
				(name "RSVD")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 71.12 180)
				(length 3.81)
				(name "RSVD")
				(number "159")
			)
			(pin bidirectional line
				(at 17.78 68.58 180)
				(length 3.81)
				(name "RSVD")
				(number "161")
			)
			(pin bidirectional line
				(at 17.78 66.04 180)
				(length 3.81)
				(name "RSVD")
				(number "163")
			)
			(pin bidirectional line
				(at 17.78 63.5 180)
				(length 3.81)
				(name "RSVD")
				(number "165")
			)
			(pin bidirectional line
				(at 17.78 60.96 180)
				(length 3.81)
				(name "RSVD")
				(number "167")
			)
			(pin bidirectional line
				(at 17.78 58.42 180)
				(length 3.81)
				(name "RSVD")
				(number "227")
			)
			(pin bidirectional line
				(at 17.78 55.88 180)
				(length 3.81)
				(name "RSVD")
				(number "229")
			)
			(pin bidirectional line
				(at 17.78 53.34 180)
				(length 3.81)
				(name "RSVD")
				(number "231")
			)
			(pin bidirectional line
				(at 17.78 50.8 180)
				(length 3.81)
				(name "RSVD")
				(number "233")
			)
			(pin bidirectional line
				(at 17.78 48.26 180)
				(length 3.81)
				(name "RSVD")
				(number "235")
			)
			(pin bidirectional line
				(at 17.78 45.72 180)
				(length 3.81)
				(name "RSVD")
				(number "237")
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 3.81)
				(name "RSVD")
				(number "238")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 3.81)
				(name "RSVD")
				(number "239")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 3.81)
				(name "RSVD")
				(number "240")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 3.81)
				(name "RSVD")
				(number "241")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 3.81)
				(name "RSVD")
				(number "242")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "RSVD")
				(number "243")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 3.81)
				(name "RSVD")
				(number "245")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "RSVD")
				(number "247")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "RSVD")
				(number "249")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "OEM")
				(number "38")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "OEM")
				(number "39")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "OEM")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "OEM")
				(number "41")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "OEM")
				(number "42")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "OEM")
				(number "43")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "OEM")
				(number "44")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "OEM")
				(number "45")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "DP_A_L0#")
				(number "253")
			)
			(pin output line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "DP_A_L0")
				(number "255")
			)
			(pin output line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "DP_A_L1#")
				(number "259")
			)
			(pin output line
				(at 17.78 -27.94 180)
				(length 3.81)
				(name "DP_A_L1")
				(number "261")
			)
			(pin output line
				(at 17.78 -30.48 180)
				(length 3.81)
				(name "DP_A_L2#")
				(number "265")
			)
			(pin output line
				(at 17.78 -33.02 180)
				(length 3.81)
				(name "DP_A_L2")
				(number "267")
			)
			(pin output line
				(at 17.78 -35.56 180)
				(length 3.81)
				(name "DP_A_L3#")
				(number "271")
			)
			(pin output line
				(at 17.78 -38.1 180)
				(length 3.81)
				(name "DP_A_L3")
				(number "273")
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 3.81)
				(name "DP_A_AUX#")
				(number "277")
			)
			(pin bidirectional line
				(at 17.78 -43.18 180)
				(length 3.81)
				(name "DP_A_AUX")
				(number "279")
			)
			(pin input line
				(at 17.78 -45.72 180)
				(length 3.81)
				(name "DP_A_HPD")
				(number "276")
			)
			(pin output line
				(at 17.78 -48.26 180)
				(length 3.81)
				(name "DP_B_L0#")
				(number "246")
			)
			(pin output line
				(at 17.78 -50.8 180)
				(length 3.81)
				(name "DP_B_L0")
				(number "248")
			)
			(pin output line
				(at 17.78 -53.34 180)
				(length 3.81)
				(name "DP_B_L1#")
				(number "252")
			)
			(pin output line
				(at 17.78 -55.88 180)
				(length 3.81)
				(name "DP_B_L1")
				(number "254")
			)
			(pin output line
				(at 17.78 -58.42 180)
				(length 3.81)
				(name "DP_B_L2#")
				(number "258")
			)
			(pin output line
				(at 17.78 -60.96 180)
				(length 3.81)
				(name "DP_B_L2")
				(number "260")
			)
			(pin output line
				(at 17.78 -63.5 180)
				(length 3.81)
				(name "DP_B_L3#")
				(number "264")
			)
			(pin output line
				(at 17.78 -66.04 180)
				(length 3.81)
				(name "DP_B_L3")
				(number "266")
			)
			(pin bidirectional line
				(at 17.78 -68.58 180)
				(length 3.81)
				(name "DP_B_AUX#")
				(number "270")
			)
			(pin bidirectional line
				(at 17.78 -71.12 180)
				(length 3.81)
				(name "DP_B_AUX")
				(number "272")
			)
			(pin input line
				(at 17.78 -73.66 180)
				(length 3.81)
				(name "DP_B_HPD")
				(number "274")
			)
			(pin output line
				(at 17.78 -76.2 180)
				(length 3.81)
				(name "DP_C_L0#")
				(number "199")
			)
			(pin output line
				(at 17.78 -78.74 180)
				(length 3.81)
				(name "DP_C_L0")
				(number "201")
			)
			(pin output line
				(at 17.78 -81.28 180)
				(length 3.81)
				(name "DP_C_L1#")
				(number "205")
			)
			(pin output line
				(at 17.78 -83.82 180)
				(length 3.81)
				(name "DP_C_L1")
				(number "207")
			)
			(pin output line
				(at 17.78 -86.36 180)
				(length 3.81)
				(name "DP_C_L2#")
				(number "211")
			)
			(pin output line
				(at 17.78 -88.9 180)
				(length 3.81)
				(name "DP_C_L2")
				(number "213")
			)
			(pin output line
				(at 17.78 -91.44 180)
				(length 3.81)
				(name "DP_C_L3#")
				(number "217")
			)
			(pin output line
				(at 17.78 -93.98 180)
				(length 3.81)
				(name "DP_C_L3")
				(number "219")
			)
			(pin bidirectional line
				(at 17.78 -96.52 180)
				(length 3.81)
				(name "DP_C_AUX#")
				(number "223")
			)
			(pin bidirectional line
				(at 17.78 -99.06 180)
				(length 3.81)
				(name "DP_C_AUX")
				(number "225")
			)
			(pin input line
				(at 17.78 -101.6 180)
				(length 3.81)
				(name "DP_C_HPD")
				(number "234")
			)
			(pin output line
				(at 17.78 -104.14 180)
				(length 3.81)
				(name "DP_D_L0#")
				(number "206")
			)
			(pin output line
				(at 17.78 -106.68 180)
				(length 3.81)
				(name "DP_D_L0")
				(number "208")
			)
			(pin output line
				(at 17.78 -109.22 180)
				(length 3.81)
				(name "DP_D_L1#")
				(number "212")
			)
			(pin output line
				(at 17.78 -111.76 180)
				(length 3.81)
				(name "DP_D_L1")
				(number "214")
			)
			(pin output line
				(at 17.78 -114.3 180)
				(length 3.81)
				(name "DP_D_L2#")
				(number "218")
			)
			(pin output line
				(at 17.78 -116.84 180)
				(length 3.81)
				(name "DP_D_L2")
				(number "220")
			)
			(pin output line
				(at 17.78 -119.38 180)
				(length 3.81)
				(name "DP_D_L3#")
				(number "224")
			)
			(pin output line
				(at 17.78 -121.92 180)
				(length 3.81)
				(name "DP_D_L3")
				(number "226")
			)
			(pin bidirectional line
				(at 17.78 -124.46 180)
				(length 3.81)
				(name "DP_D_AUX#")
				(number "230")
			)
			(pin bidirectional line
				(at 17.78 -127 180)
				(length 3.81)
				(name "DP_D_AUX")
				(number "232")
			)
			(pin input line
				(at 17.78 -129.54 180)
				(length 3.81)
				(name "DP_D_HPD")
				(number "236")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Micro_SD_Card"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -16.51 15.24 0)
		)
		(property "Value" "Micro_SD_Card"
			(at 16.51 15.24 0)
		)
		(property "Footprint" ""
			(at 29.21 7.62 0)
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/693072010801.pdf"
			(at 0 0 0)
		)
		(property "Description" "Micro SD Card Socket"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector SD microsd"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "microSD*"
			(at 0 0 0)
		)
		(symbol "Micro_SD_Card_0_1")
		(symbol "Micro_SD_Card_1_1"
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "DAT2")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "DAT3/CD")
				(number "2")
			)
			(pin input line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "CMD")
				(number "3")
			)
			(pin power_in line
				(at -22.86 0 0)
				(length 3.81)
				(name "VDD")
				(number "4")
			)
			(pin input line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "CLK")
				(number "5")
			)
			(pin power_in line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "DAT0")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "DAT1")
				(number "8")
			)
			(pin passive line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "SHIELD")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Micro_SD_Card_Det1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -16.51 17.78 0)
		)
		(property "Value" "Micro_SD_Card_Det1"
			(at 16.51 17.78 0)
		)
		(property "Footprint" ""
			(at 52.07 17.78 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2110151630_XKB-Connectivity-XKTF-015-N_C381082.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Micro SD Card Socket with one card detection pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector SD microsd"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "microSD*"
			(at 0 0 0)
		)
		(symbol "Micro_SD_Card_Det1_0_1")
		(symbol "Micro_SD_Card_Det1_1_1"
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "DAT2")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "DAT3/CD")
				(number "2")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "CMD")
				(number "3")
			)
			(pin power_in line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "VDD")
				(number "4")
			)
			(pin input line
				(at -22.86 0 0)
				(length 3.81)
				(name "CLK")
				(number "5")
			)
			(pin power_in line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "DAT0")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "DAT1")
				(number "8")
			)
			(pin passive line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "DET")
				(number "9")
			)
			(pin passive line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "SHIELD")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Micro_SD_Card_Det2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -16.51 17.78 0)
		)
		(property "Value" "Micro_SD_Card_Det2"
			(at 16.51 17.78 0)
		)
		(property "Footprint" ""
			(at 52.07 17.78 0)
		)
		(property "Datasheet" "https://www.hirose.com/en/product/document?clcode=&productname=&series=DM3&documenttype=Catalog&lang=en&documentid=D49662_en"
			(at 2.54 2.54 0)
		)
		(property "Description" "Micro SD Card Socket with two card detection pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector SD microsd"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "microSD*"
			(at 0 0 0)
		)
		(symbol "Micro_SD_Card_Det2_0_1")
		(symbol "Micro_SD_Card_Det2_1_1"
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "DAT2")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "DAT3/CD")
				(number "2")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "CMD")
				(number "3")
			)
			(pin power_in line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "VDD")
				(number "4")
			)
			(pin input line
				(at -22.86 0 0)
				(length 3.81)
				(name "CLK")
				(number "5")
			)
			(pin power_in line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "DAT0")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "DAT1")
				(number "8")
			)
			(pin passive line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "DET_A")
				(number "10")
			)
			(pin passive line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "DET_B")
				(number "9")
			)
			(pin passive line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "SHIELD")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Microsemi_FlashPro-JTAG-10"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 4.445 12.7 0)
		)
		(property "Value" "Microsemi_FlashPro-JTAG-10"
			(at 2.54 -12.7 0)
		)
		(property "Footprint" ""
			(at -3.81 3.81 90)
		)
		(property "Datasheet" "https://www.microsemi.com/document-portal/doc_view/129973-lpf-ac386-an"
			(at -32.385 -13.97 0)
		)
		(property "Description" "ACTEL FLASH PRO 3/4, JTAG, IDC10 Pinheader Connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "JTAG IDC10 Pinheader Pins Connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "IDC?Header*2x05* Pin?Header*2x05*"
			(at 0 0 0)
		)
		(symbol "Microsemi_FlashPro-JTAG-10_0_1")
		(symbol "Microsemi_FlashPro-JTAG-10_1_1"
			(pin power_in line
				(at -2.54 15.24 270)
				(length 3.81)
				(name "VJTAG")
				(number "6")
			)
			(pin power_out line
				(at 0 15.24 270)
				(length 3.81)
				(name "VPUMP")
				(number "7")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "~{TRST}")
				(number "8")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "TCK")
				(number "1")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "TMS")
				(number "5")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 3.81)
				(name "TDO")
				(number "3")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "TDI")
				(number "9")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "PGM/NC")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Mini-DIN-3"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 3.302 6.35 0)
		)
		(property "Value" "Mini-DIN-3"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.assmann-wsw.com/fileadmin/catalogue/10_MiniDIN_rev4-0.pdf"
			(at 0 0 0)
		)
		(property "Description" "3-pin Mini-DIN connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-DIN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MINI?DIN*"
			(at 0 0 0)
		)
		(symbol "Mini-DIN-3_0_1")
		(symbol "Mini-DIN-3_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Mini-DIN-4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 6.35 0)
		)
		(property "Value" "Mini-DIN-4"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://service.powerdynamics.com/ec/Catalog17/Section%2011.pdf"
			(at 0 0 0)
		)
		(property "Description" "4-pin Mini-DIN connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-DIN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MINI?DIN*"
			(at 0 0 0)
		)
		(symbol "Mini-DIN-4_0_1")
		(symbol "Mini-DIN-4_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Mini-DIN-5"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 6.35 0)
		)
		(property "Value" "Mini-DIN-5"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://service.powerdynamics.com/ec/Catalog17/Section%2011.pdf"
			(at 0 0 0)
		)
		(property "Description" "5-pin Mini-DIN connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-DIN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MINI?DIN*"
			(at 0 0 0)
		)
		(symbol "Mini-DIN-5_0_1")
		(symbol "Mini-DIN-5_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Mini-DIN-6"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 6.35 0)
		)
		(property "Value" "Mini-DIN-6"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://service.powerdynamics.com/ec/Catalog17/Section%2011.pdf"
			(at 0 0 0)
		)
		(property "Description" "6-pin Mini-DIN connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-DIN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MINI?DIN*"
			(at 0 0 0)
		)
		(symbol "Mini-DIN-6_0_1")
		(symbol "Mini-DIN-6_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Mini-DIN-7"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 5.08 5.08 0)
		)
		(property "Value" "Mini-DIN-7"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at -0.254 -0.254 90)
		)
		(property "Datasheet" "http://service.powerdynamics.com/ec/Catalog17/Section%2011.pdf"
			(at -0.254 -0.254 90)
		)
		(property "Description" "7-pin Mini-DIN connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-DIN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MINI?DIN*"
			(at 0 0 0)
		)
		(symbol "Mini-DIN-7_0_1")
		(symbol "Mini-DIN-7_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Mini-DIN-8"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 5.08 5.08 0)
		)
		(property "Value" "Mini-DIN-8"
			(at 10.668 -5.08 0)
		)
		(property "Footprint" ""
			(at -0.254 -0.254 90)
		)
		(property "Datasheet" "http://service.powerdynamics.com/ec/Catalog17/Section%2011.pdf"
			(at -0.254 -0.254 90)
		)
		(property "Description" "8-pin Mini-DIN connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "Mini-DIN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MINI?DIN*"
			(at 0 0 0)
		)
		(symbol "Mini-DIN-8_0_1")
		(symbol "Mini-DIN-8_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RJ45_Abracon_ARJP11A-MASA-B-A-EMU2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 18.415 12.7 0)
		)
		(property "Value" "RJ45_Abracon_ARJP11A-MASA-B-A-EMU2"
			(at -4.445 12.7 0)
		)
		(property "Footprint" "Connector_RJ:RJ45_Abracon_ARJP11A-MA_Horizontal"
			(at 0 15.24 0)
		)
		(property "Datasheet" "https://abracon.com/Magnetics/lan/ARJP11A.PDF"
			(at 0 17.78 0)
		)
		(property "Description" "RJ45 PoE 10/100 Base-TX Jack with Magnetic Module"
			(at 0 0 0)
		)
		(property "ki_keywords" "single port ethernet transformer socket poe center-tap"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RJ45*Abracon*ARJP11A?MA*"
			(at 0 0 0)
		)
		(symbol "RJ45_Abracon_ARJP11A-MASA-B-A-EMU2_0_0"
			(text "XMIT"
				(at -10.16 3.81 0)
			)
			(text "RCV"
				(at -10.16 -3.81 0)
			)
			(text "C1"
				(at 4.699 9.525 0)
			)
			(text "C4"
				(at 4.699 8.255 0)
			)
			(text "C5"
				(at 4.699 6.985 0)
			)
			(text "C2"
				(at 4.699 5.715 0)
			)
			(text "C3"
				(at 4.699 1.905 0)
			)
			(text "C7"
				(at 4.699 0.635 0)
			)
			(text "C8"
				(at 4.699 -0.635 0)
			)
			(text "C6"
				(at 4.699 -1.905 0)
			)
			(text "C1"
				(at 10.16 -0.635 0)
			)
		)
		(symbol "RJ45_Abracon_ARJP11A-MASA-B-A-EMU2_0_1")
		(symbol "RJ45_Abracon_ARJP11A-MASA-B-A-EMU2_1_0"
			(text "1000pF"
				(at -5.08 5.08 0)
			)
			(text "1000pF"
				(at -5.08 -2.54 0)
			)
		)
		(symbol "RJ45_Abracon_ARJP11A-MASA-B-A-EMU2_1_1"
			(text "75"
				(at 7.112 -3.175 0)
			)
			(text "75"
				(at 7.112 -4.953 0)
			)
			(text "Y"
				(at 19.558 -1.27 0)
			)
			(text "G"
				(at 19.685 8.89 0)
			)
			(pin passive line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "TD+")
				(number "1")
			)
			(pin passive line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "TCT")
				(number "4")
			)
			(pin passive line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "TD-")
				(number "2")
			)
			(pin passive line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "RD+")
				(number "3")
			)
			(pin passive line
				(at -20.32 0 0)
				(length 2.54)
				(name "RCT")
				(number "5")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RD-")
				(number "6")
			)
			(pin power_out line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "V+")
				(number "9")
			)
			(pin power_out line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "V-")
				(number "10")
			)
			(pin power_in line
				(at 10.16 -12.7 90)
				(length 2.54)
				(name "")
				(number "7")
			)
			(pin passive line
				(at 15.24 -12.7 90)
				(length 2.54)
				(name "")
				(number "SH")
			)
			(pin no_connect line
				(at 20.32 5.08 0)
				(length 0)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin passive line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "")
				(number "13")
			)
			(pin passive line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "")
				(number "14")
			)
			(pin passive line
				(at 22.86 0 180)
				(length 2.54)
				(name "")
				(number "11")
			)
			(pin passive line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RJ45_Amphenol_RJMG1BD3B8K1ANR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 18.415 10.16 0)
		)
		(property "Value" "RJ45_Amphenol_RJMG1BD3B8K1ANR"
			(at -19.05 10.16 0)
		)
		(property "Footprint" "Connector_RJ:RJ45_Amphenol_RJMG1BD3B8K1ANR"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.amphenol-cs.com/media/wysiwyg/files/drawing/rjmg1bd3b8k1anr.pdf"
			(at 0 15.24 0)
		)
		(property "Description" "1 Port RJ45 Magjack Connector Through Hole 10/100 Base-T, AutoMDIX"
			(at 0 0 0)
		)
		(property "ki_keywords" "RJ45 Magjack Socket"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RJ45*Amphenol*RJMG1BD3B8K1ANR*"
			(at 0 0 0)
		)
		(symbol "RJ45_Amphenol_RJMG1BD3B8K1ANR_0_0"
			(text "XMIT"
				(at -8.255 1.905 0)
			)
			(text "RCV"
				(at -8.255 -5.715 0)
			)
			(text "C1"
				(at 4.699 6.985 0)
			)
			(text "C4"
				(at 4.699 5.715 0)
			)
			(text "C5"
				(at 4.699 4.445 0)
			)
			(text "C2"
				(at 4.699 3.175 0)
			)
			(text "C3"
				(at 4.699 -0.635 0)
			)
			(text "C7"
				(at 4.699 -1.905 0)
			)
			(text "C8"
				(at 4.699 -3.175 0)
			)
			(text "C6"
				(at 4.699 -4.445 0)
			)
			(text "C1"
				(at 10.16 -3.175 0)
			)
		)
		(symbol "RJ45_Amphenol_RJMG1BD3B8K1ANR_0_1")
		(symbol "RJ45_Amphenol_RJMG1BD3B8K1ANR_1_0"
			(text "1000pF"
				(at 3.302 -6.477 0)
			)
		)
		(symbol "RJ45_Amphenol_RJMG1BD3B8K1ANR_1_1"
			(text "75"
				(at -3.556 5.08 0)
			)
			(text "75"
				(at -3.556 -2.54 0)
			)
			(text "75"
				(at 1.016 5.08 0)
			)
			(text "75"
				(at 1.016 -2.54 0)
			)
			(text "Y"
				(at 19.558 6.35 0)
			)
			(text "G"
				(at 19.685 -3.81 0)
			)
			(pin passive line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "TD+")
				(number "R1")
			)
			(pin passive line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "TCT")
				(number "R4")
			)
			(pin passive line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "TD-")
				(number "R2")
			)
			(pin passive line
				(at -20.32 0 0)
				(length 2.54)
				(name "RD+")
				(number "R3")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RCT")
				(number "R5")
			)
			(pin passive line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RD-")
				(number "R6")
			)
			(pin power_in line
				(at 10.16 -10.16 90)
				(length 2.54)
				(name "")
				(number "R8")
			)
			(pin passive line
				(at 15.24 -10.16 90)
				(length 2.54)
				(name "")
				(number "SH")
			)
			(pin no_connect line
				(at 20.32 0 0)
				(length 0)
				(hide yes)
				(name "NC")
				(number "R7")
			)
			(pin passive line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "")
				(number "L1")
			)
			(pin passive line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "")
				(number "L2")
			)
			(pin passive line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "")
				(number "L4")
			)
			(pin passive line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "")
				(number "L3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RJ45_Bel_SI-60062-F"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 19.05 10.16 0)
		)
		(property "Value" "RJ45_Bel_SI-60062-F"
			(at -19.05 10.16 0)
		)
		(property "Footprint" "Connector_RJ:RJ45_Bel_SI-60062-F"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://belfuse.com/resources/drawings/magneticsolutions/dr-mag-si-60062-f.pdf"
			(at 0 15.24 0)
		)
		(property "Description" "1 Port RJ45 Magjack Connector Through Hole 10/100 Base-T, AutoMDIX"
			(at 0 0 0)
		)
		(property "ki_keywords" "RJ45 Magjack Socket"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RJ45*Bel*SI*60062*F*"
			(at 0 0 0)
		)
		(symbol "RJ45_Bel_SI-60062-F_0_0"
			(text "XMIT"
				(at -8.255 1.905 0)
			)
			(text "RCV"
				(at -8.255 -5.715 0)
			)
			(text "C1"
				(at 4.699 6.985 0)
			)
			(text "C4"
				(at 4.699 5.715 0)
			)
			(text "C5"
				(at 4.699 4.445 0)
			)
			(text "C2"
				(at 4.699 3.175 0)
			)
			(text "C3"
				(at 4.699 -0.635 0)
			)
			(text "C7"
				(at 4.699 -1.905 0)
			)
			(text "C8"
				(at 4.699 -3.175 0)
			)
			(text "C6"
				(at 4.699 -4.445 0)
			)
			(text "C1"
				(at 10.16 -3.175 0)
			)
		)
		(symbol "RJ45_Bel_SI-60062-F_0_1")
		(symbol "RJ45_Bel_SI-60062-F_1_0"
			(text "1000pF"
				(at 3.302 -6.477 0)
			)
		)
		(symbol "RJ45_Bel_SI-60062-F_1_1"
			(text "75"
				(at -3.556 5.08 0)
			)
			(text "75"
				(at -3.556 -2.54 0)
			)
			(text "75"
				(at 1.016 5.08 0)
			)
			(text "75"
				(at 1.016 -2.54 0)
			)
			(text "Y"
				(at 19.558 -3.81 0)
			)
			(text "G"
				(at 19.685 6.35 0)
			)
			(pin passive line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "TD+")
				(number "1")
			)
			(pin passive line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "TCT")
				(number "2")
			)
			(pin passive line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "TD-")
				(number "3")
			)
			(pin passive line
				(at -20.32 0 0)
				(length 2.54)
				(name "RD+")
				(number "4")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RCT")
				(number "5")
			)
			(pin passive line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RD-")
				(number "6")
			)
			(pin power_in line
				(at 10.16 -10.16 90)
				(length 2.54)
				(name "")
				(number "8")
			)
			(pin passive line
				(at 15.24 -10.16 90)
				(length 2.54)
				(name "")
				(number "SH")
			)
			(pin no_connect line
				(at 20.32 0 0)
				(length 0)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "")
				(number "L3")
			)
			(pin passive line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "")
				(number "L4")
			)
			(pin passive line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "")
				(number "L1")
			)
			(pin passive line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "")
				(number "L2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RJ45_Bel_V895-1001-AW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 16.51 15.24 0)
		)
		(property "Value" "RJ45_Bel_V895-1001-AW"
			(at -5.715 15.24 0)
		)
		(property "Footprint" "Connector_RJ:RJ45_Bel_V895-1001-AW_Vertical"
			(at 0 18.415 0)
		)
		(property "Datasheet" "https://www.belfuse.com/resources/drawings/magneticsolutions/dr-mag-v895-1001-aw.pdf"
			(at 0 18.415 0)
		)
		(property "Description" "RJ45 PoE 10/100 Base-TX Jack with Magnetic Module"
			(at 0 2.54 0)
		)
		(property "ki_keywords" "single port ethernet transformer socket poe center-tap"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RJ45*Bel*V895*1001*AW*"
			(at 0 0 0)
		)
		(symbol "RJ45_Bel_V895-1001-AW_0_0"
			(text "XMIT"
				(at -10.16 6.35 0)
			)
			(text "RCV"
				(at -10.16 -1.27 0)
			)
			(text "C1"
				(at 4.699 12.065 0)
			)
			(text "C4"
				(at 4.699 10.795 0)
			)
			(text "C5"
				(at 4.699 9.525 0)
			)
			(text "C2"
				(at 4.699 8.255 0)
			)
			(text "C3"
				(at 4.699 4.445 0)
			)
			(text "C7"
				(at 4.699 3.175 0)
			)
			(text "C8"
				(at 4.699 1.905 0)
			)
			(text "C6"
				(at 4.699 0.635 0)
			)
			(text "C1"
				(at 10.16 1.905 0)
			)
		)
		(symbol "RJ45_Bel_V895-1001-AW_0_1")
		(symbol "RJ45_Bel_V895-1001-AW_1_0"
			(text "4 x 15nF"
				(at 3.175 -6.985 0)
			)
			(text "1000pF"
				(at 13.335 -5.08 0)
			)
		)
		(symbol "RJ45_Bel_V895-1001-AW_1_1"
			(text "75"
				(at 7.112 -0.762 0)
			)
			(text "75"
				(at 7.112 -2.286 0)
			)
			(text "75"
				(at 7.112 -3.81 0)
			)
			(text "75"
				(at 7.112 -5.334 0)
			)
			(pin passive line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "TD+")
				(number "1")
			)
			(pin passive line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "CT")
				(number "5")
			)
			(pin passive line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "TD-")
				(number "2")
			)
			(pin passive line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "RD+")
				(number "3")
			)
			(pin passive line
				(at -20.32 0 0)
				(length 2.54)
				(name "RD-")
				(number "4")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "Vc4")
				(number "10")
			)
			(pin passive line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "Vc3")
				(number "9")
			)
			(pin passive line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "Vc2")
				(number "8")
			)
			(pin passive line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "Vc1")
				(number "7")
			)
			(pin passive line
				(at 10.16 -15.24 90)
				(length 2.54)
				(name "")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RJ45_Halo_HFJ11-x2450E-LxxRL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 19.05 10.16 0)
		)
		(property "Value" "RJ45_Halo_HFJ11-x2450E-LxxRL"
			(at -17.78 10.16 0)
		)
		(property "Footprint" "Connector_RJ:RJ45_HALO_HFJ11-x2450E-LxxRL_Horizontal"
			(at 0 12.065 0)
		)
		(property "Datasheet" "https://www.haloelectronics.com/pdf/fastjack-100baset.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "Halo HFJ11, 10/100 Base-TX, two LEDs, RJ45, Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "FastJack socket"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RJ45*HALO*HFJ11*x2450E*LxxRL*"
			(at 0 0 0)
		)
		(symbol "RJ45_Halo_HFJ11-x2450E-LxxRL_0_0"
			(text "XMIT"
				(at -8.255 1.905 0)
			)
			(text "RCV"
				(at -8.255 -5.715 0)
			)
			(text "C1"
				(at 4.699 6.985 0)
			)
			(text "C4"
				(at 4.699 5.715 0)
			)
			(text "C5"
				(at 4.699 4.445 0)
			)
			(text "C2"
				(at 4.699 3.175 0)
			)
			(text "C3"
				(at 4.699 -0.635 0)
			)
			(text "C7"
				(at 4.699 -1.905 0)
			)
			(text "C8"
				(at 4.699 -3.175 0)
			)
			(text "C6"
				(at 4.699 -4.445 0)
			)
			(text "C1"
				(at 10.16 -3.175 0)
			)
		)
		(symbol "RJ45_Halo_HFJ11-x2450E-LxxRL_0_1")
		(symbol "RJ45_Halo_HFJ11-x2450E-LxxRL_1_0"
			(text "1000pF"
				(at 3.302 -6.477 0)
			)
		)
		(symbol "RJ45_Halo_HFJ11-x2450E-LxxRL_1_1"
			(text "75"
				(at -3.556 5.08 0)
			)
			(text "75"
				(at -3.556 -2.54 0)
			)
			(text "75"
				(at 1.016 5.08 0)
			)
			(text "75"
				(at 1.016 -2.54 0)
			)
			(pin passive line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "TD+")
				(number "1")
			)
			(pin passive line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "TCT")
				(number "4")
			)
			(pin passive line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "TD-")
				(number "2")
			)
			(pin passive line
				(at -20.32 0 0)
				(length 2.54)
				(name "RD+")
				(number "3")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RCT")
				(number "5")
			)
			(pin passive line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RD-")
				(number "6")
			)
			(pin power_in line
				(at 10.16 -10.16 90)
				(length 2.54)
				(name "")
				(number "8")
			)
			(pin passive line
				(at 15.24 -10.16 90)
				(length 2.54)
				(name "")
				(number "SH")
			)
			(pin no_connect line
				(at 20.32 0 0)
				(length 0)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "")
				(number "11")
			)
			(pin passive line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "")
				(number "12")
			)
			(pin passive line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "")
				(number "9")
			)
			(pin passive line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RJ45_Halo_HFJ11-x2450ERL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 19.05 10.16 0)
		)
		(property "Value" "RJ45_Halo_HFJ11-x2450ERL"
			(at -17.78 10.16 0)
		)
		(property "Footprint" "Connector_RJ:RJ45_HALO_HFJ11-x2450ERL_Horizontal"
			(at 0 12.065 0)
		)
		(property "Datasheet" "https://www.haloelectronics.com/pdf/fastjack-100baset.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "Halo HFJ11, 10/100 Base-TX, no LED, RJ45, Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "FastJack socket"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RJ45*HALO*HFJ11*x2450ERL*"
			(at 0 0 0)
		)
		(symbol "RJ45_Halo_HFJ11-x2450ERL_0_0"
			(text "XMIT"
				(at -8.255 1.905 0)
			)
			(text "RCV"
				(at -8.255 -5.715 0)
			)
			(text "C1"
				(at 4.699 6.985 0)
			)
			(text "C4"
				(at 4.699 5.715 0)
			)
			(text "C5"
				(at 4.699 4.445 0)
			)
			(text "C2"
				(at 4.699 3.175 0)
			)
			(text "C3"
				(at 4.699 -0.635 0)
			)
			(text "C7"
				(at 4.699 -1.905 0)
			)
			(text "C8"
				(at 4.699 -3.175 0)
			)
			(text "C6"
				(at 4.699 -4.445 0)
			)
			(text "C1"
				(at 10.16 -3.175 0)
			)
		)
		(symbol "RJ45_Halo_HFJ11-x2450ERL_0_1")
		(symbol "RJ45_Halo_HFJ11-x2450ERL_1_0"
			(text "1000pF"
				(at 3.302 -6.477 0)
			)
		)
		(symbol "RJ45_Halo_HFJ11-x2450ERL_1_1"
			(text "75"
				(at -3.556 5.08 0)
			)
			(text "75"
				(at -3.556 -2.54 0)
			)
			(text "75"
				(at 1.016 5.08 0)
			)
			(text "75"
				(at 1.016 -2.54 0)
			)
			(pin passive line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "TD+")
				(number "1")
			)
			(pin passive line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "TCT")
				(number "4")
			)
			(pin passive line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "TD-")
				(number "2")
			)
			(pin passive line
				(at -20.32 0 0)
				(length 2.54)
				(name "RD+")
				(number "3")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RCT")
				(number "5")
			)
			(pin passive line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RD-")
				(number "6")
			)
			(pin power_in line
				(at 10.16 -10.16 90)
				(length 2.54)
				(name "")
				(number "8")
			)
			(pin passive line
				(at 15.24 -10.16 90)
				(length 2.54)
				(name "")
				(number "SH")
			)
			(pin no_connect line
				(at 20.32 0 0)
				(length 0)
				(hide yes)
				(name "NC")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RJ45_Halo_HFJ11-x2450HRL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 19.05 10.16 0)
		)
		(property "Value" "RJ45_Halo_HFJ11-x2450HRL"
			(at -17.78 10.16 0)
		)
		(property "Footprint" "Connector_RJ:RJ45_HALO_HFJ11-x2450HRL_Horizontal"
			(at 0 12.065 0)
		)
		(property "Datasheet" "https://www.haloelectronics.com/pdf/fastjack-100baset.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "Halo HFJ11, 10/100 Base-TX, no LED, RJ45, Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "FastJack socket"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RJ45*HALO*HFJ11*x2450HRL*"
			(at 0 0 0)
		)
		(symbol "RJ45_Halo_HFJ11-x2450HRL_0_0"
			(text "XMIT"
				(at -8.255 1.905 0)
			)
			(text "RCV"
				(at -8.255 -5.715 0)
			)
			(text "C1"
				(at 4.699 6.985 0)
			)
			(text "C4"
				(at 4.699 5.715 0)
			)
			(text "C5"
				(at 4.699 4.445 0)
			)
			(text "C2"
				(at 4.699 3.175 0)
			)
			(text "C3"
				(at 4.699 -0.635 0)
			)
			(text "C7"
				(at 4.699 -1.905 0)
			)
			(text "C8"
				(at 4.699 -3.175 0)
			)
			(text "C6"
				(at 4.699 -4.445 0)
			)
			(text "C1"
				(at 10.16 -3.175 0)
			)
		)
		(symbol "RJ45_Halo_HFJ11-x2450HRL_0_1")
		(symbol "RJ45_Halo_HFJ11-x2450HRL_1_0"
			(text "1000pF"
				(at 3.302 -6.477 0)
			)
		)
		(symbol "RJ45_Halo_HFJ11-x2450HRL_1_1"
			(text "75"
				(at -3.556 5.08 0)
			)
			(text "75"
				(at -3.556 -2.54 0)
			)
			(text "75"
				(at 1.016 5.08 0)
			)
			(text "75"
				(at 1.016 -2.54 0)
			)
			(pin passive line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "TD+")
				(number "1")
			)
			(pin passive line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "TCT")
				(number "4")
			)
			(pin passive line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "TD-")
				(number "2")
			)
			(pin passive line
				(at -20.32 0 0)
				(length 2.54)
				(name "RD+")
				(number "3")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RCT")
				(number "5")
			)
			(pin passive line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RD-")
				(number "6")
			)
			(pin power_in line
				(at 10.16 -10.16 90)
				(length 2.54)
				(name "")
				(number "8")
			)
			(pin passive line
				(at 15.24 -10.16 90)
				(length 2.54)
				(name "")
				(number "SH")
			)
			(pin no_connect line
				(at 20.32 0 0)
				(length 0)
				(hide yes)
				(name "NC")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RJ45_Hanrun_HR911105A_Horizontal"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 18.415 10.16 0)
		)
		(property "Value" "RJ45_Hanrun_HR911105A_Horizontal"
			(at -19.05 10.16 0)
		)
		(property "Footprint" "Connector_RJ:RJ45_Hanrun_HR911105A_Horizontal"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/1811141815_HANRUN-Zhongshan-HanRun-Elec-HR911105A_C12074.pdf"
			(at 0 15.24 0)
		)
		(property "Description" "1 Port RJ45 Magjack Connector Through Hole 10/100 Base-T, AutoMDIX"
			(at 0 0 0)
		)
		(property "ki_keywords" "RJ45 Magjack Socket"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RJ45*Hanrun*HR911105A*"
			(at 0 0 0)
		)
		(symbol "RJ45_Hanrun_HR911105A_Horizontal_0_0"
			(text "XMIT"
				(at -8.255 1.905 0)
			)
			(text "RCV"
				(at -8.255 -5.715 0)
			)
			(text "C1"
				(at 4.699 6.985 0)
			)
			(text "C4"
				(at 4.699 5.715 0)
			)
			(text "C5"
				(at 4.699 4.445 0)
			)
			(text "C2"
				(at 4.699 3.175 0)
			)
			(text "C3"
				(at 4.699 -0.635 0)
			)
			(text "C7"
				(at 4.699 -1.905 0)
			)
			(text "C8"
				(at 4.699 -3.175 0)
			)
			(text "C6"
				(at 4.699 -4.445 0)
			)
			(text "C1"
				(at 10.16 -3.175 0)
			)
		)
		(symbol "RJ45_Hanrun_HR911105A_Horizontal_0_1")
		(symbol "RJ45_Hanrun_HR911105A_Horizontal_1_0"
			(text "1000pF"
				(at 3.302 -6.477 0)
			)
		)
		(symbol "RJ45_Hanrun_HR911105A_Horizontal_1_1"
			(text "75"
				(at -3.556 5.08 0)
			)
			(text "75"
				(at -3.556 -2.54 0)
			)
			(text "75"
				(at 1.016 5.08 0)
			)
			(text "75"
				(at 1.016 -2.54 0)
			)
			(text "Y"
				(at 19.558 6.35 0)
			)
			(text "G"
				(at 19.685 -3.81 0)
			)
			(pin passive line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "TD+")
				(number "1")
			)
			(pin passive line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "TCT")
				(number "4")
			)
			(pin passive line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "TD-")
				(number "2")
			)
			(pin passive line
				(at -20.32 0 0)
				(length 2.54)
				(name "RD+")
				(number "3")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RCT")
				(number "5")
			)
			(pin passive line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RD-")
				(number "6")
			)
			(pin power_in line
				(at 10.16 -10.16 90)
				(length 2.54)
				(name "")
				(number "8")
			)
			(pin passive line
				(at 15.24 -10.16 90)
				(length 2.54)
				(name "")
				(number "SH")
			)
			(pin no_connect line
				(at 20.32 0 0)
				(length 0)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "")
				(number "12")
			)
			(pin passive line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "")
				(number "11")
			)
			(pin passive line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "")
				(number "9")
			)
			(pin passive line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RJ45_JK00177"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -15.24 29.21 0)
		)
		(property "Value" "RJ45_JK00177"
			(at 10.16 29.21 0)
		)
		(property "Footprint" "Connector_RJ:RJ45_Pulse_JK00177NL_Horizontal"
			(at -0.127 -32.893 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/doc_type/WEB301/doc_num/J432/doc_part/J432.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "1 Port RJ45 Magjack Connector Through Hole 10/100/1000 Base-T, AutoMDIX, 75W POE"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket jack connector POE"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RJ45*Pulse*JK00177NL*"
			(at 0 0 0)
		)
		(symbol "RJ45_JK00177_0_0"
			(text "Y"
				(at -8.001 25.019 0)
			)
			(text ""
				(at -7.874 24.892 900)
			)
			(text "G"
				(at -7.112 -23.114 0)
			)
			(text "G"
				(at -5.461 25.019 0)
			)
			(text "1"
				(at 10.16 18.415 0)
			)
			(text "2"
				(at 10.16 13.335 0)
			)
			(text "3"
				(at 10.16 8.255 0)
			)
			(text "6"
				(at 10.16 3.175 0)
			)
			(text "4"
				(at 10.16 -1.905 0)
			)
			(text "5"
				(at 10.16 -6.985 0)
			)
			(text "7"
				(at 10.16 -12.065 0)
			)
			(text "8"
				(at 10.16 -17.145 0)
			)
		)
		(symbol "RJ45_JK00177_0_1")
		(symbol "RJ45_JK00177_1_1"
			(pin passive line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "LED1+")
				(number "16")
			)
			(pin passive line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "LED1-")
				(number "15")
			)
			(pin passive line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "MX1+")
				(number "11")
			)
			(pin passive line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "MXCT1")
				(number "12")
			)
			(pin passive line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "MX1-")
				(number "10")
			)
			(pin passive line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "MX2+")
				(number "4")
			)
			(pin passive line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "MXCT2")
				(number "6")
			)
			(pin passive line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "MX2-")
				(number "5")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "MX3+")
				(number "3")
			)
			(pin passive line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "MXCT3")
				(number "1")
			)
			(pin passive line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "MX3-")
				(number "2")
			)
			(pin passive line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "MX4+")
				(number "8")
			)
			(pin passive line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "MXCT4")
				(number "7")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "MX4-")
				(number "9")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "LED2+")
				(number "13")
			)
			(pin passive line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "LED2-")
				(number "14")
			)
			(pin passive line
				(at -5.08 -30.48 90)
				(length 2.54)
				(name "VDC1-")
				(number "18")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VDC1+")
				(number "17")
			)
			(pin passive line
				(at -2.54 -30.48 90)
				(length 2.54)
				(name "VDC2-")
				(number "20")
			)
			(pin passive line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDC2+")
				(number "19")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(name "~")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RJ45_JK0654219"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -15.24 29.21 0)
		)
		(property "Value" "RJ45_JK0654219"
			(at 10.16 29.21 0)
		)
		(property "Footprint" "Connector_RJ:RJ45_Pulse_JK0654219NL_Horizontal"
			(at -0.127 -32.893 0)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/Pulse%20PDFs/JK%20Series.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "1 Port RJ45 Magjack Connector Through Hole 10/100/1000 Base-T, AutoMDIX"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket jack connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RJ45*Pulse*JK0654219NL*"
			(at 0 0 0)
		)
		(symbol "RJ45_JK0654219_0_0")
		(symbol "RJ45_JK0654219_0_1")
		(symbol "RJ45_JK0654219_1_1"
			(pin passive line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "LED1+")
				(number "16")
			)
			(pin passive line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "LED1-")
				(number "15")
			)
			(pin passive line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "MX1+")
				(number "11")
			)
			(pin passive line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "MXCT1")
				(number "12")
			)
			(pin passive line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "MX1-")
				(number "10")
			)
			(pin passive line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "MX2+")
				(number "4")
			)
			(pin passive line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "MXCT2")
				(number "6")
			)
			(pin passive line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "MX2-")
				(number "5")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "MX3+")
				(number "3")
			)
			(pin passive line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "MXCT3")
				(number "1")
			)
			(pin passive line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "MX3-")
				(number "2")
			)
			(pin passive line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "MX4+")
				(number "8")
			)
			(pin passive line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "MXCT4")
				(number "7")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "MX4-")
				(number "9")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "LED2+")
				(number "14")
			)
			(pin passive line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "LED2-")
				(number "13")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(name "~")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RJ45_Kycon_G7LX-A88S7-BP-GY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 17.78 24.13 0)
		)
		(property "Value" "RJ45_Kycon_G7LX-A88S7-BP-GY"
			(at -20.32 24.13 0)
		)
		(property "Footprint" "Connector_RJ:RJ45_Kycon_G7LX-A88S7-BP-xx_Horizontal"
			(at 0 27.94 0)
		)
		(property "Datasheet" "http://www.kycon.com/Pub_Eng_Draw/G7LX-A88S7-BP-GY.pdf"
			(at 0 30.48 0)
		)
		(property "Description" "1 Port RJ45 Magjack Connector Through Hole 10/100 Base-T, AutoMDIX"
			(at 0 0 0)
		)
		(property "ki_keywords" "RJ45 Magjack"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RJ45*Kycon*G7LX*A88S7*BP*Horizontal*"
			(at 0 0 0)
		)
		(symbol "RJ45_Kycon_G7LX-A88S7-BP-GY_0_0"
			(text "GREEN"
				(at -5.715 19.05 0)
			)
			(text "YELLOW"
				(at -5.715 13.97 0)
			)
			(text "C1"
				(at 3.175 6.985 0)
			)
			(text "C4"
				(at 3.175 5.715 0)
			)
			(text "C5"
				(at 3.175 4.445 0)
			)
			(text "C2"
				(at 3.175 3.175 0)
			)
			(text "C3"
				(at 3.175 -0.635 0)
			)
			(text "C7"
				(at 3.175 -1.905 0)
			)
			(text "C8"
				(at 3.175 -3.175 0)
			)
			(text "C6"
				(at 3.175 -4.445 0)
			)
			(text "C1"
				(at 6.2865 2.7305 900)
			)
		)
		(symbol "RJ45_Kycon_G7LX-A88S7-BP-GY_0_1")
		(symbol "RJ45_Kycon_G7LX-A88S7-BP-GY_1_1"
			(pin passive line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "LEDG_A")
				(number "14")
			)
			(pin passive line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "LEDG_K")
				(number "13")
			)
			(pin passive line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "LEDY_A")
				(number "12")
			)
			(pin passive line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "LEDY_K")
				(number "11")
			)
			(pin passive line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "TD+")
				(number "1")
			)
			(pin passive line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "TCT")
				(number "4")
			)
			(pin passive line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "TD-")
				(number "2")
			)
			(pin passive line
				(at -20.32 0 0)
				(length 2.54)
				(name "RD+")
				(number "3")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RCT")
				(number "7")
			)
			(pin passive line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RD-")
				(number "6")
			)
			(pin passive line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "R1")
				(number "5")
			)
			(pin passive line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "R2")
				(number "8")
			)
			(pin passive line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "R3")
				(number "10")
			)
			(pin passive line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "R4")
				(number "9")
			)
			(pin passive line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "SHIELD")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RJ45_Pulse_JXD6-0001NL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 17.78 10.16 0)
		)
		(property "Value" "RJ45_Pulse_JXD6-0001NL"
			(at -6.35 10.16 0)
		)
		(property "Footprint" "Connector_RJ:RJ45_Pulse_JXD6-0001NL_Horizontal"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://productfinder.pulseeng.com/doc_type/WEB301/doc_num/JXD6-0001NL/doc_part/JXD6-0001NL.pdf"
			(at 0 16.51 0)
		)
		(property "Description" "LAN Transformer Jack, RJ45, 10/100 BaseT"
			(at 0 0 0)
		)
		(property "ki_keywords" "lan jack socket transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RJ45*Pulse*JXD6?0001NL*"
			(at 0 0 0)
		)
		(symbol "RJ45_Pulse_JXD6-0001NL_0_0"
			(text "XMIT"
				(at -8.255 1.905 0)
			)
			(text "RCV"
				(at -8.255 -5.715 0)
			)
			(text "C1"
				(at 4.699 6.985 0)
			)
			(text "C4"
				(at 4.699 5.715 0)
			)
			(text "C5"
				(at 4.699 4.445 0)
			)
			(text "C2"
				(at 4.699 3.175 0)
			)
			(text "C3"
				(at 4.699 -0.635 0)
			)
			(text "C7"
				(at 4.699 -1.905 0)
			)
			(text "C8"
				(at 4.699 -3.175 0)
			)
			(text "C6"
				(at 4.699 -4.445 0)
			)
			(text "C1"
				(at 10.16 -3.175 0)
			)
		)
		(symbol "RJ45_Pulse_JXD6-0001NL_0_1")
		(symbol "RJ45_Pulse_JXD6-0001NL_1_0"
			(text "1000pF"
				(at 3.302 -6.477 0)
			)
		)
		(symbol "RJ45_Pulse_JXD6-0001NL_1_1"
			(text "75"
				(at -3.556 5.08 0)
			)
			(text "75"
				(at -3.556 -2.54 0)
			)
			(text "75"
				(at 1.016 5.08 0)
			)
			(text "75"
				(at 1.016 -2.54 0)
			)
			(text "Y"
				(at 19.558 6.35 0)
			)
			(text "G"
				(at 19.685 -3.81 0)
			)
			(pin passive line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "TD+")
				(number "4")
			)
			(pin passive line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "TCT")
				(number "3")
			)
			(pin passive line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "TD-")
				(number "5")
			)
			(pin passive line
				(at -20.32 0 0)
				(length 2.54)
				(name "RD+")
				(number "6")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RCT")
				(number "8")
			)
			(pin passive line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RD-")
				(number "7")
			)
			(pin power_in line
				(at 10.16 -10.16 90)
				(length 2.54)
				(name "")
				(number "SH")
			)
			(pin passive line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "")
				(number "10")
			)
			(pin passive line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "")
				(number "9")
			)
			(pin passive line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "")
				(number "2")
			)
			(pin passive line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RJ45_RB1-125B8G1A"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -7.62 20.32 0)
		)
		(property "Value" "RJ45_RB1-125B8G1A"
			(at 15.24 20.32 0)
		)
		(property "Footprint" "Connector_RJ:RJ45_UDE_RB1-125B8G1A"
			(at 1.27 2.54 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/szlcsc/1901091107_UDE-Corp-RB1-125B8G1A_C363353.pdf"
			(at -6.096 1.143 0)
		)
		(property "Description" "LAN Transformer Jack, RJ45, 10/100/1000 BaseT"
			(at 0 0 0)
		)
		(property "ki_keywords" "lan jack socket transformer ethernet gigabit 10 100 1000 baset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RJ45*UDE*RB1*125B8G1A*"
			(at 0 0 0)
		)
		(symbol "RJ45_RB1-125B8G1A_0_0"
			(text "C1"
				(at -5.08 13.97 0)
			)
			(text "C2"
				(at -5.08 11.684 0)
			)
			(text "C3"
				(at -5.08 6.096 0)
			)
			(text "C6"
				(at -5.08 4.064 0)
			)
			(text "C4"
				(at -5.08 -1.524 0)
			)
			(text "C5"
				(at -5.08 -3.556 0)
			)
			(text "C7"
				(at -5.08 -9.144 0)
			)
			(text "C8"
				(at -5.08 -11.176 0)
			)
			(text "G"
				(at -2.54 16.51 0)
			)
			(text "Y"
				(at 2.54 16.51 0)
			)
			(text "1000pF 2kV"
				(at 2.54 -13.716 0)
			)
		)
		(symbol "RJ45_RB1-125B8G1A_0_1"
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "R10")
			)
		)
		(symbol "RJ45_RB1-125B8G1A_1_0"
			(text "75"
				(at 0.762 10.922 0)
			)
			(text "75"
				(at 0.762 3.302 0)
			)
			(text "75"
				(at 0.762 -4.318 0)
			)
			(text "75"
				(at 0.762 -11.938 0)
			)
		)
		(symbol "RJ45_RB1-125B8G1A_1_1"
			(pin passive line
				(at -2.54 22.86 270)
				(length 3.81)
				(name "~")
				(number "L3")
			)
			(pin passive line
				(at 0 22.86 270)
				(length 3.81)
				(name "~")
				(number "L4")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 3.81)
				(name "~")
				(number "L1")
			)
			(pin passive line
				(at 2.54 -20.32 90)
				(length 3.81)
				(name "SH")
				(number "SH")
			)
			(pin passive line
				(at 5.08 22.86 270)
				(length 3.81)
				(name "~")
				(number "L2")
			)
			(pin passive line
				(at 12.7 17.78 180)
				(length 3.81)
				(name "CT")
				(number "R1")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 3.81)
				(name "TD1+")
				(number "R2")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 3.81)
				(name "TD1-")
				(number "R3")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "TD2+")
				(number "R4")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "TD2-")
				(number "R5")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 3.81)
				(name "TD3+")
				(number "R6")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "TD3-")
				(number "R7")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "TD4+")
				(number "R8")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 3.81)
				(name "TD4-")
				(number "R9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RJ45_Wuerth_74980111211"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 19.05 10.16 0)
		)
		(property "Value" "RJ45_Wuerth_74980111211"
			(at -6.35 10.16 0)
		)
		(property "Footprint" "Connector_RJ:RJ45_Wuerth_74980111211_Horizontal"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.we-online.de/katalog/datasheet/74980111211.pdf"
			(at 0 16.51 0)
		)
		(property "Description" "LAN Transformer Jack, RJ45, 10/100 BaseT"
			(at 0 0 0)
		)
		(property "ki_keywords" "lan jack socket transformer smt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RJ45*Wuerth*74980111211*"
			(at 0 0 0)
		)
		(symbol "RJ45_Wuerth_74980111211_0_0"
			(text "XMIT"
				(at -8.255 1.905 0)
			)
			(text "RCV"
				(at -8.255 -5.715 0)
			)
			(text "C1"
				(at 4.699 6.985 0)
			)
			(text "C4"
				(at 4.699 5.715 0)
			)
			(text "C5"
				(at 4.699 4.445 0)
			)
			(text "C2"
				(at 4.699 3.175 0)
			)
			(text "C3"
				(at 4.699 -0.635 0)
			)
			(text "C7"
				(at 4.699 -1.905 0)
			)
			(text "C8"
				(at 4.699 -3.175 0)
			)
			(text "C6"
				(at 4.699 -4.445 0)
			)
			(text "C1"
				(at 10.16 -3.175 0)
			)
		)
		(symbol "RJ45_Wuerth_74980111211_0_1")
		(symbol "RJ45_Wuerth_74980111211_1_0"
			(text "1000pF"
				(at 3.302 -6.477 0)
			)
		)
		(symbol "RJ45_Wuerth_74980111211_1_1"
			(text "75"
				(at -3.556 5.08 0)
			)
			(text "75"
				(at -3.556 -2.54 0)
			)
			(text "75"
				(at 1.016 5.08 0)
			)
			(text "75"
				(at 1.016 -2.54 0)
			)
			(text "Y"
				(at 19.558 6.35 0)
			)
			(text "G"
				(at 19.685 -3.81 0)
			)
			(pin passive line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "TD+")
				(number "3")
			)
			(pin passive line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "TCT")
				(number "4")
			)
			(pin passive line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "TD-")
				(number "5")
			)
			(pin passive line
				(at -20.32 0 0)
				(length 2.54)
				(name "RD+")
				(number "6")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RCT")
				(number "7")
			)
			(pin passive line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RD-")
				(number "8")
			)
			(pin power_in line
				(at 10.16 -10.16 90)
				(length 2.54)
				(name "")
				(number "10")
			)
			(pin passive line
				(at 15.24 -10.16 90)
				(length 2.54)
				(name "")
				(number "SH")
			)
			(pin no_connect line
				(at 20.32 0 0)
				(length 0)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin passive line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "")
				(number "12")
			)
			(pin passive line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "")
				(number "11")
			)
			(pin passive line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "")
				(number "1")
			)
			(pin passive line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RJ45_Wuerth_7499010121A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 17.78 10.16 0)
		)
		(property "Value" "RJ45_Wuerth_7499010121A"
			(at -6.35 10.16 0)
		)
		(property "Footprint" "Connector_RJ:RJ45_Wuerth_7499010121A_Horizontal"
			(at 0 12.7 0)
		)
		(property "Datasheet" "http://katalog.we-online.de/pbs/datasheet/7499010121A.pdf"
			(at 0 16.51 0)
		)
		(property "Description" "LAN Transformer Jack, RJ45, 10/100 BaseT"
			(at 0 0 0)
		)
		(property "ki_keywords" "lan jack socket transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RJ45*Wuerth*7499010121A*"
			(at 0 0 0)
		)
		(symbol "RJ45_Wuerth_7499010121A_0_0"
			(text "XMIT"
				(at -8.255 1.905 0)
			)
			(text "RCV"
				(at -8.255 -5.715 0)
			)
			(text "C1"
				(at 4.699 6.985 0)
			)
			(text "C4"
				(at 4.699 5.715 0)
			)
			(text "C5"
				(at 4.699 4.445 0)
			)
			(text "C2"
				(at 4.699 3.175 0)
			)
			(text "C3"
				(at 4.699 -0.635 0)
			)
			(text "C7"
				(at 4.699 -1.905 0)
			)
			(text "C8"
				(at 4.699 -3.175 0)
			)
			(text "C6"
				(at 4.699 -4.445 0)
			)
			(text "C1"
				(at 10.16 -3.175 0)
			)
		)
		(symbol "RJ45_Wuerth_7499010121A_0_1")
		(symbol "RJ45_Wuerth_7499010121A_1_0"
			(text "1000pF"
				(at 3.302 -6.477 0)
			)
		)
		(symbol "RJ45_Wuerth_7499010121A_1_1"
			(text "75"
				(at -3.556 5.08 0)
			)
			(text "75"
				(at -3.556 -2.54 0)
			)
			(text "75"
				(at 1.016 5.08 0)
			)
			(text "75"
				(at 1.016 -2.54 0)
			)
			(text "Y"
				(at 19.558 6.35 0)
			)
			(text "G"
				(at 19.685 -3.81 0)
			)
			(pin passive line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "TD+")
				(number "1")
			)
			(pin passive line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "TCT")
				(number "2")
			)
			(pin passive line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "TD-")
				(number "3")
			)
			(pin passive line
				(at -20.32 0 0)
				(length 2.54)
				(name "RD+")
				(number "4")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RCT")
				(number "5")
			)
			(pin passive line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RD-")
				(number "6")
			)
			(pin power_in line
				(at 10.16 -10.16 90)
				(length 2.54)
				(name "")
				(number "8")
			)
			(pin passive line
				(at 15.24 -10.16 90)
				(length 2.54)
				(name "")
				(number "SH")
			)
			(pin no_connect line
				(at 20.32 0 0)
				(length 0)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "")
				(number "12")
			)
			(pin passive line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "")
				(number "11")
			)
			(pin passive line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "")
				(number "10")
			)
			(pin passive line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RJ45_Wuerth_7499010211A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 17.78 10.16 0)
		)
		(property "Value" "RJ45_Wuerth_7499010211A"
			(at -6.35 10.16 0)
		)
		(property "Footprint" "Connector_RJ:RJ45_Wuerth_7499010211A_Horizontal"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/7499010211A.pdf"
			(at 0 16.51 0)
		)
		(property "Description" "LAN Transformer Jack, RJ45, 10/100 BaseT, tab down"
			(at 0 0 0)
		)
		(property "ki_keywords" "magjack socket ethernet"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RJ45*Wuerth*7499010211A*"
			(at 0 0 0)
		)
		(symbol "RJ45_Wuerth_7499010211A_0_0"
			(text "XMIT"
				(at -8.255 1.905 0)
			)
			(text "RCV"
				(at -8.255 -5.715 0)
			)
			(text "C1"
				(at 4.699 6.985 0)
			)
			(text "C4"
				(at 4.699 5.715 0)
			)
			(text "C5"
				(at 4.699 4.445 0)
			)
			(text "C2"
				(at 4.699 3.175 0)
			)
			(text "C3"
				(at 4.699 -0.635 0)
			)
			(text "C7"
				(at 4.699 -1.905 0)
			)
			(text "C8"
				(at 4.699 -3.175 0)
			)
			(text "C6"
				(at 4.699 -4.445 0)
			)
			(text "C1"
				(at 10.16 -3.175 0)
			)
		)
		(symbol "RJ45_Wuerth_7499010211A_0_1")
		(symbol "RJ45_Wuerth_7499010211A_1_0"
			(text "1000pF"
				(at 3.302 -6.477 0)
			)
		)
		(symbol "RJ45_Wuerth_7499010211A_1_1"
			(text "75"
				(at -3.556 5.08 0)
			)
			(text "75"
				(at -3.556 -2.54 0)
			)
			(text "75"
				(at 1.016 5.08 0)
			)
			(text "75"
				(at 1.016 -2.54 0)
			)
			(text "Y"
				(at 19.558 6.35 0)
			)
			(text "G"
				(at 19.685 -3.81 0)
			)
			(pin passive line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "TD+")
				(number "1")
			)
			(pin passive line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "CTD")
				(number "4")
			)
			(pin passive line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "TD-")
				(number "2")
			)
			(pin passive line
				(at -20.32 0 0)
				(length 2.54)
				(name "RD+")
				(number "3")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "CRD")
				(number "5")
			)
			(pin passive line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RD-")
				(number "6")
			)
			(pin power_in line
				(at 10.16 -10.16 90)
				(length 2.54)
				(name "")
				(number "8")
			)
			(pin passive line
				(at 15.24 -10.16 90)
				(length 2.54)
				(name "")
				(number "SH")
			)
			(pin no_connect line
				(at 20.32 0 0)
				(length 0)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "")
				(number "12")
			)
			(pin passive line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "")
				(number "11")
			)
			(pin passive line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "")
				(number "9")
			)
			(pin passive line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RJ45_Wuerth_7499151120"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 25.4 0)
		)
		(property "Value" "RJ45_Wuerth_7499151120"
			(at 0 22.86 0)
		)
		(property "Footprint" "Connector_RJ:RJ45_Wuerth_7499151120_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "http://katalog.we-online.de/pbs/datasheet/7499151120.pdf"
			(at -6.096 -1.397 0)
		)
		(property "Description" "Dual LAN Transformer Jack, RJ45, 10/100/1000 BaseT"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "dual lan jack socket transformer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RJ45*Wuerth*7499151120*"
			(at 0 0 0)
		)
		(symbol "RJ45_Wuerth_7499151120_0_0"
			(text "J1"
				(at -5.08 11.43 0)
			)
			(text "J2"
				(at -5.08 9.144 0)
			)
			(text "J3"
				(at -5.08 3.556 0)
			)
			(text "J4"
				(at -5.08 1.524 0)
			)
			(text "J5"
				(at -5.08 -4.064 0)
			)
			(text "J6"
				(at -5.08 -6.096 0)
			)
			(text "J7"
				(at -5.08 -11.684 0)
			)
			(text "J8"
				(at -5.08 -13.716 0)
			)
			(text "75"
				(at -0.508 8.382 0)
			)
			(text "75"
				(at -0.508 0.762 0)
			)
			(text "75"
				(at -0.508 -6.858 0)
			)
			(text "75"
				(at -0.508 -14.478 0)
			)
			(text "1000pF 2kV"
				(at 1.27 -16.256 0)
			)
		)
		(symbol "RJ45_Wuerth_7499151120_0_1"
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "~")
				(number "SH")
			)
		)
		(symbol "RJ45_Wuerth_7499151120_1_1"
			(text "G"
				(at -5.08 14.732 0)
			)
			(text "Y"
				(at 0 14.732 0)
			)
			(pin passive line
				(at -5.08 20.32 270)
				(length 2.54)
				(name "~")
				(number "11U")
			)
			(pin passive line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "~")
				(number "12U")
			)
			(pin passive line
				(at 0 20.32 270)
				(length 2.54)
				(name "~")
				(number "14U")
			)
			(pin no_connect line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "10U")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "~")
				(number "13U")
			)
			(pin passive line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "~")
				(number "1U")
			)
			(pin passive line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "~")
				(number "2U")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~")
				(number "3U")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~")
				(number "4U")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "7U")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "5U")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~")
				(number "6U")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "~")
				(number "8U")
			)
			(pin passive line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "~")
				(number "9U")
			)
		)
		(symbol "RJ45_Wuerth_7499151120_2_1"
			(text "G"
				(at -5.08 14.732 0)
			)
			(text "Y"
				(at 0 14.732 0)
			)
			(pin passive line
				(at -5.08 20.32 270)
				(length 2.54)
				(name "~")
				(number "11D")
			)
			(pin passive line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "~")
				(number "12D")
			)
			(pin passive line
				(at 0 20.32 270)
				(length 2.54)
				(name "~")
				(number "14D")
			)
			(pin no_connect line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "10D")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "~")
				(number "13D")
			)
			(pin passive line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "~")
				(number "1D")
			)
			(pin passive line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "~")
				(number "2D")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~")
				(number "3D")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~")
				(number "4D")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "7D")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "5D")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~")
				(number "6D")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "~")
				(number "8D")
			)
			(pin passive line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "~")
				(number "9D")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Raspberry_Pi_2_3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -17.78 31.75 0)
		)
		(property "Value" "Raspberry_Pi_2_3"
			(at 10.16 -31.75 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.raspberrypi.org/documentation/hardware/raspberrypi/schematics/rpi_SCH_3bplus_1p0_reduced.pdf"
			(at 60.96 -44.45 0)
		)
		(property "Description" "expansion header for Raspberry Pi 2 & 3"
			(at 0 0 0)
		)
		(property "ki_keywords" "raspberrypi gpio"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader*2x20*P2.54mm*Vertical* PinSocket*2x20*P2.54mm*Vertical*"
			(at 0 0 0)
		)
		(symbol "Raspberry_Pi_2_3_0_1")
		(symbol "Raspberry_Pi_2_3_1_1"
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "GPIO14/TXD")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "GPIO15/RXD")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "GPIO16")
				(number "36")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "GPIO17")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "GPIO18/PWM0")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "GPIO19/MISO1")
				(number "35")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "GPIO20/MOSI1")
				(number "38")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "GPIO21/SCLK1")
				(number "40")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "GPIO22")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "GPIO23")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "GPIO24")
				(number "18")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "GPIO25")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "GPIO26")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "GPIO27")
				(number "13")
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 2.54)
				(name "5V")
				(number "2")
			)
			(pin passive line
				(at -5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "5V")
				(number "4")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 2.54)
				(name "3V3")
				(number "1")
			)
			(pin passive line
				(at 5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "3V3")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "ID_SD/GPIO0")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "ID_SC/GPIO1")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "SDA/GPIO2")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "SCL/GPIO3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "GCLK0/GPIO4")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "GCLK1/GPIO5")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "GCLK2/GPIO6")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "~{CE1}/GPIO7")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "~{CE0}/GPIO8")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "MISO0/GPIO9")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "MOSI0/GPIO10")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "SCLK0/GPIO11")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PWM0/GPIO12")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PWM1/GPIO13")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Raspberry_Pi_4"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -17.526 48.768 0)
		)
		(property "Value" "Raspberry_Pi_4"
			(at 15.748 -26.416 0)
		)
		(property "Footprint" ""
			(at 70.104 -47.498 0)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/rpi4/raspberry-pi-4-datasheet.pdf"
			(at 15.748 -32.258 0)
		)
		(property "Description" "Raspberry Pi 4 Model B"
			(at 15.748 -29.718 0)
		)
		(property "ki_keywords" "SBC RPi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PinHeader*2x20*P2.54mm*Vertical* PinSocket*2x20*P2.54mm*Vertical*"
			(at 0 0 0)
		)
		(symbol "Raspberry_Pi_4_0_1")
		(symbol "Raspberry_Pi_4_1_1"
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 2.54)
				(name "GPIO12/PWM0")
				(number "32")
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 2.54)
				(name "GPIO13/PWM1")
				(number "33")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 2.54)
				(name "GPIO14/UART_TXD")
				(number "8")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 2.54)
				(name "GPIO15/UART_RXD")
				(number "10")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 2.54)
				(name "GPIO16/SPI1_~{CE2}")
				(number "36")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 2.54)
				(name "GPIO17/SPI1_~{CE1}")
				(number "11")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 2.54)
				(name "GPIO18/SPI1_~{CE0}/PCM_CLK/PWM0")
				(number "12")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 2.54)
				(name "GPIO19/SPI1_MISO/PCM_FS")
				(number "35")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 2.54)
				(name "GPIO20/SPI1_MOSI/PCM_DIN/PWM1")
				(number "38")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 2.54)
				(name "GPIO21/SPI1_SCLK/PCM_DOUT")
				(number "40")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 2.54)
				(name "GPIO22/SDIO_CLK")
				(number "15")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 2.54)
				(name "GPIO23/SDIO_CMD")
				(number "16")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 2.54)
				(name "GPIO24/SDIO_DAT0")
				(number "18")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 2.54)
				(name "GPIO25/SDIO_DAT1")
				(number "22")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 2.54)
				(name "GPIO26/SDIO_DAT2")
				(number "37")
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 2.54)
				(name "GPIO27/SDIO_DAT3")
				(number "13")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin power_out line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 33.02 22.86 180)
				(length 2.54)
				(name "5V")
				(number "2")
			)
			(pin passive line
				(at 33.02 22.86 180)
				(length 2.54)
				(hide yes)
				(name "5V")
				(number "4")
			)
			(pin power_out line
				(at 33.02 20.32 180)
				(length 2.54)
				(name "3V3")
				(number "1")
			)
			(pin passive line
				(at 33.02 20.32 180)
				(length 2.54)
				(hide yes)
				(name "3V3")
				(number "17")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 2.54)
				(name "ID_SD_I2C0/GPIO00")
				(number "27")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 2.54)
				(name "ID_SC_I2C0/GPIO01")
				(number "28")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 2.54)
				(name "SDA_I2C1/GPIO02")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 2.54)
				(name "SCL_I2C1/GPIO03")
				(number "5")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 2.54)
				(name "GPCLK0/GPIO04")
				(number "7")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 2.54)
				(name "GPCLK1/GPIO05")
				(number "29")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 2.54)
				(name "GPCLK2/GPIO06")
				(number "31")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 2.54)
				(name "~{CE1}_SPI0/GPIO07")
				(number "26")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 2.54)
				(name "~{CE0}_SPI0/GPIO08")
				(number "24")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 2.54)
				(name "MISO_SPI0/GPIO09")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 2.54)
				(name "MOSI_SPI0/GPIO10")
				(number "19")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 2.54)
				(name "SCLK_SPI0/GPIO11")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SCART-F"
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 31.75 0)
		)
		(property "Value" "SCART-F"
			(at 1.016 -29.21 0)
		)
		(property "Footprint" ""
			(at 0 1.27 0)
		)
		(property "Datasheet" "~"
			(at 0 1.27 0)
		)
		(property "Description" "Prise Peritel"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(symbol "SCART-F_0_1"
			(text "+"
				(at -1.778 29.21 0)
			)
		)
		(symbol "SCART-F_1_1"
			(pin passive line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "P21")
				(number "21")
			)
			(pin passive line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "P19")
				(number "19")
			)
			(pin passive line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "P17")
				(number "17")
			)
			(pin passive line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "P13")
				(number "13")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 2.54)
				(name "P11")
				(number "11")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "P9")
				(number "9")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "P7")
				(number "7")
			)
			(pin passive line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "P5")
				(number "5")
			)
			(pin passive line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "P3")
				(number "3")
			)
			(pin passive line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "P1")
				(number "1")
			)
			(pin passive line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "P20")
				(number "20")
			)
			(pin passive line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "P18")
				(number "18")
			)
			(pin passive line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "P16")
				(number "16")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "P12")
				(number "12")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "P10")
				(number "10")
			)
			(pin passive line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "P8")
				(number "8")
			)
			(pin passive line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "P6")
				(number "6")
			)
			(pin passive line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "P4")
				(number "4")
			)
			(pin passive line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "P2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SD_Card_Device"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -11.938 17.018 0)
		)
		(property "Value" "SD_Card_Device"
			(at 9.144 -17.272 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.convict.lu/pdf/ProdManualSDCardv1.9.pdf"
			(at 0 0 0)
		)
		(property "Description" "SD card device/card"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector SD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SD*Device*"
			(at 0 0 0)
		)
		(symbol "SD_Card_Device_0_1")
		(symbol "SD_Card_Device_1_1"
			(text "9"
				(at -1.778 3.556 0)
			)
			(text "1"
				(at 0 4.826 0)
			)
			(text "8"
				(at 10.668 4.826 0)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "DAT0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "DAT1")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DAT2")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "CD/DAT3")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CLK")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CMD")
				(number "2")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SD_Card_Receptacle"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -11.938 19.304 0)
		)
		(property "Value" "SD_Card_Receptacle"
			(at 10.922 -19.558 0)
		)
		(property "Footprint" ""
			(at 8.89 -3.302 0)
		)
		(property "Datasheet" "http://portal.fciconnect.com/Comergent//fci/drawing/10067847.pdf"
			(at 0 0 0)
		)
		(property "Description" "SD card receptacle"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector SD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SD*"
			(at 0 0 0)
		)
		(symbol "SD_Card_Receptacle_0_1")
		(symbol "SD_Card_Receptacle_1_1"
			(text "8"
				(at -1.778 1.524 0)
			)
			(text "1"
				(at 8.89 1.524 0)
			)
			(text "9"
				(at 10.668 0.254 0)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "DAT0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "DAT1")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DAT2")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "CD/DAT3")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CLK")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CMD")
				(number "2")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "SHELL1")
				(number "12")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "SHELL2")
				(number "13")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "6")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "CARD_DETECT")
				(number "10")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "WRITE_PROTECT")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SIM_Card"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -2.54 12.7 0)
		)
		(property "Value" "SIM_Card"
			(at -1.27 10.16 0)
		)
		(property "Footprint" ""
			(at 0 8.89 0)
		)
		(property "Datasheet" "~"
			(at -1.27 0 0)
		)
		(property "Description" "SIM Card"
			(at 0 0 0)
		)
		(property "ki_keywords" "SIM card UICC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SIM*Card*Holder*"
			(at 0 0 0)
		)
		(symbol "SIM_Card_0_1")
		(symbol "SIM_Card_1_1"
			(pin power_in line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "RST")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CLK")
				(number "3")
			)
			(pin power_in line
				(at -12.7 0 0)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VPP")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "I/O")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SIM_Card_Shielded"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -2.54 12.7 0)
		)
		(property "Value" "SIM_Card_Shielded"
			(at -1.27 10.16 0)
		)
		(property "Footprint" ""
			(at 0 8.89 0)
		)
		(property "Datasheet" "~"
			(at -1.27 0 0)
		)
		(property "Description" "SIM Card"
			(at 0 0 0)
		)
		(property "ki_keywords" "SIM card UICC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SIM*Card*Holder*"
			(at 0 0 0)
		)
		(symbol "SIM_Card_Shielded_0_1")
		(symbol "SIM_Card_Shielded_1_1"
			(pin power_in line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "RST")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CLK")
				(number "3")
			)
			(pin power_in line
				(at -12.7 0 0)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VPP")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "I/O")
				(number "7")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SH")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SODIMM-200"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 1.27 0)
		)
		(property "Value" "SODIMM-200"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 35.56 97.79 0)
		)
		(property "Datasheet" "~"
			(at 35.56 97.79 0)
		)
		(property "Description" "SODIMM 200 Pin socket"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "SODIMM SO-DIMM DDR1 DDR2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SODIMM*"
			(at 0 0 0)
		)
		(symbol "SODIMM-200_1_1"
			(pin passive line
				(at -17.78 22.86 0)
				(length 5.08)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "13")
				(number "13")
			)
			(pin passive line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "15")
				(number "15")
			)
			(pin passive line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "17")
				(number "17")
			)
			(pin passive line
				(at -17.78 0 0)
				(length 5.08)
				(name "19")
				(number "19")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "21")
				(number "21")
			)
			(pin passive line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "23")
				(number "23")
			)
			(pin passive line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "25")
				(number "25")
			)
			(pin passive line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "27")
				(number "27")
			)
			(pin passive line
				(at -17.78 -12.7 0)
				(length 5.08)
				(name "29")
				(number "29")
			)
			(pin passive line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "31")
				(number "31")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "33")
				(number "33")
			)
			(pin passive line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "35")
				(number "35")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 5.08)
				(name "37")
				(number "37")
			)
			(pin passive line
				(at -17.78 -25.4 0)
				(length 5.08)
				(name "39")
				(number "39")
			)
			(pin passive line
				(at 17.78 22.86 180)
				(length 5.08)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "12")
				(number "12")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "14")
				(number "14")
			)
			(pin passive line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "16")
				(number "16")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "18")
				(number "18")
			)
			(pin passive line
				(at 17.78 0 180)
				(length 5.08)
				(name "20")
				(number "20")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "22")
				(number "22")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "24")
				(number "24")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "26")
				(number "26")
			)
			(pin passive line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "28")
				(number "28")
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "30")
				(number "30")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "32")
				(number "32")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "34")
				(number "34")
			)
			(pin passive line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "36")
				(number "36")
			)
			(pin passive line
				(at 17.78 -22.86 180)
				(length 5.08)
				(name "38")
				(number "38")
			)
			(pin passive line
				(at 17.78 -25.4 180)
				(length 5.08)
				(name "40")
				(number "40")
			)
		)
		(symbol "SODIMM-200_2_1"
			(pin passive line
				(at -17.78 99.06 0)
				(length 5.08)
				(name "41")
				(number "41")
			)
			(pin passive line
				(at -17.78 96.52 0)
				(length 5.08)
				(name "43")
				(number "43")
			)
			(pin passive line
				(at -17.78 93.98 0)
				(length 5.08)
				(name "45")
				(number "45")
			)
			(pin passive line
				(at -17.78 91.44 0)
				(length 5.08)
				(name "47")
				(number "47")
			)
			(pin passive line
				(at -17.78 88.9 0)
				(length 5.08)
				(name "49")
				(number "49")
			)
			(pin passive line
				(at -17.78 86.36 0)
				(length 5.08)
				(name "51")
				(number "51")
			)
			(pin passive line
				(at -17.78 83.82 0)
				(length 5.08)
				(name "53")
				(number "53")
			)
			(pin passive line
				(at -17.78 81.28 0)
				(length 5.08)
				(name "55")
				(number "55")
			)
			(pin passive line
				(at -17.78 78.74 0)
				(length 5.08)
				(name "57")
				(number "57")
			)
			(pin passive line
				(at -17.78 76.2 0)
				(length 5.08)
				(name "59")
				(number "59")
			)
			(pin passive line
				(at -17.78 73.66 0)
				(length 5.08)
				(name "61")
				(number "61")
			)
			(pin passive line
				(at -17.78 71.12 0)
				(length 5.08)
				(name "63")
				(number "63")
			)
			(pin passive line
				(at -17.78 68.58 0)
				(length 5.08)
				(name "65")
				(number "65")
			)
			(pin passive line
				(at -17.78 66.04 0)
				(length 5.08)
				(name "67")
				(number "67")
			)
			(pin passive line
				(at -17.78 63.5 0)
				(length 5.08)
				(name "69")
				(number "69")
			)
			(pin passive line
				(at -17.78 60.96 0)
				(length 5.08)
				(name "71")
				(number "71")
			)
			(pin passive line
				(at -17.78 58.42 0)
				(length 5.08)
				(name "73")
				(number "73")
			)
			(pin passive line
				(at -17.78 55.88 0)
				(length 5.08)
				(name "75")
				(number "75")
			)
			(pin passive line
				(at -17.78 53.34 0)
				(length 5.08)
				(name "77")
				(number "77")
			)
			(pin passive line
				(at -17.78 50.8 0)
				(length 5.08)
				(name "79")
				(number "79")
			)
			(pin passive line
				(at -17.78 48.26 0)
				(length 5.08)
				(name "81")
				(number "81")
			)
			(pin passive line
				(at -17.78 45.72 0)
				(length 5.08)
				(name "83")
				(number "83")
			)
			(pin passive line
				(at -17.78 43.18 0)
				(length 5.08)
				(name "85")
				(number "85")
			)
			(pin passive line
				(at -17.78 40.64 0)
				(length 5.08)
				(name "87")
				(number "87")
			)
			(pin passive line
				(at -17.78 38.1 0)
				(length 5.08)
				(name "89")
				(number "89")
			)
			(pin passive line
				(at -17.78 35.56 0)
				(length 5.08)
				(name "91")
				(number "91")
			)
			(pin passive line
				(at -17.78 33.02 0)
				(length 5.08)
				(name "93")
				(number "93")
			)
			(pin passive line
				(at -17.78 30.48 0)
				(length 5.08)
				(name "95")
				(number "95")
			)
			(pin passive line
				(at -17.78 27.94 0)
				(length 5.08)
				(name "97")
				(number "97")
			)
			(pin passive line
				(at -17.78 25.4 0)
				(length 5.08)
				(name "99")
				(number "99")
			)
			(pin passive line
				(at -17.78 22.86 0)
				(length 5.08)
				(name "101")
				(number "101")
			)
			(pin passive line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "103")
				(number "103")
			)
			(pin passive line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "105")
				(number "105")
			)
			(pin passive line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "107")
				(number "107")
			)
			(pin passive line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "109")
				(number "109")
			)
			(pin passive line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "111")
				(number "111")
			)
			(pin passive line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "113")
				(number "113")
			)
			(pin passive line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "115")
				(number "115")
			)
			(pin passive line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "117")
				(number "117")
			)
			(pin passive line
				(at -17.78 0 0)
				(length 5.08)
				(name "119")
				(number "119")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "121")
				(number "121")
			)
			(pin passive line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "123")
				(number "123")
			)
			(pin passive line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "125")
				(number "125")
			)
			(pin passive line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "127")
				(number "127")
			)
			(pin passive line
				(at -17.78 -12.7 0)
				(length 5.08)
				(name "129")
				(number "129")
			)
			(pin passive line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "131")
				(number "131")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "133")
				(number "133")
			)
			(pin passive line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "135")
				(number "135")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 5.08)
				(name "137")
				(number "137")
			)
			(pin passive line
				(at -17.78 -25.4 0)
				(length 5.08)
				(name "139")
				(number "139")
			)
			(pin passive line
				(at -17.78 -27.94 0)
				(length 5.08)
				(name "141")
				(number "141")
			)
			(pin passive line
				(at -17.78 -30.48 0)
				(length 5.08)
				(name "143")
				(number "143")
			)
			(pin passive line
				(at -17.78 -33.02 0)
				(length 5.08)
				(name "145")
				(number "145")
			)
			(pin passive line
				(at -17.78 -35.56 0)
				(length 5.08)
				(name "147")
				(number "147")
			)
			(pin passive line
				(at -17.78 -38.1 0)
				(length 5.08)
				(name "149")
				(number "149")
			)
			(pin passive line
				(at -17.78 -40.64 0)
				(length 5.08)
				(name "151")
				(number "151")
			)
			(pin passive line
				(at -17.78 -43.18 0)
				(length 5.08)
				(name "153")
				(number "153")
			)
			(pin passive line
				(at -17.78 -45.72 0)
				(length 5.08)
				(name "155")
				(number "155")
			)
			(pin passive line
				(at -17.78 -48.26 0)
				(length 5.08)
				(name "157")
				(number "157")
			)
			(pin passive line
				(at -17.78 -50.8 0)
				(length 5.08)
				(name "159")
				(number "159")
			)
			(pin passive line
				(at -17.78 -53.34 0)
				(length 5.08)
				(name "161")
				(number "161")
			)
			(pin passive line
				(at -17.78 -55.88 0)
				(length 5.08)
				(name "163")
				(number "163")
			)
			(pin passive line
				(at -17.78 -58.42 0)
				(length 5.08)
				(name "165")
				(number "165")
			)
			(pin passive line
				(at -17.78 -60.96 0)
				(length 5.08)
				(name "167")
				(number "167")
			)
			(pin passive line
				(at -17.78 -63.5 0)
				(length 5.08)
				(name "169")
				(number "169")
			)
			(pin passive line
				(at -17.78 -66.04 0)
				(length 5.08)
				(name "171")
				(number "171")
			)
			(pin passive line
				(at -17.78 -68.58 0)
				(length 5.08)
				(name "173")
				(number "173")
			)
			(pin passive line
				(at -17.78 -71.12 0)
				(length 5.08)
				(name "175")
				(number "175")
			)
			(pin passive line
				(at -17.78 -73.66 0)
				(length 5.08)
				(name "177")
				(number "177")
			)
			(pin passive line
				(at -17.78 -76.2 0)
				(length 5.08)
				(name "179")
				(number "179")
			)
			(pin passive line
				(at -17.78 -78.74 0)
				(length 5.08)
				(name "181")
				(number "181")
			)
			(pin passive line
				(at -17.78 -81.28 0)
				(length 5.08)
				(name "183")
				(number "183")
			)
			(pin passive line
				(at -17.78 -83.82 0)
				(length 5.08)
				(name "185")
				(number "185")
			)
			(pin passive line
				(at -17.78 -86.36 0)
				(length 5.08)
				(name "187")
				(number "187")
			)
			(pin passive line
				(at -17.78 -88.9 0)
				(length 5.08)
				(name "189")
				(number "189")
			)
			(pin passive line
				(at -17.78 -91.44 0)
				(length 5.08)
				(name "191")
				(number "191")
			)
			(pin passive line
				(at -17.78 -93.98 0)
				(length 5.08)
				(name "193")
				(number "193")
			)
			(pin passive line
				(at -17.78 -96.52 0)
				(length 5.08)
				(name "195")
				(number "195")
			)
			(pin passive line
				(at -17.78 -99.06 0)
				(length 5.08)
				(name "197")
				(number "197")
			)
			(pin passive line
				(at -17.78 -101.6 0)
				(length 5.08)
				(name "199")
				(number "199")
			)
			(pin passive line
				(at 17.78 99.06 180)
				(length 5.08)
				(name "42")
				(number "42")
			)
			(pin passive line
				(at 17.78 96.52 180)
				(length 5.08)
				(name "44")
				(number "44")
			)
			(pin passive line
				(at 17.78 93.98 180)
				(length 5.08)
				(name "46")
				(number "46")
			)
			(pin passive line
				(at 17.78 91.44 180)
				(length 5.08)
				(name "48")
				(number "48")
			)
			(pin passive line
				(at 17.78 88.9 180)
				(length 5.08)
				(name "50")
				(number "50")
			)
			(pin passive line
				(at 17.78 86.36 180)
				(length 5.08)
				(name "52")
				(number "52")
			)
			(pin passive line
				(at 17.78 83.82 180)
				(length 5.08)
				(name "54")
				(number "54")
			)
			(pin passive line
				(at 17.78 81.28 180)
				(length 5.08)
				(name "56")
				(number "56")
			)
			(pin passive line
				(at 17.78 78.74 180)
				(length 5.08)
				(name "58")
				(number "58")
			)
			(pin passive line
				(at 17.78 76.2 180)
				(length 5.08)
				(name "60")
				(number "60")
			)
			(pin passive line
				(at 17.78 73.66 180)
				(length 5.08)
				(name "62")
				(number "62")
			)
			(pin passive line
				(at 17.78 71.12 180)
				(length 5.08)
				(name "64")
				(number "64")
			)
			(pin passive line
				(at 17.78 68.58 180)
				(length 5.08)
				(name "66")
				(number "66")
			)
			(pin passive line
				(at 17.78 66.04 180)
				(length 5.08)
				(name "68")
				(number "68")
			)
			(pin passive line
				(at 17.78 63.5 180)
				(length 5.08)
				(name "70")
				(number "70")
			)
			(pin passive line
				(at 17.78 60.96 180)
				(length 5.08)
				(name "72")
				(number "72")
			)
			(pin passive line
				(at 17.78 58.42 180)
				(length 5.08)
				(name "74")
				(number "74")
			)
			(pin passive line
				(at 17.78 55.88 180)
				(length 5.08)
				(name "76")
				(number "76")
			)
			(pin passive line
				(at 17.78 53.34 180)
				(length 5.08)
				(name "78")
				(number "78")
			)
			(pin passive line
				(at 17.78 50.8 180)
				(length 5.08)
				(name "80")
				(number "80")
			)
			(pin passive line
				(at 17.78 48.26 180)
				(length 5.08)
				(name "82")
				(number "82")
			)
			(pin passive line
				(at 17.78 45.72 180)
				(length 5.08)
				(name "84")
				(number "84")
			)
			(pin passive line
				(at 17.78 43.18 180)
				(length 5.08)
				(name "86")
				(number "86")
			)
			(pin passive line
				(at 17.78 40.64 180)
				(length 5.08)
				(name "88")
				(number "88")
			)
			(pin passive line
				(at 17.78 38.1 180)
				(length 5.08)
				(name "90")
				(number "90")
			)
			(pin passive line
				(at 17.78 35.56 180)
				(length 5.08)
				(name "92")
				(number "92")
			)
			(pin passive line
				(at 17.78 33.02 180)
				(length 5.08)
				(name "94")
				(number "94")
			)
			(pin passive line
				(at 17.78 30.48 180)
				(length 5.08)
				(name "96")
				(number "96")
			)
			(pin passive line
				(at 17.78 27.94 180)
				(length 5.08)
				(name "98")
				(number "98")
			)
			(pin passive line
				(at 17.78 25.4 180)
				(length 5.08)
				(name "100")
				(number "100")
			)
			(pin passive line
				(at 17.78 22.86 180)
				(length 5.08)
				(name "102")
				(number "102")
			)
			(pin passive line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "104")
				(number "104")
			)
			(pin passive line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "106")
				(number "106")
			)
			(pin passive line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "108")
				(number "108")
			)
			(pin passive line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "110")
				(number "110")
			)
			(pin passive line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "112")
				(number "112")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "114")
				(number "114")
			)
			(pin passive line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "116")
				(number "116")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "118")
				(number "118")
			)
			(pin passive line
				(at 17.78 0 180)
				(length 5.08)
				(name "120")
				(number "120")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "122")
				(number "122")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "124")
				(number "124")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "126")
				(number "126")
			)
			(pin passive line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "128")
				(number "128")
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "130")
				(number "130")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "132")
				(number "132")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "134")
				(number "134")
			)
			(pin passive line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "136")
				(number "136")
			)
			(pin passive line
				(at 17.78 -22.86 180)
				(length 5.08)
				(name "138")
				(number "138")
			)
			(pin passive line
				(at 17.78 -25.4 180)
				(length 5.08)
				(name "140")
				(number "140")
			)
			(pin passive line
				(at 17.78 -27.94 180)
				(length 5.08)
				(name "142")
				(number "142")
			)
			(pin passive line
				(at 17.78 -30.48 180)
				(length 5.08)
				(name "144")
				(number "144")
			)
			(pin passive line
				(at 17.78 -33.02 180)
				(length 5.08)
				(name "146")
				(number "146")
			)
			(pin passive line
				(at 17.78 -35.56 180)
				(length 5.08)
				(name "148")
				(number "148")
			)
			(pin passive line
				(at 17.78 -38.1 180)
				(length 5.08)
				(name "150")
				(number "150")
			)
			(pin passive line
				(at 17.78 -40.64 180)
				(length 5.08)
				(name "152")
				(number "152")
			)
			(pin passive line
				(at 17.78 -43.18 180)
				(length 5.08)
				(name "154")
				(number "154")
			)
			(pin passive line
				(at 17.78 -45.72 180)
				(length 5.08)
				(name "156")
				(number "156")
			)
			(pin passive line
				(at 17.78 -48.26 180)
				(length 5.08)
				(name "158")
				(number "158")
			)
			(pin passive line
				(at 17.78 -50.8 180)
				(length 5.08)
				(name "160")
				(number "160")
			)
			(pin passive line
				(at 17.78 -53.34 180)
				(length 5.08)
				(name "162")
				(number "162")
			)
			(pin passive line
				(at 17.78 -55.88 180)
				(length 5.08)
				(name "164")
				(number "164")
			)
			(pin passive line
				(at 17.78 -58.42 180)
				(length 5.08)
				(name "166")
				(number "166")
			)
			(pin passive line
				(at 17.78 -60.96 180)
				(length 5.08)
				(name "168")
				(number "168")
			)
			(pin passive line
				(at 17.78 -63.5 180)
				(length 5.08)
				(name "170")
				(number "170")
			)
			(pin passive line
				(at 17.78 -66.04 180)
				(length 5.08)
				(name "172")
				(number "172")
			)
			(pin passive line
				(at 17.78 -68.58 180)
				(length 5.08)
				(name "174")
				(number "174")
			)
			(pin passive line
				(at 17.78 -71.12 180)
				(length 5.08)
				(name "176")
				(number "176")
			)
			(pin passive line
				(at 17.78 -73.66 180)
				(length 5.08)
				(name "178")
				(number "178")
			)
			(pin passive line
				(at 17.78 -76.2 180)
				(length 5.08)
				(name "180")
				(number "180")
			)
			(pin passive line
				(at 17.78 -78.74 180)
				(length 5.08)
				(name "182")
				(number "182")
			)
			(pin passive line
				(at 17.78 -81.28 180)
				(length 5.08)
				(name "184")
				(number "184")
			)
			(pin passive line
				(at 17.78 -83.82 180)
				(length 5.08)
				(name "186")
				(number "186")
			)
			(pin passive line
				(at 17.78 -86.36 180)
				(length 5.08)
				(name "188")
				(number "188")
			)
			(pin passive line
				(at 17.78 -88.9 180)
				(length 5.08)
				(name "190")
				(number "190")
			)
			(pin passive line
				(at 17.78 -91.44 180)
				(length 5.08)
				(name "192")
				(number "192")
			)
			(pin passive line
				(at 17.78 -93.98 180)
				(length 5.08)
				(name "194")
				(number "194")
			)
			(pin passive line
				(at 17.78 -96.52 180)
				(length 5.08)
				(name "196")
				(number "196")
			)
			(pin passive line
				(at 17.78 -99.06 180)
				(length 5.08)
				(name "198")
				(number "198")
			)
			(pin passive line
				(at 17.78 -101.6 180)
				(length 5.08)
				(name "200")
				(number "200")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SODIMM-200_Split"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 1.27 0)
		)
		(property "Value" "SODIMM-200_Split"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 35.56 21.59 0)
		)
		(property "Datasheet" "~"
			(at 35.56 21.59 0)
		)
		(property "Description" "SODIMM 200 Pin socket"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "SODIMM SO-DIMM DDR1 DDR2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SODIMM*"
			(at 0 0 0)
		)
		(symbol "SODIMM-200_Split_1_1"
			(pin passive line
				(at -17.78 22.86 0)
				(length 5.08)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "13")
				(number "13")
			)
			(pin passive line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "15")
				(number "15")
			)
			(pin passive line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "17")
				(number "17")
			)
			(pin passive line
				(at -17.78 0 0)
				(length 5.08)
				(name "19")
				(number "19")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "21")
				(number "21")
			)
			(pin passive line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "23")
				(number "23")
			)
			(pin passive line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "25")
				(number "25")
			)
			(pin passive line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "27")
				(number "27")
			)
			(pin passive line
				(at -17.78 -12.7 0)
				(length 5.08)
				(name "29")
				(number "29")
			)
			(pin passive line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "31")
				(number "31")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "33")
				(number "33")
			)
			(pin passive line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "35")
				(number "35")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 5.08)
				(name "37")
				(number "37")
			)
			(pin passive line
				(at -17.78 -25.4 0)
				(length 5.08)
				(name "39")
				(number "39")
			)
			(pin passive line
				(at 17.78 22.86 180)
				(length 5.08)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "12")
				(number "12")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "14")
				(number "14")
			)
			(pin passive line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "16")
				(number "16")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "18")
				(number "18")
			)
			(pin passive line
				(at 17.78 0 180)
				(length 5.08)
				(name "20")
				(number "20")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "22")
				(number "22")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "24")
				(number "24")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "26")
				(number "26")
			)
			(pin passive line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "28")
				(number "28")
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "30")
				(number "30")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "32")
				(number "32")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "34")
				(number "34")
			)
			(pin passive line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "36")
				(number "36")
			)
			(pin passive line
				(at 17.78 -22.86 180)
				(length 5.08)
				(name "38")
				(number "38")
			)
			(pin passive line
				(at 17.78 -25.4 180)
				(length 5.08)
				(name "40")
				(number "40")
			)
		)
		(symbol "SODIMM-200_Split_2_1"
			(pin passive line
				(at -17.78 22.86 0)
				(length 5.08)
				(name "41")
				(number "41")
			)
			(pin passive line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "43")
				(number "43")
			)
			(pin passive line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "45")
				(number "45")
			)
			(pin passive line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "47")
				(number "47")
			)
			(pin passive line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "49")
				(number "49")
			)
			(pin passive line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "51")
				(number "51")
			)
			(pin passive line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "53")
				(number "53")
			)
			(pin passive line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "55")
				(number "55")
			)
			(pin passive line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "57")
				(number "57")
			)
			(pin passive line
				(at -17.78 0 0)
				(length 5.08)
				(name "59")
				(number "59")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "61")
				(number "61")
			)
			(pin passive line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "63")
				(number "63")
			)
			(pin passive line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "65")
				(number "65")
			)
			(pin passive line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "67")
				(number "67")
			)
			(pin passive line
				(at -17.78 -12.7 0)
				(length 5.08)
				(name "69")
				(number "69")
			)
			(pin passive line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "71")
				(number "71")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "73")
				(number "73")
			)
			(pin passive line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "75")
				(number "75")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 5.08)
				(name "77")
				(number "77")
			)
			(pin passive line
				(at -17.78 -25.4 0)
				(length 5.08)
				(name "79")
				(number "79")
			)
			(pin passive line
				(at 17.78 22.86 180)
				(length 5.08)
				(name "42")
				(number "42")
			)
			(pin passive line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "44")
				(number "44")
			)
			(pin passive line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "46")
				(number "46")
			)
			(pin passive line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "48")
				(number "48")
			)
			(pin passive line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "50")
				(number "50")
			)
			(pin passive line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "52")
				(number "52")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "54")
				(number "54")
			)
			(pin passive line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "56")
				(number "56")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "58")
				(number "58")
			)
			(pin passive line
				(at 17.78 0 180)
				(length 5.08)
				(name "60")
				(number "60")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "62")
				(number "62")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "64")
				(number "64")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "66")
				(number "66")
			)
			(pin passive line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "68")
				(number "68")
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "70")
				(number "70")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "72")
				(number "72")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "74")
				(number "74")
			)
			(pin passive line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "76")
				(number "76")
			)
			(pin passive line
				(at 17.78 -22.86 180)
				(length 5.08)
				(name "78")
				(number "78")
			)
			(pin passive line
				(at 17.78 -25.4 180)
				(length 5.08)
				(name "80")
				(number "80")
			)
		)
		(symbol "SODIMM-200_Split_3_1"
			(pin passive line
				(at -17.78 22.86 0)
				(length 5.08)
				(name "81")
				(number "81")
			)
			(pin passive line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "83")
				(number "83")
			)
			(pin passive line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "85")
				(number "85")
			)
			(pin passive line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "87")
				(number "87")
			)
			(pin passive line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "89")
				(number "89")
			)
			(pin passive line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "91")
				(number "91")
			)
			(pin passive line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "93")
				(number "93")
			)
			(pin passive line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "95")
				(number "95")
			)
			(pin passive line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "97")
				(number "97")
			)
			(pin passive line
				(at -17.78 0 0)
				(length 5.08)
				(name "99")
				(number "99")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "101")
				(number "101")
			)
			(pin passive line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "103")
				(number "103")
			)
			(pin passive line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "105")
				(number "105")
			)
			(pin passive line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "107")
				(number "107")
			)
			(pin passive line
				(at -17.78 -12.7 0)
				(length 5.08)
				(name "109")
				(number "109")
			)
			(pin passive line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "111")
				(number "111")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "113")
				(number "113")
			)
			(pin passive line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "115")
				(number "115")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 5.08)
				(name "117")
				(number "117")
			)
			(pin passive line
				(at -17.78 -25.4 0)
				(length 5.08)
				(name "119")
				(number "119")
			)
			(pin passive line
				(at 17.78 22.86 180)
				(length 5.08)
				(name "82")
				(number "82")
			)
			(pin passive line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "84")
				(number "84")
			)
			(pin passive line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "86")
				(number "86")
			)
			(pin passive line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "88")
				(number "88")
			)
			(pin passive line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "90")
				(number "90")
			)
			(pin passive line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "92")
				(number "92")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "94")
				(number "94")
			)
			(pin passive line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "96")
				(number "96")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "98")
				(number "98")
			)
			(pin passive line
				(at 17.78 0 180)
				(length 5.08)
				(name "100")
				(number "100")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "102")
				(number "102")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "104")
				(number "104")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "106")
				(number "106")
			)
			(pin passive line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "108")
				(number "108")
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "110")
				(number "110")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "112")
				(number "112")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "114")
				(number "114")
			)
			(pin passive line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "116")
				(number "116")
			)
			(pin passive line
				(at 17.78 -22.86 180)
				(length 5.08)
				(name "118")
				(number "118")
			)
			(pin passive line
				(at 17.78 -25.4 180)
				(length 5.08)
				(name "120")
				(number "120")
			)
		)
		(symbol "SODIMM-200_Split_4_1"
			(pin passive line
				(at -17.78 22.86 0)
				(length 5.08)
				(name "121")
				(number "121")
			)
			(pin passive line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "123")
				(number "123")
			)
			(pin passive line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "125")
				(number "125")
			)
			(pin passive line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "127")
				(number "127")
			)
			(pin passive line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "129")
				(number "129")
			)
			(pin passive line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "131")
				(number "131")
			)
			(pin passive line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "133")
				(number "133")
			)
			(pin passive line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "135")
				(number "135")
			)
			(pin passive line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "137")
				(number "137")
			)
			(pin passive line
				(at -17.78 0 0)
				(length 5.08)
				(name "139")
				(number "139")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "141")
				(number "141")
			)
			(pin passive line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "143")
				(number "143")
			)
			(pin passive line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "145")
				(number "145")
			)
			(pin passive line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "147")
				(number "147")
			)
			(pin passive line
				(at -17.78 -12.7 0)
				(length 5.08)
				(name "149")
				(number "149")
			)
			(pin passive line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "151")
				(number "151")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "153")
				(number "153")
			)
			(pin passive line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "155")
				(number "155")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 5.08)
				(name "157")
				(number "157")
			)
			(pin passive line
				(at -17.78 -25.4 0)
				(length 5.08)
				(name "159")
				(number "159")
			)
			(pin passive line
				(at 17.78 22.86 180)
				(length 5.08)
				(name "122")
				(number "122")
			)
			(pin passive line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "124")
				(number "124")
			)
			(pin passive line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "126")
				(number "126")
			)
			(pin passive line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "128")
				(number "128")
			)
			(pin passive line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "130")
				(number "130")
			)
			(pin passive line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "132")
				(number "132")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "134")
				(number "134")
			)
			(pin passive line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "136")
				(number "136")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "138")
				(number "138")
			)
			(pin passive line
				(at 17.78 0 180)
				(length 5.08)
				(name "140")
				(number "140")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "142")
				(number "142")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "144")
				(number "144")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "146")
				(number "146")
			)
			(pin passive line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "148")
				(number "148")
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "150")
				(number "150")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "152")
				(number "152")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "154")
				(number "154")
			)
			(pin passive line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "156")
				(number "156")
			)
			(pin passive line
				(at 17.78 -22.86 180)
				(length 5.08)
				(name "158")
				(number "158")
			)
			(pin passive line
				(at 17.78 -25.4 180)
				(length 5.08)
				(name "160")
				(number "160")
			)
		)
		(symbol "SODIMM-200_Split_5_1"
			(pin passive line
				(at -17.78 22.86 0)
				(length 5.08)
				(name "161")
				(number "161")
			)
			(pin passive line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "163")
				(number "163")
			)
			(pin passive line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "165")
				(number "165")
			)
			(pin passive line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "167")
				(number "167")
			)
			(pin passive line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "169")
				(number "169")
			)
			(pin passive line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "171")
				(number "171")
			)
			(pin passive line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "173")
				(number "173")
			)
			(pin passive line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "175")
				(number "175")
			)
			(pin passive line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "177")
				(number "177")
			)
			(pin passive line
				(at -17.78 0 0)
				(length 5.08)
				(name "179")
				(number "179")
			)
			(pin passive line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "181")
				(number "181")
			)
			(pin passive line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "183")
				(number "183")
			)
			(pin passive line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "185")
				(number "185")
			)
			(pin passive line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "187")
				(number "187")
			)
			(pin passive line
				(at -17.78 -12.7 0)
				(length 5.08)
				(name "189")
				(number "189")
			)
			(pin passive line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "191")
				(number "191")
			)
			(pin passive line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "193")
				(number "193")
			)
			(pin passive line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "195")
				(number "195")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 5.08)
				(name "197")
				(number "197")
			)
			(pin passive line
				(at -17.78 -25.4 0)
				(length 5.08)
				(name "199")
				(number "199")
			)
			(pin passive line
				(at 17.78 22.86 180)
				(length 5.08)
				(name "162")
				(number "162")
			)
			(pin passive line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "164")
				(number "164")
			)
			(pin passive line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "166")
				(number "166")
			)
			(pin passive line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "168")
				(number "168")
			)
			(pin passive line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "170")
				(number "170")
			)
			(pin passive line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "172")
				(number "172")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "174")
				(number "174")
			)
			(pin passive line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "176")
				(number "176")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "178")
				(number "178")
			)
			(pin passive line
				(at 17.78 0 180)
				(length 5.08)
				(name "180")
				(number "180")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "182")
				(number "182")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "184")
				(number "184")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "186")
				(number "186")
			)
			(pin passive line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "188")
				(number "188")
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "190")
				(number "190")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "192")
				(number "192")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "194")
				(number "194")
			)
			(pin passive line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "196")
				(number "196")
			)
			(pin passive line
				(at 17.78 -22.86 180)
				(length 5.08)
				(name "198")
				(number "198")
			)
			(pin passive line
				(at 17.78 -25.4 180)
				(length 5.08)
				(name "200")
				(number "200")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Samtec_ASP-134602-01"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 50.8 0)
		)
		(property "Value" "Samtec_ASP-134602-01"
			(at 0 -53.34 0)
		)
		(property "Footprint" ""
			(at 1.27 54.61 0)
		)
		(property "Datasheet" "http://suddendocs.samtec.com/prints/asp-134602-01-mkt.pdf"
			(at 3.81 53.34 0)
		)
		(property "Description" "Connector array, 10x40, 1.27mm pitch, mezzanine-card, plug, gold finish, VITA 57.1 FMC, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA Mezzanine Card FMC Terminal Connector Header"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*FMC*ASP*134602?01*10x40*P1.27mm* *FMC*ASP*134486?01*10x40*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "Samtec_ASP-134602-01_1_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_1")
				(number "A1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_2")
				(number "A2")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_3")
				(number "A3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_4")
				(number "A4")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_5")
				(number "A5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_6")
				(number "A6")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_7")
				(number "A7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_8")
				(number "A8")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_9")
				(number "A9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_10")
				(number "A10")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_11")
				(number "A11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_12")
				(number "A12")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_13")
				(number "A13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_14")
				(number "A14")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_15")
				(number "A15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_16")
				(number "A16")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_17")
				(number "A17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_18")
				(number "A18")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_19")
				(number "A19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_20")
				(number "A20")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_21")
				(number "A21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_22")
				(number "A22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_23")
				(number "A23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_24")
				(number "A24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_25")
				(number "A25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_26")
				(number "A26")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_27")
				(number "A27")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_28")
				(number "A28")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_29")
				(number "A29")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_30")
				(number "A30")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_31")
				(number "A31")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_32")
				(number "A32")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_33")
				(number "A33")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_34")
				(number "A34")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_35")
				(number "A35")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_36")
				(number "A36")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_37")
				(number "A37")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_38")
				(number "A38")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_39")
				(number "A39")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_40")
				(number "A40")
			)
		)
		(symbol "Samtec_ASP-134602-01_2_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_1")
				(number "B1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_2")
				(number "B2")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_3")
				(number "B3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_4")
				(number "B4")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_5")
				(number "B5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_6")
				(number "B6")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_7")
				(number "B7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_8")
				(number "B8")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_9")
				(number "B9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_10")
				(number "B10")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_11")
				(number "B11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_12")
				(number "B12")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_13")
				(number "B13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_14")
				(number "B14")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_15")
				(number "B15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_16")
				(number "B16")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_17")
				(number "B17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_18")
				(number "B18")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_19")
				(number "B19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_20")
				(number "B20")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_21")
				(number "B21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_22")
				(number "B22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_23")
				(number "B23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_24")
				(number "B24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_25")
				(number "B25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_26")
				(number "B26")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_27")
				(number "B27")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_28")
				(number "B28")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_29")
				(number "B29")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_30")
				(number "B30")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_31")
				(number "B31")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_32")
				(number "B32")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_33")
				(number "B33")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_34")
				(number "B34")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_35")
				(number "B35")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_36")
				(number "B36")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_37")
				(number "B37")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_38")
				(number "B38")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_39")
				(number "B39")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_40")
				(number "B40")
			)
		)
		(symbol "Samtec_ASP-134602-01_3_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_1")
				(number "C1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_2")
				(number "C2")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_3")
				(number "C3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_4")
				(number "C4")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_5")
				(number "C5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_6")
				(number "C6")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_7")
				(number "C7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_8")
				(number "C8")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_9")
				(number "C9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_10")
				(number "C10")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_11")
				(number "C11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_12")
				(number "C12")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_13")
				(number "C13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_14")
				(number "C14")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_15")
				(number "C15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_16")
				(number "C16")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_17")
				(number "C17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_18")
				(number "C18")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_19")
				(number "C19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_20")
				(number "C20")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_21")
				(number "C21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_22")
				(number "C22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_23")
				(number "C23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_24")
				(number "C24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_25")
				(number "C25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_26")
				(number "C26")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_27")
				(number "C27")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_28")
				(number "C28")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_29")
				(number "C29")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_30")
				(number "C30")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_31")
				(number "C31")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_32")
				(number "C32")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_33")
				(number "C33")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_34")
				(number "C34")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_35")
				(number "C35")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_36")
				(number "C36")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_37")
				(number "C37")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_38")
				(number "C38")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_39")
				(number "C39")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_40")
				(number "C40")
			)
		)
		(symbol "Samtec_ASP-134602-01_4_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_1")
				(number "D1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_2")
				(number "D2")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_3")
				(number "D3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_4")
				(number "D4")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_5")
				(number "D5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_6")
				(number "D6")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_7")
				(number "D7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_8")
				(number "D8")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_9")
				(number "D9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_10")
				(number "D10")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_11")
				(number "D11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_12")
				(number "D12")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_13")
				(number "D13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_14")
				(number "D14")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_15")
				(number "D15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_16")
				(number "D16")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_17")
				(number "D17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_18")
				(number "D18")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_19")
				(number "D19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_20")
				(number "D20")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_21")
				(number "D21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_22")
				(number "D22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_23")
				(number "D23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_24")
				(number "D24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_25")
				(number "D25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_26")
				(number "D26")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_27")
				(number "D27")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_28")
				(number "D28")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_29")
				(number "D29")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_30")
				(number "D30")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_31")
				(number "D31")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_32")
				(number "D32")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_33")
				(number "D33")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_34")
				(number "D34")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_35")
				(number "D35")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_36")
				(number "D36")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_37")
				(number "D37")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_38")
				(number "D38")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_39")
				(number "D39")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_40")
				(number "D40")
			)
		)
		(symbol "Samtec_ASP-134602-01_5_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_1")
				(number "E1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_2")
				(number "E2")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_3")
				(number "E3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_4")
				(number "E4")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_5")
				(number "E5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_6")
				(number "E6")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_7")
				(number "E7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_8")
				(number "E8")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_9")
				(number "E9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_10")
				(number "E10")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_11")
				(number "E11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_12")
				(number "E12")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_13")
				(number "E13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_14")
				(number "E14")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_15")
				(number "E15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_16")
				(number "E16")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_17")
				(number "E17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_18")
				(number "E18")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_19")
				(number "E19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_20")
				(number "E20")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_21")
				(number "E21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_22")
				(number "E22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_23")
				(number "E23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_24")
				(number "E24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_25")
				(number "E25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_26")
				(number "E26")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_27")
				(number "E27")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_28")
				(number "E28")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_29")
				(number "E29")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_30")
				(number "E30")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_31")
				(number "E31")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_32")
				(number "E32")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_33")
				(number "E33")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_34")
				(number "E34")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_35")
				(number "E35")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_36")
				(number "E36")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_37")
				(number "E37")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_38")
				(number "E38")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_39")
				(number "E39")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_40")
				(number "E40")
			)
		)
		(symbol "Samtec_ASP-134602-01_6_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_1")
				(number "F1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_2")
				(number "F2")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_3")
				(number "F3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_4")
				(number "F4")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_5")
				(number "F5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_6")
				(number "F6")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_7")
				(number "F7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_8")
				(number "F8")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_9")
				(number "F9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_10")
				(number "F10")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_11")
				(number "F11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_12")
				(number "F12")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_13")
				(number "F13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_14")
				(number "F14")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_15")
				(number "F15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_16")
				(number "F16")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_17")
				(number "F17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_18")
				(number "F18")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_19")
				(number "F19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_20")
				(number "F20")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_21")
				(number "F21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_22")
				(number "F22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_23")
				(number "F23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_24")
				(number "F24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_25")
				(number "F25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_26")
				(number "F26")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_27")
				(number "F27")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_28")
				(number "F28")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_29")
				(number "F29")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_30")
				(number "F30")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_31")
				(number "F31")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_32")
				(number "F32")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_33")
				(number "F33")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_34")
				(number "F34")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_35")
				(number "F35")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_36")
				(number "F36")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_37")
				(number "F37")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_38")
				(number "F38")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_39")
				(number "F39")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_40")
				(number "F40")
			)
		)
		(symbol "Samtec_ASP-134602-01_7_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_1")
				(number "G1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_2")
				(number "G2")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_3")
				(number "G3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_4")
				(number "G4")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_5")
				(number "G5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_6")
				(number "G6")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_7")
				(number "G7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_8")
				(number "G8")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_9")
				(number "G9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_10")
				(number "G10")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_11")
				(number "G11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_12")
				(number "G12")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_13")
				(number "G13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_14")
				(number "G14")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_15")
				(number "G15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_16")
				(number "G16")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_17")
				(number "G17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_18")
				(number "G18")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_19")
				(number "G19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_20")
				(number "G20")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_21")
				(number "G21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_22")
				(number "G22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_23")
				(number "G23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_24")
				(number "G24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_25")
				(number "G25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_26")
				(number "G26")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_27")
				(number "G27")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_28")
				(number "G28")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_29")
				(number "G29")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_30")
				(number "G30")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_31")
				(number "G31")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_32")
				(number "G32")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_33")
				(number "G33")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_34")
				(number "G34")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_35")
				(number "G35")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_36")
				(number "G36")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_37")
				(number "G37")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_38")
				(number "G38")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_39")
				(number "G39")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_40")
				(number "G40")
			)
		)
		(symbol "Samtec_ASP-134602-01_8_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_1")
				(number "H1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_2")
				(number "H2")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_3")
				(number "H3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_4")
				(number "H4")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_5")
				(number "H5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_6")
				(number "H6")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_7")
				(number "H7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_8")
				(number "H8")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_9")
				(number "H9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_10")
				(number "H10")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_11")
				(number "H11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_12")
				(number "H12")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_13")
				(number "H13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_14")
				(number "H14")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_15")
				(number "H15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_16")
				(number "H16")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_17")
				(number "H17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_18")
				(number "H18")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_19")
				(number "H19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_20")
				(number "H20")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_21")
				(number "H21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_22")
				(number "H22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_23")
				(number "H23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_24")
				(number "H24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_25")
				(number "H25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_26")
				(number "H26")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_27")
				(number "H27")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_28")
				(number "H28")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_29")
				(number "H29")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_30")
				(number "H30")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_31")
				(number "H31")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_32")
				(number "H32")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_33")
				(number "H33")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_34")
				(number "H34")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_35")
				(number "H35")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_36")
				(number "H36")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_37")
				(number "H37")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_38")
				(number "H38")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_39")
				(number "H39")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_40")
				(number "H40")
			)
		)
		(symbol "Samtec_ASP-134602-01_9_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_1")
				(number "J1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_2")
				(number "J2")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_3")
				(number "J3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_4")
				(number "J4")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_5")
				(number "J5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_6")
				(number "J6")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_7")
				(number "J7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_8")
				(number "J8")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_9")
				(number "J9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_10")
				(number "J10")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_11")
				(number "J11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_12")
				(number "J12")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_13")
				(number "J13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_14")
				(number "J14")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_15")
				(number "J15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_16")
				(number "J16")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_17")
				(number "J17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_18")
				(number "J18")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_19")
				(number "J19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_20")
				(number "J20")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_21")
				(number "J21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_22")
				(number "J22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_23")
				(number "J23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_24")
				(number "J24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_25")
				(number "J25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_26")
				(number "J26")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_27")
				(number "J27")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_28")
				(number "J28")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_29")
				(number "J29")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_30")
				(number "J30")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_31")
				(number "J31")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_32")
				(number "J32")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_33")
				(number "J33")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_34")
				(number "J34")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_35")
				(number "J35")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_36")
				(number "J36")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_37")
				(number "J37")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_38")
				(number "J38")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_39")
				(number "J39")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_40")
				(number "J40")
			)
		)
		(symbol "Samtec_ASP-134602-01_10_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 3.81)
				(name "Pin_1")
				(number "K1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 3.81)
				(name "Pin_2")
				(number "K2")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 3.81)
				(name "Pin_3")
				(number "K3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 3.81)
				(name "Pin_4")
				(number "K4")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 3.81)
				(name "Pin_5")
				(number "K5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 3.81)
				(name "Pin_6")
				(number "K6")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 3.81)
				(name "Pin_7")
				(number "K7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 3.81)
				(name "Pin_8")
				(number "K8")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 3.81)
				(name "Pin_9")
				(number "K9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 3.81)
				(name "Pin_10")
				(number "K10")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_11")
				(number "K11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_12")
				(number "K12")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_13")
				(number "K13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_14")
				(number "K14")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_15")
				(number "K15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_16")
				(number "K16")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_17")
				(number "K17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_18")
				(number "K18")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_19")
				(number "K19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_20")
				(number "K20")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_21")
				(number "K21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_22")
				(number "K22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_23")
				(number "K23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_24")
				(number "K24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_25")
				(number "K25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_26")
				(number "K26")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_27")
				(number "K27")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_28")
				(number "K28")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_29")
				(number "K29")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_30")
				(number "K30")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 3.81)
				(name "Pin_31")
				(number "K31")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 3.81)
				(name "Pin_32")
				(number "K32")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 3.81)
				(name "Pin_33")
				(number "K33")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 3.81)
				(name "Pin_34")
				(number "K34")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 3.81)
				(name "Pin_35")
				(number "K35")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 3.81)
				(name "Pin_36")
				(number "K36")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 3.81)
				(name "Pin_37")
				(number "K37")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 3.81)
				(name "Pin_38")
				(number "K38")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 3.81)
				(name "Pin_39")
				(number "K39")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 3.81)
				(name "Pin_40")
				(number "K40")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Screw_Terminal_01x01"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 2.54 0)
		)
		(property "Value" "Screw_Terminal_01x01"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic screw terminal, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "screw terminal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TerminalBlock*:*"
			(at 0 0 0)
		)
		(symbol "Screw_Terminal_01x01_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Screw_Terminal_01x02"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 2.54 0)
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "screw terminal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TerminalBlock*:*"
			(at 0 0 0)
		)
		(symbol "Screw_Terminal_01x02_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Screw_Terminal_01x03"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 5.08 0)
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic screw terminal, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "screw terminal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TerminalBlock*:*"
			(at 0 0 0)
		)
		(symbol "Screw_Terminal_01x03_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Screw_Terminal_01x04"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 5.08 0)
		)
		(property "Value" "Screw_Terminal_01x04"
			(at 0 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic screw terminal, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "screw terminal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TerminalBlock*:*"
			(at 0 0 0)
		)
		(symbol "Screw_Terminal_01x04_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Screw_Terminal_01x05"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 7.62 0)
		)
		(property "Value" "Screw_Terminal_01x05"
			(at 0 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic screw terminal, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "screw terminal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TerminalBlock*:*"
			(at 0 0 0)
		)
		(symbol "Screw_Terminal_01x05_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Screw_Terminal_01x06"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 7.62 0)
		)
		(property "Value" "Screw_Terminal_01x06"
			(at 0 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic screw terminal, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "screw terminal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TerminalBlock*:*"
			(at 0 0 0)
		)
		(symbol "Screw_Terminal_01x06_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Screw_Terminal_01x07"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "Screw_Terminal_01x07"
			(at 0 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic screw terminal, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "screw terminal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TerminalBlock*:*"
			(at 0 0 0)
		)
		(symbol "Screw_Terminal_01x07_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Screw_Terminal_01x08"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "Screw_Terminal_01x08"
			(at 0 -12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic screw terminal, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "screw terminal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TerminalBlock*:*"
			(at 0 0 0)
		)
		(symbol "Screw_Terminal_01x08_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Screw_Terminal_01x09"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 12.7 0)
		)
		(property "Value" "Screw_Terminal_01x09"
			(at 0 -12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic screw terminal, single row, 01x09, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "screw terminal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TerminalBlock*:*"
			(at 0 0 0)
		)
		(symbol "Screw_Terminal_01x09_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Screw_Terminal_01x10"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 12.7 0)
		)
		(property "Value" "Screw_Terminal_01x10"
			(at 0 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic screw terminal, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "screw terminal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TerminalBlock*:*"
			(at 0 0 0)
		)
		(symbol "Screw_Terminal_01x10_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Screw_Terminal_01x11"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 15.24 0)
		)
		(property "Value" "Screw_Terminal_01x11"
			(at 0 -15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic screw terminal, single row, 01x11, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "screw terminal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TerminalBlock*:*"
			(at 0 0 0)
		)
		(symbol "Screw_Terminal_01x11_1_1"
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Screw_Terminal_01x12"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 15.24 0)
		)
		(property "Value" "Screw_Terminal_01x12"
			(at 0 -17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic screw terminal, single row, 01x12, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "screw terminal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TerminalBlock*:*"
			(at 0 0 0)
		)
		(symbol "Screw_Terminal_01x12_1_1"
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Screw_Terminal_01x13"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 17.78 0)
		)
		(property "Value" "Screw_Terminal_01x13"
			(at 0 -17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic screw terminal, single row, 01x13, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "screw terminal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TerminalBlock*:*"
			(at 0 0 0)
		)
		(symbol "Screw_Terminal_01x13_1_1"
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Screw_Terminal_01x14"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 17.78 0)
		)
		(property "Value" "Screw_Terminal_01x14"
			(at 0 -20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic screw terminal, single row, 01x14, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "screw terminal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TerminalBlock*:*"
			(at 0 0 0)
		)
		(symbol "Screw_Terminal_01x14_1_1"
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Screw_Terminal_01x15"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 20.32 0)
		)
		(property "Value" "Screw_Terminal_01x15"
			(at 0 -20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic screw terminal, single row, 01x15, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "screw terminal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TerminalBlock*:*"
			(at 0 0 0)
		)
		(symbol "Screw_Terminal_01x15_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Screw_Terminal_01x16"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 20.32 0)
		)
		(property "Value" "Screw_Terminal_01x16"
			(at 0 -22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic screw terminal, single row, 01x16, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "screw terminal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TerminalBlock*:*"
			(at 0 0 0)
		)
		(symbol "Screw_Terminal_01x16_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Screw_Terminal_01x17"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 22.86 0)
		)
		(property "Value" "Screw_Terminal_01x17"
			(at 0 -22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic screw terminal, single row, 01x17, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "screw terminal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TerminalBlock*:*"
			(at 0 0 0)
		)
		(symbol "Screw_Terminal_01x17_1_1"
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Screw_Terminal_01x18"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 22.86 0)
		)
		(property "Value" "Screw_Terminal_01x18"
			(at 0 -25.4 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic screw terminal, single row, 01x18, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "screw terminal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TerminalBlock*:*"
			(at 0 0 0)
		)
		(symbol "Screw_Terminal_01x18_1_1"
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Screw_Terminal_01x19"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 25.4 0)
		)
		(property "Value" "Screw_Terminal_01x19"
			(at 0 -25.4 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic screw terminal, single row, 01x19, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "screw terminal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TerminalBlock*:*"
			(at 0 0 0)
		)
		(symbol "Screw_Terminal_01x19_1_1"
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Screw_Terminal_01x20"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 25.4 0)
		)
		(property "Value" "Screw_Terminal_01x20"
			(at 0 -27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic screw terminal, single row, 01x20, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "screw terminal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TerminalBlock*:*"
			(at 0 0 0)
		)
		(symbol "Screw_Terminal_01x20_1_1"
			(pin passive line
				(at -5.08 22.86 0)
				(length 3.81)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 3.81)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 3.81)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 3.81)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 3.81)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 3.81)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 3.81)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 3.81)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 3.81)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 3.81)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 3.81)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 3.81)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 3.81)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 3.81)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 3.81)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 3.81)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 3.81)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 3.81)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 3.81)
				(name "Pin_20")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TC2030"
		(exclude_from_sim no)
		(in_bom no)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 8.89 0)
		)
		(property "Value" "TC2030"
			(at 1.27 -8.89 0)
		)
		(property "Footprint" "Connector:Tag-Connect_TC2030-IDC-NL_2x03_P1.27mm_Vertical"
			(at 1.27 0 0)
		)
		(property "Datasheet" "https://www.tag-connect.com/wp-content/uploads/bsk-pdf-manager/2019/12/TC2030-IDC-NL-Datasheet-Rev-B.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "Tag-Connect’s 6-pins connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "Debug plug-of-nails"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TC2030*"
			(at 0 0 0)
		)
		(symbol "TC2030_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TC2050"
		(exclude_from_sim no)
		(in_bom no)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 11.43 0)
		)
		(property "Value" "TC2050"
			(at 1.27 -11.43 0)
		)
		(property "Footprint" "Connector:Tag-Connect_TC2050-IDC-NL_2x05_P1.27mm_Vertical"
			(at 1.27 0 0)
		)
		(property "Datasheet" "https://www.tag-connect.com/wp-content/uploads/bsk-pdf-manager/TC2050-IDC-NL_Datasheet_8.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "Tag-Connect’s 10-pins connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "Debug plug-of-nails"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TC2050*"
			(at 0 0 0)
		)
		(symbol "TC2050_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TC2070"
		(exclude_from_sim no)
		(in_bom no)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 13.97 0)
		)
		(property "Value" "TC2070"
			(at 1.27 -13.97 0)
		)
		(property "Footprint" "Connector:Tag-Connect_TC2070-IDC-FP_2x07_P1.27mm_Vertical"
			(at 1.27 -2.54 0)
		)
		(property "Datasheet" "https://www.tag-connect.com/wp-content/uploads/bsk-pdf-manager/TC2070-IDC-NL_Datasheet_12.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "Tag-Connect’s 14-pins connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "Debug plug-of-nails"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TC2070*"
			(at 0 0 0)
		)
		(symbol "TC2070_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TestPoint"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TP"
			(at 0 6.858 0)
		)
		(property "Value" "TestPoint"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 5.08 0 0)
		)
		(property "Datasheet" "~"
			(at 5.08 0 0)
		)
		(property "Description" "test point"
			(at 0 0 0)
		)
		(property "ki_keywords" "test point tp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pin* Test*"
			(at 0 0 0)
		)
		(symbol "TestPoint_0_1")
		(symbol "TestPoint_1_1"
			(pin passive line
				(at 0 0 90)
				(length 2.54)
				(name "1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TestPoint_2Pole"
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TP"
			(at 0 1.524 0)
		)
		(property "Value" "TestPoint_2Pole"
			(at 0 -1.778 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "2-polar test point"
			(at 0 0 0)
		)
		(property "ki_keywords" "point tp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pin* Test*"
			(at 0 0 0)
		)
		(symbol "TestPoint_2Pole_0_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TestPoint_Alt"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TP"
			(at 0 6.858 0)
		)
		(property "Value" "TestPoint_Alt"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 5.08 0 0)
		)
		(property "Datasheet" "~"
			(at 5.08 0 0)
		)
		(property "Description" "test point (alternative shape)"
			(at 0 0 0)
		)
		(property "ki_keywords" "test point tp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pin* Test*"
			(at 0 0 0)
		)
		(symbol "TestPoint_Alt_0_1")
		(symbol "TestPoint_Alt_1_1"
			(pin passive line
				(at 0 0 90)
				(length 2.54)
				(name "1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TestPoint_Flag"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TP"
			(at 3.429 1.778 0)
		)
		(property "Value" "TestPoint_Flag"
			(at 3.302 4.191 0)
		)
		(property "Footprint" ""
			(at 5.08 0 0)
		)
		(property "Datasheet" "~"
			(at 5.08 0 0)
		)
		(property "Description" "test point (alternative flag-style design)"
			(at 0 0 0)
		)
		(property "ki_keywords" "test point tp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pin* Test*"
			(at 0 0 0)
		)
		(symbol "TestPoint_Flag_0_1")
		(symbol "TestPoint_Flag_1_1"
			(pin passive line
				(at 0 0 90)
				(length 0)
				(name "1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TestPoint_Probe"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TP"
			(at 1.651 5.842 0)
		)
		(property "Value" "TestPoint_Probe"
			(at 1.651 4.064 0)
		)
		(property "Footprint" ""
			(at 5.08 0 0)
		)
		(property "Datasheet" "~"
			(at 5.08 0 0)
		)
		(property "Description" "test point (alternative probe-style design)"
			(at 0 0 0)
		)
		(property "ki_keywords" "test point tp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pin* Test*"
			(at 0 0 0)
		)
		(symbol "TestPoint_Probe_0_1")
		(symbol "TestPoint_Probe_1_1"
			(pin passive line
				(at 0 0 90)
				(length 0)
				(name "1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TestPoint_Small"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TP"
			(at 0 3.81 0)
		)
		(property "Value" "TestPoint_Small"
			(at 0 2.032 0)
		)
		(property "Footprint" ""
			(at 5.08 0 0)
		)
		(property "Datasheet" "~"
			(at 5.08 0 0)
		)
		(property "Description" "test point"
			(at 0 0 0)
		)
		(property "ki_keywords" "test point tp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pin* Test*"
			(at 0 0 0)
		)
		(symbol "TestPoint_Small_0_1")
		(symbol "TestPoint_Small_1_1"
			(pin passive line
				(at 0 0 90)
				(length 0)
				(name "1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UEXT_Host"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 5.08 10.16 0)
		)
		(property "Value" "UEXT_Host"
			(at 6.35 -10.16 0)
		)
		(property "Footprint" ""
			(at -3.81 0 0)
		)
		(property "Datasheet" "https://www.olimex.com/Products/Modules/UEXT/resources/UEXT_rev_B.pdf"
			(at -3.81 0 0)
		)
		(property "Description" "Universal EXTension (UEXT) is a connector layout which includes power and three serial buses: Asynchronous, I2C, and SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "UEXT, SPI, UART, I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Connector*:2x05*"
			(at 0 0 0)
		)
		(symbol "UEXT_Host_1_1"
			(pin output line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "TXD")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "RXD")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "SDA")
				(number "6")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "SCL")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 3.81)
				(name "3V3")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "MISO")
				(number "7")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "MOSI")
				(number "8")
			)
			(pin output line
				(at 12.7 0 180)
				(length 3.81)
				(name "SCK")
				(number "9")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "~{SSEL}")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UEXT_Slave"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 6.35 10.16 0)
		)
		(property "Value" "UEXT_Slave"
			(at 6.35 -10.16 0)
		)
		(property "Footprint" ""
			(at -3.81 0 0)
		)
		(property "Datasheet" "https://www.olimex.com/Products/Modules/UEXT/resources/UEXT_rev_B.pdf"
			(at -3.81 0 0)
		)
		(property "Description" "Universal EXTension (UEXT) is a connector layout which includes power and three serial buses: Asynchronous, I2C, and SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "UEXT, SPI, UART, I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Connector*:2x05*"
			(at 0 0 0)
		)
		(symbol "UEXT_Slave_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "TXD")
				(number "3")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "RXD")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "SCL")
				(number "5")
			)
			(pin power_out line
				(at 0 12.7 270)
				(length 3.81)
				(name "3V3")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "MISO")
				(number "7")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "MOSI")
				(number "8")
			)
			(pin input line
				(at 12.7 0 180)
				(length 3.81)
				(name "SCK")
				(number "9")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "~{SSEL}")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB3_A"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -10.16 15.24 0)
		)
		(property "Value" "USB3_A"
			(at 10.16 15.24 0)
		)
		(property "Footprint" ""
			(at 3.81 2.54 0)
		)
		(property "Datasheet" "~"
			(at 3.81 2.54 0)
		)
		(property "Description" "USB 3.0 A connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb universal serial bus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "USB3*"
			(at 0 0 0)
		)
		(symbol "USB3_A_0_0")
		(symbol "USB3_A_0_1")
		(symbol "USB3_A_1_1"
			(pin passive line
				(at -5.08 -17.78 90)
				(length 2.54)
				(name "SHIELD")
				(number "10")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "DRAIN")
				(number "7")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VBUS")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "D-")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "D+")
				(number "3")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SSRX-")
				(number "5")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SSRX+")
				(number "6")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SSTX-")
				(number "8")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SSTX+")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB3_A_Stacked"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -10.16 15.24 0)
		)
		(property "Value" "USB3_A_Stacked"
			(at 10.16 15.24 0)
		)
		(property "Footprint" ""
			(at 3.81 2.54 0)
		)
		(property "Datasheet" "~"
			(at 3.81 2.54 0)
		)
		(property "Description" "USB 3.0 A connector, stacked"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb universal serial bus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "USB3?A*Stacked*"
			(at 0 0 0)
		)
		(symbol "USB3_A_Stacked_0_0")
		(symbol "USB3_A_Stacked_0_1"
			(pin passive line
				(at -5.08 -17.78 90)
				(length 2.54)
				(name "SHIELD")
				(number "19")
			)
		)
		(symbol "USB3_A_Stacked_1_1"
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "DRAIN1")
				(number "7")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND1")
				(number "4")
			)
			(pin power_in line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VBUS1")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "D1-")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "D1+")
				(number "3")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SSRX1-")
				(number "5")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SSRX1+")
				(number "6")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SSTX1-")
				(number "8")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SSTX1+")
				(number "9")
			)
		)
		(symbol "USB3_A_Stacked_2_1"
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "DRAIN2")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND2")
				(number "13")
			)
			(pin power_in line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VBUS2")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "D2-")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "D2+")
				(number "12")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SSRX2-")
				(number "14")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SSRX2+")
				(number "15")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SSTX2-")
				(number "17")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SSTX2+")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB3_B"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -10.16 15.24 0)
		)
		(property "Value" "USB3_B"
			(at 10.16 15.24 0)
		)
		(property "Footprint" ""
			(at 3.81 2.54 0)
		)
		(property "Datasheet" "~"
			(at 3.81 2.54 0)
		)
		(property "Description" "USB 3.0 B connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb universal serial bus"
			(at 0 0 0)
		)
		(symbol "USB3_B_0_0")
		(symbol "USB3_B_0_1")
		(symbol "USB3_B_1_1"
			(pin passive line
				(at -5.08 -17.78 90)
				(length 2.54)
				(name "SHIELD")
				(number "10")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "DRAIN")
				(number "7")
			)
			(pin power_out line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VBUS")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "D-")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "D+")
				(number "3")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SSTX-")
				(number "5")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SSTX+")
				(number "6")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SSRX-")
				(number "8")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SSRX+")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB3_B_Micro"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -10.16 15.24 0)
		)
		(property "Value" "USB3_B_Micro"
			(at 10.16 15.24 0)
		)
		(property "Footprint" ""
			(at 3.81 3.81 0)
		)
		(property "Datasheet" "~"
			(at 3.81 5.08 0)
		)
		(property "Description" "USB 3.0 Micro-B connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb universal serial bus"
			(at 0 0 0)
		)
		(symbol "USB3_B_Micro_0_0")
		(symbol "USB3_B_Micro_0_1")
		(symbol "USB3_B_Micro_1_1"
			(pin passive line
				(at -5.08 -17.78 90)
				(length 2.54)
				(name "SHIELD")
				(number "11")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "DRAIN")
				(number "8")
			)
			(pin power_out line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_out line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VBUS")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "D-")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "D+")
				(number "3")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "ID")
				(number "4")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SSTX-")
				(number "6")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SSTX+")
				(number "7")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SSRX-")
				(number "9")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SSRX+")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB_A"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "USB_A"
			(at -5.08 8.89 0)
		)
		(property "Footprint" ""
			(at 3.81 -1.27 0)
		)
		(property "Datasheet" "~"
			(at 3.81 -1.27 0)
		)
		(property "Description" "USB Type A connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "USB*"
			(at 0 0 0)
		)
		(symbol "USB_A_0_1")
		(symbol "USB_A_1_1"
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "Shield")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "VBUS")
				(number "1")
			)
			(pin bidirectional line
				(at 7.62 0 180)
				(length 2.54)
				(name "D+")
				(number "3")
			)
			(pin bidirectional line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "D-")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB_A_Stacked"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 15.875 0)
		)
		(property "Value" "USB_A_Stacked"
			(at 0 13.97 0)
		)
		(property "Footprint" ""
			(at 3.81 -13.97 0)
		)
		(property "Datasheet" "~"
			(at 5.08 1.27 0)
		)
		(property "Description" "USB Type A connector, stacked"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "USB*"
			(at 0 0 0)
		)
		(symbol "USB_A_Stacked_0_1")
		(symbol "USB_A_Stacked_1_1"
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "Shield")
				(number "9")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "8")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VBUS1")
				(number "1")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VBUS2")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "D1+")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "D1-")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "D2+")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "D2-")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB_B"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "USB_B"
			(at -5.08 8.89 0)
		)
		(property "Footprint" ""
			(at 3.81 -1.27 0)
		)
		(property "Datasheet" "~"
			(at 3.81 -1.27 0)
		)
		(property "Description" "USB Type B connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "USB*"
			(at 0 0 0)
		)
		(symbol "USB_B_0_1")
		(symbol "USB_B_1_1"
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "Shield")
				(number "5")
			)
			(pin power_out line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "VBUS")
				(number "1")
			)
			(pin bidirectional line
				(at 7.62 0 180)
				(length 2.54)
				(name "D+")
				(number "3")
			)
			(pin bidirectional line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "D-")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB_B_Micro"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "USB_B_Micro"
			(at -5.08 8.89 0)
		)
		(property "Footprint" ""
			(at 3.81 -1.27 0)
		)
		(property "Datasheet" "~"
			(at 3.81 -1.27 0)
		)
		(property "Description" "USB Micro Type B connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector USB micro"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "USB*"
			(at 0 0 0)
		)
		(symbol "USB_B_Micro_0_1")
		(symbol "USB_B_Micro_1_1"
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "Shield")
				(number "6")
			)
			(pin power_out line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_out line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "VBUS")
				(number "1")
			)
			(pin bidirectional line
				(at 7.62 0 180)
				(length 2.54)
				(name "D+")
				(number "3")
			)
			(pin bidirectional line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "D-")
				(number "2")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "ID")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB_C_Plug"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at -10.16 29.21 0)
		)
		(property "Value" "USB_C_Plug"
			(at 10.16 29.21 0)
		)
		(property "Footprint" ""
			(at 3.81 0 0)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 3.81 0 0)
		)
		(property "Description" "USB Type-C Plug connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb universal serial bus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "USB*C*Plug*"
			(at 0 0 0)
		)
		(symbol "USB_C_Plug_0_0")
		(symbol "USB_C_Plug_0_1")
		(symbol "USB_C_Plug_1_1"
			(pin passive line
				(at -7.62 -40.64 90)
				(length 5.08)
				(name "SHIELD")
				(number "S1")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 5.08)
				(name "GND")
				(number "A1")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "A12")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B1")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B12")
			)
			(pin passive line
				(at 15.24 25.4 180)
				(length 5.08)
				(name "VBUS")
				(number "A4")
			)
			(pin passive line
				(at 15.24 25.4 180)
				(length 5.08)
				(hide yes)
				(name "VBUS")
				(number "A9")
			)
			(pin passive line
				(at 15.24 25.4 180)
				(length 5.08)
				(hide yes)
				(name "VBUS")
				(number "B4")
			)
			(pin passive line
				(at 15.24 25.4 180)
				(length 5.08)
				(hide yes)
				(name "VBUS")
				(number "B9")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 5.08)
				(name "CC")
				(number "A5")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 5.08)
				(name "VCONN")
				(number "B5")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 5.08)
				(name "D-")
				(number "A7")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "D+")
				(number "A6")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "RX1-")
				(number "B10")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "RX1+")
				(number "B11")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 5.08)
				(name "TX1-")
				(number "A3")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 5.08)
				(name "TX1+")
				(number "A2")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 5.08)
				(name "RX2-")
				(number "A10")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 5.08)
				(name "RX2+")
				(number "A11")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 5.08)
				(name "TX2-")
				(number "B3")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 5.08)
				(name "TX2+")
				(number "B2")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 5.08)
				(name "SBU1")
				(number "A8")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 5.08)
				(name "SBU2")
				(number "B8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB_C_Plug_USB2.0"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at -10.16 19.05 0)
		)
		(property "Value" "USB_C_Plug_USB2.0"
			(at 12.7 19.05 0)
		)
		(property "Footprint" ""
			(at 3.81 0 0)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 3.81 0 0)
		)
		(property "Description" "USB 2.0-only Type-C Plug connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb universal serial bus type-C USB2.0"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "USB*C*Plug*"
			(at 0 0 0)
		)
		(symbol "USB_C_Plug_USB2.0_0_0")
		(symbol "USB_C_Plug_USB2.0_0_1")
		(symbol "USB_C_Plug_USB2.0_1_1"
			(pin passive line
				(at -7.62 -22.86 90)
				(length 5.08)
				(name "SHIELD")
				(number "S1")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 5.08)
				(name "GND")
				(number "A1")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "A12")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B1")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B12")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 5.08)
				(name "VBUS")
				(number "A4")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 5.08)
				(hide yes)
				(name "VBUS")
				(number "A9")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 5.08)
				(hide yes)
				(name "VBUS")
				(number "B4")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 5.08)
				(hide yes)
				(name "VBUS")
				(number "B9")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 5.08)
				(name "CC")
				(number "A5")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "VCONN")
				(number "B5")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "D-")
				(number "A7")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "D+")
				(number "A6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB_C_Receptacle"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -10.16 29.21 0)
		)
		(property "Value" "USB_C_Receptacle"
			(at 10.16 29.21 0)
		)
		(property "Footprint" ""
			(at 3.81 0 0)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 3.81 0 0)
		)
		(property "Description" "USB Full-Featured Type-C Receptacle connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb universal serial bus type-C full-featured"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "USB*C*Receptacle*"
			(at 0 0 0)
		)
		(symbol "USB_C_Receptacle_0_0")
		(symbol "USB_C_Receptacle_0_1")
		(symbol "USB_C_Receptacle_1_1"
			(pin passive line
				(at -7.62 -40.64 90)
				(length 5.08)
				(name "SHIELD")
				(number "S1")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 5.08)
				(name "GND")
				(number "A1")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "A12")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B1")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B12")
			)
			(pin passive line
				(at 15.24 25.4 180)
				(length 5.08)
				(name "VBUS")
				(number "A4")
			)
			(pin passive line
				(at 15.24 25.4 180)
				(length 5.08)
				(hide yes)
				(name "VBUS")
				(number "A9")
			)
			(pin passive line
				(at 15.24 25.4 180)
				(length 5.08)
				(hide yes)
				(name "VBUS")
				(number "B4")
			)
			(pin passive line
				(at 15.24 25.4 180)
				(length 5.08)
				(hide yes)
				(name "VBUS")
				(number "B9")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 5.08)
				(name "CC1")
				(number "A5")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 5.08)
				(name "CC2")
				(number "B5")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 5.08)
				(name "D-")
				(number "A7")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 5.08)
				(name "D-")
				(number "B7")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "D+")
				(number "A6")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "D+")
				(number "B6")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "RX1-")
				(number "B10")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "RX1+")
				(number "B11")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 5.08)
				(name "TX1-")
				(number "A3")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 5.08)
				(name "TX1+")
				(number "A2")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 5.08)
				(name "RX2-")
				(number "A10")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 5.08)
				(name "RX2+")
				(number "A11")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 5.08)
				(name "TX2-")
				(number "B3")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 5.08)
				(name "TX2+")
				(number "B2")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 5.08)
				(name "SBU1")
				(number "A8")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 5.08)
				(name "SBU2")
				(number "B8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB_C_Receptacle_PowerOnly_24P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 16.51 0)
		)
		(property "Value" "USB_C_Receptacle_PowerOnly_24P"
			(at 0 13.97 0)
		)
		(property "Footprint" ""
			(at 3.81 2.54 0)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 0 0 0)
		)
		(property "Description" "USB Power-Only 24P Type-C Receptacle connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb universal serial bus type-C power-only charging-only 24P 24C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "USB*C*Receptacle*"
			(at 0 0 0)
		)
		(symbol "USB_C_Receptacle_PowerOnly_24P_0_0")
		(symbol "USB_C_Receptacle_PowerOnly_24P_0_1")
		(symbol "USB_C_Receptacle_PowerOnly_24P_1_1"
			(pin passive line
				(at -7.62 -17.78 90)
				(length 5.08)
				(name "SHIELD")
				(number "S1")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "A12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B1")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B12")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 5.08)
				(hide yes)
				(name "VBUS")
				(number "A4")
			)
			(pin power_in line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "VBUS")
				(number "A9")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 5.08)
				(hide yes)
				(name "VBUS")
				(number "B4")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 5.08)
				(hide yes)
				(name "VBUS")
				(number "B9")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "CC1")
				(number "A5")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 5.08)
				(name "CC2")
				(number "B5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB_C_Receptacle_PowerOnly_6P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 16.51 0)
		)
		(property "Value" "USB_C_Receptacle_PowerOnly_6P"
			(at 0 13.97 0)
		)
		(property "Footprint" ""
			(at 3.81 2.54 0)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 0 0 0)
		)
		(property "Description" "USB Power-Only 6P Type-C Receptacle connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb universal serial bus type-C power-only charging-only 6P 6C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "USB*C*Receptacle*"
			(at 0 0 0)
		)
		(symbol "USB_C_Receptacle_PowerOnly_6P_0_0")
		(symbol "USB_C_Receptacle_PowerOnly_6P_0_1")
		(symbol "USB_C_Receptacle_PowerOnly_6P_1_1"
			(pin passive line
				(at -7.62 -17.78 90)
				(length 5.08)
				(name "SHIELD")
				(number "S1")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "A12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B12")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "VBUS")
				(number "A9")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 5.08)
				(hide yes)
				(name "VBUS")
				(number "B9")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "CC1")
				(number "A5")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 5.08)
				(name "CC2")
				(number "B5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB_C_Receptacle_USB2.0_14P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 22.225 0)
		)
		(property "Value" "USB_C_Receptacle_USB2.0_14P"
			(at 0 19.685 0)
		)
		(property "Footprint" ""
			(at 3.81 0 0)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 3.81 0 0)
		)
		(property "Description" "USB 2.0-only 14P Type-C Receptacle connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb universal serial bus type-C USB2.0"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "USB*C*Receptacle*"
			(at 0 0 0)
		)
		(symbol "USB_C_Receptacle_USB2.0_14P_0_0")
		(symbol "USB_C_Receptacle_USB2.0_14P_0_1")
		(symbol "USB_C_Receptacle_USB2.0_14P_1_1"
			(pin passive line
				(at -7.62 -22.86 90)
				(length 5.08)
				(name "SHIELD")
				(number "S1")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 5.08)
				(name "GND")
				(number "A1")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "A12")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B1")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B12")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 5.08)
				(name "VBUS")
				(number "A4")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 5.08)
				(hide yes)
				(name "VBUS")
				(number "A9")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 5.08)
				(hide yes)
				(name "VBUS")
				(number "B4")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 5.08)
				(hide yes)
				(name "VBUS")
				(number "B9")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 5.08)
				(name "CC1")
				(number "A5")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "CC2")
				(number "B5")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "D-")
				(number "A7")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "D-")
				(number "B7")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "D+")
				(number "A6")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "D+")
				(number "B6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB_C_Receptacle_USB2.0_16P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 22.225 0)
		)
		(property "Value" "USB_C_Receptacle_USB2.0_16P"
			(at 0 19.685 0)
		)
		(property "Footprint" ""
			(at 3.81 0 0)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 3.81 0 0)
		)
		(property "Description" "USB 2.0-only 16P Type-C Receptacle connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb universal serial bus type-C USB2.0"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "USB*C*Receptacle*"
			(at 0 0 0)
		)
		(symbol "USB_C_Receptacle_USB2.0_16P_0_0")
		(symbol "USB_C_Receptacle_USB2.0_16P_0_1")
		(symbol "USB_C_Receptacle_USB2.0_16P_1_1"
			(pin passive line
				(at -7.62 -22.86 90)
				(length 5.08)
				(name "SHIELD")
				(number "S1")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 5.08)
				(name "GND")
				(number "A1")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "A12")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B1")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B12")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 5.08)
				(name "VBUS")
				(number "A4")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 5.08)
				(hide yes)
				(name "VBUS")
				(number "A9")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 5.08)
				(hide yes)
				(name "VBUS")
				(number "B4")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 5.08)
				(hide yes)
				(name "VBUS")
				(number "B9")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 5.08)
				(name "CC1")
				(number "A5")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "CC2")
				(number "B5")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "D-")
				(number "A7")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "D-")
				(number "B7")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "D+")
				(number "A6")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "D+")
				(number "B6")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 5.08)
				(name "SBU1")
				(number "A8")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 5.08)
				(name "SBU2")
				(number "B8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB_OTG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "USB_OTG"
			(at -5.08 8.89 0)
		)
		(property "Footprint" ""
			(at 3.81 -1.27 0)
		)
		(property "Datasheet" "~"
			(at 3.81 -1.27 0)
		)
		(property "Description" "USB mini/micro connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "USB*"
			(at 0 0 0)
		)
		(symbol "USB_OTG_0_1")
		(symbol "USB_OTG_1_1"
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "Shield")
				(number "6")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "VBUS")
				(number "1")
			)
			(pin bidirectional line
				(at 7.62 0 180)
				(length 2.54)
				(name "D+")
				(number "3")
			)
			(pin bidirectional line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "D-")
				(number "2")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "ID")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_ARM_SWD_TagConnect_TC2030-NL"
		(extends "Conn_ARM_SWD_TagConnect_TC2030")
		(property "Reference" "J"
			(at 2.54 11.43 0)
		)
		(property "Value" "Conn_ARM_SWD_TagConnect_TC2030-NL"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Connector:Tag-Connect_TC2030-IDC-NL_2x03_P1.27mm_Vertical"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.tag-connect.com/wp-content/uploads/bsk-pdf-manager/TC2030-CTX_1.pdf"
			(at 0 -15.24 0)
		)
		(property "Description" "Tag-Connect ARM Cortex SWD JTAG connector, 6 pin, no legs"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cortex Debug Connector ARM SWD JTAG"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TC2030*"
			(at 0 0 0)
		)
	)
	(symbol "Jack-DC"
		(extends "Barrel_Jack")
		(property "Reference" "J"
			(at 0 5.334 0)
		)
		(property "Value" "Jack-DC"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 1.27 -1.016 0)
		)
		(property "Datasheet" "~"
			(at 1.27 -1.016 0)
		)
		(property "Description" "DC Barrel Jack"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC power barrel jack connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BarrelJack*"
			(at 0 0 0)
		)
	)
	(symbol "Micro_SD_Card_Det_Hirose_DM3AT"
		(extends "Micro_SD_Card_Det2")
		(property "Reference" "J"
			(at -16.51 17.78 0)
		)
		(property "Value" "Micro_SD_Card_Det_Hirose_DM3AT"
			(at 16.51 17.78 0)
		)
		(property "Footprint" ""
			(at 52.07 17.78 0)
		)
		(property "Datasheet" "https://www.hirose.com/product/en/download_file/key_name/DM3/category/Catalog/doc_file_id/49662/?file_category_id=4&item_id=195&is_series=1"
			(at 0 2.54 0)
		)
		(property "Description" "Micro SD Card Socket with card detection pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector SD microsd"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "microSD*"
			(at 0 0 0)
		)
	)
	(symbol "RJ10"
		(extends "4P4C")
		(property "Reference" "J"
			(at -5.08 8.89 0)
		)
		(property "Value" "RJ10"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 0 1.27 90)
		)
		(property "Datasheet" "~"
			(at 0 1.27 90)
		)
		(property "Description" "RJ connector, 4P4C (4 positions 4 connected)"
			(at 0 0 0)
		)
		(property "ki_keywords" "4P4C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "4P4C* RJ9* RJ10* RJ22*"
			(at 0 0 0)
		)
	)
	(symbol "RJ10_Shielded"
		(extends "4P4C_Shielded")
		(property "Reference" "J"
			(at -5.08 8.89 0)
		)
		(property "Value" "RJ10_Shielded"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 0 1.27 90)
		)
		(property "Datasheet" "~"
			(at 0 1.27 90)
		)
		(property "Description" "RJ connector, 4P4C (4 positions 4 connected), Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "4P4C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "4P4C* RJ9* RJ10* RJ22*"
			(at 0 0 0)
		)
	)
	(symbol "RJ11"
		(extends "6P2C")
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "RJ11"
			(at 2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 6P2C (6 positions 2 connected)"
			(at 0 0 0)
		)
		(property "ki_keywords" "6P2C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "6P2C* RJ11*"
			(at 0 0 0)
		)
	)
	(symbol "RJ11_Shielded"
		(extends "6P2C_Shielded")
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "RJ11_Shielded"
			(at 2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 6P2C (6 positions 2 connected), Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "6P2C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "6P2C* RJ11*"
			(at 0 0 0)
		)
	)
	(symbol "RJ12"
		(extends "6P6C")
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "RJ12"
			(at 2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 6P6C (6 positions 6 connected)"
			(at 0 0 0)
		)
		(property "ki_keywords" "6P6C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "6P6C* RJ12* RJ18* RJ25*"
			(at 0 0 0)
		)
	)
	(symbol "RJ12_Shielded"
		(extends "6P6C_Shielded")
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "RJ12_Shielded"
			(at 2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 6P6C (6 positions 6 connected), Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "6P6C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "6P6C* RJ12* RJ18* RJ25*"
			(at 0 0 0)
		)
	)
	(symbol "RJ13"
		(extends "6P4C")
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "RJ13"
			(at 2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 6P4C (6 positions 4 connected)"
			(at 0 0 0)
		)
		(property "ki_keywords" "6P4C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "6P4C* RJ13* RJ14*"
			(at 0 0 0)
		)
	)
	(symbol "RJ13_Shielded"
		(extends "6P4C_Shielded")
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "RJ13_Shielded"
			(at 2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 6P4C (6 positions 4 connected), Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "6P4C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "6P4C* RJ13* RJ14*"
			(at 0 0 0)
		)
	)
	(symbol "RJ14"
		(extends "6P4C")
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "RJ14"
			(at 2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 6P4C (6 positions 4 connected)"
			(at 0 0 0)
		)
		(property "ki_keywords" "6P4C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "6P4C* RJ13* RJ14*"
			(at 0 0 0)
		)
	)
	(symbol "RJ14_Shielded"
		(extends "6P4C_Shielded")
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "RJ14_Shielded"
			(at 2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 6P4C (6 positions 4 connected), Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "6P4C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "6P4C* RJ13* RJ14*"
			(at 0 0 0)
		)
	)
	(symbol "RJ18"
		(extends "6P6C")
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "RJ18"
			(at 2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 6P6C (6 positions 6 connected)"
			(at 0 0 0)
		)
		(property "ki_keywords" "6P6C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "6P6C* RJ12* RJ18* RJ25*"
			(at 0 0 0)
		)
	)
	(symbol "RJ18_Shielded"
		(extends "6P6C_Shielded")
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "RJ18_Shielded"
			(at 2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 6P6C (6 positions 6 connected), Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "6P6C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "6P6C* RJ12* RJ18* RJ25*"
			(at 0 0 0)
		)
	)
	(symbol "RJ22"
		(extends "4P4C")
		(property "Reference" "J"
			(at -5.08 8.89 0)
		)
		(property "Value" "RJ22"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 0 1.27 90)
		)
		(property "Datasheet" "~"
			(at 0 1.27 90)
		)
		(property "Description" "RJ connector, 4P4C (4 positions 4 connected)"
			(at 0 0 0)
		)
		(property "ki_keywords" "4P4C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "4P4C* RJ9* RJ10* RJ22*"
			(at 0 0 0)
		)
	)
	(symbol "RJ22_Shielded"
		(extends "4P4C_Shielded")
		(property "Reference" "J"
			(at -5.08 8.89 0)
		)
		(property "Value" "RJ22_Shielded"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 0 1.27 90)
		)
		(property "Datasheet" "~"
			(at 0 1.27 90)
		)
		(property "Description" "RJ connector, 4P4C (4 positions 4 connected), Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "4P4C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "4P4C* RJ9* RJ10* RJ22*"
			(at 0 0 0)
		)
	)
	(symbol "RJ25"
		(extends "6P6C")
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "RJ25"
			(at 2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 6P6C (6 positions 6 connected)"
			(at 0 0 0)
		)
		(property "ki_keywords" "6P6C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "6P6C* RJ12* RJ18* RJ25*"
			(at 0 0 0)
		)
	)
	(symbol "RJ25_Shielded"
		(extends "6P6C_Shielded")
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "RJ25_Shielded"
			(at 2.54 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 6P6C (6 positions 6 connected), Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "6P6C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "6P6C* RJ12* RJ18* RJ25*"
			(at 0 0 0)
		)
	)
	(symbol "RJ31"
		(extends "8P8C")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ31"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ31* RJ32* RJ33* RJ34* RJ35* RJ41* RJ45* RJ49* RJ61*"
			(at 0 0 0)
		)
	)
	(symbol "RJ31_Shielded"
		(extends "8P8C_Shielded")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ31_Shielded"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected), Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ31* RJ32* RJ33* RJ34* RJ35* RJ41* RJ45* RJ49* RJ61*"
			(at 0 0 0)
		)
	)
	(symbol "RJ32"
		(extends "8P8C")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ32"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ31* RJ32* RJ33* RJ34* RJ35* RJ41* RJ45* RJ49* RJ61*"
			(at 0 0 0)
		)
	)
	(symbol "RJ32_Shielded"
		(extends "8P8C_Shielded")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ32_Shielded"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected), Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ31* RJ32* RJ33* RJ34* RJ35* RJ41* RJ45* RJ49* RJ61*"
			(at 0 0 0)
		)
	)
	(symbol "RJ33"
		(extends "8P8C")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ33"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ31* RJ32* RJ33* RJ34* RJ35* RJ41* RJ45* RJ49* RJ61*"
			(at 0 0 0)
		)
	)
	(symbol "RJ33_Shielded"
		(extends "8P8C_Shielded")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ33_Shielded"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected), Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ31* RJ32* RJ33* RJ34* RJ35* RJ41* RJ45* RJ49* RJ61*"
			(at 0 0 0)
		)
	)
	(symbol "RJ34"
		(extends "8P8C")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ34"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ31* RJ32* RJ33* RJ34* RJ35* RJ41* RJ45* RJ49* RJ61*"
			(at 0 0 0)
		)
	)
	(symbol "RJ34_Shielded"
		(extends "8P8C_Shielded")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ34_Shielded"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected), Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ31* RJ32* RJ33* RJ34* RJ35* RJ41* RJ45* RJ49* RJ61*"
			(at 0 0 0)
		)
	)
	(symbol "RJ35"
		(extends "8P8C")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ35"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ31* RJ32* RJ33* RJ34* RJ35* RJ41* RJ45* RJ49* RJ61*"
			(at 0 0 0)
		)
	)
	(symbol "RJ35_Shielded"
		(extends "8P8C_Shielded")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ35_Shielded"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected), Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ31* RJ32* RJ33* RJ34* RJ35* RJ41* RJ45* RJ49* RJ61*"
			(at 0 0 0)
		)
	)
	(symbol "RJ38"
		(extends "8P4C")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ38"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P4C (8 positions 4 connected)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P4C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P4C* RJ38* RJ48*"
			(at 0 0 0)
		)
	)
	(symbol "RJ38_Shielded"
		(extends "8P4C_Shielded")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ38_Shielded"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P4C (8 positions 4 connected), Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P4C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P4C* RJ38* RJ48*"
			(at 0 0 0)
		)
	)
	(symbol "RJ41"
		(extends "8P8C")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ41"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ31* RJ32* RJ33* RJ34* RJ35* RJ41* RJ45* RJ49* RJ61*"
			(at 0 0 0)
		)
	)
	(symbol "RJ41_Shielded"
		(extends "8P8C_Shielded")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ41_Shielded"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected), Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ31* RJ32* RJ33* RJ34* RJ35* RJ41* RJ45* RJ49* RJ61*"
			(at 0 0 0)
		)
	)
	(symbol "RJ45"
		(extends "8P8C")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ45"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ31* RJ32* RJ33* RJ34* RJ35* RJ41* RJ45* RJ49* RJ61*"
			(at 0 0 0)
		)
	)
	(symbol "RJ45_LED"
		(extends "8P8C_LED")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ45_LED"
			(at 1.27 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected), two LEDs"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket jack connector led"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ45*"
			(at 0 0 0)
		)
	)
	(symbol "RJ45_LED_Shielded"
		(extends "8P8C_LED_Shielded")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ45_LED_Shielded"
			(at 1.27 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected), two LEDs, Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket jack connector led"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ45*"
			(at 0 0 0)
		)
	)
	(symbol "RJ45_LED_Shielded_x2"
		(extends "8P8C_LED_Shielded_x2")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ45_LED_Shielded_x2"
			(at 1.27 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected), two LEDs, Shielded, two ports"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket jack connector led"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C*02* RJ45*02*"
			(at 0 0 0)
		)
	)
	(symbol "RJ45_Shielded"
		(extends "8P8C_Shielded")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ45_Shielded"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected), Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ jack socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ31* RJ32* RJ33* RJ34* RJ35* RJ41* RJ45* RJ49* RJ61*"
			(at 0 0 0)
		)
	)
	(symbol "RJ48"
		(extends "8P4C")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ48"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P4C (8 positions 4 connected)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P4C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P4C* RJ38* RJ48*"
			(at 0 0 0)
		)
	)
	(symbol "RJ48_Shielded"
		(extends "8P4C_Shielded")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ48_Shielded"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P4C (8 positions 4 connected), Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P4C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P4C* RJ38* RJ48*"
			(at 0 0 0)
		)
	)
	(symbol "RJ49"
		(extends "8P8C")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ49"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ31* RJ32* RJ33* RJ34* RJ35* RJ41* RJ45* RJ49* RJ61*"
			(at 0 0 0)
		)
	)
	(symbol "RJ49_Shielded"
		(extends "8P8C_Shielded")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ49_Shielded"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected), Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ31* RJ32* RJ33* RJ34* RJ35* RJ41* RJ45* RJ49* RJ61*"
			(at 0 0 0)
		)
	)
	(symbol "RJ61"
		(extends "8P8C")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ61"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ31* RJ32* RJ33* RJ34* RJ35* RJ41* RJ45* RJ49* RJ61*"
			(at 0 0 0)
		)
	)
	(symbol "RJ61_Shielded"
		(extends "8P8C_Shielded")
		(property "Reference" "J"
			(at -5.08 13.97 0)
		)
		(property "Value" "RJ61_Shielded"
			(at 2.54 13.97 0)
		)
		(property "Footprint" ""
			(at 0 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0.635 90)
		)
		(property "Description" "RJ connector, 8P8C (8 positions 8 connected), Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "8P8C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "8P8C* RJ31* RJ32* RJ33* RJ34* RJ35* RJ41* RJ45* RJ49* RJ61*"
			(at 0 0 0)
		)
	)
	(symbol "RJ9"
		(extends "4P4C")
		(property "Reference" "J"
			(at -5.08 8.89 0)
		)
		(property "Value" "RJ9"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 0 1.27 90)
		)
		(property "Datasheet" "~"
			(at 0 1.27 90)
		)
		(property "Description" "RJ connector, 4P4C (4 positions 4 connected)"
			(at 0 0 0)
		)
		(property "ki_keywords" "4P4C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "4P4C* RJ9* RJ10* RJ22*"
			(at 0 0 0)
		)
	)
	(symbol "RJ9_Shielded"
		(extends "4P4C_Shielded")
		(property "Reference" "J"
			(at -5.08 8.89 0)
		)
		(property "Value" "RJ9_Shielded"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 0 1.27 90)
		)
		(property "Datasheet" "~"
			(at 0 1.27 90)
		)
		(property "Description" "RJ connector, 4P4C (4 positions 4 connected), Shielded"
			(at 0 0 0)
		)
		(property "ki_keywords" "4P4C RJ socket connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "4P4C* RJ9* RJ10* RJ22*"
			(at 0 0 0)
		)
	)
	(symbol "Samtec_ASP-134486-01"
		(extends "Samtec_ASP-134602-01")
		(property "Reference" "J"
			(at 0 50.8 0)
		)
		(property "Value" "Samtec_ASP-134486-01"
			(at 0 -53.34 0)
		)
		(property "Footprint" ""
			(at 1.27 54.61 0)
		)
		(property "Datasheet" "http://suddendocs.samtec.com/prints/asp-134486-01-mkt.pdf"
			(at 3.81 53.34 0)
		)
		(property "Description" "Connector array, 10x40, 1.27mm pitch, carrier-card, receptacle, gold finish, VITA 57.1 FMC, SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA Mezzanine Card FMC Terminal Connector Header"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*FMC*ASP*134602?01*10x40*P1.27mm* *FMC*ASP*134486?01*10x40*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "USB_B_Mini"
		(extends "USB_B_Micro")
		(property "Reference" "J"
			(at -5.08 11.43 0)
		)
		(property "Value" "USB_B_Mini"
			(at -5.08 8.89 0)
		)
		(property "Footprint" ""
			(at 3.81 -1.27 0)
		)
		(property "Datasheet" "~"
			(at 3.81 -1.27 0)
		)
		(property "Description" "USB Mini Type B connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector USB mini"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "USB*"
			(at 0 0 0)
		)
	)
)
