(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AudioJack2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "AudioJack2"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Audio Jack, 2 Poles (Mono / TS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle mono phone headphone TS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack2_0_1")
		(symbol "AudioJack2_1_1"
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack2_Dual_Ground_Switch"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "AudioJack2_Dual_Ground_Switch"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at -1.27 5.08 0)
		)
		(property "Datasheet" "~"
			(at -1.27 5.08 0)
		)
		(property "Description" "Audio Jack, Dual, 2 Poles (Mono / TS), Grounded Sleeve, Switched Pole (Normalling)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack dual receptacle mono headphones phone TS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack2_Dual_Ground_Switch_0_1")
		(symbol "AudioJack2_Dual_Ground_Switch_1_1"
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "G")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "S1")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "SN1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "T1")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "TN1")
			)
		)
		(symbol "AudioJack2_Dual_Ground_Switch_2_1"
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "S2")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "SN2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "T2")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "TN2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack2_Dual_Switch"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "AudioJack2_Dual_Switch"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at -1.27 5.08 0)
		)
		(property "Datasheet" "~"
			(at -1.27 5.08 0)
		)
		(property "Description" "Audio Jack, Dual, 2 Poles (Mono / TS), Switched Pole (Normalling)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack dual receptacle mono headphones phone TS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack2_Dual_Switch_0_1")
		(symbol "AudioJack2_Dual_Switch_1_1"
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "S1")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "SN1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "T1")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "TN1")
			)
		)
		(symbol "AudioJack2_Dual_Switch_2_1"
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "S2")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "SN2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "T2")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "TN2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack2_Ground"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "AudioJack2_Ground"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Audio Jack, 2 Poles (Mono / TS), Grounded Sleeve"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle mono phone headphone TS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack2_Ground_0_1")
		(symbol "AudioJack2_Ground_1_1"
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "G")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack2_Ground_Switch"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "AudioJack2_Ground_Switch"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at 0 5.08 0)
		)
		(property "Datasheet" "~"
			(at 0 5.08 0)
		)
		(property "Description" "Audio Jack, 2 Poles (Mono / TS), Grounded Sleeve, Switched Pole (Normalling)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle mono headphones phone TS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack2_Ground_Switch_0_1")
		(symbol "AudioJack2_Ground_Switch_1_1"
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "G")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "SN")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "TN")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack2_Ground_SwitchT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "AudioJack2_Ground_SwitchT"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Audio Jack, 2 Poles (Mono / TS), Grounded Sleeve, Switched T Pole (Normalling)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle mono headphones phone TS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack2_Ground_SwitchT_0_1")
		(symbol "AudioJack2_Ground_SwitchT_1_1"
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "G")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "TN")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack2_Switch"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "AudioJack2_Switch"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at 0 5.08 0)
		)
		(property "Datasheet" "~"
			(at 0 5.08 0)
		)
		(property "Description" "Audio Jack, 2 Poles (Mono / TS), Switched Pole (Normalling)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle mono headphones phone TS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack2_Switch_0_1")
		(symbol "AudioJack2_Switch_1_1"
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "SN")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "TN")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack2_SwitchT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "AudioJack2_SwitchT"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle mono headphones phone TS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack2_SwitchT_0_1")
		(symbol "AudioJack2_SwitchT_1_1"
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "TN")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "AudioJack3"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Audio Jack, 3 Poles (Stereo / TRS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack3_0_1")
		(symbol "AudioJack3_1_1"
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack3_Dual_Ground_Switch"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "AudioJack3_Dual_Ground_Switch"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at -1.27 0 0)
		)
		(property "Datasheet" "~"
			(at -1.27 0 0)
		)
		(property "Description" "Audio Jack, Dual, 3 Poles (Stereo / TRS), Grounded Sleeve, Switched Poles (Normalling)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack dual receptacle stereo headphones phones TRS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack3_Dual_Ground_Switch_0_1")
		(symbol "AudioJack3_Dual_Ground_Switch_1_1"
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(name "~")
				(number "G")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "S1")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "SN1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R1")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "RN1")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "T1")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "~")
				(number "TN1")
			)
		)
		(symbol "AudioJack3_Dual_Ground_Switch_2_1"
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "S2")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "SN2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R2")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "RN2")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "T2")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "~")
				(number "TN2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack3_Dual_Switch"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "AudioJack3_Dual_Switch"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at -1.27 0 0)
		)
		(property "Datasheet" "~"
			(at -1.27 0 0)
		)
		(property "Description" "Audio Jack, Dual, 3 Poles (Stereo / TRS), Switched Poles (Normalling)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack dual receptacle stereo headphones phones TRS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack3_Dual_Switch_0_1")
		(symbol "AudioJack3_Dual_Switch_1_1"
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "S1")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "SN1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R1")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "RN1")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "T1")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "~")
				(number "TN1")
			)
		)
		(symbol "AudioJack3_Dual_Switch_2_1"
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "S2")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "SN2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R2")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "RN2")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "T2")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "~")
				(number "TN2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack3_Ground"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "AudioJack3_Ground"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Audio Jack, 3 Poles (Stereo / TRS), Grounded Sleeve"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack3_Ground_0_1")
		(symbol "AudioJack3_Ground_1_1"
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "G")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack3_Ground_Switch"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "AudioJack3_Ground_Switch"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Audio Jack, 3 Poles (Stereo / TRS), Grounded Sleeve, Switched Poles (Normalling)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack3_Ground_Switch_0_1")
		(symbol "AudioJack3_Ground_Switch_1_1"
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(name "~")
				(number "G")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "SN")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "RN")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "~")
				(number "TN")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack3_Ground_SwitchTR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "AudioJack3_Ground_SwitchTR"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Audio Jack, 3 Poles (Stereo / TRS), Grounded Sleeve, Switched TR Poles (Normalling)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack3_Ground_SwitchTR_0_1")
		(symbol "AudioJack3_Ground_SwitchTR_1_1"
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(name "~")
				(number "G")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "RN")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "~")
				(number "TN")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack3_Switch"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "AudioJack3_Switch"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Audio Jack, 3 Poles (Stereo / TRS), Switched Poles (Normalling)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack3_Switch_0_1")
		(symbol "AudioJack3_Switch_1_1"
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "SN")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "RN")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "~")
				(number "TN")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack3_SwitchT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "AudioJack3_SwitchT"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Audio Jack, 3 Poles (Stereo / TRS), Switched T Pole (Normalling)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack3_SwitchT_0_1")
		(symbol "AudioJack3_SwitchT_1_1"
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "~")
				(number "TN")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack3_SwitchTR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "AudioJack3_SwitchTR"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Audio Jack, 3 Poles (Stereo / TRS), Switched TR Poles (Normalling)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack3_SwitchTR_0_1")
		(symbol "AudioJack3_SwitchTR_1_1"
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "RN")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "~")
				(number "TN")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack4"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "AudioJack4"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Audio Jack, 4 Poles (TRRS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones TRRS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack4_0_1")
		(symbol "AudioJack4_1_1"
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R2")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "R1")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack4_Ground"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "AudioJack4_Ground"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Audio Jack, 4 Poles (TRRS), Grounded Sleeve"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones TRRS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack4_Ground_0_1")
		(symbol "AudioJack4_Ground_1_1"
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "~")
				(number "G")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R2")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "R1")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack4_Ground_SwitchTR1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "AudioJack4_Ground_SwitchTR1"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at -1.27 0 0)
		)
		(property "Datasheet" "~"
			(at -1.27 0 0)
		)
		(property "Description" "Audio Jack, 4 Poles (Stereo / TRRS), Grounded Sleeve, Switched TR1 Poles (Normalling)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack4_Ground_SwitchTR1_0_1")
		(symbol "AudioJack4_Ground_SwitchTR1_1_1"
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(name "~")
				(number "G")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "R2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R1")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "R1N")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "~")
				(number "TN")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack4_SwitchT1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "AudioJack4_SwitchT1"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at -1.27 0 0)
		)
		(property "Datasheet" "~"
			(at -1.27 0 0)
		)
		(property "Description" "Audio Jack, 4 Poles (Stereo / TRRS), Switched T1 Pole (Normalling)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones phones connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack4_SwitchT1_0_1")
		(symbol "AudioJack4_SwitchT1_1_1"
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "R2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R1")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "~")
				(number "TN")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack4_SwitchTR1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "AudioJack4_SwitchTR1"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at -1.27 0 0)
		)
		(property "Datasheet" "~"
			(at -1.27 0 0)
		)
		(property "Description" "Audio Jack, 4 Poles (Stereo / TRRS), Switched TR1 Poles (Normalling)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack4_SwitchTR1_0_1")
		(symbol "AudioJack4_SwitchTR1_1_1"
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "R2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R1")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "R1N")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "~")
				(number "TN")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "AudioJack5"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Audio Jack, 5 Poles (TRRRS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones TRRRS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack5_0_1")
		(symbol "AudioJack5_1_1"
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "R3")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R2")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "R1")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioJack5_Ground"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "AudioJack5_Ground"
			(at 0 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Audio Jack, 5 Poles (TRRRS), Grounded Sleeve"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones TRRRS connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
		(symbol "AudioJack5_Ground_0_1")
		(symbol "AudioJack5_Ground_1_1"
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "~")
				(number "G")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "R3")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R2")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "R1")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioPlug2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 10.16 6.35 0)
		)
		(property "Value" "AudioPlug2"
			(at 10.16 -6.35 0)
		)
		(property "Footprint" ""
			(at 8.89 -1.27 0)
		)
		(property "Datasheet" "~"
			(at 8.89 -1.27 0)
		)
		(property "Description" "Audio Jack, 2 Poles (Mono / TS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack plug stereo headphones TRRS connector 2.5mm 3.5mm 6.35mm"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Plug*"
			(at 0 0 0)
		)
		(symbol "AudioPlug2_0_0"
			(text "T"
				(at -8.89 0 0)
			)
			(text "S"
				(at 3.81 0 0)
			)
		)
		(symbol "AudioPlug2_0_1")
		(symbol "AudioPlug2_1_1"
			(pin passive line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioPlug3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 6.35 0)
		)
		(property "Value" "AudioPlug3"
			(at 1.27 -6.35 0)
		)
		(property "Footprint" ""
			(at 2.54 -1.27 0)
		)
		(property "Datasheet" "~"
			(at 2.54 -1.27 0)
		)
		(property "Description" "Audio Jack, 3 Poles (Stereo / TRS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack plug stereo headphones TRRS connector 2.5mm 3.5mm 6.35mm"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Plug*"
			(at 0 0 0)
		)
		(symbol "AudioPlug3_0_0"
			(text "R"
				(at -2.54 0 900)
			)
		)
		(symbol "AudioPlug3_0_1")
		(symbol "AudioPlug3_1_0"
			(text "T"
				(at -8.89 0 0)
			)
			(text "S"
				(at 3.81 0 0)
			)
		)
		(symbol "AudioPlug3_1_1"
			(pin passive line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "~")
				(number "R")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AudioPlug4"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 10.16 5.08 0)
		)
		(property "Value" "AudioPlug4"
			(at 11.43 -7.62 0)
		)
		(property "Footprint" ""
			(at 8.89 -2.54 0)
		)
		(property "Datasheet" "~"
			(at 8.89 -2.54 0)
		)
		(property "Description" "Audio Jack, 4 Poles (Stereo / TRRS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack plug stereo headphones TRRS connector 2.5mm 3.5mm"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Plug*"
			(at 0 0 0)
		)
		(symbol "AudioPlug4_0_0"
			(text "T"
				(at -8.89 -1.27 0)
			)
			(text "R1"
				(at -2.54 -1.27 900)
			)
			(text "R2"
				(at 0 -1.27 900)
			)
			(text "S"
				(at 5.08 -1.27 0)
			)
		)
		(symbol "AudioPlug4_0_1")
		(symbol "AudioPlug4_1_1"
			(pin passive line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "~")
				(number "R2")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~")
				(number "R1")
			)
			(pin passive line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SpeakON_NL2"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 2.54 8.89 0)
		)
		(property "Value" "SpeakON_NL2"
			(at 7.62 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.neutrik.com/en/speakon/"
			(at 0 0 0)
		)
		(property "Description" "speakON Connector, Male or Female, NL2"
			(at 0 0 0)
		)
		(property "ki_keywords" "speakon connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*speakON*"
			(at 0 0 0)
		)
		(symbol "SpeakON_NL2_0_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "1-")
				(number "1-")
			)
		)
		(symbol "SpeakON_NL2_1_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "1+")
				(number "1+")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SpeakON_NL2_AudioJack2_Combo"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 2.54 8.89 0)
		)
		(property "Value" "SpeakON_NL2_AudioJack2_Combo"
			(at 17.78 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.neutrik.com/en/speakon/"
			(at 0 0 0)
		)
		(property "Description" "speakON NL2 (Male or Female) and Audio Jack (Mono / TS) Combo Connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "speakon connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*speakON*"
			(at 0 0 0)
		)
		(symbol "SpeakON_NL2_AudioJack2_Combo_0_0"
			(text "S"
				(at -3.81 1.016 0)
			)
			(text "T"
				(at 1.016 3.556 0)
			)
		)
		(symbol "SpeakON_NL2_AudioJack2_Combo_0_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "1-")
				(number "1-")
			)
		)
		(symbol "SpeakON_NL2_AudioJack2_Combo_1_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "1+")
				(number "1+")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SpeakON_NL4"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 2.54 8.89 0)
		)
		(property "Value" "SpeakON_NL4"
			(at 7.62 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.neutrik.com/en/speakon/"
			(at 0 0 0)
		)
		(property "Description" "speakON Connector, Male or Female, NL4"
			(at 0 0 0)
		)
		(property "ki_keywords" "speakon connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*speakON*"
			(at 0 0 0)
		)
		(symbol "SpeakON_NL4_0_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "1-")
				(number "1-")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "2+")
				(number "2+")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "2-")
				(number "2-")
			)
		)
		(symbol "SpeakON_NL4_1_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "1+")
				(number "1+")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SpeakON_NL4_Switch"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 5.08 8.89 0)
		)
		(property "Value" "SpeakON_NL4_Switch"
			(at 13.97 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.neutrik.com/en/speakon/"
			(at 0 0 0)
		)
		(property "Description" "speakON Connector, Male or Female, NL4, Switched Pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "speakon connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*speakON*"
			(at 0 0 0)
		)
		(symbol "SpeakON_NL4_Switch_0_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "1-N")
				(number "1-N")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "1-")
				(number "1-")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "2+N")
				(number "2+N")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "2+")
				(number "2+")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "2-")
				(number "2-")
			)
		)
		(symbol "SpeakON_NL4_Switch_1_1"
			(pin passive line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "1+N")
				(number "1+N")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "1+")
				(number "1+")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "2-N")
				(number "2-N")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SpeakON_NL8"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 2.54 10.16 0)
		)
		(property "Value" "SpeakON_NL8"
			(at 7.62 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.neutrik.com/en/speakon/"
			(at 0 0 0)
		)
		(property "Description" "speakON Connector, Male or Female, NL8"
			(at 0 0 0)
		)
		(property "ki_keywords" "speakon connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*speakON*"
			(at 0 0 0)
		)
		(symbol "SpeakON_NL8_0_1"
			(pin passive line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "1-")
				(number "1-")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "2+")
				(number "2+")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "2-")
				(number "2-")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "3+")
				(number "3+")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "4-")
				(number "4-")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "4+")
				(number "4+")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "3-")
				(number "3-")
			)
		)
		(symbol "SpeakON_NL8_1_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "1+")
				(number "1+")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XLR3"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "XLR3"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "XLR Connector, Male or Female, 3 Pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
		(symbol "XLR3_0_1"
			(text "1"
				(at -3.556 1.778 0)
			)
			(text "3"
				(at 0 -1.778 0)
			)
			(text "2"
				(at 3.556 1.778 0)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XLR3_AudioJack2_Combo"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "XLR3_AudioJack2_Combo"
			(at 0 7.62 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 2.54 0)
		)
		(property "Description" "XLR (Male or Female) and Audio Jack (Mono / TS) Combo Connector, Discrete Ground Pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
		(symbol "XLR3_AudioJack2_Combo_1_1"
			(text "1"
				(at -3.556 1.778 0)
			)
			(text "3"
				(at 0 -1.778 0)
			)
			(text "2"
				(at 3.556 1.778 0)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "XLR3_AudioJack2_Combo_2_1"
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XLR3_AudioJack2_Combo_Ground"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "XLR3_AudioJack2_Combo_Ground"
			(at 0 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "XLR (Male or Female) and Audio Jack (Mono / TS) Combo Connector, Discrete Ground Pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
		(symbol "XLR3_AudioJack2_Combo_Ground_1_1"
			(text "1"
				(at -3.556 1.778 0)
			)
			(text "3"
				(at 0 -1.778 0)
			)
			(text "2"
				(at 3.556 1.778 0)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "~")
				(number "G")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "XLR3_AudioJack2_Combo_Ground_2_1"
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XLR3_AudioJack3_Combo"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "XLR3_AudioJack3_Combo"
			(at 0 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "XLR (Male or Female) and Audio Jack (Stereo / TRS) Combo Connector, Discrete Ground Pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
		(symbol "XLR3_AudioJack3_Combo_1_1"
			(text "1"
				(at -3.556 1.778 0)
			)
			(text "3"
				(at 0 -1.778 0)
			)
			(text "2"
				(at 3.556 1.778 0)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "XLR3_AudioJack3_Combo_2_1"
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XLR3_AudioJack3_Combo_Ground"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "XLR3_AudioJack3_Combo_Ground"
			(at 0 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "XLR (Male or Female) and Audio Jack (Stereo / TRS) Combo Connector, Discrete Ground Pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
		(symbol "XLR3_AudioJack3_Combo_Ground_1_1"
			(text "1"
				(at -3.556 1.778 0)
			)
			(text "3"
				(at 0 -1.778 0)
			)
			(text "2"
				(at 3.556 1.778 0)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "~")
				(number "G")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "XLR3_AudioJack3_Combo_Ground_2_1"
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XLR3_AudioJack3_Combo_GroundSwitch_Switch"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "XLR3_AudioJack3_Combo_GroundSwitch_Switch"
			(at 0 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "XLR (Male or Female) and Audio Jack (Stereo / TRS, Switched Poles (Normalling)) Combo Connector, Discrete Switched Ground Pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
		(symbol "XLR3_AudioJack3_Combo_GroundSwitch_Switch_1_1"
			(text "1"
				(at -3.556 1.778 0)
			)
			(text "3"
				(at 0 -1.778 0)
			)
			(text "2"
				(at 3.556 1.778 0)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "~")
				(number "GN")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "~")
				(number "G")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "XLR3_AudioJack3_Combo_GroundSwitch_Switch_2_1"
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "SN")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "RN")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "~")
				(number "TN")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XLR3_AudioJack3_Combo_Ground_Switch"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "XLR3_AudioJack3_Combo_Ground_Switch"
			(at 0 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "XLR (Male or Female) and Audio Jack (Stereo / TRS, Switched Poles (Normalling)) Combo Connector, Discrete Ground Pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
		(symbol "XLR3_AudioJack3_Combo_Ground_Switch_1_1"
			(text "1"
				(at -3.556 1.778 0)
			)
			(text "3"
				(at 0 -1.778 0)
			)
			(text "2"
				(at 3.556 1.778 0)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "~")
				(number "G")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "XLR3_AudioJack3_Combo_Ground_Switch_2_1"
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "SN")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "RN")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "~")
				(number "TN")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XLR3_AudioJack3_Combo_Switch"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "XLR3_AudioJack3_Combo_Switch"
			(at 0 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "XLR (Male or Female) and Audio Jack (Stereo / TRS, Switched Poles (Normalling)) Combo Connector"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
		(symbol "XLR3_AudioJack3_Combo_Switch_1_1"
			(text "1"
				(at -3.556 1.778 0)
			)
			(text "3"
				(at 0 -1.778 0)
			)
			(text "2"
				(at 3.556 1.778 0)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "XLR3_AudioJack3_Combo_Switch_2_1"
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "~")
				(number "S")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "~")
				(number "SN")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "~")
				(number "R")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "~")
				(number "RN")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "~")
				(number "T")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "~")
				(number "TN")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XLR3_Ground"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "XLR3_Ground"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "XLR Connector, Male or Female, 3 Pins, Discrete Ground Pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
		(symbol "XLR3_Ground_0_1"
			(text "1"
				(at -3.556 1.778 0)
			)
			(text "3"
				(at 0 -1.778 0)
			)
			(text "2"
				(at 3.556 1.778 0)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "XLR3_Ground_1_1"
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "~")
				(number "G")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XLR3_Ground_Switched"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "XLR3_Ground_Switched"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 2.54 0)
		)
		(property "Description" "XLR Connector, Male or Female, 3 Pins, Discrete Ground Pin, SPDT Switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
		(symbol "XLR3_Ground_Switched_1_1"
			(text "1"
				(at -3.556 1.778 0)
			)
			(text "3"
				(at 0 -1.778 0)
			)
			(text "2"
				(at 3.556 1.778 0)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "~")
				(number "G")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "XLR3_Ground_Switched_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "N")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "NC")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "NO")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XLR3_Switched"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "XLR3_Switched"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 2.54 0)
		)
		(property "Description" "XLR Connector, Male or Female, 3 Pins, SPDT Switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
		(symbol "XLR3_Switched_1_1"
			(text "1"
				(at -3.556 1.778 0)
			)
			(text "3"
				(at 0 -1.778 0)
			)
			(text "2"
				(at 3.556 1.778 0)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(symbol "XLR3_Switched_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "N")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "NC")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "NO")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XLR4"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "XLR4"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "XLR Connector, Male or Female, 4 Pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
		(symbol "XLR4_0_1"
			(text "1"
				(at -3.556 1.778 0)
			)
			(text "2"
				(at -2.032 -0.762 0)
			)
			(text "3"
				(at 2.032 -0.762 0)
			)
			(text "4"
				(at 3.556 1.778 0)
			)
		)
		(symbol "XLR4_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XLR4_Ground"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "XLR4_Ground"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "XLR Connector, Male or Female, 4 Pins, Discrete Ground Pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
		(symbol "XLR4_Ground_0_1"
			(text "1"
				(at -3.556 1.778 0)
			)
			(text "2"
				(at -2.032 -0.762 0)
			)
			(text "3"
				(at 2.032 -0.762 0)
			)
			(text "4"
				(at 3.556 1.778 0)
			)
		)
		(symbol "XLR4_Ground_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "G")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XLR5"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "XLR5"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "XLR Connector, Male or Female, 5 Pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
		(symbol "XLR5_0_1"
			(text "1"
				(at -3.556 1.778 0)
			)
			(text "2"
				(at -2.032 -0.762 0)
			)
			(text "3"
				(at 0 -1.778 0)
			)
			(text "4"
				(at 2.032 -0.762 0)
			)
			(text "5"
				(at 3.556 1.778 0)
			)
		)
		(symbol "XLR5_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "P1")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "P2")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "P3")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "P5")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "P3")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XLR5_Ground"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "XLR5_Ground"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "XLR Connector, Male or Female, 5 Pins, Discrete Ground Pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
		(symbol "XLR5_Ground_0_1"
			(text "1"
				(at -3.556 1.778 0)
			)
			(text "2"
				(at -2.032 -0.762 0)
			)
			(text "3"
				(at 0 -1.778 0)
			)
			(text "4"
				(at 2.032 -0.762 0)
			)
			(text "5"
				(at 3.556 1.778 0)
			)
		)
		(symbol "XLR5_Ground_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "P1")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "P2")
				(number "2")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "~")
				(number "G")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "P3")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "P5")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "P3")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XLR5_Ground_Switched"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "XLR5_Ground_Switched"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "XLR Connector, Male or Female, 5 Pins, Discrete Ground Pin, SPDT Switch"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
		(symbol "XLR5_Ground_Switched_1_1"
			(text "1"
				(at -3.556 1.778 0)
			)
			(text "2"
				(at -2.032 -0.762 0)
			)
			(text "3"
				(at 0 -1.778 0)
			)
			(text "4"
				(at 2.032 -0.762 0)
			)
			(text "5"
				(at 3.556 1.778 0)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "P1")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "P2")
				(number "2")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "~")
				(number "G")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "P3")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "P5")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "P3")
				(number "4")
			)
		)
		(symbol "XLR5_Ground_Switched_2_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "~")
				(number "N")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "NC")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "NO")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XLR6"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 2.54 6.35 0)
		)
		(property "Value" "XLR6"
			(at 5.08 -6.096 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "XLR Connector, Male or Female, 6 Pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
		(symbol "XLR6_0_1"
			(text "1"
				(at -3.556 1.778 0)
			)
			(text "2"
				(at -2.032 -0.762 0)
			)
			(text "3"
				(at 0 -1.778 0)
			)
			(text "6"
				(at 1.016 2.794 0)
			)
			(text "4"
				(at 2.032 -0.762 0)
			)
			(text "5"
				(at 3.556 1.778 0)
			)
		)
		(symbol "XLR6_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "P1")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "P2")
				(number "2")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "P6")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "P3")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "P5")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "P3")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NC3FAAH"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAAH"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAAH_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3faah"
			(at 0 0 0)
		)
		(property "Description" "AA Series, 3 pole female XLR receptacle, grounding: without ground/shell contact, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAAH-0"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAAH-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAAH-0_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3faah-0"
			(at 0 0 0)
		)
		(property "Description" "AA Series, 3 pole female XLR receptacle, grounding: without ground/shell contact, horizontal PCB mount, retention spring instead of latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAAH1"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAAH1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAAH1_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3faah1"
			(at 0 0 0)
		)
		(property "Description" "AA Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAAH1-0"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAAH1-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAAH1-0_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3faah1-0"
			(at 0 0 0)
		)
		(property "Description" "AA Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, retention spring instead of latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAAH1-DA"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAAH1-DA"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAAH1-DA_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3faah1-da"
			(at 0 0 0)
		)
		(property "Description" "AA Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, asymmetric push"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAAH2"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAAH2"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAAH2_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3faah2"
			(at 0 0 0)
		)
		(property "Description" "AA Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAAH2-0"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAAH2-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAAH2-0_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3faah2-0"
			(at 0 0 0)
		)
		(property "Description" "AA Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, retention spring instead of latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAAV"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAAV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAAV_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3faav"
			(at 0 0 0)
		)
		(property "Description" "AA Series, 3 pole female receptacle, grounding: without ground/shell contact, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAAV-0"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAAV-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAAV-0_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3faav-0"
			(at 0 0 0)
		)
		(property "Description" "AA Series, 3 pole female receptacle, grounding: without ground/shell contact, vertical PCB mount, retention spring instead of latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAAV1"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAAV1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAAV1_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3faav1"
			(at 0 0 0)
		)
		(property "Description" "AA Series, 3 pole female receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAAV1-0"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAAV1-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAAV1-0_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3faav1-0"
			(at 0 0 0)
		)
		(property "Description" "AA Series, 3 pole female receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount, retention spring instead of latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAAV1-DA"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAAV1-DA"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAAV1-DA_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3faav1-da"
			(at 0 0 0)
		)
		(property "Description" "AA Series, 3 pole female receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount, asymmetric push"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAAV2"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAAV2"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAAV2_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3faav2"
			(at 0 0 0)
		)
		(property "Description" "AA Series, 3 pole female receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAAV2-0"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAAV2-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAAV2-0_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3faav2-0"
			(at 0 0 0)
		)
		(property "Description" "AA Series, 3 pole female receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, retention spring instead of latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAH"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAH"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAH_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fah"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: without ground/shell contact, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAH-0"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAH-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAH-0_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fah-0"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: without ground/shell contact, horizontal PCB mount, retention spring instead of latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAH1"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAH1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAH1_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fah1"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAH1-0"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAH1-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAH1-0_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fah1-0"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, retention spring instead of latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAH1-DA"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAH1-DA"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAH1-DA_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fah1-da"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, asymmetric push"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAH2"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAH2"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAH2_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fah2"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAH2-0"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAH2-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAH2-0_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fah2-0"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, retention spring instead of latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAH2-DA"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAH2-DA"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAH2-DA_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fah2-da"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, asymmetric push"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAHL-0"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAHL-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAHL-0_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fahl-0"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: without ground/shell contact, lateral left PCB mount, retention spring instead of latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAHL1"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAHL1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAHL1_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fahl1"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, lateral left PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAHL1-0"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAHL1-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAHL1-0_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fahl1-0"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, lateral left PCB mount, retention spring instead of latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAHR-0"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAHR-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAHR-0_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fahr-0"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: without ground / shell contact, lateral right PCB mount, retention spring instead of latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAHR1"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAHR1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAHR1_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fahr1"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, lateral right PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAHR1-0"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAHR1-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAHR1-0_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fahr1-0"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, lateral right PCB mount, retention spring instead of latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAHR2"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAHR2"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAHR2_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fahr2"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, lateral right PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAHR2-0"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAHR2-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAHR2-0_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fahr2-0"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, lateral right PCB mount, retention spring instead of latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAV"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAV_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fav"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: without ground / shell contact, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAV-0"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAV-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAV-0_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fav-0"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: without ground / shell contact, vertical PCB mount, retention spring instead of latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAV1"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAV1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAV1_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fav1"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAV1-0"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAV1-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAV1-0_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fav1-0"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount, retention spring instead of latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAV1-DA"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAV1-DA"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAV1-DA_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fav1-da"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount, asymmetric push"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAV2"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAV2"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAV2_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fav2"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAV2-0"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAV2-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAV2-0_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fav2-0"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, retention spring instead of latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FAV2-DA"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FAV2-DA"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FAV2-DA_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fav2-da"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, asymmetric push"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FBH1"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FBH1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FBH1_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fbh1"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FBH1-B"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FBH1-B"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FBH1-B_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fbh1-b"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, black chrome shell"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FBH1-DA"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FBH1-DA"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FBH1-DA_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fbh1-da"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, asymmetric push"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FBH1-E"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FBH1-E"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FBH1-E_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fbh1-e"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, additional ground contacts"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FBH2"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FBH2"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FBH2_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fbh2"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FBH2-B"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FBH2-B"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FBH2-B_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fbh2-b"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, black chrome shell"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FBH2-DA"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FBH2-DA"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FBH2-DA_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fbh2-da"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, asymmetric push"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FBH2-E"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FBH2-E"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FBH2-E_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fbh2-e"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, additional ground contacts"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FBHL1"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FBHL1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FBHL1_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fbhl1"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, lateral left PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FBV1"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FBV1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FBV1_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fbv1"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FBV1-0"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FBV1-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FBV1-0_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fbv1-0"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount, retention spring, no latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FBV1-B"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FBV1-B"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FBV1-B_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fbv1-b"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount, black chrome shell"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FBV1-DA"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FBV1-DA"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FBV1-DA_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fbv1-da"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount, asymmetric push"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FBV2"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FBV2"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FBV2_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fbv2"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FBV2-B"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FBV2-B"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FBV2-B_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fbv2-b"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, black chrome shell"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FBV2-DA"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FBV2-DA"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FBV2-DA_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fbv2-da"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, asymmetric push"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3FBV2-SW"
		(extends "XLR3_Ground_Switched")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3FBV2-SW"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3FBV2-SW_Vertical"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3fbv2-sw"
			(at 0 2.54 0)
		)
		(property "Description" "B Series, 3 pole female XLR receptacle, switching contacts, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector spdt switch neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MAAH"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MAAH"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MAAH_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3maah"
			(at 0 0 0)
		)
		(property "Description" "AA Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MAAH-0"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MAAH-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MAAH-0_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3maah-0"
			(at 0 0 0)
		)
		(property "Description" "AA Series, 3 pole male XLR receptacle, grounding: ground contact connected to shell ground, but not to front panel and Pin 1, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MAAH-1"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MAAH-1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MAAH-1_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3maah-1"
			(at 0 0 0)
		)
		(property "Description" "AA Series, 3 pole male XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MAAV"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MAAV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MAAV_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3maav"
			(at 0 0 0)
		)
		(property "Description" "AA Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MAAV-0"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MAAV-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MAAV-0_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3maav-0"
			(at 0 0 0)
		)
		(property "Description" "AA Series, 3 pole male XLR receptacle, grounding: ground contact connected to shell ground, but not to front panel and Pin 1, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MAAV-1"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MAAV-1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MAAV-1_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3maav-1"
			(at 0 0 0)
		)
		(property "Description" "AA Series, 3 pole male XLR receptacle, grounding: mating connector shell to pin1 and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MAFH-PH"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MAFH-PH"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MAFH-PH_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mafh-ph"
			(at 0 0 0)
		)
		(property "Description" "A Series, Chassis connector H female (A series layout), mates with Phoenix MSTB2,5/3-ST, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MAH"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MAH"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MAH_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mah"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MAH-0"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MAH-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MAH-0_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mah-0"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole male XLR receptacle, grounding: ground contact connected to shell ground, but not to front panel and Pin 1, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MAHL"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MAHL"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MAHL_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mahl"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, lateral left PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MAHR"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MAHR"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MAHR_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mahr"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, lateral right PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MAMH-PH"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MAMH-PH"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MAMH-PH_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mamh-ph"
			(at 0 0 0)
		)
		(property "Description" "A Series, Chassis connector Phoenix H male (A series layout), mates with Phoenix MSTB 2,5/3-ST, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MAV"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MAV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MAV_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mav"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MAV-0"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MAV-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MAV-0_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mav-0"
			(at 0 0 0)
		)
		(property "Description" "A Series, 3 pole male XLR receptacle, grounding: ground contact connected to shell ground, but not to front panel and Pin 1, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MBH"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MBH"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MBH_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mbh"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MBH-0"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MBH-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MBH-0_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mbh-0"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole male XLR receptacle, grounding: ground contact connected to shell ground, but not to front panel and Pin 1, steel retention lug, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MBH-1"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MBH-1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MBH-1_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mbh-1"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole male XLR receptacle, grounding: mating connector shell to pin1 and front panel, steel retention lug, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MBH-B"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MBH-B"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MBH-B_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mbh-b"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, horizontal PCB mount, black chrome shell"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MBH-E"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MBH-E"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MBH-E_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mbh-e"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, horizontal PCB mount, additional ground contacts"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MBHL"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MBHL"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MBHL_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mbhl"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, lateral left PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MBHL-B"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MBHL-B"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MBHL-B_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mbhl-b"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, lateral left PCB mount, black chrome shell"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MBHR"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MBHR"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MBHR_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mbhr"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, lateral right PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MBHR-B"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MBHR-B"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MBHR-B_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mbhr-b"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, lateral right PCB mount, black chrome shell"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MBV"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MBV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MBV_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mbv"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MBV-0"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MBV-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MBV-0_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mbv-0"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole male XLR receptacle, grounding: ground contact connected to shell ground, but not to front panel and Pin 1, steel retention lug, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MBV-1"
		(extends "XLR3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MBV-1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MBV-1_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mbv-1"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole male XLR receptacle, grounding: mating connector shell to pin1 and front panel, steel retention lug, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MBV-B"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MBV-B"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MBV-B_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mbv-b"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, vertical PCB mount, black chrome shell"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MBV-E"
		(extends "XLR3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MBV-E"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MBV-E_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mbv-e"
			(at 0 0 0)
		)
		(property "Description" "B Series, 3 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, steel retention lug, vertical PCB mount, additional ground contacts"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC3MBV-SW"
		(extends "XLR3_Ground_Switched")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC3MBV-SW"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC3MBV-SW_Vertical"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc3mbv-sw"
			(at 0 2.54 0)
		)
		(property "Description" "B Series, 3 pole male XLR receptacle, switching contacts, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector spdt switch neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC4FAH"
		(extends "XLR4_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC4FAH"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC4FAH_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc4fah"
			(at 0 0 0)
		)
		(property "Description" "A Series, 4 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC4FAH-0"
		(extends "XLR4_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC4FAH-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC4FAH-0_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc4fah-0"
			(at 0 0 0)
		)
		(property "Description" "A Series, 4 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, retention spring instead of latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC4FAV"
		(extends "XLR4_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC4FAV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC4FAV_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc4fav"
			(at 0 0 0)
		)
		(property "Description" "A Series, 4 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC4FAV-0"
		(extends "XLR4_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC4FAV-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC4FAV-0_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc4fav-0"
			(at 0 0 0)
		)
		(property "Description" "A Series, 4 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, retention spring instead of latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC4FBH"
		(extends "XLR4_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC4FBH"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC4FBH_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc4fbh"
			(at 0 0 0)
		)
		(property "Description" "B Series, 4 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC4FBV"
		(extends "XLR4_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC4FBV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC4FBV_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc4fbv"
			(at 0 0 0)
		)
		(property "Description" "B Series, 4 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC4MAH"
		(extends "XLR4_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC4MAH"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC4MAH_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc4mah"
			(at 0 0 0)
		)
		(property "Description" "A Series, 4 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC4MAV"
		(extends "XLR4_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC4MAV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC4MAV_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc4mav"
			(at 0 0 0)
		)
		(property "Description" "A Series, 4 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC4MBH"
		(extends "XLR4_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC4MBH"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC4MBH_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc4mbh"
			(at 0 0 0)
		)
		(property "Description" "B Series, 4 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC4MBV"
		(extends "XLR4_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC4MBV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC4MBV_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc4mbv"
			(at 0 0 0)
		)
		(property "Description" "B Series, 4 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC5FAH"
		(extends "XLR5_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC5FAH"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC5FAH_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc5fah"
			(at 0 0 0)
		)
		(property "Description" "A Series, 5 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC5FAH-0"
		(extends "XLR5_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC5FAH-0"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC5FAH-0_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc5fah-0"
			(at 0 0 0)
		)
		(property "Description" "A Series, 5 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, retention spring instead of latch"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC5FAH-DA"
		(extends "XLR5_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC5FAH-DA"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC5FAH-DA_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc5fah-da"
			(at 0 0 0)
		)
		(property "Description" "A Series, 5 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, asymmetric push"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC5FAV"
		(extends "XLR5_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC5FAV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC5FAV_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc5fav"
			(at 0 0 0)
		)
		(property "Description" "A Series, 5 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC5FAV-DA"
		(extends "XLR5_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC5FAV-DA"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC5FAV-DA_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc5fav-da"
			(at 0 0 0)
		)
		(property "Description" "A Series, 5 pole female XLR receptacle, grounding: mating connector shell to pin1 and front panel, horizontal PCB mount, asymmetric push"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC5FAV-SW"
		(extends "XLR5_Ground_Switched")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC5FAV-SW"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC5FAV-SW_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc5fav-sw"
			(at 0 0 0)
		)
		(property "Description" "A Series, 5 pole female XLR receptacle, switching contacts, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, color coding possible"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector spdt switch neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC5FBH"
		(extends "XLR5_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC5FBH"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC5FBH_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc5fbh"
			(at 0 0 0)
		)
		(property "Description" "B Series, 5 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC5FBH-B"
		(extends "XLR5_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC5FBH-B"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC5FBH-B_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc5fbh-b"
			(at 0 0 0)
		)
		(property "Description" "B Series, 5 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, black chrome shell"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC5FBV"
		(extends "XLR5_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC5FBV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC5FBV_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc5fbv"
			(at 0 0 0)
		)
		(property "Description" "B Series, 5 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC5FBV-B"
		(extends "XLR5_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC5FBV-B"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC5FBV-B_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc5fbv-b"
			(at 0 0 0)
		)
		(property "Description" "B Series, 5 pole female XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, black chrome shell"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC5FBV-SW"
		(extends "XLR5_Ground_Switched")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC5FBV-SW"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC5FBV-SW_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc5fbv-sw"
			(at 0 0 0)
		)
		(property "Description" "B Series, 5 pole female XLR receptacle, switching contacts, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector spdt switch neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC5MAH"
		(extends "XLR5_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC5MAH"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC5MAH_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc5mah"
			(at 0 0 0)
		)
		(property "Description" "A Series, 5 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC5MAV"
		(extends "XLR5_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC5MAV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC5MAV_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc5mav"
			(at 0 0 0)
		)
		(property "Description" "A Series, 5 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC5MAV-SW"
		(extends "XLR5_Ground_Switched")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC5MAV-SW"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC5MAV-SW_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc5mav-sw"
			(at 0 0 0)
		)
		(property "Description" "A Series, 5 pole male XLR receptacle, switching contacts, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector spdt switch neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC5MBH"
		(extends "XLR5_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC5MBH"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC5MBH_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc5mbh"
			(at 0 0 0)
		)
		(property "Description" "B Series, 5 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC5MBH-B"
		(extends "XLR5_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC5MBH-B"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC5MBH-B_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc5mbh-b"
			(at 0 0 0)
		)
		(property "Description" "B Series, 5 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, horizontal PCB mount, black chrome shell"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC5MBV"
		(extends "XLR5_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC5MBV"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC5MBV_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc5mbv"
			(at 0 0 0)
		)
		(property "Description" "B Series, 5 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC5MBV-B"
		(extends "XLR5_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC5MBV-B"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC5MBV-B_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc5mbv-b"
			(at 0 0 0)
		)
		(property "Description" "B Series, 5 pole male XLR receptacle, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount, black chrome shell"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NC5MBV-SW"
		(extends "XLR5_Ground_Switched")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NC5MBV-SW"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR_Neutrik_NC5MBV-SW_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nc5mbv-sw"
			(at 0 0 0)
		)
		(property "Description" "B Series, 5 pole male XLR receptacle, switching contacts, grounding: separate ground contact to mating connector shell and front panel, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector spdt switch neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ10FI-H"
		(extends "XLR3_AudioJack3_Combo_GroundSwitch_Switch")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ10FI-H"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ10FI-H_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj10fi-h"
			(at 0 0 0)
		)
		(property "Description" "Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) switching stereo jack and switching ground contact, horizontal PCB mount, retention spring"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ10FI-H-0"
		(extends "XLR3_AudioJack3_Combo_GroundSwitch_Switch")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ10FI-H-0"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ10FI-H-0_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj10fi-h-0"
			(at 0 0 0)
		)
		(property "Description" "Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) switching stereo jack and switching ground contact, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ10FI-V"
		(extends "XLR3_AudioJack3_Combo_GroundSwitch_Switch")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ10FI-V"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ10FI-V_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj10fi-v"
			(at 0 0 0)
		)
		(property "Description" "Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) switching stereo jack and switching ground contact, vertical PCB mount, retention spring"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ10FI-V-0"
		(extends "XLR3_AudioJack3_Combo_GroundSwitch_Switch")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ10FI-V-0"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ10FI-V-0_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj10fi-v-0"
			(at 0 0 0)
		)
		(property "Description" "Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) switching stereo jack and switching ground contact, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ5FI-H"
		(extends "XLR3_AudioJack2_Combo_Ground")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ5FI-H"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ5FI-H_Horizontal"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj5fi-h"
			(at 0 2.54 0)
		)
		(property "Description" "Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) mono jack without switching contact, horizontal PCB mount, retention spring"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ5FI-H-0"
		(extends "XLR3_AudioJack2_Combo_Ground")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ5FI-H-0"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ5FI-H-0_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj5fi-h-0"
			(at 0 0 0)
		)
		(property "Description" "Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) mono jack without switching contact, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ5FI-V"
		(extends "XLR3_AudioJack2_Combo_Ground")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ5FI-V"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ5FI-V_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj5fi-v"
			(at 0 0 0)
		)
		(property "Description" "Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) mono jack without switching contact, vertical PCB mount, retention spring"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ5FI-V-0"
		(extends "XLR3_AudioJack2_Combo_Ground")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ5FI-V-0"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ5FI-V-0_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj5fi-v-0"
			(at 0 0 0)
		)
		(property "Description" "Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) mono jack without switching contact, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ6FA-H"
		(extends "XLR3_AudioJack3_Combo_Ground")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ6FA-H"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ6FA-H_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj6fa-h"
			(at 0 0 0)
		)
		(property "Description" "Combo A series, 3 pole XLR female receptacle with 6.35mm (1/4in) stereo jack, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ6FA-H-0"
		(extends "XLR3_AudioJack3_Combo_Ground")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ6FA-H-0"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ6FA-H-0_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj6fa-h-0"
			(at 0 0 0)
		)
		(property "Description" "Combo A series, 3 pole XLR female receptacle with 6.35mm (1/4in) stereo jack, horizontal PCB mount, retention spring"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ6FA-H-DA"
		(extends "XLR3_AudioJack3_Combo_Ground")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ6FA-H-DA"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ6FA-H-DA_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj6fa-h-da"
			(at 0 0 0)
		)
		(property "Description" "Combo A series, 3 pole XLR female receptacle with 6.35mm (1/4in) stereo jack, horizontal PCB mount, asymmetric push"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ6FA-V"
		(extends "XLR3_AudioJack3_Combo_Ground")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ6FA-V"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ6FA-V_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj6fa-v"
			(at 0 0 0)
		)
		(property "Description" "Combo A series, 3 pole XLR female receptacle with 6.35mm (1/4in) stereo jack, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ6FA-V-0"
		(extends "XLR3_AudioJack3_Combo_Ground")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ6FA-V-0"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ6FA-V-0_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj6fa-v-0"
			(at 0 0 0)
		)
		(property "Description" "Combo A series, 3 pole XLR female receptacle with 6.35mm (1/4in) stereo jack, vertical PCB mount, retention spring"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ6FA-V-DA"
		(extends "XLR3_AudioJack3_Combo_Ground")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ6FA-V-DA"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ6FA-V-DA_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj6fa-v-da"
			(at 0 0 0)
		)
		(property "Description" "Combo A series, 3 pole XLR female receptacle with 6.35mm (1/4in) stereo jack, vertical PCB mount, asymmetric push"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ6FI-H"
		(extends "XLR3_AudioJack3_Combo_Ground")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ6FI-H"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ6FI-H_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj6fi-h"
			(at 0 0 0)
		)
		(property "Description" "Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) stereo jack without switching contact, horizontal PCB mount, retention spring"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ6FI-H-0"
		(extends "XLR3_AudioJack3_Combo_Ground")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ6FI-H-0"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ6FI-H-0_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj6fi-h-0"
			(at 0 0 0)
		)
		(property "Description" "Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) stereo jack without switching contact, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ6FI-V"
		(extends "XLR3_AudioJack3_Combo_Ground")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ6FI-V"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ6FI-V_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj6fi-v"
			(at 0 0 0)
		)
		(property "Description" "Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) stereo jack without switching contact, vertical PCB mount, retention spring"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ6FI-V-0"
		(extends "XLR3_AudioJack3_Combo_Ground")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ6FI-V-0"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ6FI-V-0_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj6fi-v-0"
			(at 0 0 0)
		)
		(property "Description" "Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) stereo jack without switching contact, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ9FI-H"
		(extends "XLR3_AudioJack3_Combo_Ground_Switch")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ9FI-H"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ9FI-H_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj9fi-h"
			(at 0 0 0)
		)
		(property "Description" "Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) switching stereo jack, horizontal PCB mount, retention spring"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ9FI-H-0"
		(extends "XLR3_AudioJack3_Combo_Ground_Switch")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ9FI-H-0"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ9FI-H-0_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj9fi-h-0"
			(at 0 0 0)
		)
		(property "Description" "Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) switching stereo jack, horizontal PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ9FI-V"
		(extends "XLR3_AudioJack3_Combo_Ground_Switch")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ9FI-V"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ9FI-V_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj9fi-v"
			(at 0 0 0)
		)
		(property "Description" "Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) switching stereo jack, vertical PCB mount, retention spring"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCJ9FI-V-0"
		(extends "XLR3_AudioJack3_Combo_Ground_Switch")
		(property "Reference" "J"
			(at 0 10.16 0)
		)
		(property "Value" "NCJ9FI-V-0"
			(at 0 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_XLR-6.35mm_Neutrik_NCJ9FI-V-0_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/ncj9fi-v-0"
			(at 0 0 0)
		)
		(property "Description" "Combo I series, 3 pole XLR female receptacle with 6.35mm (1/4in) switching stereo jack, vertical PCB mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "xlr connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*XLR*6.35mm*"
			(at 0 0 0)
		)
	)
	(symbol "NJ2FD-V"
		(extends "AudioJack2")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NJ2FD-V"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NJ2FD-V_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nj2fd-v"
			(at 0 0 0)
		)
		(property "Description" "6.35mm (1/4 in) Vertical Jack, Non-switching mono jack (T/S)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle mono phone headphone TS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NJ3FD-V"
		(extends "AudioJack3")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NJ3FD-V"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NJ3FD-V_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nj3fd-v"
			(at 0 0 0)
		)
		(property "Description" "6.35mm (1/4 in) Vertical Jack, Non-switching stereo jack (T/R/S)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NJ5FD-V"
		(extends "AudioJack3_SwitchTR")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NJ5FD-V"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NJ5FD-V_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nj5fd-v"
			(at 0 0 0)
		)
		(property "Description" "6.35mm (1/4 in) Vertical Jack, 2 x switching (normalling) stereo jack (T/TN/R/RN/S)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NJ6FD-V"
		(extends "AudioJack3_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NJ6FD-V"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NJ6FD-V_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nj6fd-v"
			(at 0 0 0)
		)
		(property "Description" "6.35mm (1/4 in) Vertical Jack, 3 x switching (normalling) stereo jack (T/TN/R/RN/S/SN)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NJ6TB-V"
		(extends "AudioJack3_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NJ6TB-V"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NJ6TB-V_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nj6tb-v"
			(at 0 0 0)
		)
		(property "Description" "6.35mm (1/4 in) Vertical Jack, 3 x switching (normalling) stereo jack  B-gauge type (T/TN/R/RN/S/SN)"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NL2MDXX-H-3"
		(extends "SpeakON_NL2")
		(property "Reference" "J"
			(at 2.54 8.89 0)
		)
		(property "Value" "NL2MDXX-H-3"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_speakON_Neutrik_NL2MDXX-H-3_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nl2mdxx-h-3"
			(at 0 0 0)
		)
		(property "Description" "speakON Chassis Connectors, 2 pole chassis connector, gray D-size flange, countersunk thru holes, horizontal PCB. Replaces NL2MD-H"
			(at 0 0 0)
		)
		(property "ki_keywords" "speakon connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*speakON*"
			(at 0 0 0)
		)
	)
	(symbol "NL2MDXX-V"
		(extends "SpeakON_NL2")
		(property "Reference" "J"
			(at 2.54 8.89 0)
		)
		(property "Value" "NL2MDXX-V"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_speakON_Neutrik_NL2MDXX-V_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nl2mdxx-v"
			(at 0 0 0)
		)
		(property "Description" "speakON Chassis Connectors, 2 pole chassis connector, black D-size flange, countersunk thru holes, vertical PCB mount. Replaces NL2MD-V"
			(at 0 0 0)
		)
		(property "ki_keywords" "speakon connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*speakON*"
			(at 0 0 0)
		)
	)
	(symbol "NL4MDXX-H-2"
		(extends "SpeakON_NL4")
		(property "Reference" "J"
			(at 2.54 8.89 0)
		)
		(property "Value" "NL4MDXX-H-2"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_speakON_Neutrik_NL4MDXX-H-2_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nl4mdxx-h-2"
			(at 0 0 0)
		)
		(property "Description" "speakON Chassis Connectors, 4 pole chassis connector, black D-size flange, mirrored self tapping screw holes (A-screw), horizontal PCB mount. Replaces NL4MD-H-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "speakon connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*speakON*"
			(at 0 0 0)
		)
	)
	(symbol "NL4MDXX-H-3"
		(extends "SpeakON_NL4")
		(property "Reference" "J"
			(at 2.54 8.89 0)
		)
		(property "Value" "NL4MDXX-H-3"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_speakON_Neutrik_NL4MDXX-H-3_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nl4mdxx-h-3"
			(at 0 0 0)
		)
		(property "Description" "speakON Chassis Connectors, 4 pole chassis connector, grey D-size flange, self tapping screw holes (A-screw), horizontal PCB mount. Replaces NL4MD-H, NL4MD-V-R, and NL4MD-V-S"
			(at 0 0 0)
		)
		(property "ki_keywords" "speakon connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*speakON*"
			(at 0 0 0)
		)
	)
	(symbol "NL4MDXX-V"
		(extends "SpeakON_NL4")
		(property "Reference" "J"
			(at 2.54 8.89 0)
		)
		(property "Value" "NL4MDXX-V"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_speakON_Neutrik_NL4MDXX-V_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nl4mdxx-v"
			(at 0 0 0)
		)
		(property "Description" "speakON Chassis Connectors, 4 pole chassis connector, black D-size flange, countersunk thru holes, vertical PCB mount. Replaces NL4MD-V, NL4MD-V-R, and NL4MD-V-S"
			(at 0 0 0)
		)
		(property "ki_keywords" "speakon connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*speakON*"
			(at 0 0 0)
		)
	)
	(symbol "NL4MDXX-V-2"
		(extends "SpeakON_NL4")
		(property "Reference" "J"
			(at 2.54 8.89 0)
		)
		(property "Value" "NL4MDXX-V-2"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_speakON_Neutrik_NL4MDXX-V-2_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nl4mdxx-v-2"
			(at 0 0 0)
		)
		(property "Description" "speakON Chassis Connectors, 4 pole chassis connector, black D-size flange, mirrored self tapping screw holes (A-screw), vertical PCB mount. Replaces NL4MD-V-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "speakon connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*speakON*"
			(at 0 0 0)
		)
	)
	(symbol "NL4MDXX-V-3"
		(extends "SpeakON_NL4")
		(property "Reference" "J"
			(at 2.54 8.89 0)
		)
		(property "Value" "NL4MDXX-V-3"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_speakON_Neutrik_NL4MDXX-V-3_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nl4mdxx-v-3"
			(at 0 0 0)
		)
		(property "Description" "speakON Chassis Connectors, 4 pole chassis connector, grey D-size flange, self tapping screw holes (A-screw), vertical PCB mount. Replaces NL4MD-V-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "speakon connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*speakON*"
			(at 0 0 0)
		)
	)
	(symbol "NL8MDXX-V"
		(extends "SpeakON_NL8")
		(property "Reference" "J"
			(at 2.54 10.16 0)
		)
		(property "Value" "NL8MDXX-V"
			(at 7.62 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_speakON_Neutrik_NL8MDXX-V_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nl8mdxx-v"
			(at 0 0 0)
		)
		(property "Description" "speakON Chassis Connectors, 8 pole chassis connector, nickel metal square G-size flange, countersunk thru holes, vertical PCB mount. Replaces NL8MD-V"
			(at 0 0 0)
		)
		(property "ki_keywords" "speakon connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*speakON*"
			(at 0 0 0)
		)
	)
	(symbol "NL8MDXX-V-3"
		(extends "SpeakON_NL8")
		(property "Reference" "J"
			(at 2.54 10.16 0)
		)
		(property "Value" "NL8MDXX-V-3"
			(at 7.62 7.62 0)
		)
		(property "Footprint" "Connector_Audio:Jack_speakON_Neutrik_NL8MDXX-V-3_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nl8mdxx-v-3"
			(at 0 0 0)
		)
		(property "Description" "speakON Chassis Connectors, 8 pole chassis connector, nickel metal square G-size flange, self tapping screw holes (A-screw), vertical PCB mount. Replaces NL8MD-V-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "speakon connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*speakON*"
			(at 0 0 0)
		)
	)
	(symbol "NLJ2MDXX-H"
		(extends "SpeakON_NL2_AudioJack2_Combo")
		(property "Reference" "J"
			(at 2.54 8.89 0)
		)
		(property "Value" "NLJ2MDXX-H"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_speakON-6.35mm_Neutrik_NLJ2MDXX-H_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nlj2mdxx-h"
			(at 0 0 0)
		)
		(property "Description" "speakON Combo, 2 pole combination of speakON socket and 6.35mm (1/4in) jack receptacle, horizontal pcb mount. Replaces NLJ2MD-H"
			(at 0 0 0)
		)
		(property "ki_keywords" "speakon connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*speakON*"
			(at 0 0 0)
		)
	)
	(symbol "NLJ2MDXX-V"
		(extends "SpeakON_NL2_AudioJack2_Combo")
		(property "Reference" "J"
			(at 2.54 8.89 0)
		)
		(property "Value" "NLJ2MDXX-V"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_speakON-6.35mm_Neutrik_NLJ2MDXX-V_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nlj2mdxx-v"
			(at 0 0 0)
		)
		(property "Description" "speakON Combo, 2 pole combination of speakON socket and 6.35mm (1/4in) jack receptacle, vertical pcb mount. Replaces NLJ2MD-V"
			(at 0 0 0)
		)
		(property "ki_keywords" "speakon connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*speakON*"
			(at 0 0 0)
		)
	)
	(symbol "NLT4MD-V"
		(extends "SpeakON_NL4")
		(property "Reference" "J"
			(at 2.54 8.89 0)
		)
		(property "Value" "NLT4MD-V"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_speakON_Neutrik_NLT4MD-V_Vertical"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nlt4md-v"
			(at 0 0 0)
		)
		(property "Description" "STX Series, 4 pole male chassis connector, metal housing, vertical PCB mount,  self tapping screw holes (A-screw)"
			(at 0 0 0)
		)
		(property "ki_keywords" "speakon connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*speakON*"
			(at 0 0 0)
		)
	)
	(symbol "NMJ4HCD2"
		(extends "AudioJack2_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NMJ4HCD2"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NMJ4HCD2_Horizontal"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nmj4hcd2"
			(at 0 5.08 0)
		)
		(property "Description" "M Series, 6.35mm (1/4in) mono jack, switched, with chrome ferrule and straight PCB pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle mono headphones phone TS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NMJ4HFD2"
		(extends "AudioJack2_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NMJ4HFD2"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NMJ4HFD2_Horizontal"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nmj4hfd2"
			(at 0 5.08 0)
		)
		(property "Description" "M Series, 6.35mm (1/4in) mono jack, switched, with full threaded nose and straight PCB pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle mono headphones phone TS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NMJ4HFD3"
		(extends "AudioJack2_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NMJ4HFD3"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NMJ4HFD3_Horizontal"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nmj4hfd3"
			(at 0 5.08 0)
		)
		(property "Description" "M Series, 6.35mm (1/4in) mono jack, switched, with a full threaded nose and offset PCB pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle mono headphones phone TS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NMJ4HHD2"
		(extends "AudioJack2_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NMJ4HHD2"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NMJ4HHD2_Horizontal"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nmj4hhd2"
			(at 0 5.08 0)
		)
		(property "Description" "M Series, 6.35mm (1/4in) mono jack, switched, with a half threaded nose and offset PCB pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle mono headphones phone TS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NMJ6HCD2"
		(extends "AudioJack3_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NMJ6HCD2"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NMJ6HCD2_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nmj6hcd2"
			(at 0 0 0)
		)
		(property "Description" "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NMJ6HCD3"
		(extends "AudioJack3_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NMJ6HCD3"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NMJ6HCD3_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nmj6hcd3"
			(at 0 0 0)
		)
		(property "Description" "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and offset PCB pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NMJ6HFD2"
		(extends "AudioJack3_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NMJ6HFD2"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NMJ6HFD2_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nmj6hfd2"
			(at 0 0 0)
		)
		(property "Description" "M Series, 6.35mm (1/4in) stereo jack, switched, with full threaded nose and straight PCB pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NMJ6HFD2-AU"
		(extends "AudioJack3_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NMJ6HFD2-AU"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NMJ6HFD2-AU_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nmj6hfd2-au"
			(at 0 0 0)
		)
		(property "Description" "M Series, 6.35mm (1/4in) stereo jack, switched, full threaded nose, straight PCB pins, gold plated contacts"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NMJ6HFD3"
		(extends "AudioJack3_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NMJ6HFD3"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NMJ6HFD3_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nmj6hfd3"
			(at 0 0 0)
		)
		(property "Description" "M Series, 6.35mm (1/4in) stereo jack, switched, with full threaded nose and offset PCB pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NMJ6HFD4"
		(extends "AudioJack3_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NMJ6HFD4"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NMJ6HFD4_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nmj6hfd4"
			(at 0 0 0)
		)
		(property "Description" "Obsolete: M Series, 6.35mm (1/4in) stereo jack, switched, with full threaded nose and fishtail PCB pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NMJ6HHD2"
		(extends "AudioJack3_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NMJ6HHD2"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NMJ6HHD2_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nmj6hhd2"
			(at 0 0 0)
		)
		(property "Description" "M Series, 6.35mm (1/4in) stereo jack, switched, with half threaded nose and offset PCB pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NRJ3HF-1"
		(extends "AudioJack3_Ground")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NRJ3HF-1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NRJ3HF-1_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nrj3hf-1"
			(at 0 0 0)
		)
		(property "Description" "Slim Jacks, 6.35mm (1/4in) stereo jack, unswitched, fully threaded nose, sleeve contact/front panel connection"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NRJ4HF"
		(extends "AudioJack2_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NRJ4HF"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NRJ4HF_Horizontal"
			(at -1.27 5.08 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nrj4hf"
			(at -1.27 5.08 0)
		)
		(property "Description" "Slim Jacks, 6.35mm (1/4in) mono jack, switched, fully threaded nose"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack dual receptacle mono headphones phone TS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NRJ4HF-1"
		(extends "AudioJack2_Ground_SwitchT")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NRJ4HF-1"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NRJ4HF-1_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nrj4hf-1"
			(at 0 0 0)
		)
		(property "Description" "Slim Jacks, 6.35mm (1/4in) mono jack, switched, fully threaded nose, sleeve contact/front panel connection"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NRJ4HH"
		(extends "AudioJack2_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NRJ4HH"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NRJ4HH_Horizontal"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nrj4hh"
			(at 0 5.08 0)
		)
		(property "Description" "Slim Jacks, 6.35mm (1/4in) mono jack, switched, half threaded nose"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle mono headphones phone TS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NRJ4HH-1"
		(extends "AudioJack2_Ground_SwitchT")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NRJ4HH-1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NRJ4HH-1_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nrj4hh-1"
			(at 0 0 0)
		)
		(property "Description" "Slim Jacks, 6.35mm (1/4in) mono jack, switched, half threaded nose, sleeve contact/front panel connection"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle mono headphones phone TS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NRJ6HF"
		(extends "AudioJack3_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NRJ6HF"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NRJ6HF_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nrj6hf"
			(at 0 0 0)
		)
		(property "Description" "Slim Jacks, 6.35mm (1/4in) stereo jack, switched, fully threaded nose"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NRJ6HF-1"
		(extends "AudioJack3_Ground_SwitchTR")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NRJ6HF-1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NRJ6HF-1_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nrj6hf-1"
			(at 0 0 0)
		)
		(property "Description" "Slim Jacks, 6.35mm (1/4in) stereo jack, switched, fully threaded nose, sleeve contact/front panel connection"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NRJ6HF-1-AU"
		(extends "AudioJack3_Ground_SwitchTR")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NRJ6HF-1-AU"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NRJ6HF-1-AU_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nrj6hf-1-au"
			(at 0 0 0)
		)
		(property "Description" "Slim Jacks, 6.35mm (1/4in) stereo jack, switched, gold plated contacts, fully threaded nose, sleeve contact/front panel connection"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NRJ6HF-AU"
		(extends "AudioJack3_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NRJ6HF-AU"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NRJ6HF-AU_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nrj6hf-au"
			(at 0 0 0)
		)
		(property "Description" "Slim Jacks, 6.35mm (1/4in) stereo jack, switched, gold plated contacts, fully threaded nose"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NRJ6HH"
		(extends "AudioJack3_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NRJ6HH"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NRJ6HH_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nrj6hh"
			(at 0 0 0)
		)
		(property "Description" "Slim Jacks, 6.35mm (1/4in) stereo jack, switched, half threaded nose"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NRJ6HH-1"
		(extends "AudioJack3_Ground_SwitchTR")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NRJ6HH-1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NRJ6HH-1_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nrj6hh-1"
			(at 0 0 0)
		)
		(property "Description" "Slim Jacks, 6.35mm (1/4in) stereo jack, switched, half threaded nose, sleeve contact/front panel connection"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NRJ6HH-AU"
		(extends "AudioJack3_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NRJ6HH-AU"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NRJ6HH-AU_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nrj6hh-au"
			(at 0 0 0)
		)
		(property "Description" "Slim Jacks, 6.35mm (1/4in) stereo jack, switched, gold plated contacts, half threaded nose"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NRJ6HM-1"
		(extends "AudioJack3_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NRJ6HM-1"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NRJ6HM-1_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nrj6hm-1"
			(at 0 0 0)
		)
		(property "Description" "Slim Jacks, 6.35mm (1/4in) stereo jack, metal nose with efficient chassis ground connection, T+R+S normalling contact"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NRJ6HM-1-AU"
		(extends "AudioJack3_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NRJ6HM-1-AU"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NRJ6HM-1-AU_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nrj6hm-1-au"
			(at 0 0 0)
		)
		(property "Description" "Slim Jacks, 6.35mm (1/4in) stereo jack, metal nose, gold plated contacts, efficient chassis ground connection, T+R+S normalling contact"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NRJ6HM-1-PRE"
		(extends "AudioJack3_SwitchTR")
		(property "Reference" "J"
			(at 0 8.89 0)
		)
		(property "Value" "NRJ6HM-1-PRE"
			(at 0 6.35 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NRJ6HM-1-PRE_Horizontal"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nrj6hm-1-pre"
			(at 0 0 0)
		)
		(property "Description" "Slim Jacks, 6.35mm (1/4in) stereo jack, metal nose, efficient chassis ground connection, T+R normalling contact"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NSJ12HC"
		(extends "AudioJack3_Dual_Ground_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NSJ12HC"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NSJ12HC_Horizontal"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nsj12hc"
			(at -1.27 0 0)
		)
		(property "Description" "Stacking Jacks, Stereo dual jack, full nose"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack dual receptacle stereo headphones phones TRS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NSJ12HF-1"
		(extends "AudioJack3_Dual_Ground_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NSJ12HF-1"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NSJ12HF-1_Horizontal"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nsj12hf-1"
			(at -1.27 0 0)
		)
		(property "Description" "Stacking Jacks, Stereo dual jack, full threaded nose"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack dual receptacle stereo headphones phones TRS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NSJ12HH-1"
		(extends "AudioJack3_Dual_Ground_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NSJ12HH-1"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NSJ12HH-1_Horizontal"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nsj12hh-1"
			(at -1.27 0 0)
		)
		(property "Description" "Obsolete: Stacking Jacks, Stereo dual jack, half threaded nose"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack dual receptacle stereo headphones phones TRS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NSJ12HL"
		(extends "AudioJack3_Dual_Ground_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NSJ12HL"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NSJ12HL_Horizontal"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nsj12hl"
			(at -1.27 0 0)
		)
		(property "Description" "Obsolete: Stacking Jacks, Stereo dual jack, quick fix nose"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack dual receptacle stereo headphones phones TRS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NSJ8HC"
		(extends "AudioJack2_Dual_Ground_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NSJ8HC"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NSJ8HC_Horizontal"
			(at -1.27 5.08 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nsj8hc"
			(at -1.27 5.08 0)
		)
		(property "Description" "Obsolete: Stacking Jacks, Mono dual jack, full nose"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack dual receptacle mono headphones phone TS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
	(symbol "NSJ8HL"
		(extends "AudioJack2_Dual_Ground_Switch")
		(property "Reference" "J"
			(at 0 11.43 0)
		)
		(property "Value" "NSJ8HL"
			(at 0 8.89 0)
		)
		(property "Footprint" "Connector_Audio:Jack_6.35mm_Neutrik_NSJ8HL_Horizontal"
			(at -1.27 5.08 0)
		)
		(property "Datasheet" "https://www.neutrik.com/en/product/nsj8hl"
			(at -1.27 5.08 0)
		)
		(property "Description" "Obsolete: Stacking Jacks, Mono dual jack, quick fix nose"
			(at 0 0 0)
		)
		(property "ki_keywords" "audio jack dual receptacle mono headphones phone TS connector neutrik"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jack*"
			(at 0 0 0)
		)
	)
)
