(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "Conn_01x01_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 2.286 0)
		)
		(property "Value" "Conn_01x01_Shielded"
			(at 1.016 -2.286 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x01_Shielded_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x02_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 2.286 0)
		)
		(property "Value" "Conn_01x02_Shielded"
			(at 1.016 -4.826 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x02_Shielded_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x03_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 4.826 0)
		)
		(property "Value" "Conn_01x03_Shielded"
			(at 1.016 -4.826 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x03_Shielded_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x04_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 4.826 0)
		)
		(property "Value" "Conn_01x04_Shielded"
			(at 1.016 -7.366 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x04_Shielded_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x05_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 7.366 0)
		)
		(property "Value" "Conn_01x05_Shielded"
			(at 1.016 -7.366 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x05_Shielded_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x06_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 7.366 0)
		)
		(property "Value" "Conn_01x06_Shielded"
			(at 1.016 -9.906 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x06_Shielded_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x07_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 9.906 0)
		)
		(property "Value" "Conn_01x07_Shielded"
			(at 1.016 -9.906 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x07_Shielded_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x08_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 9.906 0)
		)
		(property "Value" "Conn_01x08_Shielded"
			(at 1.016 -12.446 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x08_Shielded_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x09_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 12.446 0)
		)
		(property "Value" "Conn_01x09_Shielded"
			(at 1.016 -12.446 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x09, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x09_Shielded_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x10_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 12.446 0)
		)
		(property "Value" "Conn_01x10_Shielded"
			(at 1.016 -14.986 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x10_Shielded_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x11_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 14.986 0)
		)
		(property "Value" "Conn_01x11_Shielded"
			(at 1.016 -14.986 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x11, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x11_Shielded_1_1"
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x12_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 14.986 0)
		)
		(property "Value" "Conn_01x12_Shielded"
			(at 1.016 -17.526 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x12, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x12_Shielded_1_1"
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x13_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 17.526 0)
		)
		(property "Value" "Conn_01x13_Shielded"
			(at 1.016 -17.526 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x13, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x13_Shielded_1_1"
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x14_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 17.526 0)
		)
		(property "Value" "Conn_01x14_Shielded"
			(at 1.016 -20.066 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x14, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x14_Shielded_1_1"
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x15_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 20.066 0)
		)
		(property "Value" "Conn_01x15_Shielded"
			(at 1.016 -20.066 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x15, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x15_Shielded_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x16_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 20.066 0)
		)
		(property "Value" "Conn_01x16_Shielded"
			(at 1.016 -22.606 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x16, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x16_Shielded_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x17_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 22.606 0)
		)
		(property "Value" "Conn_01x17_Shielded"
			(at 1.016 -22.606 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x17, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x17_Shielded_1_1"
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x18_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 22.606 0)
		)
		(property "Value" "Conn_01x18_Shielded"
			(at 1.016 -25.146 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x18, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x18_Shielded_1_1"
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x19_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 25.146 0)
		)
		(property "Value" "Conn_01x19_Shielded"
			(at 1.016 -25.146 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x19, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x19_Shielded_1_1"
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x20_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 25.146 0)
		)
		(property "Value" "Conn_01x20_Shielded"
			(at 1.016 -27.686 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x20, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x20_Shielded_1_1"
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x21_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 27.686 0)
		)
		(property "Value" "Conn_01x21_Shielded"
			(at 1.016 -27.686 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x21, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x21_Shielded_1_1"
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x22_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 27.686 0)
		)
		(property "Value" "Conn_01x22_Shielded"
			(at 1.016 -30.226 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x22, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x22_Shielded_1_1"
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x23_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 30.226 0)
		)
		(property "Value" "Conn_01x23_Shielded"
			(at 1.016 -30.226 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x23, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x23_Shielded_1_1"
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x24_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 30.226 0)
		)
		(property "Value" "Conn_01x24_Shielded"
			(at 1.016 -32.766 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x24, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x24_Shielded_1_1"
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x25_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 32.766 0)
		)
		(property "Value" "Conn_01x25_Shielded"
			(at 1.016 -32.766 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x25, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x25_Shielded_1_1"
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x26_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 32.766 0)
		)
		(property "Value" "Conn_01x26_Shielded"
			(at 1.016 -35.306 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x26, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x26_Shielded_1_1"
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x27_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 35.306 0)
		)
		(property "Value" "Conn_01x27_Shielded"
			(at 1.016 -35.306 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x27, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x27_Shielded_1_1"
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x28_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 35.306 0)
		)
		(property "Value" "Conn_01x28_Shielded"
			(at 1.016 -37.846 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x28, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x28_Shielded_1_1"
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x29_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 37.846 0)
		)
		(property "Value" "Conn_01x29_Shielded"
			(at 1.016 -37.846 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x29, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x29_Shielded_1_1"
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x30_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 37.846 0)
		)
		(property "Value" "Conn_01x30_Shielded"
			(at 1.016 -40.386 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x30, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x30_Shielded_1_1"
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x31_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 40.386 0)
		)
		(property "Value" "Conn_01x31_Shielded"
			(at 1.016 -40.386 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x31, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x31_Shielded_1_1"
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x32_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 40.386 0)
		)
		(property "Value" "Conn_01x32_Shielded"
			(at 1.016 -42.926 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x32, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x32_Shielded_1_1"
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x33_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 42.926 0)
		)
		(property "Value" "Conn_01x33_Shielded"
			(at 1.016 -42.926 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x33, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x33_Shielded_1_1"
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x34_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 42.926 0)
		)
		(property "Value" "Conn_01x34_Shielded"
			(at 1.016 -45.466 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x34, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x34_Shielded_1_1"
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x35_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 45.466 0)
		)
		(property "Value" "Conn_01x35_Shielded"
			(at 1.016 -45.466 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x35, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x35_Shielded_1_1"
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x36_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 45.466 0)
		)
		(property "Value" "Conn_01x36_Shielded"
			(at 1.016 -48.006 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x36, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x36_Shielded_1_1"
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x37_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 48.006 0)
		)
		(property "Value" "Conn_01x37_Shielded"
			(at 1.016 -48.006 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x37, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x37_Shielded_1_1"
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x38_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 48.006 0)
		)
		(property "Value" "Conn_01x38_Shielded"
			(at 1.016 -50.546 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x38, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x38_Shielded_1_1"
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x39_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 50.546 0)
		)
		(property "Value" "Conn_01x39_Shielded"
			(at 1.016 -50.546 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x39, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x39_Shielded_1_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x40_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 50.546 0)
		)
		(property "Value" "Conn_01x40_Shielded"
			(at 1.016 -53.086 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, single row, 01x40, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x40_Shielded_1_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x41_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 53.086 0)
		)
		(property "Value" "Conn_01x41_Shielded"
			(at 1.016 -53.086 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, single row, 01x41, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x41_Shielded_1_1"
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x42_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 53.086 0)
		)
		(property "Value" "Conn_01x42_Shielded"
			(at 1.016 -55.626 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, single row, 01x42, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x42_Shielded_1_1"
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x43_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 55.626 0)
		)
		(property "Value" "Conn_01x43_Shielded"
			(at 1.016 -55.626 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, single row, 01x43, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x43_Shielded_1_1"
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x44_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 55.626 0)
		)
		(property "Value" "Conn_01x44_Shielded"
			(at 1.016 -58.166 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, single row, 01x44, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x44_Shielded_1_1"
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 0 -60.96 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x45_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 58.166 0)
		)
		(property "Value" "Conn_01x45_Shielded"
			(at 1.016 -58.166 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, single row, 01x45, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x45_Shielded_1_1"
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 0 -60.96 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x46_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 58.166 0)
		)
		(property "Value" "Conn_01x46_Shielded"
			(at 1.016 -60.706 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, single row, 01x46, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x46_Shielded_1_1"
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x47_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 60.706 0)
		)
		(property "Value" "Conn_01x47_Shielded"
			(at 1.016 -60.706 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, single row, 01x47, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x47_Shielded_1_1"
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x48_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 60.706 0)
		)
		(property "Value" "Conn_01x48_Shielded"
			(at 1.016 -63.246 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, single row, 01x48, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x48_Shielded_1_1"
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x49_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 63.246 0)
		)
		(property "Value" "Conn_01x49_Shielded"
			(at 1.016 -63.246 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, single row, 01x49, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x49_Shielded_1_1"
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x50_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 63.246 0)
		)
		(property "Value" "Conn_01x50_Shielded"
			(at 1.016 -65.786 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, single row, 01x50, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x50_Shielded_1_1"
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x51_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 65.786 0)
		)
		(property "Value" "Conn_01x51_Shielded"
			(at 1.016 -65.786 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, single row, 01x51, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x51_Shielded_1_1"
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x52_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 65.786 0)
		)
		(property "Value" "Conn_01x52_Shielded"
			(at 1.016 -68.326 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, single row, 01x52, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x52_Shielded_1_1"
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x53_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 68.326 0)
		)
		(property "Value" "Conn_01x53_Shielded"
			(at 1.016 -68.326 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, single row, 01x53, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x53_Shielded_1_1"
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x54_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 68.326 0)
		)
		(property "Value" "Conn_01x54_Shielded"
			(at 1.016 -70.866 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, single row, 01x54, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x54_Shielded_1_1"
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x55_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 70.866 0)
		)
		(property "Value" "Conn_01x55_Shielded"
			(at 1.016 -70.866 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, single row, 01x55, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x55_Shielded_1_1"
			(pin passive line
				(at -5.08 68.58 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x56_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 70.866 0)
		)
		(property "Value" "Conn_01x56_Shielded"
			(at 1.016 -73.406 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, single row, 01x56, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x56_Shielded_1_1"
			(pin passive line
				(at -5.08 68.58 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 0 -76.2 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x57_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 73.406 0)
		)
		(property "Value" "Conn_01x57_Shielded"
			(at 1.016 -73.406 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, single row, 01x57, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x57_Shielded_1_1"
			(pin passive line
				(at -5.08 71.12 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 68.58 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 0 -76.2 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x58_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 73.406 0)
		)
		(property "Value" "Conn_01x58_Shielded"
			(at 1.016 -75.946 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, single row, 01x58, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x58_Shielded_1_1"
			(pin passive line
				(at -5.08 71.12 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 68.58 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -73.66 0)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 0 -78.74 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x59_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 75.946 0)
		)
		(property "Value" "Conn_01x59_Shielded"
			(at 1.016 -75.946 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, single row, 01x59, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x59_Shielded_1_1"
			(pin passive line
				(at -5.08 73.66 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 71.12 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 68.58 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at -5.08 -73.66 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 0 -78.74 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_01x60_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0.254 75.946 0)
		)
		(property "Value" "Conn_01x60_Shielded"
			(at 1.016 -78.486 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, single row, 01x60, script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_1x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_01x60_Shielded_1_1"
			(pin passive line
				(at -5.08 73.66 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 71.12 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 68.58 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at -5.08 -73.66 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at -5.08 -76.2 0)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 0 -81.28 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x01_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 2.286 0)
		)
		(property "Value" "Conn_02x01_Row_Letter_First_Shielded"
			(at 2.286 -2.286 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x01, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x01_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at 1.27 -5.08 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x01_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 2.286 0)
		)
		(property "Value" "Conn_02x01_Row_Letter_Last_Shielded"
			(at 2.286 -2.286 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x01, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x01_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at 1.27 -5.08 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x01_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 2.286 0)
		)
		(property "Value" "Conn_02x01_Shielded"
			(at 2.286 -2.286 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x01, this symbol is compatible with counter-clockwise, top-bottom and odd-even numbering schemes., script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x01_Shielded_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at 1.27 -5.08 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x02_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 2.286 0)
		)
		(property "Value" "Conn_02x02_Counter_Clockwise_Shielded"
			(at 2.286 -4.826 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x02, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x02_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 1.27 -7.62 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x02_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 2.286 0)
		)
		(property "Value" "Conn_02x02_Odd_Even_Shielded"
			(at 2.286 -4.826 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x02_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 1.27 -7.62 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x02_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 2.286 0)
		)
		(property "Value" "Conn_02x02_Row_Letter_First_Shielded"
			(at 2.286 -4.826 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x02, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x02_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at 1.27 -7.62 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x02_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 2.286 0)
		)
		(property "Value" "Conn_02x02_Row_Letter_Last_Shielded"
			(at 2.286 -4.826 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x02, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x02_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at 1.27 -7.62 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x02_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 2.286 0)
		)
		(property "Value" "Conn_02x02_Top_Bottom_Shielded"
			(at 2.286 -4.826 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x02, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x02_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 1.27 -7.62 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x03_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 4.826 0)
		)
		(property "Value" "Conn_02x03_Counter_Clockwise_Shielded"
			(at 2.286 -4.826 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x03, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x03_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 1.27 -7.62 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x03_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 4.826 0)
		)
		(property "Value" "Conn_02x03_Odd_Even_Shielded"
			(at 2.286 -4.826 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x03_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 1.27 -7.62 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x03_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 4.826 0)
		)
		(property "Value" "Conn_02x03_Row_Letter_First_Shielded"
			(at 2.286 -4.826 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x03, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x03_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at 1.27 -7.62 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x03_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 4.826 0)
		)
		(property "Value" "Conn_02x03_Row_Letter_Last_Shielded"
			(at 2.286 -4.826 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x03, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x03_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at 1.27 -7.62 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x03_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 4.826 0)
		)
		(property "Value" "Conn_02x03_Top_Bottom_Shielded"
			(at 2.286 -4.826 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x03, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x03_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at 1.27 -7.62 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x04_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 4.826 0)
		)
		(property "Value" "Conn_02x04_Counter_Clockwise_Shielded"
			(at 2.286 -7.366 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x04, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x04_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 1.27 -10.16 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x04_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 4.826 0)
		)
		(property "Value" "Conn_02x04_Odd_Even_Shielded"
			(at 2.286 -7.366 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x04, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x04_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 1.27 -10.16 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x04_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 4.826 0)
		)
		(property "Value" "Conn_02x04_Row_Letter_First_Shielded"
			(at 2.286 -7.366 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x04, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x04_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at 1.27 -10.16 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x04_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 4.826 0)
		)
		(property "Value" "Conn_02x04_Row_Letter_Last_Shielded"
			(at 2.286 -7.366 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x04, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x04_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at 1.27 -10.16 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x04_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 4.826 0)
		)
		(property "Value" "Conn_02x04_Top_Bottom_Shielded"
			(at 2.286 -7.366 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x04, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x04_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 1.27 -10.16 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x05_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 7.366 0)
		)
		(property "Value" "Conn_02x05_Counter_Clockwise_Shielded"
			(at 2.286 -7.366 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x05, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x05_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 1.27 -10.16 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x05_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 7.366 0)
		)
		(property "Value" "Conn_02x05_Odd_Even_Shielded"
			(at 2.286 -7.366 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x05_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 1.27 -10.16 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x05_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 7.366 0)
		)
		(property "Value" "Conn_02x05_Row_Letter_First_Shielded"
			(at 2.286 -7.366 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x05, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x05_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at 1.27 -10.16 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x05_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 7.366 0)
		)
		(property "Value" "Conn_02x05_Row_Letter_Last_Shielded"
			(at 2.286 -7.366 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x05, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x05_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at 1.27 -10.16 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x05_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 7.366 0)
		)
		(property "Value" "Conn_02x05_Top_Bottom_Shielded"
			(at 2.286 -7.366 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x05, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x05_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 1.27 -10.16 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x06_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 7.366 0)
		)
		(property "Value" "Conn_02x06_Counter_Clockwise_Shielded"
			(at 2.286 -9.906 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x06, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x06_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 1.27 -12.7 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x06_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 7.366 0)
		)
		(property "Value" "Conn_02x06_Odd_Even_Shielded"
			(at 2.286 -9.906 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x06, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x06_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 1.27 -12.7 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x06_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 7.366 0)
		)
		(property "Value" "Conn_02x06_Row_Letter_First_Shielded"
			(at 2.286 -9.906 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x06, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x06_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at 1.27 -12.7 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x06_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 7.366 0)
		)
		(property "Value" "Conn_02x06_Row_Letter_Last_Shielded"
			(at 2.286 -9.906 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x06, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x06_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at 1.27 -12.7 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x06_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 7.366 0)
		)
		(property "Value" "Conn_02x06_Top_Bottom_Shielded"
			(at 2.286 -9.906 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x06, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x06_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 1.27 -12.7 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x07_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 9.906 0)
		)
		(property "Value" "Conn_02x07_Counter_Clockwise_Shielded"
			(at 2.286 -9.906 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x07, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x07_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 1.27 -12.7 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x07_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 9.906 0)
		)
		(property "Value" "Conn_02x07_Odd_Even_Shielded"
			(at 2.286 -9.906 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x07, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x07_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 1.27 -12.7 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x07_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 9.906 0)
		)
		(property "Value" "Conn_02x07_Row_Letter_First_Shielded"
			(at 2.286 -9.906 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x07, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x07_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at 1.27 -12.7 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x07_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 9.906 0)
		)
		(property "Value" "Conn_02x07_Row_Letter_Last_Shielded"
			(at 2.286 -9.906 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x07, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x07_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at 1.27 -12.7 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x07_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 9.906 0)
		)
		(property "Value" "Conn_02x07_Top_Bottom_Shielded"
			(at 2.286 -9.906 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x07, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x07_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 1.27 -12.7 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x08_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 9.906 0)
		)
		(property "Value" "Conn_02x08_Counter_Clockwise_Shielded"
			(at 2.286 -12.446 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x08, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x08_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 1.27 -15.24 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x08_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 9.906 0)
		)
		(property "Value" "Conn_02x08_Odd_Even_Shielded"
			(at 2.286 -12.446 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x08, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x08_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 1.27 -15.24 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x08_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 9.906 0)
		)
		(property "Value" "Conn_02x08_Row_Letter_First_Shielded"
			(at 2.286 -12.446 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x08, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x08_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at 1.27 -15.24 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x08_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 9.906 0)
		)
		(property "Value" "Conn_02x08_Row_Letter_Last_Shielded"
			(at 2.286 -12.446 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x08, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x08_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at 1.27 -15.24 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x08_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 9.906 0)
		)
		(property "Value" "Conn_02x08_Top_Bottom_Shielded"
			(at 2.286 -12.446 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x08, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x08_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 1.27 -15.24 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x09_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 12.446 0)
		)
		(property "Value" "Conn_02x09_Counter_Clockwise_Shielded"
			(at 2.286 -12.446 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x09, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x09_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 1.27 -15.24 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x09_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 12.446 0)
		)
		(property "Value" "Conn_02x09_Odd_Even_Shielded"
			(at 2.286 -12.446 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x09, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x09_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 1.27 -15.24 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x09_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 12.446 0)
		)
		(property "Value" "Conn_02x09_Row_Letter_First_Shielded"
			(at 2.286 -12.446 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x09, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x09_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at 1.27 -15.24 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x09_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 12.446 0)
		)
		(property "Value" "Conn_02x09_Row_Letter_Last_Shielded"
			(at 2.286 -12.446 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x09, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x09_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at 1.27 -15.24 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x09_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 12.446 0)
		)
		(property "Value" "Conn_02x09_Top_Bottom_Shielded"
			(at 2.286 -12.446 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x09, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x09_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 1.27 -15.24 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x10_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 12.446 0)
		)
		(property "Value" "Conn_02x10_Counter_Clockwise_Shielded"
			(at 2.286 -14.986 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x10, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x10_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 1.27 -17.78 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x10_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 12.446 0)
		)
		(property "Value" "Conn_02x10_Odd_Even_Shielded"
			(at 2.286 -14.986 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x10_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 1.27 -17.78 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x10_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 12.446 0)
		)
		(property "Value" "Conn_02x10_Row_Letter_First_Shielded"
			(at 2.286 -14.986 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x10, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x10_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at 1.27 -17.78 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x10_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 12.446 0)
		)
		(property "Value" "Conn_02x10_Row_Letter_Last_Shielded"
			(at 2.286 -14.986 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x10, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x10_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at 1.27 -17.78 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x10_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 12.446 0)
		)
		(property "Value" "Conn_02x10_Top_Bottom_Shielded"
			(at 2.286 -14.986 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x10, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x10_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 1.27 -17.78 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x11_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 14.986 0)
		)
		(property "Value" "Conn_02x11_Counter_Clockwise_Shielded"
			(at 2.286 -14.986 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x11, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x11_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 1.27 -17.78 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x11_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 14.986 0)
		)
		(property "Value" "Conn_02x11_Odd_Even_Shielded"
			(at 2.286 -14.986 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x11, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x11_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 1.27 -17.78 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x11_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 14.986 0)
		)
		(property "Value" "Conn_02x11_Row_Letter_First_Shielded"
			(at 2.286 -14.986 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x11, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x11_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at 1.27 -17.78 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x11_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 14.986 0)
		)
		(property "Value" "Conn_02x11_Row_Letter_Last_Shielded"
			(at 2.286 -14.986 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x11, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x11_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at 1.27 -17.78 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x11_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 14.986 0)
		)
		(property "Value" "Conn_02x11_Top_Bottom_Shielded"
			(at 2.286 -14.986 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x11, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x11_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 1.27 -17.78 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x12_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 14.986 0)
		)
		(property "Value" "Conn_02x12_Counter_Clockwise_Shielded"
			(at 2.286 -17.526 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x12, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x12_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 1.27 -20.32 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x12_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 14.986 0)
		)
		(property "Value" "Conn_02x12_Odd_Even_Shielded"
			(at 2.286 -17.526 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x12, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x12_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 1.27 -20.32 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x12_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 14.986 0)
		)
		(property "Value" "Conn_02x12_Row_Letter_First_Shielded"
			(at 2.286 -17.526 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x12, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x12_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at 1.27 -20.32 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x12_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 14.986 0)
		)
		(property "Value" "Conn_02x12_Row_Letter_Last_Shielded"
			(at 2.286 -17.526 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x12, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x12_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at 1.27 -20.32 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x12_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 14.986 0)
		)
		(property "Value" "Conn_02x12_Top_Bottom_Shielded"
			(at 2.286 -17.526 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x12, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x12_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 1.27 -20.32 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x13_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 17.526 0)
		)
		(property "Value" "Conn_02x13_Counter_Clockwise_Shielded"
			(at 2.286 -17.526 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x13, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x13_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 1.27 -20.32 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x13_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 17.526 0)
		)
		(property "Value" "Conn_02x13_Odd_Even_Shielded"
			(at 2.286 -17.526 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x13, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x13_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 1.27 -20.32 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x13_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 17.526 0)
		)
		(property "Value" "Conn_02x13_Row_Letter_First_Shielded"
			(at 2.286 -17.526 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x13, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x13_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at 1.27 -20.32 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x13_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 17.526 0)
		)
		(property "Value" "Conn_02x13_Row_Letter_Last_Shielded"
			(at 2.286 -17.526 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x13, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x13_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at 1.27 -20.32 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x13_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 17.526 0)
		)
		(property "Value" "Conn_02x13_Top_Bottom_Shielded"
			(at 2.286 -17.526 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x13, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x13_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 1.27 -20.32 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x14_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 17.526 0)
		)
		(property "Value" "Conn_02x14_Counter_Clockwise_Shielded"
			(at 2.286 -20.066 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x14, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x14_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 1.27 -22.86 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x14_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 17.526 0)
		)
		(property "Value" "Conn_02x14_Odd_Even_Shielded"
			(at 2.286 -20.066 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x14, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x14_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 1.27 -22.86 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x14_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 17.526 0)
		)
		(property "Value" "Conn_02x14_Row_Letter_First_Shielded"
			(at 2.286 -20.066 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x14, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x14_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at 1.27 -22.86 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x14_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 17.526 0)
		)
		(property "Value" "Conn_02x14_Row_Letter_Last_Shielded"
			(at 2.286 -20.066 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x14, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x14_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at 1.27 -22.86 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x14_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 17.526 0)
		)
		(property "Value" "Conn_02x14_Top_Bottom_Shielded"
			(at 2.286 -20.066 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x14, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x14_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 1.27 -22.86 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x15_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 20.066 0)
		)
		(property "Value" "Conn_02x15_Counter_Clockwise_Shielded"
			(at 2.286 -20.066 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x15, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x15_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 1.27 -22.86 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x15_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 20.066 0)
		)
		(property "Value" "Conn_02x15_Odd_Even_Shielded"
			(at 2.286 -20.066 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x15, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x15_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 1.27 -22.86 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x15_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 20.066 0)
		)
		(property "Value" "Conn_02x15_Row_Letter_First_Shielded"
			(at 2.286 -20.066 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x15, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x15_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at 1.27 -22.86 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x15_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 20.066 0)
		)
		(property "Value" "Conn_02x15_Row_Letter_Last_Shielded"
			(at 2.286 -20.066 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x15, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x15_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at 1.27 -22.86 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x15_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 20.066 0)
		)
		(property "Value" "Conn_02x15_Top_Bottom_Shielded"
			(at 2.286 -20.066 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x15, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x15_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 1.27 -22.86 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x16_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 20.066 0)
		)
		(property "Value" "Conn_02x16_Counter_Clockwise_Shielded"
			(at 2.286 -22.606 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x16, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x16_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 1.27 -25.4 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x16_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 20.066 0)
		)
		(property "Value" "Conn_02x16_Odd_Even_Shielded"
			(at 2.286 -22.606 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x16, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x16_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 1.27 -25.4 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x16_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 20.066 0)
		)
		(property "Value" "Conn_02x16_Row_Letter_First_Shielded"
			(at 2.286 -22.606 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x16, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x16_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at 1.27 -25.4 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x16_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 20.066 0)
		)
		(property "Value" "Conn_02x16_Row_Letter_Last_Shielded"
			(at 2.286 -22.606 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x16, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x16_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at 1.27 -25.4 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x16_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 20.066 0)
		)
		(property "Value" "Conn_02x16_Top_Bottom_Shielded"
			(at 2.286 -22.606 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x16, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x16_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 1.27 -25.4 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x17_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 22.606 0)
		)
		(property "Value" "Conn_02x17_Counter_Clockwise_Shielded"
			(at 2.286 -22.606 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x17, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x17_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 1.27 -25.4 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x17_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 22.606 0)
		)
		(property "Value" "Conn_02x17_Odd_Even_Shielded"
			(at 2.286 -22.606 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x17, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x17_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 1.27 -25.4 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x17_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 22.606 0)
		)
		(property "Value" "Conn_02x17_Row_Letter_First_Shielded"
			(at 2.286 -22.606 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x17, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x17_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at 1.27 -25.4 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x17_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 22.606 0)
		)
		(property "Value" "Conn_02x17_Row_Letter_Last_Shielded"
			(at 2.286 -22.606 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x17, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x17_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at 1.27 -25.4 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x17_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 22.606 0)
		)
		(property "Value" "Conn_02x17_Top_Bottom_Shielded"
			(at 2.286 -22.606 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x17, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x17_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 1.27 -25.4 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x18_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 22.606 0)
		)
		(property "Value" "Conn_02x18_Counter_Clockwise_Shielded"
			(at 2.286 -25.146 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x18, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x18_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 1.27 -27.94 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x18_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 22.606 0)
		)
		(property "Value" "Conn_02x18_Odd_Even_Shielded"
			(at 2.286 -25.146 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x18, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x18_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 1.27 -27.94 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x18_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 22.606 0)
		)
		(property "Value" "Conn_02x18_Row_Letter_First_Shielded"
			(at 2.286 -25.146 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x18, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x18_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at 1.27 -27.94 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x18_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 22.606 0)
		)
		(property "Value" "Conn_02x18_Row_Letter_Last_Shielded"
			(at 2.286 -25.146 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x18, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x18_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at 1.27 -27.94 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x18_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 22.606 0)
		)
		(property "Value" "Conn_02x18_Top_Bottom_Shielded"
			(at 2.286 -25.146 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x18, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x18_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 1.27 -27.94 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x19_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 25.146 0)
		)
		(property "Value" "Conn_02x19_Counter_Clockwise_Shielded"
			(at 2.286 -25.146 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x19, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x19_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 1.27 -27.94 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x19_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 25.146 0)
		)
		(property "Value" "Conn_02x19_Odd_Even_Shielded"
			(at 2.286 -25.146 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x19, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x19_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 1.27 -27.94 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x19_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 25.146 0)
		)
		(property "Value" "Conn_02x19_Row_Letter_First_Shielded"
			(at 2.286 -25.146 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x19, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x19_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at 1.27 -27.94 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x19_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 25.146 0)
		)
		(property "Value" "Conn_02x19_Row_Letter_Last_Shielded"
			(at 2.286 -25.146 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x19, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x19_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at 1.27 -27.94 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x19_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 25.146 0)
		)
		(property "Value" "Conn_02x19_Top_Bottom_Shielded"
			(at 2.286 -25.146 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x19, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x19_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 1.27 -27.94 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x20_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 25.146 0)
		)
		(property "Value" "Conn_02x20_Counter_Clockwise_Shielded"
			(at 2.286 -27.686 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x20, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x20_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 1.27 -30.48 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x20_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 25.146 0)
		)
		(property "Value" "Conn_02x20_Odd_Even_Shielded"
			(at 2.286 -27.686 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x20_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 1.27 -30.48 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x20_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 25.146 0)
		)
		(property "Value" "Conn_02x20_Row_Letter_First_Shielded"
			(at 2.286 -27.686 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x20, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x20_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at 1.27 -30.48 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x20_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 25.146 0)
		)
		(property "Value" "Conn_02x20_Row_Letter_Last_Shielded"
			(at 2.286 -27.686 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x20, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x20_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at 1.27 -30.48 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x20_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 25.146 0)
		)
		(property "Value" "Conn_02x20_Top_Bottom_Shielded"
			(at 2.286 -27.686 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x20, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x20_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 1.27 -30.48 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x21_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 27.686 0)
		)
		(property "Value" "Conn_02x21_Counter_Clockwise_Shielded"
			(at 2.286 -27.686 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x21, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x21_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 1.27 -30.48 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x21_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 27.686 0)
		)
		(property "Value" "Conn_02x21_Odd_Even_Shielded"
			(at 2.286 -27.686 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x21, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x21_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 1.27 -30.48 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x21_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 27.686 0)
		)
		(property "Value" "Conn_02x21_Row_Letter_First_Shielded"
			(at 2.286 -27.686 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x21, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x21_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at 1.27 -30.48 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x21_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 27.686 0)
		)
		(property "Value" "Conn_02x21_Row_Letter_Last_Shielded"
			(at 2.286 -27.686 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x21, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x21_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at 1.27 -30.48 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x21_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 27.686 0)
		)
		(property "Value" "Conn_02x21_Top_Bottom_Shielded"
			(at 2.286 -27.686 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x21, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x21_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 1.27 -30.48 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x22_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 27.686 0)
		)
		(property "Value" "Conn_02x22_Counter_Clockwise_Shielded"
			(at 2.286 -30.226 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x22, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x22_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 1.27 -33.02 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x22_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 27.686 0)
		)
		(property "Value" "Conn_02x22_Odd_Even_Shielded"
			(at 2.286 -30.226 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x22, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x22_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 1.27 -33.02 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x22_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 27.686 0)
		)
		(property "Value" "Conn_02x22_Row_Letter_First_Shielded"
			(at 2.286 -30.226 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x22, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x22_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at 1.27 -33.02 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x22_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 27.686 0)
		)
		(property "Value" "Conn_02x22_Row_Letter_Last_Shielded"
			(at 2.286 -30.226 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x22, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x22_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at 1.27 -33.02 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x22_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 27.686 0)
		)
		(property "Value" "Conn_02x22_Top_Bottom_Shielded"
			(at 2.286 -30.226 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x22, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x22_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 1.27 -33.02 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x23_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 30.226 0)
		)
		(property "Value" "Conn_02x23_Counter_Clockwise_Shielded"
			(at 2.286 -30.226 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x23, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x23_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 1.27 -33.02 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x23_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 30.226 0)
		)
		(property "Value" "Conn_02x23_Odd_Even_Shielded"
			(at 2.286 -30.226 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x23, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x23_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 1.27 -33.02 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x23_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 30.226 0)
		)
		(property "Value" "Conn_02x23_Row_Letter_First_Shielded"
			(at 2.286 -30.226 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x23, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x23_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at 1.27 -33.02 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x23_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 30.226 0)
		)
		(property "Value" "Conn_02x23_Row_Letter_Last_Shielded"
			(at 2.286 -30.226 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x23, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x23_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at 1.27 -33.02 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x23_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 30.226 0)
		)
		(property "Value" "Conn_02x23_Top_Bottom_Shielded"
			(at 2.286 -30.226 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x23, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x23_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 1.27 -33.02 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x24_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 30.226 0)
		)
		(property "Value" "Conn_02x24_Counter_Clockwise_Shielded"
			(at 2.286 -32.766 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x24, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x24_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 1.27 -35.56 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x24_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 30.226 0)
		)
		(property "Value" "Conn_02x24_Odd_Even_Shielded"
			(at 2.286 -32.766 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x24, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x24_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 1.27 -35.56 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x24_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 30.226 0)
		)
		(property "Value" "Conn_02x24_Row_Letter_First_Shielded"
			(at 2.286 -32.766 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x24, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x24_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at 1.27 -35.56 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x24_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 30.226 0)
		)
		(property "Value" "Conn_02x24_Row_Letter_Last_Shielded"
			(at 2.286 -32.766 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x24, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x24_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at 1.27 -35.56 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x24_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 30.226 0)
		)
		(property "Value" "Conn_02x24_Top_Bottom_Shielded"
			(at 2.286 -32.766 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x24, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x24_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 1.27 -35.56 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x25_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 32.766 0)
		)
		(property "Value" "Conn_02x25_Counter_Clockwise_Shielded"
			(at 2.286 -32.766 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x25, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x25_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 1.27 -35.56 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x25_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 32.766 0)
		)
		(property "Value" "Conn_02x25_Odd_Even_Shielded"
			(at 2.286 -32.766 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x25, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x25_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 1.27 -35.56 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x25_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 32.766 0)
		)
		(property "Value" "Conn_02x25_Row_Letter_First_Shielded"
			(at 2.286 -32.766 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x25, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x25_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at 1.27 -35.56 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x25_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 32.766 0)
		)
		(property "Value" "Conn_02x25_Row_Letter_Last_Shielded"
			(at 2.286 -32.766 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x25, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x25_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at 1.27 -35.56 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x25_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 32.766 0)
		)
		(property "Value" "Conn_02x25_Top_Bottom_Shielded"
			(at 2.286 -32.766 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x25, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x25_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 1.27 -35.56 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x26_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 32.766 0)
		)
		(property "Value" "Conn_02x26_Counter_Clockwise_Shielded"
			(at 2.286 -35.306 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x26, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x26_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 1.27 -38.1 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x26_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 32.766 0)
		)
		(property "Value" "Conn_02x26_Odd_Even_Shielded"
			(at 2.286 -35.306 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x26, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x26_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 1.27 -38.1 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x26_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 32.766 0)
		)
		(property "Value" "Conn_02x26_Row_Letter_First_Shielded"
			(at 2.286 -35.306 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x26, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x26_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at 1.27 -38.1 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x26_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 32.766 0)
		)
		(property "Value" "Conn_02x26_Row_Letter_Last_Shielded"
			(at 2.286 -35.306 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x26, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x26_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at 1.27 -38.1 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x26_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 32.766 0)
		)
		(property "Value" "Conn_02x26_Top_Bottom_Shielded"
			(at 2.286 -35.306 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x26, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x26_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 1.27 -38.1 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x27_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 35.306 0)
		)
		(property "Value" "Conn_02x27_Counter_Clockwise_Shielded"
			(at 2.286 -35.306 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x27, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x27_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 1.27 -38.1 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x27_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 35.306 0)
		)
		(property "Value" "Conn_02x27_Odd_Even_Shielded"
			(at 2.286 -35.306 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x27, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x27_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 1.27 -38.1 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x27_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 35.306 0)
		)
		(property "Value" "Conn_02x27_Row_Letter_First_Shielded"
			(at 2.286 -35.306 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x27, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x27_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at 1.27 -38.1 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x27_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 35.306 0)
		)
		(property "Value" "Conn_02x27_Row_Letter_Last_Shielded"
			(at 2.286 -35.306 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x27, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x27_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at 1.27 -38.1 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x27_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 35.306 0)
		)
		(property "Value" "Conn_02x27_Top_Bottom_Shielded"
			(at 2.286 -35.306 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x27, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x27_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 1.27 -38.1 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x28_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 35.306 0)
		)
		(property "Value" "Conn_02x28_Counter_Clockwise_Shielded"
			(at 2.286 -37.846 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x28, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x28_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 1.27 -40.64 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x28_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 35.306 0)
		)
		(property "Value" "Conn_02x28_Odd_Even_Shielded"
			(at 2.286 -37.846 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x28, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x28_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 1.27 -40.64 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x28_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 35.306 0)
		)
		(property "Value" "Conn_02x28_Row_Letter_First_Shielded"
			(at 2.286 -37.846 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x28, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x28_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at 1.27 -40.64 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x28_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 35.306 0)
		)
		(property "Value" "Conn_02x28_Row_Letter_Last_Shielded"
			(at 2.286 -37.846 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x28, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x28_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at 1.27 -40.64 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x28_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 35.306 0)
		)
		(property "Value" "Conn_02x28_Top_Bottom_Shielded"
			(at 2.286 -37.846 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x28, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x28_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 1.27 -40.64 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x29_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 37.846 0)
		)
		(property "Value" "Conn_02x29_Counter_Clockwise_Shielded"
			(at 2.286 -37.846 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x29, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x29_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 1.27 -40.64 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x29_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 37.846 0)
		)
		(property "Value" "Conn_02x29_Odd_Even_Shielded"
			(at 2.286 -37.846 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x29, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x29_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 1.27 -40.64 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x29_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 37.846 0)
		)
		(property "Value" "Conn_02x29_Row_Letter_First_Shielded"
			(at 2.286 -37.846 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x29, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x29_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at 1.27 -40.64 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x29_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 37.846 0)
		)
		(property "Value" "Conn_02x29_Row_Letter_Last_Shielded"
			(at 2.286 -37.846 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x29, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x29_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at 1.27 -40.64 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x29_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 37.846 0)
		)
		(property "Value" "Conn_02x29_Top_Bottom_Shielded"
			(at 2.286 -37.846 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x29, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x29_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 1.27 -40.64 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x30_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 37.846 0)
		)
		(property "Value" "Conn_02x30_Counter_Clockwise_Shielded"
			(at 2.286 -40.386 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x30, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x30_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 1.27 -43.18 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x30_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 37.846 0)
		)
		(property "Value" "Conn_02x30_Odd_Even_Shielded"
			(at 2.286 -40.386 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x30, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x30_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 1.27 -43.18 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x30_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 37.846 0)
		)
		(property "Value" "Conn_02x30_Row_Letter_First_Shielded"
			(at 2.286 -40.386 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x30, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x30_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at 1.27 -43.18 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x30_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 37.846 0)
		)
		(property "Value" "Conn_02x30_Row_Letter_Last_Shielded"
			(at 2.286 -40.386 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x30, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x30_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at 1.27 -43.18 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x30_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 37.846 0)
		)
		(property "Value" "Conn_02x30_Top_Bottom_Shielded"
			(at 2.286 -40.386 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x30, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x30_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 1.27 -43.18 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x31_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 40.386 0)
		)
		(property "Value" "Conn_02x31_Counter_Clockwise_Shielded"
			(at 2.286 -40.386 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x31, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x31_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 1.27 -43.18 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x31_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 40.386 0)
		)
		(property "Value" "Conn_02x31_Odd_Even_Shielded"
			(at 2.286 -40.386 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x31, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x31_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 1.27 -43.18 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x31_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 40.386 0)
		)
		(property "Value" "Conn_02x31_Row_Letter_First_Shielded"
			(at 2.286 -40.386 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x31, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x31_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at 1.27 -43.18 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x31_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 40.386 0)
		)
		(property "Value" "Conn_02x31_Row_Letter_Last_Shielded"
			(at 2.286 -40.386 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x31, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x31_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at 1.27 -43.18 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x31_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 40.386 0)
		)
		(property "Value" "Conn_02x31_Top_Bottom_Shielded"
			(at 2.286 -40.386 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x31, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x31_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 1.27 -43.18 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x32_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 40.386 0)
		)
		(property "Value" "Conn_02x32_Counter_Clockwise_Shielded"
			(at 2.286 -42.926 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x32, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x32_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 1.27 -45.72 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x32_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 40.386 0)
		)
		(property "Value" "Conn_02x32_Odd_Even_Shielded"
			(at 2.286 -42.926 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x32, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x32_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 1.27 -45.72 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x32_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 40.386 0)
		)
		(property "Value" "Conn_02x32_Row_Letter_First_Shielded"
			(at 2.286 -42.926 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x32, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x32_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at 1.27 -45.72 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x32_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 40.386 0)
		)
		(property "Value" "Conn_02x32_Row_Letter_Last_Shielded"
			(at 2.286 -42.926 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x32, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x32_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at 1.27 -45.72 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x32_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 40.386 0)
		)
		(property "Value" "Conn_02x32_Top_Bottom_Shielded"
			(at 2.286 -42.926 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x32, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x32_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 1.27 -45.72 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x33_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 42.926 0)
		)
		(property "Value" "Conn_02x33_Counter_Clockwise_Shielded"
			(at 2.286 -42.926 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x33, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x33_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 1.27 -45.72 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x33_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 42.926 0)
		)
		(property "Value" "Conn_02x33_Odd_Even_Shielded"
			(at 2.286 -42.926 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x33, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x33_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at 1.27 -45.72 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x33_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 42.926 0)
		)
		(property "Value" "Conn_02x33_Row_Letter_First_Shielded"
			(at 2.286 -42.926 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x33, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x33_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at 1.27 -45.72 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x33_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 42.926 0)
		)
		(property "Value" "Conn_02x33_Row_Letter_Last_Shielded"
			(at 2.286 -42.926 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x33, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x33_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at 1.27 -45.72 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x33_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 42.926 0)
		)
		(property "Value" "Conn_02x33_Top_Bottom_Shielded"
			(at 2.286 -42.926 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x33, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x33_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 1.27 -45.72 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x34_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 42.926 0)
		)
		(property "Value" "Conn_02x34_Counter_Clockwise_Shielded"
			(at 2.286 -45.466 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x34, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x34_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 1.27 -48.26 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x34_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 42.926 0)
		)
		(property "Value" "Conn_02x34_Odd_Even_Shielded"
			(at 2.286 -45.466 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x34, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x34_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at 1.27 -48.26 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x34_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 42.926 0)
		)
		(property "Value" "Conn_02x34_Row_Letter_First_Shielded"
			(at 2.286 -45.466 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x34, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x34_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at 1.27 -48.26 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x34_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 42.926 0)
		)
		(property "Value" "Conn_02x34_Row_Letter_Last_Shielded"
			(at 2.286 -45.466 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x34, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x34_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at 1.27 -48.26 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x34_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 42.926 0)
		)
		(property "Value" "Conn_02x34_Top_Bottom_Shielded"
			(at 2.286 -45.466 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x34, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x34_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 1.27 -48.26 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x35_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 45.466 0)
		)
		(property "Value" "Conn_02x35_Counter_Clockwise_Shielded"
			(at 2.286 -45.466 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x35, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x35_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 1.27 -48.26 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x35_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 45.466 0)
		)
		(property "Value" "Conn_02x35_Odd_Even_Shielded"
			(at 2.286 -45.466 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x35, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x35_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at 1.27 -48.26 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x35_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 45.466 0)
		)
		(property "Value" "Conn_02x35_Row_Letter_First_Shielded"
			(at 2.286 -45.466 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x35, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x35_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at 1.27 -48.26 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x35_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 45.466 0)
		)
		(property "Value" "Conn_02x35_Row_Letter_Last_Shielded"
			(at 2.286 -45.466 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x35, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x35_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at 1.27 -48.26 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x35_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 45.466 0)
		)
		(property "Value" "Conn_02x35_Top_Bottom_Shielded"
			(at 2.286 -45.466 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x35, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x35_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 1.27 -48.26 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x36_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 45.466 0)
		)
		(property "Value" "Conn_02x36_Counter_Clockwise_Shielded"
			(at 2.286 -48.006 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x36, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x36_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 1.27 -50.8 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_72")
				(number "72")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_71")
				(number "71")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x36_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 45.466 0)
		)
		(property "Value" "Conn_02x36_Odd_Even_Shielded"
			(at 2.286 -48.006 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x36, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x36_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_71")
				(number "71")
			)
			(pin passive line
				(at 1.27 -50.8 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_72")
				(number "72")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x36_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 45.466 0)
		)
		(property "Value" "Conn_02x36_Row_Letter_First_Shielded"
			(at 2.286 -48.006 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x36, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x36_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at 1.27 -50.8 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x36_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 45.466 0)
		)
		(property "Value" "Conn_02x36_Row_Letter_Last_Shielded"
			(at 2.286 -48.006 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x36, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x36_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at 1.27 -50.8 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x36_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 45.466 0)
		)
		(property "Value" "Conn_02x36_Top_Bottom_Shielded"
			(at 2.286 -48.006 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x36, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x36_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 1.27 -50.8 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_71")
				(number "71")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_72")
				(number "72")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x37_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 48.006 0)
		)
		(property "Value" "Conn_02x37_Counter_Clockwise_Shielded"
			(at 2.286 -48.006 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x37, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x37_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 1.27 -50.8 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_74")
				(number "74")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_73")
				(number "73")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_72")
				(number "72")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_71")
				(number "71")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x37_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 48.006 0)
		)
		(property "Value" "Conn_02x37_Odd_Even_Shielded"
			(at 2.286 -48.006 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x37, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x37_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_71")
				(number "71")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_73")
				(number "73")
			)
			(pin passive line
				(at 1.27 -50.8 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_72")
				(number "72")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_74")
				(number "74")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x37_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 48.006 0)
		)
		(property "Value" "Conn_02x37_Row_Letter_First_Shielded"
			(at 2.286 -48.006 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x37, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x37_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at 1.27 -50.8 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x37_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 48.006 0)
		)
		(property "Value" "Conn_02x37_Row_Letter_Last_Shielded"
			(at 2.286 -48.006 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x37, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x37_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at 1.27 -50.8 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x37_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 48.006 0)
		)
		(property "Value" "Conn_02x37_Top_Bottom_Shielded"
			(at 2.286 -48.006 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x37, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x37_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 1.27 -50.8 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_71")
				(number "71")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_72")
				(number "72")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_73")
				(number "73")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_74")
				(number "74")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x38_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 48.006 0)
		)
		(property "Value" "Conn_02x38_Counter_Clockwise_Shielded"
			(at 2.286 -50.546 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x38, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x38_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 1.27 -53.34 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_76")
				(number "76")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_75")
				(number "75")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_74")
				(number "74")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_73")
				(number "73")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_72")
				(number "72")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_71")
				(number "71")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x38_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 48.006 0)
		)
		(property "Value" "Conn_02x38_Odd_Even_Shielded"
			(at 2.286 -50.546 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x38, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x38_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_71")
				(number "71")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_73")
				(number "73")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_75")
				(number "75")
			)
			(pin passive line
				(at 1.27 -53.34 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_72")
				(number "72")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_74")
				(number "74")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_76")
				(number "76")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x38_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 48.006 0)
		)
		(property "Value" "Conn_02x38_Row_Letter_First_Shielded"
			(at 2.286 -50.546 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x38, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x38_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at 1.27 -53.34 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x38_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 48.006 0)
		)
		(property "Value" "Conn_02x38_Row_Letter_Last_Shielded"
			(at 2.286 -50.546 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x38, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x38_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at 1.27 -53.34 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x38_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 48.006 0)
		)
		(property "Value" "Conn_02x38_Top_Bottom_Shielded"
			(at 2.286 -50.546 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x38, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x38_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 1.27 -53.34 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_71")
				(number "71")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_72")
				(number "72")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_73")
				(number "73")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_74")
				(number "74")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_75")
				(number "75")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_76")
				(number "76")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x39_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 50.546 0)
		)
		(property "Value" "Conn_02x39_Counter_Clockwise_Shielded"
			(at 2.286 -50.546 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x39, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x39_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 1.27 -53.34 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_78")
				(number "78")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_77")
				(number "77")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_76")
				(number "76")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_75")
				(number "75")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_74")
				(number "74")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_73")
				(number "73")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_72")
				(number "72")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_71")
				(number "71")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x39_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 50.546 0)
		)
		(property "Value" "Conn_02x39_Odd_Even_Shielded"
			(at 2.286 -50.546 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x39, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x39_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_71")
				(number "71")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_73")
				(number "73")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_75")
				(number "75")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_77")
				(number "77")
			)
			(pin passive line
				(at 1.27 -53.34 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_72")
				(number "72")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_74")
				(number "74")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_76")
				(number "76")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_78")
				(number "78")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x39_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 50.546 0)
		)
		(property "Value" "Conn_02x39_Row_Letter_First_Shielded"
			(at 2.286 -50.546 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x39, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x39_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at 1.27 -53.34 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x39_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 50.546 0)
		)
		(property "Value" "Conn_02x39_Row_Letter_Last_Shielded"
			(at 2.286 -50.546 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x39, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x39_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at 1.27 -53.34 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x39_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 50.546 0)
		)
		(property "Value" "Conn_02x39_Top_Bottom_Shielded"
			(at 2.286 -50.546 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x39, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x39_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 1.27 -53.34 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_71")
				(number "71")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_72")
				(number "72")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_73")
				(number "73")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_74")
				(number "74")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_75")
				(number "75")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_76")
				(number "76")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_77")
				(number "77")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_78")
				(number "78")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x40_Counter_Clockwise_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 50.546 0)
		)
		(property "Value" "Conn_02x40_Counter_Clockwise_Shielded"
			(at 2.286 -53.086 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x40, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x40_Counter_Clockwise_Shielded_1_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 1.27 -55.88 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_80")
				(number "80")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_79")
				(number "79")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_78")
				(number "78")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_77")
				(number "77")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_76")
				(number "76")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_75")
				(number "75")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_74")
				(number "74")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_73")
				(number "73")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_72")
				(number "72")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_71")
				(number "71")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x40_Odd_Even_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 50.546 0)
		)
		(property "Value" "Conn_02x40_Odd_Even_Shielded"
			(at 2.286 -53.086 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x40, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x40_Odd_Even_Shielded_1_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_71")
				(number "71")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_73")
				(number "73")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_75")
				(number "75")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_77")
				(number "77")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_79")
				(number "79")
			)
			(pin passive line
				(at 1.27 -55.88 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_72")
				(number "72")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_74")
				(number "74")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_76")
				(number "76")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_78")
				(number "78")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_80")
				(number "80")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x40_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 50.546 0)
		)
		(property "Value" "Conn_02x40_Row_Letter_First_Shielded"
			(at 2.286 -53.086 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x40, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x40_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at 1.27 -55.88 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_b40")
				(number "b40")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x40_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 50.546 0)
		)
		(property "Value" "Conn_02x40_Row_Letter_Last_Shielded"
			(at 2.286 -53.086 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x40, row letter last pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x40_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_40a")
				(number "40a")
			)
			(pin passive line
				(at 1.27 -55.88 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_40b")
				(number "40b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x40_Top_Bottom_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 50.546 0)
		)
		(property "Value" "Conn_02x40_Top_Bottom_Shielded"
			(at 2.286 -53.086 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 02x40, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x40_Top_Bottom_Shielded_1_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 1.27 -55.88 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_71")
				(number "71")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_72")
				(number "72")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_73")
				(number "73")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_74")
				(number "74")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_75")
				(number "75")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_76")
				(number "76")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_77")
				(number "77")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_78")
				(number "78")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_79")
				(number "79")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_80")
				(number "80")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x40_Top_Bottom_Shielded_1"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 50.546 0)
		)
		(property "Value" "Conn_02x40_Top_Bottom_Shielded"
			(at 2.286 -53.086 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x40, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x40_Top_Bottom_Shielded_1_1_1"
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 1.27 -55.88 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_71")
				(number "71")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_72")
				(number "72")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_73")
				(number "73")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_74")
				(number "74")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_75")
				(number "75")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_76")
				(number "76")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_77")
				(number "77")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_78")
				(number "78")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_79")
				(number "79")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_80")
				(number "80")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x41_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 53.086 0)
		)
		(property "Value" "Conn_02x41_Row_Letter_First_Shielded"
			(at 2.286 -53.086 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x41, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x41_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_a41")
				(number "a41")
			)
			(pin passive line
				(at 1.27 -55.88 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_b41")
				(number "b41")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x41_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 53.086 0)
		)
		(property "Value" "Conn_02x41_Row_Letter_Last_Shielded"
			(at 2.286 -53.086 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x41, row letter last pin numbering scheme (pin number consists of a number for the row and a letter for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x41_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_40a")
				(number "40a")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_41a")
				(number "41a")
			)
			(pin passive line
				(at 1.27 -55.88 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_40b")
				(number "40b")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_41b")
				(number "41b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x42_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 53.086 0)
		)
		(property "Value" "Conn_02x42_Row_Letter_First_Shielded"
			(at 2.286 -55.626 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x42, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x42_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_a41")
				(number "a41")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_a42")
				(number "a42")
			)
			(pin passive line
				(at 1.27 -58.42 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_b41")
				(number "b41")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_b42")
				(number "b42")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x42_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 53.086 0)
		)
		(property "Value" "Conn_02x42_Row_Letter_Last_Shielded"
			(at 2.286 -55.626 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x42, row letter last pin numbering scheme (pin number consists of a number for the row and a letter for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x42_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_40a")
				(number "40a")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_41a")
				(number "41a")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_42a")
				(number "42a")
			)
			(pin passive line
				(at 1.27 -58.42 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_40b")
				(number "40b")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_41b")
				(number "41b")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_42b")
				(number "42b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x43_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 55.626 0)
		)
		(property "Value" "Conn_02x43_Row_Letter_First_Shielded"
			(at 2.286 -55.626 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x43, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x43_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a41")
				(number "a41")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_a42")
				(number "a42")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_a43")
				(number "a43")
			)
			(pin passive line
				(at 1.27 -58.42 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b41")
				(number "b41")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_b42")
				(number "b42")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_b43")
				(number "b43")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x43_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 55.626 0)
		)
		(property "Value" "Conn_02x43_Row_Letter_Last_Shielded"
			(at 2.286 -55.626 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x43, row letter last pin numbering scheme (pin number consists of a number for the row and a letter for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x43_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_40a")
				(number "40a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_41a")
				(number "41a")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_42a")
				(number "42a")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_43a")
				(number "43a")
			)
			(pin passive line
				(at 1.27 -58.42 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_40b")
				(number "40b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_41b")
				(number "41b")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_42b")
				(number "42b")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_43b")
				(number "43b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x44_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 55.626 0)
		)
		(property "Value" "Conn_02x44_Row_Letter_First_Shielded"
			(at 2.286 -58.166 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x44, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x44_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a41")
				(number "a41")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_a42")
				(number "a42")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_a43")
				(number "a43")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_a44")
				(number "a44")
			)
			(pin passive line
				(at 1.27 -60.96 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b41")
				(number "b41")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_b42")
				(number "b42")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_b43")
				(number "b43")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_b44")
				(number "b44")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x44_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 55.626 0)
		)
		(property "Value" "Conn_02x44_Row_Letter_Last_Shielded"
			(at 2.286 -58.166 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x44, row letter last pin numbering scheme (pin number consists of a number for the row and a letter for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x44_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_40a")
				(number "40a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_41a")
				(number "41a")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_42a")
				(number "42a")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_43a")
				(number "43a")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_44a")
				(number "44a")
			)
			(pin passive line
				(at 1.27 -60.96 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_40b")
				(number "40b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_41b")
				(number "41b")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_42b")
				(number "42b")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_43b")
				(number "43b")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_44b")
				(number "44b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x45_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 58.166 0)
		)
		(property "Value" "Conn_02x45_Row_Letter_First_Shielded"
			(at 2.286 -58.166 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x45, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x45_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a41")
				(number "a41")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a42")
				(number "a42")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_a43")
				(number "a43")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_a44")
				(number "a44")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_a45")
				(number "a45")
			)
			(pin passive line
				(at 1.27 -60.96 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b41")
				(number "b41")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b42")
				(number "b42")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_b43")
				(number "b43")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_b44")
				(number "b44")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_b45")
				(number "b45")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x45_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 58.166 0)
		)
		(property "Value" "Conn_02x45_Row_Letter_Last_Shielded"
			(at 2.286 -58.166 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x45, row letter last pin numbering scheme (pin number consists of a number for the row and a letter for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x45_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_40a")
				(number "40a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_41a")
				(number "41a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_42a")
				(number "42a")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_43a")
				(number "43a")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_44a")
				(number "44a")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_45a")
				(number "45a")
			)
			(pin passive line
				(at 1.27 -60.96 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_40b")
				(number "40b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_41b")
				(number "41b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_42b")
				(number "42b")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_43b")
				(number "43b")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_44b")
				(number "44b")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_45b")
				(number "45b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x46_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 58.166 0)
		)
		(property "Value" "Conn_02x46_Row_Letter_First_Shielded"
			(at 2.286 -60.706 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x46, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x46_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a41")
				(number "a41")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a42")
				(number "a42")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_a43")
				(number "a43")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_a44")
				(number "a44")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_a45")
				(number "a45")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_a46")
				(number "a46")
			)
			(pin passive line
				(at 1.27 -63.5 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b41")
				(number "b41")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b42")
				(number "b42")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_b43")
				(number "b43")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_b44")
				(number "b44")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_b45")
				(number "b45")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_b46")
				(number "b46")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x46_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 58.166 0)
		)
		(property "Value" "Conn_02x46_Row_Letter_Last_Shielded"
			(at 2.286 -60.706 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x46, row letter last pin numbering scheme (pin number consists of a number for the row and a letter for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x46_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_40a")
				(number "40a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_41a")
				(number "41a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_42a")
				(number "42a")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_43a")
				(number "43a")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_44a")
				(number "44a")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_45a")
				(number "45a")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_46a")
				(number "46a")
			)
			(pin passive line
				(at 1.27 -63.5 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_40b")
				(number "40b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_41b")
				(number "41b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_42b")
				(number "42b")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_43b")
				(number "43b")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_44b")
				(number "44b")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_45b")
				(number "45b")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_46b")
				(number "46b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x47_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 60.706 0)
		)
		(property "Value" "Conn_02x47_Row_Letter_First_Shielded"
			(at 2.286 -60.706 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x47, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x47_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a41")
				(number "a41")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a42")
				(number "a42")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a43")
				(number "a43")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_a44")
				(number "a44")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_a45")
				(number "a45")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_a46")
				(number "a46")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_a47")
				(number "a47")
			)
			(pin passive line
				(at 1.27 -63.5 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b41")
				(number "b41")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b42")
				(number "b42")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b43")
				(number "b43")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_b44")
				(number "b44")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_b45")
				(number "b45")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_b46")
				(number "b46")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_b47")
				(number "b47")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x47_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 60.706 0)
		)
		(property "Value" "Conn_02x47_Row_Letter_Last_Shielded"
			(at 2.286 -60.706 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x47, row letter last pin numbering scheme (pin number consists of a number for the row and a letter for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x47_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_40a")
				(number "40a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_41a")
				(number "41a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_42a")
				(number "42a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_43a")
				(number "43a")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_44a")
				(number "44a")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_45a")
				(number "45a")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_46a")
				(number "46a")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_47a")
				(number "47a")
			)
			(pin passive line
				(at 1.27 -63.5 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_40b")
				(number "40b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_41b")
				(number "41b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_42b")
				(number "42b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_43b")
				(number "43b")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_44b")
				(number "44b")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_45b")
				(number "45b")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_46b")
				(number "46b")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_47b")
				(number "47b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x48_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 60.706 0)
		)
		(property "Value" "Conn_02x48_Row_Letter_First_Shielded"
			(at 2.286 -63.246 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x48, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x48_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a41")
				(number "a41")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a42")
				(number "a42")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a43")
				(number "a43")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_a44")
				(number "a44")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_a45")
				(number "a45")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_a46")
				(number "a46")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_a47")
				(number "a47")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_a48")
				(number "a48")
			)
			(pin passive line
				(at 1.27 -66.04 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b41")
				(number "b41")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b42")
				(number "b42")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b43")
				(number "b43")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_b44")
				(number "b44")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_b45")
				(number "b45")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_b46")
				(number "b46")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_b47")
				(number "b47")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_b48")
				(number "b48")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x48_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 60.706 0)
		)
		(property "Value" "Conn_02x48_Row_Letter_Last_Shielded"
			(at 2.286 -63.246 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x48, row letter last pin numbering scheme (pin number consists of a number for the row and a letter for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x48_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_40a")
				(number "40a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_41a")
				(number "41a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_42a")
				(number "42a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_43a")
				(number "43a")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_44a")
				(number "44a")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_45a")
				(number "45a")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_46a")
				(number "46a")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_47a")
				(number "47a")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_48a")
				(number "48a")
			)
			(pin passive line
				(at 1.27 -66.04 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_40b")
				(number "40b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_41b")
				(number "41b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_42b")
				(number "42b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_43b")
				(number "43b")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_44b")
				(number "44b")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_45b")
				(number "45b")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_46b")
				(number "46b")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_47b")
				(number "47b")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_48b")
				(number "48b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x49_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 63.246 0)
		)
		(property "Value" "Conn_02x49_Row_Letter_First_Shielded"
			(at 2.286 -63.246 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x49, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x49_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a41")
				(number "a41")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a42")
				(number "a42")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a43")
				(number "a43")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a44")
				(number "a44")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_a45")
				(number "a45")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_a46")
				(number "a46")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_a47")
				(number "a47")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_a48")
				(number "a48")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_a49")
				(number "a49")
			)
			(pin passive line
				(at 1.27 -66.04 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b41")
				(number "b41")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b42")
				(number "b42")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b43")
				(number "b43")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b44")
				(number "b44")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_b45")
				(number "b45")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_b46")
				(number "b46")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_b47")
				(number "b47")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_b48")
				(number "b48")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_b49")
				(number "b49")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x49_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 63.246 0)
		)
		(property "Value" "Conn_02x49_Row_Letter_Last_Shielded"
			(at 2.286 -63.246 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x49, row letter last pin numbering scheme (pin number consists of a number for the row and a letter for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x49_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_40a")
				(number "40a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_41a")
				(number "41a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_42a")
				(number "42a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_43a")
				(number "43a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_44a")
				(number "44a")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_45a")
				(number "45a")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_46a")
				(number "46a")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_47a")
				(number "47a")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_48a")
				(number "48a")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_49a")
				(number "49a")
			)
			(pin passive line
				(at 1.27 -66.04 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_40b")
				(number "40b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_41b")
				(number "41b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_42b")
				(number "42b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_43b")
				(number "43b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_44b")
				(number "44b")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_45b")
				(number "45b")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_46b")
				(number "46b")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_47b")
				(number "47b")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_48b")
				(number "48b")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_49b")
				(number "49b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x50_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 63.246 0)
		)
		(property "Value" "Conn_02x50_Row_Letter_First_Shielded"
			(at 2.286 -65.786 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x50, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x50_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a41")
				(number "a41")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a42")
				(number "a42")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a43")
				(number "a43")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a44")
				(number "a44")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_a45")
				(number "a45")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_a46")
				(number "a46")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_a47")
				(number "a47")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_a48")
				(number "a48")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_a49")
				(number "a49")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_a50")
				(number "a50")
			)
			(pin passive line
				(at 1.27 -68.58 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b41")
				(number "b41")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b42")
				(number "b42")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b43")
				(number "b43")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b44")
				(number "b44")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_b45")
				(number "b45")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_b46")
				(number "b46")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_b47")
				(number "b47")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_b48")
				(number "b48")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_b49")
				(number "b49")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_b50")
				(number "b50")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x50_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 63.246 0)
		)
		(property "Value" "Conn_02x50_Row_Letter_Last_Shielded"
			(at 2.286 -65.786 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x50, row letter last pin numbering scheme (pin number consists of a number for the row and a letter for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x50_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_40a")
				(number "40a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_41a")
				(number "41a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_42a")
				(number "42a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_43a")
				(number "43a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_44a")
				(number "44a")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_45a")
				(number "45a")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_46a")
				(number "46a")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_47a")
				(number "47a")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_48a")
				(number "48a")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_49a")
				(number "49a")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_50a")
				(number "50a")
			)
			(pin passive line
				(at 1.27 -68.58 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_40b")
				(number "40b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_41b")
				(number "41b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_42b")
				(number "42b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_43b")
				(number "43b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_44b")
				(number "44b")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_45b")
				(number "45b")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_46b")
				(number "46b")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_47b")
				(number "47b")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_48b")
				(number "48b")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_49b")
				(number "49b")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_50b")
				(number "50b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x51_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 65.786 0)
		)
		(property "Value" "Conn_02x51_Row_Letter_First_Shielded"
			(at 2.286 -65.786 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x51, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x51_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a41")
				(number "a41")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a42")
				(number "a42")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a43")
				(number "a43")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a44")
				(number "a44")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a45")
				(number "a45")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_a46")
				(number "a46")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_a47")
				(number "a47")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_a48")
				(number "a48")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_a49")
				(number "a49")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_a50")
				(number "a50")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_a51")
				(number "a51")
			)
			(pin passive line
				(at 1.27 -68.58 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 63.5 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b41")
				(number "b41")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b42")
				(number "b42")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b43")
				(number "b43")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b44")
				(number "b44")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b45")
				(number "b45")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_b46")
				(number "b46")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_b47")
				(number "b47")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_b48")
				(number "b48")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_b49")
				(number "b49")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_b50")
				(number "b50")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_b51")
				(number "b51")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x51_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 65.786 0)
		)
		(property "Value" "Conn_02x51_Row_Letter_Last_Shielded"
			(at 2.286 -65.786 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x51, row letter last pin numbering scheme (pin number consists of a number for the row and a letter for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x51_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_40a")
				(number "40a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_41a")
				(number "41a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_42a")
				(number "42a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_43a")
				(number "43a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_44a")
				(number "44a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_45a")
				(number "45a")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_46a")
				(number "46a")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_47a")
				(number "47a")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_48a")
				(number "48a")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_49a")
				(number "49a")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_50a")
				(number "50a")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_51a")
				(number "51a")
			)
			(pin passive line
				(at 1.27 -68.58 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 63.5 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_40b")
				(number "40b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_41b")
				(number "41b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_42b")
				(number "42b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_43b")
				(number "43b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_44b")
				(number "44b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_45b")
				(number "45b")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_46b")
				(number "46b")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_47b")
				(number "47b")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_48b")
				(number "48b")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_49b")
				(number "49b")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_50b")
				(number "50b")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_51b")
				(number "51b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x52_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 65.786 0)
		)
		(property "Value" "Conn_02x52_Row_Letter_First_Shielded"
			(at 2.286 -68.326 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x52, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x52_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a41")
				(number "a41")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a42")
				(number "a42")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a43")
				(number "a43")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a44")
				(number "a44")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a45")
				(number "a45")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_a46")
				(number "a46")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_a47")
				(number "a47")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_a48")
				(number "a48")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_a49")
				(number "a49")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_a50")
				(number "a50")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_a51")
				(number "a51")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_a52")
				(number "a52")
			)
			(pin passive line
				(at 1.27 -71.12 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 63.5 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b41")
				(number "b41")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b42")
				(number "b42")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b43")
				(number "b43")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b44")
				(number "b44")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b45")
				(number "b45")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_b46")
				(number "b46")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_b47")
				(number "b47")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_b48")
				(number "b48")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_b49")
				(number "b49")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_b50")
				(number "b50")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_b51")
				(number "b51")
			)
			(pin passive line
				(at 7.62 -66.04 180)
				(length 4.064)
				(name "Pin_b52")
				(number "b52")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x52_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 65.786 0)
		)
		(property "Value" "Conn_02x52_Row_Letter_Last_Shielded"
			(at 2.286 -68.326 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x52, row letter last pin numbering scheme (pin number consists of a number for the row and a letter for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x52_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_40a")
				(number "40a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_41a")
				(number "41a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_42a")
				(number "42a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_43a")
				(number "43a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_44a")
				(number "44a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_45a")
				(number "45a")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_46a")
				(number "46a")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_47a")
				(number "47a")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_48a")
				(number "48a")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_49a")
				(number "49a")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_50a")
				(number "50a")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_51a")
				(number "51a")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_52a")
				(number "52a")
			)
			(pin passive line
				(at 1.27 -71.12 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 63.5 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_40b")
				(number "40b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_41b")
				(number "41b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_42b")
				(number "42b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_43b")
				(number "43b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_44b")
				(number "44b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_45b")
				(number "45b")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_46b")
				(number "46b")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_47b")
				(number "47b")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_48b")
				(number "48b")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_49b")
				(number "49b")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_50b")
				(number "50b")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_51b")
				(number "51b")
			)
			(pin passive line
				(at 7.62 -66.04 180)
				(length 4.064)
				(name "Pin_52b")
				(number "52b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x53_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 68.326 0)
		)
		(property "Value" "Conn_02x53_Row_Letter_First_Shielded"
			(at 2.286 -68.326 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x53, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x53_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a41")
				(number "a41")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a42")
				(number "a42")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a43")
				(number "a43")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a44")
				(number "a44")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a45")
				(number "a45")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a46")
				(number "a46")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_a47")
				(number "a47")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_a48")
				(number "a48")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_a49")
				(number "a49")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_a50")
				(number "a50")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_a51")
				(number "a51")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_a52")
				(number "a52")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_a53")
				(number "a53")
			)
			(pin passive line
				(at 1.27 -71.12 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 66.04 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 63.5 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b41")
				(number "b41")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b42")
				(number "b42")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b43")
				(number "b43")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b44")
				(number "b44")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b45")
				(number "b45")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b46")
				(number "b46")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_b47")
				(number "b47")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_b48")
				(number "b48")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_b49")
				(number "b49")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_b50")
				(number "b50")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_b51")
				(number "b51")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_b52")
				(number "b52")
			)
			(pin passive line
				(at 7.62 -66.04 180)
				(length 4.064)
				(name "Pin_b53")
				(number "b53")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x53_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 68.326 0)
		)
		(property "Value" "Conn_02x53_Row_Letter_Last_Shielded"
			(at 2.286 -68.326 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x53, row letter last pin numbering scheme (pin number consists of a number for the row and a letter for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x53_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_40a")
				(number "40a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_41a")
				(number "41a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_42a")
				(number "42a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_43a")
				(number "43a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_44a")
				(number "44a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_45a")
				(number "45a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_46a")
				(number "46a")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_47a")
				(number "47a")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_48a")
				(number "48a")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_49a")
				(number "49a")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_50a")
				(number "50a")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_51a")
				(number "51a")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_52a")
				(number "52a")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_53a")
				(number "53a")
			)
			(pin passive line
				(at 1.27 -71.12 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 66.04 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 63.5 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_40b")
				(number "40b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_41b")
				(number "41b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_42b")
				(number "42b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_43b")
				(number "43b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_44b")
				(number "44b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_45b")
				(number "45b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_46b")
				(number "46b")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_47b")
				(number "47b")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_48b")
				(number "48b")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_49b")
				(number "49b")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_50b")
				(number "50b")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_51b")
				(number "51b")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_52b")
				(number "52b")
			)
			(pin passive line
				(at 7.62 -66.04 180)
				(length 4.064)
				(name "Pin_53b")
				(number "53b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x54_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 68.326 0)
		)
		(property "Value" "Conn_02x54_Row_Letter_First_Shielded"
			(at 2.286 -70.866 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x54, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x54_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a41")
				(number "a41")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a42")
				(number "a42")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a43")
				(number "a43")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a44")
				(number "a44")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a45")
				(number "a45")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a46")
				(number "a46")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_a47")
				(number "a47")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_a48")
				(number "a48")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_a49")
				(number "a49")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_a50")
				(number "a50")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_a51")
				(number "a51")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_a52")
				(number "a52")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_a53")
				(number "a53")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 4.064)
				(name "Pin_a54")
				(number "a54")
			)
			(pin passive line
				(at 1.27 -73.66 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 66.04 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 63.5 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b41")
				(number "b41")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b42")
				(number "b42")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b43")
				(number "b43")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b44")
				(number "b44")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b45")
				(number "b45")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b46")
				(number "b46")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_b47")
				(number "b47")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_b48")
				(number "b48")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_b49")
				(number "b49")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_b50")
				(number "b50")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_b51")
				(number "b51")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_b52")
				(number "b52")
			)
			(pin passive line
				(at 7.62 -66.04 180)
				(length 4.064)
				(name "Pin_b53")
				(number "b53")
			)
			(pin passive line
				(at 7.62 -68.58 180)
				(length 4.064)
				(name "Pin_b54")
				(number "b54")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x54_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 68.326 0)
		)
		(property "Value" "Conn_02x54_Row_Letter_Last_Shielded"
			(at 2.286 -70.866 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x54, row letter last pin numbering scheme (pin number consists of a number for the row and a letter for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x54_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_40a")
				(number "40a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_41a")
				(number "41a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_42a")
				(number "42a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_43a")
				(number "43a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_44a")
				(number "44a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_45a")
				(number "45a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_46a")
				(number "46a")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_47a")
				(number "47a")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_48a")
				(number "48a")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_49a")
				(number "49a")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_50a")
				(number "50a")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_51a")
				(number "51a")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_52a")
				(number "52a")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_53a")
				(number "53a")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 4.064)
				(name "Pin_54a")
				(number "54a")
			)
			(pin passive line
				(at 1.27 -73.66 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 66.04 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 63.5 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_40b")
				(number "40b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_41b")
				(number "41b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_42b")
				(number "42b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_43b")
				(number "43b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_44b")
				(number "44b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_45b")
				(number "45b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_46b")
				(number "46b")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_47b")
				(number "47b")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_48b")
				(number "48b")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_49b")
				(number "49b")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_50b")
				(number "50b")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_51b")
				(number "51b")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_52b")
				(number "52b")
			)
			(pin passive line
				(at 7.62 -66.04 180)
				(length 4.064)
				(name "Pin_53b")
				(number "53b")
			)
			(pin passive line
				(at 7.62 -68.58 180)
				(length 4.064)
				(name "Pin_54b")
				(number "54b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x55_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 70.866 0)
		)
		(property "Value" "Conn_02x55_Row_Letter_First_Shielded"
			(at 2.286 -70.866 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x55, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x55_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 68.58 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a41")
				(number "a41")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a42")
				(number "a42")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a43")
				(number "a43")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a44")
				(number "a44")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a45")
				(number "a45")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a46")
				(number "a46")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a47")
				(number "a47")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_a48")
				(number "a48")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_a49")
				(number "a49")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_a50")
				(number "a50")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_a51")
				(number "a51")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_a52")
				(number "a52")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_a53")
				(number "a53")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_a54")
				(number "a54")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 4.064)
				(name "Pin_a55")
				(number "a55")
			)
			(pin passive line
				(at 1.27 -73.66 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 68.58 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 66.04 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 63.5 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b41")
				(number "b41")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b42")
				(number "b42")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b43")
				(number "b43")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b44")
				(number "b44")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b45")
				(number "b45")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b46")
				(number "b46")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b47")
				(number "b47")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_b48")
				(number "b48")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_b49")
				(number "b49")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_b50")
				(number "b50")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_b51")
				(number "b51")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_b52")
				(number "b52")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_b53")
				(number "b53")
			)
			(pin passive line
				(at 7.62 -66.04 180)
				(length 4.064)
				(name "Pin_b54")
				(number "b54")
			)
			(pin passive line
				(at 7.62 -68.58 180)
				(length 4.064)
				(name "Pin_b55")
				(number "b55")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x55_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 70.866 0)
		)
		(property "Value" "Conn_02x55_Row_Letter_Last_Shielded"
			(at 2.286 -70.866 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x55, row letter last pin numbering scheme (pin number consists of a number for the row and a letter for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x55_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 68.58 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_40a")
				(number "40a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_41a")
				(number "41a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_42a")
				(number "42a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_43a")
				(number "43a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_44a")
				(number "44a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_45a")
				(number "45a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_46a")
				(number "46a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_47a")
				(number "47a")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_48a")
				(number "48a")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_49a")
				(number "49a")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_50a")
				(number "50a")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_51a")
				(number "51a")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_52a")
				(number "52a")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_53a")
				(number "53a")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_54a")
				(number "54a")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 4.064)
				(name "Pin_55a")
				(number "55a")
			)
			(pin passive line
				(at 1.27 -73.66 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 68.58 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 66.04 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 63.5 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_40b")
				(number "40b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_41b")
				(number "41b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_42b")
				(number "42b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_43b")
				(number "43b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_44b")
				(number "44b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_45b")
				(number "45b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_46b")
				(number "46b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_47b")
				(number "47b")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_48b")
				(number "48b")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_49b")
				(number "49b")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_50b")
				(number "50b")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_51b")
				(number "51b")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_52b")
				(number "52b")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_53b")
				(number "53b")
			)
			(pin passive line
				(at 7.62 -66.04 180)
				(length 4.064)
				(name "Pin_54b")
				(number "54b")
			)
			(pin passive line
				(at 7.62 -68.58 180)
				(length 4.064)
				(name "Pin_55b")
				(number "55b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x56_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 70.866 0)
		)
		(property "Value" "Conn_02x56_Row_Letter_First_Shielded"
			(at 2.286 -73.406 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x56, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x56_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 68.58 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a41")
				(number "a41")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a42")
				(number "a42")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a43")
				(number "a43")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a44")
				(number "a44")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a45")
				(number "a45")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a46")
				(number "a46")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a47")
				(number "a47")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_a48")
				(number "a48")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_a49")
				(number "a49")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_a50")
				(number "a50")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_a51")
				(number "a51")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_a52")
				(number "a52")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_a53")
				(number "a53")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_a54")
				(number "a54")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 4.064)
				(name "Pin_a55")
				(number "a55")
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 4.064)
				(name "Pin_a56")
				(number "a56")
			)
			(pin passive line
				(at 1.27 -76.2 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 68.58 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 66.04 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 63.5 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b41")
				(number "b41")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b42")
				(number "b42")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b43")
				(number "b43")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b44")
				(number "b44")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b45")
				(number "b45")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b46")
				(number "b46")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b47")
				(number "b47")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_b48")
				(number "b48")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_b49")
				(number "b49")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_b50")
				(number "b50")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_b51")
				(number "b51")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_b52")
				(number "b52")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_b53")
				(number "b53")
			)
			(pin passive line
				(at 7.62 -66.04 180)
				(length 4.064)
				(name "Pin_b54")
				(number "b54")
			)
			(pin passive line
				(at 7.62 -68.58 180)
				(length 4.064)
				(name "Pin_b55")
				(number "b55")
			)
			(pin passive line
				(at 7.62 -71.12 180)
				(length 4.064)
				(name "Pin_b56")
				(number "b56")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x56_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 70.866 0)
		)
		(property "Value" "Conn_02x56_Row_Letter_Last_Shielded"
			(at 2.286 -73.406 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x56, row letter last pin numbering scheme (pin number consists of a number for the row and a letter for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x56_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 68.58 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_40a")
				(number "40a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_41a")
				(number "41a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_42a")
				(number "42a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_43a")
				(number "43a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_44a")
				(number "44a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_45a")
				(number "45a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_46a")
				(number "46a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_47a")
				(number "47a")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_48a")
				(number "48a")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_49a")
				(number "49a")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_50a")
				(number "50a")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_51a")
				(number "51a")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_52a")
				(number "52a")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_53a")
				(number "53a")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_54a")
				(number "54a")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 4.064)
				(name "Pin_55a")
				(number "55a")
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 4.064)
				(name "Pin_56a")
				(number "56a")
			)
			(pin passive line
				(at 1.27 -76.2 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 68.58 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 66.04 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 63.5 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_40b")
				(number "40b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_41b")
				(number "41b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_42b")
				(number "42b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_43b")
				(number "43b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_44b")
				(number "44b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_45b")
				(number "45b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_46b")
				(number "46b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_47b")
				(number "47b")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_48b")
				(number "48b")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_49b")
				(number "49b")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_50b")
				(number "50b")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_51b")
				(number "51b")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_52b")
				(number "52b")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_53b")
				(number "53b")
			)
			(pin passive line
				(at 7.62 -66.04 180)
				(length 4.064)
				(name "Pin_54b")
				(number "54b")
			)
			(pin passive line
				(at 7.62 -68.58 180)
				(length 4.064)
				(name "Pin_55b")
				(number "55b")
			)
			(pin passive line
				(at 7.62 -71.12 180)
				(length 4.064)
				(name "Pin_56b")
				(number "56b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x57_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 73.406 0)
		)
		(property "Value" "Conn_02x57_Row_Letter_First_Shielded"
			(at 2.286 -73.406 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x57, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x57_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 71.12 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 68.58 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a41")
				(number "a41")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a42")
				(number "a42")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a43")
				(number "a43")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a44")
				(number "a44")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a45")
				(number "a45")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a46")
				(number "a46")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a47")
				(number "a47")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a48")
				(number "a48")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_a49")
				(number "a49")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_a50")
				(number "a50")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_a51")
				(number "a51")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_a52")
				(number "a52")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_a53")
				(number "a53")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_a54")
				(number "a54")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_a55")
				(number "a55")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 4.064)
				(name "Pin_a56")
				(number "a56")
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 4.064)
				(name "Pin_a57")
				(number "a57")
			)
			(pin passive line
				(at 1.27 -76.2 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 71.12 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 68.58 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 66.04 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 63.5 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b41")
				(number "b41")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b42")
				(number "b42")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b43")
				(number "b43")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b44")
				(number "b44")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b45")
				(number "b45")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b46")
				(number "b46")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b47")
				(number "b47")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b48")
				(number "b48")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_b49")
				(number "b49")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_b50")
				(number "b50")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_b51")
				(number "b51")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_b52")
				(number "b52")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_b53")
				(number "b53")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_b54")
				(number "b54")
			)
			(pin passive line
				(at 7.62 -66.04 180)
				(length 4.064)
				(name "Pin_b55")
				(number "b55")
			)
			(pin passive line
				(at 7.62 -68.58 180)
				(length 4.064)
				(name "Pin_b56")
				(number "b56")
			)
			(pin passive line
				(at 7.62 -71.12 180)
				(length 4.064)
				(name "Pin_b57")
				(number "b57")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x57_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 73.406 0)
		)
		(property "Value" "Conn_02x57_Row_Letter_Last_Shielded"
			(at 2.286 -73.406 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x57, row letter last pin numbering scheme (pin number consists of a number for the row and a letter for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x57_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 71.12 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 68.58 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_40a")
				(number "40a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_41a")
				(number "41a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_42a")
				(number "42a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_43a")
				(number "43a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_44a")
				(number "44a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_45a")
				(number "45a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_46a")
				(number "46a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_47a")
				(number "47a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_48a")
				(number "48a")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_49a")
				(number "49a")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_50a")
				(number "50a")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_51a")
				(number "51a")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_52a")
				(number "52a")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_53a")
				(number "53a")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_54a")
				(number "54a")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_55a")
				(number "55a")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 4.064)
				(name "Pin_56a")
				(number "56a")
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 4.064)
				(name "Pin_57a")
				(number "57a")
			)
			(pin passive line
				(at 1.27 -76.2 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 71.12 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 68.58 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 66.04 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 63.5 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_40b")
				(number "40b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_41b")
				(number "41b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_42b")
				(number "42b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_43b")
				(number "43b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_44b")
				(number "44b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_45b")
				(number "45b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_46b")
				(number "46b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_47b")
				(number "47b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_48b")
				(number "48b")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_49b")
				(number "49b")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_50b")
				(number "50b")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_51b")
				(number "51b")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_52b")
				(number "52b")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_53b")
				(number "53b")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_54b")
				(number "54b")
			)
			(pin passive line
				(at 7.62 -66.04 180)
				(length 4.064)
				(name "Pin_55b")
				(number "55b")
			)
			(pin passive line
				(at 7.62 -68.58 180)
				(length 4.064)
				(name "Pin_56b")
				(number "56b")
			)
			(pin passive line
				(at 7.62 -71.12 180)
				(length 4.064)
				(name "Pin_57b")
				(number "57b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x58_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 73.406 0)
		)
		(property "Value" "Conn_02x58_Row_Letter_First_Shielded"
			(at 2.286 -75.946 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x58, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x58_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 71.12 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 68.58 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a41")
				(number "a41")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a42")
				(number "a42")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a43")
				(number "a43")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a44")
				(number "a44")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a45")
				(number "a45")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a46")
				(number "a46")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a47")
				(number "a47")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a48")
				(number "a48")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_a49")
				(number "a49")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_a50")
				(number "a50")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_a51")
				(number "a51")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_a52")
				(number "a52")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_a53")
				(number "a53")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_a54")
				(number "a54")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_a55")
				(number "a55")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 4.064)
				(name "Pin_a56")
				(number "a56")
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 4.064)
				(name "Pin_a57")
				(number "a57")
			)
			(pin passive line
				(at -5.08 -73.66 0)
				(length 4.064)
				(name "Pin_a58")
				(number "a58")
			)
			(pin passive line
				(at 1.27 -78.74 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 71.12 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 68.58 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 66.04 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 63.5 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b41")
				(number "b41")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b42")
				(number "b42")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b43")
				(number "b43")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b44")
				(number "b44")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b45")
				(number "b45")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b46")
				(number "b46")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b47")
				(number "b47")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b48")
				(number "b48")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_b49")
				(number "b49")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_b50")
				(number "b50")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_b51")
				(number "b51")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_b52")
				(number "b52")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_b53")
				(number "b53")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_b54")
				(number "b54")
			)
			(pin passive line
				(at 7.62 -66.04 180)
				(length 4.064)
				(name "Pin_b55")
				(number "b55")
			)
			(pin passive line
				(at 7.62 -68.58 180)
				(length 4.064)
				(name "Pin_b56")
				(number "b56")
			)
			(pin passive line
				(at 7.62 -71.12 180)
				(length 4.064)
				(name "Pin_b57")
				(number "b57")
			)
			(pin passive line
				(at 7.62 -73.66 180)
				(length 4.064)
				(name "Pin_b58")
				(number "b58")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x58_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 73.406 0)
		)
		(property "Value" "Conn_02x58_Row_Letter_Last_Shielded"
			(at 2.286 -75.946 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x58, row letter last pin numbering scheme (pin number consists of a number for the row and a letter for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x58_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 71.12 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 68.58 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_40a")
				(number "40a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_41a")
				(number "41a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_42a")
				(number "42a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_43a")
				(number "43a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_44a")
				(number "44a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_45a")
				(number "45a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_46a")
				(number "46a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_47a")
				(number "47a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_48a")
				(number "48a")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_49a")
				(number "49a")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_50a")
				(number "50a")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_51a")
				(number "51a")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_52a")
				(number "52a")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_53a")
				(number "53a")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_54a")
				(number "54a")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_55a")
				(number "55a")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 4.064)
				(name "Pin_56a")
				(number "56a")
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 4.064)
				(name "Pin_57a")
				(number "57a")
			)
			(pin passive line
				(at -5.08 -73.66 0)
				(length 4.064)
				(name "Pin_58a")
				(number "58a")
			)
			(pin passive line
				(at 1.27 -78.74 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 71.12 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 68.58 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 66.04 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 63.5 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_40b")
				(number "40b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_41b")
				(number "41b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_42b")
				(number "42b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_43b")
				(number "43b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_44b")
				(number "44b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_45b")
				(number "45b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_46b")
				(number "46b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_47b")
				(number "47b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_48b")
				(number "48b")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_49b")
				(number "49b")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_50b")
				(number "50b")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_51b")
				(number "51b")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_52b")
				(number "52b")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_53b")
				(number "53b")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_54b")
				(number "54b")
			)
			(pin passive line
				(at 7.62 -66.04 180)
				(length 4.064)
				(name "Pin_55b")
				(number "55b")
			)
			(pin passive line
				(at 7.62 -68.58 180)
				(length 4.064)
				(name "Pin_56b")
				(number "56b")
			)
			(pin passive line
				(at 7.62 -71.12 180)
				(length 4.064)
				(name "Pin_57b")
				(number "57b")
			)
			(pin passive line
				(at 7.62 -73.66 180)
				(length 4.064)
				(name "Pin_58b")
				(number "58b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x59_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 75.946 0)
		)
		(property "Value" "Conn_02x59_Row_Letter_First_Shielded"
			(at 2.286 -75.946 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x59, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x59_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 73.66 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 71.12 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 68.58 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a41")
				(number "a41")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a42")
				(number "a42")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a43")
				(number "a43")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a44")
				(number "a44")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a45")
				(number "a45")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a46")
				(number "a46")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a47")
				(number "a47")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a48")
				(number "a48")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a49")
				(number "a49")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_a50")
				(number "a50")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_a51")
				(number "a51")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_a52")
				(number "a52")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_a53")
				(number "a53")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_a54")
				(number "a54")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_a55")
				(number "a55")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_a56")
				(number "a56")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 4.064)
				(name "Pin_a57")
				(number "a57")
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 4.064)
				(name "Pin_a58")
				(number "a58")
			)
			(pin passive line
				(at -5.08 -73.66 0)
				(length 4.064)
				(name "Pin_a59")
				(number "a59")
			)
			(pin passive line
				(at 1.27 -78.74 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 73.66 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 71.12 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 68.58 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 66.04 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 63.5 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b41")
				(number "b41")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b42")
				(number "b42")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b43")
				(number "b43")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b44")
				(number "b44")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b45")
				(number "b45")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b46")
				(number "b46")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b47")
				(number "b47")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b48")
				(number "b48")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b49")
				(number "b49")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_b50")
				(number "b50")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_b51")
				(number "b51")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_b52")
				(number "b52")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_b53")
				(number "b53")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_b54")
				(number "b54")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_b55")
				(number "b55")
			)
			(pin passive line
				(at 7.62 -66.04 180)
				(length 4.064)
				(name "Pin_b56")
				(number "b56")
			)
			(pin passive line
				(at 7.62 -68.58 180)
				(length 4.064)
				(name "Pin_b57")
				(number "b57")
			)
			(pin passive line
				(at 7.62 -71.12 180)
				(length 4.064)
				(name "Pin_b58")
				(number "b58")
			)
			(pin passive line
				(at 7.62 -73.66 180)
				(length 4.064)
				(name "Pin_b59")
				(number "b59")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x59_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 75.946 0)
		)
		(property "Value" "Conn_02x59_Row_Letter_Last_Shielded"
			(at 2.286 -75.946 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x59, row letter last pin numbering scheme (pin number consists of a number for the row and a letter for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x59_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 73.66 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 71.12 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 68.58 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_40a")
				(number "40a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_41a")
				(number "41a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_42a")
				(number "42a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_43a")
				(number "43a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_44a")
				(number "44a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_45a")
				(number "45a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_46a")
				(number "46a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_47a")
				(number "47a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_48a")
				(number "48a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_49a")
				(number "49a")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_50a")
				(number "50a")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_51a")
				(number "51a")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_52a")
				(number "52a")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_53a")
				(number "53a")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_54a")
				(number "54a")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_55a")
				(number "55a")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_56a")
				(number "56a")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 4.064)
				(name "Pin_57a")
				(number "57a")
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 4.064)
				(name "Pin_58a")
				(number "58a")
			)
			(pin passive line
				(at -5.08 -73.66 0)
				(length 4.064)
				(name "Pin_59a")
				(number "59a")
			)
			(pin passive line
				(at 1.27 -78.74 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 73.66 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 71.12 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 68.58 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 66.04 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 63.5 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_40b")
				(number "40b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_41b")
				(number "41b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_42b")
				(number "42b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_43b")
				(number "43b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_44b")
				(number "44b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_45b")
				(number "45b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_46b")
				(number "46b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_47b")
				(number "47b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_48b")
				(number "48b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_49b")
				(number "49b")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_50b")
				(number "50b")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_51b")
				(number "51b")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_52b")
				(number "52b")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_53b")
				(number "53b")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_54b")
				(number "54b")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_55b")
				(number "55b")
			)
			(pin passive line
				(at 7.62 -66.04 180)
				(length 4.064)
				(name "Pin_56b")
				(number "56b")
			)
			(pin passive line
				(at 7.62 -68.58 180)
				(length 4.064)
				(name "Pin_57b")
				(number "57b")
			)
			(pin passive line
				(at 7.62 -71.12 180)
				(length 4.064)
				(name "Pin_58b")
				(number "58b")
			)
			(pin passive line
				(at 7.62 -73.66 180)
				(length 4.064)
				(name "Pin_59b")
				(number "59b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x60_Row_Letter_First_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 75.946 0)
		)
		(property "Value" "Conn_02x60_Row_Letter_First_Shielded"
			(at 2.286 -78.486 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x60, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x60_Row_Letter_First_Shielded_1_1"
			(pin passive line
				(at -5.08 73.66 0)
				(length 4.064)
				(name "Pin_a1")
				(number "a1")
			)
			(pin passive line
				(at -5.08 71.12 0)
				(length 4.064)
				(name "Pin_a2")
				(number "a2")
			)
			(pin passive line
				(at -5.08 68.58 0)
				(length 4.064)
				(name "Pin_a3")
				(number "a3")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_a4")
				(number "a4")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_a5")
				(number "a5")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_a6")
				(number "a6")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_a7")
				(number "a7")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_a8")
				(number "a8")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_a9")
				(number "a9")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_a10")
				(number "a10")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_a11")
				(number "a11")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_a12")
				(number "a12")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_a13")
				(number "a13")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_a14")
				(number "a14")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_a15")
				(number "a15")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_a16")
				(number "a16")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_a17")
				(number "a17")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_a18")
				(number "a18")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_a19")
				(number "a19")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_a20")
				(number "a20")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_a21")
				(number "a21")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_a22")
				(number "a22")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_a23")
				(number "a23")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_a24")
				(number "a24")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_a25")
				(number "a25")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_a26")
				(number "a26")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_a27")
				(number "a27")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_a28")
				(number "a28")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_a29")
				(number "a29")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_a30")
				(number "a30")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_a31")
				(number "a31")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_a32")
				(number "a32")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_a33")
				(number "a33")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_a34")
				(number "a34")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_a35")
				(number "a35")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_a36")
				(number "a36")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_a37")
				(number "a37")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_a38")
				(number "a38")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_a39")
				(number "a39")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_a40")
				(number "a40")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_a41")
				(number "a41")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_a42")
				(number "a42")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_a43")
				(number "a43")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_a44")
				(number "a44")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_a45")
				(number "a45")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_a46")
				(number "a46")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_a47")
				(number "a47")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_a48")
				(number "a48")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_a49")
				(number "a49")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_a50")
				(number "a50")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_a51")
				(number "a51")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_a52")
				(number "a52")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_a53")
				(number "a53")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_a54")
				(number "a54")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_a55")
				(number "a55")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_a56")
				(number "a56")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 4.064)
				(name "Pin_a57")
				(number "a57")
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 4.064)
				(name "Pin_a58")
				(number "a58")
			)
			(pin passive line
				(at -5.08 -73.66 0)
				(length 4.064)
				(name "Pin_a59")
				(number "a59")
			)
			(pin passive line
				(at -5.08 -76.2 0)
				(length 4.064)
				(name "Pin_a60")
				(number "a60")
			)
			(pin passive line
				(at 1.27 -81.28 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 73.66 180)
				(length 4.064)
				(name "Pin_b1")
				(number "b1")
			)
			(pin passive line
				(at 7.62 71.12 180)
				(length 4.064)
				(name "Pin_b2")
				(number "b2")
			)
			(pin passive line
				(at 7.62 68.58 180)
				(length 4.064)
				(name "Pin_b3")
				(number "b3")
			)
			(pin passive line
				(at 7.62 66.04 180)
				(length 4.064)
				(name "Pin_b4")
				(number "b4")
			)
			(pin passive line
				(at 7.62 63.5 180)
				(length 4.064)
				(name "Pin_b5")
				(number "b5")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_b6")
				(number "b6")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_b7")
				(number "b7")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_b8")
				(number "b8")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_b9")
				(number "b9")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_b10")
				(number "b10")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_b11")
				(number "b11")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_b12")
				(number "b12")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_b13")
				(number "b13")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_b14")
				(number "b14")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_b15")
				(number "b15")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_b16")
				(number "b16")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_b17")
				(number "b17")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_b18")
				(number "b18")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_b19")
				(number "b19")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_b20")
				(number "b20")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_b21")
				(number "b21")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_b22")
				(number "b22")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_b23")
				(number "b23")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_b24")
				(number "b24")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_b25")
				(number "b25")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_b26")
				(number "b26")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_b27")
				(number "b27")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_b28")
				(number "b28")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_b29")
				(number "b29")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_b30")
				(number "b30")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_b31")
				(number "b31")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_b32")
				(number "b32")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_b33")
				(number "b33")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_b34")
				(number "b34")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_b35")
				(number "b35")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_b36")
				(number "b36")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_b37")
				(number "b37")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_b38")
				(number "b38")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_b39")
				(number "b39")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_b40")
				(number "b40")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_b41")
				(number "b41")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_b42")
				(number "b42")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_b43")
				(number "b43")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_b44")
				(number "b44")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_b45")
				(number "b45")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_b46")
				(number "b46")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_b47")
				(number "b47")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_b48")
				(number "b48")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_b49")
				(number "b49")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_b50")
				(number "b50")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_b51")
				(number "b51")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_b52")
				(number "b52")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_b53")
				(number "b53")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_b54")
				(number "b54")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_b55")
				(number "b55")
			)
			(pin passive line
				(at 7.62 -66.04 180)
				(length 4.064)
				(name "Pin_b56")
				(number "b56")
			)
			(pin passive line
				(at 7.62 -68.58 180)
				(length 4.064)
				(name "Pin_b57")
				(number "b57")
			)
			(pin passive line
				(at 7.62 -71.12 180)
				(length 4.064)
				(name "Pin_b58")
				(number "b58")
			)
			(pin passive line
				(at 7.62 -73.66 180)
				(length 4.064)
				(name "Pin_b59")
				(number "b59")
			)
			(pin passive line
				(at 7.62 -76.2 180)
				(length 4.064)
				(name "Pin_b60")
				(number "b60")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_02x60_Row_Letter_Last_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 75.946 0)
		)
		(property "Value" "Conn_02x60_Row_Letter_Last_Shielded"
			(at 2.286 -78.486 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "\"Generic shielded connector, double row, 02x60, row letter last pin numbering scheme (pin number consists of a number for the row and a letter for the pin index in this row. 1a, ..., Na; 1b, ..., Nb)), script generated\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*_2x??-1SH*"
			(at 0 0 0)
		)
		(symbol "Conn_02x60_Row_Letter_Last_Shielded_1_1"
			(pin passive line
				(at -5.08 73.66 0)
				(length 4.064)
				(name "Pin_1a")
				(number "1a")
			)
			(pin passive line
				(at -5.08 71.12 0)
				(length 4.064)
				(name "Pin_2a")
				(number "2a")
			)
			(pin passive line
				(at -5.08 68.58 0)
				(length 4.064)
				(name "Pin_3a")
				(number "3a")
			)
			(pin passive line
				(at -5.08 66.04 0)
				(length 4.064)
				(name "Pin_4a")
				(number "4a")
			)
			(pin passive line
				(at -5.08 63.5 0)
				(length 4.064)
				(name "Pin_5a")
				(number "5a")
			)
			(pin passive line
				(at -5.08 60.96 0)
				(length 4.064)
				(name "Pin_6a")
				(number "6a")
			)
			(pin passive line
				(at -5.08 58.42 0)
				(length 4.064)
				(name "Pin_7a")
				(number "7a")
			)
			(pin passive line
				(at -5.08 55.88 0)
				(length 4.064)
				(name "Pin_8a")
				(number "8a")
			)
			(pin passive line
				(at -5.08 53.34 0)
				(length 4.064)
				(name "Pin_9a")
				(number "9a")
			)
			(pin passive line
				(at -5.08 50.8 0)
				(length 4.064)
				(name "Pin_10a")
				(number "10a")
			)
			(pin passive line
				(at -5.08 48.26 0)
				(length 4.064)
				(name "Pin_11a")
				(number "11a")
			)
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_12a")
				(number "12a")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_13a")
				(number "13a")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_14a")
				(number "14a")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_15a")
				(number "15a")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_16a")
				(number "16a")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_17a")
				(number "17a")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_18a")
				(number "18a")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_19a")
				(number "19a")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_20a")
				(number "20a")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_21a")
				(number "21a")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_22a")
				(number "22a")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_23a")
				(number "23a")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_24a")
				(number "24a")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_25a")
				(number "25a")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_26a")
				(number "26a")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_27a")
				(number "27a")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_28a")
				(number "28a")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_29a")
				(number "29a")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_30a")
				(number "30a")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_31a")
				(number "31a")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_32a")
				(number "32a")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_33a")
				(number "33a")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_34a")
				(number "34a")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_35a")
				(number "35a")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_36a")
				(number "36a")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_37a")
				(number "37a")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_38a")
				(number "38a")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_39a")
				(number "39a")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_40a")
				(number "40a")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_41a")
				(number "41a")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_42a")
				(number "42a")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_43a")
				(number "43a")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_44a")
				(number "44a")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_45a")
				(number "45a")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_46a")
				(number "46a")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_47a")
				(number "47a")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_48a")
				(number "48a")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_49a")
				(number "49a")
			)
			(pin passive line
				(at -5.08 -50.8 0)
				(length 4.064)
				(name "Pin_50a")
				(number "50a")
			)
			(pin passive line
				(at -5.08 -53.34 0)
				(length 4.064)
				(name "Pin_51a")
				(number "51a")
			)
			(pin passive line
				(at -5.08 -55.88 0)
				(length 4.064)
				(name "Pin_52a")
				(number "52a")
			)
			(pin passive line
				(at -5.08 -58.42 0)
				(length 4.064)
				(name "Pin_53a")
				(number "53a")
			)
			(pin passive line
				(at -5.08 -60.96 0)
				(length 4.064)
				(name "Pin_54a")
				(number "54a")
			)
			(pin passive line
				(at -5.08 -63.5 0)
				(length 4.064)
				(name "Pin_55a")
				(number "55a")
			)
			(pin passive line
				(at -5.08 -66.04 0)
				(length 4.064)
				(name "Pin_56a")
				(number "56a")
			)
			(pin passive line
				(at -5.08 -68.58 0)
				(length 4.064)
				(name "Pin_57a")
				(number "57a")
			)
			(pin passive line
				(at -5.08 -71.12 0)
				(length 4.064)
				(name "Pin_58a")
				(number "58a")
			)
			(pin passive line
				(at -5.08 -73.66 0)
				(length 4.064)
				(name "Pin_59a")
				(number "59a")
			)
			(pin passive line
				(at -5.08 -76.2 0)
				(length 4.064)
				(name "Pin_60a")
				(number "60a")
			)
			(pin passive line
				(at 1.27 -81.28 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 73.66 180)
				(length 4.064)
				(name "Pin_1b")
				(number "1b")
			)
			(pin passive line
				(at 7.62 71.12 180)
				(length 4.064)
				(name "Pin_2b")
				(number "2b")
			)
			(pin passive line
				(at 7.62 68.58 180)
				(length 4.064)
				(name "Pin_3b")
				(number "3b")
			)
			(pin passive line
				(at 7.62 66.04 180)
				(length 4.064)
				(name "Pin_4b")
				(number "4b")
			)
			(pin passive line
				(at 7.62 63.5 180)
				(length 4.064)
				(name "Pin_5b")
				(number "5b")
			)
			(pin passive line
				(at 7.62 60.96 180)
				(length 4.064)
				(name "Pin_6b")
				(number "6b")
			)
			(pin passive line
				(at 7.62 58.42 180)
				(length 4.064)
				(name "Pin_7b")
				(number "7b")
			)
			(pin passive line
				(at 7.62 55.88 180)
				(length 4.064)
				(name "Pin_8b")
				(number "8b")
			)
			(pin passive line
				(at 7.62 53.34 180)
				(length 4.064)
				(name "Pin_9b")
				(number "9b")
			)
			(pin passive line
				(at 7.62 50.8 180)
				(length 4.064)
				(name "Pin_10b")
				(number "10b")
			)
			(pin passive line
				(at 7.62 48.26 180)
				(length 4.064)
				(name "Pin_11b")
				(number "11b")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_12b")
				(number "12b")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_13b")
				(number "13b")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_14b")
				(number "14b")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_15b")
				(number "15b")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_16b")
				(number "16b")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_17b")
				(number "17b")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_18b")
				(number "18b")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_19b")
				(number "19b")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_20b")
				(number "20b")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_21b")
				(number "21b")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_22b")
				(number "22b")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_23b")
				(number "23b")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_24b")
				(number "24b")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_25b")
				(number "25b")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_26b")
				(number "26b")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_27b")
				(number "27b")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_28b")
				(number "28b")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_29b")
				(number "29b")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_30b")
				(number "30b")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_31b")
				(number "31b")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_32b")
				(number "32b")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_33b")
				(number "33b")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_34b")
				(number "34b")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_35b")
				(number "35b")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_36b")
				(number "36b")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_37b")
				(number "37b")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_38b")
				(number "38b")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_39b")
				(number "39b")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_40b")
				(number "40b")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_41b")
				(number "41b")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_42b")
				(number "42b")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_43b")
				(number "43b")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_44b")
				(number "44b")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_45b")
				(number "45b")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_46b")
				(number "46b")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_47b")
				(number "47b")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_48b")
				(number "48b")
			)
			(pin passive line
				(at 7.62 -48.26 180)
				(length 4.064)
				(name "Pin_49b")
				(number "49b")
			)
			(pin passive line
				(at 7.62 -50.8 180)
				(length 4.064)
				(name "Pin_50b")
				(number "50b")
			)
			(pin passive line
				(at 7.62 -53.34 180)
				(length 4.064)
				(name "Pin_51b")
				(number "51b")
			)
			(pin passive line
				(at 7.62 -55.88 180)
				(length 4.064)
				(name "Pin_52b")
				(number "52b")
			)
			(pin passive line
				(at 7.62 -58.42 180)
				(length 4.064)
				(name "Pin_53b")
				(number "53b")
			)
			(pin passive line
				(at 7.62 -60.96 180)
				(length 4.064)
				(name "Pin_54b")
				(number "54b")
			)
			(pin passive line
				(at 7.62 -63.5 180)
				(length 4.064)
				(name "Pin_55b")
				(number "55b")
			)
			(pin passive line
				(at 7.62 -66.04 180)
				(length 4.064)
				(name "Pin_56b")
				(number "56b")
			)
			(pin passive line
				(at 7.62 -68.58 180)
				(length 4.064)
				(name "Pin_57b")
				(number "57b")
			)
			(pin passive line
				(at 7.62 -71.12 180)
				(length 4.064)
				(name "Pin_58b")
				(number "58b")
			)
			(pin passive line
				(at 7.62 -73.66 180)
				(length 4.064)
				(name "Pin_59b")
				(number "59b")
			)
			(pin passive line
				(at 7.62 -76.2 180)
				(length 4.064)
				(name "Pin_60b")
				(number "60b")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-05Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 4.826 0)
		)
		(property "Value" "Conn_2Rows-05Pins_Shielded"
			(at 2.286 -4.826 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 05 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-05Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at 1.27 -7.62 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-07Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 4.826 0)
		)
		(property "Value" "Conn_2Rows-07Pins_Shielded"
			(at 2.286 -7.366 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 07 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-07Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at 1.27 -10.16 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-09Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 7.366 0)
		)
		(property "Value" "Conn_2Rows-09Pins_Shielded"
			(at 2.286 -7.366 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 09 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-09Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at 1.27 -10.16 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-11Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 7.366 0)
		)
		(property "Value" "Conn_2Rows-11Pins_Shielded"
			(at 2.286 -9.906 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 11 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-11Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at 1.27 -12.7 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-13Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 9.906 0)
		)
		(property "Value" "Conn_2Rows-13Pins_Shielded"
			(at 2.286 -9.906 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 13 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-13Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at 1.27 -12.7 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-15Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 9.906 0)
		)
		(property "Value" "Conn_2Rows-15Pins_Shielded"
			(at 2.286 -12.446 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 15 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-15Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at 1.27 -15.24 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-17Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 12.446 0)
		)
		(property "Value" "Conn_2Rows-17Pins_Shielded"
			(at 2.286 -12.446 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 17 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-17Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at 1.27 -15.24 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-19Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 12.446 0)
		)
		(property "Value" "Conn_2Rows-19Pins_Shielded"
			(at 2.286 -14.986 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 19 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-19Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at 1.27 -17.78 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-21Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 14.986 0)
		)
		(property "Value" "Conn_2Rows-21Pins_Shielded"
			(at 2.286 -14.986 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 21 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-21Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at 1.27 -17.78 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-23Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 14.986 0)
		)
		(property "Value" "Conn_2Rows-23Pins_Shielded"
			(at 2.286 -17.526 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 23 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-23Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at 1.27 -20.32 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-25Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 17.526 0)
		)
		(property "Value" "Conn_2Rows-25Pins_Shielded"
			(at 2.286 -17.526 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 25 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-25Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at 1.27 -20.32 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-27Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 17.526 0)
		)
		(property "Value" "Conn_2Rows-27Pins_Shielded"
			(at 2.286 -20.066 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 27 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-27Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at 1.27 -22.86 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-29Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 20.066 0)
		)
		(property "Value" "Conn_2Rows-29Pins_Shielded"
			(at 2.286 -20.066 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 29 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-29Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at 1.27 -22.86 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-31Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 20.066 0)
		)
		(property "Value" "Conn_2Rows-31Pins_Shielded"
			(at 2.286 -22.606 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 31 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-31Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at 1.27 -25.4 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-33Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 22.606 0)
		)
		(property "Value" "Conn_2Rows-33Pins_Shielded"
			(at 2.286 -22.606 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 33 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-33Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at 1.27 -25.4 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-35Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 22.606 0)
		)
		(property "Value" "Conn_2Rows-35Pins_Shielded"
			(at 2.286 -25.146 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 35 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-35Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at 1.27 -27.94 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-37Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 25.146 0)
		)
		(property "Value" "Conn_2Rows-37Pins_Shielded"
			(at 2.286 -25.146 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 37 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-37Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at 1.27 -27.94 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-39Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 25.146 0)
		)
		(property "Value" "Conn_2Rows-39Pins_Shielded"
			(at 2.286 -27.686 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 39 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-39Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at 1.27 -30.48 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-41Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 27.686 0)
		)
		(property "Value" "Conn_2Rows-41Pins_Shielded"
			(at 2.286 -27.686 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 41 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-41Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at 1.27 -30.48 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-43Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 27.686 0)
		)
		(property "Value" "Conn_2Rows-43Pins_Shielded"
			(at 2.286 -30.226 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 43 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-43Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at 1.27 -33.02 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-45Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 30.226 0)
		)
		(property "Value" "Conn_2Rows-45Pins_Shielded"
			(at 2.286 -30.226 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 45 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-45Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at 1.27 -33.02 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-47Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 30.226 0)
		)
		(property "Value" "Conn_2Rows-47Pins_Shielded"
			(at 2.286 -32.766 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 47 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-47Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at 1.27 -35.56 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-49Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 32.766 0)
		)
		(property "Value" "Conn_2Rows-49Pins_Shielded"
			(at 2.286 -32.766 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 49 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-49Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at 1.27 -35.56 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-51Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 32.766 0)
		)
		(property "Value" "Conn_2Rows-51Pins_Shielded"
			(at 2.286 -35.306 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 51 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-51Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at 1.27 -38.1 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-53Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 35.306 0)
		)
		(property "Value" "Conn_2Rows-53Pins_Shielded"
			(at 2.286 -35.306 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 53 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-53Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at 1.27 -38.1 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-55Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 35.306 0)
		)
		(property "Value" "Conn_2Rows-55Pins_Shielded"
			(at 2.286 -37.846 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 55 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-55Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at 1.27 -40.64 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-57Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 37.846 0)
		)
		(property "Value" "Conn_2Rows-57Pins_Shielded"
			(at 2.286 -37.846 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 57 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-57Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at 1.27 -40.64 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-59Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 37.846 0)
		)
		(property "Value" "Conn_2Rows-59Pins_Shielded"
			(at 2.286 -40.386 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 59 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-59Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at 1.27 -43.18 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-61Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 40.386 0)
		)
		(property "Value" "Conn_2Rows-61Pins_Shielded"
			(at 2.286 -40.386 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 61 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-61Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at 1.27 -43.18 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-63Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 40.386 0)
		)
		(property "Value" "Conn_2Rows-63Pins_Shielded"
			(at 2.286 -42.926 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 63 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-63Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at 1.27 -45.72 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-65Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 42.926 0)
		)
		(property "Value" "Conn_2Rows-65Pins_Shielded"
			(at 2.286 -42.926 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 65 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-65Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at 1.27 -45.72 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-67Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 42.926 0)
		)
		(property "Value" "Conn_2Rows-67Pins_Shielded"
			(at 2.286 -45.466 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 67 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-67Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at 1.27 -48.26 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-69Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 45.466 0)
		)
		(property "Value" "Conn_2Rows-69Pins_Shielded"
			(at 2.286 -45.466 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 69 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-69Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at 1.27 -48.26 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-71Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 45.466 0)
		)
		(property "Value" "Conn_2Rows-71Pins_Shielded"
			(at 2.286 -48.006 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 71 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-71Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_71")
				(number "71")
			)
			(pin passive line
				(at 1.27 -50.8 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-73Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 48.006 0)
		)
		(property "Value" "Conn_2Rows-73Pins_Shielded"
			(at 2.286 -48.006 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 73 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-73Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_71")
				(number "71")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_73")
				(number "73")
			)
			(pin passive line
				(at 1.27 -50.8 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_72")
				(number "72")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Conn_2Rows-75Pins_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.524 48.006 0)
		)
		(property "Value" "Conn_2Rows-75Pins_Shielded"
			(at 2.286 -50.546 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Generic shielded connector, double row, 75 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
		)
		(property "ki_keywords" "connector"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Connector*:*2Rows*Pins-1SH_* *FCC*2Rows*Pins-1SH_*"
			(at 0 0 0)
		)
		(symbol "Conn_2Rows-75Pins_Shielded_1_1"
			(pin passive line
				(at -5.08 45.72 0)
				(length 4.064)
				(name "Pin_1")
				(number "1")
			)
			(pin passive line
				(at -5.08 43.18 0)
				(length 4.064)
				(name "Pin_3")
				(number "3")
			)
			(pin passive line
				(at -5.08 40.64 0)
				(length 4.064)
				(name "Pin_5")
				(number "5")
			)
			(pin passive line
				(at -5.08 38.1 0)
				(length 4.064)
				(name "Pin_7")
				(number "7")
			)
			(pin passive line
				(at -5.08 35.56 0)
				(length 4.064)
				(name "Pin_9")
				(number "9")
			)
			(pin passive line
				(at -5.08 33.02 0)
				(length 4.064)
				(name "Pin_11")
				(number "11")
			)
			(pin passive line
				(at -5.08 30.48 0)
				(length 4.064)
				(name "Pin_13")
				(number "13")
			)
			(pin passive line
				(at -5.08 27.94 0)
				(length 4.064)
				(name "Pin_15")
				(number "15")
			)
			(pin passive line
				(at -5.08 25.4 0)
				(length 4.064)
				(name "Pin_17")
				(number "17")
			)
			(pin passive line
				(at -5.08 22.86 0)
				(length 4.064)
				(name "Pin_19")
				(number "19")
			)
			(pin passive line
				(at -5.08 20.32 0)
				(length 4.064)
				(name "Pin_21")
				(number "21")
			)
			(pin passive line
				(at -5.08 17.78 0)
				(length 4.064)
				(name "Pin_23")
				(number "23")
			)
			(pin passive line
				(at -5.08 15.24 0)
				(length 4.064)
				(name "Pin_25")
				(number "25")
			)
			(pin passive line
				(at -5.08 12.7 0)
				(length 4.064)
				(name "Pin_27")
				(number "27")
			)
			(pin passive line
				(at -5.08 10.16 0)
				(length 4.064)
				(name "Pin_29")
				(number "29")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 4.064)
				(name "Pin_31")
				(number "31")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 4.064)
				(name "Pin_33")
				(number "33")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 4.064)
				(name "Pin_35")
				(number "35")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 4.064)
				(name "Pin_37")
				(number "37")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 4.064)
				(name "Pin_39")
				(number "39")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 4.064)
				(name "Pin_41")
				(number "41")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 4.064)
				(name "Pin_43")
				(number "43")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 4.064)
				(name "Pin_45")
				(number "45")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 4.064)
				(name "Pin_47")
				(number "47")
			)
			(pin passive line
				(at -5.08 -15.24 0)
				(length 4.064)
				(name "Pin_49")
				(number "49")
			)
			(pin passive line
				(at -5.08 -17.78 0)
				(length 4.064)
				(name "Pin_51")
				(number "51")
			)
			(pin passive line
				(at -5.08 -20.32 0)
				(length 4.064)
				(name "Pin_53")
				(number "53")
			)
			(pin passive line
				(at -5.08 -22.86 0)
				(length 4.064)
				(name "Pin_55")
				(number "55")
			)
			(pin passive line
				(at -5.08 -25.4 0)
				(length 4.064)
				(name "Pin_57")
				(number "57")
			)
			(pin passive line
				(at -5.08 -27.94 0)
				(length 4.064)
				(name "Pin_59")
				(number "59")
			)
			(pin passive line
				(at -5.08 -30.48 0)
				(length 4.064)
				(name "Pin_61")
				(number "61")
			)
			(pin passive line
				(at -5.08 -33.02 0)
				(length 4.064)
				(name "Pin_63")
				(number "63")
			)
			(pin passive line
				(at -5.08 -35.56 0)
				(length 4.064)
				(name "Pin_65")
				(number "65")
			)
			(pin passive line
				(at -5.08 -38.1 0)
				(length 4.064)
				(name "Pin_67")
				(number "67")
			)
			(pin passive line
				(at -5.08 -40.64 0)
				(length 4.064)
				(name "Pin_69")
				(number "69")
			)
			(pin passive line
				(at -5.08 -43.18 0)
				(length 4.064)
				(name "Pin_71")
				(number "71")
			)
			(pin passive line
				(at -5.08 -45.72 0)
				(length 4.064)
				(name "Pin_73")
				(number "73")
			)
			(pin passive line
				(at -5.08 -48.26 0)
				(length 4.064)
				(name "Pin_75")
				(number "75")
			)
			(pin passive line
				(at 1.27 -53.34 90)
				(length 3.81)
				(name "Shield")
				(number "SH")
			)
			(pin passive line
				(at 7.62 45.72 180)
				(length 4.064)
				(name "Pin_2")
				(number "2")
			)
			(pin passive line
				(at 7.62 43.18 180)
				(length 4.064)
				(name "Pin_4")
				(number "4")
			)
			(pin passive line
				(at 7.62 40.64 180)
				(length 4.064)
				(name "Pin_6")
				(number "6")
			)
			(pin passive line
				(at 7.62 38.1 180)
				(length 4.064)
				(name "Pin_8")
				(number "8")
			)
			(pin passive line
				(at 7.62 35.56 180)
				(length 4.064)
				(name "Pin_10")
				(number "10")
			)
			(pin passive line
				(at 7.62 33.02 180)
				(length 4.064)
				(name "Pin_12")
				(number "12")
			)
			(pin passive line
				(at 7.62 30.48 180)
				(length 4.064)
				(name "Pin_14")
				(number "14")
			)
			(pin passive line
				(at 7.62 27.94 180)
				(length 4.064)
				(name "Pin_16")
				(number "16")
			)
			(pin passive line
				(at 7.62 25.4 180)
				(length 4.064)
				(name "Pin_18")
				(number "18")
			)
			(pin passive line
				(at 7.62 22.86 180)
				(length 4.064)
				(name "Pin_20")
				(number "20")
			)
			(pin passive line
				(at 7.62 20.32 180)
				(length 4.064)
				(name "Pin_22")
				(number "22")
			)
			(pin passive line
				(at 7.62 17.78 180)
				(length 4.064)
				(name "Pin_24")
				(number "24")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 4.064)
				(name "Pin_26")
				(number "26")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 4.064)
				(name "Pin_28")
				(number "28")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 4.064)
				(name "Pin_30")
				(number "30")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 4.064)
				(name "Pin_32")
				(number "32")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 4.064)
				(name "Pin_34")
				(number "34")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 4.064)
				(name "Pin_36")
				(number "36")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 4.064)
				(name "Pin_38")
				(number "38")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 4.064)
				(name "Pin_40")
				(number "40")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 4.064)
				(name "Pin_42")
				(number "42")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 4.064)
				(name "Pin_44")
				(number "44")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 4.064)
				(name "Pin_46")
				(number "46")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 4.064)
				(name "Pin_48")
				(number "48")
			)
			(pin passive line
				(at 7.62 -15.24 180)
				(length 4.064)
				(name "Pin_50")
				(number "50")
			)
			(pin passive line
				(at 7.62 -17.78 180)
				(length 4.064)
				(name "Pin_52")
				(number "52")
			)
			(pin passive line
				(at 7.62 -20.32 180)
				(length 4.064)
				(name "Pin_54")
				(number "54")
			)
			(pin passive line
				(at 7.62 -22.86 180)
				(length 4.064)
				(name "Pin_56")
				(number "56")
			)
			(pin passive line
				(at 7.62 -25.4 180)
				(length 4.064)
				(name "Pin_58")
				(number "58")
			)
			(pin passive line
				(at 7.62 -27.94 180)
				(length 4.064)
				(name "Pin_60")
				(number "60")
			)
			(pin passive line
				(at 7.62 -30.48 180)
				(length 4.064)
				(name "Pin_62")
				(number "62")
			)
			(pin passive line
				(at 7.62 -33.02 180)
				(length 4.064)
				(name "Pin_64")
				(number "64")
			)
			(pin passive line
				(at 7.62 -35.56 180)
				(length 4.064)
				(name "Pin_66")
				(number "66")
			)
			(pin passive line
				(at 7.62 -38.1 180)
				(length 4.064)
				(name "Pin_68")
				(number "68")
			)
			(pin passive line
				(at 7.62 -40.64 180)
				(length 4.064)
				(name "Pin_70")
				(number "70")
			)
			(pin passive line
				(at 7.62 -43.18 180)
				(length 4.064)
				(name "Pin_72")
				(number "72")
			)
			(pin passive line
				(at 7.62 -45.72 180)
				(length 4.064)
				(name "Pin_74")
				(number "74")
			)
		)
		(embedded_fonts no)
	)
)
