(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ADAU1450"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 46.99 0)
		)
		(property "Value" "ADAU1450"
			(at 15.24 46.99 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-72-1EP_10x10mm_P0.5mm_EP5.3x5.3mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADAU1452_1451_1450.pdf"
			(at 0 0 0)
		)
		(property "Description" "SigmaDSP SigmaDSP Digital Audio Processor, 147.456 MHz, 8kword Data RAM, I2C/SPI, LFCSP-72"
			(at 0 0 0)
		)
		(property "ki_keywords" "sigmadsp audio"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADAU1450_0_1")
		(symbol "ADAU1450_1_1"
			(pin passive line
				(at -22.86 43.18 0)
				(length 2.54)
				(name "PLLFILT")
				(number "16")
			)
			(pin input line
				(at -22.86 38.1 0)
				(length 2.54)
				(name "SPDIFIN")
				(number "4")
			)
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "XTALIN/MCLK")
				(number "21")
			)
			(pin output line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "XTALOUT")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "BCLK_IN0")
				(number "57")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "LRCLK_IN0/MP10")
				(number "58")
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "SDATA_IN0")
				(number "59")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "BCLK_IN1")
				(number "60")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "LRCLK_IN1/MP11")
				(number "61")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "SDATA_IN1")
				(number "62")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "BCLK_IN2")
				(number "65")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "LRCLK_IN2/MP12")
				(number "66")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "SDATA_IN2")
				(number "67")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "BCLK_IN3")
				(number "68")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "LRCLK_IN3/MP13")
				(number "69")
			)
			(pin input line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "SDATA_IN3")
				(number "70")
			)
			(pin input line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "SELFBOOT")
				(number "34")
			)
			(pin input line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "~{RESET}")
				(number "24")
			)
			(pin input line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "AUXADC0")
				(number "8")
			)
			(pin input line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "AUXADC1")
				(number "9")
			)
			(pin input line
				(at -22.86 -33.02 0)
				(length 2.54)
				(name "AUXADC2")
				(number "10")
			)
			(pin input line
				(at -22.86 -35.56 0)
				(length 2.54)
				(name "AUXADC3")
				(number "11")
			)
			(pin input line
				(at -22.86 -38.1 0)
				(length 2.54)
				(name "AUXADC4")
				(number "12")
			)
			(pin input line
				(at -22.86 -40.64 0)
				(length 2.54)
				(name "AUXADC5")
				(number "13")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "PVDD")
				(number "15")
			)
			(pin power_in line
				(at -5.08 -48.26 90)
				(length 2.54)
				(name "PGND")
				(number "14")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "AVDD")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "AGND")
				(number "6")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "IOVDD")
				(number "18")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "IOVDD")
				(number "2")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "IOVDD")
				(number "38")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "IOVDD")
				(number "56")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "EP")
				(number "73")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "DVDD")
				(number "20")
			)
			(pin passive line
				(at 2.54 48.26 270)
				(length 2.54)
				(hide yes)
				(name "DVDD")
				(number "35")
			)
			(pin passive line
				(at 2.54 48.26 270)
				(length 2.54)
				(hide yes)
				(name "DVDD")
				(number "53")
			)
			(pin passive line
				(at 2.54 48.26 270)
				(length 2.54)
				(hide yes)
				(name "DVDD")
				(number "71")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "DGND")
				(number "1")
			)
			(pin passive line
				(at 2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "17")
			)
			(pin passive line
				(at 2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "19")
			)
			(pin passive line
				(at 2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "25")
			)
			(pin passive line
				(at 2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "36")
			)
			(pin passive line
				(at 2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "37")
			)
			(pin passive line
				(at 2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "54")
			)
			(pin passive line
				(at 2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "55")
			)
			(pin passive line
				(at 2.54 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "72")
			)
			(pin output line
				(at 22.86 43.18 180)
				(length 2.54)
				(name "VDRIVE")
				(number "3")
			)
			(pin output line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "SPDIFOUT")
				(number "5")
			)
			(pin output line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "CLKOUT")
				(number "23")
			)
			(pin passive line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "THD_P")
				(number "64")
			)
			(pin passive line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "THD_M")
				(number "63")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "LRCLK_OUT0/MP4")
				(number "39")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "BCLK_OUT0")
				(number "40")
			)
			(pin output line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "SDATA_OUT0")
				(number "41")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "LRCLK_OUT1/MP5")
				(number "42")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "BCLK_OUT1")
				(number "43")
			)
			(pin output line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "SDATA_OUT1")
				(number "44")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "LRCLK_OUT2/MP8")
				(number "47")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "BCLK_OUT2")
				(number "48")
			)
			(pin output line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "SDATA_OUT2")
				(number "49")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "LRCLK_OUT3/MP9")
				(number "50")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "BCLK_OUT3")
				(number "51")
			)
			(pin output line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "SDATA_OUT3")
				(number "52")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "SS_M/MP0")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "MOSI_M/MP1")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "SCL_M/SCLK_M/MP2")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "SDA_M/MISO_M/MP3")
				(number "29")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "MISO/SDA")
				(number "30")
			)
			(pin input line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "SCLK/SCL")
				(number "31")
			)
			(pin input line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "MOSI/ADDR1")
				(number "32")
			)
			(pin input line
				(at 22.86 -38.1 180)
				(length 2.54)
				(name "SS/ADDR0")
				(number "33")
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 2.54)
				(name "MP6")
				(number "45")
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 2.54)
				(name "MP7")
				(number "46")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADAU1701"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 31.75 0)
		)
		(property "Value" "ADAU1701"
			(at 3.81 31.75 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADAU1701.pdf"
			(at 0 0 0)
		)
		(property "Description" "SigmaDSP 28-/56-Bit Audio Processor with Two ADCs and Four DACs, 50 MIPS, 1kword Program RAM, 2kword Data RAM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "sigmadsp audio adc dac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADAU1701_0_1")
		(symbol "ADAU1701_1_1"
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "ADC0")
				(number "2")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "ADC1")
				(number "4")
			)
			(pin passive line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "ADC_RES")
				(number "3")
			)
			(pin passive line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "OSCO")
				(number "31")
			)
			(pin passive line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "MCLKI")
				(number "32")
			)
			(pin passive line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PLL_LF")
				(number "35")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PLL_MODE0")
				(number "38")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "PLL_MODE1")
				(number "39")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "ADDR0")
				(number "7")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "ADDR1/CDATA/WB")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "CLATCH/WP")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "SDA/COUT")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "SCL/CCLK")
				(number "23")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "~{RESET}")
				(number "5")
			)
			(pin input line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "SELFBOOT")
				(number "6")
			)
			(pin output line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "FILTA")
				(number "47")
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 2.54)
				(name "AVDD")
				(number "36")
			)
			(pin passive line
				(at -5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "48")
			)
			(pin power_in line
				(at -5.08 -33.02 90)
				(length 2.54)
				(name "AGND")
				(number "1")
			)
			(pin passive line
				(at -5.08 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "37")
			)
			(pin passive line
				(at -5.08 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "42")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "PVDD")
				(number "34")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 2.54)
				(name "PGND")
				(number "33")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "IOVDD")
				(number "18")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(name "RSVD")
				(number "30")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "DVDD")
				(number "13")
			)
			(pin passive line
				(at 2.54 33.02 270)
				(length 2.54)
				(hide yes)
				(name "DVDD")
				(number "24")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 2.54)
				(name "DGND")
				(number "12")
			)
			(pin passive line
				(at 2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "25")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "VDRIVE")
				(number "17")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "VOUT0")
				(number "46")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "VOUT1")
				(number "45")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "VOUT2")
				(number "44")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "VOUT3")
				(number "43")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "CM")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "MP0")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "MP1")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "MP2")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "MP3")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "MP4")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "MP5")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "MP6")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "MP7")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "MP8")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "MP9")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "MP10")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "MP11")
				(number "19")
			)
			(pin output line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "FILTD")
				(number "41")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADAU1451"
		(extends "ADAU1450")
		(property "Reference" "U"
			(at -17.78 46.99 0)
		)
		(property "Value" "ADAU1451"
			(at 15.24 46.99 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-72-1EP_10x10mm_P0.5mm_EP5.3x5.3mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADAU1452_1451_1450.pdf"
			(at 0 0 0)
		)
		(property "Description" "SigmaDSP SigmaDSP Digital Audio Processor, 294.912 MHz, 40kword Data RAM, I2C/SPI, S/PDIF I/O, 16-Channel ASRC, LFCSP-72"
			(at 0 0 0)
		)
		(property "ki_keywords" "sigmadsp audio"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADAU1452"
		(extends "ADAU1450")
		(property "Reference" "U"
			(at -17.78 46.99 0)
		)
		(property "Value" "ADAU1452"
			(at 15.24 46.99 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-72-1EP_10x10mm_P0.5mm_EP5.3x5.3mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADAU1452_1451_1450.pdf"
			(at 0 0 0)
		)
		(property "Description" "SigmaDSP SigmaDSP Digital Audio Processor, 294.912 MHz, 40kword Data RAM, I2C/SPI, S/PDIF I/O, 16-Channel ASRC, LFCSP-72"
			(at 0 0 0)
		)
		(property "ki_keywords" "sigmadsp audio"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADAU1702"
		(extends "ADAU1701")
		(property "Reference" "U"
			(at -12.7 31.75 0)
		)
		(property "Value" "ADAU1702"
			(at 3.81 31.75 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADAU1702.pdf"
			(at 0 0 0)
		)
		(property "Description" "SigmaDSP 28-/56-Bit Audio Processor with Two ADCs and Four DACs, 25 MIPS, 512kword Program RAM, 512kword Data RAM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "sigmadsp audio adc dac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
