(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "DSP96002"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -41.91 127 0)
		)
		(property "Value" "DSP96002"
			(at 31.75 127 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://cache.freescale.com/files/dsp/doc/inactive/DSP96002.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit General Purpose Floating-point DSP, Dual Port, PGA-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSP 32bit Dual Port Processor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PGA-223*"
			(at 0 0 0)
		)
		(symbol "DSP96002_0_1")
		(symbol "DSP96002_1_1"
			(pin tri_state line
				(at -45.72 121.92 0)
				(length 3.81)
				(name "A.D0")
				(number "V17")
			)
			(pin tri_state line
				(at -45.72 119.38 0)
				(length 3.81)
				(name "A.D1")
				(number "V18")
			)
			(pin tri_state line
				(at -45.72 116.84 0)
				(length 3.81)
				(name "A.D2")
				(number "T16")
			)
			(pin tri_state line
				(at -45.72 114.3 0)
				(length 3.81)
				(name "A.D3")
				(number "U17")
			)
			(pin tri_state line
				(at -45.72 111.76 0)
				(length 3.81)
				(name "A.D4")
				(number "U18")
			)
			(pin tri_state line
				(at -45.72 109.22 0)
				(length 3.81)
				(name "A.D5")
				(number "R16")
			)
			(pin tri_state line
				(at -45.72 106.68 0)
				(length 3.81)
				(name "A.D6")
				(number "T17")
			)
			(pin tri_state line
				(at -45.72 104.14 0)
				(length 3.81)
				(name "A.D7")
				(number "P16")
			)
			(pin tri_state line
				(at -45.72 101.6 0)
				(length 3.81)
				(name "A.D8")
				(number "T18")
			)
			(pin tri_state line
				(at -45.72 99.06 0)
				(length 3.81)
				(name "A.D9")
				(number "R17")
			)
			(pin tri_state line
				(at -45.72 96.52 0)
				(length 3.81)
				(name "A.D10")
				(number "R18")
			)
			(pin tri_state line
				(at -45.72 93.98 0)
				(length 3.81)
				(name "A.D11")
				(number "N16")
			)
			(pin tri_state line
				(at -45.72 91.44 0)
				(length 3.81)
				(name "A.D12")
				(number "P17")
			)
			(pin tri_state line
				(at -45.72 88.9 0)
				(length 3.81)
				(name "A.D13")
				(number "P18")
			)
			(pin tri_state line
				(at -45.72 86.36 0)
				(length 3.81)
				(name "A.D14")
				(number "N17")
			)
			(pin tri_state line
				(at -45.72 83.82 0)
				(length 3.81)
				(name "A.D15")
				(number "N18")
			)
			(pin tri_state line
				(at -45.72 81.28 0)
				(length 3.81)
				(name "A.D16")
				(number "L16")
			)
			(pin tri_state line
				(at -45.72 78.74 0)
				(length 3.81)
				(name "A.D17")
				(number "M18")
			)
			(pin tri_state line
				(at -45.72 76.2 0)
				(length 3.81)
				(name "A.D18")
				(number "L17")
			)
			(pin tri_state line
				(at -45.72 73.66 0)
				(length 3.81)
				(name "A.D19")
				(number "L18")
			)
			(pin tri_state line
				(at -45.72 71.12 0)
				(length 3.81)
				(name "A.D20")
				(number "K16")
			)
			(pin tri_state line
				(at -45.72 68.58 0)
				(length 3.81)
				(name "A.D21")
				(number "K17")
			)
			(pin tri_state line
				(at -45.72 66.04 0)
				(length 3.81)
				(name "A.D22")
				(number "K18")
			)
			(pin tri_state line
				(at -45.72 63.5 0)
				(length 3.81)
				(name "A.D23")
				(number "J18")
			)
			(pin tri_state line
				(at -45.72 60.96 0)
				(length 3.81)
				(name "A.D24")
				(number "J16")
			)
			(pin tri_state line
				(at -45.72 58.42 0)
				(length 3.81)
				(name "A.D25")
				(number "J17")
			)
			(pin tri_state line
				(at -45.72 55.88 0)
				(length 3.81)
				(name "A.D26")
				(number "H18")
			)
			(pin tri_state line
				(at -45.72 53.34 0)
				(length 3.81)
				(name "A.D27")
				(number "H17")
			)
			(pin tri_state line
				(at -45.72 50.8 0)
				(length 3.81)
				(name "A.D28")
				(number "H16")
			)
			(pin tri_state line
				(at -45.72 48.26 0)
				(length 3.81)
				(name "A.D29")
				(number "G18")
			)
			(pin tri_state line
				(at -45.72 45.72 0)
				(length 3.81)
				(name "A.D30")
				(number "G17")
			)
			(pin tri_state line
				(at -45.72 43.18 0)
				(length 3.81)
				(name "A.D31")
				(number "F18")
			)
			(pin tri_state line
				(at -45.72 38.1 0)
				(length 3.81)
				(name "A.A0")
				(number "B11")
			)
			(pin tri_state line
				(at -45.72 35.56 0)
				(length 3.81)
				(name "A.A1")
				(number "C10")
			)
			(pin tri_state line
				(at -45.72 33.02 0)
				(length 3.81)
				(name "A.A2")
				(number "A13")
			)
			(pin tri_state line
				(at -45.72 30.48 0)
				(length 3.81)
				(name "A.A3")
				(number "B12")
			)
			(pin tri_state line
				(at -45.72 27.94 0)
				(length 3.81)
				(name "A.A4")
				(number "A14")
			)
			(pin tri_state line
				(at -45.72 25.4 0)
				(length 3.81)
				(name "A.A5")
				(number "C11")
			)
			(pin tri_state line
				(at -45.72 22.86 0)
				(length 3.81)
				(name "A.A6")
				(number "B13")
			)
			(pin tri_state line
				(at -45.72 20.32 0)
				(length 3.81)
				(name "A.A7")
				(number "A15")
			)
			(pin tri_state line
				(at -45.72 17.78 0)
				(length 3.81)
				(name "A.A8")
				(number "C12")
			)
			(pin tri_state line
				(at -45.72 15.24 0)
				(length 3.81)
				(name "A.A9")
				(number "B14")
			)
			(pin tri_state line
				(at -45.72 12.7 0)
				(length 3.81)
				(name "A.A10")
				(number "A16")
			)
			(pin tri_state line
				(at -45.72 10.16 0)
				(length 3.81)
				(name "A.A11")
				(number "B15")
			)
			(pin tri_state line
				(at -45.72 7.62 0)
				(length 3.81)
				(name "A.A12")
				(number "C13")
			)
			(pin tri_state line
				(at -45.72 5.08 0)
				(length 3.81)
				(name "A.A13")
				(number "A17")
			)
			(pin tri_state line
				(at -45.72 2.54 0)
				(length 3.81)
				(name "A.A14")
				(number "B16")
			)
			(pin tri_state line
				(at -45.72 0 0)
				(length 3.81)
				(name "A.A15")
				(number "C14")
			)
			(pin tri_state line
				(at -45.72 -2.54 0)
				(length 3.81)
				(name "A.A16")
				(number "A18")
			)
			(pin tri_state line
				(at -45.72 -5.08 0)
				(length 3.81)
				(name "A.A17")
				(number "C15")
			)
			(pin tri_state line
				(at -45.72 -7.62 0)
				(length 3.81)
				(name "A.A18")
				(number "B17")
			)
			(pin tri_state line
				(at -45.72 -10.16 0)
				(length 3.81)
				(name "A.A19")
				(number "C16")
			)
			(pin tri_state line
				(at -45.72 -12.7 0)
				(length 3.81)
				(name "A.A20")
				(number "B18")
			)
			(pin tri_state line
				(at -45.72 -15.24 0)
				(length 3.81)
				(name "A.A21")
				(number "C17")
			)
			(pin tri_state line
				(at -45.72 -17.78 0)
				(length 3.81)
				(name "A.A22")
				(number "D16")
			)
			(pin tri_state line
				(at -45.72 -20.32 0)
				(length 3.81)
				(name "A.A23")
				(number "C18")
			)
			(pin tri_state line
				(at -45.72 -22.86 0)
				(length 3.81)
				(name "A.A24")
				(number "E16")
			)
			(pin tri_state line
				(at -45.72 -25.4 0)
				(length 3.81)
				(name "A.A25")
				(number "D17")
			)
			(pin tri_state line
				(at -45.72 -27.94 0)
				(length 3.81)
				(name "A.A26")
				(number "D18")
			)
			(pin tri_state line
				(at -45.72 -30.48 0)
				(length 3.81)
				(name "A.A27")
				(number "F16")
			)
			(pin tri_state line
				(at -45.72 -33.02 0)
				(length 3.81)
				(name "A.A28")
				(number "E17")
			)
			(pin tri_state line
				(at -45.72 -35.56 0)
				(length 3.81)
				(name "A.A29")
				(number "E18")
			)
			(pin tri_state line
				(at -45.72 -38.1 0)
				(length 3.81)
				(name "A.A30")
				(number "F17")
			)
			(pin tri_state line
				(at -45.72 -40.64 0)
				(length 3.81)
				(name "A.A31")
				(number "G16")
			)
			(pin tri_state line
				(at -45.72 -45.72 0)
				(length 3.81)
				(name "A.R/W")
				(number "A9")
			)
			(pin output inverted
				(at -45.72 -50.8 0)
				(length 3.81)
				(name "A.BUS_STR")
				(number "B10")
			)
			(pin output inverted
				(at -45.72 -53.34 0)
				(length 3.81)
				(name "A.BUS_LOCK")
				(number "C7")
			)
			(pin output inverted
				(at -45.72 -58.42 0)
				(length 3.81)
				(name "A.T_TYPE")
				(number "C8")
			)
			(pin tri_state inverted
				(at -45.72 -60.96 0)
				(length 3.81)
				(name "A.T_STROBE")
				(number "A11")
			)
			(pin input inverted
				(at -45.72 -63.5 0)
				(length 3.81)
				(name "A.TACK")
				(number "J1")
			)
			(pin input inverted
				(at -45.72 -68.58 0)
				(length 3.81)
				(name "A.AENB")
				(number "A12")
			)
			(pin input inverted
				(at -45.72 -71.12 0)
				(length 3.81)
				(name "A.DENB")
				(number "M17")
			)
			(pin input inverted
				(at -45.72 -76.2 0)
				(length 3.81)
				(name "A.HOSTSEL")
				(number "T5")
			)
			(pin input inverted
				(at -45.72 -78.74 0)
				(length 3.81)
				(name "A.HOSTACK")
				(number "U4")
			)
			(pin output inverted
				(at -45.72 -81.28 0)
				(length 3.81)
				(name "A.HOSTREQ")
				(number "T3")
			)
			(pin output inverted
				(at -45.72 -86.36 0)
				(length 3.81)
				(name "A.BR")
				(number "A7")
			)
			(pin input inverted
				(at -45.72 -88.9 0)
				(length 3.81)
				(name "A.BG")
				(number "B6")
			)
			(pin open_collector inverted
				(at -45.72 -91.44 0)
				(length 3.81)
				(name "A.BA")
				(number "B7")
			)
			(pin input inverted
				(at -45.72 -93.98 0)
				(length 3.81)
				(name "A.BB")
				(number "A6")
			)
			(pin tri_state inverted
				(at -45.72 -99.06 0)
				(length 3.81)
				(name "A.S0")
				(number "A10")
			)
			(pin tri_state inverted
				(at -45.72 -101.6 0)
				(length 3.81)
				(name "A.S1")
				(number "B9")
			)
			(pin input line
				(at -45.72 -106.68 0)
				(length 3.81)
				(name "MODA/IRQA")
				(number "A5")
			)
			(pin input line
				(at -45.72 -109.22 0)
				(length 3.81)
				(name "MODB/IRQB")
				(number "B5")
			)
			(pin input line
				(at -45.72 -111.76 0)
				(length 3.81)
				(name "MODC/IRQC")
				(number "C5")
			)
			(pin input clock
				(at -45.72 -116.84 0)
				(length 3.81)
				(name "CLK")
				(number "H2")
			)
			(pin input inverted
				(at -45.72 -119.38 0)
				(length 3.81)
				(name "RESET")
				(number "C6")
			)
			(pin power_in line
				(at -35.56 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "C4")
			)
			(pin power_in line
				(at -33.02 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "D5")
			)
			(pin power_in line
				(at -30.48 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "D6")
			)
			(pin power_in line
				(at -27.94 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "D7")
			)
			(pin power_in line
				(at -25.4 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "D11")
			)
			(pin power_in line
				(at -22.86 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "D13")
			)
			(pin power_in line
				(at -20.32 129.54 270)
				(length 3.81)
				(name "VCC")
				(number "G3")
			)
			(pin power_in line
				(at -20.32 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "D14")
			)
			(pin power_in line
				(at -17.78 129.54 270)
				(length 3.81)
				(name "VCC")
				(number "G4")
			)
			(pin power_in line
				(at -17.78 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "D15")
			)
			(pin power_in line
				(at -15.24 129.54 270)
				(length 3.81)
				(name "VCC")
				(number "H4")
			)
			(pin power_in line
				(at -15.24 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "E4")
			)
			(pin power_in line
				(at -12.7 129.54 270)
				(length 3.81)
				(name "VCC")
				(number "K4")
			)
			(pin power_in line
				(at -12.7 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -10.16 129.54 270)
				(length 3.81)
				(name "VCC")
				(number "L4")
			)
			(pin power_in line
				(at -10.16 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at -7.62 129.54 270)
				(length 3.81)
				(name "VCC")
				(number "D8")
			)
			(pin power_in line
				(at -7.62 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "F15")
			)
			(pin power_in line
				(at -5.08 129.54 270)
				(length 3.81)
				(name "VCC")
				(number "D9")
			)
			(pin power_in line
				(at -5.08 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "G15")
			)
			(pin power_in line
				(at -2.54 129.54 270)
				(length 3.81)
				(name "VCC")
				(number "R7")
			)
			(pin power_in line
				(at -2.54 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "J4")
			)
			(pin power_in line
				(at 0 129.54 270)
				(length 3.81)
				(name "VCC")
				(number "R9")
			)
			(pin power_in line
				(at 0 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at 2.54 129.54 270)
				(length 3.81)
				(name "VCC")
				(number "D10")
			)
			(pin power_in line
				(at 2.54 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "K15")
			)
			(pin power_in line
				(at 5.08 129.54 270)
				(length 3.81)
				(name "VCC")
				(number "D12")
			)
			(pin power_in line
				(at 5.08 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "M4")
			)
			(pin power_in line
				(at 7.62 129.54 270)
				(length 3.81)
				(name "VCC")
				(number "H15")
			)
			(pin power_in line
				(at 7.62 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "N4")
			)
			(pin power_in line
				(at 10.16 129.54 270)
				(length 3.81)
				(name "VCC")
				(number "L15")
			)
			(pin power_in line
				(at 10.16 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "N15")
			)
			(pin power_in line
				(at 12.7 129.54 270)
				(length 3.81)
				(name "VCC")
				(number "M15")
			)
			(pin power_in line
				(at 12.7 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "P4")
			)
			(pin power_in line
				(at 15.24 129.54 270)
				(length 3.81)
				(name "VCC")
				(number "M16")
			)
			(pin power_in line
				(at 15.24 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "P15")
			)
			(pin power_in line
				(at 17.78 129.54 270)
				(length 3.81)
				(name "VCC")
				(number "R10")
			)
			(pin power_in line
				(at 17.78 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "R4")
			)
			(pin power_in line
				(at 20.32 129.54 270)
				(length 3.81)
				(name "VCC")
				(number "R11")
			)
			(pin power_in line
				(at 20.32 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 22.86 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "R6")
			)
			(pin power_in line
				(at 25.4 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "R8")
			)
			(pin power_in line
				(at 27.94 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "R12")
			)
			(pin power_in line
				(at 30.48 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "R13")
			)
			(pin power_in line
				(at 33.02 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "R14")
			)
			(pin power_in line
				(at 35.56 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "R15")
			)
			(pin power_in line
				(at 38.1 -129.54 90)
				(length 3.81)
				(name "GND")
				(number "T7")
			)
			(pin tri_state line
				(at 45.72 121.92 180)
				(length 3.81)
				(name "B.D0")
				(number "U16")
			)
			(pin tri_state line
				(at 45.72 119.38 180)
				(length 3.81)
				(name "B.D1")
				(number "T15")
			)
			(pin tri_state line
				(at 45.72 116.84 180)
				(length 3.81)
				(name "B.D2")
				(number "V16")
			)
			(pin tri_state line
				(at 45.72 114.3 180)
				(length 3.81)
				(name "B.D3")
				(number "U15")
			)
			(pin tri_state line
				(at 45.72 111.76 180)
				(length 3.81)
				(name "B.D4")
				(number "T14")
			)
			(pin tri_state line
				(at 45.72 109.22 180)
				(length 3.81)
				(name "B.D5")
				(number "V15")
			)
			(pin tri_state line
				(at 45.72 106.68 180)
				(length 3.81)
				(name "B.D6")
				(number "U14")
			)
			(pin tri_state line
				(at 45.72 104.14 180)
				(length 3.81)
				(name "B.D7")
				(number "T13")
			)
			(pin tri_state line
				(at 45.72 101.6 180)
				(length 3.81)
				(name "B.D8")
				(number "V14")
			)
			(pin tri_state line
				(at 45.72 99.06 180)
				(length 3.81)
				(name "B.D9")
				(number "U13")
			)
			(pin tri_state line
				(at 45.72 96.52 180)
				(length 3.81)
				(name "B.D10")
				(number "V13")
			)
			(pin tri_state line
				(at 45.72 93.98 180)
				(length 3.81)
				(name "B.D11")
				(number "T12")
			)
			(pin tri_state line
				(at 45.72 91.44 180)
				(length 3.81)
				(name "B.D12")
				(number "U12")
			)
			(pin tri_state line
				(at 45.72 88.9 180)
				(length 3.81)
				(name "B.D13")
				(number "V12")
			)
			(pin tri_state line
				(at 45.72 86.36 180)
				(length 3.81)
				(name "B.D14")
				(number "T11")
			)
			(pin tri_state line
				(at 45.72 83.82 180)
				(length 3.81)
				(name "B.D15")
				(number "U11")
			)
			(pin tri_state line
				(at 45.72 81.28 180)
				(length 3.81)
				(name "B.D16")
				(number "V11")
			)
			(pin tri_state line
				(at 45.72 78.74 180)
				(length 3.81)
				(name "B.D17")
				(number "T10")
			)
			(pin tri_state line
				(at 45.72 76.2 180)
				(length 3.81)
				(name "B.D18")
				(number "U10")
			)
			(pin tri_state line
				(at 45.72 73.66 180)
				(length 3.81)
				(name "B.D19")
				(number "V10")
			)
			(pin tri_state line
				(at 45.72 71.12 180)
				(length 3.81)
				(name "B.D20")
				(number "V9")
			)
			(pin tri_state line
				(at 45.72 68.58 180)
				(length 3.81)
				(name "B.D21")
				(number "U9")
			)
			(pin tri_state line
				(at 45.72 66.04 180)
				(length 3.81)
				(name "B.D22")
				(number "T9")
			)
			(pin tri_state line
				(at 45.72 63.5 180)
				(length 3.81)
				(name "B.D23")
				(number "V8")
			)
			(pin tri_state line
				(at 45.72 60.96 180)
				(length 3.81)
				(name "B.D24")
				(number "U8")
			)
			(pin tri_state line
				(at 45.72 58.42 180)
				(length 3.81)
				(name "B.D25")
				(number "V7")
			)
			(pin tri_state line
				(at 45.72 55.88 180)
				(length 3.81)
				(name "B.D26")
				(number "T8")
			)
			(pin tri_state line
				(at 45.72 53.34 180)
				(length 3.81)
				(name "B.D27")
				(number "U7")
			)
			(pin tri_state line
				(at 45.72 50.8 180)
				(length 3.81)
				(name "B.D28")
				(number "V6")
			)
			(pin tri_state line
				(at 45.72 48.26 180)
				(length 3.81)
				(name "B.D29")
				(number "U6")
			)
			(pin tri_state line
				(at 45.72 45.72 180)
				(length 3.81)
				(name "B.D30")
				(number "V5")
			)
			(pin tri_state line
				(at 45.72 43.18 180)
				(length 3.81)
				(name "B.D31")
				(number "T6")
			)
			(pin tri_state line
				(at 45.72 38.1 180)
				(length 3.81)
				(name "B.A0")
				(number "M1")
			)
			(pin tri_state line
				(at 45.72 35.56 180)
				(length 3.81)
				(name "B.A1")
				(number "L2")
			)
			(pin tri_state line
				(at 45.72 33.02 180)
				(length 3.81)
				(name "B.A2")
				(number "L3")
			)
			(pin tri_state line
				(at 45.72 30.48 180)
				(length 3.81)
				(name "B.A3")
				(number "L1")
			)
			(pin tri_state line
				(at 45.72 27.94 180)
				(length 3.81)
				(name "B.A4")
				(number "K1")
			)
			(pin tri_state line
				(at 45.72 25.4 180)
				(length 3.81)
				(name "B.A5")
				(number "K2")
			)
			(pin tri_state line
				(at 45.72 22.86 180)
				(length 3.81)
				(name "B.A6")
				(number "K3")
			)
			(pin tri_state line
				(at 45.72 20.32 180)
				(length 3.81)
				(name "B.A7")
				(number "J3")
			)
			(pin tri_state line
				(at 45.72 17.78 180)
				(length 3.81)
				(name "B.A8")
				(number "H1")
			)
			(pin tri_state line
				(at 45.72 15.24 180)
				(length 3.81)
				(name "B.A9")
				(number "G1")
			)
			(pin tri_state line
				(at 45.72 12.7 180)
				(length 3.81)
				(name "B.A10")
				(number "G2")
			)
			(pin tri_state line
				(at 45.72 10.16 180)
				(length 3.81)
				(name "B.A11")
				(number "H3")
			)
			(pin tri_state line
				(at 45.72 7.62 180)
				(length 3.81)
				(name "B.A12")
				(number "F1")
			)
			(pin tri_state line
				(at 45.72 5.08 180)
				(length 3.81)
				(name "B.A13")
				(number "E1")
			)
			(pin tri_state line
				(at 45.72 2.54 180)
				(length 3.81)
				(name "B.A14")
				(number "F2")
			)
			(pin tri_state line
				(at 45.72 0 180)
				(length 3.81)
				(name "B.A15")
				(number "D1")
			)
			(pin tri_state line
				(at 45.72 -2.54 180)
				(length 3.81)
				(name "B.A16")
				(number "E2")
			)
			(pin tri_state line
				(at 45.72 -5.08 180)
				(length 3.81)
				(name "B.A17")
				(number "C1")
			)
			(pin tri_state line
				(at 45.72 -7.62 180)
				(length 3.81)
				(name "B.A18")
				(number "D2")
			)
			(pin tri_state line
				(at 45.72 -10.16 180)
				(length 3.81)
				(name "B.A19")
				(number "F3")
			)
			(pin tri_state line
				(at 45.72 -12.7 180)
				(length 3.81)
				(name "B.A20")
				(number "B1")
			)
			(pin tri_state line
				(at 45.72 -15.24 180)
				(length 3.81)
				(name "B.A21")
				(number "C2")
			)
			(pin tri_state line
				(at 45.72 -17.78 180)
				(length 3.81)
				(name "B.A22")
				(number "E3")
			)
			(pin tri_state line
				(at 45.72 -20.32 180)
				(length 3.81)
				(name "B.A23")
				(number "A1")
			)
			(pin tri_state line
				(at 45.72 -22.86 180)
				(length 3.81)
				(name "B.A24")
				(number "D3")
			)
			(pin tri_state line
				(at 45.72 -25.4 180)
				(length 3.81)
				(name "B.A25")
				(number "B2")
			)
			(pin tri_state line
				(at 45.72 -27.94 180)
				(length 3.81)
				(name "B.A26")
				(number "C3")
			)
			(pin tri_state line
				(at 45.72 -30.48 180)
				(length 3.81)
				(name "B.A27")
				(number "A2")
			)
			(pin tri_state line
				(at 45.72 -33.02 180)
				(length 3.81)
				(name "B.A28")
				(number "B3")
			)
			(pin tri_state line
				(at 45.72 -35.56 180)
				(length 3.81)
				(name "B.A29")
				(number "A3")
			)
			(pin tri_state line
				(at 45.72 -38.1 180)
				(length 3.81)
				(name "B.A30")
				(number "B4")
			)
			(pin tri_state line
				(at 45.72 -40.64 180)
				(length 3.81)
				(name "B.A31")
				(number "A4")
			)
			(pin tri_state line
				(at 45.72 -45.72 180)
				(length 3.81)
				(name "B.R/W")
				(number "P1")
			)
			(pin output inverted
				(at 45.72 -50.8 180)
				(length 3.81)
				(name "B.BUS_STR")
				(number "R1")
			)
			(pin output inverted
				(at 45.72 -53.34 180)
				(length 3.81)
				(name "B.BUS_LOCK")
				(number "P3")
			)
			(pin output inverted
				(at 45.72 -58.42 180)
				(length 3.81)
				(name "B.T_TYPE")
				(number "B8")
			)
			(pin tri_state inverted
				(at 45.72 -60.96 180)
				(length 3.81)
				(name "B.T_STROBE")
				(number "P2")
			)
			(pin input inverted
				(at 45.72 -63.5 180)
				(length 3.81)
				(name "B.TACK")
				(number "J2")
			)
			(pin input inverted
				(at 45.72 -68.58 180)
				(length 3.81)
				(name "B.AENB")
				(number "N1")
			)
			(pin input inverted
				(at 45.72 -71.12 180)
				(length 3.81)
				(name "B.DENB")
				(number "U5")
			)
			(pin input inverted
				(at 45.72 -76.2 180)
				(length 3.81)
				(name "B.HOSTSEL")
				(number "V4")
			)
			(pin input inverted
				(at 45.72 -78.74 180)
				(length 3.81)
				(name "B.HOSTACK")
				(number "V3")
			)
			(pin output inverted
				(at 45.72 -81.28 180)
				(length 3.81)
				(name "B.HOSTREQ")
				(number "U1")
			)
			(pin output inverted
				(at 45.72 -86.36 180)
				(length 3.81)
				(name "B.BR")
				(number "R2")
			)
			(pin input inverted
				(at 45.72 -88.9 180)
				(length 3.81)
				(name "B.BG")
				(number "T1")
			)
			(pin open_collector inverted
				(at 45.72 -91.44 180)
				(length 3.81)
				(name "B.BA")
				(number "T2")
			)
			(pin input inverted
				(at 45.72 -93.98 180)
				(length 3.81)
				(name "B.BB")
				(number "R3")
			)
			(pin tri_state inverted
				(at 45.72 -99.06 180)
				(length 3.81)
				(name "B.S0")
				(number "M3")
			)
			(pin tri_state inverted
				(at 45.72 -101.6 180)
				(length 3.81)
				(name "B.S1")
				(number "M2")
			)
			(pin output line
				(at 45.72 -109.22 180)
				(length 3.81)
				(name "DSO")
				(number "V1")
			)
			(pin bidirectional line
				(at 45.72 -111.76 180)
				(length 3.81)
				(name "DSI/OS0")
				(number "V2")
			)
			(pin bidirectional line
				(at 45.72 -114.3 180)
				(length 3.81)
				(name "DSCK/OS1")
				(number "U2")
			)
			(pin input inverted
				(at 45.72 -116.84 180)
				(length 3.81)
				(name "DEBUGREQ")
				(number "T4")
			)
		)
		(embedded_fonts no)
	)
)
