(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "DSPIC33EP256MU810-xPT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 19.05 69.85 0)
		)
		(property "Value" "DSPIC33EP256MU810-xPT"
			(at 0 -2.54 90)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at -2.54 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/70616g.pdf"
			(at -2.54 7.62 0)
		)
		(property "Description" "High-Performance, 16-bit Digital Signal Controller, 40MIPS, 256k Flash, 30k SRAM, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit Digital Signal Controller Microchip dsPIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "DSPIC33EP256MU810-xPT_0_1")
		(symbol "DSPIC33EP256MU810-xPT_1_1"
			(pin input line
				(at -25.4 58.42 0)
				(length 2.54)
				(name "~{MCLR}")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 50.8 0)
				(length 2.54)
				(name "RA0/TMS")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 2.54)
				(name "RA1/TCK")
				(number "38")
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 2.54)
				(name "RA2/ASCL2")
				(number "58")
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 2.54)
				(name "RA3/ASDA2")
				(number "59")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "RA4/TDI")
				(number "60")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 2.54)
				(name "RA5/TDO")
				(number "61")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "RA6/AN22")
				(number "91")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "RA7/AN23")
				(number "92")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "RA9/VREF-")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "RA10/VREF+")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "RA14")
				(number "66")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "RA15")
				(number "67")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "RB0/AN0/PGED3")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "RB1/AN1/PGEC3")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "RB2/AN2")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "RB3/AN3")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "RB4/AN4")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "RB5/AN5")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "RB6/AN6/PGEC1")
				(number "26")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "RB7/AN7/PGED1")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "RB8/PMA6/AN8")
				(number "32")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "RB9/PMA7/AN9")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "RB10/PMA13/AN10")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "RB11/PMA12/AN11")
				(number "35")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "RB12/PMA11/AN12")
				(number "41")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "RB13/PMA10/AN13")
				(number "42")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "RB14/PMA1/AN14")
				(number "43")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "RB15/PMA0/AN15")
				(number "44")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "RC1/PWM5L/AN16")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "RC2/PWM5H/AN17")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "RC3/PWM6L/AN18")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 2.54)
				(name "RC4/PWM6H/AN19")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 2.54)
				(name "RC12/OSC1")
				(number "63")
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 2.54)
				(name "RC13/SOSCI/PGED2")
				(number "73")
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 2.54)
				(name "RC14/T1CK/SOSCO/PGEC2")
				(number "74")
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 2.54)
				(name "RC15/CLKO/OSC2")
				(number "64")
			)
			(pin passive line
				(at -17.78 71.12 270)
				(length 2.54)
				(name "VCAP")
				(number "85")
			)
			(pin power_in line
				(at -10.16 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "37")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "46")
			)
			(pin power_in line
				(at -2.54 -71.12 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "36")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "45")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "65")
			)
			(pin passive line
				(at -2.54 -71.12 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "75")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "86")
			)
			(pin power_in line
				(at 10.16 71.12 270)
				(length 2.54)
				(name "AVDD")
				(number "30")
			)
			(pin power_in line
				(at 10.16 -71.12 90)
				(length 2.54)
				(name "AVSS")
				(number "31")
			)
			(pin bidirectional line
				(at 25.4 66.04 180)
				(length 2.54)
				(name "INT0/RD0")
				(number "72")
			)
			(pin bidirectional line
				(at 25.4 63.5 180)
				(length 2.54)
				(name "RD1")
				(number "76")
			)
			(pin bidirectional line
				(at 25.4 60.96 180)
				(length 2.54)
				(name "DPH/RD2")
				(number "77")
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 2.54)
				(name "PMBE/RD3")
				(number "78")
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 2.54)
				(name "PMWR/RD4")
				(number "81")
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 2.54)
				(name "PMRD/RD5")
				(number "82")
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 2.54)
				(name "RD6")
				(number "83")
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 2.54)
				(name "RD7")
				(number "84")
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 2.54)
				(name "RTCC/RD8")
				(number "68")
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 2.54)
				(name "ASDA1/RD9")
				(number "69")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "ASCL1/RD10")
				(number "70")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "RD11")
				(number "71")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "RD12")
				(number "79")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "RD13")
				(number "80")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "RD14")
				(number "47")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "RD15")
				(number "48")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "AN24/PWM1L/RE0")
				(number "93")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "AN25/PWM1H/RE1")
				(number "94")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "AN26/PWM2L/PMD2/RE2")
				(number "98")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "AN27/PWM2H/PMD3/RE3")
				(number "99")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "AN28/PWM3L/PMD4/RE4")
				(number "100")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PWM3H/RE5")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PWM4L/RE6")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PWM4H/RE7")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "AN20/RE8")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "AN21/RE9")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "RF0")
				(number "87")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "RF1")
				(number "88")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "RF2")
				(number "52")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "RF3")
				(number "51")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "SDA2/PMA9/RF4")
				(number "49")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "SCL2/PMA8/RF5")
				(number "50")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "RF8")
				(number "53")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "RF12")
				(number "40")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "RF13")
				(number "39")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "RG0")
				(number "90")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "RG1")
				(number "89")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "D+/RG2")
				(number "57")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "D-/RG3")
				(number "56")
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 2.54)
				(name "VUSB3V3")
				(number "55")
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 2.54)
				(name "VBUS")
				(number "54")
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 2.54)
				(name "SCK2/PMA5/RG6")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 2.54)
				(name "SDI2/PMA4/RG7")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 2.54)
				(name "SDO2/PMA3/RG8")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 2.54)
				(name "PMA2/RG9")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 2.54)
				(name "RG12")
				(number "96")
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 2.54)
				(name "RG13")
				(number "97")
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 2.54)
				(name "RG14")
				(number "95")
			)
			(pin bidirectional line
				(at 25.4 -63.5 180)
				(length 2.54)
				(name "RG15")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DSPIC33FJ128GP204"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 48.26 0)
		)
		(property "Value" "DSPIC33FJ128GP204"
			(at -29.21 -48.26 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/70292G.pdf"
			(at 0 0 0)
		)
		(property "Description" "40MIPS, 128k Flash, 8k SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit Digital Signal Controller Microchip dsPIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN?44*1EP*8x8mm*P0.65mm* TQFP?44*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "DSPIC33FJ128GP204_1_1"
			(pin input line
				(at -33.02 45.72 0)
				(length 3.81)
				(name "~{MCLR}")
				(number "18")
			)
			(pin power_in line
				(at -7.62 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -7.62 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "40")
			)
			(pin power_in line
				(at -5.08 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "39")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 3.81)
				(name "AVDD")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 3.81)
				(name "AVSS")
				(number "16")
			)
			(pin power_in line
				(at 5.08 50.8 270)
				(length 3.81)
				(name "VCAP")
				(number "7")
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 3.81)
				(name "AN0/VREF+/CN2/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 3.81)
				(name "AN1/VREF-/CN3/RA1")
				(number "20")
			)
			(pin input line
				(at 33.02 40.64 180)
				(length 3.81)
				(name "OSC1/CLKI/CN30/RA2")
				(number "30")
			)
			(pin input line
				(at 33.02 38.1 180)
				(length 3.81)
				(name "OSC2/CLKO/CN29/RA3")
				(number "31")
			)
			(pin input line
				(at 33.02 35.56 180)
				(length 3.81)
				(name "SOSCO/T1CK/CN0/RA4")
				(number "34")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 3.81)
				(name "TCK/PMA7/RA7")
				(number "13")
			)
			(pin input line
				(at 33.02 30.48 180)
				(length 3.81)
				(name "TDO/PMA8/RA8")
				(number "32")
			)
			(pin input line
				(at 33.02 27.94 180)
				(length 3.81)
				(name "TDI/PMA9/RA9")
				(number "35")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "TMS/PMA10/RA10")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "PGED1/AN2/C2IN-/RP0/CN4/RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "PGEC1/AN3/C2IN+/RP1/CN5/RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "AN4/C1IN-/RP2/CN6/RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "AN5/C1IN+/RP3/CN7/RB3")
				(number "24")
			)
			(pin input line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "SOSCI/RP4/CN1/RB4")
				(number "33")
			)
			(pin input line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "PGED3/ASDA1/RP5/CN27/PMD7/RB5")
				(number "41")
			)
			(pin input line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "PGEC3/ASCL1/RP6/CN24/PMD6/RB6")
				(number "42")
			)
			(pin input line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "INT0/RP7/CN23/PMD5/RB7")
				(number "43")
			)
			(pin input line
				(at 33.02 0 180)
				(length 3.81)
				(name "SCL1/RP8/CN22/PMD4/RB8")
				(number "44")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "SDA1/RP9/CN21/PMD3/RB9")
				(number "1")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "PGED2/EMCD2/RP10/CN16/PMD2/RB10")
				(number "8")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "PGEC2/RP11/CN15/PMD1/RB11")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "AN12/RP12/CN14/PMD0/RB12")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "AN11/RP13/CN13/PMRD/RB13")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "AN10/RTCC/RP14/CN12/PMWR/RB14")
				(number "14")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "AN9/RP15/CN11/PMCS1/RB15")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 3.81)
				(name "AN6/RP16/CN8/RC0")
				(number "25")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 3.81)
				(name "AN7/RP17/CN9/RC1")
				(number "26")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 3.81)
				(name "AN8/CVREF/RP18/PMA2/CN10/RC2")
				(number "27")
			)
			(pin input line
				(at 33.02 -30.48 180)
				(length 3.81)
				(name "RP19/CN28/PMBE/RC3")
				(number "36")
			)
			(pin input line
				(at 33.02 -33.02 180)
				(length 3.81)
				(name "RP20/CN25/PMA4/RC4")
				(number "37")
			)
			(pin input line
				(at 33.02 -35.56 180)
				(length 3.81)
				(name "RP21/CN26/PMA3/RC5")
				(number "38")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 3.81)
				(name "RP22/CN18/PMA1/RC6")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 3.81)
				(name "RP23/CN17/PMA0/RC7")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 3.81)
				(name "RP24/CN20/PMA5/RC8")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 3.81)
				(name "RP25/CN19/PMA6/RC9")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DSPIC33FJ128GP804"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 48.26 0)
		)
		(property "Value" "DSPIC33FJ128GP804"
			(at -29.21 -48.26 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/70292G.pdf"
			(at 0 0 0)
		)
		(property "Description" "40MIPS, 128k Flash, 16k SRAM, ECAN, Audio DAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit Digital Signal Controller Microchip dsPIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN?44*1EP*8x8mm*P0.65mm* TQFP?44*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "DSPIC33FJ128GP804_1_1"
			(pin input line
				(at -33.02 45.72 0)
				(length 3.81)
				(name "~{MCLR}")
				(number "18")
			)
			(pin power_in line
				(at -7.62 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -7.62 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "40")
			)
			(pin power_in line
				(at -5.08 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "39")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 3.81)
				(name "AVDD")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 3.81)
				(name "AVSS")
				(number "16")
			)
			(pin power_in line
				(at 5.08 50.8 270)
				(length 3.81)
				(name "VCAP")
				(number "7")
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 3.81)
				(name "AN0/VREF+/CN2/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 3.81)
				(name "AN1/VREF-/CN3/RA1")
				(number "20")
			)
			(pin input line
				(at 33.02 40.64 180)
				(length 3.81)
				(name "OSC1/CLKI/CN30/RA2")
				(number "30")
			)
			(pin input line
				(at 33.02 38.1 180)
				(length 3.81)
				(name "OSC2/CLKO/CN29/RA3")
				(number "31")
			)
			(pin input line
				(at 33.02 35.56 180)
				(length 3.81)
				(name "SOSCO/T1CK/CN0/RA4")
				(number "34")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 3.81)
				(name "TCK/PMA7/RA7")
				(number "13")
			)
			(pin input line
				(at 33.02 30.48 180)
				(length 3.81)
				(name "TDO/PMA8/RA8")
				(number "32")
			)
			(pin input line
				(at 33.02 27.94 180)
				(length 3.81)
				(name "TDI/PMA9/RA9")
				(number "35")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "TMS/PMA10/RA10")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "PGED1/AN2/C2IN-/RP0/CN4/RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "PGEC1/AN3/C2IN+/RP1/CN5/RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "AN4/C1IN-/RP2/CN6/RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "AN5/C1IN+/RP3/CN7/RB3")
				(number "24")
			)
			(pin input line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "SOSCI/RP4/CN1/RB4")
				(number "33")
			)
			(pin input line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "PGED3/ASDA1/RP5/CN27/PMD7/RB5")
				(number "41")
			)
			(pin input line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "PGEC3/ASCL1/RP6/CN24/PMD6/RB6")
				(number "42")
			)
			(pin input line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "INT0/RP7/CN23/PMD5/RB7")
				(number "43")
			)
			(pin input line
				(at 33.02 0 180)
				(length 3.81)
				(name "SCL1/RP8/CN22/PMD4/RB8")
				(number "44")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "SDA1/RP9/CN21/PMD3/RB9")
				(number "1")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "PGED2/EMCD2/RP10/CN16/PMD2/RB10")
				(number "8")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "PGEC2/RP11/CN15/PMD1/RB11")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "AN12/DAC1RP/RP12/CN14/PMD0/RB12")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "AN11/DAC1RN/RP13/CN13/PMRD/RB13")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "AN10/DAC1LP/RTCC/RP14/CN12/PMWR/RB14")
				(number "14")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "AN9/DAC1LN/RP15/CN11/PMCS1/RB15")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 3.81)
				(name "AN6/DAC1RM/RP16/CN8/RC0")
				(number "25")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 3.81)
				(name "AN7/DAC1LM/RP17/CN9/RC1")
				(number "26")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 3.81)
				(name "AN8/CVREF/RP18/PMA2/CN10/RC2")
				(number "27")
			)
			(pin input line
				(at 33.02 -30.48 180)
				(length 3.81)
				(name "RP19/CN28/PMBE/RC3")
				(number "36")
			)
			(pin input line
				(at 33.02 -33.02 180)
				(length 3.81)
				(name "RP20/CN25/PMA4/RC4")
				(number "37")
			)
			(pin input line
				(at 33.02 -35.56 180)
				(length 3.81)
				(name "RP21/CN26/PMA3/RC5")
				(number "38")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 3.81)
				(name "RP22/CN18/PMA1/RC6")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 3.81)
				(name "RP23/CN17/PMA0/RC7")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 3.81)
				(name "RP24/CN20/PMA5/RC8")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 3.81)
				(name "RP25/CN19/PMA6/RC9")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DSPIC33FJ128MC204"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 48.26 0)
		)
		(property "Value" "DSPIC33FJ128MC204"
			(at -29.21 -48.26 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/70291G.pdf"
			(at 0 0 0)
		)
		(property "Description" "40MIPS, 128k Flash, 8k SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit Digital Signal Controller Microchip dsPIC Motor Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN?44*1EP*8x8mm*P0.65mm* TQFP?44*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "DSPIC33FJ128MC204_1_1"
			(pin input line
				(at -33.02 45.72 0)
				(length 3.81)
				(name "~{MCLR}")
				(number "18")
			)
			(pin power_in line
				(at -7.62 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -7.62 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "40")
			)
			(pin power_in line
				(at -5.08 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "39")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 3.81)
				(name "AVDD")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 3.81)
				(name "AVSS")
				(number "16")
			)
			(pin power_in line
				(at 5.08 50.8 270)
				(length 3.81)
				(name "VCAP")
				(number "7")
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 3.81)
				(name "AN0/VREF+/CN2/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 3.81)
				(name "AN1/VREF-/CN3/RA1")
				(number "20")
			)
			(pin input line
				(at 33.02 40.64 180)
				(length 3.81)
				(name "OSC1/CLKI/CN30/RA2")
				(number "30")
			)
			(pin input line
				(at 33.02 38.1 180)
				(length 3.81)
				(name "OSC2/CLKO/CN29/RA3")
				(number "31")
			)
			(pin input line
				(at 33.02 35.56 180)
				(length 3.81)
				(name "SOSCO/T1CK/CN0/RA4")
				(number "34")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 3.81)
				(name "TCK/PMA7/RA7")
				(number "13")
			)
			(pin input line
				(at 33.02 30.48 180)
				(length 3.81)
				(name "TDO/PMA8/RA8")
				(number "32")
			)
			(pin input line
				(at 33.02 27.94 180)
				(length 3.81)
				(name "TDI/PMA9/RA9")
				(number "35")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "TMS/PMA10/RA10")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "PGED1/AN2/C2IN-/RP0/CN4/RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "PGEC1/AN3/C2IN+/RP1/CN5/RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "AN4/C1IN-/RP2/CN6/RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "AN5/C1IN+/RP3/CN7/RB3")
				(number "24")
			)
			(pin input line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "SOSCI/RP4/CN1/RB4")
				(number "33")
			)
			(pin input line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "PGED3/ASDA1/RP5/CN27/PMD7/RB5")
				(number "41")
			)
			(pin input line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "PGEC3/ASCL1/RP6/CN24/PMD6/RB6")
				(number "42")
			)
			(pin input line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "INT0/RP7/CN23/PMD5/RB7")
				(number "43")
			)
			(pin input line
				(at 33.02 0 180)
				(length 3.81)
				(name "SCL1/RP8/CN22/PMD4/RB8")
				(number "44")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "SDA1/RP9/CN21/PMD3/RB9")
				(number "1")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "PGED2/PWM1H3/RP10/CN16/PMD2/RB10")
				(number "8")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "PGEC2/PWM1L3/RP11/CN15/PMD1/RB11")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "PWM1H2/RP12/CN14/PMD0/RB12")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "PWM1L2/RP13/CN13/PMRD/RB13")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "PWM1H1/RTCC/RP14/CN12/PMWR/RB14")
				(number "14")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "PWM1L/RP15/CN11/PMCS1/RB15")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 3.81)
				(name "AN6/RP16/CN8/RC0")
				(number "25")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 3.81)
				(name "AN7/RP17/CN9/RC1")
				(number "26")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 3.81)
				(name "AN8/CVREF/RP18/PMA2/CN10/RC2")
				(number "27")
			)
			(pin input line
				(at 33.02 -30.48 180)
				(length 3.81)
				(name "RP19/CN28/PMBE/RC3")
				(number "36")
			)
			(pin input line
				(at 33.02 -33.02 180)
				(length 3.81)
				(name "RP20/CN25/PMA4/RC4")
				(number "37")
			)
			(pin input line
				(at 33.02 -35.56 180)
				(length 3.81)
				(name "RP21/CN26/PMA3/RC5")
				(number "38")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 3.81)
				(name "PWM2H1/RP22/CN18/PMA1/RC6")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 3.81)
				(name "PWM2L1/RP23/CN17/PMA0/RC7")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 3.81)
				(name "RP24/CN20/PMA5/RC8")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 3.81)
				(name "RP25/CN19/PMA6/RC9")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DSPIC33FJ128MC804"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 48.26 0)
		)
		(property "Value" "DSPIC33FJ128MC804"
			(at -29.21 -48.26 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/70291G.pdf"
			(at 0 0 0)
		)
		(property "Description" "40MIPS, 128k Flash, 16k SRAM, ECAN, 16-bit DAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit Digital Signal Controller Microchip dsPIC Motor Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN?44*1EP*8x8mm*P0.65mm* TQFP?44*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "DSPIC33FJ128MC804_1_1"
			(pin input line
				(at -33.02 45.72 0)
				(length 3.81)
				(name "~{MCLR}")
				(number "18")
			)
			(pin power_in line
				(at -7.62 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -7.62 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "40")
			)
			(pin power_in line
				(at -5.08 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "39")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 3.81)
				(name "AVDD")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 3.81)
				(name "AVSS")
				(number "16")
			)
			(pin power_in line
				(at 5.08 50.8 270)
				(length 3.81)
				(name "VCAP")
				(number "7")
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 3.81)
				(name "AN0/VREF+/CN2/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 3.81)
				(name "AN1/VREF-/CN3/RA1")
				(number "20")
			)
			(pin input line
				(at 33.02 40.64 180)
				(length 3.81)
				(name "OSC1/CLKI/CN30/RA2")
				(number "30")
			)
			(pin input line
				(at 33.02 38.1 180)
				(length 3.81)
				(name "OSC2/CLKO/CN29/RA3")
				(number "31")
			)
			(pin input line
				(at 33.02 35.56 180)
				(length 3.81)
				(name "SOSCO/T1CK/CN0/RA4")
				(number "34")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 3.81)
				(name "TCK/PMA7/RA7")
				(number "13")
			)
			(pin input line
				(at 33.02 30.48 180)
				(length 3.81)
				(name "TDO/PMA8/RA8")
				(number "32")
			)
			(pin input line
				(at 33.02 27.94 180)
				(length 3.81)
				(name "TDI/PMA9/RA9")
				(number "35")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "TMS/PMA10/RA10")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "PGED1/AN2/C2IN-/RP0/CN4/RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "PGEC1/AN3/C2IN+/RP1/CN5/RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "AN4/C1IN-/RP2/CN6/RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "AN5/C1IN+/RP3/CN7/RB3")
				(number "24")
			)
			(pin input line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "SOSCI/RP4/CN1/RB4")
				(number "33")
			)
			(pin input line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "PGED3/ASDA1/RP5/CN27/PMD7/RB5")
				(number "41")
			)
			(pin input line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "PGEC3/ASCL1/RP6/CN24/PMD6/RB6")
				(number "42")
			)
			(pin input line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "INT0/RP7/CN23/PMD5/RB7")
				(number "43")
			)
			(pin input line
				(at 33.02 0 180)
				(length 3.81)
				(name "SCL1/RP8/CN22/PMD4/RB8")
				(number "44")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "SDA1/RP9/CN21/PMD3/RB9")
				(number "1")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "PGED2/PWM1H3/RP10/CN16/PMD2/RB10")
				(number "8")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "PGEC2/PWM1L3/RP11/CN15/PMD1/RB11")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "PWM1H2/DAC1RP/RP12/CN14/PMD0/RB12")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "PWM1L2/DAC1RN/RP13/CN13/PMRD/RB13")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "PWM1H1/DAC1LP/RTCC/RP14/CN12/PMWR/RB14")
				(number "14")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "PWM1L/DAC1LN/RP15/CN11/PMCS1/RB15")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 3.81)
				(name "AN6/DAC1RM/RP16/CN8/RC0")
				(number "25")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 3.81)
				(name "AN7/DAC1LM/RP17/CN9/RC1")
				(number "26")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 3.81)
				(name "AN8/CVREF/RP18/PMA2/CN10/RC2")
				(number "27")
			)
			(pin input line
				(at 33.02 -30.48 180)
				(length 3.81)
				(name "RP19/CN28/PMBE/RC3")
				(number "36")
			)
			(pin input line
				(at 33.02 -33.02 180)
				(length 3.81)
				(name "RP20/CN25/PMA4/RC4")
				(number "37")
			)
			(pin input line
				(at 33.02 -35.56 180)
				(length 3.81)
				(name "RP21/CN26/PMA3/RC5")
				(number "38")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 3.81)
				(name "PWM2H1/RP22/CN18/PMA1/RC6")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 3.81)
				(name "PWM2L1/RP23/CN17/PMA0/RC7")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 3.81)
				(name "RP24/CN20/PMA5/RC8")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 3.81)
				(name "RP25/CN19/PMA6/RC9")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DSPIC33FJ256MC710A"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 21.59 69.85 0)
		)
		(property "Value" "DSPIC33FJ256MC710A"
			(at 0 7.62 90)
		)
		(property "Footprint" ""
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/70594C.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "High-Performance, 16-bit Digital Signal Controller, 40MIPS, 256k Flash, 30k SRAM, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit Digital Signal Controller Microchip dsPIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*12x12mm*P0.4mm* TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "DSPIC33FJ256MC710A_0_1")
		(symbol "DSPIC33FJ256MC710A_1_1"
			(pin input line
				(at -27.94 63.5 0)
				(length 2.54)
				(name "~{MCLR}")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 2.54)
				(name "TMS/RA0")
				(number "17")
			)
			(pin bidirectional line
				(at -27.94 48.26 0)
				(length 2.54)
				(name "TCK/RA1")
				(number "38")
			)
			(pin bidirectional line
				(at -27.94 45.72 0)
				(length 2.54)
				(name "SCL2/RA2")
				(number "58")
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 2.54)
				(name "SDA2/RA3")
				(number "59")
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 2.54)
				(name "TDI/RA4")
				(number "60")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 2.54)
				(name "TDO/RA5")
				(number "61")
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "AN22/CN22/RA6")
				(number "91")
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "AN23/CN23/RA7")
				(number "92")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "VREF-/RA9")
				(number "28")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 2.54)
				(name "VREF+/RA10")
				(number "29")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "INT3/RA14")
				(number "66")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "INT4/RA15")
				(number "67")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "PGED3/AN0/CN2/RB0")
				(number "25")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "PGEC3/AN1/CN3/RB1")
				(number "24")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "AN2/~{SS1}/CN4/RB2")
				(number "23")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "AN3/INDX/CN5/RB3")
				(number "22")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "AN4/QEA/CN6/RB4")
				(number "21")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "AN5/QEB/CN7/RB5")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PGEC1/AN6/OCFA/RB6")
				(number "26")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 2.54)
				(name "PGED1/AN7/RB7")
				(number "27")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "AN8/RB8")
				(number "32")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "AN9/RB9")
				(number "33")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "AN10/RB10")
				(number "34")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "AN11/RB11")
				(number "35")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "AN12/RB12")
				(number "41")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "AN13/RB13")
				(number "42")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "AN14/RB14")
				(number "43")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "AN15/OCFB/CN12/RB15")
				(number "44")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "AN16/T2CK/T7CK/RC1")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 2.54)
				(name "AN17/T3CK/T6CK/RC2")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 2.54)
				(name "AN18/T4CK/T9CK/RC3")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "AN19/T5CK/T8CK/RC4")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 2.54)
				(name "OSC1/CLKIN/RC12")
				(number "63")
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 2.54)
				(name "PGED2/SOSCI/CN1/RC13")
				(number "73")
			)
			(pin bidirectional line
				(at -27.94 -40.64 0)
				(length 2.54)
				(name "PGEC2/SOSCO/T1CK/CN0/RC14")
				(number "74")
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 2.54)
				(name "OSC2/CLKO/RC15")
				(number "64")
			)
			(pin passive line
				(at -15.24 71.12 270)
				(length 2.54)
				(name "VCAP")
				(number "85")
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "37")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "36")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "45")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "65")
			)
			(pin power_in line
				(at -2.54 -68.58 90)
				(length 2.54)
				(name "VSS")
				(number "75")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "46")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at 2.54 -68.58 90)
				(length 2.54)
				(name "AVSS")
				(number "31")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "86")
			)
			(pin power_in line
				(at 12.7 71.12 270)
				(length 2.54)
				(name "AVDD")
				(number "30")
			)
			(pin bidirectional line
				(at 27.94 66.04 180)
				(length 2.54)
				(name "OC1/RD0")
				(number "72")
			)
			(pin bidirectional line
				(at 27.94 63.5 180)
				(length 2.54)
				(name "OC2/RD1")
				(number "76")
			)
			(pin bidirectional line
				(at 27.94 60.96 180)
				(length 2.54)
				(name "OC3/RD2")
				(number "77")
			)
			(pin bidirectional line
				(at 27.94 58.42 180)
				(length 2.54)
				(name "OC4/RD3")
				(number "78")
			)
			(pin bidirectional line
				(at 27.94 55.88 180)
				(length 2.54)
				(name "OC5/CN13/RD4")
				(number "81")
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 2.54)
				(name "OC6/CN14/RD5")
				(number "82")
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 2.54)
				(name "OC7/CN15/RD6")
				(number "83")
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 2.54)
				(name "OC8/UPDN/CN16/RD7")
				(number "84")
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 2.54)
				(name "IC1/RD8")
				(number "68")
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 2.54)
				(name "IC2/RD9")
				(number "69")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 2.54)
				(name "IC3/RD10")
				(number "70")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "IC4/RD11")
				(number "71")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "IC5/RD12")
				(number "79")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "IC6/CN19/RD13")
				(number "80")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "IC7/~{U1CTS}/CN20/RD14")
				(number "47")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "IC8/~{U1RTS}/CN21/RD15")
				(number "48")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "PWM1L/RE0")
				(number "93")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "PWM1H/RE1")
				(number "94")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PWM2L/RE2")
				(number "98")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "PWM2H/RE3")
				(number "99")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PWM3L/RE4")
				(number "100")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PWM3H/RE5")
				(number "3")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PWM4L/RE6")
				(number "4")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PWM4H/RE7")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "AN20/~{FLTA}/INT1/RE8")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "AN21/~{FLTB}/INT2/RE9")
				(number "19")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "C1RX/RF0")
				(number "87")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "C1TX/RF1")
				(number "88")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "U1RX/RF2")
				(number "52")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "U1TX/RF3")
				(number "51")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "U2RX/CN17/RF4")
				(number "49")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "U2TX/CN18/RF5")
				(number "50")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "SCK1/INT0/RF6")
				(number "55")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "SDI1/RF7")
				(number "54")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "SDO1/RF8")
				(number "53")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "~{U2CTS}/RF12")
				(number "40")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "~{U2RTS}/RF13")
				(number "39")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 2.54)
				(name "C2RX/RG0")
				(number "90")
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 2.54)
				(name "C2TX/RG1")
				(number "89")
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 2.54)
				(name "SCL1/RG2")
				(number "57")
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 2.54)
				(name "SDA1/RG3")
				(number "56")
			)
			(pin bidirectional line
				(at 27.94 -45.72 180)
				(length 2.54)
				(name "SCK2/CN8/RG6")
				(number "10")
			)
			(pin bidirectional line
				(at 27.94 -48.26 180)
				(length 2.54)
				(name "SDI2/CN9/RG7")
				(number "11")
			)
			(pin bidirectional line
				(at 27.94 -50.8 180)
				(length 2.54)
				(name "SDO2/CN10/RG8")
				(number "12")
			)
			(pin bidirectional line
				(at 27.94 -53.34 180)
				(length 2.54)
				(name "~{SS2}/CN11/RG9")
				(number "14")
			)
			(pin bidirectional line
				(at 27.94 -55.88 180)
				(length 2.54)
				(name "RG12")
				(number "96")
			)
			(pin bidirectional line
				(at 27.94 -58.42 180)
				(length 2.54)
				(name "RG13")
				(number "97")
			)
			(pin bidirectional line
				(at 27.94 -60.96 180)
				(length 2.54)
				(name "RG14")
				(number "95")
			)
			(pin bidirectional line
				(at 27.94 -63.5 180)
				(length 2.54)
				(name "RG15")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DSPIC33FJ32GP304"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 48.26 0)
		)
		(property "Value" "DSPIC33FJ32GP304"
			(at -29.21 -48.26 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/70292G.pdf"
			(at 0 0 0)
		)
		(property "Description" "40MIPS, 32k Flash, 4k SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit Digital Signal Controller Microchip dsPIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN?44*1EP*8x8mm*P0.65mm* TQFP?44*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "DSPIC33FJ32GP304_1_1"
			(pin input line
				(at -33.02 45.72 0)
				(length 3.81)
				(name "~{MCLR}")
				(number "18")
			)
			(pin power_in line
				(at -7.62 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -7.62 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "40")
			)
			(pin power_in line
				(at -5.08 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "39")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 3.81)
				(name "AVDD")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 3.81)
				(name "AVSS")
				(number "16")
			)
			(pin power_in line
				(at 5.08 50.8 270)
				(length 3.81)
				(name "VCAP")
				(number "7")
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 3.81)
				(name "AN0/VREF+/CN2/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 3.81)
				(name "AN1/VREF-/CN3/RA1")
				(number "20")
			)
			(pin input line
				(at 33.02 40.64 180)
				(length 3.81)
				(name "OSC1/CLKI/CN30/RA2")
				(number "30")
			)
			(pin input line
				(at 33.02 38.1 180)
				(length 3.81)
				(name "OSC2/CLKO/CN29/RA3")
				(number "31")
			)
			(pin input line
				(at 33.02 35.56 180)
				(length 3.81)
				(name "SOSCO/T1CK/CN0/RA4")
				(number "34")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 3.81)
				(name "TCK/PMA7/RA7")
				(number "13")
			)
			(pin input line
				(at 33.02 30.48 180)
				(length 3.81)
				(name "TDO/PMA8/RA8")
				(number "32")
			)
			(pin input line
				(at 33.02 27.94 180)
				(length 3.81)
				(name "TDI/PMA9/RA9")
				(number "35")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "TMS/PMA10/RA10")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "PGED1/AN2/C2IN-/RP0/CN4/RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "PGEC1/AN3/C2IN+/RP1/CN5/RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "AN4/C1IN-/RP2/CN6/RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "AN5/C1IN+/RP3/CN7/RB3")
				(number "24")
			)
			(pin input line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "SOSCI/RP4/CN1/RB4")
				(number "33")
			)
			(pin input line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "PGED3/ASDA1/RP5/CN27/PMD7/RB5")
				(number "41")
			)
			(pin input line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "PGEC3/ASCL1/RP6/CN24/PMD6/RB6")
				(number "42")
			)
			(pin input line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "INT0/RP7/CN23/PMD5/RB7")
				(number "43")
			)
			(pin input line
				(at 33.02 0 180)
				(length 3.81)
				(name "SCL1/RP8/CN22/PMD4/RB8")
				(number "44")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "SDA1/RP9/CN21/PMD3/RB9")
				(number "1")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "PGED2/EMCD2/RP10/CN16/PMD2/RB10")
				(number "8")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "PGEC2/RP11/CN15/PMD1/RB11")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "AN12/RP12/CN14/PMD0/RB12")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "AN11/RP13/CN13/PMRD/RB13")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "AN10/RTCC/RP14/CN12/PMWR/RB14")
				(number "14")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "AN9/RP15/CN11/PMCS1/RB15")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 3.81)
				(name "AN6/RP16/CN8/RC0")
				(number "25")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 3.81)
				(name "AN7/RP17/CN9/RC1")
				(number "26")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 3.81)
				(name "AN8/CVREF/RP18/PMA2/CN10/RC2")
				(number "27")
			)
			(pin input line
				(at 33.02 -30.48 180)
				(length 3.81)
				(name "RP19/CN28/PMBE/RC3")
				(number "36")
			)
			(pin input line
				(at 33.02 -33.02 180)
				(length 3.81)
				(name "RP20/CN25/PMA4/RC4")
				(number "37")
			)
			(pin input line
				(at 33.02 -35.56 180)
				(length 3.81)
				(name "RP21/CN26/PMA3/RC5")
				(number "38")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 3.81)
				(name "RP22/CN18/PMA1/RC6")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 3.81)
				(name "RP23/CN17/PMA0/RC7")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 3.81)
				(name "RP24/CN20/PMA5/RC8")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 3.81)
				(name "RP25/CN19/PMA6/RC9")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DSPIC33FJ32MC304"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 48.26 0)
		)
		(property "Value" "DSPIC33FJ32MC304"
			(at -29.21 -48.26 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/70291G.pdf"
			(at 0 0 0)
		)
		(property "Description" "40MIPS, 32k Flash, 8k SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit Digital Signal Controller Microchip dsPIC Motor Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN?44*1EP*8x8mm*P0.65mm* TQFP?44*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "DSPIC33FJ32MC304_1_1"
			(pin input line
				(at -33.02 45.72 0)
				(length 3.81)
				(name "~{MCLR}")
				(number "18")
			)
			(pin power_in line
				(at -7.62 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -7.62 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "40")
			)
			(pin power_in line
				(at -5.08 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "39")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 3.81)
				(name "AVDD")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 3.81)
				(name "AVSS")
				(number "16")
			)
			(pin power_in line
				(at 5.08 50.8 270)
				(length 3.81)
				(name "VCAP")
				(number "7")
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 3.81)
				(name "AN0/VREF+/CN2/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 3.81)
				(name "AN1/VREF-/CN3/RA1")
				(number "20")
			)
			(pin input line
				(at 33.02 40.64 180)
				(length 3.81)
				(name "OSC1/CLKI/CN30/RA2")
				(number "30")
			)
			(pin input line
				(at 33.02 38.1 180)
				(length 3.81)
				(name "OSC2/CLKO/CN29/RA3")
				(number "31")
			)
			(pin input line
				(at 33.02 35.56 180)
				(length 3.81)
				(name "SOSCO/T1CK/CN0/RA4")
				(number "34")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 3.81)
				(name "TCK/PMA7/RA7")
				(number "13")
			)
			(pin input line
				(at 33.02 30.48 180)
				(length 3.81)
				(name "TDO/PMA8/RA8")
				(number "32")
			)
			(pin input line
				(at 33.02 27.94 180)
				(length 3.81)
				(name "TDI/PMA9/RA9")
				(number "35")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "TMS/PMA10/RA10")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "PGED1/AN2/C2IN-/RP0/CN4/RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "PGEC1/AN3/C2IN+/RP1/CN5/RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "AN4/C1IN-/RP2/CN6/RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "AN5/C1IN+/RP3/CN7/RB3")
				(number "24")
			)
			(pin input line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "SOSCI/RP4/CN1/RB4")
				(number "33")
			)
			(pin input line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "PGED3/ASDA1/RP5/CN27/PMD7/RB5")
				(number "41")
			)
			(pin input line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "PGEC3/ASCL1/RP6/CN24/PMD6/RB6")
				(number "42")
			)
			(pin input line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "INT0/RP7/CN23/PMD5/RB7")
				(number "43")
			)
			(pin input line
				(at 33.02 0 180)
				(length 3.81)
				(name "SCL1/RP8/CN22/PMD4/RB8")
				(number "44")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "SDA1/RP9/CN21/PMD3/RB9")
				(number "1")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "PGED2/PWM1H3/RP10/CN16/PMD2/RB10")
				(number "8")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "PGEC2/PWM1L3/RP11/CN15/PMD1/RB11")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "PWM1H2/RP12/CN14/PMD0/RB12")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "PWM1L2/RP13/CN13/PMRD/RB13")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "PWM1H1/RTCC/RP14/CN12/PMWR/RB14")
				(number "14")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "PWM1L/RP15/CN11/PMCS1/RB15")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 3.81)
				(name "AN6/RP16/CN8/RC0")
				(number "25")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 3.81)
				(name "AN7/RP17/CN9/RC1")
				(number "26")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 3.81)
				(name "AN8/CVREF/RP18/PMA2/CN10/RC2")
				(number "27")
			)
			(pin input line
				(at 33.02 -30.48 180)
				(length 3.81)
				(name "RP19/CN28/PMBE/RC3")
				(number "36")
			)
			(pin input line
				(at 33.02 -33.02 180)
				(length 3.81)
				(name "RP20/CN25/PMA4/RC4")
				(number "37")
			)
			(pin input line
				(at 33.02 -35.56 180)
				(length 3.81)
				(name "RP21/CN26/PMA3/RC5")
				(number "38")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 3.81)
				(name "PWM2H1/RP22/CN18/PMA1/RC6")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 3.81)
				(name "PWM2L1/RP23/CN17/PMA0/RC7")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 3.81)
				(name "RP24/CN20/PMA5/RC8")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 3.81)
				(name "RP25/CN19/PMA6/RC9")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DSPIC33FJ64GP204"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 48.26 0)
		)
		(property "Value" "DSPIC33FJ64GP204"
			(at -29.21 -48.26 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/70292G.pdf"
			(at 0 0 0)
		)
		(property "Description" "40MIPS, 64k Flash, 8k SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit Digital Signal Controller Microchip dsPIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN?44*1EP*8x8mm*P0.65mm* TQFP?44*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "DSPIC33FJ64GP204_1_1"
			(pin input line
				(at -33.02 45.72 0)
				(length 3.81)
				(name "~{MCLR}")
				(number "18")
			)
			(pin power_in line
				(at -7.62 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -7.62 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "40")
			)
			(pin power_in line
				(at -5.08 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "39")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 3.81)
				(name "AVDD")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 3.81)
				(name "AVSS")
				(number "16")
			)
			(pin power_in line
				(at 5.08 50.8 270)
				(length 3.81)
				(name "VCAP")
				(number "7")
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 3.81)
				(name "AN0/VREF+/CN2/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 3.81)
				(name "AN1/VREF-/CN3/RA1")
				(number "20")
			)
			(pin input line
				(at 33.02 40.64 180)
				(length 3.81)
				(name "OSC1/CLKI/CN30/RA2")
				(number "30")
			)
			(pin input line
				(at 33.02 38.1 180)
				(length 3.81)
				(name "OSC2/CLKO/CN29/RA3")
				(number "31")
			)
			(pin input line
				(at 33.02 35.56 180)
				(length 3.81)
				(name "SOSCO/T1CK/CN0/RA4")
				(number "34")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 3.81)
				(name "TCK/PMA7/RA7")
				(number "13")
			)
			(pin input line
				(at 33.02 30.48 180)
				(length 3.81)
				(name "TDO/PMA8/RA8")
				(number "32")
			)
			(pin input line
				(at 33.02 27.94 180)
				(length 3.81)
				(name "TDI/PMA9/RA9")
				(number "35")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "TMS/PMA10/RA10")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "PGED1/AN2/C2IN-/RP0/CN4/RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "PGEC1/AN3/C2IN+/RP1/CN5/RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "AN4/C1IN-/RP2/CN6/RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "AN5/C1IN+/RP3/CN7/RB3")
				(number "24")
			)
			(pin input line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "SOSCI/RP4/CN1/RB4")
				(number "33")
			)
			(pin input line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "PGED3/ASDA1/RP5/CN27/PMD7/RB5")
				(number "41")
			)
			(pin input line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "PGEC3/ASCL1/RP6/CN24/PMD6/RB6")
				(number "42")
			)
			(pin input line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "INT0/RP7/CN23/PMD5/RB7")
				(number "43")
			)
			(pin input line
				(at 33.02 0 180)
				(length 3.81)
				(name "SCL1/RP8/CN22/PMD4/RB8")
				(number "44")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "SDA1/RP9/CN21/PMD3/RB9")
				(number "1")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "PGED2/EMCD2/RP10/CN16/PMD2/RB10")
				(number "8")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "PGEC2/RP11/CN15/PMD1/RB11")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "AN12/RP12/CN14/PMD0/RB12")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "AN11/RP13/CN13/PMRD/RB13")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "AN10/RTCC/RP14/CN12/PMWR/RB14")
				(number "14")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "AN9/RP15/CN11/PMCS1/RB15")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 3.81)
				(name "AN6/RP16/CN8/RC0")
				(number "25")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 3.81)
				(name "AN7/RP17/CN9/RC1")
				(number "26")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 3.81)
				(name "AN8/CVREF/RP18/PMA2/CN10/RC2")
				(number "27")
			)
			(pin input line
				(at 33.02 -30.48 180)
				(length 3.81)
				(name "RP19/CN28/PMBE/RC3")
				(number "36")
			)
			(pin input line
				(at 33.02 -33.02 180)
				(length 3.81)
				(name "RP20/CN25/PMA4/RC4")
				(number "37")
			)
			(pin input line
				(at 33.02 -35.56 180)
				(length 3.81)
				(name "RP21/CN26/PMA3/RC5")
				(number "38")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 3.81)
				(name "RP22/CN18/PMA1/RC6")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 3.81)
				(name "RP23/CN17/PMA0/RC7")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 3.81)
				(name "RP24/CN20/PMA5/RC8")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 3.81)
				(name "RP25/CN19/PMA6/RC9")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DSPIC33FJ64GP306A-IMR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -34.29 43.18 0)
		)
		(property "Value" "DSPIC33FJ64GP306A-IMR"
			(at -34.29 -43.18 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/70593d.pdf"
			(at 0 0 0)
		)
		(property "Description" "40MIPS, 64k Flash, 16k SRAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit Digital Signal Controller Microchip dsPIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "DSPIC33FJ64GP306A-IMR_1_1"
			(pin input line
				(at -38.1 40.64 0)
				(length 3.81)
				(name "~{MCLR}")
				(number "7")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 3.81)
				(name "PGED3/AN0/Vref+/CN2/RB0")
				(number "16")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 3.81)
				(name "PGEC3/AN1/Vref-/CN3/RB1")
				(number "15")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 3.81)
				(name "AN2/~{SS1}/CN4/RB2")
				(number "14")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 3.81)
				(name "AN3/CN5/RB3")
				(number "13")
			)
			(pin input line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "AN4/IC7/CN6/RB4")
				(number "12")
			)
			(pin input line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "AN5/IC8/CN7/RB5")
				(number "11")
			)
			(pin input line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "PGEC1/AN6/OCFA/RB6")
				(number "17")
			)
			(pin input line
				(at -38.1 0 0)
				(length 3.81)
				(name "PGED1/AN7/RB7")
				(number "18")
			)
			(pin input line
				(at -38.1 -2.54 0)
				(length 3.81)
				(name "~{U2CTS}/AN8/RB8")
				(number "21")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "AN9/RB9")
				(number "22")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 3.81)
				(name "TMS/AN10/RB10")
				(number "23")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 3.81)
				(name "TDO/AN11/RB11")
				(number "24")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 3.81)
				(name "TCK/AN12/RB12")
				(number "27")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 3.81)
				(name "TDI/AN13/RB13")
				(number "28")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 3.81)
				(name "~{U2RTS}/AN14/RB14")
				(number "29")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 3.81)
				(name "AN15/OCFB/CN12/RB15")
				(number "30")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 3.81)
				(name "AN16/T2CK/T7CK/RC1")
				(number "2")
			)
			(pin bidirectional line
				(at -38.1 -27.94 0)
				(length 3.81)
				(name "AN17/T3CK/T6CK/RC2")
				(number "3")
			)
			(pin bidirectional line
				(at -38.1 -30.48 0)
				(length 3.81)
				(name "OSC1/CLKIN/RC12")
				(number "39")
			)
			(pin bidirectional line
				(at -38.1 -33.02 0)
				(length 3.81)
				(name "PGED2/SOSCI/T4CK/CN1/RC13")
				(number "47")
			)
			(pin bidirectional line
				(at -38.1 -35.56 0)
				(length 3.81)
				(name "PGEC2/SOSCO/T1CK/CN0/RC14")
				(number "48")
			)
			(pin bidirectional line
				(at -38.1 -38.1 0)
				(length 3.81)
				(name "OSC2/CLKO/RC15")
				(number "40")
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 3.81)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at -7.62 -45.72 90)
				(length 3.81)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 3.81)
				(name "VDD")
				(number "26")
			)
			(pin power_in line
				(at -5.08 -45.72 90)
				(length 3.81)
				(name "VSS")
				(number "25")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 3.81)
				(name "VDD")
				(number "38")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 3.81)
				(name "VSS")
				(number "41")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 3.81)
				(name "VDD")
				(number "57")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 3.81)
				(name "AVSS")
				(number "20")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 3.81)
				(name "AVDD")
				(number "19")
			)
			(pin power_in line
				(at 7.62 -45.72 90)
				(length 3.81)
				(name "EP")
				(number "65")
			)
			(pin power_in line
				(at 10.16 45.72 270)
				(length 3.81)
				(name "VCAP")
				(number "56")
			)
			(pin bidirectional line
				(at 38.1 40.64 180)
				(length 3.81)
				(name "OC1/RD0")
				(number "46")
			)
			(pin bidirectional line
				(at 38.1 38.1 180)
				(length 3.81)
				(name "OC2/RD1")
				(number "49")
			)
			(pin bidirectional line
				(at 38.1 35.56 180)
				(length 3.81)
				(name "OC3/RD2")
				(number "50")
			)
			(pin bidirectional line
				(at 38.1 33.02 180)
				(length 3.81)
				(name "OC4/RD3")
				(number "51")
			)
			(pin bidirectional line
				(at 38.1 30.48 180)
				(length 3.81)
				(name "OC5/IC5/CN13/RD4")
				(number "52")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 3.81)
				(name "OC6/IC6/CN14/RD5")
				(number "53")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 3.81)
				(name "OC7/CN15/RD6")
				(number "54")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 3.81)
				(name "OC8/CN16/RD7")
				(number "55")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 3.81)
				(name "IC1/INT1/RD8")
				(number "42")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 3.81)
				(name "IC2/~{U1CTS}/INT2/RD9")
				(number "43")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 3.81)
				(name "IC3/INT3/RD10")
				(number "44")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 3.81)
				(name "IC4/INT4/RD11")
				(number "45")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "RF0")
				(number "58")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "RF1")
				(number "59")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "U1RX/SDI1/RF2")
				(number "34")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "U1TX/SDO1/RF3")
				(number "33")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 3.81)
				(name "U2RX/SDA2/CN17/RF4")
				(number "31")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "U2TX/SCL2/CN18/RF5")
				(number "32")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 3.81)
				(name "~{U1RTS}/SCK1/INT0/RF6")
				(number "35")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 3.81)
				(name "RG0")
				(number "61")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 3.81)
				(name "RG1")
				(number "60")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 3.81)
				(name "SCL1/RG2")
				(number "37")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 3.81)
				(name "SDA1/RG3")
				(number "36")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 3.81)
				(name "SCK2/CN8/RG6")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 3.81)
				(name "SDI2/CN9/RG7")
				(number "5")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 3.81)
				(name "SDO2/CN10/RG8")
				(number "6")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 3.81)
				(name "~{SS2}/CN11/RG9")
				(number "8")
			)
			(pin bidirectional line
				(at 38.1 -33.02 180)
				(length 3.81)
				(name "CSDI/RG12")
				(number "63")
			)
			(pin bidirectional line
				(at 38.1 -35.56 180)
				(length 3.81)
				(name "CSDO/RG13")
				(number "64")
			)
			(pin bidirectional line
				(at 38.1 -38.1 180)
				(length 3.81)
				(name "CSCK/RG14")
				(number "62")
			)
			(pin bidirectional line
				(at 38.1 -40.64 180)
				(length 3.81)
				(name "COFS/RG15")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DSPIC33FJ64GP804"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 48.26 0)
		)
		(property "Value" "DSPIC33FJ64GP804"
			(at -29.21 -48.26 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/70292G.pdf"
			(at 0 0 0)
		)
		(property "Description" "40MIPS, 64k Flash, 16k SRAM, ECAN, Audio DAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit Digital Signal Controller Microchip dsPIC33"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN?44*1EP*8x8mm*P0.65mm* TQFP?44*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "DSPIC33FJ64GP804_1_1"
			(pin input line
				(at -33.02 45.72 0)
				(length 3.81)
				(name "~{MCLR}")
				(number "18")
			)
			(pin power_in line
				(at -7.62 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -7.62 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "40")
			)
			(pin power_in line
				(at -5.08 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "39")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 3.81)
				(name "AVDD")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 3.81)
				(name "AVSS")
				(number "16")
			)
			(pin power_in line
				(at 5.08 50.8 270)
				(length 3.81)
				(name "VCAP")
				(number "7")
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 3.81)
				(name "AN0/VREF+/CN2/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 3.81)
				(name "AN1/VREF-/CN3/RA1")
				(number "20")
			)
			(pin input line
				(at 33.02 40.64 180)
				(length 3.81)
				(name "OSC1/CLKI/CN30/RA2")
				(number "30")
			)
			(pin input line
				(at 33.02 38.1 180)
				(length 3.81)
				(name "OSC2/CLKO/CN29/RA3")
				(number "31")
			)
			(pin input line
				(at 33.02 35.56 180)
				(length 3.81)
				(name "SOSCO/T1CK/CN0/RA4")
				(number "34")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 3.81)
				(name "TCK/PMA7/RA7")
				(number "13")
			)
			(pin input line
				(at 33.02 30.48 180)
				(length 3.81)
				(name "TDO/PMA8/RA8")
				(number "32")
			)
			(pin input line
				(at 33.02 27.94 180)
				(length 3.81)
				(name "TDI/PMA9/RA9")
				(number "35")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "TMS/PMA10/RA10")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "PGED1/AN2/C2IN-/RP0/CN4/RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "PGEC1/AN3/C2IN+/RP1/CN5/RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "AN4/C1IN-/RP2/CN6/RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "AN5/C1IN+/RP3/CN7/RB3")
				(number "24")
			)
			(pin input line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "SOSCI/RP4/CN1/RB4")
				(number "33")
			)
			(pin input line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "PGED3/ASDA1/RP5/CN27/PMD7/RB5")
				(number "41")
			)
			(pin input line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "PGEC3/ASCL1/RP6/CN24/PMD6/RB6")
				(number "42")
			)
			(pin input line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "INT0/RP7/CN23/PMD5/RB7")
				(number "43")
			)
			(pin input line
				(at 33.02 0 180)
				(length 3.81)
				(name "SCL1/RP8/CN22/PMD4/RB8")
				(number "44")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "SDA1/RP9/CN21/PMD3/RB9")
				(number "1")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "PGED2/EMCD2/RP10/CN16/PMD2/RB10")
				(number "8")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "PGEC2/RP11/CN15/PMD1/RB11")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "AN12/DAC1RP/RP12/CN14/PMD0/RB12")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "AN11/DAC1RN/RP13/CN13/PMRD/RB13")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "AN10/DAC1LP/RTCC/RP14/CN12/PMWR/RB14")
				(number "14")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "AN9/DAC1LN/RP15/CN11/PMCS1/RB15")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 3.81)
				(name "AN6/DAC1RM/RP16/CN8/RC0")
				(number "25")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 3.81)
				(name "AN7/DAC1LM/RP17/CN9/RC1")
				(number "26")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 3.81)
				(name "AN8/CVREF/RP18/PMA2/CN10/RC2")
				(number "27")
			)
			(pin input line
				(at 33.02 -30.48 180)
				(length 3.81)
				(name "RP19/CN28/PMBE/RC3")
				(number "36")
			)
			(pin input line
				(at 33.02 -33.02 180)
				(length 3.81)
				(name "RP20/CN25/PMA4/RC4")
				(number "37")
			)
			(pin input line
				(at 33.02 -35.56 180)
				(length 3.81)
				(name "RP21/CN26/PMA3/RC5")
				(number "38")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 3.81)
				(name "RP22/CN18/PMA1/RC6")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 3.81)
				(name "RP23/CN17/PMA0/RC7")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 3.81)
				(name "RP24/CN20/PMA5/RC8")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 3.81)
				(name "RP25/CN19/PMA6/RC9")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DSPIC33FJ64MC204"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 48.26 0)
		)
		(property "Value" "DSPIC33FJ64MC204"
			(at -29.21 -48.26 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/70291G.pdf"
			(at 0 0 0)
		)
		(property "Description" "40MIPS, 64k Flash, 8k SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit Digital Signal Controller Microchip dsPIC Motor Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN?44*1EP*8x8mm*P0.65mm* TQFP?44*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "DSPIC33FJ64MC204_1_1"
			(pin input line
				(at -33.02 45.72 0)
				(length 3.81)
				(name "~{MCLR}")
				(number "18")
			)
			(pin power_in line
				(at -7.62 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -7.62 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "40")
			)
			(pin power_in line
				(at -5.08 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "39")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 3.81)
				(name "AVDD")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 3.81)
				(name "AVSS")
				(number "16")
			)
			(pin power_in line
				(at 5.08 50.8 270)
				(length 3.81)
				(name "VCAP")
				(number "7")
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 3.81)
				(name "AN0/VREF+/CN2/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 3.81)
				(name "AN1/VREF-/CN3/RA1")
				(number "20")
			)
			(pin input line
				(at 33.02 40.64 180)
				(length 3.81)
				(name "OSC1/CLKI/CN30/RA2")
				(number "30")
			)
			(pin input line
				(at 33.02 38.1 180)
				(length 3.81)
				(name "OSC2/CLKO/CN29/RA3")
				(number "31")
			)
			(pin input line
				(at 33.02 35.56 180)
				(length 3.81)
				(name "SOSCO/T1CK/CN0/RA4")
				(number "34")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 3.81)
				(name "TCK/PMA7/RA7")
				(number "13")
			)
			(pin input line
				(at 33.02 30.48 180)
				(length 3.81)
				(name "TDO/PMA8/RA8")
				(number "32")
			)
			(pin input line
				(at 33.02 27.94 180)
				(length 3.81)
				(name "TDI/PMA9/RA9")
				(number "35")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "TMS/PMA10/RA10")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "PGED1/AN2/C2IN-/RP0/CN4/RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "PGEC1/AN3/C2IN+/RP1/CN5/RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "AN4/C1IN-/RP2/CN6/RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "AN5/C1IN+/RP3/CN7/RB3")
				(number "24")
			)
			(pin input line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "SOSCI/RP4/CN1/RB4")
				(number "33")
			)
			(pin input line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "PGED3/ASDA1/RP5/CN27/PMD7/RB5")
				(number "41")
			)
			(pin input line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "PGEC3/ASCL1/RP6/CN24/PMD6/RB6")
				(number "42")
			)
			(pin input line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "INT0/RP7/CN23/PMD5/RB7")
				(number "43")
			)
			(pin input line
				(at 33.02 0 180)
				(length 3.81)
				(name "SCL1/RP8/CN22/PMD4/RB8")
				(number "44")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "SDA1/RP9/CN21/PMD3/RB9")
				(number "1")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "PGED2/PWM1H3/RP10/CN16/PMD2/RB10")
				(number "8")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "PGEC2/PWM1L3/RP11/CN15/PMD1/RB11")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "PWM1H2/RP12/CN14/PMD0/RB12")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "PWM1L2/RP13/CN13/PMRD/RB13")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "PWM1H1/RTCC/RP14/CN12/PMWR/RB14")
				(number "14")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "PWM1L/RP15/CN11/PMCS1/RB15")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 3.81)
				(name "AN6/RP16/CN8/RC0")
				(number "25")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 3.81)
				(name "AN7/RP17/CN9/RC1")
				(number "26")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 3.81)
				(name "AN8/CVREF/RP18/PMA2/CN10/RC2")
				(number "27")
			)
			(pin input line
				(at 33.02 -30.48 180)
				(length 3.81)
				(name "RP19/CN28/PMBE/RC3")
				(number "36")
			)
			(pin input line
				(at 33.02 -33.02 180)
				(length 3.81)
				(name "RP20/CN25/PMA4/RC4")
				(number "37")
			)
			(pin input line
				(at 33.02 -35.56 180)
				(length 3.81)
				(name "RP21/CN26/PMA3/RC5")
				(number "38")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 3.81)
				(name "PWM2H1/RP22/CN18/PMA1/RC6")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 3.81)
				(name "PWM2L1/RP23/CN17/PMA0/RC7")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 3.81)
				(name "RP24/CN20/PMA5/RC8")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 3.81)
				(name "RP25/CN19/PMA6/RC9")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DSPIC33FJ64MC802-xSP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -31.75 29.21 0)
		)
		(property "Value" "DSPIC33FJ64MC802-xSP"
			(at 22.86 29.21 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/70291G.pdf"
			(at 0 0 0)
		)
		(property "Description" "40 MIPS, 64k Flash, 16k SRAM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit Digital Signal Controller Microchip dsPIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DSPIC33FJ64MC802-xSP_0_1")
		(symbol "DSPIC33FJ64MC802-xSP_1_1"
			(pin input line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "~{MCLR}")
				(number "1")
			)
			(pin passive line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "VCAP")
				(number "20")
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "AN0/VREF+/CN2/RA0")
				(number "2")
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "AN1/VREF-/CN3/RA1")
				(number "3")
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "OSC1/CLKI/CN30/RA2")
				(number "9")
			)
			(pin bidirectional line
				(at -40.64 -17.78 0)
				(length 5.08)
				(name "OSC2/CLKO/CN29/PMA0/RA3")
				(number "10")
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "SOSCO/T1CK/CN0/PMA1/RA4")
				(number "12")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 5.08)
				(name "VDD")
				(number "13")
			)
			(pin passive line
				(at -2.54 -33.02 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "19")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 5.08)
				(name "AVDD")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 5.08)
				(name "AVSS")
				(number "27")
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "PGED1/AN2/C2IN-/RP0/CN4/RB0")
				(number "4")
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "PGEC1/AN3/C2IN+/RP1/CN5/RB1")
				(number "5")
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "AN4/C1IN-/RP2/CN6/RB2")
				(number "6")
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "AN5/C1IN+/RP3/CN7/RB3")
				(number "7")
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "SOSCI/RP4/CN1/PMBE/RB4")
				(number "11")
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "PGED3/ASDA1/RP5/CN27/PMD7/RB5")
				(number "14")
			)
			(pin bidirectional line
				(at 40.64 2.54 180)
				(length 5.08)
				(name "PGEC3/ASCL1/RP6/CN24/PMD6/RB6")
				(number "15")
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "INT0/RP7/CN23/PMD5/RB7")
				(number "16")
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "TCK/PWM2H1/SCL1/RP8/CN22/PMD4/RB8")
				(number "17")
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "TDO/PWM2L1/SDA1/RP9/CN21/PMD3/RB9")
				(number "18")
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "PGED2/TDI/PWM1H3/RP10/CN16/PMD2/RB10")
				(number "21")
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "PGEC2/TMS/PWM1L3/RP11/CN15/PMD1/RB11")
				(number "22")
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "PWM1H2/RP12/CN14/PMD0/RB12")
				(number "23")
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "PWM1L2/RP13/CN13/PMRD/RB13")
				(number "24")
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "PWM1H1/RTCC/RP14/CN12/PMWR/RB14")
				(number "25")
			)
			(pin bidirectional line
				(at 40.64 -20.32 180)
				(length 5.08)
				(name "PWM1L1/RP15/CN11/PMCS1/RB15")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DSPIC33FJ64MC804"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 48.26 0)
		)
		(property "Value" "DSPIC33FJ64MC804"
			(at -29.21 -48.26 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/70291G.pdf"
			(at 0 0 0)
		)
		(property "Description" "40MIPS, 64k Flash, 16k SRAM, ECAN, 16-bit DAC"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit Digital Signal Controller Microchip dsPIC Motor Control"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN?44*1EP*8x8mm*P0.65mm* TQFP?44*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "DSPIC33FJ64MC804_1_1"
			(pin input line
				(at -33.02 45.72 0)
				(length 3.81)
				(name "~{MCLR}")
				(number "18")
			)
			(pin power_in line
				(at -7.62 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -7.62 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "40")
			)
			(pin power_in line
				(at -5.08 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "39")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 3.81)
				(name "AVDD")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 3.81)
				(name "AVSS")
				(number "16")
			)
			(pin power_in line
				(at 5.08 50.8 270)
				(length 3.81)
				(name "VCAP")
				(number "7")
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 3.81)
				(name "AN0/VREF+/CN2/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 3.81)
				(name "AN1/VREF-/CN3/RA1")
				(number "20")
			)
			(pin input line
				(at 33.02 40.64 180)
				(length 3.81)
				(name "OSC1/CLKI/CN30/RA2")
				(number "30")
			)
			(pin input line
				(at 33.02 38.1 180)
				(length 3.81)
				(name "OSC2/CLKO/CN29/RA3")
				(number "31")
			)
			(pin input line
				(at 33.02 35.56 180)
				(length 3.81)
				(name "SOSCO/T1CK/CN0/RA4")
				(number "34")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 3.81)
				(name "TCK/PMA7/RA7")
				(number "13")
			)
			(pin input line
				(at 33.02 30.48 180)
				(length 3.81)
				(name "TDO/PMA8/RA8")
				(number "32")
			)
			(pin input line
				(at 33.02 27.94 180)
				(length 3.81)
				(name "TDI/PMA9/RA9")
				(number "35")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "TMS/PMA10/RA10")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "PGED1/AN2/C2IN-/RP0/CN4/RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "PGEC1/AN3/C2IN+/RP1/CN5/RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "AN4/C1IN-/RP2/CN6/RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "AN5/C1IN+/RP3/CN7/RB3")
				(number "24")
			)
			(pin input line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "SOSCI/RP4/CN1/RB4")
				(number "33")
			)
			(pin input line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "PGED3/ASDA1/RP5/CN27/PMD7/RB5")
				(number "41")
			)
			(pin input line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "PGEC3/ASCL1/RP6/CN24/PMD6/RB6")
				(number "42")
			)
			(pin input line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "INT0/RP7/CN23/PMD5/RB7")
				(number "43")
			)
			(pin input line
				(at 33.02 0 180)
				(length 3.81)
				(name "SCL1/RP8/CN22/PMD4/RB8")
				(number "44")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "SDA1/RP9/CN21/PMD3/RB9")
				(number "1")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "PGED2/PWM1H3/RP10/CN16/PMD2/RB10")
				(number "8")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "PGEC2/PWM1L3/RP11/CN15/PMD1/RB11")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "PWM1H2/DAC1RP/RP12/CN14/PMD0/RB12")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "PWM1L2/DAC1RN/RP13/CN13/PMRD/RB13")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "PWM1H1/DAC1LP/RTCC/RP14/CN12/PMWR/RB14")
				(number "14")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "PWM1L/DAC1LN/RP15/CN11/PMCS1/RB15")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 3.81)
				(name "AN6/DAC1RM/RP16/CN8/RC0")
				(number "25")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 3.81)
				(name "AN7/DAC1LM/RP17/CN9/RC1")
				(number "26")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 3.81)
				(name "AN8/CVREF/RP18/PMA2/CN10/RC2")
				(number "27")
			)
			(pin input line
				(at 33.02 -30.48 180)
				(length 3.81)
				(name "RP19/CN28/PMBE/RC3")
				(number "36")
			)
			(pin input line
				(at 33.02 -33.02 180)
				(length 3.81)
				(name "RP20/CN25/PMA4/RC4")
				(number "37")
			)
			(pin input line
				(at 33.02 -35.56 180)
				(length 3.81)
				(name "RP21/CN26/PMA3/RC5")
				(number "38")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 3.81)
				(name "PWM2H1/RP22/CN18/PMA1/RC6")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 3.81)
				(name "PWM2L1/RP23/CN17/PMA0/RC7")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 3.81)
				(name "RP24/CN20/PMA5/RC8")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 3.81)
				(name "RP25/CN19/PMA6/RC9")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DSPIC33FJ128MC510A"
		(extends "DSPIC33FJ256MC710A")
		(property "Reference" "U"
			(at 21.59 69.85 0)
		)
		(property "Value" "DSPIC33FJ128MC510A"
			(at 0 7.62 90)
		)
		(property "Footprint" ""
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/70594C.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "High-Performance, 16-bit Digital Signal Controller, 40MIPS, 128k Flash, 8k SRAM, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit Digital Signal Controller Microchip dsPIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*12x12mm*P0.4mm* TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "DSPIC33FJ128MC710A"
		(extends "DSPIC33FJ256MC710A")
		(property "Reference" "U"
			(at 21.59 69.85 0)
		)
		(property "Value" "DSPIC33FJ128MC710A"
			(at 0 7.62 90)
		)
		(property "Footprint" ""
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/70594C.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "High-Performance, 16-bit Digital Signal Controller,40MIPS, 128k Flash, 16k SRAM, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit Digital Signal Controller Microchip dsPIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*12x12mm*P0.4mm* TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "DSPIC33FJ256MC510A"
		(extends "DSPIC33FJ256MC710A")
		(property "Reference" "U"
			(at 21.59 69.85 0)
		)
		(property "Value" "DSPIC33FJ256MC510A"
			(at 0 7.62 90)
		)
		(property "Footprint" ""
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/70594C.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "High-Performance, 16-bit Digital Signal Controller, 40MIPS, 256k Flash, 16k SRAM, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit Digital Signal Controller Microchip dsPIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*12x12mm*P0.4mm* TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "DSPIC33FJ64MC510A"
		(extends "DSPIC33FJ256MC710A")
		(property "Reference" "U"
			(at 21.59 69.85 0)
		)
		(property "Value" "DSPIC33FJ64MC510A"
			(at 0 7.62 90)
		)
		(property "Footprint" ""
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/70594C.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "High-Performance, 16-bit Digital Signal Controller, 40MIPS, 64k Flash, 8k SRAM, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit Digital Signal Controller Microchip dsPIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*12x12mm*P0.4mm* TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "DSPIC33FJ64MC710A"
		(extends "DSPIC33FJ256MC710A")
		(property "Reference" "U"
			(at 21.59 69.85 0)
		)
		(property "Value" "DSPIC33FJ64MC710A"
			(at 0 7.62 90)
		)
		(property "Footprint" ""
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/70594C.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "High-Performance, 16-bit Digital Signal Controller, 40MIPS, 64k Flash, 16k SRAM, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "16-bit Digital Signal Controller Microchip dsPIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*12x12mm*P0.4mm* TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
