(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "DSP56301"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "DSP56301"
			(at 1.27 -8.89 0)
		)
		(property "Footprint" "Package_QFP:PQFP-208_28x28mm_P0.5mm"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/DSP56301DS.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "24-Bit Digital Signal Processor with PCI bus interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "DSP PCI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PQFP*28x28mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "DSP56301_0_1"
			(text "PORT_A"
				(at -30.48 86.36 0)
			)
			(text "PLL"
				(at -21.59 -78.74 0)
			)
			(text "PORT_E"
				(at -19.05 -88.9 0)
			)
			(text "PORT_C"
				(at 24.13 -52.07 0)
			)
			(text "PORT_D"
				(at 24.13 -69.85 0)
			)
			(text "PCI"
				(at 27.94 12.7 0)
			)
			(text "Timers"
				(at 33.02 -83.82 0)
			)
			(text "JTAG"
				(at 36.83 101.6 0)
			)
		)
		(symbol "DSP56301_1_1"
			(pin output line
				(at -50.8 106.68 0)
				(length 7.62)
				(name "A0")
				(number "29")
			)
			(pin output line
				(at -50.8 104.14 0)
				(length 7.62)
				(name "A1")
				(number "30")
			)
			(pin output line
				(at -50.8 101.6 0)
				(length 7.62)
				(name "A2")
				(number "33")
			)
			(pin output line
				(at -50.8 99.06 0)
				(length 7.62)
				(name "A3")
				(number "34")
			)
			(pin output line
				(at -50.8 96.52 0)
				(length 7.62)
				(name "A4")
				(number "35")
			)
			(pin output line
				(at -50.8 93.98 0)
				(length 7.62)
				(name "A5")
				(number "36")
			)
			(pin output line
				(at -50.8 91.44 0)
				(length 7.62)
				(name "A6")
				(number "39")
			)
			(pin output line
				(at -50.8 88.9 0)
				(length 7.62)
				(name "A7")
				(number "40")
			)
			(pin output line
				(at -50.8 86.36 0)
				(length 7.62)
				(name "A8")
				(number "41")
			)
			(pin output line
				(at -50.8 83.82 0)
				(length 7.62)
				(name "A9")
				(number "42")
			)
			(pin output line
				(at -50.8 81.28 0)
				(length 7.62)
				(name "A10")
				(number "45")
			)
			(pin output line
				(at -50.8 78.74 0)
				(length 7.62)
				(name "A11")
				(number "46")
			)
			(pin output line
				(at -50.8 76.2 0)
				(length 7.62)
				(name "A12")
				(number "47")
			)
			(pin output line
				(at -50.8 73.66 0)
				(length 7.62)
				(name "A13")
				(number "48")
			)
			(pin output line
				(at -50.8 71.12 0)
				(length 7.62)
				(name "A14")
				(number "51")
			)
			(pin output line
				(at -50.8 68.58 0)
				(length 7.62)
				(name "A15")
				(number "52")
			)
			(pin output line
				(at -50.8 66.04 0)
				(length 7.62)
				(name "A16")
				(number "55")
			)
			(pin output line
				(at -50.8 63.5 0)
				(length 7.62)
				(name "A17")
				(number "56")
			)
			(pin output line
				(at -50.8 60.96 0)
				(length 7.62)
				(name "A18")
				(number "59")
			)
			(pin output line
				(at -50.8 58.42 0)
				(length 7.62)
				(name "A19")
				(number "60")
			)
			(pin output line
				(at -50.8 55.88 0)
				(length 7.62)
				(name "A20")
				(number "61")
			)
			(pin output line
				(at -50.8 53.34 0)
				(length 7.62)
				(name "A21")
				(number "62")
			)
			(pin output line
				(at -50.8 50.8 0)
				(length 7.62)
				(name "A22")
				(number "65")
			)
			(pin output line
				(at -50.8 48.26 0)
				(length 7.62)
				(name "A23")
				(number "66")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 7.62)
				(name "D0")
				(number "67")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 7.62)
				(name "D1")
				(number "68")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 7.62)
				(name "D2")
				(number "69")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 7.62)
				(name "D3")
				(number "72")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 7.62)
				(name "D4")
				(number "73")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 7.62)
				(name "D5")
				(number "74")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 7.62)
				(name "D6")
				(number "75")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 7.62)
				(name "D7")
				(number "76")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 7.62)
				(name "D8")
				(number "77")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 7.62)
				(name "D9")
				(number "82")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 7.62)
				(name "D10")
				(number "83")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 7.62)
				(name "D11")
				(number "84")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 7.62)
				(name "D12")
				(number "85")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 7.62)
				(name "D13")
				(number "86")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 7.62)
				(name "D14")
				(number "87")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 7.62)
				(name "D15")
				(number "90")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 7.62)
				(name "D16")
				(number "91")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 7.62)
				(name "D17")
				(number "92")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 7.62)
				(name "D18")
				(number "93")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 7.62)
				(name "D19")
				(number "94")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 7.62)
				(name "D20")
				(number "95")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 7.62)
				(name "D21")
				(number "98")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 7.62)
				(name "D22")
				(number "99")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 7.62)
				(name "D23")
				(number "100")
			)
			(pin output line
				(at -50.8 -20.32 0)
				(length 7.62)
				(name "AA0/RAS0")
				(number "1")
			)
			(pin output line
				(at -50.8 -22.86 0)
				(length 7.62)
				(name "AA1/RAS1")
				(number "2")
			)
			(pin output line
				(at -50.8 -25.4 0)
				(length 7.62)
				(name "AA2/RAS2")
				(number "20")
			)
			(pin output line
				(at -50.8 -27.94 0)
				(length 7.62)
				(name "AA3/RAS3")
				(number "21")
			)
			(pin output inverted
				(at -50.8 -30.48 0)
				(length 7.62)
				(name "/RD")
				(number "23")
			)
			(pin output inverted
				(at -50.8 -33.02 0)
				(length 7.62)
				(name "/WR")
				(number "22")
			)
			(pin output inverted
				(at -50.8 -35.56 0)
				(length 7.62)
				(name "/BS")
				(number "205")
			)
			(pin input inverted
				(at -50.8 -38.1 0)
				(length 7.62)
				(name "/TA")
				(number "8")
			)
			(pin output inverted
				(at -50.8 -40.64 0)
				(length 7.62)
				(name "/BR")
				(number "17")
			)
			(pin input inverted
				(at -50.8 -43.18 0)
				(length 7.62)
				(name "/BG")
				(number "16")
			)
			(pin bidirectional inverted
				(at -50.8 -45.72 0)
				(length 7.62)
				(name "/BB")
				(number "15")
			)
			(pin output inverted
				(at -50.8 -48.26 0)
				(length 7.62)
				(name "/BL")
				(number "206")
			)
			(pin output inverted
				(at -50.8 -50.8 0)
				(length 7.62)
				(name "/CAS")
				(number "7")
			)
			(pin output clock
				(at -50.8 -53.34 0)
				(length 7.62)
				(name "BCLK")
				(number "6")
			)
			(pin output inverted_clock
				(at -50.8 -55.88 0)
				(length 7.62)
				(name "/BCLK")
				(number "28")
			)
			(pin input line
				(at -50.8 -60.96 0)
				(length 7.62)
				(name "MODA/IRQA")
				(number "101")
			)
			(pin input line
				(at -50.8 -63.5 0)
				(length 7.62)
				(name "MODB/IRQB")
				(number "102")
			)
			(pin input line
				(at -50.8 -66.04 0)
				(length 7.62)
				(name "MODC/IRQC")
				(number "105")
			)
			(pin input line
				(at -50.8 -68.58 0)
				(length 7.62)
				(name "MODD/IRQD")
				(number "106")
			)
			(pin input inverted
				(at -50.8 -71.12 0)
				(length 7.62)
				(name "/RESET")
				(number "10")
			)
			(pin input line
				(at -50.8 -76.2 0)
				(length 7.62)
				(name "PINIT/NMI")
				(number "9")
			)
			(pin output clock
				(at -50.8 -78.74 0)
				(length 7.62)
				(name "CLKOUT")
				(number "5")
			)
			(pin input line
				(at -50.8 -81.28 0)
				(length 7.62)
				(name "PCAP")
				(number "12")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 7.62)
				(name "PE0/RXD")
				(number "177")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 7.62)
				(name "PE1/TXD")
				(number "184")
			)
			(pin bidirectional clock
				(at -50.8 -91.44 0)
				(length 7.62)
				(name "PE2/SCLK")
				(number "178")
			)
			(pin input clock
				(at -50.8 -96.52 0)
				(length 7.62)
				(name "EXTAL")
				(number "26")
			)
			(pin output clock
				(at -50.8 -99.06 0)
				(length 7.62)
				(name "XTAL")
				(number "24")
			)
			(pin power_in line
				(at -33.02 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "32")
			)
			(pin power_in line
				(at -33.02 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "31")
			)
			(pin power_in line
				(at -30.48 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "38")
			)
			(pin power_in line
				(at -30.48 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "37")
			)
			(pin power_in line
				(at -27.94 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "44")
			)
			(pin power_in line
				(at -27.94 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "43")
			)
			(pin power_in line
				(at -25.4 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "50")
			)
			(pin power_in line
				(at -25.4 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at -22.86 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "58")
			)
			(pin power_in line
				(at -22.86 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "57")
			)
			(pin power_in line
				(at -20.32 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "64")
			)
			(pin power_in line
				(at -20.32 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "63")
			)
			(pin power_in line
				(at -17.78 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "71")
			)
			(pin power_in line
				(at -17.78 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "70")
			)
			(pin power_in line
				(at -15.24 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "81")
			)
			(pin power_in line
				(at -15.24 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "80")
			)
			(pin power_in line
				(at -12.7 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "89")
			)
			(pin power_in line
				(at -12.7 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "88")
			)
			(pin power_in line
				(at -10.16 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "97")
			)
			(pin power_in line
				(at -10.16 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "96")
			)
			(pin power_in line
				(at -7.62 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "111")
			)
			(pin power_in line
				(at -7.62 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "112")
			)
			(pin power_in line
				(at -5.08 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "122")
			)
			(pin power_in line
				(at -5.08 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "123")
			)
			(pin power_in line
				(at -2.54 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "135")
			)
			(pin power_in line
				(at -2.54 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "136")
			)
			(pin power_in line
				(at 0 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "144")
			)
			(pin power_in line
				(at 0 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "143")
			)
			(pin power_in line
				(at 2.54 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "156")
			)
			(pin power_in line
				(at 2.54 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "155")
			)
			(pin power_in line
				(at 5.08 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "169")
			)
			(pin power_in line
				(at 5.08 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "168")
			)
			(pin power_in line
				(at 7.62 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 7.62 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 10.16 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "18")
			)
			(pin power_in line
				(at 10.16 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "19")
			)
			(pin power_in line
				(at 12.7 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "193")
			)
			(pin power_in line
				(at 12.7 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "180")
			)
			(pin power_in line
				(at 15.24 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "179")
			)
			(pin power_in line
				(at 15.24 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "194")
			)
			(pin power_in line
				(at 17.78 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "25")
			)
			(pin power_in line
				(at 17.78 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "27")
			)
			(pin power_in line
				(at 20.32 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "79")
			)
			(pin power_in line
				(at 20.32 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "78")
			)
			(pin power_in line
				(at 22.86 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "131")
			)
			(pin power_in line
				(at 22.86 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "132")
			)
			(pin power_in line
				(at 25.4 119.38 270)
				(length 7.62)
				(name "VCC")
				(number "182")
			)
			(pin power_in line
				(at 25.4 -124.46 90)
				(length 7.62)
				(name "GND")
				(number "183")
			)
			(pin power_in line
				(at 27.94 119.38 270)
				(length 7.62)
				(name "VCCPLL")
				(number "11")
			)
			(pin power_in line
				(at 27.94 -124.46 90)
				(length 7.62)
				(name "GNDP")
				(number "13")
			)
			(pin power_in line
				(at 30.48 -124.46 90)
				(length 7.62)
				(name "GND1P")
				(number "14")
			)
			(pin input line
				(at 55.88 106.68 180)
				(length 7.62)
				(name "TDI")
				(number "202")
			)
			(pin input line
				(at 55.88 104.14 180)
				(length 7.62)
				(name "TCK")
				(number "201")
			)
			(pin output line
				(at 55.88 101.6 180)
				(length 7.62)
				(name "TDO")
				(number "203")
			)
			(pin output inverted
				(at 55.88 99.06 180)
				(length 7.62)
				(name "/DE")
				(number "199")
			)
			(pin input inverted
				(at 55.88 96.52 180)
				(length 7.62)
				(name "/TRST")
				(number "204")
			)
			(pin input line
				(at 55.88 93.98 180)
				(length 7.62)
				(name "TMS")
				(number "200")
			)
			(pin bidirectional line
				(at 55.88 88.9 180)
				(length 7.62)
				(name "HAD0")
				(number "173")
			)
			(pin bidirectional line
				(at 55.88 86.36 180)
				(length 7.62)
				(name "HAD1")
				(number "172")
			)
			(pin bidirectional line
				(at 55.88 83.82 180)
				(length 7.62)
				(name "HAD2")
				(number "171")
			)
			(pin bidirectional line
				(at 55.88 81.28 180)
				(length 7.62)
				(name "HAD3")
				(number "170")
			)
			(pin bidirectional line
				(at 55.88 78.74 180)
				(length 7.62)
				(name "HAD4")
				(number "167")
			)
			(pin bidirectional line
				(at 55.88 76.2 180)
				(length 7.62)
				(name "HAD5")
				(number "166")
			)
			(pin bidirectional line
				(at 55.88 73.66 180)
				(length 7.62)
				(name "HAD6")
				(number "165")
			)
			(pin bidirectional line
				(at 55.88 71.12 180)
				(length 7.62)
				(name "HAD7")
				(number "164")
			)
			(pin bidirectional line
				(at 55.88 68.58 180)
				(length 7.62)
				(name "HAD8")
				(number "162")
			)
			(pin bidirectional line
				(at 55.88 66.04 180)
				(length 7.62)
				(name "HAD9")
				(number "161")
			)
			(pin bidirectional line
				(at 55.88 63.5 180)
				(length 7.62)
				(name "HAD10")
				(number "160")
			)
			(pin bidirectional line
				(at 55.88 60.96 180)
				(length 7.62)
				(name "HAD11")
				(number "159")
			)
			(pin bidirectional line
				(at 55.88 58.42 180)
				(length 7.62)
				(name "HAD12")
				(number "154")
			)
			(pin bidirectional line
				(at 55.88 55.88 180)
				(length 7.62)
				(name "HAD13")
				(number "153")
			)
			(pin bidirectional line
				(at 55.88 53.34 180)
				(length 7.62)
				(name "HAD14")
				(number "152")
			)
			(pin bidirectional line
				(at 55.88 50.8 180)
				(length 7.62)
				(name "HAD15")
				(number "151")
			)
			(pin bidirectional line
				(at 55.88 48.26 180)
				(length 7.62)
				(name "HAD16")
				(number "127")
			)
			(pin bidirectional line
				(at 55.88 45.72 180)
				(length 7.62)
				(name "HAD17")
				(number "126")
			)
			(pin bidirectional line
				(at 55.88 43.18 180)
				(length 7.62)
				(name "HAD18")
				(number "125")
			)
			(pin bidirectional line
				(at 55.88 40.64 180)
				(length 7.62)
				(name "HAD19")
				(number "124")
			)
			(pin bidirectional line
				(at 55.88 38.1 180)
				(length 7.62)
				(name "HAD20")
				(number "121")
			)
			(pin bidirectional line
				(at 55.88 35.56 180)
				(length 7.62)
				(name "HAD21")
				(number "120")
			)
			(pin bidirectional line
				(at 55.88 33.02 180)
				(length 7.62)
				(name "HAD22")
				(number "119")
			)
			(pin bidirectional line
				(at 55.88 30.48 180)
				(length 7.62)
				(name "HAD23")
				(number "118")
			)
			(pin bidirectional line
				(at 55.88 27.94 180)
				(length 7.62)
				(name "HAD24")
				(number "116")
			)
			(pin bidirectional line
				(at 55.88 25.4 180)
				(length 7.62)
				(name "HAD25")
				(number "115")
			)
			(pin bidirectional line
				(at 55.88 22.86 180)
				(length 7.62)
				(name "HAD26")
				(number "114")
			)
			(pin bidirectional line
				(at 55.88 20.32 180)
				(length 7.62)
				(name "HAD27")
				(number "113")
			)
			(pin bidirectional line
				(at 55.88 17.78 180)
				(length 7.62)
				(name "HAD28")
				(number "110")
			)
			(pin bidirectional line
				(at 55.88 15.24 180)
				(length 7.62)
				(name "HAD29")
				(number "109")
			)
			(pin bidirectional line
				(at 55.88 12.7 180)
				(length 7.62)
				(name "HAD30")
				(number "108")
			)
			(pin bidirectional line
				(at 55.88 10.16 180)
				(length 7.62)
				(name "HAD31")
				(number "107")
			)
			(pin bidirectional line
				(at 55.88 5.08 180)
				(length 7.62)
				(name "HC0/HBE0")
				(number "163")
			)
			(pin bidirectional line
				(at 55.88 2.54 180)
				(length 7.62)
				(name "HC1/HBE1")
				(number "150")
			)
			(pin bidirectional line
				(at 55.88 0 180)
				(length 7.62)
				(name "HC2/HBE2")
				(number "128")
			)
			(pin bidirectional line
				(at 55.88 -2.54 180)
				(length 7.62)
				(name "HC3/HBE3")
				(number "117")
			)
			(pin bidirectional inverted
				(at 55.88 -5.08 180)
				(length 7.62)
				(name "/HTRDY")
				(number "134")
			)
			(pin bidirectional inverted
				(at 55.88 -7.62 180)
				(length 7.62)
				(name "/HIRDY")
				(number "133")
			)
			(pin bidirectional inverted
				(at 55.88 -10.16 180)
				(length 7.62)
				(name "/HDEVSEL")
				(number "138")
			)
			(pin bidirectional inverted
				(at 55.88 -12.7 180)
				(length 7.62)
				(name "/HLOCK")
				(number "140")
			)
			(pin bidirectional line
				(at 55.88 -15.24 180)
				(length 7.62)
				(name "HPAR")
				(number "145")
			)
			(pin bidirectional inverted
				(at 55.88 -17.78 180)
				(length 7.62)
				(name "/HPERR")
				(number "141")
			)
			(pin input inverted
				(at 55.88 -20.32 180)
				(length 7.62)
				(name "/HGNT")
				(number "149")
			)
			(pin output inverted
				(at 55.88 -22.86 180)
				(length 7.62)
				(name "/HREQ")
				(number "146")
			)
			(pin output inverted
				(at 55.88 -25.4 180)
				(length 7.62)
				(name "/HSERR")
				(number "142")
			)
			(pin bidirectional inverted
				(at 55.88 -27.94 180)
				(length 7.62)
				(name "/HSTOP")
				(number "139")
			)
			(pin input line
				(at 55.88 -30.48 180)
				(length 7.62)
				(name "HIDSEL")
				(number "129")
			)
			(pin bidirectional inverted
				(at 55.88 -33.02 180)
				(length 7.62)
				(name "/HFRAME")
				(number "130")
			)
			(pin input clock
				(at 55.88 -35.56 180)
				(length 7.62)
				(name "HCLK")
				(number "148")
			)
			(pin input inverted
				(at 55.88 -38.1 180)
				(length 7.62)
				(name "/HRST")
				(number "147")
			)
			(pin output inverted
				(at 55.88 -40.64 180)
				(length 7.62)
				(name "/HINTA")
				(number "181")
			)
			(pin bidirectional line
				(at 55.88 -45.72 180)
				(length 7.62)
				(name "PC0/SC00")
				(number "196")
			)
			(pin bidirectional line
				(at 55.88 -48.26 180)
				(length 7.62)
				(name "PC1/SC01")
				(number "197")
			)
			(pin bidirectional line
				(at 55.88 -50.8 180)
				(length 7.62)
				(name "PC2/SC02")
				(number "198")
			)
			(pin bidirectional line
				(at 55.88 -53.34 180)
				(length 7.62)
				(name "PC3/SCK0")
				(number "192")
			)
			(pin bidirectional line
				(at 55.88 -55.88 180)
				(length 7.62)
				(name "PC4/SRD0")
				(number "191")
			)
			(pin bidirectional line
				(at 55.88 -58.42 180)
				(length 7.62)
				(name "PC5/STD0")
				(number "195")
			)
			(pin bidirectional line
				(at 55.88 -63.5 180)
				(length 7.62)
				(name "PD0/SC10")
				(number "187")
			)
			(pin bidirectional line
				(at 55.88 -66.04 180)
				(length 7.62)
				(name "PD1/SC11")
				(number "186")
			)
			(pin bidirectional line
				(at 55.88 -68.58 180)
				(length 7.62)
				(name "PD2/SC12")
				(number "185")
			)
			(pin bidirectional line
				(at 55.88 -71.12 180)
				(length 7.62)
				(name "PD3/SCK1")
				(number "189")
			)
			(pin bidirectional line
				(at 55.88 -73.66 180)
				(length 7.62)
				(name "PD4/SRD1")
				(number "190")
			)
			(pin bidirectional line
				(at 55.88 -76.2 180)
				(length 7.62)
				(name "PD5/STD1")
				(number "188")
			)
			(pin bidirectional line
				(at 55.88 -81.28 180)
				(length 7.62)
				(name "TIO0")
				(number "176")
			)
			(pin bidirectional line
				(at 55.88 -83.82 180)
				(length 7.62)
				(name "TIO1")
				(number "175")
			)
			(pin bidirectional line
				(at 55.88 -86.36 180)
				(length 7.62)
				(name "TIO2")
				(number "174")
			)
			(pin input line
				(at 55.88 -93.98 180)
				(length 7.62)
				(name "PVCL")
				(number "137")
			)
		)
		(embedded_fonts no)
	)
)
