(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "TMS320LF2406PZ"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -26.67 66.04 0)
		)
		(property "Value" "TMS320LF2406PZ"
			(at 13.97 66.04 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tms320lf2406.pdf"
			(at 0 0 0)
		)
		(property "Description" "16bit DSP Controller 32Kx16B Flash 2.5Kx16B RAM, Obsolete NRND, PQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "16BIT DSP TMS320 Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PQFP-100*"
			(at 0 0 0)
		)
		(symbol "TMS320LF2406PZ_0_1")
		(symbol "TMS320LF2406PZ_1_1"
			(pin input line
				(at -30.48 58.42 0)
				(length 3.81)
				(name "ADCIN00")
				(number "79")
			)
			(pin input line
				(at -30.48 55.88 0)
				(length 3.81)
				(name "ADCIN01")
				(number "77")
			)
			(pin input line
				(at -30.48 53.34 0)
				(length 3.81)
				(name "ADCIN02")
				(number "74")
			)
			(pin input line
				(at -30.48 50.8 0)
				(length 3.81)
				(name "ADCIN03")
				(number "72")
			)
			(pin input line
				(at -30.48 48.26 0)
				(length 3.81)
				(name "ADCIN04")
				(number "70")
			)
			(pin input line
				(at -30.48 45.72 0)
				(length 3.81)
				(name "ADCIN05")
				(number "69")
			)
			(pin input line
				(at -30.48 43.18 0)
				(length 3.81)
				(name "ADCIN06")
				(number "67")
			)
			(pin input line
				(at -30.48 40.64 0)
				(length 3.81)
				(name "ADCIN07")
				(number "66")
			)
			(pin input line
				(at -30.48 38.1 0)
				(length 3.81)
				(name "ADCIN08")
				(number "80")
			)
			(pin input line
				(at -30.48 35.56 0)
				(length 3.81)
				(name "ADCIN09")
				(number "78")
			)
			(pin input line
				(at -30.48 33.02 0)
				(length 3.81)
				(name "ADCIN10")
				(number "76")
			)
			(pin input line
				(at -30.48 30.48 0)
				(length 3.81)
				(name "ADCIN11")
				(number "75")
			)
			(pin input line
				(at -30.48 27.94 0)
				(length 3.81)
				(name "ADCIN12")
				(number "73")
			)
			(pin input line
				(at -30.48 25.4 0)
				(length 3.81)
				(name "ADCIN13")
				(number "71")
			)
			(pin input line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "ADCIN14")
				(number "68")
			)
			(pin input line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "ADCIN15")
				(number "65")
			)
			(pin passive line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "VrefHI")
				(number "82")
			)
			(pin passive line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "VrefLO")
				(number "81")
			)
			(pin power_in line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "VCCA")
				(number "83")
			)
			(pin power_in line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "VSSA")
				(number "84")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 3.81)
				(name "CANRX/IOPC7")
				(number "49")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "CANTX/IOPC6")
				(number "50")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "TXD/IOPA0")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 3.81)
				(name "RXD/IOPA1")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "SPI_SIMO/IOPC2")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "SPI_SOMI/IOPC3")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "SPI_CLK/IOPC4")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "SPI_TE-/IOPC5")
				(number "23")
			)
			(pin input inverted
				(at -30.48 -27.94 0)
				(length 3.81)
				(name "RESET")
				(number "93")
			)
			(pin input clock
				(at -30.48 -33.02 0)
				(length 3.81)
				(name "XTAL/CLKIN")
				(number "87")
			)
			(pin output line
				(at -30.48 -35.56 0)
				(length 3.81)
				(name "XTAL2")
				(number "88")
			)
			(pin output line
				(at -30.48 -40.64 0)
				(length 3.81)
				(name "~{BOOT_EN}/XF")
				(number "86")
			)
			(pin passive line
				(at -30.48 -45.72 0)
				(length 3.81)
				(name "PLLF")
				(number "9")
			)
			(pin passive line
				(at -30.48 -48.26 0)
				(length 3.81)
				(name "PLLF2")
				(number "8")
			)
			(pin passive line
				(at -30.48 -50.8 0)
				(length 3.81)
				(name "PLLVcca")
				(number "10")
			)
			(pin passive line
				(at -30.48 -55.88 0)
				(length 3.81)
				(name "VccPROG_5V")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 3.81)
				(name "EMU0")
				(number "61")
			)
			(pin bidirectional line
				(at -30.48 -63.5 0)
				(length 3.81)
				(name "EMU1/OFF-")
				(number "62")
			)
			(pin power_in line
				(at -12.7 68.58 270)
				(length 3.81)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at -10.16 68.58 270)
				(length 3.81)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at -10.16 -73.66 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at -7.62 68.58 270)
				(length 3.81)
				(name "VCC")
				(number "30")
			)
			(pin power_in line
				(at -7.62 -73.66 90)
				(length 3.81)
				(name "GND")
				(number "19")
			)
			(pin power_in line
				(at -5.08 68.58 270)
				(length 3.81)
				(name "VCC")
				(number "35")
			)
			(pin power_in line
				(at -5.08 -73.66 90)
				(length 3.81)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at -2.54 68.58 270)
				(length 3.81)
				(name "VCC")
				(number "54")
			)
			(pin power_in line
				(at -2.54 -73.66 90)
				(length 3.81)
				(name "GND")
				(number "34")
			)
			(pin power_in line
				(at 0 68.58 270)
				(length 3.81)
				(name "VCC")
				(number "47")
			)
			(pin power_in line
				(at 0 -73.66 90)
				(length 3.81)
				(name "GND")
				(number "46")
			)
			(pin power_in line
				(at 2.54 68.58 270)
				(length 3.81)
				(name "VCC")
				(number "59")
			)
			(pin power_in line
				(at 2.54 -73.66 90)
				(length 3.81)
				(name "GND")
				(number "53")
			)
			(pin power_in line
				(at 5.08 68.58 270)
				(length 3.81)
				(name "VCC")
				(number "64")
			)
			(pin power_in line
				(at 5.08 -73.66 90)
				(length 3.81)
				(name "GND")
				(number "58")
			)
			(pin power_in line
				(at 7.62 68.58 270)
				(length 3.81)
				(name "VCC")
				(number "91")
			)
			(pin power_in line
				(at 7.62 -73.66 90)
				(length 3.81)
				(name "GND")
				(number "63")
			)
			(pin power_in line
				(at 10.16 68.58 270)
				(length 3.81)
				(name "VCC")
				(number "98")
			)
			(pin power_in line
				(at 10.16 -73.66 90)
				(length 3.81)
				(name "GND")
				(number "90")
			)
			(pin power_in line
				(at 12.7 -73.66 90)
				(length 3.81)
				(name "GND")
				(number "97")
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 3.81)
				(name "CAP1/QEP1/IOPA3")
				(number "57")
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 3.81)
				(name "CAP2/QEP2/IOPA4")
				(number "55")
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 3.81)
				(name "CAP3/IOPA5")
				(number "52")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 3.81)
				(name "PWM1/IOPA6")
				(number "39")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 3.81)
				(name "PWM2/IOPA7")
				(number "37")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 3.81)
				(name "PWM3/IOPB0")
				(number "36")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 3.81)
				(name "PWM4/IOPB1")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 3.81)
				(name "PWM5/IOPB2")
				(number "31")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 3.81)
				(name "PWM6/IOPB3")
				(number "28")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 3.81)
				(name "T1PWM/T1CMP/IOPB4")
				(number "12")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 3.81)
				(name "T2PWM/T2CMP/IOPB5")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 3.81)
				(name "TDIRA/IOPB6")
				(number "11")
			)
			(pin passive line
				(at 30.48 22.86 180)
				(length 3.81)
				(name "TCLKINA/IOPB7")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "CAP4/QEP3/IOPE7")
				(number "60")
			)
			(pin passive line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "CAP5/QEP4/IOPF0")
				(number "56")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "CAP6/IOPF1")
				(number "48")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 3.81)
				(name "PWM7/IOPE1")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "PWM8/IOPE2")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 3.81)
				(name "PWM9/IOPE3")
				(number "41")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "PWM10/IOPE4")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "PWM11/IOPE5")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 3.81)
				(name "PWM12/IOPE6")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "T3PWM/T3CMP/IOPF2")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 3.81)
				(name "T4PWM/T4CMP/IOPF3")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "TDIRB/IOPF4")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "TCLKINB/IOPF5")
				(number "89")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 3.81)
				(name "IOPF6")
				(number "92")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 3.81)
				(name "IOPC0")
				(number "14")
			)
			(pin input inverted_clock
				(at 30.48 -25.4 180)
				(length 3.81)
				(name "PDPINTA")
				(number "6")
			)
			(pin input inverted_clock
				(at 30.48 -27.94 180)
				(length 3.81)
				(name "PDPINTB")
				(number "95")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 3.81)
				(name "CLKOUT/IOPE0")
				(number "51")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 3.81)
				(name "XINT1/IOPA2")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 3.81)
				(name "XINT2/IOPD0")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 3.81)
				(name "BIO-/IOPC1")
				(number "85")
			)
			(pin input line
				(at 30.48 -50.8 180)
				(length 3.81)
				(name "TCK")
				(number "94")
			)
			(pin input line
				(at 30.48 -53.34 180)
				(length 3.81)
				(name "TDI")
				(number "96")
			)
			(pin input line
				(at 30.48 -55.88 180)
				(length 3.81)
				(name "TMS")
				(number "100")
			)
			(pin output line
				(at 30.48 -58.42 180)
				(length 3.81)
				(name "TDO")
				(number "99")
			)
			(pin input line
				(at 30.48 -60.96 180)
				(length 3.81)
				(name "TMS2")
				(number "25")
			)
			(pin input inverted
				(at 30.48 -63.5 180)
				(length 3.81)
				(name "TRST")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
)
