(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ABS2"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "ABS2"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_SMD:Diode_Bridge_Diotec_ABS"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/abs2.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Surface Mount Bridge Rectifiers, 140V Vrms, 0.8A If, ABS SMD package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Diotec*ABS*"
			(at 0 0 0)
		)
		(symbol "ABS2_0_1")
		(symbol "ABS2_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "+")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "B40C1500G"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B40C1500G"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.8mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88501/b40c1500g.pdf"
			(at 0 0 0)
		)
		(property "Description" "Glass Passivated Single-Phase Bridge Rectifier, 40V Vrms, 1.5A If, WOG package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.8mm*"
			(at 0 0 0)
		)
		(symbol "B40C1500G_0_1")
		(symbol "B40C1500G_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "+")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "B40C2300-1500A"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B40C2300-1500A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_19.0x3.5x10.0mm_P5.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c2300.pdf"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 40V Vrms, 1.5A If, pins=-AA+, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*19.0x3.5x10.0mm*P5.0mm*"
			(at 0 0 0)
		)
		(symbol "B40C2300-1500A_0_1")
		(symbol "B40C2300-1500A_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "+")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "B40C2300-1500B"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B40C2300-1500B"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_19.0x3.5x10.0mm_P5.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c2300.pdf"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 40V Vrms, 1.5A If, pins=-A+A, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*19.0x3.5x10.0mm*P5.0mm*"
			(at 0 0 0)
		)
		(symbol "B40C2300-1500B_0_1")
		(symbol "B40C2300-1500B_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "+")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "B40C5000-3x00A"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B40C5000-3x00A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_32.0x5.6x17.0mm_P10.0mm_P7.5mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c500033"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 40V Vrms, 3.3A If, pins=-AA+, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*32.0x5.6x17.0mm*P10.0mm*P7.5mm*"
			(at 0 0 0)
		)
		(symbol "B40C5000-3x00A_0_1")
		(symbol "B40C5000-3x00A_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "+")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "B40C800DM"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B40C800DM"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_DIP-4_W7.62mm_P5.08mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88533/800dm.pdf"
			(at 0 0 0)
		)
		(property "Description" "Glass Passivated Single-Phase Bridge Rectifier, 40V Vrms, 0.8A If, DIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*DIP*W7.62mm*P5.08mm*"
			(at 0 0 0)
		)
		(symbol "B40C800DM_0_1")
		(symbol "B40C800DM_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "+")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "B40R"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B40R"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40r.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 40V Vrms, 1.6A If, WOG-like package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.0mm*"
			(at 0 0 0)
		)
		(symbol "B40R_0_1")
		(symbol "B40R_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "+")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DF005S"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "DF005S"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_SMD:Diode_Bridge_OnSemi_SDIP-4L"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/df10s-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Bridge Rectifier, 35V Vrms, 1.5A If, SMDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*OnSemi*SDIP*4L*"
			(at 0 0 0)
		)
		(symbol "DF005S_0_1")
		(symbol "DF005S_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "+")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "GBU4A"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "GBU4A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_GBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/gbu4a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 35V Vrms, 4.0A If, GBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*GBU*"
			(at 0 0 0)
		)
		(symbol "GBU4A_0_1")
		(symbol "GBU4A_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "+")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "GUO40-08NO1"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 17.78 0)
		)
		(property "Value" "GUO40-08NO1"
			(at 0 15.24 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_IXYS_GUFP"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://ixapps.ixys.com/DataSheet/GUO40-08NO1.pdf"
			(at 0 17.78 0)
		)
		(property "Description" "250V Vrms, 40A If, GUFP(X025B)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-Phase Bridge Rectifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*IXYS*GUFP*"
			(at 0 0 0)
		)
		(symbol "GUO40-08NO1_0_1")
		(symbol "GUO40-08NO1_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "-")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KBU4A"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "KBU4A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/kbu4.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 35V Vrms, 4.0A If, KBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*KBU*"
			(at 0 0 0)
		)
		(symbol "KBU4A_0_1")
		(symbol "KBU4A_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "+")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MB2S"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "MB2S"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-269AA"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88661/mb2s.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Surface Mount Bridge Rectifiers, 140V Vrms, 0.5A If, TO-269AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?269AA*"
			(at 0 0 0)
		)
		(symbol "MB2S_0_1")
		(symbol "MB2S_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "+")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MBL104S"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "MBL104S"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_SMD:Diode_Bridge_Vishay_MBLS"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/89959/mbl104s.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Surface Mount Bridge Rectifiers, 280V Vrms, 1.0A If, MBLS SMD package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*MBLS*"
			(at 0 0 0)
		)
		(symbol "MBL104S_0_1")
		(symbol "MBL104S_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "-")
				(number "4")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "+")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MDB6S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 3.81 6.35 0)
		)
		(property "Value" "MDB6S"
			(at 6.35 3.81 0)
		)
		(property "Footprint" "Package_SO:TSSOP-4_4.4x5mm_P4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MDB8S-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 420V Vrms, 1A If, TSSOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "bridge diode rectifier ac dc acdc ac-dc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P4mm*"
			(at 0 0 0)
		)
		(symbol "MDB6S_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "+")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SC35VB80S-G"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.24 0)
		)
		(property "Value" "SC35VB80S-G"
			(at 0 12.7 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Comchip_SCVB-L"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.comchiptech.com/admin/files/product/SC35VB80S-G%20Thru506369.%20SC35VB160S-G%20RevB.pdf"
			(at 0 0 0)
		)
		(property "Description" "560V Vrms, 35A If, SCVB-L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-Phase Bridge Rectifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Comchip*SCVB?L*"
			(at 0 0 0)
		)
		(symbol "SC35VB80S-G_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "-")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VS-KBPC1005"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "VS-KBPC1005"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBPC1"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/93585/vs-kbpc1series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 20V Vrms, 3.0A If, KBPC1 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Vishay*KBPC1*"
			(at 0 0 0)
		)
		(symbol "VS-KBPC1005_0_1")
		(symbol "VS-KBPC1005_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "+")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VS-KBPC6005"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "VS-KBPC6005"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBPC6"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/93585/vs-kbpc1series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 20V Vrms, 6.0A If, KBPC6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Vishay*KBPC6*"
			(at 0 0 0)
		)
		(symbol "VS-KBPC6005_0_1")
		(symbol "VS-KBPC6005_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "+")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VS-KBPC8005"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "VS-KBPC8005"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBPC6"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/93586/kbpc8series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 20V Vrms, 8.0A If, KBPC6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Vishay*KBPC6*"
			(at 0 0 0)
		)
		(symbol "VS-KBPC8005_0_1")
		(symbol "VS-KBPC8005_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "+")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ABS10"
		(extends "ABS2")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "ABS10"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_SMD:Diode_Bridge_Diotec_ABS"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/abs2.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Surface Mount Bridge Rectifiers, 700V Vrms, 0.8A If, ABS SMD package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Diotec*ABS*"
			(at 0 0 0)
		)
	)
	(symbol "ABS4"
		(extends "ABS2")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "ABS4"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_SMD:Diode_Bridge_Diotec_ABS"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/abs2.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Surface Mount Bridge Rectifiers, 280V Vrms, 0.8A If, ABS SMD package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Diotec*ABS*"
			(at 0 0 0)
		)
	)
	(symbol "ABS6"
		(extends "ABS2")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "ABS6"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_SMD:Diode_Bridge_Diotec_ABS"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/abs2.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Surface Mount Bridge Rectifiers, 420V Vrms, 0.8A If, ABS SMD package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Diotec*ABS*"
			(at 0 0 0)
		)
	)
	(symbol "ABS8"
		(extends "ABS2")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "ABS8"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_SMD:Diode_Bridge_Diotec_ABS"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/abs2.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Surface Mount Bridge Rectifiers, 450V Vrms, 0.8A If, ABS SMD package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Diotec*ABS*"
			(at 0 0 0)
		)
	)
	(symbol "B125C1500G"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B125C1500G"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.8mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88501/b40c1500g.pdf"
			(at 0 0 0)
		)
		(property "Description" "Glass Passivated Single-Phase Bridge Rectifier, 125V Vrms, 1.5A If, WOG package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "B125C2300-1500A"
		(extends "B40C2300-1500A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B125C2300-1500A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_19.0x3.5x10.0mm_P5.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c2300.pdf"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 125V Vrms, 1.5A If, pins=-AA+, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*19.0x3.5x10.0mm*P5.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "B125C2300-1500B"
		(extends "B40C2300-1500B")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B125C2300-1500B"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_19.0x3.5x10.0mm_P5.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c2300.pdf"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 125V Vrms, 1.5A If, pins=-A+A, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*19.0x3.5x10.0mm*P5.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "B125C3x00-2200A"
		(extends "B40C5000-3x00A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B125C3x00-2200A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_32.0x5.6x17.0mm_P10.0mm_P7.5mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c3700"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 125V Vrms, 2.2A If, pins=-AA+, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*32.0x5.6x17.0mm*P10.0mm*P7.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "B125C5000-3x00A"
		(extends "B40C5000-3x00A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B125C5000-3x00A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_32.0x5.6x17.0mm_P10.0mm_P7.5mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c500033"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 125V Vrms, 3.3A If, pins=-AA+, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*32.0x5.6x17.0mm*P10.0mm*P7.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "B125C800DM"
		(extends "B40C800DM")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B125C800DM"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_DIP-4_W7.62mm_P5.08mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88533/800dm.pdf"
			(at 0 0 0)
		)
		(property "Description" "Glass Passivated Single-Phase Bridge Rectifier, 125V Vrms, 0.8A If, DIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*DIP*W7.62mm*P5.08mm*"
			(at 0 0 0)
		)
	)
	(symbol "B125R"
		(extends "B40R")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B125R"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40r.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 125V Vrms, 1.6A If, WOG-like package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "B250C1500G"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B250C1500G"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.8mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88501/b40c1500g.pdf"
			(at 0 0 0)
		)
		(property "Description" "Glass Passivated Single-Phase Bridge Rectifier, 250V Vrms, 1.5A If, WOG package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "B250C2300-1500A"
		(extends "B40C2300-1500A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B250C2300-1500A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_19.0x3.5x10.0mm_P5.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c2300.pdf"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 250V Vrms, 1.5A If, pins=-AA+, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*19.0x3.5x10.0mm*P5.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "B250C2300-1500B"
		(extends "B40C2300-1500B")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B250C2300-1500B"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_19.0x3.5x10.0mm_P5.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c2300.pdf"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 250V Vrms, 1.5A If, pins=-A+A, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*19.0x3.5x10.0mm*P5.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "B250C3x00-2200A"
		(extends "B40C5000-3x00A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B250C3x00-2200A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_32.0x5.6x17.0mm_P10.0mm_P7.5mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c3700"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 250V Vrms, 2.2A If, pins=-AA+, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*32.0x5.6x17.0mm*P10.0mm*P7.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "B250C5000-3x00A"
		(extends "B40C5000-3x00A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B250C5000-3x00A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_32.0x5.6x17.0mm_P10.0mm_P7.5mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c500033"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 250V Vrms, 3.3A If, pins=-AA+, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*32.0x5.6x17.0mm*P10.0mm*P7.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "B250C800DM"
		(extends "B40C800DM")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B250C800DM"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_DIP-4_W7.62mm_P5.08mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88533/800dm.pdf"
			(at 0 0 0)
		)
		(property "Description" "Glass Passivated Single-Phase Bridge Rectifier, 250V Vrms, 0.8A If, DIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*DIP*W7.62mm*P5.08mm*"
			(at 0 0 0)
		)
	)
	(symbol "B250R"
		(extends "B40R")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B250R"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40r.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 250V Vrms, 1.6A If, WOG-like package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "B380C1500G"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B380C1500G"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.8mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88501/b40c1500g.pdf"
			(at 0 0 0)
		)
		(property "Description" "Glass Passivated Single-Phase Bridge Rectifier, 380V Vrms, 1.5A If, WOG package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "B380C2300-1500A"
		(extends "B40C2300-1500A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B380C2300-1500A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_19.0x3.5x10.0mm_P5.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c2300.pdf"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 380V Vrms, 1.5A If, pins=-AA+, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*19.0x3.5x10.0mm*P5.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "B380C2300-1500B"
		(extends "B40C2300-1500B")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B380C2300-1500B"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_19.0x3.5x10.0mm_P5.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c2300.pdf"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 380V Vrms, 1.5A If, pins=-A+A, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*19.0x3.5x10.0mm*P5.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "B380C3x00-2200A"
		(extends "B40C5000-3x00A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B380C3x00-2200A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_32.0x5.6x17.0mm_P10.0mm_P7.5mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c3700"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 380V Vrms, 2.2A If, pins=-AA+, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*32.0x5.6x17.0mm*P10.0mm*P7.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "B380C5000-3x00A"
		(extends "B40C5000-3x00A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B380C5000-3x00A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_32.0x5.6x17.0mm_P10.0mm_P7.5mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c500033"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 380V Vrms, 3.3A If, pins=-AA+, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*32.0x5.6x17.0mm*P10.0mm*P7.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "B380C800DM"
		(extends "B40C800DM")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B380C800DM"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_DIP-4_W7.62mm_P5.08mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88533/800dm.pdf"
			(at 0 0 0)
		)
		(property "Description" "Glass Passivated Single-Phase Bridge Rectifier, 380V Vrms, 0.8A If, DIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*DIP*W7.62mm*P5.08mm*"
			(at 0 0 0)
		)
	)
	(symbol "B380R"
		(extends "B40R")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B380R"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40r.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 380V Vrms, 1.6A If, WOG-like package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "B40C3x00-2200A"
		(extends "B40C5000-3x00A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B40C3x00-2200A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_32.0x5.6x17.0mm_P10.0mm_P7.5mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c3700"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 40V Vrms, 2.2A If, pins=-AA+, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*32.0x5.6x17.0mm*P10.0mm*P7.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "B500C2300-1500A"
		(extends "B40C2300-1500A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B500C2300-1500A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_19.0x3.5x10.0mm_P5.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c2300.pdf"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 500V Vrms, 1.5A If, pins=-AA+, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*19.0x3.5x10.0mm*P5.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "B500C3x00-2200A"
		(extends "B40C5000-3x00A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B500C3x00-2200A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_32.0x5.6x17.0mm_P10.0mm_P7.5mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c3700"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 500V Vrms, 2.2A If, pins=-AA+, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*32.0x5.6x17.0mm*P10.0mm*P7.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "B500C5000-3x00A"
		(extends "B40C5000-3x00A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B500C5000-3x00A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_32.0x5.6x17.0mm_P10.0mm_P7.5mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c500033"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 500V Vrms, 3.3A If, pins=-AA+, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*32.0x5.6x17.0mm*P10.0mm*P7.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "B500R"
		(extends "B40R")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B500R"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40r.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 500V Vrms, 1.6A If, WOG-like package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "B700C2300-1500B"
		(extends "B40C2300-1500B")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B700C2300-1500B"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_19.0x3.5x10.0mm_P5.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c2300.pdf"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 500V Vrms, 1.5A If, pins=-A+A, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*19.0x3.5x10.0mm*P5.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "B80C1500G"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B80C1500G"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.8mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88501/b40c1500g.pdf"
			(at 0 0 0)
		)
		(property "Description" "Glass Passivated Single-Phase Bridge Rectifier, 80V Vrms, 1.5A If, WOG package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "B80C2300-1500A"
		(extends "B40C2300-1500A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B80C2300-1500A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_19.0x3.5x10.0mm_P5.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c2300.pdf"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 80V Vrms, 1.5A If, pins=-AA+, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*19.0x3.5x10.0mm*P5.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "B80C2300-1500B"
		(extends "B40C2300-1500B")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B80C2300-1500B"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_19.0x3.5x10.0mm_P5.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c2300.pdf"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 80V Vrms, 1.5A If, pins=-A+A, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*19.0x3.5x10.0mm*P5.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "B80C3x00-2200A"
		(extends "B40C5000-3x00A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B80C3x00-2200A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_32.0x5.6x17.0mm_P10.0mm_P7.5mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c3700"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 80V Vrms, 2.2A If, pins=-AA+, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*32.0x5.6x17.0mm*P10.0mm*P7.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "B80C5000-3x00A"
		(extends "B40C5000-3x00A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B80C5000-3x00A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_32.0x5.6x17.0mm_P10.0mm_P7.5mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40c500033"
			(at 0 0 0)
		)
		(property "Description" "Silicon Bridge Rectifier, 80V Vrms, 3.3A If, pins=-AA+, SIL-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*32.0x5.6x17.0mm*P10.0mm*P7.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "B80C800DM"
		(extends "B40C800DM")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B80C800DM"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_DIP-4_W7.62mm_P5.08mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88533/800dm.pdf"
			(at 0 0 0)
		)
		(property "Description" "Glass Passivated Single-Phase Bridge Rectifier, 80V Vrms, 0.8A If, DIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*DIP*W7.62mm*P5.08mm*"
			(at 0 0 0)
		)
	)
	(symbol "B80R"
		(extends "B40R")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "B80R"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40r.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 80V Vrms, 1.6A If, WOG-like package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "DF005M"
		(extends "B40C800DM")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "DF005M"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_DIP-4_W7.62mm_P5.08mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88571/dfm.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Bridge Rectifiers, 35V Vrms, 1.0A If, DIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*DIP*W7.62mm*P5.08mm*"
			(at 0 0 0)
		)
	)
	(symbol "DF01M"
		(extends "B40C800DM")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "DF01M"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_DIP-4_W7.62mm_P5.08mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88571/dfm.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Bridge Rectifiers, 70V Vrms, 1.0A If, DIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*DIP*W7.62mm*P5.08mm*"
			(at 0 0 0)
		)
	)
	(symbol "DF01S"
		(extends "DF005S")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "DF01S"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_SMD:Diode_Bridge_OnSemi_SDIP-4L"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/df10s-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Bridge Rectifier, 70V Vrms, 1.5A If, SMDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*OnSemi*SDIP*4L*"
			(at 0 0 0)
		)
	)
	(symbol "DF01S1"
		(extends "DF005S")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "DF01S1"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_SMD:Diode_Bridge_OnSemi_SDIP-4L"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/df10s1-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Bridge Rectifier, 70V Vrms, 1.0A If, Obsolete, SMDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*OnSemi*SDIP*4L*"
			(at 0 0 0)
		)
	)
	(symbol "DF02M"
		(extends "B40C800DM")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "DF02M"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_DIP-4_W7.62mm_P5.08mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88571/dfm.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Bridge Rectifiers, 140V Vrms, 1.0A If, DIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*DIP*W7.62mm*P5.08mm*"
			(at 0 0 0)
		)
	)
	(symbol "DF02S"
		(extends "DF005S")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "DF02S"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_SMD:Diode_Bridge_OnSemi_SDIP-4L"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/df10s-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Bridge Rectifier, 140V Vrms, 1.5A If, SMDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*OnSemi*SDIP*4L*"
			(at 0 0 0)
		)
	)
	(symbol "DF04M"
		(extends "B40C800DM")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "DF04M"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_DIP-4_W7.62mm_P5.08mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88571/dfm.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Bridge Rectifiers, 280V Vrms, 1.0A If, DIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*DIP*W7.62mm*P5.08mm*"
			(at 0 0 0)
		)
	)
	(symbol "DF04S"
		(extends "DF005S")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "DF04S"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_SMD:Diode_Bridge_OnSemi_SDIP-4L"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/df10s-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Bridge Rectifier, 280V Vrms, 1.5A If, SMDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*OnSemi*SDIP*4L*"
			(at 0 0 0)
		)
	)
	(symbol "DF06M"
		(extends "B40C800DM")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "DF06M"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_DIP-4_W7.62mm_P5.08mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88571/dfm.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Bridge Rectifiers, 420V Vrms, 1.0A If, DIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*DIP*W7.62mm*P5.08mm*"
			(at 0 0 0)
		)
	)
	(symbol "DF06S"
		(extends "DF005S")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "DF06S"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_SMD:Diode_Bridge_OnSemi_SDIP-4L"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/df10s-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Bridge Rectifier, 420V Vrms, 1.5A If, SMDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*OnSemi*SDIP*4L*"
			(at 0 0 0)
		)
	)
	(symbol "DF08M"
		(extends "B40C800DM")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "DF08M"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_DIP-4_W7.62mm_P5.08mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88571/dfm.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Bridge Rectifiers, 560V Vrms, 1.0A If, DIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*DIP*W7.62mm*P5.08mm*"
			(at 0 0 0)
		)
	)
	(symbol "DF08S"
		(extends "DF005S")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "DF08S"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_SMD:Diode_Bridge_OnSemi_SDIP-4L"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/df10s-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Bridge Rectifier, 560V Vrms, 1.5A If, SMDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*OnSemi*SDIP*4L*"
			(at 0 0 0)
		)
	)
	(symbol "DF10M"
		(extends "B40C800DM")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "DF10M"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_DIP-4_W7.62mm_P5.08mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88571/dfm.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Bridge Rectifiers, 700V Vrms, 1.0A If, DIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*DIP*W7.62mm*P5.08mm*"
			(at 0 0 0)
		)
	)
	(symbol "DF10S"
		(extends "DF005S")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "DF10S"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_SMD:Diode_Bridge_OnSemi_SDIP-4L"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.onsemi.com/download/data-sheet/pdf/df10s-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "Bridge Rectifier, 700V Vrms, 1.5A If, SMDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*OnSemi*SDIP*4L*"
			(at 0 0 0)
		)
	)
	(symbol "DMA40U1800GU"
		(extends "GUO40-08NO1")
		(property "Reference" "D"
			(at 0 17.78 0)
		)
		(property "Value" "DMA40U1800GU"
			(at 0 15.24 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_IXYS_GUFP"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://ixapps.ixys.com/Datasheet/DMA40U1800GU.pdf"
			(at 0 17.78 0)
		)
		(property "Description" "575V Vrms, 40A If, GUFP(X025B)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-Phase Bridge Rectifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*IXYS*GUFP*"
			(at 0 0 0)
		)
	)
	(symbol "DNA40U2200GU"
		(extends "GUO40-08NO1")
		(property "Reference" "D"
			(at 0 17.78 0)
		)
		(property "Value" "DNA40U2200GU"
			(at 0 15.24 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_IXYS_GUFP"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://ixapps.ixys.com/Datasheet/DNA40U2200GU.pdf"
			(at 0 17.78 0)
		)
		(property "Description" "690V Vrms, 40A If, GUFP(X025B)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-Phase Bridge Rectifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*IXYS*GUFP*"
			(at 0 0 0)
		)
	)
	(symbol "GBU4B"
		(extends "GBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "GBU4B"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_GBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/gbu4a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 70V Vrms, 4.0A If, GBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*GBU*"
			(at 0 0 0)
		)
	)
	(symbol "GBU4D"
		(extends "GBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "GBU4D"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_GBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/gbu4a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 140V Vrms, 4.0A If, GBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*GBU*"
			(at 0 0 0)
		)
	)
	(symbol "GBU4G"
		(extends "GBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "GBU4G"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_GBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/gbu4a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 280V Vrms, 4.0A If, GBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*GBU*"
			(at 0 0 0)
		)
	)
	(symbol "GBU4J"
		(extends "GBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "GBU4J"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_GBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/gbu4a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 420V Vrms, 4.0A If, GBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*GBU*"
			(at 0 0 0)
		)
	)
	(symbol "GBU4K"
		(extends "GBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "GBU4K"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_GBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/gbu4a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 560V Vrms, 4.0A If, GBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*GBU*"
			(at 0 0 0)
		)
	)
	(symbol "GBU4M"
		(extends "GBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "GBU4M"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_GBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/gbu4a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 700V Vrms, 4.0A If, GBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*GBU*"
			(at 0 0 0)
		)
	)
	(symbol "GBU6A"
		(extends "GBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "GBU6A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_GBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/gbu6a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 35V Vrms, 6.0A If, GBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*GBU*"
			(at 0 0 0)
		)
	)
	(symbol "GBU6B"
		(extends "GBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "GBU6B"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_GBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/gbu6a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 70V Vrms, 6.0A If, GBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*GBU*"
			(at 0 0 0)
		)
	)
	(symbol "GBU6D"
		(extends "GBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "GBU6D"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_GBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/gbu6a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 140V Vrms, 6.0A If, GBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*GBU*"
			(at 0 0 0)
		)
	)
	(symbol "GBU6G"
		(extends "GBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "GBU6G"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_GBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/gbu6a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 280V Vrms, 6.0A If, GBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*GBU*"
			(at 0 0 0)
		)
	)
	(symbol "GBU6J"
		(extends "GBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "GBU6J"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_GBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/gbu6a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 420V Vrms, 6.0A If, GBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*GBU*"
			(at 0 0 0)
		)
	)
	(symbol "GBU6K"
		(extends "GBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "GBU6K"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_GBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/gbu6a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 560V Vrms, 6.0A If, GBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*GBU*"
			(at 0 0 0)
		)
	)
	(symbol "GBU6M"
		(extends "GBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "GBU6M"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_GBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/gbu6a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 700V Vrms, 6.0A If, GBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*GBU*"
			(at 0 0 0)
		)
	)
	(symbol "GBU8A"
		(extends "GBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "GBU8A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_GBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/gbu8a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 35V Vrms, 8.0A If, GBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*GBU*"
			(at 0 0 0)
		)
	)
	(symbol "GBU8B"
		(extends "GBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "GBU8B"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_GBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/gbu8a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 70V Vrms, 8.0A If, GBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*GBU*"
			(at 0 0 0)
		)
	)
	(symbol "GBU8D"
		(extends "GBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "GBU8D"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_GBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/gbu8a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 140V Vrms, 8.0A If, GBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*GBU*"
			(at 0 0 0)
		)
	)
	(symbol "GBU8G"
		(extends "GBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "GBU8G"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_GBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/gbu8a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 280V Vrms, 8.0A If, GBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*GBU*"
			(at 0 0 0)
		)
	)
	(symbol "GBU8J"
		(extends "GBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "GBU8J"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_GBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/gbu8a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 420V Vrms, 8.0A If, GBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*GBU*"
			(at 0 0 0)
		)
	)
	(symbol "GBU8K"
		(extends "GBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "GBU8K"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_GBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/gbu8a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 560V Vrms, 8.0A If, GBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*GBU*"
			(at 0 0 0)
		)
	)
	(symbol "GBU8M"
		(extends "GBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "GBU8M"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_GBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/gbu8a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 700V Vrms, 8.0A If, GBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*GBU*"
			(at 0 0 0)
		)
	)
	(symbol "GUO40-12NO1"
		(extends "GUO40-08NO1")
		(property "Reference" "D"
			(at 0 17.78 0)
		)
		(property "Value" "GUO40-12NO1"
			(at 0 15.24 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_IXYS_GUFP"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://ixapps.ixys.com/DataSheet/GUO40-12NO1.pdf"
			(at 0 17.78 0)
		)
		(property "Description" "400V Vrms, 40A If, GUFP(X025B)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-Phase Bridge Rectifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*IXYS*GUFP*"
			(at 0 0 0)
		)
	)
	(symbol "GUO40-16NO1"
		(extends "GUO40-08NO1")
		(property "Reference" "D"
			(at 0 17.78 0)
		)
		(property "Value" "GUO40-16NO1"
			(at 0 15.24 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_IXYS_GUFP"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://ixapps.ixys.com/DataSheet/GUO40-16NO1.pdf"
			(at 0 17.78 0)
		)
		(property "Description" "500V Vrms, 40A If, GUFP(X025B)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-Phase Bridge Rectifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*IXYS*GUFP*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC15005T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC15005T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc15005t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 35V Vrms, 15A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC15005W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC15005W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc15005t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 35V Vrms, 15A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC1501T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC1501T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc1501t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 70V Vrms, 15A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC1501W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC1501W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc1501t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 70V Vrms, 15A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC1502T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC1502T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc1502t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 140V Vrms, 15A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC1502W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC1502W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc1502t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 140V Vrms, 15A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC1504T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC1504T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc1504t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 280V Vrms, 15A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC1504W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC1504W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc1504t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 280V Vrms, 15A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC1506T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC1506T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc1506t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 420V Vrms, 15A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC1506W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC1506W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc1506t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 420V Vrms, 15A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC1508T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC1508T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc1508t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 560V Vrms, 15A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC1508W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC1508W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc1508t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 560V Vrms, 15A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC1510T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC1510T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc1510t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 700V Vrms, 15A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC1510W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC1510W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc1510t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 700V Vrms, 15A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC25005T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC25005T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc25005t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 35V Vrms, 25A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC25005W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC25005W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc25005t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 35V Vrms, 25A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC2501T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC2501T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc2501t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 70V Vrms, 25A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC2501W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC2501W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc2501t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 70V Vrms, 25A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC2502T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC2502T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc2502t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 140V Vrms, 25A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC2502W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC2502W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc2502t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 140V Vrms, 25A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC2504T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC2504T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc2504t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 280V Vrms, 25A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC2504W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC2504W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc2504t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 280V Vrms, 25A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC2506T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC2506T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc2506t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 420V Vrms, 25A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC2506W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC2506W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc2506t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 420V Vrms, 25A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC2508T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC2508T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc2508t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 560V Vrms, 25A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC2508W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC2508W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc2508t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 560V Vrms, 25A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC2510T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC2510T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc2510t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 700V Vrms, 25A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC2510W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC2510W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc2510t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 700V Vrms, 25A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC35005T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC35005T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc35005t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 35V Vrms, 35A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC35005W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC35005W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc35005t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 35V Vrms, 35A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC3501T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC3501T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc3501t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 70V Vrms, 35A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC3501W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC3501W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc3501t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 70V Vrms, 35A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC3502T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC3502T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc3502t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 140V Vrms, 35A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC3502W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC3502W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc3502t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 140V Vrms, 35A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC3504T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC3504T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc3504t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 280V Vrms, 35A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC3504W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC3504W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc3504t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 280V Vrms, 35A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC3506T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC3506T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc3506t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 420V Vrms, 35A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC3506W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC3506W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc3506t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 420V Vrms, 35A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC3508T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC3508T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc3508t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 560V Vrms, 35A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC3508W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC3508W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc3508t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 560V Vrms, 35A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC3510T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC3510T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc3510t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 700V Vrms, 35A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC3510W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC3510W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc3510t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 700V Vrms, 35A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC50005T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC50005T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc50005t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 35V Vrms, 50A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC50005W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC50005W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc50005t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 35V Vrms, 50A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC5001T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC5001T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc5001t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 70V Vrms, 50A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC5001W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC5001W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc5001t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 70V Vrms, 50A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC5002T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC5002T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc5002t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 140V Vrms, 50A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC5002W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC5002W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc5002t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 140V Vrms, 50A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC5004T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC5004T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc5004t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 280V Vrms, 50A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC5004W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC5004W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc5004t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 280V Vrms, 50A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC5006T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC5006T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc5006t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 420V Vrms, 50A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC5006W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC5006W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc5006t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 420V Vrms, 50A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC5008T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC5008T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc5008t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 560V Vrms, 50A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC5008W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC5008W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc5008t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 560V Vrms, 50A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC5010T"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC5010T"
			(at 7.62 5.08 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc5010t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 700V Vrms, 50A If, KBPC-T(FP)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?T*"
			(at 0 0 0)
		)
	)
	(symbol "KBPC5010W"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 7.62 7.62 0)
		)
		(property "Value" "KBPC5010W"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_GeneSiC_KBPC_W"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.diodemodule.com/bridge-rectifier/kbpc/kbpc5010t.pdf"
			(at 22.86 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 700V Vrms, 50A If, KBPC-W(WS)"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode full"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*KBPC?W*"
			(at 0 0 0)
		)
	)
	(symbol "KBU4B"
		(extends "KBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "KBU4B"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/kbu4.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 70V Vrms, 4.0A If, KBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*KBU*"
			(at 0 0 0)
		)
	)
	(symbol "KBU4D"
		(extends "KBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "KBU4D"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/kbu4.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 140V Vrms, 4.0A If, KBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*KBU*"
			(at 0 0 0)
		)
	)
	(symbol "KBU4G"
		(extends "KBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "KBU4G"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/kbu4.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 280V Vrms, 4.0A If, KBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*KBU*"
			(at 0 0 0)
		)
	)
	(symbol "KBU4J"
		(extends "KBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "KBU4J"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/kbu4.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 420V Vrms, 4.0A If, KBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*KBU*"
			(at 0 0 0)
		)
	)
	(symbol "KBU4K"
		(extends "KBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "KBU4K"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/kbu4.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 560V Vrms, 4.0A If, KBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*KBU*"
			(at 0 0 0)
		)
	)
	(symbol "KBU4M"
		(extends "KBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "KBU4M"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/kbu4.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 700V Vrms, 4.0A If, KBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*KBU*"
			(at 0 0 0)
		)
	)
	(symbol "KBU6A"
		(extends "KBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "KBU6A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/kbu6.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 35V Vrms, 6.0A If, KBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*KBU*"
			(at 0 0 0)
		)
	)
	(symbol "KBU6B"
		(extends "KBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "KBU6B"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/kbu6.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 70V Vrms, 6.0A If, KBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*KBU*"
			(at 0 0 0)
		)
	)
	(symbol "KBU6D"
		(extends "KBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "KBU6D"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/kbu6.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 140V Vrms, 6.0A If, KBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*KBU*"
			(at 0 0 0)
		)
	)
	(symbol "KBU6G"
		(extends "KBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "KBU6G"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/kbu6.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 280V Vrms, 6.0A If, KBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*KBU*"
			(at 0 0 0)
		)
	)
	(symbol "KBU6J"
		(extends "KBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "KBU6J"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/kbu6.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 420V Vrms, 6.0A If, KBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*KBU*"
			(at 0 0 0)
		)
	)
	(symbol "KBU6K"
		(extends "KBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "KBU6K"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/kbu6.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 560V Vrms, 6.0A If, KBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*KBU*"
			(at 0 0 0)
		)
	)
	(symbol "KBU6M"
		(extends "KBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "KBU6M"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/kbu6.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 700V Vrms, 6.0A If, KBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*KBU*"
			(at 0 0 0)
		)
	)
	(symbol "KBU8A"
		(extends "KBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "KBU8A"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/kbu8.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 35V Vrms, 8.0A If, KBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*KBU*"
			(at 0 0 0)
		)
	)
	(symbol "KBU8B"
		(extends "KBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "KBU8B"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/kbu8.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 70V Vrms, 8.0A If, KBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*KBU*"
			(at 0 0 0)
		)
	)
	(symbol "KBU8D"
		(extends "KBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "KBU8D"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/kbu8.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 140V Vrms, 8.0A If, KBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*KBU*"
			(at 0 0 0)
		)
	)
	(symbol "KBU8G"
		(extends "KBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "KBU8G"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/kbu8.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 280V Vrms, 8.0A If, KBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*KBU*"
			(at 0 0 0)
		)
	)
	(symbol "KBU8J"
		(extends "KBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "KBU8J"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/kbu8.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 420V Vrms, 8.0A If, KBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*KBU*"
			(at 0 0 0)
		)
	)
	(symbol "KBU8K"
		(extends "KBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "KBU8K"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/kbu8.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 560V Vrms, 8.0A If, KBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*KBU*"
			(at 0 0 0)
		)
	)
	(symbol "KBU8M"
		(extends "KBU4A")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "KBU8M"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBU"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88656/kbu8.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 700V Vrms, 8.0A If, KBU package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*KBU*"
			(at 0 0 0)
		)
	)
	(symbol "MB4S"
		(extends "MB2S")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "MB4S"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-269AA"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88661/mb2s.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Surface Mount Bridge Rectifiers, 280V Vrms, 0.5A If, TO-269AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?269AA*"
			(at 0 0 0)
		)
	)
	(symbol "MB6S"
		(extends "MB2S")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "MB6S"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-269AA"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88573/dfs.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Surface Mount Bridge Rectifiers, 700V Vrms, 1.0A If, DFS SMD package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?269AA*"
			(at 0 0 0)
		)
	)
	(symbol "MBL106S"
		(extends "MBL104S")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "MBL106S"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_SMD:Diode_Bridge_Vishay_MBLS"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/89959/mbl104s.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Surface Mount Bridge Rectifiers, 420V Vrms, 1.0A If, MBLS SMD package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*MBLS*"
			(at 0 0 0)
		)
	)
	(symbol "MBL108S"
		(extends "MBL104S")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "MBL108S"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_SMD:Diode_Bridge_Vishay_MBLS"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/89959/mbl104s.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Surface Mount Bridge Rectifiers, 560V Vrms, 1.0A If, MBLS SMD package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*MBLS*"
			(at 0 0 0)
		)
	)
	(symbol "MBL110S"
		(extends "MBL104S")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "MBL110S"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_SMD:Diode_Bridge_Vishay_MBLS"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/89959/mbl104s.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Surface Mount Bridge Rectifiers, 700V Vrms, 1.0A If, MBLS SMD package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Vishay*MBLS*"
			(at 0 0 0)
		)
	)
	(symbol "MDB10S"
		(extends "MDB6S")
		(property "Reference" "D"
			(at 3.81 6.35 0)
		)
		(property "Value" "MDB10S"
			(at 6.35 3.81 0)
		)
		(property "Footprint" "Package_SO:TSSOP-4_4.4x5mm_P4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MDB8S-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 700V Vrms, 1A If, TSSOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "bridge diode rectifier ac dc acdc ac-dc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MDB8S"
		(extends "MDB6S")
		(property "Reference" "D"
			(at 3.81 6.35 0)
		)
		(property "Value" "MDB8S"
			(at 6.35 3.81 0)
		)
		(property "Footprint" "Package_SO:TSSOP-4_4.4x5mm_P4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MDB8S-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 560V Vrms, 1A If, TSSOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "bridge diode rectifier ac dc acdc ac-dc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P4mm*"
			(at 0 0 0)
		)
	)
	(symbol "RB151"
		(extends "B40R")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "RB151"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.rectron.com/public/product_datasheets/rb151-rb157.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 35V Vrms, 1.5A If, WOG-like package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "RB152"
		(extends "B40R")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "RB152"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.rectron.com/public/product_datasheets/rb151-rb157.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 70V Vrms, 1.5A If, WOG-like package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "RB153"
		(extends "B40R")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "RB153"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.rectron.com/public/product_datasheets/rb151-rb157.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 140V Vrms, 1.5A If, WOG-like package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "RB154"
		(extends "B40R")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "RB154"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.rectron.com/public/product_datasheets/rb151-rb157.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 280V Vrms, 1.5A If, WOG-like package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "RB155"
		(extends "B40R")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "RB155"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.rectron.com/public/product_datasheets/rb151-rb157.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 420V Vrms, 1.5A If, WOG-like package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "RB156"
		(extends "B40R")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "RB156"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.rectron.com/public/product_datasheets/rb151-rb157.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 560V Vrms, 1.5A If, WOG-like package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "RB157"
		(extends "B40R")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "RB157"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.0mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.rectron.com/public/product_datasheets/rb151-rb157.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 700V Vrms, 1.5A If, WOG-like package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "RMB2S"
		(extends "MB2S")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "RMB2S"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-269AA"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88705/rmbs.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Surface Mount Bridge Rectifiers, 140V Vrms, 0.5A If, TO-269AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?269AA*"
			(at 0 0 0)
		)
	)
	(symbol "RMB4S"
		(extends "MB2S")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "RMB4S"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-269AA"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/88705/rmbs.pdf"
			(at 0 0 0)
		)
		(property "Description" "Miniature Glass Passivated Single-Phase Surface Mount Bridge Rectifiers, 280V Vrms, 0.5A If, TO-269AA"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?269AA*"
			(at 0 0 0)
		)
	)
	(symbol "SC35VB160S-G"
		(extends "SC35VB80S-G")
		(property "Reference" "U"
			(at 0 15.24 0)
		)
		(property "Value" "SC35VB160S-G"
			(at 0 12.7 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Comchip_SCVB-L"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.comchiptech.com/admin/files/product/SC35VB80S-G%20Thru506369.%20SC35VB160S-G%20RevB.pdf"
			(at 0 0 0)
		)
		(property "Description" "1120V Vrms, 35A If, SCVB-L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Three-Phase Bridge Rectifier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diode*Bridge*Comchip*SCVB?L*"
			(at 0 0 0)
		)
	)
	(symbol "VS-KBPC101"
		(extends "VS-KBPC1005")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "VS-KBPC101"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBPC1"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/93585/vs-kbpc1series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 40V Vrms, 3.0A If, KBPC1 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Vishay*KBPC1*"
			(at 0 0 0)
		)
	)
	(symbol "VS-KBPC102"
		(extends "VS-KBPC1005")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "VS-KBPC102"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBPC1"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/93585/vs-kbpc1series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 80V Vrms, 3.0A If, KBPC1 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Vishay*KBPC1*"
			(at 0 0 0)
		)
	)
	(symbol "VS-KBPC104"
		(extends "VS-KBPC1005")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "VS-KBPC104"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBPC1"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/93585/vs-kbpc1series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 125V Vrms, 3.0A If, KBPC1 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Vishay*KBPC1*"
			(at 0 0 0)
		)
	)
	(symbol "VS-KBPC106"
		(extends "VS-KBPC1005")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "VS-KBPC106"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBPC1"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/93585/vs-kbpc1series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 250V Vrms, 3.0A If, KBPC1 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Vishay*KBPC1*"
			(at 0 0 0)
		)
	)
	(symbol "VS-KBPC108"
		(extends "VS-KBPC1005")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "VS-KBPC108"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBPC1"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/93585/vs-kbpc1series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 380V Vrms, 3.0A If, KBPC1 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Vishay*KBPC1*"
			(at 0 0 0)
		)
	)
	(symbol "VS-KBPC110"
		(extends "VS-KBPC1005")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "VS-KBPC110"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBPC1"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/93585/vs-kbpc1series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 500V Vrms, 3.0A If, KBPC1 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Vishay*KBPC1*"
			(at 0 0 0)
		)
	)
	(symbol "VS-KBPC601"
		(extends "VS-KBPC6005")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "VS-KBPC601"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBPC6"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/93585/vs-kbpc1series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 40V Vrms, 6.0A If, KBPC6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Vishay*KBPC6*"
			(at 0 0 0)
		)
	)
	(symbol "VS-KBPC602"
		(extends "VS-KBPC6005")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "VS-KBPC602"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBPC6"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/93585/vs-kbpc1series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 80V Vrms, 6.0A If, KBPC6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Vishay*KBPC6*"
			(at 0 0 0)
		)
	)
	(symbol "VS-KBPC604"
		(extends "VS-KBPC6005")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "VS-KBPC604"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBPC6"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/93585/vs-kbpc1series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 125V Vrms, 6.0A If, KBPC6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Vishay*KBPC6*"
			(at 0 0 0)
		)
	)
	(symbol "VS-KBPC606"
		(extends "VS-KBPC6005")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "VS-KBPC606"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBPC6"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/93585/vs-kbpc1series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 250V Vrms, 6.0A If, KBPC6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Vishay*KBPC6*"
			(at 0 0 0)
		)
	)
	(symbol "VS-KBPC608"
		(extends "VS-KBPC6005")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "VS-KBPC608"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBPC6"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/93585/vs-kbpc1series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 380V Vrms, 6.0A If, KBPC6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Vishay*KBPC6*"
			(at 0 0 0)
		)
	)
	(symbol "VS-KBPC610"
		(extends "VS-KBPC6005")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "VS-KBPC610"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBPC6"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/93585/vs-kbpc1series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 500V Vrms, 6.0A If, KBPC6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Vishay*KBPC6*"
			(at 0 0 0)
		)
	)
	(symbol "VS-KBPC801"
		(extends "VS-KBPC8005")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "VS-KBPC801"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBPC6"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/93586/kbpc8series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 40V Vrms, 8.0A If, KBPC6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Vishay*KBPC6*"
			(at 0 0 0)
		)
	)
	(symbol "VS-KBPC802"
		(extends "VS-KBPC8005")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "VS-KBPC802"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBPC6"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/93586/kbpc8series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 80V Vrms, 8.0A If, KBPC6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Vishay*KBPC6*"
			(at 0 0 0)
		)
	)
	(symbol "VS-KBPC804"
		(extends "VS-KBPC8005")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "VS-KBPC804"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBPC6"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/93586/kbpc8series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 125V Vrms, 8.0A If, KBPC6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Vishay*KBPC6*"
			(at 0 0 0)
		)
	)
	(symbol "VS-KBPC806"
		(extends "VS-KBPC8005")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "VS-KBPC806"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBPC6"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/93586/kbpc8series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 250V Vrms, 8.0A If, KBPC6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Vishay*KBPC6*"
			(at 0 0 0)
		)
	)
	(symbol "VS-KBPC808"
		(extends "VS-KBPC8005")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "VS-KBPC808"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBPC6"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/93586/kbpc8series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 380V Vrms, 8.0A If, KBPC6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Vishay*KBPC6*"
			(at 0 0 0)
		)
	)
	(symbol "VS-KBPC810"
		(extends "VS-KBPC8005")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "VS-KBPC810"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Vishay_KBPC6"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/93586/kbpc8series.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Phase Bridge Rectifier, 500V Vrms, 8.0A If, KBPC6 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Vishay*KBPC6*"
			(at 0 0 0)
		)
	)
	(symbol "W005G"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "W005G"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.8mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88769/woo5g.pdf"
			(at 0 0 0)
		)
		(property "Description" "Glass Passivated Single-Phase Bridge Rectifier, 35V Vrms, 1.5A If, WOG package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bridge Rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "W01G"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "W01G"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.8mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88769/woo5g.pdf"
			(at 0 0 0)
		)
		(property "Description" "Glass Passivated Single-Phase Bridge Rectifier, 70V Vrms, 1.5A If, WOG package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bridge Rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "W02G"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "W02G"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.8mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88769/woo5g.pdf"
			(at 0 0 0)
		)
		(property "Description" "Glass Passivated Single-Phase Bridge Rectifier, 140V Vrms, 1.5A If, WOG package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bridge Rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "W04G"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "W04G"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.8mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88769/woo5g.pdf"
			(at 0 0 0)
		)
		(property "Description" "Glass Passivated Single-Phase Bridge Rectifier, 280V Vrms, 1.5A If, WOG package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bridge Rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "W06G"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "W06G"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.8mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88769/woo5g.pdf"
			(at 0 0 0)
		)
		(property "Description" "Glass Passivated Single-Phase Bridge Rectifier, 420V Vrms, 1.5A If, WOG package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bridge Rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "W08G"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "W08G"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.8mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88769/woo5g.pdf"
			(at 0 0 0)
		)
		(property "Description" "Glass Passivated Single-Phase Bridge Rectifier, 560V Vrms, 1.5A If, WOG package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bridge Rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "W10G"
		(extends "B40C1500G")
		(property "Reference" "D"
			(at 2.54 6.985 0)
		)
		(property "Value" "W10G"
			(at 2.54 5.08 0)
		)
		(property "Footprint" "Diode_THT:Diode_Bridge_Round_D9.8mm"
			(at 3.81 3.175 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/88769/woo5g.pdf"
			(at 0 0 0)
		)
		(property "Description" "Glass Passivated Single-Phase Bridge Rectifier, 700V Vrms, 1.5A If, WOG package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bridge Rectifier acdc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D*Bridge*Round*D9.8mm*"
			(at 0 0 0)
		)
	)
)
