(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AD-121F2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at -21.59 21.59 0)
		)
		(property "Value" "AD-121F2"
			(at -21.59 19.05 0)
		)
		(property "Footprint" "Display_7Segment:AD-121F2"
			(at -21.59 24.13 0)
		)
		(property "Datasheet" "http://usasyck.com/products/AD-121F2_cat_e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Digit 7-segment RGB LED Display, 1-inch digit height, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display RGB LED digit 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AD*121F2*"
			(at 0 0 0)
		)
		(symbol "AD-121F2_0_1"
			(text "e"
				(at -7.0866 -6.223 0)
			)
			(text "f"
				(at -5.3594 6.223 0)
			)
			(text "d"
				(at -1.7526 -12.446 0)
			)
			(text "g"
				(at 0 0 0)
			)
			(text "a"
				(at 1.7526 12.446 0)
			)
			(text "c"
				(at 5.3594 -6.223 0)
			)
			(text "b"
				(at 7.0866 6.223 0)
			)
			(pin passive line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "anode")
				(number "17")
			)
			(pin passive line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "a-red")
				(number "23")
			)
			(pin passive line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "a-green")
				(number "22")
			)
			(pin passive line
				(at -25.4 0 0)
				(length 3.81)
				(name "a-blue")
				(number "21")
			)
			(pin passive line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "b-red")
				(number "25")
			)
			(pin passive line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "b-green")
				(number "16")
			)
			(pin passive line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "b-blue")
				(number "24")
			)
			(pin passive line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "c-red")
				(number "6")
			)
			(pin passive line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "c-green")
				(number "11")
			)
			(pin passive line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "c-blue")
				(number "5")
			)
			(pin passive line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "d-red")
				(number "4")
			)
			(pin passive line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "d-green")
				(number "3")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "d-blue")
				(number "2")
			)
			(pin passive line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "e-red")
				(number "10")
			)
			(pin passive line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "e-green")
				(number "1")
			)
			(pin passive line
				(at 25.4 0 180)
				(length 3.81)
				(name "e-blue")
				(number "9")
			)
			(pin passive line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "f-red")
				(number "14")
			)
			(pin passive line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "f-green")
				(number "13")
			)
			(pin passive line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "f-blue")
				(number "18")
			)
			(pin passive line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "g-red")
				(number "20")
			)
			(pin passive line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "g-green")
				(number "15")
			)
			(pin passive line
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "g-blue")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CA56-12CGKWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 13.97 0)
		)
		(property "Value" "CA56-12CGKWA"
			(at 17.78 13.97 0)
		)
		(property "Footprint" "Display_7Segment:CA56-12CGKWA"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/CA56-12CGKWA(Ver.9A).pdf"
			(at -10.922 0.762 0)
		)
		(property "Description" "4 digit 7 segment Green LED, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*CA56*12CGKWA*"
			(at 0 0 0)
		)
		(symbol "CA56-12CGKWA_0_0"
			(text "e"
				(at -21.336 -1.524 0)
			)
			(text "f"
				(at -19.558 3.048 0)
			)
			(text "d"
				(at -17.78 -2.794 0)
			)
			(text "g"
				(at -16.51 1.524 0)
			)
			(text "a"
				(at -15.24 6.35 0)
			)
			(text "DP1"
				(at -13.716 -6.35 0)
			)
			(text "c"
				(at -13.208 -1.778 0)
			)
			(text "b"
				(at -12.192 2.794 0)
			)
			(text "DP2"
				(at -2.286 -6.35 0)
			)
			(text "DP3"
				(at 7.62 -6.35 0)
			)
			(text "DP4"
				(at 17.78 -6.096 0)
			)
		)
		(symbol "CA56-12CGKWA_0_1")
		(symbol "CA56-12CGKWA_1_0")
		(symbol "CA56-12CGKWA_1_1"
			(pin input line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "a")
				(number "11")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "b")
				(number "7")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "c")
				(number "4")
			)
			(pin input line
				(at -27.94 0 0)
				(length 2.54)
				(name "d")
				(number "2")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "e")
				(number "1")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "f")
				(number "10")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "g")
				(number "5")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "DPX")
				(number "3")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "CA1")
				(number "12")
			)
			(pin input line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "CA2")
				(number "9")
			)
			(pin input line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "CA3")
				(number "8")
			)
			(pin input line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "CA4")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CA56-12EWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 13.97 0)
		)
		(property "Value" "CA56-12EWA"
			(at 19.05 13.97 0)
		)
		(property "Footprint" "Display_7Segment:CA56-12EWA"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/CA56-12EWA.pdf"
			(at -10.922 0.762 0)
		)
		(property "Description" "4 digit 7 segment high efficiency red LED, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*CA56*12EWA*"
			(at 0 0 0)
		)
		(symbol "CA56-12EWA_0_0"
			(text "e"
				(at -21.336 -1.524 0)
			)
			(text "f"
				(at -19.558 3.048 0)
			)
			(text "d"
				(at -17.78 -2.794 0)
			)
			(text "g"
				(at -16.51 1.524 0)
			)
			(text "a"
				(at -15.24 6.35 0)
			)
			(text "DP1"
				(at -13.716 -6.35 0)
			)
			(text "c"
				(at -13.208 -1.778 0)
			)
			(text "b"
				(at -12.192 2.794 0)
			)
			(text "DP2"
				(at -2.286 -6.35 0)
			)
			(text "DP3"
				(at 7.62 -6.35 0)
			)
			(text "DP4"
				(at 17.78 -6.096 0)
			)
		)
		(symbol "CA56-12EWA_0_1")
		(symbol "CA56-12EWA_1_0")
		(symbol "CA56-12EWA_1_1"
			(pin input line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "a")
				(number "11")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "b")
				(number "7")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "c")
				(number "4")
			)
			(pin input line
				(at -27.94 0 0)
				(length 2.54)
				(name "d")
				(number "2")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "e")
				(number "1")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "f")
				(number "10")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "g")
				(number "5")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "DPX")
				(number "3")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "CA1")
				(number "12")
			)
			(pin input line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "CA2")
				(number "9")
			)
			(pin input line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "CA3")
				(number "8")
			)
			(pin input line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "CA4")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CA56-12SEKWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 13.97 0)
		)
		(property "Value" "CA56-12SEKWA"
			(at 17.78 13.97 0)
		)
		(property "Footprint" "Display_7Segment:CA56-12SEKWA"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/CA56-12SEKWA(Ver.7A).pdf"
			(at -10.922 0.762 0)
		)
		(property "Description" "4 digit 7 segment super bright orange LED, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*CA56*12SEKWA*"
			(at 0 0 0)
		)
		(symbol "CA56-12SEKWA_0_0"
			(text "e"
				(at -21.336 -1.524 0)
			)
			(text "f"
				(at -19.558 3.048 0)
			)
			(text "d"
				(at -17.78 -2.794 0)
			)
			(text "g"
				(at -16.51 1.524 0)
			)
			(text "a"
				(at -15.24 6.35 0)
			)
			(text "DP1"
				(at -13.716 -6.35 0)
			)
			(text "c"
				(at -13.208 -1.778 0)
			)
			(text "b"
				(at -12.192 2.794 0)
			)
			(text "DP2"
				(at -2.286 -6.35 0)
			)
			(text "DP3"
				(at 7.62 -6.35 0)
			)
			(text "DP4"
				(at 17.78 -6.096 0)
			)
		)
		(symbol "CA56-12SEKWA_0_1")
		(symbol "CA56-12SEKWA_1_0")
		(symbol "CA56-12SEKWA_1_1"
			(pin input line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "a")
				(number "11")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "b")
				(number "7")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "c")
				(number "4")
			)
			(pin input line
				(at -27.94 0 0)
				(length 2.54)
				(name "d")
				(number "2")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "e")
				(number "1")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "f")
				(number "10")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "g")
				(number "5")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "DPX")
				(number "3")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "CA1")
				(number "12")
			)
			(pin input line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "CA2")
				(number "9")
			)
			(pin input line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "CA3")
				(number "8")
			)
			(pin input line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "CA4")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CA56-12SRWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 13.97 0)
		)
		(property "Value" "CA56-12SRWA"
			(at 17.78 13.97 0)
		)
		(property "Footprint" "Display_7Segment:CA56-12SRWA"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/CA56-12SRWA.pdf"
			(at -10.922 0.762 0)
		)
		(property "Description" "4 digit 7 segment super bright red LED, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*CA56*12SRWA*"
			(at 0 0 0)
		)
		(symbol "CA56-12SRWA_0_0"
			(text "e"
				(at -21.336 -1.524 0)
			)
			(text "f"
				(at -19.558 3.048 0)
			)
			(text "d"
				(at -17.78 -2.794 0)
			)
			(text "g"
				(at -16.51 1.524 0)
			)
			(text "a"
				(at -15.24 6.35 0)
			)
			(text "DP1"
				(at -13.716 -6.35 0)
			)
			(text "c"
				(at -13.208 -1.778 0)
			)
			(text "b"
				(at -12.192 2.794 0)
			)
			(text "DP2"
				(at -2.286 -6.35 0)
			)
			(text "DP3"
				(at 7.62 -6.35 0)
			)
			(text "DP4"
				(at 17.78 -6.096 0)
			)
		)
		(symbol "CA56-12SRWA_0_1")
		(symbol "CA56-12SRWA_1_0")
		(symbol "CA56-12SRWA_1_1"
			(pin input line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "a")
				(number "11")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "b")
				(number "7")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "c")
				(number "4")
			)
			(pin input line
				(at -27.94 0 0)
				(length 2.54)
				(name "d")
				(number "2")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "e")
				(number "1")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "f")
				(number "10")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "g")
				(number "5")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "DPX")
				(number "3")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "CA1")
				(number "12")
			)
			(pin input line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "CA2")
				(number "9")
			)
			(pin input line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "CA3")
				(number "8")
			)
			(pin input line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "CA4")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CA56-12SURKWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 13.97 0)
		)
		(property "Value" "CA56-12SURKWA"
			(at 17.78 13.97 0)
		)
		(property "Footprint" "Display_7Segment:CA56-12SURKWA"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/CA56-12SURKWA(Ver.8A).pdf"
			(at -10.922 0.762 0)
		)
		(property "Description" "4 digit 7 segment hyper red LED, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*CA56*12SURKWA*"
			(at 0 0 0)
		)
		(symbol "CA56-12SURKWA_0_0"
			(text "e"
				(at -21.336 -1.524 0)
			)
			(text "f"
				(at -19.558 3.048 0)
			)
			(text "d"
				(at -17.78 -2.794 0)
			)
			(text "g"
				(at -16.51 1.524 0)
			)
			(text "a"
				(at -15.24 6.35 0)
			)
			(text "DP1"
				(at -13.716 -6.35 0)
			)
			(text "c"
				(at -13.208 -1.778 0)
			)
			(text "b"
				(at -12.192 2.794 0)
			)
			(text "DP2"
				(at -2.286 -6.35 0)
			)
			(text "DP3"
				(at 7.62 -6.35 0)
			)
			(text "DP4"
				(at 17.78 -6.096 0)
			)
		)
		(symbol "CA56-12SURKWA_0_1")
		(symbol "CA56-12SURKWA_1_0")
		(symbol "CA56-12SURKWA_1_1"
			(pin input line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "a")
				(number "11")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "b")
				(number "7")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "c")
				(number "4")
			)
			(pin input line
				(at -27.94 0 0)
				(length 2.54)
				(name "d")
				(number "2")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "e")
				(number "1")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "f")
				(number "10")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "g")
				(number "5")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "DPX")
				(number "3")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "CA1")
				(number "12")
			)
			(pin input line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "CA2")
				(number "9")
			)
			(pin input line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "CA3")
				(number "8")
			)
			(pin input line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "CA4")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CA56-12SYKWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 13.97 0)
		)
		(property "Value" "CA56-12SYKWA"
			(at 17.78 13.97 0)
		)
		(property "Footprint" "Display_7Segment:CA56-12SYKWA"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/CA56-12SYKWA(Ver.6A).pdf"
			(at -10.922 0.762 0)
		)
		(property "Description" "4 digit 7 segment super bright yellow LED, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*CA56*12SYKWA*"
			(at 0 0 0)
		)
		(symbol "CA56-12SYKWA_0_0"
			(text "e"
				(at -21.336 -1.524 0)
			)
			(text "f"
				(at -19.558 3.048 0)
			)
			(text "d"
				(at -17.78 -2.794 0)
			)
			(text "g"
				(at -16.51 1.524 0)
			)
			(text "a"
				(at -15.24 6.35 0)
			)
			(text "DP1"
				(at -13.716 -6.35 0)
			)
			(text "c"
				(at -13.208 -1.778 0)
			)
			(text "b"
				(at -12.192 2.794 0)
			)
			(text "DP2"
				(at -2.286 -6.35 0)
			)
			(text "DP3"
				(at 7.62 -6.35 0)
			)
			(text "DP4"
				(at 17.78 -6.096 0)
			)
		)
		(symbol "CA56-12SYKWA_0_1")
		(symbol "CA56-12SYKWA_1_0")
		(symbol "CA56-12SYKWA_1_1"
			(pin input line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "a")
				(number "11")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "b")
				(number "7")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "c")
				(number "4")
			)
			(pin input line
				(at -27.94 0 0)
				(length 2.54)
				(name "d")
				(number "2")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "e")
				(number "1")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "f")
				(number "10")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "g")
				(number "5")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "DPX")
				(number "3")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "CA1")
				(number "12")
			)
			(pin input line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "CA2")
				(number "9")
			)
			(pin input line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "CA3")
				(number "8")
			)
			(pin input line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "CA4")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CC56-12CGKWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 13.97 0)
		)
		(property "Value" "CC56-12CGKWA"
			(at 17.78 13.97 0)
		)
		(property "Footprint" "Display_7Segment:CA56-12CGKWA"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/CC56-12CGKWA(Ver.8A).pdf"
			(at -10.922 0.762 0)
		)
		(property "Description" "4 digit 7 segment green LED, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*CA56*12CGKWA*"
			(at 0 0 0)
		)
		(symbol "CC56-12CGKWA_0_0"
			(text "e"
				(at -21.336 -1.524 0)
			)
			(text "f"
				(at -19.558 3.048 0)
			)
			(text "d"
				(at -17.78 -2.794 0)
			)
			(text "g"
				(at -16.51 1.524 0)
			)
			(text "a"
				(at -15.24 6.35 0)
			)
			(text "DP1"
				(at -13.716 -6.35 0)
			)
			(text "c"
				(at -13.208 -1.778 0)
			)
			(text "b"
				(at -12.192 2.794 0)
			)
			(text "DP2"
				(at -2.286 -6.35 0)
			)
			(text "DP3"
				(at 7.62 -6.35 0)
			)
			(text "DP4"
				(at 17.78 -6.096 0)
			)
		)
		(symbol "CC56-12CGKWA_0_1")
		(symbol "CC56-12CGKWA_1_0")
		(symbol "CC56-12CGKWA_1_1"
			(pin input line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "a")
				(number "11")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "b")
				(number "7")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "c")
				(number "4")
			)
			(pin input line
				(at -27.94 0 0)
				(length 2.54)
				(name "d")
				(number "2")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "e")
				(number "1")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "f")
				(number "10")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "g")
				(number "5")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "DPX")
				(number "3")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "CC1")
				(number "12")
			)
			(pin input line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "CC2")
				(number "9")
			)
			(pin input line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "CC3")
				(number "8")
			)
			(pin input line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "CC4")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CC56-12EWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 13.97 0)
		)
		(property "Value" "CC56-12EWA"
			(at 19.05 13.97 0)
		)
		(property "Footprint" "Display_7Segment:CA56-12EWA"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/CA56-12EWA.pdf"
			(at -10.922 0.762 0)
		)
		(property "Description" "4 digit 7 segment high efficiency red LED, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*CA56*12EWA*"
			(at 0 0 0)
		)
		(symbol "CC56-12EWA_0_0"
			(text "e"
				(at -21.336 -1.524 0)
			)
			(text "f"
				(at -19.558 3.048 0)
			)
			(text "d"
				(at -17.78 -2.794 0)
			)
			(text "g"
				(at -16.51 1.524 0)
			)
			(text "a"
				(at -15.24 6.35 0)
			)
			(text "DP1"
				(at -13.716 -6.35 0)
			)
			(text "c"
				(at -13.208 -1.778 0)
			)
			(text "b"
				(at -12.192 2.794 0)
			)
			(text "DP2"
				(at -2.286 -6.35 0)
			)
			(text "DP3"
				(at 7.62 -6.35 0)
			)
			(text "DP4"
				(at 17.78 -6.096 0)
			)
		)
		(symbol "CC56-12EWA_0_1")
		(symbol "CC56-12EWA_1_0")
		(symbol "CC56-12EWA_1_1"
			(pin input line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "a")
				(number "11")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "b")
				(number "7")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "c")
				(number "4")
			)
			(pin input line
				(at -27.94 0 0)
				(length 2.54)
				(name "d")
				(number "2")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "e")
				(number "1")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "f")
				(number "10")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "g")
				(number "5")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "DPX")
				(number "3")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "CC1")
				(number "12")
			)
			(pin input line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "CC2")
				(number "9")
			)
			(pin input line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "CC3")
				(number "8")
			)
			(pin input line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "CC4")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CC56-12GWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 13.97 0)
		)
		(property "Value" "CC56-12GWA"
			(at 19.05 13.97 0)
		)
		(property "Footprint" "Display_7Segment:CC56-12GWA"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/CC56-12GWA.pdf"
			(at -10.922 0.762 0)
		)
		(property "Description" "4 digit 7 segment green LED, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CC56?12GWA*"
			(at 0 0 0)
		)
		(symbol "CC56-12GWA_0_0"
			(text "e"
				(at -21.336 -1.524 0)
			)
			(text "f"
				(at -19.558 3.048 0)
			)
			(text "d"
				(at -17.78 -2.794 0)
			)
			(text "g"
				(at -16.51 1.524 0)
			)
			(text "a"
				(at -15.24 6.35 0)
			)
			(text "DP1"
				(at -13.716 -6.35 0)
			)
			(text "c"
				(at -13.208 -1.778 0)
			)
			(text "b"
				(at -12.192 2.794 0)
			)
			(text "DP2"
				(at -2.286 -6.35 0)
			)
			(text "DP3"
				(at 7.62 -6.35 0)
			)
			(text "DP4"
				(at 17.78 -6.096 0)
			)
		)
		(symbol "CC56-12GWA_0_1")
		(symbol "CC56-12GWA_1_0")
		(symbol "CC56-12GWA_1_1"
			(pin input line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "a")
				(number "11")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "b")
				(number "7")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "c")
				(number "4")
			)
			(pin input line
				(at -27.94 0 0)
				(length 2.54)
				(name "d")
				(number "2")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "e")
				(number "1")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "f")
				(number "10")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "g")
				(number "5")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "DPX")
				(number "3")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "CC1")
				(number "12")
			)
			(pin input line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "CC2")
				(number "9")
			)
			(pin input line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "CC3")
				(number "8")
			)
			(pin input line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "CC4")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CC56-12SEKWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 13.97 0)
		)
		(property "Value" "CC56-12SEKWA"
			(at 17.78 13.97 0)
		)
		(property "Footprint" "Display_7Segment:CA56-12SEKWA"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/CC56-12SEKWA(Ver.7A).pdf"
			(at -10.922 0.762 0)
		)
		(property "Description" "4 digit 7 segment super bright orange LED, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*CA56*12SEKWA*"
			(at 0 0 0)
		)
		(symbol "CC56-12SEKWA_0_0"
			(text "e"
				(at -21.336 -1.524 0)
			)
			(text "f"
				(at -19.558 3.048 0)
			)
			(text "d"
				(at -17.78 -2.794 0)
			)
			(text "g"
				(at -16.51 1.524 0)
			)
			(text "a"
				(at -15.24 6.35 0)
			)
			(text "DP1"
				(at -13.716 -6.35 0)
			)
			(text "c"
				(at -13.208 -1.778 0)
			)
			(text "b"
				(at -12.192 2.794 0)
			)
			(text "DP2"
				(at -2.286 -6.35 0)
			)
			(text "DP3"
				(at 7.62 -6.35 0)
			)
			(text "DP4"
				(at 17.78 -6.096 0)
			)
		)
		(symbol "CC56-12SEKWA_0_1")
		(symbol "CC56-12SEKWA_1_0")
		(symbol "CC56-12SEKWA_1_1"
			(pin input line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "a")
				(number "11")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "b")
				(number "7")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "c")
				(number "4")
			)
			(pin input line
				(at -27.94 0 0)
				(length 2.54)
				(name "d")
				(number "2")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "e")
				(number "1")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "f")
				(number "10")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "g")
				(number "5")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "DPX")
				(number "3")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "CC1")
				(number "12")
			)
			(pin input line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "CC2")
				(number "9")
			)
			(pin input line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "CC3")
				(number "8")
			)
			(pin input line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "CC4")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CC56-12SRWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 13.97 0)
		)
		(property "Value" "CC56-12SRWA"
			(at 17.78 13.97 0)
		)
		(property "Footprint" "Display_7Segment:CA56-12SRWA"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/CC56-12SRWA.pdf"
			(at -10.922 0.762 0)
		)
		(property "Description" "4 digit 7 segment super bright red LED, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*CA56*12SRWA*"
			(at 0 0 0)
		)
		(symbol "CC56-12SRWA_0_0"
			(text "e"
				(at -21.336 -1.524 0)
			)
			(text "f"
				(at -19.558 3.048 0)
			)
			(text "d"
				(at -17.78 -2.794 0)
			)
			(text "g"
				(at -16.51 1.524 0)
			)
			(text "a"
				(at -15.24 6.35 0)
			)
			(text "DP1"
				(at -13.716 -6.35 0)
			)
			(text "c"
				(at -13.208 -1.778 0)
			)
			(text "b"
				(at -12.192 2.794 0)
			)
			(text "DP2"
				(at -2.286 -6.35 0)
			)
			(text "DP3"
				(at 7.62 -6.35 0)
			)
			(text "DP4"
				(at 17.78 -6.096 0)
			)
		)
		(symbol "CC56-12SRWA_0_1")
		(symbol "CC56-12SRWA_1_0")
		(symbol "CC56-12SRWA_1_1"
			(pin input line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "a")
				(number "11")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "b")
				(number "7")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "c")
				(number "4")
			)
			(pin input line
				(at -27.94 0 0)
				(length 2.54)
				(name "d")
				(number "2")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "e")
				(number "1")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "f")
				(number "10")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "g")
				(number "5")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "DPX")
				(number "3")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "CC1")
				(number "12")
			)
			(pin input line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "CC2")
				(number "9")
			)
			(pin input line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "CC3")
				(number "8")
			)
			(pin input line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "CC4")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CC56-12SURKWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 13.97 0)
		)
		(property "Value" "CC56-12SURKWA"
			(at 16.51 13.97 0)
		)
		(property "Footprint" "Display_7Segment:CA56-12SURKWA"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/CC56-12SURKWA(Ver.7A).pdf"
			(at -10.922 0.762 0)
		)
		(property "Description" "4 digit 7 segment hyper red LED, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*CA56*12SURKWA*"
			(at 0 0 0)
		)
		(symbol "CC56-12SURKWA_0_0"
			(text "e"
				(at -21.336 -1.524 0)
			)
			(text "f"
				(at -19.558 3.048 0)
			)
			(text "d"
				(at -17.78 -2.794 0)
			)
			(text "g"
				(at -16.51 1.524 0)
			)
			(text "a"
				(at -15.24 6.35 0)
			)
			(text "DP1"
				(at -13.716 -6.35 0)
			)
			(text "c"
				(at -13.208 -1.778 0)
			)
			(text "b"
				(at -12.192 2.794 0)
			)
			(text "DP2"
				(at -2.286 -6.35 0)
			)
			(text "DP3"
				(at 7.62 -6.35 0)
			)
			(text "DP4"
				(at 17.78 -6.096 0)
			)
		)
		(symbol "CC56-12SURKWA_0_1")
		(symbol "CC56-12SURKWA_1_0")
		(symbol "CC56-12SURKWA_1_1"
			(pin input line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "a")
				(number "11")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "b")
				(number "7")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "c")
				(number "4")
			)
			(pin input line
				(at -27.94 0 0)
				(length 2.54)
				(name "d")
				(number "2")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "e")
				(number "1")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "f")
				(number "10")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "g")
				(number "5")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "DPX")
				(number "3")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "CC1")
				(number "12")
			)
			(pin input line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "CC2")
				(number "9")
			)
			(pin input line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "CC3")
				(number "8")
			)
			(pin input line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "CC4")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CC56-12SYKWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 13.97 0)
		)
		(property "Value" "CC56-12SYKWA"
			(at 17.78 13.97 0)
		)
		(property "Footprint" "Display_7Segment:CA56-12SYKWA"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/CC56-12SYKWA(Ver.6A).pdf"
			(at -10.922 0.762 0)
		)
		(property "Description" "4 digit 7 segment super bright yellow LED, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*CA56*12SYKWA*"
			(at 0 0 0)
		)
		(symbol "CC56-12SYKWA_0_0"
			(text "e"
				(at -21.336 -1.524 0)
			)
			(text "f"
				(at -19.558 3.048 0)
			)
			(text "d"
				(at -17.78 -2.794 0)
			)
			(text "g"
				(at -16.51 1.524 0)
			)
			(text "a"
				(at -15.24 6.35 0)
			)
			(text "DP1"
				(at -13.716 -6.35 0)
			)
			(text "c"
				(at -13.208 -1.778 0)
			)
			(text "b"
				(at -12.192 2.794 0)
			)
			(text "DP2"
				(at -2.286 -6.35 0)
			)
			(text "DP3"
				(at 7.62 -6.35 0)
			)
			(text "DP4"
				(at 17.78 -6.096 0)
			)
		)
		(symbol "CC56-12SYKWA_0_1")
		(symbol "CC56-12SYKWA_1_0")
		(symbol "CC56-12SYKWA_1_1"
			(pin input line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "a")
				(number "11")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "b")
				(number "7")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "c")
				(number "4")
			)
			(pin input line
				(at -27.94 0 0)
				(length 2.54)
				(name "d")
				(number "2")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "e")
				(number "1")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "f")
				(number "10")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "g")
				(number "5")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "DPX")
				(number "3")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "CC1")
				(number "12")
			)
			(pin input line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "CC2")
				(number "9")
			)
			(pin input line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "CC3")
				(number "8")
			)
			(pin input line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "CC4")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CC56-12YWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 13.97 0)
		)
		(property "Value" "CC56-12YWA"
			(at 17.78 13.97 0)
		)
		(property "Footprint" "Display_7Segment:CC56-12YWA"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/CC56-12YWA.pdf"
			(at -10.922 0.762 0)
		)
		(property "Description" "4 digit 7 segment  yellow LED, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CC56?12YWA*"
			(at 0 0 0)
		)
		(symbol "CC56-12YWA_0_0"
			(text "e"
				(at -21.336 -1.524 0)
			)
			(text "f"
				(at -19.558 3.048 0)
			)
			(text "d"
				(at -17.78 -2.794 0)
			)
			(text "g"
				(at -16.51 1.524 0)
			)
			(text "a"
				(at -15.24 6.35 0)
			)
			(text "DP1"
				(at -13.716 -6.35 0)
			)
			(text "c"
				(at -13.208 -1.778 0)
			)
			(text "b"
				(at -12.192 2.794 0)
			)
			(text "DP2"
				(at -2.286 -6.35 0)
			)
			(text "DP3"
				(at 7.62 -6.35 0)
			)
			(text "DP4"
				(at 17.78 -6.096 0)
			)
		)
		(symbol "CC56-12YWA_0_1")
		(symbol "CC56-12YWA_1_0")
		(symbol "CC56-12YWA_1_1"
			(pin input line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "a")
				(number "11")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "b")
				(number "7")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "c")
				(number "4")
			)
			(pin input line
				(at -27.94 0 0)
				(length 2.54)
				(name "d")
				(number "2")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "e")
				(number "1")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "f")
				(number "10")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "g")
				(number "5")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "DPX")
				(number "3")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "CC1")
				(number "12")
			)
			(pin input line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "CC2")
				(number "9")
			)
			(pin input line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "CC3")
				(number "8")
			)
			(pin input line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "CC4")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "D168K"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "D168K"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Display_7Segment:D1X8K"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://ia800903.us.archive.org/24/items/CTKD1x8K/Cromatek%20D168K.pdf"
			(at -12.7 12.065 0)
		)
		(property "Description" "One digit 7 segment ultra bright red LED, low current, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D1X8K*"
			(at 0 0 0)
		)
		(symbol "D168K_0_0"
			(text "E"
				(at -2.54 1.778 0)
			)
			(text "F"
				(at -2.286 4.826 0)
			)
			(text "D"
				(at -0.254 1.016 0)
			)
			(text "G"
				(at 0 4.064 0)
			)
			(text "A"
				(at 0.254 5.588 0)
			)
			(text "C"
				(at 2.286 1.778 0)
			)
			(text "B"
				(at 2.54 4.826 0)
			)
			(text "DP"
				(at 3.556 0.254 0)
			)
		)
		(symbol "D168K_0_1")
		(symbol "D168K_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "6")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "1")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "9")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "10")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "5")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CC")
				(number "3")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CC")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DA04-11CGKWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 13.97 0)
		)
		(property "Value" "DA04-11CGKWA"
			(at 15.24 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA04-11CGKWA"
			(at 0.635 -15.875 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/DA04-11CGKWA(Ver.6A).pdf"
			(at -3.048 -10.16 0)
		)
		(property "Description" "Double 7 segment green LED common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA04*11*"
			(at 0 0 0)
		)
		(symbol "DA04-11CGKWA_0_0"
			(text "DIG1"
				(at -1.651 7.62 0)
			)
			(text "8.8."
				(at 0.635 5.08 0)
			)
			(text "DIG2"
				(at 1.651 7.62 0)
			)
		)
		(symbol "DA04-11CGKWA_0_1")
		(symbol "DA04-11CGKWA_1_1"
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "DIG1_A")
				(number "15")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "DIG1_B")
				(number "13")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "DIG1_C")
				(number "1")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "DIG1_D")
				(number "3")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "DIG1_E")
				(number "2")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "DIG1_F")
				(number "14")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "DIG1_G")
				(number "16")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "DIG1_CA")
				(number "4")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "DIG2_A")
				(number "10")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DIG2_B")
				(number "12")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "DIG2_C")
				(number "8")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "DIG2_D")
				(number "6")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "DIG2_E")
				(number "7")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "DIG2_F")
				(number "11")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "DIG2_G")
				(number "9")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "DIG2_CA")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DA04-11SEKWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 13.97 0)
		)
		(property "Value" "DA04-11SEKWA"
			(at 15.24 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA04-11SEKWA"
			(at 0.635 -15.875 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/DA04-11SEKWA(Ver.9A).pdf"
			(at -3.048 -10.16 0)
		)
		(property "Description" "Double 7 segment super bright orange LED common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA04*11*"
			(at 0 0 0)
		)
		(symbol "DA04-11SEKWA_0_0"
			(text "DIG1"
				(at -1.651 7.62 0)
			)
			(text "8.8."
				(at 0.635 5.08 0)
			)
			(text "DIG2"
				(at 1.651 7.62 0)
			)
		)
		(symbol "DA04-11SEKWA_0_1")
		(symbol "DA04-11SEKWA_1_1"
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "DIG1_A")
				(number "15")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "DIG1_B")
				(number "13")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "DIG1_C")
				(number "1")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "DIG1_D")
				(number "3")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "DIG1_E")
				(number "2")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "DIG1_F")
				(number "14")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "DIG1_G")
				(number "16")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "DIG1_CA")
				(number "4")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "DIG2_A")
				(number "10")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DIG2_B")
				(number "12")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "DIG2_C")
				(number "8")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "DIG2_D")
				(number "6")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "DIG2_E")
				(number "7")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "DIG2_F")
				(number "11")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "DIG2_G")
				(number "9")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "DIG2_CA")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DA04-11SURKWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 13.97 0)
		)
		(property "Value" "DA04-11SURKWA"
			(at 15.24 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA04-11SURKWA"
			(at 0.635 -15.875 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/DA04-11SURKWA(Ver.10A).pdf"
			(at -3.048 -10.16 0)
		)
		(property "Description" "Double 7 segment hyper red LED common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA04*11*"
			(at 0 0 0)
		)
		(symbol "DA04-11SURKWA_0_0"
			(text "DIG1"
				(at -1.651 7.62 0)
			)
			(text "8.8."
				(at 0.635 5.08 0)
			)
			(text "DIG2"
				(at 1.651 7.62 0)
			)
		)
		(symbol "DA04-11SURKWA_0_1")
		(symbol "DA04-11SURKWA_1_1"
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "DIG1_A")
				(number "15")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "DIG1_B")
				(number "13")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "DIG1_C")
				(number "1")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "DIG1_D")
				(number "3")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "DIG1_E")
				(number "2")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "DIG1_F")
				(number "14")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "DIG1_G")
				(number "16")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "DIG1_CA")
				(number "4")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "DIG2_A")
				(number "10")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DIG2_B")
				(number "12")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "DIG2_C")
				(number "8")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "DIG2_D")
				(number "6")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "DIG2_E")
				(number "7")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "DIG2_F")
				(number "11")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "DIG2_G")
				(number "9")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "DIG2_CA")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DA04-11SYKWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 13.97 0)
		)
		(property "Value" "DA04-11SYKWA"
			(at 13.97 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA04-11SYKWA"
			(at 0.635 -15.875 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/DA04-11SYKWA(Ver.6A).pdf"
			(at -3.048 -10.16 0)
		)
		(property "Description" "Double 7 segment super bright yellow LED common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA04*11*"
			(at 0 0 0)
		)
		(symbol "DA04-11SYKWA_0_0"
			(text "DIG1"
				(at -1.651 7.62 0)
			)
			(text "8.8."
				(at 0.635 5.08 0)
			)
			(text "DIG2"
				(at 1.651 7.62 0)
			)
		)
		(symbol "DA04-11SYKWA_0_1")
		(symbol "DA04-11SYKWA_1_1"
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "DIG1_A")
				(number "15")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "DIG1_B")
				(number "13")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "DIG1_C")
				(number "1")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "DIG1_D")
				(number "3")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "DIG1_E")
				(number "2")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "DIG1_F")
				(number "14")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "DIG1_G")
				(number "16")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "DIG1_CA")
				(number "4")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "DIG2_A")
				(number "10")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DIG2_B")
				(number "12")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "DIG2_C")
				(number "8")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "DIG2_D")
				(number "6")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "DIG2_E")
				(number "7")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "DIG2_F")
				(number "11")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "DIG2_G")
				(number "9")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "DIG2_CA")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DA56-11CGKWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "DA56-11CGKWA"
			(at 12.7 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA56-11CGKWA"
			(at 0.508 -16.51 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/DA56-11CGKWA(Ver.16A).pdf"
			(at -3.048 2.54 0)
		)
		(property "Description" "Double digit 7 segment green LED common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA56*11*"
			(at 0 0 0)
		)
		(symbol "DA56-11CGKWA_0_0"
			(text "DIG1"
				(at -2.286 10.922 0)
			)
			(text "DP1"
				(at -0.762 6.604 0)
			)
			(text "8.8."
				(at 0 8.636 0)
			)
			(text "DIG2"
				(at 1.27 10.922 0)
			)
			(text "DP2"
				(at 3.048 6.604 0)
			)
		)
		(symbol "DA56-11CGKWA_0_1")
		(symbol "DA56-11CGKWA_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "DIG1_A")
				(number "16")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "DIG1_B")
				(number "15")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DIG1_C")
				(number "3")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "DIG1_D")
				(number "2")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "DIG1_E")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "DIG1_F")
				(number "18")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "DIG1_G")
				(number "17")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DP1")
				(number "4")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "DIG1_CA")
				(number "14")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "DIG2_A")
				(number "11")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "DIG2_B")
				(number "10")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "DIG2_C")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "DIG2_D")
				(number "6")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "DIG2_E")
				(number "5")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "DIG2_F")
				(number "12")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "DIG2_G")
				(number "7")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "DP2")
				(number "9")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "DIG2_CA")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DA56-11SEKWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "DA56-11SEKWA"
			(at 12.7 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA56-11SEKWA"
			(at 0.508 -16.51 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/DA56-11SEKWA(Ver.9A).pdf"
			(at -3.048 2.54 0)
		)
		(property "Description" "Double digit 7 segment super bright orange LED common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA56*11*"
			(at 0 0 0)
		)
		(symbol "DA56-11SEKWA_0_0"
			(text "DIG1"
				(at -2.286 10.922 0)
			)
			(text "DP1"
				(at -0.762 6.604 0)
			)
			(text "8.8."
				(at 0 8.636 0)
			)
			(text "DIG2"
				(at 1.27 10.922 0)
			)
			(text "DP2"
				(at 3.048 6.604 0)
			)
		)
		(symbol "DA56-11SEKWA_0_1")
		(symbol "DA56-11SEKWA_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "DIG1_A")
				(number "16")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "DIG1_B")
				(number "15")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DIG1_C")
				(number "3")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "DIG1_D")
				(number "2")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "DIG1_E")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "DIG1_F")
				(number "18")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "DIG1_G")
				(number "17")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DP1")
				(number "4")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "DIG1_CA")
				(number "14")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "DIG2_A")
				(number "11")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "DIG2_B")
				(number "10")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "DIG2_C")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "DIG2_D")
				(number "6")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "DIG2_E")
				(number "5")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "DIG2_F")
				(number "12")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "DIG2_G")
				(number "7")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "DP2")
				(number "9")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "DIG2_CA")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DA56-11SURKWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "DA56-11SURKWA"
			(at 12.7 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA56-11SURKWA"
			(at 0.508 -16.51 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/DA56-11SURKWA(Ver.11A).pdf"
			(at -3.048 2.54 0)
		)
		(property "Description" "Double digit 7 segment hyper red LED common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA56*11*"
			(at 0 0 0)
		)
		(symbol "DA56-11SURKWA_0_0"
			(text "DIG1"
				(at -2.286 10.922 0)
			)
			(text "DP1"
				(at -0.762 6.604 0)
			)
			(text "8.8."
				(at 0 8.636 0)
			)
			(text "DIG2"
				(at 1.27 10.922 0)
			)
			(text "DP2"
				(at 3.048 6.604 0)
			)
		)
		(symbol "DA56-11SURKWA_0_1")
		(symbol "DA56-11SURKWA_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "DIG1_A")
				(number "16")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "DIG1_B")
				(number "15")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DIG1_C")
				(number "3")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "DIG1_D")
				(number "2")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "DIG1_E")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "DIG1_F")
				(number "18")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "DIG1_G")
				(number "17")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DP1")
				(number "4")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "DIG1_CA")
				(number "14")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "DIG2_A")
				(number "11")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "DIG2_B")
				(number "10")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "DIG2_C")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "DIG2_D")
				(number "6")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "DIG2_E")
				(number "5")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "DIG2_F")
				(number "12")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "DIG2_G")
				(number "7")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "DP2")
				(number "9")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "DIG2_CA")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DA56-11SYKWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "DA56-11SYKWA"
			(at 12.065 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA56-11SYKWA"
			(at 0.508 -16.51 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/DA56-11SYKWA(Ver.11A).pdf"
			(at -3.048 2.54 0)
		)
		(property "Description" "Double digit 7 segment super bright yellow LED common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA56*11*"
			(at 0 0 0)
		)
		(symbol "DA56-11SYKWA_0_0"
			(text "DIG1"
				(at -2.286 10.922 0)
			)
			(text "DP1"
				(at -0.762 6.604 0)
			)
			(text "8.8."
				(at 0 8.636 0)
			)
			(text "DIG2"
				(at 1.27 10.922 0)
			)
			(text "DP2"
				(at 3.048 6.604 0)
			)
		)
		(symbol "DA56-11SYKWA_0_1")
		(symbol "DA56-11SYKWA_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "DIG1_A")
				(number "16")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "DIG1_B")
				(number "15")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DIG1_C")
				(number "3")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "DIG1_D")
				(number "2")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "DIG1_E")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "DIG1_F")
				(number "18")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "DIG1_G")
				(number "17")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DP1")
				(number "4")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "DIG1_CA")
				(number "14")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "DIG2_A")
				(number "11")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "DIG2_B")
				(number "10")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "DIG2_C")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "DIG2_D")
				(number "6")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "DIG2_E")
				(number "5")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "DIG2_F")
				(number "12")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "DIG2_G")
				(number "7")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "DP2")
				(number "9")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "DIG2_CA")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DC56-11CGKWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "DC56-11CGKWA"
			(at 12.065 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA56-11CGKWA"
			(at 0.508 -16.51 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/DC56-11CGKWA(Ver.7A).pdf"
			(at -3.048 2.54 0)
		)
		(property "Description" "Double digit 7 segment green LED common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA56*11*"
			(at 0 0 0)
		)
		(symbol "DC56-11CGKWA_0_0"
			(text "DIG1"
				(at -2.286 10.922 0)
			)
			(text "DP1"
				(at -0.762 6.604 0)
			)
			(text "8.8."
				(at 0 8.636 0)
			)
			(text "DIG2"
				(at 1.27 10.922 0)
			)
			(text "DP2"
				(at 3.048 6.604 0)
			)
		)
		(symbol "DC56-11CGKWA_0_1")
		(symbol "DC56-11CGKWA_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "DIG1_A")
				(number "16")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "DIG1_B")
				(number "15")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DIG1_C")
				(number "3")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "DIG1_D")
				(number "2")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "DIG1_E")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "DIG1_F")
				(number "18")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "DIG1_G")
				(number "17")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DP1")
				(number "4")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "DIG1_CC")
				(number "14")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "DIG2_A")
				(number "11")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "DIG2_B")
				(number "10")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "DIG2_C")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "DIG2_D")
				(number "6")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "DIG2_E")
				(number "5")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "DIG2_F")
				(number "12")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "DIG2_G")
				(number "7")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "DP2")
				(number "9")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "DIG2_CC")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DC56-11SEKWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "DC56-11SEKWA"
			(at 12.065 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA56-11SEKWA"
			(at 0.508 -16.51 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/DA56-11SEKWA(Ver.9A).pdf"
			(at -3.048 2.54 0)
		)
		(property "Description" "Double digit 7 segment super bright orange LED common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA56*11*"
			(at 0 0 0)
		)
		(symbol "DC56-11SEKWA_0_0"
			(text "DIG1"
				(at -2.286 10.922 0)
			)
			(text "DP1"
				(at -0.762 6.604 0)
			)
			(text "8.8."
				(at 0 8.636 0)
			)
			(text "DIG2"
				(at 1.27 10.922 0)
			)
			(text "DP2"
				(at 3.048 6.604 0)
			)
		)
		(symbol "DC56-11SEKWA_0_1")
		(symbol "DC56-11SEKWA_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "DIG1_A")
				(number "16")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "DIG1_B")
				(number "15")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DIG1_C")
				(number "3")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "DIG1_D")
				(number "2")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "DIG1_E")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "DIG1_F")
				(number "18")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "DIG1_G")
				(number "17")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DP1")
				(number "4")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "DIG1_CC")
				(number "14")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "DIG2_A")
				(number "11")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "DIG2_B")
				(number "10")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "DIG2_C")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "DIG2_D")
				(number "6")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "DIG2_E")
				(number "5")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "DIG2_F")
				(number "12")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "DIG2_G")
				(number "7")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "DP2")
				(number "9")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "DIG2_CC")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DC56-11SURKWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "DC56-11SURKWA"
			(at 12.065 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA56-11SURKWA"
			(at 0.508 -16.51 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/DC56-11SURKWA(Ver.8A).pdf"
			(at -3.048 2.54 0)
		)
		(property "Description" "Double digit 7 segment hyper red LED common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA56*11*"
			(at 0 0 0)
		)
		(symbol "DC56-11SURKWA_0_0"
			(text "DIG1"
				(at -2.286 10.922 0)
			)
			(text "DP1"
				(at -0.762 6.604 0)
			)
			(text "8.8."
				(at 0 8.636 0)
			)
			(text "DIG2"
				(at 1.27 10.922 0)
			)
			(text "DP2"
				(at 3.048 6.604 0)
			)
		)
		(symbol "DC56-11SURKWA_0_1")
		(symbol "DC56-11SURKWA_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "DIG1_A")
				(number "16")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "DIG1_B")
				(number "15")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DIG1_C")
				(number "3")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "DIG1_D")
				(number "2")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "DIG1_E")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "DIG1_F")
				(number "18")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "DIG1_G")
				(number "17")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DP1")
				(number "4")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "DIG1_CC")
				(number "14")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "DIG2_A")
				(number "11")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "DIG2_B")
				(number "10")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "DIG2_C")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "DIG2_D")
				(number "6")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "DIG2_E")
				(number "5")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "DIG2_F")
				(number "12")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "DIG2_G")
				(number "7")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "DP2")
				(number "9")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "DIG2_CC")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DC56-11SYKWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "DC56-11SYKWA"
			(at 12.065 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA56-11SYKWA"
			(at 0.508 -16.51 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/DC56-11SYKWA(Ver.7A).pdf"
			(at -3.048 2.54 0)
		)
		(property "Description" "Double digit 7 segment super bright yellow LED common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA56*11*"
			(at 0 0 0)
		)
		(symbol "DC56-11SYKWA_0_0"
			(text "DIG1"
				(at -2.286 10.922 0)
			)
			(text "DP1"
				(at -0.762 6.604 0)
			)
			(text "8.8."
				(at 0 8.636 0)
			)
			(text "DIG2"
				(at 1.27 10.922 0)
			)
			(text "DP2"
				(at 3.048 6.604 0)
			)
		)
		(symbol "DC56-11SYKWA_0_1")
		(symbol "DC56-11SYKWA_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "DIG1_A")
				(number "16")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "DIG1_B")
				(number "15")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DIG1_C")
				(number "3")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "DIG1_D")
				(number "2")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "DIG1_E")
				(number "1")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "DIG1_F")
				(number "18")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "DIG1_G")
				(number "17")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DP1")
				(number "4")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "DIG1_CC")
				(number "14")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "DIG2_A")
				(number "11")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "DIG2_B")
				(number "10")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "DIG2_C")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "DIG2_D")
				(number "6")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "DIG2_E")
				(number "5")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "DIG2_F")
				(number "12")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "DIG2_G")
				(number "7")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "DP2")
				(number "9")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "DIG2_CC")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DE113-XX-XX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 29.21 0)
		)
		(property "Value" "DE113-XX-XX"
			(at -11.938 -30.226 0)
		)
		(property "Footprint" "Display_7Segment:DE113-XX-XX"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "http://www.display-elektronik.de/filter/DE113-MS-20_75.pdf"
			(at -5.08 5.08 0)
		)
		(property "Description" "3 and half digit 7 segment transmissive standard LCD with LO BAT, pin length 7.5mm, -20°C to +70°C, 3V-5V VDD"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DE*113*"
			(at 0 0 0)
		)
		(symbol "DE113-XX-XX_0_0"
			(text "+"
				(at -5.461 23.876 0)
			)
			(text "LO BAT"
				(at -5.334 24.892 0)
			)
			(text "1"
				(at -2.413 24.384 0)
			)
			(text "."
				(at -1.143 24.384 0)
			)
			(text "8"
				(at 0.254 24.384 0)
			)
			(text ":"
				(at 1.778 25.654 0)
			)
			(text "."
				(at 1.778 24.384 0)
			)
			(text "8"
				(at 3.302 24.384 0)
			)
			(text "."
				(at 4.572 24.384 0)
			)
			(text "8"
				(at 5.842 24.384 0)
			)
		)
		(symbol "DE113-XX-XX_0_1")
		(symbol "DE113-XX-XX_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "DP1")
				(number "8")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "1A")
				(number "30")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "1B")
				(number "29")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "1C")
				(number "11")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "1D")
				(number "10")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "1E")
				(number "9")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "1F")
				(number "31")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "1G")
				(number "32")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DP2")
				(number "12")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "2A")
				(number "25")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "2B")
				(number "24")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "2C")
				(number "15")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "2D")
				(number "14")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "2E")
				(number "13")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "2F")
				(number "26")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "2G")
				(number "27")
			)
			(pin no_connect line
				(at -12.7 22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -12.7 20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -12.7 17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -12.7 15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 12.7 22.86 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "37")
			)
			(pin no_connect line
				(at 12.7 20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "36")
			)
			(pin no_connect line
				(at 12.7 17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "35")
			)
			(pin no_connect line
				(at 12.7 15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin no_connect line
				(at 12.7 12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "33")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "DP3")
				(number "16")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "3A")
				(number "21")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "3B")
				(number "20")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "3C")
				(number "19")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "3D")
				(number "18")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "3E")
				(number "17")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "3F")
				(number "22")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "3G")
				(number "23")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "LO_BAT")
				(number "38")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "BP")
				(number "40")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "BP")
				(number "1")
			)
			(pin input line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin input line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name ":")
				(number "39")
			)
			(pin input line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin input line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "COL")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DE114-RS-20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 29.21 0)
		)
		(property "Value" "DE114-RS-20"
			(at -11.938 -30.48 0)
		)
		(property "Footprint" "Display_7Segment:DE114-RS-20"
			(at 2.54 -33.02 0)
		)
		(property "Datasheet" "http://www.display-elektronik.de/filter/DE114-RS-20_635.pdf"
			(at -5.08 5.08 0)
		)
		(property "Description" "3 and half digit 7 segment reflective standard LCD with ~~ and BAT, pin length 6.35mm, -20°C to +70°C, 3V-5V VDD"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DE*114*RS*20*"
			(at 0 0 0)
		)
		(symbol "DE114-RS-20_0_0"
			(text "BAT"
				(at -6.477 22.733 0)
			)
			(text "+"
				(at -6.35 24.257 0)
			)
			(text "1"
				(at -2.286 24.257 0)
			)
			(text "."
				(at -1.016 24.257 0)
			)
			(text "8"
				(at 0.635 24.257 0)
			)
			(text ":"
				(at 2.159 25.146 0)
			)
			(text "."
				(at 2.159 24.257 0)
			)
			(text "8"
				(at 3.683 24.257 0)
			)
			(text "."
				(at 4.953 24.257 0)
			)
			(text "8"
				(at 6.223 24.257 0)
			)
		)
		(symbol "DE114-RS-20_0_1")
		(symbol "DE114-RS-20_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "DP1")
				(number "8")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "1A")
				(number "30")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "1B")
				(number "29")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "1C")
				(number "11")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "1D")
				(number "10")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "1E")
				(number "9")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "1F")
				(number "31")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "1G")
				(number "32")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DP2")
				(number "12")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "2A")
				(number "25")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "2B")
				(number "24")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "2C")
				(number "15")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "2D")
				(number "14")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "2E")
				(number "13")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "2F")
				(number "26")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "2G")
				(number "27")
			)
			(pin no_connect line
				(at -12.7 22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -12.7 20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -12.7 17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -12.7 15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 12.7 22.86 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "36")
			)
			(pin no_connect line
				(at 12.7 20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "35")
			)
			(pin no_connect line
				(at 12.7 17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin no_connect line
				(at 12.7 15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "33")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "~")
				(number "37")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "DP3")
				(number "16")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "3A")
				(number "21")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "3B")
				(number "20")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "3C")
				(number "19")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "3D")
				(number "18")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "3E")
				(number "17")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "3F")
				(number "22")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "3G")
				(number "23")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "~")
				(number "38")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "BAT")
				(number "40")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "BP")
				(number "1")
			)
			(pin input line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin input line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name ":")
				(number "39")
			)
			(pin input line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin input line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "COL")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DE122-XX-XX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 34.29 0)
		)
		(property "Value" "DE122-XX-XX"
			(at -12.7 -34.29 0)
		)
		(property "Footprint" "Display_7Segment:DE122-XX-XX"
			(at 2.54 -36.83 0)
		)
		(property "Datasheet" "http://www.display-elektronik.de/filter/DE122-RS-20_635.pdf"
			(at -5.08 7.62 0)
		)
		(property "Description" "6 digit 7 segment reflective standard LCD, pin length 6.35mm, -20°C to +70°C, 3V-5V VDD"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DE122?XX?XX*"
			(at 0 0 0)
		)
		(symbol "DE122-XX-XX_0_0"
			(text ":"
				(at -2.667 29.972 0)
			)
			(text "8.8.8.8.8.8"
				(at 0.127 29.337 0)
			)
			(text ":"
				(at 3.048 29.972 0)
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "1A")
				(number "48")
			)
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "1B")
				(number "47")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "1F")
				(number "49")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "1G")
				(number "50")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "2A")
				(number "44")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "2B")
				(number "43")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "2F")
				(number "45")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "2G")
				(number "46")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "COL1")
				(number "42")
			)
			(pin input line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "3G")
				(number "41")
			)
		)
		(symbol "DE122-XX-XX_0_1")
		(symbol "DE122-XX-XX_1_1"
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "1C")
				(number "4")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "1D")
				(number "3")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "1E")
				(number "2")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "DP1")
				(number "5")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "2C")
				(number "8")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "2D")
				(number "7")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "2E")
				(number "6")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DP2")
				(number "9")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "3A")
				(number "39")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "3B")
				(number "38")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "3C")
				(number "12")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "3D")
				(number "11")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "3E")
				(number "10")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "3F")
				(number "40")
			)
			(pin input line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "DP3")
				(number "13")
			)
			(pin input line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "4A")
				(number "35")
			)
			(pin input line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "4B")
				(number "34")
			)
			(pin input line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "4C")
				(number "16")
			)
			(pin input line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "4D")
				(number "15")
			)
			(pin input line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "4E")
				(number "14")
			)
			(pin input line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "4F")
				(number "36")
			)
			(pin input line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "4G")
				(number "37")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "DP4")
				(number "17")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "COL2")
				(number "33")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "5A")
				(number "30")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "5B")
				(number "29")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "5C")
				(number "20")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "5D")
				(number "19")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "5E")
				(number "18")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "5F")
				(number "31")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "5G")
				(number "32")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "DP5")
				(number "21")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "6A")
				(number "26")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "6B")
				(number "25")
			)
			(pin input line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "6C")
				(number "24")
			)
			(pin input line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "6D")
				(number "23")
			)
			(pin input line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "6E")
				(number "22")
			)
			(pin input line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "6F")
				(number "27")
			)
			(pin input line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "6G")
				(number "28")
			)
			(pin input line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "BP")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DE170-XX-XX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 29.21 0)
		)
		(property "Value" "DE170-XX-XX"
			(at -11.938 -30.099 0)
		)
		(property "Footprint" "Display_7Segment:DE170-XX-XX"
			(at 1.27 -33.02 0)
		)
		(property "Datasheet" "http://www.display-elektronik.de/filter/DE170-RS-20_75.pdf"
			(at -5.08 5.08 0)
		)
		(property "Description" "3 and half digit 7 segment reflective standard LCD with arrow, pin length 7.5mm, -20°C to +70°C, 3V-5V VDD"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DE170?XX?XX*"
			(at 0 0 0)
		)
		(symbol "DE170-XX-XX_0_0"
			(text "+"
				(at -5.08 23.749 0)
			)
			(text "1"
				(at -2.159 24.638 0)
			)
			(text "."
				(at -0.889 24.638 0)
			)
			(text "8"
				(at 0.635 24.638 0)
			)
			(text "."
				(at 2.159 24.638 0)
			)
			(text ":"
				(at 2.286 25.654 0)
			)
			(text "8"
				(at 3.81 24.638 0)
			)
			(text "."
				(at 5.207 24.638 0)
			)
			(text "8"
				(at 6.604 24.638 0)
			)
		)
		(symbol "DE170-XX-XX_0_1")
		(symbol "DE170-XX-XX_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "DP1")
				(number "8")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "1A")
				(number "30")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "1B")
				(number "29")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "1C")
				(number "11")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "1D")
				(number "10")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "1E")
				(number "9")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "1F")
				(number "31")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "1G")
				(number "32")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DP2")
				(number "12")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "2A")
				(number "25")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "2B")
				(number "24")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "2C")
				(number "15")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "2D")
				(number "14")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "2E")
				(number "13")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "2F")
				(number "26")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "2G")
				(number "27")
			)
			(pin no_connect line
				(at -12.7 22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -12.7 20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -12.7 17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -12.7 15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 12.7 22.86 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "37")
			)
			(pin no_connect line
				(at 12.7 20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "36")
			)
			(pin no_connect line
				(at 12.7 17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "35")
			)
			(pin no_connect line
				(at 12.7 15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin no_connect line
				(at 12.7 12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "33")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "DP3")
				(number "16")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "3A")
				(number "21")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "3B")
				(number "20")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "3C")
				(number "19")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "3D")
				(number "18")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "3E")
				(number "17")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "3F")
				(number "22")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "3G")
				(number "23")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "~")
				(number "38")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "BP")
				(number "40")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "BP")
				(number "1")
			)
			(pin input line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin input line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name ":")
				(number "39")
			)
			(pin input line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin input line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "COL")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EA_T123X-I2C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "EA_T123X-I2C"
			(at 3.556 11.684 0)
		)
		(property "Footprint" "Display:EA_T123X-I2C"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.lcd-module.de/pdf/doma/t123-i2c.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "3 Lines, 12 character alpha numeric LCD, transreflective STN and FSTN Gray, I2C, single or dual power"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "EA?T123X?I2C*"
			(at 0 0 0)
		)
		(symbol "EA_T123X-I2C_0_0"
			(text "12 Character"
				(at -7.366 -1.524 0)
			)
			(text "3 Lines"
				(at -4.826 1.016 0)
			)
		)
		(symbol "EA_T123X-I2C_0_1")
		(symbol "EA_T123X-I2C_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "VLCD")
				(number "3")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "V0")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ELD-426SYGWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "ELD-426SYGWA"
			(at -2.794 -14.224 0)
		)
		(property "Footprint" "Display_7Segment:ELD_426XXXX"
			(at -0.254 -17.272 0)
		)
		(property "Datasheet" "http://www.everlight.com/file/ProductFile/D426SYGWA-S530-E2.pdf"
			(at -6.477 4.572 0)
		)
		(property "Description" "Double 7 segment brilliant yellow green LED common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*ELD*426*"
			(at 0 0 0)
		)
		(symbol "ELD-426SYGWA_0_0"
			(text "D1"
				(at -3.937 11.684 0)
			)
			(text "f"
				(at 1.3716 8.1026 0)
			)
			(text "e"
				(at 1.3716 5.6388 0)
			)
			(text "D2"
				(at 3.429 11.684 0)
			)
			(text "a"
				(at 3.4544 10.1854 0)
			)
			(text "g"
				(at 3.5052 7.7216 0)
			)
			(text "d"
				(at 3.6068 3.683 0)
			)
			(text "b"
				(at 5.842 8.0772 0)
			)
			(text "c"
				(at 5.9436 5.5372 0)
			)
			(text "DP"
				(at 7.239 3.429 0)
			)
		)
		(symbol "ELD-426SYGWA_0_1")
		(symbol "ELD-426SYGWA_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "a")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "b")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "c")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "d")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "e")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "f")
				(number "8")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "g")
				(number "9")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "2")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "CA_D1")
				(number "10")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "CA_D2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSM-441B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "HDSM-441B"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Display:HDSM-441B_HDSM-443B"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-1589EN"
			(at -5.588 2.54 0)
		)
		(property "Description" "Double 7 segment Blue LED common anode SMD mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*HDSM*441B*"
			(at 0 0 0)
		)
		(symbol "HDSM-441B_0_1")
		(symbol "HDSM-441B_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DP")
				(number "2")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "F")
				(number "4")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "E")
				(number "7")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "B")
				(number "9")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "CA_DIG1")
				(number "10")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "CA_DIG2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSM-443B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "HDSM-443B"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display:HDSM-441B_HDSM-443B"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-1589EN"
			(at -5.588 2.54 0)
		)
		(property "Description" "Double 7 segment Blue LED common cathode SMD mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*HDSM*441B*"
			(at 0 0 0)
		)
		(symbol "HDSM-443B_0_1")
		(symbol "HDSM-443B_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DP")
				(number "2")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "F")
				(number "4")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "E")
				(number "7")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "B")
				(number "9")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "CC_DIG1")
				(number "10")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "CC_DIG2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSM-541B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "HDSM-541B"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display:HDSM-441B_HDSM-443B"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-1588EN"
			(at -2.54 2.54 0)
		)
		(property "Description" "Double 7 segment Blue LED common anode SMD mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSM?441B?HDSM?443B*"
			(at 0 0 0)
		)
		(symbol "HDSM-541B_0_1")
		(symbol "HDSM-541B_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DP")
				(number "2")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "F")
				(number "4")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "E")
				(number "7")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "B")
				(number "9")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "CA_DIG1")
				(number "10")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "CA_DIG2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSM-543B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "HDSM-543B"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display:HDSM-541B_HDSM-543B"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-1588EN"
			(at -2.54 2.54 0)
		)
		(property "Description" "Double 7 segment Blue LED common cathode SMD mount"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSM?541B?HDSM?543B*"
			(at 0 0 0)
		)
		(symbol "HDSM-543B_0_1")
		(symbol "HDSM-543B_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DP")
				(number "2")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "F")
				(number "4")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "E")
				(number "7")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "B")
				(number "9")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "CC_DIG1")
				(number "10")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "CC_DIG2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-7401"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "HDSP-7401"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:HDSP-7401"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-2553EN"
			(at 0 0 0)
		)
		(property "Description" "One digit 7 segment yellow, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?7401*"
			(at 0 0 0)
		)
		(symbol "HDSP-7401_1_0"
			(text "E"
				(at -2.54 -1.397 0)
			)
			(text "F"
				(at -2.286 1.651 0)
			)
			(text "D"
				(at -0.254 -2.159 0)
			)
			(text "G"
				(at 0 0.889 0)
			)
			(text "A"
				(at 0.254 2.413 0)
			)
			(text "C"
				(at 2.286 -1.397 0)
			)
			(text "B"
				(at 2.54 1.651 0)
			)
			(text "DP"
				(at 3.556 -2.921 0)
			)
		)
		(symbol "HDSP-7401_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "9")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "4")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "2")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "7")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CA")
				(number "1")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CA")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-7403"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "HDSP-7403"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:HDSP-7401"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-2553EN"
			(at 0 0 0)
		)
		(property "Description" "One digit 7 segment yellow, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?7401*"
			(at 0 0 0)
		)
		(symbol "HDSP-7403_1_0"
			(text "E"
				(at -2.54 -1.397 0)
			)
			(text "F"
				(at -2.286 1.651 0)
			)
			(text "D"
				(at -0.254 -2.159 0)
			)
			(text "G"
				(at 0 0.889 0)
			)
			(text "A"
				(at 0.254 2.413 0)
			)
			(text "C"
				(at 2.286 -1.397 0)
			)
			(text "B"
				(at 2.54 1.651 0)
			)
			(text "DP"
				(at 3.556 -2.921 0)
			)
		)
		(symbol "HDSP-7403_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "9")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "4")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "2")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "7")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CC")
				(number "1")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CC")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-7507"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 8.89 0)
		)
		(property "Value" "HDSP-7507"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Display_7Segment:HDSP-7507"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-2553EN"
			(at -0.254 3.556 0)
		)
		(property "Description" "+-1 overflow 7 segment high efficiency red, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?7507*"
			(at 0 0 0)
		)
		(symbol "HDSP-7507_0_1")
		(symbol "HDSP-7507_1_0"
			(text "P"
				(at -1.397 6.2992 0)
			)
			(text "M"
				(at -0.9906 1.6002 0)
			)
			(text "C"
				(at 2.54 2.032 0)
			)
			(text "B"
				(at 2.921 5.08 0)
			)
			(text "DP"
				(at 4.318 1.016 0)
			)
		)
		(symbol "HDSP-7507_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "P")
				(number "2")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "M")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "B")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "DP")
				(number "7")
			)
			(pin no_connect line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 5.08 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "CA")
				(number "1")
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "CA")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-7508"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 8.89 0)
		)
		(property "Value" "HDSP-7508"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Display_7Segment:HDSP-7507"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-2553EN"
			(at 0 0 0)
		)
		(property "Description" "+-1 overflow 7 segment high efficiency red, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?7507*"
			(at 0 0 0)
		)
		(symbol "HDSP-7508_0_1")
		(symbol "HDSP-7508_1_0"
			(text "P"
				(at -1.397 6.2992 0)
			)
			(text "M"
				(at -0.9906 1.6002 0)
			)
			(text "C"
				(at 2.54 2.032 0)
			)
			(text "B"
				(at 2.921 5.08 0)
			)
			(text "DP"
				(at 4.318 1.016 0)
			)
		)
		(symbol "HDSP-7508_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "P")
				(number "2")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "M")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "B")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "DP")
				(number "7")
			)
			(pin no_connect line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 5.08 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "CC")
				(number "1")
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "CC")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-7801"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "HDSP-7801"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:HDSP-7801"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-2553EN"
			(at 0 0 0)
		)
		(property "Description" "One digit 7 segment green, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?7801*"
			(at 0 0 0)
		)
		(symbol "HDSP-7801_1_0"
			(text "E"
				(at -2.54 -1.397 0)
			)
			(text "F"
				(at -2.286 1.651 0)
			)
			(text "D"
				(at -0.254 -2.159 0)
			)
			(text "G"
				(at 0 0.889 0)
			)
			(text "A"
				(at 0.254 2.413 0)
			)
			(text "C"
				(at 2.286 -1.397 0)
			)
			(text "B"
				(at 2.54 1.651 0)
			)
			(text "DP"
				(at 3.556 -2.921 0)
			)
		)
		(symbol "HDSP-7801_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "9")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "4")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "2")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "7")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CA")
				(number "1")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CA")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-7803"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "HDSP-7803"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:HDSP-7801"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-2553EN"
			(at 0 0 0)
		)
		(property "Description" "One digit 7 segment green, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?7801*"
			(at 0 0 0)
		)
		(symbol "HDSP-7803_1_0"
			(text "E"
				(at -2.54 -1.397 0)
			)
			(text "F"
				(at -2.286 1.651 0)
			)
			(text "D"
				(at -0.254 -2.159 0)
			)
			(text "G"
				(at 0 0.889 0)
			)
			(text "A"
				(at 0.254 2.413 0)
			)
			(text "C"
				(at 2.286 -1.397 0)
			)
			(text "B"
				(at 2.54 1.651 0)
			)
			(text "DP"
				(at 3.556 -2.921 0)
			)
		)
		(symbol "HDSP-7803_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "9")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "4")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "2")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "7")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CC")
				(number "1")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CC")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-7807"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 8.89 0)
		)
		(property "Value" "HDSP-7807"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Display_7Segment:HDSP-7807"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-2553EN"
			(at 0 0 0)
		)
		(property "Description" "+-1 overflow 7 segment green, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?7807*"
			(at 0 0 0)
		)
		(symbol "HDSP-7807_0_1")
		(symbol "HDSP-7807_1_0"
			(text "P"
				(at -1.397 6.2992 0)
			)
			(text "M"
				(at -0.9906 1.6002 0)
			)
			(text "C"
				(at 2.54 2.032 0)
			)
			(text "B"
				(at 2.921 5.08 0)
			)
			(text "DP"
				(at 4.318 1.016 0)
			)
		)
		(symbol "HDSP-7807_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "P")
				(number "2")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "M")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "B")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "DP")
				(number "7")
			)
			(pin no_connect line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 5.08 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "CA")
				(number "1")
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "CA")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-7808"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 8.89 0)
		)
		(property "Value" "HDSP-7808"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Display_7Segment:HDSP-7807"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-2553EN"
			(at 0 0 0)
		)
		(property "Description" "+-1 overflow 7 segment green, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?7807*"
			(at 0 0 0)
		)
		(symbol "HDSP-7808_0_1")
		(symbol "HDSP-7808_1_0"
			(text "P"
				(at -1.397 6.2992 0)
			)
			(text "M"
				(at -0.9906 1.6002 0)
			)
			(text "C"
				(at 2.54 2.032 0)
			)
			(text "B"
				(at 2.921 5.08 0)
			)
			(text "DP"
				(at 4.318 1.016 0)
			)
		)
		(symbol "HDSP-7808_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "P")
				(number "2")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "M")
				(number "3")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "B")
				(number "9")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "DP")
				(number "7")
			)
			(pin no_connect line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 5.08 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "CC")
				(number "1")
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "CC")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-A151"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "HDSP-A151"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:HDSP-A151"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-2553EN"
			(at -12.7 13.97 0)
		)
		(property "Description" "One digit 7 segment red, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?A151*"
			(at 0 0 0)
		)
		(symbol "HDSP-A151_1_0"
			(text "E"
				(at -2.54 -1.397 0)
			)
			(text "F"
				(at -2.286 1.651 0)
			)
			(text "D"
				(at -0.254 -2.159 0)
			)
			(text "G"
				(at 0 0.889 0)
			)
			(text "A"
				(at 0.254 2.413 0)
			)
			(text "C"
				(at 2.286 -1.397 0)
			)
			(text "B"
				(at 2.54 1.651 0)
			)
			(text "DP"
				(at 3.556 -2.921 0)
			)
		)
		(symbol "HDSP-A151_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "9")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "4")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "2")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "7")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CA")
				(number "1")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CA")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-A153"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "HDSP-A153"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:HDSP-A151"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-2553EN"
			(at -10.16 13.97 0)
		)
		(property "Description" "One digit 7 segment red, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?A151*"
			(at 0 0 0)
		)
		(symbol "HDSP-A153_1_0"
			(text "E"
				(at -2.54 -1.397 0)
			)
			(text "F"
				(at -2.286 1.651 0)
			)
			(text "D"
				(at -0.254 -2.159 0)
			)
			(text "G"
				(at 0 0.889 0)
			)
			(text "A"
				(at 0.254 2.413 0)
			)
			(text "C"
				(at 2.286 -1.397 0)
			)
			(text "B"
				(at 2.54 1.651 0)
			)
			(text "DP"
				(at 3.556 -2.921 0)
			)
		)
		(symbol "HDSP-A153_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "9")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "4")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "2")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "7")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CC")
				(number "1")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CC")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-A401"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "HDSP-A401"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:HDSP-A401"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-2553EN"
			(at -20.32 25.4 0)
		)
		(property "Description" "One digit 7 segment orange, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?A401*"
			(at 0 0 0)
		)
		(symbol "HDSP-A401_1_0"
			(text "E"
				(at -2.54 -1.397 0)
			)
			(text "F"
				(at -2.286 1.651 0)
			)
			(text "D"
				(at -0.254 -2.159 0)
			)
			(text "G"
				(at 0 0.889 0)
			)
			(text "A"
				(at 0.254 2.413 0)
			)
			(text "C"
				(at 2.286 -1.397 0)
			)
			(text "B"
				(at 2.54 1.651 0)
			)
			(text "DP"
				(at 3.556 -2.921 0)
			)
		)
		(symbol "HDSP-A401_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "9")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "4")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "2")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "7")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CA")
				(number "1")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CA")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-A403"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "HDSP-A403"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:HDSP-A401"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-2553EN"
			(at 0 0 0)
		)
		(property "Description" "One digit 7 segment orange, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?A401*"
			(at 0 0 0)
		)
		(symbol "HDSP-A403_1_0"
			(text "E"
				(at -2.54 -1.397 0)
			)
			(text "F"
				(at -2.286 1.651 0)
			)
			(text "D"
				(at -0.254 -2.159 0)
			)
			(text "G"
				(at 0 0.889 0)
			)
			(text "A"
				(at 0.254 2.413 0)
			)
			(text "C"
				(at 2.286 -1.397 0)
			)
			(text "B"
				(at 2.54 1.651 0)
			)
			(text "DP"
				(at 3.556 -2.921 0)
			)
		)
		(symbol "HDSP-A403_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "9")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "4")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "2")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "7")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CC")
				(number "1")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CC")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HY1602E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "DS"
			(at -6.096 19.05 0)
		)
		(property "Value" "HY1602E"
			(at 5.08 19.05 0)
		)
		(property "Footprint" "Display:HY1602E"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "http://www.icbank.com/data/ICBShop/board/HY1602E.pdf"
			(at 5.08 2.54 0)
		)
		(property "Description" "LCD 16x2 Alphanumeric 16pin Blue/Yellow/Green Backlight, 8bit parallel, 5V VDD"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*HY1602E*"
			(at 0 0 0)
		)
		(symbol "HY1602E_0_1")
		(symbol "HY1602E_1_1"
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "E")
				(number "8")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "R/~{W}")
				(number "7")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "RS")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DB0")
				(number "9")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "DB1")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DB2")
				(number "11")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DB3")
				(number "12")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "DB4")
				(number "13")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "DB5")
				(number "14")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "DB6")
				(number "15")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "DB7")
				(number "16")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin input line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "Vo")
				(number "5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "LEDA")
				(number "2")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "LEDK")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KCSA02-105"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "KCSA02-105"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Display_7Segment:KCSC02-105"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/KCSA02-105(Ver.10A).pdf"
			(at -12.7 12.065 0)
		)
		(property "Description" "One digit 7 segment hyper red LED, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*KCSC02*105*"
			(at 0 0 0)
		)
		(symbol "KCSA02-105_0_0"
			(text "E"
				(at -2.54 1.778 0)
			)
			(text "F"
				(at -2.286 4.826 0)
			)
			(text "D"
				(at -0.254 1.016 0)
			)
			(text "G"
				(at 0 4.064 0)
			)
			(text "A"
				(at 0.254 5.588 0)
			)
			(text "C"
				(at 2.286 1.778 0)
			)
			(text "B"
				(at 2.54 4.826 0)
			)
			(text "DP"
				(at 3.556 0.254 0)
			)
		)
		(symbol "KCSA02-105_0_1")
		(symbol "KCSA02-105_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "6")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "1")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "9")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "10")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "5")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CA")
				(number "3")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CA")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KCSA02-106"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "KCSA02-106"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Display_7Segment:KCSC02-106"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/KCSA02-106(Ver.11A).pdf"
			(at -12.7 12.065 0)
		)
		(property "Description" "One digit 7 segment super bright orange LED, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "KCSC02?106*"
			(at 0 0 0)
		)
		(symbol "KCSA02-106_0_0"
			(text "E"
				(at -2.54 1.778 0)
			)
			(text "F"
				(at -2.286 4.826 0)
			)
			(text "D"
				(at -0.254 1.016 0)
			)
			(text "G"
				(at 0 4.064 0)
			)
			(text "A"
				(at 0.254 5.588 0)
			)
			(text "C"
				(at 2.286 1.778 0)
			)
			(text "B"
				(at 2.54 4.826 0)
			)
			(text "DP"
				(at 3.556 0.254 0)
			)
		)
		(symbol "KCSA02-106_0_1")
		(symbol "KCSA02-106_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "6")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "1")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "9")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "10")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "5")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CA")
				(number "3")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CA")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KCSA02-107"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "KCSA02-107"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Display_7Segment:KCSC02-107"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/KCSA02-107(Ver.10A).pdf"
			(at -12.7 12.065 0)
		)
		(property "Description" "One digit 7 segment super bright orange LED, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "KCSC02?107*"
			(at 0 0 0)
		)
		(symbol "KCSA02-107_0_0"
			(text "E"
				(at -2.54 1.778 0)
			)
			(text "F"
				(at -2.286 4.826 0)
			)
			(text "D"
				(at -0.254 1.016 0)
			)
			(text "G"
				(at 0 4.064 0)
			)
			(text "A"
				(at 0.254 5.588 0)
			)
			(text "C"
				(at 2.286 1.778 0)
			)
			(text "B"
				(at 2.54 4.826 0)
			)
			(text "DP"
				(at 3.556 0.254 0)
			)
		)
		(symbol "KCSA02-107_0_1")
		(symbol "KCSA02-107_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "6")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "1")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "9")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "10")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "5")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CA")
				(number "3")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CA")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KCSA02-123"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "KCSA02-123"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Display_7Segment:KCSC02-123"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/KCSA02-123(Ver.9A).pdf"
			(at -12.7 12.065 0)
		)
		(property "Description" "One digit 7 segment green LED, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "KCSC02?123*"
			(at 0 0 0)
		)
		(symbol "KCSA02-123_0_0"
			(text "E"
				(at -2.54 1.778 0)
			)
			(text "F"
				(at -2.286 4.826 0)
			)
			(text "D"
				(at -0.254 1.016 0)
			)
			(text "G"
				(at 0 4.064 0)
			)
			(text "A"
				(at 0.254 5.588 0)
			)
			(text "C"
				(at 2.286 1.778 0)
			)
			(text "B"
				(at 2.54 4.826 0)
			)
			(text "DP"
				(at 3.556 0.254 0)
			)
		)
		(symbol "KCSA02-123_0_1")
		(symbol "KCSA02-123_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "6")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "1")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "9")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "10")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "5")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CA")
				(number "3")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CA")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KCSA02-136"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "KCSA02-136"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Display_7Segment:KCSC02-136"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/KCSA02-136(Ver.7B).pdf"
			(at -12.7 12.065 0)
		)
		(property "Description" "One digit 7 segment blue LED, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "KCSC02?136*"
			(at 0 0 0)
		)
		(symbol "KCSA02-136_0_0"
			(text "E"
				(at -2.54 1.778 0)
			)
			(text "F"
				(at -2.286 4.826 0)
			)
			(text "D"
				(at -0.254 1.016 0)
			)
			(text "G"
				(at 0 4.064 0)
			)
			(text "A"
				(at 0.254 5.588 0)
			)
			(text "C"
				(at 2.286 1.778 0)
			)
			(text "B"
				(at 2.54 4.826 0)
			)
			(text "DP"
				(at 3.556 0.254 0)
			)
		)
		(symbol "KCSA02-136_0_1")
		(symbol "KCSA02-136_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "6")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "1")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "9")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "10")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "5")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CA")
				(number "3")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CA")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KCSC02-105"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "KCSC02-105"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Display_7Segment:KCSC02-105"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/KCSC02-105(Ver.9A).pdf"
			(at -12.7 12.065 0)
		)
		(property "Description" "One digit 7 segment hyper red LED, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*KCSC02*105*"
			(at 0 0 0)
		)
		(symbol "KCSC02-105_0_0"
			(text "E"
				(at -2.54 1.778 0)
			)
			(text "F"
				(at -2.286 4.826 0)
			)
			(text "D"
				(at -0.254 1.016 0)
			)
			(text "G"
				(at 0 4.064 0)
			)
			(text "A"
				(at 0.254 5.588 0)
			)
			(text "C"
				(at 2.286 1.778 0)
			)
			(text "B"
				(at 2.54 4.826 0)
			)
			(text "DP"
				(at 3.556 0.254 0)
			)
		)
		(symbol "KCSC02-105_0_1")
		(symbol "KCSC02-105_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "6")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "1")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "9")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "10")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "5")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CC")
				(number "3")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CC")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KCSC02-106"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "KCSC02-106"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Display_7Segment:KCSC02-106"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/KCSC02-106(Ver.10A).pdf"
			(at -12.7 12.065 0)
		)
		(property "Description" "One digit 7 segment super bright orange LED, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "KCSC02?106*"
			(at 0 0 0)
		)
		(symbol "KCSC02-106_0_0"
			(text "E"
				(at -2.54 1.778 0)
			)
			(text "F"
				(at -2.286 4.826 0)
			)
			(text "D"
				(at -0.254 1.016 0)
			)
			(text "G"
				(at 0 4.064 0)
			)
			(text "A"
				(at 0.254 5.588 0)
			)
			(text "C"
				(at 2.286 1.778 0)
			)
			(text "B"
				(at 2.54 4.826 0)
			)
			(text "DP"
				(at 3.556 0.254 0)
			)
		)
		(symbol "KCSC02-106_0_1")
		(symbol "KCSC02-106_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "6")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "1")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "9")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "10")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "5")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CC")
				(number "3")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CC")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KCSC02-107"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "KCSC02-107"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Display_7Segment:KCSC02-107"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/KCSC02-106(Ver.10A).pdf"
			(at -12.7 12.065 0)
		)
		(property "Description" "One digit 7 segment super bright orange LED, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "KCSC02?107*"
			(at 0 0 0)
		)
		(symbol "KCSC02-107_0_0"
			(text "E"
				(at -2.54 1.778 0)
			)
			(text "F"
				(at -2.286 4.826 0)
			)
			(text "D"
				(at -0.254 1.016 0)
			)
			(text "G"
				(at 0 4.064 0)
			)
			(text "A"
				(at 0.254 5.588 0)
			)
			(text "C"
				(at 2.286 1.778 0)
			)
			(text "B"
				(at 2.54 4.826 0)
			)
			(text "DP"
				(at 3.556 0.254 0)
			)
		)
		(symbol "KCSC02-107_0_1")
		(symbol "KCSC02-107_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "6")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "1")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "9")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "10")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "5")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CC")
				(number "3")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CC")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KCSC02-123"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "KCSC02-123"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Display_7Segment:KCSC02-123"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/KCSC02-123(Ver.10A).pdf"
			(at -12.7 12.065 0)
		)
		(property "Description" "One digit 7 segment green LED, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "KCSC02?123*"
			(at 0 0 0)
		)
		(symbol "KCSC02-123_0_0"
			(text "E"
				(at -2.54 1.778 0)
			)
			(text "F"
				(at -2.286 4.826 0)
			)
			(text "D"
				(at -0.254 1.016 0)
			)
			(text "G"
				(at 0 4.064 0)
			)
			(text "A"
				(at 0.254 5.588 0)
			)
			(text "C"
				(at 2.286 1.778 0)
			)
			(text "B"
				(at 2.54 4.826 0)
			)
			(text "DP"
				(at 3.556 0.254 0)
			)
		)
		(symbol "KCSC02-123_0_1")
		(symbol "KCSC02-123_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "6")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "1")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "9")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "10")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "5")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CC")
				(number "3")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CC")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KCSC02-136"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "KCSC02-136"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Display_7Segment:KCSC02-136"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/KCSC02-136(Ver.6B).pdf"
			(at -12.7 12.065 0)
		)
		(property "Description" "One digit 7 segment blue LED, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "KCSC02?136*"
			(at 0 0 0)
		)
		(symbol "KCSC02-136_0_0"
			(text "E"
				(at -2.54 1.778 0)
			)
			(text "F"
				(at -2.286 4.826 0)
			)
			(text "D"
				(at -0.254 1.016 0)
			)
			(text "G"
				(at 0 4.064 0)
			)
			(text "A"
				(at 0.254 5.588 0)
			)
			(text "C"
				(at 2.286 1.778 0)
			)
			(text "B"
				(at 2.54 4.826 0)
			)
			(text "DP"
				(at 3.556 0.254 0)
			)
		)
		(symbol "KCSC02-136_0_1")
		(symbol "KCSC02-136_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "6")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "1")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "9")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "10")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "5")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CC")
				(number "3")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CC")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LCD-016N002L"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 18.796 0)
		)
		(property "Value" "LCD-016N002L"
			(at 8.636 18.796 0)
		)
		(property "Footprint" "Display:LCD-016N002L"
			(at 0.508 -23.368 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/37299/37299.pdf"
			(at 12.7 -7.62 0)
		)
		(property "Description" "LCD 12x2, 8 bit parallel bus, 3V or 5V VDD"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD dot-matrix"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LCD*016N002L*"
			(at 0 0 0)
		)
		(symbol "LCD-016N002L_1_1"
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "E")
				(number "6")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "R/~{W}")
				(number "5")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "RS")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DB0")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "DB1")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DB2")
				(number "9")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DB3")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "DB4")
				(number "11")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "DB5")
				(number "12")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "DB6")
				(number "13")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "DB7")
				(number "14")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin input line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "A/VEE")
				(number "15")
			)
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "K")
				(number "16")
			)
			(pin power_in line
				(at 10.16 0 180)
				(length 2.54)
				(name "A1")
				(number "A1")
			)
			(pin power_in line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "K1")
				(number "K1")
			)
			(pin power_in line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "A2")
				(number "A2")
			)
			(pin power_in line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "K2")
				(number "K2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM16255K"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "LM16255K"
			(at 4.318 16.51 0)
		)
		(property "Footprint" "Display:LM16255"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/Sharp/mXvtrzw.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "2 Lines, 12 character reflective LCD"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD dot-matrix"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LM16255*"
			(at 0 0 0)
		)
		(symbol "LM16255K_0_1")
		(symbol "LM16255K_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "RS")
				(number "4")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "R/W")
				(number "5")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "E")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "DB0")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DB1")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "DB2")
				(number "9")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DB3")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DB4")
				(number "11")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "DB5")
				(number "12")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "DB6")
				(number "13")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "DB7")
				(number "14")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC-4627JG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 12.7 0)
		)
		(property "Value" "LTC-4627JG"
			(at 17.78 12.7 0)
		)
		(property "Footprint" "Display_7Segment:LTC-4627Jx"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS30-2001-393/C4627JG.pdf"
			(at -10.16 0 0)
		)
		(property "Description" "4 digit 7 segment green, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LTC?4627J*"
			(at 0 0 0)
		)
		(symbol "LTC-4627JG_0_1")
		(symbol "LTC-4627JG_1_0"
			(text "E"
				(at -12.7 -1.397 0)
			)
			(text "F"
				(at -12.446 1.651 0)
			)
			(text "D"
				(at -10.414 -2.159 0)
			)
			(text "G"
				(at -10.16 0.889 0)
			)
			(text "A"
				(at -9.906 2.413 0)
			)
			(text "C"
				(at -7.874 -1.397 0)
			)
			(text "B"
				(at -7.62 1.651 0)
			)
			(text "DP"
				(at -6.604 -2.921 0)
			)
			(text "L2"
				(at -0.762 -1.905 0)
			)
			(text "L1"
				(at -0.508 2.159 0)
			)
			(text "L3"
				(at 6.096 2.159 0)
			)
		)
		(symbol "LTC-4627JG_1_1"
			(pin input line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "A")
				(number "14")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "B")
				(number "16")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "C")
				(number "13")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin input line
				(at -20.32 0 0)
				(length 2.54)
				(name "E")
				(number "5")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "F")
				(number "11")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "G")
				(number "15")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "7")
			)
			(pin no_connect line
				(at 17.78 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin input line
				(at 20.32 0 180)
				(length 2.54)
				(name "CA1")
				(number "1")
			)
			(pin input line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "CA2")
				(number "2")
			)
			(pin input line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "CA3")
				(number "6")
			)
			(pin input line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "CA4")
				(number "8")
			)
			(pin input line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "CAL")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTS-6960HR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "AFF"
			(at -7.874 13.97 0)
		)
		(property "Value" "LTS-6960HR"
			(at -2.032 13.97 0)
		)
		(property "Footprint" "Display_7Segment:7SegmentLED_LTS6760_LTS6780"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://datasheet.octopart.com/LTS-6960HR-Lite-On-datasheet-11803242.pdf"
			(at 0 0 0)
		)
		(property "Description" "DISPLAY 7 SEGMENTS common A."
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "7SegmentLED?LTS6760?LTS6780*"
			(at 0 0 0)
		)
		(symbol "LTS-6960HR_0_1")
		(symbol "LTS-6960HR_1_1"
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "a")
				(number "7")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "b")
				(number "6")
			)
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "c")
				(number "4")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "d")
				(number "2")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "e")
				(number "1")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "f")
				(number "9")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "g")
				(number "10")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "C.A.")
				(number "8")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "C.A.")
				(number "3")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "DP")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTS-6980HR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "AFF"
			(at -7.874 13.97 0)
		)
		(property "Value" "LTS-6980HR"
			(at 4.064 13.97 0)
		)
		(property "Footprint" "Display_7Segment:7SegmentLED_LTS6760_LTS6780"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://datasheet.octopart.com/LTS-6960HR-Lite-On-datasheet-11803242.pdf"
			(at 0 0 0)
		)
		(property "Description" "DISPLAY 7 SEGMENTS common K, high efficient red"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "7SegmentLED?LTS6760?LTS6780*"
			(at 0 0 0)
		)
		(symbol "LTS-6980HR_0_1")
		(symbol "LTS-6980HR_1_1"
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "a")
				(number "7")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "b")
				(number "6")
			)
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "c")
				(number "4")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "d")
				(number "2")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "e")
				(number "1")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "f")
				(number "9")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "g")
				(number "10")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "C.K.")
				(number "8")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "C.K.")
				(number "3")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "DP")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAN3410A"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "MAN3410A"
			(at 5.08 -14.224 0)
		)
		(property "Footprint" "Display_7Segment:MAN3410A"
			(at -12.7 -17.78 0)
		)
		(property "Datasheet" "https://www.digchip.com/datasheets/parts/datasheet/161/MAN3640A-pdf.php"
			(at 0.254 8.636 0)
		)
		(property "Description" "Single digit 7 segment high efficient green LED common anode right hand decimal"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MAN3410A*"
			(at 0 0 0)
		)
		(symbol "MAN3410A_0_0"
			(text "E"
				(at -2.286 6.858 0)
			)
			(text "F"
				(at -2.032 9.906 0)
			)
			(text "D"
				(at 0 6.096 0)
			)
			(text "G"
				(at 0.254 9.144 0)
			)
			(text "A"
				(at 0.508 10.668 0)
			)
			(text "C"
				(at 2.54 6.858 0)
			)
			(text "B"
				(at 2.794 9.906 0)
			)
			(text "DP"
				(at 3.81 5.334 0)
			)
		)
		(symbol "MAN3410A_0_1")
		(symbol "MAN3410A_1_1"
			(pin input line
				(at -7.62 10.16 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "B")
				(number "13")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "C")
				(number "10")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "E")
				(number "7")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "F")
				(number "2")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "G")
				(number "11")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "D.P.")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CA")
				(number "14")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CA")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAN3420A"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "MAN3420A"
			(at 5.08 -14.224 0)
		)
		(property "Footprint" "Display_7Segment:MAN3420A"
			(at -12.7 -17.78 0)
		)
		(property "Datasheet" "https://www.digchip.com/datasheets/parts/datasheet/161/MAN3640A-pdf.php"
			(at 2.032 8.89 0)
		)
		(property "Description" "Single digit 7 segment high efficient green LED common anode left hand decimal"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MAN3420A*"
			(at 0 0 0)
		)
		(symbol "MAN3420A_0_0"
			(text "DP"
				(at -1.778 5.588 0)
			)
			(text "E"
				(at -0.508 7.112 0)
			)
			(text "F"
				(at -0.254 10.16 0)
			)
			(text "D"
				(at 1.778 6.35 0)
			)
			(text "G"
				(at 2.032 9.398 0)
			)
			(text "A"
				(at 2.286 10.922 0)
			)
			(text "C"
				(at 4.318 7.112 0)
			)
			(text "B"
				(at 4.572 10.16 0)
			)
		)
		(symbol "MAN3420A_0_1")
		(symbol "MAN3420A_1_1"
			(pin input line
				(at -7.62 10.16 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "B")
				(number "13")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "C")
				(number "10")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "E")
				(number "7")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "F")
				(number "2")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "G")
				(number "11")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "D.P.")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CA")
				(number "14")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CA")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAN3440A"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "MAN3440A"
			(at 5.08 -14.224 0)
		)
		(property "Footprint" "Display_7Segment:MAN3410A"
			(at -12.7 -17.78 0)
		)
		(property "Datasheet" "https://www.digchip.com/datasheets/parts/datasheet/161/MAN3640A-pdf.php"
			(at 0.254 8.636 0)
		)
		(property "Description" "Single digit 7 segment high efficient green LED common anode right hand decimal"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MAN3410A*"
			(at 0 0 0)
		)
		(symbol "MAN3440A_0_0"
			(text "E"
				(at -2.286 6.858 0)
			)
			(text "F"
				(at -2.032 9.906 0)
			)
			(text "D"
				(at 0 6.096 0)
			)
			(text "G"
				(at 0.254 9.144 0)
			)
			(text "A"
				(at 0.508 10.668 0)
			)
			(text "C"
				(at 2.54 6.858 0)
			)
			(text "B"
				(at 2.794 9.906 0)
			)
			(text "DP"
				(at 3.81 5.334 0)
			)
		)
		(symbol "MAN3440A_0_1")
		(symbol "MAN3440A_1_1"
			(pin input line
				(at -7.62 10.16 0)
				(length 2.54)
				(name "A")
				(number "14")
			)
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "B")
				(number "13")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "E")
				(number "6")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "F")
				(number "1")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "D.P.")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 5.08 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CC")
				(number "12")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CC")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAN3610A"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "MAN3610A"
			(at 5.08 -14.224 0)
		)
		(property "Footprint" "Display_7Segment:MAN3610A"
			(at -12.7 -17.78 0)
		)
		(property "Datasheet" "https://www.digchip.com/datasheets/parts/datasheet/161/MAN3640A-pdf.php"
			(at 0.254 8.636 0)
		)
		(property "Description" "Single digit 7 segment orange LED common anode right hand decimal"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MAN3610A*"
			(at 0 0 0)
		)
		(symbol "MAN3610A_0_0"
			(text "E"
				(at -2.286 6.858 0)
			)
			(text "F"
				(at -2.032 9.906 0)
			)
			(text "D"
				(at 0 6.096 0)
			)
			(text "G"
				(at 0.254 9.144 0)
			)
			(text "A"
				(at 0.508 10.668 0)
			)
			(text "C"
				(at 2.54 6.858 0)
			)
			(text "B"
				(at 2.794 9.906 0)
			)
			(text "DP"
				(at 3.81 5.334 0)
			)
		)
		(symbol "MAN3610A_0_1")
		(symbol "MAN3610A_1_1"
			(pin input line
				(at -7.62 10.16 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "B")
				(number "13")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "C")
				(number "10")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "E")
				(number "7")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "F")
				(number "2")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "G")
				(number "11")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "D.P.")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CA")
				(number "14")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CA")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAN3620A"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "MAN3620A"
			(at 5.08 -14.224 0)
		)
		(property "Footprint" "Display_7Segment:MAN3620A"
			(at -12.7 -17.78 0)
		)
		(property "Datasheet" "https://www.digchip.com/datasheets/parts/datasheet/161/MAN3640A-pdf.php"
			(at 2.032 8.89 0)
		)
		(property "Description" "Single digit 7 segment orange LED common anode left hand decimal"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MAN3620A*"
			(at 0 0 0)
		)
		(symbol "MAN3620A_0_0"
			(text "DP"
				(at -1.778 5.588 0)
			)
			(text "E"
				(at -0.508 7.112 0)
			)
			(text "F"
				(at -0.254 10.16 0)
			)
			(text "D"
				(at 1.778 6.35 0)
			)
			(text "G"
				(at 2.032 9.398 0)
			)
			(text "A"
				(at 2.286 10.922 0)
			)
			(text "C"
				(at 4.318 7.112 0)
			)
			(text "B"
				(at 4.572 10.16 0)
			)
		)
		(symbol "MAN3620A_0_1")
		(symbol "MAN3620A_1_1"
			(pin input line
				(at -7.62 10.16 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "B")
				(number "13")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "C")
				(number "10")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "E")
				(number "7")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "F")
				(number "2")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "G")
				(number "11")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "D.P.")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CA")
				(number "14")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CA")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAN3630A"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "MAN3630A"
			(at 5.08 -14.224 0)
		)
		(property "Footprint" "Display_7Segment:MAN3630A"
			(at -12.7 -17.78 0)
		)
		(property "Datasheet" "https://www.digchip.com/datasheets/parts/datasheet/161/MAN3640A-pdf.php"
			(at 2.032 8.89 0)
		)
		(property "Description" "Overflow 7 segment orange LED common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MAN3630A*"
			(at 0 0 0)
		)
		(symbol "MAN3630A_0_0"
			(text "C"
				(at -1.905 9.3472 0)
			)
			(text "D"
				(at -0.7366 6.4262 0)
			)
			(text "B"
				(at 2.794 7.112 0)
			)
			(text "A"
				(at 3.175 10.16 0)
			)
		)
		(symbol "MAN3630A_0_1")
		(symbol "MAN3630A_1_1"
			(pin input line
				(at -7.62 10.16 0)
				(length 2.54)
				(name "A")
				(number "11")
			)
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "B")
				(number "10")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "CA_CD")
				(number "1")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "CA_CD")
				(number "3")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "CA_AB")
				(number "14")
			)
			(pin no_connect line
				(at 5.08 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 5.08 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAN3640A"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "MAN3640A"
			(at 5.08 -14.224 0)
		)
		(property "Footprint" "Display_7Segment:MAN3610A"
			(at -12.7 -17.78 0)
		)
		(property "Datasheet" "https://www.digchip.com/datasheets/parts/datasheet/161/MAN3640A-pdf.php"
			(at 0.254 8.636 0)
		)
		(property "Description" "Single digit 7 segment orange LED common anode right hand decimal"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MAN3610A*"
			(at 0 0 0)
		)
		(symbol "MAN3640A_0_0"
			(text "E"
				(at -2.286 6.858 0)
			)
			(text "F"
				(at -2.032 9.906 0)
			)
			(text "D"
				(at 0 6.096 0)
			)
			(text "G"
				(at 0.254 9.144 0)
			)
			(text "A"
				(at 0.508 10.668 0)
			)
			(text "C"
				(at 2.54 6.858 0)
			)
			(text "B"
				(at 2.794 9.906 0)
			)
			(text "DP"
				(at 3.81 5.334 0)
			)
		)
		(symbol "MAN3640A_0_1")
		(symbol "MAN3640A_1_1"
			(pin input line
				(at -7.62 10.16 0)
				(length 2.54)
				(name "A")
				(number "14")
			)
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "B")
				(number "13")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "E")
				(number "6")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "F")
				(number "1")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "D.P.")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 5.08 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CC")
				(number "12")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CC")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAN3810A"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "MAN3810A"
			(at 5.08 -14.224 0)
		)
		(property "Footprint" "Display_7Segment:MAN3810A"
			(at -12.7 -17.78 0)
		)
		(property "Datasheet" "https://www.digchip.com/datasheets/parts/datasheet/161/MAN3640A-pdf.php"
			(at 0.254 8.636 0)
		)
		(property "Description" "Single digit 7 segment yellow LED common anode right hand decimal"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MAN3810A*"
			(at 0 0 0)
		)
		(symbol "MAN3810A_0_0"
			(text "E"
				(at -2.286 6.858 0)
			)
			(text "F"
				(at -2.032 9.906 0)
			)
			(text "D"
				(at 0 6.096 0)
			)
			(text "G"
				(at 0.254 9.144 0)
			)
			(text "A"
				(at 0.508 10.668 0)
			)
			(text "C"
				(at 2.54 6.858 0)
			)
			(text "B"
				(at 2.794 9.906 0)
			)
			(text "DP"
				(at 3.81 5.334 0)
			)
		)
		(symbol "MAN3810A_0_1")
		(symbol "MAN3810A_1_1"
			(pin input line
				(at -7.62 10.16 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "B")
				(number "13")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "C")
				(number "10")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "E")
				(number "7")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "F")
				(number "2")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "G")
				(number "11")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "D.P.")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CA")
				(number "14")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CA")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAN3820A"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "MAN3820A"
			(at 5.08 -14.224 0)
		)
		(property "Footprint" "Display_7Segment:MAN3820A"
			(at -12.7 -17.78 0)
		)
		(property "Datasheet" "https://www.digchip.com/datasheets/parts/datasheet/161/MAN3640A-pdf.php"
			(at 2.032 8.89 0)
		)
		(property "Description" "Single digit 7 segment yellow LED common anode left hand decimal"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MAN3820A*"
			(at 0 0 0)
		)
		(symbol "MAN3820A_0_0"
			(text "DP"
				(at -1.778 5.588 0)
			)
			(text "E"
				(at -0.508 7.112 0)
			)
			(text "F"
				(at -0.254 10.16 0)
			)
			(text "D"
				(at 1.778 6.35 0)
			)
			(text "G"
				(at 2.032 9.398 0)
			)
			(text "A"
				(at 2.286 10.922 0)
			)
			(text "C"
				(at 4.318 7.112 0)
			)
			(text "B"
				(at 4.572 10.16 0)
			)
		)
		(symbol "MAN3820A_0_1")
		(symbol "MAN3820A_1_1"
			(pin input line
				(at -7.62 10.16 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "B")
				(number "13")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "C")
				(number "10")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "E")
				(number "7")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "F")
				(number "2")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "G")
				(number "11")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "D.P.")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CA")
				(number "14")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CA")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAN3840A"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "MAN3840A"
			(at 5.08 -14.224 0)
		)
		(property "Footprint" "Display_7Segment:MAN3810A"
			(at -12.7 -17.78 0)
		)
		(property "Datasheet" "https://www.digchip.com/datasheets/parts/datasheet/161/MAN3640A-pdf.php"
			(at 0.254 8.636 0)
		)
		(property "Description" "Single digit 7 segment yellow LED common anode right hand decimal"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MAN3810A*"
			(at 0 0 0)
		)
		(symbol "MAN3840A_0_0"
			(text "E"
				(at -2.286 6.858 0)
			)
			(text "F"
				(at -2.032 9.906 0)
			)
			(text "D"
				(at 0 6.096 0)
			)
			(text "G"
				(at 0.254 9.144 0)
			)
			(text "A"
				(at 0.508 10.668 0)
			)
			(text "C"
				(at 2.54 6.858 0)
			)
			(text "B"
				(at 2.794 9.906 0)
			)
			(text "DP"
				(at 3.81 5.334 0)
			)
		)
		(symbol "MAN3840A_0_1")
		(symbol "MAN3840A_1_1"
			(pin input line
				(at -7.62 10.16 0)
				(length 2.54)
				(name "A")
				(number "14")
			)
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "B")
				(number "13")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "E")
				(number "6")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "F")
				(number "1")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "D.P.")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 5.08 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CC")
				(number "12")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CC")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAN71A"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "MAN71A"
			(at 3.556 -14.224 0)
		)
		(property "Footprint" "Display_7Segment:MAN71A"
			(at -12.7 -17.78 0)
		)
		(property "Datasheet" "https://www.digchip.com/datasheets/parts/datasheet/161/MAN3640A-pdf.php"
			(at 0.254 8.636 0)
		)
		(property "Description" "Single digit 7 segment red LED common anode right hand decimal"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MAN71A*"
			(at 0 0 0)
		)
		(symbol "MAN71A_0_0"
			(text "E"
				(at -2.286 6.858 0)
			)
			(text "F"
				(at -2.032 9.906 0)
			)
			(text "D"
				(at 0 6.096 0)
			)
			(text "G"
				(at 0.254 9.144 0)
			)
			(text "A"
				(at 0.508 10.668 0)
			)
			(text "C"
				(at 2.54 6.858 0)
			)
			(text "B"
				(at 2.794 9.906 0)
			)
			(text "DP"
				(at 3.81 5.334 0)
			)
		)
		(symbol "MAN71A_0_1")
		(symbol "MAN71A_1_1"
			(pin input line
				(at -7.62 10.16 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "B")
				(number "13")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "C")
				(number "10")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "E")
				(number "7")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "F")
				(number "2")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "G")
				(number "11")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "D.P.")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CA")
				(number "14")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CA")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAN72A"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "MAN72A"
			(at 2.794 -14.224 0)
		)
		(property "Footprint" "Display_7Segment:MAN72A"
			(at -12.7 -17.78 0)
		)
		(property "Datasheet" "https://www.digchip.com/datasheets/parts/datasheet/161/MAN3640A-pdf.php"
			(at 2.032 8.89 0)
		)
		(property "Description" "Single digit 7 segment red LED common anode left hand decimal"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MAN72A*"
			(at 0 0 0)
		)
		(symbol "MAN72A_0_0"
			(text "DP"
				(at -1.778 5.588 0)
			)
			(text "E"
				(at -0.508 7.112 0)
			)
			(text "F"
				(at -0.254 10.16 0)
			)
			(text "D"
				(at 1.778 6.35 0)
			)
			(text "G"
				(at 2.032 9.398 0)
			)
			(text "A"
				(at 2.286 10.922 0)
			)
			(text "C"
				(at 4.318 7.112 0)
			)
			(text "B"
				(at 4.572 10.16 0)
			)
		)
		(symbol "MAN72A_0_1")
		(symbol "MAN72A_1_1"
			(pin input line
				(at -7.62 10.16 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "B")
				(number "13")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "C")
				(number "10")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "E")
				(number "7")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "F")
				(number "2")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "G")
				(number "11")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "D.P.")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CA")
				(number "14")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CA")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAN73A"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "MAN73A"
			(at 2.54 -14.224 0)
		)
		(property "Footprint" "Display_7Segment:MAN73A"
			(at -12.7 -17.78 0)
		)
		(property "Datasheet" "https://www.digchip.com/datasheets/parts/datasheet/161/MAN3640A-pdf.php"
			(at 2.032 8.89 0)
		)
		(property "Description" "Overflow 7 segment red LED common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MAN73A*"
			(at 0 0 0)
		)
		(symbol "MAN73A_0_0"
			(text "C"
				(at -1.905 9.3472 0)
			)
			(text "D"
				(at -0.7366 6.4262 0)
			)
			(text "B"
				(at 2.794 7.112 0)
			)
			(text "A"
				(at 3.175 10.16 0)
			)
		)
		(symbol "MAN73A_0_1")
		(symbol "MAN73A_1_1"
			(pin input line
				(at -7.62 10.16 0)
				(length 2.54)
				(name "A")
				(number "11")
			)
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "B")
				(number "10")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "CA_CD")
				(number "1")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "CA_CD")
				(number "3")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "CA_AB")
				(number "14")
			)
			(pin no_connect line
				(at 5.08 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 5.08 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAN74A"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "MAN74A"
			(at 2.794 -14.224 0)
		)
		(property "Footprint" "Display_7Segment:MAN71A"
			(at -12.7 -17.78 0)
		)
		(property "Datasheet" "https://www.digchip.com/datasheets/parts/datasheet/161/MAN3640A-pdf.php"
			(at 0.254 8.636 0)
		)
		(property "Description" "Single digit 7 segment red LED common anode right hand decimal"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MAN71A*"
			(at 0 0 0)
		)
		(symbol "MAN74A_0_0"
			(text "E"
				(at -2.286 6.858 0)
			)
			(text "F"
				(at -2.032 9.906 0)
			)
			(text "D"
				(at 0 6.096 0)
			)
			(text "G"
				(at 0.254 9.144 0)
			)
			(text "A"
				(at 0.508 10.668 0)
			)
			(text "C"
				(at 2.54 6.858 0)
			)
			(text "B"
				(at 2.794 9.906 0)
			)
			(text "DP"
				(at 3.81 5.334 0)
			)
		)
		(symbol "MAN74A_0_1")
		(symbol "MAN74A_1_1"
			(pin input line
				(at -7.62 10.16 0)
				(length 2.54)
				(name "A")
				(number "14")
			)
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "B")
				(number "13")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D")
				(number "7")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "E")
				(number "6")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "F")
				(number "1")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "D.P.")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 5.08 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CC")
				(number "12")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CC")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NHD-0420H1Z"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 19.05 0)
		)
		(property "Value" "NHD-0420H1Z"
			(at 5.08 19.05 0)
		)
		(property "Footprint" "Display:NHD-0420H1Z"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "http://www.newhavendisplay.com/specs/NHD-0420H1Z-FSW-GBW-33V3.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "LCD 20x4 Alphanumeric 16pin Blue/White/Green Backlight, 8bit parallel, 3.3V VDD"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD 20x4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "NHD*0420H1Z*"
			(at 0 0 0)
		)
		(symbol "NHD-0420H1Z_0_1")
		(symbol "NHD-0420H1Z_1_1"
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "RS")
				(number "4")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "R/W")
				(number "5")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "E")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DB0")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "DB1")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DB2")
				(number "9")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DB3")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "DB4")
				(number "11")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "DB5")
				(number "12")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "DB6")
				(number "13")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "DB7")
				(number "14")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VO")
				(number "3")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "K")
				(number "16")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "A")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NHD-C0220BIZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "NHD-C0220BIZ"
			(at 8.89 11.43 0)
		)
		(property "Footprint" "Display:NHD-C0220BiZ"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.newhavendisplay.com/specs/NHD-C0220BiZ-FSW-FBW-3V3M.pdf"
			(at -7.62 15.24 0)
		)
		(property "Description" "LCD 20x2 Alphanumeric 10pin Blue/White/Green Backlight, i2c, 3.3V VDD"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD 20x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "NHD*C0220BiZ*"
			(at 0 0 0)
		)
		(symbol "NHD-C0220BIZ_0_1")
		(symbol "NHD-C0220BIZ_1_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{RST}")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "VOUT")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "C1+")
				(number "7")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "C1-")
				(number "8")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "A")
				(number "9")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "K")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NHD-C0220BIZ-FSRGB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.335 0)
		)
		(property "Value" "NHD-C0220BIZ-FSRGB"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Display:NHD-C0220BiZ-FSRGB"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://newhavendisplay.com/content/specs/NHD-C0220BiZ-FSRGB-FBW-3VM.pdf"
			(at 0 0 0)
		)
		(property "Description" "2x20 character LCD module with common anode RGB backlight, I2C, 3.3V"
			(at 0 0 0)
		)
		(property "ki_keywords" "lcd rgb character st736i i2c 2-wire twi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "NHD?C0220BiZ?FSRGB*"
			(at 0 0 0)
		)
		(symbol "NHD-C0220BIZ-FSRGB_0_1")
		(symbol "NHD-C0220BIZ-FSRGB_1_1"
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "LED+")
				(number "9")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "(R)LED-")
				(number "12")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "(G)LED-")
				(number "11")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "(B)LED-")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SDA")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "~{RST}")
				(number "1")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V_{DD}")
				(number "5")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "V_{SS}")
				(number "4")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "C1+")
				(number "7")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "C1-")
				(number "8")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "V_{out}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RC1602A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "RC1602A"
			(at 2.794 16.51 0)
		)
		(property "Footprint" "Display:RC1602A"
			(at 2.54 -20.32 0)
		)
		(property "Datasheet" "http://www.raystar-optronics.com/down.php?ProID=18"
			(at 2.54 -2.54 0)
		)
		(property "Description" "LCD 16x2 Alphanumeric gray backlight, 3 or 5V VDD"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD dot-matrix"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*RC1602A*"
			(at 0 0 0)
		)
		(symbol "RC1602A_0_1")
		(symbol "RC1602A_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "RS")
				(number "4")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "R/W")
				(number "5")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "E")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "DB0")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DB1")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "DB2")
				(number "9")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DB3")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DB4")
				(number "11")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "DB5")
				(number "12")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "DB6")
				(number "13")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "DB7")
				(number "14")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "K")
				(number "16")
			)
			(pin power_in line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "A/VEE")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RC1602A-GHW-ESX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.842 19.05 0)
		)
		(property "Value" "RC1602A-GHW-ESX"
			(at 3.81 19.05 0)
		)
		(property "Footprint" "Display:RC1602A"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "http://www.raystar-optronics.com/down.php?ProID=18"
			(at -12.7 17.78 0)
		)
		(property "Description" "LCD 16x2 Alphanumeric 16pin Gray Backlight"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD dot-matrix"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RC1602A*"
			(at 0 0 0)
		)
		(symbol "RC1602A-GHW-ESX_0_0"
			(text "16x2"
				(at 0.254 6.35 0)
			)
		)
		(symbol "RC1602A-GHW-ESX_0_1")
		(symbol "RC1602A-GHW-ESX_1_1"
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "RS")
				(number "4")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "R/~{W}")
				(number "5")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "~{E}")
				(number "6")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "Vo")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DB0")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "DB1")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DB2")
				(number "9")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DB3")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "DB4")
				(number "11")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "DB5")
				(number "12")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "DB6")
				(number "13")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "DB7")
				(number "14")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "K")
				(number "16")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "A/VEE")
				(number "15")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "A")
				(number "A1")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "K")
				(number "K1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SA15-11SRWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "SA15-11SRWA"
			(at 0 13.97 0)
		)
		(property "Footprint" "Display_7Segment:SA15-11xxx"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/SA15-11SRWA.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Super Bright Red Single-digit Numeric Display with white white diffused lens, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SA15?11*"
			(at 0 0 0)
		)
		(symbol "SA15-11SRWA_1_0"
			(text "E"
				(at -2.54 3.048 0)
			)
			(text "F"
				(at -2.286 6.096 0)
			)
			(text "D"
				(at -0.254 2.286 0)
			)
			(text "G"
				(at 0 5.334 0)
			)
			(text "A"
				(at 0.254 6.858 0)
			)
			(text "C"
				(at 2.286 3.048 0)
			)
			(text "B"
				(at 2.54 6.096 0)
			)
			(text "DP"
				(at 3.556 1.524 0)
			)
		)
		(symbol "SA15-11SRWA_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "6")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "2")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "9")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "10")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "8")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CA")
				(number "5")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CA")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SA39-11EWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "SA39-11EWA"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:Sx39-1xxxxx"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/sa39-11ewa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single digit 7 segment display, high efficiency red, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "S?39?1*"
			(at 0 0 0)
		)
		(symbol "SA39-11EWA_1_0"
			(text "E"
				(at -2.54 -1.397 0)
			)
			(text "F"
				(at -2.286 1.651 0)
			)
			(text "D"
				(at -0.254 -2.159 0)
			)
			(text "G"
				(at 0 0.889 0)
			)
			(text "A"
				(at 0.254 2.413 0)
			)
			(text "C"
				(at 2.286 -1.397 0)
			)
			(text "B"
				(at 2.54 1.651 0)
			)
			(text "DP"
				(at 3.556 -2.921 0)
			)
		)
		(symbol "SA39-11EWA_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "9")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "7")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "4")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "2")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "6")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CA")
				(number "3")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CA")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SA39-12EWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "SA39-12EWA"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:Sx39-1xxxxx"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/sa39-12ewa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single digit 7 segment display, high efficiency red, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "S?39?1*"
			(at 0 0 0)
		)
		(symbol "SA39-12EWA_1_0"
			(text "E"
				(at -2.54 -1.397 0)
			)
			(text "F"
				(at -2.286 1.651 0)
			)
			(text "D"
				(at -0.254 -2.159 0)
			)
			(text "G"
				(at 0 0.889 0)
			)
			(text "A"
				(at 0.254 2.413 0)
			)
			(text "C"
				(at 2.286 -1.397 0)
			)
			(text "B"
				(at 2.54 1.651 0)
			)
			(text "DP"
				(at 3.556 -2.921 0)
			)
		)
		(symbol "SA39-12EWA_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "9")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "4")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "2")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "7")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CA")
				(number "1")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CA")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SBC18-11SURKCGKWA"
		(pin_names
			(offset 0.635)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "SBC18-11SURKCGKWA"
			(at -4.826 -14.224 0)
		)
		(property "Footprint" "Display_7Segment:SBC18-11SURKCGKWA"
			(at -18.542 -18.034 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/SBC18-11SURKCGKWA(Ver.6A).pdf"
			(at 0 4.826 0)
		)
		(property "Description" "Single digit 7 segment hyper red and green LED display, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SBC18*11*"
			(at 0 0 0)
		)
		(symbol "SBC18-11SURKCGKWA_0_0"
			(text "E"
				(at -2.54 3.048 0)
			)
			(text "F"
				(at -2.286 6.096 0)
			)
			(text "D"
				(at -0.254 2.286 0)
			)
			(text "G"
				(at 0 5.334 0)
			)
			(text "A"
				(at 0.254 6.858 0)
			)
			(text "C"
				(at 2.286 3.048 0)
			)
			(text "B"
				(at 2.54 6.096 0)
			)
			(text "DP"
				(at 3.556 1.524 0)
			)
		)
		(symbol "SBC18-11SURKCGKWA_0_1")
		(symbol "SBC18-11SURKCGKWA_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "6")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "2")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "9")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "10")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "8")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CC")
				(number "5")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CC")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SC39-11EWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "SC39-11EWA"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:Sx39-1xxxxx"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/sc39-11ewa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single digit 7 segment display, high efficiency red, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "S?39?1*"
			(at 0 0 0)
		)
		(symbol "SC39-11EWA_1_0"
			(text "E"
				(at -2.54 -1.397 0)
			)
			(text "F"
				(at -2.286 1.651 0)
			)
			(text "D"
				(at -0.254 -2.159 0)
			)
			(text "G"
				(at 0 0.889 0)
			)
			(text "A"
				(at 0.254 2.413 0)
			)
			(text "C"
				(at 2.286 -1.397 0)
			)
			(text "B"
				(at 2.54 1.651 0)
			)
			(text "DP"
				(at 3.556 -2.921 0)
			)
		)
		(symbol "SC39-11EWA_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "9")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "7")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "4")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "2")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "6")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CC")
				(number "3")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CC")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SC39-12EWA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "SC39-12EWA"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:Sx39-1xxxxx"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/sc39-12ewa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single digit 7 segment display, high efficiency red, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "S?39?1*"
			(at 0 0 0)
		)
		(symbol "SC39-12EWA_1_0"
			(text "E"
				(at -2.54 -1.397 0)
			)
			(text "F"
				(at -2.286 1.651 0)
			)
			(text "D"
				(at -0.254 -2.159 0)
			)
			(text "G"
				(at 0 0.889 0)
			)
			(text "A"
				(at 0.254 2.413 0)
			)
			(text "C"
				(at 2.286 -1.397 0)
			)
			(text "B"
				(at 2.54 1.651 0)
			)
			(text "DP"
				(at 3.556 -2.921 0)
			)
		)
		(symbol "SC39-12EWA_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "9")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "8")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "4")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "2")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "7")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CC")
				(number "1")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CC")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SM420561N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "SM420561N"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Display_7Segment:7SegmentLED_LTS6760_LTS6780"
			(at 1.27 -15.24 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/szlcsc/Wuxi-ARK-Tech-Elec-SM420561N_C141367.pdf"
			(at -12.7 12.065 0)
		)
		(property "Description" "One digit 7 segment blue LED, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "7SegmentLED?LTS6760?LTS6780*"
			(at 0 0 0)
		)
		(symbol "SM420561N_0_0"
			(text "E"
				(at -2.54 1.778 0)
			)
			(text "F"
				(at -2.286 4.826 0)
			)
			(text "D"
				(at -0.254 1.016 0)
			)
			(text "G"
				(at 0 4.064 0)
			)
			(text "A"
				(at 0.254 5.588 0)
			)
			(text "C"
				(at 2.286 1.778 0)
			)
			(text "B"
				(at 2.54 4.826 0)
			)
			(text "DP"
				(at 3.556 0.254 0)
			)
		)
		(symbol "SM420561N_0_1")
		(symbol "SM420561N_1_1"
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "B")
				(number "6")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "E")
				(number "1")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "F")
				(number "9")
			)
			(pin input line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "G")
				(number "10")
			)
			(pin input line
				(at -7.62 -10.16 0)
				(length 2.54)
				(name "DP")
				(number "5")
			)
			(pin input line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "CC")
				(number "3")
			)
			(pin input line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "CC")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "WC1602A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "DS"
			(at -5.842 19.05 0)
		)
		(property "Value" "WC1602A"
			(at 5.334 19.05 0)
		)
		(property "Footprint" "Display:WC1602A"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "http://www.wincomlcd.com/pdf/WC1602A-SFYLYHTC06.pdf"
			(at 17.78 0 0)
		)
		(property "Description" "LCD 16x2 Alphanumeric , 8 bit parallel bus, 5V VDD"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD dot-matrix"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*WC*1602A*"
			(at 0 0 0)
		)
		(symbol "WC1602A_1_1"
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "E")
				(number "6")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "R/W")
				(number "5")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "RS")
				(number "4")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D0")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "D1")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "D2")
				(number "9")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "D3")
				(number "10")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "D4")
				(number "11")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "D5")
				(number "12")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "D6")
				(number "13")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "D7")
				(number "14")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin input line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "LED(+)")
				(number "15")
			)
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "LED(-)")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "D148K"
		(extends "D168K")
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "D148K"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Display_7Segment:D1X8K"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://ia800903.us.archive.org/24/items/CTKD1x8K/Cromatek%20D168K.pdf"
			(at -12.7 12.065 0)
		)
		(property "Description" "One digit 7 segment yellowish-green LED, low current, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D1X8K*"
			(at 0 0 0)
		)
	)
	(symbol "D198K"
		(extends "D168K")
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "D198K"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Display_7Segment:D1X8K"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://ia800903.us.archive.org/24/items/CTKD1x8K/Cromatek%20D168K.pdf"
			(at -12.7 12.065 0)
		)
		(property "Description" "One digit 7 segment orangish-red LED, low current, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D1X8K*"
			(at 0 0 0)
		)
	)
	(symbol "D1X8K-14BL"
		(extends "D168K")
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "D1X8K-14BL"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Display_7Segment:D1X8K"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://ia800903.us.archive.org/24/items/CTKD1x8K/Cromatek%20D168K.pdf"
			(at -12.7 12.065 0)
		)
		(property "Description" "One digit 7 segment ultra bright blue LED, low current, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D1X8K*"
			(at 0 0 0)
		)
	)
	(symbol "DA04-11EWA"
		(extends "DA04-11SURKWA")
		(property "Reference" "U"
			(at -13.97 13.97 0)
		)
		(property "Value" "DA04-11EWA"
			(at 15.24 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA04-11SURKWA"
			(at 0.635 -15.875 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/DA04-11EWA.pdf"
			(at -3.048 -10.16 0)
		)
		(property "Description" "Double 7 segment high efficient red LED common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA04*11*"
			(at 0 0 0)
		)
	)
	(symbol "DA04-11GWA"
		(extends "DA04-11CGKWA")
		(property "Reference" "U"
			(at -13.97 13.97 0)
		)
		(property "Value" "DA04-11GWA"
			(at 15.24 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA04-11CGKWA"
			(at 0.635 -15.875 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/DA04-11GWA.pdf"
			(at -3.048 -10.16 0)
		)
		(property "Description" "Double 7 segment green LED common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA04*11*"
			(at 0 0 0)
		)
	)
	(symbol "DA04-11SRWA"
		(extends "DA04-11SURKWA")
		(property "Reference" "U"
			(at -13.97 13.97 0)
		)
		(property "Value" "DA04-11SRWA"
			(at 15.24 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA04-11SURKWA"
			(at 0.635 -15.875 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/DA04-11SRWA.pdf"
			(at -3.048 -10.16 0)
		)
		(property "Description" "Double 7 segment super bright red LED common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA04*11*"
			(at 0 0 0)
		)
	)
	(symbol "DA56-11EWA"
		(extends "DA56-11SURKWA")
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "DA56-11EWA"
			(at 12.7 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA56-11SURKWA"
			(at 0.508 -16.51 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/DA56-11EWA.pdf"
			(at -3.048 2.54 0)
		)
		(property "Description" "Double digit 7 segment high efficient red LED common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA56*11*"
			(at 0 0 0)
		)
	)
	(symbol "DA56-11GWA"
		(extends "DA56-11CGKWA")
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "DA56-11GWA"
			(at 12.7 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA56-11CGKWA"
			(at 0.508 -16.51 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/DA56-11GWA.pdf"
			(at -3.048 2.54 0)
		)
		(property "Description" "Double digit 7 segment green LED common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA56*11*"
			(at 0 0 0)
		)
	)
	(symbol "DA56-11SRWA"
		(extends "DA56-11SURKWA")
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "DA56-11SRWA"
			(at 12.7 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA56-11SURKWA"
			(at 0.508 -16.51 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/DA56-11SRWA.pdf"
			(at -3.048 2.54 0)
		)
		(property "Description" "Double digit 7 segment super bright red LED common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA56*11*"
			(at 0 0 0)
		)
	)
	(symbol "DA56-11YWA"
		(extends "DA56-11SYKWA")
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "DA56-11YWA"
			(at 12.065 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA56-11SYKWA"
			(at 0.508 -16.51 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/DA56-11YWA.pdf"
			(at -3.048 2.54 0)
		)
		(property "Description" "Double digit 7 segment super bright yellow LED common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA56*11*"
			(at 0 0 0)
		)
	)
	(symbol "DC56-11EWA"
		(extends "DC56-11SURKWA")
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "DC56-11EWA"
			(at 12.065 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA56-11SURKWA"
			(at 0.508 -16.51 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/DC56-11EWA.pdf"
			(at -3.048 2.54 0)
		)
		(property "Description" "Double digit 7 segment super bright red LED common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA56*11*"
			(at 0 0 0)
		)
	)
	(symbol "DC56-11GWA"
		(extends "DC56-11CGKWA")
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "DC56-11GWA"
			(at 12.065 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA56-11CGKWA"
			(at 0.508 -16.51 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/DC56-11GWA.pdf"
			(at -3.048 2.54 0)
		)
		(property "Description" "Double digit 7 segment green LED common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA56*11*"
			(at 0 0 0)
		)
	)
	(symbol "DC56-11SRWA"
		(extends "DC56-11SURKWA")
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "DC56-11SRWA"
			(at 12.065 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA56-11SURKWA"
			(at 0.508 -16.51 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/DC56-11SRWA.pdf"
			(at -3.048 2.54 0)
		)
		(property "Description" "Double digit 7 segment super bright red LED common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA56*11*"
			(at 0 0 0)
		)
	)
	(symbol "DC56-11YWA"
		(extends "DC56-11SYKWA")
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "DC56-11YWA"
			(at 12.065 13.97 0)
		)
		(property "Footprint" "Display_7Segment:DA56-11SYKWA"
			(at 0.508 -16.51 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/DC56-11YWA.pdf"
			(at -3.048 2.54 0)
		)
		(property "Description" "Double digit 7 segment yellow LED common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DA56*11*"
			(at 0 0 0)
		)
	)
	(symbol "HDSP-7501"
		(extends "HDSP-A151")
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "HDSP-7501"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:HDSP-A151"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-2553EN"
			(at -12.7 13.97 0)
		)
		(property "Description" "One digit 7 segment high efficiency red, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?A151*"
			(at 0 0 0)
		)
	)
	(symbol "HDSP-7503"
		(extends "HDSP-A153")
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "HDSP-7503"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:HDSP-A151"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-2553EN"
			(at -10.16 13.97 0)
		)
		(property "Description" "One digit 7 segment high efficiency red, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?A151*"
			(at 0 0 0)
		)
	)
	(symbol "LTC-4627JD"
		(extends "LTC-4627JG")
		(property "Reference" "U"
			(at -17.78 12.7 0)
		)
		(property "Value" "LTC-4627JD"
			(at 17.78 12.7 0)
		)
		(property "Footprint" "Display_7Segment:LTC-4627Jx"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS30-2001-093/LTC-4627JD.pdf"
			(at -10.16 0 0)
		)
		(property "Description" "4 digit 7 segment hyper red, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LTC?4627J*"
			(at 0 0 0)
		)
	)
	(symbol "LTC-4627JD-01"
		(extends "LTC-4627JG")
		(property "Reference" "U"
			(at -17.78 12.7 0)
		)
		(property "Value" "LTC-4627JD-01"
			(at 17.78 12.7 0)
		)
		(property "Footprint" "Display_7Segment:LTC-4627Jx"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS30-2008-0116/LTC-4627JD-01.pdf"
			(at -10.16 0 0)
		)
		(property "Description" "4 digit 7 segment hyper red, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LTC?4627J*"
			(at 0 0 0)
		)
	)
	(symbol "LTC-4627JF"
		(extends "LTC-4627JG")
		(property "Reference" "U"
			(at -17.78 12.7 0)
		)
		(property "Value" "LTC-4627JF"
			(at 17.78 12.7 0)
		)
		(property "Footprint" "Display_7Segment:LTC-4627Jx"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS30-2000-192/C4627JF.pdf"
			(at -10.16 0 0)
		)
		(property "Description" "4 digit 7 segment yellow orange, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LTC?4627J*"
			(at 0 0 0)
		)
	)
	(symbol "LTC-4627JR"
		(extends "LTC-4627JG")
		(property "Reference" "U"
			(at -17.78 12.7 0)
		)
		(property "Value" "LTC-4627JR"
			(at 17.78 12.7 0)
		)
		(property "Footprint" "Display_7Segment:LTC-4627Jx"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS30-2000-185/LTC-4627JR.pdf"
			(at -10.16 0 0)
		)
		(property "Description" "4 digit 7 segment super red, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LTC?4627J*"
			(at 0 0 0)
		)
	)
	(symbol "LTC-4627JS"
		(extends "LTC-4627JG")
		(property "Reference" "U"
			(at -17.78 12.7 0)
		)
		(property "Value" "LTC-4627JS"
			(at 17.78 12.7 0)
		)
		(property "Footprint" "Display_7Segment:LTC-4627Jx"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS30-2000-186/LTC-4627JS.pdf"
			(at -10.16 0 0)
		)
		(property "Description" "4 digit 7 segment yellow, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LTC?4627J*"
			(at 0 0 0)
		)
	)
	(symbol "SA15-11EWA"
		(extends "SA15-11SRWA")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "SA15-11EWA"
			(at 0 13.97 0)
		)
		(property "Footprint" "Display_7Segment:SA15-11xxx"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/SA15-11EWA.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "High Efficiency Red Single-digit Numeric Display with white white diffused lens, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SA15?11*"
			(at 0 0 0)
		)
	)
	(symbol "SA15-11GWA"
		(extends "SA15-11SRWA")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "SA15-11GWA"
			(at 0 13.97 0)
		)
		(property "Footprint" "Display_7Segment:SA15-11xxx"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/SA15-11GWA.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Green Single-digit Numeric Display with white white diffused lens, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SA15?11*"
			(at 0 0 0)
		)
	)
	(symbol "SA39-11GWA"
		(extends "SA39-11EWA")
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "SA39-11GWA"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:Sx39-1xxxxx"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/sa39-11gwa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single digit 7 segment display, green, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "S?39?1*"
			(at 0 0 0)
		)
	)
	(symbol "SA39-11SRWA"
		(extends "SA39-11EWA")
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "SA39-11SRWA"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:Sx39-1xxxxx"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/sa39-11srwa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single digit 7 segment display, super bright red, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "S?39?1*"
			(at 0 0 0)
		)
	)
	(symbol "SA39-11YWA"
		(extends "SA39-11EWA")
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "SA39-11YWA"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:Sx39-1xxxxx"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/sa39-11ywa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single digit 7 segment display, yellow, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "S?39?1*"
			(at 0 0 0)
		)
	)
	(symbol "SA39-12GWA"
		(extends "SA39-12EWA")
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "SA39-12GWA"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:Sx39-1xxxxx"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/sa39-12gwa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single digit 7 segment display, green, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "S?39?1*"
			(at 0 0 0)
		)
	)
	(symbol "SA39-12SRWA"
		(extends "SA39-12EWA")
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "SA39-12SRWA"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:Sx39-1xxxxx"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/sa39-12srwa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single digit 7 segment display, super bright red, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "S?39?1*"
			(at 0 0 0)
		)
	)
	(symbol "SA39-12YWA"
		(extends "SA39-12EWA")
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "SA39-12YWA"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:Sx39-1xxxxx"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/sa39-12ywa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single digit 7 segment display, yellow, common anode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "S?39?1*"
			(at 0 0 0)
		)
	)
	(symbol "SBC18-11EGWA"
		(extends "SBC18-11SURKCGKWA")
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "SBC18-11EGWA"
			(at -4.826 -14.224 0)
		)
		(property "Footprint" "Display_7Segment:SBC18-11SURKCGKWA"
			(at -18.542 -18.034 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/SBC18-11EGWA.pdf"
			(at 0 4.826 0)
		)
		(property "Description" "Single digit 7 segment hyper red and green LED display, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SBC18*11*"
			(at 0 0 0)
		)
	)
	(symbol "SC39-11GWA"
		(extends "SC39-11EWA")
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "SC39-11GWA"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:Sx39-1xxxxx"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/sc39-11gwa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single digit 7 segment display, green, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "S?39?1*"
			(at 0 0 0)
		)
	)
	(symbol "SC39-11SRWA"
		(extends "SC39-11EWA")
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "SC39-11SRWA"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:Sx39-1xxxxx"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/sc39-11srwa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single digit 7 segment display, super bright red, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "S?39?1*"
			(at 0 0 0)
		)
	)
	(symbol "SC39-11YWA"
		(extends "SC39-11EWA")
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "SC39-11YWA"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:Sx39-1xxxxx"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/sc39-11ywa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single digit 7 segment display, yellow, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "S?39?1*"
			(at 0 0 0)
		)
	)
	(symbol "SC39-12GWA"
		(extends "SC39-12EWA")
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "SC39-12GWA"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:Sx39-1xxxxx"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/sc39-12gwa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single digit 7 segment display, green, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "S?39?1*"
			(at 0 0 0)
		)
	)
	(symbol "SC39-12SRWA"
		(extends "SC39-12EWA")
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "SC39-12SRWA"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:Sx39-1xxxxx"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/sc39-12srwa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single digit 7 segment display, super bright red, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "S?39?1*"
			(at 0 0 0)
		)
	)
	(symbol "SC39-12YWA"
		(extends "SC39-12EWA")
		(property "Reference" "U"
			(at -3.81 13.97 0)
		)
		(property "Value" "SC39-12YWA"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Display_7Segment:Sx39-1xxxxx"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/sc39-12ywa.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single digit 7 segment display, yellow, common cathode"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "S?39?1*"
			(at 0 0 0)
		)
	)
)
