(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AG12864E"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "DS"
			(at -8.382 19.05 0)
		)
		(property "Value" "AG12864E"
			(at 5.588 19.05 0)
		)
		(property "Footprint" "Display:AG12864E"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.digchip.com/datasheets/parts/datasheet/1121/AG-12864E-pdf.php"
			(at 5.08 -5.08 0)
		)
		(property "Description" "Graphics Display 128x64px,  8b parallel, 1/64 Duty, 3.3V or 5V VDD"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*AG12864E*"
			(at 0 0 0)
		)
		(symbol "AG12864E_0_1")
		(symbol "AG12864E_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "E")
				(number "17")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D/~{I}")
				(number "16")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{RST}")
				(number "14")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "R/~{W}")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "DB0")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "DB1")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DB2")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "DB3")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "DB4")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "DB5")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "DB6")
				(number "10")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "DB7")
				(number "11")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VEE")
				(number "18")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "LEDA/EL")
				(number "19")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "LEDK/EL")
				(number "20")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "~{CS1}")
				(number "12")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "~{CS2}")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EA_DOGL128X-6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 19.05 0)
		)
		(property "Value" "EA_DOGL128X-6"
			(at 19.05 19.05 0)
		)
		(property "Footprint" "Display:EA_DOGL128-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.lcd-module.com/eng/pdf/grafik/dogl128-6e.pdf"
			(at 0 0 0)
		)
		(property "Description" "EA DOGL128X-6 Graphical Display 128x64 optional backlight SPI 3.0-3.3V"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "EA*DOGL128*6*"
			(at 0 0 0)
		)
		(symbol "EA_DOGL128X-6_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "~{RST}")
				(number "39")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "~{CS1B}")
				(number "40")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "A0")
				(number "38")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SI")
				(number "36")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "37")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CAP1P")
				(number "29")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CAP1N")
				(number "30")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "CAP3P")
				(number "31")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "CAP2N")
				(number "27")
			)
			(pin passive line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "CAP2P")
				(number "28")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VDD2")
				(number "34")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "26")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 5.08 20.32 270)
				(length 2.54)
				(name "A1+")
				(number "1")
			)
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 2.54)
				(name "C1-")
				(number "18")
			)
			(pin power_in line
				(at 7.62 20.32 270)
				(length 2.54)
				(name "A2+")
				(number "2")
			)
			(pin power_in line
				(at 7.62 -20.32 90)
				(length 2.54)
				(name "C2-")
				(number "19")
			)
			(pin power_in line
				(at 10.16 20.32 270)
				(length 2.54)
				(name "A3+")
				(number "3")
			)
			(pin power_in line
				(at 10.16 -20.32 90)
				(length 2.54)
				(name "C3-")
				(number "20")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "V0")
				(number "21")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "V1")
				(number "22")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "V2")
				(number "23")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "V3")
				(number "24")
			)
			(pin passive line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "V4")
				(number "25")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "VOUT")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EA_DOGM128X-6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 19.05 0)
		)
		(property "Value" "EA_DOGM128X-6"
			(at 19.05 19.05 0)
		)
		(property "Footprint" "Display:EA_DOGM128-6"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.lcd-module.de/eng/pdf/grafik/dogm128e.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "EA DOGM128X-6 Graphical Display 128x64 optional backlight SPI 3.0-3.3V"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "EA*DOGM128*6*"
			(at 0 0 0)
		)
		(symbol "EA_DOGM128X-6_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "~{RST}")
				(number "39")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "~{CS1B}")
				(number "40")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "A0")
				(number "38")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SI")
				(number "36")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "37")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CAP1P")
				(number "29")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CAP1N")
				(number "30")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "CAP3P")
				(number "31")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "CAP2N")
				(number "27")
			)
			(pin passive line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "CAP2P")
				(number "28")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VDD2")
				(number "34")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "26")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 5.08 20.32 270)
				(length 2.54)
				(name "A1+")
				(number "1")
			)
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 2.54)
				(name "C1-")
				(number "18")
			)
			(pin power_in line
				(at 7.62 20.32 270)
				(length 2.54)
				(name "A2+")
				(number "2")
			)
			(pin power_in line
				(at 7.62 -20.32 90)
				(length 2.54)
				(name "C2-")
				(number "19")
			)
			(pin power_in line
				(at 10.16 20.32 270)
				(length 2.54)
				(name "A3+")
				(number "3")
			)
			(pin power_in line
				(at 10.16 -20.32 90)
				(length 2.54)
				(name "C3-")
				(number "20")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "V0")
				(number "21")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "V1")
				(number "22")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "V2")
				(number "23")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "V3")
				(number "24")
			)
			(pin passive line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "V4")
				(number "25")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "VOUT")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EA_DOGS104B-A"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.842 11.684 0)
		)
		(property "Value" "EA_DOGS104B-A"
			(at 1.524 11.684 0)
		)
		(property "Footprint" "Display:EA_DOGS104X-A"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/doma/dogs104e.pdf"
			(at 10.16 -7.62 0)
		)
		(property "Description" "LCD 4x10 character display blue transmissive background, +3.3V VDD, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*DOGS104*"
			(at 0 0 0)
		)
		(symbol "EA_DOGS104B-A_0_1")
		(symbol "EA_DOGS104B-A_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SID")
				(number "16")
			)
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SOD")
				(number "15")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCLK")
				(number "17")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{RST}")
				(number "20")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SA0")
				(number "19")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "18")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "14")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "IM1")
				(number "12")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOUT")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EA_DOGXL160-7"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.684 16.51 0)
		)
		(property "Value" "EA_DOGXL160-7"
			(at 19.05 16.51 0)
		)
		(property "Footprint" "Display:EA_DOGXL160-7"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/eng/pdf/grafik/dogxl160-7e.pdf"
			(at -59.69 29.21 0)
		)
		(property "Description" "EA DOGXL160-7 Graphical Display 160x104 no back light I2C SPI 2.7-3.3V"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "EA*DOGXL160*7*"
			(at 0 0 0)
		)
		(symbol "EA_DOGXL160-7_0_1")
		(symbol "EA_DOGXL160-7_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "~{RST}")
				(number "29")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "~{CS0}/A2")
				(number "28")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "CD")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "D3/SDA")
				(number "31")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "D0/SCK")
				(number "32")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "D6")
				(number "30")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "BM0")
				(number "26")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VDD2/3")
				(number "23")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "VSS2")
				(number "24")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "25")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "A1+")
				(number "1")
			)
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 2.54)
				(name "C1-")
				(number "14")
			)
			(pin power_in line
				(at 7.62 17.78 270)
				(length 2.54)
				(name "A2+")
				(number "2")
			)
			(pin power_in line
				(at 7.62 -20.32 90)
				(length 2.54)
				(name "C2-")
				(number "15")
			)
			(pin power_in line
				(at 10.16 17.78 270)
				(length 2.54)
				(name "A3+")
				(number "3")
			)
			(pin power_in line
				(at 10.16 -20.32 90)
				(length 2.54)
				(name "C3-")
				(number "16")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VB0+")
				(number "18")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "VB1+")
				(number "19")
			)
			(pin passive line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "VB1-")
				(number "20")
			)
			(pin passive line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "VB0-")
				(number "21")
			)
			(pin passive line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "VLCD")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EA_eDIP128B-6LW"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.636 24.13 0)
		)
		(property "Value" "EA_eDIP128B-6LW"
			(at 4.064 24.384 0)
		)
		(property "Footprint" "Display:EA-eDIP128B-XXX"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/edip128-6e.pdf"
			(at 12.7 -15.24 0)
		)
		(property "Description" "LCD-graphical display with LED backlight blue negative, 3.3V - 5V VDD, RS-232. I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIP128B*"
			(at 0 0 0)
		)
		(symbol "EA_eDIP128B-6LW_0_1")
		(symbol "EA_eDIP128B-6LW_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "RxD")
				(number "10")
			)
			(pin output line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "TxD")
				(number "11")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "5")
			)
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "BUZZ")
				(number "16")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "EN485")
				(number "12")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "BAUD0")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "BAUD1")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "BAUD2")
				(number "8")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "ADR0")
				(number "9")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "ADR1")
				(number "14")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "ADR2")
				(number "15")
			)
			(pin no_connect line
				(at -10.16 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -10.16 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "21")
			)
			(pin no_connect line
				(at 10.16 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at 10.16 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "IN8/OUT1")
				(number "25")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "IN7/OUT2")
				(number "26")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "IN6/OUT3")
				(number "27")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "IN5/OUT4")
				(number "28")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "IN4/OUT5")
				(number "29")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "IN3/OUT6")
				(number "30")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "IN2/OUT7")
				(number "31")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "IN1/OUT8")
				(number "32")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PWR")
				(number "18")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "DPROT")
				(number "17")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "WUP")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EA_eDIP160B-7LW"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.382 29.464 0)
		)
		(property "Value" "EA_eDIP160B-7LW"
			(at 4.064 29.464 0)
		)
		(property "Footprint" "Display:EA_eDIP160-XXX"
			(at 0 -36.83 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/edip160-7e.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "LCD-graphical display 160x104 with LED backlight, blue negative, 3.3V - 5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIP160*"
			(at 0 0 0)
		)
		(symbol "EA_eDIP160B-7LW_0_1")
		(symbol "EA_eDIP160B-7LW_1_1"
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "RxD")
				(number "10")
			)
			(pin output line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "TxD")
				(number "11")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "~{RESET}")
				(number "5")
			)
			(pin output line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "BUZZ")
				(number "16")
			)
			(pin output line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "EN485")
				(number "12")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "BAUD0")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "BAUD1")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "BAUD2")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "ADR0")
				(number "9")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "ADR1")
				(number "14")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "ADR2")
				(number "15")
			)
			(pin open_collector line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "TEST_SBUF")
				(number "20")
			)
			(pin no_connect line
				(at -10.16 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -10.16 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at -10.16 -25.4 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at -10.16 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "21")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "33")
			)
			(pin no_connect line
				(at 10.16 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin no_connect line
				(at 10.16 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "35")
			)
			(pin no_connect line
				(at 10.16 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "36")
			)
			(pin no_connect line
				(at 10.16 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "37")
			)
			(pin no_connect line
				(at 10.16 -22.86 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "38")
			)
			(pin no_connect line
				(at 10.16 -25.4 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "39")
			)
			(pin no_connect line
				(at 10.16 -27.94 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "40")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "IN8/OUT1")
				(number "25")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "IN7/OUT2")
				(number "26")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "IN6/OUT3")
				(number "27")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "IN5/OUT4")
				(number "28")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "IN4/OUT5")
				(number "29")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "IN3/OUT6")
				(number "30")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "IN2/OUT7")
				(number "31")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "IN1/OUT8")
				(number "32")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PWR")
				(number "18")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "DPROT")
				(number "17")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "WUP")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EA_eDIP240B-7LW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.382 29.21 0)
		)
		(property "Value" "EA_eDIP240B-7LW"
			(at 3.556 29.464 0)
		)
		(property "Footprint" "Display:EA_eDIP240-XXX"
			(at 0 -36.068 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/edip240-7e.pdf"
			(at -8.382 29.21 0)
		)
		(property "Description" "LCD graphical display with white LED background blue negative, 240x128, +5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIP240*"
			(at 0 0 0)
		)
		(symbol "EA_eDIP240B-7LW_0_1")
		(symbol "EA_eDIP240B-7LW_1_1"
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "RxD")
				(number "10")
			)
			(pin output line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "TxD")
				(number "11")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "~{RESET}")
				(number "5")
			)
			(pin output line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "BUZZ")
				(number "16")
			)
			(pin output line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "EN485")
				(number "12")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "BAUD0")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "BAUD1")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "BAUD2")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "ADR0")
				(number "9")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "ADR1")
				(number "14")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "ADR2")
				(number "15")
			)
			(pin open_collector line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "TEST_SBUF")
				(number "20")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "VADJ")
				(number "3")
			)
			(pin output line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 -25.4 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin no_connect line
				(at -10.16 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin no_connect line
				(at 10.16 25.4 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at 10.16 22.86 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin no_connect line
				(at 10.16 20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "25")
			)
			(pin no_connect line
				(at 10.16 17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "26")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "27")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "29")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "30")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "31")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "32")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "33")
			)
			(pin no_connect line
				(at 10.16 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin no_connect line
				(at 10.16 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "35")
			)
			(pin no_connect line
				(at 10.16 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "36")
			)
			(pin no_connect line
				(at 10.16 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "37")
			)
			(pin no_connect line
				(at 10.16 -22.86 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "38")
			)
			(pin no_connect line
				(at 10.16 -25.4 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "39")
			)
			(pin no_connect line
				(at 10.16 -27.94 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "40")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "DPOM")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "EEP_SDA")
				(number "17")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "EEP_SCL")
				(number "18")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "EEP_WP")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EA_eDIP320B-8LW"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.636 29.464 0)
		)
		(property "Value" "EA_eDIP320B-8LW"
			(at 4.318 29.718 0)
		)
		(property "Footprint" "Display:EA_eDIP320X-XXX"
			(at 0 -47.498 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/edip320-8e.pdf"
			(at -8.636 29.464 0)
		)
		(property "Description" "LCD graphical display 320x240 white LED backlight blue negative, +5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIP320*"
			(at 0 0 0)
		)
		(symbol "EA_eDIP320B-8LW_0_1")
		(symbol "EA_eDIP320B-8LW_1_1"
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "RxD")
				(number "10")
			)
			(pin output line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "TxD")
				(number "11")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "~{RESET}")
				(number "5")
			)
			(pin output line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "BUZZ")
				(number "16")
			)
			(pin output line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "EN485")
				(number "12")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "BAUD0")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "BAUD1")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "BAUD2")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "ADR0")
				(number "9")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "ADR1")
				(number "14")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "ADR2")
				(number "15")
			)
			(pin open_collector line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "TEST_SBUF")
				(number "20")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "VADJ")
				(number "3")
			)
			(pin output line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
			(pin input line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "PDI")
				(number "21")
			)
			(pin output line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "PDO")
				(number "22")
			)
			(pin no_connect line
				(at -10.16 -30.48 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at -10.16 -33.02 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin no_connect line
				(at -10.16 -35.56 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "25")
			)
			(pin no_connect line
				(at -10.16 -38.1 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "26")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin no_connect line
				(at 10.16 25.4 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "27")
			)
			(pin no_connect line
				(at 10.16 22.86 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin no_connect line
				(at 10.16 20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "29")
			)
			(pin no_connect line
				(at 10.16 17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "30")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "31")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "32")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "33")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "35")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "36")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "37")
			)
			(pin no_connect line
				(at 10.16 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "38")
			)
			(pin no_connect line
				(at 10.16 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "39")
			)
			(pin no_connect line
				(at 10.16 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "40")
			)
			(pin no_connect line
				(at 10.16 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "41")
			)
			(pin no_connect line
				(at 10.16 -22.86 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "42")
			)
			(pin no_connect line
				(at 10.16 -25.4 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "43")
			)
			(pin no_connect line
				(at 10.16 -27.94 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "44")
			)
			(pin no_connect line
				(at 10.16 -30.48 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "45")
			)
			(pin no_connect line
				(at 10.16 -33.02 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "46")
			)
			(pin no_connect line
				(at 10.16 -35.56 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "47")
			)
			(pin no_connect line
				(at 10.16 -38.1 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "78")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "WUP")
				(number "13")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "DPROT")
				(number "17")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "DPWR")
				(number "18")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "WP")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EA_eDIPTFT32-A"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 31.75 0)
		)
		(property "Value" "EA_eDIPTFT32-A"
			(at 1.524 31.75 0)
		)
		(property "Footprint" "Display:EA_eDIPTFT32-XXX"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/ediptft43-ae.pdf"
			(at 7.62 -5.08 0)
		)
		(property "Description" "TFT graphical display, 320x240, 16 bit colour, LED backlight, 3.3V - 5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display TFT LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIPTFT32*"
			(at 0 0 0)
		)
		(symbol "EA_eDIPTFT32-A_0_1")
		(symbol "EA_eDIPTFT32-A_1_1"
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "SDA")
				(number "14")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "SCL")
				(number "15")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "~{RESET}")
				(number "5")
			)
			(pin output line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BUZZ")
				(number "16")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "AIN1")
				(number "23")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "AIN2")
				(number "24")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "I2CMO")
				(number "12")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "BA0")
				(number "6")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "BA1")
				(number "7")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "BA2")
				(number "11")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "SA0")
				(number "8")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "SA1")
				(number "9")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "SA2")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "TEST_SBUF")
				(number "20")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "WP")
				(number "19")
			)
			(pin no_connect line
				(at -12.7 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "21")
			)
			(pin no_connect line
				(at 10.16 -27.94 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin input line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "IN1/MI8")
				(number "33")
			)
			(pin input line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "IN2/MI7")
				(number "34")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "IN3/MI6")
				(number "35")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "IN4/MI5")
				(number "36")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "IN5/MI4")
				(number "37")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "IN6/MI3")
				(number "38")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "IN7/MI2")
				(number "39")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "IN8/MI1")
				(number "40")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT1/MO8")
				(number "25")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT2/MO7")
				(number "26")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT3/MO6")
				(number "27")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUT4/MO5")
				(number "28")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT5/MO4")
				(number "29")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "OUT6/MO3")
				(number "30")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "OUT7/MO2")
				(number "31")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "OUT8/MO1")
				(number "32")
			)
			(pin output line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "DNC")
				(number "18")
			)
			(pin input line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "DPROT")
				(number "17")
			)
			(pin input line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "DPOM")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EA_eDIPTFT43-A"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.176 31.75 0)
		)
		(property "Value" "EA_eDIPTFT43-A"
			(at 1.778 31.75 0)
		)
		(property "Footprint" "Display:EA_eDIPTFT43-XXX"
			(at -0.254 -36.322 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/ediptft43-ae.pdf"
			(at 0 0 0)
		)
		(property "Description" "TFT graphical display, 480x272, 16 bit colour, LED backlight, 5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display TFT LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "EA*eDIPTFT43*XXX*"
			(at 0 0 0)
		)
		(symbol "EA_eDIPTFT43-A_0_1")
		(symbol "EA_eDIPTFT43-A_1_1"
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "RxD")
				(number "10")
			)
			(pin output line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "TxD")
				(number "11")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "~{RESET}")
				(number "5")
			)
			(pin output line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BUZZ")
				(number "16")
			)
			(pin output line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "EN485")
				(number "12")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "AIN1")
				(number "23")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "AIN2")
				(number "24")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "BAUD0")
				(number "6")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "BAUD1")
				(number "7")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "BAUD2")
				(number "8")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "ADR0")
				(number "9")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "ADR1")
				(number "14")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "ADR2")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "TEST_SBUF")
				(number "20")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "WP")
				(number "19")
			)
			(pin no_connect line
				(at -12.7 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "21")
			)
			(pin no_connect line
				(at 10.16 -27.94 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin input line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "IN1/MI8")
				(number "33")
			)
			(pin input line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "IN2/MI7")
				(number "34")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "IN3/MI6")
				(number "35")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "IN4/MI5")
				(number "36")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "IN5/MI4")
				(number "37")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "IN6/MI3")
				(number "38")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "IN7/MI2")
				(number "39")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "IN8/MI1")
				(number "40")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT1/MO8")
				(number "25")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT2/MO7")
				(number "26")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT3/MO6")
				(number "27")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUT4/MO5")
				(number "28")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT5/MO4")
				(number "29")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "OUT6/MO3")
				(number "30")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "OUT7/MO2")
				(number "31")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "OUT8/MO1")
				(number "32")
			)
			(pin output line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "DNC")
				(number "18")
			)
			(pin input line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "DPROT")
				(number "17")
			)
			(pin input line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "DPOM")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EA_eDIPTFT43-ATC"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.176 31.75 0)
		)
		(property "Value" "EA_eDIPTFT43-ATC"
			(at 1.778 31.75 0)
		)
		(property "Footprint" "Display:EA_eDIPTFT43-ATC"
			(at -0.254 -36.322 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/ediptft43-ae.pdf"
			(at 0 0 0)
		)
		(property "Description" "TFT graphical display, 480x272, 16 bit colour, LED backlight, 5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display TFT LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "EA*eDIPTFT43*ATC*"
			(at 0 0 0)
		)
		(symbol "EA_eDIPTFT43-ATC_0_1")
		(symbol "EA_eDIPTFT43-ATC_1_1"
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "RxD")
				(number "10")
			)
			(pin output line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "TxD")
				(number "11")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "~{RESET}")
				(number "5")
			)
			(pin output line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BUZZ")
				(number "16")
			)
			(pin output line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "EN485")
				(number "12")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "AIN1")
				(number "23")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "AIN2")
				(number "24")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "BAUD0")
				(number "6")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "BAUD1")
				(number "7")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "BAUD2")
				(number "8")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "ADR0")
				(number "9")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "ADR1")
				(number "14")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "ADR2")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "TEST_SBUF")
				(number "20")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "WP")
				(number "19")
			)
			(pin no_connect line
				(at -12.7 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "21")
			)
			(pin no_connect line
				(at 10.16 -27.94 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin input line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "IN1/MI8")
				(number "33")
			)
			(pin input line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "IN2/MI7")
				(number "34")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "IN3/MI6")
				(number "35")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "IN4/MI5")
				(number "36")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "IN5/MI4")
				(number "37")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "IN6/MI3")
				(number "38")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "IN7/MI2")
				(number "39")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "IN8/MI1")
				(number "40")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT1/MO8")
				(number "25")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT2/MO7")
				(number "26")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT3/MO6")
				(number "27")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUT4/MO5")
				(number "28")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT5/MO4")
				(number "29")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "OUT6/MO3")
				(number "30")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "OUT7/MO2")
				(number "31")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "OUT8/MO1")
				(number "32")
			)
			(pin output line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "DNC")
				(number "18")
			)
			(pin input line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "DPROT")
				(number "17")
			)
			(pin input line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "DPOM")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EA_eDIPTFT57-A"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.636 36.83 0)
		)
		(property "Value" "EA_eDIPTFT57-A"
			(at 3.81 36.83 0)
		)
		(property "Footprint" "Display:EA_eDIPTFT57-XXX"
			(at 1.27 -44.45 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/ediptft57-ae.pdf"
			(at 12.7 -10.16 0)
		)
		(property "Description" "TFT-graphical display. 640x480, LED backlight, +5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display TFT LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIPTFT57*"
			(at 0 0 0)
		)
		(symbol "EA_eDIPTFT57-A_0_1")
		(symbol "EA_eDIPTFT57-A_1_1"
			(pin input line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "RxD")
				(number "10")
			)
			(pin output line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "TxD")
				(number "11")
			)
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "~{RESET}")
				(number "5")
			)
			(pin output line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "BUZZ")
				(number "16")
			)
			(pin output line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "EN485")
				(number "12")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "AIN1")
				(number "31")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "AIN2")
				(number "32")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "BAUD0")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "BAUD1")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "BAUD2")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ADR0")
				(number "9")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "ADR1")
				(number "14")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "ADR2")
				(number "15")
			)
			(pin output line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SND+")
				(number "3")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "SND-")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "TEST_SBUF")
				(number "20")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "WP")
				(number "19")
			)
			(pin no_connect line
				(at -10.16 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin no_connect line
				(at -10.16 -30.48 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin no_connect line
				(at -10.16 -33.02 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at -10.16 -35.56 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin no_connect line
				(at 12.7 -27.94 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin no_connect line
				(at 12.7 -30.48 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "27")
			)
			(pin no_connect line
				(at 12.7 -33.02 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "26")
			)
			(pin no_connect line
				(at 12.7 -35.56 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "25")
			)
			(pin input line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "IN1/MI8")
				(number "41")
			)
			(pin input line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "IN2/MI7")
				(number "42")
			)
			(pin input line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "IN3/MI6")
				(number "43")
			)
			(pin input line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "IN4/MI5")
				(number "44")
			)
			(pin input line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "IN5/MI4")
				(number "45")
			)
			(pin input line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "IN6/MI3")
				(number "46")
			)
			(pin input line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "IN7/MI2")
				(number "47")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "IN8/MI1")
				(number "48")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "OUT1/MO8")
				(number "33")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUT2/MO7")
				(number "34")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUT3/MO6")
				(number "35")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUT4/MO5")
				(number "36")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUT5/MO4")
				(number "37")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OUT6/MO3")
				(number "38")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "OUT7/MO2")
				(number "39")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "OUT8/MO1")
				(number "40")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "DNC")
				(number "18")
			)
			(pin input line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "DPROT")
				(number "17")
			)
			(pin input line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "DPOM")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EA_eDIPTFT70-A"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.636 36.83 0)
		)
		(property "Value" "EA_eDIPTFT70-A"
			(at 11.43 36.83 0)
		)
		(property "Footprint" "Display:EA_eDIPTFT70-XXX"
			(at 0.762 -43.688 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/ediptft70-ae.pdf"
			(at -52.07 13.97 0)
		)
		(property "Description" "TFT-graphical display with LED background, 800x480, 16-bit colours, +5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display TFT LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIPTFT70*XXX*"
			(at 0 0 0)
		)
		(symbol "EA_eDIPTFT70-A_0_1")
		(symbol "EA_eDIPTFT70-A_1_1"
			(pin input line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "RxD")
				(number "10")
			)
			(pin output line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "TxD")
				(number "11")
			)
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "~{RESET}")
				(number "5")
			)
			(pin output line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "BUZZ")
				(number "16")
			)
			(pin output line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "EN485")
				(number "12")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "AIN1")
				(number "31")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "AIN2")
				(number "32")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "BAUD0")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "BAUD1")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "BAUD2")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ADR0")
				(number "9")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "ADR1")
				(number "14")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "ADR2")
				(number "15")
			)
			(pin output line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SND+")
				(number "3")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "SND-")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "TEST_SBUF")
				(number "20")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "WP")
				(number "19")
			)
			(pin no_connect line
				(at -10.16 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin no_connect line
				(at -10.16 -30.48 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin no_connect line
				(at -10.16 -33.02 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at -10.16 -35.56 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin no_connect line
				(at 12.7 -27.94 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin no_connect line
				(at 12.7 -30.48 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "27")
			)
			(pin no_connect line
				(at 12.7 -33.02 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "26")
			)
			(pin no_connect line
				(at 12.7 -35.56 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "25")
			)
			(pin input line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "IN1/MI8")
				(number "41")
			)
			(pin input line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "IN2/MI7")
				(number "42")
			)
			(pin input line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "IN3/MI6")
				(number "43")
			)
			(pin input line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "IN4/MI5")
				(number "44")
			)
			(pin input line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "IN5/MI4")
				(number "45")
			)
			(pin input line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "IN6/MI3")
				(number "46")
			)
			(pin input line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "IN7/MI2")
				(number "47")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "IN8/MI1")
				(number "48")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "OUT1/MO8")
				(number "33")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUT2/MO7")
				(number "34")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUT3/MO6")
				(number "35")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUT4/MO5")
				(number "36")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUT5/MO4")
				(number "37")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OUT6/MO3")
				(number "38")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "OUT7/MO2")
				(number "39")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "OUT8/MO1")
				(number "40")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "DNC")
				(number "18")
			)
			(pin input line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "DPROT")
				(number "17")
			)
			(pin input line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "DPOM")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EA_eDIPTFT70-ATC"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.636 36.83 0)
		)
		(property "Value" "EA_eDIPTFT70-ATC"
			(at 11.43 36.83 0)
		)
		(property "Footprint" "Display:EA_eDIPTFT70-ATC"
			(at 0.762 -43.688 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/ediptft70-ae.pdf"
			(at -52.07 13.97 0)
		)
		(property "Description" "TFT-graphical display with LED background and capacitive touch panel, 800x480, 16-bit colours, +5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display TFT LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIPTFT70*ATC*"
			(at 0 0 0)
		)
		(symbol "EA_eDIPTFT70-ATC_0_1")
		(symbol "EA_eDIPTFT70-ATC_1_1"
			(pin input line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "RxD")
				(number "10")
			)
			(pin output line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "TxD")
				(number "11")
			)
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "~{RESET}")
				(number "5")
			)
			(pin output line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "BUZZ")
				(number "16")
			)
			(pin output line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "EN485")
				(number "12")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "AIN1")
				(number "31")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "AIN2")
				(number "32")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "BAUD0")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "BAUD1")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "BAUD2")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ADR0")
				(number "9")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "ADR1")
				(number "14")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "ADR2")
				(number "15")
			)
			(pin output line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SND+")
				(number "3")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "SND-")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "TEST_SBUF")
				(number "20")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "WP")
				(number "19")
			)
			(pin no_connect line
				(at -10.16 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin no_connect line
				(at -10.16 -30.48 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin no_connect line
				(at -10.16 -33.02 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at -10.16 -35.56 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin no_connect line
				(at 12.7 -27.94 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin no_connect line
				(at 12.7 -30.48 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "27")
			)
			(pin no_connect line
				(at 12.7 -33.02 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "26")
			)
			(pin no_connect line
				(at 12.7 -35.56 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "25")
			)
			(pin input line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "IN1/MI8")
				(number "41")
			)
			(pin input line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "IN2/MI7")
				(number "42")
			)
			(pin input line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "IN3/MI6")
				(number "43")
			)
			(pin input line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "IN4/MI5")
				(number "44")
			)
			(pin input line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "IN5/MI4")
				(number "45")
			)
			(pin input line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "IN6/MI3")
				(number "46")
			)
			(pin input line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "IN7/MI2")
				(number "47")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "IN8/MI1")
				(number "48")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "OUT1/MO8")
				(number "33")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUT2/MO7")
				(number "34")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUT3/MO6")
				(number "35")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUT4/MO5")
				(number "36")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUT5/MO4")
				(number "37")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OUT6/MO3")
				(number "38")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "OUT7/MO2")
				(number "39")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "OUT8/MO1")
				(number "40")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "DNC")
				(number "18")
			)
			(pin input line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "DPROT")
				(number "17")
			)
			(pin input line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "DPOM")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ERM19264"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "DS"
			(at -8.382 19.05 0)
		)
		(property "Value" "ERM19264"
			(at 5.588 19.05 0)
		)
		(property "Footprint" "Display:ERM19264"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.buydisplay.com/download/manual/ERM19264-1_Series_Datasheet.pdf"
			(at 5.08 -5.08 0)
		)
		(property "Description" "Graphics Display 192x64px,  8b parallel, 1/64 Duty, 3.3V or 5V VDD"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ERM19264*"
			(at 0 0 0)
		)
		(symbol "ERM19264_0_0"
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "~{CS3}")
				(number "18")
			)
		)
		(symbol "ERM19264_0_1")
		(symbol "ERM19264_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "E")
				(number "6")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "RS")
				(number "4")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{RST}")
				(number "16")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "R/~{W}")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "DB0")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "DB1")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DB2")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "DB3")
				(number "10")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "DB4")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "DB5")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "DB6")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "DB7")
				(number "14")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VOUT")
				(number "19")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "BLA")
				(number "20")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{CS1}")
				(number "15")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "~{CS2}")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NHD-C12832A1Z-FSRGB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 15.875 0)
		)
		(property "Value" "NHD-C12832A1Z-FSRGB"
			(at 2.54 -16.51 0)
		)
		(property "Footprint" "Display:NHD-C12832A1Z-FSRGB"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.newhavendisplay.com/specs/NHD-C12832A1Z-FSRGB-FBW-3V.pdf"
			(at 0 0 0)
		)
		(property "Description" "128x32 graphical LCD module with common anode RGB backlight, 1/33 duty, 3.3V"
			(at 0 0 0)
		)
		(property "ki_keywords" "lcd rgb st7565r spi 4-wire"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "NHD?C12832A1Z?FSRGB*"
			(at 0 0 0)
		)
		(symbol "NHD-C12832A1Z-FSRGB_0_1")
		(symbol "NHD-C12832A1Z-FSRGB_1_1"
			(pin passive line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "LED+")
				(number "18")
			)
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "(R)LED-")
				(number "19")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "(G)LED-")
				(number "20")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "(B)LED-")
				(number "21")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDA(SI)")
				(number "13")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCL")
				(number "14")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{CS1B}")
				(number "17")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A0")
				(number "15")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "~{RST}")
				(number "16")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "V_{dd}")
				(number "12")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "V_{ss}")
				(number "11")
			)
			(pin passive line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "C1+")
				(number "8")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "C1-")
				(number "9")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "C2+")
				(number "7")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "C2-")
				(number "6")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "V0")
				(number "1")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "V1")
				(number "2")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "V2")
				(number "3")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "V3")
				(number "4")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "V4")
				(number "5")
			)
			(pin passive line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "V_{out}")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OLED-128O064D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "DS"
			(at -10.16 38.1 0)
		)
		(property "Value" "OLED-128O064D"
			(at 12.7 38.1 0)
		)
		(property "Footprint" "Display:OLED-128O064D"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/37902/oled128o064dbpp3n00000.pdf"
			(at 0 20.32 0)
		)
		(property "Description" "OLED display 128x64"
			(at 0 0 0)
		)
		(property "ki_keywords" "display oled"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "OLED?128O064D*"
			(at 0 0 0)
		)
		(symbol "OLED-128O064D_0_1")
		(symbol "OLED-128O064D_1_1"
			(pin passive line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "C2N")
				(number "2")
			)
			(pin passive line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "C2P")
				(number "3")
			)
			(pin passive line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "C1P")
				(number "4")
			)
			(pin passive line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "C1N")
				(number "5")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "BS0")
				(number "10")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "BS1")
				(number "11")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "BS2")
				(number "12")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{CS}")
				(number "13")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{RES}")
				(number "14")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D/~{C}")
				(number "15")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "R/~{W}")
				(number "16")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "E/~{RD}")
				(number "17")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "D0")
				(number "18")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "D1")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "D2")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "D3")
				(number "21")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "D4")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "D5")
				(number "23")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "D6")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "D7")
				(number "25")
			)
			(pin passive line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "IREF")
				(number "26")
			)
			(pin passive line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "VCOMH")
				(number "27")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at -2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "9")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VLSS")
				(number "29")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EA_eDIP128B-6LWTP"
		(extends "EA_eDIP128B-6LW")
		(property "Reference" "U"
			(at -8.636 24.13 0)
		)
		(property "Value" "EA_eDIP128B-6LWTP"
			(at 4.064 24.384 0)
		)
		(property "Footprint" "Display:EA-eDIP128B-XXX"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/edip128-6e.pdf"
			(at 12.7 -15.24 0)
		)
		(property "Description" "LCD-graphical display with LED backlight and touch panel blue negative, 3.3V - 5V VDD, RS-232. I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIP128B*"
			(at 0 0 0)
		)
	)
	(symbol "EA_eDIP128W-6LW"
		(extends "EA_eDIP128B-6LW")
		(property "Reference" "U"
			(at -8.636 24.13 0)
		)
		(property "Value" "EA_eDIP128W-6LW"
			(at 4.064 24.384 0)
		)
		(property "Footprint" "Display:EA-eDIP128B-XXX"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/edip128-6e.pdf"
			(at 12.7 -15.24 0)
		)
		(property "Description" "LCD-graphical display with LED backlight positive mode FSTN, 3.3V - 5V VDD, RS-232. I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIP128B*"
			(at 0 0 0)
		)
	)
	(symbol "EA_eDIP128W-6LWTP"
		(extends "EA_eDIP128B-6LW")
		(property "Reference" "U"
			(at -8.636 24.13 0)
		)
		(property "Value" "EA_eDIP128W-6LWTP"
			(at 4.064 24.384 0)
		)
		(property "Footprint" "Display:EA-eDIP128B-XXX"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/edip128-6e.pdf"
			(at 12.7 -15.24 0)
		)
		(property "Description" "LCD-graphical display with LED backlight and touch panel positive mode FSTN, 3.3V - 5V VDD, RS-232. I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIP128B*"
			(at 0 0 0)
		)
	)
	(symbol "EA_eDIP160B-7LWTP"
		(extends "EA_eDIP160B-7LW")
		(property "Reference" "U"
			(at -8.382 29.464 0)
		)
		(property "Value" "EA_eDIP160B-7LWTP"
			(at 4.064 29.464 0)
		)
		(property "Footprint" "Display:EA_eDIP160-XXX"
			(at 0 -36.83 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/edip160-7e.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "LCD-graphical display 160x104 with LED backlight and touch panel, blue negative, 3.3V - 5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIP160*"
			(at 0 0 0)
		)
	)
	(symbol "EA_eDIP160W-7LW"
		(extends "EA_eDIP160B-7LW")
		(property "Reference" "U"
			(at -8.382 29.464 0)
		)
		(property "Value" "EA_eDIP160W-7LW"
			(at 4.064 29.464 0)
		)
		(property "Footprint" "Display:EA_eDIP160-XXX"
			(at 0 -36.83 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/edip160-7e.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "LCD-graphical display 160x104 with LED backlight, positive mode FSTN, 3.3V - 5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIP160*"
			(at 0 0 0)
		)
	)
	(symbol "EA_eDIP160W-7LWTP"
		(extends "EA_eDIP160B-7LW")
		(property "Reference" "U"
			(at -8.382 29.464 0)
		)
		(property "Value" "EA_eDIP160W-7LWTP"
			(at 4.064 29.464 0)
		)
		(property "Footprint" "Display:EA_eDIP160-XXX"
			(at 0 -36.83 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/edip160-7e.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "LCD-graphical display 160x104 with LED backlight and touch panel, positive mode FSTN, 3.3V - 5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIP160*"
			(at 0 0 0)
		)
	)
	(symbol "EA_eDIP240B-7LWTP"
		(extends "EA_eDIP240B-7LW")
		(property "Reference" "U"
			(at -8.382 29.21 0)
		)
		(property "Value" "EA_eDIP240B-7LWTP"
			(at 3.556 29.464 0)
		)
		(property "Footprint" "Display:EA_eDIP240-XXX"
			(at 0 -36.068 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/edip240-7e.pdf"
			(at -8.382 29.21 0)
		)
		(property "Description" "LCD graphical display with white LED background and touch panel blue negative, 240x128, +5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIP240*"
			(at 0 0 0)
		)
	)
	(symbol "EA_eDIP240J-7LA"
		(extends "EA_eDIP240B-7LW")
		(property "Reference" "U"
			(at -8.382 29.21 0)
		)
		(property "Value" "EA_eDIP240J-7LA"
			(at 3.556 29.464 0)
		)
		(property "Footprint" "Display:EA_eDIP240-XXX"
			(at 0 -36.068 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/edip240-7e.pdf"
			(at -8.382 29.21 0)
		)
		(property "Description" "LCD graphical display with amber LED background blue positive mode FSTN 240x128, +5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIP240*"
			(at 0 0 0)
		)
	)
	(symbol "EA_eDIP240J-7LATP"
		(extends "EA_eDIP240B-7LW")
		(property "Reference" "U"
			(at -8.382 29.21 0)
		)
		(property "Value" "EA_eDIP240J-7LATP"
			(at 3.556 29.464 0)
		)
		(property "Footprint" "Display:EA_eDIP240-XXX"
			(at 0 -36.068 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/edip240-7e.pdf"
			(at -8.382 29.21 0)
		)
		(property "Description" "LCD graphical display with amber LED background and touch panel blue positive mode FSTN, 240x128, +5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIP240*"
			(at 0 0 0)
		)
	)
	(symbol "EA_eDIP240J-7LW"
		(extends "EA_eDIP240B-7LW")
		(property "Reference" "U"
			(at -8.382 29.21 0)
		)
		(property "Value" "EA_eDIP240J-7LW"
			(at 3.556 29.464 0)
		)
		(property "Footprint" "Display:EA_eDIP240-XXX"
			(at 0 -36.068 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/edip240-7e.pdf"
			(at -8.382 29.21 0)
		)
		(property "Description" "LCD graphical display with white LED background blue positive mode FSTN, 240x128, +5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIP240*"
			(at 0 0 0)
		)
	)
	(symbol "EA_eDIP240J-7LWTP"
		(extends "EA_eDIP240B-7LW")
		(property "Reference" "U"
			(at -8.382 29.21 0)
		)
		(property "Value" "EA_eDIP240J-7LWTP"
			(at 3.556 29.464 0)
		)
		(property "Footprint" "Display:EA_eDIP240-XXX"
			(at 0 -36.068 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/edip240-7e.pdf"
			(at -8.382 29.21 0)
		)
		(property "Description" "LCD graphical display with amber LED background blue positive mode FSTN, 240x128, +5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIP240*"
			(at 0 0 0)
		)
	)
	(symbol "EA_eDIP320B-8LWTP"
		(extends "EA_eDIP320B-8LW")
		(property "Reference" "U"
			(at -8.636 29.464 0)
		)
		(property "Value" "EA_eDIP320B-8LWTP"
			(at 4.318 29.718 0)
		)
		(property "Footprint" "Display:EA_eDIP320X-XXX"
			(at 0 -47.498 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/edip320-8e.pdf"
			(at -8.636 29.464 0)
		)
		(property "Description" "LCD graphical display 320x240 white LED backlight with touch panel blue negative, +5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIP320*"
			(at 0 0 0)
		)
	)
	(symbol "EA_eDIP320J-8LA"
		(extends "EA_eDIP320B-8LW")
		(property "Reference" "U"
			(at -8.636 29.464 0)
		)
		(property "Value" "EA_eDIP320J-8LA"
			(at 4.318 29.718 0)
		)
		(property "Footprint" "Display:EA_eDIP320X-XXX"
			(at 0 -47.498 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/edip320-8e.pdf"
			(at -8.636 29.464 0)
		)
		(property "Description" "LCD graphical display 320x240 amber LED backlight blue positive FSTN, +5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIP320*"
			(at 0 0 0)
		)
	)
	(symbol "EA_eDIP320J-8LATP"
		(extends "EA_eDIP320B-8LW")
		(property "Reference" "U"
			(at -8.636 29.464 0)
		)
		(property "Value" "EA_eDIP320J-8LATP"
			(at 4.318 29.718 0)
		)
		(property "Footprint" "Display:EA_eDIP320X-XXX"
			(at 0 -47.498 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/edip320-8e.pdf"
			(at -8.636 29.464 0)
		)
		(property "Description" "LCD graphical display 320x240 amber LED backlight with touch panel blue positive mode FSTN, +5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIP320*"
			(at 0 0 0)
		)
	)
	(symbol "EA_eDIP320J-8LW"
		(extends "EA_eDIP320B-8LW")
		(property "Reference" "U"
			(at -8.636 29.464 0)
		)
		(property "Value" "EA_eDIP320J-8LW"
			(at 4.318 29.718 0)
		)
		(property "Footprint" "Display:EA_eDIP320X-XXX"
			(at 0 -47.498 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/edip320-8e.pdf"
			(at -8.636 29.464 0)
		)
		(property "Description" "LCD graphical display 320x240 white LED backlight blue positive mode FSTN, +5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIP320*"
			(at 0 0 0)
		)
	)
	(symbol "EA_eDIP320J-8LWTP"
		(extends "EA_eDIP320B-8LW")
		(property "Reference" "U"
			(at -8.636 29.464 0)
		)
		(property "Value" "EA_eDIP320J-8LWTP"
			(at 4.318 29.718 0)
		)
		(property "Footprint" "Display:EA_eDIP320X-XXX"
			(at 0 -47.498 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/edip320-8e.pdf"
			(at -8.636 29.464 0)
		)
		(property "Description" "LCD graphical display 320x240 white LED backlight with touch panel blue positive mode FSTN, +5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIP320*"
			(at 0 0 0)
		)
	)
	(symbol "EA_eDIPTFT32-ATP"
		(extends "EA_eDIPTFT32-A")
		(property "Reference" "U"
			(at -11.43 31.75 0)
		)
		(property "Value" "EA_eDIPTFT32-ATP"
			(at 1.524 31.75 0)
		)
		(property "Footprint" "Display:EA_eDIPTFT32-XXX"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/ediptft43-ae.pdf"
			(at 7.62 -5.08 0)
		)
		(property "Description" "TFT graphical display with touch panel, 320x240, 16 bit colour, LED backlight, 3.3V - 5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display TFT LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIPTFT32*"
			(at 0 0 0)
		)
	)
	(symbol "EA_eDIPTFT43-ATP"
		(extends "EA_eDIPTFT43-A")
		(property "Reference" "U"
			(at -11.176 31.75 0)
		)
		(property "Value" "EA_eDIPTFT43-ATP"
			(at 1.778 31.75 0)
		)
		(property "Footprint" "Display:EA_eDIPTFT43-XXX"
			(at -0.254 -36.322 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/ediptft43-ae.pdf"
			(at 0 0 0)
		)
		(property "Description" "TFT graphical display with resistive touch panel, 480x272, 16 bit colour, LED backlight, 5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display TFT LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "EA*eDIPTFT43*XXX*"
			(at 0 0 0)
		)
	)
	(symbol "EA_eDIPTFT43-ATS"
		(extends "EA_eDIPTFT43-A")
		(property "Reference" "U"
			(at -11.176 31.75 0)
		)
		(property "Value" "EA_eDIPTFT43-ATS"
			(at 1.778 31.75 0)
		)
		(property "Footprint" "Display:EA_eDIPTFT43-XXX"
			(at -0.254 -36.322 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/ediptft43-ae.pdf"
			(at 0 0 0)
		)
		(property "Description" "TFT graphical display with capacitive touch panel, 480x272, 16 bit colour, LED backlight, 5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display TFT LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "EA*eDIPTFT43*XXX*"
			(at 0 0 0)
		)
	)
	(symbol "EA_eDIPTFT57-ATP"
		(extends "EA_eDIPTFT57-A")
		(property "Reference" "U"
			(at -8.636 36.83 0)
		)
		(property "Value" "EA_eDIPTFT57-ATP"
			(at 3.81 36.83 0)
		)
		(property "Footprint" "Display:EA_eDIPTFT57-XXX"
			(at 1.27 -44.45 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/ediptft57-ae.pdf"
			(at 12.7 -10.16 0)
		)
		(property "Description" "TFT-graphical display with touch panel. 640x480, LED backlight, +5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display TFT LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIPTFT57*"
			(at 0 0 0)
		)
	)
	(symbol "EA_eDIPTFT70-ATP"
		(extends "EA_eDIPTFT70-A")
		(property "Reference" "U"
			(at -8.636 36.83 0)
		)
		(property "Value" "EA_eDIPTFT70-ATP"
			(at 11.43 36.83 0)
		)
		(property "Footprint" "Display:EA_eDIPTFT70-XXX"
			(at 0.762 -43.688 0)
		)
		(property "Datasheet" "http://www.lcd-module.com/fileadmin/eng/pdf/grafik/ediptft70-ae.pdf"
			(at -52.07 13.97 0)
		)
		(property "Description" "TFT-graphical display with LED background, 800x480, 16-bit colours, +5V VDD, RS-232, I2C or SPI"
			(at 0 0 0)
		)
		(property "ki_keywords" "display TFT LCD graphic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EA*eDIPTFT70*XXX*"
			(at 0 0 0)
		)
	)
)
