(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "82720"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 33.02 0)
		)
		(property "Value" "82720"
			(at 12.7 33.02 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 -2.54 0)
		)
		(property "Description" "Graphics Display Controller, PDIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Graphics Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "82720_0_0")
		(symbol "82720_1_1"
			(pin input line
				(at -22.86 27.94 0)
				(length 3.81)
				(name "2xWCLK")
				(number "1")
			)
			(pin input line
				(at -22.86 25.4 0)
				(length 3.81)
				(name "~{DBIN}")
				(number "2")
			)
			(pin output line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "HSYNC")
				(number "3")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "VSYNC")
				(number "4")
			)
			(pin output line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "BLANK")
				(number "5")
			)
			(pin output line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "DREQ")
				(number "7")
			)
			(pin input line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "~{DACK}")
				(number "8")
			)
			(pin input line
				(at -22.86 0 0)
				(length 3.81)
				(name "~{RD}")
				(number "9")
			)
			(pin input line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "~{WR}")
				(number "10")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "A0")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "DB0")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "DB1")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "DB2")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 3.81)
				(name "DB3")
				(number "15")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "DB4")
				(number "16")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 3.81)
				(name "DB5")
				(number "17")
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 3.81)
				(name "DB6")
				(number "18")
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 3.81)
				(name "DB7")
				(number "19")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "GND")
				(number "20")
			)
			(pin input line
				(at 22.86 27.94 180)
				(length 3.81)
				(name "LPEN")
				(number "21")
			)
			(pin output line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "(ALE)~{RAS}")
				(number "6")
			)
			(pin output line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "A17")
				(number "39")
			)
			(pin output line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "A16")
				(number "38")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "AD15")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "AD14")
				(number "36")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "AD13")
				(number "35")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "AD12")
				(number "34")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "AD14")
				(number "33")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "AD10")
				(number "32")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "AD9")
				(number "31")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "AD8")
				(number "30")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "AD7")
				(number "29")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "AD6")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "AD5")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "AD4")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 3.81)
				(name "AD3")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "AD2")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 3.81)
				(name "AD1")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 3.81)
				(name "AD0")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS7843E"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.176 0)
		)
		(property "Value" "ADS7843E"
			(at 3.556 11.43 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads7843.pdf"
			(at 5.08 -13.97 0)
		)
		(property "Description" "Single-supply, 12bit, 4 ch, touch screen driver, 2.2 - 5.25 VDD, -40 to +85 C, QSPI, SPI, 3-wire serial interface, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single-supply, 12bit, 4 ch, touch screen driver, 2.2 - 5.25 VDD, -40 to +85 C, QSPI, SPI, 3-wire serial interface, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "ADS7843E_0_1")
		(symbol "ADS7843E_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "X+")
				(number "2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "Y+")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "X-")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "Y-")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN3")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "IN4")
				(number "8")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "VREF")
				(number "9")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "+VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "+VCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DIN")
				(number "14")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DOUT")
				(number "12")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DCLK")
				(number "16")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "BUSY")
				(number "13")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{CS}")
				(number "15")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "~{PENIRQ}")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AY0438X-L"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.176 47.244 0)
		)
		(property "Value" "AY0438X-L"
			(at 1.27 47.244 0)
		)
		(property "Footprint" "Package_LCC:PLCC-44"
			(at 0 -53.34 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/43336.pdf"
			(at -40.64 31.75 0)
		)
		(property "Description" "32-Segment CMOS LCD Driver, CMOS and TTL-compatible inputs, VDD +3.0V to +8.5V, PLCC-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "driver display"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC*"
			(at 0 0 0)
		)
		(symbol "AY0438X-L_0_1")
		(symbol "AY0438X-L_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "DATA_IN")
				(number "37")
			)
			(pin input line
				(at -15.24 40.64 0)
				(length 2.54)
				(name "CLOCK")
				(number "44")
			)
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "LOAD")
				(number "2")
			)
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "LCD0")
				(number "34")
			)
			(pin no_connect line
				(at -12.7 -33.02 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "39")
			)
			(pin no_connect line
				(at -12.7 -35.56 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "29")
			)
			(pin no_connect line
				(at -12.7 -38.1 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin no_connect line
				(at -12.7 -40.64 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "VSS")
				(number "40")
			)
			(pin output line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "DATA_OUT")
				(number "38")
			)
			(pin output line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "SEG_1")
				(number "43")
			)
			(pin output line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "SEG_2")
				(number "42")
			)
			(pin output line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "SEG_3")
				(number "41")
			)
			(pin output line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "SEG_4")
				(number "36")
			)
			(pin output line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "SEG_5")
				(number "35")
			)
			(pin output line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "SEG_6")
				(number "32")
			)
			(pin output line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "SEG_7")
				(number "31")
			)
			(pin output line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "SEG_8")
				(number "30")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "SEG_9")
				(number "27")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "SEG_10")
				(number "26")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "SEG_11")
				(number "25")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "SEG_12")
				(number "24")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "SEG_13")
				(number "23")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "SEG_14")
				(number "22")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "SEG_15")
				(number "21")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "SEG_16")
				(number "20")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "SEG_17")
				(number "19")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "SEG_18")
				(number "18")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "SEG_19")
				(number "17")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "SEG_20")
				(number "16")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "SEG_21")
				(number "15")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "SEG_22")
				(number "14")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "SEG_23")
				(number "13")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "SEG_24")
				(number "12")
			)
			(pin output line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "SEG_25")
				(number "11")
			)
			(pin output line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "SEG_26")
				(number "10")
			)
			(pin output line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "SEG_27")
				(number "9")
			)
			(pin output line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "SEG_28")
				(number "8")
			)
			(pin output line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "SEG_29")
				(number "7")
			)
			(pin output line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "SEG_30")
				(number "5")
			)
			(pin output line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "SEG_31")
				(number "4")
			)
			(pin output line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "SEG_32")
				(number "3")
			)
			(pin output line
				(at 15.24 -45.72 180)
				(length 2.54)
				(name "BP")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AY0438X-P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.176 47.244 0)
		)
		(property "Value" "AY0438X-P"
			(at 1.27 47.244 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -53.34 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/43336.pdf"
			(at -40.64 31.75 0)
		)
		(property "Description" "32-Segment CMOS LCD Driver, CMOS and TTL-compatible inputs, VDD +3.0V to +8.5V, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "driver display"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "AY0438X-P_0_1")
		(symbol "AY0438X-P_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "DATA_IN")
				(number "34")
			)
			(pin input line
				(at -15.24 40.64 0)
				(length 2.54)
				(name "CLOCK")
				(number "40")
			)
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "LOAD")
				(number "2")
			)
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "LCD0")
				(number "31")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "VSS")
				(number "36")
			)
			(pin output line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "DATA_OUT")
				(number "35")
			)
			(pin output line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "SEG_1")
				(number "39")
			)
			(pin output line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "SEG_2")
				(number "38")
			)
			(pin output line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "SEG_3")
				(number "37")
			)
			(pin output line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "SEG_4")
				(number "33")
			)
			(pin output line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "SEG_5")
				(number "32")
			)
			(pin output line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "SEG_6")
				(number "29")
			)
			(pin output line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "SEG_7")
				(number "28")
			)
			(pin output line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "SEG_8")
				(number "27")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "SEG_9")
				(number "26")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "SEG_10")
				(number "25")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "SEG_11")
				(number "24")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "SEG_12")
				(number "23")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "SEG_13")
				(number "22")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "SEG_14")
				(number "21")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "SEG_15")
				(number "20")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "SEG_16")
				(number "19")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "SEG_17")
				(number "18")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "SEG_18")
				(number "17")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "SEG_19")
				(number "16")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "SEG_20")
				(number "15")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "SEG_21")
				(number "14")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "SEG_22")
				(number "13")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "SEG_23")
				(number "12")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "SEG_24")
				(number "11")
			)
			(pin output line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "SEG_25")
				(number "10")
			)
			(pin output line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "SEG_26")
				(number "9")
			)
			(pin output line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "SEG_27")
				(number "8")
			)
			(pin output line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "SEG_28")
				(number "7")
			)
			(pin output line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "SEG_29")
				(number "6")
			)
			(pin output line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "SEG_30")
				(number "5")
			)
			(pin output line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "SEG_31")
				(number "4")
			)
			(pin output line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "SEG_32")
				(number "3")
			)
			(pin output line
				(at 15.24 -45.72 180)
				(length 2.54)
				(name "BP")
				(number "30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CR2013-MI2120"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.526 13.97 0)
		)
		(property "Value" "CR2013-MI2120"
			(at 1.905 13.97 0)
		)
		(property "Footprint" "Display:CR2013-MI2120"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://pan.baidu.com/s/11Y990"
			(at -16.51 12.7 0)
		)
		(property "Description" "ILI9341 controller, SPI TFT LCD Display, 9-pin breakout PCB, 4-pin SD card interface, 5V/3.3V"
			(at 0 0 0)
		)
		(property "ki_keywords" "driver display"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*CR2013*MI2120*"
			(at 0 0 0)
		)
		(symbol "CR2013-MI2120_0_0"
			(text "ILI9341"
				(at -5.461 4.572 0)
			)
			(text "SPI Interface"
				(at -5.461 -0.508 0)
			)
			(text "SD Card Slot"
				(at -5.461 -3.048 0)
			)
			(text "320x240 LCD"
				(at 0.889 2.032 0)
			)
		)
		(symbol "CR2013-MI2120_0_1")
		(symbol "CR2013-MI2120_1_1"
			(pin input line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "SD_CS")
				(number "10")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "SD_MOSI")
				(number "11")
			)
			(pin output line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "SD_MISO")
				(number "12")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "SD_SCK")
				(number "13")
			)
			(pin input line
				(at -20.32 0 0)
				(length 2.54)
				(name "FLASH_CD")
				(number "14")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "D/~{C}")
				(number "5")
			)
			(pin input line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "~{CS}")
				(number "3")
			)
			(pin input line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "MOSI")
				(number "6")
			)
			(pin output line
				(at 20.32 0 180)
				(length 2.54)
				(name "MISO")
				(number "9")
			)
			(pin input line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "SCK")
				(number "7")
			)
			(pin input line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "LED")
				(number "8")
			)
			(pin input line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "RESET")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XPT2046QF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "XPT2046QF"
			(at 4.064 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.xptek.cn/uploadfile/download/201707171401161883.pdf"
			(at 5.08 -13.97 0)
		)
		(property "Description" "Single-supply, 12bit, 4 ch, touch screen driver, 2.2 - 5.25 VDD, -40 to +85 C, QSPI, SPI, 3-wire serial interface, QFN-16"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*1EP*4x4mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "XPT2046QF_0_1")
		(symbol "XPT2046QF_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "XP")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "YP")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "XN")
				(number "8")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "YN")
				(number "9")
			)
			(pin power_in line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VBAT")
				(number "11")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "AUX")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "VREF")
				(number "13")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "IOVDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DIN")
				(number "2")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DOUT")
				(number "16")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DCLK")
				(number "4")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "BUSY")
				(number "1")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{CS}")
				(number "3")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "~{PENIRQ}")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XPT2046TS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "XPT2046TS"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.xptek.cn/uploadfile/download/201707171401161883.pdf"
			(at 5.08 -13.97 0)
		)
		(property "Description" "Single-supply, 12bit, 4 ch, touch screen driver, 2.2 - 5.25 VDD, -40 to +85 C, QSPI, SPI, 3-wire serial interface, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single-supply, 12bit, 4 ch, touch screen driver, 2.2 - 5.25 VDD, -40 to +85 C, QSPI, SPI, 3-wire serial interface, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "XPT2046TS_0_1")
		(symbol "XPT2046TS_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "XP")
				(number "2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "YP")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "XN")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "YN")
				(number "5")
			)
			(pin power_in line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VBAT")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "VREF")
				(number "9")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "IOVDD")
				(number "10")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DIN")
				(number "14")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DOUT")
				(number "12")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DCLK")
				(number "16")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "BUSY")
				(number "13")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{CS}")
				(number "15")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "~{PENIRQ}")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADS7843E-2K5"
		(extends "ADS7843E")
		(property "Reference" "U"
			(at -10.16 11.176 0)
		)
		(property "Value" "ADS7843E-2K5"
			(at 3.556 11.43 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads7843.pdf"
			(at 5.08 -13.97 0)
		)
		(property "Description" "Single-supply, 12bit, 4 ch, touch screen driver, 2.2 - 5.25 VDD, -40 to +85 C, QSPI, SPI, 3-wire serial interface, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single-supply, 12bit, 4 ch, touch screen driver, 2.2 - 5.25 VDD, -40 to +85 C, QSPI, SPI, 3-wire serial interface, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADS7843EG4"
		(extends "ADS7843E")
		(property "Reference" "U"
			(at -10.16 11.176 0)
		)
		(property "Value" "ADS7843EG4"
			(at 3.556 11.43 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads7843.pdf"
			(at 5.08 -13.97 0)
		)
		(property "Description" "Single-supply, 12bit, 4 ch, touch screen driver, 2.2 - 5.25 VDD, -40 to +85 C, QSPI, SPI, 3-wire serial interface, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single-supply, 12bit, 4 ch, touch screen driver, 2.2 - 5.25 VDD, -40 to +85 C, QSPI, SPI, 3-wire serial interface, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADS7843IDBQRQ1"
		(extends "ADS7843E")
		(property "Reference" "U"
			(at -10.16 11.176 0)
		)
		(property "Value" "ADS7843IDBQRQ1"
			(at 3.556 11.43 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads7843-q1.pdf"
			(at 5.08 -13.97 0)
		)
		(property "Description" "Single-supply, 12bit, 4 ch, touch screen driver, 2.2 - 5.25 VDD, -40 to +125 C, QSPI, SPI, 3-wire serial interface, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Single-supply, 12bit, 4 ch, touch screen driver, 2.2 - 5.25 VDD, -40 to +125 C, QSPI, SPI, 3-wire serial interface, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
)
