(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "1EDN7550B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "1EDN7550B"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-1EDN7550B-DS-v02_00-EN.pdf?fileId=5546d46262b31d2e01635d9799ef264f"
			(at 0 -7.62 0)
		)
		(property "Description" "Single-Channel EiceDRIVER With True Differential Inputs, 4V UVLO, +4/-8A, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Driver, Dual MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "1EDN7550B_0_1")
		(symbol "1EDN7550B_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN-")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT_SRC")
				(number "5")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT_SNK")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "2ED1324S12P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "2ED1324S12P"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:Infineon_PG-DSO-20-U03_7.5x12.8mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-2ED1323S12P_2ED1324S12P-DataSheet-v01_01-EN.pdf?fileId=8ac78c8c869190210186e92f0f506d0c"
			(at 1.27 -15.24 0)
		)
		(property "Description" "1200V Half Bridge Gate Driver with active Miller clamp, OCP, SCC , 380ns integrated deadtime, Bootstrap Diode, ±2.3A drive current, PG-DSO-20-U03"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver MOSFET IGBT SiC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG?DSO?20?U03*7.5x12.8mm*"
			(at 0 0 0)
		)
		(symbol "2ED1324S12P_0_1")
		(symbol "2ED1324S12P_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "HIN")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "LIN")
				(number "5")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{RFE}")
				(number "6")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "ITRIP")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "12")
			)
			(pin no_connect line
				(at 2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VB")
				(number "14")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "HO")
				(number "15")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "HC")
				(number "16")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VS")
				(number "17")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "LO")
				(number "11")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "LC")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "2ED21824S06J"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "2ED21824S06J"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 24.13 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-2ED2182-4-S06F-J-DataSheet-v02_10-EN.pdf?fileId=5546d4626cb27db2016cb8d7368a29e3"
			(at 0 0 0)
		)
		(property "Description" "650V Half Bridge Gate Driver with Integrated Bootstrap Diode, 2.5A drive current, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver MOSFET IGBT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "2ED21824S06J_0_1")
		(symbol "2ED21824S06J_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "HIN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "LIN")
				(number "2")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DT")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "5")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VB")
				(number "13")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "HO")
				(number "12")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "11")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "2EDL23N06PJXUMA1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "2EDL23N06PJXUMA1"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 24.13 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-2EDL23x06xx-DS-v02_01-EN.pdf?fileId=5546d46146d18cb4014738a20c5236f0"
			(at 0 0 0)
		)
		(property "Description" "600V Half Bridge Gate Driver with OCP and Integrated Bootstrap Diode, +1.8A/-2.5A drive current, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver MOSFET IGBT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "2EDL23N06PJXUMA1_0_1")
		(symbol "2EDL23N06PJXUMA1_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "HIN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "LIN")
				(number "3")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN/FLT")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "PGND")
				(number "6")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VB")
				(number "12")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "HO")
				(number "11")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "10")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACPL-336J"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "ACPL-336J"
			(at -5.08 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 5.08 -15.24 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-4391EN"
			(at 6.35 -5.08 0)
		)
		(property "Description" "2.5A Gate Drive Optocoupler with Integrated LED Driver, Active Miller Clamp, DESAT Detection, and Fault & UVLO Status Feedback, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver IGBT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ACPL-336J_0_1")
		(symbol "ACPL-336J_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "VIN+")
				(number "2")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VLEDDRV")
				(number "4")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "ANODE")
				(number "7")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "CATHODE")
				(number "8")
			)
			(pin open_collector line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{UVLO}")
				(number "5")
			)
			(pin open_collector line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "6")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCC1")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "VEE1")
				(number "1")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VCC2")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "VEE2")
				(number "16")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "VEE2")
				(number "9")
			)
			(pin power_in line
				(at 7.62 15.24 270)
				(length 2.54)
				(name "VE")
				(number "13")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VLED")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DESAT")
				(number "14")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "VOUT")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VCLAMP")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACPL-P343"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 12.7 0)
		)
		(property "Value" "ACPL-P343"
			(at 0 10.16 0)
		)
		(property "Footprint" "Package_SO:SSO-6_6.8x4.6mm_P1.27mm_Clearance7mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-2928EN"
			(at -2.286 0.127 0)
		)
		(property "Description" "Gate Drive Optocoupler, Output Current 4.0/4.0A, Propagation Delay 200ns, SSO-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "MOSFET Driver IGBT Driver Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSO*6.8x4.6mm*P1.27mm*Clearance7mm*"
			(at 0 0 0)
		)
		(symbol "ACPL-P343_0_1")
		(symbol "ACPL-P343_1_1"
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VO")
				(number "5")
			)
			(pin power_in line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VEE")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACPL-W343"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 12.7 0)
		)
		(property "Value" "ACPL-W343"
			(at 0 10.16 0)
		)
		(property "Footprint" "Package_SO:SSO-6_6.8x4.6mm_P1.27mm_Clearance8mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.avagotech.com/docs/AV02-2928EN"
			(at -2.286 0.127 0)
		)
		(property "Description" "Gate Drive Optocoupler, Output Current 4.0/4.0A, Propagation Delay 200ns, SSO-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "MOSFET Driver IGBT Driver Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSO*6.8x4.6mm*P1.27mm*Clearance8mm*"
			(at 0 0 0)
		)
		(symbol "ACPL-W343_0_1")
		(symbol "ACPL-W343_1_1"
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VO")
				(number "5")
			)
			(pin power_in line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VEE")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AN34092B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "AN34092B"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:Panasonic_HQFN-16-1EP_4x4mm_P0.65mm_EP2.9x2.9mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://industrial.panasonic.com/content/data/SC/ds/ds4/AN34092B_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Channel GaN-Tr High-Speed Gate Driver, Output Current 6.0A, 24V, -5V Negative Gate Voltage, HQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "GaN Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Panasonic*HQFN*1EP*4x4mm*P0.65mm*EP2.9x2.9mm*"
			(at 0 0 0)
		)
		(symbol "AN34092B_0_1")
		(symbol "AN34092B_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "INP")
				(number "7")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "INN")
				(number "8")
			)
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "14")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "VREG")
				(number "10")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IGCNT")
				(number "11")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VRCNT")
				(number "12")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "VR")
				(number "13")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "TEST")
				(number "9")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VEE")
				(number "4")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUT1")
				(number "1")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT2")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT3")
				(number "3")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CP")
				(number "15")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "CN")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BSP75N"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 8.89 0)
		)
		(property "Value" "BSP75N"
			(at -10.16 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at -3.175 -12.065 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BSP75N-DS-v01_04-en.pdf?fileId=db3a30431ed1d7b2011f471f5a0256d1"
			(at 7.62 -10.16 0)
		)
		(property "Description" "Self-Protected Low Side Driver with Temperature and Current Limit, SOT−223"
			(at 0 0 0)
		)
		(property "ki_keywords" "MOSFET ESD Overcurrent"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
		(symbol "BSP75N_0_0"
			(text "Limit"
				(at -1.524 -3.429 0)
			)
			(text "Temp & Current"
				(at -1.27 -2.286 0)
			)
		)
		(symbol "BSP75N_0_1")
		(symbol "BSP75N_1_0")
		(symbol "BSP75N_1_1"
			(text "Limit"
				(at -3.429 0.381 0)
			)
			(text "dV/dt"
				(at -3.302 1.524 0)
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 7.62 -10.16 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
			(pin passive line
				(at 7.62 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "S")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BTS4140N"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 6.35 0)
		)
		(property "Value" "BTS4140N"
			(at -10.16 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at -1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BTS4140N-DS-v01_01-EN.pdf?fileId=5546d46259d9a4bf015a852aac8b7785"
			(at 10.16 -6.35 0)
		)
		(property "Description" "60V, 0.2A, 1ohm Rds, self-Protected High Side Driver with Temperature and Current Limit, SOT−223"
			(at 0 0 0)
		)
		(property "ki_keywords" "MOSFET ESD Overcurrent"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
		(symbol "BTS4140N_0_0")
		(symbol "BTS4140N_0_1")
		(symbol "BTS4140N_1_0")
		(symbol "BTS4140N_1_1"
			(text "1K"
				(at -8.255 0 0)
			)
			(text "Current Limit"
				(at -1.905 0.381 0)
			)
			(text "dV/dt, Temp &"
				(at -1.778 1.524 0)
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 7.62 7.62 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "4")
			)
			(pin passive line
				(at 7.62 -7.62 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EL7202CN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "EL7202CN"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.mouser.com/catalog/specsheets/intersil_fn7282.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "High Speed, Dual Channel Power MOSFET Driver, 4.5...15V supply, I(PK)=2A, non-inverting drivers, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "DS0026 Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "EL7202CN_0_1")
		(symbol "EL7202CN_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN_A")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN_B")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT_A")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT_B")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EL7212CN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "EL7212CN"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.mouser.com/catalog/specsheets/intersil_fn7282.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "High Speed, Dual Channel Power MOSFET Driver, 4.5...15V supply, I(PK)=2A, inverting drivers, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "DS0026 Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "EL7212CN_0_1")
		(symbol "EL7212CN_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN_A")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN_B")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{OUT_A}")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{OUT_B}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EL7222CN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "EL7222CN"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.mouser.com/catalog/specsheets/intersil_fn7282.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "High Speed, Dual Channel Power MOSFET Driver, 4.5...15V supply, I(PK)=2A, complementary drivers, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "DS0026 Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "EL7222CN_0_1")
		(symbol "EL7222CN_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN_A")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN_B")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{OUT_A}")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT_B")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FAN3111C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 7.62 0)
		)
		(property "Value" "FAN3111C"
			(at 2.54 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 16.51 -7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/fan3111c-d.pdf"
			(at 29.21 -10.16 0)
		)
		(property "Description" "High Speed Low Side MOSFET Gate Driver with CMOS inverting and non-inverting inputs, 4.5-18 V, 1.0 A, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "MOSFET gate driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
		(symbol "FAN3111C_0_1")
		(symbol "FAN3111C_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{IN-}")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FAN3111E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 7.62 0)
		)
		(property "Value" "FAN3111E"
			(at 2.54 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 16.51 -7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/fan3111c-d.pdf"
			(at 29.21 -10.16 0)
		)
		(property "Description" "High Speed Low Side MOSFET Gate Driver with logic voltage reference input, 4.5-18 V, 1.0 A, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "MOSFET gate driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?5*"
			(at 0 0 0)
		)
		(symbol "FAN3111E_0_1")
		(symbol "FAN3111E_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "XREF")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FAN3268"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "FAN3268"
			(at -2.54 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FAN3268T_F085-D.PDF"
			(at 0 2.54 0)
		)
		(property "Description" "Low-Voltage 18V PMOS-NMOS Bridge Driver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Driver MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "FAN3268_0_1")
		(symbol "FAN3268_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "INA")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INB")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ENA")
				(number "1")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "ENB")
				(number "8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUTA")
				(number "7")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{OUTB}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FAN7371"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "FAN7371"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FAN7371-D.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "High-Current High-Side Gate Driver, 600V Vs, 4A Io, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "high-side gate driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "FAN7371_0_1")
		(symbol "FAN7371_1_1"
			(pin power_in line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 5.08 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "8")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FAN7842"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "FAN7842"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FAN7842-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Gate Driver, 200V operation, Output Current 350/650mA, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "FAN7842_0_1")
		(symbol "FAN7842_1_1"
			(pin power_in line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "HIN")
				(number "2")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "LIN")
				(number "3")
			)
			(pin power_in line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "COM")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "8")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FAN7888"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 24.13 0)
		)
		(property "Value" "FAN7888"
			(at -2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 1.27 -19.05 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FAN7888-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "3 Half-Bridge Gate-Drive IC, 200V operation, Output Current 350/650mA, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "3 Phase Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "FAN7888_0_1")
		(symbol "FAN7888_1_1"
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "HIN1")
				(number "1")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "LIN1")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "HIN2")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "LIN2")
				(number "4")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "HIN3")
				(number "5")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "LIN3")
				(number "6")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "12")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "VB1")
				(number "20")
			)
			(pin output line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "HO1")
				(number "19")
			)
			(pin passive line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "VS1")
				(number "18")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "LO1")
				(number "17")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VB2")
				(number "16")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "HO2")
				(number "15")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "VS2")
				(number "14")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "LO2")
				(number "13")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VB3")
				(number "10")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "HO3")
				(number "9")
			)
			(pin passive line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "VS3")
				(number "8")
			)
			(pin output line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "LO3")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FL5150MX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 -12.7 0)
		)
		(property "Value" "FL5150MX"
			(at 7.62 -15.24 0)
		)
		(property "Footprint" "Package_SO:SSOP-10_3.9x4.9mm_P1.00mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FL5150-D.pdf"
			(at -2.54 -2.54 0)
		)
		(property "Description" "IGBT and MOSFET, AC Phase Cut, Dimmer Controller, SSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "dimmer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP?10?3.9x4.9mm*1.00mm*"
			(at 0 0 0)
		)
		(symbol "FL5150MX_0_1")
		(symbol "FL5150MX_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "ZC_Monitor")
				(number "1")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "DIM_Control")
				(number "2")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DIM_Mode")
				(number "4")
			)
			(pin power_out line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_out line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "OC_Sense1")
				(number "10")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "DRV_Gate")
				(number "9")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OC_Sense2")
				(number "8")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "Low_Power")
				(number "7")
			)
			(pin power_in line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HCPL-3120"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 12.7 0)
		)
		(property "Value" "HCPL-3120"
			(at 0 10.16 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0161EN"
			(at -2.286 0.127 0)
		)
		(property "Description" "Gate Drive Optocoupler, Output Current 2.5/2.5A, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "MOSFET Driver IGBT Driver Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "HCPL-3120_0_1")
		(symbol "HCPL-3120_1_1"
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VO")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VO")
				(number "7")
			)
			(pin power_out line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VEE")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HCPL-314J"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 12.7 0)
		)
		(property "Value" "HCPL-314J"
			(at 0 10.16 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W-12_7.5x10.3mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0169EN"
			(at -2.286 0.127 0)
		)
		(property "Description" "Gate Drive Optocoupler, Output Current 0.4/0.4A, SOIC-16(12)"
			(at 0 0 0)
		)
		(property "ki_keywords" "MOSFET Driver IGBT Driver Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*16*12*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HCPL-314J_0_1")
		(symbol "HCPL-314J_1_1"
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VO")
				(number "15")
			)
			(pin power_in line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VEE")
				(number "14")
			)
		)
		(symbol "HCPL-314J_2_1"
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "C")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VCC")
				(number "11")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VO")
				(number "10")
			)
			(pin power_in line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VEE")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HIP2100_DFN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 13.335 0)
		)
		(property "Value" "HIP2100_DFN"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-12-1EP_4x4mm_P0.5mm_EP2.66x3.38mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/hip2/hip2100.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "High Frequency Half Bridge Driver, Output Current 2.0A, 100V, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "HIP2100_DFN_0_1")
		(symbol "HIP2100_DFN_1_1"
			(pin power_in line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "HI")
				(number "7")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "LI")
				(number "8")
			)
			(pin power_in line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "VSS")
				(number "11")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin output line
				(at 0 -12.7 90)
				(length 2.54)
				(name "EP")
				(number "13")
			)
			(pin no_connect line
				(at 5.08 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "HB")
				(number "4")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "HO")
				(number "5")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "HS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HIP2100_EPSOIC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 13.335 0)
		)
		(property "Value" "HIP2100_EPSOIC"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.514x3.2mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/hip2/hip2100.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "High Frequency Half Bridge Driver, Output Current 2.0A, 100V, EPSOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HIP2100_EPSOIC_0_1")
		(symbol "HIP2100_EPSOIC_1_1"
			(pin power_in line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "HI")
				(number "5")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "LI")
				(number "6")
			)
			(pin power_in line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin output line
				(at 0 -12.7 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "HB")
				(number "2")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "HO")
				(number "3")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "HS")
				(number "4")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HIP2100_QFN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 13.335 0)
		)
		(property "Value" "HIP2100_QFN"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_5x5mm_P0.8mm_EP2.7x2.7mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/hip2/hip2100.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "High Frequency Half Bridge Driver, Output Current 2.0A, 100V, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "HIP2100_QFN_0_1")
		(symbol "HIP2100_QFN_1_1"
			(pin power_in line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "HI")
				(number "7")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "LI")
				(number "10")
			)
			(pin power_in line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "VSS")
				(number "11")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -5.08 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin output line
				(at 0 -12.7 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
			(pin no_connect line
				(at 5.08 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 5.08 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "HB")
				(number "2")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "HO")
				(number "3")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "HS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HIP2100_SOIC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 13.335 0)
		)
		(property "Value" "HIP2100_SOIC"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/hip2/hip2100.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "High Frequency Half Bridge Driver, Output Current 2.0A, 100V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HIP2100_SOIC_0_1")
		(symbol "HIP2100_SOIC_1_1"
			(pin power_in line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "HI")
				(number "5")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "LI")
				(number "6")
			)
			(pin power_in line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "HB")
				(number "2")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "HO")
				(number "3")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "HS")
				(number "4")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HIP4080A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 21.59 0)
		)
		(property "Value" "HIP4080A"
			(at 5.08 19.05 0)
		)
		(property "Footprint" ""
			(at -1.27 3.81 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/hip4/hip4080a.pdf"
			(at -1.27 -10.16 0)
		)
		(property "Description" "High Frequency Full Bridge FET Driver, Input Comparator, 2.5A, 80V, DIP-20/SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "HIP4080A_0_1")
		(symbol "HIP4080A_1_1"
			(pin output line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "HEN")
				(number "2")
			)
			(pin output line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "DIS")
				(number "3")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "IN+")
				(number "6")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "IN-")
				(number "7")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "HDEL")
				(number "8")
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "LDEL")
				(number "9")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "BHB")
				(number "1")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "AHB")
				(number "10")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "BHO")
				(number "20")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "BHS")
				(number "19")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "BLO")
				(number "18")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "BLS")
				(number "17")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "ALS")
				(number "14")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ALO")
				(number "13")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "AHS")
				(number "12")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "AHO")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HIP4081A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 21.59 0)
		)
		(property "Value" "HIP4081A"
			(at 5.08 19.05 0)
		)
		(property "Footprint" ""
			(at -1.27 3.81 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/hip4/hip4080a.pdf"
			(at -1.27 -10.16 0)
		)
		(property "Description" "High Frequency Full Bridge FET Driver, 2.5A, 80V, DIP-20/SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "HIP4081A_0_1")
		(symbol "HIP4081A_1_1"
			(pin output line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "DIS")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "AHI")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "ALI")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "BHI")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "BLI")
				(number "5")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "HDEL")
				(number "8")
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "LDEL")
				(number "9")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "BHB")
				(number "1")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "AHB")
				(number "10")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "BHO")
				(number "20")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "BHS")
				(number "19")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "BLO")
				(number "18")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "BLS")
				(number "17")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "ALS")
				(number "14")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ALO")
				(number "13")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "AHS")
				(number "12")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "AHO")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HIP4082xB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 16.51 0)
		)
		(property "Value" "HIP4082xB"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 2.54 19.05 0)
		)
		(property "Datasheet" "https://www.renesas.com/www/doc/datasheet/hip4082.pdf"
			(at 2.54 19.05 0)
		)
		(property "Description" "80V, 1.25A Peak Current H-Bridge FET Driver, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Driver H-bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HIP4082xB_0_0"
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "DEL")
				(number "5")
			)
		)
		(symbol "HIP4082xB_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "DIS")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "AHI")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "ALI")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "BHI")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "BLI")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "12")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "BHB")
				(number "1")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "AHB")
				(number "9")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "BHO")
				(number "16")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "BHS")
				(number "15")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "BLO")
				(number "14")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "ALO")
				(number "13")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "AHS")
				(number "11")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "AHO")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HIP4082xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 16.51 0)
		)
		(property "Value" "HIP4082xP"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 2.54 19.05 0)
		)
		(property "Datasheet" "https://www.renesas.com/www/doc/datasheet/hip4082.pdf"
			(at 2.54 19.05 0)
		)
		(property "Description" "80V, 1.25A Peak Current H-Bridge FET Driver, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Driver H-bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "HIP4082xP_0_0"
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "DEL")
				(number "5")
			)
		)
		(symbol "HIP4082xP_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "DIS")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "AHI")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "ALI")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "BHI")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "BLI")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "12")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "BHB")
				(number "1")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "AHB")
				(number "9")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "BHO")
				(number "16")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "BHS")
				(number "15")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "BLO")
				(number "14")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "ALO")
				(number "13")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "AHS")
				(number "11")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "AHO")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ICL7667"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "ICL7667"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 3.81 -21.59 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/icl7/icl7667.pdf"
			(at 5.08 -7.62 0)
		)
		(property "Description" "Dual Power MOSFET Driver, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "MOSFET driver array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ICL7667_0_1")
		(symbol "ICL7667_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INA")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "INB")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "V-")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{OUTA}")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{OUTB}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR2010"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2010"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2010.pdf?fileId=5546d462533600a4015355c48f901660"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 200V, 3.0/3.0A, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IR2010_0_1")
		(symbol "IR2010_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "HIN")
				(number "10")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "LIN")
				(number "12")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "SD")
				(number "11")
			)
			(pin no_connect line
				(at -5.08 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "13")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "9")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "2")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "6")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "VS")
				(number "5")
			)
			(pin power_in line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR2010S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2010S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2010.pdf?fileId=5546d462533600a4015355c48f901660"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 200V, 3.0/3.0A, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IR2010S_0_1")
		(symbol "IR2010S_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "HIN")
				(number "12")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "LIN")
				(number "14")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "SD")
				(number "13")
			)
			(pin no_connect line
				(at -5.08 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "7")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin power_in line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR2011"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2011"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2011.pdf?fileId=5546d462533600a4015355c49b831663"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 200V, 1.0/1.0A, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IR2011_0_1")
		(symbol "IR2011_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "HIN")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "LIN")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "7")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "2")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "3")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "4")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR2085S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2085S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IR2085S-DS-v01_02-EN.pdf?fileId=5546d4625b62cd8a015bb0f752184828"
			(at 0 0 0)
		)
		(property "Description" "High Speed, 100V, Self Oscillating 50% Duty Cycle, Half-Bridge Driver, 1.0/1.0A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Oscillating Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IR2085S_0_1")
		(symbol "IR2085S_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "OSC")
				(number "2")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "CS")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "8")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR2101"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2101"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2101.pdf?fileId=5546d462533600a4015355c7a755166c"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 210/360mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IR2101_0_1")
		(symbol "IR2101_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "HIN")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "LIN")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "8")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR2102"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2102"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2101.pdf?fileId=5546d462533600a4015355c7a755166c"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 210/360mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IR2102_0_1")
		(symbol "IR2102_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "~{HIN}")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{LIN}")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "8")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR2103"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2103"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2103.pdf?fileId=5546d462533600a4015355c7b54b166f"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 210/360mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IR2103_0_1")
		(symbol "IR2103_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "HIN")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{LIN}")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "8")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR2104"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2104"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2104.pdf?fileId=5546d462533600a4015355c7c1c31671"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 210/360mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IR2104_0_1")
		(symbol "IR2104_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{SD}")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "8")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR21064"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR21064"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2106.pdf?fileId=5546d462533600a4015355c7cfc51673"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 200/350mA, PDIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IR21064_0_1")
		(symbol "IR21064_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "HIN")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "LIN")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "13")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "12")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "11")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR21084"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "IR21084"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2108.pdf?fileId=5546d462533600a4015355c7dc321676"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 210/350mA, PDIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IR21084_0_1")
		(symbol "IR21084_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "HIN")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{LIN}")
				(number "3")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "DT")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "13")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "12")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "11")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR21091"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR21091"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir21091.pdf?fileId=5546d462533600a4015355c7f66f167c"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 200/350mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IR21091_0_1")
		(symbol "IR21091_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "DT/SD")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "8")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR21094"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "IR21094"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2109.pdf?fileId=5546d462533600a4015355c7e85b1679"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 200/350mA, PDIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IR21094_0_1")
		(symbol "IR21094_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{SD}")
				(number "3")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "DT")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "13")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "12")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "11")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR2111"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2111"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2111.pdf?fileId=5546d462533600a4015355c810e51682"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 250/500mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IR2111_0_1")
		(symbol "IR2111_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "3")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "8")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR2114S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 18.415 0)
		)
		(property "Value" "IR2114S"
			(at 1.27 16.51 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2114ss.pdf?fileId=5546d462533600a4015355c836cd168a"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Gate Driver IC, 600V, 1.0/1.5A, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x8.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "IR2114S_0_1")
		(symbol "IR2114S_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "HIN")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "LIN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "FLT_CLR")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SY_FLT}")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{FAULT/SD}")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -7.62 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at -7.62 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at -7.62 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -7.62 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "11")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "COM")
				(number "8")
			)
			(pin passive line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "VB")
				(number "23")
			)
			(pin input line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "DSH")
				(number "24")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "HOP")
				(number "21")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "HON")
				(number "20")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SSDH")
				(number "18")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VS")
				(number "19")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "DSL")
				(number "12")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "LOP")
				(number "10")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "LON")
				(number "9")
			)
			(pin input line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "SSDL")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR2133"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 22.86 0)
		)
		(property "Value" "IR2133"
			(at 7.62 22.86 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IR2x33-IR2x35-DataSheet-v01_00-EN.pdf?fileId=5546d462533600a4015355c890ba169f"
			(at 0 0 0)
		)
		(property "Description" "600V, Vout 10-20V, PDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "3 Phase Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "IR2133_0_1")
		(symbol "IR2133_1_1"
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "~{HIN1}")
				(number "22")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "~{HIN2}")
				(number "23")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "~{HIN3}")
				(number "24")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "~{LIN1}")
				(number "25")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{LIN2}")
				(number "26")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{LIN3}")
				(number "27")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "28")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{FLT-CLR}")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SD")
				(number "6")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "ITRIP")
				(number "1")
			)
			(pin output line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "CAO")
				(number "3")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "CA+")
				(number "5")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "CA-")
				(number "4")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin passive line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "VB1")
				(number "20")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "HO1")
				(number "19")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VS1")
				(number "18")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VB2")
				(number "17")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "HO2")
				(number "16")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VS2")
				(number "15")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "VB3")
				(number "14")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "HO3")
				(number "13")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VS3")
				(number "12")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "LO1")
				(number "11")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "LO2")
				(number "10")
			)
			(pin output line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "LO3")
				(number "9")
			)
			(pin passive line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "COM")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR2133S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 22.86 0)
		)
		(property "Value" "IR2133S"
			(at 7.62 22.86 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IR2x33-IR2x35-DataSheet-v01_00-EN.pdf?fileId=5546d462533600a4015355c890ba169f"
			(at 0 0 0)
		)
		(property "Description" "600V, Vout 10-20V, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "3 Phase Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IR2133S_1_1"
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "~{HIN1}")
				(number "22")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "~{HIN2}")
				(number "23")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "~{HIN3}")
				(number "24")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "~{LIN1}")
				(number "25")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{LIN2}")
				(number "26")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{LIN3}")
				(number "27")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "28")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{FLT-CLR}")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SD")
				(number "6")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "ITRIP")
				(number "1")
			)
			(pin output line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "CAO")
				(number "3")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "CA+")
				(number "5")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "CA-")
				(number "4")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin passive line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "VB1")
				(number "20")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "HO1")
				(number "19")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VS1")
				(number "18")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VB2")
				(number "17")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "HO2")
				(number "16")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VS2")
				(number "15")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "VB3")
				(number "14")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "HO3")
				(number "13")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VS3")
				(number "12")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "LO1")
				(number "11")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "LO2")
				(number "10")
			)
			(pin output line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "LO3")
				(number "9")
			)
			(pin passive line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "COM")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR2153"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2153"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2153.pdf?fileId=5546d462533600a4015355c8c5fc16af"
			(at 0 0 0)
		)
		(property "Description" "Self-Oscillating Half-Bridge Driver, 600V, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Oscillating Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IR2153_0_1")
		(symbol "IR2153_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "RT")
				(number "2")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "CT")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "8")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR2181"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2181"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2181.pdf?fileId=5546d462533600a4015355c93cdd16ce"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 1.4/1.8A, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IR2181_0_1")
		(symbol "IR2181_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "HIN")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "LIN")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "3")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "8")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR21814"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "IR21814"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2181.pdf?fileId=5546d462533600a4015355c93cdd16ce"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 1.4/1.8A, PDIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IR21814_0_1")
		(symbol "IR21814_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "HIN")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "LIN")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "13")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "12")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "11")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR2183"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2183"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2183.pdf?fileId=5546d462533600a4015355c9490e16d1"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 1.4/1.8A, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IR2183_0_1")
		(symbol "IR2183_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "HIN")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{LIN}")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "3")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "8")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR21834"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "IR21834"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2183.pdf?fileId=5546d462533600a4015355c9490e16d1"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 1.4/1.8A, PDIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IR21834_0_1")
		(symbol "IR21834_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "HIN")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{LIN}")
				(number "2")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "DT")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "13")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "12")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "11")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR2184"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2184"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2184.pdf?fileId=5546d462533600a4015355c955e616d4"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 1.4/1.8A, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IR2184_0_1")
		(symbol "IR2184_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{SD}")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "3")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "8")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR21844"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "IR21844"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2184.pdf?fileId=5546d462533600a4015355c955e616d4"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 1.4/1.8A, PDIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IR21844_0_1")
		(symbol "IR21844_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{SD}")
				(number "2")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "DT")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "13")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "12")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "11")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR2304"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2304"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2304.pdf?fileId=5546d462533600a4015355c9954a16e0"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 60/130mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IR2304_0_1")
		(symbol "IR2304_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "HIN")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "LIN")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "8")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR25602S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR25602S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir25602.pdf?fileId=5546d462533600a4015355c9d6c216eb"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 210/360mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IR25602S_0_1")
		(symbol "IR25602S_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{SD}")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "8")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR25603"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR25603"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir25603.pdf?fileId=5546d462533600a4015355c9e46716ef"
			(at 0 0 0)
		)
		(property "Description" "Self-Oscillating Half-Bridge Driver, 600V, 180/260mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Oscillating Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "IR25603_0_1")
		(symbol "IR25603_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "RT")
				(number "2")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "CT")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "8")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR25604S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR25604S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir25604.pdf?fileId=5546d462533600a4015355c9f1ca16f1"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 200/350mA, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IR25604S_0_1")
		(symbol "IR25604S_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "HIN")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "LIN")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "8")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR7184S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR7184S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir7184s.pdf?fileId=5546d462533600a4015355d62230182c"
			(at 0 0 0)
		)
		(property "Description" "700V Half-Bridge Driver, 1.9/2.3A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IR7184S_0_1")
		(symbol "IR7184S_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{SD}")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "3")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "8")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR7304S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR7304S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir7304s.pdf?fileId=5546d462533600a4015355d62a63182e"
			(at 0 0 0)
		)
		(property "Description" "700V Half-Bridge Driver, 60/130mA, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IR7304S_0_1")
		(symbol "IR7304S_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "HIN")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "LIN")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "8")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRS2001M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2001M"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:Infineon_MLPQ-16-14-1EP_4x4mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2001mpbf.pdf?fileId=5546d462533600a4015356759e20277c"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 200V, 290/600mA, MLPQ-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*MLPQ*EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "IRS2001M_0_1")
		(symbol "IRS2001M_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "HIN")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "LIN")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "COM")
				(number "17")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "13")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "12")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "11")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRS2113M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2113M"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:Infineon_MLPQ-16-14-1EP_4x4mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2113mpbf.pdf?fileId=5546d462533600a40153567676a227b7"
			(at 0 0 0)
		)
		(property "Description" "High- and Low-Side Driver, 600V, 2.5/2.5A, MLPQ-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*MLPQ*EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "IRS2113M_0_1")
		(symbol "IRS2113M_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "HIN")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "LIN")
				(number "4")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "SD")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "COM")
				(number "17")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "7")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "13")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "VS")
				(number "12")
			)
			(pin power_in line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRS21814M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS21814M"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:Infineon_MLPQ-16-14-1EP_4x4mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs21814mpbf.pdf?fileId=5546d462533600a401535676c8a827d6"
			(at 0 0 0)
		)
		(property "Description" "High- and Low-Side Driver, 600V, 1.9/2.3A, MLPQ-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*MLPQ*EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "IRS21814M_0_1")
		(symbol "IRS21814M_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "HIN")
				(number "16")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "LIN")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "COM")
				(number "17")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "13")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "12")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "11")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRS21844M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS21844M"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:Infineon_MLPQ-16-14-1EP_4x4mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs21844mpbf.pdf?fileId=5546d462533600a401535676dfb027de"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 1.9/2.3A, MLPQ-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*MLPQ*EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "IRS21844M_0_1")
		(symbol "IRS21844M_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "16")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{SD}")
				(number "1")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "DT")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "COM")
				(number "17")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "13")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "12")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "11")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRS2890DS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2890DS"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IRS2890DS-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aad6fbc8a4bf4"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver with Overcurrent Protection, 600V, 220/480mA, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IRS2890DS_0_1")
		(symbol "IRS2890DS_1_1"
			(pin open_collector line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "RFE")
				(number "7")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "HIN")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "LIN")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(name "ITRIP")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VB")
				(number "14")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "13")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VS")
				(number "12")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ITS724G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "ITS724G"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-ITS724G-DS-v01_01-en.pdf?fileId=db3a304412b407950112b428d6083e90"
			(at 0 0 0)
		)
		(property "Description" "Smart High-Side Power Switch for Industrial Applications, Four Channels, Rds 90mΩ, SOIC-20W"
			(at 0 0 0)
		)
		(property "ki_keywords" "driver fet quad"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ITS724G_0_1")
		(symbol "ITS724G_1_1"
			(pin open_collector line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "ST1/2")
				(number "4")
			)
			(pin open_collector line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "ST3/4")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN1")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN2")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IN3")
				(number "7")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "IN4")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND1/2")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VBB")
				(number "1")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "VBB")
				(number "10")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "VBB")
				(number "11")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "VBB")
				(number "12")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "VBB")
				(number "15")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "VBB")
				(number "16")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "VBB")
				(number "19")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "VBB")
				(number "20")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND3/4")
				(number "6")
			)
			(pin open_emitter line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUT1")
				(number "18")
			)
			(pin open_emitter line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "17")
			)
			(pin open_emitter line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT3")
				(number "14")
			)
			(pin open_emitter line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "OUT4")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L6491"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 15.24 0)
		)
		(property "Value" "L6491"
			(at 7.62 15.24 0)
		)
		(property "Footprint" "Package_SO:SO-14_3.9x8.65mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/l6491.pdf"
			(at 0 0 0)
		)
		(property "Description" "High voltage high and low-side 4 A gate driver, SO-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "fet driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x8.65mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "L6491_0_1")
		(symbol "L6491_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "HIN")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{LIN}")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{SD}/OD")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DT")
				(number "5")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "SGND")
				(number "6")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "PGND")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "BOOT")
				(number "14")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "HVG")
				(number "13")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "12")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "LVG")
				(number "8")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "CP+")
				(number "10")
			)
			(pin input line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "CP-")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LF2190N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "LF2190N"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 22.86 -12.7 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=4c945cfe-ef54-4349-b2fb-9c1330d8240c&filename=littelfuse-gate-drivers-lf2190ntr-datasheet"
			(at 2.54 -15.24 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 4.5/4.5A, SO-8"
			(at 2.54 -17.78 0)
		)
		(property "ki_keywords" "ixys littelfuse boosted bootstrapped dual"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LF2190N_0_1")
		(symbol "LF2190N_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "HIN")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "LIN")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V_{CC}")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "COM")
				(number "3")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "V_{B}")
				(number "8")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "V_{S}")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2105D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "LM2105D"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.254 -27.178 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm2105.pdf"
			(at 1.524 -30.226 0)
		)
		(property "Description" "107-V, 0.5-A, 0.8-A Half-Bridge Driver with 5-V UVLO and Integrated Bootstrap Diode, SOIC-8"
			(at 0.254 -24.384 0)
		)
		(property "ki_keywords" "gate driver bootstrap half bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27*"
			(at 0 0 0)
		)
		(symbol "LM2105D_0_1")
		(symbol "LM2105D_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "INH")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "INL")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "GVDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "BST")
				(number "8")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "GH")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "SH")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "GL")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM2105DSG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "LM2105DSG"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm"
			(at 0.254 -27.178 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm2105.pdf"
			(at 1.524 -30.226 0)
		)
		(property "Description" "107-V, 0.5-A, 0.8-A Half-Bridge Driver with 5-V UVLO and Integrated Bootstrap Diode, WSON-8-1EP"
			(at 0.254 -24.384 0)
		)
		(property "ki_keywords" "gate driver bootstrap half bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.5mm*EP0.9x1.6*"
			(at 0 0 0)
		)
		(symbol "LM2105DSG_0_1")
		(symbol "LM2105DSG_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "INH")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "INL")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "GVDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "BST")
				(number "8")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "GH")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "SH")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "GL")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5109ASD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "LM5109ASD"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_4x4mm_P0.8mm_EP2.6x3mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5109a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Gate Driver, Output Current 1.0A, 100V, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half-Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "LM5109ASD_0_1")
		(symbol "LM5109ASD_1_1"
			(pin power_in line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "HI")
				(number "2")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "LI")
				(number "3")
			)
			(pin power_in line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "9")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "HB")
				(number "8")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "HS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM5109MA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "LM5109MA"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5109.pdf"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Gate Driver, Output Current 1.0A, 100V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half-Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM5109MA_0_1")
		(symbol "LM5109MA_1_1"
			(pin power_in line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "HI")
				(number "2")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "LI")
				(number "3")
			)
			(pin power_in line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "HB")
				(number "8")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "HO")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "HS")
				(number "6")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "LO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMG1020YFF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.715 5.715 0)
		)
		(property "Value" "LMG1020YFF"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-6_0.855x1.255mm_Layout2x3_P0.4mm_LevelB"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lmg1020.pdf"
			(at 0 -19.05 0)
		)
		(property "Description" "5-V, 7-A, 5-A Low-Side GaN and MOSFET Driver For 1-ns Pulse Width, DSBGA-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "gan hemt gate driver low side fast rise time"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas?DSBGA?6?0.855x1.255mm?Layout2x3?P0.4mm*"
			(at 0 0 0)
		)
		(symbol "LMG1020YFF_0_1")
		(symbol "LMG1020YFF_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "C1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN-")
				(number "C2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "A1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "B1")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTH")
				(number "A2")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTL")
				(number "B2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4440EMS8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LTC4440EMS8"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4440fb.pdf"
			(at -2.54 11.43 0)
		)
		(property "Description" "High-side, N-Channel, Mosfet driver, 80V input, -40°C to +85°C, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "high-side mosfet-driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC4440EMS8_0_1")
		(symbol "LTC4440EMS8_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "INP")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "PAD")
				(number "9")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BOOST")
				(number "6")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "TG")
				(number "7")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "TS")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4440ES6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LTC4440ES6"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4440fb.pdf"
			(at -2.54 11.43 0)
		)
		(property "Description" "High-side, N-Channel, Mosfet driver, 80V input, -40°C to +85°C, SOT23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "high-side mosfet-driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LTC4440ES6_0_1")
		(symbol "LTC4440ES6_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "INP")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "BOOST")
				(number "6")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "TG")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "TS")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX15012AxSA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 13.335 0)
		)
		(property "Value" "MAX15012AxSA"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX15012-MAX15013B.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "High Frequency Half Bridge Driver, Output Current 2.0A, 175V, CMOS Input, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX15012AxSA_0_1")
		(symbol "MAX15012AxSA_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN_H")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "IN_L")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "BST")
				(number "2")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "DH")
				(number "3")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "HS")
				(number "4")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "DL")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX15012BxSA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 13.335 0)
		)
		(property "Value" "MAX15012BxSA"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX15012-MAX15013B.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "High Frequency Half Bridge Driver, Output Current 2.0A, 175V, CMOS Input, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX15012BxSA_0_1")
		(symbol "MAX15012BxSA_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN_H")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{IN_L}")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "BST")
				(number "2")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "DH")
				(number "3")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "HS")
				(number "4")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "DL")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX15012CxSA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 13.335 0)
		)
		(property "Value" "MAX15012CxSA"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.514x3.2mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX15012-MAX15013B.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "High Frequency Half Bridge Driver, Output Current 2.0A, 175V, CMOS Input, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX15012CxSA_0_1")
		(symbol "MAX15012CxSA_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN_H")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "IN_L")
				(number "6")
			)
			(pin output line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "BST")
				(number "2")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "DH")
				(number "3")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "HS")
				(number "4")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "DL")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX15012DxSA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 13.335 0)
		)
		(property "Value" "MAX15012DxSA"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.514x3.2mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX15012-MAX15013B.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "High Frequency Half Bridge Driver, Output Current 2.0A, 175V, CMOS Input, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX15012DxSA_0_1")
		(symbol "MAX15012DxSA_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN_H")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{IN_L}")
				(number "6")
			)
			(pin output line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "BST")
				(number "2")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "DH")
				(number "3")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "HS")
				(number "4")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "DL")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1415"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MCP1415"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002092F.pdf"
			(at -5.08 6.35 0)
		)
		(property "Description" "1.5A High speed power MOSFET driver with inverting output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "mosfet gate driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP1415_0_1")
		(symbol "MCP1415_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vdd")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{OUT}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1415R"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MCP1415R"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002092F.pdf"
			(at -5.08 6.35 0)
		)
		(property "Description" "1.5A High speed power MOSFET driver with inverting output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "mosfet gate driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP1415R_0_1")
		(symbol "MCP1415R_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vdd")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{OUT}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1416"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MCP1416"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002092F.pdf"
			(at -5.08 6.35 0)
		)
		(property "Description" "1.5A High speed power MOSFET driver with non-inverting output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "mosfet gate driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP1416_0_1")
		(symbol "MCP1416_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vdd")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1416R"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MCP1416R"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002092F.pdf"
			(at -5.08 6.35 0)
		)
		(property "Description" "1.5A High speed power MOSFET driver with non-inverting output, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "mosfet gate driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP1416R_0_1")
		(symbol "MCP1416R_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vdd")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP14A0303xMNY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP14A0303xMNY"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.4mm"
			(at 0 19.05 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP14A0303_4_5-Data-Sheet-20006046A.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "Dual 3A-Peak MOSFET Driver, inverting outputs, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Driver, Dual MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*1EP*3x2mm*P0.5mm*EP1.3x1.4mm*"
			(at 0 0 0)
		)
		(symbol "MCP14A0303xMNY_0_1")
		(symbol "MCP14A0303xMNY_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "ENA")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INA")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "INB")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "ENB")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{OUTA}")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{OUTB}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP14A0304xMNY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP14A0304xMNY"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.4mm"
			(at 0 19.05 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP14A0303_4_5-Data-Sheet-20006046A.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "Dual 3A-Peak MOSFET Driver, non-inverting outputs, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Driver, Dual MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*1EP*3x2mm*P0.5mm*EP1.3x1.4mm*"
			(at 0 0 0)
		)
		(symbol "MCP14A0304xMNY_0_1")
		(symbol "MCP14A0304xMNY_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "ENA")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INA")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "INB")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "ENB")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTA")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP14A0305xMNY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP14A0305xMNY"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.4mm"
			(at 0 19.05 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP14A0303_4_5-Data-Sheet-20006046A.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "Dual 3A-Peak MOSFET Driver, inverting/non-inverting outputs, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Driver, Dual MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*1EP*3x2mm*P0.5mm*EP1.3x1.4mm*"
			(at 0 0 0)
		)
		(symbol "MCP14A0305xMNY_0_1")
		(symbol "MCP14A0305xMNY_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "ENA")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INA")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "INB")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "ENB")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{OUTA}")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP14A0901xMNY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "MCP14A0901xMNY"
			(at 2.54 7.62 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.4mm"
			(at 0 19.05 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP14A0901_2-Data-Sheet-20006183A.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Dual 9A-Peak MOSFET Driver, inverting outputs, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Driver, Dual MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP14A0901xMNY_0_1")
		(symbol "MCP14A0901xMNY_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~{OUT}")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "~{OUT}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP14A0902xMNY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP14A0902xMNY"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.4mm"
			(at 0 19.05 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP14A0901_2-Data-Sheet-20006183A.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "Dual 9A-Peak MOSFET Driver, non-inverting outputs, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Driver, Dual MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP14A0902xMNY_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "OUT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC4426"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MIC4426"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/el72/el7202-12-22.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "Dual 1.5A-Peak Low-Side MOSFET Driver, DIP-8/SOIC-8/MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Driver, Dual MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* MSOP*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MIC4426_0_1")
		(symbol "MIC4426_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN_A")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN_B")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{OUT_A}")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{OUT_B}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC4427"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MIC4427"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic4426.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "Dual 1.5A-Peak Low-Side MOSFET Driver, DIP-8/SOIC-8/MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Driver, Dual MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* MSOP*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MIC4427_0_1")
		(symbol "MIC4427_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN_A")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN_B")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT_A")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT_B")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC4428"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MIC4428"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/mic4426.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "Dual 1.5A-Peak Low-Side MOSFET Driver, DIP-8/SOIC-8/MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Driver, Dual MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* MSOP*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MIC4428_0_1")
		(symbol "MIC4428_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN_A")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN_B")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{OUT_A}")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT_B")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MIC4604YM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 -8.89 0)
		)
		(property "Value" "MIC4604YM"
			(at -8.89 -11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005852A.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "85V Half-Bridge MOSFET Driver with up to 16V Programmable Gate Drive, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half-Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MIC4604YM_0_1")
		(symbol "MIC4604YM_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "HI")
				(number "5")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "LI")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "HB")
				(number "2")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "HO")
				(number "3")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "HS")
				(number "4")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "LO")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCD5702"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 13.97 0)
		)
		(property "Value" "NCD5702"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCD5702-D.PDF"
			(at 0 2.54 0)
		)
		(property "Description" "High Current IGBT Gate, +4/-6A, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "igbt gate driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "NCD5702_0_1")
		(symbol "NCD5702_1_1"
			(pin power_out line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VREF")
				(number "3")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin open_collector line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{FLT}")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "GNDA")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "VEEA")
				(number "15")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VEE")
				(number "14")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin input line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "DESAT")
				(number "9")
			)
			(pin open_emitter line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VOH")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "VOL")
				(number "12")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "CLAMP")
				(number "16")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "RSVD")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCV8402xST"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 8.89 0)
		)
		(property "Value" "NCV8402xST"
			(at -11.43 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 0 -7.112 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCV8402-D.PDF"
			(at 7.62 0 0)
		)
		(property "Description" "Self-Protected Low Side Driver with Temperature and Current Limit, SOT−223"
			(at 0 0 0)
		)
		(property "ki_keywords" "MOSFET ESD Overcurrent"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
		(symbol "NCV8402xST_0_0"
			(text "Limit"
				(at -1.524 -3.429 0)
			)
			(text "Temp & Current"
				(at -1.27 -2.286 0)
			)
		)
		(symbol "NCV8402xST_0_1")
		(symbol "NCV8402xST_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "2")
			)
			(pin passive line
				(at 7.62 10.16 270)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin passive line
				(at 7.62 -10.16 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PE29101"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "PE29101"
			(at 6.35 16.51 0)
		)
		(property "Footprint" "Package_CSP:pSemi_CSP-16_1.64x2.04mm_P0.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.psemi.com/pdf/datasheets/pe29101ds.pdf"
			(at 0 0 0)
		)
		(property "Description" "UltraCMOS High-Speed FET Driver, 40 MHz, Output Current 2.0A/4.0A, 80V, Half Bridge, Low Side Output, CSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "GaN Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "pSemi*CSP*1.64x2.04mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "PE29101_0_1")
		(symbol "PE29101_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "7")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "LSO")
				(number "10")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "RDLH")
				(number "5")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "RDHL")
				(number "16")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "VDDSYNC")
				(number "4")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "HSB")
				(number "3")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "HSGpu")
				(number "6")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "HSGpd")
				(number "1")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "HSS")
				(number "2")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "LSB")
				(number "14")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "LSGpu")
				(number "9")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "LSGpd")
				(number "12")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "LSS")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PE29102"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "PE29102"
			(at 6.35 16.51 0)
		)
		(property "Footprint" "Package_CSP:pSemi_CSP-16_1.64x2.04mm_P0.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.psemi.com/pdf/datasheets/pe29102ds.pdf"
			(at 0 0 0)
		)
		(property "Description" "UltraCMOS High-Speed FET Driver, 40 MHz, Output Current 2.0A/4.0A, 80V, Half Bridge, Phase Control, CSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "GaN Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "pSemi*CSP*1.64x2.04mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "PE29102_0_1")
		(symbol "PE29102_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IN")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PHCTL")
				(number "10")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "RDLH")
				(number "5")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "RDHL")
				(number "16")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin no_connect line
				(at 10.16 12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "HSB")
				(number "3")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "HSGpu")
				(number "6")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "HSGpd")
				(number "1")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "HSS")
				(number "2")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "LSB")
				(number "14")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "LSGpu")
				(number "9")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "LSGpd")
				(number "12")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "LSS")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PM8834"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "PM8834"
			(at 12.7 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/pm8834.pdf"
			(at 0 0 0)
		)
		(property "Description" "4A dual low-side MOSFET driver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "mosfet driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PM8834_0_1")
		(symbol "PM8834_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "EN1")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "PWM1")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN2")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PWM2")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT1")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PM8834M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "PM8834M"
			(at 12.7 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.95x2.15mm"
			(at -2.54 -20.32 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/pm8834.pdf"
			(at 0 0 0)
		)
		(property "Description" "4A dual low-side MOSFET driver, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "mosfet driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PM8834M_0_1")
		(symbol "PM8834M_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "EN1")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "PWM1")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "EN2")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PWM2")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT1")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SM72295MA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 26.67 0)
		)
		(property "Value" "SM72295MA"
			(at 6.35 24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 26.67 -24.13 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sm72295"
			(at -1.27 -10.16 0)
		)
		(property "Description" "Full Bridge Gate Driver with integrated Current Sense Amplifier, 3A, 115V, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Full Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SM72295MA_0_1")
		(symbol "SM72295MA_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "SIA")
				(number "1")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "SOA")
				(number "2")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "OVS")
				(number "16")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "HIA")
				(number "7")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "HIB")
				(number "8")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "LIA")
				(number "6")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "LIB")
				(number "9")
			)
			(pin output line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "BIN")
				(number "4")
			)
			(pin output line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "BOUT")
				(number "11")
			)
			(pin passive line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "IIN")
				(number "3")
			)
			(pin passive line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "IOUT")
				(number "12")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "AGND")
				(number "5")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCCA")
				(number "21")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VCCB")
				(number "25")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "PGND")
				(number "23")
			)
			(pin input line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "SIB")
				(number "14")
			)
			(pin input line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "SOB")
				(number "13")
			)
			(pin passive line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "HBA")
				(number "20")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "HSA")
				(number "18")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "HOA")
				(number "19")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "LOA")
				(number "22")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "HBB")
				(number "26")
			)
			(pin passive line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "HSB")
				(number "28")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "HOB")
				(number "27")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "LOB")
				(number "24")
			)
			(pin open_collector line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PGOOD")
				(number "10")
			)
			(pin open_collector line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "OVP")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STGAP1AS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 20.32 0)
		)
		(property "Value" "STGAP1AS"
			(at 10.16 20.32 0)
		)
		(property "Footprint" "Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stgap1as.pdf"
			(at 0 0 0)
		)
		(property "Description" "Galvanically isolated 5 A advanced single gate driver, Dual Output, Miller Clamp, Sense, Desaturation, UVLO, OVLO, SPI, AEC-Q100, SOIC-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "isolated fet driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x15.4mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "STGAP1AS_0_1")
		(symbol "STGAP1AS_1_1"
			(pin output line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SDO")
				(number "2")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SDI")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "CK")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "IN+")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN-/DIAG2")
				(number "8")
			)
			(pin open_collector line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "DIAG1")
				(number "10")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{SD}")
				(number "11")
			)
			(pin power_in line
				(at -5.08 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at -5.08 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GNDISO")
				(number "13")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VH")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "VL")
				(number "14")
			)
			(pin passive line
				(at 2.54 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "VL")
				(number "23")
			)
			(pin power_out line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "VREG")
				(number "6")
			)
			(pin power_out line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VREGISO")
				(number "15")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VCECLAMP")
				(number "19")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DESAT")
				(number "18")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "GON")
				(number "20")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GOFF")
				(number "21")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "CLAMP")
				(number "22")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SENSE")
				(number "16")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "ASC")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STGAP2SCM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "STGAP2SCM"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stgap2s.pdf"
			(at 0 0 0)
		)
		(property "Description" "Galvanically isolated 4 A single gate driver, Single Output, Miller Clamp, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "isolated fet driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "STGAP2SCM_0_1")
		(symbol "STGAP2SCM_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VH")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GNDISO")
				(number "8")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "GOUT")
				(number "6")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CLAMP")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STGAP2SM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "STGAP2SM"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stgap2s.pdf"
			(at 0 0 0)
		)
		(property "Description" "Galvanically isolated 4 A single gate driver, Dual Output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "isolated fet driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "STGAP2SM_0_1")
		(symbol "STGAP2SM_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VH")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GNDISO")
				(number "8")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "GON")
				(number "6")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "GOFF")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TC4421"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 6.35 0)
		)
		(property "Value" "TC4421"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001420F.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "9A High-Speed inverting MOSFET Driver"
			(at 0 0 0)
		)
		(property "ki_keywords" "MOSFET IGBT driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TC4421_0_1")
		(symbol "TC4421_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "INPUT")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{OUTPUT}")
				(number "6")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(hide yes)
				(name "~{OUTPUT}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TC4422"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 6.35 0)
		)
		(property "Value" "TC4422"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001420F.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "9A High-Speed non-inverting MOSFET Driver"
			(at 0 0 0)
		)
		(property "ki_keywords" "MOSFET IGBT driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TC4422_0_1")
		(symbol "TC4422_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "INPUT")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUTPUT")
				(number "6")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(hide yes)
				(name "OUTPUT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TC4426xOA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "TC4426xOA"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.508 -15.24 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/20001422G.pdf"
			(at 0.508 -13.208 0)
		)
		(property "Description" "1.5A Dual High-Speed Power MOSFET Drivers, 4.5...18V supply, TTL/CMOS compatible inputs, inverting drivers, SOIC-8"
			(at 0 -11.176 0)
		)
		(property "ki_keywords" "ESD push-pull"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SO*3.9*4.*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TC4426xOA_0_1")
		(symbol "TC4426xOA_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN_A")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN_B")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{OUT_A}")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{OUT_B}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TC4427xOA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "TC4427xOA"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.508 -15.24 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/20001422G.pdf"
			(at 0.508 -13.208 0)
		)
		(property "Description" "1.5A Dual High-Speed Power MOSFET Drivers, 4.5...18V supply, TTL/CMOS compatible inputs, non-inverting drivers, SOIC-8"
			(at 0 -11.176 0)
		)
		(property "ki_keywords" "ESD push-pull"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SO*3.9*4.*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TC4427xOA_0_1")
		(symbol "TC4427xOA_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN_A")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN_B")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT_A")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT_B")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TC4428xOA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "TC4428xOA"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.508 -15.24 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/20001422G.pdf"
			(at 0.508 -13.208 0)
		)
		(property "Description" "1.5A Dual High-Speed Power MOSFET Drivers, 4.5...18V supply, TTL/CMOS compatible inputs, complementary drivers, SOIC-8"
			(at 0.508 -11.176 0)
		)
		(property "ki_keywords" "ESD push-pull"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SO*3.9*4.*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TC4428xOA_0_1")
		(symbol "TC4428xOA_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN_A")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN_B")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{OUT_A}")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT_B")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP250"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 12.7 0)
		)
		(property "Value" "TLP250"
			(at 0 10.16 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://toshiba.semicon-storage.com/info/docget.jsp?did=16821&prodName=TLP250"
			(at -2.286 0.127 0)
		)
		(property "Description" "Gate Drive Optocoupler, Output Current 1.5/1.5A, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "MOSFET Driver IGBT Driver Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TLP250_0_1")
		(symbol "TLP250_1_1"
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VO")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VO")
				(number "7")
			)
			(pin power_in line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VEE")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UCC21520DW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "UCC21520DW"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc21520.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Isolated Dual-Channel Gate Driver, Output Current 4.0/6.0A, 5.7kV Isolation, 8V UVLO, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Isolated Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "UCC21520DW_0_0"
			(text "Logic Input"
				(at -3.302 0 900)
			)
		)
		(symbol "UCC21520DW_0_1")
		(symbol "UCC21520DW_1_1"
			(pin power_in line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "VCCI")
				(number "3")
			)
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(hide yes)
				(name "VCCI")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "INA")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "INB")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DIS")
				(number "5")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "DT")
				(number "6")
			)
			(pin power_in line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin power_in line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VDDA")
				(number "16")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUTA")
				(number "15")
			)
			(pin power_in line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VSSA")
				(number "14")
			)
			(pin power_in line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VDDB")
				(number "11")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUTB")
				(number "10")
			)
			(pin power_in line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "VSSB")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UCC27511ADBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "UCC27511ADBV"
			(at 8.89 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -12.065 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ucc27511a.pdf"
			(at 0 19.05 0)
		)
		(property "Description" "Single-Channel High-Speed Low-Side Gate Driver With 4-A Peak Source and 8-A Peak Sink, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "single channel low side gate drive dual input split output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "UCC27511ADBV_0_1")
		(symbol "UCC27511ADBV_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN-")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTH")
				(number "2")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTL")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UCC27714D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "UCC27714D"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc27714.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "High-Speed, 600-V High-Side Low-Side Gate Driver, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "gate driver bootstrap"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "UCC27714D_0_1")
		(symbol "UCC27714D_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "HI")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "LI")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN/NC")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -7.62 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "HB")
				(number "13")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "HO")
				(number "12")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "HS")
				(number "11")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "LO")
				(number "6")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "COM")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ZXGD3001E6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 6.35 0)
		)
		(property "Value" "ZXGD3001E6"
			(at 10.16 -7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ZXGD3001E6.pdf"
			(at -8.89 6.35 0)
		)
		(property "Description" "9A (peak) Gate driver, 12V, 3ns delay, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "gate driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "ZXGD3001E6_0_1")
		(symbol "ZXGD3001E6_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "IN1")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN2")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin open_emitter line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SOURCE")
				(number "6")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SINK")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ZXGD3006E6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 8.89 0)
		)
		(property "Value" "ZXGD3006E6"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ZXGD3006E6.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V 10A gate driver, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "mosfet igbt driver buffer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "ZXGD3006E6_0_1")
		(symbol "ZXGD3006E6_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VEE")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin open_emitter line
				(at 10.16 0 180)
				(length 2.54)
				(name "SRC")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SINK")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ZXGD3009E6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 6.35 0)
		)
		(property "Value" "ZXGD3009E6"
			(at 10.16 -7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ZXGD3009E6.pdf"
			(at -8.89 6.35 0)
		)
		(property "Description" "2A (peak) Gate driver, 40V, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "gate driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "ZXGD3009E6_0_1")
		(symbol "ZXGD3009E6_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VEE")
				(number "3")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin open_emitter line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SOURCE")
				(number "6")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SINK")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "1EDN8550B"
		(extends "1EDN7550B")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "1EDN8550B"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-1EDN7550B-DS-v02_00-EN.pdf?fileId=5546d46262b31d2e01635d9799ef264f"
			(at 0 -7.62 0)
		)
		(property "Description" "Single-Channel EiceDRIVER With True Differential Inputs, 8V UVLO, +4/-8A, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Driver, Dual MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "2ED1323S12P"
		(extends "2ED1324S12P")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "2ED1323S12P"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:Infineon_PG-DSO-20-U03_7.5x12.8mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-2ED1323S12P_2ED1324S12P-DataSheet-v01_01-EN.pdf?fileId=8ac78c8c869190210186e92f0f506d0c"
			(at 1.27 -15.24 0)
		)
		(property "Description" "1200V Half Bridge Gate Driver with active Miller clamp, OCP, SCC, Bootstrap Diode, ±2.3A drive current, PG-DSO-20-U03"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver MOSFET IGBT SiC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*PG?DSO?20?U03*7.5x12.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "BSP76"
		(extends "BSP75N")
		(property "Reference" "Q"
			(at 5.08 8.89 0)
		)
		(property "Value" "BSP76"
			(at -10.16 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at -3.175 -12.065 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-BSP76-DS-v01_03-en.pdf?fileId=db3a3043271faefd01274d00e2695d45"
			(at 7.62 -10.16 0)
		)
		(property "Description" "Self-Protected Low Side Driver with Temperature and Current Limit, 42 V Vds, 1.4 A Id, 200 mOhm Rds, SOT-223"
			(at 0 -17.272 0)
			(show_name)
		)
		(property "ki_keywords" "MOSFET ESD Overcurrent LowSideSwitch automotive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "EL7202CS"
		(extends "EL7202CN")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "EL7202CS"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.mouser.com/catalog/specsheets/intersil_fn7282.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "High Speed, Dual Channel Power MOSFET Driver, 4.5...15V supply, I(PK)=2A, non-inverting drivers, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "DS0026"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*3.9*4.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "EL7212CS"
		(extends "EL7212CN")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "EL7212CS"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.mouser.com/catalog/specsheets/intersil_fn7282.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "High Speed, Dual Channel Power MOSFET Driver, 4.5...15V supply, I(PK)=2A, inverting drivers, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "DS0026"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*3.9*4.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "EL7222CS"
		(extends "EL7222CN")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "EL7222CS"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.mouser.com/catalog/specsheets/intersil_fn7282.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "High Speed, Dual Channel Power MOSFET Driver, 4.5...15V supply, I(PK)=2A, complementary drivers, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "DS0026"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*3.9*4.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FAN3278"
		(extends "FAN3268")
		(property "Reference" "U"
			(at -2.54 13.97 0)
		)
		(property "Value" "FAN3278"
			(at -2.54 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FAN3278-D.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "8-27V PMOS-NMOS Bridge Driver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Driver MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FAN7388"
		(extends "FAN7888")
		(property "Reference" "U"
			(at -2.54 24.13 0)
		)
		(property "Value" "FAN7388"
			(at -2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 1.27 -19.05 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FAN7388-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "3 Half-Bridge Gate-Drive IC, 600V operation, Output Current 350/650mA, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "3 Phase Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FL5160MX"
		(extends "FL5150MX")
		(property "Reference" "U"
			(at 5.08 -12.7 0)
		)
		(property "Value" "FL5160MX"
			(at 7.62 -15.24 0)
		)
		(property "Footprint" "Package_SO:SSOP-10_3.9x4.9mm_P1.00mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FL5150-D.pdf"
			(at -2.54 -2.54 0)
		)
		(property "Description" "IGBT and MOSFET, AC Phase Cut, Dimmer Controller, SSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "dimmer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP?10?3.9x4.9mm*1.00mm*"
			(at 0 0 0)
		)
	)
	(symbol "HIP2101_DFN"
		(extends "HIP2100_DFN")
		(property "Reference" "U"
			(at 0 13.335 0)
		)
		(property "Value" "HIP2101_DFN"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-12-1EP_4x4mm_P0.5mm_EP2.66x3.38mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/hip2/hip2101.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "High Frequency Half Bridge Driver, TTL/CMOS inputs, Output Current 2.0A, 100V, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "HIP2101_EPSOIC"
		(extends "HIP2100_EPSOIC")
		(property "Reference" "U"
			(at 0 13.335 0)
		)
		(property "Value" "HIP2101_EPSOIC"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.514x3.2mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/hip2/hip2101.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "High Frequency Half Bridge Driver, TTL/CMOS inputs, Output Current 2.0A, 100V, EPSOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HIP2101_QFN"
		(extends "HIP2100_QFN")
		(property "Reference" "U"
			(at 0 13.335 0)
		)
		(property "Value" "HIP2101_QFN"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_5x5mm_P0.8mm_EP2.7x2.7mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/hip2/hip2101.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "High Frequency Half Bridge Driver, TTL/CMOS inputs, Output Current 2.0A, 100V, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "HIP2101_SOIC"
		(extends "HIP2100_SOIC")
		(property "Reference" "U"
			(at 0 13.335 0)
		)
		(property "Value" "HIP2101_SOIC"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/hip2/hip2101.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "High Frequency Half Bridge Driver, TTL/CMOS inputs, Output Current 2.0A, 100V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2106"
		(extends "IR2101")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2106"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2106.pdf?fileId=5546d462533600a4015355c7cfc51673"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 200/350mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2108"
		(extends "IR2103")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2108"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2108.pdf?fileId=5546d462533600a4015355c7dc321676"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 210/350mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2109"
		(extends "IR2104")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2109"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2109.pdf?fileId=5546d462533600a4015355c7e85b1679"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 200/350mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2110"
		(extends "IR2010")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2110"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2110.pdf?fileId=5546d462533600a4015355c80333167e"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 500V, 2.0/2.0A, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2110S"
		(extends "IR2010S")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2110S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2110.pdf?fileId=5546d462533600a4015355c80333167e"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 500V, 2.0/2.0A, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2112"
		(extends "IR2010")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2112"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2112.pdf?fileId=5546d462533600a4015355c81cb71685"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 250/500mA, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2112S"
		(extends "IR2010S")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2112S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2112.pdf?fileId=5546d462533600a4015355c81cb71685"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 500V, 250/500mA, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2113"
		(extends "IR2010")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2113"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2110.pdf?fileId=5546d462533600a4015355c80333167e"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 2.0/2.0A, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2113S"
		(extends "IR2010S")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2113S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2110.pdf?fileId=5546d462533600a4015355c80333167e"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 500V, 2.0/2.0A, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2135"
		(extends "IR2133")
		(property "Reference" "U"
			(at -7.62 22.86 0)
		)
		(property "Value" "IR2135"
			(at 7.62 22.86 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IR2x33-IR2x35-DataSheet-v01_00-EN.pdf?fileId=5546d462533600a4015355c890ba169f"
			(at 0 0 0)
		)
		(property "Description" "600V, Vout 12-20V, PDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "3 Phase Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2135S"
		(extends "IR2133S")
		(property "Reference" "U"
			(at -7.62 22.86 0)
		)
		(property "Value" "IR2135S"
			(at 7.62 22.86 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IR2x33-IR2x35-DataSheet-v01_00-EN.pdf?fileId=5546d462533600a4015355c890ba169f"
			(at 0 0 0)
		)
		(property "Description" "600V, Vout 12-20V, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "3 Phase Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR21531"
		(extends "IR2153")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR21531"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir21531.pdf?fileId=5546d462533600a4015355c8d26316b3"
			(at 0 0 0)
		)
		(property "Description" "Self-Oscillating Half-Bridge Driver, 600V, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Oscillating Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2155"
		(extends "IR2153")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2155"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2155.pdf?fileId=5546d462533600a4015355c8dec316b6"
			(at 0 0 0)
		)
		(property "Description" "Self-Oscillating Half-Bridge Driver, 600V, 250/500mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Oscillating Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2213"
		(extends "IR2010")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2213"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IR2213-DS-v00_02-EN.pdf?fileId=5546d462533600a4015355c9621716d8"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 1200V, 1.7/2.0A, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2213S"
		(extends "IR2010S")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2213S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IR2213-DS-v00_02-EN.pdf?fileId=5546d462533600a4015355c9621716d8"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 1200V, 1.7/2.0A, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2214S"
		(extends "IR2114S")
		(property "Reference" "U"
			(at 1.27 18.415 0)
		)
		(property "Value" "IR2214S"
			(at 1.27 16.51 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2114ss.pdf?fileId=5546d462533600a4015355c836cd168a"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Gate Driver IC, 1200V, 1.0/1.5A, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x8.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2233"
		(extends "IR2133")
		(property "Reference" "U"
			(at -7.62 22.86 0)
		)
		(property "Value" "IR2233"
			(at 7.62 22.86 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IR2x33-IR2x35-DataSheet-v01_00-EN.pdf?fileId=5546d462533600a4015355c890ba169f"
			(at 0 0 0)
		)
		(property "Description" "1200V, Vout 10-20V, PDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "3 Phase Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2233S"
		(extends "IR2133S")
		(property "Reference" "U"
			(at -7.62 22.86 0)
		)
		(property "Value" "IR2233S"
			(at 7.62 22.86 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IR2x33-IR2x35-DataSheet-v01_00-EN.pdf?fileId=5546d462533600a4015355c890ba169f"
			(at 0 0 0)
		)
		(property "Description" "1200V, Vout 10-20V, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "3 Phase Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2235"
		(extends "IR2133")
		(property "Reference" "U"
			(at -7.62 22.86 0)
		)
		(property "Value" "IR2235"
			(at 7.62 22.86 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IR2x33-IR2x35-DataSheet-v01_00-EN.pdf?fileId=5546d462533600a4015355c890ba169f"
			(at 0 0 0)
		)
		(property "Description" "1200V, Vout 12-20V, PDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "3 Phase Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2235S"
		(extends "IR2133S")
		(property "Reference" "U"
			(at -7.62 22.86 0)
		)
		(property "Value" "IR2235S"
			(at 7.62 22.86 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IR2x33-IR2x35-DataSheet-v01_00-EN.pdf?fileId=5546d462533600a4015355c890ba169f"
			(at 0 0 0)
		)
		(property "Description" "1200V, Vout 12-20V, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "3 Phase Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2301"
		(extends "IR2101")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2301"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2301.pdf?fileId=5546d462533600a4015355c97bb216dc"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 200/350mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2302"
		(extends "IR2104")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2302"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2302.pdf?fileId=5546d462533600a4015355c988b216de"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 200/350mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR2308"
		(extends "IR2101")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR2308"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2308.pdf?fileId=5546d462533600a4015355c9a2b816e2"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 200/350mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR25607S"
		(extends "IR2010S")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR25607S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir25607.pdf?fileId=5546d462533600a4015355ca0e7916f5"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 2.0/2.0A, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IR7106S"
		(extends "IR25604S")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IR7106S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir7106s.pdf?fileId=5546d462533600a4015355d61a06182a"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 700V, 200/350mA, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2001"
		(extends "IR2101")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2001"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2001pbf.pdf?fileId=5546d462533600a401535675a760277e"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 200V, 200/420mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2003"
		(extends "IR2103")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2003"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2003pbf.pdf?fileId=5546d462533600a401535675afec2780"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 200V, 290/600mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2004"
		(extends "IR2104")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2004"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2004pbf.pdf?fileId=5546d462533600a401535675b86b2782"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 200V, 290/600mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2005M"
		(extends "IRS2001M")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2005M"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:Infineon_MLPQ-16-14-1EP_4x4mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IRS2005S-DS-v02_00-EN.pdf?fileId=5546d462533600a4015364c4246229e1"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 200V, 290/600mA, MLPQ-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Infineon*MLPQ*EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2005S"
		(extends "IR25604S")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2005S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IRS2005S-DS-v02_00-EN.pdf?fileId=5546d462533600a4015364c4246229e1"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 200V, 290/600mA, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2008S"
		(extends "IR25602S")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2008S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IRS2008S-DS-v01_00-EN.pdf?fileId=5546d46259d9a4bf015a3e76b6361c1a"
			(at 0 0 0)
		)
		(property "Description" "200-V Half-Bridge Driver With Shutdown Input, 200V, 290/600mA, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2011"
		(extends "IR2011")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2011"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2011pbf.pdf?fileId=5546d462533600a401535675c19f2784"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 200V, 1.0/1.0A, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2101"
		(extends "IR2101")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2101"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir2101.pdf?fileId=5546d462533600a4015355c7a755166c"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 290/600mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2103"
		(extends "IR2103")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2103"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2103.pdf?fileId=5546d462533600a4015356762b71279f"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 290/600mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2104"
		(extends "IR2104")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2104"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2104.pdf?fileId=5546d462533600a40153567633f727a1"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 290/600mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2106"
		(extends "IR2101")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2106"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2106.pdf?fileId=5546d462533600a4015356763aa527a3"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 290/600mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS21064"
		(extends "IR21064")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS21064"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2106.pdf?fileId=5546d462533600a4015356763aa527a3"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 290/600mA, PDIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2108"
		(extends "IR2103")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2108"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2108.pdf?fileId=5546d462533600a40153567649d627a8"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 290/600mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS21084"
		(extends "IR21084")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "IRS21084"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2108.pdf?fileId=5546d462533600a40153567649d627a8"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 290/600mA, PDIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2109"
		(extends "IR2104")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2109"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2109.pdf?fileId=5546d462533600a401535676508f27ab"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 290/600mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS21091"
		(extends "IR21091")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS21091"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs21091.pdf?fileId=5546d462533600a401535676573d27ae"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 290/600mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS21094"
		(extends "IR21094")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "IRS21094"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2109.pdf?fileId=5546d462533600a401535676508f27ab"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 290/600mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2110"
		(extends "IR2010")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2110"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2110.pdf?fileId=5546d462533600a40153567660ff27b0"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 500V, 2.0/2.0A, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2110S"
		(extends "IR2010S")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2110S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2110.pdf?fileId=5546d462533600a40153567660ff27b0"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 500V, 2.0/2.0A, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2111"
		(extends "IR2111")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2111"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2111pbf.pdf?fileId=5546d462533600a401535676679b27b3"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 290/600mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2112"
		(extends "IR2010")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2112"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2112pbf.pdf?fileId=5546d462533600a401535676702827b5"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 290/600mA, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2112S"
		(extends "IR2010S")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2112S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2112pbf.pdf?fileId=5546d462533600a401535676702827b5"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 500V, 290/600mA, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2113"
		(extends "IR2010")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2113"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2110.pdf?fileId=5546d462533600a40153567660ff27b0"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 2.0/2.0A, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2113S"
		(extends "IR2010S")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2113S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2110.pdf?fileId=5546d462533600a40153567660ff27b0"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 500V, 2.0/2.0A, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS21531D"
		(extends "IR2153")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS21531D"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2153d.pdf?fileId=5546d462533600a401535676951e27c3"
			(at 0 0 0)
		)
		(property "Description" "Self-Oscillating Half-Bridge Driver IC, 600V, 180/260mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Oscillating Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2153D"
		(extends "IR2153")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2153D"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2153d.pdf?fileId=5546d462533600a401535676951e27c3"
			(at 0 0 0)
		)
		(property "Description" "Self-Oscillating Half-Bridge Driver IC, 600V, 180/260mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Oscillating Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2181"
		(extends "IR2181")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2181"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2181.pdf?fileId=5546d462533600a401535676c12b27d3"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 1.4/1.8A, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS21814"
		(extends "IR21814")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "IRS21814"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2181.pdf?fileId=5546d462533600a401535676c12b27d3"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 1.4/1.8A, PDIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2183"
		(extends "IR2183")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2183"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2183.pdf?fileId=5546d462533600a401535676d20c27d8"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 1.4/1.8A, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS21834"
		(extends "IR21834")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "IRS21834"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2183.pdf?fileId=5546d462533600a401535676d20c27d8"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 1.4/1.8A, PDIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2184"
		(extends "IR2184")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2184"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2184.pdf?fileId=5546d462533600a401535676d8da27db"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 1.4/1.8A, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS21844"
		(extends "IR21844")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "IRS21844"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2184.pdf?fileId=5546d462533600a401535676d8da27db"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 1.4/1.8A, PDIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2186"
		(extends "IR2181")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2186"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2186pbf.pdf?fileId=5546d462533600a40153567716c427ed"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 4A, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "gate driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS21864"
		(extends "IR21814")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "IRS21864"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2186pbf.pdf?fileId=5546d462533600a40153567716c427ed"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 4A, PDIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "gate driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS21867S"
		(extends "IR25604S")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS21867S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/irs21867spbf.pdf?fileId=5546d462533600a4015356770e8327eb"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 4.0/4.0A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2301S"
		(extends "IR25604S")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2301S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2301pbf.pdf?fileId=5546d462533600a40153567a7ec527fe"
			(at 0 0 0)
		)
		(property "Description" "High and Low Side Driver, 600V, 200/350mA, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2302S"
		(extends "IR25602S")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2302S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IRS2302-DS-v02_01-EN.pdf?fileId=5546d462533600a40153567a87382800"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 200/350mA, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2304"
		(extends "IR2304")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2304"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2304spbf.pdf?fileId=5546d462533600a40153567a8fe72802"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 290/600mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS2308"
		(extends "IR2101")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS2308"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/irs2308.pdf?fileId=5546d462533600a40153567a98ac2804"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 290/600mA, PDIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "IRS25606S"
		(extends "IR25604S")
		(property "Reference" "U"
			(at 1.27 13.335 0)
		)
		(property "Value" "IRS25606S"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/ir25606.pdf?fileId=5546d462533600a4015355ca002316f3"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Driver, 600V, 200/350mA, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ITS711L1"
		(extends "ITS724G")
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "ITS711L1"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-ITS711L1-DS-v01_03-en.pdf?fileId=db3a30432239cccd0122e560bae03c62"
			(at 0 0 0)
		)
		(property "Description" "Smart High-Side Power Switch for Industrial Applications, Four Channels, Rds 200mΩ, SOIC-20W"
			(at 0 0 0)
		)
		(property "ki_keywords" "driver fet quad"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ITS716G"
		(extends "ITS724G")
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "ITS716G"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-ITS716G-DS-v01_01-en.pdf?fileId=db3a304412b407950112b428c2cf3e6d"
			(at 0 0 0)
		)
		(property "Description" "Smart High-Side Power Switch for Industrial Applications, Four Channels, Rds 140mΩ, SOIC-20W"
			(at 0 0 0)
		)
		(property "ki_keywords" "driver fet quad"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM5109AMA"
		(extends "LM5109MA")
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "LM5109AMA"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5109a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Gate Driver, Output Current 1.0A, 100V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half-Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM5109BMA"
		(extends "LM5109MA")
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "LM5109BMA"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5109b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Gate Driver, Output Current 1.0A, 100V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half-Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM5109BSD"
		(extends "LM5109ASD")
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "LM5109BSD"
			(at 0 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_4x4mm_P0.8mm_EP2.6x3mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm5109b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Half-Bridge Gate Driver, Output Current 1.0A, 100V, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half-Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC4440IMS8"
		(extends "LTC4440EMS8")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LTC4440IMS8"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4440fb.pdf"
			(at -2.54 11.43 0)
		)
		(property "Description" "High-side, N-Channel, Mosfet driver, 80V input, -40°C to +125°C, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "high-side mosfet-driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC4440IS6"
		(extends "LTC4440ES6")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LTC4440IS6"
			(at -1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4440fb.pdf"
			(at -2.54 11.43 0)
		)
		(property "Description" "High-side, N-Channel, Mosfet driver, 80V input, -40°C to +85°C, SOT23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "high-side mosfet-driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MAX15013AxSA"
		(extends "MAX15012AxSA")
		(property "Reference" "U"
			(at 2.54 13.335 0)
		)
		(property "Value" "MAX15013AxSA"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX15012-MAX15013B.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "High Frequency Half Bridge Driver, Output Current 2.0A, 175V, TTL Input, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX15013BxSA"
		(extends "MAX15012BxSA")
		(property "Reference" "U"
			(at 2.54 13.335 0)
		)
		(property "Value" "MAX15013BxSA"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX15012-MAX15013B.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "High Frequency Half Bridge Driver, Output Current 2.0A, 175V, TTL Input, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX15013CxSA"
		(extends "MAX15012CxSA")
		(property "Reference" "U"
			(at 2.54 13.335 0)
		)
		(property "Value" "MAX15013CxSA"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.514x3.2mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX15012-MAX15013B.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "High Frequency Half Bridge Driver, Output Current 2.0A, 175V, TTL Input, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX15013DxSA"
		(extends "MAX15012DxSA")
		(property "Reference" "U"
			(at 2.54 13.335 0)
		)
		(property "Value" "MAX15013DxSA"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.514x3.2mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX15012-MAX15013B.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "High Frequency Half Bridge Driver, Output Current 2.0A, 175V, TTL Input, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half Bridge Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC33152"
		(extends "EL7202CN")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MC33152"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC34152-D.PDF"
			(at 0 -7.62 0)
		)
		(property "Description" "High Speed Dual MOSFET Drivers, 1.5A, -40 to 125C, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Driver, Dual MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC34152"
		(extends "EL7202CN")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MC34152"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC34152-D.PDF"
			(at 0 -7.62 0)
		)
		(property "Description" "High Speed Dual MOSFET Drivers, 1.5A, 0 to 70C, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Driver, Dual MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP14A1201xMNY"
		(extends "MCP14A0901xMNY")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "MCP14A1201xMNY"
			(at 2.54 7.62 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.4mm"
			(at 0 19.05 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP14A1201-Family-Data-Sheet-DS20006228A.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Dual 12A-Peak MOSFET Driver, inverting outputs, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Driver, Dual MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP14A1202xMNY"
		(extends "MCP14A0902xMNY")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MCP14A1202xMNY"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.4mm"
			(at 0 19.05 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP14A1201-Family-Data-Sheet-DS20006228A.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "Dual 12A-Peak MOSFET Driver, non-inverting outputs, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Driver, Dual MOSFET"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "UCC21520ADW"
		(extends "UCC21520DW")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "UCC21520ADW"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ucc21520.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Isolated Dual-Channel Gate Driver, Output Current 4.0/6.0A, 5.7kV Isolation, 5V UVLO, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Isolated Gate Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ZXGD3002E6"
		(extends "ZXGD3001E6")
		(property "Reference" "U"
			(at -8.89 6.35 0)
		)
		(property "Value" "ZXGD3002E6"
			(at 10.16 -7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ZXGD3002E6.pdf"
			(at -8.89 6.35 0)
		)
		(property "Description" "9A (peak) Gate driver, 20V, 2ns delay, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "gate driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZXGD3003E6"
		(extends "ZXGD3001E6")
		(property "Reference" "U"
			(at -8.89 6.35 0)
		)
		(property "Value" "ZXGD3003E6"
			(at 10.16 -7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ZXGD3003E6.pdf"
			(at -8.89 6.35 0)
		)
		(property "Description" "5A (peak) Gate driver, 40V, 2ns delay, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "gate driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ZXGD3004E6"
		(extends "ZXGD3001E6")
		(property "Reference" "U"
			(at -8.89 6.35 0)
		)
		(property "Value" "ZXGD3004E6"
			(at 10.16 -7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.diodes.com/_files/datasheets/ZXGD3004E6.pdf"
			(at -8.89 6.35 0)
		)
		(property "Description" "8A (peak) Gate driver, 40V, 1ns delay, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "gate driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
)
