(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "DRV2510-Q1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 -13.97 0)
		)
		(property "Value" "DRV2510-Q1"
			(at 1.27 -16.51 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask3x3mm_ThermalVias"
			(at 1.27 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv2510-q1.pdf"
			(at 1.27 -19.05 0)
		)
		(property "Description" "Haptic driver for solenoids and voice coils, up to 3A output, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "driver haptic solenoid coil"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*1EP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DRV2510-Q1_0_0"
			(pin open_collector line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "INTZ")
				(number "14")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "EN")
				(number "2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "STDBY")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "IN+")
				(number "6")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "IN-")
				(number "7")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "BSTP")
				(number "13")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT+")
				(number "12")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT-")
				(number "11")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "BSTN")
				(number "10")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "REG")
				(number "3")
			)
		)
		(symbol "DRV2510-Q1_0_1")
		(embedded_fonts no)
	)
	(symbol "DRV2605LDGS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.255 0)
		)
		(property "Value" "DRV2605LDGS"
			(at 2.54 -8.89 0)
		)
		(property "Footprint" "Package_SO:VSSOP-10_3x3mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv2605l.pdf"
			(at 0 0 0)
		)
		(property "Description" "Haptic driver for LRAs and ERMs with effect library, 2-5.2V, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "haptic driver i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "DRV2605LDGS_0_1")
		(symbol "DRV2605LDGS_1_1"
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN/TRIG")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD/NC")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT+")
				(number "7")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT-")
				(number "9")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "REG")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
)
