(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AL8860MP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "AL8860MP"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.5x1.8mm"
			(at 6.35 8.89 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AL8860.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V 1.5A Constant Current Buck LED Driver IC, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver Buck Constant Current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AL8860MP_0_1")
		(symbol "AL8860MP_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CTRL")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SET")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SW")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AL8860WT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "AL8860WT"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AL8860.pdf"
			(at 0 0 0)
		)
		(property "Description" "40V 1.5A Constant Current Buck LED Driver IC, TSOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver Buck Constant Current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "AL8860WT_0_1")
		(symbol "AL8860WT_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CTRL")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SET")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP3019AKTR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AP3019AKTR"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at -16.002 -28.448 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP3019A.pdf"
			(at 1.016 -23.114 0)
		)
		(property "Description" "1.2MHz White LED Boost Drivers with Built-in Schottky, 2.5..16Vin, <30Vout, SOT-23-6"
			(at 3.81 -25.654 0)
		)
		(property "ki_keywords" "Switching driver backlight"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "AP3019AKTR_0_1")
		(symbol "AP3019AKTR_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CTRL")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{IN}")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BCR430UW6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 6.35 0)
		)
		(property "Value" "BCR430UW6"
			(at -7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SC-74-6_1.55x2.9mm_P0.95mm"
			(at 1.905 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/BCR430UW6.pdf"
			(at 1.905 -8.89 0)
		)
		(property "Description" "100 mA adjustable constant current driver (linear), max 42V, SOT26 (SC-74)"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED driver constant current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SC?74*"
			(at 0 0 0)
		)
		(symbol "BCR430UW6_0_1")
		(symbol "BCR430UW6_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "REXT")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VS")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH455G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 4.064 21.59 0)
		)
		(property "Value" "CH455G"
			(at 4.318 19.05 0)
		)
		(property "Footprint" "Package_SO:SOP-16_3.9x9.9mm_P1.27mm"
			(at 0 0.254 0)
		)
		(property "Datasheet" "https://www.wch-ic.com/products/CH455.html"
			(at 0 0 0)
		)
		(property "Description" "Digital tube driver and keyboard scan (common cathode only), SOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "WCH Nixie I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*-16*"
			(at 0 0 0)
		)
		(symbol "CH455G_0_0"
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin tri_state line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "SEG0")
				(number "12")
			)
			(pin tri_state line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "SEG1")
				(number "13")
			)
			(pin tri_state line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SEG2")
				(number "15")
			)
			(pin tri_state line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SEG3")
				(number "16")
			)
			(pin tri_state line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SEG4")
				(number "1")
			)
			(pin tri_state line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SEG5")
				(number "2")
			)
			(pin tri_state line
				(at 10.16 0 180)
				(length 2.54)
				(name "SEG6")
				(number "3")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SEG7")
				(number "4")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "DIG0")
				(number "5")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "DIG1")
				(number "9")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "DIG2")
				(number "10")
			)
			(pin output line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "DIG3")
				(number "11")
			)
		)
		(symbol "CH455G_1_1")
		(embedded_fonts no)
	)
	(symbol "CH455K"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 21.844 0)
		)
		(property "Value" "CH455K"
			(at 5.334 19.304 0)
		)
		(property "Footprint" "Package_DIP:DIP-18_W7.62mm"
			(at 0.508 -2.54 0)
		)
		(property "Datasheet" "https://www.wch-ic.com/products/CH455.html"
			(at 0.762 0 0)
		)
		(property "Description" "Digital tube driver and keyboard scan (common cathode only), with interrupt/current setting, DIP-18"
			(at 0.254 0 0)
		)
		(property "ki_keywords" "WCH Nixie I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP-18*"
			(at 0 0 0)
		)
		(symbol "CH455K_0_0"
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "SDA")
				(number "3")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "11")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin tri_state line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "SEG0")
				(number "9")
			)
			(pin tri_state line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "SEG1")
				(number "10")
			)
			(pin tri_state line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SEG2")
				(number "12")
			)
			(pin tri_state line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SEG3")
				(number "13")
			)
			(pin tri_state line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SEG4")
				(number "14")
			)
			(pin tri_state line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SEG5")
				(number "15")
			)
			(pin tri_state line
				(at 10.16 0 180)
				(length 2.54)
				(name "SEG6")
				(number "16")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SEG7")
				(number "17")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "DIG0")
				(number "1")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "DIG1")
				(number "5")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "DIG2")
				(number "6")
			)
			(pin output line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "DIG3")
				(number "7")
			)
		)
		(symbol "CH455K_1_0"
			(pin output line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{INT}")
				(number "18")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "ISET")
				(number "8")
			)
		)
		(symbol "CH455K_1_1")
		(embedded_fonts no)
	)
	(symbol "CL220K4-G"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "CL220K4-G"
			(at 3.81 1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TO-252-2"
			(at 3.81 -1.27 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005413A.pdf"
			(at 0.254 0 0)
		)
		(property "Description" "Temperature Compensated Constant Current LED IC, D-PAK"
			(at 0 0 0)
		)
		(property "ki_keywords" "Constant Current LED Driver IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?252*"
			(at 0 0 0)
		)
		(symbol "CL220K4-G_0_1")
		(symbol "CL220K4-G_1_1"
			(pin input line
				(at 0 5.08 270)
				(length 2.54)
				(name "VA")
				(number "1")
			)
			(pin no_connect line
				(at 0 -2.54 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "VB")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CL220N5-G"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.81 0)
		)
		(property "Value" "CL220N5-G"
			(at 3.81 1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 3.81 -1.27 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005413A.pdf"
			(at 0 0 0)
		)
		(property "Description" "Temperature Compensated Constant Current LED IC, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Constant Current LED Driver IC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "CL220N5-G_0_1")
		(symbol "CL220N5-G_1_1"
			(pin input line
				(at 0 5.08 270)
				(length 2.54)
				(name "VA")
				(number "1")
			)
			(pin input line
				(at 0 -5.08 90)
				(length 2.54)
				(name "VB")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIO5661CD6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 10.16 0)
		)
		(property "Value" "DIO5661CD6"
			(at 7.62 7.62 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 2.54 7.62 0)
		)
		(property "Datasheet" "http://www.dioo.com/uploads/product/20190311/e6c7f30c0fbe92fbfa6965c8ef1c5b19.pdf"
			(at 2.54 7.62 0)
		)
		(property "Description" "37V Step-up LED driver with PWM, 2.7-5.5Vin, 1.3A Iout max, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED driver single"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DIO5661CD6_0_1")
		(symbol "DIO5661CD6_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin open_collector line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "LX")
				(number "4")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIO5661ST6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 10.16 0)
		)
		(property "Value" "DIO5661ST6"
			(at 7.62 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 2.54 7.62 0)
		)
		(property "Datasheet" "http://www.dioo.com/uploads/product/20190311/e6c7f30c0fbe92fbfa6965c8ef1c5b19.pdf"
			(at 2.54 7.62 0)
		)
		(property "Description" "37V Step-up LED driver with PWM, 2.7-5.5Vin, 1.3A Iout max, SOT23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED driver single"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "DIO5661ST6_0_1")
		(symbol "DIO5661ST6_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "LX")
				(number "1")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIO5661TST6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 10.16 0)
		)
		(property "Value" "DIO5661TST6"
			(at 7.62 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 2.54 7.62 0)
		)
		(property "Datasheet" "http://www.dioo.com/uploads/product/20190311/e6c7f30c0fbe92fbfa6965c8ef1c5b19.pdf"
			(at 2.54 7.62 0)
		)
		(property "Description" "37V Step-up LED driver with PWM, 2.7-5.5Vin, 1.3A Iout max, TSOT23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED driver single"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "DIO5661TST6_0_1")
		(symbol "DIO5661TST6_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "LX")
				(number "1")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HT1632C-52LQFP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 54.61 0)
		)
		(property "Value" "HT1632C-52LQFP"
			(at 11.43 54.61 0)
		)
		(property "Footprint" "Package_QFP:LQFP-52_14x14mm_P1mm"
			(at -5.08 1.27 90)
		)
		(property "Datasheet" "http://www.holtek.com/documents/10179/116711/HT1632Cv170.pdf"
			(at -5.08 1.27 90)
		)
		(property "Description" "LED Matrix Driver, 32×8 or 24×16, 52-LQFP"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Matrix Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P1mm*"
			(at 0 0 0)
		)
		(symbol "HT1632C-52LQFP_0_1")
		(symbol "HT1632C-52LQFP_1_1"
			(pin input line
				(at -17.78 50.8 0)
				(length 5.08)
				(name "~{CS}")
				(number "19")
			)
			(pin input line
				(at -17.78 48.26 0)
				(length 5.08)
				(name "~{WR}")
				(number "17")
			)
			(pin input line
				(at -17.78 45.72 0)
				(length 5.08)
				(name "~{RD}")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 43.18 0)
				(length 5.08)
				(name "DATA")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 5.08)
				(name "OSC")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 5.08)
				(name "SYNC")
				(number "20")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 5.08)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 5.08)
				(name "VDD")
				(number "21")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 5.08)
				(name "VSS")
				(number "14")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "25")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "36")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 5.08)
				(name "VDD")
				(number "38")
			)
			(pin output line
				(at 17.78 50.8 180)
				(length 5.08)
				(name "ROW0")
				(number "13")
			)
			(pin output line
				(at 17.78 48.26 180)
				(length 5.08)
				(name "ROW1")
				(number "12")
			)
			(pin output line
				(at 17.78 45.72 180)
				(length 5.08)
				(name "ROW2")
				(number "11")
			)
			(pin output line
				(at 17.78 43.18 180)
				(length 5.08)
				(name "ROW3")
				(number "10")
			)
			(pin output line
				(at 17.78 40.64 180)
				(length 5.08)
				(name "ROW4")
				(number "9")
			)
			(pin output line
				(at 17.78 38.1 180)
				(length 5.08)
				(name "ROW5")
				(number "8")
			)
			(pin output line
				(at 17.78 35.56 180)
				(length 5.08)
				(name "ROW6")
				(number "6")
			)
			(pin output line
				(at 17.78 33.02 180)
				(length 5.08)
				(name "ROW7")
				(number "5")
			)
			(pin output line
				(at 17.78 30.48 180)
				(length 5.08)
				(name "ROW8")
				(number "4")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 5.08)
				(name "ROW9")
				(number "3")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 5.08)
				(name "ROW10")
				(number "2")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 5.08)
				(name "ROW11")
				(number "1")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "ROW12")
				(number "52")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "ROW13")
				(number "51")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "ROW14")
				(number "50")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "ROW15")
				(number "49")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "ROW16")
				(number "48")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "ROW17")
				(number "47")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "ROW18")
				(number "46")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "ROW19")
				(number "45")
			)
			(pin output line
				(at 17.78 0 180)
				(length 5.08)
				(name "ROW20")
				(number "44")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "ROW21")
				(number "43")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "ROW22")
				(number "42")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "ROW23")
				(number "41")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "ROW24/COM15")
				(number "40")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "ROW25/COM14")
				(number "39")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "ROW26/COM13")
				(number "37")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "ROW27/COM12")
				(number "35")
			)
			(pin output line
				(at 17.78 -22.86 180)
				(length 5.08)
				(name "ROW28/COM11")
				(number "34")
			)
			(pin output line
				(at 17.78 -25.4 180)
				(length 5.08)
				(name "ROW29/COM10")
				(number "33")
			)
			(pin output line
				(at 17.78 -27.94 180)
				(length 5.08)
				(name "ROW30/COM9")
				(number "32")
			)
			(pin output line
				(at 17.78 -30.48 180)
				(length 5.08)
				(name "ROW31/COM8")
				(number "31")
			)
			(pin output line
				(at 17.78 -33.02 180)
				(length 5.08)
				(name "COM7")
				(number "30")
			)
			(pin output line
				(at 17.78 -35.56 180)
				(length 5.08)
				(name "COM6")
				(number "29")
			)
			(pin output line
				(at 17.78 -38.1 180)
				(length 5.08)
				(name "COM5")
				(number "28")
			)
			(pin output line
				(at 17.78 -40.64 180)
				(length 5.08)
				(name "COM4")
				(number "27")
			)
			(pin output line
				(at 17.78 -43.18 180)
				(length 5.08)
				(name "COM3")
				(number "26")
			)
			(pin output line
				(at 17.78 -45.72 180)
				(length 5.08)
				(name "COM2")
				(number "24")
			)
			(pin output line
				(at 17.78 -48.26 180)
				(length 5.08)
				(name "COM1")
				(number "23")
			)
			(pin output line
				(at 17.78 -50.8 180)
				(length 5.08)
				(name "COM0")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HV9921N8-G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "HV9921N8-G"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005311A.pdf"
			(at 0 0 0)
		)
		(property "Description" "3pin Constant Current 20mA LED Driver, SOT89"
			(at 0 0 0)
		)
		(property "ki_keywords" "CC LED Driver High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
		(symbol "HV9921N8-G_0_1")
		(symbol "HV9921N8-G_1_1"
			(pin output line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "D")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HV9925SG-G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "HV9925SG-G"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/hv9925.pdf"
			(at 0 0 0)
		)
		(property "Description" "Programmable Current LED Lamp Driver, SO8 w/Heat Slug"
			(at 0 0 0)
		)
		(property "ki_keywords" "Programmable Current LED Lamp Driver High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HV9925SG-G_0_1")
		(symbol "HV9925SG-G_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PWMD")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "Rs")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_out line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "7")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "D")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HV9930LG-G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "HV9930LG-G"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/hv9930.pdf"
			(at 0 0 0)
		)
		(property "Description" "Boost-Buck LED Lamp Driver, SO8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck-Boost LED Lamp Driver High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HV9930LG-G_0_1")
		(symbol "HV9930LG-G_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "CS1")
				(number "2")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "PWMD")
				(number "5")
			)
			(pin power_out line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "GATE")
				(number "4")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "CS2")
				(number "7")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "REF")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HV9931LG-G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "HV9931LG-G"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/hv9931.pdf"
			(at 0 0 0)
		)
		(property "Description" "PFC Boost-Buck LED Lamp Driver, SO8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck-Boost LED Lamp Driver High Voltage PFC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HV9931LG-G_0_1")
		(symbol "HV9931LG-G_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "CS1")
				(number "2")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "PWMD")
				(number "5")
			)
			(pin power_out line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "GATE")
				(number "4")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "CS2")
				(number "7")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "REF")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HV9961LG-G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "HV9961LG-G"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005588A.pdf"
			(at 0 0 0)
		)
		(property "Description" "Buck LED Lamp Driver Average-Mode Constant Current, 8V-450V, SO8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck LED Lamp Driver High Voltage Average CC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HV9961LG-G_0_1")
		(symbol "HV9961LG-G_1_1"
			(pin power_out line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PWMD")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "LD")
				(number "7")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "RT")
				(number "8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "GATE")
				(number "4")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CS")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HV9961NG-G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "HV9961NG-G"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005588A.pdf"
			(at 0 0 0)
		)
		(property "Description" "Buck LED Lamp Driver Average-Mode Constant Current, 8V-450V, SO16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck LED Lamp Driver High Voltage Average CC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HV9961NG-G_0_1")
		(symbol "HV9961NG-G_1_1"
			(pin power_out line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VDD")
				(number "12")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PWMD")
				(number "9")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "LD")
				(number "13")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "RT")
				(number "14")
			)
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 7.62 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "GATE")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CS")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HV9967BK7-G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "HV9967BK7-G"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/hv9967b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Buck LED Lamp Driver Average-Mode Constant Current, DFN8 (3x3mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck LED Lamp Driver Low Voltage Average CC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "HV9967BK7-G_0_1")
		(symbol "HV9967BK7-G_1_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "PWMD")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "RT")
				(number "6")
			)
			(pin power_out line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Rs")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HV9967BMG-G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "HV9967BMG-G"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/hv9967b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Buck LED Lamp Driver Average-Mode Constant Current, MSOP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Buck LED Lamp Driver Low Voltage Average CC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "HV9967BMG-G_0_1")
		(symbol "HV9967BMG-G_1_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "PWMD")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "RT")
				(number "6")
			)
			(pin power_out line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Rs")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HV9972LG-G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "HV9972LG-G"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.mouser.com/ds/2/268/HV9972-272498-1181261.pdf"
			(at 0 0 0)
		)
		(property "Description" "Isolated LED Lamp Driver Constant Current, SO8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Isolated LED Lamp Driver High Voltage CC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HV9972LG-G_0_1")
		(symbol "HV9972LG-G_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "PWMD")
				(number "4")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "BIAS")
				(number "1")
			)
			(pin power_out line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "GATE")
				(number "7")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "CS")
				(number "5")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VD")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS31FL3216"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 23.495 0)
		)
		(property "Value" "IS31FL3216"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.4mm_EP2.4x2.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/IS31FL3216.pdf"
			(at 0 0 0)
		)
		(property "Description" "16 channel LED controller with audio modulation mode, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "led pwm audio"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "IS31FL3216_0_1")
		(symbol "IS31FL3216_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "SCL")
				(number "23")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "SDA")
				(number "24")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "AD")
				(number "25")
			)
			(pin output line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "~{INTB}")
				(number "21")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "~{SDB}")
				(number "22")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "CLK")
				(number "1")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "C_FILT")
				(number "27")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "R_EXT")
				(number "28")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "26")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin open_collector line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "OUT1")
				(number "3")
			)
			(pin open_collector line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "OUT2")
				(number "4")
			)
			(pin open_collector line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "OUT3")
				(number "5")
			)
			(pin open_collector line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "OUT4")
				(number "6")
			)
			(pin open_collector line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "OUT5")
				(number "8")
			)
			(pin open_collector line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "OUT6")
				(number "9")
			)
			(pin open_collector line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUT7")
				(number "10")
			)
			(pin open_collector line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUT8")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "GPIO9/OUT9")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "GPIO10/OUT10")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "GPIO11/OUT11")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "GPIO12/OUT12")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "GPIO13/OUT13")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "GPIO14/OUT14")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "GPIO15/OUT15")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "GPIO16/OUT16")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS31FL3218-GR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.035 0)
		)
		(property "Value" "IS31FL3218-GR"
			(at 2.54 -24.13 0)
		)
		(property "Footprint" "Package_SO:SOP-24_7.5x15.4mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/31FL3218.pdf"
			(at 0 0 0)
		)
		(property "Description" "18 LED matrix driver with 8-bit PWM, SOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "led matrix pwm"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*7.5x15.4mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "IS31FL3218-GR_0_1")
		(symbol "IS31FL3218-GR_1_1"
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "~{SDB}")
				(number "24")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "R_EXT")
				(number "2")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin open_collector line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "OUT1")
				(number "7")
			)
			(pin open_collector line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "OUT2")
				(number "8")
			)
			(pin open_collector line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "OUT3")
				(number "9")
			)
			(pin open_collector line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "OUT4")
				(number "10")
			)
			(pin open_collector line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "OUT5")
				(number "11")
			)
			(pin open_collector line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUT6")
				(number "12")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT7")
				(number "13")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT8")
				(number "14")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT9")
				(number "15")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT10")
				(number "16")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT11")
				(number "17")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUT12")
				(number "18")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT13")
				(number "19")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "OUT14")
				(number "20")
			)
			(pin open_collector line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "OUT15")
				(number "21")
			)
			(pin open_collector line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "OUT16")
				(number "22")
			)
			(pin open_collector line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "OUT17")
				(number "23")
			)
			(pin open_collector line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "OUT18")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS31FL3218-QF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.035 0)
		)
		(property "Value" "IS31FL3218-QF"
			(at 2.54 -24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/31FL3218.pdf"
			(at 0 0 0)
		)
		(property "Description" "18 LED matrix driver with 8-bit PWM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "led matrix pwm"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "IS31FL3218-QF_0_1")
		(symbol "IS31FL3218-QF_1_1"
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "~{SDB}")
				(number "24")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "R_EXT")
				(number "2")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin open_collector line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "OUT1")
				(number "7")
			)
			(pin open_collector line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "OUT2")
				(number "8")
			)
			(pin open_collector line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "OUT3")
				(number "9")
			)
			(pin open_collector line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "OUT4")
				(number "10")
			)
			(pin open_collector line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "OUT5")
				(number "11")
			)
			(pin open_collector line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUT6")
				(number "12")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT7")
				(number "13")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT8")
				(number "14")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT9")
				(number "15")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT10")
				(number "16")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT11")
				(number "17")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUT12")
				(number "18")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT13")
				(number "19")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "OUT14")
				(number "20")
			)
			(pin open_collector line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "OUT15")
				(number "21")
			)
			(pin open_collector line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "OUT16")
				(number "22")
			)
			(pin open_collector line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "OUT17")
				(number "23")
			)
			(pin open_collector line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "OUT18")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS31FL3236-TQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 46.99 0)
		)
		(property "Value" "IS31FL3236-TQ"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48-1EP_7x7mm_P0.5mm_EP4.11x4.11mm"
			(at 2.54 -49.53 0)
		)
		(property "Datasheet" "https://www.lumissil.com/assets/pdf/core/IS31FL3236_DS.pdf"
			(at 0 -62.23 0)
		)
		(property "Description" "36 LED matrix driver with 8-bit PWM, eTQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "led matrix pwm"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "IS31FL3236-TQ_0_1")
		(symbol "IS31FL3236-TQ_1_1"
			(pin open_collector line
				(at -12.7 43.18 0)
				(length 2.54)
				(name "SDA")
				(number "45")
			)
			(pin input line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "SCL")
				(number "46")
			)
			(pin input line
				(at -12.7 38.1 0)
				(length 2.54)
				(name "AD")
				(number "40")
			)
			(pin input line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "~{SDB}")
				(number "39")
			)
			(pin passive line
				(at -12.7 -45.72 0)
				(length 2.54)
				(name "R_EXT")
				(number "44")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VCC")
				(number "41")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "42")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "49")
			)
			(pin output line
				(at 12.7 43.18 180)
				(length 2.54)
				(name "OUT1")
				(number "47")
			)
			(pin output line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "OUT2")
				(number "48")
			)
			(pin output line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "OUT3")
				(number "1")
			)
			(pin output line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "OUT4")
				(number "2")
			)
			(pin output line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "OUT5")
				(number "3")
			)
			(pin output line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "OUT6")
				(number "5")
			)
			(pin output line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "OUT7")
				(number "6")
			)
			(pin output line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "OUT8")
				(number "7")
			)
			(pin output line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "OUT9")
				(number "8")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "OUT10")
				(number "9")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "OUT11")
				(number "10")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "OUT12")
				(number "11")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "OUT13")
				(number "12")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUT14")
				(number "13")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT15")
				(number "14")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT16")
				(number "15")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT17")
				(number "16")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT18")
				(number "17")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT19")
				(number "20")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUT20")
				(number "21")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT21")
				(number "22")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "OUT22")
				(number "23")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "OUT23")
				(number "24")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "OUT24")
				(number "25")
			)
			(pin output line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "OUT25")
				(number "26")
			)
			(pin output line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "OUT26")
				(number "27")
			)
			(pin output line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "OUT27")
				(number "28")
			)
			(pin output line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "OUT28")
				(number "29")
			)
			(pin output line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "OUT29")
				(number "30")
			)
			(pin output line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "OUT30")
				(number "31")
			)
			(pin output line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "OUT31")
				(number "32")
			)
			(pin output line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "OUT32")
				(number "34")
			)
			(pin output line
				(at 12.7 -38.1 180)
				(length 2.54)
				(name "OUT33")
				(number "35")
			)
			(pin output line
				(at 12.7 -40.64 180)
				(length 2.54)
				(name "OUT34")
				(number "36")
			)
			(pin output line
				(at 12.7 -43.18 180)
				(length 2.54)
				(name "OUT35")
				(number "37")
			)
			(pin output line
				(at 12.7 -45.72 180)
				(length 2.54)
				(name "OUT36")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS31FL3731-QF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.035 0)
		)
		(property "Value" "IS31FL3731-QF"
			(at 2.54 -26.035 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.4mm_EP2.3x2.3mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/31FL3731.pdf"
			(at 0 0 0)
		)
		(property "Description" "9x16 LED matrix driver with 8-bit PWM and breathing, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "led matrix pwm"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "IS31FL3731-QF_0_1")
		(symbol "IS31FL3731-QF_1_1"
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "SDA")
				(number "19")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "SCL")
				(number "20")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "AD")
				(number "18")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "~{SDB}")
				(number "3")
			)
			(pin open_collector line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{INTB}")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "IN")
				(number "17")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "C_FILT")
				(number "16")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "R_EXT")
				(number "6")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "CA1")
				(number "21")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "CA2")
				(number "22")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "CA3")
				(number "23")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "CA4")
				(number "24")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "CA5")
				(number "25")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "CA6")
				(number "26")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "CA7")
				(number "27")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "CA8")
				(number "28")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CA9")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CB1")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CB2")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "CB3")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "CB4")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "CB5")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "CB6")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "CB7")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "CB8")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "CB9")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS31FL3731-SA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.035 0)
		)
		(property "Value" "IS31FL3731-SA"
			(at 2.54 -26.035 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/31FL3731.pdf"
			(at 0 0 0)
		)
		(property "Description" "9x16 LED matrix driver with 8-bit PWM and breathing, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "led matrix pwm"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "IS31FL3731-SA_0_1")
		(symbol "IS31FL3731-SA_1_1"
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "SDA")
				(number "19")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "SCL")
				(number "20")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "AD")
				(number "18")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "~{SDB}")
				(number "3")
			)
			(pin open_collector line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{INTB}")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "IN")
				(number "17")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "C_FILT")
				(number "16")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "R_EXT")
				(number "6")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "CA1")
				(number "21")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "CA2")
				(number "22")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "CA3")
				(number "23")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "CA4")
				(number "24")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "CA5")
				(number "25")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "CA6")
				(number "26")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "CA7")
				(number "27")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "CA8")
				(number "28")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CA9")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CB1")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CB2")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "CB3")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "CB4")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "CB5")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "CB6")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "CB7")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "CB8")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "CB9")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS31FL3733-QF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "IS31FL3733-QF"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_6x6mm_P0.4mm_EP4.2x4.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/IS31FL3733.pdf"
			(at 0 0 0)
		)
		(property "Description" "12x16 LED matrix driver with 8-bit PWM and breathing, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "led matrix pwm"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "IS31FL3733-QF_0_1")
		(symbol "IS31FL3733-QF_1_1"
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "VIO")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "SDA")
				(number "41")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "SCL")
				(number "42")
			)
			(pin open_collector line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "~{INTB}")
				(number "45")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "~{SDB}")
				(number "46")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "IICRST")
				(number "47")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SYNC")
				(number "40")
			)
			(pin passive line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "RSET")
				(number "35")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "ADDR1")
				(number "43")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "ADDR2")
				(number "44")
			)
			(pin no_connect line
				(at -15.24 -33.02 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -15.24 -35.56 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "36")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "AVCC")
				(number "37")
			)
			(pin power_in line
				(at -2.54 -40.64 90)
				(length 2.54)
				(name "AGND")
				(number "34")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "DVCC")
				(number "38")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "GND")
				(number "48")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "PVCC")
				(number "20")
			)
			(pin passive line
				(at 2.54 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "PGND")
				(number "5")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "PVCC")
				(number "29")
			)
			(pin output line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "CS1")
				(number "16")
			)
			(pin output line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "CS2")
				(number "17")
			)
			(pin output line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "CS3")
				(number "18")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "CS4")
				(number "19")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "CS5")
				(number "21")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "CS6")
				(number "22")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "CS7")
				(number "23")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "CS8")
				(number "24")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "CS9")
				(number "25")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "CS10")
				(number "26")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "CS11")
				(number "27")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "CS12")
				(number "28")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "CS13")
				(number "30")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "CS14")
				(number "31")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "CS15")
				(number "32")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "CS16")
				(number "33")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "SW1")
				(number "2")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "SW2")
				(number "3")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "SW3")
				(number "4")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "SW4")
				(number "6")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "SW5")
				(number "7")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "SW6")
				(number "8")
			)
			(pin input line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "SW7")
				(number "9")
			)
			(pin input line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "SW8")
				(number "10")
			)
			(pin input line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "SW9")
				(number "11")
			)
			(pin input line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "SW10")
				(number "13")
			)
			(pin input line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "SW11")
				(number "14")
			)
			(pin input line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "SW12")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS31FL3733-TQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "IS31FL3733-TQ"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48-1EP_7x7mm_P0.5mm_EP5x5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/IS31FL3733.pdf"
			(at 0 0 0)
		)
		(property "Description" "12x16 LED matrix driver with 8-bit PWM and breathing, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "led matrix pwm"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "IS31FL3733-TQ_0_1")
		(symbol "IS31FL3733-TQ_1_1"
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "VIO")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "SDA")
				(number "41")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "SCL")
				(number "42")
			)
			(pin open_collector line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "~{INTB}")
				(number "45")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "~{SDB}")
				(number "46")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "IICRST")
				(number "47")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SYNC")
				(number "40")
			)
			(pin passive line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "RSET")
				(number "35")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "ADDR1")
				(number "43")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "ADDR2")
				(number "44")
			)
			(pin no_connect line
				(at -15.24 -33.02 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -15.24 -35.56 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "36")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "AVCC")
				(number "37")
			)
			(pin power_in line
				(at -2.54 -40.64 90)
				(length 2.54)
				(name "AGND")
				(number "34")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "DVCC")
				(number "38")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "GND")
				(number "48")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "PVCC")
				(number "20")
			)
			(pin passive line
				(at 2.54 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "PGND")
				(number "5")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "PVCC")
				(number "29")
			)
			(pin output line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "CS1")
				(number "16")
			)
			(pin output line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "CS2")
				(number "17")
			)
			(pin output line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "CS3")
				(number "18")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "CS4")
				(number "19")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "CS5")
				(number "21")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "CS6")
				(number "22")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "CS7")
				(number "23")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "CS8")
				(number "24")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "CS9")
				(number "25")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "CS10")
				(number "26")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "CS11")
				(number "27")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "CS12")
				(number "28")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "CS13")
				(number "30")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "CS14")
				(number "31")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "CS15")
				(number "32")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "CS16")
				(number "33")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "SW1")
				(number "2")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "SW2")
				(number "3")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "SW3")
				(number "4")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "SW4")
				(number "6")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "SW5")
				(number "7")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "SW6")
				(number "8")
			)
			(pin input line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "SW7")
				(number "9")
			)
			(pin input line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "SW8")
				(number "10")
			)
			(pin input line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "SW9")
				(number "11")
			)
			(pin input line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "SW10")
				(number "13")
			)
			(pin input line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "SW11")
				(number "14")
			)
			(pin input line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "SW12")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS31FL3736"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 28.575 0)
		)
		(property "Value" "IS31FL3736"
			(at 5.08 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-40-1EP_5x5mm_P0.4mm_EP3.8x3.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/31FL3736.pdf"
			(at 0 0 0)
		)
		(property "Description" "12x8 LED matrix driver with 8-bit PWM and breathing, QFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "led matrix pwm"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "IS31FL3736_0_1")
		(symbol "IS31FL3736_1_1"
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "VIO")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "SDA")
				(number "33")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "SCL")
				(number "34")
			)
			(pin open_collector line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "~{INTB}")
				(number "37")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "~{SDB}")
				(number "38")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "IICRST")
				(number "39")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SYNC")
				(number "32")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "RSET")
				(number "30")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "ADDR1")
				(number "35")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "ADDR2")
				(number "36")
			)
			(pin no_connect line
				(at -12.7 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at -12.7 -25.4 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "29")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "AVCC")
				(number "28")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 2.54)
				(name "AGND")
				(number "26")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "DVCC")
				(number "27")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "40")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "PVCC")
				(number "17")
			)
			(pin passive line
				(at 2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 2.54)
				(name "PGND")
				(number "4")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 2.54)
				(name "PVCC")
				(number "23")
			)
			(pin output line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "CS1")
				(number "15")
			)
			(pin output line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "CS2")
				(number "16")
			)
			(pin output line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "CS3")
				(number "18")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "CS4")
				(number "19")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "CS5")
				(number "21")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "CS6")
				(number "22")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "CS7")
				(number "24")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "CS8")
				(number "25")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "SW1")
				(number "1")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "SW2")
				(number "2")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "SW3")
				(number "3")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "SW4")
				(number "5")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "SW5")
				(number "6")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "SW6")
				(number "7")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "SW7")
				(number "8")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "SW8")
				(number "9")
			)
			(pin input line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "SW9")
				(number "10")
			)
			(pin input line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "SW10")
				(number "12")
			)
			(pin input line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "SW11")
				(number "13")
			)
			(pin input line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "SW12")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS31FL3737"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 33.655 0)
		)
		(property "Value" "IS31FL3737"
			(at 5.08 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-40-1EP_5x5mm_P0.4mm_EP3.8x3.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/31FL3737.pdf"
			(at 0 0 0)
		)
		(property "Description" "12x12 LED matrix driver with 8-bit PWM and breathing, QFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "led matrix pwm"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "IS31FL3737_0_1")
		(symbol "IS31FL3737_1_1"
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "VIO")
				(number "32")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "SDA")
				(number "34")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "SCL")
				(number "35")
			)
			(pin open_collector line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "~{INTB}")
				(number "37")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "~{SDB}")
				(number "38")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "IICRST")
				(number "39")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "SYNC")
				(number "33")
			)
			(pin passive line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "RSET")
				(number "30")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "ADDR")
				(number "36")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 2.54)
				(name "AGND")
				(number "29")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "31")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "40")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "PVCC")
				(number "19")
			)
			(pin passive line
				(at 2.54 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 2.54)
				(name "PGND")
				(number "4")
			)
			(pin power_in line
				(at 5.08 35.56 270)
				(length 2.54)
				(name "PVCC")
				(number "26")
			)
			(pin output line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "CS1")
				(number "15")
			)
			(pin output line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "CS2")
				(number "16")
			)
			(pin output line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "CS3")
				(number "17")
			)
			(pin output line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "CS4")
				(number "18")
			)
			(pin output line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "CS5")
				(number "20")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "CS6")
				(number "21")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "CS7")
				(number "22")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "CS8")
				(number "23")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "CS9")
				(number "24")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "CS10")
				(number "25")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "CS11")
				(number "27")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "CS12")
				(number "28")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "SW1")
				(number "1")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "SW2")
				(number "2")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "SW3")
				(number "3")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "SW4")
				(number "5")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "SW5")
				(number "6")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "SW6")
				(number "7")
			)
			(pin input line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "SW7")
				(number "8")
			)
			(pin input line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "SW8")
				(number "9")
			)
			(pin input line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "SW9")
				(number "10")
			)
			(pin input line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "SW10")
				(number "12")
			)
			(pin input line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "SW11")
				(number "13")
			)
			(pin input line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "SW12")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS31LT3360"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "IS31LT3360"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-5"
			(at 1.27 -3.81 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/31LT3360.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "Constant current  LED driver, internal switch, up to 40V/1.2A, SOT-89-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switching LED driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
		(symbol "IS31LT3360_0_1")
		(symbol "IS31LT3360_1_1"
			(pin power_in line
				(at -8.89 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin input line
				(at -8.89 0 0)
				(length 2.54)
				(name "ADJ")
				(number "3")
			)
			(pin power_in line
				(at 0 -5.08 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "ISENSE")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "LX")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KTD2026"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.604 8.636 0)
		)
		(property "Value" "KTD2026"
			(at -6.985 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_1.5x1.5mm_P0.4mm_EP0.7x1.2mm"
			(at 0.635 -23.495 0)
		)
		(property "Datasheet" "https://www.kinet-ic.com/uploads/KTD2026-7-04h.pdf"
			(at -1.905 -28.575 0)
		)
		(property "Description" "4-channel constant-current linear LED Driver, I2C interface, 0.125..24mAout, VIN 2.7..5.5V, DFN-8"
			(at 0.635 -26.035 0)
		)
		(property "ki_keywords" "kinetic cc sink RGB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1.5x1.5mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "KTD2026_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at -7.62 0 0)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "D1")
				(number "4")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "D2")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "D3")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "ST")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KTD2027"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.604 8.636 0)
		)
		(property "Value" "KTD2027"
			(at -6.985 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_1.5x1.5mm_P0.4mm_EP0.7x1.2mm"
			(at 0.635 -23.495 0)
		)
		(property "Datasheet" "https://www.kinet-ic.com/uploads/KTD2026-7-04h.pdf"
			(at -1.905 -28.575 0)
		)
		(property "Description" "4-channel constant-current linear LED Driver, I2C interface, 0.125..24mAout, VIN 2.7..5.5V DFN-8"
			(at 0.635 -26.035 0)
		)
		(property "ki_keywords" "kinetic cc sink RGB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1.5x1.5mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "KTD2027_1_1"
			(pin bidirectional line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at -7.62 0 0)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "D1")
				(number "4")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "D2")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "D3")
				(number "2")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "D4")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KTD2061xxUAC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.652 21.844 0)
		)
		(property "Value" "KTD2061xxUAC"
			(at 4.064 21.844 0)
		)
		(property "Footprint" "Package_DFN_QFN:UQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm_ThermalVias"
			(at 2.54 -35.56 0)
		)
		(property "Datasheet" "https://www.kinet-ic.com/uploads/web/KTD2058,%20KTD2059,%20KTD2060,%20KTD2061/KTD2061-58-59-60-04e.pdf"
			(at -2.54 -30.226 0)
		)
		(property "Description" "36-channel (12xRGB) LED driver with I²C Control, VCC = VIN = 2.5..5.5V, 23kHz MUX frequency, UQFN-20"
			(at 1.27 -32.766 0)
		)
		(property "ki_keywords" "KTD2058Q KTD2059Q KTD2060Q KTD2061Q I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*UQFN*3x3mm*P0.4mm*EP1.7x1.7mm*"
			(at 0 0 0)
		)
		(symbol "KTD2061xxUAC_0_1")
		(symbol "KTD2061xxUAC_1_1"
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SCL")
				(number "4")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin passive line
				(at 0 22.86 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "2")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "LEDA1")
				(number "6")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "LEDA2")
				(number "7")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "LEDA3")
				(number "9")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "LEDA4")
				(number "10")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "LEDB1")
				(number "11")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "LEDB2")
				(number "12")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "LEDB3")
				(number "14")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "LEDB4")
				(number "15")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "LEDC1")
				(number "16")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "LEDC2")
				(number "17")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "LEDC3")
				(number "19")
			)
			(pin output line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "LEDC4")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LED1642GWPTR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "LED1642GWPTR"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:QSOP-24_3.9x8.7mm_P0.635mm"
			(at 0.635 -24.765 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/led1642gw.pdf"
			(at -10.16 17.78 0)
		)
		(property "Description" "16-channel LED driver with error detection, current gain control and 12/16 bit PWM brightness control, QSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "PWM LED driver error detection brightness QSOP-24"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "LED1642GWPTR_0_1")
		(symbol "LED1642GWPTR_1_1"
			(pin output line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "SDO")
				(number "22")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "SDI")
				(number "2")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "CLK")
				(number "3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "LE")
				(number "4")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "PWCLK")
				(number "21")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "R-EXT")
				(number "23")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "OUT0")
				(number "5")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "OUT1")
				(number "6")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "OUT2")
				(number "7")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "OUT3")
				(number "8")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "OUT4")
				(number "9")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUT5")
				(number "10")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUT6")
				(number "11")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUT7")
				(number "12")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUT8")
				(number "13")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OUT9")
				(number "14")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "OUT10")
				(number "15")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "OUT11")
				(number "16")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "OUT12")
				(number "17")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "OUT13")
				(number "18")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "OUT14")
				(number "19")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "OUT15")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LED1642GWQTR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "LED1642GWQTR"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.15x2.15mm"
			(at 0.635 -24.765 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/led1642gw.pdf"
			(at -10.16 17.78 0)
		)
		(property "Description" "16-channel LED driver with error detection, current gain control and 12/16 bit PWM brightness control, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "PWM LED driver error detection brightness QFN-24"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LED1642GWQTR_0_1")
		(symbol "LED1642GWQTR_1_1"
			(pin output line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "SDO")
				(number "19")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "SDI")
				(number "23")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "CLK")
				(number "24")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "LE")
				(number "1")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "PWCLK")
				(number "18")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "R-EXT")
				(number "20")
			)
			(pin passive line
				(at -5.08 -25.4 90)
				(length 2.54)
				(name "EP")
				(number "25")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "21")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "OUT0")
				(number "2")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "OUT1")
				(number "3")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "OUT2")
				(number "4")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "OUT3")
				(number "5")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "OUT4")
				(number "6")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUT5")
				(number "7")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUT6")
				(number "8")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUT7")
				(number "9")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUT8")
				(number "10")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OUT9")
				(number "11")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "OUT10")
				(number "12")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "OUT11")
				(number "13")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "OUT12")
				(number "14")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "OUT13")
				(number "15")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "OUT14")
				(number "16")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "OUT15")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LED1642GWTTR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "LED1642GWTTR"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 0.635 -24.765 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/led1642gw.pdf"
			(at -10.16 17.78 0)
		)
		(property "Description" "16-channel LED driver with error detection, current gain control and 12/16 bit PWM brightness control, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "PWM LED driver error detection brightness TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LED1642GWTTR_0_1")
		(symbol "LED1642GWTTR_1_1"
			(pin output line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "SDO")
				(number "22")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "SDI")
				(number "2")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "CLK")
				(number "3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "LE")
				(number "4")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "PWCLK")
				(number "21")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "R-EXT")
				(number "23")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "OUT0")
				(number "5")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "OUT1")
				(number "6")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "OUT2")
				(number "7")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "OUT3")
				(number "8")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "OUT4")
				(number "9")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUT5")
				(number "10")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUT6")
				(number "11")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUT7")
				(number "12")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUT8")
				(number "13")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OUT9")
				(number "14")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "OUT10")
				(number "15")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "OUT11")
				(number "16")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "OUT12")
				(number "17")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "OUT13")
				(number "18")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "OUT14")
				(number "19")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "OUT15")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LED1642GWXTTR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "LED1642GWXTTR"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.2x5mm"
			(at 0.635 -24.765 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/led1642gw.pdf"
			(at -10.16 17.78 0)
		)
		(property "Description" "16-channel LED driver with error detection, current gain control and 12/16 bit PWM brightness control, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "PWM LED driver error detection brightness TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*1EP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LED1642GWXTTR_0_1")
		(symbol "LED1642GWXTTR_1_1"
			(pin output line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "SDO")
				(number "22")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "SDI")
				(number "2")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "CLK")
				(number "3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "LE")
				(number "4")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "PWCLK")
				(number "21")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "R-EXT")
				(number "23")
			)
			(pin passive line
				(at -5.08 -25.4 90)
				(length 2.54)
				(name "EP")
				(number "25")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "OUT0")
				(number "5")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "OUT1")
				(number "6")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "OUT2")
				(number "7")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "OUT3")
				(number "8")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "OUT4")
				(number "9")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUT5")
				(number "10")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUT6")
				(number "11")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUT7")
				(number "12")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUT8")
				(number "13")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OUT9")
				(number "14")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "OUT10")
				(number "15")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "OUT11")
				(number "16")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "OUT12")
				(number "17")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "OUT13")
				(number "18")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "OUT14")
				(number "19")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "OUT15")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LED5000"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LED5000"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SO:HSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.1mm"
			(at 6.35 -8.89 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/led5000.pdf"
			(at -2.54 -8.89 0)
		)
		(property "Description" "3A monolithic step-down current source with dimming, HSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED buck driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HSOP*1EP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LED5000_1_0"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DIM")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "INH")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "COMP")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "BOOT")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "SW")
				(number "8")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(symbol "LED5000_1_1")
		(embedded_fonts no)
	)
	(symbol "LM3914N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 14.224 0)
		)
		(property "Value" "LM3914N"
			(at 5.588 14.224 0)
		)
		(property "Footprint" "Package_DIP:DIP-18_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm3914.pdf"
			(at 0 0 0)
		)
		(property "Description" "10 LED Dot/Bar Display Driver, DIP-18"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED driver bar dot"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LM3914N_0_1")
		(symbol "LM3914N_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SIG")
				(number "5")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RHI")
				(number "6")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "RLO")
				(number "4")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "REFOUT")
				(number "7")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "REFADJ")
				(number "8")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "MODE")
				(number "9")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V+")
				(number "3")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "V-")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "LED1")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "LED2")
				(number "18")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "LED3")
				(number "17")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "LED4")
				(number "16")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "LED5")
				(number "15")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "LED6")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "LED7")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "LED8")
				(number "12")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "LED9")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "LED10")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM3914V"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "LM3914V"
			(at 5.08 13.97 0)
		)
		(property "Footprint" "Package_LCC:PLCC-20"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm3914.pdf"
			(at 0 0 0)
		)
		(property "Description" "10 LED Dot/Bar Display Driver, PLCC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED driver bar dot"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC*"
			(at 0 0 0)
		)
		(symbol "LM3914V_0_1")
		(symbol "LM3914V_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SIG")
				(number "5")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RHI")
				(number "6")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "RLO")
				(number "4")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "REFOUT")
				(number "8")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "REFADJ")
				(number "10")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "MODE")
				(number "11")
			)
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V+")
				(number "3")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "V-")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "LED1")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "LED2")
				(number "20")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "LED3")
				(number "19")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "LED4")
				(number "18")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "LED5")
				(number "17")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "LED6")
				(number "16")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "LED7")
				(number "15")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "LED8")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "LED9")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "LED10")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP5036"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 49.53 0)
		)
		(property "Value" "LP5036"
			(at 6.35 49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-46-1EP_5x6mm_P0.4mm_EP2.8x3.8mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lp5036.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "36-Channel 12-Bit PWM Ultra-low Quiescent Current I2C RGB LED Driver"
			(at 0 0 0)
		)
		(property "ki_keywords" "PWM LED driver I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN?46?1EP?5x6mm?P0.4mm?EP2.8x3.8mm*"
			(at 0 0 0)
		)
		(symbol "LP5036_0_1")
		(symbol "LP5036_1_1"
			(pin input line
				(at -12.7 45.72 0)
				(length 2.54)
				(name "EN")
				(number "43")
			)
			(pin input line
				(at -12.7 43.18 0)
				(length 2.54)
				(name "SCL")
				(number "42")
			)
			(pin bidirectional line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "SDA")
				(number "41")
			)
			(pin input line
				(at -12.7 38.1 0)
				(length 2.54)
				(name "ADDR0")
				(number "38")
			)
			(pin input line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "ADDR1")
				(number "39")
			)
			(pin passive line
				(at -12.7 -40.64 0)
				(length 2.54)
				(name "VCAP")
				(number "45")
			)
			(pin passive line
				(at -12.7 -43.18 0)
				(length 2.54)
				(name "IREF")
				(number "44")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "37")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "46")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "47")
			)
			(pin power_out line
				(at 12.7 45.72 180)
				(length 2.54)
				(name "OUT0")
				(number "1")
			)
			(pin power_out line
				(at 12.7 43.18 180)
				(length 2.54)
				(name "OUT1")
				(number "2")
			)
			(pin power_out line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "OUT2")
				(number "3")
			)
			(pin power_out line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "OUT3")
				(number "4")
			)
			(pin power_out line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "OUT4")
				(number "5")
			)
			(pin power_out line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "OUT5")
				(number "6")
			)
			(pin power_out line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "OUT6")
				(number "7")
			)
			(pin power_out line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "OUT7")
				(number "8")
			)
			(pin power_out line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "OUT8")
				(number "9")
			)
			(pin power_out line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "OUT9")
				(number "10")
			)
			(pin power_out line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "OUT10")
				(number "11")
			)
			(pin power_out line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "OUT11")
				(number "12")
			)
			(pin power_out line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "OUT12")
				(number "13")
			)
			(pin power_out line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "OUT13")
				(number "14")
			)
			(pin power_out line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUT14")
				(number "15")
			)
			(pin power_out line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT15")
				(number "16")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT16")
				(number "17")
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT17")
				(number "18")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT18")
				(number "19")
			)
			(pin power_out line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT19")
				(number "20")
			)
			(pin power_out line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUT20")
				(number "21")
			)
			(pin power_out line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT21")
				(number "22")
			)
			(pin power_out line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "OUT22")
				(number "23")
			)
			(pin power_out line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "OUT23")
				(number "24")
			)
			(pin power_out line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "OUT24")
				(number "25")
			)
			(pin power_out line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "OUT25")
				(number "26")
			)
			(pin power_out line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "OUT26")
				(number "27")
			)
			(pin power_out line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "OUT27")
				(number "28")
			)
			(pin power_out line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "OUT28")
				(number "29")
			)
			(pin power_out line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "OUT29")
				(number "30")
			)
			(pin power_out line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "OUT30")
				(number "31")
			)
			(pin power_out line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "OUT31")
				(number "32")
			)
			(pin power_out line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "OUT32")
				(number "33")
			)
			(pin power_out line
				(at 12.7 -38.1 180)
				(length 2.54)
				(name "OUT33")
				(number "34")
			)
			(pin power_out line
				(at 12.7 -40.64 180)
				(length 2.54)
				(name "OUT34")
				(number "35")
			)
			(pin power_out line
				(at 12.7 -43.18 180)
				(length 2.54)
				(name "OUT35")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LP8868XQDMT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "LP8868XQDMT"
			(at 10.922 -16.764 0)
		)
		(property "Footprint" "Package_SON:VSON-14-1EP_3x4.45mm_P0.65mm_EP1.6x4.2mm"
			(at 0 -33.274 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lp8868x-q1.pdf"
			(at -0.254 19.304 0)
		)
		(property "Description" "LED Driver Boost , Input 4.5-65V, with PWM Dimming, Automotive, VSON-14"
			(at 0.254 -30.734 0)
		)
		(property "ki_keywords" "LED Driver Boost PWM Dimming"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*14*"
			(at 0 0 0)
		)
		(symbol "LP8868XQDMT_1_1"
			(pin power_in line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "VIN")
				(number "3")
			)
			(pin power_in line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "ADIM/HD")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "PWM/EN")
				(number "6")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "FAULT")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "TEMP")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "PGND")
				(number "1")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "AGND")
				(number "2")
			)
			(pin power_out line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "SW")
				(number "14")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "CSP")
				(number "13")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "CSN")
				(number "12")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "OVP")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "COMP")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "FSET")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3465"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LT3465"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3465fa.pdf"
			(at 1.27 -12.7 0)
		)
		(property "Description" "1.2MHz White LED Drivers with Built-in Schottky, ThinSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switching LED driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "LT3465_0_1")
		(symbol "LT3465_1_1"
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SW")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CTRL")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3755xMSE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 19.05 0)
		)
		(property "Value" "LT3755xMSE"
			(at 8.89 19.05 0)
		)
		(property "Footprint" "Package_SO:MSOP-16-1EP_3x4.039mm_P0.5mm_EP1.651x2.845mm"
			(at 25.4 -19.05 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/37551fd.pdf"
			(at -1.27 -27.94 0)
		)
		(property "Description" "40 Vin, 75 Vout, DC/DC LED Controllers, Hysteresis Open led Status pin, MSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost Buck Buck-Boost SEPIC Flyback"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x4.039mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT3755xMSE_0_1")
		(symbol "LT3755xMSE_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "~{SHDN}/UVLO")
				(number "12")
			)
			(pin output line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "VREF")
				(number "7")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "CTRL")
				(number "6")
			)
			(pin open_collector line
				(at -17.78 0 0)
				(length 2.54)
				(name "~{OPENLED}")
				(number "9")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PWM")
				(number "8")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "SS")
				(number "10")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "RT")
				(number "11")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VIN")
				(number "14")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin power_out line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "INTVCC")
				(number "13")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "ISN")
				(number "3")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "ISP")
				(number "4")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "GATE")
				(number "16")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "SENSE")
				(number "15")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PWMOUT")
				(number "1")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "VC")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3755xMSE-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 19.05 0)
		)
		(property "Value" "LT3755xMSE-1"
			(at 8.89 19.05 0)
		)
		(property "Footprint" "Package_SO:MSOP-16-1EP_3x4.039mm_P0.5mm_EP1.651x2.845mm"
			(at 25.4 -19.05 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/37551fd.pdf"
			(at -1.27 -27.94 0)
		)
		(property "Description" "40 Vin, 75 Vout, DC/DC LED Controllers, Frequency Synchronisation, MSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost Buck Buck-Boost SEPIC Flyback"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x4.039mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT3755xMSE-1_0_1")
		(symbol "LT3755xMSE-1_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "~{SHDN}/UVLO")
				(number "12")
			)
			(pin output line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "VREF")
				(number "7")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "CTRL")
				(number "6")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "SYNC")
				(number "9")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PWM")
				(number "8")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "SS")
				(number "10")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "RT")
				(number "11")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VIN")
				(number "14")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin power_out line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "INTVCC")
				(number "13")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "FB")
				(number "2")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "ISN")
				(number "3")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "ISP")
				(number "4")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "GATE")
				(number "16")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "SENSE")
				(number "15")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PWMOUT")
				(number "1")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "VC")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3755xUD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 19.05 0)
		)
		(property "Value" "LT3755xUD"
			(at 8.89 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.45x1.45mm"
			(at 26.67 -19.05 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/37551fd.pdf"
			(at -1.27 -27.94 0)
		)
		(property "Description" "40 Vin, 75 Vout, DC/DC LED Controller, Hysteresis Open led Status pins, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost Buck Buck-Boost SEPIC Flyback"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT3755xUD_0_1")
		(symbol "LT3755xUD_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "~{SHDN}/UVLO")
				(number "6")
			)
			(pin output line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "VREF")
				(number "1")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "CTRL")
				(number "16")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "~{OPENLED}")
				(number "3")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PWM")
				(number "2")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "SS")
				(number "4")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "RT")
				(number "5")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin power_out line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "INTVCC")
				(number "7")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "FB")
				(number "12")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "ISN")
				(number "13")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "ISP")
				(number "14")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "GATE")
				(number "10")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "SENSE")
				(number "9")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PWMOUT")
				(number "11")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "VC")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT3755xUD-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 19.05 0)
		)
		(property "Value" "LT3755xUD-1"
			(at 8.89 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.45x1.45mm"
			(at 26.67 -19.05 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/37551fd.pdf"
			(at -1.27 -27.94 0)
		)
		(property "Description" "40 Vin, 75 Vout, DC/DC LED Controllers, Frequency Synchronisation, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost Buck Buck-Boost SEPIC Flyback"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LT3755xUD-1_0_1")
		(symbol "LT3755xUD-1_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SHDN/UVLO")
				(number "6")
			)
			(pin output line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "VREF")
				(number "1")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "CTRL")
				(number "16")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "SYNC")
				(number "3")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PWM")
				(number "2")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "SS")
				(number "4")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "RT")
				(number "5")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin power_out line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "INTVCC")
				(number "7")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "FB")
				(number "12")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "ISN")
				(number "13")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "ISP")
				(number "14")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "GATE")
				(number "10")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "SENSE")
				(number "9")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PWMOUT")
				(number "11")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "VC")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT8391xFE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 -24.13 0)
		)
		(property "Value" "LT8391xFE"
			(at 6.35 -24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP2.74x4.75mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt8391.pdf"
			(at -1.27 -1.27 0)
		)
		(property "Description" "60V Synchronous 4-Switch Buck-Boost LED Controller, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "60V Synchronous 4-Switch Buck-Boost LED Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*1EP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LT8391xFE_0_1")
		(symbol "LT8391xFE_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "EN/UVLO")
				(number "9")
			)
			(pin power_out line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "INTVCC")
				(number "8")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SYNC/SPRD")
				(number "22")
			)
			(pin open_collector line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "17")
			)
			(pin power_out line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VREF")
				(number "12")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "CTRL2")
				(number "16")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CTRL1")
				(number "13")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PWM")
				(number "11")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "RP")
				(number "10")
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "VC")
				(number "20")
			)
			(pin passive line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "SS")
				(number "18")
			)
			(pin passive line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "RT")
				(number "21")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VIN")
				(number "7")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "TG1")
				(number "4")
			)
			(pin passive line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "BST1")
				(number "2")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SW1")
				(number "3")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "LSP")
				(number "5")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "LSN")
				(number "6")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "BG1")
				(number "1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "BG2")
				(number "28")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SW2")
				(number "26")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "BST2")
				(number "27")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "TG2")
				(number "25")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "FB")
				(number "19")
			)
			(pin power_in line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "VOUT")
				(number "24")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "ISP")
				(number "14")
			)
			(pin input line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "ISN")
				(number "15")
			)
			(pin output line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "PWMTG")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX7219"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 24.13 0)
		)
		(property "Value" "MAX7219"
			(at 1.27 25.4 0)
		)
		(property "Footprint" ""
			(at -1.27 1.27 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX7219-MAX7221.pdf"
			(at 1.27 -3.81 0)
		)
		(property "Description" "8-Digit LED Display Driver"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED 8-Digit Display Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x15.4mm*P1.27mm* DIP*7.62mm*"
			(at 0 0 0)
		)
		(symbol "MAX7219_0_1")
		(symbol "MAX7219_1_1"
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "ISET")
				(number "18")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "LOAD")
				(number "12")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "CLK")
				(number "13")
			)
			(pin input line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "DIN")
				(number "1")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "V+")
				(number "19")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "SEG_A")
				(number "14")
			)
			(pin output line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "SEG_B")
				(number "16")
			)
			(pin output line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "SEG_C")
				(number "20")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "SEG_D")
				(number "23")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SEG_E")
				(number "21")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SEG_F")
				(number "15")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SEG_G")
				(number "17")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SEG_DP")
				(number "22")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "DIG_0")
				(number "2")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DIG_1")
				(number "11")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "DIG_2")
				(number "6")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "DIG_3")
				(number "7")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "DIG_4")
				(number "3")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "DIG_5")
				(number "10")
			)
			(pin output line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "DIG_6")
				(number "5")
			)
			(pin output line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "DIG_7")
				(number "8")
			)
			(pin output line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "DOUT")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX7221xNG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 24.13 0)
		)
		(property "Value" "MAX7221xNG"
			(at 1.27 25.4 0)
		)
		(property "Footprint" "Package_DIP:DIP-24_W7.62mm"
			(at -1.27 1.27 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX7219-MAX7221.pdf"
			(at 1.27 -3.81 0)
		)
		(property "Description" "Serially Interfaced, 8-Digit LED Display Driver, PDIP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "spi qspi microwire"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MAX7221xNG_0_1")
		(symbol "MAX7221xNG_1_1"
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "ISET")
				(number "18")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "~{CS}")
				(number "12")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "CLK")
				(number "13")
			)
			(pin input line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "DIN")
				(number "1")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "V+")
				(number "19")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin open_emitter line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "SEG_A")
				(number "14")
			)
			(pin open_emitter line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "SEG_B")
				(number "16")
			)
			(pin open_emitter line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "SEG_C")
				(number "20")
			)
			(pin open_emitter line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "SEG_D")
				(number "23")
			)
			(pin open_emitter line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SEG_E")
				(number "21")
			)
			(pin open_emitter line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SEG_F")
				(number "15")
			)
			(pin open_emitter line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SEG_G")
				(number "17")
			)
			(pin open_emitter line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SEG_DP")
				(number "22")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "DIG_0")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DIG_1")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "DIG_2")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "DIG_3")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "DIG_4")
				(number "3")
			)
			(pin open_collector line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "DIG_5")
				(number "10")
			)
			(pin open_collector line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "DIG_6")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "DIG_7")
				(number "8")
			)
			(pin output line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "DOUT")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX7221xWG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 24.13 0)
		)
		(property "Value" "MAX7221xWG"
			(at 1.27 25.4 0)
		)
		(property "Footprint" "Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm"
			(at -1.27 1.27 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX7219-MAX7221.pdf"
			(at 1.27 -3.81 0)
		)
		(property "Description" "Serially Interfaced, 8-Digit LED Display Driver, SOIC-24W"
			(at 0 0 0)
		)
		(property "ki_keywords" "spi qspi microwire"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x15.4mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX7221xWG_0_1")
		(symbol "MAX7221xWG_1_1"
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "ISET")
				(number "18")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "~{CS}")
				(number "12")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "CLK")
				(number "13")
			)
			(pin input line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "DIN")
				(number "1")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "V+")
				(number "19")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin open_emitter line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "SEG_A")
				(number "14")
			)
			(pin open_emitter line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "SEG_B")
				(number "16")
			)
			(pin open_emitter line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "SEG_C")
				(number "20")
			)
			(pin open_emitter line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "SEG_D")
				(number "23")
			)
			(pin open_emitter line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SEG_E")
				(number "21")
			)
			(pin open_emitter line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SEG_F")
				(number "15")
			)
			(pin open_emitter line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SEG_G")
				(number "17")
			)
			(pin open_emitter line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SEG_DP")
				(number "22")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "DIG_0")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DIG_1")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "DIG_2")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "DIG_3")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "DIG_4")
				(number "3")
			)
			(pin open_collector line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "DIG_5")
				(number "10")
			)
			(pin open_collector line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "DIG_6")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "DIG_7")
				(number "8")
			)
			(pin output line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "DOUT")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MBI5252GFN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "MBI5252GFN"
			(at 1.27 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:HVQFN-24-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/1809031521_MBI-MBI5252GP-A_C261127.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-Channel, 14-bit PWM constant current LED sink driver with built-in 8K-bit SRAM, 6-bit current gain, LED open detection, HVQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Shift Register LED driver 16 bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*4x4mm*P0.5mm*2.5x2.5mm*"
			(at 0 0 0)
		)
		(symbol "MBI5252GFN_0_1")
		(symbol "MBI5252GFN_1_1"
			(pin input line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "SDI")
				(number "23")
			)
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "DCLK")
				(number "24")
			)
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "LE")
				(number "1")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "GCLK")
				(number "20")
			)
			(pin passive line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "R-EXT")
				(number "21")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 2.54)
				(name "PAD")
				(number "25")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin output line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "SDO")
				(number "19")
			)
			(pin open_collector line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "~{OUT0}")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "~{OUT1}")
				(number "3")
			)
			(pin open_collector line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "~{OUT2}")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "~{OUT3}")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~{OUT4}")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~{OUT5}")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{OUT6}")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{OUT7}")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{OUT8}")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{OUT9}")
				(number "12")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~{OUT10}")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "~{OUT11}")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "~{OUT12}")
				(number "15")
			)
			(pin open_collector line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "~{OUT13}")
				(number "16")
			)
			(pin open_collector line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "~{OUT14}")
				(number "17")
			)
			(pin open_collector line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "~{OUT15}")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MBI5252GP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "MBI5252GP"
			(at 1.27 26.67 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_3.9x8.7mm_P0.635mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/1809031521_MBI-MBI5252GP-A_C261127.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-Channel, 14-bit PWM constant current LED sink driver with built-in 8K-bit SRAM, 6-bit current gain, LED open detection, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Shift Register LED driver 16 bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "MBI5252GP_0_1")
		(symbol "MBI5252GP_1_1"
			(pin input line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "SDI")
				(number "2")
			)
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "DCLK")
				(number "3")
			)
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "LE")
				(number "4")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "GCLK")
				(number "21")
			)
			(pin passive line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "R-EXT")
				(number "23")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "SDO")
				(number "22")
			)
			(pin open_collector line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "~{OUT0}")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "~{OUT1}")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "~{OUT2}")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "~{OUT3}")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~{OUT4}")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~{OUT5}")
				(number "10")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{OUT6}")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{OUT7}")
				(number "12")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{OUT8}")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{OUT9}")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~{OUT10}")
				(number "15")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "~{OUT11}")
				(number "16")
			)
			(pin open_collector line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "~{OUT12}")
				(number "17")
			)
			(pin open_collector line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "~{OUT13}")
				(number "18")
			)
			(pin open_collector line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "~{OUT14}")
				(number "19")
			)
			(pin open_collector line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "~{OUT15}")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC14495P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 16.51 0)
		)
		(property "Value" "MC14495P"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 2.54 16.51 0)
		)
		(property "Datasheet" "https://www.futurlec.com/Datasheet/Motorola/MC14495.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "C-MOS BCD-TO-SEVEN-SEGMENT 4-BIT LATCH / DECODER DRIVER, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "driver 7-segment"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16?W7.62*"
			(at 0 0 0)
		)
		(symbol "MC14495P_1_1"
			(pin input line
				(at -7.62 10.16 0)
				(length 2.54)
				(name "A")
				(number "5")
			)
			(pin input line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "B")
				(number "6")
			)
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "C")
				(number "9")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D")
				(number "10")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{CLK}")
				(number "7")
			)
			(pin input line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "~{VCR}")
				(number "11")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 7.62 10.16 180)
				(length 2.54)
				(name "a")
				(number "12")
			)
			(pin output line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "b")
				(number "13")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "c")
				(number "14")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "d")
				(number "15")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "e")
				(number "1")
			)
			(pin output line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "f")
				(number "2")
			)
			(pin output line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "g")
				(number "3")
			)
			(pin output line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "h+i")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1643xMS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 12.7 0)
		)
		(property "Value" "MCP1643xMS"
			(at 10.16 12.7 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at -1.27 -16.51 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/20005208A.pdf"
			(at -1.27 -16.51 0)
		)
		(property "Description" "Constant-current LED boost regulator, 0.65V startup, 550mA output, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED driver low voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP1643xMS_0_1")
		(symbol "MCP1643xMS_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "SGND")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "PGND")
				(number "6")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SW")
				(number "5")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "4")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VFB")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP1662-xOT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "MCP1662-xOT"
			(at 8.89 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/20005316E.pdf"
			(at 0 8.89 0)
		)
		(property "Description" "Step-Up LED Driver w/ UVLO and Open Load Protection, 500kHz, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "step-up led driver uvlo"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP1662-xOT_0_1")
		(symbol "MCP1662-xOT_1_1"
			(pin power_in line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "V_{IN}")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_out line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "V_{FB}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MP3362GJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "MP3362GJ"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-8"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.monolithicpower.com/en/documentview/productdocument/index/version/2/document_type/Datasheet/lang/en/sku/MP3362GJ/document_id/9117/"
			(at 2.54 -11.43 0)
		)
		(property "Description" "Single string LED driver, 3V to 36V input, 4A peak current limit, 200Khz to 2Mhz, SOT23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "MP3362GJ_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
				(alternate "DIM" input line)
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "OSC")
				(number "5")
				(alternate "SYNC" input line)
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "COMP")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "OVP")
				(number "7")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MPQ2483DQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MPQ2483DQ"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.7x2.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.monolithicpower.com/pub/media/document/MPQ2483_r1.05.pdf"
			(at -5.08 -5.08 0)
		)
		(property "Description" "55V, 2.5A Programmable Frequency LED Driver, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MPQ2483DQ_0_1")
		(symbol "MPQ2483DQ_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN/DIM")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "RSET")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "COMP")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "INGND")
				(number "8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at 2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "BST")
				(number "9")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "SW")
				(number "10")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OVP")
				(number "3")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "FB")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCP5623DTBR2G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 15.24 0)
		)
		(property "Value" "NCP5623DTBR2G"
			(at 12.7 12.7 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCP5623-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "Triple Output I2C Controlled RGB LED Driver, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED RGB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "NCP5623DTBR2G_0_1")
		(symbol "NCP5623DTBR2G_1_1"
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SDA")
				(number "9")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "11")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "I_{REF}")
				(number "10")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "V_{DET}")
				(number "12")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IC")
				(number "1")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "IC")
				(number "14")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V_{BAT}")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin no_connect line
				(at 7.62 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "LED1")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "LED2")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "LED3")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCR401U"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 6.35 0)
		)
		(property "Value" "NCR401U"
			(at -6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SC-74-6_1.55x2.9mm_P0.95mm"
			(at 1.905 -6.35 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/NCR401U.pdf"
			(at 1.905 -8.89 0)
		)
		(property "Description" "10mA (with external R up to 65mA) constant current driver (linear), max 40V, SOT457 (SC-74)"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED driver constant current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SC?74*"
			(at 0 0 0)
		)
		(symbol "NCR401U_0_1")
		(symbol "NCR401U_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "REXT")
				(number "6")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VS")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "IOUT")
				(number "2")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "IOUT")
				(number "3")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "IOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9531PW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "PCA9531PW"
			(at 6.35 -13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9531.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "8-bit PWM I2C eight LED driver, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "led pwm rgb smbus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCA9531PW_0_1")
		(symbol "PCA9531PW_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "SCL")
				(number "14")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SDA")
				(number "15")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "13")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V_{DD}")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "V_{SS}")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "LED0")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "LED1")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "LED2")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "LED3")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "LED4")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "LED5")
				(number "10")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "LED6")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "LED7")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9635"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "PCA9635"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9635.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-bit PWM Fm+ I2C-bus LED driver, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "led pwm rgb rgba"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCA9635_0_1")
		(symbol "PCA9635_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "SCL")
				(number "26")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "SDA")
				(number "27")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "~{OE}")
				(number "23")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A5")
				(number "24")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A6")
				(number "25")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "14")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "LED0")
				(number "6")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "LED1")
				(number "7")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "LED2")
				(number "8")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "LED3")
				(number "9")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "LED4")
				(number "10")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "LED5")
				(number "11")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "LED6")
				(number "12")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "LED7")
				(number "13")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "LED8")
				(number "15")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "LED9")
				(number "16")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "LED10")
				(number "17")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "LED11")
				(number "18")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "LED12")
				(number "19")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "LED13")
				(number "20")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "LED14")
				(number "21")
			)
			(pin output line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "LED15")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9685BS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 22.225 0)
		)
		(property "Value" "PCA9685BS"
			(at 1.27 22.225 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 0.635 -24.765 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/PCA9685.pdf"
			(at -10.16 17.78 0)
		)
		(property "Description" "16-channel 12-bit PWM Fm+ I2C-bus LED controller RGBA QFN"
			(at 0 0 0)
		)
		(property "ki_keywords" "PWM LED driver I2C QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCA9685BS_0_1")
		(symbol "PCA9685BS_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "SCL")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "SDA")
				(number "24")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "EXTCLK")
				(number "22")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "~{OE}")
				(number "20")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "A0")
				(number "26")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "A1")
				(number "27")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "A2")
				(number "28")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 5.08)
				(name "A3")
				(number "1")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "A4")
				(number "2")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "A5")
				(number "21")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VDD")
				(number "25")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "11")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "LED0")
				(number "3")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "LED1")
				(number "4")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "LED2")
				(number "5")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "LED3")
				(number "6")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "LED4")
				(number "7")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "LED5")
				(number "8")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "LED6")
				(number "9")
			)
			(pin output line
				(at 17.78 0 180)
				(length 5.08)
				(name "LED7")
				(number "10")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "LED8")
				(number "12")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "LED9")
				(number "13")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "LED10")
				(number "14")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "LED11")
				(number "15")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "LED12")
				(number "16")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "LED13")
				(number "17")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "LED14")
				(number "18")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "LED15")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9685PW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 22.225 0)
		)
		(property "Value" "PCA9685PW"
			(at 1.27 22.225 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 0.635 -24.765 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/PCA9685.pdf"
			(at -10.16 17.78 0)
		)
		(property "Description" "16-channel 12-bit PWM Fm+ I2C-bus LED controller RGBA TSSOP"
			(at 0 0 0)
		)
		(property "ki_keywords" "PWM LED driver I2C TSSOP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCA9685PW_0_1")
		(symbol "PCA9685PW_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "SCL")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "SDA")
				(number "27")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "EXTCLK")
				(number "25")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "~{OE}")
				(number "23")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 5.08)
				(name "A3")
				(number "4")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "A4")
				(number "5")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "A5")
				(number "24")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "14")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "LED0")
				(number "6")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "LED1")
				(number "7")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "LED2")
				(number "8")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "LED3")
				(number "9")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "LED4")
				(number "10")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "LED5")
				(number "11")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "LED6")
				(number "12")
			)
			(pin output line
				(at 17.78 0 180)
				(length 5.08)
				(name "LED7")
				(number "13")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "LED8")
				(number "15")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "LED9")
				(number "16")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "LED10")
				(number "17")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "LED11")
				(number "18")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "LED12")
				(number "19")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "LED13")
				(number "20")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "LED14")
				(number "21")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "LED15")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9745BTW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "PCA9745BTW"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:NXP_HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP2.2x3.4mm"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9745B.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-channel, 8-bit PWM, Constant Current, Dimming, LED controller, SPI, HTSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "pwm led current spi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "NXP*HTSSOP*28*1EP*4.4x9.7mm*P0.65mm*EP2.2x3.4mm*"
			(at 0 0 0)
		)
		(symbol "PCA9745BTW_0_1")
		(symbol "PCA9745BTW_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "~{CS}")
				(number "4")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "SCLK")
				(number "26")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "SDI")
				(number "27")
			)
			(pin output line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SDO")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{OE}")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "25")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "REXT")
				(number "1")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "V_{DD}")
				(number "28")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "V_{SS}")
				(number "10")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "V_{SS}")
				(number "19")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "V_{SS}")
				(number "2")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "V_{SS}")
				(number "24")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "V_{SS}")
				(number "29")
			)
			(pin open_collector line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "LED0")
				(number "6")
			)
			(pin open_collector line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "LED1")
				(number "7")
			)
			(pin open_collector line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "LED2")
				(number "8")
			)
			(pin open_collector line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "LED3")
				(number "9")
			)
			(pin open_collector line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "LED4")
				(number "11")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "LED5")
				(number "12")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "LED6")
				(number "13")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "LED7")
				(number "14")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "LED8")
				(number "15")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "LED9")
				(number "16")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "LED10")
				(number "17")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "LED11")
				(number "18")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "LED12")
				(number "20")
			)
			(pin open_collector line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "LED13")
				(number "21")
			)
			(pin open_collector line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "LED14")
				(number "22")
			)
			(pin open_collector line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "LED15")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RCD-24"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "RCD-24"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_RCD-24_THT"
			(at 26.67 -11.43 0)
		)
		(property "Datasheet" "https://g.recomcdn.com/media/Datasheet/pdf/.fYUQjOlW/.t2a80a771bdbb0ef300f7/Datasheet-93/RCD-24.pdf"
			(at 0 0 0)
		)
		(property "Description" "LED Driver DC/DC Converter, input 4.5 to 36V, output current 0.3 to 1.2A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Led Driver DC-DC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Converter*DCDC*RECOM*RCD?24*"
			(at 0 0 0)
		)
		(symbol "RCD-24_1_1"
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "PWM/ON/OFF")
				(number "3")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "Analogue_Dimming")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "+Vin")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "+Vout")
				(number "6")
			)
			(pin power_out line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "-Vout")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ST1CC40DR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 5.715 0)
		)
		(property "Value" "ST1CC40DR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 3.175 -6.35 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/group3/71/e8/26/3c/c8/cc/46/e6/CD00292360/files/CD00292360.pdf/jcr:content/translations/en.CD00292360.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A monolithic step-down current source with synchronous rectification, 3-18V Input Voltage, 850kHz, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC/DC Buck Conwerter 3A Low Voltage Input LED Lighting"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ST1CC40DR_0_1")
		(symbol "ST1CC40DR_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VINSW")
				(number "8")
			)
			(pin power_in line
				(at -12.7 0 0)
				(length 2.54)
				(name "VINA")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "INH")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "AGND")
				(number "6")
			)
			(pin power_out line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "PGND")
				(number "2")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ST1CC40PUR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 5.715 0)
		)
		(property "Value" "ST1CC40PUR"
			(at 0 5.715 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_4x4mm_P0.8mm_EP2.5x3.6mm"
			(at 5.715 -6.35 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/group3/71/e8/26/3c/c8/cc/46/e6/CD00292360/files/CD00292360.pdf/jcr:content/translations/en.CD00292360.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A monolithic step-down current source with synchronous rectification, 3-18V Input Voltage, 850kHz, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC/DC Buck Conwerter 3A Low Voltage Input LED Lighting"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ST1CC40PUR_0_1")
		(symbol "ST1CC40PUR_1_1"
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VINSW")
				(number "6")
			)
			(pin power_in line
				(at -12.7 0 0)
				(length 2.54)
				(name "VINA")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "INH")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "PAD")
				(number "9")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "AGND")
				(number "4")
			)
			(pin power_out line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "PGND")
				(number "8")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SW")
				(number "7")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STP08CP05B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 19.304 0)
		)
		(property "Value" "STP08CP05B"
			(at 1.27 19.304 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stp08cp05.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit constant current LED sink driver, 5..100mA output current, 20V driving capability, 3.0..5.5V power supply, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Shift Register"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "STP08CP05B_0_1")
		(symbol "STP08CP05B_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "SDI")
				(number "2")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "CLK")
				(number "3")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "LE")
				(number "4")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{OE}")
				(number "13")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "R-EXT")
				(number "15")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "~{OUT0}")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "~{OUT1}")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~{OUT2}")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~{OUT3}")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{OUT4}")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{OUT5}")
				(number "10")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{OUT6}")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{OUT7}")
				(number "12")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "SDO")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STP08CP05XT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 19.304 0)
		)
		(property "Value" "STP08CP05XT"
			(at 1.27 19.304 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3x3mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stp08cp05.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit constant current LED sink driver, 5..100mA output current, 20V driving capability, 3.0..5.5V power supply, HTSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Shift Register"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*1EP*4.4*5*P0.65mm*EP3x3mm*"
			(at 0 0 0)
		)
		(symbol "STP08CP05XT_0_1")
		(symbol "STP08CP05XT_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "SDI")
				(number "2")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "CLK")
				(number "3")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "LE")
				(number "4")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{OE}")
				(number "13")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "R-EXT")
				(number "15")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "EPAD")
				(number "17")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "~{OUT0}")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "~{OUT1}")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~{OUT2}")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~{OUT3}")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{OUT4}")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{OUT5}")
				(number "10")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{OUT6}")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{OUT7}")
				(number "12")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "SDO")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STP16CP05M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 29.464 0)
		)
		(property "Value" "STP16CP05M"
			(at 1.27 29.464 0)
		)
		(property "Footprint" "Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stp16cp05.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-bit constant current LED sink driver, 5..100mA output current, 20V driving capability, 3.0..5.5V power supply, SOIC-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Shift Register"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*7.5*15.*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "STP16CP05M_0_1")
		(symbol "STP16CP05M_1_1"
			(pin input line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "SDI")
				(number "2")
			)
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "CLK")
				(number "3")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "LE/DM1")
				(number "4")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "~{OE/DM2}")
				(number "21")
			)
			(pin output line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "R-EXT")
				(number "23")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "~{OUT0}")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "~{OUT1}")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "~{OUT2}")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "~{OUT3}")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "~{OUT4}")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "~{OUT5}")
				(number "10")
			)
			(pin open_collector line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~{OUT6}")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~{OUT7}")
				(number "12")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{OUT8}")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{OUT9}")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{OUT10}")
				(number "15")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{OUT11}")
				(number "16")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~{OUT12}")
				(number "17")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "~{OUT13}")
				(number "18")
			)
			(pin open_collector line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "~{OUT14}")
				(number "19")
			)
			(pin open_collector line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "~{OUT15}")
				(number "20")
			)
			(pin output line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "SDO")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STP16CP05XT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 29.464 0)
		)
		(property "Value" "STP16CP05XT"
			(at 1.27 29.464 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.2x5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stp16cp05.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-bit constant current LED sink driver, 5..100mA output current, 20V driving capability, 3.0..5.5V power supply, HTSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Shift Register"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*HTSSOP*1EP*4.4*7.8*P0.65mm*EP3.2x5mm*"
			(at 0 0 0)
		)
		(symbol "STP16CP05XT_0_1")
		(symbol "STP16CP05XT_1_1"
			(pin input line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "SDI")
				(number "2")
			)
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "CLK")
				(number "3")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "LE/DM1")
				(number "4")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "~{OE/DM2}")
				(number "21")
			)
			(pin output line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "R-EXT")
				(number "23")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "EPAD")
				(number "25")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "~{OUT0}")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "~{OUT1}")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "~{OUT2}")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "~{OUT3}")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "~{OUT4}")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "~{OUT5}")
				(number "10")
			)
			(pin open_collector line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~{OUT6}")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~{OUT7}")
				(number "12")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{OUT8}")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{OUT9}")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{OUT10}")
				(number "15")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{OUT11}")
				(number "16")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~{OUT12}")
				(number "17")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "~{OUT13}")
				(number "18")
			)
			(pin open_collector line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "~{OUT14}")
				(number "19")
			)
			(pin open_collector line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "~{OUT15}")
				(number "20")
			)
			(pin output line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "SDO")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STP16CPC26T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 28.956 0)
		)
		(property "Value" "STP16CPC26T"
			(at 2.54 28.956 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/STP16CPC26.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-bit constant current LED sink driver, 5..90mA output current, 20V driving capability, 3..5.5V power supply, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Shift Register "
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSSOP*4.4*7.*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STP16CPC26T_0_1")
		(symbol "STP16CPC26T_1_1"
			(pin input line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "SDI")
				(number "2")
			)
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "CLK")
				(number "3")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "LE")
				(number "4")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "~{OE}")
				(number "21")
			)
			(pin output line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "R-EXT")
				(number "23")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "~{OUT0}")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "~{OUT1}")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "~{OUT2}")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "~{OUT3}")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "~{OUT4}")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "~{OUT5}")
				(number "10")
			)
			(pin open_collector line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~{OUT6}")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~{OUT7}")
				(number "12")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{OUT8}")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{OUT9}")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{OUT10}")
				(number "15")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{OUT11}")
				(number "16")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~{OUT12}")
				(number "17")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "~{OUT13}")
				(number "18")
			)
			(pin open_collector line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "~{OUT14}")
				(number "19")
			)
			(pin open_collector line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "~{OUT15}")
				(number "20")
			)
			(pin output line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "SDO")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STP16CPC26X"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 28.956 0)
		)
		(property "Value" "STP16CPC26X"
			(at 2.54 28.956 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.2x5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/STP16CPC26.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-bit constant current LED sink driver, 5..90mA output current, 20V driving capability, 3..5.5V power supply, HTSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Shift Register"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*HTSSOP*1EP*4.4*7.*P0.65*EP3.2x5mm*"
			(at 0 0 0)
		)
		(symbol "STP16CPC26X_0_1")
		(symbol "STP16CPC26X_1_1"
			(pin input line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "SDI")
				(number "2")
			)
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "CLK")
				(number "3")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "LE")
				(number "4")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "~{OE}")
				(number "21")
			)
			(pin output line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "R-EXT")
				(number "23")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "EPAD")
				(number "25")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "~{OUT0}")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "~{OUT1}")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "~{OUT2}")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "~{OUT3}")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "~{OUT4}")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "~{OUT5}")
				(number "10")
			)
			(pin open_collector line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~{OUT6}")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~{OUT7}")
				(number "12")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{OUT8}")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{OUT9}")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{OUT10}")
				(number "15")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{OUT11}")
				(number "16")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~{OUT12}")
				(number "17")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "~{OUT13}")
				(number "18")
			)
			(pin open_collector line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "~{OUT14}")
				(number "19")
			)
			(pin open_collector line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "~{OUT15}")
				(number "20")
			)
			(pin output line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "SDO")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCA6507RUE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 15.24 0)
		)
		(property "Value" "TCA6507RUE"
			(at 7.62 12.7 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_X2QFN-RUE-12_1.4x2mm_P0.4mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tca6507"
			(at 0 1.27 0)
		)
		(property "Description" "7-bit I2C/SMBus LED driver with intensity control, X2QFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "led driver i2c 7-bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*X2QFN*RUE*"
			(at 0 0 0)
		)
		(symbol "TCA6507RUE_1_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V_{CC}")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "P0")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "P1")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "P2")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "P3")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "P4")
				(number "10")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "P5")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "P6")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLC59108xPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "TLC59108xPW"
			(at 8.89 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlc59108.pdf"
			(at -5.08 -1.27 0)
		)
		(property "Description" "8-Channel, 8-Bit Fm+ I2C-Bus Constant-Current LED Sink Driver, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED current driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TLC59108xPW_0_1")
		(symbol "TLC59108xPW_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "17")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "18")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "19")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A0")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A3")
				(number "5")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "REXT")
				(number "1")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin open_collector line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "~{OUT0}")
				(number "6")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{OUT1}")
				(number "7")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{OUT2}")
				(number "9")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{OUT3}")
				(number "10")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{OUT4}")
				(number "11")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{OUT5}")
				(number "12")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "~{OUT6}")
				(number "14")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{OUT7}")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLC5916"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "TLC5916"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlc5916.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "8-Channel Constant-Current LED Sink Driver"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Constant-Current Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TLC5916_1_0"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "SDI")
				(number "2")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "CLK")
				(number "3")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "LE(ED1)")
				(number "4")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{OE}(ED2)")
				(number "13")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "R-EXT")
				(number "15")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "~{OUT0}")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~{OUT1}")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~{OUT2}")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{OUT3}")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{OUT4}")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{OUT5}")
				(number "10")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{OUT6}")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~{OUT7}")
				(number "12")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "SDO")
				(number "14")
			)
		)
		(symbol "TLC5916_1_1")
		(embedded_fonts no)
	)
	(symbol "TLC5940NT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 22.225 0)
		)
		(property "Value" "TLC5940NT"
			(at 12.7 22.225 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 1.27 -24.765 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc5940.pdf"
			(at -10.16 17.78 0)
		)
		(property "Description" "16-Channel LED Driver With DOT Correction and Grayscale PWM Control, DIP package"
			(at 0 0 0)
		)
		(property "ki_keywords" "PWM LED driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TLC5940NT_0_1")
		(symbol "TLC5940NT_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "VPRG")
				(number "27")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "IREF")
				(number "20")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "DCPRG")
				(number "19")
			)
			(pin input clock
				(at -17.78 10.16 0)
				(length 5.08)
				(name "GSCLK")
				(number "18")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "BLANK")
				(number "23")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "XLAT")
				(number "24")
			)
			(pin open_collector line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "XERR")
				(number "16")
			)
			(pin input clock
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "SCLK")
				(number "25")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "SIN")
				(number "26")
			)
			(pin output line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "SOUT")
				(number "17")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VCC")
				(number "21")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "22")
			)
			(pin open_collector line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "OUT0")
				(number "28")
			)
			(pin open_collector line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "OUT1")
				(number "1")
			)
			(pin open_collector line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "OUT2")
				(number "2")
			)
			(pin open_collector line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "OUT3")
				(number "3")
			)
			(pin open_collector line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "OUT4")
				(number "4")
			)
			(pin open_collector line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "OUT5")
				(number "5")
			)
			(pin open_collector line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "OUT6")
				(number "6")
			)
			(pin open_collector line
				(at 17.78 0 180)
				(length 5.08)
				(name "OUT7")
				(number "7")
			)
			(pin open_collector line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "OUT8")
				(number "8")
			)
			(pin open_collector line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "OUT9")
				(number "9")
			)
			(pin open_collector line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "OUT10")
				(number "10")
			)
			(pin open_collector line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "OUT11")
				(number "11")
			)
			(pin open_collector line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "OUT12")
				(number "12")
			)
			(pin open_collector line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "OUT13")
				(number "13")
			)
			(pin open_collector line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "OUT14")
				(number "14")
			)
			(pin open_collector line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "OUT15")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLC5940PWP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 22.225 0)
		)
		(property "Value" "TLC5940PWP"
			(at 1.27 22.225 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP3.4x9.5mm_Mask2.4x6.17mm_ThermalVias"
			(at 0.635 -24.765 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc5940.pdf"
			(at -10.16 17.78 0)
		)
		(property "Description" "16-Channel LED Driver With DOT Correction and Grayscale PWM Control, TSSOP package with thermal pad"
			(at 0 0 0)
		)
		(property "ki_keywords" "PWM LED driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TLC5940PWP_0_1")
		(symbol "TLC5940PWP_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "VPRG")
				(number "6")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "IREF")
				(number "27")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "DCPRG")
				(number "26")
			)
			(pin input clock
				(at -17.78 10.16 0)
				(length 5.08)
				(name "GSCLK")
				(number "25")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "BLANK")
				(number "2")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "XLAT")
				(number "3")
			)
			(pin open_collector line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "XERR")
				(number "23")
			)
			(pin input clock
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "SCLK")
				(number "4")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "SIN")
				(number "5")
			)
			(pin output line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "SOUT")
				(number "24")
			)
			(pin input line
				(at -2.54 -27.94 90)
				(length 5.08)
				(name "PAD")
				(number "29")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin open_collector line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "OUT0")
				(number "7")
			)
			(pin open_collector line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "OUT1")
				(number "8")
			)
			(pin open_collector line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "OUT2")
				(number "9")
			)
			(pin open_collector line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "OUT3")
				(number "10")
			)
			(pin open_collector line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "OUT4")
				(number "11")
			)
			(pin open_collector line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "OUT5")
				(number "12")
			)
			(pin open_collector line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "OUT6")
				(number "13")
			)
			(pin open_collector line
				(at 17.78 0 180)
				(length 5.08)
				(name "OUT7")
				(number "14")
			)
			(pin open_collector line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "OUT8")
				(number "15")
			)
			(pin open_collector line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "OUT9")
				(number "16")
			)
			(pin open_collector line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "OUT10")
				(number "17")
			)
			(pin open_collector line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "OUT11")
				(number "18")
			)
			(pin open_collector line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "OUT12")
				(number "19")
			)
			(pin open_collector line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "OUT13")
				(number "20")
			)
			(pin open_collector line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "OUT14")
				(number "21")
			)
			(pin open_collector line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "OUT15")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLC5947DAP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 38.1 0)
		)
		(property "Value" "TLC5947DAP"
			(at -13.97 35.56 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-32-1EP_6.1x11mm_P0.65mm_EP5.2x11mm_Mask4.11x4.36mm_ThermalVias"
			(at -13.97 40.64 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc5947.pdf"
			(at 0 0 0)
		)
		(property "Description" "24-Channel, 12-Bit PWM LED Driver, HTSSOP"
			(at 0 0 0)
		)
		(property "ki_keywords" "PWM LED driver HTSSOP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*"
			(at 0 0 0)
		)
		(symbol "TLC5947DAP_0_1"
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "IREF")
				(number "31")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "BLANK")
				(number "2")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "XLAT")
				(number "30")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "SCLK")
				(number "3")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "SIN")
				(number "4")
			)
			(pin output line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "SOUT")
				(number "29")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 3.81)
				(name "PowerPAD")
				(number "33")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 3.81)
				(name "VCC")
				(number "32")
			)
			(pin output line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "OUT0")
				(number "5")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 3.81)
				(name "OUT1")
				(number "6")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "OUT2")
				(number "7")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "OUT3")
				(number "8")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "OUT4")
				(number "9")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "OUT5")
				(number "10")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "OUT6")
				(number "11")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "OUT7")
				(number "12")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "OUT8")
				(number "13")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "OUT9")
				(number "14")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "OUT10")
				(number "15")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "OUT11")
				(number "16")
			)
			(pin output line
				(at 17.78 0 180)
				(length 3.81)
				(name "OUT12")
				(number "17")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "OUT13")
				(number "18")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "OUT14")
				(number "19")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "OUT15")
				(number "20")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "OUT16")
				(number "21")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "OUT17")
				(number "22")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "OUT18")
				(number "23")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "OUT19")
				(number "24")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "OUT20")
				(number "25")
			)
			(pin output line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "OUT21")
				(number "26")
			)
			(pin output line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "OUT22")
				(number "27")
			)
			(pin output line
				(at 17.78 -27.94 180)
				(length 3.81)
				(name "OUT23")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLC5947RHB"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 38.1 0)
		)
		(property "Value" "TLC5947RHB"
			(at -13.97 35.56 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -13.97 40.64 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc5947.pdf"
			(at 0 0 0)
		)
		(property "Description" "24-Channel, 12-Bit PWM LED Driver, QFN"
			(at 0 0 0)
		)
		(property "ki_keywords" "PWM LED driver QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*"
			(at 0 0 0)
		)
		(symbol "TLC5947RHB_0_1"
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "IREF")
				(number "27")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "BLANK")
				(number "30")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "XLAT")
				(number "26")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "SCLK")
				(number "31")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "SIN")
				(number "32")
			)
			(pin output line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "SOUT")
				(number "25")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 3.81)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 3.81)
				(name "PowerPAD")
				(number "33")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 3.81)
				(name "VCC")
				(number "28")
			)
			(pin output line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "OUT0")
				(number "1")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 3.81)
				(name "OUT1")
				(number "2")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "OUT2")
				(number "3")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "OUT3")
				(number "4")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "OUT4")
				(number "5")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "OUT5")
				(number "6")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "OUT6")
				(number "7")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "OUT7")
				(number "8")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "OUT8")
				(number "9")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "OUT9")
				(number "10")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "OUT10")
				(number "11")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "OUT11")
				(number "12")
			)
			(pin output line
				(at 17.78 0 180)
				(length 3.81)
				(name "OUT12")
				(number "13")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "OUT13")
				(number "14")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "OUT14")
				(number "15")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "OUT15")
				(number "16")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "OUT16")
				(number "17")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "OUT17")
				(number "18")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "OUT18")
				(number "19")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "OUT19")
				(number "20")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "OUT20")
				(number "21")
			)
			(pin output line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "OUT21")
				(number "22")
			)
			(pin output line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "OUT22")
				(number "23")
			)
			(pin output line
				(at 17.78 -27.94 180)
				(length 3.81)
				(name "OUT23")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLC5949PWP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 26.67 0)
		)
		(property "Value" "TLC5949PWP"
			(at 6.35 -26.67 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.4x7.8mm_Mask2.4x2.98mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlc5949.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-channel, 12bit ES-PWM, constant-current sink LED driver, HTSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "led driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TLC5949PWP_0_1")
		(symbol "TLC5949PWP_1_1"
			(pin input line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "SIN")
				(number "2")
			)
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "SCLK")
				(number "3")
			)
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "LAT")
				(number "4")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "GSCLK")
				(number "21")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "IREF")
				(number "23")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin output line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "SOUT")
				(number "22")
			)
			(pin open_collector line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "OUT0")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "OUT1")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "OUT2")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "OUT3")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUT4")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT5")
				(number "10")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT6")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT7")
				(number "12")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT8")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUT9")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "OUT10")
				(number "15")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "OUT11")
				(number "16")
			)
			(pin open_collector line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "OUT12")
				(number "17")
			)
			(pin open_collector line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "OUT13")
				(number "18")
			)
			(pin open_collector line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "OUT14")
				(number "19")
			)
			(pin open_collector line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "OUT15")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLC5951DAP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 34.29 0)
		)
		(property "Value" "TLC5951DAP"
			(at 1.27 -34.29 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-38-1EP_6.1x12.5mm_P0.65mm_EP5.2x12.5mm_Mask3.39x6.35mm_ThermalVias"
			(at 0 -43.18 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc5951.pdf"
			(at 0 -43.18 0)
		)
		(property "Description" "24-Channel, 12-Bit PWM LED Driver With 7-Bit Dot Correction and 3-Group, 8-Bit Global Brightness Control, HTSSOP-38"
			(at 0 0 0)
		)
		(property "ki_keywords" "led driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*1EP*6.1x12.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TLC5951DAP_0_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "GSSIN")
				(number "1")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "DCSIN")
				(number "38")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "GSSCK")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "GSLAT")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "DCSCK")
				(number "37")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "XBLNK")
				(number "36")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "GSCKR")
				(number "5")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "GSCKG")
				(number "4")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "GSCKB")
				(number "6")
			)
			(pin passive line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "IREF")
				(number "34")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "35")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin open_collector line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "OUTR0")
				(number "8")
			)
			(pin open_collector line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "OUTG0")
				(number "7")
			)
			(pin open_collector line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "OUTB0")
				(number "9")
			)
			(pin open_collector line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "OUTR1")
				(number "11")
			)
			(pin open_collector line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "OUTG1")
				(number "10")
			)
			(pin open_collector line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "OUTB1")
				(number "12")
			)
			(pin open_collector line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "OUTR2")
				(number "14")
			)
			(pin open_collector line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "OUTG2")
				(number "13")
			)
			(pin open_collector line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUTB2")
				(number "15")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUTR3")
				(number "17")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUTG3")
				(number "16")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUTB3")
				(number "18")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUTR4")
				(number "22")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUTG4")
				(number "23")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUTB4")
				(number "21")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "OUTR5")
				(number "25")
			)
			(pin open_collector line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "OUTG5")
				(number "26")
			)
			(pin open_collector line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "OUTB5")
				(number "24")
			)
			(pin open_collector line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "OUTR6")
				(number "28")
			)
			(pin open_collector line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "OUTG6")
				(number "29")
			)
			(pin open_collector line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "OUTB6")
				(number "27")
			)
			(pin open_collector line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "OUTR7")
				(number "31")
			)
			(pin open_collector line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "OUTG7")
				(number "32")
			)
			(pin open_collector line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "OUTB7")
				(number "30")
			)
		)
		(symbol "TLC5951DAP_1_1"
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "GSSOUT")
				(number "19")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "DCSOUT")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLC5951RHA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 34.29 0)
		)
		(property "Value" "TLC5951RHA"
			(at 1.27 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHA0040B_VQFN-40-1EP_6x6mm_P0.5mm_EP4.15x4.15mm_ThermalVias"
			(at 0 -44.45 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc5951.pdf"
			(at 0 -43.18 0)
		)
		(property "Description" "24-Channel, 12-Bit PWM LED Driver With 7-Bit Dot Correction and 3-Group, 8-Bit Global Brightness Control, Texas S-PVQFN-N40"
			(at 0 0 0)
		)
		(property "ki_keywords" "led driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RHA0040B*"
			(at 0 0 0)
		)
		(symbol "TLC5951RHA_0_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "GSSIN")
				(number "26")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "DCSIN")
				(number "25")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "GSSCK")
				(number "27")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "GSLAT")
				(number "28")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "DCSCK")
				(number "24")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "XBLNK")
				(number "23")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "GSCKR")
				(number "30")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "GSCKG")
				(number "29")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "GSCKB")
				(number "31")
			)
			(pin passive line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "IREF")
				(number "21")
			)
			(pin no_connect line
				(at -10.16 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 -25.4 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "22")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin open_collector line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "OUTR0")
				(number "33")
			)
			(pin open_collector line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "OUTG0")
				(number "32")
			)
			(pin open_collector line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "OUTB0")
				(number "34")
			)
			(pin open_collector line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "OUTR1")
				(number "36")
			)
			(pin open_collector line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "OUTG1")
				(number "35")
			)
			(pin open_collector line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "OUTB1")
				(number "37")
			)
			(pin open_collector line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "OUTR2")
				(number "39")
			)
			(pin open_collector line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "OUTG2")
				(number "38")
			)
			(pin open_collector line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUTB2")
				(number "40")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUTR3")
				(number "2")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUTG3")
				(number "1")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUTB3")
				(number "3")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUTR4")
				(number "9")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUTG4")
				(number "10")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUTB4")
				(number "8")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "OUTR5")
				(number "12")
			)
			(pin open_collector line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "OUTG5")
				(number "13")
			)
			(pin open_collector line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "OUTB5")
				(number "11")
			)
			(pin open_collector line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "OUTR6")
				(number "15")
			)
			(pin open_collector line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "OUTG6")
				(number "16")
			)
			(pin open_collector line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "OUTB6")
				(number "14")
			)
			(pin open_collector line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "OUTR7")
				(number "18")
			)
			(pin open_collector line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "OUTG7")
				(number "19")
			)
			(pin open_collector line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "OUTB7")
				(number "17")
			)
		)
		(symbol "TLC5951RHA_1_1"
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "GSSOUT")
				(number "5")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "DCSOUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLC5957RTQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 67.31 0)
		)
		(property "Value" "TLC5957RTQ"
			(at 1.27 -67.31 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_8x8mm_P0.5mm_EP5.6x5.6mm_ThermalVias"
			(at 3.81 -71.12 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc5957.pdf"
			(at 0 -78.74 0)
		)
		(property "Description" "48-channel, 16bit ES-PWM LED driver with Pre-charge FET, LED OPEN Detection and Caterpillar Cancelling, QFN-56"
			(at 0 0 0)
		)
		(property "ki_keywords" "led driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TLC5957RTQ_0_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "GCLK")
				(number "29")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "LAT")
				(number "27")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SCLK")
				(number "28")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SIN")
				(number "26")
			)
			(pin passive line
				(at -12.7 -53.34 0)
				(length 2.54)
				(name "IREF")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -68.58 90)
				(length 2.54)
				(name "IREFGND")
				(number "56")
			)
			(pin power_in line
				(at 0 68.58 270)
				(length 2.54)
				(name "VCC")
				(number "43")
			)
			(pin power_in line
				(at 0 -68.58 90)
				(length 2.54)
				(name "GND")
				(number "57")
			)
			(pin open_collector line
				(at 12.7 63.5 180)
				(length 2.54)
				(name "OUTR0")
				(number "8")
			)
			(pin open_collector line
				(at 12.7 60.96 180)
				(length 2.54)
				(name "OUTG0")
				(number "9")
			)
			(pin open_collector line
				(at 12.7 58.42 180)
				(length 2.54)
				(name "OUTB0")
				(number "10")
			)
			(pin open_collector line
				(at 12.7 55.88 180)
				(length 2.54)
				(name "OUTR1")
				(number "11")
			)
			(pin open_collector line
				(at 12.7 53.34 180)
				(length 2.54)
				(name "OUTG1")
				(number "12")
			)
			(pin open_collector line
				(at 12.7 50.8 180)
				(length 2.54)
				(name "OUTB1")
				(number "13")
			)
			(pin open_collector line
				(at 12.7 48.26 180)
				(length 2.54)
				(name "OUTR2")
				(number "14")
			)
			(pin open_collector line
				(at 12.7 45.72 180)
				(length 2.54)
				(name "OUTG2")
				(number "15")
			)
			(pin open_collector line
				(at 12.7 43.18 180)
				(length 2.54)
				(name "OUTB2")
				(number "16")
			)
			(pin open_collector line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "OUTR3")
				(number "17")
			)
			(pin open_collector line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "OUTG3")
				(number "18")
			)
			(pin open_collector line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "OUTB3")
				(number "19")
			)
			(pin open_collector line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "OUTR4")
				(number "20")
			)
			(pin open_collector line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "OUTG4")
				(number "21")
			)
			(pin open_collector line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "OUTB4")
				(number "22")
			)
			(pin open_collector line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "OUTR5")
				(number "23")
			)
			(pin open_collector line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "OUTG5")
				(number "24")
			)
			(pin open_collector line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "OUTB5")
				(number "25")
			)
			(pin open_collector line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "OUTR6")
				(number "30")
			)
			(pin open_collector line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "OUTG6")
				(number "31")
			)
			(pin open_collector line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUTB6")
				(number "32")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUTR7")
				(number "33")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUTG7")
				(number "34")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUTB7")
				(number "35")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUTR8")
				(number "36")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUTG8")
				(number "37")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUTB8")
				(number "38")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "OUTR9")
				(number "39")
			)
			(pin open_collector line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "OUTG9")
				(number "40")
			)
			(pin open_collector line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "OUTB9")
				(number "41")
			)
			(pin open_collector line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "OUTR10")
				(number "44")
			)
			(pin open_collector line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "OUTG10")
				(number "45")
			)
			(pin open_collector line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "OUTB10")
				(number "46")
			)
			(pin open_collector line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "OUTR11")
				(number "47")
			)
			(pin open_collector line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "OUTG11")
				(number "48")
			)
			(pin open_collector line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "OUTB11")
				(number "49")
			)
			(pin open_collector line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "OUTR12")
				(number "50")
			)
			(pin open_collector line
				(at 12.7 -38.1 180)
				(length 2.54)
				(name "OUTG12")
				(number "51")
			)
			(pin open_collector line
				(at 12.7 -40.64 180)
				(length 2.54)
				(name "OUTB12")
				(number "52")
			)
			(pin open_collector line
				(at 12.7 -43.18 180)
				(length 2.54)
				(name "OUTR13")
				(number "53")
			)
			(pin open_collector line
				(at 12.7 -45.72 180)
				(length 2.54)
				(name "OUTG13")
				(number "54")
			)
			(pin open_collector line
				(at 12.7 -48.26 180)
				(length 2.54)
				(name "OUTB13")
				(number "55")
			)
			(pin open_collector line
				(at 12.7 -50.8 180)
				(length 2.54)
				(name "OUTR14")
				(number "2")
			)
			(pin open_collector line
				(at 12.7 -53.34 180)
				(length 2.54)
				(name "OUTG14")
				(number "3")
			)
			(pin open_collector line
				(at 12.7 -55.88 180)
				(length 2.54)
				(name "OUTB14")
				(number "4")
			)
			(pin open_collector line
				(at 12.7 -58.42 180)
				(length 2.54)
				(name "OUTR15")
				(number "5")
			)
			(pin open_collector line
				(at 12.7 -60.96 180)
				(length 2.54)
				(name "OUTG15")
				(number "6")
			)
			(pin open_collector line
				(at 12.7 -63.5 180)
				(length 2.54)
				(name "OUTB15")
				(number "7")
			)
		)
		(symbol "TLC5957RTQ_1_1"
			(pin output line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SOUT")
				(number "42")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLC5971PWP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 19.05 0)
		)
		(property "Value" "TLC5971PWP"
			(at 1.27 -19.05 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_Mask2.75x3.43mm_ThermalVias"
			(at 1.27 -21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc5971.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "12-Channel, 16-Bit, Enhanced Spectrum, PWM, RGB, LED Driver With 3.3-V Linear Regulator, HTSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "led driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*1EP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TLC5971PWP_0_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCKI")
				(number "10")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDTI")
				(number "9")
			)
			(pin passive line
				(at -5.08 20.32 270)
				(length 2.54)
				(name "VREG")
				(number "20")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "19")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin open_collector line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "OUTR0")
				(number "3")
			)
			(pin open_collector line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "OUTG0")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "OUTB0")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUTR1")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUTG1")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTB1")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUTR2")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTG2")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUTB2")
				(number "15")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "OUTR3")
				(number "16")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "OUTG3")
				(number "17")
			)
			(pin open_collector line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "OUTB3")
				(number "18")
			)
		)
		(symbol "TLC5971PWP_1_1"
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCKO")
				(number "11")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SDTO")
				(number "12")
			)
			(pin passive line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "IREF")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLC5971RGE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 19.05 0)
		)
		(property "Value" "TLC5971RGE"
			(at 1.27 -19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024H_VQFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm_ThermalVias"
			(at 1.27 -21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc5971.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "12-Channel, 16-Bit, Enhanced Spectrum, PWM, RGB, LED Driver With 3.3-V Linear Regulator, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "led driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGE0024H*"
			(at 0 0 0)
		)
		(symbol "TLC5971RGE_0_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCKI")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDTI")
				(number "1")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SDTO")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at -7.62 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "13")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin open_collector line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "OUTR0")
				(number "19")
			)
			(pin open_collector line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "OUTG0")
				(number "20")
			)
			(pin open_collector line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "OUTB0")
				(number "21")
			)
			(pin open_collector line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUTR1")
				(number "22")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUTG1")
				(number "23")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTB1")
				(number "24")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUTR2")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTG2")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUTB2")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "OUTR3")
				(number "10")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "OUTG3")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "OUTB3")
				(number "12")
			)
		)
		(symbol "TLC5971RGE_1_1"
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SCKO")
				(number "5")
			)
			(pin passive line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "IREF")
				(number "16")
			)
			(pin passive line
				(at -5.08 20.32 270)
				(length 2.54)
				(name "VREG")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLC5973"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "TLC5973"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 11.43 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc5973.pdf"
			(at -7.62 8.89 0)
		)
		(property "Description" "3 Channel 12bit PWM constant currend LED Driver with single wire interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED current driver 12bit PWM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLC5973_0_1")
		(symbol "TLC5973_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDI")
				(number "6")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDO")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IREF")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT0")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT1")
				(number "2")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS61165DBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "TPS61165DBV"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps61165.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "High-Brightness, Constant current LED Driver, 3V to 18V input voltage range, internal switch, up to 38V/1.2A output,  SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "led backlight display driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS61165DBV_1_1"
			(pin power_in line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "CTRL")
				(number "2")
			)
			(pin output line
				(at -7.62 0 0)
				(length 2.54)
				(name "COMP")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "SW")
				(number "3")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "FB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS92692PWP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 25.4 0)
		)
		(property "Value" "TPS92692PWP"
			(at 11.43 25.4 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_Mask2.4x3.7mm"
			(at 0 3.81 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps92692-q1.pdf"
			(at 0 6.35 0)
		)
		(property "Description" "LED Driver Buck Boost Sepic Flyback, Input 4.5-65V, with PWM Dimming, HTSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Driver Buck Boost Sepic Flyback PWM Dimming"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*1EP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TPS92692PWP_0_1")
		(symbol "TPS92692PWP_1_1"
			(pin power_out line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "VREF")
				(number "2")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "DIM/PWM")
				(number "10")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "IADJ")
				(number "9")
			)
			(pin open_collector line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{FLT}")
				(number "3")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "IMON")
				(number "8")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SS")
				(number "4")
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "DM")
				(number "5")
			)
			(pin passive line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "RT")
				(number "6")
			)
			(pin passive line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "COMP")
				(number "7")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "GATE")
				(number "19")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "IS")
				(number "18")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "OV")
				(number "15")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CSP")
				(number "14")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CSN")
				(number "13")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PDRV")
				(number "12")
			)
			(pin power_out line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
			(pin passive line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "SLOPE")
				(number "16")
			)
			(pin passive line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "RAMP")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "WS2811"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "WS2811"
			(at 5.08 6.35 0)
		)
		(property "Footprint" ""
			(at -7.62 3.81 0)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/datasheets/WS2811.pdf"
			(at -5.08 6.35 0)
		)
		(property "Description" "3-Channel 8-Bit PWM LED Driver, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "PWM LED driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "WS2811_0_1")
		(symbol "WS2811_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DIN")
				(number "6")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "DO")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SET")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTR")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUTG")
				(number "2")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "iC-HTG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "iC-HTG"
			(at 7.62 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:HVQFN-24-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 38.1 -29.21 0)
		)
		(property "Datasheet" "https://www.ichaus.de/product/ic-htg/#documents"
			(at 34.29 -33.02 0)
		)
		(property "Description" "CW power laser diode driver, external driver transistor, integrated DAC & ADC, SPI or I2C, 3 to 24V supply, temperature monitor, HVQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "ichaus continous wave monitoring adc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HVQFN*1EP*4x4mm*P0.5mm*EP2.5x2.5mm*"
			(at 0 0 0)
		)
		(symbol "iC-HTG_0_0"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "MOD")
				(number "12")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "ID")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "MISO/SDA")
				(number "8")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "EC")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "ANIN")
				(number "9")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VB")
				(number "24")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "20")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VBL")
				(number "17")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "CI")
				(number "13")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "CIL")
				(number "14")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "MCH")
				(number "10")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "MCL")
				(number "11")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "MR")
				(number "19")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "MD")
				(number "18")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "DCO")
				(number "21")
			)
		)
		(symbol "iC-HTG_1_0"
			(pin open_collector line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "~{CHK}")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{CS}/A1")
				(number "3")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "MOSI/A0")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCLK/SCL")
				(number "7")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "INS")
				(number "22")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{STBY}")
				(number "2")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "VRP")
				(number "16")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "VRN")
				(number "15")
			)
			(pin output line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "VDD")
				(number "23")
			)
		)
		(symbol "iC-HTG_1_1")
		(embedded_fonts no)
	)
	(symbol "AP3019AKTTR"
		(extends "AP3019AKTR")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "AP3019AKTTR"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP3019A.pdf"
			(at 1.27 -12.7 0)
		)
		(property "Description" "1.2MHz White LED Boost Drivers with Built-in Schottky, 2.5..16Vin, <30Vout, ThinSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switching driver backlight"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "CH455H"
		(extends "CH455K")
		(property "Reference" "U"
			(at 5.08 24.13 0)
		)
		(property "Value" "CH455H"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_SO:SOP-18_7.495x11.515mm_P1.27mm"
			(at 0.508 0 0)
		)
		(property "Datasheet" "https://www.wch-ic.com/products/CH455.html"
			(at 0.762 0 0)
		)
		(property "Description" "Digital tube driver and keyboard scan (common cathode only), with interrupt/current setting, SOP-18"
			(at 0.254 0 0)
		)
		(property "ki_keywords" "WCH Nixie I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*-18*"
			(at 0 0 0)
		)
	)
	(symbol "HV9922N8-G"
		(extends "HV9921N8-G")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "HV9922N8-G"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005311A.pdf"
			(at 0 0 0)
		)
		(property "Description" "3pin Constant Current 50mA LED Driver, SOT89"
			(at 0 0 0)
		)
		(property "ki_keywords" "CC LED Driver High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "HV9923N8-G"
		(extends "HV9921N8-G")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "HV9923N8-G"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-89-3"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005311A.pdf"
			(at 0 0 0)
		)
		(property "Description" "3pin Constant Current 30mA LED Driver, SOT89"
			(at 0 0 0)
		)
		(property "ki_keywords" "CC LED Driver High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?89*"
			(at 0 0 0)
		)
	)
	(symbol "IS31FL3216A"
		(extends "IS31FL3216")
		(property "Reference" "U"
			(at -12.7 23.495 0)
		)
		(property "Value" "IS31FL3216A"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.4mm_EP2.4x2.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.issi.com/WW/pdf/IS31FL3216A.pdf"
			(at 0 0 0)
		)
		(property "Description" "16 channel LED controller with audio modulation mode, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "led pwm audio"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "IS31FL3236A-TQ"
		(extends "IS31FL3236-TQ")
		(property "Reference" "U"
			(at -8.89 46.99 0)
		)
		(property "Value" "IS31FL3236A-TQ"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48-1EP_7x7mm_P0.5mm_EP4.11x4.11mm"
			(at 2.54 -49.53 0)
		)
		(property "Datasheet" "https://www.lumissil.com/assets/pdf/core/IS31FL3236A_DS.pdf"
			(at 0 -62.23 0)
		)
		(property "Description" "36 LED matrix driver with 8-bit PWM, 3kHz/22kHz, eTQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "led matrix pwm"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT3465A"
		(extends "LT3465")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "LT3465A"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3465fa.pdf"
			(at 1.27 -12.7 0)
		)
		(property "Description" "2.4MHz White LED Drivers with Built-in Schottky in ThinSOT"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switching LED driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LT3755xMSE-2"
		(extends "LT3755xMSE")
		(property "Reference" "U"
			(at -13.97 19.05 0)
		)
		(property "Value" "LT3755xMSE-2"
			(at 8.89 19.05 0)
		)
		(property "Footprint" "Package_SO:MSOP-16-1EP_3x4.039mm_P0.5mm_EP1.651x2.845mm"
			(at 25.4 -19.05 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/37551fd.pdf"
			(at -1.27 -27.94 0)
		)
		(property "Description" "40 Vin, 75 Vout, DC/DC LED Controllers, Improved Open Led Status Pin, MSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost Buck Buck-Boost SEPIC Flyback"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x4.039mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT3755xUD-2"
		(extends "LT3755xUD")
		(property "Reference" "U"
			(at -13.97 19.05 0)
		)
		(property "Value" "LT3755xUD-2"
			(at 8.89 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.45x1.45mm"
			(at 26.67 -19.05 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/37551fd.pdf"
			(at -1.27 -27.94 0)
		)
		(property "Description" "40 Vin, 75 Vout, DC/DC LED Controllers, Improved Open led Status pin, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost Buck Buck-Boost SEPIC Flyback"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT3756xMSE"
		(extends "LT3755xMSE")
		(property "Reference" "U"
			(at -13.97 19.05 0)
		)
		(property "Value" "LT3756xMSE"
			(at 8.89 19.05 0)
		)
		(property "Footprint" "Package_SO:MSOP-16-1EP_3x4.039mm_P0.5mm_EP1.651x2.845mm"
			(at 25.4 -19.05 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/375612fb.pdf"
			(at -1.27 -27.94 0)
		)
		(property "Description" "100 Vin, 100 Vout, DC/DC LED Controllers, Hysteresis Open led Status pin, MSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost Buck Buck-Boost SEPIC Flyback"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x4.039mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT3756xMSE-1"
		(extends "LT3755xMSE-1")
		(property "Reference" "U"
			(at -13.97 19.05 0)
		)
		(property "Value" "LT3756xMSE-1"
			(at 8.89 19.05 0)
		)
		(property "Footprint" "Package_SO:MSOP-16-1EP_3x4.039mm_P0.5mm_EP1.651x2.845mm"
			(at 25.4 -19.05 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/375612fb.pdf"
			(at -1.27 -27.94 0)
		)
		(property "Description" "100 Vin, 100 Vout, DC/DC LED Controllers, Frequency Synchronisation, MSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost Buck Buck-Boost SEPIC Flyback"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x4.039mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT3756xMSE-2"
		(extends "LT3755xMSE")
		(property "Reference" "U"
			(at -13.97 19.05 0)
		)
		(property "Value" "LT3756xMSE-2"
			(at 8.89 19.05 0)
		)
		(property "Footprint" "Package_SO:MSOP-16-1EP_3x4.039mm_P0.5mm_EP1.651x2.845mm"
			(at 25.4 -19.05 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/375612fb.pdf"
			(at -1.27 -27.94 0)
		)
		(property "Description" "100 Vin, 100 Vout, DC/DC LED Controllers, Improved Open Led Status Pin, MSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost Buck Buck-Boost SEPIC Flyback"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x4.039mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT3756xUD"
		(extends "LT3755xUD")
		(property "Reference" "U"
			(at -13.97 19.05 0)
		)
		(property "Value" "LT3756xUD"
			(at 8.89 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.45x1.45mm"
			(at 26.67 -19.05 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/375612fb.pdf"
			(at -1.27 -27.94 0)
		)
		(property "Description" "100 Vin, 100 Vout, DC/DC LED Controller, Hysteresis Open led Status pins, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost Buck Buck-Boost SEPIC Flyback"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT3756xUD-1"
		(extends "LT3755xUD-1")
		(property "Reference" "U"
			(at -13.97 19.05 0)
		)
		(property "Value" "LT3756xUD-1"
			(at 8.89 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.45x1.45mm"
			(at 26.67 -19.05 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/375612fb.pdf"
			(at -1.27 -27.94 0)
		)
		(property "Description" "100 Vin, 100 Vout, DC/DC LED Controllers, Frequency Synchronisation, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost Buck Buck-Boost SEPIC Flyback"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT3756xUD-2"
		(extends "LT3755xUD")
		(property "Reference" "U"
			(at -13.97 19.05 0)
		)
		(property "Value" "LT3756xUD-2"
			(at 8.89 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.45x1.45mm"
			(at 26.67 -19.05 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/375612fb.pdf"
			(at -1.27 -27.94 0)
		)
		(property "Description" "100 Vin, 100 Vout, DC/DC LED Controllers, Improved Open led Status pin, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Boost Buck Buck-Boost SEPIC Flyback"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX7221xRG"
		(extends "MAX7221xNG")
		(property "Reference" "U"
			(at -6.35 24.13 0)
		)
		(property "Value" "MAX7221xRG"
			(at 1.27 25.4 0)
		)
		(property "Footprint" "Package_DIP:DIP-24_W7.62mm"
			(at -1.27 1.27 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX7219-MAX7221.pdf"
			(at 1.27 -3.81 0)
		)
		(property "Description" "Serially Interfaced, 8-Digit LED Display Driver, CDIP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "spi qspi microwire"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MPQ3362GJ-AEC1"
		(extends "MP3362GJ")
		(property "Reference" "U"
			(at 2.54 6.35 0)
		)
		(property "Value" "MPQ3362GJ-AEC1"
			(at 8.89 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-8"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.monolithicpower.com/en/documentview/productdocument/index/version/2/document_type/Datasheet/lang/en/sku/MPQ3362GJ-AEC1/document_id/9116/"
			(at 2.54 -11.43 0)
		)
		(property "Description" "Single string LED driver, 3V to 36V input, 4A peak current limit, 200Khz to 2Mhz, AEC1-Q100, SOT23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED driver AEC AEC1-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "STP08CP05M"
		(extends "STP08CP05B")
		(property "Reference" "U"
			(at -7.62 19.304 0)
		)
		(property "Value" "STP08CP05M"
			(at 1.27 19.304 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stp08cp05.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit constant current LED sink driver, 5..100mA output current, 20V driving capability, 3.0..5.5V power supply, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Shift Register"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*3.9*9.9*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "STP08CP05T"
		(extends "STP08CP05B")
		(property "Reference" "U"
			(at -7.62 19.304 0)
		)
		(property "Value" "STP08CP05T"
			(at 1.27 19.304 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stp08cp05.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit constant current LED sink driver, 5..100mA output current, 20V driving capability, 3.0..5.5V power supply, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Shift Register"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSSOP*4.4*5**P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STP16CP05P"
		(extends "STP16CP05M")
		(property "Reference" "U"
			(at -7.62 29.464 0)
		)
		(property "Value" "STP16CP05P"
			(at 1.27 29.464 0)
		)
		(property "Footprint" "Package_SO:QSOP-24_3.9x8.7mm_P0.635mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stp16cp05.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-bit constant current LED sink driver, 5..100mA output current, 20V driving capability, 3.0..5.5V power supply, QSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Shift Register"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QSOP*3.9*8.*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "STP16CP05T"
		(extends "STP16CP05M")
		(property "Reference" "U"
			(at -7.62 29.464 0)
		)
		(property "Value" "STP16CP05T"
			(at 1.27 29.464 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stp16cp05.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-bit constant current LED sink driver, 5..100mA output current, 20V driving capability, 3.0..5.5V power supply, SOIC-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Shift Register"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSSOP*4.4*7.8*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STP16CPC26M"
		(extends "STP16CPC26T")
		(property "Reference" "U"
			(at -7.62 28.956 0)
		)
		(property "Value" "STP16CPC26M"
			(at 0.762 29.21 0)
		)
		(property "Footprint" "Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/STP16CPC26.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-bit constant current LED sink driver, 5..90mA output current, 20V driving capability, 3..5.5V power supply, SOIC-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Shift Register "
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*7.5*15.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "STP16CPC26P"
		(extends "STP16CPC26T")
		(property "Reference" "U"
			(at -7.62 28.956 0)
		)
		(property "Value" "STP16CPC26P"
			(at 0.762 29.21 0)
		)
		(property "Footprint" "Package_SO:QSOP-24_3.9x8.7mm_P0.635mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/STP16CPC26.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-bit constant current LED sink driver, 5..90mA output current, 20V driving capability, 3..5.5V power supply, QSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Shift Register "
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QSOP*3.9*8.*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLC5917"
		(extends "TLC5916")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "TLC5917"
			(at -7.62 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlc5917.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "8-Channel Constant-Current LED Sink Driver, Short to VLED detection"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED Constant-Current Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLC5951RTA"
		(extends "TLC5951RHA")
		(property "Reference" "U"
			(at 2.54 34.29 0)
		)
		(property "Value" "TLC5951RTA"
			(at 1.27 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHA0040B_VQFN-40-1EP_6x6mm_P0.5mm_EP4.15x4.15mm_ThermalVias"
			(at 0 -44.45 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc5951.pdf"
			(at 0 -43.18 0)
		)
		(property "Description" "24-Channel, 12-Bit PWM LED Driver With 7-Bit Dot Correction and 3-Group, 8-Bit Global Brightness Control, Texas S-PVQFN-N40"
			(at 0 0 0)
		)
		(property "ki_keywords" "led driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RHA0040B*"
			(at 0 0 0)
		)
	)
)
