(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "A4950E"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "A4950E"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.3mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A4950-Datasheet.ashx"
			(at -7.62 8.89 0)
		)
		(property "Description" "Full-Bridge, DMOS PWM, Motor Driver, 40V, 3.5A, -40 to +85C"
			(at 0 0 0)
		)
		(property "ki_keywords" "full-bridge h-bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC-*1EP*"
			(at 0 0 0)
		)
		(symbol "A4950E_0_1")
		(symbol "A4950E_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN1")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN2")
				(number "2")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VREF")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBB")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "PAD")
				(number "9")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT1")
				(number "6")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "8")
			)
			(pin power_in line
				(at 10.16 0 180)
				(length 2.54)
				(name "LSS")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "A4952_LY"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "A4952_LY"
			(at 5.08 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-10-1EP_3x3mm_P0.5mm_EP1.73x1.98mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "www.allegromicro.com/~/media/Files/Datasheets/A4952-3-Datasheet.ashx?la=en"
			(at -7.62 11.43 0)
		)
		(property "Description" "Full-Bridge, DMOS PWM, Motor Driver, 40V, 2A, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Full-bridge h-bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "A4952_LY_0_1")
		(symbol "A4952_LY_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IN1")
				(number "4")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN2")
				(number "3")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "VREF")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RTRY")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VBB")
				(number "6")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "PAD")
				(number "11")
			)
			(pin power_out line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUT1")
				(number "7")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT2")
				(number "9")
			)
			(pin power_in line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "LSS")
				(number "8")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{FLTn}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "A4954"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 11.43 0)
		)
		(property "Value" "A4954"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16-1EP_4.4x5mm_P0.65mm_EP3x3mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.allegromicro.com/-/media/Files/Datasheets/A4954-Datasheet.ashx"
			(at -17.78 -12.7 0)
		)
		(property "Description" "Fullbridge PWM Motor Driver, UVLO, OCP, Current Limit, Short Circuit Protection, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fullbridge, Stepper Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*1EP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "A4954_0_1")
		(symbol "A4954_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "IN1")
				(number "6")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "IN2")
				(number "5")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "VREF12")
				(number "7")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "IN3")
				(number "3")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "IN4")
				(number "4")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "VREF34")
				(number "2")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "VBB")
				(number "16")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VBB")
				(number "9")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin power_out line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "OUT1")
				(number "10")
			)
			(pin power_out line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUT2")
				(number "12")
			)
			(pin power_in line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "LSS12")
				(number "11")
			)
			(pin power_out line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUT3")
				(number "13")
			)
			(pin power_out line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OUT4")
				(number "15")
			)
			(pin power_in line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "LSS34")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AMT49413"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 44.45 0)
		)
		(property "Value" "AMT49413"
			(at -10.16 -45.72 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm_ThermalVias"
			(at 22.86 48.26 0)
		)
		(property "Datasheet" "https://www.allegromicro.com/-/media/Files/Datasheets/AMT49413-Datasheet.ashx"
			(at -13.97 44.45 0)
		)
		(property "Description" "3-Phase BLDC Controller and MOSFET Driver, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "BLDC 3-Phase"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AMT49413_0_1")
		(symbol "AMT49413_1_1"
			(pin power_out line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "V5")
				(number "4")
			)
			(pin power_out line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "V5DB")
				(number "3")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "MODE")
				(number "15")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "COAST")
				(number "46")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BRAKE")
				(number "8")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "~{RESET}")
				(number "2")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "DIR")
				(number "9")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "H1")
				(number "10")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "H2")
				(number "11")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "H3")
				(number "12")
			)
			(pin passive line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "RDEAD")
				(number "18")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PWM")
				(number "14")
			)
			(pin output line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "TACHO")
				(number "7")
			)
			(pin output line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "DIRO")
				(number "44")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "ESF")
				(number "39")
			)
			(pin open_collector line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "FF1")
				(number "6")
			)
			(pin open_collector line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "FF2")
				(number "5")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "RC")
				(number "16")
			)
			(pin input line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "VDSTH")
				(number "23")
			)
			(pin passive line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "CP1")
				(number "42")
			)
			(pin passive line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "CP2")
				(number "43")
			)
			(pin input line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "TEST")
				(number "17")
			)
			(pin no_connect line
				(at -7.62 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "N.C.")
				(number "48")
			)
			(pin no_connect line
				(at -5.08 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "N.C.")
				(number "1")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VBB")
				(number "45")
			)
			(pin no_connect line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "N.C.")
				(number "13")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "41")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDRAIN")
				(number "24")
			)
			(pin no_connect line
				(at 5.08 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "N.C.")
				(number "37")
			)
			(pin no_connect line
				(at 7.62 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "N.C.")
				(number "47")
			)
			(pin power_out line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "VREG")
				(number "40")
			)
			(pin output line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "GHA")
				(number "32")
			)
			(pin passive line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "CA")
				(number "33")
			)
			(pin input line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "SA")
				(number "31")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "GLA")
				(number "36")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "GHB")
				(number "29")
			)
			(pin passive line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "CB")
				(number "30")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "SB")
				(number "28")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "GLB")
				(number "35")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "GHC")
				(number "26")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "CC")
				(number "27")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "SC")
				(number "25")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "GLC")
				(number "34")
			)
			(pin input line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "LSS")
				(number "38")
			)
			(pin input line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "REF")
				(number "20")
			)
			(pin input line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "CSOUT")
				(number "19")
			)
			(pin input line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "CSP")
				(number "22")
			)
			(pin input line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "CSN")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8308"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 36.83 0)
		)
		(property "Value" "DRV8308"
			(at -17.78 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RHA0040E_VQFN-40-1EP_6x6mm_P0.5mm_EP3.52x2.62mm"
			(at 1.27 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv8308.pdf"
			(at -17.78 36.83 0)
		)
		(property "Description" "Brushless DC motor controller, closed loop, hall sensor inputs, current limiting, SPI interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "bldc mosfet-driver hall-sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RHA0040E*"
			(at 0 0 0)
		)
		(symbol "DRV8308_0_0"
			(text "Hall Sensors"
				(at 16.51 -2.54 0)
			)
			(text "Phase U"
				(at 17.145 25.4 0)
			)
			(text "Phase V"
				(at 17.145 15.24 0)
			)
			(text "Phase W"
				(at 17.145 5.08 0)
			)
		)
		(symbol "DRV8308_0_1")
		(symbol "DRV8308_1_1"
			(pin passive line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "CP1")
				(number "30")
			)
			(pin passive line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "CP2")
				(number "29")
			)
			(pin input line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "SCLK")
				(number "11")
			)
			(pin input line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "SCS")
				(number "12")
			)
			(pin input line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "SDATAI")
				(number "14")
			)
			(pin output line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "SDATAO")
				(number "15")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "SMODE")
				(number "13")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RESET")
				(number "23")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "BRAKE")
				(number "20")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "CLKIN")
				(number "19")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "DIR")
				(number "21")
			)
			(pin input line
				(at -20.32 0 0)
				(length 2.54)
				(name "ENABLE")
				(number "22")
			)
			(pin output line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "FGFB")
				(number "8")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "FGINN_TACH")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "FGINP")
				(number "10")
			)
			(pin output line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "FGOUT")
				(number "16")
			)
			(pin output line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "~{FAULTn}")
				(number "17")
			)
			(pin output line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "~{LOCKn}")
				(number "18")
			)
			(pin passive line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VINT")
				(number "25")
			)
			(pin passive line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VCP")
				(number "28")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "26")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VM")
				(number "27")
			)
			(pin power_out line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VSW")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "41")
			)
			(pin power_out line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VREG")
				(number "24")
			)
			(pin output line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "UHSG")
				(number "32")
			)
			(pin input line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "U")
				(number "33")
			)
			(pin output line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "ULSG")
				(number "34")
			)
			(pin output line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "VHSG")
				(number "35")
			)
			(pin input line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "V")
				(number "36")
			)
			(pin output line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "VLSG")
				(number "37")
			)
			(pin output line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "WHSG")
				(number "38")
			)
			(pin input line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "W")
				(number "39")
			)
			(pin output line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "WLSG")
				(number "40")
			)
			(pin input line
				(at 20.32 0 180)
				(length 2.54)
				(name "ISEN")
				(number "31")
			)
			(pin input line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "UHP")
				(number "1")
			)
			(pin input line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "UHN")
				(number "2")
			)
			(pin input line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "VHP")
				(number "3")
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "VHN")
				(number "4")
			)
			(pin input line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "WHP")
				(number "5")
			)
			(pin input line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "WHN")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8412"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 -3.81 90)
		)
		(property "Value" "DRV8412"
			(at 1.27 -3.81 90)
		)
		(property "Footprint" "Package_SO:HTSSOP-44-1EP_6.1x14mm_P0.635mm_EP5.2x14mm_Mask4.31x8.26mm_ThermalVias"
			(at 8.89 -1.27 90)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/DRV8412"
			(at 6.35 -1.27 90)
		)
		(property "Description" "Dual Full-Bridge PWM Motor Driver 50V 2x6A Peak, HTSSOP-44 EP ThermalVias"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Full-Bridge PWM Motor Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*HTSSOP*44*6.1x14mm*P0.635mm*EP*ThermalVias*"
			(at 0 0 0)
		)
		(symbol "DRV8412_0_1")
		(symbol "DRV8412_1_0"
			(pin open_collector line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "~{OTW}")
				(number "21")
			)
			(pin open_collector line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "18")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "~{RESET_AB}")
				(number "16")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "~{RESET_CD}")
				(number "6")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PWM_A")
				(number "17")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PWM_B")
				(number "15")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PWM_C")
				(number "7")
			)
			(pin input line
				(at -20.32 0 0)
				(length 2.54)
				(name "PWM_D")
				(number "5")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "M1")
				(number "8")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "M2")
				(number "9")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "M3")
				(number "10")
			)
			(pin input line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "OC_ADJ")
				(number "14")
			)
			(pin output line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "VREG")
				(number "11")
			)
			(pin power_in line
				(at -15.24 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at -15.24 -38.1 90)
				(length 2.54)
				(name "AGND")
				(number "12")
			)
			(pin power_in line
				(at -12.7 38.1 270)
				(length 2.54)
				(name "GVDD_A")
				(number "23")
			)
			(pin power_in line
				(at -10.16 38.1 270)
				(length 2.54)
				(name "GVDD_B")
				(number "22")
			)
			(pin power_in line
				(at -10.16 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "GVDD_C")
				(number "1")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "GVDD_D")
				(number "44")
			)
			(pin passive line
				(at -5.08 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "NC/GND")
				(number "19")
			)
			(pin passive line
				(at -5.08 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "NC/GND")
				(number "20")
			)
			(pin passive line
				(at -5.08 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "NC/GND")
				(number "25")
			)
			(pin passive line
				(at -5.08 -38.1 90)
				(length 2.54)
				(name "NC/GND")
				(number "3")
			)
			(pin passive line
				(at -5.08 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "NC/GND")
				(number "4")
			)
			(pin passive line
				(at -5.08 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "NC/GND")
				(number "42")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "EP")
				(number "45")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "PVDD_A")
				(number "26")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "PVDD_A")
				(number "27")
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "PVDD_B")
				(number "32")
			)
			(pin power_in line
				(at 7.62 -38.1 90)
				(length 2.54)
				(name "GND_A")
				(number "29")
			)
			(pin power_in line
				(at 10.16 38.1 270)
				(length 2.54)
				(name "PVDD_C")
				(number "35")
			)
			(pin power_in line
				(at 10.16 -38.1 90)
				(length 2.54)
				(name "GND_B")
				(number "30")
			)
			(pin power_in line
				(at 12.7 38.1 270)
				(length 2.54)
				(name "PVDD_D")
				(number "40")
			)
			(pin power_in line
				(at 12.7 -38.1 90)
				(length 2.54)
				(name "GND_C")
				(number "37")
			)
			(pin power_in line
				(at 15.24 38.1 270)
				(length 2.54)
				(name "PVDD_D")
				(number "41")
			)
			(pin power_in line
				(at 15.24 -38.1 90)
				(length 2.54)
				(name "GND_D")
				(number "38")
			)
			(pin input line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "BST_A")
				(number "24")
			)
			(pin output line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "OUT_A")
				(number "28")
			)
			(pin input line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "BST_B")
				(number "33")
			)
			(pin output line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "OUT_B")
				(number "31")
			)
			(pin input line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "BST_C")
				(number "34")
			)
			(pin output line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "OUT_C")
				(number "36")
			)
			(pin input line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "BST_D")
				(number "43")
			)
			(pin output line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "OUT_D")
				(number "39")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8432"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 -3.81 90)
		)
		(property "Value" "DRV8432"
			(at 1.27 -3.81 90)
		)
		(property "Footprint" "Package_SO:HSOP-36-1EP_11.0x15.9mm_P0.65mm_SlugUp"
			(at 6.35 1.27 90)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/DRV8412"
			(at 8.89 -2.54 90)
		)
		(property "Description" "Dual Full-Bridge PWM Motor Driver 50V 2x12A Peak, HSOP-36, Slug-up"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Full-Bridge PWM Motor Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*HSOP*11.0x15.9mm*P0.65mm*SlugUp*"
			(at 0 0 0)
		)
		(symbol "DRV8432_0_1")
		(symbol "DRV8432_1_0"
			(pin open_collector line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "~{OTW}")
				(number "2")
			)
			(pin open_collector line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "3")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "~{RESET_AB}")
				(number "5")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "~{RESET_CD}")
				(number "15")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PWM_A")
				(number "4")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PWM_B")
				(number "6")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PWM_C")
				(number "14")
			)
			(pin input line
				(at -20.32 0 0)
				(length 2.54)
				(name "PWM_D")
				(number "16")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "M1")
				(number "13")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "M2")
				(number "12")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "M3")
				(number "11")
			)
			(pin input line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "OC_ADJ")
				(number "7")
			)
			(pin output line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "VREG")
				(number "10")
			)
			(pin power_in line
				(at -15.24 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -15.24 -38.1 90)
				(length 2.54)
				(name "AGND")
				(number "9")
			)
			(pin power_in line
				(at -12.7 38.1 270)
				(length 2.54)
				(name "GVDD_A")
				(number "36")
			)
			(pin power_in line
				(at -10.16 38.1 270)
				(length 2.54)
				(name "GVDD_B")
				(number "1")
			)
			(pin power_in line
				(at -10.16 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "GVDD_C")
				(number "18")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "GVDD_D")
				(number "19")
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "PVDD_A")
				(number "34")
			)
			(pin power_in line
				(at 7.62 -38.1 90)
				(length 2.54)
				(name "GND_A")
				(number "32")
			)
			(pin power_in line
				(at 10.16 38.1 270)
				(length 2.54)
				(name "PVDD_B")
				(number "29")
			)
			(pin power_in line
				(at 10.16 -38.1 90)
				(length 2.54)
				(name "GND_B")
				(number "31")
			)
			(pin power_in line
				(at 12.7 38.1 270)
				(length 2.54)
				(name "PVDD_C")
				(number "26")
			)
			(pin power_in line
				(at 12.7 -38.1 90)
				(length 2.54)
				(name "GND_C")
				(number "24")
			)
			(pin power_in line
				(at 15.24 38.1 270)
				(length 2.54)
				(name "PVDD_D")
				(number "21")
			)
			(pin power_in line
				(at 15.24 -38.1 90)
				(length 2.54)
				(name "GND_D")
				(number "23")
			)
			(pin input line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "BST_A")
				(number "35")
			)
			(pin output line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "OUT_A")
				(number "33")
			)
			(pin input line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "BST_B")
				(number "28")
			)
			(pin output line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "OUT_B")
				(number "30")
			)
			(pin input line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "BST_C")
				(number "27")
			)
			(pin output line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "OUT_C")
				(number "25")
			)
			(pin input line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "BST_D")
				(number "20")
			)
			(pin output line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "OUT_D")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8461SPWP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 21.59 0)
		)
		(property "Value" "DRV8461SPWP"
			(at 12.7 21.59 0)
		)
		(property "Footprint" "Package_SO:Texas_PWP0020A"
			(at 20.32 -26.67 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/drv8461.pdf"
			(at 20.32 -29.21 0)
		)
		(property "Description" "65V, 3A SPI Stepper motor controller with integrated MOSFETs, automatic torque, automatic microstep, HTSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "texas ti microstep driver silent STEP DIR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*PWP*"
			(at 0 0 0)
		)
		(symbol "DRV8461SPWP_0_0"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "VREF")
				(number "17")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SCLK")
				(number "22")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDI")
				(number "21")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDO")
				(number "20")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{SCS}")
				(number "18")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "STEP")
				(number "23")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "DIR")
				(number "24")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "ENABLE")
				(number "25")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{SLEEP}")
				(number "26")
			)
			(pin open_collector line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "16")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "19")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "VCP")
				(number "1")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "AOUT1")
				(number "4")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "AOUT2")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "BOUT2")
				(number "8")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "BOUT1")
				(number "10")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "CPL")
				(number "27")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "CPH")
				(number "28")
			)
		)
		(symbol "DRV8461SPWP_1_0"
			(pin power_out line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "DVDD")
				(number "15")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 5.08 22.86 270)
				(length 2.54)
				(hide yes)
				(name "VM")
				(number "13")
			)
			(pin power_in line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "VM")
				(number "2")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "AOUT1")
				(number "5")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(hide yes)
				(name "AOUT2")
				(number "7")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(hide yes)
				(name "BOUT2")
				(number "9")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "BOUT1")
				(number "11")
			)
		)
		(symbol "DRV8461SPWP_1_1")
		(embedded_fonts no)
	)
	(symbol "DRV8662"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "DRV8662"
			(at -11.43 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGP0020D_VQFN-20-1EP_4x4mm_P0.5mm_EP2.7x2.7mm_ThermalVias"
			(at 1.27 -21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv8662.pdf"
			(at -3.81 22.86 0)
		)
		(property "Description" "Piezo Haptic Driver with Integrated Boost Converter"
			(at 0 0 0)
		)
		(property "ki_keywords" "piezo driver boost"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGP0020D*"
			(at 0 0 0)
		)
		(symbol "DRV8662_0_1")
		(symbol "DRV8662_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "SW")
				(number "7")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(hide yes)
				(name "SW")
				(number "8")
			)
			(pin output line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VPUMP")
				(number "1")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "GAIN0")
				(number "18")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "GAIN1")
				(number "19")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "20")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "IN+")
				(number "17")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "IN-")
				(number "16")
			)
			(pin no_connect line
				(at -12.7 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin power_out line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VBST")
				(number "10")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 2.54)
				(hide yes)
				(name "VBST")
				(number "11")
			)
			(pin power_in line
				(at 7.62 22.86 270)
				(length 2.54)
				(name "PVDD")
				(number "12")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "FB")
				(number "3")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "REXT")
				(number "15")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "OUT+")
				(number "13")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "OUT-")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8711"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 33.655 0)
		)
		(property "Value" "DRV8711"
			(at 0 31.75 0)
		)
		(property "Footprint" ""
			(at 0 -31.75 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/slvsc40f/slvsc40f.pdf"
			(at 0 0 0)
		)
		(property "Description" "Stepper motor controller, external N-channel MOSFET, single bipolar stepper motor, dual brushed DC motors"
			(at 0 0 0)
		)
		(property "ki_keywords" "Stepper driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP-38"
			(at 0 0 0)
		)
		(symbol "DRV8711_0_1")
		(symbol "DRV8711_1_1"
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "CP1")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "CP2")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "VCP")
				(number "3")
			)
			(pin power_in line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "VM")
				(number "4")
			)
			(pin power_out line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "V5")
				(number "6")
			)
			(pin power_in line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "VINT")
				(number "7")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "SLEEPn")
				(number "8")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "RESET")
				(number "9")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "STEP/AIN1")
				(number "10")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "DIR/AIN2")
				(number "11")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "BIN1")
				(number "12")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "BIN2")
				(number "13")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "SCLK")
				(number "14")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "SDATI")
				(number "15")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "SCS")
				(number "16")
			)
			(pin output line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "SDATO")
				(number "17")
			)
			(pin output line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "FAULTn")
				(number "18")
			)
			(pin output line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "STALLn/BEMFVn")
				(number "19")
			)
			(pin output line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "BEMF")
				(number "20")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "AOUT1")
				(number "37")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "A1HS")
				(number "36")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "A1LS")
				(number "35")
			)
			(pin input line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "AISENP")
				(number "34")
			)
			(pin input line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "AISENN")
				(number "33")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "A2LS")
				(number "32")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "A2HS")
				(number "31")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "AOUT2")
				(number "30")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "BOUT1")
				(number "28")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "B1HS")
				(number "27")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "B1LS")
				(number "26")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "BISENP")
				(number "25")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "BISENN")
				(number "24")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "B2LS")
				(number "23")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "B2HS")
				(number "22")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "BOUT2")
				(number "21")
			)
			(pin power_in line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "GND")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8800PWP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "DRV8800PWP"
			(at -12.7 13.97 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask3x3mm_ThermalVias"
			(at 30.48 13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv8801.pdf"
			(at 1.27 22.86 0)
		)
		(property "Description" "H-Bridge Motor Driver, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "H-Bridge Motor Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DRV8800PWP_0_1")
		(symbol "DRV8800PWP_1_1"
			(pin power_in line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "VBB")
				(number "9")
			)
			(pin power_in line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "VCP")
				(number "14")
			)
			(pin power_in line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "CP1")
				(number "11")
			)
			(pin power_in line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "CP2")
				(number "12")
			)
			(pin input line
				(at -17.78 0 0)
				(length 5.08)
				(name "MODE")
				(number "2")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "PHASE")
				(number "3")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "ENABLE")
				(number "6")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "~{SLEEP}")
				(number "5")
			)
			(pin no_connect line
				(at -12.7 -2.54 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 5.08)
				(name "GND(PPAD)")
				(number "17")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "13")
			)
			(pin power_out line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "OUT+")
				(number "7")
			)
			(pin power_out line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "OUT-")
				(number "10")
			)
			(pin power_out line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "SENSE")
				(number "8")
			)
			(pin open_collector line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "~{FAULT}")
				(number "1")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "VREG")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8800RTY"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "DRV8800RTY"
			(at -12.7 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RTY_WQFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm_ThermalVias"
			(at 29.21 13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv8801.pdf"
			(at 1.27 22.86 0)
		)
		(property "Description" "H-Bridge Motor Driver, WQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "H-Bridge Motor Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RTY*EP2.1x2.1mm*"
			(at 0 0 0)
		)
		(symbol "DRV8800RTY_0_1")
		(symbol "DRV8800RTY_1_1"
			(pin power_in line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "VBB")
				(number "8")
			)
			(pin power_in line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "VCP")
				(number "13")
			)
			(pin power_in line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "CP1")
				(number "10")
			)
			(pin power_in line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "CP2")
				(number "11")
			)
			(pin input line
				(at -17.78 0 0)
				(length 5.08)
				(name "MODE")
				(number "16")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "PHASE")
				(number "1")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "ENABLE")
				(number "4")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "~{SLEEP}")
				(number "3")
			)
			(pin no_connect line
				(at -12.7 -2.54 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 5.08)
				(name "GND(PPAD)")
				(number "17")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "12")
			)
			(pin power_out line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "OUT+")
				(number "6")
			)
			(pin power_out line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "OUT-")
				(number "9")
			)
			(pin power_out line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "SENSE")
				(number "7")
			)
			(pin open_collector line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "~{FAULT}")
				(number "15")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "VREG")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8801PWP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "DRV8801PWP"
			(at -12.7 13.97 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask3x3mm_ThermalVias"
			(at 30.48 13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv8801.pdf"
			(at 1.27 22.86 0)
		)
		(property "Description" "H-Bridge Motor Driver, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "H-Bridge Motor Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DRV8801PWP_0_1")
		(symbol "DRV8801PWP_1_1"
			(pin power_in line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "VBB")
				(number "9")
			)
			(pin power_in line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "VCP")
				(number "14")
			)
			(pin power_in line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "CP1")
				(number "11")
			)
			(pin power_in line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "CP2")
				(number "12")
			)
			(pin input line
				(at -17.78 0 0)
				(length 5.08)
				(name "MODE1")
				(number "2")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "MODE2")
				(number "16")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "PHASE")
				(number "3")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "ENABLE")
				(number "6")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "~{SLEEP}")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 5.08)
				(name "GND(PPAD)")
				(number "17")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "13")
			)
			(pin power_out line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "OUT+")
				(number "7")
			)
			(pin power_out line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "OUT-")
				(number "10")
			)
			(pin power_out line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "SENSE")
				(number "8")
			)
			(pin open_collector line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "~{FAULT}")
				(number "1")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "VPROPI")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8801RTY"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "DRV8801RTY"
			(at -12.7 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RTY_WQFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm_ThermalVias"
			(at 29.21 13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv8801.pdf"
			(at 1.27 20.32 0)
		)
		(property "Description" "H-Bridge Motor Driver, WQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "H-Bridge Motor Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RTY*EP2.1x2.1mm*"
			(at 0 0 0)
		)
		(symbol "DRV8801RTY_0_1")
		(symbol "DRV8801RTY_1_1"
			(pin power_in line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "VBB")
				(number "8")
			)
			(pin power_in line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "VCP")
				(number "13")
			)
			(pin power_in line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "CP1")
				(number "10")
			)
			(pin power_in line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "CP2")
				(number "11")
			)
			(pin input line
				(at -17.78 0 0)
				(length 5.08)
				(name "MODE1")
				(number "16")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "MODE2")
				(number "5")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "PHASE")
				(number "1")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "ENABLE")
				(number "4")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "~{SLEEP}")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 5.08)
				(name "GND(PPAD)")
				(number "17")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "12")
			)
			(pin power_out line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "OUT+")
				(number "6")
			)
			(pin power_out line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "OUT-")
				(number "9")
			)
			(pin power_out line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "SENSE")
				(number "7")
			)
			(pin open_collector line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "~{FAULT}")
				(number "15")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "VPROPI")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8833PW"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 16.51 0)
		)
		(property "Value" "DRV8833PW"
			(at -3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 5.08 -17.78 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv8833.pdf"
			(at 5.08 -20.32 0)
		)
		(property "Description" "Dual H-Bridge Motor Driver, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "H-bridge motor driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP-16*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DRV8833PW_0_1")
		(symbol "DRV8833PW_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "~{SLEEP}")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "VCP")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "AISEN")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "BISEN")
				(number "6")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "AIN1")
				(number "16")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "AIN2")
				(number "15")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "BIN1")
				(number "9")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "BIN2")
				(number "10")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 5.08)
				(name "VINT")
				(number "14")
			)
			(pin power_in line
				(at 7.62 17.78 270)
				(length 5.08)
				(name "VM")
				(number "12")
			)
			(pin open_collector line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "~{FAULT}")
				(number "8")
			)
			(pin power_out line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "AOUT1")
				(number "2")
			)
			(pin power_out line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "AOUT2")
				(number "4")
			)
			(pin power_out line
				(at 15.24 -7.62 180)
				(length 5.08)
				(name "BOUT1")
				(number "7")
			)
			(pin power_out line
				(at 15.24 -10.16 180)
				(length 5.08)
				(name "BOUT2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8833PWP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 16.51 0)
		)
		(property "Value" "DRV8833PWP"
			(at -3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm_ThermalVias"
			(at 5.08 -15.24 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv8833.pdf"
			(at 5.08 -17.78 0)
		)
		(property "Description" "Dual H-Bridge Motor Driver, HTSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "H-bridge motor driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP-16-1EP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DRV8833PWP_0_1")
		(symbol "DRV8833PWP_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "~{SLEEP}")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "VCP")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "AISEN")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "BISEN")
				(number "6")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "AIN1")
				(number "16")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "AIN2")
				(number "15")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "BIN1")
				(number "9")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "BIN2")
				(number "10")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 5.08)
				(name "VINT")
				(number "14")
			)
			(pin power_in line
				(at 7.62 17.78 270)
				(length 5.08)
				(name "VM")
				(number "12")
			)
			(pin open_collector line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "~{FAULT}")
				(number "8")
			)
			(pin power_out line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "AOUT1")
				(number "2")
			)
			(pin power_out line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "AOUT2")
				(number "4")
			)
			(pin power_out line
				(at 15.24 -7.62 180)
				(length 5.08)
				(name "BOUT1")
				(number "7")
			)
			(pin power_out line
				(at 15.24 -10.16 180)
				(length 5.08)
				(name "BOUT2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8833RTY"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 16.51 0)
		)
		(property "Value" "DRV8833RTY"
			(at -3.81 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RTY_WQFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm_ThermalVias"
			(at 5.08 -17.78 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv8833.pdf"
			(at 5.08 -20.32 0)
		)
		(property "Description" "Dual H-Bridge Motor Driver, WQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "H-bridge motor driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RTY*EP2.1x2.1mm*"
			(at 0 0 0)
		)
		(symbol "DRV8833RTY_0_1")
		(symbol "DRV8833RTY_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "~{SLEEP}")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "VCP")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "AISEN")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "BISEN")
				(number "4")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "AIN1")
				(number "14")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "AIN2")
				(number "13")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "BIN1")
				(number "7")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "BIN2")
				(number "8")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 5.08)
				(name "VINT")
				(number "12")
			)
			(pin power_in line
				(at 7.62 17.78 270)
				(length 5.08)
				(name "VM")
				(number "10")
			)
			(pin open_collector line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "~{FAULT}")
				(number "6")
			)
			(pin power_out line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "AOUT1")
				(number "16")
			)
			(pin power_out line
				(at 15.24 -5.08 180)
				(length 5.08)
				(name "AOUT2")
				(number "2")
			)
			(pin power_out line
				(at 15.24 -7.62 180)
				(length 5.08)
				(name "BOUT1")
				(number "5")
			)
			(pin power_out line
				(at 15.24 -10.16 180)
				(length 5.08)
				(name "BOUT2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8837C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 11.43 0)
		)
		(property "Value" "DRV8837C"
			(at -10.16 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv8837c.pdf"
			(at 0 0 0)
		)
		(property "Description" "H-Bridge driver, 1A, Low Voltage, PWM input, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "half bridge driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "DRV8837C_0_1")
		(symbol "DRV8837C_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{SLEEP}")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN1")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN2")
				(number "5")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VM")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUT1")
				(number "2")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "OUT2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8838"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 11.43 0)
		)
		(property "Value" "DRV8838"
			(at -10.16 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv8837.pdf"
			(at 0 0 0)
		)
		(property "Description" "H-Bridge driver, 1.8A, Low Voltage, PH/EN input, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "half bridge driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "DRV8838_0_1")
		(symbol "DRV8838_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{SLEEP}")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "PH")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VM")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUT1")
				(number "2")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "OUT2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8847PWP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "DRV8847PWP"
			(at 8.89 13.97 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm_ThermalVias"
			(at 0 16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/drv8847.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual H-Bridge Motor Driver, 1A, HTSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual H-Bridge motor driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*1EP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DRV8847PWP_0_1")
		(symbol "DRV8847PWP_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{SLEEP}")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "MODE")
				(number "14")
			)
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "TRQ")
				(number "11")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN1")
				(number "16")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "IN2")
				(number "15")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "IN3")
				(number "9")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "IN4")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VM")
				(number "12")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "PPAD")
				(number "17")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUT1")
				(number "2")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT2")
				(number "4")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT3")
				(number "7")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT4")
				(number "5")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "ISEN12")
				(number "3")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ISEN34")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8847PWR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "DRV8847PWR"
			(at 8.89 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/drv8847.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual H-Bridge Motor Driver, 1A, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual H-Bridge motor driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DRV8847PWR_0_1")
		(symbol "DRV8847PWR_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{SLEEP}")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "MODE")
				(number "14")
			)
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "TRQ")
				(number "11")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN1")
				(number "16")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "IN2")
				(number "15")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "IN3")
				(number "9")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "IN4")
				(number "10")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VM")
				(number "12")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUT1")
				(number "2")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT2")
				(number "4")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT3")
				(number "7")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT4")
				(number "5")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "ISEN12")
				(number "3")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ISEN34")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8847RTE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "DRV8847RTE"
			(at 8.89 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.7x1.7mm_ThermalVias"
			(at 0 16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/drv8847.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual H-Bridge Motor Driver, 1A, WQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual H-Bridge motor driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "DRV8847RTE_0_1")
		(symbol "DRV8847RTE_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{SLEEP}")
				(number "15")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "MODE")
				(number "12")
			)
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "TRQ")
				(number "9")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN1")
				(number "14")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "IN2")
				(number "13")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "IN3")
				(number "7")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "IN4")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VM")
				(number "10")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "PPAD")
				(number "17")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUT1")
				(number "16")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT2")
				(number "2")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT3")
				(number "5")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT4")
				(number "3")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "ISEN12")
				(number "1")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ISEN34")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8847SPWR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "DRV8847SPWR"
			(at 8.89 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/drv8847.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual H-Bridge Motor Driver, 1A, I2C Interface, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual H-Bridge motor driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DRV8847SPWR_0_1")
		(symbol "DRV8847SPWR_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{SLEEP}")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SDA")
				(number "14")
			)
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "11")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IN1")
				(number "16")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "IN2")
				(number "15")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "IN3")
				(number "9")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "IN4")
				(number "10")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VM")
				(number "12")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUT1")
				(number "2")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT2")
				(number "4")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT3")
				(number "7")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT4")
				(number "5")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "ISEN12")
				(number "3")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "ISEN34")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8848"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 14.224 0)
		)
		(property "Value" "DRV8848"
			(at 7.366 14.224 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16-1EP_4.4x5mm_P0.65mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv8848.pdf"
			(at -29.21 34.29 0)
		)
		(property "Description" "Dual H-Bridge motor driver, PWM controlled, single/dual brushed DC stepper, +2 to +18 VDD, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual H-Bridge motor driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*1EP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DRV8848_0_1")
		(symbol "DRV8848_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "VREF")
				(number "11")
			)
			(pin open_collector line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "8")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "~{SLEEP}")
				(number "1")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "AIN1")
				(number "16")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "AIN2")
				(number "15")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "BIN1")
				(number "9")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "BIN2")
				(number "10")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VM")
				(number "12")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "VINT")
				(number "14")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "AOUT1")
				(number "2")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "AOUT2")
				(number "4")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "AISEN")
				(number "3")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "BOUT1")
				(number "7")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "BOUT2")
				(number "5")
			)
			(pin passive line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "BISEN")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8870DDA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "DRV8870DDA"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:Texas_HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.95x4.9mm_Mask2.4x3.1mm_ThermalVias"
			(at 2.54 -2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv8870.pdf"
			(at -6.35 8.89 0)
		)
		(property "Description" "Brushed DC Motor Driver, PWM Control, 45V, 3.6A, Dynamic current limiting, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "H-bridge driver motor current limit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*HTSOP*1EP*3.9x4.9mm*P1.27mm*EP2.95x4.9mm*Mask2.4x3.1mm*"
			(at 0 0 0)
		)
		(symbol "DRV8870DDA_0_1")
		(symbol "DRV8870DDA_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN1")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN2")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "VREF")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VM")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT1")
				(number "6")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT2")
				(number "8")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "ISEN")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8871DDA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "DRV8871DDA"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:Texas_HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.95x4.9mm_Mask2.4x3.1mm_ThermalVias"
			(at 6.35 -1.27 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv8871.pdf"
			(at 6.35 -1.27 0)
		)
		(property "Description" "Brushed DC Motor Driver, PWM Control, 45V, 3.6A, Current limiting, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "H-bridge driver motor current limit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*HTSOP*1EP*3.9x4.9mm*P1.27mm*EP2.95x4.9mm*Mask2.4x3.1mm*"
			(at 0 0 0)
		)
		(symbol "DRV8871DDA_0_1")
		(symbol "DRV8871DDA_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN1")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN2")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VM")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT1")
				(number "6")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT2")
				(number "8")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "ILIM")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8872DDA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "DRV8872DDA"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:Texas_HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.95x4.9mm_Mask2.4x3.1mm_ThermalVias"
			(at 5.08 -2.54 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv8872.pdf"
			(at -6.35 8.89 0)
		)
		(property "Description" "Brushed DC Motor Driver, PWM Control, 45V, 3.6A, Current limiting, Fault Reporting, HTSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "H-bridge driver motor current limit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*HTSOP*1EP*3.9x4.9mm*P1.27mm*EP2.95x4.9mm*Mask2.4x3.1mm*"
			(at 0 0 0)
		)
		(symbol "DRV8872DDA_0_1")
		(symbol "DRV8872DDA_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN1")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN2")
				(number "2")
			)
			(pin open_collector line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "nFAULT")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VM")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT1")
				(number "6")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT2")
				(number "8")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "ISEN")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EMC2301-x-ACZL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.652 12.446 0)
		)
		(property "Value" "EMC2301-x-ACZL"
			(at 8.382 12.446 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MSLD/ProductDocuments/DataSheets/EMC2301-2-3-5-Data-Sheet-DS20006532A.pdf"
			(at 0 -21.844 0)
		)
		(property "Description" "Single RPM-Based PWM Fan Controller, up to 26 kHz, 3.3V power supply, MSOP-8"
			(at 0 -19.812 0)
		)
		(property "ki_keywords" "DRIVER MOTOR SMBus I2C 4-wire"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "EMC2301-x-ACZL_1_1"
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SMDATA")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SMCLK")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CLK")
				(number "7")
			)
			(pin open_collector line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{ALERT}")
				(number "8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PWM")
				(number "5")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "TACH")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EMC2302-x-AIZL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.652 12.446 0)
		)
		(property "Value" "EMC2302-x-AIZL"
			(at 8.382 12.446 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MSLD/ProductDocuments/DataSheets/EMC2301-2-3-5-Data-Sheet-DS20006532A.pdf"
			(at 0 -21.844 0)
		)
		(property "Description" "Dual RPM-Based PWM Fan Controller, up to 26 kHz, 3.3V power supply, MSOP-10"
			(at 0 -19.812 0)
		)
		(property "ki_keywords" "DRIVER MOTOR SMBus I2C 4-wire"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EMC2302-x-AIZL_1_1"
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SMDATA")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SMCLK")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CLK")
				(number "9")
			)
			(pin open_collector line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{ALERT}")
				(number "10")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PWM1")
				(number "5")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "TACH1")
				(number "6")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PWM2")
				(number "7")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "TACH2")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EMC2303-x-KP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.652 14.986 0)
		)
		(property "Value" "EMC2303-x-KP"
			(at 8.382 14.986 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-12-1EP_4x4mm_P0.8mm_EP2.1x2.1mm_ThermalVias"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MSLD/ProductDocuments/DataSheets/EMC2301-2-3-5-Data-Sheet-DS20006532A.pdf"
			(at 0 -26.924 0)
		)
		(property "Description" "Multiple RPM-Based PWM Fan Controller for 3 Fans, up to 26 kHz, 3.3V power supply, VQFN-12"
			(at 0 -24.892 0)
		)
		(property "ki_keywords" "DRIVER MOTOR SMBus I2C 4-wire"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*VQFN*1EP*4x4mm*P0.8mm*EP2.1x2.1mm*"
			(at 0 0 0)
		)
		(symbol "EMC2303-x-KP_1_1"
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SMDATA")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SMCLK")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "ADDR_SEL")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CLK")
				(number "9")
			)
			(pin open_collector line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{ALERT}")
				(number "10")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PWM1")
				(number "5")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "TACH1")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "PWM2")
				(number "7")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "TACH2")
				(number "8")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PWM3")
				(number "11")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "TACH3")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EMC2305-x-AP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.652 17.526 0)
		)
		(property "Value" "EMC2305-x-AP"
			(at 8.382 17.526 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGV0016A_VQFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm_ThermalVias"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MSLD/ProductDocuments/DataSheets/EMC2301-2-3-5-Data-Sheet-DS20006532A.pdf"
			(at 0 -27.94 0)
		)
		(property "Description" "Multiple RPM-Based PWM Fan Controller for 5 Fans, up to 26 kHz, 3.3V power supply, VQFN-16"
			(at 0 -25.4 0)
		)
		(property "ki_keywords" "DRIVER MOTOR SMBus I2C 4-wire"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*VQFN*1EP*4x4mm*P0.65mm*EP2.1x2.1mm*"
			(at 0 0 0)
		)
		(symbol "EMC2305-x-AP_1_1"
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SMDATA")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SMCLK")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "ADDR_SEL")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CLK")
				(number "11")
			)
			(pin open_collector line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{ALERT}")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PWM1")
				(number "5")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "TACH1")
				(number "6")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PWM2")
				(number "7")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "TACH2")
				(number "8")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "PWM3")
				(number "9")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "TACH3")
				(number "10")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PWM4")
				(number "13")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "TACH4")
				(number "14")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PWM5")
				(number "15")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "TACH5")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L293"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 26.035 0)
		)
		(property "Value" "L293"
			(at -5.08 24.13 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 6.35 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/l293.pdf"
			(at -7.62 17.78 0)
		)
		(property "Description" "Quadruple Half-H Drivers"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half-H Driver Motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "L293_0_1")
		(symbol "L293_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "1A")
				(number "2")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "2A")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "EN1,2")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "3A")
				(number "10")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "4A")
				(number "15")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "EN3,4")
				(number "9")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VCC1")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VCC2")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "1Y")
				(number "3")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "2Y")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "3Y")
				(number "11")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "4Y")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L293E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 11.43 0)
		)
		(property "Value" "L293E"
			(at 8.89 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 20.32 -12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/l293e.pdf"
			(at -10.16 -19.05 0)
		)
		(property "Description" "Push-pull four-channel driver, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half-H Driver Motor Sense"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "L293E_0_1")
		(symbol "L293E_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "EN12")
				(number "1")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "IN1")
				(number "2")
			)
			(pin output line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "OUT1")
				(number "3")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 2.54)
				(name "SENSE1")
				(number "4")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "SENSE2")
				(number "7")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "OUT2")
				(number "8")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "IN2")
				(number "9")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VS")
				(number "10")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "EN34")
				(number "11")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "IN4")
				(number "19")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUT4")
				(number "18")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "SENSE4")
				(number "17")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "SENSE3")
				(number "14")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OUT3")
				(number "13")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "IN3")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L297"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 19.05 0)
		)
		(property "Value" "L297"
			(at -6.35 16.51 0)
		)
		(property "Footprint" ""
			(at -6.35 16.51 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/cd00000063.pdf"
			(at -6.35 16.51 0)
		)
		(property "Description" "Stepper Motor Controller, DIP-20/SO-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Stepper Motor Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* SO*"
			(at 0 0 0)
		)
		(symbol "L297_0_1")
		(symbol "L297_1_0"
			(pin input line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "HALF")
				(number "19")
			)
			(pin input inverted
				(at -17.78 10.16 0)
				(length 5.08)
				(name "CLOCK")
				(number "18")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "CW")
				(number "17")
			)
			(pin input inverted
				(at -17.78 2.54 0)
				(length 5.08)
				(name "RESET")
				(number "20")
			)
			(pin input line
				(at -17.78 0 0)
				(length 5.08)
				(name "CONTROL")
				(number "11")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "SENS1")
				(number "14")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "SENS2")
				(number "13")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "OSC")
				(number "16")
			)
			(pin power_in line
				(at 5.08 20.32 270)
				(length 5.08)
				(name "Vs")
				(number "12")
			)
			(pin input line
				(at 7.62 20.32 270)
				(length 5.08)
				(name "Vref")
				(number "15")
			)
		)
		(symbol "L297_1_1"
			(pin input line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "ENABLE")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 5.08)
				(name "SYNC")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "A")
				(number "4")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "B")
				(number "6")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "C")
				(number "7")
			)
			(pin output line
				(at 17.78 0 180)
				(length 5.08)
				(name "D")
				(number "9")
			)
			(pin output inverted
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "INH1")
				(number "5")
			)
			(pin output inverted
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "INH2")
				(number "8")
			)
			(pin open_collector line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "HOME")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L298HN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "L298HN"
			(at 12.7 16.51 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead5.84mm_TabDown"
			(at 1.27 -16.51 0)
		)
		(property "Datasheet" "http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/CD00000240.pdf"
			(at 3.81 6.35 0)
		)
		(property "Description" "Dual full bridge motor driver, up to 46V, 4A, Multiwatt15-H"
			(at 0 0 0)
		)
		(property "ki_keywords" "H-bridge motor driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*TabDown*"
			(at 0 0 0)
		)
		(symbol "L298HN_0_1")
		(symbol "L298HN_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "IN1")
				(number "5")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "IN2")
				(number "7")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "EnA")
				(number "6")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "IN3")
				(number "10")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "IN4")
				(number "12")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "EnB")
				(number "11")
			)
			(pin power_in line
				(at -7.62 -17.78 90)
				(length 2.54)
				(name "SENSE_A")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -17.78 90)
				(length 2.54)
				(name "SENSE_B")
				(number "15")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "Vss")
				(number "9")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "Vs")
				(number "4")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUT1")
				(number "2")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "3")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUT3")
				(number "13")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OUT4")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "L298P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "L298P"
			(at 10.16 -16.51 0)
		)
		(property "Footprint" ""
			(at 3.81 6.35 0)
		)
		(property "Datasheet" "http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/CD00000240.pdf"
			(at 3.81 6.35 0)
		)
		(property "Description" "Dual full bridge motor driver, up to 46V, 4A"
			(at 0 0 0)
		)
		(property "ki_keywords" "H-bridge motor driver"
			(at 0 0 0)
		)
		(symbol "L298P_0_1")
		(symbol "L298P_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "IN1")
				(number "7")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "IN2")
				(number "9")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "EnA")
				(number "8")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "IN3")
				(number "13")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "IN4")
				(number "15")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "EnB")
				(number "14")
			)
			(pin power_in line
				(at -10.16 -17.78 90)
				(length 2.54)
				(name "SENSE_A")
				(number "2")
			)
			(pin power_in line
				(at -7.62 -17.78 90)
				(length 2.54)
				(name "SENSE_B")
				(number "19")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "Vss")
				(number "12")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "Vs")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "20")
			)
			(pin no_connect line
				(at 12.7 12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUT1")
				(number "4")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "5")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUT3")
				(number "16")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OUT4")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMD18200"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 19.05 0)
		)
		(property "Value" "LMD18200"
			(at 15.24 19.05 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-11_P3.4x5.08mm_StaggerOdd_Lead4.85mm_Vertical"
			(at -36.83 -34.29 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmd18200.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "3A, 55V H-Bridge, Motion Control Applications, TO-220-11"
			(at 0 0 0)
		)
		(property "ki_keywords" "H-Bridge DC stepper servo motor driver Motion Control Applications"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "LMD18200_0_1")
		(symbol "LMD18200_1_1"
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PWM")
				(number "5")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "DIRECTION")
				(number "3")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "BRAKE")
				(number "4")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "OUTPUT1")
				(number "2")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "BOOTSTRAP1")
				(number "1")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "BOOTSTRAP2")
				(number "11")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "OUTPUT2")
				(number "10")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "CURRENT_SENSE_OUTPUT")
				(number "8")
			)
			(pin open_collector line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "~{THERMAL_FLAG_OUTPUT}")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX22201"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 -13.97 0)
		)
		(property "Value" "MAX22201"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DFN_QFN:Maxim_TDFN-12-1EP_3x3mm_P0.5mm_EP1.7x2.5mm_ThermalVias"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max22201-max22207.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "36V, 3.5A Brushed Motor Driver with Integrated Current Sense and Configurable Off Time, 12-TDFN"
			(at 0 0 0)
		)
		(property "ki_keywords" "Brushed Motor Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Maxim*TDFN*12*1EP*3x3mm*P0.5mm*EP1.7x2.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX22201_0_1")
		(symbol "MAX22201_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "IN1")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IN2")
				(number "5")
			)
			(pin open_collector line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "12")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ISEN")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "ILIM")
				(number "1")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "ROFF")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GNDA")
				(number "8")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V_{M}")
				(number "10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(name "PAD")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GNDP")
				(number "3")
			)
			(pin power_out line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "V_{18}")
				(number "7")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUT1")
				(number "11")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX22202"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 -13.97 0)
		)
		(property "Value" "MAX22202"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DFN_QFN:Maxim_TDFN-12-1EP_3x3mm_P0.5mm_EP1.7x2.5mm_ThermalVias"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max22201-max22207.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "36V, 3.5A Brushed Motor Driver with Integrated Current Sense and Enable/Phase Inputs, 12-TDFN"
			(at 0 0 0)
		)
		(property "ki_keywords" "Brushed Motor Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Maxim*TDFN*12*1EP*3x3mm*P0.5mm*EP1.7x2.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX22202_0_1")
		(symbol "MAX22202_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PHASE")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "ENBL")
				(number "5")
			)
			(pin open_collector line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "12")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ISEN")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "MODE")
				(number "2")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "ILIM")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GNDA")
				(number "8")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V_{M}")
				(number "10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(name "PAD")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GNDP")
				(number "3")
			)
			(pin power_out line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "V_{18}")
				(number "7")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUT1")
				(number "11")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX22207"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 -13.97 0)
		)
		(property "Value" "MAX22207"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DFN_QFN:Maxim_TDFN-12-1EP_3x3mm_P0.5mm_EP1.7x2.5mm_ThermalVias"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max22201-max22207.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "36V, 3.5A Brushed Motor Driver with Integrated Current Sense and Current Driver Regulation output, 12-TDFN"
			(at 0 0 0)
		)
		(property "ki_keywords" "Brushed Motor Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Maxim*TDFN*12*1EP*3x3mm*P0.5mm*EP1.7x2.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX22207_0_1")
		(symbol "MAX22207_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "IN1")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IN2")
				(number "5")
			)
			(pin open_collector line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "12")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ISEN")
				(number "6")
			)
			(pin open_collector line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{CDROUT}")
				(number "2")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "ILIM")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GNDA")
				(number "8")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V_{M}")
				(number "10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(name "PAD")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GNDP")
				(number "3")
			)
			(pin power_out line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "V_{18}")
				(number "7")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUT1")
				(number "11")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MP6536DU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.144 15.748 0)
		)
		(property "Value" "MP6536DU"
			(at 5.08 15.748 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-40-1EP_5x5mm_P0.4mm_EP3.5x3.5mm_ThermalVias"
			(at -3.556 -20.32 0)
		)
		(property "Datasheet" "https://www.monolithicpower.com/en/documentview/productdocument/index/version/2/document_type/Datasheet/lang/en/sku/MP6536/document_id/3761/"
			(at 25.4 -22.606 0)
		)
		(property "Description" "3-Channel Half-Bridge Driver, 5..26V power supply, 5.5A peak current output, up to 1MHz PWM frequency, QFN-40"
			(at -0.508 -25.146 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "BLDC 3-Phase Brushless DC Motor Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*1EP*5x5mm*P0.4mm*EP3.5x3.5mm*"
			(at 0 0 0)
		)
		(symbol "MP6536DU_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PWM1")
				(number "12")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PWM2")
				(number "13")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PWM3")
				(number "16")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{SHDNB}")
				(number "15")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{STBYB}")
				(number "17")
			)
			(pin open_collector line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{FAULTB}")
				(number "14")
			)
			(pin open_collector line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{FLT2B}")
				(number "20")
			)
			(pin open_collector line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{FLT3B}")
				(number "19")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SW1")
				(number "6")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "SW1")
				(number "7")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SW2")
				(number "1")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "SW2")
				(number "2")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SW3")
				(number "29")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 2.54)
				(hide yes)
				(name "SW3")
				(number "30")
			)
			(pin open_emitter line
				(at 12.7 0 180)
				(length 2.54)
				(name "LS1")
				(number "8")
			)
			(pin open_emitter line
				(at 12.7 0 180)
				(length 2.54)
				(hide yes)
				(name "LS1")
				(number "9")
			)
			(pin open_emitter line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "LS2")
				(number "39")
			)
			(pin open_emitter line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "LS2")
				(number "40")
			)
			(pin open_emitter line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "LS3")
				(number "31")
			)
			(pin open_emitter line
				(at 12.7 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "LS3")
				(number "32")
			)
		)
		(symbol "MP6536DU_2_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "BST1")
				(number "10")
			)
			(pin power_in line
				(at -12.7 0 0)
				(length 2.54)
				(name "BST2")
				(number "38")
			)
			(pin power_in line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "BST3")
				(number "33")
			)
			(pin no_connect line
				(at -2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "VSP")
				(number "26")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "VSP")
				(number "27")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "VSP")
				(number "28")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VSP")
				(number "3")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "VSP")
				(number "4")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "VSP")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "PGND")
				(number "22")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "23")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "41")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "AGND")
				(number "18")
			)
			(pin passive line
				(at 2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "35")
			)
			(pin passive line
				(at 2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "36")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "25")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VDR1")
				(number "37")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "VDR2")
				(number "34")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PAC5527QM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -14.605 52.07 0)
		)
		(property "Value" "PAC5527QM"
			(at 15.494 52.07 0)
		)
		(property "Footprint" "Package_DFN_QFN:Qorvo_TQFN66-48-1EP_6x6mm_P0.4mm_EP4.2x4.2mm"
			(at 0 -66.04 0)
		)
		(property "Datasheet" "https://www.qorvo.com/products/d/da006847"
			(at 0 -63.5 0)
		)
		(property "Description" "48V Charge Pump Motor Controller and Driver for BLDC Motors, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "mcu motor driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Qorvo*TQFN66*1EP*6x6mm*P0.4mm*EP4.2x4.2mm*"
			(at 0 0 0)
		)
		(symbol "PAC5527QM_1_1"
			(pin passive line
				(at -17.78 48.26 0)
				(length 2.54)
				(name "VCP")
				(number "32")
			)
			(pin input line
				(at -17.78 43.18 0)
				(length 2.54)
				(name "CPH")
				(number "22")
			)
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "CPL")
				(number "21")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "SW1")
				(number "18")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "SW2")
				(number "19")
			)
			(pin power_out line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "VP")
				(number "20")
			)
			(pin power_out line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "VSYS")
				(number "16")
			)
			(pin power_out line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "VCCIO")
				(number "43")
			)
			(pin power_out line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "VCORE")
				(number "42")
			)
			(pin power_out line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "VCC33")
				(number "4")
			)
			(pin power_out line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "VCC18")
				(number "41")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 2.54)
				(name "VM")
				(number "17")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 -53.34 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 48.26 180)
				(length 2.54)
				(name "AIO0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 45.72 180)
				(length 2.54)
				(name "AIO1")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 2.54)
				(name "AIO2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "AIO3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "AIO4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "AIO5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "AIO6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "AIO7")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "AIO8")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "AIO9")
				(number "15")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "DRH0")
				(number "27")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "DRS0")
				(number "26")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "DRL0")
				(number "23")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "DRH1")
				(number "29")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "DRS1")
				(number "28")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "DRL1")
				(number "24")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DRH2")
				(number "31")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "DRS2")
				(number "30")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "DRL2")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PD4")
				(number "36")
				(alternate "TBPWM4" output line)
				(alternate "TBQEPIDX" input line)
				(alternate "TCPWM4" output line)
				(alternate "TDQEPIDX" input line)
				(alternate "TRACED3" output line)
				(alternate "USDMOSI" output line)
				(alternate "USDSCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PD5")
				(number "35")
				(alternate "CANRXD" input line)
				(alternate "TBPWM5" output line)
				(alternate "TBQEPPHA" input line)
				(alternate "TCPWM5" output line)
				(alternate "TDQEPPHA" input line)
				(alternate "USDMISO" input line)
				(alternate "USDSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PD6")
				(number "34")
				(alternate "CANTXD" output line)
				(alternate "I2CSDA" bidirectional line)
				(alternate "TBPWM6" output line)
				(alternate "TBQEPPHB" input line)
				(alternate "TCPWM6" output line)
				(alternate "TDQEPPHB" input line)
				(alternate "USDMOSI" output line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PD7")
				(number "33")
				(alternate "CANRXD" input line)
				(alternate "I2CSCL" bidirectional line)
				(alternate "TBPWM7" output line)
				(alternate "TCPWM7" output line)
				(alternate "USDMISO" input line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PE0")
				(number "37")
				(alternate "EMUXC" output line)
				(alternate "I2CSCL" bidirectional line)
				(alternate "TAQEPIDX" input line)
				(alternate "TBQEPIDX" input line)
				(alternate "TCPWM4" output line)
				(alternate "TDPWM0" output line)
				(alternate "USCSCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PE1")
				(number "38")
				(alternate "EMUXD" output line)
				(alternate "I2CSDA" bidirectional line)
				(alternate "TAQEPPHA" input line)
				(alternate "TBQEPPHA" input line)
				(alternate "TCPWM5" output line)
				(alternate "TDPWM1" output line)
				(alternate "USCSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PE2")
				(number "39")
				(alternate "CANRXD" input line)
				(alternate "EXTCLK" output line)
				(alternate "TAQEPPHA" input line)
				(alternate "TAQEPPHB" input line)
				(alternate "TCPWM6" output line)
				(alternate "TDPWM2" output line)
				(alternate "USCMOSI" output line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PE3")
				(number "40")
				(alternate "CANTXD" output line)
				(alternate "FRCLK" output line)
				(alternate "TCPWM7" output line)
				(alternate "TDPWM3" output line)
				(alternate "USCMISO" input line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PF0")
				(number "3")
				(alternate "SWDCLK" input line)
				(alternate "TBQEPIDX" input line)
				(alternate "TCK" input line)
				(alternate "TCPWM0" output line)
				(alternate "TDPWM0" output line)
				(alternate "TRACECLK" output line)
				(alternate "USBSCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PF1")
				(number "2")
				(alternate "SWDIO" bidirectional line)
				(alternate "TBQEPPHA" input line)
				(alternate "TCPWM1" output line)
				(alternate "TDPWM1" output line)
				(alternate "TMS" input line)
				(alternate "TRACED0" output line)
				(alternate "USBSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PF2")
				(number "1")
				(alternate "TBQEPPHB" input line)
				(alternate "TCPWM2" output line)
				(alternate "TDI" input line)
				(alternate "TDPWM2" output line)
				(alternate "TRACED1" output line)
				(alternate "USBMOSI" output line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PF3")
				(number "48")
				(alternate "FRCLK" output line)
				(alternate "TCPWM3" output line)
				(alternate "TDO" output line)
				(alternate "TDPWM3" output line)
				(alternate "TRACED2" output line)
				(alternate "USBMISO" input line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PF4")
				(number "47")
				(alternate "EMUXD" output line)
				(alternate "TCPWM4" output line)
				(alternate "TCQEPIDX" input line)
				(alternate "TDPWM4" output line)
				(alternate "TRACED3" output line)
				(alternate "USDSCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -43.18 180)
				(length 2.54)
				(name "PF5")
				(number "46")
				(alternate "EMUXD" output line)
				(alternate "TCPWM5" output line)
				(alternate "TCQEPPHA" input line)
				(alternate "TDPWM5" output line)
				(alternate "USDSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -45.72 180)
				(length 2.54)
				(name "PF6")
				(number "45")
				(alternate "CANRXD" input line)
				(alternate "I2CSCL" bidirectional line)
				(alternate "TCPWM6" output line)
				(alternate "TCQEPPHB" input line)
				(alternate "TDPWM6" output line)
				(alternate "USDMOSI" output line)
			)
			(pin bidirectional line
				(at 17.78 -48.26 180)
				(length 2.54)
				(name "PF7")
				(number "44")
				(alternate "CANTXD" output line)
				(alternate "I2CSDA" bidirectional line)
				(alternate "TCPWM7" output line)
				(alternate "TDPWM7" output line)
				(alternate "USDMISO" input line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "PG001M"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "PG001M"
			(at 7.62 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Sanken/Datasheets/PG001M-Datasheet.ashx"
			(at 0 -2.54 0)
		)
		(property "Description" "Parallel to serial data converter for SLA7042M/SLA7044M"
			(at 0 0 0)
		)
		(property "ki_keywords" "Support IC for SLA7042M/SLA7044M"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PG001M_0_1")
		(symbol "PG001M_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "1")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "CLK_IN")
				(number "2")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "~{CW}")
				(number "3")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "MSEL_1")
				(number "6")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "MSEL_2")
				(number "7")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "VECTOR")
				(number "15")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "~{MONITOR}")
				(number "9")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "Vdd")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "DATA_A")
				(number "11")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "DATA_B")
				(number "10")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{STROBE}")
				(number "13")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "CLK_OUT")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Pololu_Breakout_A4988"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -2.54 19.05 0)
		)
		(property "Value" "Pololu_Breakout_A4988"
			(at -2.54 16.51 0)
		)
		(property "Footprint" "Module:Pololu_Breakout-16_15.2x20.3mm"
			(at 6.985 -19.05 0)
		)
		(property "Datasheet" "https://www.pololu.com/product/2980/pictures"
			(at 2.54 -7.62 0)
		)
		(property "Description" "Pololu Breakout Board, Stepper Driver A4988"
			(at 0 0 0)
		)
		(property "ki_keywords" "Pololu Breakout Board Stepper Driver A4988"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pololu*Breakout*15.2x20.3mm*"
			(at 0 0 0)
		)
		(symbol "Pololu_Breakout_A4988_0_1")
		(symbol "Pololu_Breakout_A4988_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "13")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{SLEEP}")
				(number "14")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{ENABLE}")
				(number "9")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "STEP")
				(number "15")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DIR")
				(number "16")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "MS1")
				(number "10")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "MS2")
				(number "11")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "MS3")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "VMOT")
				(number "8")
			)
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "1B")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "1A")
				(number "4")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "2A")
				(number "5")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "2B")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Pololu_Breakout_DRV8825"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -2.54 16.51 0)
		)
		(property "Value" "Pololu_Breakout_DRV8825"
			(at -2.54 13.97 0)
		)
		(property "Footprint" "Module:Pololu_Breakout-16_15.2x20.3mm"
			(at 5.08 -20.32 0)
		)
		(property "Datasheet" "https://www.pololu.com/product/2982"
			(at 2.54 -7.62 0)
		)
		(property "Description" "Pololu Breakout Board, Stepper Driver DRV8825"
			(at 0 0 0)
		)
		(property "ki_keywords" "Pololu Breakout Board Stepper Driver DRV8825"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Pololu*Breakout*15.2x20.3mm*"
			(at 0 0 0)
		)
		(symbol "Pololu_Breakout_DRV8825_0_1")
		(symbol "Pololu_Breakout_DRV8825_1_1"
			(pin output line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "~{FLT}")
				(number "2")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{RST}")
				(number "13")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{SLP}")
				(number "14")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{EN}")
				(number "9")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "STEP")
				(number "15")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DIR")
				(number "16")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "M0")
				(number "10")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "M1")
				(number "11")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "M2")
				(number "12")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VMOT")
				(number "8")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "A1")
				(number "4")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B1")
				(number "5")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SLA7044M"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "SLA7044M"
			(at 7.62 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.sumzi.com/upload/files/2007/07/2007073114282034189.PDF"
			(at 0 0 0)
		)
		(property "Description" "Unipolar PWM high-current motor driver"
			(at 0 0 0)
		)
		(property "ki_keywords" "Stepper driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SLA704XM"
			(at 0 0 0)
		)
		(symbol "SLA7044M_0_1")
		(symbol "SLA7044M_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "DATA")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{CLOCK}")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{STROBE}")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "REF")
				(number "3")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "RS")
				(number "9")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "Vdd")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{OUT}")
				(number "8")
			)
		)
		(symbol "SLA7044M_2_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "DATA")
				(number "17")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{CLOCK}")
				(number "16")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{STROBE}")
				(number "13")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "REF")
				(number "14")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "RS")
				(number "10")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "Vdd")
				(number "15")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "11")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{OUT}")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SLA7070MPRT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 25.4 0)
		)
		(property "Value" "SLA7070MPRT"
			(at 7.62 -25.4 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.semicon.sanken-ele.co.jp/sk_content/sla7070mprt_ds_en.pdf"
			(at 0 0 0)
		)
		(property "Description" "Unipolar 2-phase stepper motor driver, Full and Half step, 1A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Stepper driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ZIP23"
			(at 0 0 0)
		)
		(symbol "SLA7070MPRT_0_1")
		(symbol "SLA7070MPRT_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 3.81)
				(name "RESET")
				(number "15")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "REF/SLEEP1")
				(number "13")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "M1")
				(number "7")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "M2")
				(number "8")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "M3")
				(number "9")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "CLOCK")
				(number "10")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "CW/CCW")
				(number "16")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "SYNC")
				(number "17")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 3.81)
				(name "VBB")
				(number "11")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 3.81)
				(name "VDD")
				(number "14")
			)
			(pin no_connect line
				(at 10.16 -20.32 180)
				(length 3.81)
				(hide yes)
				(name "N.C.")
				(number "6")
			)
			(pin output line
				(at 15.24 20.32 180)
				(length 3.81)
				(name "OUTA")
				(number "1")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 3.81)
				(name "OUTA")
				(number "2")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 3.81)
				(name "~{OUTA}")
				(number "3")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "~{OUTA}")
				(number "4")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "~{OUTB}")
				(number "20")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "~{OUTB}")
				(number "21")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "OUTB")
				(number "22")
			)
			(pin output line
				(at 15.24 0 180)
				(length 3.81)
				(name "OUTB")
				(number "23")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "SENSE_A")
				(number "5")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "SENSE_B")
				(number "19")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 3.81)
				(name "FLAG")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SLA7075MPRT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 25.4 0)
		)
		(property "Value" "SLA7075MPRT"
			(at 7.62 -25.4 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.semicon.sanken-ele.co.jp/sk_content/sla7075mprt_ds_en.pdf"
			(at 0 0 0)
		)
		(property "Description" "Unipolar 2-phase stepper motor driver, Microstep, 1A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Stepper driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ZIP23"
			(at 0 0 0)
		)
		(symbol "SLA7075MPRT_0_1")
		(symbol "SLA7075MPRT_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 3.81)
				(name "RESET")
				(number "15")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "REF/SLEEP1")
				(number "13")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "M1")
				(number "7")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "M2")
				(number "8")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "M3")
				(number "9")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "CLOCK")
				(number "10")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "CW/CCW")
				(number "16")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "SYNC")
				(number "17")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 3.81)
				(name "VBB")
				(number "11")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 3.81)
				(name "VDD")
				(number "14")
			)
			(pin output line
				(at 15.24 20.32 180)
				(length 3.81)
				(name "OUTA")
				(number "1")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 3.81)
				(name "OUTA")
				(number "2")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 3.81)
				(name "~{OUTA}")
				(number "3")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "~{OUTA}")
				(number "4")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "~{OUTB}")
				(number "20")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "~{OUTB}")
				(number "21")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "OUTB")
				(number "22")
			)
			(pin output line
				(at 15.24 0 180)
				(length 3.81)
				(name "OUTB")
				(number "23")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "SENSE_A")
				(number "5")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "SENSE_B")
				(number "19")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 3.81)
				(name "FLAG")
				(number "18")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 3.81)
				(name "MO")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN754410NE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 17.78 0)
		)
		(property "Value" "SN754410NE"
			(at -7.62 15.24 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at -2.54 22.86 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn754410.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "Quadruple Half-H Driver, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "h-bridge motor driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "SN754410NE_0_1")
		(symbol "SN754410NE_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "1,2EN")
				(number "1")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "1A")
				(number "2")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "2A")
				(number "7")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "3,4EN")
				(number "9")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "3A")
				(number "10")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "4A")
				(number "15")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCC1")
				(number "16")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VCC2")
				(number "8")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "1Y")
				(number "3")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "2Y")
				(number "6")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "3Y")
				(number "11")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "4Y")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STK672-040-E"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "STK672-040-E"
			(at 0 0 90)
		)
		(property "Footprint" ""
			(at 3.81 1.27 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/EN5227-D.PDF"
			(at 3.81 1.27 0)
		)
		(property "Description" "Stepper motor driver with microstepping controller, 1.5A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Stepper driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "STK672-040-E"
			(at 0 0 0)
		)
		(symbol "STK672-040-E_0_1")
		(symbol "STK672-040-E_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "M1")
				(number "9")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "M2")
				(number "10")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "M3")
				(number "11")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "M4")
				(number "12")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "M5")
				(number "13")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "CLK")
				(number "14")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CWB")
				(number "15")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RETURN")
				(number "17")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "ENABLE")
				(number "18")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "16")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "Vref")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "PG")
				(number "4")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "PG")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "SG")
				(number "22")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "~{A}")
				(number "5")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "~{B}")
				(number "1")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "MOI")
				(number "19")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "MO1")
				(number "20")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "MO2")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STK672-080-E"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "STK672-080-E"
			(at 0 0 90)
		)
		(property "Footprint" ""
			(at 1.27 -1.27 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/EN6507-D.PDF"
			(at 1.27 -1.27 0)
		)
		(property "Description" "Stepper motor driver with microstepping controller, 2.8A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Stepper driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "STK672-080-E"
			(at 0 0 0)
		)
		(symbol "STK672-080-E_0_1")
		(symbol "STK672-080-E_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "M1")
				(number "8")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "M2")
				(number "9")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "M3")
				(number "12")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CLOCK")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "CWB")
				(number "10")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "ENABLE")
				(number "15")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "13")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "Vref")
				(number "7")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "PG")
				(number "1")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "A")
				(number "5")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "AB")
				(number "4")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "B")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "BB")
				(number "2")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "MOI")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STSPIN220"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "STSPIN220"
			(at 5.08 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 5.08 19.05 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/stspin220.pdf"
			(at 3.81 6.35 0)
		)
		(property "Description" "Low voltage stepper motor driver, 1.8V to 10V input, 1.3Arms output, 0.4Ω Rdson per phase (typical), QFN-16 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "motor driver stepper"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STSPIN220_0_1")
		(symbol "STSPIN220_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "DIR")
				(number "1")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "STCK")
				(number "2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "MODE1")
				(number "16")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "MODE2")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "EN/FLT")
				(number "13")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "STBY/RESET")
				(number "14")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "REF")
				(number "11")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "TOFF")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "EPAD")
				(number "17")
			)
			(pin power_out line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "OUTA1")
				(number "3")
			)
			(pin power_out line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "OUTA2")
				(number "5")
			)
			(pin power_out line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "SENSEA")
				(number "4")
			)
			(pin power_out line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUTB1")
				(number "10")
			)
			(pin power_out line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUTB2")
				(number "8")
			)
			(pin power_out line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "SENSEB")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STSPIN230"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "STSPIN230"
			(at 2.54 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 5.08 19.05 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/stspin230.pdf"
			(at 3.81 6.35 0)
		)
		(property "Description" "Low voltage triple half-bridge motor driver, 1.8V to 10V input, 1.3Arms output, 0.4Ω Rdson per phase (typical), QFN-16 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "motor driver half-bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STSPIN230_0_1")
		(symbol "STSPIN230_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "INUH")
				(number "2")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "INUL")
				(number "1")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "INVH")
				(number "16")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "INVL")
				(number "15")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "INWH")
				(number "12")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "INWL")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "EN/FLT")
				(number "13")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "STBY")
				(number "14")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin no_connect line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_out line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "OUTU")
				(number "3")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUTV")
				(number "8")
			)
			(pin power_out line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUTW")
				(number "10")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "SENSEU")
				(number "4")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SENSEVW")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STSPIN233"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "STSPIN233"
			(at 5.08 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 5.08 19.05 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/stspin233.pdf"
			(at 3.81 6.35 0)
		)
		(property "Description" "Low voltage three phase and three sense motor driver, 1.8V to 10V input, 1.3Arms output, 0.4Ω Rdson per phase (typical), QFN-16 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "motor driver half-bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STSPIN233_0_1")
		(symbol "STSPIN233_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "ENU")
				(number "2")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "INU")
				(number "1")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "ENV")
				(number "16")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "INV")
				(number "15")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "ENW")
				(number "12")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "INW")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "EN/FAULT")
				(number "13")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "STBY/RESET")
				(number "14")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VS")
				(number "5")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_out line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "OUTU")
				(number "3")
			)
			(pin power_out line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUTV")
				(number "7")
			)
			(pin power_out line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUTW")
				(number "10")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "SENSEU")
				(number "4")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "SENSEV")
				(number "8")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "SENSEW")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STSPIN240"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "STSPIN240"
			(at 5.08 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 5.08 19.05 0)
		)
		(property "Datasheet" "www.st.com/resource/en/datasheet/stspin240.pdf"
			(at 3.81 6.35 0)
		)
		(property "Description" "Low voltage dual brush DC motor driver, 1.8V to 10V input, 1.3Arms output, 0.4Ω Rdson per phase (typical), QFN-16 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "motor driver dc brushed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STSPIN240_0_1")
		(symbol "STSPIN240_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PHA")
				(number "1")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PWMA")
				(number "2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PHB")
				(number "15")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PWMB")
				(number "16")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "EN/FLT")
				(number "13")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "STBY/RESET")
				(number "14")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "REF")
				(number "11")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "TOFF")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VS")
				(number "6")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "EPAD")
				(number "17")
			)
			(pin power_out line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "OUTA1")
				(number "3")
			)
			(pin power_out line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "OUTA2")
				(number "5")
			)
			(pin power_out line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "SENSEA")
				(number "4")
			)
			(pin power_out line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUTB1")
				(number "10")
			)
			(pin power_out line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUTB2")
				(number "8")
			)
			(pin power_out line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "SENSEB")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TB6612FNG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 11.43 17.78 0)
		)
		(property "Value" "TB6612FNG"
			(at 11.43 15.24 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
			(at 33.02 -22.86 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/us/product/linear/motordriver/detail.TB6612FNG.html"
			(at 11.43 15.24 0)
		)
		(property "Description" "Driver IC for Dual DC motor, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "H-bridge motor driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP-24*5.3x8.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TB6612FNG_0_1")
		(symbol "TB6612FNG_1_1"
			(pin input inverted
				(at -15.24 10.16 0)
				(length 5.08)
				(name "STBY")
				(number "19")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "PWMA")
				(number "23")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "PWMB")
				(number "15")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "AIN1")
				(number "21")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "AIN2")
				(number "22")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "BIN1")
				(number "17")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "BIN2")
				(number "16")
			)
			(pin power_in line
				(at -7.62 25.4 270)
				(length 5.08)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at -7.62 -25.4 90)
				(length 5.08)
				(name "GND")
				(number "18")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 5.08)
				(name "VM1")
				(number "24")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 5.08)
				(name "PGND1")
				(number "3")
			)
			(pin passive line
				(at 2.54 -25.4 90)
				(length 5.08)
				(hide yes)
				(name "PGND1")
				(number "4")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 5.08)
				(name "VM2")
				(number "13")
			)
			(pin power_in line
				(at 7.62 25.4 270)
				(length 5.08)
				(name "VM3")
				(number "14")
			)
			(pin passive line
				(at 7.62 -25.4 90)
				(length 5.08)
				(hide yes)
				(name "PGND2")
				(number "10")
			)
			(pin power_in line
				(at 7.62 -25.4 90)
				(length 5.08)
				(name "PGND2")
				(number "9")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 5.08)
				(name "AO1")
				(number "1")
			)
			(pin passive line
				(at 15.24 10.16 180)
				(length 5.08)
				(hide yes)
				(name "AO1")
				(number "2")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "AO2")
				(number "5")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 5.08)
				(hide yes)
				(name "AO2")
				(number "6")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "BO1")
				(number "11")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 5.08)
				(hide yes)
				(name "BO1")
				(number "12")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 5.08)
				(name "BO2")
				(number "7")
			)
			(pin passive line
				(at 15.24 -7.62 180)
				(length 5.08)
				(hide yes)
				(name "BO2")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TC78H670FTG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 -3.81 0)
		)
		(property "Value" "TC78H670FTG"
			(at 10.16 17.78 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 15.24 -7.62 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/TC78H670FTG_datasheet_en_20210209.pdf?did=68606&prodName=TC78H670FTG"
			(at 7.62 3.81 0)
		)
		(property "Description" "Bipolar stepping motor driver IC, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "stepping motor driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TC78H670FTG_0_0"
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "AGND")
				(number "2")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VM")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "PGND_A")
				(number "4")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "OUT_A+")
				(number "5")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "OUT_A-")
				(number "6")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUT_B+")
				(number "8")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUT_B-")
				(number "7")
			)
		)
		(symbol "TC78H670FTG_1_0"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "~{STBY}")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "EN/~{ERR}")
				(number "13")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "MODE0")
				(number "14")
				(alternate "S_DATA" input line)
				(alternate "UP-DW" input line)
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "MODE1")
				(number "15")
				(alternate "LATCH" input line)
				(alternate "SET_EN" input line)
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "MODE2")
				(number "16")
				(alternate "CLK" input line)
				(alternate "S_CLK" input line)
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "MODE3")
				(number "1")
				(alternate "CW-CCW" input line)
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "VREF")
				(number "10")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "OSCM")
				(number "11")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND_PAD")
				(number "17")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "PGND_B")
				(number "9")
			)
		)
		(symbol "TC78H670FTG_1_1")
		(embedded_fonts no)
	)
	(symbol "TMC2041-LA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "TMC2041-LA"
			(at 8.89 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.3x5.3mm_ThermalVias"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "https://www.trinamic.com/fileadmin/assets/Products/ICs_Documents/TMC2041_datasheet.pdf"
			(at 15.24 45.72 0)
		)
		(property "Description" "Standalone Dual driver for two-phase bipolar stepper motor, 2.2A, 4.75-26V, SPI, UART, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual driver stepper motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TMC2041-LA_0_1")
		(symbol "TMC2041-LA_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "~{DRV_ENN}")
				(number "29")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "CLK")
				(number "11")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "STEP1")
				(number "28")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "DIR1")
				(number "27")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "STEP2")
				(number "26")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DIR2")
				(number "25")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "CSN/IO0")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "SCK/IO1")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "SDI/IO2")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "SDO")
				(number "8")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "NEXTADDR")
				(number "24")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "SWIOP")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "SWION")
				(number "10")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "SWSEL")
				(number "12")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "TST_MODE")
				(number "48")
			)
			(pin power_in line
				(at -7.62 27.94 270)
				(length 2.54)
				(name "VSA")
				(number "30")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 2.54)
				(name "VS")
				(number "17")
			)
			(pin passive line
				(at -5.08 27.94 270)
				(length 2.54)
				(hide yes)
				(name "VS")
				(number "19")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VS")
				(number "42")
			)
			(pin passive line
				(at -2.54 27.94 270)
				(length 2.54)
				(hide yes)
				(name "VS")
				(number "44")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC_IO")
				(number "7")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GNDD")
				(number "1")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GNDD")
				(number "13")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GNDD")
				(number "2")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GNDD")
				(number "23")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GNDD")
				(number "34")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GNDD")
				(number "38")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GNDD")
				(number "49")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GNDD")
				(number "6")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "33")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "GNDP")
				(number "18")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GNDP")
				(number "43")
			)
			(pin power_out line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "5VOUT")
				(number "32")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 2.54)
				(name "GNDA")
				(number "31")
			)
			(pin passive line
				(at 7.62 27.94 270)
				(length 2.54)
				(name "VCP")
				(number "37")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "O1A1")
				(number "47")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "O1A2")
				(number "45")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "O1B1")
				(number "41")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "O1B2")
				(number "39")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "BR1A")
				(number "46")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "BR1B")
				(number "40")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "O2A1")
				(number "14")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "O2A2")
				(number "16")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "O2B1")
				(number "20")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "O2B2")
				(number "22")
			)
			(pin passive line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "BR2A")
				(number "15")
			)
			(pin passive line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "BR2B")
				(number "21")
			)
			(pin passive line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "CPI")
				(number "36")
			)
			(pin passive line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "CPO")
				(number "35")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMC2100-LA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "TMC2100-LA"
			(at 8.89 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-36-1EP_5x6mm_P0.5mm_EP3.6x4.1mm_ThermalVias"
			(at -5.08 -27.94 0)
		)
		(property "Datasheet" "https://www.trinamic.com/fileadmin/assets/Products/ICs_Documents/TMC2100_datasheet_Rev1.08.pdf"
			(at -29.21 26.67 0)
		)
		(property "Description" "Standalone driver for two-phase bipolar stepper motor, 2.0A, 4.75-46V, QFN-36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Driver stepper motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x6mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TMC2100-LA_0_1")
		(symbol "TMC2100-LA_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "AIN_REF")
				(number "23")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "~{CFG6_ENN}")
				(number "22")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "CLK")
				(number "1")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "STEP")
				(number "6")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "DIR")
				(number "7")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CFG0")
				(number "5")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CFG1")
				(number "4")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "CFG2")
				(number "3")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "CFG3")
				(number "2")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "CFG4")
				(number "18")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "CFG5")
				(number "19")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "TST_MODE")
				(number "36")
			)
			(pin power_in line
				(at -7.62 25.4 270)
				(length 2.54)
				(name "VSA")
				(number "30")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "VS")
				(number "16")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VS")
				(number "31")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCC_IO")
				(number "8")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GNDD")
				(number "10")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GNDD")
				(number "11")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GNDD")
				(number "37")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "26")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "GNDP")
				(number "12")
			)
			(pin passive line
				(at 2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GNDP")
				(number "35")
			)
			(pin power_out line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "5VOUT")
				(number "25")
			)
			(pin power_in line
				(at 5.08 -25.4 90)
				(length 2.54)
				(name "GNDA")
				(number "24")
			)
			(pin no_connect line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "17")
			)
			(pin no_connect line
				(at 12.7 0 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "9")
			)
			(pin passive line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "VCP")
				(number "29")
			)
			(pin open_collector line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "ERROR")
				(number "20")
			)
			(pin open_collector line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "INDEX")
				(number "21")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "OA1")
				(number "34")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OA2")
				(number "32")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "BRA")
				(number "33")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "BRB")
				(number "14")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OB2")
				(number "15")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "OB1")
				(number "13")
			)
			(pin passive line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "CPI")
				(number "28")
			)
			(pin passive line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "CP0")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMC2100-TA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "TMC2100-TA"
			(at 8.89 24.13 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48-1EP_7x7mm_P0.5mm_EP5x5mm_ThermalVias"
			(at 0 -27.94 0)
		)
		(property "Datasheet" "https://www.trinamic.com/fileadmin/assets/Products/ICs_Documents/TMC2100_datasheet_Rev1.08.pdf"
			(at -29.21 26.67 0)
		)
		(property "Description" "Standalone driver for two-phase bipolar stepper motor, 2.0A, 4.75-46V, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Standalone driver stepper motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TMC2100-TA_0_1")
		(symbol "TMC2100-TA_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "AIN_REF")
				(number "30")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "~{CFG6_ENN}")
				(number "29")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "CLK")
				(number "2")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "STEP")
				(number "8")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "DIR")
				(number "9")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "CFG0")
				(number "7")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CFG1")
				(number "5")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "CFG2")
				(number "4")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "CFG3")
				(number "3")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "CFG4")
				(number "24")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "CFG5")
				(number "25")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "TST_MODE")
				(number "1")
			)
			(pin no_connect line
				(at -12.7 17.78 0)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "11")
			)
			(pin no_connect line
				(at -12.7 7.62 0)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "14")
			)
			(pin no_connect line
				(at -12.7 0 0)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "16")
			)
			(pin no_connect line
				(at -12.7 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "18")
			)
			(pin power_in line
				(at -7.62 25.4 270)
				(length 2.54)
				(name "VSA")
				(number "39")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "VS")
				(number "21")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VS")
				(number "40")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCC_IO")
				(number "10")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GNDD")
				(number "12")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GNDD")
				(number "31")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GNDD")
				(number "36")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GNDD")
				(number "49")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GNDD")
				(number "6")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "34")
			)
			(pin passive line
				(at 2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GNDP")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "GNDP")
				(number "48")
			)
			(pin power_out line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "5VOUT")
				(number "33")
			)
			(pin power_in line
				(at 5.08 -25.4 90)
				(length 2.54)
				(name "GNDA")
				(number "32")
			)
			(pin passive line
				(at 7.62 25.4 270)
				(length 2.54)
				(name "VCP")
				(number "38")
			)
			(pin no_connect line
				(at 7.62 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "22")
			)
			(pin no_connect line
				(at 12.7 20.32 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "23")
			)
			(pin no_connect line
				(at 12.7 17.78 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "20")
			)
			(pin no_connect line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "47")
			)
			(pin no_connect line
				(at 12.7 0 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "45")
			)
			(pin no_connect line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "43")
			)
			(pin no_connect line
				(at 12.7 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "41")
			)
			(pin no_connect line
				(at 12.7 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "28")
			)
			(pin open_collector line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "ERROR")
				(number "26")
			)
			(pin open_collector line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "INDEX")
				(number "27")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "OA1")
				(number "46")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OA2")
				(number "42")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "BRA")
				(number "44")
			)
			(pin passive line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "BRB")
				(number "17")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "OB2")
				(number "19")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "OB1")
				(number "15")
			)
			(pin passive line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "CPI")
				(number "37")
			)
			(pin passive line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "CP0")
				(number "35")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMC2130-LA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 38.1 0)
		)
		(property "Value" "TMC2130-LA"
			(at 17.78 38.1 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-36-1EP_5x6mm_P0.5mm_EP3.6x4.1mm"
			(at 0 -66.04 0)
		)
		(property "Datasheet" "http://www.trinamic.com/fileadmin/assets/Products/ICs_Documents/TMC2130_datasheet.pdf"
			(at 0 -68.58 0)
		)
		(property "Description" "Driver for two-phase bipolar stepper motor, 2.0A, SPI, 4.75-46V, QFN-36"
			(at 0 0 0)
		)
		(property "ki_keywords" "stepper motor driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x6mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TMC2130-LA_0_1")
		(symbol "TMC2130-LA_1_1"
			(pin passive line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "VCP")
				(number "29")
			)
			(pin passive line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "CPO")
				(number "27")
			)
			(pin passive line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "CPI")
				(number "28")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "CLK")
				(number "1")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "~{CS}_CFG3")
				(number "2")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "SCK_CFG2")
				(number "3")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SDI_CFG1")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "SDO_CFG0")
				(number "5")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "STEP")
				(number "6")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "DIR")
				(number "7")
			)
			(pin output line
				(at -17.78 0 0)
				(length 2.54)
				(name "DCO")
				(number "17")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "DCEN_CFG4")
				(number "18")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "DCIN_CFG5")
				(number "19")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "~{DRV_EN}_CFG6")
				(number "22")
			)
			(pin output line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "DIAG0")
				(number "20")
			)
			(pin output line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "DIAG1")
				(number "21")
			)
			(pin input line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "AIN_IREF")
				(number "23")
			)
			(pin input line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "SPI_MODE")
				(number "10")
			)
			(pin input line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "TST_MODE")
				(number "36")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VCC_IO")
				(number "8")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "26")
			)
			(pin power_out line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "5VOUT")
				(number "25")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 2.54)
				(name "GNDP")
				(number "12")
			)
			(pin passive line
				(at -2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GNDP")
				(number "35")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GNDA")
				(number "24")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VSA")
				(number "30")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "EP")
				(number "37")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VS")
				(number "31")
			)
			(pin passive line
				(at 5.08 -38.1 90)
				(length 2.54)
				(name "NC")
				(number "11")
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "VS")
				(number "16")
			)
			(pin no_connect line
				(at 15.24 33.02 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "9")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "OA1")
				(number "34")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "OA2")
				(number "32")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "OB1")
				(number "13")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "OB2")
				(number "15")
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "BRA")
				(number "33")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "BRB")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMC2130-TA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 38.1 0)
		)
		(property "Value" "TMC2130-TA"
			(at 17.78 38.1 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48-1EP_7x7mm_P0.5mm_EP5x5mm"
			(at 0 -68.58 0)
		)
		(property "Datasheet" "http://www.trinamic.com/fileadmin/assets/Products/ICs_Documents/TMC2130_datasheet.pdf"
			(at 53.34 -45.72 0)
		)
		(property "Description" "Driver for two-phase bipolar stepper motor, 2.0A, SPI, 4.75-46V, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "stepper motor driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TMC2130-TA_1_1"
			(pin passive line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "VCP")
				(number "38")
			)
			(pin passive line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "CPO")
				(number "35")
			)
			(pin passive line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "CPI")
				(number "37")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "CLK")
				(number "2")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "~{CS}_CFG3")
				(number "3")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "SCK_CFG2")
				(number "4")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SDI_CFG1")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "SDO_CFG0")
				(number "7")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "STEP")
				(number "8")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "DIR")
				(number "9")
			)
			(pin output line
				(at -17.78 0 0)
				(length 2.54)
				(name "DCO")
				(number "23")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "DCEN_CFG4")
				(number "24")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "DCIN_CFG5")
				(number "25")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "~{DRV_EN}_CFG6")
				(number "29")
			)
			(pin output line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "DIAG0")
				(number "26")
			)
			(pin output line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "DIAG1")
				(number "27")
			)
			(pin input line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "AIN_IREF")
				(number "30")
			)
			(pin input line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "SPI_MODE")
				(number "12")
			)
			(pin input line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "TST_MODE")
				(number "1")
			)
			(pin no_connect line
				(at -15.24 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "28")
			)
			(pin no_connect line
				(at -15.24 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "11")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VCC_IO")
				(number "10")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "34")
			)
			(pin power_out line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "5VOUT")
				(number "33")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 2.54)
				(name "GNDP")
				(number "13")
			)
			(pin passive line
				(at -2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GNDP")
				(number "48")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GNDA")
				(number "32")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VSA")
				(number "39")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "EP")
				(number "49")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VS")
				(number "40")
			)
			(pin passive line
				(at 5.08 -38.1 90)
				(length 2.54)
				(name "NC")
				(number "31")
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "VS")
				(number "21")
			)
			(pin passive line
				(at 7.62 -38.1 90)
				(length 2.54)
				(name "NC")
				(number "6")
			)
			(pin passive line
				(at 10.16 -38.1 90)
				(length 2.54)
				(name "NC")
				(number "36")
			)
			(pin no_connect line
				(at 15.24 33.02 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "41")
			)
			(pin no_connect line
				(at 15.24 30.48 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "43")
			)
			(pin no_connect line
				(at 15.24 27.94 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "45")
			)
			(pin no_connect line
				(at 15.24 25.4 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "47")
			)
			(pin no_connect line
				(at 15.24 12.7 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "14")
			)
			(pin no_connect line
				(at 15.24 10.16 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "16")
			)
			(pin no_connect line
				(at 15.24 7.62 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "18")
			)
			(pin no_connect line
				(at 15.24 5.08 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "20")
			)
			(pin no_connect line
				(at 15.24 2.54 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "22")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "OA1")
				(number "46")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "OA2")
				(number "42")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "OB1")
				(number "15")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "OB2")
				(number "19")
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "BRA")
				(number "44")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "BRB")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMC2160"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 -33.02 0)
		)
		(property "Value" "TMC2160"
			(at 17.78 -33.02 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48-1EP_7x7mm_P0.5mm_EP5x5mm"
			(at -30.48 -48.26 0)
		)
		(property "Datasheet" "https://www.trinamic.com/fileadmin/assets/Products/ICs_Documents/TMC2160A-datasheet_Rev1.06.pdf"
			(at 1.27 -50.8 0)
		)
		(property "Description" "Standalone driver for two-phase bipolar stepper motor, 8-60V, external FETs, TQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Standalone driver stepper motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*1EP?7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TMC2160_1_1"
			(pin input line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "CLK")
				(number "12")
			)
			(pin input line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "~{DRV_EN}")
				(number "28")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "SDI_CFG1")
				(number "15")
			)
			(pin passive line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "SDO_CFG0")
				(number "16")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "SCK_CFG2")
				(number "14")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "~{CS}_CFG3")
				(number "13")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "SPI_MODE")
				(number "22")
			)
			(pin input line
				(at -20.32 0 0)
				(length 2.54)
				(name "DIR")
				(number "18")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "STEP")
				(number "17")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "DCEN_CFG4")
				(number "23")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "DCIN_CFG5")
				(number "24")
			)
			(pin output line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "DCO_CFG6")
				(number "25")
			)
			(pin output line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "DIAG0")
				(number "26")
			)
			(pin output line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "DIAG1")
				(number "27")
			)
			(pin passive line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "CPI")
				(number "32")
			)
			(pin passive line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "CPO")
				(number "31")
			)
			(pin input line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "TST_MODE")
				(number "11")
			)
			(pin power_in line
				(at -15.24 33.02 270)
				(length 2.54)
				(name "VCC_IO")
				(number "20")
			)
			(pin passive line
				(at -15.24 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VCC_IO")
				(number "21")
			)
			(pin passive line
				(at -10.16 33.02 270)
				(length 2.54)
				(name "VCP")
				(number "34")
			)
			(pin power_in line
				(at -5.08 -33.02 90)
				(length 2.54)
				(name "GNDD")
				(number "19")
			)
			(pin passive line
				(at -5.08 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GNDD")
				(number "30")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "VS")
				(number "33")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VSA")
				(number "4")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 2.54)
				(name "12VOUT")
				(number "3")
			)
			(pin power_in line
				(at 5.08 -33.02 90)
				(length 2.54)
				(name "GNDA")
				(number "6")
			)
			(pin power_out line
				(at 10.16 33.02 270)
				(length 2.54)
				(name "5VOUT")
				(number "5")
			)
			(pin power_in line
				(at 15.24 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "29")
			)
			(pin passive line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "CB2")
				(number "43")
			)
			(pin output line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "HB2")
				(number "44")
			)
			(pin output line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "CB1")
				(number "2")
			)
			(pin output line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "HB1")
				(number "1")
			)
			(pin passive line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "BMB1")
				(number "48")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "BMB2")
				(number "45")
			)
			(pin output line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "LB1")
				(number "47")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "LB2")
				(number "46")
			)
			(pin input line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "SRBH")
				(number "9")
			)
			(pin input line
				(at 20.32 0 180)
				(length 2.54)
				(name "SRBL")
				(number "10")
			)
			(pin passive line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "CA2")
				(number "35")
			)
			(pin output line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "HA2")
				(number "36")
			)
			(pin output line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "CA1")
				(number "42")
			)
			(pin output line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "HA1")
				(number "41")
			)
			(pin passive line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "BMA1")
				(number "40")
			)
			(pin passive line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "BMA2")
				(number "37")
			)
			(pin output line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "LA1")
				(number "39")
			)
			(pin output line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "LA2")
				(number "38")
			)
			(pin input line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "SRAH")
				(number "8")
			)
			(pin input line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "SRAL")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMC2202-WA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 -27.94 0)
		)
		(property "Value" "TMC2202-WA"
			(at 7.62 -27.94 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-32-1EP_5x5mm_P0.5mm_EP3.4x3.4mm_ThermalVias"
			(at -2.54 -38.1 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/TMC2202_TMC2208_TMC2224_datasheet_rev1.13.pdf"
			(at 0 -40.64 0)
		)
		(property "Description" "Standalone driver for two-phase bipolar stepper motor, 2A, 4.75… 36V, UART, internal FETs, QFN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Standalone driver stepper motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFN*1EP?5x5mm?P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TMC2202-WA_1_1"
			(pin passive line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "VCP")
				(number "9")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "MS1")
				(number "11")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "MS2")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PDN_UART")
				(number "15")
			)
			(pin passive line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "CPO")
				(number "7")
			)
			(pin passive line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "CPI")
				(number "8")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "CLK")
				(number "14")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "STEP")
				(number "17")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "DIR")
				(number "20")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "ENN")
				(number "5")
			)
			(pin output line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "DIAG")
				(number "13")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "VREF")
				(number "18")
			)
			(pin no_connect line
				(at -5.08 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VCC_IO")
				(number "16")
			)
			(pin passive line
				(at 0 27.94 270)
				(length 2.54)
				(hide yes)
				(name "VS")
				(number "22")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VS")
				(number "3")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin no_connect line
				(at 12.7 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "31")
			)
			(pin no_connect line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "29")
			)
			(pin no_connect line
				(at 12.7 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin no_connect line
				(at 12.7 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "26")
			)
			(pin no_connect line
				(at 12.7 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at 12.7 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin no_connect line
				(at 12.7 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin output line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "OB2")
				(number "1")
			)
			(pin output line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "OB1")
				(number "30")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "OA2")
				(number "24")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "OA1")
				(number "27")
			)
			(pin power_out line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "5VOUT")
				(number "10")
			)
			(pin passive line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "BRB")
				(number "32")
			)
			(pin passive line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "BRA")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMC2208-LA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 -26.67 0)
		)
		(property "Value" "TMC2208-LA"
			(at 7.62 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-32-1EP_5x5mm_P0.5mm_EP3.4x3.4mm_ThermalVias"
			(at 0 -40.64 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/TMC2202_TMC2208_TMC2224_datasheet_rev1.13.pdf"
			(at 0 -45.72 0)
		)
		(property "Description" "Standalone driver for two-phase bipolar stepper motor, 2A, 4.75… 36V, UART, internal FETs, QFN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Standalone driver stepper motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFN*1EP?5x5mm?P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TMC2208-LA_1_1"
			(pin passive line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "VCP")
				(number "6")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "MS1")
				(number "9")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "MS2")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PDN_UART")
				(number "14")
			)
			(pin passive line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "CPO")
				(number "4")
			)
			(pin passive line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "CPI")
				(number "5")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "CLK")
				(number "13")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "STEP")
				(number "16")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "DIR")
				(number "19")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "ENN")
				(number "2")
			)
			(pin output line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "DIAG")
				(number "11")
			)
			(pin output line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "INDEX")
				(number "12")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "VREF")
				(number "17")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VCC_IO")
				(number "15")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VS")
				(number "22")
			)
			(pin passive line
				(at 0 27.94 270)
				(length 2.54)
				(hide yes)
				(name "VS")
				(number "28")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 12.7 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "25")
			)
			(pin no_connect line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at 12.7 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin output line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "OB2")
				(number "1")
			)
			(pin output line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "OB1")
				(number "26")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "OA2")
				(number "21")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "OA1")
				(number "24")
			)
			(pin power_out line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "5VOUT")
				(number "8")
			)
			(pin passive line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "BRB")
				(number "27")
			)
			(pin passive line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "BRA")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMC2224-LA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 -26.67 0)
		)
		(property "Value" "TMC2224-LA"
			(at 7.62 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-32-1EP_5x5mm_P0.5mm_EP3.4x3.4mm_ThermalVias"
			(at 0 -45.72 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/TMC2202_TMC2208_TMC2224_datasheet_rev1.13.pdf"
			(at 0 -50.8 0)
		)
		(property "Description" "Standalone driver for two-phase bipolar stepper motor, 2A, 4.75… 36V, UART, internal FETs, QFN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Standalone driver stepper motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFN*1EP?5x5mm?P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TMC2224-LA_1_1"
			(pin passive line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "VCP")
				(number "6")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "MS1")
				(number "28")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "MS2")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PDN_UART")
				(number "20")
			)
			(pin passive line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "CPO")
				(number "4")
			)
			(pin passive line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "CPI")
				(number "5")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "CLK")
				(number "27")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SPREAD")
				(number "22")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "STEP")
				(number "25")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "DIR")
				(number "23")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "ENN")
				(number "24")
			)
			(pin output line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "DIAG")
				(number "21")
			)
			(pin output line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "INDEX")
				(number "2")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "VREF")
				(number "15")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VCC_IO")
				(number "19")
			)
			(pin passive line
				(at 0 27.94 270)
				(length 2.54)
				(hide yes)
				(name "VS")
				(number "14")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VS")
				(number "7")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "26")
			)
			(pin output line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "OB2")
				(number "13")
			)
			(pin output line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "OB1")
				(number "11")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "OA2")
				(number "8")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "OA1")
				(number "10")
			)
			(pin power_out line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "5VOUT")
				(number "18")
			)
			(pin passive line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "BRB")
				(number "12")
			)
			(pin passive line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "BRA")
				(number "9")
			)
			(pin input line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "TEST")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMC2226-SA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "TMC2226-SA"
			(at 5.08 -2.54 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP2.75x6.2mm_ThermalVias"
			(at 0 -45.72 0)
		)
		(property "Datasheet" "https://www.trinamic.com/fileadmin/assets/Products/ICs_Documents/TMC2226_datasheet_rev1.10.pdf"
			(at 0 -48.26 0)
		)
		(property "Description" "Power Driver For Stepper Motors, 2.0A, 4.75-29V, HTSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Standalone driver stepper motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*1EP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TMC2226-SA_1_1"
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "VCP")
				(number "9")
			)
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "CPO")
				(number "7")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "CPI")
				(number "8")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "CLK")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PDN_UART")
				(number "18")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "STEP")
				(number "20")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "DIR")
				(number "23")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "MS1_AD0")
				(number "12")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "MS2_AD1")
				(number "14")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "~{EN}")
				(number "5")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "STDBY")
				(number "24")
			)
			(pin output line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "DIAG")
				(number "15")
			)
			(pin output line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "INDEX")
				(number "16")
			)
			(pin passive line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "VREF")
				(number "21")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "SPREAD")
				(number "10")
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 2.54)
				(name "VCC_IO")
				(number "19")
			)
			(pin power_out line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "5VOUT")
				(number "11")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "VS")
				(number "26")
			)
			(pin passive line
				(at 2.54 -33.02 90)
				(length 2.54)
				(name "NC")
				(number "13")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 2.54)
				(name "VS")
				(number "3")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "OA1")
				(number "28")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "OA2")
				(number "25")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "OB1")
				(number "1")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "OB2")
				(number "4")
			)
			(pin passive line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "BRA")
				(number "27")
			)
			(pin passive line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "BRB")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMC262"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "TMC262"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 0 -35.56 0)
		)
		(property "Datasheet" "https://www.trinamic.com/fileadmin/assets/Products/ICs_Documents/TMC262_Datasheet.pdf"
			(at 1.27 -34.29 0)
		)
		(property "Description" "Driver for two-phase stepper motors with external mosfet"
			(at 0 0 0)
		)
		(property "ki_keywords" "trinamic tlc262 stepper"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TMC262_0_1")
		(symbol "TMC262_1_1"
			(pin input line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "DIR")
				(number "30")
			)
			(pin input line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "STEP")
				(number "31")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "~{ENN}")
				(number "15")
			)
			(pin input clock
				(at -20.32 5.08 0)
				(length 2.54)
				(name "CLK")
				(number "16")
			)
			(pin tri_state line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "SD0")
				(number "10")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "SDI")
				(number "11")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "SCK")
				(number "12")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "CSN")
				(number "14")
			)
			(pin input line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "TST_MODE")
				(number "32")
			)
			(pin power_out line
				(at -7.62 33.02 270)
				(length 2.54)
				(name "5VOUT")
				(number "9")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "VCC_IO")
				(number "29")
			)
			(pin input line
				(at -2.54 -33.02 90)
				(length 2.54)
				(name "DIE_PAD")
				(number "33")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VS")
				(number "25")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GNDP")
				(number "28")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "VHS")
				(number "24")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 5.08 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "HA1")
				(number "2")
			)
			(pin output line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "HA2")
				(number "3")
			)
			(pin input line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "BMA1")
				(number "5")
			)
			(pin input line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "BMA2")
				(number "4")
			)
			(pin output line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "LA1")
				(number "6")
			)
			(pin output line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "LA2")
				(number "7")
			)
			(pin input line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "SRA")
				(number "8")
			)
			(pin input line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "SRB")
				(number "17")
			)
			(pin output line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "LB1")
				(number "19")
			)
			(pin output line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "LB2")
				(number "18")
			)
			(pin input line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "BMB1")
				(number "20")
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "BMB2")
				(number "21")
			)
			(pin output line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "HB1")
				(number "23")
			)
			(pin output line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "HB2")
				(number "22")
			)
			(pin output line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "TST_ANA")
				(number "26")
			)
			(pin output line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "SG_TST")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMC2660"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 27.94 0)
		)
		(property "Value" "TMC2660"
			(at 22.86 25.4 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at -12.7 -43.18 0)
		)
		(property "Datasheet" "https://www.trinamic.com/fileadmin/assets/Products/ICs_Documents/TMC2660_datasheet_Rev1.07.pdf"
			(at -2.54 -39.37 0)
		)
		(property "Description" "Standalone driver for two-phase bipolar stepper motor, 0-30V, 2.4A, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Standalone driver stepper motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*44*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "TMC2660_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SDI")
				(number "15")
			)
			(pin passive line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "SDO")
				(number "14")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "SCK")
				(number "16")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "18")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "DIR")
				(number "41")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "STEP")
				(number "42")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "ST_ALONE/TST_ANA")
				(number "37")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "TST_MODE")
				(number "43")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "~{EN}")
				(number "19")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "CLK")
				(number "21")
			)
			(pin power_in line
				(at -10.16 25.4 270)
				(length 2.54)
				(name "VCC_IO")
				(number "40")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "VHS")
				(number "35")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VS")
				(number "36")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin free line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "n.c.")
				(number "1")
			)
			(pin no_connect line
				(at 2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "n.c.")
				(number "20")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "VSA")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "n.c.")
				(number "34")
			)
			(pin power_in line
				(at 7.62 25.4 270)
				(length 2.54)
				(name "VSB")
				(number "30")
			)
			(pin free line
				(at 10.16 25.4 270)
				(length 2.54)
				(name "n.c.")
				(number "33")
			)
			(pin power_out line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "5VOUT")
				(number "13")
			)
			(pin power_out line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "OA1")
				(number "2")
			)
			(pin passive line
				(at 17.78 12.7 180)
				(length 2.54)
				(hide yes)
				(name "OA1")
				(number "3")
			)
			(pin passive line
				(at 17.78 12.7 180)
				(length 2.54)
				(hide yes)
				(name "OA1")
				(number "7")
			)
			(pin passive line
				(at 17.78 12.7 180)
				(length 2.54)
				(hide yes)
				(name "OA1")
				(number "8")
			)
			(pin passive line
				(at 17.78 10.16 180)
				(length 2.54)
				(hide yes)
				(name "OA2")
				(number "10")
			)
			(pin passive line
				(at 17.78 10.16 180)
				(length 2.54)
				(hide yes)
				(name "OA2")
				(number "11")
			)
			(pin power_out line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "OA2")
				(number "5")
			)
			(pin passive line
				(at 17.78 10.16 180)
				(length 2.54)
				(hide yes)
				(name "OA2")
				(number "6")
			)
			(pin power_out line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "OB1")
				(number "26")
			)
			(pin passive line
				(at 17.78 5.08 180)
				(length 2.54)
				(hide yes)
				(name "OB1")
				(number "27")
			)
			(pin passive line
				(at 17.78 5.08 180)
				(length 2.54)
				(hide yes)
				(name "OB1")
				(number "31")
			)
			(pin passive line
				(at 17.78 5.08 180)
				(length 2.54)
				(hide yes)
				(name "OB1")
				(number "32")
			)
			(pin power_out line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "OB2")
				(number "23")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OB2")
				(number "24")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OB2")
				(number "28")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OB2")
				(number "29")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "BRA")
				(number "9")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "SRA")
				(number "12")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "BRB")
				(number "25")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "SRB")
				(number "22")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "SG_TST")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMC5130A-TA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 38.1 0)
		)
		(property "Value" "TMC5130A-TA"
			(at 11.43 38.1 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48-1EP_7x7mm_P0.5mm_EP5x5mm_ThermalVias"
			(at 0 -66.04 0)
		)
		(property "Datasheet" "https://www.trinamic.com/fileadmin/assets/Products/ICs_Documents/TMC5130_datasheet_Rev1.17.pdf"
			(at -26.67 24.13 0)
		)
		(property "Description" "Power Driver For Stepper Motors, 2.0A, 4.75-46V, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Standalone driver stepper motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TMC5130A-TA_0_1")
		(symbol "TMC5130A-TA_1_1"
			(pin passive line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "VCP")
				(number "38")
			)
			(pin passive line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "CP0")
				(number "35")
			)
			(pin passive line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "CPI")
				(number "37")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "CLK")
				(number "2")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "~{CS}_CFG3")
				(number "3")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "SCK_CFG2")
				(number "4")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SDI_NAI_CFG1")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "SDO_NAO_CFG0")
				(number "7")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "REFL_STEP")
				(number "8")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "REFR_DIR")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "ENCN_DCO")
				(number "23")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "ENCB_DCEN_CFG4")
				(number "24")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "ENCA_DCIN_CFG5")
				(number "25")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "~{DRV_EN}_CFG6")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "SWN_DIAG0")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "SWP_DIAG1")
				(number "27")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "SWSEL")
				(number "28")
			)
			(pin input line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "AIN_IREF")
				(number "30")
			)
			(pin input line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "SD_MODE")
				(number "11")
			)
			(pin input line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "SPI_MODE")
				(number "12")
			)
			(pin input line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "TST_MODE")
				(number "1")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VCC_IO")
				(number "10")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "34")
			)
			(pin power_out line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "5VOUT")
				(number "33")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 2.54)
				(name "GNDP")
				(number "13")
			)
			(pin passive line
				(at -2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GNDP")
				(number "48")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GNDA")
				(number "32")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VSA")
				(number "39")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "EP")
				(number "49")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VS")
				(number "40")
			)
			(pin passive line
				(at 5.08 -38.1 90)
				(length 2.54)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "VS")
				(number "21")
			)
			(pin passive line
				(at 7.62 -38.1 90)
				(length 2.54)
				(name "NC")
				(number "31")
			)
			(pin passive line
				(at 10.16 -38.1 90)
				(length 2.54)
				(name "NC")
				(number "36")
			)
			(pin no_connect line
				(at 15.24 33.02 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "41")
			)
			(pin no_connect line
				(at 15.24 30.48 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "43")
			)
			(pin no_connect line
				(at 15.24 27.94 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "45")
			)
			(pin no_connect line
				(at 15.24 25.4 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "47")
			)
			(pin no_connect line
				(at 15.24 12.7 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "14")
			)
			(pin no_connect line
				(at 15.24 10.16 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "16")
			)
			(pin no_connect line
				(at 15.24 7.62 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "18")
			)
			(pin no_connect line
				(at 15.24 5.08 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "20")
			)
			(pin no_connect line
				(at 15.24 2.54 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "22")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "OA1")
				(number "46")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "OA2")
				(number "42")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "OB1")
				(number "15")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "OB2")
				(number "19")
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "BRA")
				(number "44")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "BRB")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMC5160A-TA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 38.1 0)
		)
		(property "Value" "TMC5160A-TA"
			(at 10.16 38.1 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48-1EP_7x7mm_P0.5mm_EP5x5mm_ThermalVias"
			(at 0 -50.8 0)
		)
		(property "Datasheet" "https://www.trinamic.com/fileadmin/assets/Products/ICs_Documents/TMC5160A_Datasheet_Rev1.14.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "20A Driver for two-phase bipolar stepper motor, SPI, UART, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "stepper motor driver trinamic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TMC5160A-TA_1_0")
		(symbol "TMC5160A-TA_1_1"
			(pin passive line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "VCP")
				(number "34")
			)
			(pin passive line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "CPO")
				(number "31")
			)
			(pin passive line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "CPI")
				(number "32")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "CLK")
				(number "12")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "~{CS}/CFG3")
				(number "13")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "SCK/CFG2")
				(number "14")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SDI/CFG1")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "SDO/CFG0")
				(number "16")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "REFL/STEP")
				(number "17")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "REFR/DIR")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "ENCN/DCO/CFG6")
				(number "25")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "ENCB/DCEN/CFG4")
				(number "23")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "ENCA/DCIN/CFG5")
				(number "24")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "~{DRV_EN}")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "SWN/DIAG0")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "SWP/DIAG1")
				(number "27")
			)
			(pin input line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "SD_MODE")
				(number "21")
			)
			(pin input line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "SPI_MODE")
				(number "22")
			)
			(pin input line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "TST_MODE")
				(number "11")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VCC_IO")
				(number "20")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "29")
			)
			(pin power_out line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "5VOUT")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 2.54)
				(name "GNDD")
				(number "19")
			)
			(pin passive line
				(at -2.54 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GNDD")
				(number "30")
			)
			(pin power_out line
				(at 0 38.1 270)
				(length 2.54)
				(name "12VOUT")
				(number "3")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GNDA")
				(number "6")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VSA")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "EP")
				(number "49")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VS")
				(number "33")
			)
			(pin output line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "HA1")
				(number "41")
			)
			(pin passive line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "BMA1")
				(number "40")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "LA1")
				(number "39")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "HA2")
				(number "36")
			)
			(pin passive line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "BMA2")
				(number "37")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "LA2")
				(number "38")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "HB1")
				(number "1")
			)
			(pin passive line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "BMB1")
				(number "48")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "LB1")
				(number "47")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "HB2")
				(number "44")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "BMB2")
				(number "45")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "LB2")
				(number "46")
			)
			(pin passive line
				(at 17.78 0 180)
				(length 2.54)
				(name "SRAH")
				(number "8")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "SRAL")
				(number "7")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "SRBH")
				(number "9")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "SRBL")
				(number "10")
			)
			(pin passive line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "CA1")
				(number "42")
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "CA2")
				(number "35")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "CB1")
				(number "2")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "CB2")
				(number "43")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VNH2SP30"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "VNH2SP30"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_SO:ST_MultiPowerSO-30"
			(at 0 23.495 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/group2/66/b8/f5/2c/9a/66/41/c7/CD00043711/files/CD00043711.pdf/jcr:content/translations/en.CD00043711.pdf"
			(at -12.7 25.4 0)
		)
		(property "Description" "Full Bridge Motor Driver, 41V, 30A, -40 to 150C"
			(at 0 0 0)
		)
		(property "ki_keywords" "full-bridge h-bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*MultiPowerSO*"
			(at 0 0 0)
		)
		(symbol "VNH2SP30_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "INA")
				(number "5")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "INB")
				(number "11")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "PWM")
				(number "8")
			)
			(pin no_connect line
				(at -12.7 0 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -12.7 -2.54 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -12.7 -5.08 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -12.7 -7.62 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -12.7 -10.16 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at -12.7 -12.7 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "29")
			)
			(pin no_connect line
				(at -12.7 -15.24 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin no_connect line
				(at -12.7 -17.78 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin no_connect line
				(at -12.7 -20.32 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 5.08)
				(name "GNDB")
				(number "18")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "GNDB")
				(number "19")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "GNDB")
				(number "20")
			)
			(pin passive line
				(at 0 27.94 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "13")
			)
			(pin passive line
				(at 0 27.94 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "23")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 5.08)
				(name "VCC")
				(number "3")
			)
			(pin passive line
				(at 0 27.94 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "31")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 5.08)
				(name "GNDA")
				(number "26")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "GNDA")
				(number "27")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "GNDA")
				(number "28")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "EN/DIAA")
				(number "6")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "EN/DIAB")
				(number "10")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "OUTA")
				(number "1")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 5.08)
				(hide yes)
				(name "OUTA")
				(number "25")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 5.08)
				(hide yes)
				(name "OUTA")
				(number "30")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 5.08)
				(hide yes)
				(name "OUTA")
				(number "33")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "OUTB")
				(number "15")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 5.08)
				(hide yes)
				(name "OUTB")
				(number "16")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 5.08)
				(hide yes)
				(name "OUTB")
				(number "21")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 5.08)
				(hide yes)
				(name "OUTB")
				(number "32")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "CS")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VNH5019A-E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "VNH5019A-E"
			(at 12.7 13.97 0)
		)
		(property "Footprint" "Package_SO:ST_MultiPowerSO-30"
			(at 22.86 -13.97 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/vnh5019a-e.pdf"
			(at -11.43 21.59 0)
		)
		(property "Description" "Full Bridge Motor Driver, 41V, 30A, -40 to 150C, MultiPowerSO-30"
			(at 0 0 0)
		)
		(property "ki_keywords" "full-bridge h-bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*MultiPowerSO*"
			(at 0 0 0)
		)
		(symbol "VNH5019A-E_0_1")
		(symbol "VNH5019A-E_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "INA")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "INB")
				(number "10")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PWM")
				(number "7")
			)
			(pin open_collector line
				(at -12.7 0 0)
				(length 2.54)
				(name "EN/DIAGA")
				(number "5")
			)
			(pin open_collector line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "EN/DIAGB")
				(number "9")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "CS_DIS")
				(number "6")
			)
			(pin output line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "CS")
				(number "8")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VBAT")
				(number "12")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GNDA")
				(number "26")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GNDA")
				(number "27")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GNDA")
				(number "28")
			)
			(pin passive line
				(at 5.08 15.24 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "13")
			)
			(pin passive line
				(at 5.08 15.24 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "23")
			)
			(pin power_in line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin passive line
				(at 5.08 15.24 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "31")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "GNDB")
				(number "18")
			)
			(pin passive line
				(at 5.08 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GNDB")
				(number "19")
			)
			(pin passive line
				(at 5.08 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GNDB")
				(number "20")
			)
			(pin no_connect line
				(at 10.16 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "29")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "CP")
				(number "11")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUTA")
				(number "1")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUTA")
				(number "25")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUTA")
				(number "30")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUTA")
				(number "33")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "15")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUTB")
				(number "16")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUTB")
				(number "21")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "OUTB")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ZXBM5210-S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "ZXBM5210-S"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ZXBM5210.pdf"
			(at 0 0 0)
		)
		(property "Description" "Reversible DC motor drive with speed control, 3-18V, 0.85A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "H-bridge, motor driver, PWM, single coil"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ZXBM5210-S_0_0"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VREF")
				(number "6")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "FWD")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "REV")
				(number "5")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VM")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT1")
				(number "1")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "7")
			)
		)
		(symbol "ZXBM5210-S_0_1")
		(embedded_fonts no)
	)
	(symbol "ZXBM5210-SP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "ZXBM5210-SP"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Package_SO:Diodes_SO-8EP"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ZXBM5210.pdf"
			(at 0 0 0)
		)
		(property "Description" "Reversible DC motor drive with speed control, 3-18V, 0.85A, SOIC-8EP"
			(at 0 0 0)
		)
		(property "ki_keywords" "H-bridge, motor driver, PWM, single coil"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Diodes*SO*EP*"
			(at 0 0 0)
		)
		(symbol "ZXBM5210-SP_0_0"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VREF")
				(number "6")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "FWD")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "REV")
				(number "5")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VM")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT1")
				(number "1")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "7")
			)
		)
		(symbol "ZXBM5210-SP_0_1")
		(embedded_fonts no)
	)
	(symbol "A4950K"
		(extends "A4950E")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "A4950K"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.3mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.allegromicro.com/~/media/Files/Datasheets/A4950-Datasheet.ashx"
			(at -7.62 8.89 0)
		)
		(property "Description" "Full-Bridge, DMOS PWM, Motor Driver, 40V, 3.5A, -40 to +125C"
			(at 0 0 0)
		)
		(property "ki_keywords" "full-bridge h-bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC-*1EP*"
			(at 0 0 0)
		)
	)
	(symbol "A4953_LJ"
		(extends "A4950E")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "A4953_LJ"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.3mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "www.allegromicro.com/~/media/Files/Datasheets/A4952-3-Datasheet.ashx?la=en"
			(at -7.62 8.89 0)
		)
		(property "Description" "Full-Bridge, DMOS PWM, Motor Driver, 40V, 2A, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Full-bridge h-bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC-*1EP*"
			(at 0 0 0)
		)
	)
	(symbol "DRV8212P"
		(extends "DRV8837C")
		(property "Reference" "U"
			(at 6.35 11.43 0)
		)
		(property "Value" "DRV8212P"
			(at -10.16 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm_ThermalVias"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/drv8212p.pdf"
			(at 0 0 0)
		)
		(property "Description" "H-Bridge driver, 4A, Low Voltage, PWM input, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "half bridge driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "DRV8837"
		(extends "DRV8837C")
		(property "Reference" "U"
			(at 6.35 11.43 0)
		)
		(property "Value" "DRV8837"
			(at -10.16 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv8837.pdf"
			(at 0 0 0)
		)
		(property "Description" "H-Bridge driver, 1.8A, Low Voltage, PWM input, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "half bridge driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "L293D"
		(extends "L293")
		(property "Reference" "U"
			(at -5.08 26.035 0)
		)
		(property "Value" "L293D"
			(at -5.08 24.13 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 6.35 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/l293.pdf"
			(at -7.62 17.78 0)
		)
		(property "Description" "Quadruple Half-H Drivers"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half-H Driver Motor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "L298N"
		(extends "L298HN")
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "L298N"
			(at 12.7 16.51 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical"
			(at 1.27 -16.51 0)
		)
		(property "Datasheet" "http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/CD00000240.pdf"
			(at 3.81 6.35 0)
		)
		(property "Description" "Dual full bridge motor driver, up to 46V, 4A, Multiwatt15-V"
			(at 0 0 0)
		)
		(property "ki_keywords" "H-bridge motor driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*StaggerOdd*Vertical*"
			(at 0 0 0)
		)
	)
	(symbol "SLA7042M"
		(extends "SLA7044M")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "SLA7042M"
			(at 7.62 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "www.sumzi.com/upload/files/2007/07/2007073114282034189.PDF"
			(at 0 0 0)
		)
		(property "Description" "Unipolar PWM high-current motor driver"
			(at 0 0 0)
		)
		(property "ki_keywords" "Stepper driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SLA704XM"
			(at 0 0 0)
		)
	)
	(symbol "SLA7071MPRT"
		(extends "SLA7070MPRT")
		(property "Reference" "U"
			(at -10.16 25.4 0)
		)
		(property "Value" "SLA7071MPRT"
			(at 7.62 -25.4 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.semicon.sanken-ele.co.jp/sk_content/sla7071mprt_ds_en.pdf"
			(at 0 0 0)
		)
		(property "Description" "Unipolar 2-phase stepper motor driver, Full and Half step, 1.5A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Stepper driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ZIP23"
			(at 0 0 0)
		)
	)
	(symbol "SLA7072MPRT"
		(extends "SLA7070MPRT")
		(property "Reference" "U"
			(at -10.16 25.4 0)
		)
		(property "Value" "SLA7072MPRT"
			(at 7.62 -25.4 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.semicon.sanken-ele.co.jp/sk_content/sla7072mprt_ds_en.pdf"
			(at 0 0 0)
		)
		(property "Description" "Unipolar 2-phase stepper motor driver, Full and Half step, 2A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Stepper driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ZIP23"
			(at 0 0 0)
		)
	)
	(symbol "SLA7073MPRT"
		(extends "SLA7070MPRT")
		(property "Reference" "U"
			(at -10.16 25.4 0)
		)
		(property "Value" "SLA7073MPRT"
			(at 7.62 -25.4 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.semicon.sanken-ele.co.jp/sk_content/sla7073mprt_ds_en.pdf"
			(at 0 0 0)
		)
		(property "Description" "Unipolar 2-phase stepper motor driver, Full and Half step, 3A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Stepper driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ZIP23"
			(at 0 0 0)
		)
	)
	(symbol "SLA7076MPRT"
		(extends "SLA7075MPRT")
		(property "Reference" "U"
			(at -10.16 25.4 0)
		)
		(property "Value" "SLA7076MPRT"
			(at 7.62 -25.4 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.semicon.sanken-ele.co.jp/sk_content/sla7076mprt_ds_en.pdf"
			(at 0 0 0)
		)
		(property "Description" "Unipolar 2-phase stepper motor driver, Microstep, 1.5A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Stepper driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ZIP23"
			(at 0 0 0)
		)
	)
	(symbol "SLA7077MPRT"
		(extends "SLA7075MPRT")
		(property "Reference" "U"
			(at -10.16 25.4 0)
		)
		(property "Value" "SLA7077MPRT"
			(at 7.62 -25.4 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.semicon.sanken-ele.co.jp/sk_content/sla7077mprt_ds_en.pdf"
			(at 0 0 0)
		)
		(property "Description" "Unipolar 2-phase stepper motor driver, Microstep, 2A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Stepper driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ZIP23"
			(at 0 0 0)
		)
	)
	(symbol "SLA7078MPRT"
		(extends "SLA7075MPRT")
		(property "Reference" "U"
			(at -10.16 25.4 0)
		)
		(property "Value" "SLA7078MPRT"
			(at 7.62 -25.4 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.semicon.sanken-ele.co.jp/sk_content/sla7078mprt_ds_en.pdf"
			(at 0 0 0)
		)
		(property "Description" "Unipolar 2-phase stepper motor driver, Microstep, 3A"
			(at 0 0 0)
		)
		(property "ki_keywords" "Stepper driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ZIP23"
			(at 0 0 0)
		)
	)
)
