(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "DRV8860"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 17.78 0)
		)
		(property "Value" "DRV8860"
			(at 10.16 15.24 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 10.16 12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv8860.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "8-Channel Serial Interface Low-Side Driver"
			(at 0 0 0)
		)
		(property "ki_keywords" "Relay Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DRV8860_0_1")
		(symbol "DRV8860_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "ENABLE")
				(number "8")
			)
			(pin input inverted
				(at -12.7 5.08 0)
				(length 2.54)
				(name "Latch")
				(number "4")
			)
			(pin input clock
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCLK")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "DIN")
				(number "2")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DOUT")
				(number "6")
			)
			(pin open_collector inverted
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "FAULT")
				(number "7")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VM")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUT1")
				(number "16")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT2")
				(number "15")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT3")
				(number "14")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT4")
				(number "13")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT5")
				(number "12")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT6")
				(number "11")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUT7")
				(number "10")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT8")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DRV8860_PWPR"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 17.78 0)
		)
		(property "Value" "DRV8860_PWPR"
			(at 10.16 15.24 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16-1EP_4.4x5mm_P0.65mm"
			(at 10.16 12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/drv8860.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "8-Channel Serial Interface Low-Side Driver"
			(at 0 0 0)
		)
		(property "ki_keywords" "Relay Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DRV8860_PWPR_0_1")
		(symbol "DRV8860_PWPR_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "ENABLE")
				(number "8")
			)
			(pin input inverted
				(at -12.7 5.08 0)
				(length 2.54)
				(name "Latch")
				(number "4")
			)
			(pin input clock
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCLK")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "DIN")
				(number "2")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DOUT")
				(number "6")
			)
			(pin open_collector inverted
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "FAULT")
				(number "7")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VM")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in inverted
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "PAD")
				(number "17")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "OUT1")
				(number "16")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT2")
				(number "15")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT3")
				(number "14")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT4")
				(number "13")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT5")
				(number "12")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT6")
				(number "11")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUT7")
				(number "10")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT8")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX4820xUP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 17.78 0)
		)
		(property "Value" "MAX4820xUP"
			(at 10.16 15.24 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP2.85x4mm"
			(at 10.16 12.7 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX4820-MAX4821.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "8-Channel Serial Interface Low-Side Driver, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Relay Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX4820xUP_0_0"
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT1")
				(number "20")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT2")
				(number "19")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT3")
				(number "17")
			)
		)
		(symbol "MAX4820xUP_0_1")
		(symbol "MAX4820xUP_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{SET}")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCLK")
				(number "6")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "DOUT")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "4")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "DIN")
				(number "5")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "COM")
				(number "15")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT4")
				(number "16")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT5")
				(number "14")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUT6")
				(number "13")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT7")
				(number "11")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "OUT8")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX4821xUP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 17.78 0)
		)
		(property "Value" "MAX4821xUP"
			(at 10.16 15.24 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP2.85x4mm"
			(at 10.16 12.7 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX4820-MAX4821.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "8-Channel Parallel Interface Low-Side Driver, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Relay Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX4821xUP_0_0"
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT1")
				(number "20")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUT2")
				(number "19")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT3")
				(number "17")
			)
		)
		(symbol "MAX4821xUP_0_1")
		(symbol "MAX4821xUP_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{SET}")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A0")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A1")
				(number "7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "4")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "LVL")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "COM")
				(number "15")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT4")
				(number "16")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT5")
				(number "14")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUT6")
				(number "13")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "OUT7")
				(number "11")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "OUT8")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPL9201_TSSOP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 17.78 0)
		)
		(property "Value" "TPL9201_TSSOP"
			(at 10.16 15.24 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_ThermalVias"
			(at 10.16 12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpl9201.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "8-CHANNEL RELAY DRIVER WITH INTEGRATED 5-V LDO AND ZERO-VOLT DETECTION TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Relay Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x6.5mm*P0.65mm*ThermalVias*"
			(at 0 0 0)
		)
		(symbol "TPL9201_TSSOP_0_1")
		(symbol "TPL9201_TSSOP_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 5.08)
				(name "EN1")
				(number "12")
			)
			(pin input inverted
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "CS")
				(number "16")
			)
			(pin input clock
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "SCLK")
				(number "17")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 5.08)
				(name "MOSI")
				(number "15")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 5.08)
				(name "SYN")
				(number "20")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "Vin")
				(number "19")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 5.08)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 5.08)
				(name "PAD")
				(number "21")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 5.08)
				(name "OUT1")
				(number "2")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 5.08)
				(name "OUT2")
				(number "3")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 5.08)
				(name "OUT3")
				(number "4")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "OUT4")
				(number "5")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "OUT5")
				(number "6")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "OUT6")
				(number "7")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "OUT7")
				(number "8")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 5.08)
				(name "OUT8")
				(number "9")
			)
			(pin power_out line
				(at 12.7 -12.7 180)
				(length 5.08)
				(name "5Vout")
				(number "18")
			)
			(pin bidirectional inverted
				(at 12.7 -15.24 180)
				(length 5.08)
				(name "RST")
				(number "14")
			)
			(pin output line
				(at 12.7 -20.32 180)
				(length 5.08)
				(name "Rdelay")
				(number "13")
			)
			(pin output line
				(at 12.7 -22.86 180)
				(length 5.08)
				(name "ZVS")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
)
