(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "MAX1968xUI"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "MAX1968xUI"
			(at 5.08 16.51 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP2.85x5.4mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1968-MAX1969.pdf"
			(at 0 0 0)
		)
		(property "Description" "Power Driver for Peltier TEC Modules, ±3A, HTSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "thermoelectric cooler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX1968xUI_0_1")
		(symbol "MAX1968xUI_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "~{SHDN}")
				(number "17")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "CTLI")
				(number "3")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "FREQ")
				(number "12")
			)
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "REF")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "MAXIN")
				(number "26")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "MAXIP")
				(number "27")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "MAXV")
				(number "28")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "COMP")
				(number "25")
			)
			(pin output line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "ITEC")
				(number "13")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "PVDD1")
				(number "18")
			)
			(pin passive line
				(at 2.54 17.78 270)
				(length 2.54)
				(hide yes)
				(name "PVDD1")
				(number "20")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "22")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "24")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "PGND")
				(number "5")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "7")
			)
			(pin passive line
				(at 5.08 17.78 270)
				(length 2.54)
				(hide yes)
				(name "PVDD2")
				(number "11")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "PVDD2")
				(number "9")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "LX1")
				(number "19")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "LX1")
				(number "21")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "LX1")
				(number "23")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OS1")
				(number "15")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "CS")
				(number "16")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OS2")
				(number "14")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "LX2")
				(number "10")
			)
			(pin power_out line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "LX2")
				(number "6")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "LX2")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX1969xUI"
		(extends "MAX1968xUI")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "MAX1969xUI"
			(at 5.08 16.51 0)
		)
		(property "Footprint" "Package_SO:HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP2.85x5.4mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1968-MAX1969.pdf"
			(at 0 0 0)
		)
		(property "Description" "Power Driver for Peltier TEC Modules, 6A, HTSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "thermoelectric cooler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
)
