(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "CCGM1A1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 8.89 0)
		)
		(property "Value" "CCGM1A1"
			(at 11.43 8.89 0)
		)
		(property "Footprint" "Package_BGA:BGA-324_15x15mm_Layout18x18_P0.8mm"
			(at -5.08 16.51 0)
		)
		(property "Datasheet" "https://colognechip.com/docs/ds1001-gatemate1-datasheet-2022-05.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "Cologne Chip GateMate FPGA, BGA-324"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "GateMate FPGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*15x15mm*Layout18x18*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "CCGM1A1_1_1"
			(text "SERDES"
				(at 0 0 0)
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "SER_RX_P")
				(number "U11")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "SER_RX_N")
				(number "V11")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "SER_TX_P")
				(number "U13")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "SER_TX_N")
				(number "V13")
			)
			(pin passive line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "SER_RTERM")
				(number "V12")
			)
		)
		(symbol "CCGM1A1_2_1"
			(text "CONFIGURATION"
				(at -11.43 6.35 0)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 3.81)
				(name "CFG_MD0/IO_WA_A0")
				(number "R5")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 3.81)
				(name "CFG_MD1/IO_WA_B0")
				(number "T5")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 3.81)
				(name "CFG_MD2/IO_WA_A1")
				(number "U4")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 3.81)
				(name "CFG_MD3/IO_WA_B1")
				(number "V4")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "JTAG_TCK/IO_WA_A5")
				(number "R3")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "JTAG_TMS/IO_WA_B4")
				(number "T3")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "JTAG_TDI/IO_WA_A4")
				(number "T2")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "JTAG_TDO/IO_WA_B3")
				(number "U2")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 3.81)
				(name "POR_EN/IO_WA_A3")
				(number "U1")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VDD_WA")
				(number "N5")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 3.81)
				(hide yes)
				(name "VDD_WA")
				(number "P3")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 3.81)
				(hide yes)
				(name "VDD_WA")
				(number "P5")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 3.81)
				(hide yes)
				(name "VDD_WA")
				(number "T1")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 3.81)
				(hide yes)
				(name "VDD_WA")
				(number "U3")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 3.81)
				(name "IO_WA_A2/~{CFG_FAILED}")
				(number "V2")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 3.81)
				(name "IO_WA_B2/CFG_DONE")
				(number "V3")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "IO_WA_B7/SPI_D0")
				(number "P2")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "IO_WA_A7/SPI_D1")
				(number "P1")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "IO_WA_B6/SPI_D2")
				(number "R2")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "IO_WA_A6/SPI_D3")
				(number "R1")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "IO_WA_A8/~{SPI_CS}")
				(number "N3")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 3.81)
				(name "IO_WA_B8/SPI_CLK")
				(number "N4")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 3.81)
				(name "IO_WA_B5/SPI_FWD")
				(number "R4")
			)
		)
		(symbol "CCGM1A1_3_1"
			(text "IO North"
				(at 0 2.54 0)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 3.81)
				(name "IO_NA_A0")
				(number "A3")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "IO_NA_B0")
				(number "B3")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "IO_NA_A1")
				(number "A4")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "IO_NA_B1")
				(number "B4")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "IO_NA_A2")
				(number "B5")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "IO_NA_B2")
				(number "C5")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "IO_NA_A3")
				(number "C6")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "IO_NA_B3")
				(number "D6")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "IO_NA_A4")
				(number "A6")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "IO_NA_B4")
				(number "B6")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "IO_NA_A5")
				(number "C7")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "IO_NA_B5")
				(number "D7")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "IO_NA_A6")
				(number "C8")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "IO_NA_B6")
				(number "D8")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "IO_NA_A7")
				(number "A8")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "IO_NA_B7")
				(number "B8")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "IO_NA_A8")
				(number "C9")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 3.81)
				(name "IO_NA_B8")
				(number "D9")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 3.81)
				(name "VDD_NA")
				(number "A5")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_NA")
				(number "B7")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_NA")
				(number "E6")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_NA")
				(number "E8")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_NA")
				(number "F7")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 3.81)
				(name "VDD_NB")
				(number "B10")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_NB")
				(number "B13")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_NB")
				(number "E10")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_NB")
				(number "E12")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_NB")
				(number "F11")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "IO_NB_A0")
				(number "B9")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "IO_NB_B0")
				(number "A9")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "IO_NB_A1")
				(number "D10")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "IO_NB_B1")
				(number "C10")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "IO_NB_A2")
				(number "B11")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "IO_NB_B2")
				(number "A11")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "IO_NB_A3")
				(number "D11")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "IO_NB_B3")
				(number "C11")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "IO_NB_A4")
				(number "B12")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "IO_NB_B4")
				(number "A12")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "IO_NB_A5")
				(number "D12")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "IO_NB_B5")
				(number "C12")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "IO_NB_A6")
				(number "D13")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "IO_NB_B6")
				(number "C13")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "IO_NB_A7")
				(number "B14")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "IO_NB_B7")
				(number "A14")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "IO_NB_A8")
				(number "D14")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "IO_NB_B8")
				(number "C14")
			)
		)
		(symbol "CCGM1A1_4_1"
			(text "IO East"
				(at 0 2.54 0)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 3.81)
				(name "IO_EA_A0")
				(number "M15")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "IO_EA_B0")
				(number "M14")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "IO_EA_A1")
				(number "L16")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "IO_EA_B1")
				(number "L15")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "IO_EA_A2")
				(number "K18")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "IO_EA_B2")
				(number "K17")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "IO_EA_A3")
				(number "K16")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "IO_EA_B3")
				(number "K15")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "IO_EA_A4")
				(number "J18")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "IO_EA_B4")
				(number "J17")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "IO_EA_A5")
				(number "J16")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "IO_EA_B5")
				(number "J15")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "IO_EA_A6")
				(number "H16")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "IO_EA_B6")
				(number "H15")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "IO_EA_A7")
				(number "G18")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "IO_EA_B7")
				(number "G17")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "IO_EA_A8")
				(number "G16")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 3.81)
				(name "IO_EA_B8")
				(number "G15")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 3.81)
				(name "VDD_EA")
				(number "G14")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_EA")
				(number "H17")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_EA")
				(number "J14")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_EA")
				(number "L14")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_EA")
				(number "L17")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 3.81)
				(name "VDD_EB")
				(number "A16")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_EB")
				(number "B18")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_EB")
				(number "E14")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_EB")
				(number "E17")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_EB")
				(number "F13")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "IO_EB_A0")
				(number "F18")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "IO_EB_B0")
				(number "F17")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "IO_EB_A1")
				(number "F16")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "IO_EB_B1")
				(number "F15")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "IO_EB_A2")
				(number "D18")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "IO_EB_B2")
				(number "D17")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "IO_EB_A3")
				(number "E16")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "IO_EB_B3")
				(number "E15")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "IO_EB_A4")
				(number "C18")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "IO_EB_B4")
				(number "C17")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "IO_EB_A5")
				(number "B17")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "IO_EB_B5")
				(number "A17")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "IO_EB_A6")
				(number "D16")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "IO_EB_B6")
				(number "C16")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "IO_EB_A7")
				(number "D15")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "IO_EB_B7")
				(number "C15")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "IO_EB_A8")
				(number "B15")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "IO_EB_B8")
				(number "A15")
			)
		)
		(symbol "CCGM1A1_5_1"
			(text "IO South"
				(at 0 2.54 0)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 3.81)
				(name "IO_SA_A0")
				(number "U5")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "IO_SA_B0")
				(number "V5")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "IO_SA_A1")
				(number "R6")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "IO_SA_B1")
				(number "T6")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "IO_SA_A2")
				(number "R7")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "IO_SA_B2")
				(number "T7")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "IO_SA_A3")
				(number "U7")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "IO_SA_B3")
				(number "V7")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "IO_SA_A4")
				(number "R8")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "IO_SA_B4")
				(number "T8")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "IO_SA_A5")
				(number "U8")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "IO_SA_B5")
				(number "V8")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "IO_SA_A6")
				(number "R9")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "IO_SA_B6")
				(number "T9")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "IO_SA_A7")
				(number "R10")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "IO_SA_B7")
				(number "T10")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "IO_SA_A8")
				(number "U10")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 3.81)
				(name "IO_SA_B8")
				(number "V10")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_SA")
				(number "P10")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 3.81)
				(name "VDD_SA")
				(number "P6")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_SA")
				(number "P8")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_SA")
				(number "U6")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_SA")
				(number "U9")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 3.81)
				(name "VDD_SB")
				(number "N11")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_SB")
				(number "N13")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_SB")
				(number "N18")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_SB")
				(number "R15")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_SB")
				(number "T18")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "IO_SB_A0")
				(number "U17")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "IO_SB_B0")
				(number "U18")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "IO_SB_A1")
				(number "R17")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "IO_SB_B1")
				(number "R18")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "IO_SB_A2")
				(number "P17")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "IO_SB_B2")
				(number "P18")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "IO_SB_A3")
				(number "M17")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "IO_SB_B3")
				(number "M18")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "IO_SB_A4")
				(number "P11")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "IO_SB_B4")
				(number "R11")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "CLK3/IO_SB_A5")
				(number "R13")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "IO_SB_B5")
				(number "R14")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "CLK2/IO_SB_A6")
				(number "P14")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "IO_SB_B6")
				(number "P15")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "CLK1/IO_SB_A7")
				(number "P12")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "IO_SB_B7")
				(number "P13")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "CLK0/IO_SB_A8")
				(number "N14")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "IO_SB_B8")
				(number "N15")
			)
		)
		(symbol "CCGM1A1_6_1"
			(text "IO West"
				(at 0 2.54 0)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 3.81)
				(name "IO_WB_A0")
				(number "N1")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "IO_WB_B0")
				(number "N2")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "IO_WB_A1")
				(number "M3")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "IO_WB_B1")
				(number "M4")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "IO_WB_A2")
				(number "L3")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "IO_WB_B2")
				(number "L4")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "IO_WB_A3")
				(number "L1")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "IO_WB_B3")
				(number "L2")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "IO_WB_A4")
				(number "K3")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "IO_WB_B4")
				(number "K4")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "IO_WB_A5")
				(number "K1")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "IO_WB_B5")
				(number "K2")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "IO_WB_A6")
				(number "J3")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "IO_WB_B6")
				(number "J4")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "IO_WB_A7")
				(number "H1")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "IO_WB_B7")
				(number "H2")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "IO_WB_A8")
				(number "H3")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 3.81)
				(name "IO_WB_B8")
				(number "H4")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 3.81)
				(name "VDD_WB")
				(number "H5")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_WB")
				(number "J2")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_WB")
				(number "K5")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_WB")
				(number "M2")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_WB")
				(number "M5")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 3.81)
				(name "VDD_WC")
				(number "A2")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_WC")
				(number "C2")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_WC")
				(number "D5")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_WC")
				(number "F2")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 3.81)
				(hide yes)
				(name "VDD_WC")
				(number "F5")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "IO_WC_A0")
				(number "G1")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "IO_WC_B0")
				(number "G2")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "IO_WC_A1")
				(number "G3")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "IO_WC_B1")
				(number "G4")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "IO_WC_A2")
				(number "F3")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "IO_WC_B2")
				(number "F4")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "IO_WC_A3")
				(number "E1")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "IO_WC_B3")
				(number "E2")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "IO_WC_A4")
				(number "E3")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "IO_WC_B4")
				(number "E4")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "IO_WC_A5")
				(number "D1")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "IO_WC_B5")
				(number "D2")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "IO_WC_A6")
				(number "D3")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "IO_WC_B6")
				(number "D4")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "IO_WC_A7")
				(number "C3")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "IO_WC_B7")
				(number "C4")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "IO_WC_A8")
				(number "B1")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "IO_WC_B8")
				(number "B2")
			)
		)
		(symbol "CCGM1A1_7_1"
			(text "Power"
				(at 2.54 -3.81 0)
			)
			(pin power_in line
				(at -7.62 15.24 270)
				(length 3.81)
				(name "VDD_SER")
				(number "U12")
			)
			(pin passive line
				(at -7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD_SER")
				(number "V17")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 3.81)
				(name "VDD_SER_PLL")
				(number "T16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "GND")
				(number "A1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "C1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "J1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "J11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "J13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "J5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "J7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "J9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "L11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "L13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "L18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "L5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "L7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "L9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "M1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "M10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "M12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "M16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "M6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "M8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "N12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "N17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "N7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "N9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "P4")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "P7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "P9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "R12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "R16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "T11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "T17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "T4")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "U14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "U15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "U16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "V1")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "V14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "V16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "V18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "V6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "V9")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 3.81)
				(name "VDD_PLL")
				(number "P16")
			)
			(pin power_in line
				(at 7.62 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "F9")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "G10")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "G12")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "G6")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "G8")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "H11")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "H13")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "H7")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "H9")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "J10")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "J12")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "J6")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "J8")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "K11")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "K13")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "K7")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "K9")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "L10")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "L12")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "L6")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "L8")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "M11")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "M13")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "M7")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "M9")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "N10")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "N6")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "N8")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "N16")
			)
		)
		(symbol "CCGM1A1_8_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "SER_CLK")
				(number "T12")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "SER_CLK_N")
				(number "T13")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 3.81)
				(name "VDD_CLK")
				(number "T14")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "~{RESET}")
				(number "T15")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "POR_ADJ")
				(number "V15")
			)
		)
		(embedded_fonts no)
	)
)
