(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "T8Q144xx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 16.51 0)
		)
		(property "Value" "T8Q144xx"
			(at 19.05 -16.51 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "https://www.efinixinc.com/docs/trion8-ds-v4.4.pdf"
			(at 0 -26.67 0)
		)
		(property "Description" "Efinix Trion FPGA, 7384 LEs, LQFP-144"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "T8Q144xx_1_1"
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "CDONE")
				(number "34")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "CRESET_N")
				(number "35")
			)
			(pin input line
				(at -22.86 0 0)
				(length 5.08)
				(name "TCK")
				(number "26")
			)
			(pin input line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "TDI")
				(number "27")
			)
			(pin output line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "TDO")
				(number "24")
			)
			(pin input line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "TMS")
				(number "25")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VCCIO1A")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "GPIOL_00_SS_N")
				(number "31")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "GPIOL_01_CCK")
				(number "30")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "GPIOL_04_CSI")
				(number "32")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "GPIOL_05_CSO")
				(number "33")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "GPIOL_08_CDI0")
				(number "29")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "GPIOL_09_CDI1")
				(number "28")
			)
		)
		(symbol "T8Q144xx_2_1"
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "GPIOL_12_CDI2")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "GPIOL_13_CDI3")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "GPIOL_20_CTRL0_CDI4")
				(number "18")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "GPIOL_21_CTRL1_CDI5")
				(number "17")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCCIO1B")
				(number "21")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "GPIOL_22_CTRL2")
				(number "16")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "GPIOL_24_CLK0")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "GPIOL_25_CLK1")
				(number "14")
			)
		)
		(symbol "T8Q144xx_3_1"
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "GPIOL_31_CLK7_CDI6")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "GPIOL_32_CTRL4_CDI7")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "GPIOL_40_CDI8")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "GPIOL_41_CDI9")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCCIO1C_1D")
				(number "12")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "GPIOL_46")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "GPIOL_53_CDI10")
				(number "3")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "GPIOL_54_CDI11")
				(number "4")
			)
		)
		(symbol "T8Q144xx_4_1"
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "GPIOL_64")
				(number "144")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "GPIOL_65")
				(number "141")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "GPIOL_66_CDI12")
				(number "142")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "GPIOL_67_CDI13")
				(number "140")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "GPIOL_68")
				(number "139")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "GPIOL_69_CBSEL1")
				(number "138")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VCCIO1E")
				(number "143")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "GPIOL_70_CBSEL0")
				(number "137")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "GPIOL_71_NSTATUS")
				(number "136")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "GPIOL_72_EXTFB0_CDI14")
				(number "135")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "GPIOL_73_EXTFB1_CDI15")
				(number "134")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "GPIOL_74_PLLIN0")
				(number "132")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "GPIOL_75_PLLIN1")
				(number "131")
			)
		)
		(symbol "T8Q144xx_5_1"
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "GPIOR_76_PLLIN0")
				(number "124")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "GPIOR_77_PLLIN1")
				(number "123")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "GPIOR_78_EXTFB0_CDI31")
				(number "119")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "GPIOR_79_EXTFB1_CDI30")
				(number "118")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "GPIOR_80")
				(number "117")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "GPIOR_81_MREFCLK")
				(number "116")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "GPIOR_82")
				(number "115")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VCCIO3A")
				(number "122")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "GPIOR_83")
				(number "114")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "GPIOR_84")
				(number "113")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "GPIOR_85")
				(number "111")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "GPIOR_86")
				(number "112")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "GPIOR_87_CDI29")
				(number "110")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "GPIOR_88_CDI28")
				(number "109")
			)
		)
		(symbol "T8Q144xx_6_1"
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "GPIOR_104_CDI25")
				(number "103")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "GPIOR_105_CDI24")
				(number "102")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "GPIOR_94_CDI27")
				(number "106")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "GPIOR_95_CDI26")
				(number "105")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "GPIOR_112_CDI23")
				(number "101")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCCIO3B_3C")
				(number "95")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "GPIOR_113_CDI22")
				(number "100")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "GPIOR_116_CTRL15")
				(number "99")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "GPIOR_117_CTRL14")
				(number "98")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "GPIOR_122_CLK13_CDI21")
				(number "97")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "GPIOR_123_CLK12_CDI20")
				(number "93")
			)
		)
		(symbol "T8Q144xx_7_1"
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "GPIOR_125_CLK10")
				(number "92")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "GPIOR_128_CTRL11")
				(number "90")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "GPIOR_129_CTRL10")
				(number "89")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "GPIOR_132_CDI19")
				(number "87")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "GPIOR_133_CDI18")
				(number "86")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCCIO3D")
				(number "91")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "GPIOR_135_CDI17")
				(number "84")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "GPIOR_136_CDI16")
				(number "83")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "GPIOR_138")
				(number "82")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "GPIOR_139")
				(number "81")
			)
		)
		(symbol "T8Q144xx_8_1"
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "GPIOR_149_CBUS2")
				(number "80")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "GPIOR_150_CBUS1")
				(number "79")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "GPIOR_151_CBUS0")
				(number "78")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "GPIOR_154")
				(number "77")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCCIO3E")
				(number "88")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "GPIOR_155")
				(number "76")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "GPIOR_157_PLLIN")
				(number "75")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "GPIOR_158_TEST_N")
				(number "74")
			)
		)
		(symbol "T8Q144xx_9_1"
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "GPIOB_CLKP0")
				(number "71")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "GPIOB_CLKN0")
				(number "72")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "GPIOB_RXP00")
				(number "55")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "GPIOB_RXN00")
				(number "56")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "GPIOB_RXP02")
				(number "58")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "GPIOB_RXN02")
				(number "59")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "GPIOB_RXP03")
				(number "61")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "GPIOB_RXN03")
				(number "60")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCCIO4A")
				(number "62")
			)
			(pin passive line
				(at 0 20.32 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO4A")
				(number "63")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "GPIOB_RXP07")
				(number "66")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "GPIOB_RXN07")
				(number "65")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "GPIOB_RXP10")
				(number "67")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "GPIOB_RXN10")
				(number "68")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "GPIOB_RXP12_EXTFB0")
				(number "70")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "GPIOB_RXN12_EXTFB0")
				(number "69")
			)
		)
		(symbol "T8Q144xx_10_1"
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "GPIOB_TXP00")
				(number "38")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "GPIOB_TXN00")
				(number "39")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "GPIOB_TXP02")
				(number "40")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "GPIOB_TXN02")
				(number "41")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "GPIOB_TXP04")
				(number "42")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "GPIOB_TXN04")
				(number "43")
			)
			(pin passive line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "REF_RES")
				(number "36")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VCCIO4B")
				(number "51")
			)
			(pin passive line
				(at 0 20.32 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO4B")
				(number "52")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "GPIOB_TXP06")
				(number "45")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "GPIOB_TXN06")
				(number "46")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "GPIOB_TXP09")
				(number "47")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "GPIOB_TXN09")
				(number "48")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "GPIOB_TXP11")
				(number "53")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "GPIOB_TXN11")
				(number "54")
			)
		)
		(symbol "T8Q144xx_11_1"
			(pin power_in line
				(at -15.24 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "13")
			)
			(pin power_in line
				(at -12.7 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "22")
			)
			(pin power_in line
				(at -10.16 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "49")
			)
			(pin power_in line
				(at -7.62 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "57")
			)
			(pin power_in line
				(at -5.08 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "85")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "96")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "125")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "104")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "108")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "120")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "121")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "126")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "127")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "129")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "133")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "37")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "50")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "64")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "94")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "128")
			)
			(pin power_in line
				(at 5.08 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "130")
			)
			(pin power_in line
				(at 10.16 12.7 270)
				(length 5.08)
				(name "VCCA_BR")
				(number "73")
			)
			(pin power_in line
				(at 12.7 12.7 270)
				(length 5.08)
				(name "VCCA_TL")
				(number "2")
			)
			(pin power_in line
				(at 15.24 12.7 270)
				(length 5.08)
				(name "VCCA_TR")
				(number "107")
			)
		)
		(embedded_fonts no)
	)
)
