(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ICE40HX1K-TQ144"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 36.83 0)
		)
		(property "Value" "ICE40HX1K-TQ144"
			(at 10.16 36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-144_20x20mm_P0.5mm"
			(at 0 -36.83 0)
		)
		(property "Datasheet" "http://www.latticesemi.com/Products/FPGAandCPLD/iCE40"
			(at -21.59 35.56 0)
		)
		(property "Description" "iCE40 HX FPGA, 1280 LUTs, 1.2V, TQFP-144"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ICE40HX1K-TQ144_1_1"
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 3.81)
				(name "IOT_73")
				(number "112")
			)
			(pin bidirectional line
				(at -12.7 25.4 0)
				(length 3.81)
				(name "IOT_74")
				(number "113")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 3.81)
				(name "IOT_75")
				(number "114")
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 3.81)
				(name "IOT_76")
				(number "115")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 3.81)
				(name "IOT_77")
				(number "116")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 3.81)
				(name "IOT_78")
				(number "117")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "IOT_79")
				(number "118")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "IOT_80")
				(number "119")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "IOT_81")
				(number "120")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "IOT_82")
				(number "121")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "IOT_83")
				(number "122")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 3.81)
				(name "IOT_84_GBIN1")
				(number "128")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "IOT_85_GBIN0")
				(number "129")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "IOT_87")
				(number "134")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "IOT_88")
				(number "135")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "IOT_89")
				(number "136")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "IOT_90")
				(number "137")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 3.81)
				(name "IOT_91")
				(number "138")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 3.81)
				(name "IOT_92")
				(number "139")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 3.81)
				(name "IOT_93")
				(number "141")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 3.81)
				(name "IOT_94")
				(number "142")
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 3.81)
				(name "IOT_95")
				(number "143")
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 3.81)
				(name "IOT_96")
				(number "144")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VCCIO_0")
				(number "123")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 3.81)
				(hide yes)
				(name "VCCIO_0")
				(number "133")
			)
			(pin no_connect line
				(at 7.62 10.16 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at 7.62 7.62 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at 7.62 5.08 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at 7.62 -10.16 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "77")
			)
		)
		(symbol "ICE40HX1K-TQ144_2_1"
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 3.81)
				(name "IOR_48")
				(number "73")
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 3.81)
				(name "IOR_49")
				(number "74")
			)
			(pin bidirectional line
				(at -12.7 25.4 0)
				(length 3.81)
				(name "IOR_50")
				(number "75")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 3.81)
				(name "IOR_51")
				(number "76")
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 3.81)
				(name "IOR_52")
				(number "78")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 3.81)
				(name "IOR_53")
				(number "79")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 3.81)
				(name "IOR_54")
				(number "80")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "IOR_55")
				(number "81")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "IOR_56")
				(number "87")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "IOR_57")
				(number "88")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "IOR_58")
				(number "90")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "IOR_59")
				(number "91")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 3.81)
				(name "IOR_60_GBIN3")
				(number "93")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "IOR_61_GBIN2")
				(number "94")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "IOR_62")
				(number "95")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "IOR_63")
				(number "96")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "IOR_64")
				(number "97")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "IOR_65")
				(number "98")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 3.81)
				(name "IOR_66")
				(number "99")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 3.81)
				(name "IOR_67")
				(number "101")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 3.81)
				(name "IOR_68")
				(number "102")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 3.81)
				(name "IOR_69")
				(number "104")
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 3.81)
				(name "IOR_70")
				(number "105")
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 3.81)
				(name "IOR_71")
				(number "106")
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 3.81)
				(name "IOR_72")
				(number "107")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 3.81)
				(hide yes)
				(name "VCCIO_1")
				(number "100")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 3.81)
				(name "VCCIO_1")
				(number "89")
			)
			(pin no_connect line
				(at 7.62 10.16 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "40")
			)
			(pin no_connect line
				(at 7.62 7.62 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "53")
			)
			(pin no_connect line
				(at 7.62 5.08 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "54")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "55")
			)
			(pin no_connect line
				(at 7.62 -10.16 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "82")
			)
		)
		(symbol "ICE40HX1K-TQ144_3_1"
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 3.81)
				(name "IOB_24")
				(number "37")
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 3.81)
				(name "IOB_25")
				(number "38")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 3.81)
				(name "IOB_26")
				(number "39")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 3.81)
				(name "IOB_27")
				(number "41")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "IOB_28")
				(number "42")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "IOB_29")
				(number "43")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "IOB_30")
				(number "44")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "IOB_31")
				(number "45")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "IOB_32")
				(number "47")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 3.81)
				(name "IOB_33")
				(number "48")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "IOB_35_GBIN5")
				(number "49")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "IOB_36_GBIN4")
				(number "50")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "IOB_34")
				(number "52")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "IOB_37")
				(number "56")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "IOB_38")
				(number "58")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 3.81)
				(name "IOB_39")
				(number "60")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 3.81)
				(name "IOB_40")
				(number "61")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 3.81)
				(name "IOB_41")
				(number "62")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 3.81)
				(name "IOB_42_CBSEL0")
				(number "63")
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 3.81)
				(name "IOB_43_CBSEL1")
				(number "64")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 3.81)
				(name "VCCIO_2")
				(number "46")
			)
			(pin passive line
				(at 0 33.02 270)
				(length 3.81)
				(hide yes)
				(name "VCCIO_2")
				(number "57")
			)
			(pin no_connect line
				(at 7.62 10.16 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "83")
			)
			(pin no_connect line
				(at 7.62 7.62 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "84")
			)
			(pin no_connect line
				(at 7.62 -10.16 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "110")
			)
			(pin no_connect line
				(at 7.62 -12.7 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "85")
			)
			(pin no_connect line
				(at 7.62 -17.78 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "124")
			)
		)
		(symbol "ICE40HX1K-TQ144_4_1"
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 3.81)
				(name "IOL_1A")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 25.4 0)
				(length 3.81)
				(name "IOL_1B")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 3.81)
				(name "IOL_2A")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 3.81)
				(name "IOL_2B")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 3.81)
				(name "IOL_3A")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 3.81)
				(name "IOL_3B")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "IOL_4A")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "IOL_4B")
				(number "10")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "IOL_5A")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "IOL_5B")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "IOL_6A")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 3.81)
				(name "IOL_6B_GBIN7")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "IOL_7A_GBIN6")
				(number "21")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "IOL_7B")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "IOL_8A")
				(number "23")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "IOL_8B")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "IOL_9A")
				(number "25")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 3.81)
				(name "IOL_9B")
				(number "26")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 3.81)
				(name "IOL_10A")
				(number "28")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 3.81)
				(name "IOL_10B")
				(number "29")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 3.81)
				(name "IOL_11A")
				(number "31")
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 3.81)
				(name "IOL_11B")
				(number "32")
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 3.81)
				(name "IOL_12A")
				(number "33")
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 3.81)
				(name "IOL_12B")
				(number "34")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 3.81)
				(hide yes)
				(name "VCCIO_3")
				(number "30")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 3.81)
				(name "VCCIO_3")
				(number "6")
			)
			(pin no_connect line
				(at 7.62 10.16 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "125")
			)
			(pin no_connect line
				(at 7.62 7.62 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "126")
			)
			(pin no_connect line
				(at 7.62 5.08 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "127")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "130")
			)
			(pin no_connect line
				(at 7.62 -10.16 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "131")
			)
		)
		(symbol "ICE40HX1K-TQ144_5_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "IOB_44_SDO")
				(number "67")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 3.81)
				(name "IOB_45_SDI")
				(number "68")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "IOB_46_SCK")
				(number "70")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "IOB_47_SS")
				(number "71")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "~{CRESET_B}")
				(number "66")
			)
			(pin power_in line
				(at -7.62 17.78 270)
				(length 3.81)
				(name "VCC_SPI")
				(number "72")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 3.81)
				(name "VPP_FAST")
				(number "109")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "111")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "27")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "51")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "92")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "103")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "132")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "140")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "59")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "69")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "86")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "VPP_2V5")
				(number "108")
			)
			(pin power_in line
				(at 7.62 17.78 270)
				(length 3.81)
				(name "VCCPLL")
				(number "36")
			)
			(pin power_in line
				(at 7.62 -17.78 90)
				(length 3.81)
				(name "GNDPLL")
				(number "35")
			)
			(pin open_collector line
				(at 15.24 0 180)
				(length 3.81)
				(name "CDONE")
				(number "65")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ICE40HX4K-TQ144"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 53.34 0)
		)
		(property "Value" "ICE40HX4K-TQ144"
			(at 30.48 48.26 0)
		)
		(property "Footprint" "Package_QFP:TQFP-144_20x20mm_P0.5mm"
			(at 25.4 -48.26 0)
		)
		(property "Datasheet" "http://www.latticesemi.com/Products/FPGAandCPLD/iCE40"
			(at -25.4 63.5 0)
		)
		(property "Description" "iCE40 HX FPGA, 3520 LUTs, 1.2V, TQFP-144"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ICE40HX4K-TQ144_1_1"
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 3.81)
				(name "IOT_168")
				(number "110")
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 3.81)
				(name "IOT_169")
				(number "112")
			)
			(pin bidirectional line
				(at -12.7 25.4 0)
				(length 3.81)
				(name "IOT_170")
				(number "113")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 3.81)
				(name "IOT_171")
				(number "114")
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 3.81)
				(name "IOT_172")
				(number "115")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 3.81)
				(name "IOT_173")
				(number "116")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 3.81)
				(name "IOT_174")
				(number "117")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "IOT_177")
				(number "118")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "IOT_178")
				(number "119")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "IOT_179")
				(number "120")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "IOT_181")
				(number "121")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "IOT_190")
				(number "122")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 3.81)
				(name "IOT_191")
				(number "124")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "IOT_192")
				(number "125")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "IOT_197_GBIN1")
				(number "128")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "IOT_198_GBIN0")
				(number "129")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "IOT_206")
				(number "130")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "IOT_212")
				(number "134")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 3.81)
				(name "IOT_213")
				(number "135")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 3.81)
				(name "IOT_214")
				(number "136")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 3.81)
				(name "IOT_215")
				(number "137")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 3.81)
				(name "IOT_216")
				(number "138")
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 3.81)
				(name "IOT_217")
				(number "139")
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 3.81)
				(name "IOT_219")
				(number "141")
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 3.81)
				(name "IOT_220")
				(number "142")
			)
			(pin bidirectional line
				(at -12.7 -33.02 0)
				(length 3.81)
				(name "IOT_221")
				(number "143")
			)
			(pin bidirectional line
				(at -12.7 -35.56 0)
				(length 3.81)
				(name "IOT_222")
				(number "144")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 3.81)
				(name "VCCIO_0")
				(number "123")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 3.81)
				(hide yes)
				(name "VCCIO_0")
				(number "131")
			)
		)
		(symbol "ICE40HX4K-TQ144_2_1"
			(pin bidirectional line
				(at -12.7 33.02 0)
				(length 3.81)
				(name "IOR_109")
				(number "73")
			)
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 3.81)
				(name "IOR_110")
				(number "74")
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 3.81)
				(name "IOR_111")
				(number "75")
			)
			(pin bidirectional line
				(at -12.7 25.4 0)
				(length 3.81)
				(name "IOR_112")
				(number "76")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 3.81)
				(name "IOR_114")
				(number "78")
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 3.81)
				(name "IOR_115")
				(number "79")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 3.81)
				(name "IOR_116")
				(number "80")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 3.81)
				(name "IOR_117")
				(number "81")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "IOR_118")
				(number "82")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "IOR_119")
				(number "83")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "IOR_120")
				(number "84")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "IOR_128")
				(number "85")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "IOR_136")
				(number "87")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 3.81)
				(name "IOR_137")
				(number "88")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "IOR_138")
				(number "90")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "IOR_139")
				(number "91")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "IOR_140_GBIN3")
				(number "93")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "IOR_141_GBIN2")
				(number "94")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "IOR_144")
				(number "95")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 3.81)
				(name "IOR_146")
				(number "96")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 3.81)
				(name "IOR_147")
				(number "97")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 3.81)
				(name "IOR_148")
				(number "98")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 3.81)
				(name "IOR_152")
				(number "99")
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 3.81)
				(name "IOR_160")
				(number "101")
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 3.81)
				(name "IOR_161")
				(number "102")
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 3.81)
				(name "IOR_164")
				(number "104")
			)
			(pin bidirectional line
				(at -12.7 -33.02 0)
				(length 3.81)
				(name "IOR_165")
				(number "105")
			)
			(pin bidirectional line
				(at -12.7 -35.56 0)
				(length 3.81)
				(name "IOR_166")
				(number "106")
			)
			(pin bidirectional line
				(at -12.7 -38.1 0)
				(length 3.81)
				(name "IOR_167")
				(number "107")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 3.81)
				(hide yes)
				(name "VCCIO_1")
				(number "100")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 3.81)
				(name "VCCIO_1")
				(number "89")
			)
		)
		(symbol "ICE40HX4K-TQ144_3_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 3.81)
				(name "IOB_56")
				(number "37")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 3.81)
				(name "IOB_57")
				(number "38")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 3.81)
				(name "IOB_61")
				(number "39")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "IOB_63")
				(number "41")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "IOB_64")
				(number "42")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "IOB_71")
				(number "43")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "IOB_72")
				(number "44")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "IOB_73")
				(number "45")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 3.81)
				(name "IOB_79")
				(number "47")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "IOB_80")
				(number "48")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "IOB_81_GBIN5")
				(number "49")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "IOB_82_GBIN4")
				(number "52")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "IOB_91")
				(number "55")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "IOB_94")
				(number "56")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 3.81)
				(name "IOB_95")
				(number "60")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 3.81)
				(name "IOB_96")
				(number "61")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 3.81)
				(name "IOB_102")
				(number "62")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 3.81)
				(name "IOB_103_CBSEL0")
				(number "63")
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 3.81)
				(name "IOB_104_CBSEL1")
				(number "64")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VCCIO_2")
				(number "46")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 3.81)
				(hide yes)
				(name "VCCIO_2")
				(number "57")
			)
		)
		(symbol "ICE40HX4K-TQ144_4_1"
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 3.81)
				(name "IOL_2A")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 3.81)
				(name "IOL_2B")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 25.4 0)
				(length 3.81)
				(name "IOL_3A")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 3.81)
				(name "IOL_3B")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 3.81)
				(name "IOL_4A")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 3.81)
				(name "IOL_4B")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 3.81)
				(name "IOL_5A")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "IOL_5B")
				(number "10")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "IOL_8A")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "IOL_8B")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "IOL_10A")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "IOL_10B")
				(number "16")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 3.81)
				(name "IOL_12A")
				(number "17")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "IOL_12B")
				(number "18")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "IOL_13A")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "IOL_13B_GBIN7")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "IOL_14A_GBIN6")
				(number "21")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "IOL_14B")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 3.81)
				(name "IOL_17A")
				(number "23")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 3.81)
				(name "IOL_17B")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 3.81)
				(name "IOL_18A")
				(number "25")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 3.81)
				(name "IOL_18B")
				(number "26")
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 3.81)
				(name "IOL_23A")
				(number "28")
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 3.81)
				(name "IOL_23B")
				(number "29")
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 3.81)
				(name "IOL_24A")
				(number "31")
			)
			(pin bidirectional line
				(at -12.7 -33.02 0)
				(length 3.81)
				(name "IOL_24B")
				(number "32")
			)
			(pin bidirectional line
				(at -12.7 -35.56 0)
				(length 3.81)
				(name "IOL_25A")
				(number "33")
			)
			(pin bidirectional line
				(at -12.7 -38.1 0)
				(length 3.81)
				(name "IOL_25B")
				(number "34")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 3.81)
				(hide yes)
				(name "VCCIO_3")
				(number "30")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 3.81)
				(name "VCCIO_3")
				(number "6")
			)
		)
		(symbol "ICE40HX4K-TQ144_5_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "IOB_105_SDO")
				(number "67")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 3.81)
				(name "IOB_106_SDI")
				(number "68")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "IOB_107_SCK")
				(number "70")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "IOB_108_SS")
				(number "71")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "~{CRESET}")
				(number "66")
			)
			(pin power_in line
				(at -7.62 17.78 270)
				(length 3.81)
				(name "VCC_SPI")
				(number "72")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 3.81)
				(name "VPP_FAST")
				(number "109")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "111")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "27")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "40")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "92")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "103")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "132")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "140")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "59")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "69")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "86")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "VPP_2V5")
				(number "108")
			)
			(pin power_in line
				(at 7.62 17.78 270)
				(length 3.81)
				(name "VCCPLL0")
				(number "54")
			)
			(pin power_in line
				(at 7.62 -17.78 90)
				(length 3.81)
				(name "GNDPLL0")
				(number "53")
			)
			(pin power_in line
				(at 10.16 17.78 270)
				(length 3.81)
				(name "VCCPLL1")
				(number "126")
			)
			(pin power_in line
				(at 10.16 -17.78 90)
				(length 3.81)
				(name "GNDPLL1")
				(number "127")
			)
			(pin no_connect line
				(at 12.7 7.62 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "77")
			)
			(pin no_connect line
				(at 12.7 5.08 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "35")
			)
			(pin no_connect line
				(at 12.7 2.54 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "36")
			)
			(pin no_connect line
				(at 12.7 -2.54 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "50")
			)
			(pin no_connect line
				(at 12.7 -5.08 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "51")
			)
			(pin no_connect line
				(at 12.7 -7.62 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "58")
			)
			(pin no_connect line
				(at 12.7 -10.16 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "133")
			)
			(pin open_collector line
				(at 17.78 0 180)
				(length 3.81)
				(name "CDONE")
				(number "65")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ICE40HX8K-BG121"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 44.45 0)
		)
		(property "Value" "ICE40HX8K-BG121"
			(at 10.16 41.91 0)
		)
		(property "Footprint" "Package_BGA:BGA-121_9.0x9.0mm_Layout11x11_P0.8mm_Ball0.4mm_Pad0.35mm_NSMD"
			(at 0 -36.83 0)
		)
		(property "Datasheet" "http://www.latticesemi.com/Products/FPGAandCPLD/iCE40"
			(at -21.59 25.4 0)
		)
		(property "Description" "iCE40 HX FPGA, 7680 LUTs, 1.2V, BGA-121"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*9.0x9.0mm*Layout11x11*P0.8mm*Ball0.4mm*"
			(at 0 0 0)
		)
		(symbol "ICE40HX8K-BG121_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 3.81)
				(name "IOT_168")
				(number "A11")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 3.81)
				(name "IOT_170")
				(number "A10")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 3.81)
				(name "IOT_172")
				(number "C9")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "IOT_174")
				(number "B9")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "IOT_177")
				(number "B8")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "IOT_178")
				(number "A9")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "IOT_179")
				(number "C8")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "IOT_181")
				(number "D7")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 3.81)
				(name "IOT_190")
				(number "A8")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "IOT_191")
				(number "C7")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "IOT_192")
				(number "A7")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "IOT_197_GBIN1")
				(number "B7")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "IOT_198_GBIN0")
				(number "B6")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "IOT_206")
				(number "A6")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 3.81)
				(name "IOT_207")
				(number "A5")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 3.81)
				(name "IOT_208")
				(number "B5")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 3.81)
				(name "IOT_211")
				(number "A4")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 3.81)
				(name "IOT_212")
				(number "D5")
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 3.81)
				(name "IOT_219")
				(number "B4")
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 3.81)
				(name "IOT_221")
				(number "B3")
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 3.81)
				(name "IOT_222")
				(number "A2")
			)
			(pin bidirectional line
				(at -12.7 -33.02 0)
				(length 3.81)
				(name "IOT_223")
				(number "A3")
			)
			(pin bidirectional line
				(at -12.7 -35.56 0)
				(length 3.81)
				(name "IOT_225")
				(number "A1")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VCCIO_0")
				(number "D6")
			)
		)
		(symbol "ICE40HX8K-BG121_2_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 3.81)
				(name "IOR_114")
				(number "J11")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 3.81)
				(name "IOR_115")
				(number "K11")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 3.81)
				(name "IOR_116")
				(number "H10")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "IOR_117")
				(number "J10")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "IOR_118")
				(number "G8")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "IOR_119")
				(number "H11")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "IOR_120")
				(number "G10")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "IOR_128")
				(number "G9")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 3.81)
				(name "IOR_129")
				(number "G11")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "IOR_136")
				(number "F10")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "IOR_137")
				(number "F9")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "IOR_140_GBIN3")
				(number "F11")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "IOR_141_GBIN2")
				(number "E10")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "IOR_144")
				(number "E9")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 3.81)
				(name "IOR_146")
				(number "E8")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 3.81)
				(name "IOR_147")
				(number "D9")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 3.81)
				(name "IOR_148")
				(number "E11")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 3.81)
				(name "IOR_152")
				(number "D11")
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 3.81)
				(name "IOR_154")
				(number "D10")
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 3.81)
				(name "IOR_160")
				(number "C11")
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 3.81)
				(name "IOR_161")
				(number "B11")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VCCIO_1")
				(number "F8")
			)
		)
		(symbol "ICE40HX8K-BG121_3_1"
			(pin input line
				(at -15.24 25.4 0)
				(length 3.81)
				(name "~{CRESET}")
				(number "L9")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 3.81)
				(name "IOB_56")
				(number "L1")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 3.81)
				(name "IOB_57")
				(number "J3")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "IOB_61")
				(number "L2")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "IOB_63")
				(number "K3")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "IOB_64")
				(number "J4")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "IOB_71")
				(number "L3")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "IOB_72")
				(number "L4")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 3.81)
				(name "IOB_73")
				(number "K4")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "IOB_78")
				(number "J5")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "IOB_79")
				(number "K5")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "IOB_81_GBIN5")
				(number "L5")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "IOB_82_GBIN4")
				(number "K6")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "IOB_86")
				(number "J7")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 3.81)
				(name "IOB_87")
				(number "H7")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 3.81)
				(name "IOB_89")
				(number "K7")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 3.81)
				(name "IOB_91")
				(number "J8")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 3.81)
				(name "IOB_94")
				(number "L7")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 3.81)
				(name "IOB_103_CBSEL0")
				(number "L8")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 3.81)
				(name "IOB_104_CBSEL1")
				(number "H9")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 3.81)
				(name "VCCIO_2")
				(number "H6")
			)
			(pin open_collector line
				(at 15.24 25.4 180)
				(length 3.81)
				(name "CDONE")
				(number "K8")
			)
		)
		(symbol "ICE40HX8K-BG121_4_1"
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 3.81)
				(name "IOL_2A")
				(number "B1")
			)
			(pin bidirectional line
				(at -12.7 25.4 0)
				(length 3.81)
				(name "IOL_2B")
				(number "B2")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 3.81)
				(name "IOL_4A")
				(number "C4")
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 3.81)
				(name "IOL_4B")
				(number "C3")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 3.81)
				(name "IOL_5A")
				(number "C2")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 3.81)
				(name "IOL_5B")
				(number "C1")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "IOL_8A")
				(number "E1")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "IOL_8B")
				(number "D1")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "IOL_9A")
				(number "D2")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "IOL_9B")
				(number "D3")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "IOL_10A")
				(number "E2")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 3.81)
				(name "IOL_10B")
				(number "E3")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "IOL_12A")
				(number "F1")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "IOL_12B")
				(number "F2")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "IOL_13A")
				(number "F4")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "IOL_13B_GBIN7")
				(number "F3")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "IOL_14A_GBIN6")
				(number "G1")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 3.81)
				(name "IOL_14B")
				(number "G2")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 3.81)
				(name "IOL_17A")
				(number "G3")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 3.81)
				(name "IOL_17B")
				(number "H3")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 3.81)
				(name "IOL_18A")
				(number "H1")
			)
			(pin bidirectional line
				(at -12.7 -25.4 0)
				(length 3.81)
				(name "IOL_18B")
				(number "H2")
			)
			(pin bidirectional line
				(at -12.7 -27.94 0)
				(length 3.81)
				(name "IOL_23A")
				(number "J1")
			)
			(pin bidirectional line
				(at -12.7 -30.48 0)
				(length 3.81)
				(name "IOL_23B")
				(number "K1")
			)
			(pin bidirectional line
				(at -12.7 -33.02 0)
				(length 3.81)
				(name "IOL_25A")
				(number "K2")
			)
			(pin bidirectional line
				(at -12.7 -35.56 0)
				(length 3.81)
				(name "IOL_25B")
				(number "J2")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 3.81)
				(name "VCCIO_3")
				(number "E4")
			)
			(pin passive line
				(at 0 43.18 270)
				(length 3.81)
				(hide yes)
				(name "VCCIO_3")
				(number "G4")
			)
		)
		(symbol "ICE40HX8K-BG121_5_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "IOB_105_SDO")
				(number "K9")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 3.81)
				(name "IOB_106_SDI")
				(number "J9")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "IOB_107_SCK")
				(number "L10")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "IOB_108_SS")
				(number "K10")
			)
			(pin power_in line
				(at -7.62 17.78 270)
				(length 3.81)
				(name "VCC_SPI")
				(number "L11")
			)
			(pin power_in line
				(at -7.62 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "E5")
			)
			(pin passive line
				(at -7.62 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E6")
			)
			(pin passive line
				(at -7.62 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "E7")
			)
			(pin passive line
				(at -7.62 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F5")
			)
			(pin passive line
				(at -7.62 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F6")
			)
			(pin passive line
				(at -7.62 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F7")
			)
			(pin passive line
				(at -7.62 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G5")
			)
			(pin passive line
				(at -7.62 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G6")
			)
			(pin passive line
				(at -7.62 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G7")
			)
			(pin passive line
				(at -7.62 -17.78 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "H5")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 3.81)
				(name "VPP_FAST")
				(number "B10")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VPP_2V5")
				(number "C10")
			)
			(pin passive line
				(at 2.54 17.78 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "D4")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "D8")
			)
			(pin passive line
				(at 2.54 17.78 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "H4")
			)
			(pin passive line
				(at 2.54 17.78 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "H8")
			)
			(pin power_in line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "VCCPLL0")
				(number "J6")
			)
			(pin power_in line
				(at 15.24 0 180)
				(length 3.81)
				(name "GNDPLL0")
				(number "L6")
			)
			(pin power_in line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "VCCPLL1")
				(number "C6")
			)
			(pin power_in line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "GNDPLL1")
				(number "C5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ICE40UL1K-SWG16"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 27.94 0)
		)
		(property "Value" "ICE40UL1K-SWG16"
			(at 17.78 25.4 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-16_1.409x1.409mm_Layout4x4_P0.35mm"
			(at -6.35 -1.27 0)
		)
		(property "Datasheet" "https://www.latticesemi.com/view_document?document_id=50945"
			(at -6.35 3.81 0)
		)
		(property "Description" "iCE40 UltraPlus FPGA, 1.2V, WLCSP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*1.409x1.409mm*Layout4x4*P0.35mm*"
			(at 0 0 0)
		)
		(symbol "ICE40UL1K-SWG16_0_1")
		(symbol "ICE40UL1K-SWG16_1_1"
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "IOB_15B_SI")
				(number "D2")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "IOB_14A_SO")
				(number "C2")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "IOB_17B_SS")
				(number "D1")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "IOB_16A_SCK")
				(number "C1")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "CRESET_B")
				(number "B2")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "IOB_8A_G4_CDONE")
				(number "C3")
			)
			(pin power_in line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "VCCIO")
				(number "D3")
			)
			(pin power_in line
				(at -5.08 -22.86 90)
				(length 2.54)
				(name "GND_LED")
				(number "B1")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VPP_2V5_VCCIO0")
				(number "B3")
			)
			(pin power_in line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "D4")
			)
			(pin power_in line
				(at 5.08 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "A3")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "IRLED")
				(number "A1")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "BARCODE")
				(number "A2")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "RGB2")
				(number "C4")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RGB1")
				(number "A4")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RGB0")
				(number "B4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ICE40UP5K-SG48ITR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 -29.21 0)
		)
		(property "Value" "ICE40UP5K-SG48ITR"
			(at 0 -31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "http://www.latticesemi.com/Products/FPGAandCPLD/iCE40Ultra"
			(at -10.16 25.4 0)
		)
		(property "Description" "iCE40 UltraPlus FPGA, 5280 LUTs, 1.2V, 48-pin QFN"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ICE40UP5K-SG48ITR_1_1"
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "IOT_36b")
				(number "25")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "IOT_37a")
				(number "23")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "IOT_38b")
				(number "27")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IOT_39a")
				(number "26")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IOT_41a")
				(number "28")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IOT_42b")
				(number "31")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "IOT_43a")
				(number "32")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IOT_44b")
				(number "34")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IOT_45a_G1")
				(number "37")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "IOT_46b_G0")
				(number "35")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "IOT_48b")
				(number "36")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "IOT_49a")
				(number "43")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "IOT_50b")
				(number "38")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "IOT_51a")
				(number "42")
			)
			(pin open_collector line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "RGB0")
				(number "39")
			)
			(pin open_collector line
				(at -10.16 -22.86 0)
				(length 2.54)
				(name "RGB1")
				(number "40")
			)
			(pin open_collector line
				(at -10.16 -25.4 0)
				(length 2.54)
				(name "RGB2")
				(number "41")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCCIO_0")
				(number "33")
			)
		)
		(symbol "ICE40UP5K-SG48ITR_2_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "~{CRESET}")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "IOB_13b")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IOB_16a")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "IOB_18a")
				(number "10")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "IOB_20a")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "IOB_22a")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "IOB_23b")
				(number "21")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "IOB_24a")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "IOB_25b_G3")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "IOB_29b")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "IOB_31b")
				(number "18")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "IOB_32a_SPI_SO")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "IOB_33b_SPI_SI")
				(number "17")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "IOB_34a_SPI_SCK")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "IOB_35b_SPI_SS")
				(number "16")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "SPI_VCCIO1")
				(number "22")
			)
			(pin open_collector line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "CDONE")
				(number "7")
			)
		)
		(symbol "ICE40UP5K-SG48ITR_3_1"
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IOB_0a")
				(number "46")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IOB_2a")
				(number "47")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "IOB_3b_G6")
				(number "44")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IOB_4a")
				(number "48")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IOB_5b")
				(number "45")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "IOB_6a")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "IOB_8a")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "IOB_9b")
				(number "3")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCCIO_2")
				(number "1")
			)
		)
		(symbol "ICE40UP5K-SG48ITR_4_1"
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VPP_2V5")
				(number "24")
			)
			(pin passive line
				(at 0 10.16 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "30")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "49")
			)
			(pin power_out line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VCCPLL")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LFE5U-85F-8BG381x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 24.13 16.51 0)
		)
		(property "Value" "LFE5U-85F-8BG381x"
			(at 24.13 13.97 0)
		)
		(property "Footprint" "Package_BGA:Lattice_caBGA-381_17x17mm_Layout20x20_P0.8mm"
			(at 11.43 72.39 0)
		)
		(property "Datasheet" "https://www.latticesemi.com/view_document?document_id=50461"
			(at 11.43 72.39 0)
		)
		(property "Description" "ECP5 FPGA, 84K LUTs, 1.2V, BGA-381"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Lattice?caBGA*17x17mm*Layout20x20*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "LFE5U-85F-8BG381x_1_1"
			(pin no_connect line
				(at -25.4 2.54 0)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "W4")
			)
			(pin no_connect line
				(at -25.4 0 0)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "W5")
			)
			(pin no_connect line
				(at -25.4 -2.54 0)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "W8")
			)
			(pin no_connect line
				(at -25.4 -5.08 0)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "W9")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "H10")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "H11")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "H12")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VCC")
				(number "H13")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "H8")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "H9")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "J13")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "J8")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "K13")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "K8")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "L13")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "L8")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M13")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M8")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "N10")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "N11")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "N12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "N13")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "N8")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "N9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "C19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "D4")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "F13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "F14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "F7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "F8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G4")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "H19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y8")
			)
			(pin passive line
				(at 12.7 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUX")
				(number "F15")
			)
			(pin passive line
				(at 12.7 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUX")
				(number "F6")
			)
			(pin power_in line
				(at 12.7 15.24 270)
				(length 5.08)
				(name "VCCAUX")
				(number "P15")
			)
			(pin passive line
				(at 12.7 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUX")
				(number "P6")
			)
			(pin no_connect line
				(at 25.4 2.54 180)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "W18")
			)
			(pin no_connect line
				(at 25.4 0 180)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "W17")
			)
			(pin no_connect line
				(at 25.4 -2.54 180)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "W14")
			)
			(pin no_connect line
				(at 25.4 -5.08 180)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "W13")
			)
		)
		(symbol "LFE5U-85F-8BG381x_2_1"
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PT4A")
				(number "A6")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PT4B")
				(number "B6")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PT6A")
				(number "E6")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PT6B")
				(number "D6")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PT9A")
				(number "E7")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PT9B")
				(number "D7")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PT11A")
				(number "C6")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PT11B")
				(number "C7")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PT13A")
				(number "E8")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PT13B")
				(number "D8")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PT15A")
				(number "C8")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PT15B")
				(number "B8")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PT18A")
				(number "A7")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PT18B")
				(number "A8")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PT20A")
				(number "D9")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PT20B")
				(number "E9")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PT54A")
				(number "C9")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PT56A")
				(number "D10")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PT56B")
				(number "E10")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PT58A")
				(number "B9")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PT58B")
				(number "C10")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PT60A")
				(number "A9")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PT60B")
				(number "B10")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PT63A")
				(number "A10")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PT63B")
				(number "A11")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PT65A")
				(number "B11")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PT65B")
				(number "C11")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 5.08)
				(name "VCCIO0")
				(number "F10")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO0")
				(number "F9")
			)
		)
		(symbol "LFE5U-85F-8BG381x_3_1"
			(pin bidirectional line
				(at -10.16 38.1 0)
				(length 5.08)
				(name "PT69A")
				(number "D11")
			)
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PT69B")
				(number "E11")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PT71A")
				(number "B12")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PT71B")
				(number "C12")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PT74A")
				(number "D12")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PT74B")
				(number "E12")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PT76A")
				(number "A12")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PT76B")
				(number "A13")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PT78A")
				(number "B13")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PT78B")
				(number "C13")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PT80A")
				(number "D13")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PT80B")
				(number "E13")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PT83A")
				(number "A14")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PT83B")
				(number "C14")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PT85A")
				(number "D14")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PT85B")
				(number "E14")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PT103A")
				(number "A15")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PT105A")
				(number "B15")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PT105B")
				(number "C15")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PT107A")
				(number "D15")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PT107B")
				(number "E15")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PT110A")
				(number "A16")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PT110B")
				(number "B16")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PT112A")
				(number "C16")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PT112B")
				(number "D16")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PT114A")
				(number "B17")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PT114B")
				(number "C17")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PT116A")
				(number "A17")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PT116B")
				(number "B18")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PT119A")
				(number "A18")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PT119B")
				(number "B19")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PT121A")
				(number "A19")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PT121B")
				(number "B20")
			)
			(pin passive line
				(at 0 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO1")
				(number "F11")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 5.08)
				(name "VCCIO1")
				(number "F12")
			)
		)
		(symbol "LFE5U-85F-8BG381x_4_1"
			(pin bidirectional line
				(at -10.16 38.1 0)
				(length 5.08)
				(name "PR11A")
				(number "C18")
			)
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PR11B")
				(number "D17")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PR11C")
				(number "E16")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PR11D")
				(number "F16")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PR14A")
				(number "D18")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PR14B")
				(number "E17")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PR14C")
				(number "E18")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PR14D")
				(number "F18")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PR17A")
				(number "F17")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PR17B")
				(number "G18")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PR17C")
				(number "G16")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PR17D")
				(number "H16")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PR20A")
				(number "H18")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PR20B")
				(number "H17")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PR20C")
				(number "J17")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PR20D")
				(number "J16")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PR29A")
				(number "K16")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PR29B")
				(number "K17")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PR35A")
				(number "C20")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PR35B")
				(number "D19")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PR35C")
				(number "D20")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PR35D")
				(number "E19")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PR38A")
				(number "E20")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PR38B")
				(number "F19")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PR38C")
				(number "F20")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PR38D")
				(number "G20")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PR41A")
				(number "G19")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PR41B")
				(number "H20")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PR41C")
				(number "J18")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PR41D")
				(number "K18")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PR44A")
				(number "J19")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PR44B")
				(number "K19")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PR44C")
				(number "J20")
			)
			(pin bidirectional line
				(at -10.16 -45.72 0)
				(length 5.08)
				(name "PR44D")
				(number "K20")
			)
			(pin passive line
				(at 0 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO2")
				(number "H14")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 5.08)
				(name "VCCIO2")
				(number "H15")
			)
			(pin passive line
				(at 0 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO2")
				(number "J15")
			)
		)
		(symbol "LFE5U-85F-8BG381x_5_1"
			(pin bidirectional line
				(at -10.16 38.1 0)
				(length 5.08)
				(name "PR47A")
				(number "L20")
			)
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PR47B")
				(number "M20")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PR47C")
				(number "L19")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PR47D")
				(number "M19")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PR50A")
				(number "L16")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PR50B")
				(number "L17")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PR50C")
				(number "L18")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PR50D")
				(number "M18")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PR53A")
				(number "N16")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PR53B")
				(number "M17")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PR53C")
				(number "N18")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PR53D")
				(number "P17")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PR56A")
				(number "N17")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PR56B")
				(number "P16")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PR56C")
				(number "R16")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PR56D")
				(number "R17")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PR77A")
				(number "T16")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PR83A")
				(number "N19")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PR83B")
				(number "N20")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PR83C")
				(number "P19")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PR83D")
				(number "P18")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PR86A")
				(number "P20")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PR86B")
				(number "R20")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PR86C")
				(number "T20")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PR86D")
				(number "U20")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PR89A")
				(number "T19")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PR89B")
				(number "R18")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PR89C")
				(number "U19")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PR89D")
				(number "T18")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PR92A")
				(number "U18")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PR92B")
				(number "U17")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PR92C")
				(number "U16")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PR92D")
				(number "T17")
			)
			(pin passive line
				(at 0 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO3")
				(number "L14")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 5.08)
				(name "VCCIO3")
				(number "L15")
			)
			(pin passive line
				(at 0 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO3")
				(number "M15")
			)
		)
		(symbol "LFE5U-85F-8BG381x_6_1"
			(pin bidirectional line
				(at -10.16 38.1 0)
				(length 5.08)
				(name "PL47A")
				(number "G2")
			)
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PL47B")
				(number "F1")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PL47C")
				(number "H2")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PL47D")
				(number "G1")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PL50A")
				(number "J4")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PL50B")
				(number "J5")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PL50C")
				(number "J3")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PL50D")
				(number "K3")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PL53A")
				(number "K2")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PL53B")
				(number "J1")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PL53C")
				(number "H1")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PL53D")
				(number "K1")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PL56A")
				(number "K4")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PL56B")
				(number "K5")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PL56C")
				(number "L4")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PL56D")
				(number "L5")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PL77A")
				(number "M5")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PL83A")
				(number "M4")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PL83B")
				(number "N5")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PL83C")
				(number "N4")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PL83D")
				(number "P5")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PL86A")
				(number "N3")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PL86B")
				(number "M3")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PL86C")
				(number "L3")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PL86D")
				(number "L2")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PL89A")
				(number "N2")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PL89B")
				(number "M1")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PL89C")
				(number "L1")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PL89D")
				(number "N1")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PL92A")
				(number "P1")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PL92B")
				(number "P2")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PL92C")
				(number "P3")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PL92D")
				(number "P4")
			)
			(pin passive line
				(at 0 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO6")
				(number "L6")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 5.08)
				(name "VCCIO6")
				(number "L7")
			)
			(pin passive line
				(at 0 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO6")
				(number "M6")
			)
		)
		(symbol "LFE5U-85F-8BG381x_7_1"
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PL11A")
				(number "A4")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PL11B")
				(number "A5")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PL11C")
				(number "B5")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PL11D")
				(number "C5")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PL14A")
				(number "C4")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PL14B")
				(number "B4")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PL14C")
				(number "A3")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PL14D")
				(number "B3")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PL17A")
				(number "E4")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PL17B")
				(number "D5")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PL17C")
				(number "C3")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PL17D")
				(number "D3")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PL20A")
				(number "F4")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PL20B")
				(number "E3")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PL20C")
				(number "E5")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PL20D")
				(number "F5")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PL35A")
				(number "A2")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PL35B")
				(number "B1")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PL35C")
				(number "B2")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PL35D")
				(number "C2")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PL38A")
				(number "C1")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PL38B")
				(number "D1")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PL38C")
				(number "D2")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PL38D")
				(number "E1")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PL41A")
				(number "H4")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PL41B")
				(number "G5")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PL41C")
				(number "H5")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PL41D")
				(number "H3")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PL44A")
				(number "G3")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PL44B")
				(number "F3")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PL44C")
				(number "F2")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PL44D")
				(number "E2")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO7")
				(number "H6")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 5.08)
				(name "VCCIO7")
				(number "H7")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO7")
				(number "J6")
			)
		)
		(symbol "LFE5U-85F-8BG381x_8_1"
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PB4A")
				(number "R1")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PB4B")
				(number "T1")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PB6A")
				(number "U1")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PB6B")
				(number "V1")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PB9A")
				(number "W1")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PB9B")
				(number "Y2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PB11A")
				(number "V2")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PB11B")
				(number "W2")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PB13A")
				(number "T2")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PB13B")
				(number "U2")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PB15A")
				(number "R2")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PB15B")
				(number "R3")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PB18A")
				(number "T3")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 5.08)
				(name "VCCIO8")
				(number "P10")
			)
			(pin passive line
				(at 0 27.94 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO8")
				(number "P9")
			)
		)
		(symbol "LFE5U-85F-8BG381x_9_1"
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "CCLK")
				(number "U3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "~{PROGRAM}")
				(number "W3")
			)
			(pin open_collector line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "~{INIT}")
				(number "V3")
			)
			(pin open_collector line
				(at -15.24 0 0)
				(length 5.08)
				(name "DONE")
				(number "Y3")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "CFG_0")
				(number "U4")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "CFG_1")
				(number "T4")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "CFG_2")
				(number "R4")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "W10")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "W11")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 5.08)
				(name "TDO")
				(number "V4")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "TCK")
				(number "T5")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "TDI")
				(number "R5")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "TMS")
				(number "U5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LFE5U-85F-8BG756x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 24.13 16.51 0)
		)
		(property "Value" "LFE5U-85F-8BG756x"
			(at 24.13 13.97 0)
		)
		(property "Footprint" "Package_BGA:Lattice_caBGA-756_27x27mm_Layout32x32_P0.8mm"
			(at 11.43 72.39 0)
		)
		(property "Datasheet" "https://www.latticesemi.com/view_document?document_id=50461"
			(at 11.43 72.39 0)
		)
		(property "Description" "ECP5 FPGA, 84K LUTs, 1.2V, BGA-756"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Lattice*caBGA*27x27mm*Layout32x32*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "LFE5U-85F-8BG756x_1_1"
			(pin no_connect line
				(at -25.4 2.54 0)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "AK9")
			)
			(pin no_connect line
				(at -25.4 0 0)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "AK10")
			)
			(pin no_connect line
				(at -25.4 -2.54 0)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "AK12")
			)
			(pin no_connect line
				(at -25.4 -5.08 0)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "AK13")
			)
			(pin no_connect line
				(at -22.86 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G15")
			)
			(pin no_connect line
				(at -20.32 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G14")
			)
			(pin no_connect line
				(at -17.78 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "AG24")
			)
			(pin no_connect line
				(at -15.24 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G23")
			)
			(pin no_connect line
				(at -12.7 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G22")
			)
			(pin no_connect line
				(at -10.16 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G19")
			)
			(pin no_connect line
				(at -7.62 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G18")
			)
			(pin no_connect line
				(at -5.08 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G17")
			)
			(pin no_connect line
				(at -2.54 10.16 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G9")
			)
			(pin no_connect line
				(at -2.54 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G16")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "AA12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "AA13")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VCC")
				(number "AA14")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "AA15")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "AA16")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "AA17")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "AA18")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "AA19")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "AA20")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "AA21")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M13")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M14")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M15")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M16")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M17")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M18")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M19")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M20")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M21")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "N12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "N21")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "P12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "P21")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "R12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "R21")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "T12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "T21")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "U12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "U21")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "V12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "V21")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "W12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "W21")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "Y12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "Y21")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AA11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AA22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB21")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AC12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AC13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AC14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AC15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AC16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AC17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AC18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AC19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AC20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AC21")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD28")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD31")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AF11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AF12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AF14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AF15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AF16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AF17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AF19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AF20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AF22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AF23")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AG11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AG12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AG14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AG15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AG16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AG17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AG19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AG20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AG22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AG23")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AG9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH23")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH24")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH25")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH26")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH29")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH31")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ21")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ23")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ24")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ25")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ26")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AK11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AK14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AK17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AK20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AK23")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AK26")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AK7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AK8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL21")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL23")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL24")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL26")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL29")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL31")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AM11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AM12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AM14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AM15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AM17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AM18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AM20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AM21")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AM23")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AM24")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AM26")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AM7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AM8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AM9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B24")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B28")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "B31")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E24")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E28")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E31")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J28")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J31")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K23")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L21")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L23")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N28")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N31")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R28")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R31")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V28")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V31")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y31")
			)
			(pin no_connect line
				(at 2.54 10.16 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "E7")
			)
			(pin no_connect line
				(at 2.54 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G11")
			)
			(pin no_connect line
				(at 5.08 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "AC29")
			)
			(pin no_connect line
				(at 7.62 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "L28")
			)
			(pin no_connect line
				(at 10.16 10.16 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G24")
			)
			(pin no_connect line
				(at 10.16 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "W27")
			)
			(pin passive line
				(at 12.7 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUX")
				(number "AC11")
			)
			(pin passive line
				(at 12.7 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUX")
				(number "AC22")
			)
			(pin passive line
				(at 12.7 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUX")
				(number "K13")
			)
			(pin passive line
				(at 12.7 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUX")
				(number "K20")
			)
			(pin passive line
				(at 12.7 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUX")
				(number "N10")
			)
			(pin power_in line
				(at 12.7 15.24 270)
				(length 5.08)
				(name "VCCAUX")
				(number "N23")
			)
			(pin passive line
				(at 12.7 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUX")
				(number "Y10")
			)
			(pin passive line
				(at 12.7 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUX")
				(number "Y23")
			)
			(pin no_connect line
				(at 12.7 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "H29")
			)
			(pin no_connect line
				(at 15.24 10.16 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "E26")
			)
			(pin no_connect line
				(at 15.24 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "V30")
			)
			(pin no_connect line
				(at 17.78 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "AG31")
			)
			(pin no_connect line
				(at 20.32 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G10")
			)
			(pin no_connect line
				(at 22.86 10.16 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "AE7")
			)
			(pin no_connect line
				(at 22.86 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "AE26")
			)
			(pin no_connect line
				(at 25.4 2.54 180)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "AK18")
			)
			(pin no_connect line
				(at 25.4 0 180)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "AK19")
			)
			(pin no_connect line
				(at 25.4 -2.54 180)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "AK21")
			)
			(pin no_connect line
				(at 25.4 -5.08 180)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "AK22")
			)
		)
		(symbol "LFE5U-85F-8BG756x_2_1"
			(pin bidirectional line
				(at -10.16 66.04 0)
				(length 5.08)
				(name "PT4A")
				(number "B3")
			)
			(pin bidirectional line
				(at -10.16 63.5 0)
				(length 5.08)
				(name "PT4B")
				(number "B4")
			)
			(pin bidirectional line
				(at -10.16 60.96 0)
				(length 5.08)
				(name "PT6A")
				(number "A2")
			)
			(pin bidirectional line
				(at -10.16 58.42 0)
				(length 5.08)
				(name "PT6B")
				(number "A3")
			)
			(pin bidirectional line
				(at -10.16 55.88 0)
				(length 5.08)
				(name "PT9A")
				(number "A4")
			)
			(pin bidirectional line
				(at -10.16 53.34 0)
				(length 5.08)
				(name "PT9B")
				(number "A5")
			)
			(pin bidirectional line
				(at -10.16 50.8 0)
				(length 5.08)
				(name "PT11A")
				(number "D7")
			)
			(pin bidirectional line
				(at -10.16 48.26 0)
				(length 5.08)
				(name "PT11B")
				(number "C7")
			)
			(pin bidirectional line
				(at -10.16 45.72 0)
				(length 5.08)
				(name "PT13A")
				(number "B7")
			)
			(pin bidirectional line
				(at -10.16 43.18 0)
				(length 5.08)
				(name "PT13B")
				(number "A7")
			)
			(pin bidirectional line
				(at -10.16 40.64 0)
				(length 5.08)
				(name "PT15A")
				(number "F8")
			)
			(pin bidirectional line
				(at -10.16 38.1 0)
				(length 5.08)
				(name "PT15B")
				(number "E8")
			)
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PT18A")
				(number "D8")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PT18B")
				(number "C8")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PT20A")
				(number "B8")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PT20B")
				(number "A8")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PT22A")
				(number "F9")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PT22B")
				(number "D9")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PT24A")
				(number "C9")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PT24B")
				(number "A9")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PT27A")
				(number "F10")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PT27B")
				(number "E10")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PT29A")
				(number "D10")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PT29B")
				(number "C10")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PT31A")
				(number "B10")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PT31B")
				(number "A10")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PT33A")
				(number "F11")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PT33B")
				(number "E11")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PT36A")
				(number "D11")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PT36B")
				(number "C11")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PT38A")
				(number "B11")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PT38B")
				(number "A11")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PT40A")
				(number "F13")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PT40B")
				(number "D13")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PT42A")
				(number "C13")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PT42B")
				(number "A13")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PT45A")
				(number "F14")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PT45B")
				(number "E14")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PT47A")
				(number "D14")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PT47B")
				(number "C14")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PT49A")
				(number "B14")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PT49B")
				(number "A14")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PT51A")
				(number "F15")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PT51B")
				(number "D15")
			)
			(pin bidirectional line
				(at -10.16 -45.72 0)
				(length 5.08)
				(name "PT54A")
				(number "C15")
			)
			(pin bidirectional line
				(at -10.16 -48.26 0)
				(length 5.08)
				(name "PT54B")
				(number "A15")
			)
			(pin bidirectional line
				(at -10.16 -50.8 0)
				(length 5.08)
				(name "PT56A")
				(number "F16")
			)
			(pin bidirectional line
				(at -10.16 -53.34 0)
				(length 5.08)
				(name "PT56B")
				(number "E16")
			)
			(pin bidirectional line
				(at -10.16 -55.88 0)
				(length 5.08)
				(name "PT58A")
				(number "D16")
			)
			(pin bidirectional line
				(at -10.16 -58.42 0)
				(length 5.08)
				(name "PT58B")
				(number "C16")
			)
			(pin bidirectional line
				(at -10.16 -60.96 0)
				(length 5.08)
				(name "PT60A")
				(number "B16")
			)
			(pin bidirectional line
				(at -10.16 -63.5 0)
				(length 5.08)
				(name "PT60B")
				(number "A16")
			)
			(pin bidirectional line
				(at -10.16 -66.04 0)
				(length 5.08)
				(name "PT63A")
				(number "A17")
			)
			(pin bidirectional line
				(at -10.16 -68.58 0)
				(length 5.08)
				(name "PT63B")
				(number "B17")
			)
			(pin bidirectional line
				(at -10.16 -71.12 0)
				(length 5.08)
				(name "PT65A")
				(number "C17")
			)
			(pin bidirectional line
				(at -10.16 -73.66 0)
				(length 5.08)
				(name "PT65B")
				(number "D17")
			)
			(pin passive line
				(at 0 81.28 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO0")
				(number "K12")
			)
			(pin passive line
				(at 0 81.28 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO0")
				(number "K14")
			)
			(pin passive line
				(at 0 81.28 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO0")
				(number "K15")
			)
			(pin power_in line
				(at 0 81.28 270)
				(length 5.08)
				(name "VCCIO0")
				(number "K16")
			)
			(pin no_connect line
				(at 2.54 76.2 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "W6")
			)
		)
		(symbol "LFE5U-85F-8BG756x_3_1"
			(pin bidirectional line
				(at -10.16 55.88 0)
				(length 5.08)
				(name "PT69A")
				(number "E17")
			)
			(pin bidirectional line
				(at -10.16 53.34 0)
				(length 5.08)
				(name "PT69B")
				(number "F17")
			)
			(pin bidirectional line
				(at -10.16 50.8 0)
				(length 5.08)
				(name "PT71A")
				(number "A18")
			)
			(pin bidirectional line
				(at -10.16 48.26 0)
				(length 5.08)
				(name "PT71B")
				(number "C18")
			)
			(pin bidirectional line
				(at -10.16 45.72 0)
				(length 5.08)
				(name "PT74A")
				(number "D18")
			)
			(pin bidirectional line
				(at -10.16 43.18 0)
				(length 5.08)
				(name "PT74B")
				(number "F18")
			)
			(pin bidirectional line
				(at -10.16 40.64 0)
				(length 5.08)
				(name "PT76A")
				(number "A19")
			)
			(pin bidirectional line
				(at -10.16 38.1 0)
				(length 5.08)
				(name "PT76B")
				(number "B19")
			)
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PT78A")
				(number "C19")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PT78B")
				(number "D19")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PT80A")
				(number "E19")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PT80B")
				(number "F19")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PT83A")
				(number "A20")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PT83B")
				(number "C20")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PT85A")
				(number "D20")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PT85B")
				(number "F20")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PT87A")
				(number "A22")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PT87B")
				(number "B22")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PT89A")
				(number "C22")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PT89B")
				(number "D22")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PT92A")
				(number "E22")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PT92B")
				(number "F22")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PT94A")
				(number "A23")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PT94B")
				(number "B23")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PT96A")
				(number "C23")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PT96B")
				(number "D23")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PT98A")
				(number "E23")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PT98B")
				(number "F23")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PT101A")
				(number "A24")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PT101B")
				(number "C24")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PT103A")
				(number "D24")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PT103B")
				(number "F24")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PT105A")
				(number "A25")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PT105B")
				(number "B25")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PT107A")
				(number "C25")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PT107B")
				(number "D25")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PT110A")
				(number "E25")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PT110B")
				(number "F25")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PT112A")
				(number "A26")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PT112B")
				(number "B26")
			)
			(pin bidirectional line
				(at -10.16 -45.72 0)
				(length 5.08)
				(name "PT114A")
				(number "C26")
			)
			(pin bidirectional line
				(at -10.16 -48.26 0)
				(length 5.08)
				(name "PT114B")
				(number "D26")
			)
			(pin bidirectional line
				(at -10.16 -50.8 0)
				(length 5.08)
				(name "PT116A")
				(number "A28")
			)
			(pin bidirectional line
				(at -10.16 -53.34 0)
				(length 5.08)
				(name "PT116B")
				(number "A29")
			)
			(pin bidirectional line
				(at -10.16 -55.88 0)
				(length 5.08)
				(name "PT119A")
				(number "A30")
			)
			(pin bidirectional line
				(at -10.16 -58.42 0)
				(length 5.08)
				(name "PT119B")
				(number "A31")
			)
			(pin bidirectional line
				(at -10.16 -60.96 0)
				(length 5.08)
				(name "PT121A")
				(number "B29")
			)
			(pin bidirectional line
				(at -10.16 -63.5 0)
				(length 5.08)
				(name "PT121B")
				(number "B30")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO1")
				(number "K17")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO1")
				(number "K18")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO1")
				(number "K19")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VCCIO1")
				(number "K21")
			)
			(pin no_connect line
				(at 2.54 66.04 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "L5")
			)
		)
		(symbol "LFE5U-85F-8BG756x_4_1"
			(pin bidirectional line
				(at -10.16 55.88 0)
				(length 5.08)
				(name "PR11A")
				(number "C28")
			)
			(pin bidirectional line
				(at -10.16 53.34 0)
				(length 5.08)
				(name "PR11B")
				(number "D28")
			)
			(pin bidirectional line
				(at -10.16 50.8 0)
				(length 5.08)
				(name "PR11C")
				(number "C29")
			)
			(pin bidirectional line
				(at -10.16 48.26 0)
				(length 5.08)
				(name "PR11D")
				(number "C30")
			)
			(pin bidirectional line
				(at -10.16 45.72 0)
				(length 5.08)
				(name "PR14A")
				(number "D29")
			)
			(pin bidirectional line
				(at -10.16 43.18 0)
				(length 5.08)
				(name "PR14B")
				(number "E29")
			)
			(pin bidirectional line
				(at -10.16 40.64 0)
				(length 5.08)
				(name "PR14C")
				(number "F29")
			)
			(pin bidirectional line
				(at -10.16 38.1 0)
				(length 5.08)
				(name "PR14D")
				(number "F28")
			)
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PR17A")
				(number "B32")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PR17B")
				(number "C31")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PR17C")
				(number "D30")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PR17D")
				(number "D31")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PR20A")
				(number "F30")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PR20B")
				(number "E30")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PR20C")
				(number "C32")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PR20D")
				(number "D32")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PR23A")
				(number "F31")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PR23B")
				(number "E32")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PR23C")
				(number "F32")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PR23D")
				(number "H32")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PR26A")
				(number "H31")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PR26B")
				(number "H30")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PR26C")
				(number "J30")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PR26D")
				(number "K30")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PR29A")
				(number "K31")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PR29B")
				(number "J32")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PR29C")
				(number "K32")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PR29D")
				(number "L32")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PR32A")
				(number "L31")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PR32B")
				(number "L30")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PR32C")
				(number "J29")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PR32D")
				(number "K29")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PR35A")
				(number "H27")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PR35B")
				(number "H28")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PR35C")
				(number "J26")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PR35D")
				(number "J27")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PR38A")
				(number "K27")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PR38B")
				(number "K26")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PR38C")
				(number "K28")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PR38D")
				(number "L29")
			)
			(pin bidirectional line
				(at -10.16 -45.72 0)
				(length 5.08)
				(name "PR41A")
				(number "N30")
			)
			(pin bidirectional line
				(at -10.16 -48.26 0)
				(length 5.08)
				(name "PR41B")
				(number "N29")
			)
			(pin bidirectional line
				(at -10.16 -50.8 0)
				(length 5.08)
				(name "PR41C")
				(number "L26")
			)
			(pin bidirectional line
				(at -10.16 -53.34 0)
				(length 5.08)
				(name "PR41D")
				(number "L27")
			)
			(pin bidirectional line
				(at -10.16 -55.88 0)
				(length 5.08)
				(name "PR44A")
				(number "N27")
			)
			(pin bidirectional line
				(at -10.16 -58.42 0)
				(length 5.08)
				(name "PR44B")
				(number "N26")
			)
			(pin bidirectional line
				(at -10.16 -60.96 0)
				(length 5.08)
				(name "PR44C")
				(number "P27")
			)
			(pin bidirectional line
				(at -10.16 -63.5 0)
				(length 5.08)
				(name "PR44D")
				(number "P26")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VCCIO2")
				(number "M23")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO2")
				(number "P23")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO2")
				(number "R23")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO2")
				(number "T23")
			)
			(pin no_connect line
				(at 2.54 66.04 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "H4")
			)
		)
		(symbol "LFE5U-85F-8BG756x_5_1"
			(pin bidirectional line
				(at -10.16 76.2 0)
				(length 5.08)
				(name "PR47A")
				(number "P28")
			)
			(pin bidirectional line
				(at -10.16 73.66 0)
				(length 5.08)
				(name "PR47B")
				(number "P29")
			)
			(pin bidirectional line
				(at -10.16 71.12 0)
				(length 5.08)
				(name "PR47C")
				(number "R26")
			)
			(pin bidirectional line
				(at -10.16 68.58 0)
				(length 5.08)
				(name "PR47D")
				(number "T26")
			)
			(pin bidirectional line
				(at -10.16 66.04 0)
				(length 5.08)
				(name "PR50A")
				(number "R27")
			)
			(pin bidirectional line
				(at -10.16 63.5 0)
				(length 5.08)
				(name "PR50B")
				(number "T27")
			)
			(pin bidirectional line
				(at -10.16 60.96 0)
				(length 5.08)
				(name "PR50C")
				(number "U27")
			)
			(pin bidirectional line
				(at -10.16 58.42 0)
				(length 5.08)
				(name "PR50D")
				(number "U26")
			)
			(pin bidirectional line
				(at -10.16 55.88 0)
				(length 5.08)
				(name "PR53A")
				(number "R29")
			)
			(pin bidirectional line
				(at -10.16 53.34 0)
				(length 5.08)
				(name "PR53B")
				(number "T28")
			)
			(pin bidirectional line
				(at -10.16 50.8 0)
				(length 5.08)
				(name "PR53C")
				(number "T29")
			)
			(pin bidirectional line
				(at -10.16 48.26 0)
				(length 5.08)
				(name "PR53D")
				(number "U28")
			)
			(pin bidirectional line
				(at -10.16 45.72 0)
				(length 5.08)
				(name "PR56A")
				(number "U29")
			)
			(pin bidirectional line
				(at -10.16 43.18 0)
				(length 5.08)
				(name "PR56B")
				(number "V29")
			)
			(pin bidirectional line
				(at -10.16 40.64 0)
				(length 5.08)
				(name "PR56C")
				(number "V27")
			)
			(pin bidirectional line
				(at -10.16 38.1 0)
				(length 5.08)
				(name "PR56D")
				(number "V26")
			)
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PR59A")
				(number "P31")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PR59B")
				(number "P30")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PR59C")
				(number "R30")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PR59D")
				(number "T30")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PR62A")
				(number "N32")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PR62B")
				(number "P32")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PR62C")
				(number "U31")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PR62D")
				(number "U30")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PR65A")
				(number "R32")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PR65B")
				(number "T31")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PR65C")
				(number "W30")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PR65D")
				(number "Y30")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PR68A")
				(number "T32")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PR68B")
				(number "U32")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PR68C")
				(number "V32")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PR68D")
				(number "W32")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PR71A")
				(number "Y26")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PR71B")
				(number "Y27")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PR71C")
				(number "Y28")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PR71D")
				(number "W28")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PR74A")
				(number "Y29")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PR74B")
				(number "W29")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PR74C")
				(number "AB26")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PR74D")
				(number "AC27")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PR77A")
				(number "AB28")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PR77B")
				(number "AB27")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PR77C")
				(number "AC26")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PR77D")
				(number "AD26")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PR80A")
				(number "AD27")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PR80B")
				(number "AE27")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PR80C")
				(number "AE28")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PR80D")
				(number "AE29")
			)
			(pin bidirectional line
				(at -10.16 -45.72 0)
				(length 5.08)
				(name "PR83A")
				(number "AB30")
			)
			(pin bidirectional line
				(at -10.16 -48.26 0)
				(length 5.08)
				(name "PR83B")
				(number "AB29")
			)
			(pin bidirectional line
				(at -10.16 -50.8 0)
				(length 5.08)
				(name "PR83C")
				(number "AC28")
			)
			(pin bidirectional line
				(at -10.16 -53.34 0)
				(length 5.08)
				(name "PR83D")
				(number "AD29")
			)
			(pin bidirectional line
				(at -10.16 -55.88 0)
				(length 5.08)
				(name "PR86A")
				(number "W31")
			)
			(pin bidirectional line
				(at -10.16 -58.42 0)
				(length 5.08)
				(name "PR86B")
				(number "Y32")
			)
			(pin bidirectional line
				(at -10.16 -60.96 0)
				(length 5.08)
				(name "PR86C")
				(number "AD30")
			)
			(pin bidirectional line
				(at -10.16 -63.5 0)
				(length 5.08)
				(name "PR86D")
				(number "AE30")
			)
			(pin bidirectional line
				(at -10.16 -66.04 0)
				(length 5.08)
				(name "PR89A")
				(number "AC30")
			)
			(pin bidirectional line
				(at -10.16 -68.58 0)
				(length 5.08)
				(name "PR89B")
				(number "AB31")
			)
			(pin bidirectional line
				(at -10.16 -71.12 0)
				(length 5.08)
				(name "PR89C")
				(number "AC31")
			)
			(pin bidirectional line
				(at -10.16 -73.66 0)
				(length 5.08)
				(name "PR89D")
				(number "AE31")
			)
			(pin bidirectional line
				(at -10.16 -76.2 0)
				(length 5.08)
				(name "PR92A")
				(number "AB32")
			)
			(pin bidirectional line
				(at -10.16 -78.74 0)
				(length 5.08)
				(name "PR92B")
				(number "AC32")
			)
			(pin bidirectional line
				(at -10.16 -81.28 0)
				(length 5.08)
				(name "PR92C")
				(number "AD32")
			)
			(pin bidirectional line
				(at -10.16 -83.82 0)
				(length 5.08)
				(name "PR92D")
				(number "AE32")
			)
			(pin passive line
				(at 0 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO3")
				(number "AA23")
			)
			(pin power_in line
				(at 0 91.44 270)
				(length 5.08)
				(name "VCCIO3")
				(number "U23")
			)
			(pin passive line
				(at 0 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO3")
				(number "V23")
			)
			(pin passive line
				(at 0 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO3")
				(number "W23")
			)
			(pin no_connect line
				(at 2.54 86.36 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "AC4")
			)
		)
		(symbol "LFE5U-85F-8BG756x_6_1"
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PB96A")
				(number "AM28")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PB96B")
				(number "AM29")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PB98A")
				(number "AL28")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PB98B")
				(number "AK28")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PB101A")
				(number "AK32")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PB101B")
				(number "AJ32")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PB103A")
				(number "AM30")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PB103B")
				(number "AL30")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PB105A")
				(number "AK31")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PB105B")
				(number "AJ31")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PB107A")
				(number "AM31")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PB107B")
				(number "AL32")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PB110A")
				(number "AG28")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PB110B")
				(number "AG29")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PB112A")
				(number "AJ28")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PB112B")
				(number "AH28")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PB114A")
				(number "AH30")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PB114B")
				(number "AG30")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PB116A")
				(number "AK29")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PB116B")
				(number "AK30")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PB119A")
				(number "AH32")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PB119B")
				(number "AG32")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PB121A")
				(number "AJ29")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PB121B")
				(number "AJ30")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 5.08)
				(name "VCCIO4")
				(number "AB23")
			)
			(pin passive line
				(at 0 40.64 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO4")
				(number "AC23")
			)
			(pin no_connect line
				(at 2.54 35.56 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "V3")
			)
		)
		(symbol "LFE5U-85F-8BG756x_7_1"
			(pin bidirectional line
				(at -10.16 76.2 0)
				(length 5.08)
				(name "PL47A")
				(number "P5")
			)
			(pin bidirectional line
				(at -10.16 73.66 0)
				(length 5.08)
				(name "PL47B")
				(number "P4")
			)
			(pin bidirectional line
				(at -10.16 71.12 0)
				(length 5.08)
				(name "PL47C")
				(number "R7")
			)
			(pin bidirectional line
				(at -10.16 68.58 0)
				(length 5.08)
				(name "PL47D")
				(number "T7")
			)
			(pin bidirectional line
				(at -10.16 66.04 0)
				(length 5.08)
				(name "PL50A")
				(number "R6")
			)
			(pin bidirectional line
				(at -10.16 63.5 0)
				(length 5.08)
				(name "PL50B")
				(number "T6")
			)
			(pin bidirectional line
				(at -10.16 60.96 0)
				(length 5.08)
				(name "PL50C")
				(number "U6")
			)
			(pin bidirectional line
				(at -10.16 58.42 0)
				(length 5.08)
				(name "PL50D")
				(number "U7")
			)
			(pin bidirectional line
				(at -10.16 55.88 0)
				(length 5.08)
				(name "PL53A")
				(number "R4")
			)
			(pin bidirectional line
				(at -10.16 53.34 0)
				(length 5.08)
				(name "PL53B")
				(number "T5")
			)
			(pin bidirectional line
				(at -10.16 50.8 0)
				(length 5.08)
				(name "PL53C")
				(number "T4")
			)
			(pin bidirectional line
				(at -10.16 48.26 0)
				(length 5.08)
				(name "PL53D")
				(number "U5")
			)
			(pin bidirectional line
				(at -10.16 45.72 0)
				(length 5.08)
				(name "PL56A")
				(number "U4")
			)
			(pin bidirectional line
				(at -10.16 43.18 0)
				(length 5.08)
				(name "PL56B")
				(number "V4")
			)
			(pin bidirectional line
				(at -10.16 40.64 0)
				(length 5.08)
				(name "PL56C")
				(number "V6")
			)
			(pin bidirectional line
				(at -10.16 38.1 0)
				(length 5.08)
				(name "PL56D")
				(number "V7")
			)
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PL59A")
				(number "P2")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PL59B")
				(number "P3")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PL59C")
				(number "R3")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PL59D")
				(number "T3")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PL62A")
				(number "N1")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PL62B")
				(number "P1")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PL62C")
				(number "U2")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PL62D")
				(number "U3")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PL65A")
				(number "R1")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PL65B")
				(number "T2")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PL65C")
				(number "W3")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PL65D")
				(number "Y3")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PL68A")
				(number "T1")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PL68B")
				(number "U1")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PL68C")
				(number "V1")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PL68D")
				(number "W1")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PL71A")
				(number "Y7")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PL71B")
				(number "Y6")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PL71C")
				(number "Y5")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PL71D")
				(number "W5")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PL74A")
				(number "Y4")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PL74B")
				(number "W4")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PL74C")
				(number "AB7")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PL74D")
				(number "AC6")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PL77A")
				(number "AB5")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PL77B")
				(number "AB6")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PL77C")
				(number "AC7")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PL77D")
				(number "AD7")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PL80A")
				(number "AD6")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PL80B")
				(number "AE6")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PL80C")
				(number "AE5")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PL80D")
				(number "AE4")
			)
			(pin bidirectional line
				(at -10.16 -45.72 0)
				(length 5.08)
				(name "PL83A")
				(number "AB3")
			)
			(pin bidirectional line
				(at -10.16 -48.26 0)
				(length 5.08)
				(name "PL83B")
				(number "AB4")
			)
			(pin bidirectional line
				(at -10.16 -50.8 0)
				(length 5.08)
				(name "PL83C")
				(number "AC5")
			)
			(pin bidirectional line
				(at -10.16 -53.34 0)
				(length 5.08)
				(name "PL83D")
				(number "AD4")
			)
			(pin bidirectional line
				(at -10.16 -55.88 0)
				(length 5.08)
				(name "PL86A")
				(number "W2")
			)
			(pin bidirectional line
				(at -10.16 -58.42 0)
				(length 5.08)
				(name "PL86B")
				(number "Y1")
			)
			(pin bidirectional line
				(at -10.16 -60.96 0)
				(length 5.08)
				(name "PL86C")
				(number "AD3")
			)
			(pin bidirectional line
				(at -10.16 -63.5 0)
				(length 5.08)
				(name "PL86D")
				(number "AE3")
			)
			(pin bidirectional line
				(at -10.16 -66.04 0)
				(length 5.08)
				(name "PL89A")
				(number "AC3")
			)
			(pin bidirectional line
				(at -10.16 -68.58 0)
				(length 5.08)
				(name "PL89B")
				(number "AB2")
			)
			(pin bidirectional line
				(at -10.16 -71.12 0)
				(length 5.08)
				(name "PL89C")
				(number "AC2")
			)
			(pin bidirectional line
				(at -10.16 -73.66 0)
				(length 5.08)
				(name "PL89D")
				(number "AE2")
			)
			(pin bidirectional line
				(at -10.16 -76.2 0)
				(length 5.08)
				(name "PL92A")
				(number "AB1")
			)
			(pin bidirectional line
				(at -10.16 -78.74 0)
				(length 5.08)
				(name "PL92B")
				(number "AC1")
			)
			(pin bidirectional line
				(at -10.16 -81.28 0)
				(length 5.08)
				(name "PL92C")
				(number "AD1")
			)
			(pin bidirectional line
				(at -10.16 -83.82 0)
				(length 5.08)
				(name "PL92D")
				(number "AE1")
			)
			(pin passive line
				(at 0 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO6")
				(number "AA10")
			)
			(pin power_in line
				(at 0 91.44 270)
				(length 5.08)
				(name "VCCIO6")
				(number "U10")
			)
			(pin passive line
				(at 0 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO6")
				(number "V10")
			)
			(pin passive line
				(at 0 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO6")
				(number "W10")
			)
			(pin no_connect line
				(at 2.54 86.36 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "AG2")
			)
		)
		(symbol "LFE5U-85F-8BG756x_8_1"
			(pin bidirectional line
				(at -10.16 55.88 0)
				(length 5.08)
				(name "PL11A")
				(number "C5")
			)
			(pin bidirectional line
				(at -10.16 53.34 0)
				(length 5.08)
				(name "PL11B")
				(number "D5")
			)
			(pin bidirectional line
				(at -10.16 50.8 0)
				(length 5.08)
				(name "PL11C")
				(number "C4")
			)
			(pin bidirectional line
				(at -10.16 48.26 0)
				(length 5.08)
				(name "PL11D")
				(number "C3")
			)
			(pin bidirectional line
				(at -10.16 45.72 0)
				(length 5.08)
				(name "PL14A")
				(number "D4")
			)
			(pin bidirectional line
				(at -10.16 43.18 0)
				(length 5.08)
				(name "PL14B")
				(number "E4")
			)
			(pin bidirectional line
				(at -10.16 40.64 0)
				(length 5.08)
				(name "PL14C")
				(number "F4")
			)
			(pin bidirectional line
				(at -10.16 38.1 0)
				(length 5.08)
				(name "PL14D")
				(number "F5")
			)
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PL17A")
				(number "B1")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PL17B")
				(number "C2")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PL17C")
				(number "D3")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PL17D")
				(number "D2")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PL20A")
				(number "F3")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PL20B")
				(number "E3")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PL20C")
				(number "C1")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PL20D")
				(number "D1")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PL23A")
				(number "F2")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PL23B")
				(number "E1")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PL23C")
				(number "F1")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PL23D")
				(number "H1")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PL26A")
				(number "H2")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PL26B")
				(number "H3")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PL26C")
				(number "J3")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PL26D")
				(number "K3")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PL29A")
				(number "K2")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PL29B")
				(number "J1")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PL29C")
				(number "K1")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PL29D")
				(number "L1")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PL32A")
				(number "L2")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PL32B")
				(number "L3")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PL32C")
				(number "J4")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PL32D")
				(number "K4")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PL35A")
				(number "H6")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PL35B")
				(number "H5")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PL35C")
				(number "J7")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PL35D")
				(number "J6")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PL38A")
				(number "K6")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PL38B")
				(number "K7")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PL38C")
				(number "K5")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PL38D")
				(number "L4")
			)
			(pin bidirectional line
				(at -10.16 -45.72 0)
				(length 5.08)
				(name "PL41A")
				(number "N3")
			)
			(pin bidirectional line
				(at -10.16 -48.26 0)
				(length 5.08)
				(name "PL41B")
				(number "N4")
			)
			(pin bidirectional line
				(at -10.16 -50.8 0)
				(length 5.08)
				(name "PL41C")
				(number "L7")
			)
			(pin bidirectional line
				(at -10.16 -53.34 0)
				(length 5.08)
				(name "PL41D")
				(number "L6")
			)
			(pin bidirectional line
				(at -10.16 -55.88 0)
				(length 5.08)
				(name "PL44A")
				(number "N6")
			)
			(pin bidirectional line
				(at -10.16 -58.42 0)
				(length 5.08)
				(name "PL44B")
				(number "N7")
			)
			(pin bidirectional line
				(at -10.16 -60.96 0)
				(length 5.08)
				(name "PL44C")
				(number "P6")
			)
			(pin bidirectional line
				(at -10.16 -63.5 0)
				(length 5.08)
				(name "PL44D")
				(number "P7")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VCCIO7")
				(number "M10")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO7")
				(number "P10")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO7")
				(number "R10")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO7")
				(number "T10")
			)
		)
		(symbol "LFE5U-85F-8BG756x_9_1"
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PB4A")
				(number "AG1")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PB4B")
				(number "AH1")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PB6A")
				(number "AJ1")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PB6B")
				(number "AK1")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PB9A")
				(number "AL1")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PB9B")
				(number "AM2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PB11A")
				(number "AJ2")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PB11B")
				(number "AK2")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PB13A")
				(number "AG3")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PB13B")
				(number "AH3")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PB15A")
				(number "AJ3")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PB15B")
				(number "AK3")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PB18A")
				(number "AL3")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 5.08)
				(name "VCCIO8")
				(number "AB10")
			)
			(pin passive line
				(at 0 27.94 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO8")
				(number "AC10")
			)
		)
		(symbol "LFE5U-85F-8BG756x_10_1"
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "CCLK")
				(number "AM3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "~{PROGRAM}")
				(number "AH4")
			)
			(pin open_collector line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "~{INIT}")
				(number "AG4")
			)
			(pin open_collector line
				(at -15.24 0 0)
				(length 5.08)
				(name "DONE")
				(number "AJ4")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "CFG_0")
				(number "AM4")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "CFG_1")
				(number "AL4")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "CFG_2")
				(number "AK4")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "AK15")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "AK16")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "AK24")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "AK25")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 5.08)
				(name "TDO")
				(number "AG5")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "TCK")
				(number "AK5")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "TDI")
				(number "AJ5")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "TMS")
				(number "AM5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LFE5UM5G-85F-8BG381x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 24.13 16.51 0)
		)
		(property "Value" "LFE5UM5G-85F-8BG381x"
			(at 24.13 13.97 0)
		)
		(property "Footprint" "Package_BGA:Lattice_caBGA-381_17x17mm_Layout20x20_P0.8mm"
			(at 11.43 72.39 0)
		)
		(property "Datasheet" "https://www.latticesemi.com/view_document?document_id=50461"
			(at 11.43 72.39 0)
		)
		(property "Description" "ECP5-5G FPGA, 84K LUTs, 1.2V, 5Gbps SERDES, BGA-381"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Lattice?caBGA*17x17mm*Layout20x20*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "LFE5UM5G-85F-8BG381x_1_1"
			(pin power_in line
				(at -22.86 15.24 270)
				(length 5.08)
				(name "VCCHTX0_D0CH0")
				(number "T7")
			)
			(pin power_in line
				(at -20.32 15.24 270)
				(length 5.08)
				(name "VCCHRX0_D0CH0")
				(number "T8")
			)
			(pin power_in line
				(at -17.78 15.24 270)
				(length 5.08)
				(name "VCCHRX1_D0CH1")
				(number "T9")
			)
			(pin power_in line
				(at -15.24 15.24 270)
				(length 5.08)
				(name "VCCHTX1_D0CH1")
				(number "T10")
			)
			(pin power_in line
				(at -12.7 15.24 270)
				(length 5.08)
				(name "VCCHTX0_D1CH0")
				(number "T11")
			)
			(pin power_in line
				(at -10.16 15.24 270)
				(length 5.08)
				(name "VCCHRX0_D1CH0")
				(number "T12")
			)
			(pin power_in line
				(at -7.62 15.24 270)
				(length 5.08)
				(name "VCCHRX1_D1CH1")
				(number "T13")
			)
			(pin power_in line
				(at -5.08 15.24 270)
				(length 5.08)
				(name "VCCHTX1_D1CH1")
				(number "T14")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "H10")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "H11")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "H12")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VCC")
				(number "H13")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "H8")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "H9")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "J13")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "J8")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "K13")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "K8")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "L13")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "L8")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M13")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M8")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "N10")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "N11")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "N12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "N13")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "N8")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "N9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "C19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "D4")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "F13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "F14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "F7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "F8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G4")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "G9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "H19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W7")
			)
			(pin passive line
				(at 5.08 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUXA0")
				(number "V10")
			)
			(pin power_in line
				(at 5.08 15.24 270)
				(length 5.08)
				(name "VCCAUXA0")
				(number "V11")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUXA1")
				(number "V17")
			)
			(pin power_in line
				(at 7.62 15.24 270)
				(length 5.08)
				(name "VCCAUXA1")
				(number "V18")
			)
			(pin passive line
				(at 12.7 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUX")
				(number "F15")
			)
			(pin passive line
				(at 12.7 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUX")
				(number "F6")
			)
			(pin power_in line
				(at 12.7 15.24 270)
				(length 5.08)
				(name "VCCAUX")
				(number "P15")
			)
			(pin passive line
				(at 12.7 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUX")
				(number "P6")
			)
			(pin power_in line
				(at 17.78 15.24 270)
				(length 5.08)
				(name "VCCA0")
				(number "T6")
			)
			(pin passive line
				(at 17.78 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCA0")
				(number "U6")
			)
			(pin power_in line
				(at 20.32 15.24 270)
				(length 5.08)
				(name "VCCA1")
				(number "T15")
			)
			(pin passive line
				(at 20.32 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCA1")
				(number "U15")
			)
		)
		(symbol "LFE5UM5G-85F-8BG381x_2_1"
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PT4A")
				(number "A6")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PT4B")
				(number "B6")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PT6A")
				(number "E6")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PT6B")
				(number "D6")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PT9A")
				(number "E7")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PT9B")
				(number "D7")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PT11A")
				(number "C6")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PT11B")
				(number "C7")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PT13A")
				(number "E8")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PT13B")
				(number "D8")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PT15A")
				(number "C8")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PT15B")
				(number "B8")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PT18A")
				(number "A7")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PT18B")
				(number "A8")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PT20A")
				(number "D9")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PT20B")
				(number "E9")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PT54A")
				(number "C9")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PT56A")
				(number "D10")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PT56B")
				(number "E10")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PT58A")
				(number "B9")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PT58B")
				(number "C10")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PT60A")
				(number "A9")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PT60B")
				(number "B10")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PT63A")
				(number "A10")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PT63B")
				(number "A11")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PT65A")
				(number "B11")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PT65B")
				(number "C11")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 5.08)
				(name "VCCIO0")
				(number "F10")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO0")
				(number "F9")
			)
		)
		(symbol "LFE5UM5G-85F-8BG381x_3_1"
			(pin bidirectional line
				(at -10.16 38.1 0)
				(length 5.08)
				(name "PT69A")
				(number "D11")
			)
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PT69B")
				(number "E11")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PT71A")
				(number "B12")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PT71B")
				(number "C12")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PT74A")
				(number "D12")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PT74B")
				(number "E12")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PT76A")
				(number "A12")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PT76B")
				(number "A13")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PT78A")
				(number "B13")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PT78B")
				(number "C13")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PT80A")
				(number "D13")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PT80B")
				(number "E13")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PT83A")
				(number "A14")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PT83B")
				(number "C14")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PT85A")
				(number "D14")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PT85B")
				(number "E14")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PT103A")
				(number "A15")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PT105A")
				(number "B15")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PT105B")
				(number "C15")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PT107A")
				(number "D15")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PT107B")
				(number "E15")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PT110A")
				(number "A16")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PT110B")
				(number "B16")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PT112A")
				(number "C16")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PT112B")
				(number "D16")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PT114A")
				(number "B17")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PT114B")
				(number "C17")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PT116A")
				(number "A17")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PT116B")
				(number "B18")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PT119A")
				(number "A18")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PT119B")
				(number "B19")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PT121A")
				(number "A19")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PT121B")
				(number "B20")
			)
			(pin passive line
				(at 0 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO1")
				(number "F11")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 5.08)
				(name "VCCIO1")
				(number "F12")
			)
		)
		(symbol "LFE5UM5G-85F-8BG381x_4_1"
			(pin bidirectional line
				(at -10.16 38.1 0)
				(length 5.08)
				(name "PR11A")
				(number "C18")
			)
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PR11B")
				(number "D17")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PR11C")
				(number "E16")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PR11D")
				(number "F16")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PR14A")
				(number "D18")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PR14B")
				(number "E17")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PR14C")
				(number "E18")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PR14D")
				(number "F18")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PR17A")
				(number "F17")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PR17B")
				(number "G18")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PR17C")
				(number "G16")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PR17D")
				(number "H16")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PR20A")
				(number "H18")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PR20B")
				(number "H17")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PR20C")
				(number "J17")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PR20D")
				(number "J16")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PR29A")
				(number "K16")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PR29B")
				(number "K17")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PR35A")
				(number "C20")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PR35B")
				(number "D19")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PR35C")
				(number "D20")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PR35D")
				(number "E19")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PR38A")
				(number "E20")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PR38B")
				(number "F19")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PR38C")
				(number "F20")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PR38D")
				(number "G20")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PR41A")
				(number "G19")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PR41B")
				(number "H20")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PR41C")
				(number "J18")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PR41D")
				(number "K18")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PR44A")
				(number "J19")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PR44B")
				(number "K19")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PR44C")
				(number "J20")
			)
			(pin bidirectional line
				(at -10.16 -45.72 0)
				(length 5.08)
				(name "PR44D")
				(number "K20")
			)
			(pin passive line
				(at 0 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO2")
				(number "H14")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 5.08)
				(name "VCCIO2")
				(number "H15")
			)
			(pin passive line
				(at 0 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO2")
				(number "J15")
			)
		)
		(symbol "LFE5UM5G-85F-8BG381x_5_1"
			(pin bidirectional line
				(at -10.16 38.1 0)
				(length 5.08)
				(name "PR47A")
				(number "L20")
			)
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PR47B")
				(number "M20")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PR47C")
				(number "L19")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PR47D")
				(number "M19")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PR50A")
				(number "L16")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PR50B")
				(number "L17")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PR50C")
				(number "L18")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PR50D")
				(number "M18")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PR53A")
				(number "N16")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PR53B")
				(number "M17")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PR53C")
				(number "N18")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PR53D")
				(number "P17")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PR56A")
				(number "N17")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PR56B")
				(number "P16")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PR56C")
				(number "R16")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PR56D")
				(number "R17")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PR77A")
				(number "T16")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PR83A")
				(number "N19")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PR83B")
				(number "N20")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PR83C")
				(number "P19")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PR83D")
				(number "P18")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PR86A")
				(number "P20")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PR86B")
				(number "R20")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PR86C")
				(number "T20")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PR86D")
				(number "U20")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PR89A")
				(number "T19")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PR89B")
				(number "R18")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PR89C")
				(number "U19")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PR89D")
				(number "T18")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PR92A")
				(number "U18")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PR92B")
				(number "U17")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PR92C")
				(number "U16")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PR92D")
				(number "T17")
			)
			(pin passive line
				(at 0 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO3")
				(number "L14")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 5.08)
				(name "VCCIO3")
				(number "L15")
			)
			(pin passive line
				(at 0 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO3")
				(number "M15")
			)
		)
		(symbol "LFE5UM5G-85F-8BG381x_6_1"
			(pin bidirectional line
				(at -10.16 38.1 0)
				(length 5.08)
				(name "PL47A")
				(number "G2")
			)
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PL47B")
				(number "F1")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PL47C")
				(number "H2")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PL47D")
				(number "G1")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PL50A")
				(number "J4")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PL50B")
				(number "J5")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PL50C")
				(number "J3")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PL50D")
				(number "K3")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PL53A")
				(number "K2")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PL53B")
				(number "J1")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PL53C")
				(number "H1")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PL53D")
				(number "K1")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PL56A")
				(number "K4")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PL56B")
				(number "K5")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PL56C")
				(number "L4")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PL56D")
				(number "L5")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PL77A")
				(number "M5")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PL83A")
				(number "M4")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PL83B")
				(number "N5")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PL83C")
				(number "N4")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PL83D")
				(number "P5")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PL86A")
				(number "N3")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PL86B")
				(number "M3")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PL86C")
				(number "L3")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PL86D")
				(number "L2")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PL89A")
				(number "N2")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PL89B")
				(number "M1")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PL89C")
				(number "L1")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PL89D")
				(number "N1")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PL92A")
				(number "P1")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PL92B")
				(number "P2")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PL92C")
				(number "P3")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PL92D")
				(number "P4")
			)
			(pin passive line
				(at 0 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO6")
				(number "L6")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 5.08)
				(name "VCCIO6")
				(number "L7")
			)
			(pin passive line
				(at 0 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO6")
				(number "M6")
			)
		)
		(symbol "LFE5UM5G-85F-8BG381x_7_1"
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PL11A")
				(number "A4")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PL11B")
				(number "A5")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PL11C")
				(number "B5")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PL11D")
				(number "C5")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PL14A")
				(number "C4")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PL14B")
				(number "B4")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PL14C")
				(number "A3")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PL14D")
				(number "B3")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PL17A")
				(number "E4")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PL17B")
				(number "D5")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PL17C")
				(number "C3")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PL17D")
				(number "D3")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PL20A")
				(number "F4")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PL20B")
				(number "E3")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PL20C")
				(number "E5")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PL20D")
				(number "F5")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PL35A")
				(number "A2")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PL35B")
				(number "B1")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PL35C")
				(number "B2")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PL35D")
				(number "C2")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PL38A")
				(number "C1")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PL38B")
				(number "D1")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PL38C")
				(number "D2")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PL38D")
				(number "E1")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PL41A")
				(number "H4")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PL41B")
				(number "G5")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PL41C")
				(number "H5")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PL41D")
				(number "H3")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PL44A")
				(number "G3")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PL44B")
				(number "F3")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PL44C")
				(number "F2")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PL44D")
				(number "E2")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO7")
				(number "H6")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 5.08)
				(name "VCCIO7")
				(number "H7")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO7")
				(number "J6")
			)
		)
		(symbol "LFE5UM5G-85F-8BG381x_8_1"
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PB4A")
				(number "R1")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PB4B")
				(number "T1")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PB6A")
				(number "U1")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PB6B")
				(number "V1")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PB9A")
				(number "W1")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PB9B")
				(number "Y2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PB11A")
				(number "V2")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PB11B")
				(number "W2")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PB13A")
				(number "T2")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PB13B")
				(number "U2")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PB15A")
				(number "R2")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PB15B")
				(number "R3")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PB18A")
				(number "T3")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 5.08)
				(name "VCCIO8")
				(number "P10")
			)
			(pin passive line
				(at 0 27.94 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO8")
				(number "P9")
			)
		)
		(symbol "LFE5UM5G-85F-8BG381x_9_1"
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "CCLK")
				(number "U3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "~{PROGRAM}")
				(number "W3")
			)
			(pin open_collector line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "~{INIT}")
				(number "V3")
			)
			(pin open_collector line
				(at -15.24 0 0)
				(length 5.08)
				(name "DONE")
				(number "Y3")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "CFG_0")
				(number "U4")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "CFG_1")
				(number "T4")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "CFG_2")
				(number "R4")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "W10")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "W11")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 5.08)
				(name "TDO")
				(number "V4")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "TCK")
				(number "T5")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "TDI")
				(number "R5")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "TMS")
				(number "U5")
			)
		)
		(symbol "LFE5UM5G-85F-8BG381x_10_1"
			(pin output line
				(at -15.24 15.24 0)
				(length 5.08)
				(name "HDTXP0_D0CH0")
				(number "W4")
			)
			(pin output line
				(at -15.24 12.7 0)
				(length 5.08)
				(name "HDTXN0_D0CH0")
				(number "W5")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "HDRXP0_D0CH0")
				(number "Y5")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "HDRXN0_D0CH0")
				(number "Y6")
			)
			(pin output line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "HDTXP0_D0CH1")
				(number "W8")
			)
			(pin output line
				(at -15.24 0 0)
				(length 5.08)
				(name "HDTXN0_D0CH1")
				(number "W9")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "HDRXP0_D0CH1")
				(number "Y7")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "HDRXN0_D0CH1")
				(number "Y8")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "REFCLKP_D0")
				(number "Y11")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 5.08)
				(name "REFCLKN_D0")
				(number "Y12")
			)
		)
		(symbol "LFE5UM5G-85F-8BG381x_11_1"
			(pin output line
				(at -15.24 15.24 0)
				(length 5.08)
				(name "HDTXP0_D1CH0")
				(number "W13")
			)
			(pin output line
				(at -15.24 12.7 0)
				(length 5.08)
				(name "HDTXN0_D1CH0")
				(number "W14")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "HDRXP0_D1CH0")
				(number "Y14")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "HDRXN0_D1CH0")
				(number "Y15")
			)
			(pin output line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "HDTXP0_D1CH1")
				(number "W17")
			)
			(pin output line
				(at -15.24 0 0)
				(length 5.08)
				(name "HDTXN0_D1CH1")
				(number "W18")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "HDRXP0_D1CH1")
				(number "Y16")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "HDRXN0_D1CH1")
				(number "Y17")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "REFCLKP_D1")
				(number "Y19")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 5.08)
				(name "REFCLKN_D1")
				(number "W20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LFE5UM5G-85F-8BG756x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 24.13 16.51 0)
		)
		(property "Value" "LFE5UM5G-85F-8BG756x"
			(at 24.13 13.97 0)
		)
		(property "Footprint" "Package_BGA:Lattice_caBGA-756_27x27mm_Layout32x32_P0.8mm"
			(at 11.43 72.39 0)
		)
		(property "Datasheet" "https://www.latticesemi.com/view_document?document_id=50461"
			(at 11.43 72.39 0)
		)
		(property "Description" "ECP5-5G FPGA, 84K LUTs, 1.2V, 5Gbps SERDES, BGA-756"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Lattice*caBGA*27x27mm*Layout32x32*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "LFE5UM5G-85F-8BG756x_1_1"
			(pin power_in line
				(at -22.86 15.24 270)
				(length 5.08)
				(name "VCCHTX0_D0CH0")
				(number "AC13")
			)
			(pin no_connect line
				(at -22.86 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G15")
			)
			(pin power_in line
				(at -20.32 15.24 270)
				(length 5.08)
				(name "VCCHRX0_D0CH0")
				(number "AC14")
			)
			(pin no_connect line
				(at -20.32 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G14")
			)
			(pin power_in line
				(at -17.78 15.24 270)
				(length 5.08)
				(name "VCCHRX1_D0CH1")
				(number "AC15")
			)
			(pin no_connect line
				(at -17.78 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "AG24")
			)
			(pin power_in line
				(at -15.24 15.24 270)
				(length 5.08)
				(name "VCCHTX1_D0CH1")
				(number "AC16")
			)
			(pin no_connect line
				(at -15.24 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G23")
			)
			(pin power_in line
				(at -12.7 15.24 270)
				(length 5.08)
				(name "VCCHTX0_D1CH0")
				(number "AC17")
			)
			(pin no_connect line
				(at -12.7 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G22")
			)
			(pin power_in line
				(at -10.16 15.24 270)
				(length 5.08)
				(name "VCCHRX0_D1CH0")
				(number "AC18")
			)
			(pin no_connect line
				(at -10.16 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G19")
			)
			(pin power_in line
				(at -7.62 15.24 270)
				(length 5.08)
				(name "VCCHRX1_D1CH1")
				(number "AC19")
			)
			(pin no_connect line
				(at -7.62 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G18")
			)
			(pin power_in line
				(at -5.08 15.24 270)
				(length 5.08)
				(name "VCCHTX1_D1CH1")
				(number "AC20")
			)
			(pin no_connect line
				(at -5.08 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G17")
			)
			(pin no_connect line
				(at -2.54 10.16 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G9")
			)
			(pin no_connect line
				(at -2.54 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G16")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "AA12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "AA13")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VCC")
				(number "AA14")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "AA15")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "AA16")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "AA17")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "AA18")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "AA19")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "AA20")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "AA21")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M13")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M14")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M15")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M16")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M17")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M18")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M19")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M20")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "M21")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "N12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "N21")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "P12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "P21")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "R12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "R21")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "T12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "T21")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "U12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "U21")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "V12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "V21")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "W12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "W21")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "Y12")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCC")
				(number "Y21")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AA11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AA22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB21")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AB22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AC12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AC21")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD28")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD31")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AD5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AF11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AF12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AF14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AF15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AF16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AF17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AF19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AF20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AF23")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AG11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AG14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AG15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AG16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AG17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AG20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AG23")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH23")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH24")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH25")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH26")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH29")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH31")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AH8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ23")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ26")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AJ8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AK11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AK14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AK17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AK20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AK23")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AK26")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AK7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AK8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL21")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL23")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL24")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL26")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL29")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL31")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AL9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AM26")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "AM7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B24")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B28")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "B31")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "B9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E24")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E28")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E31")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "E9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J28")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J31")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "J5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "K23")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L12")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L21")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "L23")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "M22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N28")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N31")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "N5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "P22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R28")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R31")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "R5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "T22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "U22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V28")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V31")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "V5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "W22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y11")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y14")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y19")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "Y31")
			)
			(pin no_connect line
				(at 2.54 10.16 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "E7")
			)
			(pin no_connect line
				(at 2.54 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G11")
			)
			(pin passive line
				(at 5.08 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUXA0")
				(number "AJ15")
			)
			(pin power_in line
				(at 5.08 15.24 270)
				(length 5.08)
				(name "VCCAUXA0")
				(number "AJ16")
			)
			(pin no_connect line
				(at 5.08 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "AC29")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUXA1")
				(number "AJ24")
			)
			(pin power_in line
				(at 7.62 15.24 270)
				(length 5.08)
				(name "VCCAUXA1")
				(number "AJ25")
			)
			(pin no_connect line
				(at 7.62 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "L28")
			)
			(pin no_connect line
				(at 10.16 10.16 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G24")
			)
			(pin no_connect line
				(at 10.16 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "W27")
			)
			(pin passive line
				(at 12.7 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUX")
				(number "AC11")
			)
			(pin passive line
				(at 12.7 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUX")
				(number "AC22")
			)
			(pin passive line
				(at 12.7 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUX")
				(number "K13")
			)
			(pin passive line
				(at 12.7 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUX")
				(number "K20")
			)
			(pin passive line
				(at 12.7 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUX")
				(number "N10")
			)
			(pin power_in line
				(at 12.7 15.24 270)
				(length 5.08)
				(name "VCCAUX")
				(number "N23")
			)
			(pin passive line
				(at 12.7 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUX")
				(number "Y10")
			)
			(pin passive line
				(at 12.7 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCAUX")
				(number "Y23")
			)
			(pin no_connect line
				(at 12.7 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "H29")
			)
			(pin no_connect line
				(at 15.24 10.16 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "E26")
			)
			(pin no_connect line
				(at 15.24 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "V30")
			)
			(pin passive line
				(at 17.78 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCA0")
				(number "AG12")
			)
			(pin passive line
				(at 17.78 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCA0")
				(number "AG9")
			)
			(pin passive line
				(at 17.78 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCA0")
				(number "AH12")
			)
			(pin passive line
				(at 17.78 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCA0")
				(number "AH9")
			)
			(pin passive line
				(at 17.78 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCA0")
				(number "AJ10")
			)
			(pin passive line
				(at 17.78 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCA0")
				(number "AJ12")
			)
			(pin power_in line
				(at 17.78 15.24 270)
				(length 5.08)
				(name "VCCA0")
				(number "AJ13")
			)
			(pin passive line
				(at 17.78 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCA0")
				(number "AJ9")
			)
			(pin no_connect line
				(at 17.78 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "AG31")
			)
			(pin power_in line
				(at 20.32 15.24 270)
				(length 5.08)
				(name "VCCA1")
				(number "AF22")
			)
			(pin passive line
				(at 20.32 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCA1")
				(number "AG19")
			)
			(pin passive line
				(at 20.32 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCA1")
				(number "AG22")
			)
			(pin passive line
				(at 20.32 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCA1")
				(number "AH19")
			)
			(pin passive line
				(at 20.32 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCA1")
				(number "AH22")
			)
			(pin passive line
				(at 20.32 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCA1")
				(number "AJ18")
			)
			(pin passive line
				(at 20.32 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCA1")
				(number "AJ19")
			)
			(pin passive line
				(at 20.32 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCA1")
				(number "AJ21")
			)
			(pin passive line
				(at 20.32 15.24 270)
				(length 5.08)
				(hide yes)
				(name "VCCA1")
				(number "AJ22")
			)
			(pin no_connect line
				(at 20.32 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "G10")
			)
			(pin no_connect line
				(at 22.86 10.16 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "AE7")
			)
			(pin no_connect line
				(at 22.86 -10.16 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "AE26")
			)
		)
		(symbol "LFE5UM5G-85F-8BG756x_2_1"
			(pin bidirectional line
				(at -10.16 66.04 0)
				(length 5.08)
				(name "PT4A")
				(number "B3")
			)
			(pin bidirectional line
				(at -10.16 63.5 0)
				(length 5.08)
				(name "PT4B")
				(number "B4")
			)
			(pin bidirectional line
				(at -10.16 60.96 0)
				(length 5.08)
				(name "PT6A")
				(number "A2")
			)
			(pin bidirectional line
				(at -10.16 58.42 0)
				(length 5.08)
				(name "PT6B")
				(number "A3")
			)
			(pin bidirectional line
				(at -10.16 55.88 0)
				(length 5.08)
				(name "PT9A")
				(number "A4")
			)
			(pin bidirectional line
				(at -10.16 53.34 0)
				(length 5.08)
				(name "PT9B")
				(number "A5")
			)
			(pin bidirectional line
				(at -10.16 50.8 0)
				(length 5.08)
				(name "PT11A")
				(number "D7")
			)
			(pin bidirectional line
				(at -10.16 48.26 0)
				(length 5.08)
				(name "PT11B")
				(number "C7")
			)
			(pin bidirectional line
				(at -10.16 45.72 0)
				(length 5.08)
				(name "PT13A")
				(number "B7")
			)
			(pin bidirectional line
				(at -10.16 43.18 0)
				(length 5.08)
				(name "PT13B")
				(number "A7")
			)
			(pin bidirectional line
				(at -10.16 40.64 0)
				(length 5.08)
				(name "PT15A")
				(number "F8")
			)
			(pin bidirectional line
				(at -10.16 38.1 0)
				(length 5.08)
				(name "PT15B")
				(number "E8")
			)
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PT18A")
				(number "D8")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PT18B")
				(number "C8")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PT20A")
				(number "B8")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PT20B")
				(number "A8")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PT22A")
				(number "F9")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PT22B")
				(number "D9")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PT24A")
				(number "C9")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PT24B")
				(number "A9")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PT27A")
				(number "F10")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PT27B")
				(number "E10")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PT29A")
				(number "D10")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PT29B")
				(number "C10")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PT31A")
				(number "B10")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PT31B")
				(number "A10")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PT33A")
				(number "F11")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PT33B")
				(number "E11")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PT36A")
				(number "D11")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PT36B")
				(number "C11")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PT38A")
				(number "B11")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PT38B")
				(number "A11")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PT40A")
				(number "F13")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PT40B")
				(number "D13")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PT42A")
				(number "C13")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PT42B")
				(number "A13")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PT45A")
				(number "F14")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PT45B")
				(number "E14")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PT47A")
				(number "D14")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PT47B")
				(number "C14")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PT49A")
				(number "B14")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PT49B")
				(number "A14")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PT51A")
				(number "F15")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PT51B")
				(number "D15")
			)
			(pin bidirectional line
				(at -10.16 -45.72 0)
				(length 5.08)
				(name "PT54A")
				(number "C15")
			)
			(pin bidirectional line
				(at -10.16 -48.26 0)
				(length 5.08)
				(name "PT54B")
				(number "A15")
			)
			(pin bidirectional line
				(at -10.16 -50.8 0)
				(length 5.08)
				(name "PT56A")
				(number "F16")
			)
			(pin bidirectional line
				(at -10.16 -53.34 0)
				(length 5.08)
				(name "PT56B")
				(number "E16")
			)
			(pin bidirectional line
				(at -10.16 -55.88 0)
				(length 5.08)
				(name "PT58A")
				(number "D16")
			)
			(pin bidirectional line
				(at -10.16 -58.42 0)
				(length 5.08)
				(name "PT58B")
				(number "C16")
			)
			(pin bidirectional line
				(at -10.16 -60.96 0)
				(length 5.08)
				(name "PT60A")
				(number "B16")
			)
			(pin bidirectional line
				(at -10.16 -63.5 0)
				(length 5.08)
				(name "PT60B")
				(number "A16")
			)
			(pin bidirectional line
				(at -10.16 -66.04 0)
				(length 5.08)
				(name "PT63A")
				(number "A17")
			)
			(pin bidirectional line
				(at -10.16 -68.58 0)
				(length 5.08)
				(name "PT63B")
				(number "B17")
			)
			(pin bidirectional line
				(at -10.16 -71.12 0)
				(length 5.08)
				(name "PT65A")
				(number "C17")
			)
			(pin bidirectional line
				(at -10.16 -73.66 0)
				(length 5.08)
				(name "PT65B")
				(number "D17")
			)
			(pin passive line
				(at 0 81.28 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO0")
				(number "K12")
			)
			(pin passive line
				(at 0 81.28 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO0")
				(number "K14")
			)
			(pin passive line
				(at 0 81.28 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO0")
				(number "K15")
			)
			(pin power_in line
				(at 0 81.28 270)
				(length 5.08)
				(name "VCCIO0")
				(number "K16")
			)
			(pin no_connect line
				(at 2.54 76.2 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "W6")
			)
		)
		(symbol "LFE5UM5G-85F-8BG756x_3_1"
			(pin bidirectional line
				(at -10.16 55.88 0)
				(length 5.08)
				(name "PT69A")
				(number "E17")
			)
			(pin bidirectional line
				(at -10.16 53.34 0)
				(length 5.08)
				(name "PT69B")
				(number "F17")
			)
			(pin bidirectional line
				(at -10.16 50.8 0)
				(length 5.08)
				(name "PT71A")
				(number "A18")
			)
			(pin bidirectional line
				(at -10.16 48.26 0)
				(length 5.08)
				(name "PT71B")
				(number "C18")
			)
			(pin bidirectional line
				(at -10.16 45.72 0)
				(length 5.08)
				(name "PT74A")
				(number "D18")
			)
			(pin bidirectional line
				(at -10.16 43.18 0)
				(length 5.08)
				(name "PT74B")
				(number "F18")
			)
			(pin bidirectional line
				(at -10.16 40.64 0)
				(length 5.08)
				(name "PT76A")
				(number "A19")
			)
			(pin bidirectional line
				(at -10.16 38.1 0)
				(length 5.08)
				(name "PT76B")
				(number "B19")
			)
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PT78A")
				(number "C19")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PT78B")
				(number "D19")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PT80A")
				(number "E19")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PT80B")
				(number "F19")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PT83A")
				(number "A20")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PT83B")
				(number "C20")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PT85A")
				(number "D20")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PT85B")
				(number "F20")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PT87A")
				(number "A22")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PT87B")
				(number "B22")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PT89A")
				(number "C22")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PT89B")
				(number "D22")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PT92A")
				(number "E22")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PT92B")
				(number "F22")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PT94A")
				(number "A23")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PT94B")
				(number "B23")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PT96A")
				(number "C23")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PT96B")
				(number "D23")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PT98A")
				(number "E23")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PT98B")
				(number "F23")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PT101A")
				(number "A24")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PT101B")
				(number "C24")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PT103A")
				(number "D24")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PT103B")
				(number "F24")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PT105A")
				(number "A25")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PT105B")
				(number "B25")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PT107A")
				(number "C25")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PT107B")
				(number "D25")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PT110A")
				(number "E25")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PT110B")
				(number "F25")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PT112A")
				(number "A26")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PT112B")
				(number "B26")
			)
			(pin bidirectional line
				(at -10.16 -45.72 0)
				(length 5.08)
				(name "PT114A")
				(number "C26")
			)
			(pin bidirectional line
				(at -10.16 -48.26 0)
				(length 5.08)
				(name "PT114B")
				(number "D26")
			)
			(pin bidirectional line
				(at -10.16 -50.8 0)
				(length 5.08)
				(name "PT116A")
				(number "A28")
			)
			(pin bidirectional line
				(at -10.16 -53.34 0)
				(length 5.08)
				(name "PT116B")
				(number "A29")
			)
			(pin bidirectional line
				(at -10.16 -55.88 0)
				(length 5.08)
				(name "PT119A")
				(number "A30")
			)
			(pin bidirectional line
				(at -10.16 -58.42 0)
				(length 5.08)
				(name "PT119B")
				(number "A31")
			)
			(pin bidirectional line
				(at -10.16 -60.96 0)
				(length 5.08)
				(name "PT121A")
				(number "B29")
			)
			(pin bidirectional line
				(at -10.16 -63.5 0)
				(length 5.08)
				(name "PT121B")
				(number "B30")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO1")
				(number "K17")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO1")
				(number "K18")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO1")
				(number "K19")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VCCIO1")
				(number "K21")
			)
			(pin no_connect line
				(at 2.54 66.04 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "L5")
			)
		)
		(symbol "LFE5UM5G-85F-8BG756x_4_1"
			(pin bidirectional line
				(at -10.16 55.88 0)
				(length 5.08)
				(name "PR11A")
				(number "C28")
			)
			(pin bidirectional line
				(at -10.16 53.34 0)
				(length 5.08)
				(name "PR11B")
				(number "D28")
			)
			(pin bidirectional line
				(at -10.16 50.8 0)
				(length 5.08)
				(name "PR11C")
				(number "C29")
			)
			(pin bidirectional line
				(at -10.16 48.26 0)
				(length 5.08)
				(name "PR11D")
				(number "C30")
			)
			(pin bidirectional line
				(at -10.16 45.72 0)
				(length 5.08)
				(name "PR14A")
				(number "D29")
			)
			(pin bidirectional line
				(at -10.16 43.18 0)
				(length 5.08)
				(name "PR14B")
				(number "E29")
			)
			(pin bidirectional line
				(at -10.16 40.64 0)
				(length 5.08)
				(name "PR14C")
				(number "F29")
			)
			(pin bidirectional line
				(at -10.16 38.1 0)
				(length 5.08)
				(name "PR14D")
				(number "F28")
			)
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PR17A")
				(number "B32")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PR17B")
				(number "C31")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PR17C")
				(number "D30")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PR17D")
				(number "D31")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PR20A")
				(number "F30")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PR20B")
				(number "E30")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PR20C")
				(number "C32")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PR20D")
				(number "D32")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PR23A")
				(number "F31")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PR23B")
				(number "E32")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PR23C")
				(number "F32")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PR23D")
				(number "H32")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PR26A")
				(number "H31")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PR26B")
				(number "H30")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PR26C")
				(number "J30")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PR26D")
				(number "K30")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PR29A")
				(number "K31")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PR29B")
				(number "J32")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PR29C")
				(number "K32")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PR29D")
				(number "L32")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PR32A")
				(number "L31")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PR32B")
				(number "L30")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PR32C")
				(number "J29")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PR32D")
				(number "K29")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PR35A")
				(number "H27")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PR35B")
				(number "H28")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PR35C")
				(number "J26")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PR35D")
				(number "J27")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PR38A")
				(number "K27")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PR38B")
				(number "K26")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PR38C")
				(number "K28")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PR38D")
				(number "L29")
			)
			(pin bidirectional line
				(at -10.16 -45.72 0)
				(length 5.08)
				(name "PR41A")
				(number "N30")
			)
			(pin bidirectional line
				(at -10.16 -48.26 0)
				(length 5.08)
				(name "PR41B")
				(number "N29")
			)
			(pin bidirectional line
				(at -10.16 -50.8 0)
				(length 5.08)
				(name "PR41C")
				(number "L26")
			)
			(pin bidirectional line
				(at -10.16 -53.34 0)
				(length 5.08)
				(name "PR41D")
				(number "L27")
			)
			(pin bidirectional line
				(at -10.16 -55.88 0)
				(length 5.08)
				(name "PR44A")
				(number "N27")
			)
			(pin bidirectional line
				(at -10.16 -58.42 0)
				(length 5.08)
				(name "PR44B")
				(number "N26")
			)
			(pin bidirectional line
				(at -10.16 -60.96 0)
				(length 5.08)
				(name "PR44C")
				(number "P27")
			)
			(pin bidirectional line
				(at -10.16 -63.5 0)
				(length 5.08)
				(name "PR44D")
				(number "P26")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VCCIO2")
				(number "M23")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO2")
				(number "P23")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO2")
				(number "R23")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO2")
				(number "T23")
			)
			(pin no_connect line
				(at 2.54 66.04 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "H4")
			)
		)
		(symbol "LFE5UM5G-85F-8BG756x_5_1"
			(pin bidirectional line
				(at -10.16 76.2 0)
				(length 5.08)
				(name "PR47A")
				(number "P28")
			)
			(pin bidirectional line
				(at -10.16 73.66 0)
				(length 5.08)
				(name "PR47B")
				(number "P29")
			)
			(pin bidirectional line
				(at -10.16 71.12 0)
				(length 5.08)
				(name "PR47C")
				(number "R26")
			)
			(pin bidirectional line
				(at -10.16 68.58 0)
				(length 5.08)
				(name "PR47D")
				(number "T26")
			)
			(pin bidirectional line
				(at -10.16 66.04 0)
				(length 5.08)
				(name "PR50A")
				(number "R27")
			)
			(pin bidirectional line
				(at -10.16 63.5 0)
				(length 5.08)
				(name "PR50B")
				(number "T27")
			)
			(pin bidirectional line
				(at -10.16 60.96 0)
				(length 5.08)
				(name "PR50C")
				(number "U27")
			)
			(pin bidirectional line
				(at -10.16 58.42 0)
				(length 5.08)
				(name "PR50D")
				(number "U26")
			)
			(pin bidirectional line
				(at -10.16 55.88 0)
				(length 5.08)
				(name "PR53A")
				(number "R29")
			)
			(pin bidirectional line
				(at -10.16 53.34 0)
				(length 5.08)
				(name "PR53B")
				(number "T28")
			)
			(pin bidirectional line
				(at -10.16 50.8 0)
				(length 5.08)
				(name "PR53C")
				(number "T29")
			)
			(pin bidirectional line
				(at -10.16 48.26 0)
				(length 5.08)
				(name "PR53D")
				(number "U28")
			)
			(pin bidirectional line
				(at -10.16 45.72 0)
				(length 5.08)
				(name "PR56A")
				(number "U29")
			)
			(pin bidirectional line
				(at -10.16 43.18 0)
				(length 5.08)
				(name "PR56B")
				(number "V29")
			)
			(pin bidirectional line
				(at -10.16 40.64 0)
				(length 5.08)
				(name "PR56C")
				(number "V27")
			)
			(pin bidirectional line
				(at -10.16 38.1 0)
				(length 5.08)
				(name "PR56D")
				(number "V26")
			)
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PR59A")
				(number "P31")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PR59B")
				(number "P30")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PR59C")
				(number "R30")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PR59D")
				(number "T30")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PR62A")
				(number "N32")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PR62B")
				(number "P32")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PR62C")
				(number "U31")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PR62D")
				(number "U30")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PR65A")
				(number "R32")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PR65B")
				(number "T31")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PR65C")
				(number "W30")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PR65D")
				(number "Y30")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PR68A")
				(number "T32")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PR68B")
				(number "U32")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PR68C")
				(number "V32")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PR68D")
				(number "W32")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PR71A")
				(number "Y26")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PR71B")
				(number "Y27")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PR71C")
				(number "Y28")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PR71D")
				(number "W28")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PR74A")
				(number "Y29")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PR74B")
				(number "W29")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PR74C")
				(number "AB26")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PR74D")
				(number "AC27")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PR77A")
				(number "AB28")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PR77B")
				(number "AB27")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PR77C")
				(number "AC26")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PR77D")
				(number "AD26")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PR80A")
				(number "AD27")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PR80B")
				(number "AE27")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PR80C")
				(number "AE28")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PR80D")
				(number "AE29")
			)
			(pin bidirectional line
				(at -10.16 -45.72 0)
				(length 5.08)
				(name "PR83A")
				(number "AB30")
			)
			(pin bidirectional line
				(at -10.16 -48.26 0)
				(length 5.08)
				(name "PR83B")
				(number "AB29")
			)
			(pin bidirectional line
				(at -10.16 -50.8 0)
				(length 5.08)
				(name "PR83C")
				(number "AC28")
			)
			(pin bidirectional line
				(at -10.16 -53.34 0)
				(length 5.08)
				(name "PR83D")
				(number "AD29")
			)
			(pin bidirectional line
				(at -10.16 -55.88 0)
				(length 5.08)
				(name "PR86A")
				(number "W31")
			)
			(pin bidirectional line
				(at -10.16 -58.42 0)
				(length 5.08)
				(name "PR86B")
				(number "Y32")
			)
			(pin bidirectional line
				(at -10.16 -60.96 0)
				(length 5.08)
				(name "PR86C")
				(number "AD30")
			)
			(pin bidirectional line
				(at -10.16 -63.5 0)
				(length 5.08)
				(name "PR86D")
				(number "AE30")
			)
			(pin bidirectional line
				(at -10.16 -66.04 0)
				(length 5.08)
				(name "PR89A")
				(number "AC30")
			)
			(pin bidirectional line
				(at -10.16 -68.58 0)
				(length 5.08)
				(name "PR89B")
				(number "AB31")
			)
			(pin bidirectional line
				(at -10.16 -71.12 0)
				(length 5.08)
				(name "PR89C")
				(number "AC31")
			)
			(pin bidirectional line
				(at -10.16 -73.66 0)
				(length 5.08)
				(name "PR89D")
				(number "AE31")
			)
			(pin bidirectional line
				(at -10.16 -76.2 0)
				(length 5.08)
				(name "PR92A")
				(number "AB32")
			)
			(pin bidirectional line
				(at -10.16 -78.74 0)
				(length 5.08)
				(name "PR92B")
				(number "AC32")
			)
			(pin bidirectional line
				(at -10.16 -81.28 0)
				(length 5.08)
				(name "PR92C")
				(number "AD32")
			)
			(pin bidirectional line
				(at -10.16 -83.82 0)
				(length 5.08)
				(name "PR92D")
				(number "AE32")
			)
			(pin passive line
				(at 0 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO3")
				(number "AA23")
			)
			(pin power_in line
				(at 0 91.44 270)
				(length 5.08)
				(name "VCCIO3")
				(number "U23")
			)
			(pin passive line
				(at 0 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO3")
				(number "V23")
			)
			(pin passive line
				(at 0 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO3")
				(number "W23")
			)
			(pin no_connect line
				(at 2.54 86.36 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "AC4")
			)
		)
		(symbol "LFE5UM5G-85F-8BG756x_6_1"
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PB96A")
				(number "AM28")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PB96B")
				(number "AM29")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PB98A")
				(number "AL28")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PB98B")
				(number "AK28")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PB101A")
				(number "AK32")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PB101B")
				(number "AJ32")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PB103A")
				(number "AM30")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PB103B")
				(number "AL30")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PB105A")
				(number "AK31")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PB105B")
				(number "AJ31")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PB107A")
				(number "AM31")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PB107B")
				(number "AL32")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PB110A")
				(number "AG28")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PB110B")
				(number "AG29")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PB112A")
				(number "AJ28")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PB112B")
				(number "AH28")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PB114A")
				(number "AH30")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PB114B")
				(number "AG30")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PB116A")
				(number "AK29")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PB116B")
				(number "AK30")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PB119A")
				(number "AH32")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PB119B")
				(number "AG32")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PB121A")
				(number "AJ29")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PB121B")
				(number "AJ30")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 5.08)
				(name "VCCIO4")
				(number "AB23")
			)
			(pin passive line
				(at 0 40.64 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO4")
				(number "AC23")
			)
			(pin no_connect line
				(at 2.54 35.56 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "V3")
			)
		)
		(symbol "LFE5UM5G-85F-8BG756x_7_1"
			(pin bidirectional line
				(at -10.16 76.2 0)
				(length 5.08)
				(name "PL47A")
				(number "P5")
			)
			(pin bidirectional line
				(at -10.16 73.66 0)
				(length 5.08)
				(name "PL47B")
				(number "P4")
			)
			(pin bidirectional line
				(at -10.16 71.12 0)
				(length 5.08)
				(name "PL47C")
				(number "R7")
			)
			(pin bidirectional line
				(at -10.16 68.58 0)
				(length 5.08)
				(name "PL47D")
				(number "T7")
			)
			(pin bidirectional line
				(at -10.16 66.04 0)
				(length 5.08)
				(name "PL50A")
				(number "R6")
			)
			(pin bidirectional line
				(at -10.16 63.5 0)
				(length 5.08)
				(name "PL50B")
				(number "T6")
			)
			(pin bidirectional line
				(at -10.16 60.96 0)
				(length 5.08)
				(name "PL50C")
				(number "U6")
			)
			(pin bidirectional line
				(at -10.16 58.42 0)
				(length 5.08)
				(name "PL50D")
				(number "U7")
			)
			(pin bidirectional line
				(at -10.16 55.88 0)
				(length 5.08)
				(name "PL53A")
				(number "R4")
			)
			(pin bidirectional line
				(at -10.16 53.34 0)
				(length 5.08)
				(name "PL53B")
				(number "T5")
			)
			(pin bidirectional line
				(at -10.16 50.8 0)
				(length 5.08)
				(name "PL53C")
				(number "T4")
			)
			(pin bidirectional line
				(at -10.16 48.26 0)
				(length 5.08)
				(name "PL53D")
				(number "U5")
			)
			(pin bidirectional line
				(at -10.16 45.72 0)
				(length 5.08)
				(name "PL56A")
				(number "U4")
			)
			(pin bidirectional line
				(at -10.16 43.18 0)
				(length 5.08)
				(name "PL56B")
				(number "V4")
			)
			(pin bidirectional line
				(at -10.16 40.64 0)
				(length 5.08)
				(name "PL56C")
				(number "V6")
			)
			(pin bidirectional line
				(at -10.16 38.1 0)
				(length 5.08)
				(name "PL56D")
				(number "V7")
			)
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PL59A")
				(number "P2")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PL59B")
				(number "P3")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PL59C")
				(number "R3")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PL59D")
				(number "T3")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PL62A")
				(number "N1")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PL62B")
				(number "P1")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PL62C")
				(number "U2")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PL62D")
				(number "U3")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PL65A")
				(number "R1")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PL65B")
				(number "T2")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PL65C")
				(number "W3")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PL65D")
				(number "Y3")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PL68A")
				(number "T1")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PL68B")
				(number "U1")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PL68C")
				(number "V1")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PL68D")
				(number "W1")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PL71A")
				(number "Y7")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PL71B")
				(number "Y6")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PL71C")
				(number "Y5")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PL71D")
				(number "W5")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PL74A")
				(number "Y4")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PL74B")
				(number "W4")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PL74C")
				(number "AB7")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PL74D")
				(number "AC6")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PL77A")
				(number "AB5")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PL77B")
				(number "AB6")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PL77C")
				(number "AC7")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PL77D")
				(number "AD7")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PL80A")
				(number "AD6")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PL80B")
				(number "AE6")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PL80C")
				(number "AE5")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PL80D")
				(number "AE4")
			)
			(pin bidirectional line
				(at -10.16 -45.72 0)
				(length 5.08)
				(name "PL83A")
				(number "AB3")
			)
			(pin bidirectional line
				(at -10.16 -48.26 0)
				(length 5.08)
				(name "PL83B")
				(number "AB4")
			)
			(pin bidirectional line
				(at -10.16 -50.8 0)
				(length 5.08)
				(name "PL83C")
				(number "AC5")
			)
			(pin bidirectional line
				(at -10.16 -53.34 0)
				(length 5.08)
				(name "PL83D")
				(number "AD4")
			)
			(pin bidirectional line
				(at -10.16 -55.88 0)
				(length 5.08)
				(name "PL86A")
				(number "W2")
			)
			(pin bidirectional line
				(at -10.16 -58.42 0)
				(length 5.08)
				(name "PL86B")
				(number "Y1")
			)
			(pin bidirectional line
				(at -10.16 -60.96 0)
				(length 5.08)
				(name "PL86C")
				(number "AD3")
			)
			(pin bidirectional line
				(at -10.16 -63.5 0)
				(length 5.08)
				(name "PL86D")
				(number "AE3")
			)
			(pin bidirectional line
				(at -10.16 -66.04 0)
				(length 5.08)
				(name "PL89A")
				(number "AC3")
			)
			(pin bidirectional line
				(at -10.16 -68.58 0)
				(length 5.08)
				(name "PL89B")
				(number "AB2")
			)
			(pin bidirectional line
				(at -10.16 -71.12 0)
				(length 5.08)
				(name "PL89C")
				(number "AC2")
			)
			(pin bidirectional line
				(at -10.16 -73.66 0)
				(length 5.08)
				(name "PL89D")
				(number "AE2")
			)
			(pin bidirectional line
				(at -10.16 -76.2 0)
				(length 5.08)
				(name "PL92A")
				(number "AB1")
			)
			(pin bidirectional line
				(at -10.16 -78.74 0)
				(length 5.08)
				(name "PL92B")
				(number "AC1")
			)
			(pin bidirectional line
				(at -10.16 -81.28 0)
				(length 5.08)
				(name "PL92C")
				(number "AD1")
			)
			(pin bidirectional line
				(at -10.16 -83.82 0)
				(length 5.08)
				(name "PL92D")
				(number "AE1")
			)
			(pin passive line
				(at 0 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO6")
				(number "AA10")
			)
			(pin power_in line
				(at 0 91.44 270)
				(length 5.08)
				(name "VCCIO6")
				(number "U10")
			)
			(pin passive line
				(at 0 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO6")
				(number "V10")
			)
			(pin passive line
				(at 0 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO6")
				(number "W10")
			)
			(pin no_connect line
				(at 2.54 86.36 270)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "AG2")
			)
		)
		(symbol "LFE5UM5G-85F-8BG756x_8_1"
			(pin bidirectional line
				(at -10.16 55.88 0)
				(length 5.08)
				(name "PL11A")
				(number "C5")
			)
			(pin bidirectional line
				(at -10.16 53.34 0)
				(length 5.08)
				(name "PL11B")
				(number "D5")
			)
			(pin bidirectional line
				(at -10.16 50.8 0)
				(length 5.08)
				(name "PL11C")
				(number "C4")
			)
			(pin bidirectional line
				(at -10.16 48.26 0)
				(length 5.08)
				(name "PL11D")
				(number "C3")
			)
			(pin bidirectional line
				(at -10.16 45.72 0)
				(length 5.08)
				(name "PL14A")
				(number "D4")
			)
			(pin bidirectional line
				(at -10.16 43.18 0)
				(length 5.08)
				(name "PL14B")
				(number "E4")
			)
			(pin bidirectional line
				(at -10.16 40.64 0)
				(length 5.08)
				(name "PL14C")
				(number "F4")
			)
			(pin bidirectional line
				(at -10.16 38.1 0)
				(length 5.08)
				(name "PL14D")
				(number "F5")
			)
			(pin bidirectional line
				(at -10.16 35.56 0)
				(length 5.08)
				(name "PL17A")
				(number "B1")
			)
			(pin bidirectional line
				(at -10.16 33.02 0)
				(length 5.08)
				(name "PL17B")
				(number "C2")
			)
			(pin bidirectional line
				(at -10.16 30.48 0)
				(length 5.08)
				(name "PL17C")
				(number "D3")
			)
			(pin bidirectional line
				(at -10.16 27.94 0)
				(length 5.08)
				(name "PL17D")
				(number "D2")
			)
			(pin bidirectional line
				(at -10.16 25.4 0)
				(length 5.08)
				(name "PL20A")
				(number "F3")
			)
			(pin bidirectional line
				(at -10.16 22.86 0)
				(length 5.08)
				(name "PL20B")
				(number "E3")
			)
			(pin bidirectional line
				(at -10.16 20.32 0)
				(length 5.08)
				(name "PL20C")
				(number "C1")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 5.08)
				(name "PL20D")
				(number "D1")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 5.08)
				(name "PL23A")
				(number "F2")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PL23B")
				(number "E1")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PL23C")
				(number "F1")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PL23D")
				(number "H1")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PL26A")
				(number "H2")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PL26B")
				(number "H3")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PL26C")
				(number "J3")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PL26D")
				(number "K3")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PL29A")
				(number "K2")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PL29B")
				(number "J1")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PL29C")
				(number "K1")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PL29D")
				(number "L1")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PL32A")
				(number "L2")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PL32B")
				(number "L3")
			)
			(pin bidirectional line
				(at -10.16 -20.32 0)
				(length 5.08)
				(name "PL32C")
				(number "J4")
			)
			(pin bidirectional line
				(at -10.16 -22.86 0)
				(length 5.08)
				(name "PL32D")
				(number "K4")
			)
			(pin bidirectional line
				(at -10.16 -25.4 0)
				(length 5.08)
				(name "PL35A")
				(number "H6")
			)
			(pin bidirectional line
				(at -10.16 -27.94 0)
				(length 5.08)
				(name "PL35B")
				(number "H5")
			)
			(pin bidirectional line
				(at -10.16 -30.48 0)
				(length 5.08)
				(name "PL35C")
				(number "J7")
			)
			(pin bidirectional line
				(at -10.16 -33.02 0)
				(length 5.08)
				(name "PL35D")
				(number "J6")
			)
			(pin bidirectional line
				(at -10.16 -35.56 0)
				(length 5.08)
				(name "PL38A")
				(number "K6")
			)
			(pin bidirectional line
				(at -10.16 -38.1 0)
				(length 5.08)
				(name "PL38B")
				(number "K7")
			)
			(pin bidirectional line
				(at -10.16 -40.64 0)
				(length 5.08)
				(name "PL38C")
				(number "K5")
			)
			(pin bidirectional line
				(at -10.16 -43.18 0)
				(length 5.08)
				(name "PL38D")
				(number "L4")
			)
			(pin bidirectional line
				(at -10.16 -45.72 0)
				(length 5.08)
				(name "PL41A")
				(number "N3")
			)
			(pin bidirectional line
				(at -10.16 -48.26 0)
				(length 5.08)
				(name "PL41B")
				(number "N4")
			)
			(pin bidirectional line
				(at -10.16 -50.8 0)
				(length 5.08)
				(name "PL41C")
				(number "L7")
			)
			(pin bidirectional line
				(at -10.16 -53.34 0)
				(length 5.08)
				(name "PL41D")
				(number "L6")
			)
			(pin bidirectional line
				(at -10.16 -55.88 0)
				(length 5.08)
				(name "PL44A")
				(number "N6")
			)
			(pin bidirectional line
				(at -10.16 -58.42 0)
				(length 5.08)
				(name "PL44B")
				(number "N7")
			)
			(pin bidirectional line
				(at -10.16 -60.96 0)
				(length 5.08)
				(name "PL44C")
				(number "P6")
			)
			(pin bidirectional line
				(at -10.16 -63.5 0)
				(length 5.08)
				(name "PL44D")
				(number "P7")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VCCIO7")
				(number "M10")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO7")
				(number "P10")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO7")
				(number "R10")
			)
			(pin passive line
				(at 0 71.12 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO7")
				(number "T10")
			)
		)
		(symbol "LFE5UM5G-85F-8BG756x_9_1"
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 5.08)
				(name "PB4A")
				(number "AG1")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 5.08)
				(name "PB4B")
				(number "AH1")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "PB6A")
				(number "AJ1")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "PB6B")
				(number "AK1")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "PB9A")
				(number "AL1")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 5.08)
				(name "PB9B")
				(number "AM2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "PB11A")
				(number "AJ2")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "PB11B")
				(number "AK2")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "PB13A")
				(number "AG3")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 5.08)
				(name "PB13B")
				(number "AH3")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 5.08)
				(name "PB15A")
				(number "AJ3")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 5.08)
				(name "PB15B")
				(number "AK3")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 5.08)
				(name "PB18A")
				(number "AL3")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 5.08)
				(name "VCCIO8")
				(number "AB10")
			)
			(pin passive line
				(at 0 27.94 270)
				(length 5.08)
				(hide yes)
				(name "VCCIO8")
				(number "AC10")
			)
		)
		(symbol "LFE5UM5G-85F-8BG756x_10_1"
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "CCLK")
				(number "AM3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "~{PROGRAM}")
				(number "AH4")
			)
			(pin open_collector line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "~{INIT}")
				(number "AG4")
			)
			(pin open_collector line
				(at -15.24 0 0)
				(length 5.08)
				(name "DONE")
				(number "AJ4")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "CFG_0")
				(number "AM4")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 5.08)
				(name "CFG_1")
				(number "AL4")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "CFG_2")
				(number "AK4")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "AK15")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "AK16")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "AK24")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 5.08)
				(hide yes)
				(name "RESERVED")
				(number "AK25")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 5.08)
				(name "TDO")
				(number "AG5")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "TCK")
				(number "AK5")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "TDI")
				(number "AJ5")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "TMS")
				(number "AM5")
			)
		)
		(symbol "LFE5UM5G-85F-8BG756x_11_1"
			(pin output line
				(at -15.24 15.24 0)
				(length 5.08)
				(name "HDTXP0_D0CH0")
				(number "AK9")
			)
			(pin output line
				(at -15.24 12.7 0)
				(length 5.08)
				(name "HDTXN0_D0CH0")
				(number "AK10")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "HDRXP0_D0CH0")
				(number "AM8")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "HDRXN0_D0CH0")
				(number "AM9")
			)
			(pin output line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "HDTXP0_D0CH1")
				(number "AK12")
			)
			(pin output line
				(at -15.24 0 0)
				(length 5.08)
				(name "HDTXN0_D0CH1")
				(number "AK13")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "HDRXP0_D0CH1")
				(number "AM11")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "HDRXN0_D0CH1")
				(number "AM12")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "REFCLKP_D0")
				(number "AM14")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 5.08)
				(name "REFCLKN_D0")
				(number "AM15")
			)
		)
		(symbol "LFE5UM5G-85F-8BG756x_12_1"
			(pin output line
				(at -15.24 15.24 0)
				(length 5.08)
				(name "HDTXP0_D1CH0")
				(number "AK18")
			)
			(pin output line
				(at -15.24 12.7 0)
				(length 5.08)
				(name "HDTXN0_D1CH0")
				(number "AK19")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 5.08)
				(name "HDRXP0_D1CH0")
				(number "AM17")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "HDRXN0_D1CH0")
				(number "AM18")
			)
			(pin output line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "HDTXP0_D1CH1")
				(number "AK21")
			)
			(pin output line
				(at -15.24 0 0)
				(length 5.08)
				(name "HDTXN0_D1CH1")
				(number "AK22")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "HDRXP0_D1CH1")
				(number "AM20")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 5.08)
				(name "HDRXN0_D1CH1")
				(number "AM21")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 5.08)
				(name "REFCLKP_D1")
				(number "AM23")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 5.08)
				(name "REFCLKN_D1")
				(number "AM24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LFXP2-5E-5TN144"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "LFXP2-5E-5TN144"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_QFP:TQFP-144_20x20mm_P0.5mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.latticesemi.com/view_document?document_id=24635"
			(at 0 -10.16 0)
		)
		(property "Description" "FPGA, 5000 LUTs, 1.2V, TQFP-144"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA Lattice XP2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*20x20mm*"
			(at 0 0 0)
		)
		(symbol "LFXP2-5E-5TN144_1_0"
			(text "Bank 0"
				(at -5.08 33.02 0)
			)
			(text "Bank 1"
				(at 5.08 33.02 0)
			)
		)
		(symbol "LFXP2-5E-5TN144_1_1"
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "PT8A/ULC_GPLLT_IN_A")
				(number "144")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "PT7A/VREF1_0")
				(number "143")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "PT8B/ULC_GPLLC_IN_A")
				(number "142")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "PT7B/VREF2_0")
				(number "141")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "PT9A/ULC_GPLLT_FB_A")
				(number "138")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "PT9B/ULC_GPLLC_FB_A")
				(number "137")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "PT13A")
				(number "134")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "PT13B")
				(number "133")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "PT14A")
				(number "132")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "PT15A")
				(number "131")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "PT14B")
				(number "130")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "PT15B")
				(number "129")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "PT16A")
				(number "127")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "PT16B")
				(number "125")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "PT17A")
				(number "124")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "PT18A")
				(number "123")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "PT17B")
				(number "122")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "PT18B")
				(number "121")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "PT19A/PCLKT0_0")
				(number "120")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "PT19B/PCLKC0_0")
				(number "119")
			)
			(pin power_in line
				(at -17.78 40.64 270)
				(length 3.81)
				(name "VCCIO0")
				(number "128")
			)
			(pin power_in line
				(at -17.78 -40.64 90)
				(length 3.81)
				(name "GNDIO0")
				(number "126")
			)
			(pin power_in line
				(at -15.24 40.64 270)
				(length 3.81)
				(name "VCCIO0")
				(number "136")
			)
			(pin power_in line
				(at -15.24 -40.64 90)
				(length 3.81)
				(name "GNDIO0")
				(number "135")
			)
			(pin power_in line
				(at 17.78 40.64 270)
				(length 3.81)
				(name "VCCIO1")
				(number "112")
			)
			(pin power_in line
				(at 17.78 -40.64 90)
				(length 3.81)
				(name "GNDIO1")
				(number "111")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "PT20A/PCLKT1_0")
				(number "116")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "PT21A")
				(number "115")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "PT20B/PCLKC1_0")
				(number "114")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "PT21B")
				(number "113")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "PT28A/VREF1_1")
				(number "110")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "PT28B/VREF2_1")
				(number "109")
			)
		)
		(symbol "LFXP2-5E-5TN144_2_0"
			(text "Bank 2"
				(at -5.08 30.48 0)
			)
			(text "Bank 3"
				(at 5.08 30.48 0)
			)
		)
		(symbol "LFXP2-5E-5TN144_2_1"
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "PR2A/VREF1_2")
				(number "108")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "PR2B/VREF2_2")
				(number "107")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "PR5A")
				(number "104")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "PR5B")
				(number "103")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "PR6A")
				(number "102")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "PR7A")
				(number "101")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "PR6B")
				(number "100")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "PR7B")
				(number "99")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "PR8A")
				(number "98")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "PR8B")
				(number "96")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "PR9A")
				(number "94")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "PR10A")
				(number "93")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "PR9B")
				(number "92")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "PR10B")
				(number "91")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "PR11A")
				(number "90")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "PR11B")
				(number "89")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "PR12A/PCLKT2_0")
				(number "88")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "PR12B/PCLK2_0")
				(number "87")
			)
			(pin power_in line
				(at -17.78 38.1 270)
				(length 3.81)
				(name "VCCIO2")
				(number "95")
			)
			(pin power_in line
				(at -17.78 -38.1 90)
				(length 3.81)
				(name "GNDIO2")
				(number "97")
			)
			(pin power_in line
				(at -15.24 38.1 270)
				(length 3.81)
				(name "VCCIO2")
				(number "105")
			)
			(pin power_in line
				(at -15.24 -38.1 90)
				(length 3.81)
				(name "GNDIO2")
				(number "106")
			)
			(pin power_in line
				(at 17.78 38.1 270)
				(length 3.81)
				(name "VCCIO3")
				(number "76")
			)
			(pin power_in line
				(at 17.78 -38.1 90)
				(length 3.81)
				(name "GNDIO3")
				(number "75")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "PR14A/PCLKT3_0")
				(number "78")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "PR14B/PCLK3_0")
				(number "77")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "PR24B/VREF2_3")
				(number "74")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "PR24A/VREF1_3")
				(number "73")
			)
		)
		(symbol "LFXP2-5E-5TN144_3_0"
			(text "Bank 4"
				(at -5.08 30.48 0)
			)
			(text "Bank 5"
				(at 5.08 30.48 0)
			)
		)
		(symbol "LFXP2-5E-5TN144_3_1"
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "PB20A/PCLKT4_0")
				(number "61")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "PB20B/PCLKC4_0")
				(number "62")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "PB26A/LRC_GPLLT_IN_A")
				(number "65")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "PB26B/LRC_GPLLC_IN_A")
				(number "66")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "PB27A/LRC_GPLLT_FB_A")
				(number "69")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "PB28A/VREF1_4")
				(number "70")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "PB27B/LRC_GPLLC_FB_A")
				(number "71")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "PB28B/VREF2_4")
				(number "72")
			)
			(pin power_in line
				(at -17.78 38.1 270)
				(length 3.81)
				(name "VCCIO4")
				(number "63")
			)
			(pin power_in line
				(at -17.78 -38.1 90)
				(length 3.81)
				(name "GNDIO4")
				(number "64")
			)
			(pin power_in line
				(at 15.24 38.1 270)
				(length 3.81)
				(name "VCCIO5")
				(number "49")
			)
			(pin power_in line
				(at 15.24 -38.1 90)
				(length 3.81)
				(name "GNDIO5")
				(number "51")
			)
			(pin power_in line
				(at 17.78 38.1 270)
				(length 3.81)
				(name "VCCIO5")
				(number "42")
			)
			(pin power_in line
				(at 17.78 -38.1 90)
				(length 3.81)
				(name "GNDIO5")
				(number "41")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "PB8A")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "PB7A/VREF1_5")
				(number "38")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "PB8B")
				(number "39")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "PB7B/VREF2_5")
				(number "40")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "PB13B")
				(number "43")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "PB13A")
				(number "44")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "PB15A")
				(number "45")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "PB14A")
				(number "46")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "PB15B")
				(number "47")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "PB14B")
				(number "48")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "PB16A")
				(number "50")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "PB16B")
				(number "52")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "PB17A")
				(number "53")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "PB17B")
				(number "54")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "PB18A")
				(number "55")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "PB19A/PCLKT5_0")
				(number "56")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 3.81)
				(name "PB18B")
				(number "57")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "PB19B/PCLKC5_0")
				(number "58")
			)
		)
		(symbol "LFXP2-5E-5TN144_4_0"
			(text "Bank 6"
				(at -5.08 30.48 0)
			)
			(text "Bank 7"
				(at 5.08 30.48 0)
			)
		)
		(symbol "LFXP2-5E-5TN144_4_1"
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "PL15A")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "PL14A/PCLKT6_0")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "PL15B")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "PL14B/PCLKC6_0")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "PL16B")
				(number "31")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "PL16A")
				(number "32")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "PL25A/VREF1_6")
				(number "35")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "PL25B/VREF2_6")
				(number "36")
			)
			(pin power_in line
				(at -17.78 38.1 270)
				(length 3.81)
				(name "VCCIO6")
				(number "33")
			)
			(pin power_in line
				(at -17.78 -38.1 90)
				(length 3.81)
				(name "GNDIO6")
				(number "34")
			)
			(pin power_in line
				(at 15.24 38.1 270)
				(length 3.81)
				(name "VCCIO7")
				(number "14")
			)
			(pin power_in line
				(at 15.24 -38.1 90)
				(length 3.81)
				(name "GNDIO7")
				(number "12")
			)
			(pin power_in line
				(at 17.78 38.1 270)
				(length 3.81)
				(name "VCCIO7")
				(number "4")
			)
			(pin power_in line
				(at 17.78 -38.1 90)
				(length 3.81)
				(name "GNDIO7")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "PL2A/VREF1_7")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "PL2B/VREF2_7")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "PL5A")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "PL5B")
				(number "6")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "PL6A/PROGRAMN")
				(number "7")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "PL6B/DONE")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "PL7A/CFG1")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "PL7B")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "PL8A/CSSPISN")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "PL8B/CSSPIN")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "PL9A")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "PL10A/CCLK")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "PL9B")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "PL10B/SOSPI")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "PL11A/SISPI")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "PL11B/INITN")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 3.81)
				(name "PL12A/PCLKT7_0")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "PL12B/PCLKC7_0")
				(number "22")
			)
		)
		(symbol "LFXP2-5E-5TN144_5_1"
			(pin input line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "TOE")
				(number "25")
			)
			(pin input line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "CFG0")
				(number "26")
			)
			(pin power_in line
				(at -17.78 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "86")
			)
			(pin power_in line
				(at -12.7 20.32 270)
				(length 3.81)
				(name "VCCAUX")
				(number "117")
			)
			(pin power_in line
				(at -10.16 20.32 270)
				(length 3.81)
				(name "VCCAUX")
				(number "85")
			)
			(pin power_in line
				(at -7.62 20.32 270)
				(length 3.81)
				(name "VCCAUX")
				(number "60")
			)
			(pin power_in line
				(at -5.08 20.32 270)
				(length 3.81)
				(name "VCCAUX")
				(number "23")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 3.81)
				(name "VCC")
				(number "118")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VCC")
				(number "84")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 3.81)
				(name "VCC")
				(number "59")
			)
			(pin power_in line
				(at 5.08 20.32 270)
				(length 3.81)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 15.24 20.32 270)
				(length 3.81)
				(name "ULC_VCCPLL")
				(number "140")
			)
			(pin power_in line
				(at 15.24 -20.32 90)
				(length 3.81)
				(name "ULC_GNDPLL")
				(number "139")
			)
			(pin power_in line
				(at 17.78 20.32 270)
				(length 3.81)
				(name "LRC_VCCPLL")
				(number "67")
			)
			(pin power_in line
				(at 17.78 -20.32 90)
				(length 3.81)
				(name "LRC_GNDPLL")
				(number "68")
			)
		)
		(symbol "LFXP2-5E-5TN144_6_0"
			(text "Bank 8"
				(at 0 5.08 0)
			)
		)
		(symbol "LFXP2-5E-5TN144_6_1"
			(pin input line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "TCK")
				(number "81")
			)
			(pin input line
				(at -20.32 0 0)
				(length 3.81)
				(name "TDI")
				(number "80")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "TMS")
				(number "79")
			)
			(pin power_in line
				(at -7.62 12.7 270)
				(length 3.81)
				(name "VCCJ")
				(number "83")
			)
			(pin output line
				(at 20.32 0 180)
				(length 3.81)
				(name "TDO")
				(number "82")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ICE40HX4K-BG121"
		(extends "ICE40HX8K-BG121")
		(property "Reference" "U"
			(at 2.54 44.45 0)
		)
		(property "Value" "ICE40HX4K-BG121"
			(at 10.16 41.91 0)
		)
		(property "Footprint" "Package_BGA:BGA-121_9.0x9.0mm_Layout11x11_P0.8mm_Ball0.4mm_Pad0.35mm_NSMD"
			(at 0 -36.83 0)
		)
		(property "Datasheet" "http://www.latticesemi.com/Products/FPGAandCPLD/iCE40"
			(at -21.59 25.4 0)
		)
		(property "Description" "iCE40 HX FPGA, 3520 LUTs, 1.2V, BGA-121"
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*9.0x9.0mm*Layout11x11*P0.8mm*Ball0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "ICE5LP1K-SG48"
		(extends "ICE40UP5K-SG48ITR")
		(property "Reference" "U"
			(at -8.89 -29.21 0)
		)
		(property "Value" "ICE5LP1K-SG48"
			(at 0 -31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "http://www.latticesemi.com/Products/FPGAandCPLD/iCE40Ultra"
			(at -10.16 25.4 0)
		)
		(property "Description" "iCE40 Ultra FPGA, 1100 LUTs, 1.2V, 48-pin QFN"
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LFE5U-85F-6BG381x"
		(extends "LFE5U-85F-8BG381x")
		(property "Reference" "U"
			(at 24.13 16.51 0)
		)
		(property "Value" "LFE5U-85F-6BG381x"
			(at 24.13 13.97 0)
		)
		(property "Footprint" "Package_BGA:Lattice_caBGA-381_17x17mm_Layout20x20_P0.8mm"
			(at 11.43 72.39 0)
		)
		(property "Datasheet" "https://www.latticesemi.com/view_document?document_id=50461"
			(at 11.43 72.39 0)
		)
		(property "Description" "ECP5 FPGA, 84K LUTs, 1.2V, BGA-381"
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Lattice?caBGA*17x17mm*Layout20x20*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LFE5U-85F-6BG756x"
		(extends "LFE5U-85F-8BG756x")
		(property "Reference" "U"
			(at 24.13 16.51 0)
		)
		(property "Value" "LFE5U-85F-6BG756x"
			(at 24.13 13.97 0)
		)
		(property "Footprint" "Package_BGA:Lattice_caBGA-756_27x27mm_Layout32x32_P0.8mm"
			(at 11.43 72.39 0)
		)
		(property "Datasheet" "https://www.latticesemi.com/view_document?document_id=50461"
			(at 11.43 72.39 0)
		)
		(property "Description" "ECP5 FPGA, 84K LUTs, 1.2V, BGA-756"
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Lattice*caBGA*27x27mm*Layout32x32*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LFE5U-85F-7BG381x"
		(extends "LFE5U-85F-8BG381x")
		(property "Reference" "U"
			(at 24.13 16.51 0)
		)
		(property "Value" "LFE5U-85F-7BG381x"
			(at 24.13 13.97 0)
		)
		(property "Footprint" "Package_BGA:Lattice_caBGA-381_17x17mm_Layout20x20_P0.8mm"
			(at 11.43 72.39 0)
		)
		(property "Datasheet" "https://www.latticesemi.com/view_document?document_id=50461"
			(at 11.43 72.39 0)
		)
		(property "Description" "ECP5 FPGA, 84K LUTs, 1.2V, BGA-381"
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Lattice?caBGA*17x17mm*Layout20x20*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LFE5U-85F-7BG756x"
		(extends "LFE5U-85F-8BG756x")
		(property "Reference" "U"
			(at 24.13 16.51 0)
		)
		(property "Value" "LFE5U-85F-7BG756x"
			(at 24.13 13.97 0)
		)
		(property "Footprint" "Package_BGA:Lattice_caBGA-756_27x27mm_Layout32x32_P0.8mm"
			(at 11.43 72.39 0)
		)
		(property "Datasheet" "https://www.latticesemi.com/view_document?document_id=50461"
			(at 11.43 72.39 0)
		)
		(property "Description" "ECP5 FPGA, 84K LUTs, 1.2V, BGA-756"
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Lattice*caBGA*27x27mm*Layout32x32*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LFE5UM-85F-6BG381x"
		(extends "LFE5UM5G-85F-8BG381x")
		(property "Reference" "U"
			(at 24.13 16.51 0)
		)
		(property "Value" "LFE5UM-85F-6BG381x"
			(at 24.13 13.97 0)
		)
		(property "Footprint" "Package_BGA:Lattice_caBGA-381_17x17mm_Layout20x20_P0.8mm"
			(at 11.43 72.39 0)
		)
		(property "Datasheet" "https://www.latticesemi.com/view_document?document_id=50461"
			(at 11.43 72.39 0)
		)
		(property "Description" "ECP5 FPGA, 84K LUTs, 1.2V, 3.2Gbps SERDES, BGA-381"
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Lattice?caBGA*17x17mm*Layout20x20*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LFE5UM-85F-6BG756x"
		(extends "LFE5UM5G-85F-8BG756x")
		(property "Reference" "U"
			(at 24.13 16.51 0)
		)
		(property "Value" "LFE5UM-85F-6BG756x"
			(at 24.13 13.97 0)
		)
		(property "Footprint" "Package_BGA:Lattice_caBGA-756_27x27mm_Layout32x32_P0.8mm"
			(at 11.43 72.39 0)
		)
		(property "Datasheet" "https://www.latticesemi.com/view_document?document_id=50461"
			(at 11.43 72.39 0)
		)
		(property "Description" "ECP5 FPGA, 84K LUTs, 1.2V, 3.2Gbps SERDES, BGA-756"
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Lattice*caBGA*27x27mm*Layout32x32*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LFE5UM-85F-7BG381x"
		(extends "LFE5UM5G-85F-8BG381x")
		(property "Reference" "U"
			(at 24.13 16.51 0)
		)
		(property "Value" "LFE5UM-85F-7BG381x"
			(at 24.13 13.97 0)
		)
		(property "Footprint" "Package_BGA:Lattice_caBGA-381_17x17mm_Layout20x20_P0.8mm"
			(at 11.43 72.39 0)
		)
		(property "Datasheet" "https://www.latticesemi.com/view_document?document_id=50461"
			(at 11.43 72.39 0)
		)
		(property "Description" "ECP5 FPGA, 84K LUTs, 1.2V, 3.2Gbps SERDES, BGA-381"
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Lattice?caBGA*17x17mm*Layout20x20*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LFE5UM-85F-7BG756x"
		(extends "LFE5UM5G-85F-8BG756x")
		(property "Reference" "U"
			(at 24.13 16.51 0)
		)
		(property "Value" "LFE5UM-85F-7BG756x"
			(at 24.13 13.97 0)
		)
		(property "Footprint" "Package_BGA:Lattice_caBGA-756_27x27mm_Layout32x32_P0.8mm"
			(at 11.43 72.39 0)
		)
		(property "Datasheet" "https://www.latticesemi.com/view_document?document_id=50461"
			(at 11.43 72.39 0)
		)
		(property "Description" "ECP5 FPGA, 84K LUTs, 1.2V, 3.2Gbps SERDES, BGA-756"
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Lattice*caBGA*27x27mm*Layout32x32*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LFE5UM-85F-8BG381x"
		(extends "LFE5UM5G-85F-8BG381x")
		(property "Reference" "U"
			(at 24.13 16.51 0)
		)
		(property "Value" "LFE5UM-85F-8BG381x"
			(at 24.13 13.97 0)
		)
		(property "Footprint" "Package_BGA:Lattice_caBGA-381_17x17mm_Layout20x20_P0.8mm"
			(at 11.43 72.39 0)
		)
		(property "Datasheet" "https://www.latticesemi.com/view_document?document_id=50461"
			(at 11.43 72.39 0)
		)
		(property "Description" "ECP5 FPGA, 84K LUTs, 1.2V, 3.2Gbps SERDES, BGA-381"
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Lattice?caBGA*17x17mm*Layout20x20*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LFE5UM-85F-8BG756x"
		(extends "LFE5UM5G-85F-8BG756x")
		(property "Reference" "U"
			(at 24.13 16.51 0)
		)
		(property "Value" "LFE5UM-85F-8BG756x"
			(at 24.13 13.97 0)
		)
		(property "Footprint" "Package_BGA:Lattice_caBGA-756_27x27mm_Layout32x32_P0.8mm"
			(at 11.43 72.39 0)
		)
		(property "Datasheet" "https://www.latticesemi.com/view_document?document_id=50461"
			(at 11.43 72.39 0)
		)
		(property "Description" "ECP5 FPGA, 84K LUTs, 1.2V, 3.2Gbps SERDES, BGA-756"
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA programmable logic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Lattice*caBGA*27x27mm*Layout32x32*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LFXP2-5E-6TN144"
		(extends "LFXP2-5E-5TN144")
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "LFXP2-5E-6TN144"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_QFP:TQFP-144_20x20mm_P0.5mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.latticesemi.com/view_document?document_id=24635"
			(at 0 -10.16 0)
		)
		(property "Description" "FPGA, 5000 LUTs, 1.2V, TQFP-144"
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA Lattice XP2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*20x20mm*"
			(at 0 0 0)
		)
	)
	(symbol "LFXP2-5E-7TN144"
		(extends "LFXP2-5E-5TN144")
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "LFXP2-5E-7TN144"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_QFP:TQFP-144_20x20mm_P0.5mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.latticesemi.com/view_document?document_id=24635"
			(at 0 -10.16 0)
		)
		(property "Description" "FPGA, 5000 LUTs, 1.2V, TQFP-144"
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA Lattice XP2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*20x20mm*"
			(at 0 0 0)
		)
	)
)
