(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "A3P030-VQG100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 30.48 60.96 0)
		)
		(property "Value" "A3P030-VQG100"
			(at 30.48 58.42 0)
		)
		(property "Footprint" "Package_QFP:VQFP-100_14x14mm_P0.5mm"
			(at 30.48 55.88 0)
		)
		(property "Datasheet" "http://www.microsemi.com/document-portal/doc_download/130704-proasic3-flash-family-fpgas-datasheet"
			(at 0 5.08 0)
		)
		(property "Description" "Actel ProASIC3 Flash Family FPGAs, 256 MCLB, 100pin QFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "ProASIC3 ACTEL FLASH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "A3P030-VQG100_0_1")
		(symbol "A3P030-VQG100_1_1"
			(pin bidirectional line
				(at -33.02 58.42 0)
				(length 3.81)
				(name "VJTAG")
				(number "56")
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 3.81)
				(name "TCK")
				(number "47")
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 3.81)
				(name "TDI")
				(number "48")
			)
			(pin bidirectional line
				(at -33.02 50.8 0)
				(length 3.81)
				(name "TMS")
				(number "49")
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 3.81)
				(name "TDO")
				(number "54")
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 3.81)
				(name "TRST")
				(number "55")
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 3.81)
				(name "IO82RSB1")
				(number "2")
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 3.81)
				(name "IO81RSB1")
				(number "3")
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 3.81)
				(name "IO80RSB1")
				(number "4")
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 3.81)
				(name "IO79RSB1")
				(number "5")
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 3.81)
				(name "IO78RSB1")
				(number "6")
			)
			(pin input line
				(at -33.02 27.94 0)
				(length 3.81)
				(name "IO77RSB1")
				(number "7")
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 3.81)
				(name "IO76RSB1")
				(number "8")
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 3.81)
				(name "IO75RSB1")
				(number "10")
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 3.81)
				(name "IO74RSB1")
				(number "11")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 3.81)
				(name "IO73RSB1/GEC0")
				(number "12")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 3.81)
				(name "IO72RSB1/GEA0")
				(number "13")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 3.81)
				(name "IO71RSB1/GEB0")
				(number "14")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 3.81)
				(name "IO70RSB1")
				(number "15")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "IO69RSB1")
				(number "16")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 3.81)
				(name "IO68RSB1")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 3.81)
				(name "IO67RSB1")
				(number "20")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 3.81)
				(name "IO66RSB1")
				(number "21")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 3.81)
				(name "IO65RSB1")
				(number "22")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 3.81)
				(name "IO64RSB1")
				(number "23")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 3.81)
				(name "IO63RSB1")
				(number "24")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 3.81)
				(name "IO62RSB1")
				(number "25")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 3.81)
				(name "IO61RSB1")
				(number "26")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 3.81)
				(name "IO60RSB1")
				(number "27")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 3.81)
				(name "IO59RSB1")
				(number "28")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 3.81)
				(name "IO58RSB1")
				(number "29")
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 3.81)
				(name "IO57RSB1")
				(number "30")
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 3.81)
				(name "IO56RSB1")
				(number "31")
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 3.81)
				(name "IO55RSB1")
				(number "32")
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 3.81)
				(name "IO54RSB1")
				(number "33")
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 3.81)
				(name "IO53RSB1")
				(number "34")
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 3.81)
				(name "IO52RSB1")
				(number "35")
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 3.81)
				(name "IO51RSB1")
				(number "36")
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 3.81)
				(name "IO49RSB1")
				(number "40")
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 3.81)
				(name "IO47RSB1")
				(number "41")
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 3.81)
				(name "IO46RSB1")
				(number "42")
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 3.81)
				(name "IO45RSB1")
				(number "43")
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 3.81)
				(name "IO44RSB1")
				(number "44")
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 3.81)
				(name "IO43RSB1")
				(number "45")
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 3.81)
				(name "IO42RSB1")
				(number "46")
			)
			(pin power_in line
				(at -15.24 66.04 270)
				(length 3.81)
				(name "VCC")
				(number "17")
			)
			(pin power_in line
				(at -12.7 66.04 270)
				(length 3.81)
				(name "VCC")
				(number "37")
			)
			(pin power_in line
				(at -10.16 66.04 270)
				(length 3.81)
				(name "VCC")
				(number "68")
			)
			(pin power_in line
				(at -7.62 66.04 270)
				(length 3.81)
				(name "VCC")
				(number "89")
			)
			(pin power_in line
				(at -7.62 -66.04 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -66.04 90)
				(length 3.81)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at -2.54 66.04 270)
				(length 3.81)
				(name "VCCIB1")
				(number "18")
			)
			(pin power_in line
				(at -2.54 -66.04 90)
				(length 3.81)
				(name "GND")
				(number "38")
			)
			(pin power_in line
				(at 0 66.04 270)
				(length 3.81)
				(name "VCCIB1")
				(number "39")
			)
			(pin power_in line
				(at 0 -66.04 90)
				(length 3.81)
				(name "GND")
				(number "51")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 3.81)
				(name "VCCIB0")
				(number "66")
			)
			(pin power_in line
				(at 2.54 -66.04 90)
				(length 3.81)
				(name "GND")
				(number "67")
			)
			(pin power_in line
				(at 5.08 66.04 270)
				(length 3.81)
				(name "VCCIB0")
				(number "87")
			)
			(pin power_in line
				(at 5.08 -66.04 90)
				(length 3.81)
				(name "GND")
				(number "88")
			)
			(pin power_in line
				(at 20.32 66.04 270)
				(length 3.81)
				(name "VPUMP")
				(number "52")
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 3.81)
				(name "IO00RSB0")
				(number "100")
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 3.81)
				(name "IO01RSB0")
				(number "99")
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 3.81)
				(name "IO02RSB0")
				(number "98")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 3.81)
				(name "IO03RSB0")
				(number "97")
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 3.81)
				(name "IO04RSB0")
				(number "96")
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 3.81)
				(name "IO05RSB0")
				(number "95")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "IO06RSB0")
				(number "94")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 3.81)
				(name "IO07RSB0")
				(number "93")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "IO08RSB0")
				(number "92")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "IO10RSB0")
				(number "91")
			)
			(pin input line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "IO12RSB0")
				(number "90")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "IO14RSB0")
				(number "86")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "IO15RSB0")
				(number "85")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "IO16RSB0")
				(number "84")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "IO17RSB0")
				(number "83")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "IO18RSB0")
				(number "82")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 3.81)
				(name "IO19RSB0")
				(number "81")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "IO20RSB0")
				(number "80")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "IO21RSB0")
				(number "79")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "IO22RSB0")
				(number "78")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "IO23RSB0")
				(number "77")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "IO24RSB0")
				(number "76")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "IO25RSB0")
				(number "75")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "IO26RSB0")
				(number "74")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 3.81)
				(name "IO27RSB0")
				(number "73")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 3.81)
				(name "IO28RSB0")
				(number "72")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 3.81)
				(name "IO29RSB0")
				(number "71")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 3.81)
				(name "IO30RSB0")
				(number "70")
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 3.81)
				(name "IO31RSB0")
				(number "69")
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 3.81)
				(name "GDC0/IO32RSB0")
				(number "65")
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 3.81)
				(name "GDA0/IO33RSB0")
				(number "64")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 3.81)
				(name "GDB0/IO34RSB0")
				(number "63")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 3.81)
				(name "IO36RSB0")
				(number "62")
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 3.81)
				(name "IO37RSB0")
				(number "61")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 3.81)
				(name "IO38RSB0")
				(number "60")
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 3.81)
				(name "IO39RSB0")
				(number "59")
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 3.81)
				(name "IO40RSB0")
				(number "58")
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 3.81)
				(name "IO41RSB0")
				(number "57")
			)
		)
		(embedded_fonts no)
	)
	(symbol "A3P060-VQG100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 30.48 53.34 0)
		)
		(property "Value" "A3P060-VQG100"
			(at 30.48 50.8 0)
		)
		(property "Footprint" "Package_QFP:VQFP-100_14x14mm_P0.5mm"
			(at 30.48 48.26 0)
		)
		(property "Datasheet" "http://www.microsemi.com/document-portal/doc_download/130704-proasic3-flash-family-fpgas-datasheet"
			(at 0 0 0)
		)
		(property "Description" "Actel ProASIC3 Flash Family FPGAs, 512 MCLB, 100pin QFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "ProASIC3 ACTEL FLASH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "A3P060-VQG100_0_1")
		(symbol "A3P060-VQG100_1_1"
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 3.81)
				(name "VJTAG")
				(number "56")
			)
			(pin bidirectional line
				(at -33.02 50.8 0)
				(length 3.81)
				(name "TCK")
				(number "47")
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 3.81)
				(name "TDI")
				(number "48")
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 3.81)
				(name "TMS")
				(number "49")
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 3.81)
				(name "TDO")
				(number "54")
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 3.81)
				(name "TRST")
				(number "55")
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 3.81)
				(name "IO95RSB1")
				(number "5")
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 3.81)
				(name "IO94RSB1/GAC2")
				(number "6")
			)
			(pin input line
				(at -33.02 30.48 0)
				(length 3.81)
				(name "IO93RSB1")
				(number "7")
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 3.81)
				(name "IO92RSB1")
				(number "8")
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 3.81)
				(name "IO87RSB1/GFB1")
				(number "10")
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 3.81)
				(name "IO86RSB1/GFB0")
				(number "11")
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 3.81)
				(name "IO85RSB1/GFA0")
				(number "13")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 3.81)
				(name "IO84RSB1/GFA1")
				(number "15")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 3.81)
				(name "IO83RSB1/GFA2")
				(number "16")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 3.81)
				(name "IO77RSB1/GEC1")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 3.81)
				(name "IO74RSB1/GEB0")
				(number "21")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "IO75RSB1/GEB1")
				(number "20")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 3.81)
				(name "IO73RSB1/GEA1")
				(number "22")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 3.81)
				(name "IO72RSB1/GEA0")
				(number "23")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 3.81)
				(name "IO71RSB1/GEA2")
				(number "26")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 3.81)
				(name "IO70RSB1/GEB2")
				(number "27")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 3.81)
				(name "IO69RSB1/GEC2")
				(number "28")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 3.81)
				(name "IO68RSB1")
				(number "29")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 3.81)
				(name "IO67RSB1")
				(number "30")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 3.81)
				(name "IO66RSB1")
				(number "31")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 3.81)
				(name "IO65RSB1")
				(number "32")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 3.81)
				(name "IO64RSB1")
				(number "33")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 3.81)
				(name "IO63RSB1")
				(number "34")
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 3.81)
				(name "IO62RSB1")
				(number "35")
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 3.81)
				(name "IO61RSB1")
				(number "36")
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 3.81)
				(name "IO60RSB1")
				(number "40")
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 3.81)
				(name "IO59RSB1")
				(number "41")
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 3.81)
				(name "IO58RSB1")
				(number "42")
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 3.81)
				(name "IO57RSB1")
				(number "43")
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 3.81)
				(name "IO56RSB1/GDC2")
				(number "44")
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 3.81)
				(name "IO55RSB1/GDB2")
				(number "45")
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 3.81)
				(name "IO54RSB1/GDA2")
				(number "46")
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 3.81)
				(name "IO53RSB1/GAB2")
				(number "4")
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 3.81)
				(name "IO52RSB1")
				(number "3")
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 3.81)
				(name "IO51RSB1/GAA2")
				(number "2")
			)
			(pin power_in line
				(at -20.32 58.42 270)
				(length 3.81)
				(name "VCCPLF")
				(number "14")
			)
			(pin power_in line
				(at -15.24 58.42 270)
				(length 3.81)
				(name "VCC")
				(number "17")
			)
			(pin power_in line
				(at -12.7 58.42 270)
				(length 3.81)
				(name "VCC")
				(number "37")
			)
			(pin power_in line
				(at -12.7 -58.42 90)
				(length 3.81)
				(name "VCOMPLF")
				(number "12")
			)
			(pin power_in line
				(at -10.16 58.42 270)
				(length 3.81)
				(name "VCC")
				(number "68")
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 3.81)
				(name "VCC")
				(number "89")
			)
			(pin power_in line
				(at -7.62 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 3.81)
				(name "VCCIB1")
				(number "18")
			)
			(pin power_in line
				(at -2.54 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "38")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 3.81)
				(name "VCCIB1")
				(number "39")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "51")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 3.81)
				(name "VCCIB0")
				(number "66")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "67")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 3.81)
				(name "VCCIB0")
				(number "87")
			)
			(pin power_in line
				(at 5.08 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "88")
			)
			(pin power_in line
				(at 10.16 58.42 270)
				(length 3.81)
				(name "VMV1")
				(number "24")
			)
			(pin power_in line
				(at 10.16 -58.42 90)
				(length 3.81)
				(name "GNDQ")
				(number "25")
			)
			(pin power_in line
				(at 12.7 58.42 270)
				(length 3.81)
				(name "VMV1")
				(number "50")
			)
			(pin power_in line
				(at 12.7 -58.42 90)
				(length 3.81)
				(name "GNDQ")
				(number "75")
			)
			(pin power_in line
				(at 15.24 58.42 270)
				(length 3.81)
				(name "VMV0")
				(number "74")
			)
			(pin power_in line
				(at 20.32 58.42 270)
				(length 3.81)
				(name "VPUMP")
				(number "52")
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 3.81)
				(name "IO00RSB0")
				(number "100")
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 3.81)
				(name "IO01RSB0")
				(number "99")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 3.81)
				(name "GAA0/IO02RSB0")
				(number "98")
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 3.81)
				(name "GAA1/IO03RSB0")
				(number "97")
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 3.81)
				(name "GAB0/IO04RSB0")
				(number "96")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "GAB1/IO05RSB0")
				(number "95")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 3.81)
				(name "GAC1/IO06RSB0")
				(number "94")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "GAC1/IO07RSB0")
				(number "93")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "IO08RSB0")
				(number "92")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "IO09RSB0")
				(number "91")
			)
			(pin input line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "IO10RSB0")
				(number "90")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "IO11RSB0")
				(number "86")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "IO13RSB0")
				(number "85")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "IO15RSB0")
				(number "84")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "IO17RSB0")
				(number "83")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 3.81)
				(name "IO18RSB0")
				(number "82")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "GBC0/IO19RSB0")
				(number "81")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "GBC1/IO20RSB0")
				(number "80")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "GBB0/IO21RSB0")
				(number "79")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "GBB1/IO22RSB0")
				(number "78")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "GBA0/IO23RSB0")
				(number "77")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "GBA1/IO24RSB0")
				(number "76")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "GBA2/IO25RSB0")
				(number "73")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 3.81)
				(name "IO26RSB0")
				(number "72")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 3.81)
				(name "GBB2/IO27RSB0")
				(number "71")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 3.81)
				(name "GBC2/IO29RSB0")
				(number "70")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 3.81)
				(name "IO31RSB0")
				(number "69")
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 3.81)
				(name "GCC1/IO35RSB0")
				(number "65")
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 3.81)
				(name "GCC0/IO36RSB0")
				(number "64")
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 3.81)
				(name "GCA1/IO39RSB0")
				(number "63")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 3.81)
				(name "GCA0/IO40RSB0")
				(number "62")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 3.81)
				(name "GCB2/IO42RSB0")
				(number "61")
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 3.81)
				(name "GCC2/IO43RSB0")
				(number "60")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 3.81)
				(name "GDC1/IO45RSB0")
				(number "59")
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 3.81)
				(name "GDC0/IO46RSB0")
				(number "58")
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 3.81)
				(name "GDA1/IO49RSB0")
				(number "57")
			)
		)
		(embedded_fonts no)
	)
	(symbol "A3P1000-PQG208"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 45.72 111.76 0)
		)
		(property "Value" "A3P1000-PQG208"
			(at 45.72 109.22 0)
		)
		(property "Footprint" "Package_QFP:PQFP-208_28x28mm_P0.5mm"
			(at 45.72 106.68 0)
		)
		(property "Datasheet" "http://www.microsemi.com/document-portal/doc_download/130704-proasic3-flash-family-fpgas-datasheet"
			(at 0 -6.35 0)
		)
		(property "Description" "Actel ProASIC3 Flash Family FPGAs, 1000k Gates, 208pin QFP"
			(at 0 0 0)
		)
		(property "ki_keywords" "ProASIC3 ACTEL FLASH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFP*28x28mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "A3P1000-PQG208_1_0")
		(symbol "A3P1000-PQG208_1_1"
			(pin power_in line
				(at -48.26 109.22 0)
				(length 3.81)
				(name "VJTAG")
				(number "110")
			)
			(pin bidirectional line
				(at -48.26 106.68 0)
				(length 3.81)
				(name "TCK")
				(number "101")
			)
			(pin bidirectional line
				(at -48.26 104.14 0)
				(length 3.81)
				(name "TDI")
				(number "102")
			)
			(pin bidirectional line
				(at -48.26 101.6 0)
				(length 3.81)
				(name "TMS")
				(number "103")
			)
			(pin bidirectional line
				(at -48.26 99.06 0)
				(length 3.81)
				(name "TDO")
				(number "108")
			)
			(pin bidirectional line
				(at -48.26 96.52 0)
				(length 3.81)
				(name "TRST")
				(number "109")
			)
			(pin bidirectional line
				(at -48.26 91.44 0)
				(length 3.81)
				(name "IO188NDB3/GEA0")
				(number "49")
			)
			(pin bidirectional line
				(at -48.26 88.9 0)
				(length 3.81)
				(name "IO188PDB3/GEA1")
				(number "48")
			)
			(pin bidirectional line
				(at -48.26 86.36 0)
				(length 3.81)
				(name "IO189NDB3/GEB0")
				(number "47")
			)
			(pin bidirectional line
				(at -48.26 83.82 0)
				(length 3.81)
				(name "IO189PDB3/GEB1")
				(number "46")
			)
			(pin bidirectional line
				(at -48.26 81.28 0)
				(length 3.81)
				(name "IO190NDB3/GEC0")
				(number "45")
			)
			(pin bidirectional line
				(at -48.26 78.74 0)
				(length 3.81)
				(name "IO190PDB3/GEC1")
				(number "44")
			)
			(pin bidirectional line
				(at -48.26 76.2 0)
				(length 3.81)
				(name "IO191NDB3")
				(number "43")
			)
			(pin bidirectional line
				(at -48.26 73.66 0)
				(length 3.81)
				(name "IO191PDB3")
				(number "42")
			)
			(pin bidirectional line
				(at -48.26 71.12 0)
				(length 3.81)
				(name "IO197PSB3")
				(number "39")
			)
			(pin bidirectional line
				(at -48.26 68.58 0)
				(length 3.81)
				(name "IO199NDB3")
				(number "38")
			)
			(pin bidirectional line
				(at -48.26 66.04 0)
				(length 3.81)
				(name "IO199PDB3")
				(number "37")
			)
			(pin bidirectional line
				(at -48.26 63.5 0)
				(length 3.81)
				(name "IO204NDB3")
				(number "35")
			)
			(pin bidirectional line
				(at -48.26 60.96 0)
				(length 3.81)
				(name "IO204PDB3/GFC2")
				(number "34")
			)
			(pin bidirectional line
				(at -48.26 58.42 0)
				(length 3.81)
				(name "IO205NDB3")
				(number "33")
			)
			(pin bidirectional line
				(at -48.26 55.88 0)
				(length 3.81)
				(name "IO205PDB3/GFB2")
				(number "32")
			)
			(pin bidirectional line
				(at -48.26 53.34 0)
				(length 3.81)
				(name "IO206NDB3")
				(number "31")
			)
			(pin bidirectional line
				(at -48.26 50.8 0)
				(length 3.81)
				(name "IO206PDB3/GFA2")
				(number "30")
			)
			(pin bidirectional line
				(at -48.26 48.26 0)
				(length 3.81)
				(name "IO207PPB3/GFA1")
				(number "28")
			)
			(pin bidirectional line
				(at -48.26 45.72 0)
				(length 3.81)
				(name "IO207NPB3/GFA0")
				(number "26")
			)
			(pin bidirectional line
				(at -48.26 43.18 0)
				(length 3.81)
				(name "IO208NDB3/GFB0")
				(number "24")
			)
			(pin bidirectional line
				(at -48.26 40.64 0)
				(length 3.81)
				(name "IO208PDB3/GFB1")
				(number "23")
			)
			(pin bidirectional line
				(at -48.26 38.1 0)
				(length 3.81)
				(name "IO209NDB3/GFC0")
				(number "22")
			)
			(pin bidirectional line
				(at -48.26 35.56 0)
				(length 3.81)
				(name "IO209PDB3/GFC1")
				(number "21")
			)
			(pin bidirectional line
				(at -48.26 33.02 0)
				(length 3.81)
				(name "IO212NDB3")
				(number "20")
			)
			(pin bidirectional line
				(at -48.26 30.48 0)
				(length 3.81)
				(name "IO212PDB3")
				(number "19")
			)
			(pin bidirectional line
				(at -48.26 27.94 0)
				(length 3.81)
				(name "IO216NDB3")
				(number "15")
			)
			(pin bidirectional line
				(at -48.26 25.4 0)
				(length 3.81)
				(name "IO216PDB3")
				(number "14")
			)
			(pin bidirectional line
				(at -48.26 22.86 0)
				(length 3.81)
				(name "IO218NDB3")
				(number "13")
			)
			(pin bidirectional line
				(at -48.26 20.32 0)
				(length 3.81)
				(name "IO218PDB3")
				(number "12")
			)
			(pin bidirectional line
				(at -48.26 17.78 0)
				(length 3.81)
				(name "IO220NDB3")
				(number "11")
			)
			(pin bidirectional line
				(at -48.26 15.24 0)
				(length 3.81)
				(name "IO220PDB3")
				(number "10")
			)
			(pin bidirectional line
				(at -48.26 12.7 0)
				(length 3.81)
				(name "IO222NDB3")
				(number "9")
			)
			(pin bidirectional line
				(at -48.26 10.16 0)
				(length 3.81)
				(name "IO222PDB3")
				(number "8")
			)
			(pin bidirectional line
				(at -48.26 7.62 0)
				(length 3.81)
				(name "IO223NDB3")
				(number "7")
			)
			(pin bidirectional line
				(at -48.26 5.08 0)
				(length 3.81)
				(name "IO223PDB3/GAC2")
				(number "6")
			)
			(pin bidirectional line
				(at -48.26 2.54 0)
				(length 3.81)
				(name "IO224NDB3")
				(number "5")
			)
			(pin bidirectional line
				(at -48.26 0 0)
				(length 3.81)
				(name "IO224PDB3/GAB2")
				(number "4")
			)
			(pin bidirectional line
				(at -48.26 -2.54 0)
				(length 3.81)
				(name "IO225NDB3")
				(number "3")
			)
			(pin bidirectional line
				(at -48.26 -5.08 0)
				(length 3.81)
				(name "IO225PDB3/GAA2")
				(number "2")
			)
			(pin bidirectional line
				(at -48.26 -10.16 0)
				(length 3.81)
				(name "IO114RSB2/GDA2")
				(number "99")
			)
			(pin bidirectional line
				(at -48.26 -12.7 0)
				(length 3.81)
				(name "IO115RSB2/GDB2")
				(number "98")
			)
			(pin bidirectional line
				(at -48.26 -15.24 0)
				(length 3.81)
				(name "IO116RSB2/GDC2")
				(number "96")
			)
			(pin bidirectional line
				(at -48.26 -17.78 0)
				(length 3.81)
				(name "IO118RSB2")
				(number "95")
			)
			(pin bidirectional line
				(at -48.26 -20.32 0)
				(length 3.81)
				(name "IO120RSB2")
				(number "94")
			)
			(pin bidirectional line
				(at -48.26 -22.86 0)
				(length 3.81)
				(name "IO122RSB2")
				(number "93")
			)
			(pin bidirectional line
				(at -48.26 -25.4 0)
				(length 3.81)
				(name "IO124RSB2")
				(number "92")
			)
			(pin bidirectional line
				(at -48.26 -27.94 0)
				(length 3.81)
				(name "IO126RSB2")
				(number "91")
			)
			(pin bidirectional line
				(at -48.26 -30.48 0)
				(length 3.81)
				(name "IO128RSB2")
				(number "90")
			)
			(pin bidirectional line
				(at -48.26 -33.02 0)
				(length 3.81)
				(name "IO133RSB2")
				(number "87")
			)
			(pin bidirectional line
				(at -48.26 -35.56 0)
				(length 3.81)
				(name "IO135RSB2")
				(number "86")
			)
			(pin bidirectional line
				(at -48.26 -38.1 0)
				(length 3.81)
				(name "IO137RSB2")
				(number "85")
			)
			(pin bidirectional line
				(at -48.26 -40.64 0)
				(length 3.81)
				(name "IO139RSB2")
				(number "84")
			)
			(pin bidirectional line
				(at -48.26 -43.18 0)
				(length 3.81)
				(name "IO141RSB2")
				(number "83")
			)
			(pin bidirectional line
				(at -48.26 -45.72 0)
				(length 3.81)
				(name "IO143RSB2")
				(number "82")
			)
			(pin bidirectional line
				(at -48.26 -48.26 0)
				(length 3.81)
				(name "IO148RSB2")
				(number "80")
			)
			(pin bidirectional line
				(at -48.26 -50.8 0)
				(length 3.81)
				(name "IO150RSB2")
				(number "79")
			)
			(pin bidirectional line
				(at -48.26 -53.34 0)
				(length 3.81)
				(name "IO152RSB2")
				(number "78")
			)
			(pin bidirectional line
				(at -48.26 -55.88 0)
				(length 3.81)
				(name "IO154RSB2")
				(number "77")
			)
			(pin bidirectional line
				(at -48.26 -58.42 0)
				(length 3.81)
				(name "IO156RSB2")
				(number "76")
			)
			(pin bidirectional line
				(at -48.26 -60.96 0)
				(length 3.81)
				(name "IO158RSB2")
				(number "75")
			)
			(pin bidirectional line
				(at -48.26 -63.5 0)
				(length 3.81)
				(name "IO160RSB2")
				(number "74")
			)
			(pin bidirectional line
				(at -48.26 -66.04 0)
				(length 3.81)
				(name "IO162RSB2")
				(number "73")
			)
			(pin bidirectional line
				(at -48.26 -68.58 0)
				(length 3.81)
				(name "IO166RSB2")
				(number "70")
			)
			(pin bidirectional line
				(at -48.26 -71.12 0)
				(length 3.81)
				(name "IO168RSB2")
				(number "69")
			)
			(pin bidirectional line
				(at -48.26 -73.66 0)
				(length 3.81)
				(name "IO170RSB2")
				(number "68")
			)
			(pin bidirectional line
				(at -48.26 -76.2 0)
				(length 3.81)
				(name "IO172RSB2")
				(number "67")
			)
			(pin bidirectional line
				(at -48.26 -78.74 0)
				(length 3.81)
				(name "IO174RSB2")
				(number "66")
			)
			(pin bidirectional line
				(at -48.26 -81.28 0)
				(length 3.81)
				(name "IO176RSB2")
				(number "64")
			)
			(pin bidirectional line
				(at -48.26 -83.82 0)
				(length 3.81)
				(name "IO178RSB2")
				(number "63")
			)
			(pin bidirectional line
				(at -48.26 -86.36 0)
				(length 3.81)
				(name "IO180RSB2")
				(number "61")
			)
			(pin bidirectional line
				(at -48.26 -88.9 0)
				(length 3.81)
				(name "IO181RSB2")
				(number "60")
			)
			(pin bidirectional line
				(at -48.26 -91.44 0)
				(length 3.81)
				(name "IO182RSB2")
				(number "59")
			)
			(pin bidirectional line
				(at -48.26 -93.98 0)
				(length 3.81)
				(name "IO183RSB2")
				(number "58")
			)
			(pin bidirectional line
				(at -48.26 -96.52 0)
				(length 3.81)
				(name "IO184RSB2")
				(number "57")
			)
			(pin bidirectional line
				(at -48.26 -99.06 0)
				(length 3.81)
				(name "IO185RSB2/GEC2")
				(number "56")
			)
			(pin bidirectional line
				(at -48.26 -101.6 0)
				(length 3.81)
				(name "IO186RSB2/GEB2")
				(number "55")
			)
			(pin bidirectional line
				(at -48.26 -104.14 0)
				(length 3.81)
				(name "IO187RSB2/GEA2")
				(number "54")
			)
			(pin power_in line
				(at -33.02 116.84 270)
				(length 3.81)
				(name "VCCPLF")
				(number "27")
			)
			(pin power_in line
				(at -27.94 116.84 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at -27.94 -116.84 90)
				(length 3.81)
				(name "VCOMPLF")
				(number "25")
			)
			(pin power_in line
				(at -25.4 116.84 270)
				(length 3.81)
				(name "VCC")
				(number "36")
			)
			(pin power_in line
				(at -22.86 116.84 270)
				(length 3.81)
				(name "VCC")
				(number "71")
			)
			(pin power_in line
				(at -22.86 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -20.32 116.84 270)
				(length 3.81)
				(name "VCC")
				(number "88")
			)
			(pin power_in line
				(at -20.32 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 3.81)
				(name "VCC")
				(number "142")
			)
			(pin power_in line
				(at -17.78 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 3.81)
				(name "VCC")
				(number "171")
			)
			(pin power_in line
				(at -15.24 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "41")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 3.81)
				(name "VCC")
				(number "187")
			)
			(pin power_in line
				(at -12.7 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "52")
			)
			(pin power_in line
				(at -10.16 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 3.81)
				(name "VCCIB0")
				(number "200")
			)
			(pin power_in line
				(at -7.62 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "81")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 3.81)
				(name "VCCIB0")
				(number "186")
			)
			(pin power_in line
				(at -5.08 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "97")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 3.81)
				(name "VCCIB0")
				(number "170")
			)
			(pin power_in line
				(at -2.54 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "105")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 3.81)
				(name "VCCIB1")
				(number "140")
			)
			(pin power_in line
				(at 0 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "122")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 3.81)
				(name "VCCIB1")
				(number "123")
			)
			(pin power_in line
				(at 2.54 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "130")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 3.81)
				(name "VCCIB2")
				(number "89")
			)
			(pin power_in line
				(at 5.08 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "141")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 3.81)
				(name "VCCIB2")
				(number "72")
			)
			(pin power_in line
				(at 7.62 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "156")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 3.81)
				(name "VCCIB2")
				(number "62")
			)
			(pin power_in line
				(at 10.16 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "162")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 3.81)
				(name "VCCIB3")
				(number "40")
			)
			(pin power_in line
				(at 12.7 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "178")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 3.81)
				(name "VCCIB3")
				(number "18")
			)
			(pin power_in line
				(at 15.24 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "195")
			)
			(pin power_in line
				(at 20.32 116.84 270)
				(length 3.81)
				(name "VMV0")
				(number "157")
			)
			(pin power_in line
				(at 20.32 -116.84 90)
				(length 3.81)
				(name "GNDQ")
				(number "51")
			)
			(pin power_in line
				(at 22.86 116.84 270)
				(length 3.81)
				(name "VMV0")
				(number "208")
			)
			(pin power_in line
				(at 22.86 -116.84 90)
				(length 3.81)
				(name "GNDQ")
				(number "100")
			)
			(pin power_in line
				(at 25.4 116.84 270)
				(length 3.81)
				(name "VMV1")
				(number "154")
			)
			(pin power_in line
				(at 25.4 -116.84 90)
				(length 3.81)
				(name "GNDQ")
				(number "107")
			)
			(pin power_in line
				(at 27.94 116.84 270)
				(length 3.81)
				(name "VMV2")
				(number "53")
			)
			(pin power_in line
				(at 27.94 -116.84 90)
				(length 3.81)
				(name "GNDQ")
				(number "155")
			)
			(pin power_in line
				(at 30.48 116.84 270)
				(length 3.81)
				(name "VMV2")
				(number "104")
			)
			(pin power_in line
				(at 30.48 -116.84 90)
				(length 3.81)
				(name "GNDQ")
				(number "207")
			)
			(pin power_in line
				(at 33.02 116.84 270)
				(length 3.81)
				(name "VMV3")
				(number "50")
			)
			(pin power_in line
				(at 38.1 116.84 270)
				(length 3.81)
				(name "VPUMP")
				(number "106")
			)
			(pin bidirectional line
				(at 48.26 91.44 180)
				(length 3.81)
				(name "GAA0/IO00RSB0")
				(number "206")
			)
			(pin bidirectional line
				(at 48.26 88.9 180)
				(length 3.81)
				(name "GAA1/IO01RSB0")
				(number "205")
			)
			(pin bidirectional line
				(at 48.26 86.36 180)
				(length 3.81)
				(name "GAB0/IO02RSB0")
				(number "204")
			)
			(pin bidirectional line
				(at 48.26 83.82 180)
				(length 3.81)
				(name "GAB1/IO03RSB0")
				(number "203")
			)
			(pin bidirectional line
				(at 48.26 81.28 180)
				(length 3.81)
				(name "GAC0/IO04RSB0")
				(number "202")
			)
			(pin bidirectional line
				(at 48.26 78.74 180)
				(length 3.81)
				(name "GAC1/IO05RSB0")
				(number "201")
			)
			(pin bidirectional line
				(at 48.26 76.2 180)
				(length 3.81)
				(name "IO09RSB0")
				(number "199")
			)
			(pin bidirectional line
				(at 48.26 73.66 180)
				(length 3.81)
				(name "IO10RSB0")
				(number "198")
			)
			(pin bidirectional line
				(at 48.26 71.12 180)
				(length 3.81)
				(name "IO11RSB0")
				(number "197")
			)
			(pin bidirectional line
				(at 48.26 68.58 180)
				(length 3.81)
				(name "IO12RSB0")
				(number "196")
			)
			(pin bidirectional line
				(at 48.26 66.04 180)
				(length 3.81)
				(name "IO13RSB0")
				(number "194")
			)
			(pin bidirectional line
				(at 48.26 63.5 180)
				(length 3.81)
				(name "IO14RSB0")
				(number "193")
			)
			(pin bidirectional line
				(at 48.26 60.96 180)
				(length 3.81)
				(name "IO15RSB0")
				(number "192")
			)
			(pin bidirectional line
				(at 48.26 58.42 180)
				(length 3.81)
				(name "IO16RSB0")
				(number "191")
			)
			(pin bidirectional line
				(at 48.26 55.88 180)
				(length 3.81)
				(name "IO18RSB0")
				(number "190")
			)
			(pin bidirectional line
				(at 48.26 53.34 180)
				(length 3.81)
				(name "IO20RSB0")
				(number "189")
			)
			(pin bidirectional line
				(at 48.26 50.8 180)
				(length 3.81)
				(name "IO22RSB0")
				(number "188")
			)
			(pin bidirectional line
				(at 48.26 48.26 180)
				(length 3.81)
				(name "IO25RSB0")
				(number "185")
			)
			(pin bidirectional line
				(at 48.26 45.72 180)
				(length 3.81)
				(name "IO27RSB0")
				(number "184")
			)
			(pin bidirectional line
				(at 48.26 43.18 180)
				(length 3.81)
				(name "IO29RSB0")
				(number "183")
			)
			(pin bidirectional line
				(at 48.26 40.64 180)
				(length 3.81)
				(name "IO31RSB0")
				(number "182")
			)
			(pin bidirectional line
				(at 48.26 38.1 180)
				(length 3.81)
				(name "IO33RSB0")
				(number "181")
			)
			(pin bidirectional line
				(at 48.26 35.56 180)
				(length 3.81)
				(name "IO35RSB0")
				(number "180")
			)
			(pin bidirectional line
				(at 48.26 33.02 180)
				(length 3.81)
				(name "IO38RSB0")
				(number "179")
			)
			(pin bidirectional line
				(at 48.26 30.48 180)
				(length 3.81)
				(name "IO40RSB0")
				(number "177")
			)
			(pin bidirectional line
				(at 48.26 27.94 180)
				(length 3.81)
				(name "IO42RSB0")
				(number "176")
			)
			(pin bidirectional line
				(at 48.26 25.4 180)
				(length 3.81)
				(name "IO45RSB0")
				(number "175")
			)
			(pin bidirectional line
				(at 48.26 22.86 180)
				(length 3.81)
				(name "IO48RSB0")
				(number "174")
			)
			(pin bidirectional line
				(at 48.26 20.32 180)
				(length 3.81)
				(name "IO51RSB0")
				(number "173")
			)
			(pin bidirectional line
				(at 48.26 17.78 180)
				(length 3.81)
				(name "IO54RSB0")
				(number "172")
			)
			(pin bidirectional line
				(at 48.26 15.24 180)
				(length 3.81)
				(name "IO57RSB0")
				(number "169")
			)
			(pin bidirectional line
				(at 48.26 12.7 180)
				(length 3.81)
				(name "IO60RSB0")
				(number "168")
			)
			(pin bidirectional line
				(at 48.26 10.16 180)
				(length 3.81)
				(name "IO63RSB0")
				(number "167")
			)
			(pin bidirectional line
				(at 48.26 7.62 180)
				(length 3.81)
				(name "IO67RSB0")
				(number "166")
			)
			(pin bidirectional line
				(at 48.26 5.08 180)
				(length 3.81)
				(name "IO70RSB0")
				(number "165")
			)
			(pin bidirectional line
				(at 48.26 2.54 180)
				(length 3.81)
				(name "GBC0/IO72RSB0")
				(number "164")
			)
			(pin bidirectional line
				(at 48.26 0 180)
				(length 3.81)
				(name "GBC1/IO73RSB0")
				(number "163")
			)
			(pin bidirectional line
				(at 48.26 -2.54 180)
				(length 3.81)
				(name "GBB0/IO74RSB0")
				(number "161")
			)
			(pin bidirectional line
				(at 48.26 -5.08 180)
				(length 3.81)
				(name "GBB1/IO75RSB0")
				(number "160")
			)
			(pin bidirectional line
				(at 48.26 -7.62 180)
				(length 3.81)
				(name "GBA0/IO76RSB0")
				(number "159")
			)
			(pin bidirectional line
				(at 48.26 -10.16 180)
				(length 3.81)
				(name "GBA1/IO77RSB0")
				(number "158")
			)
			(pin bidirectional line
				(at 48.26 -15.24 180)
				(length 3.81)
				(name "GBA2/IO78PDB1")
				(number "153")
			)
			(pin bidirectional line
				(at 48.26 -17.78 180)
				(length 3.81)
				(name "IO78NDB1")
				(number "152")
			)
			(pin bidirectional line
				(at 48.26 -20.32 180)
				(length 3.81)
				(name "GBB2/IO79PDB1")
				(number "151")
			)
			(pin bidirectional line
				(at 48.26 -22.86 180)
				(length 3.81)
				(name "IO79NDB1")
				(number "150")
			)
			(pin bidirectional line
				(at 48.26 -25.4 180)
				(length 3.81)
				(name "GBC2/IO80PDB1")
				(number "149")
			)
			(pin bidirectional line
				(at 48.26 -27.94 180)
				(length 3.81)
				(name "IO80NDB1")
				(number "148")
			)
			(pin bidirectional line
				(at 48.26 -30.48 180)
				(length 3.81)
				(name "IO82PDB1")
				(number "147")
			)
			(pin bidirectional line
				(at 48.26 -33.02 180)
				(length 3.81)
				(name "IO82NDB1")
				(number "146")
			)
			(pin bidirectional line
				(at 48.26 -35.56 180)
				(length 3.81)
				(name "IO84PDB1")
				(number "145")
			)
			(pin bidirectional line
				(at 48.26 -38.1 180)
				(length 3.81)
				(name "IO84NDB1")
				(number "144")
			)
			(pin bidirectional line
				(at 48.26 -40.64 180)
				(length 3.81)
				(name "IO86PSB1")
				(number "143")
			)
			(pin bidirectional line
				(at 48.26 -43.18 180)
				(length 3.81)
				(name "IO88PDB1")
				(number "139")
			)
			(pin bidirectional line
				(at 48.26 -45.72 180)
				(length 3.81)
				(name "IO88NDB1")
				(number "138")
			)
			(pin bidirectional line
				(at 48.26 -48.26 180)
				(length 3.81)
				(name "GCC1/IO91PDB1")
				(number "137")
			)
			(pin bidirectional line
				(at 48.26 -50.8 180)
				(length 3.81)
				(name "GCC0/IO91NDB1")
				(number "136")
			)
			(pin bidirectional line
				(at 48.26 -53.34 180)
				(length 3.81)
				(name "GCB1/IO92PDB1")
				(number "135")
			)
			(pin bidirectional line
				(at 48.26 -55.88 180)
				(length 3.81)
				(name "GCB0/IO92NDB1")
				(number "134")
			)
			(pin bidirectional line
				(at 48.26 -58.42 180)
				(length 3.81)
				(name "GCA0/IO93NDB1")
				(number "133")
			)
			(pin bidirectional line
				(at 48.26 -60.96 180)
				(length 3.81)
				(name "GCA1/IO93PDB1")
				(number "132")
			)
			(pin bidirectional line
				(at 48.26 -63.5 180)
				(length 3.81)
				(name "GCA2/IO94PSB1")
				(number "131")
			)
			(pin bidirectional line
				(at 48.26 -66.04 180)
				(length 3.81)
				(name "GCB2/IO95PSB1")
				(number "129")
			)
			(pin bidirectional line
				(at 48.26 -68.58 180)
				(length 3.81)
				(name "GCC2/IO96PDB1")
				(number "128")
			)
			(pin bidirectional line
				(at 48.26 -71.12 180)
				(length 3.81)
				(name "IO96NDB1")
				(number "127")
			)
			(pin bidirectional line
				(at 48.26 -73.66 180)
				(length 3.81)
				(name "IO99PDB1")
				(number "125")
			)
			(pin bidirectional line
				(at 48.26 -76.2 180)
				(length 3.81)
				(name "IO99NDB1")
				(number "124")
			)
			(pin bidirectional line
				(at 48.26 -78.74 180)
				(length 3.81)
				(name "IO104PSB1")
				(number "121")
			)
			(pin bidirectional line
				(at 48.26 -81.28 180)
				(length 3.81)
				(name "IO106PDB1")
				(number "120")
			)
			(pin bidirectional line
				(at 48.26 -83.82 180)
				(length 3.81)
				(name "IO106NDB1")
				(number "119")
			)
			(pin bidirectional line
				(at 48.26 -86.36 180)
				(length 3.81)
				(name "IO109PDB1")
				(number "118")
			)
			(pin bidirectional line
				(at 48.26 -88.9 180)
				(length 3.81)
				(name "IO109NDB1")
				(number "117")
			)
			(pin bidirectional line
				(at 48.26 -91.44 180)
				(length 3.81)
				(name "GDC1/IO111PDB1")
				(number "116")
			)
			(pin bidirectional line
				(at 48.26 -93.98 180)
				(length 3.81)
				(name "GDC0/IO111NDB1")
				(number "115")
			)
			(pin bidirectional line
				(at 48.26 -96.52 180)
				(length 3.81)
				(name "GDB1/IO112PDB1")
				(number "114")
			)
			(pin bidirectional line
				(at 48.26 -99.06 180)
				(length 3.81)
				(name "GDB0/IO112NDB1")
				(number "113")
			)
			(pin bidirectional line
				(at 48.26 -101.6 180)
				(length 3.81)
				(name "GDA1/IO113PDB1")
				(number "112")
			)
			(pin bidirectional line
				(at 48.26 -104.14 180)
				(length 3.81)
				(name "GDA0/IO113NDB1")
				(number "111")
			)
		)
		(embedded_fonts no)
	)
	(symbol "A3P125-PQG208"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 43.18 99.06 0)
		)
		(property "Value" "A3P125-PQG208"
			(at 43.18 96.52 0)
		)
		(property "Footprint" "Package_QFP:PQFP-208_28x28mm_P0.5mm"
			(at 43.18 93.98 0)
		)
		(property "Datasheet" "http://www.microsemi.com/document-portal/doc_download/130704-proasic3-flash-family-fpgas-datasheet"
			(at 0 -21.59 0)
		)
		(property "Description" "Actel ProASIC3 Flash Family FPGAs, 1024MCB, 208pin QFP"
			(at 0 0 0)
		)
		(property "ki_keywords" "ProASIC3 ACTEL FLASH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFP*28x28mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "A3P125-PQG208_1_0")
		(symbol "A3P125-PQG208_1_1"
			(pin power_in line
				(at -45.72 91.44 0)
				(length 3.81)
				(name "VJTAG")
				(number "110")
			)
			(pin bidirectional line
				(at -45.72 88.9 0)
				(length 3.81)
				(name "TCK")
				(number "101")
			)
			(pin bidirectional line
				(at -45.72 86.36 0)
				(length 3.81)
				(name "TDI")
				(number "102")
			)
			(pin bidirectional line
				(at -45.72 83.82 0)
				(length 3.81)
				(name "TMS")
				(number "103")
			)
			(pin bidirectional line
				(at -45.72 81.28 0)
				(length 3.81)
				(name "TDO")
				(number "108")
			)
			(pin bidirectional line
				(at -45.72 78.74 0)
				(length 3.81)
				(name "TRST")
				(number "109")
			)
			(pin bidirectional line
				(at -45.72 73.66 0)
				(length 3.81)
				(name "IO67RSB1/GAA2")
				(number "2")
			)
			(pin bidirectional line
				(at -45.72 71.12 0)
				(length 3.81)
				(name "IO68RSB1")
				(number "3")
			)
			(pin bidirectional line
				(at -45.72 68.58 0)
				(length 3.81)
				(name "IO69RSB1/GAB2")
				(number "4")
			)
			(pin bidirectional line
				(at -45.72 66.04 0)
				(length 3.81)
				(name "IO70RSB1/GDA2")
				(number "99")
			)
			(pin bidirectional line
				(at -45.72 63.5 0)
				(length 3.81)
				(name "IO71RSB1/GDB2")
				(number "98")
			)
			(pin bidirectional line
				(at -45.72 60.96 0)
				(length 3.81)
				(name "IO72RSB1/GDC2")
				(number "96")
			)
			(pin bidirectional line
				(at -45.72 58.42 0)
				(length 3.81)
				(name "IO73RSB1")
				(number "95")
			)
			(pin bidirectional line
				(at -45.72 55.88 0)
				(length 3.81)
				(name "IO74RSB1")
				(number "94")
			)
			(pin bidirectional line
				(at -45.72 53.34 0)
				(length 3.81)
				(name "IO75RSB1")
				(number "93")
			)
			(pin bidirectional line
				(at -45.72 50.8 0)
				(length 3.81)
				(name "IO76RSB1")
				(number "92")
			)
			(pin bidirectional line
				(at -45.72 48.26 0)
				(length 3.81)
				(name "IO77RSB1")
				(number "91")
			)
			(pin bidirectional line
				(at -45.72 45.72 0)
				(length 3.81)
				(name "IO78RSB1")
				(number "90")
			)
			(pin bidirectional line
				(at -45.72 43.18 0)
				(length 3.81)
				(name "IO79RSB1")
				(number "87")
			)
			(pin bidirectional line
				(at -45.72 40.64 0)
				(length 3.81)
				(name "IO80RSB1")
				(number "86")
			)
			(pin bidirectional line
				(at -45.72 38.1 0)
				(length 3.81)
				(name "IO81RSB1")
				(number "85")
			)
			(pin bidirectional line
				(at -45.72 35.56 0)
				(length 3.81)
				(name "IO82RSB1")
				(number "84")
			)
			(pin bidirectional line
				(at -45.72 33.02 0)
				(length 3.81)
				(name "IO83RSB1")
				(number "83")
			)
			(pin bidirectional line
				(at -45.72 30.48 0)
				(length 3.81)
				(name "IO84RSB1")
				(number "82")
			)
			(pin bidirectional line
				(at -45.72 27.94 0)
				(length 3.81)
				(name "IO85RSB1")
				(number "80")
			)
			(pin bidirectional line
				(at -45.72 25.4 0)
				(length 3.81)
				(name "IO86RSB1")
				(number "79")
			)
			(pin bidirectional line
				(at -45.72 22.86 0)
				(length 3.81)
				(name "IO87RSB1")
				(number "78")
			)
			(pin bidirectional line
				(at -45.72 20.32 0)
				(length 3.81)
				(name "IO88RSB1")
				(number "77")
			)
			(pin bidirectional line
				(at -45.72 17.78 0)
				(length 3.81)
				(name "IO89RSB1")
				(number "76")
			)
			(pin bidirectional line
				(at -45.72 15.24 0)
				(length 3.81)
				(name "IO90RSB1")
				(number "75")
			)
			(pin bidirectional line
				(at -45.72 12.7 0)
				(length 3.81)
				(name "IO91RSB1")
				(number "74")
			)
			(pin bidirectional line
				(at -45.72 10.16 0)
				(length 3.81)
				(name "IO92RSB1")
				(number "73")
			)
			(pin bidirectional line
				(at -45.72 7.62 0)
				(length 3.81)
				(name "IO93RSB1")
				(number "70")
			)
			(pin bidirectional line
				(at -45.72 5.08 0)
				(length 3.81)
				(name "IO94RSB1")
				(number "69")
			)
			(pin bidirectional line
				(at -45.72 2.54 0)
				(length 3.81)
				(name "IO95RSB1")
				(number "68")
			)
			(pin bidirectional line
				(at -45.72 0 0)
				(length 3.81)
				(name "IO96RSB1")
				(number "67")
			)
			(pin bidirectional line
				(at -45.72 -2.54 0)
				(length 3.81)
				(name "IO97RSB1")
				(number "66")
			)
			(pin bidirectional line
				(at -45.72 -5.08 0)
				(length 3.81)
				(name "IO98RSB1")
				(number "64")
			)
			(pin bidirectional line
				(at -45.72 -7.62 0)
				(length 3.81)
				(name "IO99RSB1")
				(number "63")
			)
			(pin bidirectional line
				(at -45.72 -10.16 0)
				(length 3.81)
				(name "IO100RSB1")
				(number "61")
			)
			(pin bidirectional line
				(at -45.72 -12.7 0)
				(length 3.81)
				(name "IO101RSB1")
				(number "60")
			)
			(pin bidirectional line
				(at -45.72 -15.24 0)
				(length 3.81)
				(name "IO102RSB1")
				(number "59")
			)
			(pin bidirectional line
				(at -45.72 -17.78 0)
				(length 3.81)
				(name "IO103RSB1")
				(number "58")
			)
			(pin bidirectional line
				(at -45.72 -20.32 0)
				(length 3.81)
				(name "IO104RSB1/GEC2")
				(number "57")
			)
			(pin bidirectional line
				(at -45.72 -22.86 0)
				(length 3.81)
				(name "IO105RSB1/GEB2")
				(number "56")
			)
			(pin bidirectional line
				(at -45.72 -25.4 0)
				(length 3.81)
				(name "IO106RSB1/GEA2")
				(number "55")
			)
			(pin bidirectional line
				(at -45.72 -27.94 0)
				(length 3.81)
				(name "IO107RSB1/GEA0")
				(number "49")
			)
			(pin bidirectional line
				(at -45.72 -30.48 0)
				(length 3.81)
				(name "IO108RSB1/GEA1")
				(number "48")
			)
			(pin bidirectional line
				(at -45.72 -33.02 0)
				(length 3.81)
				(name "IO109PDB1/GEB0")
				(number "47")
			)
			(pin bidirectional line
				(at -45.72 -35.56 0)
				(length 3.81)
				(name "IO110RSB1/GEB1")
				(number "46")
			)
			(pin bidirectional line
				(at -45.72 -38.1 0)
				(length 3.81)
				(name "IO111RSB1/GEC0")
				(number "45")
			)
			(pin bidirectional line
				(at -45.72 -40.64 0)
				(length 3.81)
				(name "IO112RSB1/GEC1")
				(number "44")
			)
			(pin bidirectional line
				(at -45.72 -43.18 0)
				(length 3.81)
				(name "IO113RSB1")
				(number "43")
			)
			(pin bidirectional line
				(at -45.72 -45.72 0)
				(length 3.81)
				(name "IO114RSB1")
				(number "42")
			)
			(pin bidirectional line
				(at -45.72 -48.26 0)
				(length 3.81)
				(name "IO115RSB1")
				(number "38")
			)
			(pin bidirectional line
				(at -45.72 -50.8 0)
				(length 3.81)
				(name "IO116PDB1")
				(number "37")
			)
			(pin bidirectional line
				(at -45.72 -53.34 0)
				(length 3.81)
				(name "IO117RSB1")
				(number "35")
			)
			(pin bidirectional line
				(at -45.72 -55.88 0)
				(length 3.81)
				(name "IO118RSB1/GFC2")
				(number "34")
			)
			(pin bidirectional line
				(at -45.72 -58.42 0)
				(length 3.81)
				(name "IO119RSB1/GFB2")
				(number "32")
			)
			(pin bidirectional line
				(at -45.72 -60.96 0)
				(length 3.81)
				(name "IO120RSB1/GFA2")
				(number "30")
			)
			(pin bidirectional line
				(at -45.72 -63.5 0)
				(length 3.81)
				(name "IO121RSB1/GFA1")
				(number "28")
			)
			(pin bidirectional line
				(at -45.72 -66.04 0)
				(length 3.81)
				(name "IO122RSB1/GFA0")
				(number "26")
			)
			(pin bidirectional line
				(at -45.72 -68.58 0)
				(length 3.81)
				(name "IO123RSB1/GFB0")
				(number "24")
			)
			(pin bidirectional line
				(at -45.72 -71.12 0)
				(length 3.81)
				(name "IO124RSB1/GFB1")
				(number "23")
			)
			(pin bidirectional line
				(at -45.72 -73.66 0)
				(length 3.81)
				(name "IO125RSB1/GFC0")
				(number "22")
			)
			(pin bidirectional line
				(at -45.72 -76.2 0)
				(length 3.81)
				(name "IO126RSB1/GFC1")
				(number "21")
			)
			(pin bidirectional line
				(at -45.72 -78.74 0)
				(length 3.81)
				(name "IO127RSB1")
				(number "19")
			)
			(pin bidirectional line
				(at -45.72 -81.28 0)
				(length 3.81)
				(name "IO128RSB1")
				(number "12")
			)
			(pin bidirectional line
				(at -45.72 -83.82 0)
				(length 3.81)
				(name "IO129RSB1")
				(number "10")
			)
			(pin bidirectional line
				(at -45.72 -86.36 0)
				(length 3.81)
				(name "IO130RSB1")
				(number "9")
			)
			(pin bidirectional line
				(at -45.72 -88.9 0)
				(length 3.81)
				(name "IO131RSB1/GAC2")
				(number "6")
			)
			(pin bidirectional line
				(at -45.72 -91.44 0)
				(length 3.81)
				(name "IO132RSB1")
				(number "5")
			)
			(pin power_in line
				(at -33.02 104.14 270)
				(length 3.81)
				(name "VCCPLF")
				(number "27")
			)
			(pin power_in line
				(at -27.94 104.14 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at -27.94 -104.14 90)
				(length 3.81)
				(name "VCOMPLF")
				(number "25")
			)
			(pin power_in line
				(at -25.4 104.14 270)
				(length 3.81)
				(name "VCC")
				(number "71")
			)
			(pin power_in line
				(at -22.86 104.14 270)
				(length 3.81)
				(name "VCC")
				(number "88")
			)
			(pin power_in line
				(at -22.86 -104.14 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -20.32 104.14 270)
				(length 3.81)
				(name "VCC")
				(number "126")
			)
			(pin power_in line
				(at -20.32 -104.14 90)
				(length 3.81)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at -17.78 104.14 270)
				(length 3.81)
				(name "VCC")
				(number "142")
			)
			(pin power_in line
				(at -17.78 -104.14 90)
				(length 3.81)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at -15.24 104.14 270)
				(length 3.81)
				(name "VCC")
				(number "171")
			)
			(pin power_in line
				(at -15.24 -104.14 90)
				(length 3.81)
				(name "GND")
				(number "41")
			)
			(pin power_in line
				(at -12.7 104.14 270)
				(length 3.81)
				(name "VCC")
				(number "187")
			)
			(pin power_in line
				(at -12.7 -104.14 90)
				(length 3.81)
				(name "GND")
				(number "52")
			)
			(pin power_in line
				(at -10.16 -104.14 90)
				(length 3.81)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at -7.62 104.14 270)
				(length 3.81)
				(name "VCCIB0")
				(number "200")
			)
			(pin power_in line
				(at -7.62 -104.14 90)
				(length 3.81)
				(name "GND")
				(number "81")
			)
			(pin power_in line
				(at -5.08 104.14 270)
				(length 3.81)
				(name "VCCIB0")
				(number "186")
			)
			(pin power_in line
				(at -5.08 -104.14 90)
				(length 3.81)
				(name "GND")
				(number "97")
			)
			(pin power_in line
				(at -2.54 104.14 270)
				(length 3.81)
				(name "VCCIB0")
				(number "170")
			)
			(pin power_in line
				(at -2.54 -104.14 90)
				(length 3.81)
				(name "GND")
				(number "105")
			)
			(pin power_in line
				(at 0 104.14 270)
				(length 3.81)
				(name "VCCIB0")
				(number "140")
			)
			(pin power_in line
				(at 0 -104.14 90)
				(length 3.81)
				(name "GND")
				(number "122")
			)
			(pin power_in line
				(at 2.54 104.14 270)
				(length 3.81)
				(name "VCCIB0")
				(number "123")
			)
			(pin power_in line
				(at 2.54 -104.14 90)
				(length 3.81)
				(name "GND")
				(number "130")
			)
			(pin power_in line
				(at 5.08 104.14 270)
				(length 3.81)
				(name "VCCIB1")
				(number "89")
			)
			(pin power_in line
				(at 5.08 -104.14 90)
				(length 3.81)
				(name "GND")
				(number "141")
			)
			(pin power_in line
				(at 7.62 104.14 270)
				(length 3.81)
				(name "VCCIB1")
				(number "72")
			)
			(pin power_in line
				(at 7.62 -104.14 90)
				(length 3.81)
				(name "GND")
				(number "156")
			)
			(pin power_in line
				(at 10.16 104.14 270)
				(length 3.81)
				(name "VCCIB1")
				(number "62")
			)
			(pin power_in line
				(at 10.16 -104.14 90)
				(length 3.81)
				(name "GND")
				(number "162")
			)
			(pin power_in line
				(at 12.7 104.14 270)
				(length 3.81)
				(name "VCCIB1")
				(number "40")
			)
			(pin power_in line
				(at 12.7 -104.14 90)
				(length 3.81)
				(name "GND")
				(number "178")
			)
			(pin power_in line
				(at 15.24 104.14 270)
				(length 3.81)
				(name "VCCIB1")
				(number "18")
			)
			(pin power_in line
				(at 15.24 -104.14 90)
				(length 3.81)
				(name "GND")
				(number "195")
			)
			(pin power_in line
				(at 20.32 104.14 270)
				(length 3.81)
				(name "VMV0")
				(number "208")
			)
			(pin power_in line
				(at 20.32 -104.14 90)
				(length 3.81)
				(name "GNDQ")
				(number "51")
			)
			(pin power_in line
				(at 22.86 104.14 270)
				(length 3.81)
				(name "VMV0")
				(number "154")
			)
			(pin power_in line
				(at 22.86 -104.14 90)
				(length 3.81)
				(name "GNDQ")
				(number "100")
			)
			(pin power_in line
				(at 25.4 104.14 270)
				(length 3.81)
				(name "VMV1")
				(number "104")
			)
			(pin power_in line
				(at 25.4 -104.14 90)
				(length 3.81)
				(name "GNDQ")
				(number "155")
			)
			(pin power_in line
				(at 27.94 104.14 270)
				(length 3.81)
				(name "VMV1")
				(number "50")
			)
			(pin power_in line
				(at 27.94 -104.14 90)
				(length 3.81)
				(name "GNDQ")
				(number "207")
			)
			(pin power_in line
				(at 33.02 104.14 270)
				(length 3.81)
				(name "VPUMP")
				(number "106")
			)
			(pin bidirectional line
				(at 45.72 76.2 180)
				(length 3.81)
				(name "GAA0/IO00RSB0")
				(number "206")
			)
			(pin bidirectional line
				(at 45.72 73.66 180)
				(length 3.81)
				(name "GAA1/IO01RSB0")
				(number "205")
			)
			(pin bidirectional line
				(at 45.72 71.12 180)
				(length 3.81)
				(name "GAB0/IO02RSB0")
				(number "204")
			)
			(pin bidirectional line
				(at 45.72 68.58 180)
				(length 3.81)
				(name "GAB1/IO03RSB0")
				(number "203")
			)
			(pin bidirectional line
				(at 45.72 66.04 180)
				(length 3.81)
				(name "GAC0/IO04RSB0")
				(number "202")
			)
			(pin bidirectional line
				(at 45.72 63.5 180)
				(length 3.81)
				(name "GAC1/IO05RSB0")
				(number "201")
			)
			(pin bidirectional line
				(at 45.72 60.96 180)
				(length 3.81)
				(name "IO06RSB0")
				(number "199")
			)
			(pin bidirectional line
				(at 45.72 58.42 180)
				(length 3.81)
				(name "IO07RSB0")
				(number "198")
			)
			(pin bidirectional line
				(at 45.72 55.88 180)
				(length 3.81)
				(name "IO08RSB0")
				(number "197")
			)
			(pin bidirectional line
				(at 45.72 53.34 180)
				(length 3.81)
				(name "IO09RSB0")
				(number "196")
			)
			(pin bidirectional line
				(at 45.72 50.8 180)
				(length 3.81)
				(name "IO10RSB0")
				(number "194")
			)
			(pin bidirectional line
				(at 45.72 48.26 180)
				(length 3.81)
				(name "IO11RSB0")
				(number "193")
			)
			(pin bidirectional line
				(at 45.72 45.72 180)
				(length 3.81)
				(name "IO12RSB0")
				(number "192")
			)
			(pin bidirectional line
				(at 45.72 43.18 180)
				(length 3.81)
				(name "IO13RSB0")
				(number "191")
			)
			(pin bidirectional line
				(at 45.72 40.64 180)
				(length 3.81)
				(name "IO14RSB0")
				(number "190")
			)
			(pin bidirectional line
				(at 45.72 38.1 180)
				(length 3.81)
				(name "IO15RSB0")
				(number "189")
			)
			(pin bidirectional line
				(at 45.72 35.56 180)
				(length 3.81)
				(name "IO16RSB0")
				(number "188")
			)
			(pin bidirectional line
				(at 45.72 33.02 180)
				(length 3.81)
				(name "IO17RSB0")
				(number "185")
			)
			(pin bidirectional line
				(at 45.72 30.48 180)
				(length 3.81)
				(name "IO18RSB0")
				(number "184")
			)
			(pin bidirectional line
				(at 45.72 27.94 180)
				(length 3.81)
				(name "IO19RSB0")
				(number "183")
			)
			(pin bidirectional line
				(at 45.72 25.4 180)
				(length 3.81)
				(name "IO20RSB0")
				(number "182")
			)
			(pin bidirectional line
				(at 45.72 22.86 180)
				(length 3.81)
				(name "IO21RSB0")
				(number "181")
			)
			(pin bidirectional line
				(at 45.72 20.32 180)
				(length 3.81)
				(name "IO22RSB0")
				(number "180")
			)
			(pin bidirectional line
				(at 45.72 17.78 180)
				(length 3.81)
				(name "IO23RSB0")
				(number "179")
			)
			(pin bidirectional line
				(at 45.72 15.24 180)
				(length 3.81)
				(name "IO24RSB0")
				(number "177")
			)
			(pin bidirectional line
				(at 45.72 12.7 180)
				(length 3.81)
				(name "IO25RSB0")
				(number "176")
			)
			(pin bidirectional line
				(at 45.72 10.16 180)
				(length 3.81)
				(name "IO26RSB0")
				(number "175")
			)
			(pin bidirectional line
				(at 45.72 7.62 180)
				(length 3.81)
				(name "IO27RSB0")
				(number "174")
			)
			(pin bidirectional line
				(at 45.72 5.08 180)
				(length 3.81)
				(name "IO28RSB0")
				(number "173")
			)
			(pin bidirectional line
				(at 45.72 2.54 180)
				(length 3.81)
				(name "IO29RSB0")
				(number "172")
			)
			(pin bidirectional line
				(at 45.72 0 180)
				(length 3.81)
				(name "IO30RSB0")
				(number "169")
			)
			(pin bidirectional line
				(at 45.72 -2.54 180)
				(length 3.81)
				(name "IO31RSB0")
				(number "168")
			)
			(pin bidirectional line
				(at 45.72 -5.08 180)
				(length 3.81)
				(name "IO32RSB0")
				(number "167")
			)
			(pin bidirectional line
				(at 45.72 -7.62 180)
				(length 3.81)
				(name "IO33RSB0")
				(number "166")
			)
			(pin bidirectional line
				(at 45.72 -10.16 180)
				(length 3.81)
				(name "IO34RSB0")
				(number "165")
			)
			(pin bidirectional line
				(at 45.72 -12.7 180)
				(length 3.81)
				(name "GBC0/IO35RSB0")
				(number "164")
			)
			(pin bidirectional line
				(at 45.72 -15.24 180)
				(length 3.81)
				(name "GBC1/IO36RSB0")
				(number "163")
			)
			(pin bidirectional line
				(at 45.72 -17.78 180)
				(length 3.81)
				(name "GBB0/IO37RSB0")
				(number "161")
			)
			(pin bidirectional line
				(at 45.72 -20.32 180)
				(length 3.81)
				(name "GBB1/IO38RSB0")
				(number "160")
			)
			(pin bidirectional line
				(at 45.72 -22.86 180)
				(length 3.81)
				(name "GBA0/IO39RSB0")
				(number "159")
			)
			(pin bidirectional line
				(at 45.72 -25.4 180)
				(length 3.81)
				(name "GBA1/IO40RSB0")
				(number "158")
			)
			(pin bidirectional line
				(at 45.72 -27.94 180)
				(length 3.81)
				(name "GBA2/IO41RSB0")
				(number "153")
			)
			(pin bidirectional line
				(at 45.72 -30.48 180)
				(length 3.81)
				(name "IO42RSB0")
				(number "152")
			)
			(pin bidirectional line
				(at 45.72 -33.02 180)
				(length 3.81)
				(name "GBB2/IO43RSB0")
				(number "151")
			)
			(pin bidirectional line
				(at 45.72 -35.56 180)
				(length 3.81)
				(name "IO44RSB0")
				(number "150")
			)
			(pin bidirectional line
				(at 45.72 -38.1 180)
				(length 3.81)
				(name "GBC2/IO45RSB0")
				(number "149")
			)
			(pin bidirectional line
				(at 45.72 -40.64 180)
				(length 3.81)
				(name "IO46RSB0")
				(number "145")
			)
			(pin bidirectional line
				(at 45.72 -43.18 180)
				(length 3.81)
				(name "IO47RSB0")
				(number "144")
			)
			(pin bidirectional line
				(at 45.72 -45.72 180)
				(length 3.81)
				(name "IO48RSB0")
				(number "143")
			)
			(pin bidirectional line
				(at 45.72 -48.26 180)
				(length 3.81)
				(name "IO49RSB0")
				(number "139")
			)
			(pin bidirectional line
				(at 45.72 -50.8 180)
				(length 3.81)
				(name "IO50RSB0")
				(number "138")
			)
			(pin bidirectional line
				(at 45.72 -53.34 180)
				(length 3.81)
				(name "GCC1/IO51RSB0")
				(number "137")
			)
			(pin bidirectional line
				(at 45.72 -55.88 180)
				(length 3.81)
				(name "GCC0/IO52RSB0")
				(number "136")
			)
			(pin bidirectional line
				(at 45.72 -58.42 180)
				(length 3.81)
				(name "GCB1/IO53RSB0")
				(number "135")
			)
			(pin bidirectional line
				(at 45.72 -60.96 180)
				(length 3.81)
				(name "GCB0/IO54RSB0")
				(number "134")
			)
			(pin bidirectional line
				(at 45.72 -63.5 180)
				(length 3.81)
				(name "GCA1/IO55RSB0")
				(number "133")
			)
			(pin bidirectional line
				(at 45.72 -66.04 180)
				(length 3.81)
				(name "GCA0/IO56RSB0")
				(number "132")
			)
			(pin bidirectional line
				(at 45.72 -68.58 180)
				(length 3.81)
				(name "GCA2/IO57RSB0")
				(number "131")
			)
			(pin bidirectional line
				(at 45.72 -71.12 180)
				(length 3.81)
				(name "GCB2/IO58RSB0")
				(number "129")
			)
			(pin bidirectional line
				(at 45.72 -73.66 180)
				(length 3.81)
				(name "GCC2/IO59RSB0")
				(number "128")
			)
			(pin bidirectional line
				(at 45.72 -76.2 180)
				(length 3.81)
				(name "IO60RSB0")
				(number "127")
			)
			(pin bidirectional line
				(at 45.72 -78.74 180)
				(length 3.81)
				(name "GDC1/IO61RSB0")
				(number "116")
			)
			(pin bidirectional line
				(at 45.72 -81.28 180)
				(length 3.81)
				(name "GDC0/IO62RSB0")
				(number "115")
			)
			(pin bidirectional line
				(at 45.72 -83.82 180)
				(length 3.81)
				(name "GDB1/IO63RSB0")
				(number "114")
			)
			(pin bidirectional line
				(at 45.72 -86.36 180)
				(length 3.81)
				(name "GDB0/IO64RSB0")
				(number "113")
			)
			(pin bidirectional line
				(at 45.72 -88.9 180)
				(length 3.81)
				(name "GDA1/IO65RSB0")
				(number "112")
			)
			(pin bidirectional line
				(at 45.72 -91.44 180)
				(length 3.81)
				(name "GDA0/IO66RSB0")
				(number "111")
			)
		)
		(embedded_fonts no)
	)
	(symbol "A3P125-VQG100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 30.48 55.88 0)
		)
		(property "Value" "A3P125-VQG100"
			(at 30.48 53.34 0)
		)
		(property "Footprint" "Package_QFP:VQFP-100_14x14mm_P0.5mm"
			(at 30.48 50.8 0)
		)
		(property "Datasheet" "http://www.microsemi.com/document-portal/doc_download/130704-proasic3-flash-family-fpgas-datasheet"
			(at 0 0 0)
		)
		(property "Description" "Actel ProASIC3 Flash Family FPGAs, 1024 MCLB, 100pin QFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "ProASIC3 ACTEL FLASH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "A3P125-VQG100_0_1")
		(symbol "A3P125-VQG100_1_1"
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 3.81)
				(name "VJTAG")
				(number "56")
			)
			(pin bidirectional line
				(at -33.02 50.8 0)
				(length 3.81)
				(name "TCK")
				(number "47")
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 3.81)
				(name "TDI")
				(number "48")
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 3.81)
				(name "TMS")
				(number "49")
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 3.81)
				(name "TDO")
				(number "54")
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 3.81)
				(name "TRST")
				(number "55")
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 3.81)
				(name "IO132RSB1")
				(number "5")
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 3.81)
				(name "IO131RSB1/GAC2")
				(number "6")
			)
			(pin input line
				(at -33.02 30.48 0)
				(length 3.81)
				(name "IO130RSB1")
				(number "7")
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 3.81)
				(name "IO129RSB1")
				(number "8")
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 3.81)
				(name "IO124RSB1/GFB1")
				(number "10")
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 3.81)
				(name "IO123RSB1/GFB0")
				(number "11")
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 3.81)
				(name "IO122RSB1/GFA0")
				(number "13")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 3.81)
				(name "IO121RSB1/GFA1")
				(number "15")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 3.81)
				(name "IO120RSB1/GFA2")
				(number "16")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 3.81)
				(name "IO111RSB1/GEC0")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 3.81)
				(name "IO109RSB1/GEB1")
				(number "21")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "IO110RSB1/GEB1")
				(number "20")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 3.81)
				(name "IO108RSB1/GEA1")
				(number "22")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 3.81)
				(name "IO107RSB1/GEA0")
				(number "23")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 3.81)
				(name "IO106RSB1/GEA2")
				(number "26")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 3.81)
				(name "IO105RSB1/GEB2")
				(number "27")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 3.81)
				(name "IO104RSB1/GEC2")
				(number "28")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 3.81)
				(name "IO102RSB1")
				(number "29")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 3.81)
				(name "IO100RSB1")
				(number "30")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 3.81)
				(name "IO99RSB1")
				(number "31")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 3.81)
				(name "IO97RSB1")
				(number "32")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 3.81)
				(name "IO96RSB1")
				(number "33")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 3.81)
				(name "IO95RSB1")
				(number "34")
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 3.81)
				(name "IO94RSB1")
				(number "35")
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 3.81)
				(name "IO93RSB1")
				(number "36")
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 3.81)
				(name "IO87RSB1")
				(number "40")
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 3.81)
				(name "IO84RSB1")
				(number "41")
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 3.81)
				(name "IO81RSB1")
				(number "42")
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 3.81)
				(name "IO75RSB1")
				(number "43")
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 3.81)
				(name "IO72RSB1/GDC2")
				(number "44")
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 3.81)
				(name "IO71RSB1/GDB2")
				(number "45")
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 3.81)
				(name "IO70RSB1/GDA2")
				(number "46")
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 3.81)
				(name "IO69RSB1/GAB2")
				(number "4")
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 3.81)
				(name "IO68RSB1")
				(number "3")
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 3.81)
				(name "IO67RSB1/GAA2")
				(number "2")
			)
			(pin power_in line
				(at -20.32 60.96 270)
				(length 3.81)
				(name "VCCPLF")
				(number "14")
			)
			(pin power_in line
				(at -15.24 60.96 270)
				(length 3.81)
				(name "VCC")
				(number "17")
			)
			(pin power_in line
				(at -12.7 60.96 270)
				(length 3.81)
				(name "VCC")
				(number "37")
			)
			(pin power_in line
				(at -12.7 -60.96 90)
				(length 3.81)
				(name "VCOMPLF")
				(number "12")
			)
			(pin power_in line
				(at -10.16 60.96 270)
				(length 3.81)
				(name "VCC")
				(number "68")
			)
			(pin power_in line
				(at -7.62 60.96 270)
				(length 3.81)
				(name "VCC")
				(number "89")
			)
			(pin power_in line
				(at -7.62 -60.96 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -60.96 90)
				(length 3.81)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at -2.54 60.96 270)
				(length 3.81)
				(name "VCCIB1")
				(number "18")
			)
			(pin power_in line
				(at -2.54 -60.96 90)
				(length 3.81)
				(name "GND")
				(number "38")
			)
			(pin power_in line
				(at 0 60.96 270)
				(length 3.81)
				(name "VCCIB1")
				(number "39")
			)
			(pin power_in line
				(at 0 -60.96 90)
				(length 3.81)
				(name "GND")
				(number "51")
			)
			(pin power_in line
				(at 2.54 60.96 270)
				(length 3.81)
				(name "VCCIB0")
				(number "66")
			)
			(pin power_in line
				(at 2.54 -60.96 90)
				(length 3.81)
				(name "GND")
				(number "67")
			)
			(pin power_in line
				(at 5.08 60.96 270)
				(length 3.81)
				(name "VCCIB0")
				(number "87")
			)
			(pin power_in line
				(at 5.08 -60.96 90)
				(length 3.81)
				(name "GND")
				(number "88")
			)
			(pin power_in line
				(at 10.16 60.96 270)
				(length 3.81)
				(name "VMV1")
				(number "24")
			)
			(pin power_in line
				(at 10.16 -60.96 90)
				(length 3.81)
				(name "GNDQ")
				(number "25")
			)
			(pin power_in line
				(at 12.7 60.96 270)
				(length 3.81)
				(name "VMV1")
				(number "50")
			)
			(pin power_in line
				(at 12.7 -60.96 90)
				(length 3.81)
				(name "GNDQ")
				(number "75")
			)
			(pin power_in line
				(at 15.24 60.96 270)
				(length 3.81)
				(name "VMV0")
				(number "74")
			)
			(pin power_in line
				(at 20.32 60.96 270)
				(length 3.81)
				(name "VPUMP")
				(number "52")
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 3.81)
				(name "GAA0/IO00RSB0")
				(number "100")
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 3.81)
				(name "GAA1/IO01RSB0")
				(number "99")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 3.81)
				(name "GAB0/IO02RSB0")
				(number "98")
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 3.81)
				(name "GAB1/IO03RSB0")
				(number "97")
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 3.81)
				(name "GAC0/IO04RSB0")
				(number "96")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "GAC1/IO05RSB0")
				(number "95")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 3.81)
				(name "IO07RSB0")
				(number "94")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "IO09RSB0")
				(number "93")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "IO11RSB0")
				(number "92")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "IO13RSB0")
				(number "91")
			)
			(pin input line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "IO15RSB0")
				(number "90")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "IO19RSB0")
				(number "86")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "IO22RSB0")
				(number "85")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "IO25RSB0")
				(number "84")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "IO28RSB0")
				(number "83")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 3.81)
				(name "IO32RSB0")
				(number "82")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "GBC0/IO35RSB0")
				(number "81")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "GBC1/IO36RSB0")
				(number "80")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "GBB0/IO37RSB0")
				(number "79")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "GBB1/IO38RSB0")
				(number "78")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "GBA0/IO39RSB0")
				(number "77")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "GBA1/IO40RSB0")
				(number "76")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "GBA2/IO41RSB0")
				(number "73")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 3.81)
				(name "IO42RSB0")
				(number "72")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 3.81)
				(name "GBB2/IO43RSB0")
				(number "71")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 3.81)
				(name "GBC2/IO45RSB0")
				(number "70")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 3.81)
				(name "IO47RSB1")
				(number "69")
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 3.81)
				(name "GCC1/IO51RSB0")
				(number "65")
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 3.81)
				(name "GCC0/IO52RSB0")
				(number "64")
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 3.81)
				(name "GCA1/IO55RSB0")
				(number "63")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 3.81)
				(name "GCA0/IO56RSB0")
				(number "62")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 3.81)
				(name "GCB2/IO58RSB0")
				(number "61")
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 3.81)
				(name "GCC2/IO59RSB0")
				(number "60")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 3.81)
				(name "GDC1/IO61RSB0")
				(number "59")
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 3.81)
				(name "GDC0/IO62RSB0")
				(number "58")
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 3.81)
				(name "GDA1/IO65RSB0")
				(number "57")
			)
		)
		(embedded_fonts no)
	)
	(symbol "A3P250-PQG208"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 43.18 111.76 0)
		)
		(property "Value" "A3P250-PQG208"
			(at 43.18 109.22 0)
		)
		(property "Footprint" "Package_QFP:PQFP-208_28x28mm_P0.5mm"
			(at 43.18 106.68 0)
		)
		(property "Datasheet" "http://www.microsemi.com/document-portal/doc_download/130704-proasic3-flash-family-fpgas-datasheet"
			(at 0 -7.62 0)
		)
		(property "Description" "Actel ProASIC3 Flash Family FPGAs, 2048MCB, 208pin QFP"
			(at 0 0 0)
		)
		(property "ki_keywords" "ProASIC3 ACTEL FLASH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFP*28x28mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "A3P250-PQG208_1_0")
		(symbol "A3P250-PQG208_1_1"
			(pin power_in line
				(at -45.72 109.22 0)
				(length 3.81)
				(name "VJTAG")
				(number "110")
			)
			(pin bidirectional line
				(at -45.72 106.68 0)
				(length 3.81)
				(name "TCK")
				(number "101")
			)
			(pin bidirectional line
				(at -45.72 104.14 0)
				(length 3.81)
				(name "TDI")
				(number "102")
			)
			(pin bidirectional line
				(at -45.72 101.6 0)
				(length 3.81)
				(name "TMS")
				(number "103")
			)
			(pin bidirectional line
				(at -45.72 99.06 0)
				(length 3.81)
				(name "TDO")
				(number "108")
			)
			(pin bidirectional line
				(at -45.72 96.52 0)
				(length 3.81)
				(name "TRST")
				(number "109")
			)
			(pin bidirectional line
				(at -45.72 91.44 0)
				(length 3.81)
				(name "IO98NDB3/GEA0")
				(number "49")
			)
			(pin bidirectional line
				(at -45.72 88.9 0)
				(length 3.81)
				(name "IO98PDB3/GEA1")
				(number "48")
			)
			(pin bidirectional line
				(at -45.72 86.36 0)
				(length 3.81)
				(name "IO99NDB3/GEB0")
				(number "47")
			)
			(pin bidirectional line
				(at -45.72 83.82 0)
				(length 3.81)
				(name "IO99PDB3/GEB1")
				(number "46")
			)
			(pin bidirectional line
				(at -45.72 81.28 0)
				(length 3.81)
				(name "IO100NDB3/GEC0")
				(number "45")
			)
			(pin bidirectional line
				(at -45.72 78.74 0)
				(length 3.81)
				(name "IO100PDB3/GEC1")
				(number "44")
			)
			(pin bidirectional line
				(at -45.72 76.2 0)
				(length 3.81)
				(name "IO101NDB3")
				(number "43")
			)
			(pin bidirectional line
				(at -45.72 73.66 0)
				(length 3.81)
				(name "IO101PDB3")
				(number "42")
			)
			(pin bidirectional line
				(at -45.72 71.12 0)
				(length 3.81)
				(name "IO103PSB3")
				(number "39")
			)
			(pin bidirectional line
				(at -45.72 68.58 0)
				(length 3.81)
				(name "IO104NDB3")
				(number "38")
			)
			(pin bidirectional line
				(at -45.72 66.04 0)
				(length 3.81)
				(name "IO104PDB3")
				(number "37")
			)
			(pin bidirectional line
				(at -45.72 63.5 0)
				(length 3.81)
				(name "IO105NDB3")
				(number "35")
			)
			(pin bidirectional line
				(at -45.72 60.96 0)
				(length 3.81)
				(name "IO105PDB3/GFC2")
				(number "34")
			)
			(pin bidirectional line
				(at -45.72 58.42 0)
				(length 3.81)
				(name "IO106NDB3")
				(number "33")
			)
			(pin bidirectional line
				(at -45.72 55.88 0)
				(length 3.81)
				(name "IO106PDB3/GFB2")
				(number "32")
			)
			(pin bidirectional line
				(at -45.72 53.34 0)
				(length 3.81)
				(name "IO107NDB3")
				(number "31")
			)
			(pin bidirectional line
				(at -45.72 50.8 0)
				(length 3.81)
				(name "IO107PDB3/GFA2")
				(number "30")
			)
			(pin bidirectional line
				(at -45.72 48.26 0)
				(length 3.81)
				(name "IO108PPB3/GFA1")
				(number "28")
			)
			(pin bidirectional line
				(at -45.72 45.72 0)
				(length 3.81)
				(name "IO108NPB3/GFA0")
				(number "26")
			)
			(pin bidirectional line
				(at -45.72 43.18 0)
				(length 3.81)
				(name "IO109NDB3/GFB0")
				(number "24")
			)
			(pin bidirectional line
				(at -45.72 40.64 0)
				(length 3.81)
				(name "IO109PDB3/GFB1")
				(number "23")
			)
			(pin bidirectional line
				(at -45.72 38.1 0)
				(length 3.81)
				(name "IO110NDB3/GFC0")
				(number "22")
			)
			(pin bidirectional line
				(at -45.72 35.56 0)
				(length 3.81)
				(name "IO110PDB3/GFC1")
				(number "21")
			)
			(pin bidirectional line
				(at -45.72 33.02 0)
				(length 3.81)
				(name "IO111NDB3")
				(number "20")
			)
			(pin bidirectional line
				(at -45.72 30.48 0)
				(length 3.81)
				(name "IO111PDB3")
				(number "19")
			)
			(pin bidirectional line
				(at -45.72 27.94 0)
				(length 3.81)
				(name "IO112NDB3")
				(number "15")
			)
			(pin bidirectional line
				(at -45.72 25.4 0)
				(length 3.81)
				(name "IO112PDB3")
				(number "14")
			)
			(pin bidirectional line
				(at -45.72 22.86 0)
				(length 3.81)
				(name "IO113NDB3")
				(number "13")
			)
			(pin bidirectional line
				(at -45.72 20.32 0)
				(length 3.81)
				(name "IO113PDB3")
				(number "12")
			)
			(pin bidirectional line
				(at -45.72 17.78 0)
				(length 3.81)
				(name "IO114VDB3")
				(number "11")
			)
			(pin bidirectional line
				(at -45.72 15.24 0)
				(length 3.81)
				(name "IO114UDB3")
				(number "10")
			)
			(pin bidirectional line
				(at -45.72 12.7 0)
				(length 3.81)
				(name "IO115VDB3")
				(number "9")
			)
			(pin bidirectional line
				(at -45.72 10.16 0)
				(length 3.81)
				(name "IO115UDB3")
				(number "8")
			)
			(pin bidirectional line
				(at -45.72 7.62 0)
				(length 3.81)
				(name "IO116VDB3")
				(number "7")
			)
			(pin bidirectional line
				(at -45.72 5.08 0)
				(length 3.81)
				(name "IO116UDB3/GAC2")
				(number "6")
			)
			(pin bidirectional line
				(at -45.72 2.54 0)
				(length 3.81)
				(name "IO117VDB3")
				(number "5")
			)
			(pin bidirectional line
				(at -45.72 0 0)
				(length 3.81)
				(name "IO117UDB3/GAB2")
				(number "4")
			)
			(pin bidirectional line
				(at -45.72 -2.54 0)
				(length 3.81)
				(name "IO118VDB3")
				(number "3")
			)
			(pin bidirectional line
				(at -45.72 -5.08 0)
				(length 3.81)
				(name "IO118UDB3/GAA2")
				(number "2")
			)
			(pin bidirectional line
				(at -45.72 -10.16 0)
				(length 3.81)
				(name "IO61RSB2/GDA2")
				(number "99")
			)
			(pin bidirectional line
				(at -45.72 -12.7 0)
				(length 3.81)
				(name "IO62RSB2/GDB2")
				(number "98")
			)
			(pin bidirectional line
				(at -45.72 -15.24 0)
				(length 3.81)
				(name "IO63RSB2/GDC2")
				(number "96")
			)
			(pin bidirectional line
				(at -45.72 -17.78 0)
				(length 3.81)
				(name "IO64RSB2")
				(number "95")
			)
			(pin bidirectional line
				(at -45.72 -20.32 0)
				(length 3.81)
				(name "IO65RSB2")
				(number "94")
			)
			(pin bidirectional line
				(at -45.72 -22.86 0)
				(length 3.81)
				(name "IO66RSB2")
				(number "93")
			)
			(pin bidirectional line
				(at -45.72 -25.4 0)
				(length 3.81)
				(name "IO67RSB2")
				(number "92")
			)
			(pin bidirectional line
				(at -45.72 -27.94 0)
				(length 3.81)
				(name "IO68RSB2")
				(number "91")
			)
			(pin bidirectional line
				(at -45.72 -30.48 0)
				(length 3.81)
				(name "IO69RSB2")
				(number "90")
			)
			(pin bidirectional line
				(at -45.72 -33.02 0)
				(length 3.81)
				(name "IO70RSB2")
				(number "87")
			)
			(pin bidirectional line
				(at -45.72 -35.56 0)
				(length 3.81)
				(name "IO71RSB2")
				(number "86")
			)
			(pin bidirectional line
				(at -45.72 -38.1 0)
				(length 3.81)
				(name "IO72RSB2")
				(number "85")
			)
			(pin bidirectional line
				(at -45.72 -40.64 0)
				(length 3.81)
				(name "IO73RSB2")
				(number "84")
			)
			(pin bidirectional line
				(at -45.72 -43.18 0)
				(length 3.81)
				(name "IO74RSB2")
				(number "83")
			)
			(pin bidirectional line
				(at -45.72 -45.72 0)
				(length 3.81)
				(name "IO75RSB2")
				(number "82")
			)
			(pin bidirectional line
				(at -45.72 -48.26 0)
				(length 3.81)
				(name "IO76RSB2")
				(number "80")
			)
			(pin bidirectional line
				(at -45.72 -50.8 0)
				(length 3.81)
				(name "IO77RSB2")
				(number "79")
			)
			(pin bidirectional line
				(at -45.72 -53.34 0)
				(length 3.81)
				(name "IO78RSB2")
				(number "78")
			)
			(pin bidirectional line
				(at -45.72 -55.88 0)
				(length 3.81)
				(name "IO79RSB2")
				(number "77")
			)
			(pin bidirectional line
				(at -45.72 -58.42 0)
				(length 3.81)
				(name "IO80RSB2")
				(number "76")
			)
			(pin bidirectional line
				(at -45.72 -60.96 0)
				(length 3.81)
				(name "IO81RSB2")
				(number "75")
			)
			(pin bidirectional line
				(at -45.72 -63.5 0)
				(length 3.81)
				(name "IO82RSB2")
				(number "74")
			)
			(pin bidirectional line
				(at -45.72 -66.04 0)
				(length 3.81)
				(name "IO83RSB2")
				(number "73")
			)
			(pin bidirectional line
				(at -45.72 -68.58 0)
				(length 3.81)
				(name "IO84RSB2")
				(number "70")
			)
			(pin bidirectional line
				(at -45.72 -71.12 0)
				(length 3.81)
				(name "IO85RSB2")
				(number "69")
			)
			(pin bidirectional line
				(at -45.72 -73.66 0)
				(length 3.81)
				(name "IO86RSB2")
				(number "68")
			)
			(pin bidirectional line
				(at -45.72 -76.2 0)
				(length 3.81)
				(name "IO87RSB2")
				(number "67")
			)
			(pin bidirectional line
				(at -45.72 -78.74 0)
				(length 3.81)
				(name "IO88RSB2")
				(number "66")
			)
			(pin bidirectional line
				(at -45.72 -81.28 0)
				(length 3.81)
				(name "IO89RSB2")
				(number "64")
			)
			(pin bidirectional line
				(at -45.72 -83.82 0)
				(length 3.81)
				(name "IO90RSB2")
				(number "63")
			)
			(pin bidirectional line
				(at -45.72 -86.36 0)
				(length 3.81)
				(name "IO91RSB2")
				(number "61")
			)
			(pin bidirectional line
				(at -45.72 -88.9 0)
				(length 3.81)
				(name "IO92RSB2")
				(number "60")
			)
			(pin bidirectional line
				(at -45.72 -91.44 0)
				(length 3.81)
				(name "IO93RSB2")
				(number "59")
			)
			(pin bidirectional line
				(at -45.72 -93.98 0)
				(length 3.81)
				(name "IO94RSB2")
				(number "58")
			)
			(pin bidirectional line
				(at -45.72 -96.52 0)
				(length 3.81)
				(name "IO95RSB2/GEC2")
				(number "57")
			)
			(pin bidirectional line
				(at -45.72 -99.06 0)
				(length 3.81)
				(name "IO96RSB2/GEB2")
				(number "56")
			)
			(pin bidirectional line
				(at -45.72 -101.6 0)
				(length 3.81)
				(name "IO97RSB2/GEA2")
				(number "55")
			)
			(pin power_in line
				(at -33.02 116.84 270)
				(length 3.81)
				(name "VCCPLF")
				(number "27")
			)
			(pin power_in line
				(at -27.94 116.84 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at -27.94 -116.84 90)
				(length 3.81)
				(name "VCOMPLF")
				(number "25")
			)
			(pin power_in line
				(at -25.4 116.84 270)
				(length 3.81)
				(name "VCC")
				(number "71")
			)
			(pin power_in line
				(at -22.86 116.84 270)
				(length 3.81)
				(name "VCC")
				(number "88")
			)
			(pin power_in line
				(at -22.86 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -20.32 116.84 270)
				(length 3.81)
				(name "VCC")
				(number "126")
			)
			(pin power_in line
				(at -20.32 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 3.81)
				(name "VCC")
				(number "142")
			)
			(pin power_in line
				(at -17.78 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 3.81)
				(name "VCC")
				(number "171")
			)
			(pin power_in line
				(at -15.24 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "41")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 3.81)
				(name "VCC")
				(number "187")
			)
			(pin power_in line
				(at -12.7 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "52")
			)
			(pin power_in line
				(at -10.16 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 3.81)
				(name "VCCIB0")
				(number "200")
			)
			(pin power_in line
				(at -7.62 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "81")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 3.81)
				(name "VCCIB0")
				(number "186")
			)
			(pin power_in line
				(at -5.08 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "97")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 3.81)
				(name "VCCIB0")
				(number "170")
			)
			(pin power_in line
				(at -2.54 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "105")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 3.81)
				(name "VCCIB1")
				(number "140")
			)
			(pin power_in line
				(at 0 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "122")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 3.81)
				(name "VCCIB1")
				(number "123")
			)
			(pin power_in line
				(at 2.54 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "130")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 3.81)
				(name "VCCIB2")
				(number "89")
			)
			(pin power_in line
				(at 5.08 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "141")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 3.81)
				(name "VCCIB2")
				(number "72")
			)
			(pin power_in line
				(at 7.62 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "156")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 3.81)
				(name "VCCIB2")
				(number "62")
			)
			(pin power_in line
				(at 10.16 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "162")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 3.81)
				(name "VCCIB3")
				(number "40")
			)
			(pin power_in line
				(at 12.7 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "178")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 3.81)
				(name "VCCIB3")
				(number "18")
			)
			(pin power_in line
				(at 15.24 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "195")
			)
			(pin power_in line
				(at 20.32 116.84 270)
				(length 3.81)
				(name "VMV0")
				(number "208")
			)
			(pin power_in line
				(at 20.32 -116.84 90)
				(length 3.81)
				(name "GNDQ")
				(number "51")
			)
			(pin power_in line
				(at 22.86 116.84 270)
				(length 3.81)
				(name "VMV1")
				(number "154")
			)
			(pin power_in line
				(at 22.86 -116.84 90)
				(length 3.81)
				(name "GNDQ")
				(number "100")
			)
			(pin power_in line
				(at 25.4 116.84 270)
				(length 3.81)
				(name "VMV2")
				(number "104")
			)
			(pin power_in line
				(at 25.4 -116.84 90)
				(length 3.81)
				(name "GNDQ")
				(number "155")
			)
			(pin power_in line
				(at 27.94 116.84 270)
				(length 3.81)
				(name "VMV3")
				(number "50")
			)
			(pin power_in line
				(at 27.94 -116.84 90)
				(length 3.81)
				(name "GNDQ")
				(number "207")
			)
			(pin power_in line
				(at 33.02 116.84 270)
				(length 3.81)
				(name "VPUMP")
				(number "106")
			)
			(pin bidirectional line
				(at 45.72 91.44 180)
				(length 3.81)
				(name "GAA0/IO00RSB0")
				(number "206")
			)
			(pin bidirectional line
				(at 45.72 88.9 180)
				(length 3.81)
				(name "GAA1/IO01RSB0")
				(number "205")
			)
			(pin bidirectional line
				(at 45.72 86.36 180)
				(length 3.81)
				(name "GAB0/IO02RSB0")
				(number "204")
			)
			(pin bidirectional line
				(at 45.72 83.82 180)
				(length 3.81)
				(name "GAB1/IO03RSB0")
				(number "203")
			)
			(pin bidirectional line
				(at 45.72 81.28 180)
				(length 3.81)
				(name "GAC0/IO04RSB0")
				(number "202")
			)
			(pin bidirectional line
				(at 45.72 78.74 180)
				(length 3.81)
				(name "GAC1/IO05RSB0")
				(number "201")
			)
			(pin bidirectional line
				(at 45.72 76.2 180)
				(length 3.81)
				(name "IO06RSB0")
				(number "199")
			)
			(pin bidirectional line
				(at 45.72 73.66 180)
				(length 3.81)
				(name "IO07RSB0")
				(number "198")
			)
			(pin bidirectional line
				(at 45.72 71.12 180)
				(length 3.81)
				(name "IO08RSB0")
				(number "197")
			)
			(pin bidirectional line
				(at 45.72 68.58 180)
				(length 3.81)
				(name "IO09RSB0")
				(number "196")
			)
			(pin bidirectional line
				(at 45.72 66.04 180)
				(length 3.81)
				(name "IO10RSB0")
				(number "194")
			)
			(pin bidirectional line
				(at 45.72 63.5 180)
				(length 3.81)
				(name "IO11RSB0")
				(number "193")
			)
			(pin bidirectional line
				(at 45.72 60.96 180)
				(length 3.81)
				(name "IO12RSB0")
				(number "192")
			)
			(pin bidirectional line
				(at 45.72 58.42 180)
				(length 3.81)
				(name "IO13RSB0")
				(number "191")
			)
			(pin bidirectional line
				(at 45.72 55.88 180)
				(length 3.81)
				(name "IO14RSB0")
				(number "190")
			)
			(pin bidirectional line
				(at 45.72 53.34 180)
				(length 3.81)
				(name "IO15RSB0")
				(number "189")
			)
			(pin bidirectional line
				(at 45.72 50.8 180)
				(length 3.81)
				(name "IO16RSB0")
				(number "188")
			)
			(pin bidirectional line
				(at 45.72 48.26 180)
				(length 3.81)
				(name "IO17RSB0")
				(number "185")
			)
			(pin bidirectional line
				(at 45.72 45.72 180)
				(length 3.81)
				(name "IO18RSB0")
				(number "184")
			)
			(pin bidirectional line
				(at 45.72 43.18 180)
				(length 3.81)
				(name "IO19RSB0")
				(number "183")
			)
			(pin bidirectional line
				(at 45.72 40.64 180)
				(length 3.81)
				(name "IO20RSB0")
				(number "182")
			)
			(pin bidirectional line
				(at 45.72 38.1 180)
				(length 3.81)
				(name "IO21RSB0")
				(number "181")
			)
			(pin bidirectional line
				(at 45.72 35.56 180)
				(length 3.81)
				(name "IO22RSB0")
				(number "180")
			)
			(pin bidirectional line
				(at 45.72 33.02 180)
				(length 3.81)
				(name "IO23RSB0")
				(number "179")
			)
			(pin bidirectional line
				(at 45.72 30.48 180)
				(length 3.81)
				(name "IO24RSB0")
				(number "177")
			)
			(pin bidirectional line
				(at 45.72 27.94 180)
				(length 3.81)
				(name "IO25RSB0")
				(number "176")
			)
			(pin bidirectional line
				(at 45.72 25.4 180)
				(length 3.81)
				(name "IO26RSB0")
				(number "175")
			)
			(pin bidirectional line
				(at 45.72 22.86 180)
				(length 3.81)
				(name "IO27RSB0")
				(number "174")
			)
			(pin bidirectional line
				(at 45.72 20.32 180)
				(length 3.81)
				(name "IO28RSB0")
				(number "173")
			)
			(pin bidirectional line
				(at 45.72 17.78 180)
				(length 3.81)
				(name "IO29RSB0")
				(number "172")
			)
			(pin bidirectional line
				(at 45.72 15.24 180)
				(length 3.81)
				(name "IO30RSB0")
				(number "169")
			)
			(pin bidirectional line
				(at 45.72 12.7 180)
				(length 3.81)
				(name "IO31RSB0")
				(number "168")
			)
			(pin bidirectional line
				(at 45.72 10.16 180)
				(length 3.81)
				(name "IO32RSB0")
				(number "167")
			)
			(pin bidirectional line
				(at 45.72 7.62 180)
				(length 3.81)
				(name "IO33RSB0")
				(number "166")
			)
			(pin bidirectional line
				(at 45.72 5.08 180)
				(length 3.81)
				(name "IO34RSB0")
				(number "165")
			)
			(pin bidirectional line
				(at 45.72 2.54 180)
				(length 3.81)
				(name "GBC0/IO35RSB0")
				(number "164")
			)
			(pin bidirectional line
				(at 45.72 0 180)
				(length 3.81)
				(name "GBC1/IO36RSB0")
				(number "163")
			)
			(pin bidirectional line
				(at 45.72 -2.54 180)
				(length 3.81)
				(name "GBB0/IO37RSB0")
				(number "161")
			)
			(pin bidirectional line
				(at 45.72 -5.08 180)
				(length 3.81)
				(name "GBB1/IO38RSB0")
				(number "160")
			)
			(pin bidirectional line
				(at 45.72 -7.62 180)
				(length 3.81)
				(name "GBA0/IO39RSB0")
				(number "159")
			)
			(pin bidirectional line
				(at 45.72 -10.16 180)
				(length 3.81)
				(name "GBA1/IO40RSB0")
				(number "158")
			)
			(pin bidirectional line
				(at 45.72 -15.24 180)
				(length 3.81)
				(name "GBA2/IO41PDB1")
				(number "153")
			)
			(pin bidirectional line
				(at 45.72 -17.78 180)
				(length 3.81)
				(name "IO41NDB1")
				(number "152")
			)
			(pin bidirectional line
				(at 45.72 -20.32 180)
				(length 3.81)
				(name "GBB2/IO42PDB1")
				(number "151")
			)
			(pin bidirectional line
				(at 45.72 -22.86 180)
				(length 3.81)
				(name "IO42NDB1")
				(number "150")
			)
			(pin bidirectional line
				(at 45.72 -25.4 180)
				(length 3.81)
				(name "GBC2/IO43PDB1")
				(number "149")
			)
			(pin bidirectional line
				(at 45.72 -27.94 180)
				(length 3.81)
				(name "IO43NDB1")
				(number "148")
			)
			(pin bidirectional line
				(at 45.72 -30.48 180)
				(length 3.81)
				(name "IO44PDB1")
				(number "147")
			)
			(pin bidirectional line
				(at 45.72 -33.02 180)
				(length 3.81)
				(name "IO44NDB1")
				(number "146")
			)
			(pin bidirectional line
				(at 45.72 -35.56 180)
				(length 3.81)
				(name "IO45PDB1")
				(number "145")
			)
			(pin bidirectional line
				(at 45.72 -38.1 180)
				(length 3.81)
				(name "IO45NDB1")
				(number "144")
			)
			(pin bidirectional line
				(at 45.72 -40.64 180)
				(length 3.81)
				(name "IO46RSB1")
				(number "143")
			)
			(pin bidirectional line
				(at 45.72 -43.18 180)
				(length 3.81)
				(name "IO47PDB1")
				(number "139")
			)
			(pin bidirectional line
				(at 45.72 -45.72 180)
				(length 3.81)
				(name "IO47NDB1")
				(number "138")
			)
			(pin bidirectional line
				(at 45.72 -48.26 180)
				(length 3.81)
				(name "GCC1/IO48PDB1")
				(number "137")
			)
			(pin bidirectional line
				(at 45.72 -50.8 180)
				(length 3.81)
				(name "GCC0/IO48NDB1")
				(number "136")
			)
			(pin bidirectional line
				(at 45.72 -53.34 180)
				(length 3.81)
				(name "GCB1/IO49PDB1")
				(number "135")
			)
			(pin bidirectional line
				(at 45.72 -55.88 180)
				(length 3.81)
				(name "GCB0/IO49NDB1")
				(number "134")
			)
			(pin bidirectional line
				(at 45.72 -58.42 180)
				(length 3.81)
				(name "GCA0/IO50NDB1")
				(number "133")
			)
			(pin bidirectional line
				(at 45.72 -60.96 180)
				(length 3.81)
				(name "GCA1/IO50PDB1")
				(number "132")
			)
			(pin bidirectional line
				(at 45.72 -63.5 180)
				(length 3.81)
				(name "GCA2/IO51PSB1")
				(number "131")
			)
			(pin bidirectional line
				(at 45.72 -66.04 180)
				(length 3.81)
				(name "GCB2/IO52PSB1")
				(number "129")
			)
			(pin bidirectional line
				(at 45.72 -68.58 180)
				(length 3.81)
				(name "GCC2/IO53PDB1")
				(number "128")
			)
			(pin bidirectional line
				(at 45.72 -71.12 180)
				(length 3.81)
				(name "IO53NDB1")
				(number "127")
			)
			(pin bidirectional line
				(at 45.72 -73.66 180)
				(length 3.81)
				(name "IO55RSB1")
				(number "121")
			)
			(pin bidirectional line
				(at 45.72 -76.2 180)
				(length 3.81)
				(name "IO56PDB1")
				(number "120")
			)
			(pin bidirectional line
				(at 45.72 -78.74 180)
				(length 3.81)
				(name "IO56NDB1")
				(number "119")
			)
			(pin bidirectional line
				(at 45.72 -81.28 180)
				(length 3.81)
				(name "IO57UDB1")
				(number "118")
			)
			(pin bidirectional line
				(at 45.72 -83.82 180)
				(length 3.81)
				(name "IO57VDB1")
				(number "117")
			)
			(pin bidirectional line
				(at 45.72 -86.36 180)
				(length 3.81)
				(name "GDC1/IO58UDB1")
				(number "116")
			)
			(pin bidirectional line
				(at 45.72 -88.9 180)
				(length 3.81)
				(name "GDC0/IO58VDB1")
				(number "115")
			)
			(pin bidirectional line
				(at 45.72 -91.44 180)
				(length 3.81)
				(name "GDB1/IO59UDB1")
				(number "114")
			)
			(pin bidirectional line
				(at 45.72 -93.98 180)
				(length 3.81)
				(name "GDB0/IO59VDB1")
				(number "113")
			)
			(pin bidirectional line
				(at 45.72 -96.52 180)
				(length 3.81)
				(name "GDA1/IO60UDB1")
				(number "112")
			)
			(pin bidirectional line
				(at 45.72 -99.06 180)
				(length 3.81)
				(name "GDA0/IO60VDB1")
				(number "111")
			)
		)
		(embedded_fonts no)
	)
	(symbol "A3P250-VQG100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 30.48 55.88 0)
		)
		(property "Value" "A3P250-VQG100"
			(at 30.48 53.34 0)
		)
		(property "Footprint" "Package_QFP:VQFP-100_14x14mm_P0.5mm"
			(at 30.48 50.8 0)
		)
		(property "Datasheet" "http://www.microsemi.com/document-portal/doc_download/130704-proasic3-flash-family-fpgas-datasheet"
			(at 0 0 0)
		)
		(property "Description" "Actel ProASIC3 Flash Family FPGAs, 2048 MCLB, 100pin QFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "ProASIC3 ACTEL FLASH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "A3P250-VQG100_0_1")
		(symbol "A3P250-VQG100_1_1"
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 3.81)
				(name "VJTAG")
				(number "56")
			)
			(pin bidirectional line
				(at -33.02 50.8 0)
				(length 3.81)
				(name "TCK")
				(number "47")
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 3.81)
				(name "TDI")
				(number "48")
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 3.81)
				(name "TMS")
				(number "49")
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 3.81)
				(name "TDO")
				(number "54")
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 3.81)
				(name "TRST")
				(number "55")
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 3.81)
				(name "IO118UDB3/GAA2")
				(number "2")
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 3.81)
				(name "IO118VDB3")
				(number "3")
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 3.81)
				(name "IO117UDB3/GAB2")
				(number "4")
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 3.81)
				(name "IO117VDB3")
				(number "5")
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 3.81)
				(name "IO116UDB3/GAC2")
				(number "6")
			)
			(pin input line
				(at -33.02 22.86 0)
				(length 3.81)
				(name "IO116VDB3")
				(number "7")
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 3.81)
				(name "IO112PSB3")
				(number "8")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 3.81)
				(name "IO109PDB3/GFB1")
				(number "10")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 3.81)
				(name "IO109NDB3/GFB0")
				(number "11")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 3.81)
				(name "IO108NPB3/GFA0")
				(number "13")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 3.81)
				(name "IO108PPB3/GFA1")
				(number "15")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "IO107PSB3/GFA2")
				(number "16")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 3.81)
				(name "IO105PSB3/GFC2")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 3.81)
				(name "IO100NDB3/GEC0")
				(number "21")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 3.81)
				(name "IO100PDB3/GEC1")
				(number "20")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 3.81)
				(name "IO98PDB3/GEA1")
				(number "22")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 3.81)
				(name "IO98NDB3/GEA0")
				(number "23")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 3.81)
				(name "IO97RSB2/GEA2")
				(number "26")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 3.81)
				(name "IO96RSB2/GEB2")
				(number "27")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 3.81)
				(name "IO95RSB2/GEC2")
				(number "28")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 3.81)
				(name "IO93RSB2")
				(number "29")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 3.81)
				(name "IO92RSB2")
				(number "30")
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 3.81)
				(name "IO91RSB2")
				(number "31")
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 3.81)
				(name "IO90RSB2")
				(number "32")
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 3.81)
				(name "IO88RSB2")
				(number "33")
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 3.81)
				(name "IO86RSB2")
				(number "34")
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 3.81)
				(name "IO85RSB2")
				(number "35")
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 3.81)
				(name "IO84RSB2")
				(number "36")
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 3.81)
				(name "IO77RSB2")
				(number "40")
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 3.81)
				(name "IO74RSB2")
				(number "41")
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 3.81)
				(name "IO71RSB2")
				(number "42")
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 3.81)
				(name "IO63RSB2/GDC2")
				(number "43")
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 3.81)
				(name "IO62RSB2/GDB2")
				(number "44")
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 3.81)
				(name "IO61RSB2/GDA2")
				(number "45")
			)
			(pin power_in line
				(at -20.32 60.96 270)
				(length 3.81)
				(name "VCCPLF")
				(number "14")
			)
			(pin power_in line
				(at -15.24 60.96 270)
				(length 3.81)
				(name "VCC")
				(number "17")
			)
			(pin power_in line
				(at -12.7 60.96 270)
				(length 3.81)
				(name "VCC")
				(number "37")
			)
			(pin power_in line
				(at -10.16 60.96 270)
				(length 3.81)
				(name "VCC")
				(number "68")
			)
			(pin power_in line
				(at -10.16 -60.96 90)
				(length 3.81)
				(name "VCOMPLF")
				(number "12")
			)
			(pin power_in line
				(at -7.62 60.96 270)
				(length 3.81)
				(name "VCC")
				(number "89")
			)
			(pin power_out line
				(at -5.08 -60.96 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -2.54 60.96 270)
				(length 3.81)
				(name "VCCIB3")
				(number "18")
			)
			(pin power_out line
				(at -2.54 -60.96 90)
				(length 3.81)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 0 60.96 270)
				(length 3.81)
				(name "VCCIB2")
				(number "39")
			)
			(pin power_out line
				(at 0 -60.96 90)
				(length 3.81)
				(name "GND")
				(number "38")
			)
			(pin bidirectional line
				(at 2.54 60.96 270)
				(length 3.81)
				(name "VCCIB1")
				(number "66")
			)
			(pin power_out line
				(at 2.54 -60.96 90)
				(length 3.81)
				(name "GND")
				(number "51")
			)
			(pin power_in line
				(at 5.08 60.96 270)
				(length 3.81)
				(name "VCCIB0")
				(number "87")
			)
			(pin power_out line
				(at 5.08 -60.96 90)
				(length 3.81)
				(name "GND")
				(number "67")
			)
			(pin power_out line
				(at 7.62 -60.96 90)
				(length 3.81)
				(name "GND")
				(number "88")
			)
			(pin bidirectional line
				(at 10.16 60.96 270)
				(length 3.81)
				(name "VMV3")
				(number "24")
			)
			(pin power_in line
				(at 12.7 60.96 270)
				(length 3.81)
				(name "VMV2")
				(number "50")
			)
			(pin bidirectional line
				(at 12.7 -60.96 90)
				(length 3.81)
				(name "GNDQ")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 60.96 270)
				(length 3.81)
				(name "VMV1")
				(number "74")
			)
			(pin power_out line
				(at 15.24 -60.96 90)
				(length 3.81)
				(name "GNDQ")
				(number "46")
			)
			(pin power_in line
				(at 17.78 60.96 270)
				(length 3.81)
				(name "VMV0")
				(number "100")
			)
			(pin bidirectional line
				(at 17.78 -60.96 90)
				(length 3.81)
				(name "GNDQ")
				(number "75")
			)
			(pin power_out line
				(at 20.32 -60.96 90)
				(length 3.81)
				(name "GNDQ")
				(number "99")
			)
			(pin power_in line
				(at 22.86 60.96 270)
				(length 3.81)
				(name "VPUMP")
				(number "52")
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 3.81)
				(name "GAA0/IO00RSB0")
				(number "98")
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 3.81)
				(name "GAA1/IO01RSB0")
				(number "97")
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 3.81)
				(name "GAB0/IO02RSB0")
				(number "96")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 3.81)
				(name "GAB1/IO03RSB0")
				(number "95")
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 3.81)
				(name "GAC0/IO04RSB0")
				(number "94")
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 3.81)
				(name "GAC1/IO05RSB0")
				(number "93")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "IO11RSB0")
				(number "92")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 3.81)
				(name "IO13RSB0")
				(number "91")
			)
			(pin input line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "IO15RSB0")
				(number "90")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "IO21RSB0")
				(number "86")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "IO23RSB0")
				(number "85")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "IO25RSB0")
				(number "84")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "IO27RSB0")
				(number "83")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "IO29RSB0")
				(number "82")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "GBC0/IO35RSB0")
				(number "81")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "GBC1/IO36RSB0")
				(number "80")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 3.81)
				(name "GBB0/IO37RSB0")
				(number "79")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "GBB1/IO38RSB0")
				(number "78")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "GBA0/IO39RSB0")
				(number "77")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "GBA1/IO40RSB0")
				(number "76")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "GBA2/IO41PDB1")
				(number "73")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "IO41NDB1")
				(number "72")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "GBB2/IO42PSB1")
				(number "71")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 3.81)
				(name "GBC2/IO43PDB1")
				(number "70")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 3.81)
				(name "IO43NDB1")
				(number "69")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 3.81)
				(name "GCC1/IO48PDB1")
				(number "65")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 3.81)
				(name "GCC0/IO48NDB1")
				(number "64")
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 3.81)
				(name "GCA0/IO50NDB1")
				(number "63")
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 3.81)
				(name "GCA1/IO50PDB1")
				(number "62")
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 3.81)
				(name "GCB2/IO52PDB1")
				(number "61")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 3.81)
				(name "IO52NDB1")
				(number "60")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 3.81)
				(name "GDC1/IO58UDB1")
				(number "59")
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 3.81)
				(name "GDC0/IO58VDB1")
				(number "58")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 3.81)
				(name "GDA1/IO60USB1")
				(number "57")
			)
		)
		(embedded_fonts no)
	)
	(symbol "A3P400-PQG208"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 45.72 109.22 0)
		)
		(property "Value" "A3P400-PQG208"
			(at 45.72 106.68 0)
		)
		(property "Footprint" "Package_QFP:PQFP-208_28x28mm_P0.5mm"
			(at 45.72 104.14 0)
		)
		(property "Datasheet" "http://www.microsemi.com/document-portal/doc_download/130704-proasic3-flash-family-fpgas-datasheet"
			(at 0 -7.62 0)
		)
		(property "Description" "Actel ProASIC3 Flash Family FPGAs, 400k Gates, 208pin QFP"
			(at 0 0 0)
		)
		(property "ki_keywords" "ProASIC3 ACTEL FLASH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFP*28x28mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "A3P400-PQG208_1_0")
		(symbol "A3P400-PQG208_1_1"
			(pin power_in line
				(at -48.26 106.68 0)
				(length 3.81)
				(name "VJTAG")
				(number "110")
			)
			(pin bidirectional line
				(at -48.26 104.14 0)
				(length 3.81)
				(name "TCK")
				(number "101")
			)
			(pin bidirectional line
				(at -48.26 101.6 0)
				(length 3.81)
				(name "TDI")
				(number "102")
			)
			(pin bidirectional line
				(at -48.26 99.06 0)
				(length 3.81)
				(name "TMS")
				(number "103")
			)
			(pin bidirectional line
				(at -48.26 96.52 0)
				(length 3.81)
				(name "TDO")
				(number "108")
			)
			(pin bidirectional line
				(at -48.26 93.98 0)
				(length 3.81)
				(name "TRST")
				(number "109")
			)
			(pin bidirectional line
				(at -48.26 88.9 0)
				(length 3.81)
				(name "IO135NDB3/GEA0")
				(number "49")
			)
			(pin bidirectional line
				(at -48.26 86.36 0)
				(length 3.81)
				(name "IO135PDB3/GEA1")
				(number "48")
			)
			(pin bidirectional line
				(at -48.26 83.82 0)
				(length 3.81)
				(name "IO136NDB3/GEB0")
				(number "47")
			)
			(pin bidirectional line
				(at -48.26 81.28 0)
				(length 3.81)
				(name "IO136PDB3/GEB1")
				(number "46")
			)
			(pin bidirectional line
				(at -48.26 78.74 0)
				(length 3.81)
				(name "IO137NDB3/GEC0")
				(number "45")
			)
			(pin bidirectional line
				(at -48.26 76.2 0)
				(length 3.81)
				(name "IO137PDB3/GEC1")
				(number "44")
			)
			(pin bidirectional line
				(at -48.26 73.66 0)
				(length 3.81)
				(name "IO138NDB3")
				(number "43")
			)
			(pin bidirectional line
				(at -48.26 71.12 0)
				(length 3.81)
				(name "IO138PDB3")
				(number "42")
			)
			(pin bidirectional line
				(at -48.26 68.58 0)
				(length 3.81)
				(name "IO140NDB3")
				(number "39")
			)
			(pin bidirectional line
				(at -48.26 66.04 0)
				(length 3.81)
				(name "IO140PDB3")
				(number "38")
			)
			(pin bidirectional line
				(at -48.26 63.5 0)
				(length 3.81)
				(name "IO141PSB3")
				(number "37")
			)
			(pin bidirectional line
				(at -48.26 60.96 0)
				(length 3.81)
				(name "IO142NDB3")
				(number "35")
			)
			(pin bidirectional line
				(at -48.26 58.42 0)
				(length 3.81)
				(name "IO142PDB3/GFC2")
				(number "34")
			)
			(pin bidirectional line
				(at -48.26 55.88 0)
				(length 3.81)
				(name "IO143NDB3")
				(number "33")
			)
			(pin bidirectional line
				(at -48.26 53.34 0)
				(length 3.81)
				(name "IO143PDB3/GFB2")
				(number "32")
			)
			(pin bidirectional line
				(at -48.26 50.8 0)
				(length 3.81)
				(name "IO144NDB3")
				(number "31")
			)
			(pin bidirectional line
				(at -48.26 48.26 0)
				(length 3.81)
				(name "IO144PDB3/GFA2")
				(number "30")
			)
			(pin bidirectional line
				(at -48.26 45.72 0)
				(length 3.81)
				(name "IO145PPB3/GFA1")
				(number "28")
			)
			(pin bidirectional line
				(at -48.26 43.18 0)
				(length 3.81)
				(name "IO145NPB3/GFA0")
				(number "26")
			)
			(pin bidirectional line
				(at -48.26 40.64 0)
				(length 3.81)
				(name "IO146NDB3/GFB0")
				(number "24")
			)
			(pin bidirectional line
				(at -48.26 38.1 0)
				(length 3.81)
				(name "IO146PDB3/GFB1")
				(number "23")
			)
			(pin bidirectional line
				(at -48.26 35.56 0)
				(length 3.81)
				(name "IO147NDB3/GFC0")
				(number "22")
			)
			(pin bidirectional line
				(at -48.26 33.02 0)
				(length 3.81)
				(name "IO147PDB3/GFC1")
				(number "21")
			)
			(pin bidirectional line
				(at -48.26 30.48 0)
				(length 3.81)
				(name "IO148NDB3")
				(number "20")
			)
			(pin bidirectional line
				(at -48.26 27.94 0)
				(length 3.81)
				(name "IO148PDB3")
				(number "19")
			)
			(pin bidirectional line
				(at -48.26 25.4 0)
				(length 3.81)
				(name "IO149NDB3")
				(number "15")
			)
			(pin bidirectional line
				(at -48.26 22.86 0)
				(length 3.81)
				(name "IO149PDB3")
				(number "14")
			)
			(pin bidirectional line
				(at -48.26 20.32 0)
				(length 3.81)
				(name "IO150NDB3")
				(number "13")
			)
			(pin bidirectional line
				(at -48.26 17.78 0)
				(length 3.81)
				(name "IO150PDB3")
				(number "12")
			)
			(pin bidirectional line
				(at -48.26 15.24 0)
				(length 3.81)
				(name "IO151VDB3")
				(number "11")
			)
			(pin bidirectional line
				(at -48.26 12.7 0)
				(length 3.81)
				(name "IO151UDB3")
				(number "10")
			)
			(pin bidirectional line
				(at -48.26 10.16 0)
				(length 3.81)
				(name "IO152VDB3")
				(number "9")
			)
			(pin bidirectional line
				(at -48.26 7.62 0)
				(length 3.81)
				(name "IO152UDB3")
				(number "8")
			)
			(pin bidirectional line
				(at -48.26 5.08 0)
				(length 3.81)
				(name "IO153VDB3")
				(number "7")
			)
			(pin bidirectional line
				(at -48.26 2.54 0)
				(length 3.81)
				(name "IO153UDB3/GAC2")
				(number "6")
			)
			(pin bidirectional line
				(at -48.26 0 0)
				(length 3.81)
				(name "IO154VDB3")
				(number "5")
			)
			(pin bidirectional line
				(at -48.26 -2.54 0)
				(length 3.81)
				(name "IO154UDB3/GAB2")
				(number "4")
			)
			(pin bidirectional line
				(at -48.26 -5.08 0)
				(length 3.81)
				(name "IO155VDB3")
				(number "3")
			)
			(pin bidirectional line
				(at -48.26 -7.62 0)
				(length 3.81)
				(name "IO155UDB3/GAA2")
				(number "2")
			)
			(pin bidirectional line
				(at -48.26 -12.7 0)
				(length 3.81)
				(name "IO80RSB2/GDA2")
				(number "99")
			)
			(pin bidirectional line
				(at -48.26 -15.24 0)
				(length 3.81)
				(name "IO81RSB2/GDB2")
				(number "98")
			)
			(pin bidirectional line
				(at -48.26 -17.78 0)
				(length 3.81)
				(name "IO82RSB2/GDC2")
				(number "96")
			)
			(pin bidirectional line
				(at -48.26 -20.32 0)
				(length 3.81)
				(name "IO84RSB2")
				(number "95")
			)
			(pin bidirectional line
				(at -48.26 -22.86 0)
				(length 3.81)
				(name "IO86RSB2")
				(number "94")
			)
			(pin bidirectional line
				(at -48.26 -25.4 0)
				(length 3.81)
				(name "IO88RSB2")
				(number "93")
			)
			(pin bidirectional line
				(at -48.26 -27.94 0)
				(length 3.81)
				(name "IO90RSB2")
				(number "92")
			)
			(pin bidirectional line
				(at -48.26 -30.48 0)
				(length 3.81)
				(name "IO92RSB2")
				(number "91")
			)
			(pin bidirectional line
				(at -48.26 -33.02 0)
				(length 3.81)
				(name "IO94RSB2")
				(number "90")
			)
			(pin bidirectional line
				(at -48.26 -35.56 0)
				(length 3.81)
				(name "IO97RSB2")
				(number "87")
			)
			(pin bidirectional line
				(at -48.26 -38.1 0)
				(length 3.81)
				(name "IO98RSB2")
				(number "86")
			)
			(pin bidirectional line
				(at -48.26 -40.64 0)
				(length 3.81)
				(name "IO99RSB2")
				(number "85")
			)
			(pin bidirectional line
				(at -48.26 -43.18 0)
				(length 3.81)
				(name "IO100RSB2")
				(number "84")
			)
			(pin bidirectional line
				(at -48.26 -45.72 0)
				(length 3.81)
				(name "IO101RSB2")
				(number "83")
			)
			(pin bidirectional line
				(at -48.26 -48.26 0)
				(length 3.81)
				(name "IO102RSB2")
				(number "82")
			)
			(pin bidirectional line
				(at -48.26 -50.8 0)
				(length 3.81)
				(name "IO104RSB2")
				(number "80")
			)
			(pin bidirectional line
				(at -48.26 -53.34 0)
				(length 3.81)
				(name "IO106RSB2")
				(number "79")
			)
			(pin bidirectional line
				(at -48.26 -55.88 0)
				(length 3.81)
				(name "IO107RSB2")
				(number "78")
			)
			(pin bidirectional line
				(at -48.26 -58.42 0)
				(length 3.81)
				(name "IO108RSB2")
				(number "77")
			)
			(pin bidirectional line
				(at -48.26 -60.96 0)
				(length 3.81)
				(name "IO109RSB2")
				(number "76")
			)
			(pin bidirectional line
				(at -48.26 -63.5 0)
				(length 3.81)
				(name "IO110RSB2")
				(number "75")
			)
			(pin bidirectional line
				(at -48.26 -66.04 0)
				(length 3.81)
				(name "IO111RSB2")
				(number "74")
			)
			(pin bidirectional line
				(at -48.26 -68.58 0)
				(length 3.81)
				(name "IO112RSB2")
				(number "73")
			)
			(pin bidirectional line
				(at -48.26 -71.12 0)
				(length 3.81)
				(name "IO113RSB2")
				(number "70")
			)
			(pin bidirectional line
				(at -48.26 -73.66 0)
				(length 3.81)
				(name "IO115RSB2")
				(number "69")
			)
			(pin bidirectional line
				(at -48.26 -76.2 0)
				(length 3.81)
				(name "IO117RSB2")
				(number "68")
			)
			(pin bidirectional line
				(at -48.26 -78.74 0)
				(length 3.81)
				(name "IO119RSB2")
				(number "67")
			)
			(pin bidirectional line
				(at -48.26 -81.28 0)
				(length 3.81)
				(name "IO121RSB2")
				(number "66")
			)
			(pin bidirectional line
				(at -48.26 -83.82 0)
				(length 3.81)
				(name "IO123RSB2")
				(number "64")
			)
			(pin bidirectional line
				(at -48.26 -86.36 0)
				(length 3.81)
				(name "IO125RSB2")
				(number "63")
			)
			(pin bidirectional line
				(at -48.26 -88.9 0)
				(length 3.81)
				(name "IO128RSB2")
				(number "61")
			)
			(pin bidirectional line
				(at -48.26 -91.44 0)
				(length 3.81)
				(name "IO129RSB2")
				(number "60")
			)
			(pin bidirectional line
				(at -48.26 -93.98 0)
				(length 3.81)
				(name "IO130RSB2")
				(number "59")
			)
			(pin bidirectional line
				(at -48.26 -96.52 0)
				(length 3.81)
				(name "IO131RSB2")
				(number "58")
			)
			(pin bidirectional line
				(at -48.26 -99.06 0)
				(length 3.81)
				(name "IO132RSB2/GEC2")
				(number "57")
			)
			(pin bidirectional line
				(at -48.26 -101.6 0)
				(length 3.81)
				(name "IO133RSB2/GEB2")
				(number "56")
			)
			(pin bidirectional line
				(at -48.26 -104.14 0)
				(length 3.81)
				(name "IO134RSB2/GEA2")
				(number "55")
			)
			(pin power_in line
				(at -35.56 114.3 270)
				(length 3.81)
				(name "VCCPLF")
				(number "27")
			)
			(pin power_in line
				(at -30.48 114.3 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at -27.94 114.3 270)
				(length 3.81)
				(name "VCC")
				(number "71")
			)
			(pin power_in line
				(at -25.4 114.3 270)
				(length 3.81)
				(name "VCC")
				(number "88")
			)
			(pin power_in line
				(at -22.86 114.3 270)
				(length 3.81)
				(name "VCC")
				(number "126")
			)
			(pin power_in line
				(at -20.32 114.3 270)
				(length 3.81)
				(name "VCC")
				(number "142")
			)
			(pin power_in line
				(at -17.78 114.3 270)
				(length 3.81)
				(name "VCC")
				(number "171")
			)
			(pin power_in line
				(at -17.78 -114.3 90)
				(length 3.81)
				(name "VCOMPLF")
				(number "25")
			)
			(pin power_in line
				(at -15.24 114.3 270)
				(length 3.81)
				(name "VCC")
				(number "187")
			)
			(pin power_in line
				(at -12.7 -114.3 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -10.16 114.3 270)
				(length 3.81)
				(name "VCCIB0")
				(number "200")
			)
			(pin power_in line
				(at -10.16 -114.3 90)
				(length 3.81)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at -7.62 114.3 270)
				(length 3.81)
				(name "VCCIB0")
				(number "186")
			)
			(pin power_in line
				(at -7.62 -114.3 90)
				(length 3.81)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at -5.08 114.3 270)
				(length 3.81)
				(name "VCCIB0")
				(number "170")
			)
			(pin power_in line
				(at -5.08 -114.3 90)
				(length 3.81)
				(name "GND")
				(number "41")
			)
			(pin power_in line
				(at -2.54 114.3 270)
				(length 3.81)
				(name "VCCIB1")
				(number "140")
			)
			(pin power_in line
				(at -2.54 -114.3 90)
				(length 3.81)
				(name "GND")
				(number "52")
			)
			(pin power_in line
				(at 0 114.3 270)
				(length 3.81)
				(name "VCCIB1")
				(number "123")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 3.81)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 114.3 270)
				(length 3.81)
				(name "VCCIB2")
				(number "89")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 3.81)
				(name "GND")
				(number "81")
			)
			(pin power_in line
				(at 5.08 114.3 270)
				(length 3.81)
				(name "VCCIB2")
				(number "72")
			)
			(pin power_in line
				(at 5.08 -114.3 90)
				(length 3.81)
				(name "GND")
				(number "97")
			)
			(pin power_in line
				(at 7.62 114.3 270)
				(length 3.81)
				(name "VCCIB2")
				(number "62")
			)
			(pin power_in line
				(at 7.62 -114.3 90)
				(length 3.81)
				(name "GND")
				(number "105")
			)
			(pin power_in line
				(at 10.16 114.3 270)
				(length 3.81)
				(name "VCCIB3")
				(number "40")
			)
			(pin power_in line
				(at 10.16 -114.3 90)
				(length 3.81)
				(name "GND")
				(number "122")
			)
			(pin power_in line
				(at 12.7 114.3 270)
				(length 3.81)
				(name "VCCIB3")
				(number "18")
			)
			(pin power_in line
				(at 12.7 -114.3 90)
				(length 3.81)
				(name "GND")
				(number "130")
			)
			(pin power_in line
				(at 15.24 -114.3 90)
				(length 3.81)
				(name "GND")
				(number "141")
			)
			(pin power_in line
				(at 17.78 114.3 270)
				(length 3.81)
				(name "VMV0")
				(number "208")
			)
			(pin power_in line
				(at 17.78 -114.3 90)
				(length 3.81)
				(name "GND")
				(number "156")
			)
			(pin power_in line
				(at 20.32 114.3 270)
				(length 3.81)
				(name "VMV0")
				(number "157")
			)
			(pin power_in line
				(at 20.32 -114.3 90)
				(length 3.81)
				(name "GND")
				(number "162")
			)
			(pin power_in line
				(at 22.86 114.3 270)
				(length 3.81)
				(name "VMV1")
				(number "154")
			)
			(pin power_in line
				(at 22.86 -114.3 90)
				(length 3.81)
				(name "GND")
				(number "178")
			)
			(pin power_in line
				(at 25.4 114.3 270)
				(length 3.81)
				(name "VMV2")
				(number "104")
			)
			(pin power_in line
				(at 25.4 -114.3 90)
				(length 3.81)
				(name "GND")
				(number "195")
			)
			(pin power_in line
				(at 27.94 114.3 270)
				(length 3.81)
				(name "VMV2")
				(number "53")
			)
			(pin power_in line
				(at 30.48 114.3 270)
				(length 3.81)
				(name "VMV3")
				(number "50")
			)
			(pin power_in line
				(at 30.48 -114.3 90)
				(length 3.81)
				(name "GNDQ")
				(number "51")
			)
			(pin power_in line
				(at 33.02 -114.3 90)
				(length 3.81)
				(name "GNDQ")
				(number "100")
			)
			(pin power_in line
				(at 35.56 114.3 270)
				(length 3.81)
				(name "VPUMP")
				(number "106")
			)
			(pin power_in line
				(at 35.56 -114.3 90)
				(length 3.81)
				(name "GNDQ")
				(number "155")
			)
			(pin power_in line
				(at 38.1 -114.3 90)
				(length 3.81)
				(name "GNDQ")
				(number "207")
			)
			(pin bidirectional line
				(at 48.26 88.9 180)
				(length 3.81)
				(name "GAA0/IO00RSB0")
				(number "206")
			)
			(pin bidirectional line
				(at 48.26 86.36 180)
				(length 3.81)
				(name "GAA1/IO01RSB0")
				(number "205")
			)
			(pin bidirectional line
				(at 48.26 83.82 180)
				(length 3.81)
				(name "GAB0/IO02RSB0")
				(number "204")
			)
			(pin bidirectional line
				(at 48.26 81.28 180)
				(length 3.81)
				(name "GAB1/IO03RSB0")
				(number "203")
			)
			(pin bidirectional line
				(at 48.26 78.74 180)
				(length 3.81)
				(name "GAC0/IO04RSB0")
				(number "202")
			)
			(pin bidirectional line
				(at 48.26 76.2 180)
				(length 3.81)
				(name "GAC1/IO05RSB0")
				(number "201")
			)
			(pin bidirectional line
				(at 48.26 73.66 180)
				(length 3.81)
				(name "IO07RSB0")
				(number "199")
			)
			(pin bidirectional line
				(at 48.26 71.12 180)
				(length 3.81)
				(name "IO09RSB0")
				(number "198")
			)
			(pin bidirectional line
				(at 48.26 68.58 180)
				(length 3.81)
				(name "IO11RSB0")
				(number "197")
			)
			(pin bidirectional line
				(at 48.26 66.04 180)
				(length 3.81)
				(name "IO13RSB0")
				(number "196")
			)
			(pin bidirectional line
				(at 48.26 63.5 180)
				(length 3.81)
				(name "IO15RSB0")
				(number "194")
			)
			(pin bidirectional line
				(at 48.26 60.96 180)
				(length 3.81)
				(name "IO16RSB0")
				(number "193")
			)
			(pin bidirectional line
				(at 48.26 58.42 180)
				(length 3.81)
				(name "IO17RSB0")
				(number "192")
			)
			(pin bidirectional line
				(at 48.26 55.88 180)
				(length 3.81)
				(name "IO18RSB0")
				(number "191")
			)
			(pin bidirectional line
				(at 48.26 53.34 180)
				(length 3.81)
				(name "IO19RSB0")
				(number "190")
			)
			(pin bidirectional line
				(at 48.26 50.8 180)
				(length 3.81)
				(name "IO20RSB0")
				(number "189")
			)
			(pin bidirectional line
				(at 48.26 48.26 180)
				(length 3.81)
				(name "IO21RSB0")
				(number "188")
			)
			(pin bidirectional line
				(at 48.26 45.72 180)
				(length 3.81)
				(name "IO23RSB0")
				(number "185")
			)
			(pin bidirectional line
				(at 48.26 43.18 180)
				(length 3.81)
				(name "IO24RSB0")
				(number "184")
			)
			(pin bidirectional line
				(at 48.26 40.64 180)
				(length 3.81)
				(name "IO25RSB0")
				(number "183")
			)
			(pin bidirectional line
				(at 48.26 38.1 180)
				(length 3.81)
				(name "IO26RSB0")
				(number "182")
			)
			(pin bidirectional line
				(at 48.26 35.56 180)
				(length 3.81)
				(name "IO27RSB0")
				(number "181")
			)
			(pin bidirectional line
				(at 48.26 33.02 180)
				(length 3.81)
				(name "IO28RSB0")
				(number "180")
			)
			(pin bidirectional line
				(at 48.26 30.48 180)
				(length 3.81)
				(name "IO29RSB0")
				(number "179")
			)
			(pin bidirectional line
				(at 48.26 27.94 180)
				(length 3.81)
				(name "IO31RSB0")
				(number "177")
			)
			(pin bidirectional line
				(at 48.26 25.4 180)
				(length 3.81)
				(name "IO32RSB0")
				(number "176")
			)
			(pin bidirectional line
				(at 48.26 22.86 180)
				(length 3.81)
				(name "IO33RSB0")
				(number "175")
			)
			(pin bidirectional line
				(at 48.26 20.32 180)
				(length 3.81)
				(name "IO34RSB0")
				(number "174")
			)
			(pin bidirectional line
				(at 48.26 17.78 180)
				(length 3.81)
				(name "IO35RSB0")
				(number "173")
			)
			(pin bidirectional line
				(at 48.26 15.24 180)
				(length 3.81)
				(name "IO36RSB0")
				(number "172")
			)
			(pin bidirectional line
				(at 48.26 12.7 180)
				(length 3.81)
				(name "IO40RSB0")
				(number "169")
			)
			(pin bidirectional line
				(at 48.26 10.16 180)
				(length 3.81)
				(name "IO43RSB0")
				(number "168")
			)
			(pin bidirectional line
				(at 48.26 7.62 180)
				(length 3.81)
				(name "IO46RSB0")
				(number "167")
			)
			(pin bidirectional line
				(at 48.26 5.08 180)
				(length 3.81)
				(name "IO49RSB0")
				(number "166")
			)
			(pin bidirectional line
				(at 48.26 2.54 180)
				(length 3.81)
				(name "IO52RSB0")
				(number "165")
			)
			(pin bidirectional line
				(at 48.26 0 180)
				(length 3.81)
				(name "GBC0/IO54RSB0")
				(number "164")
			)
			(pin bidirectional line
				(at 48.26 -2.54 180)
				(length 3.81)
				(name "GBC1/IO55RSB0")
				(number "163")
			)
			(pin bidirectional line
				(at 48.26 -5.08 180)
				(length 3.81)
				(name "GBB0/IO56RSB0")
				(number "161")
			)
			(pin bidirectional line
				(at 48.26 -7.62 180)
				(length 3.81)
				(name "GBB1/IO57RSB0")
				(number "160")
			)
			(pin bidirectional line
				(at 48.26 -10.16 180)
				(length 3.81)
				(name "GBA0/IO58RSB0")
				(number "159")
			)
			(pin bidirectional line
				(at 48.26 -12.7 180)
				(length 3.81)
				(name "GBA1/IO59RSB0")
				(number "158")
			)
			(pin bidirectional line
				(at 48.26 -17.78 180)
				(length 3.81)
				(name "GBA2/IO60PDB1")
				(number "153")
			)
			(pin bidirectional line
				(at 48.26 -20.32 180)
				(length 3.81)
				(name "IO60NDB1")
				(number "152")
			)
			(pin bidirectional line
				(at 48.26 -22.86 180)
				(length 3.81)
				(name "GBB2/IO61PDB1")
				(number "151")
			)
			(pin bidirectional line
				(at 48.26 -25.4 180)
				(length 3.81)
				(name "IO61NDB1")
				(number "150")
			)
			(pin bidirectional line
				(at 48.26 -27.94 180)
				(length 3.81)
				(name "GBC2/IO62PDB1")
				(number "149")
			)
			(pin bidirectional line
				(at 48.26 -30.48 180)
				(length 3.81)
				(name "IO62NDB1")
				(number "148")
			)
			(pin bidirectional line
				(at 48.26 -33.02 180)
				(length 3.81)
				(name "IO63PDB1")
				(number "147")
			)
			(pin bidirectional line
				(at 48.26 -35.56 180)
				(length 3.81)
				(name "IO63NDB1")
				(number "146")
			)
			(pin bidirectional line
				(at 48.26 -38.1 180)
				(length 3.81)
				(name "IO64PDB1")
				(number "145")
			)
			(pin bidirectional line
				(at 48.26 -40.64 180)
				(length 3.81)
				(name "IO64NDB1")
				(number "144")
			)
			(pin bidirectional line
				(at 48.26 -43.18 180)
				(length 3.81)
				(name "IO65RSB1")
				(number "143")
			)
			(pin bidirectional line
				(at 48.26 -45.72 180)
				(length 3.81)
				(name "IO66PDB1")
				(number "139")
			)
			(pin bidirectional line
				(at 48.26 -48.26 180)
				(length 3.81)
				(name "IO66NDB1")
				(number "138")
			)
			(pin bidirectional line
				(at 48.26 -50.8 180)
				(length 3.81)
				(name "GCC1/IO67PDB1")
				(number "137")
			)
			(pin bidirectional line
				(at 48.26 -53.34 180)
				(length 3.81)
				(name "GCC0/IO67NDB1")
				(number "136")
			)
			(pin bidirectional line
				(at 48.26 -55.88 180)
				(length 3.81)
				(name "GCB1/IO68PDB1")
				(number "135")
			)
			(pin bidirectional line
				(at 48.26 -58.42 180)
				(length 3.81)
				(name "GCB0/IO68NDB1")
				(number "134")
			)
			(pin bidirectional line
				(at 48.26 -60.96 180)
				(length 3.81)
				(name "GCA0/IO69NDB1")
				(number "133")
			)
			(pin bidirectional line
				(at 48.26 -63.5 180)
				(length 3.81)
				(name "GCA1/IO69PDB1")
				(number "132")
			)
			(pin bidirectional line
				(at 48.26 -66.04 180)
				(length 3.81)
				(name "GCA2/IO70PSB1")
				(number "131")
			)
			(pin bidirectional line
				(at 48.26 -68.58 180)
				(length 3.81)
				(name "GCB2/IO71PSB1")
				(number "129")
			)
			(pin bidirectional line
				(at 48.26 -71.12 180)
				(length 3.81)
				(name "GCC2/IO72PDB1")
				(number "128")
			)
			(pin bidirectional line
				(at 48.26 -73.66 180)
				(length 3.81)
				(name "IO72NDB1")
				(number "127")
			)
			(pin bidirectional line
				(at 48.26 -76.2 180)
				(length 3.81)
				(name "IO74RSB1")
				(number "121")
			)
			(pin bidirectional line
				(at 48.26 -78.74 180)
				(length 3.81)
				(name "IO75PDB1")
				(number "120")
			)
			(pin bidirectional line
				(at 48.26 -81.28 180)
				(length 3.81)
				(name "IO75NDB1")
				(number "119")
			)
			(pin bidirectional line
				(at 48.26 -83.82 180)
				(length 3.81)
				(name "IO76UDB1")
				(number "118")
			)
			(pin bidirectional line
				(at 48.26 -86.36 180)
				(length 3.81)
				(name "IO76VDB1")
				(number "117")
			)
			(pin bidirectional line
				(at 48.26 -88.9 180)
				(length 3.81)
				(name "GDC1/IO77UDB1")
				(number "116")
			)
			(pin bidirectional line
				(at 48.26 -91.44 180)
				(length 3.81)
				(name "GDC0/IO77VDB1")
				(number "115")
			)
			(pin bidirectional line
				(at 48.26 -93.98 180)
				(length 3.81)
				(name "GDB1/IO78UDB1")
				(number "114")
			)
			(pin bidirectional line
				(at 48.26 -96.52 180)
				(length 3.81)
				(name "GDB0/IO78VDB1")
				(number "113")
			)
			(pin bidirectional line
				(at 48.26 -99.06 180)
				(length 3.81)
				(name "GDA1/IO79UDB1")
				(number "112")
			)
			(pin bidirectional line
				(at 48.26 -101.6 180)
				(length 3.81)
				(name "GDA0/IO79VDB1")
				(number "111")
			)
		)
		(embedded_fonts no)
	)
	(symbol "A3P600-PQG208"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 45.72 111.76 0)
		)
		(property "Value" "A3P600-PQG208"
			(at 45.72 109.22 0)
		)
		(property "Footprint" "Package_QFP:PQFP-208_28x28mm_P0.5mm"
			(at 45.72 106.68 0)
		)
		(property "Datasheet" "http://www.microsemi.com/document-portal/doc_download/130704-proasic3-flash-family-fpgas-datasheet"
			(at 0 -6.35 0)
		)
		(property "Description" "Actel ProASIC3 Flash Family FPGAs, 600k Gates, 208pin QFP"
			(at 0 0 0)
		)
		(property "ki_keywords" "ProASIC3 ACTEL FLASH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PQFP*28x28mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "A3P600-PQG208_1_0")
		(symbol "A3P600-PQG208_1_1"
			(pin power_in line
				(at -48.26 109.22 0)
				(length 3.81)
				(name "VJTAG")
				(number "110")
			)
			(pin bidirectional line
				(at -48.26 106.68 0)
				(length 3.81)
				(name "TCK")
				(number "101")
			)
			(pin bidirectional line
				(at -48.26 104.14 0)
				(length 3.81)
				(name "TDI")
				(number "102")
			)
			(pin bidirectional line
				(at -48.26 101.6 0)
				(length 3.81)
				(name "TMS")
				(number "103")
			)
			(pin bidirectional line
				(at -48.26 99.06 0)
				(length 3.81)
				(name "TDO")
				(number "108")
			)
			(pin bidirectional line
				(at -48.26 96.52 0)
				(length 3.81)
				(name "TRST")
				(number "109")
			)
			(pin bidirectional line
				(at -48.26 91.44 0)
				(length 3.81)
				(name "IO144NDB3/GEA0")
				(number "49")
			)
			(pin bidirectional line
				(at -48.26 88.9 0)
				(length 3.81)
				(name "IO144PDB3/GEA1")
				(number "48")
			)
			(pin bidirectional line
				(at -48.26 86.36 0)
				(length 3.81)
				(name "IO145NDB3/GEB0")
				(number "47")
			)
			(pin bidirectional line
				(at -48.26 83.82 0)
				(length 3.81)
				(name "IO145PDB3/GEB1")
				(number "46")
			)
			(pin bidirectional line
				(at -48.26 81.28 0)
				(length 3.81)
				(name "IO146NDB3/GEC0")
				(number "45")
			)
			(pin bidirectional line
				(at -48.26 78.74 0)
				(length 3.81)
				(name "IO146PDB3/GEC1")
				(number "44")
			)
			(pin bidirectional line
				(at -48.26 76.2 0)
				(length 3.81)
				(name "IO147NDB3")
				(number "43")
			)
			(pin bidirectional line
				(at -48.26 73.66 0)
				(length 3.81)
				(name "IO147PDB3")
				(number "42")
			)
			(pin bidirectional line
				(at -48.26 71.12 0)
				(length 3.81)
				(name "IO150PSB3")
				(number "39")
			)
			(pin bidirectional line
				(at -48.26 68.58 0)
				(length 3.81)
				(name "IO152NDB3")
				(number "38")
			)
			(pin bidirectional line
				(at -48.26 66.04 0)
				(length 3.81)
				(name "IO152PDB3")
				(number "37")
			)
			(pin bidirectional line
				(at -48.26 63.5 0)
				(length 3.81)
				(name "IO159NDB3")
				(number "35")
			)
			(pin bidirectional line
				(at -48.26 60.96 0)
				(length 3.81)
				(name "IO159PDB3/GFC2")
				(number "34")
			)
			(pin bidirectional line
				(at -48.26 58.42 0)
				(length 3.81)
				(name "IO160NDB3")
				(number "33")
			)
			(pin bidirectional line
				(at -48.26 55.88 0)
				(length 3.81)
				(name "IO160PDB3/GFB2")
				(number "32")
			)
			(pin bidirectional line
				(at -48.26 53.34 0)
				(length 3.81)
				(name "IO161NDB3")
				(number "31")
			)
			(pin bidirectional line
				(at -48.26 50.8 0)
				(length 3.81)
				(name "IO161PDB3/GFA2")
				(number "30")
			)
			(pin bidirectional line
				(at -48.26 48.26 0)
				(length 3.81)
				(name "IO162PPB3/GFA1")
				(number "28")
			)
			(pin bidirectional line
				(at -48.26 45.72 0)
				(length 3.81)
				(name "IO162NPB3/GFA0")
				(number "26")
			)
			(pin bidirectional line
				(at -48.26 43.18 0)
				(length 3.81)
				(name "IO163NDB3/GFB0")
				(number "24")
			)
			(pin bidirectional line
				(at -48.26 40.64 0)
				(length 3.81)
				(name "IO163PDB3/GFB1")
				(number "23")
			)
			(pin bidirectional line
				(at -48.26 38.1 0)
				(length 3.81)
				(name "IO164NDB3/GFC0")
				(number "22")
			)
			(pin bidirectional line
				(at -48.26 35.56 0)
				(length 3.81)
				(name "IO164PDB3/GFC1")
				(number "21")
			)
			(pin bidirectional line
				(at -48.26 33.02 0)
				(length 3.81)
				(name "IO166NDB3")
				(number "20")
			)
			(pin bidirectional line
				(at -48.26 30.48 0)
				(length 3.81)
				(name "IO166PDB3")
				(number "19")
			)
			(pin bidirectional line
				(at -48.26 27.94 0)
				(length 3.81)
				(name "IO168NDB3")
				(number "15")
			)
			(pin bidirectional line
				(at -48.26 25.4 0)
				(length 3.81)
				(name "IO168PDB3")
				(number "14")
			)
			(pin bidirectional line
				(at -48.26 22.86 0)
				(length 3.81)
				(name "IO169NDB3")
				(number "13")
			)
			(pin bidirectional line
				(at -48.26 20.32 0)
				(length 3.81)
				(name "IO169PDB3")
				(number "12")
			)
			(pin bidirectional line
				(at -48.26 17.78 0)
				(length 3.81)
				(name "IO170NDB3")
				(number "11")
			)
			(pin bidirectional line
				(at -48.26 15.24 0)
				(length 3.81)
				(name "IO170PDB3")
				(number "10")
			)
			(pin bidirectional line
				(at -48.26 12.7 0)
				(length 3.81)
				(name "IO171NDB3")
				(number "9")
			)
			(pin bidirectional line
				(at -48.26 10.16 0)
				(length 3.81)
				(name "IO171PDB3")
				(number "8")
			)
			(pin bidirectional line
				(at -48.26 7.62 0)
				(length 3.81)
				(name "IO172NDB3")
				(number "7")
			)
			(pin bidirectional line
				(at -48.26 5.08 0)
				(length 3.81)
				(name "IO172PDB3/GAC2")
				(number "6")
			)
			(pin bidirectional line
				(at -48.26 2.54 0)
				(length 3.81)
				(name "IO173NDB3")
				(number "5")
			)
			(pin bidirectional line
				(at -48.26 0 0)
				(length 3.81)
				(name "IO173PDB3/GAB2")
				(number "4")
			)
			(pin bidirectional line
				(at -48.26 -2.54 0)
				(length 3.81)
				(name "IO174NDB3")
				(number "3")
			)
			(pin bidirectional line
				(at -48.26 -5.08 0)
				(length 3.81)
				(name "IO174PDB3/GAA2")
				(number "2")
			)
			(pin bidirectional line
				(at -48.26 -10.16 0)
				(length 3.81)
				(name "IO89RSB2/GDA2")
				(number "99")
			)
			(pin bidirectional line
				(at -48.26 -12.7 0)
				(length 3.81)
				(name "IO90RSB2/GDB2")
				(number "98")
			)
			(pin bidirectional line
				(at -48.26 -15.24 0)
				(length 3.81)
				(name "IO91RSB2/GDC2")
				(number "96")
			)
			(pin bidirectional line
				(at -48.26 -17.78 0)
				(length 3.81)
				(name "IO92RSB2")
				(number "95")
			)
			(pin bidirectional line
				(at -48.26 -20.32 0)
				(length 3.81)
				(name "IO96RSB2")
				(number "94")
			)
			(pin bidirectional line
				(at -48.26 -22.86 0)
				(length 3.81)
				(name "IO98RSB2")
				(number "93")
			)
			(pin bidirectional line
				(at -48.26 -25.4 0)
				(length 3.81)
				(name "IO100RSB2")
				(number "92")
			)
			(pin bidirectional line
				(at -48.26 -27.94 0)
				(length 3.81)
				(name "IO102RSB2")
				(number "91")
			)
			(pin bidirectional line
				(at -48.26 -30.48 0)
				(length 3.81)
				(name "IO104RSB2")
				(number "90")
			)
			(pin bidirectional line
				(at -48.26 -33.02 0)
				(length 3.81)
				(name "IO106RSB2")
				(number "87")
			)
			(pin bidirectional line
				(at -48.26 -35.56 0)
				(length 3.81)
				(name "IO107RSB2")
				(number "86")
			)
			(pin bidirectional line
				(at -48.26 -38.1 0)
				(length 3.81)
				(name "IO108RSB2")
				(number "85")
			)
			(pin bidirectional line
				(at -48.26 -40.64 0)
				(length 3.81)
				(name "IO109RSB2")
				(number "84")
			)
			(pin bidirectional line
				(at -48.26 -43.18 0)
				(length 3.81)
				(name "IO110RSB2")
				(number "83")
			)
			(pin bidirectional line
				(at -48.26 -45.72 0)
				(length 3.81)
				(name "IO111RSB2")
				(number "82")
			)
			(pin bidirectional line
				(at -48.26 -48.26 0)
				(length 3.81)
				(name "IO112RSB2")
				(number "80")
			)
			(pin bidirectional line
				(at -48.26 -50.8 0)
				(length 3.81)
				(name "IO114RSB2")
				(number "79")
			)
			(pin bidirectional line
				(at -48.26 -53.34 0)
				(length 3.81)
				(name "IO115RSB2")
				(number "78")
			)
			(pin bidirectional line
				(at -48.26 -55.88 0)
				(length 3.81)
				(name "IO116RSB2")
				(number "77")
			)
			(pin bidirectional line
				(at -48.26 -58.42 0)
				(length 3.81)
				(name "IO117RSB2")
				(number "76")
			)
			(pin bidirectional line
				(at -48.26 -60.96 0)
				(length 3.81)
				(name "IO118RSB2")
				(number "75")
			)
			(pin bidirectional line
				(at -48.26 -63.5 0)
				(length 3.81)
				(name "IO119RSB2")
				(number "74")
			)
			(pin bidirectional line
				(at -48.26 -66.04 0)
				(length 3.81)
				(name "IO120RSB2")
				(number "73")
			)
			(pin bidirectional line
				(at -48.26 -68.58 0)
				(length 3.81)
				(name "IO123RSB2")
				(number "70")
			)
			(pin bidirectional line
				(at -48.26 -71.12 0)
				(length 3.81)
				(name "IO125RSB2")
				(number "69")
			)
			(pin bidirectional line
				(at -48.26 -73.66 0)
				(length 3.81)
				(name "IO127RSB2")
				(number "68")
			)
			(pin bidirectional line
				(at -48.26 -76.2 0)
				(length 3.81)
				(name "IO129RSB2")
				(number "67")
			)
			(pin bidirectional line
				(at -48.26 -78.74 0)
				(length 3.81)
				(name "IO131RSB2")
				(number "66")
			)
			(pin bidirectional line
				(at -48.26 -81.28 0)
				(length 3.81)
				(name "IO133RSB2")
				(number "64")
			)
			(pin bidirectional line
				(at -48.26 -83.82 0)
				(length 3.81)
				(name "IO135RSB2")
				(number "63")
			)
			(pin bidirectional line
				(at -48.26 -86.36 0)
				(length 3.81)
				(name "IO136RSB2")
				(number "61")
			)
			(pin bidirectional line
				(at -48.26 -88.9 0)
				(length 3.81)
				(name "IO137RSB2")
				(number "60")
			)
			(pin bidirectional line
				(at -48.26 -91.44 0)
				(length 3.81)
				(name "IO138RSB2")
				(number "59")
			)
			(pin bidirectional line
				(at -48.26 -93.98 0)
				(length 3.81)
				(name "IO139RSB2")
				(number "58")
			)
			(pin bidirectional line
				(at -48.26 -96.52 0)
				(length 3.81)
				(name "IO140RSB2")
				(number "57")
			)
			(pin bidirectional line
				(at -48.26 -99.06 0)
				(length 3.81)
				(name "IO141RSB2/GEC2")
				(number "56")
			)
			(pin bidirectional line
				(at -48.26 -101.6 0)
				(length 3.81)
				(name "IO142RSB2/GEB2")
				(number "55")
			)
			(pin bidirectional line
				(at -48.26 -104.14 0)
				(length 3.81)
				(name "IO143RSB2/GEA2")
				(number "54")
			)
			(pin power_in line
				(at -35.56 116.84 270)
				(length 3.81)
				(name "VCCPLF")
				(number "27")
			)
			(pin power_in line
				(at -30.48 116.84 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at -27.94 116.84 270)
				(length 3.81)
				(name "VCC")
				(number "36")
			)
			(pin power_in line
				(at -27.94 -116.84 90)
				(length 3.81)
				(name "VCOMPLF")
				(number "25")
			)
			(pin power_in line
				(at -25.4 116.84 270)
				(length 3.81)
				(name "VCC")
				(number "71")
			)
			(pin power_in line
				(at -22.86 116.84 270)
				(length 3.81)
				(name "VCC")
				(number "88")
			)
			(pin power_in line
				(at -22.86 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -20.32 116.84 270)
				(length 3.81)
				(name "VCC")
				(number "142")
			)
			(pin power_in line
				(at -20.32 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 3.81)
				(name "VCC")
				(number "171")
			)
			(pin power_in line
				(at -17.78 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 3.81)
				(name "VCC")
				(number "187")
			)
			(pin power_in line
				(at -15.24 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "41")
			)
			(pin power_in line
				(at -12.7 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "52")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 3.81)
				(name "VCCIB0")
				(number "200")
			)
			(pin power_in line
				(at -10.16 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 3.81)
				(name "VCCIB0")
				(number "186")
			)
			(pin power_in line
				(at -7.62 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "81")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 3.81)
				(name "VCCIB0")
				(number "170")
			)
			(pin power_in line
				(at -5.08 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "97")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 3.81)
				(name "VCCIB1")
				(number "140")
			)
			(pin power_in line
				(at -2.54 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "105")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 3.81)
				(name "VCCIB1")
				(number "123")
			)
			(pin power_in line
				(at 0 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "122")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 3.81)
				(name "VCCIB2")
				(number "89")
			)
			(pin power_in line
				(at 2.54 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "130")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 3.81)
				(name "VCCIB2")
				(number "72")
			)
			(pin power_in line
				(at 5.08 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "141")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 3.81)
				(name "VCCIB2")
				(number "62")
			)
			(pin power_in line
				(at 7.62 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "156")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 3.81)
				(name "VCCIB3")
				(number "40")
			)
			(pin power_in line
				(at 10.16 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "162")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 3.81)
				(name "VCCIB3")
				(number "18")
			)
			(pin power_in line
				(at 12.7 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "178")
			)
			(pin power_in line
				(at 15.24 -116.84 90)
				(length 3.81)
				(name "GND")
				(number "195")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 3.81)
				(name "VMV0")
				(number "157")
			)
			(pin power_in line
				(at 20.32 116.84 270)
				(length 3.81)
				(name "VMV0")
				(number "208")
			)
			(pin power_in line
				(at 20.32 -116.84 90)
				(length 3.81)
				(name "GNDQ")
				(number "51")
			)
			(pin power_in line
				(at 22.86 116.84 270)
				(length 3.81)
				(name "VMV1")
				(number "154")
			)
			(pin power_in line
				(at 22.86 -116.84 90)
				(length 3.81)
				(name "GNDQ")
				(number "100")
			)
			(pin power_in line
				(at 25.4 116.84 270)
				(length 3.81)
				(name "VMV2")
				(number "53")
			)
			(pin power_in line
				(at 25.4 -116.84 90)
				(length 3.81)
				(name "GNDQ")
				(number "107")
			)
			(pin power_in line
				(at 27.94 116.84 270)
				(length 3.81)
				(name "VMV2")
				(number "104")
			)
			(pin power_in line
				(at 27.94 -116.84 90)
				(length 3.81)
				(name "GNDQ")
				(number "155")
			)
			(pin power_in line
				(at 30.48 116.84 270)
				(length 3.81)
				(name "VMV3")
				(number "50")
			)
			(pin power_in line
				(at 30.48 -116.84 90)
				(length 3.81)
				(name "GNDQ")
				(number "207")
			)
			(pin power_in line
				(at 35.56 116.84 270)
				(length 3.81)
				(name "VPUMP")
				(number "106")
			)
			(pin bidirectional line
				(at 48.26 91.44 180)
				(length 3.81)
				(name "GAA0/IO00RSB0")
				(number "206")
			)
			(pin bidirectional line
				(at 48.26 88.9 180)
				(length 3.81)
				(name "GAA1/IO01RSB0")
				(number "205")
			)
			(pin bidirectional line
				(at 48.26 86.36 180)
				(length 3.81)
				(name "GAB0/IO02RSB0")
				(number "204")
			)
			(pin bidirectional line
				(at 48.26 83.82 180)
				(length 3.81)
				(name "GAB1/IO03RSB0")
				(number "203")
			)
			(pin bidirectional line
				(at 48.26 81.28 180)
				(length 3.81)
				(name "GAC0/IO04RSB0")
				(number "202")
			)
			(pin bidirectional line
				(at 48.26 78.74 180)
				(length 3.81)
				(name "GAC1/IO05RSB0")
				(number "201")
			)
			(pin bidirectional line
				(at 48.26 76.2 180)
				(length 3.81)
				(name "IO07RSB0")
				(number "199")
			)
			(pin bidirectional line
				(at 48.26 73.66 180)
				(length 3.81)
				(name "IO08RSB0")
				(number "198")
			)
			(pin bidirectional line
				(at 48.26 71.12 180)
				(length 3.81)
				(name "IO09RSB0")
				(number "197")
			)
			(pin bidirectional line
				(at 48.26 68.58 180)
				(length 3.81)
				(name "IO10RSB0")
				(number "196")
			)
			(pin bidirectional line
				(at 48.26 66.04 180)
				(length 3.81)
				(name "IO12RSB0")
				(number "194")
			)
			(pin bidirectional line
				(at 48.26 63.5 180)
				(length 3.81)
				(name "IO14RSB0")
				(number "193")
			)
			(pin bidirectional line
				(at 48.26 60.96 180)
				(length 3.81)
				(name "IO16RSB0")
				(number "192")
			)
			(pin bidirectional line
				(at 48.26 58.42 180)
				(length 3.81)
				(name "IO17RSB0")
				(number "191")
			)
			(pin bidirectional line
				(at 48.26 55.88 180)
				(length 3.81)
				(name "IO18RSB0")
				(number "190")
			)
			(pin bidirectional line
				(at 48.26 53.34 180)
				(length 3.81)
				(name "IO19RSB0")
				(number "189")
			)
			(pin bidirectional line
				(at 48.26 50.8 180)
				(length 3.81)
				(name "IO20RSB0")
				(number "188")
			)
			(pin bidirectional line
				(at 48.26 48.26 180)
				(length 3.81)
				(name "IO23RSB0")
				(number "185")
			)
			(pin bidirectional line
				(at 48.26 45.72 180)
				(length 3.81)
				(name "IO24RSB0")
				(number "184")
			)
			(pin bidirectional line
				(at 48.26 43.18 180)
				(length 3.81)
				(name "IO25RSB0")
				(number "183")
			)
			(pin bidirectional line
				(at 48.26 40.64 180)
				(length 3.81)
				(name "IO26RSB0")
				(number "182")
			)
			(pin bidirectional line
				(at 48.26 38.1 180)
				(length 3.81)
				(name "IO27RSB0")
				(number "181")
			)
			(pin bidirectional line
				(at 48.26 35.56 180)
				(length 3.81)
				(name "IO28RSB0")
				(number "180")
			)
			(pin bidirectional line
				(at 48.26 33.02 180)
				(length 3.81)
				(name "IO29RSB0")
				(number "179")
			)
			(pin bidirectional line
				(at 48.26 30.48 180)
				(length 3.81)
				(name "IO31RSB0")
				(number "177")
			)
			(pin bidirectional line
				(at 48.26 27.94 180)
				(length 3.81)
				(name "IO32RSB0")
				(number "176")
			)
			(pin bidirectional line
				(at 48.26 25.4 180)
				(length 3.81)
				(name "IO33RSB0")
				(number "175")
			)
			(pin bidirectional line
				(at 48.26 22.86 180)
				(length 3.81)
				(name "IO34RSB0")
				(number "174")
			)
			(pin bidirectional line
				(at 48.26 20.32 180)
				(length 3.81)
				(name "IO35RSB0")
				(number "173")
			)
			(pin bidirectional line
				(at 48.26 17.78 180)
				(length 3.81)
				(name "IO36RSB0")
				(number "172")
			)
			(pin bidirectional line
				(at 48.26 15.24 180)
				(length 3.81)
				(name "IO44RSB0")
				(number "169")
			)
			(pin bidirectional line
				(at 48.26 12.7 180)
				(length 3.81)
				(name "IO46RSB0")
				(number "168")
			)
			(pin bidirectional line
				(at 48.26 10.16 180)
				(length 3.81)
				(name "IO48RSB0")
				(number "167")
			)
			(pin bidirectional line
				(at 48.26 7.62 180)
				(length 3.81)
				(name "IO50RSB0")
				(number "166")
			)
			(pin bidirectional line
				(at 48.26 5.08 180)
				(length 3.81)
				(name "IO52RSB0")
				(number "165")
			)
			(pin bidirectional line
				(at 48.26 2.54 180)
				(length 3.81)
				(name "GBC0/IO54RSB0")
				(number "164")
			)
			(pin bidirectional line
				(at 48.26 0 180)
				(length 3.81)
				(name "GBC1/IO55RSB0")
				(number "163")
			)
			(pin bidirectional line
				(at 48.26 -2.54 180)
				(length 3.81)
				(name "GBB0/IO56RSB0")
				(number "161")
			)
			(pin bidirectional line
				(at 48.26 -5.08 180)
				(length 3.81)
				(name "GBB1/IO57RSB0")
				(number "160")
			)
			(pin bidirectional line
				(at 48.26 -7.62 180)
				(length 3.81)
				(name "GBA0/IO58RSB0")
				(number "159")
			)
			(pin bidirectional line
				(at 48.26 -10.16 180)
				(length 3.81)
				(name "GBA1/IO59RSB0")
				(number "158")
			)
			(pin bidirectional line
				(at 48.26 -15.24 180)
				(length 3.81)
				(name "GBA2/IO60PDB1")
				(number "153")
			)
			(pin bidirectional line
				(at 48.26 -17.78 180)
				(length 3.81)
				(name "IO60NDB1")
				(number "152")
			)
			(pin bidirectional line
				(at 48.26 -20.32 180)
				(length 3.81)
				(name "GBB2/IO61PDB1")
				(number "151")
			)
			(pin bidirectional line
				(at 48.26 -22.86 180)
				(length 3.81)
				(name "IO61NDB1")
				(number "150")
			)
			(pin bidirectional line
				(at 48.26 -25.4 180)
				(length 3.81)
				(name "GBC2/IO62PDB1")
				(number "149")
			)
			(pin bidirectional line
				(at 48.26 -27.94 180)
				(length 3.81)
				(name "IO62NDB1")
				(number "148")
			)
			(pin bidirectional line
				(at 48.26 -30.48 180)
				(length 3.81)
				(name "IO63PDB1")
				(number "147")
			)
			(pin bidirectional line
				(at 48.26 -33.02 180)
				(length 3.81)
				(name "IO63NDB1")
				(number "146")
			)
			(pin bidirectional line
				(at 48.26 -35.56 180)
				(length 3.81)
				(name "IO64PDB1")
				(number "145")
			)
			(pin bidirectional line
				(at 48.26 -38.1 180)
				(length 3.81)
				(name "IO64NDB1")
				(number "144")
			)
			(pin bidirectional line
				(at 48.26 -40.64 180)
				(length 3.81)
				(name "IO65PSB1")
				(number "143")
			)
			(pin bidirectional line
				(at 48.26 -43.18 180)
				(length 3.81)
				(name "IO67PDB1")
				(number "139")
			)
			(pin bidirectional line
				(at 48.26 -45.72 180)
				(length 3.81)
				(name "IO67NDB1")
				(number "138")
			)
			(pin bidirectional line
				(at 48.26 -48.26 180)
				(length 3.81)
				(name "GCC1/IO69PDB1")
				(number "137")
			)
			(pin bidirectional line
				(at 48.26 -50.8 180)
				(length 3.81)
				(name "GCC0/IO69NDB1")
				(number "136")
			)
			(pin bidirectional line
				(at 48.26 -53.34 180)
				(length 3.81)
				(name "GCB1/IO70PDB1")
				(number "135")
			)
			(pin bidirectional line
				(at 48.26 -55.88 180)
				(length 3.81)
				(name "GCB0/IO70NDB1")
				(number "134")
			)
			(pin bidirectional line
				(at 48.26 -58.42 180)
				(length 3.81)
				(name "GCA0/IO71NDB1")
				(number "133")
			)
			(pin bidirectional line
				(at 48.26 -60.96 180)
				(length 3.81)
				(name "GCA1/IO71PDB1")
				(number "132")
			)
			(pin bidirectional line
				(at 48.26 -63.5 180)
				(length 3.81)
				(name "GCA2/IO72PSB1")
				(number "131")
			)
			(pin bidirectional line
				(at 48.26 -66.04 180)
				(length 3.81)
				(name "GCB2/IO73PSB1")
				(number "129")
			)
			(pin bidirectional line
				(at 48.26 -68.58 180)
				(length 3.81)
				(name "GCC2/IO74PDB1")
				(number "128")
			)
			(pin bidirectional line
				(at 48.26 -71.12 180)
				(length 3.81)
				(name "IO74NDB1")
				(number "127")
			)
			(pin bidirectional line
				(at 48.26 -73.66 180)
				(length 3.81)
				(name "IO77PDB1")
				(number "125")
			)
			(pin bidirectional line
				(at 48.26 -76.2 180)
				(length 3.81)
				(name "IO77NDB1")
				(number "124")
			)
			(pin bidirectional line
				(at 48.26 -78.74 180)
				(length 3.81)
				(name "IO81PSB1")
				(number "121")
			)
			(pin bidirectional line
				(at 48.26 -81.28 180)
				(length 3.81)
				(name "IO82PDB1")
				(number "120")
			)
			(pin bidirectional line
				(at 48.26 -83.82 180)
				(length 3.81)
				(name "IO82NDB1")
				(number "119")
			)
			(pin bidirectional line
				(at 48.26 -86.36 180)
				(length 3.81)
				(name "IO84PDB1")
				(number "118")
			)
			(pin bidirectional line
				(at 48.26 -88.9 180)
				(length 3.81)
				(name "IO84NDB1")
				(number "117")
			)
			(pin bidirectional line
				(at 48.26 -91.44 180)
				(length 3.81)
				(name "GDC1/IO86PDB1")
				(number "116")
			)
			(pin bidirectional line
				(at 48.26 -93.98 180)
				(length 3.81)
				(name "GDC0/IO86NDB1")
				(number "115")
			)
			(pin bidirectional line
				(at 48.26 -96.52 180)
				(length 3.81)
				(name "GDB1/IO87PDB1")
				(number "114")
			)
			(pin bidirectional line
				(at 48.26 -99.06 180)
				(length 3.81)
				(name "GDB0/IO87NDB1")
				(number "113")
			)
			(pin bidirectional line
				(at 48.26 -101.6 180)
				(length 3.81)
				(name "GDA1/IO88PDB1")
				(number "112")
			)
			(pin bidirectional line
				(at 48.26 -104.14 180)
				(length 3.81)
				(name "GDA0/IO88NDB1")
				(number "111")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACT1020PL44"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 16.51 38.1 0)
		)
		(property "Value" "ACT1020PL44"
			(at 16.51 35.56 0)
		)
		(property "Footprint" "Package_LCC:PLCC-44_16.6x16.6mm_P1.27mm"
			(at 16.51 33.02 0)
		)
		(property "Datasheet" "https://www.microsemi.com/document-portal/doc_download/130666-act-1-series-fpgas-datasheet"
			(at 0 0 0)
		)
		(property "Description" "ACT1020-PL44, Actel ACT1 FPGA, PLCC-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Actel FPGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PLCC*16.6x16.6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ACT1020PL44_0_1")
		(symbol "ACT1020PL44_1_1"
			(pin input line
				(at -30.48 27.94 0)
				(length 3.81)
				(name "PRA-IO38")
				(number "38")
			)
			(pin input line
				(at -30.48 25.4 0)
				(length 3.81)
				(name "PRB-IO39")
				(number "39")
			)
			(pin input line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "SDI-IO36")
				(number "36")
			)
			(pin input line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "DCLK-IO37")
				(number "37")
			)
			(pin input line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "MODE")
				(number "34")
			)
			(pin input line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "IO6")
				(number "6")
			)
			(pin input line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "IO5")
				(number "5")
			)
			(pin input line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "IO4")
				(number "4")
			)
			(pin input line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "IO2")
				(number "2")
			)
			(pin input line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "IO1")
				(number "1")
			)
			(pin input line
				(at -30.48 0 0)
				(length 3.81)
				(name "IO44")
				(number "44")
			)
			(pin input line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "IO42")
				(number "42")
			)
			(pin input line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "IO41")
				(number "41")
			)
			(pin input line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "IO40")
				(number "40")
			)
			(pin input line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "IO7")
				(number "7")
			)
			(pin input line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "IO8")
				(number "8")
			)
			(pin input line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "IO9")
				(number "9")
			)
			(pin input line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "IO11")
				(number "11")
			)
			(pin input line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "IO12")
				(number "12")
			)
			(pin input line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "IO13")
				(number "13")
			)
			(pin input line
				(at -30.48 -27.94 0)
				(length 3.81)
				(name "IO15")
				(number "15")
			)
			(pin power_in line
				(at -5.08 35.56 270)
				(length 3.81)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 3.81)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 3.81)
				(name "VCC")
				(number "25")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 3.81)
				(name "GND")
				(number "32")
			)
			(pin power_in line
				(at 5.08 35.56 270)
				(length 3.81)
				(name "VCC")
				(number "35")
			)
			(pin power_in line
				(at 5.08 -35.56 90)
				(length 3.81)
				(name "GND")
				(number "43")
			)
			(pin input line
				(at 30.48 27.94 180)
				(length 3.81)
				(name "IO-CLK")
				(number "33")
			)
			(pin input line
				(at 30.48 5.08 180)
				(length 3.81)
				(name "IO31")
				(number "31")
			)
			(pin input line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "IO30")
				(number "30")
			)
			(pin input line
				(at 30.48 0 180)
				(length 3.81)
				(name "IO29")
				(number "29")
			)
			(pin input line
				(at 30.48 -5.08 180)
				(length 3.81)
				(name "IO28")
				(number "28")
			)
			(pin input line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "IO27")
				(number "27")
			)
			(pin input line
				(at 30.48 -10.16 180)
				(length 3.81)
				(name "IO26")
				(number "26")
			)
			(pin input line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "IO24")
				(number "24")
			)
			(pin input line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "IO23")
				(number "23")
			)
			(pin input line
				(at 30.48 -17.78 180)
				(length 3.81)
				(name "IO22")
				(number "22")
			)
			(pin input line
				(at 30.48 -20.32 180)
				(length 3.81)
				(name "IO20")
				(number "20")
			)
			(pin input line
				(at 30.48 -22.86 180)
				(length 3.81)
				(name "IO19")
				(number "19")
			)
			(pin input line
				(at 30.48 -25.4 180)
				(length 3.81)
				(name "IO18")
				(number "18")
			)
			(pin input line
				(at 30.48 -27.94 180)
				(length 3.81)
				(name "IO17")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACT1020PL68"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 48.26 0)
		)
		(property "Value" "ACT1020PL68"
			(at 10.16 45.72 0)
		)
		(property "Footprint" "Package_LCC:PLCC-68_24.2x24.2mm_P1.27mm"
			(at 10.16 43.18 0)
		)
		(property "Datasheet" "https://www.microsemi.com/document-portal/doc_download/130666-act-1-series-fpgas-datasheet"
			(at 0 0 0)
		)
		(property "Description" "ACT1020-PL68, Actel ACT1 FPGA, PLCC-68"
			(at 0 0 0)
		)
		(property "ki_keywords" "Actel FPGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PLCC*24.2x24.2mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ACT1020PL68_0_1")
		(symbol "ACT1020PL68_1_1"
			(pin input line
				(at -22.86 38.1 0)
				(length 3.81)
				(name "PRA")
				(number "58")
			)
			(pin input line
				(at -22.86 35.56 0)
				(length 3.81)
				(name "PRB")
				(number "59")
			)
			(pin input line
				(at -22.86 33.02 0)
				(length 3.81)
				(name "SDI")
				(number "56")
			)
			(pin input line
				(at -22.86 30.48 0)
				(length 3.81)
				(name "DCLK")
				(number "57")
			)
			(pin input line
				(at -22.86 27.94 0)
				(length 3.81)
				(name "MODE")
				(number "54")
			)
			(pin input line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "IO44")
				(number "44")
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "IO45")
				(number "45")
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "IO46")
				(number "46")
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "IO47")
				(number "47")
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "IO48")
				(number "48")
			)
			(pin input line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "IO50")
				(number "50")
			)
			(pin input line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "IO51")
				(number "51")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "IO53")
				(number "53")
			)
			(pin input line
				(at -22.86 0 0)
				(length 3.81)
				(name "IO60")
				(number "60")
			)
			(pin input line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "IO61")
				(number "61")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "IO62")
				(number "62")
			)
			(pin input line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "IO63")
				(number "63")
			)
			(pin input line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "IO64")
				(number "64")
			)
			(pin input line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "IO65")
				(number "65")
			)
			(pin input line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "IO67")
				(number "67")
			)
			(pin input line
				(at -22.86 -17.78 0)
				(length 3.81)
				(name "IO68")
				(number "68")
			)
			(pin input line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "IO1")
				(number "1")
			)
			(pin input line
				(at -22.86 -22.86 0)
				(length 3.81)
				(name "IO2")
				(number "2")
			)
			(pin input line
				(at -22.86 -25.4 0)
				(length 3.81)
				(name "IO3")
				(number "3")
			)
			(pin input line
				(at -22.86 -27.94 0)
				(length 3.81)
				(name "IO5")
				(number "5")
			)
			(pin input line
				(at -22.86 -30.48 0)
				(length 3.81)
				(name "IO6")
				(number "6")
			)
			(pin input line
				(at -22.86 -33.02 0)
				(length 3.81)
				(name "IO7")
				(number "7")
			)
			(pin input line
				(at -22.86 -35.56 0)
				(length 3.81)
				(name "IO8")
				(number "8")
			)
			(pin input line
				(at -22.86 -38.1 0)
				(length 3.81)
				(name "IO9")
				(number "9")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 3.81)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "14")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 3.81)
				(name "VCC")
				(number "21")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 3.81)
				(name "VCC")
				(number "25")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "32")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 3.81)
				(name "VCC")
				(number "38")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 3.81)
				(name "VCC")
				(number "55")
			)
			(pin power_in line
				(at 5.08 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "66")
			)
			(pin input line
				(at 22.86 38.1 180)
				(length 3.81)
				(name "CLK")
				(number "52")
			)
			(pin input line
				(at 22.86 33.02 180)
				(length 3.81)
				(name "IO10")
				(number "10")
			)
			(pin input line
				(at 22.86 30.48 180)
				(length 3.81)
				(name "IO11")
				(number "11")
			)
			(pin input line
				(at 22.86 27.94 180)
				(length 3.81)
				(name "IO12")
				(number "12")
			)
			(pin input line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "IO13")
				(number "13")
			)
			(pin input line
				(at 22.86 22.86 180)
				(length 3.81)
				(name "IO16")
				(number "16")
			)
			(pin input line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "IO17")
				(number "17")
			)
			(pin input line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "IO18")
				(number "18")
			)
			(pin input line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "IO19")
				(number "19")
			)
			(pin input line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "IO20")
				(number "20")
			)
			(pin input line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "IO22")
				(number "22")
			)
			(pin input line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "IO23")
				(number "23")
			)
			(pin input line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "IO24")
				(number "24")
			)
			(pin input line
				(at 22.86 0 180)
				(length 3.81)
				(name "IO26")
				(number "26")
			)
			(pin input line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "IO27")
				(number "27")
			)
			(pin input line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "IO28")
				(number "28")
			)
			(pin input line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "IO29")
				(number "29")
			)
			(pin input line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "IO30")
				(number "30")
			)
			(pin input line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "IO31")
				(number "31")
			)
			(pin input line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "IO33")
				(number "33")
			)
			(pin input line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "IO34")
				(number "34")
			)
			(pin input line
				(at 22.86 -20.32 180)
				(length 3.81)
				(name "IO35")
				(number "35")
			)
			(pin input line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "IO36")
				(number "36")
			)
			(pin input line
				(at 22.86 -25.4 180)
				(length 3.81)
				(name "IO37")
				(number "37")
			)
			(pin input line
				(at 22.86 -27.94 180)
				(length 3.81)
				(name "IO39")
				(number "39")
			)
			(pin input line
				(at 22.86 -30.48 180)
				(length 3.81)
				(name "IO40")
				(number "40")
			)
			(pin input line
				(at 22.86 -33.02 180)
				(length 3.81)
				(name "IO41")
				(number "41")
			)
			(pin input line
				(at 22.86 -35.56 180)
				(length 3.81)
				(name "IO42")
				(number "42")
			)
			(pin input line
				(at 22.86 -38.1 180)
				(length 3.81)
				(name "IO43")
				(number "43")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACT1225PL84"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 63.5 0)
		)
		(property "Value" "ACT1225PL84"
			(at 10.16 60.96 0)
		)
		(property "Footprint" "Package_LCC:PLCC-84_29.3x29.3mm_P1.27mm"
			(at 10.16 58.42 0)
		)
		(property "Datasheet" "https://www.microsemi.com/document-portal/doc_download/130666-act-1-series-fpgas-datasheet"
			(at 0 0 0)
		)
		(property "Description" "ACT1225-PL84, Actel ACT1 FPGA, PLCC-84"
			(at 0 0 0)
		)
		(property "ki_keywords" "Actel FPGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PLCC*29.3x29.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ACT1225PL84_0_1")
		(symbol "ACT1225PL84_1_1"
			(pin input line
				(at -22.86 53.34 0)
				(length 3.81)
				(name "PRBA")
				(number "81")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 3.81)
				(name "SDI")
				(number "76")
			)
			(pin input line
				(at -22.86 48.26 0)
				(length 3.81)
				(name "SDO")
				(number "52")
			)
			(pin input line
				(at -22.86 45.72 0)
				(length 3.81)
				(name "BIN/OUT")
				(number "35")
			)
			(pin input line
				(at -22.86 43.18 0)
				(length 3.81)
				(name "BIN/IN")
				(number "34")
			)
			(pin input line
				(at -22.86 40.64 0)
				(length 3.81)
				(name "DCLK")
				(number "10")
			)
			(pin input line
				(at -22.86 38.1 0)
				(length 3.81)
				(name "PRBB")
				(number "4")
			)
			(pin input line
				(at -22.86 35.56 0)
				(length 3.81)
				(name "MODE")
				(number "12")
			)
			(pin input line
				(at -22.86 30.48 0)
				(length 3.81)
				(name "IO75")
				(number "75")
			)
			(pin input line
				(at -22.86 27.94 0)
				(length 3.81)
				(name "IO77")
				(number "77")
			)
			(pin input line
				(at -22.86 25.4 0)
				(length 3.81)
				(name "IO78")
				(number "78")
			)
			(pin input line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "IO79")
				(number "79")
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "IO80")
				(number "80")
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "IO82")
				(number "82")
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "IO1")
				(number "1")
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "IO3")
				(number "3")
			)
			(pin input line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "IO5")
				(number "5")
			)
			(pin input line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "IO7")
				(number "7")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "IO8")
				(number "8")
			)
			(pin input line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "IO9")
				(number "9")
			)
			(pin input line
				(at -22.86 0 0)
				(length 3.81)
				(name "IO11")
				(number "11")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "IO13")
				(number "13")
			)
			(pin input line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "IO14")
				(number "14")
			)
			(pin input line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "IO15")
				(number "15")
			)
			(pin input line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "IO16")
				(number "16")
			)
			(pin input line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "IO17")
				(number "17")
			)
			(pin input line
				(at -22.86 -17.78 0)
				(length 3.81)
				(name "IO18")
				(number "18")
			)
			(pin input line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "IO19")
				(number "19")
			)
			(pin input line
				(at -22.86 -22.86 0)
				(length 3.81)
				(name "IO20")
				(number "20")
			)
			(pin input line
				(at -22.86 -25.4 0)
				(length 3.81)
				(name "IO21")
				(number "21")
			)
			(pin input line
				(at -22.86 -27.94 0)
				(length 3.81)
				(name "IO24")
				(number "24")
			)
			(pin input line
				(at -22.86 -30.48 0)
				(length 3.81)
				(name "IO25")
				(number "25")
			)
			(pin input line
				(at -22.86 -33.02 0)
				(length 3.81)
				(name "IO26")
				(number "26")
			)
			(pin input line
				(at -22.86 -35.56 0)
				(length 3.81)
				(name "IO27")
				(number "27")
			)
			(pin input line
				(at -22.86 -38.1 0)
				(length 3.81)
				(name "IO29")
				(number "29")
			)
			(pin input line
				(at -22.86 -40.64 0)
				(length 3.81)
				(name "IO30")
				(number "30")
			)
			(pin input line
				(at -22.86 -43.18 0)
				(length 3.81)
				(name "IO31")
				(number "31")
			)
			(pin input line
				(at -22.86 -45.72 0)
				(length 3.81)
				(name "IO32")
				(number "32")
			)
			(pin input line
				(at -22.86 -53.34 0)
				(length 3.81)
				(name "CLKB")
				(number "2")
			)
			(pin power_in line
				(at -2.54 60.96 270)
				(length 3.81)
				(name "VCC")
				(number "84")
			)
			(pin power_in line
				(at -2.54 -60.96 90)
				(length 3.81)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 0 60.96 270)
				(length 3.81)
				(name "VCC")
				(number "65")
			)
			(pin power_in line
				(at 0 -60.96 90)
				(length 3.81)
				(name "GND")
				(number "28")
			)
			(pin power_in line
				(at 2.54 60.96 270)
				(length 3.81)
				(name "VCC")
				(number "43")
			)
			(pin power_in line
				(at 2.54 -60.96 90)
				(length 3.81)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at 5.08 60.96 270)
				(length 3.81)
				(name "VCC")
				(number "23")
			)
			(pin power_in line
				(at 5.08 -60.96 90)
				(length 3.81)
				(name "GND")
				(number "70")
			)
			(pin input line
				(at 22.86 53.34 180)
				(length 3.81)
				(name "CLKA")
				(number "83")
			)
			(pin input line
				(at 22.86 48.26 180)
				(length 3.81)
				(name "IO33")
				(number "33")
			)
			(pin input line
				(at 22.86 45.72 180)
				(length 3.81)
				(name "IO36")
				(number "36")
			)
			(pin input line
				(at 22.86 43.18 180)
				(length 3.81)
				(name "IO37")
				(number "37")
			)
			(pin input line
				(at 22.86 40.64 180)
				(length 3.81)
				(name "IO38")
				(number "38")
			)
			(pin input line
				(at 22.86 38.1 180)
				(length 3.81)
				(name "IO39")
				(number "39")
			)
			(pin input line
				(at 22.86 35.56 180)
				(length 3.81)
				(name "IO40")
				(number "40")
			)
			(pin input line
				(at 22.86 33.02 180)
				(length 3.81)
				(name "IO41")
				(number "41")
			)
			(pin input line
				(at 22.86 30.48 180)
				(length 3.81)
				(name "IO42")
				(number "42")
			)
			(pin input line
				(at 22.86 27.94 180)
				(length 3.81)
				(name "IO44")
				(number "44")
			)
			(pin input line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "IO45")
				(number "45")
			)
			(pin input line
				(at 22.86 22.86 180)
				(length 3.81)
				(name "IO46")
				(number "46")
			)
			(pin input line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "IO47")
				(number "47")
			)
			(pin input line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "IO48")
				(number "48")
			)
			(pin input line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "IO50")
				(number "50")
			)
			(pin input line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "IO51")
				(number "51")
			)
			(pin input line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "IO53")
				(number "53")
			)
			(pin input line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "IO54")
				(number "54")
			)
			(pin input line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "IO55")
				(number "55")
			)
			(pin input line
				(at 22.86 0 180)
				(length 3.81)
				(name "IO56")
				(number "56")
			)
			(pin input line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "IO57")
				(number "57")
			)
			(pin input line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "IO58")
				(number "58")
			)
			(pin input line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "IO59")
				(number "59")
			)
			(pin input line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "IO60")
				(number "60")
			)
			(pin input line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "IO61")
				(number "61")
			)
			(pin input line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "IO62")
				(number "62")
			)
			(pin input line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "IO66")
				(number "66")
			)
			(pin input line
				(at 22.86 -20.32 180)
				(length 3.81)
				(name "IO67")
				(number "67")
			)
			(pin input line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "IO68")
				(number "68")
			)
			(pin input line
				(at 22.86 -25.4 180)
				(length 3.81)
				(name "IO69")
				(number "69")
			)
			(pin input line
				(at 22.86 -27.94 180)
				(length 3.81)
				(name "IO71")
				(number "71")
			)
			(pin input line
				(at 22.86 -30.48 180)
				(length 3.81)
				(name "IO72")
				(number "72")
			)
			(pin input line
				(at 22.86 -33.02 180)
				(length 3.81)
				(name "IO73")
				(number "73")
			)
			(pin input line
				(at 22.86 -35.56 180)
				(length 3.81)
				(name "IO74")
				(number "74")
			)
			(pin passive line
				(at 22.86 -43.18 180)
				(length 3.81)
				(name "VSV")
				(number "22")
			)
			(pin passive line
				(at 22.86 -45.72 180)
				(length 3.81)
				(name "VPP")
				(number "64")
			)
			(pin passive line
				(at 22.86 -53.34 180)
				(length 3.81)
				(name "VKS")
				(number "63")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EX128-TQ100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 13.97 55.88 0)
		)
		(property "Value" "EX128-TQ100"
			(at 13.97 53.34 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 13.97 50.8 0)
		)
		(property "Datasheet" "http://www.microsemi.com/document-portal/doc_download/130687-ex-datasheet"
			(at 0 -6.35 0)
		)
		(property "Description" "Actel eX FPGA Family, 100pin QFP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Actel FPGA eX eX128"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EX128-TQ100_0_1")
		(symbol "EX128-TQ100_1_1"
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 3.81)
				(name "IO/TDI")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 3.81)
				(name "IO")
				(number "6")
			)
			(pin input line
				(at -25.4 38.1 0)
				(length 3.81)
				(name "TMS")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 3.81)
				(name "IO")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 3.81)
				(name "IO")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 3.81)
				(name "IO")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "IO")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "IO")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "IO")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "IO/TRST")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "IO")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "IO")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "IO")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "IO")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "IO")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "IO")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "IO")
				(number "26")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "IO")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "IO")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "IO")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "IO")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "IO")
				(number "31")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "IO")
				(number "32")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "IO")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "IO/PRB")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "IO")
				(number "38")
			)
			(pin input clock
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "HCLK")
				(number "39")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 3.81)
				(name "IO")
				(number "40")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 3.81)
				(name "IO")
				(number "41")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 3.81)
				(name "IO")
				(number "42")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 3.81)
				(name "IO")
				(number "43")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 3.81)
				(name "IO")
				(number "45")
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 3.81)
				(name "IO")
				(number "46")
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 3.81)
				(name "IO")
				(number "47")
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 3.81)
				(name "IO")
				(number "48")
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 3.81)
				(name "IO/TDO")
				(number "49")
			)
			(pin power_in line
				(at -12.7 53.34 270)
				(length 3.7846)
				(name "VCCI")
				(number "8")
			)
			(pin power_in line
				(at -10.16 53.34 270)
				(length 3.81)
				(name "VCCI")
				(number "20")
			)
			(pin power_in line
				(at -7.62 53.34 270)
				(length 3.81)
				(name "VCCI")
				(number "44")
			)
			(pin power_in line
				(at -7.62 -53.34 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -5.08 53.34 270)
				(length 3.81)
				(name "VCCI")
				(number "58")
			)
			(pin power_in line
				(at -5.08 -53.34 90)
				(length 3.81)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 3.81)
				(name "VCCI")
				(number "82")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 3.81)
				(name "GND")
				(number "36")
			)
			(pin power_in line
				(at 0 -53.34 90)
				(length 3.81)
				(name "GND")
				(number "51")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 3.81)
				(name "VCCA")
				(number "35")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 3.81)
				(name "GND")
				(number "69")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 3.81)
				(name "VCCA")
				(number "67")
			)
			(pin power_in line
				(at 5.08 -53.34 90)
				(length 3.81)
				(name "GND")
				(number "91")
			)
			(pin power_in line
				(at 7.62 53.34 270)
				(length 3.81)
				(name "VCCA")
				(number "90")
			)
			(pin power_in line
				(at 10.16 53.34 270)
				(length 3.81)
				(name "VCCA")
				(number "57")
			)
			(pin power_in line
				(at 10.16 -53.34 90)
				(length 3.81)
				(name "GND/LP")
				(number "68")
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 3.81)
				(name "TCK/IO")
				(number "100")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 3.81)
				(name "IO")
				(number "99")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 3.81)
				(name "IO")
				(number "98")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 3.81)
				(name "IO")
				(number "97")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 3.81)
				(name "IO")
				(number "96")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 3.81)
				(name "IO")
				(number "95")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "IO")
				(number "94")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "IO")
				(number "93")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "PRA/IO")
				(number "92")
			)
			(pin input clock
				(at 25.4 20.32 180)
				(length 3.81)
				(name "CLKB")
				(number "88")
			)
			(pin input clock
				(at 25.4 17.78 180)
				(length 3.81)
				(name "CLKA")
				(number "87")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "IO")
				(number "86")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "IO")
				(number "85")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "IO")
				(number "84")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "IO")
				(number "83")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "IO")
				(number "81")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "IO")
				(number "80")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "IO")
				(number "79")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "IO")
				(number "78")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "IO")
				(number "77")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "IO")
				(number "76")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "IO")
				(number "72")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "IO")
				(number "71")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "IO")
				(number "70")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 3.81)
				(name "IO")
				(number "66")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "IO")
				(number "65")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 3.81)
				(name "IO")
				(number "64")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 3.81)
				(name "IO")
				(number "63")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 3.81)
				(name "IO")
				(number "62")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 3.81)
				(name "IO")
				(number "61")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 3.81)
				(name "IO")
				(number "60")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 3.81)
				(name "IO")
				(number "59")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 3.81)
				(name "IO")
				(number "56")
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 3.81)
				(name "IO")
				(number "55")
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 3.81)
				(name "IO")
				(number "50")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EX128-TQ64"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 13.97 40.64 0)
		)
		(property "Value" "EX128-TQ64"
			(at 13.97 38.1 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 13.97 35.56 0)
		)
		(property "Datasheet" "http://www.microsemi.com/document-portal/doc_download/130687-ex-datasheet"
			(at 0 3.81 0)
		)
		(property "Description" "Actel eX Family FPGA, 64pin QFP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Actel FPGA eX eX128"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EX128-TQ64_0_1")
		(symbol "EX128-TQ64_1_1"
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "IO/TDI")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "IO")
				(number "3")
			)
			(pin input line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "TMS")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "IO")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "IO")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "IO")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "IO")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "IO/TRST")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "IO")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "IO")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "IO")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "IO")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "IO")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "IO")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "IO")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "IO/PRB")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "IO")
				(number "24")
			)
			(pin input clock
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "HCLK")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "IO")
				(number "26")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "IO")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "IO")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 3.81)
				(name "IO")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 3.81)
				(name "IO")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 3.81)
				(name "IO")
				(number "31")
			)
			(pin power_in line
				(at -12.7 38.1 270)
				(length 3.81)
				(name "VCCI")
				(number "6")
			)
			(pin power_in line
				(at -10.16 38.1 270)
				(length 3.81)
				(name "VCCI")
				(number "19")
			)
			(pin power_out line
				(at -10.16 -38.1 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 3.81)
				(name "VCCI")
				(number "37")
			)
			(pin power_out line
				(at -7.62 -38.1 90)
				(length 3.81)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 3.81)
				(name "VCCI")
				(number "52")
			)
			(pin power_out line
				(at -5.08 -38.1 90)
				(length 3.81)
				(name "GND")
				(number "14")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 3.81)
				(name "VCCI")
				(number "61")
			)
			(pin power_out line
				(at -2.54 -38.1 90)
				(length 3.81)
				(name "GND")
				(number "23")
			)
			(pin power_out line
				(at 0 -38.1 90)
				(length 3.81)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 3.81)
				(name "VCCA")
				(number "22")
			)
			(pin power_out line
				(at 2.54 -38.1 90)
				(length 3.81)
				(name "GND")
				(number "46")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 3.81)
				(name "VCCA")
				(number "44")
			)
			(pin power_out line
				(at 5.08 -38.1 90)
				(length 3.81)
				(name "GND")
				(number "58")
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 3.81)
				(name "VCCA")
				(number "57")
			)
			(pin power_in line
				(at 10.16 38.1 270)
				(length 3.81)
				(name "VCCA")
				(number "36")
			)
			(pin power_out line
				(at 10.16 -38.1 90)
				(length 3.81)
				(name "GND/LP")
				(number "45")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "TCK/IO")
				(number "64")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "IO")
				(number "63")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "IO")
				(number "62")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "IO")
				(number "60")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "PRA/IO")
				(number "59")
			)
			(pin input clock
				(at 25.4 15.24 180)
				(length 3.81)
				(name "CLKB")
				(number "56")
			)
			(pin input clock
				(at 25.4 12.7 180)
				(length 3.81)
				(name "CLKA")
				(number "55")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "IO")
				(number "54")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "IO")
				(number "53")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "IO")
				(number "51")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "IO")
				(number "50")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "IO")
				(number "49")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "IO")
				(number "48")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "IO")
				(number "47")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "IO")
				(number "43")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "IO")
				(number "42")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "IO")
				(number "41")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "IO")
				(number "40")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 3.81)
				(name "IO")
				(number "39")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "IO")
				(number "38")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 3.81)
				(name "IO")
				(number "35")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 3.81)
				(name "IO")
				(number "34")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 3.81)
				(name "TDO/IO")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EX256-TQ100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 60.96 0)
		)
		(property "Value" "EX256-TQ100"
			(at 15.24 58.42 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 15.24 55.88 0)
		)
		(property "Datasheet" "http://www.microsemi.com/document-portal/doc_download/130687-ex-datasheet"
			(at 0 0 0)
		)
		(property "Description" "Actel eX FPGA Family, 100pin QFP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Actel FPGA eX eX256"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EX256-TQ100_0_1")
		(symbol "EX256-TQ100_1_1"
			(pin bidirectional line
				(at -25.4 50.8 0)
				(length 3.81)
				(name "IO/TDI")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 3.81)
				(name "IO")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 3.81)
				(name "IO")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 3.81)
				(name "IO")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 3.81)
				(name "IO")
				(number "6")
			)
			(pin input line
				(at -25.4 38.1 0)
				(length 3.81)
				(name "TMS")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 3.81)
				(name "IO")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 3.81)
				(name "IO")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 3.81)
				(name "IO")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "IO")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "IO")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "IO")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "IO/TRST")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "IO")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "IO")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "IO")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "IO")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "IO")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "IO")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "IO")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "IO")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "IO")
				(number "26")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "IO")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "IO")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "IO")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "IO")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "IO")
				(number "31")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "IO")
				(number "32")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "IO")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "IO/PRB")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 3.81)
				(name "IO")
				(number "38")
			)
			(pin input clock
				(at -25.4 -27.94 0)
				(length 3.81)
				(name "HCLK")
				(number "39")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 3.81)
				(name "IO")
				(number "40")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 3.81)
				(name "IO")
				(number "41")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 3.81)
				(name "IO")
				(number "42")
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 3.81)
				(name "IO")
				(number "43")
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 3.81)
				(name "IO")
				(number "45")
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 3.81)
				(name "IO")
				(number "46")
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 3.81)
				(name "IO")
				(number "47")
			)
			(pin bidirectional line
				(at -25.4 -48.26 0)
				(length 3.81)
				(name "IO")
				(number "48")
			)
			(pin bidirectional line
				(at -25.4 -50.8 0)
				(length 3.81)
				(name "IO/TDO")
				(number "49")
			)
			(pin power_in line
				(at -12.7 58.42 270)
				(length 3.81)
				(name "VCCI")
				(number "8")
			)
			(pin power_in line
				(at -10.16 58.42 270)
				(length 3.81)
				(name "VCCI")
				(number "20")
			)
			(pin power_in line
				(at -10.16 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 3.81)
				(name "VCCI")
				(number "44")
			)
			(pin power_in line
				(at -7.62 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 3.81)
				(name "VCCI")
				(number "58")
			)
			(pin power_in line
				(at -5.08 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "36")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 3.81)
				(name "VCCI")
				(number "82")
			)
			(pin power_in line
				(at -2.54 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "51")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "69")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 3.81)
				(name "VCCA")
				(number "35")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 3.81)
				(name "GND")
				(number "91")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 3.81)
				(name "VCCA")
				(number "67")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 3.81)
				(name "VCCA")
				(number "90")
			)
			(pin power_in line
				(at 7.62 -58.42 90)
				(length 3.81)
				(name "GND/LP")
				(number "68")
			)
			(pin power_in line
				(at 12.7 58.42 270)
				(length 3.81)
				(name "VSV")
				(number "57")
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 3.81)
				(name "TCK/IO")
				(number "100")
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 3.81)
				(name "IO")
				(number "99")
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 3.81)
				(name "IO")
				(number "98")
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 3.81)
				(name "IO")
				(number "97")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 3.81)
				(name "IO")
				(number "96")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 3.81)
				(name "IO")
				(number "95")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 3.81)
				(name "IO")
				(number "94")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 3.81)
				(name "IO")
				(number "93")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 3.81)
				(name "PRA/IO")
				(number "92")
			)
			(pin input clock
				(at 25.4 27.94 180)
				(length 3.81)
				(name "CLKB")
				(number "88")
			)
			(pin input clock
				(at 25.4 25.4 180)
				(length 3.81)
				(name "CLKA")
				(number "87")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "IO")
				(number "86")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "IO")
				(number "85")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "IO")
				(number "84")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "IO")
				(number "83")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "IO")
				(number "81")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "IO")
				(number "80")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "IO")
				(number "79")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "IO")
				(number "78")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "IO")
				(number "77")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "IO")
				(number "76")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "IO")
				(number "75")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "IO")
				(number "74")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "IO")
				(number "73")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "IO")
				(number "72")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "IO")
				(number "71")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "IO")
				(number "70")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 3.81)
				(name "IO")
				(number "66")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "IO")
				(number "65")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 3.81)
				(name "IO")
				(number "64")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 3.81)
				(name "IO")
				(number "63")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 3.81)
				(name "IO")
				(number "62")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 3.81)
				(name "IO")
				(number "61")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 3.81)
				(name "IO")
				(number "60")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 3.81)
				(name "IO")
				(number "59")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 3.81)
				(name "IO")
				(number "56")
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 3.81)
				(name "IO")
				(number "55")
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 3.81)
				(name "IO")
				(number "54")
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 3.81)
				(name "IO")
				(number "53")
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 3.81)
				(name "IO")
				(number "52")
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 3.81)
				(name "IO")
				(number "50")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EX64-TQ100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 13.97 45.72 0)
		)
		(property "Value" "EX64-TQ100"
			(at 13.97 43.18 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 13.97 40.64 0)
		)
		(property "Datasheet" "http://www.microsemi.com/document-portal/doc_download/130687-ex-datasheet"
			(at 0 0 0)
		)
		(property "Description" "Actel eX Family FPGA, 100pin QFP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Actel FPGA eX eX64"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EX64-TQ100_0_1")
		(symbol "EX64-TQ100_1_1"
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 3.81)
				(name "IO/TDI")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 3.81)
				(name "IO")
				(number "6")
			)
			(pin input line
				(at -25.4 30.48 0)
				(length 3.81)
				(name "TMS")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "IO")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "IO")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "IO/TRST")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "IO")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "IO")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "IO")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "IO")
				(number "26")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "IO")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "IO")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "IO")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "IO")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "IO")
				(number "31")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "IO")
				(number "32")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "IO")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "IO/PRB")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "IO")
				(number "38")
			)
			(pin input clock
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "HCLK")
				(number "39")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "IO")
				(number "40")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "IO")
				(number "41")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "IO")
				(number "42")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "IO")
				(number "43")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 3.81)
				(name "IO")
				(number "45")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 3.81)
				(name "IO")
				(number "46")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 3.81)
				(name "IO")
				(number "47")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 3.81)
				(name "IO")
				(number "48")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 3.81)
				(name "TDO/IO")
				(number "49")
			)
			(pin power_in line
				(at -12.7 43.18 270)
				(length 3.81)
				(name "VCCI")
				(number "8")
			)
			(pin power_in line
				(at -10.16 43.18 270)
				(length 3.81)
				(name "VCCI")
				(number "20")
			)
			(pin power_out line
				(at -10.16 -43.18 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -7.62 43.18 270)
				(length 3.81)
				(name "VCCI")
				(number "44")
			)
			(pin power_out line
				(at -7.62 -43.18 90)
				(length 3.81)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at -5.08 43.18 270)
				(length 3.81)
				(name "VCCI")
				(number "58")
			)
			(pin power_out line
				(at -5.08 -43.18 90)
				(length 3.81)
				(name "GND")
				(number "36")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 3.81)
				(name "VCCI")
				(number "82")
			)
			(pin power_out line
				(at -2.54 -43.18 90)
				(length 3.81)
				(name "GND")
				(number "51")
			)
			(pin power_out line
				(at 0 -43.18 90)
				(length 3.81)
				(name "GND")
				(number "69")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 3.81)
				(name "VCCA")
				(number "35")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 3.81)
				(name "GND")
				(number "91")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 3.81)
				(name "VCCA")
				(number "57")
			)
			(pin power_in line
				(at 7.62 43.18 270)
				(length 3.81)
				(name "VCCA")
				(number "67")
			)
			(pin power_in line
				(at 10.16 43.18 270)
				(length 3.81)
				(name "VCCA")
				(number "90")
			)
			(pin power_out line
				(at 10.16 -43.18 90)
				(length 3.81)
				(name "GND/LP")
				(number "68")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 3.81)
				(name "TCK/IO")
				(number "100")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 3.81)
				(name "IO")
				(number "99")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 3.81)
				(name "IO")
				(number "98")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "IO")
				(number "97")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "IO")
				(number "96")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "IO")
				(number "95")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "IO")
				(number "94")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "IO")
				(number "93")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "PRA/IO")
				(number "92")
			)
			(pin input clock
				(at 25.4 12.7 180)
				(length 3.81)
				(name "CLKB")
				(number "88")
			)
			(pin input clock
				(at 25.4 10.16 180)
				(length 3.81)
				(name "CLKA")
				(number "87")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "IO")
				(number "86")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "IO")
				(number "85")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "IO")
				(number "84")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "IO")
				(number "83")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "IO")
				(number "81")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "IO")
				(number "80")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "IO")
				(number "79")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "IO")
				(number "78")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "IO")
				(number "77")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "IO")
				(number "71")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 3.81)
				(name "IO")
				(number "70")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "IO")
				(number "66")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 3.81)
				(name "IO")
				(number "64")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 3.81)
				(name "IO")
				(number "62")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 3.81)
				(name "IO")
				(number "60")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 3.81)
				(name "IO")
				(number "56")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 3.81)
				(name "IO")
				(number "55")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EX64-TQ64"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 16.51 35.56 0)
		)
		(property "Value" "EX64-TQ64"
			(at 16.51 33.02 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 16.51 30.48 0)
		)
		(property "Datasheet" "http://www.microsemi.com/document-portal/doc_download/130687-ex-datasheet"
			(at 0 0 0)
		)
		(property "Description" "Actel eX Family FPGA, 64pin QFP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Actel FPGA eX eX64"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "EX64-TQ64_0_1")
		(symbol "EX64-TQ64_1_1"
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "IO/TDI")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "IO")
				(number "3")
			)
			(pin input line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "TMS")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "IO")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "IO")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "IO/TRST")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "IO")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "IO")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "IO")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "IO")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "IO")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "IO")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "IO/PRB")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "IO")
				(number "24")
			)
			(pin input clock
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "HCLK")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "IO")
				(number "26")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "IO")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "IO")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "IO")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "IO")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 3.81)
				(name "IO")
				(number "31")
			)
			(pin power_in line
				(at -12.7 33.02 270)
				(length 3.81)
				(name "VCCI")
				(number "6")
			)
			(pin power_in line
				(at -10.16 33.02 270)
				(length 3.81)
				(name "VCCI")
				(number "19")
			)
			(pin power_out line
				(at -10.16 -33.02 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -7.62 33.02 270)
				(length 3.81)
				(name "VCCI")
				(number "37")
			)
			(pin power_out line
				(at -7.62 -33.02 90)
				(length 3.81)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 3.81)
				(name "VCCI")
				(number "52")
			)
			(pin power_out line
				(at -5.08 -33.02 90)
				(length 3.81)
				(name "GND")
				(number "14")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 3.81)
				(name "VCCI")
				(number "61")
			)
			(pin power_out line
				(at -2.54 -33.02 90)
				(length 3.81)
				(name "GND")
				(number "23")
			)
			(pin power_out line
				(at 0 -33.02 90)
				(length 3.81)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 3.81)
				(name "VCCA")
				(number "22")
			)
			(pin power_out line
				(at 2.54 -33.02 90)
				(length 3.81)
				(name "GND")
				(number "46")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 3.81)
				(name "VCCA")
				(number "44")
			)
			(pin power_out line
				(at 5.08 -33.02 90)
				(length 3.81)
				(name "GND")
				(number "58")
			)
			(pin power_in line
				(at 7.62 33.02 270)
				(length 3.81)
				(name "VCCA")
				(number "57")
			)
			(pin power_out line
				(at 10.16 -33.02 90)
				(length 3.81)
				(name "GND/LP")
				(number "45")
			)
			(pin power_in line
				(at 12.7 33.02 270)
				(length 3.81)
				(name "VSV")
				(number "36")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "TCK/IO")
				(number "64")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "IO")
				(number "63")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "IO")
				(number "62")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "IO")
				(number "60")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "PRA/IO")
				(number "59")
			)
			(pin input clock
				(at 25.4 12.7 180)
				(length 3.81)
				(name "CLKB")
				(number "56")
			)
			(pin input clock
				(at 25.4 10.16 180)
				(length 3.81)
				(name "CLKA")
				(number "55")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "IO")
				(number "54")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "IO")
				(number "53")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "IO")
				(number "51")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "IO")
				(number "50")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "IO")
				(number "49")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "IO")
				(number "48")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "IO")
				(number "47")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "IO")
				(number "43")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "IO")
				(number "42")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "IO")
				(number "39")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 3.81)
				(name "IO")
				(number "38")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "IO")
				(number "35")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 3.81)
				(name "IO")
				(number "34")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 3.81)
				(name "TDO/IO")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "M2GL090T-FG484"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 34.29 59.69 0)
		)
		(property "Value" "M2GL090T-FG484"
			(at 49.53 57.15 0)
		)
		(property "Footprint" "Package_BGA:BGA-484_23.0x23.0mm_Layout22x22_P1.0mm"
			(at 0 -58.42 0)
		)
		(property "Datasheet" "https://www.microsemi.com/document-portal/doc_download/132042-ds0128-igloo2-and-smartfusion2-datasheet"
			(at -58.42 53.34 0)
		)
		(property "Description" "IGLOO2 FPGA and SmartFusion2 SoC FPGA"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA Igloo2 BGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*484*23.0x23.0mm*Layout22x22*P1.0mm*"
			(at 0 0 0)
		)
		(symbol "M2GL090T-FG484_1_1"
			(text "Bank 1"
				(at 0 0 0)
			)
			(pin bidirectional line
				(at -55.88 53.34 0)
				(length 5.08)
				(name "DDRIO62PB1/MDDR_ADDR14")
				(number "D18")
			)
			(pin bidirectional line
				(at -55.88 50.8 0)
				(length 5.08)
				(name "DDRIO62NB1/MDDR_ADDR15")
				(number "E18")
			)
			(pin bidirectional line
				(at -55.88 48.26 0)
				(length 5.08)
				(name "DDRIO63PB1/MDDR_ADDR12")
				(number "E19")
			)
			(pin bidirectional line
				(at -55.88 45.72 0)
				(length 5.08)
				(name "DDRIO63NB1/MDDR_ADDR13")
				(number "D20")
			)
			(pin bidirectional line
				(at -55.88 43.18 0)
				(length 5.08)
				(name "DDRIO64PB1/MDDR_ADDR10")
				(number "A21")
			)
			(pin bidirectional line
				(at -55.88 40.64 0)
				(length 5.08)
				(name "DDRIO64NB1/MDDR_ADDR11")
				(number "B21")
			)
			(pin bidirectional line
				(at -55.88 38.1 0)
				(length 5.08)
				(name "DDRIO65PB1/MDDR_ADDR8")
				(number "E17")
			)
			(pin bidirectional line
				(at -55.88 35.56 0)
				(length 5.08)
				(name "DDRIO65NB1/MDDR_ADDR9")
				(number "F17")
			)
			(pin bidirectional line
				(at -55.88 33.02 0)
				(length 5.08)
				(name "DDRIO66PB1/MDDR_ODT")
				(number "C20")
			)
			(pin bidirectional line
				(at -55.88 30.48 0)
				(length 5.08)
				(name "DDRIO66NB1/MDDR_ADDR7")
				(number "C19")
			)
			(pin bidirectional line
				(at -55.88 27.94 0)
				(length 5.08)
				(name "DDRIO67PB1/MDDR_ADDR5")
				(number "B19")
			)
			(pin bidirectional line
				(at -55.88 25.4 0)
				(length 5.08)
				(name "DDRIO67NB1/MDDR_ADDR6")
				(number "A20")
			)
			(pin bidirectional line
				(at -55.88 22.86 0)
				(length 5.08)
				(name "DDRIO68PB1/MDDR_ADDR3")
				(number "C17")
			)
			(pin bidirectional line
				(at -55.88 20.32 0)
				(length 5.08)
				(name "DDRIO68NB1/MDDR_ADDR4")
				(number "C18")
			)
			(pin bidirectional line
				(at -55.88 17.78 0)
				(length 5.08)
				(name "DDRIO69PB1/MDDR_ADDR1")
				(number "D16")
			)
			(pin bidirectional line
				(at -55.88 15.24 0)
				(length 5.08)
				(name "DDRIO69NB1/MDDR_ADDR2")
				(number "E16")
			)
			(pin bidirectional line
				(at -55.88 12.7 0)
				(length 5.08)
				(name "DDRIO70PB1/MDDR_BA2")
				(number "C16")
			)
			(pin bidirectional line
				(at -55.88 10.16 0)
				(length 5.08)
				(name "DDRIO70NB1/MDDR_ADDR0")
				(number "B17")
			)
			(pin bidirectional line
				(at -55.88 5.08 0)
				(length 5.08)
				(name "DDRIO71PB1/MDDR_BA0")
				(number "A18")
			)
			(pin bidirectional line
				(at -55.88 2.54 0)
				(length 5.08)
				(name "DDRIO71NB1/MDDR_BA1")
				(number "A19")
			)
			(pin bidirectional line
				(at -55.88 0 0)
				(length 5.08)
				(name "DDRIO72PB1/MDDR_CLK")
				(number "A16")
			)
			(pin bidirectional line
				(at -55.88 -2.54 0)
				(length 5.08)
				(name "DDRIO72NB1/MDDR_CLK_N")
				(number "A17")
			)
			(pin bidirectional line
				(at -55.88 -5.08 0)
				(length 5.08)
				(name "DDRIO73PB1/MDDR_RESET_N")
				(number "E15")
			)
			(pin bidirectional line
				(at -55.88 -7.62 0)
				(length 5.08)
				(name "DDRIO73NB1/MDDR_CAS_N")
				(number "F15")
			)
			(pin bidirectional line
				(at -55.88 -10.16 0)
				(length 5.08)
				(name "DDRIO74PB1/MDDR_CKE")
				(number "B15")
			)
			(pin bidirectional line
				(at -55.88 -12.7 0)
				(length 5.08)
				(name "DDRIO74NB1/MDDR_CS_N")
				(number "C15")
			)
			(pin bidirectional line
				(at -55.88 -15.24 0)
				(length 5.08)
				(name "DDRIO75PB1/MDDR_RAS_N")
				(number "F14")
			)
			(pin bidirectional line
				(at -55.88 -17.78 0)
				(length 5.08)
				(name "DDRIO75NB1/MDDR_WE_N")
				(number "G14")
			)
			(pin input line
				(at -55.88 -25.4 0)
				(length 5.08)
				(name "MDDR_IMP_CALIB")
				(number "D7")
			)
			(pin input line
				(at -55.88 -27.94 0)
				(length 5.08)
				(name "XTLOSC_MAIN_EXTAL")
				(number "AA21")
			)
			(pin input line
				(at -55.88 -30.48 0)
				(length 5.08)
				(name "XTLOSC_MAIN_XTAL")
				(number "AB21")
			)
			(pin passive line
				(at 0 60.96 270)
				(length 5.08)
				(hide yes)
				(name "VDDI1")
				(number "B12")
			)
			(pin passive line
				(at 0 60.96 270)
				(length 5.08)
				(hide yes)
				(name "VDDI1")
				(number "B16")
			)
			(pin passive line
				(at 0 60.96 270)
				(length 5.08)
				(hide yes)
				(name "VDDI1")
				(number "B20")
			)
			(pin passive line
				(at 0 60.96 270)
				(length 5.08)
				(hide yes)
				(name "VDDI1")
				(number "B8")
			)
			(pin passive line
				(at 0 60.96 270)
				(length 5.08)
				(hide yes)
				(name "VDDI1")
				(number "C10")
			)
			(pin passive line
				(at 0 60.96 270)
				(length 5.08)
				(hide yes)
				(name "VDDI1")
				(number "C14")
			)
			(pin passive line
				(at 0 60.96 270)
				(length 5.08)
				(hide yes)
				(name "VDDI1")
				(number "C6")
			)
			(pin passive line
				(at 0 60.96 270)
				(length 5.08)
				(hide yes)
				(name "VDDI1")
				(number "D17")
			)
			(pin passive line
				(at 0 60.96 270)
				(length 5.08)
				(hide yes)
				(name "VDDI1")
				(number "E11")
			)
			(pin passive line
				(at 0 60.96 270)
				(length 5.08)
				(hide yes)
				(name "VDDI1")
				(number "F13")
			)
			(pin passive line
				(at 0 60.96 270)
				(length 5.08)
				(hide yes)
				(name "VDDI1")
				(number "F7")
			)
			(pin passive line
				(at 0 60.96 270)
				(length 5.08)
				(hide yes)
				(name "VDDI1")
				(number "F9")
			)
			(pin passive line
				(at 0 60.96 270)
				(length 5.08)
				(hide yes)
				(name "VDDI1")
				(number "H12")
			)
			(pin power_in line
				(at 0 60.96 270)
				(length 5.08)
				(name "VDDI1")
				(number "H14")
			)
			(pin bidirectional line
				(at 55.88 53.34 180)
				(length 5.08)
				(name "MDDR_DQ14/CCC_NE1_CLKI3/DDRIO76PB1")
				(number "D14")
			)
			(pin bidirectional line
				(at 55.88 50.8 180)
				(length 5.08)
				(name "MDDR_DQ15/DDRIO76NB1")
				(number "E13")
			)
			(pin bidirectional line
				(at 55.88 48.26 180)
				(length 5.08)
				(name "MDDR_DQ12/CCC_NE1_CLKI2/GB12/DDRIO77PB1")
				(number "A14")
			)
			(pin bidirectional line
				(at 55.88 45.72 180)
				(length 5.08)
				(name "MDDR_DQ13/DDRIO77NB1")
				(number "A15")
			)
			(pin bidirectional line
				(at 55.88 43.18 180)
				(length 5.08)
				(name "MDDR_TMATCH_0_IN/DDRIO78PB1")
				(number "G12")
			)
			(pin bidirectional line
				(at 55.88 40.64 180)
				(length 5.08)
				(name "MDDR_DM_RDQS1/DDRIO78NB1")
				(number "G13")
			)
			(pin bidirectional line
				(at 55.88 38.1 180)
				(length 5.08)
				(name "MDDR_DQS1/CCC_NE0_CLKI3/GB8/DDRIO79PB1")
				(number "B13")
			)
			(pin bidirectional line
				(at 55.88 35.56 180)
				(length 5.08)
				(name "MDDR_DQS1_N/DDRIO79NB1")
				(number "C13")
			)
			(pin bidirectional line
				(at 55.88 33.02 180)
				(length 5.08)
				(name "CCC_NE0_CLKI2/MDDR_DQ10/DDRIO80PB1")
				(number "D12")
			)
			(pin bidirectional line
				(at 55.88 30.48 180)
				(length 5.08)
				(name "MDDR_DQ11/DDRIO80NB1")
				(number "D13")
			)
			(pin bidirectional line
				(at 55.88 27.94 180)
				(length 5.08)
				(name "MDDR_DQ8/DDRIO81PB1")
				(number "A12")
			)
			(pin bidirectional line
				(at 55.88 25.4 180)
				(length 5.08)
				(name "MDDR_DQ9/DDRIO81NB1")
				(number "A13")
			)
			(pin bidirectional line
				(at 55.88 22.86 180)
				(length 5.08)
				(name "MDDR_DQ7/DDRIO82PB1")
				(number "E12")
			)
			(pin bidirectional line
				(at 55.88 20.32 180)
				(length 5.08)
				(name "MDDR_TMATCH_0_OUT/DDRIO82NB1")
				(number "F12")
			)
			(pin bidirectional line
				(at 55.88 17.78 180)
				(length 5.08)
				(name "MDDR_DQ5/DDRIO83PB1")
				(number "D10")
			)
			(pin bidirectional line
				(at 55.88 15.24 180)
				(length 5.08)
				(name "MDDR_DQ6/DDRIO83NB1")
				(number "D11")
			)
			(pin bidirectional line
				(at 55.88 12.7 180)
				(length 5.08)
				(name "MDDR_DM_RDQS0/DDRIO84PB1")
				(number "A10")
			)
			(pin bidirectional line
				(at 55.88 10.16 180)
				(length 5.08)
				(name "MDDR_DQ4/DDRIO84NB1")
				(number "A11")
			)
			(pin bidirectional line
				(at 55.88 7.62 180)
				(length 5.08)
				(name "MDDR_DQS0/DDRIO85PB1")
				(number "B11")
			)
			(pin bidirectional line
				(at 55.88 5.08 180)
				(length 5.08)
				(name "MDDR_DQS0_N/DDRIO85NB1")
				(number "C11")
			)
			(pin bidirectional line
				(at 55.88 2.54 180)
				(length 5.08)
				(name "MDDR_DQ2/DDRIO86PB1")
				(number "F10")
			)
			(pin bidirectional line
				(at 55.88 0 180)
				(length 5.08)
				(name "MDDR_DQ3/DDRIO86NB1")
				(number "E10")
			)
			(pin bidirectional line
				(at 55.88 -2.54 180)
				(length 5.08)
				(name "MDDR_DQ0/DDRIO87PB1")
				(number "B9")
			)
			(pin bidirectional line
				(at 55.88 -5.08 180)
				(length 5.08)
				(name "MDDR_DQ1/DDRIO87NB1")
				(number "A9")
			)
			(pin bidirectional line
				(at 55.88 -10.16 180)
				(length 5.08)
				(name "CCC_NW1_CLKI3/DDRIO88PB1")
				(number "D9")
			)
			(pin bidirectional line
				(at 55.88 -12.7 180)
				(length 5.08)
				(name "DDRIO88NB1")
				(number "C9")
			)
			(pin bidirectional line
				(at 55.88 -15.24 180)
				(length 5.08)
				(name "MDDR_DQ_ECC1/DDRIO89PB1")
				(number "A7")
			)
			(pin bidirectional line
				(at 55.88 -17.78 180)
				(length 5.08)
				(name "MDDR_DQ_ECC0/DDRIO89NB1")
				(number "A8")
			)
			(pin output line
				(at 55.88 -20.32 180)
				(length 5.08)
				(name "MDDR_TMATCH_ECC_IN/DDRIO90PB1")
				(number "E8")
			)
			(pin bidirectional line
				(at 55.88 -22.86 180)
				(length 5.08)
				(name "MDDR_DM_RDQS_ECC/DDRIO90NB1")
				(number "D8")
			)
			(pin bidirectional line
				(at 55.88 -25.4 180)
				(length 5.08)
				(name "MDDR_DQS_ECC/DDRIO91PB1")
				(number "C7")
			)
			(pin bidirectional line
				(at 55.88 -27.94 180)
				(length 5.08)
				(name "MDDR_DQS_ECC_N/DDRIO91NB1")
				(number "B7")
			)
			(pin bidirectional line
				(at 55.88 -30.48 180)
				(length 5.08)
				(name "CCC_NW0_CLKI3/GB0/DDRIO92PB1")
				(number "B6")
			)
			(pin bidirectional line
				(at 55.88 -33.02 180)
				(length 5.08)
				(name "CCC_NW1_CLKI2/GB4/DDRIO92NB1")
				(number "A6")
			)
			(pin bidirectional line
				(at 55.88 -35.56 180)
				(length 5.08)
				(name "MDDR_TMATCH_ECC_OUT/DDRIO93PB1")
				(number "E7")
			)
			(pin bidirectional line
				(at 55.88 -38.1 180)
				(length 5.08)
				(name "CCC_NW0_CLKI2/DDRIO93NB1")
				(number "F8")
			)
			(pin bidirectional line
				(at 55.88 -40.64 180)
				(length 5.08)
				(name "DDRIO97PB1")
				(number "C5")
			)
			(pin bidirectional line
				(at 55.88 -43.18 180)
				(length 5.08)
				(name "DDRIO97NB1")
				(number "D6")
			)
			(pin bidirectional line
				(at 55.88 -45.72 180)
				(length 5.08)
				(name "DDRIO98PB1")
				(number "B5")
			)
			(pin bidirectional line
				(at 55.88 -48.26 180)
				(length 5.08)
				(name "DDRIO98NB1")
				(number "A5")
			)
			(pin bidirectional line
				(at 55.88 -50.8 180)
				(length 5.08)
				(name "DDRIO99PB1")
				(number "A4")
			)
			(pin bidirectional line
				(at 55.88 -53.34 180)
				(length 5.08)
				(name "DDRIO99NB1")
				(number "A3")
			)
		)
		(symbol "M2GL090T-FG484_2_1"
			(text "Bank 2"
				(at 0 5.08 0)
			)
			(pin input line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "FLASH_GOLDEN_N")
				(number "D22")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "MSIO51PB2")
				(number "H22")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "MSIO51NB2")
				(number "H21")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "MSIO52PB2/CCC_NE0_CLKI1")
				(number "J20")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "MSIO52NB2")
				(number "J19")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "MSIO53PB2/CCC_NE1_CLKI1")
				(number "G22")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "MSIO53NB2")
				(number "G21")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "MSIO54PB2/GB10/VCCC_SE0_CLKI")
				(number "H20")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "MSIO54NB2")
				(number "H19")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "MSIO55PB2/GB14/VCCC_SE1_CLKI")
				(number "G19")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "MSIO55NB2")
				(number "G18")
			)
			(pin passive line
				(at 0 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDDI2")
				(number "E20")
			)
			(pin passive line
				(at 0 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDDI2")
				(number "F22")
			)
			(pin passive line
				(at 0 22.86 270)
				(length 5.08)
				(hide yes)
				(name "VDDI2")
				(number "H18")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VDDI2")
				(number "J21")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "MSIO56PB2")
				(number "F21")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "MSIO56NB2")
				(number "F20")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "MSIO57PB2")
				(number "F19")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "MSIO57NB2")
				(number "F18")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "MSIO58PB2")
				(number "E22")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "MSIO58NB2")
				(number "E21")
			)
			(pin input line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "MSI59NB2")
				(number "D21")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "MSIO60PB2")
				(number "C22")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "MSIO60NB2")
				(number "B22")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "MSIO61PB2")
				(number "G17")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "MSIO61NB2")
				(number "G16")
			)
		)
		(symbol "M2GL090T-FG484_3_1"
			(text "Bank 3"
				(at 0 0 0)
			)
			(pin bidirectional line
				(at -43.18 33.02 0)
				(length 5.08)
				(name "MSIO0PB3")
				(number "U19")
			)
			(pin bidirectional line
				(at -43.18 30.48 0)
				(length 5.08)
				(name "MSIO0NB3")
				(number "V19")
			)
			(pin bidirectional line
				(at -43.18 27.94 0)
				(length 5.08)
				(name "MSIO1PB3")
				(number "R17")
			)
			(pin bidirectional line
				(at -43.18 25.4 0)
				(length 5.08)
				(name "MSIO1NB3")
				(number "R18")
			)
			(pin bidirectional line
				(at -43.18 22.86 0)
				(length 5.08)
				(name "MSIO2PB3")
				(number "T18")
			)
			(pin bidirectional line
				(at -43.18 20.32 0)
				(length 5.08)
				(name "MSIO2NB3")
				(number "T19")
			)
			(pin bidirectional line
				(at -43.18 17.78 0)
				(length 5.08)
				(name "MSIO3PB3")
				(number "V22")
			)
			(pin bidirectional line
				(at -43.18 15.24 0)
				(length 5.08)
				(name "MSIO3NB3")
				(number "V21")
			)
			(pin bidirectional line
				(at -43.18 12.7 0)
				(length 5.08)
				(name "MSIO4PB3")
				(number "U22")
			)
			(pin bidirectional line
				(at -43.18 10.16 0)
				(length 5.08)
				(name "MSIO4NB3")
				(number "U21")
			)
			(pin bidirectional line
				(at -43.18 7.62 0)
				(length 5.08)
				(name "MSIO5PB3")
				(number "T20")
			)
			(pin bidirectional line
				(at -43.18 5.08 0)
				(length 5.08)
				(name "MSIO5NB3")
				(number "T21")
			)
			(pin bidirectional line
				(at -43.18 2.54 0)
				(length 5.08)
				(name "MSIO6PB3")
				(number "P17")
			)
			(pin bidirectional line
				(at -43.18 0 0)
				(length 5.08)
				(name "MSIO6NB3")
				(number "P18")
			)
			(pin bidirectional line
				(at -43.18 -2.54 0)
				(length 5.08)
				(name "MSIO7PB3")
				(number "R16")
			)
			(pin bidirectional line
				(at -43.18 -5.08 0)
				(length 5.08)
				(name "MSIO7NB3")
				(number "P16")
			)
			(pin bidirectional line
				(at -43.18 -7.62 0)
				(length 5.08)
				(name "MSIO8PB3")
				(number "N16")
			)
			(pin bidirectional line
				(at -43.18 -10.16 0)
				(length 5.08)
				(name "MSIO8NB3")
				(number "N17")
			)
			(pin bidirectional line
				(at -43.18 -15.24 0)
				(length 5.08)
				(name "MSIO11PB3/CCC_NE0_CLKI0")
				(number "P22")
			)
			(pin bidirectional line
				(at -43.18 -17.78 0)
				(length 5.08)
				(name "MSIO11NB3/CCC_NE1_CLKI0")
				(number "R22")
			)
			(pin bidirectional line
				(at -43.18 -20.32 0)
				(length 5.08)
				(name "MSIO12PB3/SPI_0_CLK")
				(number "N19")
			)
			(pin bidirectional line
				(at -43.18 -22.86 0)
				(length 5.08)
				(name "MSIO12NB3/SPI_0_SDI")
				(number "N20")
			)
			(pin bidirectional line
				(at -43.18 -25.4 0)
				(length 5.08)
				(name "MSIO13PB3/SPI_0_SDO")
				(number "N21")
			)
			(pin bidirectional line
				(at -43.18 -27.94 0)
				(length 5.08)
				(name "MSIO13NB3/SPI_0_SS0")
				(number "N22")
			)
			(pin bidirectional line
				(at -43.18 -30.48 0)
				(length 5.08)
				(name "MSIO14PB3")
				(number "M16")
			)
			(pin bidirectional line
				(at -43.18 -33.02 0)
				(length 5.08)
				(name "MSIO14NB3")
				(number "M17")
			)
			(pin passive line
				(at 0 40.64 270)
				(length 5.08)
				(hide yes)
				(name "VDDI3")
				(number "L17")
			)
			(pin passive line
				(at 0 40.64 270)
				(length 5.08)
				(hide yes)
				(name "VDDI3")
				(number "M20")
			)
			(pin passive line
				(at 0 40.64 270)
				(length 5.08)
				(hide yes)
				(name "VDDI3")
				(number "R19")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 5.08)
				(name "VDDI3")
				(number "T22")
			)
			(pin bidirectional line
				(at 43.18 33.02 180)
				(length 5.08)
				(name "MSIO15PB3")
				(number "M18")
			)
			(pin bidirectional line
				(at 43.18 30.48 180)
				(length 5.08)
				(name "MSIO15NB3")
				(number "M19")
			)
			(pin bidirectional line
				(at 43.18 27.94 180)
				(length 5.08)
				(name "MSIO16PB3")
				(number "M21")
			)
			(pin bidirectional line
				(at 43.18 25.4 180)
				(length 5.08)
				(name "MSIO16NB3")
				(number "M22")
			)
			(pin bidirectional line
				(at 43.18 22.86 180)
				(length 5.08)
				(name "MSIO17PB3")
				(number "L21")
			)
			(pin bidirectional line
				(at 43.18 20.32 180)
				(length 5.08)
				(name "MSIO17NB3")
				(number "L20")
			)
			(pin bidirectional line
				(at 43.18 17.78 180)
				(length 5.08)
				(name "MSIO18PB3")
				(number "L19")
			)
			(pin bidirectional line
				(at 43.18 15.24 180)
				(length 5.08)
				(name "MSIO18NB3")
				(number "L18")
			)
			(pin bidirectional line
				(at 43.18 12.7 180)
				(length 5.08)
				(name "MSIO19PB3")
				(number "K21")
			)
			(pin bidirectional line
				(at 43.18 10.16 180)
				(length 5.08)
				(name "MSIO19NB3")
				(number "K20")
			)
			(pin bidirectional line
				(at 43.18 7.62 180)
				(length 5.08)
				(name "VCCC_SE0_CLKI/GB9/MSIO20PB3")
				(number "K22")
			)
			(pin bidirectional line
				(at 43.18 5.08 180)
				(length 5.08)
				(name "VCCC_SE1_CLKI/GB13/MSIO20NB3")
				(number "J22")
			)
			(pin bidirectional line
				(at 43.18 0 180)
				(length 5.08)
				(name "MSIO22PB3")
				(number "L16")
			)
			(pin bidirectional line
				(at 43.18 -2.54 180)
				(length 5.08)
				(name "MSIO22NB3")
				(number "K15")
			)
			(pin bidirectional line
				(at 43.18 -5.08 180)
				(length 5.08)
				(name "MSIO23PB3")
				(number "K17")
			)
			(pin bidirectional line
				(at 43.18 -7.62 180)
				(length 5.08)
				(name "MSIO23NB3")
				(number "K16")
			)
			(pin bidirectional line
				(at 43.18 -10.16 180)
				(length 5.08)
				(name "MSIO24PB3")
				(number "K18")
			)
			(pin bidirectional line
				(at 43.18 -12.7 180)
				(length 5.08)
				(name "MSIO24NB3")
				(number "J18")
			)
			(pin output line
				(at 43.18 -17.78 180)
				(length 5.08)
				(name "SC_SPI_CLK")
				(number "R20")
			)
			(pin input line
				(at 43.18 -20.32 180)
				(length 5.08)
				(name "SC_SPI_SDI")
				(number "R21")
			)
			(pin output line
				(at 43.18 -22.86 180)
				(length 5.08)
				(name "SC_SPI_SDO")
				(number "P19")
			)
			(pin output line
				(at 43.18 -25.4 180)
				(length 5.08)
				(name "SC_SPI_SS")
				(number "P20")
			)
		)
		(symbol "M2GL090T-FG484_4_1"
			(text "Bank 4"
				(at 2.54 0 0)
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "JTAGSEL")
				(number "AA22")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "JTAG_TCK")
				(number "W20")
			)
			(pin input line
				(at -20.32 0 0)
				(length 5.08)
				(name "JTAG_TDI")
				(number "W22")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "JTAG_TMS")
				(number "V20")
			)
			(pin output line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "JTAG_TDO")
				(number "Y21")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "JTAG_TRSTB")
				(number "Y22")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDDI4")
				(number "W21")
			)
		)
		(symbol "M2GL090T-FG484_5_1"
			(text "Bank 5"
				(at 0 2.54 0)
			)
			(pin input line
				(at -55.88 40.64 0)
				(length 5.08)
				(name "DEVRST_N")
				(number "R15")
			)
			(pin bidirectional line
				(at -55.88 35.56 0)
				(length 5.08)
				(name "MSIO196PB5")
				(number "W9")
			)
			(pin bidirectional line
				(at -55.88 33.02 0)
				(length 5.08)
				(name "MSIO196NB5/CCC_SW0_CLKI2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -55.88 30.48 0)
				(length 5.08)
				(name "MSIO197PB5/PROBE_A")
				(number "W10")
			)
			(pin bidirectional line
				(at -55.88 27.94 0)
				(length 5.08)
				(name "MSIO197NB5/PROBE_B")
				(number "Y10")
			)
			(pin bidirectional line
				(at -55.88 25.4 0)
				(length 5.08)
				(name "MSIO198PB5")
				(number "AA10")
			)
			(pin bidirectional line
				(at -55.88 22.86 0)
				(length 5.08)
				(name "MSIO198NB5")
				(number "AB10")
			)
			(pin bidirectional line
				(at -55.88 20.32 0)
				(length 5.08)
				(name "MSIO199PB5")
				(number "U10")
			)
			(pin bidirectional line
				(at -55.88 17.78 0)
				(length 5.08)
				(name "MSIO199NB5")
				(number "U11")
			)
			(pin bidirectional line
				(at -55.88 12.7 0)
				(length 5.08)
				(name "MSIO201PB5/GB3/CCC_SW0_CLKI3")
				(number "V11")
			)
			(pin bidirectional line
				(at -55.88 10.16 0)
				(length 5.08)
				(name "MSIO201NB5/GB7/CCC_SW1_CLKI2")
				(number "W11")
			)
			(pin bidirectional line
				(at -55.88 7.62 0)
				(length 5.08)
				(name "MSIO203PB5")
				(number "AA11")
			)
			(pin bidirectional line
				(at -55.88 5.08 0)
				(length 5.08)
				(name "MSIO203NB5")
				(number "AB11")
			)
			(pin bidirectional line
				(at -55.88 2.54 0)
				(length 5.08)
				(name "MSIO204PB5")
				(number "AA12")
			)
			(pin bidirectional line
				(at -55.88 0 0)
				(length 5.08)
				(name "MSIO204NB5")
				(number "Y12")
			)
			(pin bidirectional line
				(at -55.88 -5.08 0)
				(length 5.08)
				(name "MSIO206PB5")
				(number "W12")
			)
			(pin bidirectional line
				(at -55.88 -7.62 0)
				(length 5.08)
				(name "MSIO206NB5")
				(number "V12")
			)
			(pin bidirectional line
				(at -55.88 -12.7 0)
				(length 5.08)
				(name "MSIO208PB5/CCC_SW1_CLKI3")
				(number "AB13")
			)
			(pin bidirectional line
				(at -55.88 -15.24 0)
				(length 5.08)
				(name "MSIO208NB5")
				(number "AB14")
			)
			(pin bidirectional line
				(at -55.88 -17.78 0)
				(length 5.08)
				(name "MSIO209PB5/VCCC_SE0_CLKI")
				(number "AA13")
			)
			(pin bidirectional line
				(at -55.88 -20.32 0)
				(length 5.08)
				(name "MSIO209NB5")
				(number "Y13")
			)
			(pin bidirectional line
				(at -55.88 -22.86 0)
				(length 5.08)
				(name "MSIO210PB5/GB11/VCCC_SE0_CLKI")
				(number "U13")
			)
			(pin bidirectional line
				(at -55.88 -25.4 0)
				(length 5.08)
				(name "MSIO210NB5")
				(number "T13")
			)
			(pin bidirectional line
				(at -55.88 -27.94 0)
				(length 5.08)
				(name "MSIO211PB5")
				(number "V13")
			)
			(pin bidirectional line
				(at -55.88 -30.48 0)
				(length 5.08)
				(name "MSIO211NB5")
				(number "V14")
			)
			(pin bidirectional line
				(at -55.88 -33.02 0)
				(length 5.08)
				(name "MSIO212PB5/GB15/VCCC_SE1_CLKI")
				(number "Y14")
			)
			(pin bidirectional line
				(at -55.88 -35.56 0)
				(length 5.08)
				(name "MSIO212NB5")
				(number "W14")
			)
			(pin bidirectional line
				(at -55.88 -38.1 0)
				(length 5.08)
				(name "MSIO213PB5/VCCC_SE1_CLKI")
				(number "AB15")
			)
			(pin bidirectional line
				(at -55.88 -40.64 0)
				(length 5.08)
				(name "MSIO213NB5")
				(number "AA15")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 5.08)
				(hide yes)
				(name "VDDI5")
				(number "AA19")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 5.08)
				(hide yes)
				(name "VDDI5")
				(number "AB12")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 5.08)
				(hide yes)
				(name "VDDI5")
				(number "T14")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 5.08)
				(hide yes)
				(name "VDDI5")
				(number "V10")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 5.08)
				(hide yes)
				(name "VDDI5")
				(number "W13")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 5.08)
				(name "VDDI5")
				(number "Y16")
			)
			(pin bidirectional line
				(at 55.88 40.64 180)
				(length 5.08)
				(name "MSIO216PB5")
				(number "Y15")
			)
			(pin bidirectional line
				(at 55.88 38.1 180)
				(length 5.08)
				(name "MSIO216NB5")
				(number "W15")
			)
			(pin bidirectional line
				(at 55.88 33.02 180)
				(length 5.08)
				(name "MSIO218PB5")
				(number "U14")
			)
			(pin bidirectional line
				(at 55.88 30.48 180)
				(length 5.08)
				(name "MSIO218NB5")
				(number "U15")
			)
			(pin bidirectional line
				(at 55.88 25.4 180)
				(length 5.08)
				(name "MSIO221PB5")
				(number "AB17")
			)
			(pin bidirectional line
				(at 55.88 22.86 180)
				(length 5.08)
				(name "MSIO221NB5")
				(number "AA18")
			)
			(pin bidirectional line
				(at 55.88 20.32 180)
				(length 5.08)
				(name "MSIO222PB5")
				(number "AA16")
			)
			(pin bidirectional line
				(at 55.88 17.78 180)
				(length 5.08)
				(name "MSIO222NB5")
				(number "AA17")
			)
			(pin bidirectional line
				(at 55.88 12.7 180)
				(length 5.08)
				(name "MSIO224PB5")
				(number "W16")
			)
			(pin bidirectional line
				(at 55.88 10.16 180)
				(length 5.08)
				(name "MSIO224NB5")
				(number "V16")
			)
			(pin bidirectional line
				(at 55.88 5.08 180)
				(length 5.08)
				(name "MSIO226PB5")
				(number "Y17")
			)
			(pin bidirectional line
				(at 55.88 2.54 180)
				(length 5.08)
				(name "MSIO226NB5")
				(number "W17")
			)
			(pin bidirectional line
				(at 55.88 -2.54 180)
				(length 5.08)
				(name "MSIO228PB5")
				(number "Y18")
			)
			(pin bidirectional line
				(at 55.88 -5.08 180)
				(length 5.08)
				(name "MSIO228NB5")
				(number "Y19")
			)
			(pin bidirectional line
				(at 55.88 -10.16 180)
				(length 5.08)
				(name "MSIO230PB5")
				(number "AB18")
			)
			(pin bidirectional line
				(at 55.88 -12.7 180)
				(length 5.08)
				(name "MSIO230NB5")
				(number "AB19")
			)
			(pin bidirectional line
				(at 55.88 -17.78 180)
				(length 5.08)
				(name "MSIO232PB5")
				(number "U16")
			)
			(pin bidirectional line
				(at 55.88 -20.32 180)
				(length 5.08)
				(name "MSIO232NB5")
				(number "T16")
			)
			(pin bidirectional line
				(at 55.88 -22.86 180)
				(length 5.08)
				(name "MSIO234PB5")
				(number "V17")
			)
			(pin bidirectional line
				(at 55.88 -25.4 180)
				(length 5.08)
				(name "MSIO234NB5")
				(number "U17")
			)
			(pin bidirectional line
				(at 55.88 -30.48 180)
				(length 5.08)
				(name "MSIO236PB5")
				(number "Y20")
			)
			(pin bidirectional line
				(at 55.88 -33.02 180)
				(length 5.08)
				(name "MSIO236NB5")
				(number "W19")
			)
			(pin bidirectional line
				(at 55.88 -38.1 180)
				(length 5.08)
				(name "MSIO238PB5")
				(number "V18")
			)
			(pin bidirectional line
				(at 55.88 -40.64 180)
				(length 5.08)
				(name "MSIO238NB5")
				(number "U18")
			)
		)
		(symbol "M2GL090T-FG484_6_1"
			(text "Bank 6"
				(at 0 7.62 0)
			)
			(pin bidirectional line
				(at -48.26 17.78 0)
				(length 5.08)
				(name "MSIOD193PB6/SERDES_0_REFCLK0_P")
				(number "U1")
			)
			(pin bidirectional line
				(at -48.26 15.24 0)
				(length 5.08)
				(name "MSIOD193NB6/SERDES_0_REFCLK0_N")
				(number "T1")
			)
			(pin bidirectional line
				(at -48.26 12.7 0)
				(length 5.08)
				(name "MSIOD194PB6/SERDES_0_REFCLK1_P")
				(number "U3")
			)
			(pin bidirectional line
				(at -48.26 10.16 0)
				(length 5.08)
				(name "MSIOD194NB6/SERDES_0_REFCLK1_N")
				(number "U4")
			)
			(pin input line
				(at -48.26 0 0)
				(length 5.08)
				(name "SERDES_0_RXD0_P")
				(number "W1")
			)
			(pin input line
				(at -48.26 -2.54 0)
				(length 5.08)
				(name "SERDES_0_RXD0_N")
				(number "Y1")
			)
			(pin input line
				(at -48.26 -5.08 0)
				(length 5.08)
				(name "SERDES_0_RXD1_P")
				(number "W3")
			)
			(pin input line
				(at -48.26 -7.62 0)
				(length 5.08)
				(name "SERDES_0_RXD1_N")
				(number "Y3")
			)
			(pin input line
				(at -48.26 -10.16 0)
				(length 5.08)
				(name "SERDES_0_RXD2_P")
				(number "W5")
			)
			(pin input line
				(at -48.26 -12.7 0)
				(length 5.08)
				(name "SERDES_0_RXD2_N")
				(number "Y5")
			)
			(pin input line
				(at -48.26 -15.24 0)
				(length 5.08)
				(name "SERDES_0_RXD3_P")
				(number "W7")
			)
			(pin input line
				(at -48.26 -17.78 0)
				(length 5.08)
				(name "SERDES_0_RXD3_N")
				(number "Y7")
			)
			(pin power_in line
				(at -7.62 -25.4 90)
				(length 5.08)
				(name "SERDES_0_L01_REFRET")
				(number "U6")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 5.08)
				(name "SERDES_0_L01_REXT")
				(number "U5")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VDDI6")
				(number "U2")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 5.08)
				(name "SERDES_0_L23_REFRET")
				(number "V9")
			)
			(pin power_in line
				(at 7.62 -25.4 90)
				(length 5.08)
				(name "SERDES_0_L23_REXT")
				(number "V8")
			)
			(pin output line
				(at 48.26 0 180)
				(length 5.08)
				(name "SERDES_0_TXD0_P")
				(number "AB2")
			)
			(pin output line
				(at 48.26 -2.54 180)
				(length 5.08)
				(name "SERDES_0_TXD0_N")
				(number "AA2")
			)
			(pin output line
				(at 48.26 -5.08 180)
				(length 5.08)
				(name "SERDES_0_TXD1_P")
				(number "AB4")
			)
			(pin output line
				(at 48.26 -7.62 180)
				(length 5.08)
				(name "SERDES_0_TXD1_N")
				(number "AA4")
			)
			(pin output line
				(at 48.26 -10.16 180)
				(length 5.08)
				(name "SERDES_0_TXD2_P")
				(number "AB6")
			)
			(pin output line
				(at 48.26 -12.7 180)
				(length 5.08)
				(name "SERDES_0_TXD2_N")
				(number "AA6")
			)
			(pin output line
				(at 48.26 -15.24 180)
				(length 5.08)
				(name "SERDES_0_TXD3_P")
				(number "AB8")
			)
			(pin output line
				(at 48.26 -17.78 180)
				(length 5.08)
				(name "SERDES_0_TXD3_N")
				(number "AA8")
			)
		)
		(symbol "M2GL090T-FG484_7_1"
			(text "Bank 7"
				(at 0 0 0)
			)
			(pin bidirectional line
				(at -40.64 20.32 0)
				(length 5.08)
				(name "MSIOD175PB7/GB5/CCC_SW1_CLKI1")
				(number "K4")
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "MSIOD175NB7")
				(number "K5")
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 5.08)
				(name "MSIOD176PB7/GB1/CCC_SW0_CLKI1")
				(number "K8")
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "MSIOD176NB7")
				(number "L8")
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "MSIOD177PB7/CCC_SW1_CLKI0")
				(number "M7")
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "MSIOD177NB7")
				(number "L7")
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "MSIOD178PB7/CCC_SW0_CLKI0")
				(number "K1")
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "MSIOD178NB7")
				(number "K2")
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "MSIOD179PB7")
				(number "L2")
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "MSIOD179NB7")
				(number "L3")
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "MSIOD180PB7")
				(number "L4")
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "MSIOD180NB7")
				(number "L5")
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "MSIOD181PB7")
				(number "M5")
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "MSIOD181NB7")
				(number "M6")
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "MSIOD182PB7")
				(number "N5")
			)
			(pin bidirectional line
				(at -40.64 -17.78 0)
				(length 5.08)
				(name "MSIOD182NB7")
				(number "N6")
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "MSIOD183PB7")
				(number "M3")
			)
			(pin bidirectional line
				(at -40.64 -22.86 0)
				(length 5.08)
				(name "MSIOD183NB7")
				(number "M2")
			)
			(pin passive line
				(at 0 30.48 270)
				(length 5.08)
				(hide yes)
				(name "VDDI7")
				(number "K3")
			)
			(pin passive line
				(at 0 30.48 270)
				(length 5.08)
				(hide yes)
				(name "VDDI7")
				(number "L6")
			)
			(pin passive line
				(at 0 30.48 270)
				(length 5.08)
				(hide yes)
				(name "VDDI7")
				(number "N2")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 5.08)
				(name "VDDI7")
				(number "P5")
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "MSIOD184PB7")
				(number "N3")
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "MSIOD184NB7")
				(number "N4")
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "MSIOD185PB7")
				(number "N1")
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "MSIOD185NB7")
				(number "M1")
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "MSIOD186PB7")
				(number "P4")
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "MSIOD186NB7")
				(number "P3")
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "MSIOD187PB7")
				(number "P1")
			)
			(pin bidirectional line
				(at 40.64 2.54 180)
				(length 5.08)
				(name "MSIOD187NB7")
				(number "P2")
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "MSIOD188PB7")
				(number "N8")
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "MSIOD188NB7")
				(number "M8")
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "MSIOD189PB7")
				(number "P6")
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "MSIOD189NB7")
				(number "P7")
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "MSIOD190PB7")
				(number "R2")
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "MSIOD190NB7")
				(number "R1")
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "MSIOD191PB7")
				(number "R3")
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "MSIOD191NB7")
				(number "R4")
			)
			(pin bidirectional line
				(at 40.64 -20.32 180)
				(length 5.08)
				(name "MSIOD192PB7")
				(number "T4")
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "MSIOD192NB7")
				(number "T3")
			)
		)
		(symbol "M2GL090T-FG484_8_1"
			(text "Bank 8"
				(at 0 0 0)
			)
			(pin bidirectional line
				(at -45.72 33.02 0)
				(length 5.08)
				(name "MSIO127PB8")
				(number "C4")
			)
			(pin bidirectional line
				(at -45.72 30.48 0)
				(length 5.08)
				(name "MSIO127NB8")
				(number "D5")
			)
			(pin bidirectional line
				(at -45.72 25.4 0)
				(length 5.08)
				(name "MSIO129PB8")
				(number "C3")
			)
			(pin bidirectional line
				(at -45.72 22.86 0)
				(length 5.08)
				(name "MSIO129NB8")
				(number "B3")
			)
			(pin bidirectional line
				(at -45.72 17.78 0)
				(length 5.08)
				(name "MSIO131PB8")
				(number "G5")
			)
			(pin bidirectional line
				(at -45.72 15.24 0)
				(length 5.08)
				(name "MSIO131NB8")
				(number "G6")
			)
			(pin bidirectional line
				(at -45.72 12.7 0)
				(length 5.08)
				(name "MSIO132PB8")
				(number "F5")
			)
			(pin bidirectional line
				(at -45.72 10.16 0)
				(length 5.08)
				(name "MSIO132NB8")
				(number "F6")
			)
			(pin bidirectional line
				(at -45.72 5.08 0)
				(length 5.08)
				(name "MSIO134PB8")
				(number "D3")
			)
			(pin bidirectional line
				(at -45.72 2.54 0)
				(length 5.08)
				(name "MSIO134NB8")
				(number "D4")
			)
			(pin bidirectional line
				(at -45.72 -2.54 0)
				(length 5.08)
				(name "MSIO136PB8")
				(number "B2")
			)
			(pin bidirectional line
				(at -45.72 -5.08 0)
				(length 5.08)
				(name "MSIO136NB8")
				(number "A2")
			)
			(pin bidirectional line
				(at -45.72 -10.16 0)
				(length 5.08)
				(name "MSIO138PB8")
				(number "E4")
			)
			(pin bidirectional line
				(at -45.72 -12.7 0)
				(length 5.08)
				(name "MSIO138NB8")
				(number "E5")
			)
			(pin bidirectional line
				(at -45.72 -17.78 0)
				(length 5.08)
				(name "MSIO140PB8")
				(number "C1")
			)
			(pin bidirectional line
				(at -45.72 -20.32 0)
				(length 5.08)
				(name "MSIO140NB8")
				(number "B1")
			)
			(pin bidirectional line
				(at -45.72 -25.4 0)
				(length 5.08)
				(name "MSIO142PB8")
				(number "D1")
			)
			(pin bidirectional line
				(at -45.72 -27.94 0)
				(length 5.08)
				(name "MSIO142NB8")
				(number "D2")
			)
			(pin bidirectional line
				(at -45.72 -30.48 0)
				(length 5.08)
				(name "MSIO143PB8")
				(number "E1")
			)
			(pin bidirectional line
				(at -45.72 -33.02 0)
				(length 5.08)
				(name "MSIO143NB8")
				(number "E2")
			)
			(pin passive line
				(at 0 40.64 270)
				(length 5.08)
				(hide yes)
				(name "VDDI8")
				(number "C2")
			)
			(pin passive line
				(at 0 40.64 270)
				(length 5.08)
				(hide yes)
				(name "VDDI8")
				(number "F1")
			)
			(pin passive line
				(at 0 40.64 270)
				(length 5.08)
				(hide yes)
				(name "VDDI8")
				(number "G4")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 5.08)
				(name "VDDI8")
				(number "J7")
			)
			(pin bidirectional line
				(at 45.72 33.02 180)
				(length 5.08)
				(name "MSIO145PB8")
				(number "F3")
			)
			(pin bidirectional line
				(at 45.72 30.48 180)
				(length 5.08)
				(name "MSIO145NB8")
				(number "F4")
			)
			(pin bidirectional line
				(at 45.72 25.4 180)
				(length 5.08)
				(name "MSIO146PB8")
				(number "H7")
			)
			(pin bidirectional line
				(at 45.72 22.86 180)
				(length 5.08)
				(name "MSIO146NB8")
				(number "G7")
			)
			(pin bidirectional line
				(at 45.72 17.78 180)
				(length 5.08)
				(name "MSIO148PB8")
				(number "H6")
			)
			(pin bidirectional line
				(at 45.72 15.24 180)
				(length 5.08)
				(name "MSIO148NB8")
				(number "J6")
			)
			(pin bidirectional line
				(at 45.72 10.16 180)
				(length 5.08)
				(name "MSIO150PB8")
				(number "H4")
			)
			(pin bidirectional line
				(at 45.72 7.62 180)
				(length 5.08)
				(name "MSIO150NB8")
				(number "H5")
			)
			(pin bidirectional line
				(at 45.72 2.54 180)
				(length 5.08)
				(name "MSIO152PB8")
				(number "G2")
			)
			(pin bidirectional line
				(at 45.72 0 180)
				(length 5.08)
				(name "MSIO152NB8")
				(number "F2")
			)
			(pin bidirectional line
				(at 45.72 -5.08 180)
				(length 5.08)
				(name "MSIO154PB8")
				(number "H3")
			)
			(pin bidirectional line
				(at 45.72 -7.62 180)
				(length 5.08)
				(name "MSIO154NB8")
				(number "G3")
			)
			(pin bidirectional line
				(at 45.72 -12.7 180)
				(length 5.08)
				(name "CCC_NW1_CLKI1/GB6/MSIO156PB8")
				(number "H1")
			)
			(pin bidirectional line
				(at 45.72 -15.24 180)
				(length 5.08)
				(name "MSIO156NB8")
				(number "G1")
			)
			(pin bidirectional line
				(at 45.72 -17.78 180)
				(length 5.08)
				(name "CCC_NW0_CLKI1/GB2/MSIO157PB8")
				(number "J3")
			)
			(pin bidirectional line
				(at 45.72 -20.32 180)
				(length 5.08)
				(name "MSIO157NB8")
				(number "J4")
			)
			(pin bidirectional line
				(at 45.72 -22.86 180)
				(length 5.08)
				(name "CCC_NW1_CLKI0/MSIO158PB8")
				(number "J1")
			)
			(pin bidirectional line
				(at 45.72 -25.4 180)
				(length 5.08)
				(name "MSIO158NB8")
				(number "J2")
			)
			(pin bidirectional line
				(at 45.72 -27.94 180)
				(length 5.08)
				(name "CCC_NW0_CLKI0/MSIO159PB8")
				(number "K6")
			)
			(pin bidirectional line
				(at 45.72 -30.48 180)
				(length 5.08)
				(name "MSIO159NB8")
				(number "K7")
			)
		)
		(symbol "M2GL090T-FG484_9_1"
			(text "Core"
				(at 0 0 0)
			)
			(pin power_in line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "HPMS_MDDR_PLL_VDDA")
				(number "H16")
			)
			(pin power_in line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "SERDES_0_L01_VDDAIO")
				(number "R8")
			)
			(pin power_in line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "SERDES_0_L01_VDDAPLL")
				(number "U7")
			)
			(pin power_in line
				(at -33.02 0 0)
				(length 5.08)
				(name "SERDES_0_L23_VDDAIO")
				(number "T10")
			)
			(pin power_in line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "SERDES_0_L23_VDDAPLL")
				(number "U8")
			)
			(pin power_in line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "SERDES_0_PLL_VDDA")
				(number "T8")
			)
			(pin power_in line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "SERDES_0_VDD")
				(number "P8")
			)
			(pin power_in line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "SERDES_0_VDD")
				(number "T9")
			)
			(pin power_in line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "VREF1")
				(number "G10")
			)
			(pin power_in line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "VREF1")
				(number "G11")
			)
			(pin power_in line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "VREF1")
				(number "G15")
			)
			(pin no_connect line
				(at -25.4 10.16 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "T11")
			)
			(pin no_connect line
				(at -25.4 7.62 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "T12")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "H10")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "J11")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "J13")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "J9")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "K10")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "K12")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "K14")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "L11")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "L13")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "L9")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "M10")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "M12")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "M14")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "N11")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "N13")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "N9")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "P10")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "P12")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "P14")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "R11")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 5.08)
				(name "VDD")
				(number "R13")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "A1")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "A22")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AA1")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AA14")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AA3")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AA5")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AA7")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AA9")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AB1")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AB16")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AB22")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AB3")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AB5")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AB7")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "AB9")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B10")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B14")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B18")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B4")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C12")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C21")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C8")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D15")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D19")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E14")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E6")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E9")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F16")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G20")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H11")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H13")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H2")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J10")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J12")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J14")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J5")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K11")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K13")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K19")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K9")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L1")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L10")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L12")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L14")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L22")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M11")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M13")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M4")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M9")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "N10")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "N12")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "N14")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "N18")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "N7")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "P11")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "P13")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "P21")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "P9")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "R10")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "R12")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "R14")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "R5")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "R9")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "T15")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "T17")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "T2")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "U12")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "U20")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "V1")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "V15")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "V2")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "V3")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "V4")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "V5")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "V6")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "V7")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "W18")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "W2")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "W4")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "W6")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "W8")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "Y11")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "Y2")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "Y4")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "Y6")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "Y8")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VPP")
				(number "AA20")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VPP")
				(number "AB20")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VPP")
				(number "L15")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 5.08)
				(hide yes)
				(name "VPP")
				(number "P15")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VPP")
				(number "U9")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 5.08)
				(name "VPPNVM")
				(number "M15")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 5.08)
				(name "VSSNVM")
				(number "N15")
			)
			(pin power_in line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "CCC_NE0_PLL_VDDA")
				(number "H15")
			)
			(pin power_in line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "CCC_NE1_PLL_VDDA")
				(number "J17")
			)
			(pin power_in line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "CCC_NW0_PLL_VDDA")
				(number "H8")
			)
			(pin power_in line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "CCC_NW1_PLL_VDDA")
				(number "G9")
			)
			(pin power_in line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "CCC_SW0_PLL_VDDA")
				(number "T5")
			)
			(pin power_in line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "CCC_SW1_PLL_VDDA")
				(number "R7")
			)
			(pin power_in line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "CCC_NE0_PLL_VSSA")
				(number "J15")
			)
			(pin power_in line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "CCC_NE1_PLL_VSSA")
				(number "J16")
			)
			(pin power_in line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "CCC_NW0_PLL_VSSA")
				(number "J8")
			)
			(pin power_in line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "CCC_NW1_PLL_VSSA")
				(number "G8")
			)
			(pin power_in line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "CCC_SW0_PLL_VSSA")
				(number "R6")
			)
			(pin power_in line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "CCC_SW1_PLL_VSSA")
				(number "T7")
			)
			(pin power_in line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "HPMS_MDDR_PLL_VSSA")
				(number "H17")
			)
			(pin power_in line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "SERDES_0_PLL_VSSA")
				(number "T6")
			)
		)
		(embedded_fonts no)
	)
)
