(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "XC2018-PC68"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XC2018-PC68"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC2018-PC68_0_1")
		(symbol "XC2018-PC68_1_1"
			(pin input line
				(at -24.13 39.37 0)
				(length 7.62)
				(name "~{PWRDWN}")
				(number "10")
			)
			(pin input line
				(at -24.13 36.83 0)
				(length 7.62)
				(name "M0")
				(number "26")
			)
			(pin input line
				(at -24.13 34.29 0)
				(length 7.62)
				(name "M1")
				(number "25")
			)
			(pin bidirectional line
				(at -24.13 31.75 0)
				(length 7.62)
				(name "M2")
				(number "27")
			)
			(pin input line
				(at -24.13 29.21 0)
				(length 7.62)
				(name "~{RESET}")
				(number "44")
			)
			(pin bidirectional line
				(at -24.13 26.67 0)
				(length 7.62)
				(name "D/PROG")
				(number "45")
			)
			(pin bidirectional line
				(at -24.13 24.13 0)
				(length 7.62)
				(name "DIN")
				(number "58")
			)
			(pin bidirectional line
				(at -24.13 21.59 0)
				(length 7.62)
				(name "DOUT")
				(number "59")
			)
			(pin input clock
				(at -24.13 19.05 0)
				(length 7.62)
				(name "CLK")
				(number "60")
			)
			(pin output line
				(at -24.13 16.51 0)
				(length 7.62)
				(name "HDC")
				(number "28")
			)
			(pin output line
				(at -24.13 13.97 0)
				(length 7.62)
				(name "LDC")
				(number "30")
			)
			(pin passive line
				(at -24.13 11.43 0)
				(length 7.62)
				(name "P2")
				(number "2")
			)
			(pin passive line
				(at -24.13 8.89 0)
				(length 7.62)
				(name "P3")
				(number "3")
			)
			(pin passive line
				(at -24.13 6.35 0)
				(length 7.62)
				(name "P4")
				(number "4")
			)
			(pin passive line
				(at -24.13 3.81 0)
				(length 7.62)
				(name "P5")
				(number "5")
			)
			(pin passive line
				(at -24.13 1.27 0)
				(length 7.62)
				(name "P6")
				(number "6")
			)
			(pin passive line
				(at -24.13 -1.27 0)
				(length 7.62)
				(name "P7")
				(number "7")
			)
			(pin passive line
				(at -24.13 -3.81 0)
				(length 7.62)
				(name "P8")
				(number "8")
			)
			(pin passive line
				(at -24.13 -6.35 0)
				(length 7.62)
				(name "P9")
				(number "9")
			)
			(pin passive line
				(at -24.13 -8.89 0)
				(length 7.62)
				(name "P11-GCLK")
				(number "11")
			)
			(pin passive line
				(at -24.13 -11.43 0)
				(length 7.62)
				(name "P12")
				(number "12")
			)
			(pin passive line
				(at -24.13 -13.97 0)
				(length 7.62)
				(name "P13")
				(number "13")
			)
			(pin passive line
				(at -24.13 -16.51 0)
				(length 7.62)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -24.13 -19.05 0)
				(length 7.62)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -24.13 -21.59 0)
				(length 7.62)
				(name "P16")
				(number "16")
			)
			(pin passive line
				(at -24.13 -24.13 0)
				(length 7.62)
				(name "P17")
				(number "17")
			)
			(pin passive line
				(at -24.13 -26.67 0)
				(length 7.62)
				(name "P19")
				(number "19")
			)
			(pin passive line
				(at -24.13 -29.21 0)
				(length 7.62)
				(name "P20")
				(number "20")
			)
			(pin passive line
				(at -24.13 -31.75 0)
				(length 7.62)
				(name "P21")
				(number "21")
			)
			(pin passive line
				(at -24.13 -34.29 0)
				(length 7.62)
				(name "P22")
				(number "22")
			)
			(pin passive line
				(at -24.13 -36.83 0)
				(length 7.62)
				(name "P23")
				(number "23")
			)
			(pin passive line
				(at -24.13 -39.37 0)
				(length 7.62)
				(name "P24")
				(number "24")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "18")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 3.81)
				(name "VCC")
				(number "52")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 24.13 39.37 180)
				(length 7.62)
				(name "P68")
				(number "68")
			)
			(pin passive line
				(at 24.13 36.83 180)
				(length 7.62)
				(name "P67")
				(number "67")
			)
			(pin passive line
				(at 24.13 34.29 180)
				(length 7.62)
				(name "P66")
				(number "66")
			)
			(pin passive line
				(at 24.13 31.75 180)
				(length 7.62)
				(name "P65")
				(number "65")
			)
			(pin passive line
				(at 24.13 29.21 180)
				(length 7.62)
				(name "P64")
				(number "64")
			)
			(pin passive line
				(at 24.13 26.67 180)
				(length 7.62)
				(name "P63")
				(number "63")
			)
			(pin passive line
				(at 24.13 24.13 180)
				(length 7.62)
				(name "P62")
				(number "62")
			)
			(pin passive line
				(at 24.13 21.59 180)
				(length 7.62)
				(name "P61")
				(number "61")
			)
			(pin passive line
				(at 24.13 19.05 180)
				(length 7.62)
				(name "P57")
				(number "57")
			)
			(pin passive line
				(at 24.13 16.51 180)
				(length 7.62)
				(name "P56")
				(number "56")
			)
			(pin passive line
				(at 24.13 13.97 180)
				(length 7.62)
				(name "P55")
				(number "55")
			)
			(pin passive line
				(at 24.13 11.43 180)
				(length 7.62)
				(name "P54")
				(number "54")
			)
			(pin passive line
				(at 24.13 8.89 180)
				(length 7.62)
				(name "P53")
				(number "53")
			)
			(pin passive line
				(at 24.13 6.35 180)
				(length 7.62)
				(name "P51")
				(number "51")
			)
			(pin passive line
				(at 24.13 3.81 180)
				(length 7.62)
				(name "P50")
				(number "50")
			)
			(pin passive line
				(at 24.13 1.27 180)
				(length 7.62)
				(name "P49")
				(number "49")
			)
			(pin passive line
				(at 24.13 -1.27 180)
				(length 7.62)
				(name "P48")
				(number "48")
			)
			(pin passive line
				(at 24.13 -3.81 180)
				(length 7.62)
				(name "P47")
				(number "47")
			)
			(pin passive line
				(at 24.13 -6.35 180)
				(length 7.62)
				(name "P46-XO")
				(number "46")
			)
			(pin passive line
				(at 24.13 -8.89 180)
				(length 7.62)
				(name "P43-XI")
				(number "43")
			)
			(pin passive line
				(at 24.13 -11.43 180)
				(length 7.62)
				(name "P42")
				(number "42")
			)
			(pin passive line
				(at 24.13 -13.97 180)
				(length 7.62)
				(name "P41")
				(number "41")
			)
			(pin passive line
				(at 24.13 -16.51 180)
				(length 7.62)
				(name "P40")
				(number "40")
			)
			(pin passive line
				(at 24.13 -19.05 180)
				(length 7.62)
				(name "P39")
				(number "39")
			)
			(pin passive line
				(at 24.13 -21.59 180)
				(length 7.62)
				(name "P38")
				(number "38")
			)
			(pin passive line
				(at 24.13 -24.13 180)
				(length 7.62)
				(name "P37")
				(number "37")
			)
			(pin passive line
				(at 24.13 -26.67 180)
				(length 7.62)
				(name "P36")
				(number "36")
			)
			(pin passive line
				(at 24.13 -29.21 180)
				(length 7.62)
				(name "P34")
				(number "34")
			)
			(pin passive line
				(at 24.13 -31.75 180)
				(length 7.62)
				(name "P33")
				(number "33")
			)
			(pin passive line
				(at 24.13 -34.29 180)
				(length 7.62)
				(name "P32")
				(number "32")
			)
			(pin passive line
				(at 24.13 -36.83 180)
				(length 7.62)
				(name "P31")
				(number "31")
			)
			(pin passive line
				(at 24.13 -39.37 180)
				(length 7.62)
				(name "P29")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC2018-PC84"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XC2018-PC84"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC2018-PC84_0_1")
		(symbol "XC2018-PC84_1_1"
			(pin input line
				(at -27.94 49.53 0)
				(length 7.62)
				(name "~{PWRDWN}")
				(number "12")
			)
			(pin input line
				(at -27.94 46.99 0)
				(length 7.62)
				(name "M0")
				(number "32")
			)
			(pin input line
				(at -27.94 44.45 0)
				(length 7.62)
				(name "M1")
				(number "31")
			)
			(pin bidirectional line
				(at -27.94 41.91 0)
				(length 7.62)
				(name "M2")
				(number "33")
			)
			(pin input line
				(at -27.94 39.37 0)
				(length 7.62)
				(name "~{RESET}")
				(number "54")
			)
			(pin bidirectional line
				(at -27.94 36.83 0)
				(length 7.62)
				(name "DONE/PROG")
				(number "55")
			)
			(pin input line
				(at -27.94 34.29 0)
				(length 7.62)
				(name "DIN")
				(number "72")
			)
			(pin passive line
				(at -27.94 31.75 0)
				(length 7.62)
				(name "DOUT")
				(number "73")
			)
			(pin bidirectional clock
				(at -27.94 29.21 0)
				(length 7.62)
				(name "CLK")
				(number "74")
			)
			(pin passive line
				(at -27.94 26.67 0)
				(length 7.62)
				(name "HDC")
				(number "34")
			)
			(pin passive line
				(at -27.94 24.13 0)
				(length 7.62)
				(name "LDC")
				(number "36")
			)
			(pin passive line
				(at -27.94 21.59 0)
				(length 7.62)
				(name "P2")
				(number "2")
			)
			(pin passive line
				(at -27.94 19.05 0)
				(length 7.62)
				(name "P3")
				(number "3")
			)
			(pin passive line
				(at -27.94 16.51 0)
				(length 7.62)
				(name "P4")
				(number "4")
			)
			(pin passive line
				(at -27.94 13.97 0)
				(length 7.62)
				(name "P5")
				(number "5")
			)
			(pin passive line
				(at -27.94 11.43 0)
				(length 7.62)
				(name "P6")
				(number "6")
			)
			(pin passive line
				(at -27.94 8.89 0)
				(length 7.62)
				(name "P7")
				(number "7")
			)
			(pin passive line
				(at -27.94 6.35 0)
				(length 7.62)
				(name "P8")
				(number "8")
			)
			(pin passive line
				(at -27.94 3.81 0)
				(length 7.62)
				(name "P9")
				(number "9")
			)
			(pin passive line
				(at -27.94 1.27 0)
				(length 7.62)
				(name "P10")
				(number "10")
			)
			(pin passive line
				(at -27.94 -1.27 0)
				(length 7.62)
				(name "P11/GCLK")
				(number "11")
			)
			(pin passive line
				(at -27.94 -3.81 0)
				(length 7.62)
				(name "P13")
				(number "13")
			)
			(pin passive line
				(at -27.94 -6.35 0)
				(length 7.62)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -27.94 -8.89 0)
				(length 7.62)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -27.94 -11.43 0)
				(length 7.62)
				(name "P16")
				(number "16")
			)
			(pin passive line
				(at -27.94 -13.97 0)
				(length 7.62)
				(name "P17")
				(number "17")
			)
			(pin passive line
				(at -27.94 -16.51 0)
				(length 7.62)
				(name "P18")
				(number "18")
			)
			(pin passive line
				(at -27.94 -19.05 0)
				(length 7.62)
				(name "P19")
				(number "19")
			)
			(pin passive line
				(at -27.94 -21.59 0)
				(length 7.62)
				(name "P20")
				(number "20")
			)
			(pin passive line
				(at -27.94 -24.13 0)
				(length 7.62)
				(name "P21")
				(number "21")
			)
			(pin passive line
				(at -27.94 -26.67 0)
				(length 7.62)
				(name "P23")
				(number "23")
			)
			(pin passive line
				(at -27.94 -29.21 0)
				(length 7.62)
				(name "P24")
				(number "24")
			)
			(pin passive line
				(at -27.94 -31.75 0)
				(length 7.62)
				(name "P25")
				(number "25")
			)
			(pin passive line
				(at -27.94 -34.29 0)
				(length 7.62)
				(name "P26")
				(number "26")
			)
			(pin passive line
				(at -27.94 -36.83 0)
				(length 7.62)
				(name "P27")
				(number "27")
			)
			(pin passive line
				(at -27.94 -39.37 0)
				(length 7.62)
				(name "P28")
				(number "28")
			)
			(pin passive line
				(at -27.94 -41.91 0)
				(length 7.62)
				(name "P29")
				(number "29")
			)
			(pin passive line
				(at -27.94 -44.45 0)
				(length 7.62)
				(name "P30")
				(number "30")
			)
			(pin passive line
				(at -27.94 -46.99 0)
				(length 7.62)
				(name "P35")
				(number "35")
			)
			(pin passive line
				(at -27.94 -49.53 0)
				(length 7.62)
				(name "P37")
				(number "37")
			)
			(pin power_in line
				(at 0 55.88 270)
				(length 3.81)
				(name "VCC")
				(number "22")
			)
			(pin passive line
				(at 0 55.88 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "64")
			)
			(pin power_in line
				(at 0 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at 27.94 49.53 180)
				(length 7.62)
				(name "P84")
				(number "84")
			)
			(pin passive line
				(at 27.94 46.99 180)
				(length 7.62)
				(name "P83")
				(number "83")
			)
			(pin passive line
				(at 27.94 44.45 180)
				(length 7.62)
				(name "P82")
				(number "82")
			)
			(pin passive line
				(at 27.94 41.91 180)
				(length 7.62)
				(name "P81")
				(number "81")
			)
			(pin passive line
				(at 27.94 39.37 180)
				(length 7.62)
				(name "P80")
				(number "80")
			)
			(pin passive line
				(at 27.94 36.83 180)
				(length 7.62)
				(name "P79")
				(number "79")
			)
			(pin passive line
				(at 27.94 34.29 180)
				(length 7.62)
				(name "P78")
				(number "78")
			)
			(pin passive line
				(at 27.94 31.75 180)
				(length 7.62)
				(name "P77")
				(number "77")
			)
			(pin passive line
				(at 27.94 29.21 180)
				(length 7.62)
				(name "P76")
				(number "76")
			)
			(pin passive line
				(at 27.94 26.67 180)
				(length 7.62)
				(name "P75")
				(number "75")
			)
			(pin passive line
				(at 27.94 24.13 180)
				(length 7.62)
				(name "P71")
				(number "71")
			)
			(pin passive line
				(at 27.94 21.59 180)
				(length 7.62)
				(name "WRT/P70")
				(number "70")
			)
			(pin passive line
				(at 27.94 19.05 180)
				(length 7.62)
				(name "P69")
				(number "69")
			)
			(pin passive line
				(at 27.94 16.51 180)
				(length 7.62)
				(name "P68")
				(number "68")
			)
			(pin passive line
				(at 27.94 13.97 180)
				(length 7.62)
				(name "P67")
				(number "67")
			)
			(pin passive line
				(at 27.94 11.43 180)
				(length 7.62)
				(name "CS2/P66")
				(number "66")
			)
			(pin passive line
				(at 27.94 8.89 180)
				(length 7.62)
				(name "P65")
				(number "65")
			)
			(pin passive line
				(at 27.94 6.35 180)
				(length 7.62)
				(name "CS1/P63")
				(number "63")
			)
			(pin passive line
				(at 27.94 3.81 180)
				(length 7.62)
				(name "CS0/P62")
				(number "62")
			)
			(pin passive line
				(at 27.94 1.27 180)
				(length 7.62)
				(name "P61")
				(number "61")
			)
			(pin passive line
				(at 27.94 -1.27 180)
				(length 7.62)
				(name "P60")
				(number "60")
			)
			(pin passive line
				(at 27.94 -3.81 180)
				(length 7.62)
				(name "P59")
				(number "59")
			)
			(pin passive line
				(at 27.94 -6.35 180)
				(length 7.62)
				(name "P58")
				(number "58")
			)
			(pin passive line
				(at 27.94 -8.89 180)
				(length 7.62)
				(name "P57")
				(number "57")
			)
			(pin passive line
				(at 27.94 -11.43 180)
				(length 7.62)
				(name "XTL1(O)/P56")
				(number "56")
			)
			(pin passive line
				(at 27.94 -13.97 180)
				(length 7.62)
				(name "XTL2(I)/P53")
				(number "53")
			)
			(pin passive line
				(at 27.94 -16.51 180)
				(length 7.62)
				(name "P52")
				(number "52")
			)
			(pin passive line
				(at 27.94 -19.05 180)
				(length 7.62)
				(name "P51")
				(number "51")
			)
			(pin passive line
				(at 27.94 -21.59 180)
				(length 7.62)
				(name "P50")
				(number "50")
			)
			(pin passive line
				(at 27.94 -24.13 180)
				(length 7.62)
				(name "P49")
				(number "49")
			)
			(pin passive line
				(at 27.94 -26.67 180)
				(length 7.62)
				(name "P48")
				(number "48")
			)
			(pin passive line
				(at 27.94 -29.21 180)
				(length 7.62)
				(name "P47")
				(number "47")
			)
			(pin passive line
				(at 27.94 -31.75 180)
				(length 7.62)
				(name "P46")
				(number "46")
			)
			(pin passive line
				(at 27.94 -34.29 180)
				(length 7.62)
				(name "P45")
				(number "45")
			)
			(pin passive line
				(at 27.94 -36.83 180)
				(length 7.62)
				(name "P44")
				(number "44")
			)
			(pin passive line
				(at 27.94 -39.37 180)
				(length 7.62)
				(name "P42")
				(number "42")
			)
			(pin passive line
				(at 27.94 -41.91 180)
				(length 7.62)
				(name "P41")
				(number "41")
			)
			(pin passive line
				(at 27.94 -44.45 180)
				(length 7.62)
				(name "P40")
				(number "40")
			)
			(pin passive line
				(at 27.94 -46.99 180)
				(length 7.62)
				(name "P39")
				(number "39")
			)
			(pin passive line
				(at 27.94 -49.53 180)
				(length 7.62)
				(name "P38")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC2C256-TQ144"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 90.17 0)
		)
		(property "Value" "XC2C256-TQ144"
			(at 21.59 -90.17 0)
		)
		(property "Footprint" "Package_QFP:TQFP-144_20x20mm_P0.5mm"
			(at 36.83 -92.71 0)
		)
		(property "Datasheet" "https://www.xilinx.com/support/documentation/data_sheets/ds094.pdf"
			(at -1.27 19.05 0)
		)
		(property "Description" "CoolRunner-II CPLD, 256 macrocells"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "XC2C256-TQ144_0_1")
		(symbol "XC2C256-TQ144_1_1"
			(pin bidirectional line
				(at -27.94 86.36 0)
				(length 5.08)
				(name "P137")
				(number "137")
			)
			(pin bidirectional line
				(at -27.94 83.82 0)
				(length 5.08)
				(name "P138")
				(number "138")
			)
			(pin bidirectional line
				(at -27.94 81.28 0)
				(length 5.08)
				(name "P139")
				(number "139")
			)
			(pin bidirectional line
				(at -27.94 78.74 0)
				(length 5.08)
				(name "P140")
				(number "140")
			)
			(pin bidirectional line
				(at -27.94 76.2 0)
				(length 5.08)
				(name "P142")
				(number "142")
			)
			(pin bidirectional line
				(at -27.94 73.66 0)
				(length 5.08)
				(name "GSR")
				(number "143")
			)
			(pin bidirectional line
				(at -27.94 68.58 0)
				(length 5.08)
				(name "GTS2")
				(number "2")
			)
			(pin bidirectional line
				(at -27.94 66.04 0)
				(length 5.08)
				(name "GTS3")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 63.5 0)
				(length 5.08)
				(name "P4")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 60.96 0)
				(length 5.08)
				(name "GTS0")
				(number "5")
			)
			(pin bidirectional line
				(at -27.94 58.42 0)
				(length 5.08)
				(name "GTS1")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 55.88 0)
				(length 5.08)
				(name "P7")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 53.34 0)
				(length 5.08)
				(name "P9")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 5.08)
				(name "P10")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 45.72 0)
				(length 5.08)
				(name "P131")
				(number "131")
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 5.08)
				(name "P132")
				(number "132")
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 5.08)
				(name "P133")
				(number "133")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "P134")
				(number "134")
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "P135")
				(number "135")
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "P136")
				(number "136")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "P11")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "P12")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "P13")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "P14")
				(number "14")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "P15")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "P16")
				(number "16")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "P17")
				(number "17")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "P18")
				(number "18")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "P28")
				(number "28")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "GCK0")
				(number "30")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "P31")
				(number "31")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "GCK1")
				(number "32")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "P33")
				(number "33")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "P34")
				(number "34")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "CDRST")
				(number "35")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "GCK2")
				(number "38")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "DGE")
				(number "39")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "P40")
				(number "40")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "P41")
				(number "41")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "P42")
				(number "42")
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "P43")
				(number "43")
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "P19")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "P20")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 5.08)
				(name "P21")
				(number "21")
			)
			(pin bidirectional line
				(at -27.94 -40.64 0)
				(length 5.08)
				(name "P22")
				(number "22")
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 5.08)
				(name "P23")
				(number "23")
			)
			(pin bidirectional line
				(at -27.94 -45.72 0)
				(length 5.08)
				(name "P24")
				(number "24")
			)
			(pin bidirectional line
				(at -27.94 -48.26 0)
				(length 5.08)
				(name "P25")
				(number "25")
			)
			(pin bidirectional line
				(at -27.94 -50.8 0)
				(length 5.08)
				(name "P26")
				(number "26")
			)
			(pin bidirectional line
				(at -27.94 -55.88 0)
				(length 5.08)
				(name "P44")
				(number "44")
			)
			(pin bidirectional line
				(at -27.94 -58.42 0)
				(length 5.08)
				(name "P45")
				(number "45")
			)
			(pin bidirectional line
				(at -27.94 -60.96 0)
				(length 5.08)
				(name "P46")
				(number "46")
			)
			(pin bidirectional line
				(at -27.94 -63.5 0)
				(length 5.08)
				(name "P48")
				(number "48")
			)
			(pin bidirectional line
				(at -27.94 -66.04 0)
				(length 5.08)
				(name "P49")
				(number "49")
			)
			(pin bidirectional line
				(at -27.94 -68.58 0)
				(length 5.08)
				(name "P50")
				(number "50")
			)
			(pin bidirectional line
				(at -27.94 -71.12 0)
				(length 5.08)
				(name "P51")
				(number "51")
			)
			(pin bidirectional line
				(at -27.94 -73.66 0)
				(length 5.08)
				(name "P52")
				(number "52")
			)
			(pin bidirectional line
				(at -27.94 -78.74 0)
				(length 5.08)
				(name "TCK")
				(number "67")
			)
			(pin bidirectional line
				(at -27.94 -81.28 0)
				(length 5.08)
				(name "TDI")
				(number "63")
			)
			(pin bidirectional line
				(at -27.94 -83.82 0)
				(length 5.08)
				(name "TDO")
				(number "122")
			)
			(pin bidirectional line
				(at -27.94 -86.36 0)
				(length 5.08)
				(name "TMS")
				(number "65")
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VCC")
				(number "37")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VCC")
				(number "84")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VCCAUX")
				(number "8")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VCCIO1")
				(number "27")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VCCIO1")
				(number "55")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VCCIO1")
				(number "73")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VCCIO1")
				(number "93")
			)
			(pin power_in line
				(at 7.62 -93.98 90)
				(length 5.08)
				(name "GND")
				(number "108")
			)
			(pin passive line
				(at 7.62 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "123")
			)
			(pin passive line
				(at 7.62 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "144")
			)
			(pin passive line
				(at 7.62 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 7.62 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "36")
			)
			(pin passive line
				(at 7.62 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "47")
			)
			(pin passive line
				(at 7.62 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "62")
			)
			(pin passive line
				(at 7.62 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "72")
			)
			(pin passive line
				(at 7.62 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "89")
			)
			(pin passive line
				(at 7.62 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "90")
			)
			(pin passive line
				(at 7.62 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "99")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VCCIO2")
				(number "109")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VCCIO2")
				(number "127")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VCCIO2")
				(number "141")
			)
			(pin bidirectional line
				(at 27.94 86.36 180)
				(length 5.08)
				(name "P112")
				(number "112")
			)
			(pin bidirectional line
				(at 27.94 83.82 180)
				(length 5.08)
				(name "P113")
				(number "113")
			)
			(pin bidirectional line
				(at 27.94 81.28 180)
				(length 5.08)
				(name "P114")
				(number "114")
			)
			(pin bidirectional line
				(at 27.94 78.74 180)
				(length 5.08)
				(name "P115")
				(number "115")
			)
			(pin bidirectional line
				(at 27.94 76.2 180)
				(length 5.08)
				(name "P116")
				(number "116")
			)
			(pin bidirectional line
				(at 27.94 73.66 180)
				(length 5.08)
				(name "P117")
				(number "117")
			)
			(pin bidirectional line
				(at 27.94 71.12 180)
				(length 5.08)
				(name "P118")
				(number "118")
			)
			(pin bidirectional line
				(at 27.94 68.58 180)
				(length 5.08)
				(name "P119")
				(number "119")
			)
			(pin bidirectional line
				(at 27.94 63.5 180)
				(length 5.08)
				(name "P101")
				(number "101")
			)
			(pin bidirectional line
				(at 27.94 60.96 180)
				(length 5.08)
				(name "P102")
				(number "102")
			)
			(pin bidirectional line
				(at 27.94 58.42 180)
				(length 5.08)
				(name "P103")
				(number "103")
			)
			(pin bidirectional line
				(at 27.94 55.88 180)
				(length 5.08)
				(name "P104")
				(number "104")
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 5.08)
				(name "P105")
				(number "105")
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 5.08)
				(name "P106")
				(number "106")
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 5.08)
				(name "P107")
				(number "107")
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 5.08)
				(name "P110")
				(number "110")
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 5.08)
				(name "P111")
				(number "111")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "P120")
				(number "120")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "P121")
				(number "121")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "P124")
				(number "124")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "P125")
				(number "125")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "P126")
				(number "126")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "P128")
				(number "128")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "P129")
				(number "129")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "P130")
				(number "130")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "P94")
				(number "94")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "P95")
				(number "95")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "P96")
				(number "96")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "P97")
				(number "97")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "P98")
				(number "98")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "P100")
				(number "100")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "P75")
				(number "75")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "P76")
				(number "76")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "P77")
				(number "77")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "P78")
				(number "78")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "P79")
				(number "79")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "P80")
				(number "80")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "P81")
				(number "81")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "P82")
				(number "82")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "P61")
				(number "61")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "P64")
				(number "64")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "P66")
				(number "66")
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "P68")
				(number "68")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "P69")
				(number "69")
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "P70")
				(number "70")
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "P71")
				(number "71")
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "P74")
				(number "74")
			)
			(pin bidirectional line
				(at 27.94 -48.26 180)
				(length 5.08)
				(name "P83")
				(number "83")
			)
			(pin bidirectional line
				(at 27.94 -50.8 180)
				(length 5.08)
				(name "P85")
				(number "85")
			)
			(pin bidirectional line
				(at 27.94 -53.34 180)
				(length 5.08)
				(name "P86")
				(number "86")
			)
			(pin bidirectional line
				(at 27.94 -55.88 180)
				(length 5.08)
				(name "P87")
				(number "87")
			)
			(pin bidirectional line
				(at 27.94 -58.42 180)
				(length 5.08)
				(name "P88")
				(number "88")
			)
			(pin bidirectional line
				(at 27.94 -60.96 180)
				(length 5.08)
				(name "P91")
				(number "91")
			)
			(pin bidirectional line
				(at 27.94 -63.5 180)
				(length 5.08)
				(name "P92")
				(number "92")
			)
			(pin bidirectional line
				(at 27.94 -68.58 180)
				(length 5.08)
				(name "P53")
				(number "53")
			)
			(pin bidirectional line
				(at 27.94 -71.12 180)
				(length 5.08)
				(name "P54")
				(number "54")
			)
			(pin bidirectional line
				(at 27.94 -73.66 180)
				(length 5.08)
				(name "P56")
				(number "56")
			)
			(pin bidirectional line
				(at 27.94 -76.2 180)
				(length 5.08)
				(name "P57")
				(number "57")
			)
			(pin bidirectional line
				(at 27.94 -78.74 180)
				(length 5.08)
				(name "P58")
				(number "58")
			)
			(pin bidirectional line
				(at 27.94 -81.28 180)
				(length 5.08)
				(name "P59")
				(number "59")
			)
			(pin bidirectional line
				(at 27.94 -83.82 180)
				(length 5.08)
				(name "P60")
				(number "60")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC2C256-VQ100"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 62.23 0)
		)
		(property "Value" "XC2C256-VQ100"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_QFP:VQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.xilinx.com/support/documentation/data_sheets/ds094.pdf"
			(at 0 0 0)
		)
		(property "Description" "CoolRunner-II CPLD, 256 macrocells, VQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "CPLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "XC2C256-VQ100_0_1")
		(symbol "XC2C256-VQ100_1_1"
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 3.81)
				(name "P1/GTS2")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 3.81)
				(name "P2/GTS3")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 3.81)
				(name "P3/GTS0")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 3.81)
				(name "P4/GTS1")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 3.81)
				(name "P6")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 3.81)
				(name "P7")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 3.81)
				(name "P8")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "P9")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "P10")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "P11")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "P12")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "P13")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "P14")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "P15")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "P16")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "P17")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "P18")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "P19")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "P22/GCK0")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "P23/GCK1")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "P24/CDRST")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "P27/GCLK2")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "P28/DGE")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "P29")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "P30")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "P32")
				(number "32")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 3.81)
				(name "P33")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 3.81)
				(name "P34")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 3.81)
				(name "P35")
				(number "35")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 3.81)
				(name "P36")
				(number "36")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 3.81)
				(name "P37")
				(number "37")
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 3.81)
				(name "P39")
				(number "39")
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 3.81)
				(name "P40")
				(number "40")
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 3.81)
				(name "P41")
				(number "41")
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 3.81)
				(name "P42")
				(number "42")
			)
			(pin bidirectional line
				(at -25.4 -48.26 0)
				(length 3.81)
				(name "P43")
				(number "43")
			)
			(pin bidirectional line
				(at -25.4 -50.8 0)
				(length 3.81)
				(name "P44")
				(number "44")
			)
			(pin bidirectional line
				(at -25.4 -53.34 0)
				(length 3.81)
				(name "P46")
				(number "46")
			)
			(pin bidirectional line
				(at -25.4 -55.88 0)
				(length 3.81)
				(name "P49")
				(number "49")
			)
			(pin bidirectional line
				(at -25.4 -58.42 0)
				(length 3.81)
				(name "P50")
				(number "50")
			)
			(pin power_in line
				(at -12.7 63.5 270)
				(length 3.81)
				(name "VCC")
				(number "26")
			)
			(pin power_in line
				(at -10.16 63.5 270)
				(length 3.81)
				(name "VCC")
				(number "57")
			)
			(pin power_in line
				(at -5.08 63.5 270)
				(length 3.81)
				(name "VAUX")
				(number "5")
			)
			(pin power_in line
				(at 0 63.5 270)
				(length 3.81)
				(name "VCCIO1")
				(number "20")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "100")
			)
			(pin power_in line
				(at 0 -63.5 90)
				(length 3.81)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "62")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "69")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "75")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "84")
			)
			(pin power_in line
				(at 2.54 63.5 270)
				(length 3.81)
				(name "VCCIO1")
				(number "38")
			)
			(pin power_in line
				(at 5.08 63.5 270)
				(length 3.81)
				(name "VCCIO1")
				(number "51")
			)
			(pin power_in line
				(at 7.62 63.5 270)
				(length 3.81)
				(name "VCCIO2")
				(number "88")
			)
			(pin power_in line
				(at 10.16 63.5 270)
				(length 3.81)
				(name "VCCIO2")
				(number "98")
			)
			(pin input line
				(at 25.4 58.42 180)
				(length 3.81)
				(name "TMS")
				(number "47")
			)
			(pin input line
				(at 25.4 55.88 180)
				(length 3.81)
				(name "TDI")
				(number "45")
			)
			(pin input line
				(at 25.4 53.34 180)
				(length 3.81)
				(name "TCK")
				(number "48")
			)
			(pin output line
				(at 25.4 50.8 180)
				(length 3.81)
				(name "TDO")
				(number "83")
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 3.81)
				(name "P52")
				(number "52")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 3.81)
				(name "P53")
				(number "53")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 3.81)
				(name "P54")
				(number "54")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 3.81)
				(name "P55")
				(number "55")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 3.81)
				(name "P56")
				(number "56")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 3.81)
				(name "P58")
				(number "58")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "P59")
				(number "59")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "P60")
				(number "60")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "P61")
				(number "61")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "P63")
				(number "63")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "P64")
				(number "64")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "P65")
				(number "65")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "P66")
				(number "66")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "P67")
				(number "67")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "P68")
				(number "68")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "P70")
				(number "70")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "P71")
				(number "71")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "P72")
				(number "72")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "P73")
				(number "73")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "P74")
				(number "74")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "P76")
				(number "76")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "P77")
				(number "77")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "P78")
				(number "78")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 3.81)
				(name "P79")
				(number "79")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "P80")
				(number "80")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 3.81)
				(name "P81")
				(number "81")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 3.81)
				(name "P82")
				(number "82")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 3.81)
				(name "P85")
				(number "85")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 3.81)
				(name "P86")
				(number "86")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 3.81)
				(name "P87")
				(number "87")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 3.81)
				(name "P89")
				(number "89")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 3.81)
				(name "P90")
				(number "90")
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 3.81)
				(name "P91")
				(number "91")
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 3.81)
				(name "P92")
				(number "92")
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 3.81)
				(name "P93")
				(number "93")
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 3.81)
				(name "P94")
				(number "94")
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 3.81)
				(name "P95")
				(number "95")
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 3.81)
				(name "P96")
				(number "96")
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 3.81)
				(name "P97")
				(number "97")
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 3.81)
				(name "P99/GSA")
				(number "99")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC2S100TQ144"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 27.94 83.82 0)
		)
		(property "Value" "XC2S100TQ144"
			(at 0 2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "xilinx/spartan2e/spartan2e.pdf"
			(at 0 0 0)
		)
		(property "Description" "spartan 2"
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC2S100TQ144_0_1")
		(symbol "XC2S100TQ144_1_1"
			(pin input line
				(at -48.26 76.2 0)
				(length 7.62)
				(name "TMS")
				(number "142")
			)
			(pin output line
				(at -48.26 73.66 0)
				(length 7.62)
				(name "TDO")
				(number "34")
			)
			(pin input line
				(at -48.26 71.12 0)
				(length 7.62)
				(name "TDI")
				(number "32")
			)
			(pin input line
				(at -48.26 68.58 0)
				(length 7.62)
				(name "TCK")
				(number "2")
			)
			(pin open_collector line
				(at -48.26 63.5 0)
				(length 7.62)
				(name "DONE")
				(number "72")
			)
			(pin input line
				(at -48.26 60.96 0)
				(length 7.62)
				(name "~{PROG}")
				(number "69")
			)
			(pin bidirectional line
				(at -48.26 58.42 0)
				(length 7.62)
				(name "~{INIT/IO}")
				(number "68")
			)
			(pin input clock
				(at -48.26 55.88 0)
				(length 7.62)
				(name "CCLK")
				(number "37")
			)
			(pin input line
				(at -48.26 50.8 0)
				(length 7.62)
				(name "M0")
				(number "109")
			)
			(pin input line
				(at -48.26 48.26 0)
				(length 7.62)
				(name "M1")
				(number "111")
			)
			(pin input line
				(at -48.26 45.72 0)
				(length 7.62)
				(name "M2")
				(number "106")
			)
			(pin bidirectional line
				(at -48.26 40.64 0)
				(length 7.62)
				(name "IO")
				(number "3")
			)
			(pin bidirectional line
				(at -48.26 38.1 0)
				(length 7.62)
				(name "IO")
				(number "4")
			)
			(pin bidirectional line
				(at -48.26 35.56 0)
				(length 7.62)
				(name "IO/VREF")
				(number "5")
			)
			(pin bidirectional line
				(at -48.26 33.02 0)
				(length 7.62)
				(name "IO/VREF")
				(number "6")
			)
			(pin bidirectional line
				(at -48.26 30.48 0)
				(length 7.62)
				(name "IO")
				(number "7")
			)
			(pin bidirectional line
				(at -48.26 27.94 0)
				(length 7.62)
				(name "IO7P10")
				(number "10")
			)
			(pin bidirectional line
				(at -48.26 25.4 0)
				(length 7.62)
				(name "IO")
				(number "11")
			)
			(pin bidirectional line
				(at -48.26 22.86 0)
				(length 7.62)
				(name "IO/VREF")
				(number "12")
			)
			(pin bidirectional line
				(at -48.26 20.32 0)
				(length 7.62)
				(name "IO")
				(number "13")
			)
			(pin input line
				(at -48.26 17.78 0)
				(length 7.62)
				(name "I/GCK3")
				(number "15")
			)
			(pin input line
				(at -48.26 10.16 0)
				(length 7.62)
				(name "I/GCK2")
				(number "18")
			)
			(pin bidirectional line
				(at -48.26 7.62 0)
				(length 7.62)
				(name "IO")
				(number "19")
			)
			(pin bidirectional line
				(at -48.26 5.08 0)
				(length 7.62)
				(name "IO")
				(number "20")
			)
			(pin bidirectional line
				(at -48.26 2.54 0)
				(length 7.62)
				(name "IO/VREF")
				(number "21")
			)
			(pin bidirectional line
				(at -48.26 0 0)
				(length 7.62)
				(name "IO")
				(number "22")
			)
			(pin bidirectional line
				(at -48.26 -2.54 0)
				(length 7.62)
				(name "IO")
				(number "23")
			)
			(pin bidirectional line
				(at -48.26 -5.08 0)
				(length 7.62)
				(name "IO")
				(number "26")
			)
			(pin bidirectional line
				(at -48.26 -7.62 0)
				(length 7.62)
				(name "IO/VREF")
				(number "27")
			)
			(pin bidirectional line
				(at -48.26 -10.16 0)
				(length 7.62)
				(name "IO/REF")
				(number "28")
			)
			(pin bidirectional line
				(at -48.26 -12.7 0)
				(length 7.62)
				(name "IO")
				(number "29")
			)
			(pin bidirectional line
				(at -48.26 -17.78 0)
				(length 7.62)
				(name "IO")
				(number "40")
			)
			(pin bidirectional line
				(at -48.26 -20.32 0)
				(length 7.62)
				(name "IO")
				(number "41")
			)
			(pin bidirectional line
				(at -48.26 -22.86 0)
				(length 7.62)
				(name "IO")
				(number "42")
			)
			(pin bidirectional line
				(at -48.26 -25.4 0)
				(length 7.62)
				(name "IO/VREF")
				(number "43")
			)
			(pin bidirectional line
				(at -48.26 -27.94 0)
				(length 7.62)
				(name "IO/D1")
				(number "44")
			)
			(pin bidirectional line
				(at -48.26 -30.48 0)
				(length 7.62)
				(name "IO/D2")
				(number "46")
			)
			(pin bidirectional line
				(at -48.26 -33.02 0)
				(length 7.62)
				(name "IO")
				(number "47")
			)
			(pin bidirectional line
				(at -48.26 -35.56 0)
				(length 7.62)
				(name "IO/VREF")
				(number "48")
			)
			(pin bidirectional line
				(at -48.26 -38.1 0)
				(length 7.62)
				(name "IO/D3")
				(number "49")
			)
			(pin bidirectional line
				(at -48.26 -40.64 0)
				(length 7.62)
				(name "IO")
				(number "50")
			)
			(pin bidirectional line
				(at -48.26 -43.18 0)
				(length 7.62)
				(name "IO/IRDY")
				(number "51")
			)
			(pin bidirectional line
				(at -48.26 -48.26 0)
				(length 7.62)
				(name "IO/TRDY")
				(number "54")
			)
			(pin bidirectional line
				(at -48.26 -50.8 0)
				(length 7.62)
				(name "IO")
				(number "56")
			)
			(pin bidirectional line
				(at -48.26 -53.34 0)
				(length 7.62)
				(name "IO/D4")
				(number "57")
			)
			(pin bidirectional line
				(at -48.26 -55.88 0)
				(length 7.62)
				(name "IO/VREF")
				(number "58")
			)
			(pin bidirectional line
				(at -48.26 -58.42 0)
				(length 7.62)
				(name "IO")
				(number "59")
			)
			(pin bidirectional line
				(at -48.26 -60.96 0)
				(length 7.62)
				(name "IO/D5")
				(number "60")
			)
			(pin bidirectional line
				(at -48.26 -63.5 0)
				(length 7.62)
				(name "IO/D6")
				(number "62")
			)
			(pin bidirectional line
				(at -48.26 -66.04 0)
				(length 7.62)
				(name "IO/VREF")
				(number "63")
			)
			(pin bidirectional line
				(at -48.26 -68.58 0)
				(length 7.62)
				(name "IO")
				(number "64")
			)
			(pin bidirectional line
				(at -48.26 -71.12 0)
				(length 7.62)
				(name "IO/VREF")
				(number "65")
			)
			(pin bidirectional line
				(at -48.26 -73.66 0)
				(length 7.62)
				(name "IO")
				(number "66")
			)
			(pin bidirectional line
				(at -48.26 -76.2 0)
				(length 7.62)
				(name "IO/D7")
				(number "67")
			)
			(pin power_in line
				(at -22.86 86.36 270)
				(length 7.62)
				(name "VCCO")
				(number "1")
			)
			(pin power_in line
				(at -20.32 86.36 270)
				(length 7.62)
				(name "VCCO")
				(number "16")
			)
			(pin power_in line
				(at -17.78 86.36 270)
				(length 7.62)
				(name "VCCO")
				(number "35")
			)
			(pin power_in line
				(at -15.24 86.36 270)
				(length 7.62)
				(name "VCCO")
				(number "36")
			)
			(pin power_in line
				(at -12.7 86.36 270)
				(length 7.62)
				(name "VCCO")
				(number "53")
			)
			(pin power_in line
				(at -10.16 86.36 270)
				(length 7.62)
				(name "VCCO")
				(number "70")
			)
			(pin power_in line
				(at -7.62 86.36 270)
				(length 7.62)
				(name "VCCO")
				(number "71")
			)
			(pin power_in line
				(at -5.08 86.36 270)
				(length 7.62)
				(name "VCCO")
				(number "90")
			)
			(pin power_in line
				(at -2.54 86.36 270)
				(length 7.62)
				(name "VCCO")
				(number "107")
			)
			(pin power_in line
				(at 0 86.36 270)
				(length 7.62)
				(name "VCCO")
				(number "108")
			)
			(pin power_in line
				(at 2.54 86.36 270)
				(length 7.62)
				(name "VCCO")
				(number "127")
			)
			(pin passive line
				(at 5.08 86.36 270)
				(length 7.62)
				(name "VCCO")
				(number "144")
			)
			(pin power_in line
				(at 8.89 -86.36 90)
				(length 7.62)
				(name "GND")
				(number "110")
			)
			(pin passive line
				(at 8.89 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "119")
			)
			(pin passive line
				(at 8.89 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "128")
			)
			(pin passive line
				(at 8.89 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "135")
			)
			(pin passive line
				(at 8.89 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "143")
			)
			(pin passive line
				(at 8.89 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 8.89 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 8.89 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 8.89 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin passive line
				(at 8.89 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "52")
			)
			(pin passive line
				(at 8.89 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "61")
			)
			(pin passive line
				(at 8.89 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "73")
			)
			(pin passive line
				(at 8.89 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 8.89 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "81")
			)
			(pin passive line
				(at 8.89 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "89")
			)
			(pin passive line
				(at 8.89 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "98")
			)
			(pin power_in line
				(at 12.7 86.36 270)
				(length 7.62)
				(name "VCCINT")
				(number "9")
			)
			(pin power_in line
				(at 15.24 86.36 270)
				(length 7.62)
				(name "VCCINT")
				(number "14")
			)
			(pin power_in line
				(at 17.78 86.36 270)
				(length 7.62)
				(name "VCCINT")
				(number "24")
			)
			(pin power_in line
				(at 20.32 86.36 270)
				(length 7.62)
				(name "VCCINT")
				(number "82")
			)
			(pin power_in line
				(at 22.86 86.36 270)
				(length 7.62)
				(name "VCCINT")
				(number "125")
			)
			(pin bidirectional line
				(at 45.72 69.85 180)
				(length 7.62)
				(name "/WR")
				(number "30")
			)
			(pin bidirectional line
				(at 45.72 67.31 180)
				(length 7.62)
				(name "/CS")
				(number "31")
			)
			(pin output line
				(at 45.72 62.23 180)
				(length 7.62)
				(name "BUSY/DOUT")
				(number "38")
			)
			(pin bidirectional line
				(at 45.72 59.69 180)
				(length 7.62)
				(name "D0/DIN")
				(number "39")
			)
			(pin bidirectional line
				(at 45.72 50.8 180)
				(length 7.62)
				(name "IO")
				(number "141")
			)
			(pin bidirectional line
				(at 45.72 48.26 180)
				(length 7.62)
				(name "IO")
				(number "140")
			)
			(pin bidirectional line
				(at 45.72 45.72 180)
				(length 7.62)
				(name "IO/VREF")
				(number "139")
			)
			(pin bidirectional line
				(at 45.72 43.18 180)
				(length 7.62)
				(name "IO")
				(number "138")
			)
			(pin bidirectional line
				(at 45.72 40.64 180)
				(length 7.62)
				(name "139/VREF")
				(number "137")
			)
			(pin bidirectional line
				(at 45.72 38.1 180)
				(length 7.62)
				(name "IO")
				(number "136")
			)
			(pin bidirectional line
				(at 45.72 35.56 180)
				(length 7.62)
				(name "IO")
				(number "134")
			)
			(pin bidirectional line
				(at 45.72 33.02 180)
				(length 7.62)
				(name "IO")
				(number "133")
			)
			(pin bidirectional line
				(at 45.72 30.48 180)
				(length 7.62)
				(name "IO/VREF")
				(number "132")
			)
			(pin bidirectional line
				(at 45.72 27.94 180)
				(length 7.62)
				(name "IO")
				(number "131")
			)
			(pin bidirectional line
				(at 45.72 25.4 180)
				(length 7.62)
				(name "IO")
				(number "130")
			)
			(pin bidirectional line
				(at 45.72 22.86 180)
				(length 7.62)
				(name "IO/IRDY")
				(number "129")
			)
			(pin bidirectional line
				(at 45.72 17.78 180)
				(length 7.62)
				(name "IO/TRDY")
				(number "126")
			)
			(pin bidirectional line
				(at 45.72 15.24 180)
				(length 7.62)
				(name "IO")
				(number "124")
			)
			(pin bidirectional line
				(at 45.72 12.7 180)
				(length 7.62)
				(name "IO")
				(number "123")
			)
			(pin bidirectional line
				(at 45.72 10.16 180)
				(length 7.62)
				(name "IO/VREF")
				(number "122")
			)
			(pin bidirectional line
				(at 45.72 7.62 180)
				(length 7.62)
				(name "IO")
				(number "121")
			)
			(pin bidirectional line
				(at 45.72 5.08 180)
				(length 7.62)
				(name "IO")
				(number "120")
			)
			(pin bidirectional line
				(at 45.72 2.54 180)
				(length 7.62)
				(name "IO")
				(number "118")
			)
			(pin bidirectional line
				(at 45.72 0 180)
				(length 7.62)
				(name "IO/VREF")
				(number "117")
			)
			(pin bidirectional line
				(at 45.72 -2.54 180)
				(length 7.62)
				(name "IO")
				(number "116")
			)
			(pin bidirectional line
				(at 45.72 -5.08 180)
				(length 7.62)
				(name "IO/VREF")
				(number "115")
			)
			(pin bidirectional line
				(at 45.72 -7.62 180)
				(length 7.62)
				(name "IO")
				(number "114")
			)
			(pin bidirectional line
				(at 45.72 -10.16 180)
				(length 7.62)
				(name "IO")
				(number "113")
			)
			(pin bidirectional line
				(at 45.72 -12.7 180)
				(length 7.62)
				(name "IO")
				(number "112")
			)
			(pin bidirectional line
				(at 45.72 -17.78 180)
				(length 7.62)
				(name "IO")
				(number "103")
			)
			(pin bidirectional line
				(at 45.72 -20.32 180)
				(length 7.62)
				(name "IO/VREF")
				(number "102")
			)
			(pin bidirectional line
				(at 45.72 -22.86 180)
				(length 7.62)
				(name "IO")
				(number "101")
			)
			(pin bidirectional line
				(at 45.72 -25.4 180)
				(length 7.62)
				(name "IO/VREF")
				(number "100")
			)
			(pin bidirectional line
				(at 45.72 -27.94 180)
				(length 7.62)
				(name "IO")
				(number "99")
			)
			(pin bidirectional line
				(at 45.72 -30.48 180)
				(length 7.62)
				(name "IO")
				(number "96")
			)
			(pin bidirectional line
				(at 45.72 -33.02 180)
				(length 7.62)
				(name "IO")
				(number "95")
			)
			(pin bidirectional line
				(at 45.72 -35.56 180)
				(length 7.62)
				(name "IO/VREF")
				(number "94")
			)
			(pin bidirectional line
				(at 45.72 -38.1 180)
				(length 7.62)
				(name "IO")
				(number "93")
			)
			(pin input line
				(at 45.72 -40.64 180)
				(length 7.62)
				(name "I/GCK1")
				(number "91")
			)
			(pin input clock
				(at 45.72 -45.72 180)
				(length 7.62)
				(name "I/CCK0")
				(number "88")
			)
			(pin bidirectional line
				(at 45.72 -48.26 180)
				(length 7.62)
				(name "IO")
				(number "87")
			)
			(pin bidirectional line
				(at 45.72 -50.8 180)
				(length 7.62)
				(name "IO")
				(number "86")
			)
			(pin bidirectional line
				(at 45.72 -53.34 180)
				(length 7.62)
				(name "IO")
				(number "85")
			)
			(pin bidirectional line
				(at 45.72 -55.88 180)
				(length 7.62)
				(name "IO")
				(number "84")
			)
			(pin bidirectional line
				(at 45.72 -58.42 180)
				(length 7.62)
				(name "IO")
				(number "83")
			)
			(pin bidirectional line
				(at 45.72 -60.96 180)
				(length 7.62)
				(name "IO")
				(number "80")
			)
			(pin bidirectional line
				(at 45.72 -63.5 180)
				(length 7.62)
				(name "IO/VREF")
				(number "79")
			)
			(pin bidirectional line
				(at 45.72 -66.04 180)
				(length 7.62)
				(name "IO")
				(number "78")
			)
			(pin bidirectional line
				(at 45.72 -68.58 180)
				(length 7.62)
				(name "IO/VREF")
				(number "77")
			)
			(pin bidirectional line
				(at 45.72 -71.12 180)
				(length 7.62)
				(name "IO")
				(number "76")
			)
			(pin bidirectional line
				(at 45.72 -73.66 180)
				(length 7.62)
				(name "IO")
				(number "75")
			)
			(pin bidirectional line
				(at 45.72 -76.2 180)
				(length 7.62)
				(name "IO")
				(number "74")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC2S150PQ208"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -2.4892 0)
		)
		(property "Value" "XC2S150PQ208"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "xilinx/spartan2e/spartan2e.pdf"
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC2S150PQ208_0_1")
		(symbol "XC2S150PQ208_1_1"
			(pin bidirectional line
				(at -54.61 106.68 0)
				(length 7.62)
				(name "TMS")
				(number "2")
			)
			(pin bidirectional line
				(at -54.61 104.14 0)
				(length 7.62)
				(name "TDO")
				(number "157")
			)
			(pin bidirectional line
				(at -54.61 101.6 0)
				(length 7.62)
				(name "TDI")
				(number "159")
			)
			(pin bidirectional line
				(at -54.61 99.06 0)
				(length 7.62)
				(name "TCK")
				(number "207")
			)
			(pin bidirectional line
				(at -54.61 93.98 0)
				(length 7.62)
				(name "DONE")
				(number "104")
			)
			(pin input line
				(at -54.61 91.44 0)
				(length 7.62)
				(name "/PROG")
				(number "106")
			)
			(pin bidirectional line
				(at -54.61 88.9 0)
				(length 7.62)
				(name "/INIT")
				(number "107")
			)
			(pin bidirectional clock
				(at -54.61 86.36 0)
				(length 7.62)
				(name "CCLK")
				(number "155")
			)
			(pin input line
				(at -54.61 81.28 0)
				(length 7.62)
				(name "M0")
				(number "52")
			)
			(pin input line
				(at -54.61 78.74 0)
				(length 7.62)
				(name "M1")
				(number "50")
			)
			(pin input line
				(at -54.61 76.2 0)
				(length 7.62)
				(name "M2")
				(number "54")
			)
			(pin bidirectional line
				(at -54.61 71.12 0)
				(length 7.62)
				(name "IO7P3")
				(number "3")
			)
			(pin bidirectional line
				(at -54.61 68.58 0)
				(length 7.62)
				(name "IO7P4")
				(number "4")
			)
			(pin bidirectional line
				(at -54.61 66.04 0)
				(length 7.62)
				(name "IO7P5")
				(number "5")
			)
			(pin bidirectional line
				(at -54.61 63.5 0)
				(length 7.62)
				(name "IO7VRP6")
				(number "6")
			)
			(pin bidirectional line
				(at -54.61 60.96 0)
				(length 7.62)
				(name "IO7P7")
				(number "7")
			)
			(pin bidirectional line
				(at -54.61 58.42 0)
				(length 7.62)
				(name "IO7P8")
				(number "8")
			)
			(pin bidirectional line
				(at -54.61 55.88 0)
				(length 7.62)
				(name "IO7P9")
				(number "9")
			)
			(pin bidirectional line
				(at -54.61 53.34 0)
				(length 7.62)
				(name "IO7P10")
				(number "10")
			)
			(pin bidirectional line
				(at -54.61 50.8 0)
				(length 7.62)
				(name "IO7P14")
				(number "14")
			)
			(pin bidirectional line
				(at -54.61 48.26 0)
				(length 7.62)
				(name "IO7P15")
				(number "15")
			)
			(pin bidirectional line
				(at -54.61 45.72 0)
				(length 7.62)
				(name "IO7P16")
				(number "16")
			)
			(pin bidirectional line
				(at -54.61 43.18 0)
				(length 7.62)
				(name "IO7P17")
				(number "17")
			)
			(pin bidirectional line
				(at -54.61 40.64 0)
				(length 7.62)
				(name "IO7P18")
				(number "18")
			)
			(pin bidirectional line
				(at -54.61 38.1 0)
				(length 7.62)
				(name "IO7VRP20")
				(number "20")
			)
			(pin bidirectional line
				(at -54.61 35.56 0)
				(length 7.62)
				(name "IO7P21")
				(number "21")
			)
			(pin bidirectional line
				(at -54.61 33.02 0)
				(length 7.62)
				(name "IO7P22")
				(number "22")
			)
			(pin bidirectional line
				(at -54.61 30.48 0)
				(length 7.62)
				(name "IO7P23")
				(number "23")
			)
			(pin bidirectional line
				(at -54.61 25.4 0)
				(length 7.62)
				(name "IO6P29")
				(number "29")
			)
			(pin bidirectional line
				(at -54.61 22.86 0)
				(length 7.62)
				(name "IO6P30")
				(number "30")
			)
			(pin bidirectional line
				(at -54.61 20.32 0)
				(length 7.62)
				(name "IO6VRP31")
				(number "31")
			)
			(pin bidirectional line
				(at -54.61 17.78 0)
				(length 7.62)
				(name "IO6P33")
				(number "33")
			)
			(pin bidirectional line
				(at -54.61 15.24 0)
				(length 7.62)
				(name "IO6P34")
				(number "34")
			)
			(pin bidirectional line
				(at -54.61 12.7 0)
				(length 7.62)
				(name "IO6P35")
				(number "35")
			)
			(pin bidirectional line
				(at -54.61 10.16 0)
				(length 7.62)
				(name "IO6P36")
				(number "36")
			)
			(pin bidirectional line
				(at -54.61 7.62 0)
				(length 7.62)
				(name "IO6P37")
				(number "37")
			)
			(pin bidirectional line
				(at -54.61 5.08 0)
				(length 7.62)
				(name "IO6P41")
				(number "41")
			)
			(pin bidirectional line
				(at -54.61 2.54 0)
				(length 7.62)
				(name "IO6P42")
				(number "42")
			)
			(pin bidirectional line
				(at -54.61 0 0)
				(length 7.62)
				(name "IO6P43")
				(number "43")
			)
			(pin bidirectional line
				(at -54.61 -2.54 0)
				(length 7.62)
				(name "IO6P44")
				(number "44")
			)
			(pin bidirectional line
				(at -54.61 -5.08 0)
				(length 7.62)
				(name "IO6VRP45")
				(number "45")
			)
			(pin bidirectional line
				(at -54.61 -7.62 0)
				(length 7.62)
				(name "IO6P46")
				(number "46")
			)
			(pin bidirectional line
				(at -54.61 -10.16 0)
				(length 7.62)
				(name "IO6P47")
				(number "47")
			)
			(pin bidirectional line
				(at -54.61 -12.7 0)
				(length 7.62)
				(name "IO6P48")
				(number "48")
			)
			(pin bidirectional line
				(at -54.61 -15.24 0)
				(length 7.62)
				(name "IO6P49")
				(number "49")
			)
			(pin bidirectional line
				(at -54.61 -20.32 0)
				(length 7.62)
				(name "IO5P57")
				(number "57")
			)
			(pin bidirectional line
				(at -54.61 -22.86 0)
				(length 7.62)
				(name "IO5P58")
				(number "58")
			)
			(pin bidirectional line
				(at -54.61 -25.4 0)
				(length 7.62)
				(name "IO5VRP59")
				(number "59")
			)
			(pin bidirectional line
				(at -54.61 -27.94 0)
				(length 7.62)
				(name "IO5P60")
				(number "60")
			)
			(pin bidirectional line
				(at -54.61 -30.48 0)
				(length 7.62)
				(name "IO5P61")
				(number "61")
			)
			(pin bidirectional line
				(at -54.61 -33.02 0)
				(length 7.62)
				(name "IO5P62")
				(number "62")
			)
			(pin bidirectional line
				(at -54.61 -35.56 0)
				(length 7.62)
				(name "IO5P63")
				(number "63")
			)
			(pin bidirectional line
				(at -54.61 -38.1 0)
				(length 7.62)
				(name "IO5P67")
				(number "67")
			)
			(pin bidirectional line
				(at -54.61 -40.64 0)
				(length 7.62)
				(name "IO5P68")
				(number "68")
			)
			(pin bidirectional line
				(at -54.61 -43.18 0)
				(length 7.62)
				(name "IO5P69")
				(number "69")
			)
			(pin bidirectional line
				(at -54.61 -45.72 0)
				(length 7.62)
				(name "IO5P70")
				(number "70")
			)
			(pin bidirectional line
				(at -54.61 -48.26 0)
				(length 7.62)
				(name "IO5P71")
				(number "71")
			)
			(pin bidirectional line
				(at -54.61 -50.8 0)
				(length 7.62)
				(name "IO5VRP73")
				(number "73")
			)
			(pin bidirectional line
				(at -54.61 -53.34 0)
				(length 7.62)
				(name "IO5P74")
				(number "74")
			)
			(pin input clock
				(at -54.61 -55.88 0)
				(length 7.62)
				(name "GCK1")
				(number "77")
			)
			(pin input clock
				(at -54.61 -60.96 0)
				(length 7.62)
				(name "GCK0")
				(number "80")
			)
			(pin bidirectional line
				(at -54.61 -63.5 0)
				(length 7.62)
				(name "IO4P81")
				(number "81")
			)
			(pin bidirectional line
				(at -54.61 -66.04 0)
				(length 7.62)
				(name "IO4P82")
				(number "82")
			)
			(pin bidirectional line
				(at -54.61 -68.58 0)
				(length 7.62)
				(name "IO4P83")
				(number "83")
			)
			(pin bidirectional line
				(at -54.61 -71.12 0)
				(length 7.62)
				(name "IO4VRP84")
				(number "84")
			)
			(pin bidirectional line
				(at -54.61 -73.66 0)
				(length 7.62)
				(name "IO4P86")
				(number "86")
			)
			(pin bidirectional line
				(at -54.61 -76.2 0)
				(length 7.62)
				(name "IO4P87")
				(number "87")
			)
			(pin bidirectional line
				(at -54.61 -78.74 0)
				(length 7.62)
				(name "IO4P88")
				(number "88")
			)
			(pin bidirectional line
				(at -54.61 -81.28 0)
				(length 7.62)
				(name "IO4P89")
				(number "89")
			)
			(pin bidirectional line
				(at -54.61 -83.82 0)
				(length 7.62)
				(name "IO4P90")
				(number "90")
			)
			(pin bidirectional line
				(at -54.61 -86.36 0)
				(length 7.62)
				(name "IO4P94")
				(number "94")
			)
			(pin bidirectional line
				(at -54.61 -88.9 0)
				(length 7.62)
				(name "IO4P95")
				(number "95")
			)
			(pin bidirectional line
				(at -54.61 -91.44 0)
				(length 7.62)
				(name "IO4P96")
				(number "96")
			)
			(pin bidirectional line
				(at -54.61 -93.98 0)
				(length 7.62)
				(name "IO4P97")
				(number "97")
			)
			(pin bidirectional line
				(at -54.61 -96.52 0)
				(length 7.62)
				(name "IO4VRP98")
				(number "98")
			)
			(pin bidirectional line
				(at -54.61 -99.06 0)
				(length 7.62)
				(name "IO4P99")
				(number "99")
			)
			(pin bidirectional line
				(at -54.61 -101.6 0)
				(length 7.62)
				(name "IO4P100")
				(number "100")
			)
			(pin bidirectional line
				(at -54.61 -104.14 0)
				(length 7.62)
				(name "IO4P101")
				(number "101")
			)
			(pin bidirectional line
				(at -54.61 -106.68 0)
				(length 7.62)
				(name "IO4P102")
				(number "102")
			)
			(pin power_in line
				(at -36.83 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "12")
			)
			(pin power_in line
				(at -34.29 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "26")
			)
			(pin power_in line
				(at -31.75 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "39")
			)
			(pin power_in line
				(at -31.75 -116.84 90)
				(length 7.62)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "103")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "116")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "124")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "131")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "137")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "145")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "158")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "169")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "177")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "183")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "190")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "198")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "40")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "51")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "64")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "72")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "79")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "85")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "93")
			)
			(pin power_in line
				(at -29.21 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "53")
			)
			(pin power_in line
				(at -26.67 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "65")
			)
			(pin power_in line
				(at -24.13 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "78")
			)
			(pin power_in line
				(at -21.59 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "92")
			)
			(pin power_in line
				(at -19.05 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "105")
			)
			(pin power_in line
				(at -16.51 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "117")
			)
			(pin power_in line
				(at -13.97 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "130")
			)
			(pin power_in line
				(at -11.43 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "144")
			)
			(pin power_in line
				(at -8.89 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "156")
			)
			(pin power_in line
				(at -6.35 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "170")
			)
			(pin power_in line
				(at -3.81 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "184")
			)
			(pin power_in line
				(at -1.27 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "197")
			)
			(pin power_in line
				(at 1.27 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "208")
			)
			(pin power_in line
				(at 8.89 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "13")
			)
			(pin power_in line
				(at 11.43 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "28")
			)
			(pin power_in line
				(at 13.97 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "38")
			)
			(pin power_in line
				(at 16.51 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "66")
			)
			(pin power_in line
				(at 19.05 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "76")
			)
			(pin power_in line
				(at 21.59 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "91")
			)
			(pin power_in line
				(at 24.13 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "118")
			)
			(pin power_in line
				(at 26.67 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "128")
			)
			(pin power_in line
				(at 29.21 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "143")
			)
			(pin power_in line
				(at 31.75 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "171")
			)
			(pin power_in line
				(at 34.29 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "186")
			)
			(pin power_in line
				(at 36.83 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "196")
			)
			(pin bidirectional line
				(at 54.61 96.52 180)
				(length 7.62)
				(name "IRDY2")
				(number "132")
			)
			(pin bidirectional line
				(at 54.61 93.98 180)
				(length 7.62)
				(name "TRDY3")
				(number "129")
			)
			(pin bidirectional line
				(at 54.61 91.44 180)
				(length 7.62)
				(name "TRDY6")
				(number "27")
			)
			(pin bidirectional line
				(at 54.61 88.9 180)
				(length 7.62)
				(name "IRDY7")
				(number "24")
			)
			(pin bidirectional line
				(at 54.61 83.82 180)
				(length 7.62)
				(name "/WR")
				(number "161")
			)
			(pin bidirectional line
				(at 54.61 81.28 180)
				(length 7.62)
				(name "/CS")
				(number "160")
			)
			(pin bidirectional line
				(at 54.61 76.2 180)
				(length 7.62)
				(name "BUSY/DOUT")
				(number "154")
			)
			(pin bidirectional line
				(at 54.61 73.66 180)
				(length 7.62)
				(name "D0/DIN")
				(number "153")
			)
			(pin bidirectional line
				(at 54.61 66.04 180)
				(length 7.62)
				(name "IO0P206")
				(number "206")
			)
			(pin bidirectional line
				(at 54.61 63.5 180)
				(length 7.62)
				(name "IO0P205")
				(number "205")
			)
			(pin bidirectional line
				(at 54.61 60.96 180)
				(length 7.62)
				(name "IO0P204")
				(number "204")
			)
			(pin bidirectional line
				(at 54.61 58.42 180)
				(length 7.62)
				(name "IO0VRP203")
				(number "203")
			)
			(pin bidirectional line
				(at 54.61 55.88 180)
				(length 7.62)
				(name "IO0P202")
				(number "202")
			)
			(pin bidirectional line
				(at 54.61 53.34 180)
				(length 7.62)
				(name "IO0P201")
				(number "201")
			)
			(pin bidirectional line
				(at 54.61 50.8 180)
				(length 7.62)
				(name "IO0P200")
				(number "200")
			)
			(pin bidirectional line
				(at 54.61 48.26 180)
				(length 7.62)
				(name "IO0P199")
				(number "199")
			)
			(pin bidirectional line
				(at 54.61 45.72 180)
				(length 7.62)
				(name "IO0P195")
				(number "195")
			)
			(pin bidirectional line
				(at 54.61 43.18 180)
				(length 7.62)
				(name "IO0P194")
				(number "194")
			)
			(pin bidirectional line
				(at 54.61 40.64 180)
				(length 7.62)
				(name "IO0P193")
				(number "193")
			)
			(pin bidirectional line
				(at 54.61 38.1 180)
				(length 7.62)
				(name "IO0P192")
				(number "192")
			)
			(pin bidirectional line
				(at 54.61 35.56 180)
				(length 7.62)
				(name "IO0P191")
				(number "191")
			)
			(pin bidirectional line
				(at 54.61 33.02 180)
				(length 7.62)
				(name "IO0VRP189")
				(number "189")
			)
			(pin bidirectional line
				(at 54.61 30.48 180)
				(length 7.62)
				(name "IO0P188")
				(number "188")
			)
			(pin bidirectional line
				(at 54.61 27.94 180)
				(length 7.62)
				(name "IO0P187")
				(number "187")
			)
			(pin input clock
				(at 54.61 25.4 180)
				(length 7.62)
				(name "GCK3")
				(number "185")
			)
			(pin input clock
				(at 54.61 20.32 180)
				(length 7.62)
				(name "GCK2")
				(number "182")
			)
			(pin bidirectional line
				(at 54.61 17.78 180)
				(length 7.62)
				(name "IO1P181")
				(number "181")
			)
			(pin bidirectional line
				(at 54.61 15.24 180)
				(length 7.62)
				(name "IO1P180")
				(number "180")
			)
			(pin bidirectional line
				(at 54.61 12.7 180)
				(length 7.62)
				(name "IO1P179")
				(number "179")
			)
			(pin bidirectional line
				(at 54.61 10.16 180)
				(length 7.62)
				(name "IO1VRP178")
				(number "178")
			)
			(pin bidirectional line
				(at 54.61 7.62 180)
				(length 7.62)
				(name "IO1P176")
				(number "176")
			)
			(pin bidirectional line
				(at 54.61 5.08 180)
				(length 7.62)
				(name "IO1P175")
				(number "175")
			)
			(pin bidirectional line
				(at 54.61 2.54 180)
				(length 7.62)
				(name "IO1P174")
				(number "174")
			)
			(pin bidirectional line
				(at 54.61 0 180)
				(length 7.62)
				(name "IO1P173")
				(number "173")
			)
			(pin bidirectional line
				(at 54.61 -2.54 180)
				(length 7.62)
				(name "IO1P172")
				(number "172")
			)
			(pin bidirectional line
				(at 54.61 -5.08 180)
				(length 7.62)
				(name "IO1P168")
				(number "168")
			)
			(pin bidirectional line
				(at 54.61 -7.62 180)
				(length 7.62)
				(name "IO1P167")
				(number "167")
			)
			(pin bidirectional line
				(at 54.61 -10.16 180)
				(length 7.62)
				(name "IO1P166")
				(number "166")
			)
			(pin bidirectional line
				(at 54.61 -12.7 180)
				(length 7.62)
				(name "IO1P165")
				(number "165")
			)
			(pin bidirectional line
				(at 54.61 -15.24 180)
				(length 7.62)
				(name "IO1VRP164")
				(number "164")
			)
			(pin bidirectional line
				(at 54.61 -17.78 180)
				(length 7.62)
				(name "IO1P163")
				(number "163")
			)
			(pin bidirectional line
				(at 54.61 -20.32 180)
				(length 7.62)
				(name "IO1P162")
				(number "162")
			)
			(pin bidirectional line
				(at 54.61 -25.4 180)
				(length 7.62)
				(name "IO2P152")
				(number "152")
			)
			(pin bidirectional line
				(at 54.61 -27.94 180)
				(length 7.62)
				(name "IO2P151")
				(number "151")
			)
			(pin bidirectional line
				(at 54.61 -30.48 180)
				(length 7.62)
				(name "IO2VRP150")
				(number "150")
			)
			(pin bidirectional line
				(at 54.61 -33.02 180)
				(length 7.62)
				(name "IO2P149")
				(number "149")
			)
			(pin bidirectional line
				(at 54.61 -35.56 180)
				(length 7.62)
				(name "IO2P148")
				(number "148")
			)
			(pin bidirectional line
				(at 54.61 -38.1 180)
				(length 7.62)
				(name "IO2P147")
				(number "147")
			)
			(pin bidirectional line
				(at 54.61 -40.64 180)
				(length 7.62)
				(name "IO2/D1P46")
				(number "146")
			)
			(pin bidirectional line
				(at 54.61 -43.18 180)
				(length 7.62)
				(name "IO2/D2P142")
				(number "142")
			)
			(pin bidirectional line
				(at 54.61 -45.72 180)
				(length 7.62)
				(name "IO2P141")
				(number "141")
			)
			(pin bidirectional line
				(at 54.61 -48.26 180)
				(length 7.62)
				(name "IO2P140")
				(number "140")
			)
			(pin bidirectional line
				(at 54.61 -50.8 180)
				(length 7.62)
				(name "IO2P139")
				(number "139")
			)
			(pin bidirectional line
				(at 54.61 -53.34 180)
				(length 7.62)
				(name "IO2P138")
				(number "138")
			)
			(pin bidirectional line
				(at 54.61 -55.88 180)
				(length 7.62)
				(name "IO2VRP136")
				(number "136")
			)
			(pin bidirectional line
				(at 54.61 -58.42 180)
				(length 7.62)
				(name "IO2/D3P135")
				(number "135")
			)
			(pin bidirectional line
				(at 54.61 -60.96 180)
				(length 7.62)
				(name "IO2P134")
				(number "134")
			)
			(pin bidirectional line
				(at 54.61 -63.5 180)
				(length 7.62)
				(name "IO2P133")
				(number "133")
			)
			(pin bidirectional line
				(at 54.61 -68.58 180)
				(length 7.62)
				(name "IO3P127")
				(number "127")
			)
			(pin bidirectional line
				(at 54.61 -71.12 180)
				(length 7.62)
				(name "IO3/D4P126")
				(number "126")
			)
			(pin bidirectional line
				(at 54.61 -73.66 180)
				(length 7.62)
				(name "IO3VRP125")
				(number "125")
			)
			(pin bidirectional line
				(at 54.61 -76.2 180)
				(length 7.62)
				(name "IO3P123")
				(number "123")
			)
			(pin bidirectional line
				(at 54.61 -78.74 180)
				(length 7.62)
				(name "IO3P122")
				(number "122")
			)
			(pin bidirectional line
				(at 54.61 -81.28 180)
				(length 7.62)
				(name "IO3P121")
				(number "121")
			)
			(pin bidirectional line
				(at 54.61 -83.82 180)
				(length 7.62)
				(name "IO3P120")
				(number "120")
			)
			(pin bidirectional line
				(at 54.61 -86.36 180)
				(length 7.62)
				(name "IO3/D5P119")
				(number "119")
			)
			(pin bidirectional line
				(at 54.61 -88.9 180)
				(length 7.62)
				(name "IO3/D6P115")
				(number "115")
			)
			(pin bidirectional line
				(at 54.61 -91.44 180)
				(length 7.62)
				(name "IO3P114")
				(number "114")
			)
			(pin bidirectional line
				(at 54.61 -93.98 180)
				(length 7.62)
				(name "IO3P113")
				(number "113")
			)
			(pin bidirectional line
				(at 54.61 -96.52 180)
				(length 7.62)
				(name "IO3P112")
				(number "112")
			)
			(pin bidirectional line
				(at 54.61 -99.06 180)
				(length 7.62)
				(name "IO3VRP111")
				(number "111")
			)
			(pin bidirectional line
				(at 54.61 -101.6 180)
				(length 7.62)
				(name "IO3P110")
				(number "110")
			)
			(pin bidirectional line
				(at 54.61 -104.14 180)
				(length 7.62)
				(name "IO3P109")
				(number "109")
			)
			(pin bidirectional line
				(at 54.61 -106.68 180)
				(length 7.62)
				(name "IO3/D7P108")
				(number "108")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC2S200PQ208"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 -2.3876 0)
		)
		(property "Value" "XC2S200PQ208"
			(at 0 2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "xilinx/spartan2e/spartan2e.pdf"
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC2S200PQ208_0_1")
		(symbol "XC2S200PQ208_1_1"
			(pin bidirectional line
				(at -54.61 107.95 0)
				(length 7.62)
				(name "TMS")
				(number "2")
			)
			(pin bidirectional line
				(at -54.61 105.41 0)
				(length 7.62)
				(name "TDO")
				(number "157")
			)
			(pin bidirectional line
				(at -54.61 102.87 0)
				(length 7.62)
				(name "TDI")
				(number "159")
			)
			(pin bidirectional line
				(at -54.61 100.33 0)
				(length 7.62)
				(name "TCK")
				(number "207")
			)
			(pin bidirectional line
				(at -54.61 95.25 0)
				(length 7.62)
				(name "DONE")
				(number "104")
			)
			(pin input line
				(at -54.61 92.71 0)
				(length 7.62)
				(name "/PROG")
				(number "106")
			)
			(pin bidirectional line
				(at -54.61 90.17 0)
				(length 7.62)
				(name "/INIT")
				(number "107")
			)
			(pin bidirectional clock
				(at -54.61 87.63 0)
				(length 7.62)
				(name "CCLK")
				(number "155")
			)
			(pin input line
				(at -54.61 82.55 0)
				(length 7.62)
				(name "M0")
				(number "52")
			)
			(pin input line
				(at -54.61 80.01 0)
				(length 7.62)
				(name "M1")
				(number "50")
			)
			(pin input line
				(at -54.61 77.47 0)
				(length 7.62)
				(name "M2")
				(number "54")
			)
			(pin bidirectional line
				(at -54.61 72.39 0)
				(length 7.62)
				(name "IO7P3")
				(number "3")
			)
			(pin bidirectional line
				(at -54.61 69.85 0)
				(length 7.62)
				(name "IO7VRP4")
				(number "4")
			)
			(pin bidirectional line
				(at -54.61 67.31 0)
				(length 7.62)
				(name "IO7P5")
				(number "5")
			)
			(pin bidirectional line
				(at -54.61 64.77 0)
				(length 7.62)
				(name "IO7VRP6")
				(number "6")
			)
			(pin bidirectional line
				(at -54.61 62.23 0)
				(length 7.62)
				(name "IO7P7")
				(number "7")
			)
			(pin bidirectional line
				(at -54.61 59.69 0)
				(length 7.62)
				(name "IO7P8")
				(number "8")
			)
			(pin bidirectional line
				(at -54.61 57.15 0)
				(length 7.62)
				(name "IO7VRP9")
				(number "9")
			)
			(pin bidirectional line
				(at -54.61 54.61 0)
				(length 7.62)
				(name "IO7P10")
				(number "10")
			)
			(pin bidirectional line
				(at -54.61 52.07 0)
				(length 7.62)
				(name "IO7P14")
				(number "14")
			)
			(pin bidirectional line
				(at -54.61 49.53 0)
				(length 7.62)
				(name "IO7P15")
				(number "15")
			)
			(pin bidirectional line
				(at -54.61 46.99 0)
				(length 7.62)
				(name "IO7P16")
				(number "16")
			)
			(pin bidirectional line
				(at -54.61 44.45 0)
				(length 7.62)
				(name "IO7P17")
				(number "17")
			)
			(pin bidirectional line
				(at -54.61 41.91 0)
				(length 7.62)
				(name "IO7P18")
				(number "18")
			)
			(pin bidirectional line
				(at -54.61 39.37 0)
				(length 7.62)
				(name "IO7VRP20")
				(number "20")
			)
			(pin bidirectional line
				(at -54.61 36.83 0)
				(length 7.62)
				(name "IO7P21")
				(number "21")
			)
			(pin bidirectional line
				(at -54.61 34.29 0)
				(length 7.62)
				(name "IO7P22")
				(number "22")
			)
			(pin bidirectional line
				(at -54.61 31.75 0)
				(length 7.62)
				(name "IO7P23")
				(number "23")
			)
			(pin bidirectional line
				(at -54.61 26.67 0)
				(length 7.62)
				(name "IO6P29")
				(number "29")
			)
			(pin bidirectional line
				(at -54.61 24.13 0)
				(length 7.62)
				(name "IO6P30")
				(number "30")
			)
			(pin bidirectional line
				(at -54.61 21.59 0)
				(length 7.62)
				(name "IO6VRP31")
				(number "31")
			)
			(pin bidirectional line
				(at -54.61 19.05 0)
				(length 7.62)
				(name "IO6P33")
				(number "33")
			)
			(pin bidirectional line
				(at -54.61 16.51 0)
				(length 7.62)
				(name "IO6P34")
				(number "34")
			)
			(pin bidirectional line
				(at -54.61 13.97 0)
				(length 7.62)
				(name "IO6P35")
				(number "35")
			)
			(pin bidirectional line
				(at -54.61 11.43 0)
				(length 7.62)
				(name "IO6P36")
				(number "36")
			)
			(pin bidirectional line
				(at -54.61 8.89 0)
				(length 7.62)
				(name "IO6P37")
				(number "37")
			)
			(pin bidirectional line
				(at -54.61 6.35 0)
				(length 7.62)
				(name "IO6P41")
				(number "41")
			)
			(pin bidirectional line
				(at -54.61 3.81 0)
				(length 7.62)
				(name "IO6VRP42")
				(number "42")
			)
			(pin bidirectional line
				(at -54.61 1.27 0)
				(length 7.62)
				(name "IO6P43")
				(number "43")
			)
			(pin bidirectional line
				(at -54.61 -1.27 0)
				(length 7.62)
				(name "IO6P44")
				(number "44")
			)
			(pin bidirectional line
				(at -54.61 -3.81 0)
				(length 7.62)
				(name "IO6VRP45")
				(number "45")
			)
			(pin bidirectional line
				(at -54.61 -6.35 0)
				(length 7.62)
				(name "IO6P46")
				(number "46")
			)
			(pin bidirectional line
				(at -54.61 -8.89 0)
				(length 7.62)
				(name "IO6VRP47")
				(number "47")
			)
			(pin bidirectional line
				(at -54.61 -11.43 0)
				(length 7.62)
				(name "IO6P48")
				(number "48")
			)
			(pin bidirectional line
				(at -54.61 -13.97 0)
				(length 7.62)
				(name "IO6P49")
				(number "49")
			)
			(pin bidirectional line
				(at -54.61 -19.05 0)
				(length 7.62)
				(name "IO5VRP57")
				(number "57")
			)
			(pin bidirectional line
				(at -54.61 -21.59 0)
				(length 7.62)
				(name "IO5P58")
				(number "58")
			)
			(pin bidirectional line
				(at -54.61 -24.13 0)
				(length 7.62)
				(name "IO5VRP59")
				(number "59")
			)
			(pin bidirectional line
				(at -54.61 -26.67 0)
				(length 7.62)
				(name "IO5P60")
				(number "60")
			)
			(pin bidirectional line
				(at -54.61 -29.21 0)
				(length 7.62)
				(name "IO5P61")
				(number "61")
			)
			(pin bidirectional line
				(at -54.61 -31.75 0)
				(length 7.62)
				(name "IO5VRP62")
				(number "62")
			)
			(pin bidirectional line
				(at -54.61 -34.29 0)
				(length 7.62)
				(name "IO5P63")
				(number "63")
			)
			(pin bidirectional line
				(at -54.61 -36.83 0)
				(length 7.62)
				(name "IO5P67")
				(number "67")
			)
			(pin bidirectional line
				(at -54.61 -39.37 0)
				(length 7.62)
				(name "IO5P68")
				(number "68")
			)
			(pin bidirectional line
				(at -54.61 -41.91 0)
				(length 7.62)
				(name "IO5P69")
				(number "69")
			)
			(pin bidirectional line
				(at -54.61 -44.45 0)
				(length 7.62)
				(name "IO5P70")
				(number "70")
			)
			(pin bidirectional line
				(at -54.61 -46.99 0)
				(length 7.62)
				(name "IO5P71")
				(number "71")
			)
			(pin bidirectional line
				(at -54.61 -49.53 0)
				(length 7.62)
				(name "IO5VRP73")
				(number "73")
			)
			(pin bidirectional line
				(at -54.61 -52.07 0)
				(length 7.62)
				(name "IO5P74")
				(number "74")
			)
			(pin bidirectional line
				(at -54.61 -54.61 0)
				(length 7.62)
				(name "IO5P75")
				(number "75")
			)
			(pin input clock
				(at -54.61 -57.15 0)
				(length 7.62)
				(name "GCK1")
				(number "77")
			)
			(pin input clock
				(at -54.61 -62.23 0)
				(length 7.62)
				(name "GCK0")
				(number "80")
			)
			(pin bidirectional line
				(at -54.61 -64.77 0)
				(length 7.62)
				(name "IO4P81")
				(number "81")
			)
			(pin bidirectional line
				(at -54.61 -67.31 0)
				(length 7.62)
				(name "IO4P82")
				(number "82")
			)
			(pin bidirectional line
				(at -54.61 -69.85 0)
				(length 7.62)
				(name "IO4P83")
				(number "83")
			)
			(pin bidirectional line
				(at -54.61 -72.39 0)
				(length 7.62)
				(name "IO4VRP84")
				(number "84")
			)
			(pin bidirectional line
				(at -54.61 -74.93 0)
				(length 7.62)
				(name "IO4P86")
				(number "86")
			)
			(pin bidirectional line
				(at -54.61 -77.47 0)
				(length 7.62)
				(name "IO4P87")
				(number "87")
			)
			(pin bidirectional line
				(at -54.61 -80.01 0)
				(length 7.62)
				(name "IO4P88")
				(number "88")
			)
			(pin bidirectional line
				(at -54.61 -82.55 0)
				(length 7.62)
				(name "IO4P89")
				(number "89")
			)
			(pin bidirectional line
				(at -54.61 -85.09 0)
				(length 7.62)
				(name "IO4P90")
				(number "90")
			)
			(pin bidirectional line
				(at -54.61 -87.63 0)
				(length 7.62)
				(name "IO4P94")
				(number "94")
			)
			(pin bidirectional line
				(at -54.61 -90.17 0)
				(length 7.62)
				(name "IO4VRP95")
				(number "95")
			)
			(pin bidirectional line
				(at -54.61 -92.71 0)
				(length 7.62)
				(name "IO4P96")
				(number "96")
			)
			(pin bidirectional line
				(at -54.61 -95.25 0)
				(length 7.62)
				(name "IO4P97")
				(number "97")
			)
			(pin bidirectional line
				(at -54.61 -97.79 0)
				(length 7.62)
				(name "IO4VRP98")
				(number "98")
			)
			(pin bidirectional line
				(at -54.61 -100.33 0)
				(length 7.62)
				(name "IO4P99")
				(number "99")
			)
			(pin bidirectional line
				(at -54.61 -102.87 0)
				(length 7.62)
				(name "IO4VRP100")
				(number "100")
			)
			(pin bidirectional line
				(at -54.61 -105.41 0)
				(length 7.62)
				(name "IO4P101")
				(number "101")
			)
			(pin bidirectional line
				(at -54.61 -107.95 0)
				(length 7.62)
				(name "IO4P102")
				(number "102")
			)
			(pin passive line
				(at -36.83 118.11 270)
				(length 7.62)
				(name "VCCO")
				(number "12")
			)
			(pin passive line
				(at -34.29 118.11 270)
				(length 7.62)
				(name "VCCO")
				(number "26")
			)
			(pin passive line
				(at -31.75 118.11 270)
				(length 7.62)
				(name "VCCO")
				(number "39")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "103")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "116")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "124")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "131")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "137")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "145")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "158")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "169")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "177")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "183")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "190")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "198")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "40")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "51")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "64")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "72")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "79")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "85")
			)
			(pin passive line
				(at -31.75 -118.11 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "93")
			)
			(pin passive line
				(at -29.21 118.11 270)
				(length 7.62)
				(name "VCCO")
				(number "53")
			)
			(pin passive line
				(at -26.67 118.11 270)
				(length 7.62)
				(name "VCCO")
				(number "65")
			)
			(pin passive line
				(at -24.13 118.11 270)
				(length 7.62)
				(name "VCCO")
				(number "78")
			)
			(pin passive line
				(at -21.59 118.11 270)
				(length 7.62)
				(name "VCCO")
				(number "92")
			)
			(pin passive line
				(at -19.05 118.11 270)
				(length 7.62)
				(name "VCCO")
				(number "105")
			)
			(pin passive line
				(at -16.51 118.11 270)
				(length 7.62)
				(name "VCCO")
				(number "117")
			)
			(pin passive line
				(at -13.97 118.11 270)
				(length 7.62)
				(name "VCCO")
				(number "130")
			)
			(pin passive line
				(at -11.43 118.11 270)
				(length 7.62)
				(name "VCCO")
				(number "144")
			)
			(pin passive line
				(at -8.89 118.11 270)
				(length 7.62)
				(name "VCCO")
				(number "156")
			)
			(pin passive line
				(at -6.35 118.11 270)
				(length 7.62)
				(name "VCCO")
				(number "170")
			)
			(pin passive line
				(at -3.81 118.11 270)
				(length 7.62)
				(name "VCCO")
				(number "184")
			)
			(pin passive line
				(at -1.27 118.11 270)
				(length 7.62)
				(name "VCCO")
				(number "197")
			)
			(pin passive line
				(at 1.27 118.11 270)
				(length 7.62)
				(name "VCCO")
				(number "208")
			)
			(pin passive line
				(at 8.89 118.11 270)
				(length 7.62)
				(name "VCCINT")
				(number "13")
			)
			(pin passive line
				(at 11.43 118.11 270)
				(length 7.62)
				(name "VCCINT")
				(number "28")
			)
			(pin passive line
				(at 13.97 118.11 270)
				(length 7.62)
				(name "VCCINT")
				(number "38")
			)
			(pin passive line
				(at 16.51 118.11 270)
				(length 7.62)
				(name "VCCINT")
				(number "66")
			)
			(pin passive line
				(at 19.05 118.11 270)
				(length 7.62)
				(name "VCCINT")
				(number "76")
			)
			(pin passive line
				(at 21.59 118.11 270)
				(length 7.62)
				(name "VCCINT")
				(number "91")
			)
			(pin passive line
				(at 24.13 118.11 270)
				(length 7.62)
				(name "VCCINT")
				(number "118")
			)
			(pin passive line
				(at 26.67 118.11 270)
				(length 7.62)
				(name "VCCINT")
				(number "128")
			)
			(pin passive line
				(at 29.21 118.11 270)
				(length 7.62)
				(name "VCCINT")
				(number "143")
			)
			(pin passive line
				(at 31.75 118.11 270)
				(length 7.62)
				(name "VCCINT")
				(number "171")
			)
			(pin passive line
				(at 34.29 118.11 270)
				(length 7.62)
				(name "VCCINT")
				(number "186")
			)
			(pin passive line
				(at 36.83 118.11 270)
				(length 7.62)
				(name "VCCINT")
				(number "196")
			)
			(pin bidirectional line
				(at 54.61 97.79 180)
				(length 7.62)
				(name "IRDY2")
				(number "132")
			)
			(pin bidirectional line
				(at 54.61 95.25 180)
				(length 7.62)
				(name "TRDY3")
				(number "129")
			)
			(pin bidirectional line
				(at 54.61 92.71 180)
				(length 7.62)
				(name "TRDY6")
				(number "27")
			)
			(pin bidirectional line
				(at 54.61 90.17 180)
				(length 7.62)
				(name "IRDY7")
				(number "24")
			)
			(pin bidirectional line
				(at 54.61 85.09 180)
				(length 7.62)
				(name "/WR")
				(number "161")
			)
			(pin bidirectional line
				(at 54.61 82.55 180)
				(length 7.62)
				(name "/CS")
				(number "160")
			)
			(pin bidirectional line
				(at 54.61 77.47 180)
				(length 7.62)
				(name "BUSY/DOUT")
				(number "154")
			)
			(pin bidirectional line
				(at 54.61 74.93 180)
				(length 7.62)
				(name "D0/DIN")
				(number "153")
			)
			(pin bidirectional line
				(at 54.61 67.31 180)
				(length 7.62)
				(name "IO0P206")
				(number "206")
			)
			(pin bidirectional line
				(at 54.61 64.77 180)
				(length 7.62)
				(name "IO0VRP205")
				(number "205")
			)
			(pin bidirectional line
				(at 54.61 62.23 180)
				(length 7.62)
				(name "IO0P204")
				(number "204")
			)
			(pin bidirectional line
				(at 54.61 59.69 180)
				(length 7.62)
				(name "IO0VRP203")
				(number "203")
			)
			(pin bidirectional line
				(at 54.61 57.15 180)
				(length 7.62)
				(name "IO0P202")
				(number "202")
			)
			(pin bidirectional line
				(at 54.61 54.61 180)
				(length 7.62)
				(name "IO0P201")
				(number "201")
			)
			(pin bidirectional line
				(at 54.61 52.07 180)
				(length 7.62)
				(name "IO0VRP200")
				(number "200")
			)
			(pin bidirectional line
				(at 54.61 49.53 180)
				(length 7.62)
				(name "IO0P199")
				(number "199")
			)
			(pin bidirectional line
				(at 54.61 46.99 180)
				(length 7.62)
				(name "IO0P195")
				(number "195")
			)
			(pin bidirectional line
				(at 54.61 44.45 180)
				(length 7.62)
				(name "IO0P194")
				(number "194")
			)
			(pin bidirectional line
				(at 54.61 41.91 180)
				(length 7.62)
				(name "IO0P193")
				(number "193")
			)
			(pin bidirectional line
				(at 54.61 39.37 180)
				(length 7.62)
				(name "IO0P192")
				(number "192")
			)
			(pin bidirectional line
				(at 54.61 36.83 180)
				(length 7.62)
				(name "IO0P191")
				(number "191")
			)
			(pin bidirectional line
				(at 54.61 34.29 180)
				(length 7.62)
				(name "IO0VRP189")
				(number "189")
			)
			(pin bidirectional line
				(at 54.61 31.75 180)
				(length 7.62)
				(name "IO0P188")
				(number "188")
			)
			(pin bidirectional line
				(at 54.61 29.21 180)
				(length 7.62)
				(name "IO0P187")
				(number "187")
			)
			(pin input clock
				(at 54.61 26.67 180)
				(length 7.62)
				(name "GCK3")
				(number "185")
			)
			(pin input clock
				(at 54.61 21.59 180)
				(length 7.62)
				(name "GCK2")
				(number "182")
			)
			(pin bidirectional line
				(at 54.61 19.05 180)
				(length 7.62)
				(name "IO1P181")
				(number "181")
			)
			(pin bidirectional line
				(at 54.61 16.51 180)
				(length 7.62)
				(name "IO1P180")
				(number "180")
			)
			(pin bidirectional line
				(at 54.61 13.97 180)
				(length 7.62)
				(name "IO1P179")
				(number "179")
			)
			(pin bidirectional line
				(at 54.61 11.43 180)
				(length 7.62)
				(name "IO1VRP178")
				(number "178")
			)
			(pin bidirectional line
				(at 54.61 8.89 180)
				(length 7.62)
				(name "IO1P176")
				(number "176")
			)
			(pin bidirectional line
				(at 54.61 6.35 180)
				(length 7.62)
				(name "IO1P175")
				(number "175")
			)
			(pin bidirectional line
				(at 54.61 3.81 180)
				(length 7.62)
				(name "IO1P174")
				(number "174")
			)
			(pin bidirectional line
				(at 54.61 1.27 180)
				(length 7.62)
				(name "IO1P173")
				(number "173")
			)
			(pin bidirectional line
				(at 54.61 -1.27 180)
				(length 7.62)
				(name "IO1P172")
				(number "172")
			)
			(pin bidirectional line
				(at 54.61 -3.81 180)
				(length 7.62)
				(name "IO1P168")
				(number "168")
			)
			(pin bidirectional line
				(at 54.61 -6.35 180)
				(length 7.62)
				(name "IO1VRP167")
				(number "167")
			)
			(pin bidirectional line
				(at 54.61 -8.89 180)
				(length 7.62)
				(name "IO1P166")
				(number "166")
			)
			(pin bidirectional line
				(at 54.61 -11.43 180)
				(length 7.62)
				(name "IO1P165")
				(number "165")
			)
			(pin bidirectional line
				(at 54.61 -13.97 180)
				(length 7.62)
				(name "IO1VRP164")
				(number "164")
			)
			(pin bidirectional line
				(at 54.61 -16.51 180)
				(length 7.62)
				(name "IO1P163")
				(number "163")
			)
			(pin bidirectional line
				(at 54.61 -19.05 180)
				(length 7.62)
				(name "IO1VRP162")
				(number "162")
			)
			(pin bidirectional line
				(at 54.61 -24.13 180)
				(length 7.62)
				(name "IO2VRP152")
				(number "152")
			)
			(pin bidirectional line
				(at 54.61 -26.67 180)
				(length 7.62)
				(name "IO2P151")
				(number "151")
			)
			(pin bidirectional line
				(at 54.61 -29.21 180)
				(length 7.62)
				(name "IO2VRP150")
				(number "150")
			)
			(pin bidirectional line
				(at 54.61 -31.75 180)
				(length 7.62)
				(name "IO2P149")
				(number "149")
			)
			(pin bidirectional line
				(at 54.61 -34.29 180)
				(length 7.62)
				(name "IO2P148")
				(number "148")
			)
			(pin bidirectional line
				(at 54.61 -36.83 180)
				(length 7.62)
				(name "IO2VRP147")
				(number "147")
			)
			(pin bidirectional line
				(at 54.61 -39.37 180)
				(length 7.62)
				(name "IO2/D1P46")
				(number "146")
			)
			(pin bidirectional line
				(at 54.61 -41.91 180)
				(length 7.62)
				(name "IO2/D2P142")
				(number "142")
			)
			(pin bidirectional line
				(at 54.61 -44.45 180)
				(length 7.62)
				(name "IO2P141")
				(number "141")
			)
			(pin bidirectional line
				(at 54.61 -46.99 180)
				(length 7.62)
				(name "IO2P140")
				(number "140")
			)
			(pin bidirectional line
				(at 54.61 -49.53 180)
				(length 7.62)
				(name "IO2P139")
				(number "139")
			)
			(pin bidirectional line
				(at 54.61 -52.07 180)
				(length 7.62)
				(name "IO2P138")
				(number "138")
			)
			(pin bidirectional line
				(at 54.61 -54.61 180)
				(length 7.62)
				(name "IO2VRP136")
				(number "136")
			)
			(pin bidirectional line
				(at 54.61 -57.15 180)
				(length 7.62)
				(name "IO2/D3P135")
				(number "135")
			)
			(pin bidirectional line
				(at 54.61 -59.69 180)
				(length 7.62)
				(name "IO2P134")
				(number "134")
			)
			(pin bidirectional line
				(at 54.61 -62.23 180)
				(length 7.62)
				(name "IO2P133")
				(number "133")
			)
			(pin bidirectional line
				(at 54.61 -67.31 180)
				(length 7.62)
				(name "IO3P127")
				(number "127")
			)
			(pin bidirectional line
				(at 54.61 -69.85 180)
				(length 7.62)
				(name "IO3/D4P126")
				(number "126")
			)
			(pin bidirectional line
				(at 54.61 -72.39 180)
				(length 7.62)
				(name "IO3VRP125")
				(number "125")
			)
			(pin bidirectional line
				(at 54.61 -74.93 180)
				(length 7.62)
				(name "IO3P123")
				(number "123")
			)
			(pin bidirectional line
				(at 54.61 -77.47 180)
				(length 7.62)
				(name "IO3P122")
				(number "122")
			)
			(pin bidirectional line
				(at 54.61 -80.01 180)
				(length 7.62)
				(name "IO3P121")
				(number "121")
			)
			(pin bidirectional line
				(at 54.61 -82.55 180)
				(length 7.62)
				(name "IO3P120")
				(number "120")
			)
			(pin bidirectional line
				(at 54.61 -85.09 180)
				(length 7.62)
				(name "IO3/D5P119")
				(number "119")
			)
			(pin bidirectional line
				(at 54.61 -87.63 180)
				(length 7.62)
				(name "IO3/D6P115")
				(number "115")
			)
			(pin bidirectional line
				(at 54.61 -90.17 180)
				(length 7.62)
				(name "IO3VRP114")
				(number "114")
			)
			(pin bidirectional line
				(at 54.61 -92.71 180)
				(length 7.62)
				(name "IO3P113")
				(number "113")
			)
			(pin bidirectional line
				(at 54.61 -95.25 180)
				(length 7.62)
				(name "IO3P112")
				(number "112")
			)
			(pin bidirectional line
				(at 54.61 -97.79 180)
				(length 7.62)
				(name "IO3VRP111")
				(number "111")
			)
			(pin bidirectional line
				(at 54.61 -100.33 180)
				(length 7.62)
				(name "IO3P110")
				(number "110")
			)
			(pin bidirectional line
				(at 54.61 -102.87 180)
				(length 7.62)
				(name "IO3VRP109")
				(number "109")
			)
			(pin bidirectional line
				(at 54.61 -105.41 180)
				(length 7.62)
				(name "IO3/D7P108")
				(number "108")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC2S300PQ208"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "XC2S300PQ208"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "xilinx/spartan2e/spartan2e.pdf"
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC2S300PQ208_0_1")
		(symbol "XC2S300PQ208_1_1"
			(pin bidirectional line
				(at -54.61 110.49 0)
				(length 7.62)
				(name "TMS")
				(number "2")
			)
			(pin bidirectional line
				(at -54.61 107.95 0)
				(length 7.62)
				(name "TDO")
				(number "157")
			)
			(pin bidirectional line
				(at -54.61 105.41 0)
				(length 7.62)
				(name "TDI")
				(number "159")
			)
			(pin bidirectional line
				(at -54.61 102.87 0)
				(length 7.62)
				(name "TCK")
				(number "207")
			)
			(pin bidirectional line
				(at -54.61 97.79 0)
				(length 7.62)
				(name "DONE")
				(number "104")
			)
			(pin input line
				(at -54.61 95.25 0)
				(length 7.62)
				(name "/PROG")
				(number "106")
			)
			(pin bidirectional line
				(at -54.61 92.71 0)
				(length 7.62)
				(name "/INIT")
				(number "107")
			)
			(pin bidirectional clock
				(at -54.61 90.17 0)
				(length 7.62)
				(name "CCLK")
				(number "155")
			)
			(pin input line
				(at -54.61 85.09 0)
				(length 7.62)
				(name "M0")
				(number "52")
			)
			(pin input line
				(at -54.61 82.55 0)
				(length 7.62)
				(name "M1")
				(number "50")
			)
			(pin input line
				(at -54.61 80.01 0)
				(length 7.62)
				(name "M2")
				(number "54")
			)
			(pin bidirectional line
				(at -54.61 74.93 0)
				(length 7.62)
				(name "IO7P3")
				(number "3")
			)
			(pin bidirectional line
				(at -54.61 72.39 0)
				(length 7.62)
				(name "IO7VRP4")
				(number "4")
			)
			(pin bidirectional line
				(at -54.61 69.85 0)
				(length 7.62)
				(name "IO7P5")
				(number "5")
			)
			(pin bidirectional line
				(at -54.61 67.31 0)
				(length 7.62)
				(name "IO7VRP6")
				(number "6")
			)
			(pin bidirectional line
				(at -54.61 64.77 0)
				(length 7.62)
				(name "IO7P7")
				(number "7")
			)
			(pin bidirectional line
				(at -54.61 62.23 0)
				(length 7.62)
				(name "IO7P8")
				(number "8")
			)
			(pin bidirectional line
				(at -54.61 59.69 0)
				(length 7.62)
				(name "IO7VRP9")
				(number "9")
			)
			(pin bidirectional line
				(at -54.61 57.15 0)
				(length 7.62)
				(name "IO7VRP10")
				(number "10")
			)
			(pin bidirectional line
				(at -54.61 54.61 0)
				(length 7.62)
				(name "IO7P11")
				(number "11")
			)
			(pin bidirectional line
				(at -54.61 52.07 0)
				(length 7.62)
				(name "IO7P15")
				(number "15")
			)
			(pin bidirectional line
				(at -54.61 49.53 0)
				(length 7.62)
				(name "IO7P16")
				(number "16")
			)
			(pin bidirectional line
				(at -54.61 46.99 0)
				(length 7.62)
				(name "IO7P17")
				(number "17")
			)
			(pin bidirectional line
				(at -54.61 44.45 0)
				(length 7.62)
				(name "IO7P18")
				(number "18")
			)
			(pin bidirectional line
				(at -54.61 41.91 0)
				(length 7.62)
				(name "IO7VRP20")
				(number "20")
			)
			(pin bidirectional line
				(at -54.61 39.37 0)
				(length 7.62)
				(name "IO7P21")
				(number "21")
			)
			(pin bidirectional line
				(at -54.61 36.83 0)
				(length 7.62)
				(name "IO7P22")
				(number "22")
			)
			(pin bidirectional line
				(at -54.61 34.29 0)
				(length 7.62)
				(name "IO7P23")
				(number "23")
			)
			(pin bidirectional line
				(at -54.61 29.21 0)
				(length 7.62)
				(name "IO6P29")
				(number "29")
			)
			(pin bidirectional line
				(at -54.61 26.67 0)
				(length 7.62)
				(name "IO6P30")
				(number "30")
			)
			(pin bidirectional line
				(at -54.61 24.13 0)
				(length 7.62)
				(name "IO6VRP31")
				(number "31")
			)
			(pin bidirectional line
				(at -54.61 21.59 0)
				(length 7.62)
				(name "IO6P33")
				(number "33")
			)
			(pin bidirectional line
				(at -54.61 19.05 0)
				(length 7.62)
				(name "IO6P34")
				(number "34")
			)
			(pin bidirectional line
				(at -54.61 16.51 0)
				(length 7.62)
				(name "IO6P35")
				(number "35")
			)
			(pin bidirectional line
				(at -54.61 13.97 0)
				(length 7.62)
				(name "IO6P36")
				(number "36")
			)
			(pin bidirectional line
				(at -54.61 11.43 0)
				(length 7.62)
				(name "IO6P40")
				(number "40")
			)
			(pin bidirectional line
				(at -54.61 8.89 0)
				(length 7.62)
				(name "IO6VRP41")
				(number "41")
			)
			(pin bidirectional line
				(at -54.61 6.35 0)
				(length 7.62)
				(name "IO6P42")
				(number "42")
			)
			(pin bidirectional line
				(at -54.61 3.81 0)
				(length 7.62)
				(name "IO6P43")
				(number "43")
			)
			(pin bidirectional line
				(at -54.61 1.27 0)
				(length 7.62)
				(name "IO6P44")
				(number "44")
			)
			(pin bidirectional line
				(at -54.61 -1.27 0)
				(length 7.62)
				(name "IO6VRP45")
				(number "45")
			)
			(pin bidirectional line
				(at -54.61 -3.81 0)
				(length 7.62)
				(name "IO6P46")
				(number "46")
			)
			(pin bidirectional line
				(at -54.61 -6.35 0)
				(length 7.62)
				(name "IO6VRP47")
				(number "47")
			)
			(pin bidirectional line
				(at -54.61 -8.89 0)
				(length 7.62)
				(name "IO6P48")
				(number "48")
			)
			(pin bidirectional line
				(at -54.61 -11.43 0)
				(length 7.62)
				(name "IO6P49")
				(number "49")
			)
			(pin bidirectional line
				(at -54.61 -16.51 0)
				(length 7.62)
				(name "IO5P55")
				(number "55")
			)
			(pin bidirectional line
				(at -54.61 -19.05 0)
				(length 7.62)
				(name "IO5P56")
				(number "56")
			)
			(pin bidirectional line
				(at -54.61 -21.59 0)
				(length 7.62)
				(name "IO5VRP57")
				(number "57")
			)
			(pin bidirectional line
				(at -54.61 -24.13 0)
				(length 7.62)
				(name "IO5P58")
				(number "58")
			)
			(pin bidirectional line
				(at -54.61 -26.67 0)
				(length 7.62)
				(name "IO5VRP59")
				(number "59")
			)
			(pin bidirectional line
				(at -54.61 -29.21 0)
				(length 7.62)
				(name "IO5P60")
				(number "60")
			)
			(pin bidirectional line
				(at -54.61 -31.75 0)
				(length 7.62)
				(name "IO5P61")
				(number "61")
			)
			(pin bidirectional line
				(at -54.61 -34.29 0)
				(length 7.62)
				(name "IO5P62")
				(number "62")
			)
			(pin bidirectional line
				(at -54.61 -36.83 0)
				(length 7.62)
				(name "IO5VRP63")
				(number "63")
			)
			(pin bidirectional line
				(at -54.61 -39.37 0)
				(length 7.62)
				(name "IO5P64")
				(number "64")
			)
			(pin bidirectional line
				(at -54.61 -41.91 0)
				(length 7.62)
				(name "IO5P68")
				(number "68")
			)
			(pin bidirectional line
				(at -54.61 -44.45 0)
				(length 7.62)
				(name "IO5P69")
				(number "69")
			)
			(pin bidirectional line
				(at -54.61 -46.99 0)
				(length 7.62)
				(name "IO5P70")
				(number "70")
			)
			(pin bidirectional line
				(at -54.61 -49.53 0)
				(length 7.62)
				(name "IO5P71")
				(number "71")
			)
			(pin bidirectional line
				(at -54.61 -52.07 0)
				(length 7.62)
				(name "IO5VRP73")
				(number "73")
			)
			(pin bidirectional line
				(at -54.61 -54.61 0)
				(length 7.62)
				(name "IO5P74")
				(number "74")
			)
			(pin bidirectional line
				(at -54.61 -57.15 0)
				(length 7.62)
				(name "IO5P75")
				(number "75")
			)
			(pin input clock
				(at -54.61 -59.69 0)
				(length 7.62)
				(name "GCK1")
				(number "77")
			)
			(pin input clock
				(at -54.61 -64.77 0)
				(length 7.62)
				(name "GCK0")
				(number "80")
			)
			(pin bidirectional line
				(at -54.61 -67.31 0)
				(length 7.62)
				(name "IO4P81")
				(number "81")
			)
			(pin bidirectional line
				(at -54.61 -69.85 0)
				(length 7.62)
				(name "IO4P82")
				(number "82")
			)
			(pin bidirectional line
				(at -54.61 -72.39 0)
				(length 7.62)
				(name "IO4P83")
				(number "83")
			)
			(pin bidirectional line
				(at -54.61 -74.93 0)
				(length 7.62)
				(name "IO4VRP84")
				(number "84")
			)
			(pin bidirectional line
				(at -54.61 -77.47 0)
				(length 7.62)
				(name "IO4P86")
				(number "86")
			)
			(pin bidirectional line
				(at -54.61 -80.01 0)
				(length 7.62)
				(name "IO4P87")
				(number "87")
			)
			(pin bidirectional line
				(at -54.61 -82.55 0)
				(length 7.62)
				(name "IO4P88")
				(number "88")
			)
			(pin bidirectional line
				(at -54.61 -85.09 0)
				(length 7.62)
				(name "IO4P89")
				(number "89")
			)
			(pin bidirectional line
				(at -54.61 -87.63 0)
				(length 7.62)
				(name "IO4P93")
				(number "93")
			)
			(pin bidirectional line
				(at -54.61 -90.17 0)
				(length 7.62)
				(name "IO4VRP94")
				(number "94")
			)
			(pin bidirectional line
				(at -54.61 -92.71 0)
				(length 7.62)
				(name "IO4P95")
				(number "95")
			)
			(pin bidirectional line
				(at -54.61 -95.25 0)
				(length 7.62)
				(name "IO4P96")
				(number "96")
			)
			(pin bidirectional line
				(at -54.61 -97.79 0)
				(length 7.62)
				(name "IO4P97")
				(number "97")
			)
			(pin bidirectional line
				(at -54.61 -100.33 0)
				(length 7.62)
				(name "IO4VRP98")
				(number "98")
			)
			(pin bidirectional line
				(at -54.61 -102.87 0)
				(length 7.62)
				(name "IO4P99")
				(number "99")
			)
			(pin bidirectional line
				(at -54.61 -105.41 0)
				(length 7.62)
				(name "IO4VRP100")
				(number "100")
			)
			(pin bidirectional line
				(at -54.61 -107.95 0)
				(length 7.62)
				(name "IO4P101")
				(number "101")
			)
			(pin bidirectional line
				(at -54.61 -110.49 0)
				(length 7.62)
				(name "IO4P102")
				(number "102")
			)
			(pin power_in line
				(at -36.83 120.65 270)
				(length 7.62)
				(name "VCCO")
				(number "13")
			)
			(pin power_in line
				(at -34.29 120.65 270)
				(length 7.62)
				(name "VCCO")
				(number "26")
			)
			(pin power_in line
				(at -31.75 120.65 270)
				(length 7.62)
				(name "VCCO")
				(number "38")
			)
			(pin power_in line
				(at -31.75 -120.65 90)
				(length 7.62)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "103")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "117")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "124")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "131")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "137")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "144")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "158")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "170")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "177")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "183")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "190")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "197")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "51")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "72")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "79")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "85")
			)
			(pin passive line
				(at -31.75 -120.65 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "92")
			)
			(pin power_in line
				(at -29.21 120.65 270)
				(length 7.62)
				(name "VCCO")
				(number "53")
			)
			(pin power_in line
				(at -26.67 120.65 270)
				(length 7.62)
				(name "VCCO")
				(number "66")
			)
			(pin power_in line
				(at -24.13 120.65 270)
				(length 7.62)
				(name "VCCO")
				(number "78")
			)
			(pin power_in line
				(at -21.59 120.65 270)
				(length 7.62)
				(name "VCCO")
				(number "91")
			)
			(pin power_in line
				(at -19.05 120.65 270)
				(length 7.62)
				(name "VCCO")
				(number "105")
			)
			(pin power_in line
				(at -16.51 120.65 270)
				(length 7.62)
				(name "VCCO")
				(number "118")
			)
			(pin power_in line
				(at -13.97 120.65 270)
				(length 7.62)
				(name "VCCO")
				(number "130")
			)
			(pin power_in line
				(at -11.43 120.65 270)
				(length 7.62)
				(name "VCCO")
				(number "143")
			)
			(pin power_in line
				(at -8.89 120.65 270)
				(length 7.62)
				(name "VCCO")
				(number "156")
			)
			(pin passive line
				(at -6.35 120.65 270)
				(length 7.62)
				(name "VCCO")
				(number "171")
			)
			(pin power_in line
				(at -3.81 120.65 270)
				(length 7.62)
				(name "VCCO")
				(number "184")
			)
			(pin power_in line
				(at -1.27 120.65 270)
				(length 7.62)
				(name "VCCO")
				(number "196")
			)
			(pin power_in line
				(at 1.27 120.65 270)
				(length 7.62)
				(name "VCCO")
				(number "208")
			)
			(pin power_in line
				(at 8.89 120.65 270)
				(length 7.62)
				(name "VCCINT")
				(number "14")
			)
			(pin power_in line
				(at 11.43 120.65 270)
				(length 7.62)
				(name "VCCINT")
				(number "28")
			)
			(pin power_in line
				(at 13.97 120.65 270)
				(length 7.62)
				(name "VCCINT")
				(number "37")
			)
			(pin power_in line
				(at 16.51 120.65 270)
				(length 7.62)
				(name "VCCINT")
				(number "67")
			)
			(pin power_in line
				(at 19.05 120.65 270)
				(length 7.62)
				(name "VCCINT")
				(number "76")
			)
			(pin power_in line
				(at 21.59 120.65 270)
				(length 7.62)
				(name "VCCINT")
				(number "90")
			)
			(pin power_in line
				(at 24.13 120.65 270)
				(length 7.62)
				(name "VCCINT")
				(number "119")
			)
			(pin power_in line
				(at 26.67 120.65 270)
				(length 7.62)
				(name "VCCINT")
				(number "128")
			)
			(pin power_in line
				(at 29.21 120.65 270)
				(length 7.62)
				(name "VCCINT")
				(number "142")
			)
			(pin power_in line
				(at 31.75 120.65 270)
				(length 7.62)
				(name "VCCINT")
				(number "172")
			)
			(pin power_in line
				(at 34.29 120.65 270)
				(length 7.62)
				(name "VCCINT")
				(number "186")
			)
			(pin power_in line
				(at 36.83 120.65 270)
				(length 7.62)
				(name "VCCINT")
				(number "195")
			)
			(pin bidirectional line
				(at 54.61 100.33 180)
				(length 7.62)
				(name "IRDY2")
				(number "132")
			)
			(pin bidirectional line
				(at 54.61 97.79 180)
				(length 7.62)
				(name "TRDY3")
				(number "129")
			)
			(pin bidirectional line
				(at 54.61 95.25 180)
				(length 7.62)
				(name "TRDY6")
				(number "27")
			)
			(pin bidirectional line
				(at 54.61 92.71 180)
				(length 7.62)
				(name "IRDY7")
				(number "24")
			)
			(pin bidirectional line
				(at 54.61 87.63 180)
				(length 7.62)
				(name "/WR")
				(number "161")
			)
			(pin bidirectional line
				(at 54.61 85.09 180)
				(length 7.62)
				(name "/CS")
				(number "160")
			)
			(pin bidirectional line
				(at 54.61 80.01 180)
				(length 7.62)
				(name "BUSY/DOUT")
				(number "154")
			)
			(pin bidirectional line
				(at 54.61 77.47 180)
				(length 7.62)
				(name "D0/DIN")
				(number "153")
			)
			(pin bidirectional line
				(at 54.61 69.85 180)
				(length 7.62)
				(name "IO0P206")
				(number "206")
			)
			(pin bidirectional line
				(at 54.61 67.31 180)
				(length 7.62)
				(name "IO0VRP205")
				(number "205")
			)
			(pin bidirectional line
				(at 54.61 64.77 180)
				(length 7.62)
				(name "IO0P204")
				(number "204")
			)
			(pin bidirectional line
				(at 54.61 62.23 180)
				(length 7.62)
				(name "IO0VRP203")
				(number "203")
			)
			(pin bidirectional line
				(at 54.61 59.69 180)
				(length 7.62)
				(name "IO0P202")
				(number "202")
			)
			(pin bidirectional line
				(at 54.61 57.15 180)
				(length 7.62)
				(name "IO0P201")
				(number "201")
			)
			(pin bidirectional line
				(at 54.61 54.61 180)
				(length 7.62)
				(name "IO0P200")
				(number "200")
			)
			(pin bidirectional line
				(at 54.61 52.07 180)
				(length 7.62)
				(name "IO0VRP199")
				(number "199")
			)
			(pin bidirectional line
				(at 54.61 49.53 180)
				(length 7.62)
				(name "IO0P198")
				(number "198")
			)
			(pin bidirectional line
				(at 54.61 46.99 180)
				(length 7.62)
				(name "IO0P194")
				(number "194")
			)
			(pin bidirectional line
				(at 54.61 44.45 180)
				(length 7.62)
				(name "IO0P193")
				(number "193")
			)
			(pin bidirectional line
				(at 54.61 41.91 180)
				(length 7.62)
				(name "IO0P192")
				(number "192")
			)
			(pin bidirectional line
				(at 54.61 39.37 180)
				(length 7.62)
				(name "IO0P191")
				(number "191")
			)
			(pin bidirectional line
				(at 54.61 36.83 180)
				(length 7.62)
				(name "IO0VRP189")
				(number "189")
			)
			(pin bidirectional line
				(at 54.61 34.29 180)
				(length 7.62)
				(name "IO0P188")
				(number "188")
			)
			(pin bidirectional line
				(at 54.61 31.75 180)
				(length 7.62)
				(name "IO0P187")
				(number "187")
			)
			(pin input clock
				(at 54.61 29.21 180)
				(length 7.62)
				(name "GCK3")
				(number "185")
			)
			(pin input clock
				(at 54.61 24.13 180)
				(length 7.62)
				(name "GCK2")
				(number "182")
			)
			(pin bidirectional line
				(at 54.61 21.59 180)
				(length 7.62)
				(name "IO1P181")
				(number "181")
			)
			(pin bidirectional line
				(at 54.61 19.05 180)
				(length 7.62)
				(name "IO1P180")
				(number "180")
			)
			(pin bidirectional line
				(at 54.61 16.51 180)
				(length 7.62)
				(name "IO1P179")
				(number "179")
			)
			(pin bidirectional line
				(at 54.61 13.97 180)
				(length 7.62)
				(name "IO1VRP178")
				(number "178")
			)
			(pin bidirectional line
				(at 54.61 11.43 180)
				(length 7.62)
				(name "IO1P176")
				(number "176")
			)
			(pin bidirectional line
				(at 54.61 8.89 180)
				(length 7.62)
				(name "IO1P175")
				(number "175")
			)
			(pin bidirectional line
				(at 54.61 6.35 180)
				(length 7.62)
				(name "IO1P174")
				(number "174")
			)
			(pin bidirectional line
				(at 54.61 3.81 180)
				(length 7.62)
				(name "IO1P173")
				(number "173")
			)
			(pin bidirectional line
				(at 54.61 1.27 180)
				(length 7.62)
				(name "IO1P169")
				(number "169")
			)
			(pin bidirectional line
				(at 54.61 -1.27 180)
				(length 7.62)
				(name "IO1VRP168")
				(number "168")
			)
			(pin bidirectional line
				(at 54.61 -3.81 180)
				(length 7.62)
				(name "IO1P167")
				(number "167")
			)
			(pin bidirectional line
				(at 54.61 -6.35 180)
				(length 7.62)
				(name "IO1P166")
				(number "166")
			)
			(pin bidirectional line
				(at 54.61 -8.89 180)
				(length 7.62)
				(name "IO1P165")
				(number "165")
			)
			(pin bidirectional line
				(at 54.61 -11.43 180)
				(length 7.62)
				(name "IO1VRP164")
				(number "164")
			)
			(pin bidirectional line
				(at 54.61 -13.97 180)
				(length 7.62)
				(name "IO1P163")
				(number "163")
			)
			(pin bidirectional line
				(at 54.61 -16.51 180)
				(length 7.62)
				(name "IO1VRP162")
				(number "162")
			)
			(pin bidirectional line
				(at 54.61 -21.59 180)
				(length 7.62)
				(name "IO2VRP152")
				(number "152")
			)
			(pin bidirectional line
				(at 54.61 -24.13 180)
				(length 7.62)
				(name "IO2P151")
				(number "151")
			)
			(pin bidirectional line
				(at 54.61 -26.67 180)
				(length 7.62)
				(name "IO2VRP150")
				(number "150")
			)
			(pin bidirectional line
				(at 54.61 -29.21 180)
				(length 7.62)
				(name "IO2P149")
				(number "149")
			)
			(pin bidirectional line
				(at 54.61 -31.75 180)
				(length 7.62)
				(name "IO2P148")
				(number "148")
			)
			(pin bidirectional line
				(at 54.61 -34.29 180)
				(length 7.62)
				(name "IO2P147")
				(number "147")
			)
			(pin bidirectional line
				(at 54.61 -36.83 180)
				(length 7.62)
				(name "IO2VRP146")
				(number "146")
			)
			(pin bidirectional line
				(at 54.61 -39.37 180)
				(length 7.62)
				(name "IO2/D1P145")
				(number "145")
			)
			(pin bidirectional line
				(at 54.61 -41.91 180)
				(length 7.62)
				(name "IO2/D2P141")
				(number "141")
			)
			(pin bidirectional line
				(at 54.61 -44.45 180)
				(length 7.62)
				(name "IO2P140")
				(number "140")
			)
			(pin bidirectional line
				(at 54.61 -46.99 180)
				(length 7.62)
				(name "IO2P139")
				(number "139")
			)
			(pin bidirectional line
				(at 54.61 -49.53 180)
				(length 7.62)
				(name "IO2P138")
				(number "138")
			)
			(pin bidirectional line
				(at 54.61 -52.07 180)
				(length 7.62)
				(name "IO2VRP136")
				(number "136")
			)
			(pin bidirectional line
				(at 54.61 -54.61 180)
				(length 7.62)
				(name "IO2/D3P135")
				(number "135")
			)
			(pin bidirectional line
				(at 54.61 -57.15 180)
				(length 7.62)
				(name "IO2P134")
				(number "134")
			)
			(pin bidirectional line
				(at 54.61 -59.69 180)
				(length 7.62)
				(name "IO2P133")
				(number "133")
			)
			(pin bidirectional line
				(at 54.61 -64.77 180)
				(length 7.62)
				(name "IO3P127")
				(number "127")
			)
			(pin bidirectional line
				(at 54.61 -67.31 180)
				(length 7.62)
				(name "IO3/D4P126")
				(number "126")
			)
			(pin bidirectional line
				(at 54.61 -69.85 180)
				(length 7.62)
				(name "IO3VRP125")
				(number "125")
			)
			(pin bidirectional line
				(at 54.61 -72.39 180)
				(length 7.62)
				(name "IO3P123")
				(number "123")
			)
			(pin bidirectional line
				(at 54.61 -74.93 180)
				(length 7.62)
				(name "IO3P122")
				(number "122")
			)
			(pin bidirectional line
				(at 54.61 -77.47 180)
				(length 7.62)
				(name "IO3P121")
				(number "121")
			)
			(pin bidirectional line
				(at 54.61 -80.01 180)
				(length 7.62)
				(name "IO3/D5P120")
				(number "120")
			)
			(pin bidirectional line
				(at 54.61 -82.55 180)
				(length 7.62)
				(name "IO3/D6P116")
				(number "116")
			)
			(pin bidirectional line
				(at 54.61 -85.09 180)
				(length 7.62)
				(name "IO3VRP115")
				(number "115")
			)
			(pin bidirectional line
				(at 54.61 -87.63 180)
				(length 7.62)
				(name "IO3P114")
				(number "114")
			)
			(pin bidirectional line
				(at 54.61 -90.17 180)
				(length 7.62)
				(name "IO3P113")
				(number "113")
			)
			(pin bidirectional line
				(at 54.61 -92.71 180)
				(length 7.62)
				(name "IO3P112")
				(number "112")
			)
			(pin bidirectional line
				(at 54.61 -95.25 180)
				(length 7.62)
				(name "IO3VRP111")
				(number "111")
			)
			(pin bidirectional line
				(at 54.61 -97.79 180)
				(length 7.62)
				(name "IO3P110")
				(number "110")
			)
			(pin bidirectional line
				(at 54.61 -100.33 180)
				(length 7.62)
				(name "IO3VRP109")
				(number "109")
			)
			(pin bidirectional line
				(at 54.61 -102.87 180)
				(length 7.62)
				(name "IO3/D7P108")
				(number "108")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC2S400FT256"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "XC2S400FT256"
			(at 0 7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC2S400FT256_0_1")
		(symbol "XC2S400FT256_1_1"
			(pin bidirectional line
				(at -54.61 132.08 0)
				(length 7.62)
				(name "TMS")
				(number "B1")
			)
			(pin bidirectional line
				(at -54.61 129.54 0)
				(length 7.62)
				(name "TDO")
				(number "B14")
			)
			(pin bidirectional line
				(at -54.61 127 0)
				(length 7.62)
				(name "TDI")
				(number "C13")
			)
			(pin bidirectional line
				(at -54.61 124.46 0)
				(length 7.62)
				(name "TCK")
				(number "A2")
			)
			(pin bidirectional line
				(at -54.61 119.38 0)
				(length 7.62)
				(name "DONE")
				(number "T15")
			)
			(pin input line
				(at -54.61 116.84 0)
				(length 7.62)
				(name "/PROG")
				(number "R16")
			)
			(pin bidirectional line
				(at -54.61 114.3 0)
				(length 7.62)
				(name "/INIT")
				(number "P15")
			)
			(pin bidirectional clock
				(at -54.61 111.76 0)
				(length 7.62)
				(name "CCLK")
				(number "A15")
			)
			(pin input line
				(at -54.61 106.68 0)
				(length 7.62)
				(name "M0")
				(number "T2")
			)
			(pin input line
				(at -54.61 104.14 0)
				(length 7.62)
				(name "M1")
				(number "R1")
			)
			(pin input line
				(at -54.61 101.6 0)
				(length 7.62)
				(name "M2")
				(number "R3")
			)
			(pin bidirectional line
				(at -54.61 93.98 0)
				(length 7.62)
				(name "IO7D3")
				(number "D3")
			)
			(pin bidirectional line
				(at -54.61 91.44 0)
				(length 7.62)
				(name "IO7C2")
				(number "C2")
			)
			(pin bidirectional line
				(at -54.61 88.9 0)
				(length 7.62)
				(name "IO7VRC1")
				(number "C1")
			)
			(pin bidirectional line
				(at -54.61 86.36 0)
				(length 7.62)
				(name "IO7D2")
				(number "D2")
			)
			(pin bidirectional line
				(at -54.61 83.82 0)
				(length 7.62)
				(name "IO7D1")
				(number "D1")
			)
			(pin bidirectional line
				(at -54.61 81.28 0)
				(length 7.62)
				(name "IO7VRE3")
				(number "E3")
			)
			(pin bidirectional line
				(at -54.61 78.74 0)
				(length 7.62)
				(name "IO7E4")
				(number "E4")
			)
			(pin bidirectional line
				(at -54.61 76.2 0)
				(length 7.62)
				(name "IO7E2")
				(number "E2")
			)
			(pin bidirectional line
				(at -54.61 73.66 0)
				(length 7.62)
				(name "IO7E1")
				(number "E1")
			)
			(pin bidirectional line
				(at -54.61 71.12 0)
				(length 7.62)
				(name "IO7VRF4")
				(number "F4")
			)
			(pin bidirectional line
				(at -54.61 68.58 0)
				(length 7.62)
				(name "IO7F3")
				(number "F3")
			)
			(pin bidirectional line
				(at -54.61 66.04 0)
				(length 7.62)
				(name "IO7F2")
				(number "F2")
			)
			(pin bidirectional line
				(at -54.61 63.5 0)
				(length 7.62)
				(name "IO7F1")
				(number "F1")
			)
			(pin bidirectional line
				(at -54.61 60.96 0)
				(length 7.62)
				(name "IO7F5")
				(number "F5")
			)
			(pin bidirectional line
				(at -54.61 58.42 0)
				(length 7.62)
				(name "IO7G5")
				(number "G5")
			)
			(pin bidirectional line
				(at -54.61 55.88 0)
				(length 7.62)
				(name "IO7G3")
				(number "G3")
			)
			(pin bidirectional line
				(at -54.61 53.34 0)
				(length 7.62)
				(name "IO7G4")
				(number "G4")
			)
			(pin bidirectional line
				(at -54.61 50.8 0)
				(length 7.62)
				(name "IO7VRG2")
				(number "G2")
			)
			(pin bidirectional line
				(at -54.61 48.26 0)
				(length 7.62)
				(name "IO7G1")
				(number "G1")
			)
			(pin bidirectional line
				(at -54.61 45.72 0)
				(length 7.62)
				(name "IO7H4")
				(number "H4")
			)
			(pin bidirectional line
				(at -54.61 43.18 0)
				(length 7.62)
				(name "IO7VRH3")
				(number "H3")
			)
			(pin bidirectional line
				(at -54.61 40.64 0)
				(length 7.62)
				(name "IO7H2")
				(number "H2")
			)
			(pin bidirectional line
				(at -54.61 35.56 0)
				(length 7.62)
				(name "IO6VRJ2")
				(number "J2")
			)
			(pin bidirectional line
				(at -54.61 33.02 0)
				(length 7.62)
				(name "IO6J3")
				(number "J3")
			)
			(pin bidirectional line
				(at -54.61 30.48 0)
				(length 7.62)
				(name "IO6J1")
				(number "J1")
			)
			(pin bidirectional line
				(at -54.61 27.94 0)
				(length 7.62)
				(name "IO6VRK1")
				(number "K1")
			)
			(pin bidirectional line
				(at -54.61 25.4 0)
				(length 7.62)
				(name "IO6K2")
				(number "K2")
			)
			(pin bidirectional line
				(at -54.61 22.86 0)
				(length 7.62)
				(name "IO6K3")
				(number "K3")
			)
			(pin bidirectional line
				(at -54.61 20.32 0)
				(length 7.62)
				(name "IO6L1")
				(number "L1")
			)
			(pin bidirectional line
				(at -54.61 17.78 0)
				(length 7.62)
				(name "IO6L2")
				(number "L2")
			)
			(pin bidirectional line
				(at -54.61 15.24 0)
				(length 7.62)
				(name "IO6K4")
				(number "K4")
			)
			(pin bidirectional line
				(at -54.61 12.7 0)
				(length 7.62)
				(name "IO6K5")
				(number "K5")
			)
			(pin bidirectional line
				(at -54.61 10.16 0)
				(length 7.62)
				(name "IO6L3")
				(number "L3")
			)
			(pin bidirectional line
				(at -54.61 7.62 0)
				(length 7.62)
				(name "IO6VRM2")
				(number "M2")
			)
			(pin bidirectional line
				(at -54.61 5.08 0)
				(length 7.62)
				(name "IO6M1")
				(number "M1")
			)
			(pin bidirectional line
				(at -54.61 2.54 0)
				(length 7.62)
				(name "IO6N1")
				(number "N1")
			)
			(pin bidirectional line
				(at -54.61 0 0)
				(length 7.62)
				(name "IO6L4")
				(number "L4")
			)
			(pin bidirectional line
				(at -54.61 -2.54 0)
				(length 7.62)
				(name "IO6VRL5")
				(number "L5")
			)
			(pin bidirectional line
				(at -54.61 -5.08 0)
				(length 7.62)
				(name "IO6M3")
				(number "M3")
			)
			(pin bidirectional line
				(at -54.61 -7.62 0)
				(length 7.62)
				(name "IO6M4")
				(number "M4")
			)
			(pin bidirectional line
				(at -54.61 -10.16 0)
				(length 7.62)
				(name "IO6N2")
				(number "N2")
			)
			(pin bidirectional line
				(at -54.61 -12.7 0)
				(length 7.62)
				(name "IO6VRN3")
				(number "N3")
			)
			(pin bidirectional line
				(at -54.61 -15.24 0)
				(length 7.62)
				(name "IO6P1")
				(number "P1")
			)
			(pin bidirectional line
				(at -54.61 -17.78 0)
				(length 7.62)
				(name "IO6P2")
				(number "P2")
			)
			(pin bidirectional line
				(at -54.61 -22.86 0)
				(length 7.62)
				(name "IO5P4")
				(number "P4")
			)
			(pin bidirectional line
				(at -54.61 -25.4 0)
				(length 7.62)
				(name "IO5R4")
				(number "R4")
			)
			(pin bidirectional line
				(at -54.61 -27.94 0)
				(length 7.62)
				(name "IO5VRT3")
				(number "T3")
			)
			(pin bidirectional line
				(at -54.61 -30.48 0)
				(length 7.62)
				(name "IO5T4")
				(number "T4")
			)
			(pin bidirectional line
				(at -54.61 -33.02 0)
				(length 7.62)
				(name "IO5N5")
				(number "N5")
			)
			(pin bidirectional line
				(at -54.61 -35.56 0)
				(length 7.62)
				(name "IO5P5")
				(number "P5")
			)
			(pin bidirectional line
				(at -54.61 -38.1 0)
				(length 7.62)
				(name "IO5VRR5")
				(number "R5")
			)
			(pin bidirectional line
				(at -54.61 -40.64 0)
				(length 7.62)
				(name "IO5T5")
				(number "T5")
			)
			(pin bidirectional line
				(at -54.61 -43.18 0)
				(length 7.62)
				(name "IO5N6")
				(number "N6")
			)
			(pin bidirectional line
				(at -54.61 -45.72 0)
				(length 7.62)
				(name "IO5P6")
				(number "P6")
			)
			(pin bidirectional line
				(at -54.61 -48.26 0)
				(length 7.62)
				(name "IO5VRR6")
				(number "R6")
			)
			(pin bidirectional line
				(at -54.61 -50.8 0)
				(length 7.62)
				(name "IO5T6")
				(number "T6")
			)
			(pin bidirectional line
				(at -54.61 -53.34 0)
				(length 7.62)
				(name "IO5M6")
				(number "M6")
			)
			(pin bidirectional line
				(at -54.61 -55.88 0)
				(length 7.62)
				(name "IO5N7")
				(number "N7")
			)
			(pin bidirectional line
				(at -54.61 -58.42 0)
				(length 7.62)
				(name "IO5P7")
				(number "P7")
			)
			(pin bidirectional line
				(at -54.61 -60.96 0)
				(length 7.62)
				(name "IO5R7")
				(number "R7")
			)
			(pin bidirectional line
				(at -54.61 -63.5 0)
				(length 7.62)
				(name "IO5T7")
				(number "T7")
			)
			(pin bidirectional line
				(at -54.61 -66.04 0)
				(length 7.62)
				(name "IO5VRM7")
				(number "M7")
			)
			(pin bidirectional line
				(at -54.61 -68.58 0)
				(length 7.62)
				(name "IO5N8")
				(number "N8")
			)
			(pin bidirectional line
				(at -54.61 -71.12 0)
				(length 7.62)
				(name "IO5VRP8")
				(number "P8")
			)
			(pin bidirectional line
				(at -54.61 -73.66 0)
				(length 7.62)
				(name "IO5DLLR8")
				(number "R8")
			)
			(pin input clock
				(at -54.61 -76.2 0)
				(length 7.62)
				(name "GCK1")
				(number "T8")
			)
			(pin input clock
				(at -54.61 -81.28 0)
				(length 7.62)
				(name "GCK0")
				(number "T9")
			)
			(pin bidirectional line
				(at -54.61 -83.82 0)
				(length 7.62)
				(name "IO4DLLR9")
				(number "R9")
			)
			(pin bidirectional line
				(at -54.61 -86.36 0)
				(length 7.62)
				(name "IO4VRP9")
				(number "P9")
			)
			(pin bidirectional line
				(at -54.61 -88.9 0)
				(length 7.62)
				(name "IO4N9")
				(number "N9")
			)
			(pin bidirectional line
				(at -54.61 -91.44 0)
				(length 7.62)
				(name "IO4T10")
				(number "T10")
			)
			(pin bidirectional line
				(at -54.61 -93.98 0)
				(length 7.62)
				(name "IO4VRR10")
				(number "R10")
			)
			(pin bidirectional line
				(at -54.61 -96.52 0)
				(length 7.62)
				(name "IO4P10")
				(number "P10")
			)
			(pin bidirectional line
				(at -54.61 -99.06 0)
				(length 7.62)
				(name "IO4R11")
				(number "R11")
			)
			(pin bidirectional line
				(at -54.61 -101.6 0)
				(length 7.62)
				(name "IO4T11")
				(number "T11")
			)
			(pin bidirectional line
				(at -54.61 -104.14 0)
				(length 7.62)
				(name "IO4N10")
				(number "N10")
			)
			(pin bidirectional line
				(at -54.61 -106.68 0)
				(length 7.62)
				(name "IO4M10")
				(number "M10")
			)
			(pin bidirectional line
				(at -54.61 -109.22 0)
				(length 7.62)
				(name "IO4P11")
				(number "P11")
			)
			(pin bidirectional line
				(at -54.61 -111.76 0)
				(length 7.62)
				(name "IO4VRR12")
				(number "R12")
			)
			(pin bidirectional line
				(at -54.61 -114.3 0)
				(length 7.62)
				(name "IO4T12")
				(number "T12")
			)
			(pin bidirectional line
				(at -54.61 -116.84 0)
				(length 7.62)
				(name "IO4T13")
				(number "T13")
			)
			(pin bidirectional line
				(at -54.61 -119.38 0)
				(length 7.62)
				(name "IO4N11")
				(number "N11")
			)
			(pin bidirectional line
				(at -54.61 -121.92 0)
				(length 7.62)
				(name "IO4VRM11")
				(number "M11")
			)
			(pin bidirectional line
				(at -54.61 -124.46 0)
				(length 7.62)
				(name "IO4P12")
				(number "P12")
			)
			(pin bidirectional line
				(at -54.61 -127 0)
				(length 7.62)
				(name "IO4N12")
				(number "N12")
			)
			(pin bidirectional line
				(at -54.61 -129.54 0)
				(length 7.62)
				(name "IO4VRR13")
				(number "R13")
			)
			(pin bidirectional line
				(at -54.61 -132.08 0)
				(length 7.62)
				(name "IO4P13")
				(number "P13")
			)
			(pin bidirectional line
				(at -54.61 -134.62 0)
				(length 7.62)
				(name "IO4T14")
				(number "T14")
			)
			(pin bidirectional line
				(at -54.61 -137.16 0)
				(length 7.62)
				(name "IO4R14")
				(number "R14")
			)
			(pin power_in line
				(at -44.45 156.21 270)
				(length 7.62)
				(name "VCCO0")
				(number "E8")
			)
			(pin power_in line
				(at -41.91 156.21 270)
				(length 7.62)
				(name "VCCO0")
				(number "F7")
			)
			(pin power_in line
				(at -39.37 156.21 270)
				(length 7.62)
				(name "VCCO0")
				(number "F8")
			)
			(pin power_in line
				(at -36.83 156.21 270)
				(length 7.62)
				(name "VCCO1")
				(number "E9")
			)
			(pin power_in line
				(at -34.29 156.21 270)
				(length 7.62)
				(name "VCCO1")
				(number "F9")
			)
			(pin power_in line
				(at -34.29 -156.21 90)
				(length 7.62)
				(name "GND")
				(number "A1")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "A16")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "B15")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "B2")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "F11")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "F6")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "G10")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "G7")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "G8")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "G9")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "H10")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "H7")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "H8")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "H9")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "J10")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "J7")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "J8")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "J9")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "K10")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "K7")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "K8")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "K9")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "L11")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "L6")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "R15")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "R2")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "T1")
			)
			(pin passive line
				(at -34.29 -156.21 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at -31.75 156.21 270)
				(length 7.62)
				(name "VCCO1")
				(number "F10")
			)
			(pin power_in line
				(at -29.21 156.21 270)
				(length 7.62)
				(name "VCCO2")
				(number "G11")
			)
			(pin power_in line
				(at -26.67 156.21 270)
				(length 7.62)
				(name "VCCO2")
				(number "H11")
			)
			(pin power_in line
				(at -24.13 156.21 270)
				(length 7.62)
				(name "VCCO2")
				(number "H12")
			)
			(pin power_in line
				(at -21.59 156.21 270)
				(length 7.62)
				(name "VCCO3")
				(number "J11")
			)
			(pin power_in line
				(at -19.05 156.21 270)
				(length 7.62)
				(name "VCCO3")
				(number "J12")
			)
			(pin power_in line
				(at -16.51 156.21 270)
				(length 7.62)
				(name "VCCO3")
				(number "K11")
			)
			(pin passive line
				(at -13.97 156.21 270)
				(length 7.62)
				(name "VCCO4")
				(number "L9")
			)
			(pin power_in line
				(at -11.43 156.21 270)
				(length 7.62)
				(name "VCCO4")
				(number "L10")
			)
			(pin power_in line
				(at -8.89 156.21 270)
				(length 7.62)
				(name "VCCO4")
				(number "M9")
			)
			(pin power_in line
				(at -6.35 156.21 270)
				(length 7.62)
				(name "VCCO5")
				(number "L7")
			)
			(pin power_in line
				(at -3.81 156.21 270)
				(length 7.62)
				(name "VCCO5")
				(number "L8")
			)
			(pin power_in line
				(at -1.27 156.21 270)
				(length 7.62)
				(name "VCCO5")
				(number "M8")
			)
			(pin power_in line
				(at 1.27 156.21 270)
				(length 7.62)
				(name "VCCO6")
				(number "J5")
			)
			(pin power_in line
				(at 3.81 156.21 270)
				(length 7.62)
				(name "VCCO6")
				(number "J6")
			)
			(pin power_in line
				(at 6.35 156.21 270)
				(length 7.62)
				(name "VCCO6")
				(number "K6")
			)
			(pin power_in line
				(at 8.89 156.21 270)
				(length 7.62)
				(name "VCCO7")
				(number "G6")
			)
			(pin power_in line
				(at 11.43 156.21 270)
				(length 7.62)
				(name "VCCO7")
				(number "H5")
			)
			(pin power_in line
				(at 13.97 156.21 270)
				(length 7.62)
				(name "VCCO7")
				(number "H6")
			)
			(pin power_in line
				(at 16.51 156.21 270)
				(length 7.62)
				(name "VCCINT")
				(number "C3")
			)
			(pin power_in line
				(at 19.05 156.21 270)
				(length 7.62)
				(name "VCCINT")
				(number "C14")
			)
			(pin power_in line
				(at 21.59 156.21 270)
				(length 7.62)
				(name "VCCINT")
				(number "D4")
			)
			(pin power_in line
				(at 24.13 156.21 270)
				(length 7.62)
				(name "VCCINT")
				(number "D13")
			)
			(pin power_in line
				(at 26.67 156.21 270)
				(length 7.62)
				(name "VCCINT")
				(number "E5")
			)
			(pin power_in line
				(at 29.21 156.21 270)
				(length 7.62)
				(name "VCCINT")
				(number "E12")
			)
			(pin power_in line
				(at 31.75 156.21 270)
				(length 7.62)
				(name "VCCINT")
				(number "M5")
			)
			(pin power_in line
				(at 34.29 156.21 270)
				(length 7.62)
				(name "VCCINT")
				(number "M12")
			)
			(pin power_in line
				(at 36.83 156.21 270)
				(length 7.62)
				(name "VCCINT")
				(number "N4")
			)
			(pin power_in line
				(at 39.37 156.21 270)
				(length 7.62)
				(name "VCCINT")
				(number "N13")
			)
			(pin power_in line
				(at 41.91 156.21 270)
				(length 7.62)
				(name "VCCINT")
				(number "P3")
			)
			(pin power_in line
				(at 44.45 156.21 270)
				(length 7.62)
				(name "VCCINT")
				(number "P14")
			)
			(pin bidirectional line
				(at 54.61 127 180)
				(length 7.62)
				(name "IRDY2")
				(number "H16")
			)
			(pin bidirectional line
				(at 54.61 124.46 180)
				(length 7.62)
				(name "TRDY3")
				(number "J13")
			)
			(pin bidirectional line
				(at 54.61 121.92 180)
				(length 7.62)
				(name "TRDY6")
				(number "J4")
			)
			(pin bidirectional line
				(at 54.61 119.38 180)
				(length 7.62)
				(name "IRDY7")
				(number "H1")
			)
			(pin bidirectional line
				(at 54.61 111.76 180)
				(length 7.62)
				(name "/WR")
				(number "A13")
			)
			(pin bidirectional line
				(at 54.61 109.22 180)
				(length 7.62)
				(name "/CS")
				(number "A14")
			)
			(pin bidirectional line
				(at 54.61 101.6 180)
				(length 7.62)
				(name "BUSY/DOUT")
				(number "C15")
			)
			(pin bidirectional line
				(at 54.61 99.06 180)
				(length 7.62)
				(name "D0/DIN")
				(number "B16")
			)
			(pin bidirectional line
				(at 54.61 86.36 180)
				(length 7.62)
				(name "IO0B3")
				(number "B3")
			)
			(pin bidirectional line
				(at 54.61 83.82 180)
				(length 7.62)
				(name "IO0VRA3")
				(number "A3")
			)
			(pin bidirectional line
				(at 54.61 81.28 180)
				(length 7.62)
				(name "IO0A4")
				(number "A4")
			)
			(pin bidirectional line
				(at 54.61 78.74 180)
				(length 7.62)
				(name "IO0C4")
				(number "C4")
			)
			(pin bidirectional line
				(at 54.61 76.2 180)
				(length 7.62)
				(name "IO0B4")
				(number "B4")
			)
			(pin bidirectional line
				(at 54.61 73.66 180)
				(length 7.62)
				(name "IO0VRC5")
				(number "C5")
			)
			(pin bidirectional line
				(at 54.61 71.12 180)
				(length 7.62)
				(name "IO0D5")
				(number "D5")
			)
			(pin bidirectional line
				(at 54.61 68.58 180)
				(length 7.62)
				(name "IO0E6")
				(number "E6")
			)
			(pin bidirectional line
				(at 54.61 66.04 180)
				(length 7.62)
				(name "IO0D6")
				(number "D6")
			)
			(pin bidirectional line
				(at 54.61 63.5 180)
				(length 7.62)
				(name "IO0VRB5")
				(number "B5")
			)
			(pin bidirectional line
				(at 54.61 60.96 180)
				(length 7.62)
				(name "IO0A5")
				(number "A5")
			)
			(pin bidirectional line
				(at 54.61 58.42 180)
				(length 7.62)
				(name "IO0C6")
				(number "C6")
			)
			(pin bidirectional line
				(at 54.61 55.88 180)
				(length 7.62)
				(name "IO0B6")
				(number "B6")
			)
			(pin bidirectional line
				(at 54.61 53.34 180)
				(length 7.62)
				(name "IO0A6")
				(number "A6")
			)
			(pin bidirectional line
				(at 54.61 50.8 180)
				(length 7.62)
				(name "IO0B7")
				(number "B7")
			)
			(pin bidirectional line
				(at 54.61 48.26 180)
				(length 7.62)
				(name "IO0C7")
				(number "C7")
			)
			(pin bidirectional line
				(at 54.61 45.72 180)
				(length 7.62)
				(name "IO0VRD7")
				(number "D7")
			)
			(pin bidirectional line
				(at 54.61 43.18 180)
				(length 7.62)
				(name "IO0E7")
				(number "E7")
			)
			(pin bidirectional line
				(at 54.61 40.64 180)
				(length 7.62)
				(name "IO0VRA7")
				(number "A7")
			)
			(pin bidirectional line
				(at 54.61 38.1 180)
				(length 7.62)
				(name "IO0DLLD8")
				(number "D8")
			)
			(pin input clock
				(at 54.61 35.56 180)
				(length 7.62)
				(name "GCK3")
				(number "C8")
			)
			(pin input clock
				(at 54.61 27.94 180)
				(length 7.62)
				(name "GCK2")
				(number "B8")
			)
			(pin bidirectional line
				(at 54.61 25.4 180)
				(length 7.62)
				(name "IO1DLLA8")
				(number "A8")
			)
			(pin bidirectional line
				(at 54.61 22.86 180)
				(length 7.62)
				(name "IO1VRA9")
				(number "A9")
			)
			(pin bidirectional line
				(at 54.61 20.32 180)
				(length 7.62)
				(name "IO1B9")
				(number "B9")
			)
			(pin bidirectional line
				(at 54.61 17.78 180)
				(length 7.62)
				(name "IO1C9")
				(number "C9")
			)
			(pin bidirectional line
				(at 54.61 15.24 180)
				(length 7.62)
				(name "IO1VRD9")
				(number "D9")
			)
			(pin bidirectional line
				(at 54.61 12.7 180)
				(length 7.62)
				(name "IO1A10")
				(number "A10")
			)
			(pin bidirectional line
				(at 54.61 10.16 180)
				(length 7.62)
				(name "IO1B10")
				(number "B10")
			)
			(pin bidirectional line
				(at 54.61 7.62 180)
				(length 7.62)
				(name "IO1C10")
				(number "C10")
			)
			(pin bidirectional line
				(at 54.61 5.08 180)
				(length 7.62)
				(name "IO1D10")
				(number "D10")
			)
			(pin bidirectional line
				(at 54.61 2.54 180)
				(length 7.62)
				(name "IO1E10")
				(number "E10")
			)
			(pin bidirectional line
				(at 54.61 0 180)
				(length 7.62)
				(name "IO1A11")
				(number "A11")
			)
			(pin bidirectional line
				(at 54.61 -2.54 180)
				(length 7.62)
				(name "IO1VRB11")
				(number "B11")
			)
			(pin bidirectional line
				(at 54.61 -5.08 180)
				(length 7.62)
				(name "IO1C11")
				(number "C11")
			)
			(pin bidirectional line
				(at 54.61 -7.62 180)
				(length 7.62)
				(name "IO1D11")
				(number "D11")
			)
			(pin bidirectional line
				(at 54.61 -10.16 180)
				(length 7.62)
				(name "IO1E11")
				(number "E11")
			)
			(pin bidirectional line
				(at 54.61 -12.7 180)
				(length 7.62)
				(name "IO1VRD12")
				(number "D12")
			)
			(pin bidirectional line
				(at 54.61 -15.24 180)
				(length 7.62)
				(name "IO1A12")
				(number "A12")
			)
			(pin bidirectional line
				(at 54.61 -17.78 180)
				(length 7.62)
				(name "IO1B12")
				(number "B12")
			)
			(pin bidirectional line
				(at 54.61 -20.32 180)
				(length 7.62)
				(name "IO1C12")
				(number "C12")
			)
			(pin bidirectional line
				(at 54.61 -22.86 180)
				(length 7.62)
				(name "IO1VRB13")
				(number "B13")
			)
			(pin bidirectional line
				(at 54.61 -27.94 180)
				(length 7.62)
				(name "IO2VRD14")
				(number "D14")
			)
			(pin bidirectional line
				(at 54.61 -30.48 180)
				(length 7.62)
				(name "IO2E13")
				(number "E13")
			)
			(pin bidirectional line
				(at 54.61 -33.02 180)
				(length 7.62)
				(name "IO2F12")
				(number "F12")
			)
			(pin bidirectional line
				(at 54.61 -35.56 180)
				(length 7.62)
				(name "IO2G12")
				(number "G12")
			)
			(pin bidirectional line
				(at 54.61 -38.1 180)
				(length 7.62)
				(name "IO2VRC16")
				(number "C16")
			)
			(pin bidirectional line
				(at 54.61 -40.64 180)
				(length 7.62)
				(name "IO2D15")
				(number "D15")
			)
			(pin bidirectional line
				(at 54.61 -43.18 180)
				(length 7.62)
				(name "IO2E14")
				(number "E14")
			)
			(pin bidirectional line
				(at 54.61 -45.72 180)
				(length 7.62)
				(name "IO2F13")
				(number "F13")
			)
			(pin bidirectional line
				(at 54.61 -48.26 180)
				(length 7.62)
				(name "IO2VRD16")
				(number "D16")
			)
			(pin bidirectional line
				(at 54.61 -50.8 180)
				(length 7.62)
				(name "IO2D1E15")
				(number "E15")
			)
			(pin bidirectional line
				(at 54.61 -53.34 180)
				(length 7.62)
				(name "IO2D2F14")
				(number "F14")
			)
			(pin bidirectional line
				(at 54.61 -55.88 180)
				(length 7.62)
				(name "IO2G13")
				(number "G13")
			)
			(pin bidirectional line
				(at 54.61 -58.42 180)
				(length 7.62)
				(name "IO2E16")
				(number "E16")
			)
			(pin bidirectional line
				(at 54.61 -60.96 180)
				(length 7.62)
				(name "IO2F15")
				(number "F15")
			)
			(pin bidirectional line
				(at 54.61 -63.5 180)
				(length 7.62)
				(name "IO2G14")
				(number "G14")
			)
			(pin bidirectional line
				(at 54.61 -66.04 180)
				(length 7.62)
				(name "IO2H13")
				(number "H13")
			)
			(pin bidirectional line
				(at 54.61 -68.58 180)
				(length 7.62)
				(name "IO2VRF16")
				(number "F16")
			)
			(pin bidirectional line
				(at 54.61 -71.12 180)
				(length 7.62)
				(name "IO2D3G15")
				(number "G15")
			)
			(pin bidirectional line
				(at 54.61 -73.66 180)
				(length 7.62)
				(name "IO2H15")
				(number "H15")
			)
			(pin bidirectional line
				(at 54.61 -76.2 180)
				(length 7.62)
				(name "IO2VRH14")
				(number "H14")
			)
			(pin bidirectional line
				(at 54.61 -78.74 180)
				(length 7.62)
				(name "IO2G16")
				(number "G16")
			)
			(pin bidirectional line
				(at 54.61 -86.36 180)
				(length 7.62)
				(name "IO3VRJ16")
				(number "J16")
			)
			(pin bidirectional line
				(at 54.61 -88.9 180)
				(length 7.62)
				(name "IO3J15")
				(number "J15")
			)
			(pin bidirectional line
				(at 54.61 -91.44 180)
				(length 7.62)
				(name "IO3D4J14")
				(number "J14")
			)
			(pin bidirectional line
				(at 54.61 -93.98 180)
				(length 7.62)
				(name "IO3VRK13")
				(number "K13")
			)
			(pin bidirectional line
				(at 54.61 -96.52 180)
				(length 7.62)
				(name "IO3K12")
				(number "K12")
			)
			(pin bidirectional line
				(at 54.61 -99.06 180)
				(length 7.62)
				(name "IO3L12")
				(number "L12")
			)
			(pin bidirectional line
				(at 54.61 -101.6 180)
				(length 7.62)
				(name "IO3K16")
				(number "K16")
			)
			(pin bidirectional line
				(at 54.61 -104.14 180)
				(length 7.62)
				(name "IO3K15")
				(number "K15")
			)
			(pin bidirectional line
				(at 54.61 -106.68 180)
				(length 7.62)
				(name "IO3K14")
				(number "K14")
			)
			(pin bidirectional line
				(at 54.61 -109.22 180)
				(length 7.62)
				(name "IO3D5L13")
				(number "L13")
			)
			(pin bidirectional line
				(at 54.61 -111.76 180)
				(length 7.62)
				(name "IO3D6L16")
				(number "L16")
			)
			(pin bidirectional line
				(at 54.61 -114.3 180)
				(length 7.62)
				(name "IO3VRL15")
				(number "L15")
			)
			(pin bidirectional line
				(at 54.61 -116.84 180)
				(length 7.62)
				(name "IO3L14")
				(number "L14")
			)
			(pin bidirectional line
				(at 54.61 -119.38 180)
				(length 7.62)
				(name "IO3M13")
				(number "M13")
			)
			(pin bidirectional line
				(at 54.61 -121.92 180)
				(length 7.62)
				(name "IO3M16")
				(number "M16")
			)
			(pin bidirectional line
				(at 54.61 -124.46 180)
				(length 7.62)
				(name "IO3VRM15")
				(number "M15")
			)
			(pin bidirectional line
				(at 54.61 -127 180)
				(length 7.62)
				(name "IO3M14")
				(number "M14")
			)
			(pin bidirectional line
				(at 54.61 -129.54 180)
				(length 7.62)
				(name "IO3N14")
				(number "N14")
			)
			(pin bidirectional line
				(at 54.61 -132.08 180)
				(length 7.62)
				(name "IO3VRN16")
				(number "N16")
			)
			(pin bidirectional line
				(at 54.61 -134.62 180)
				(length 7.62)
				(name "IO3N15")
				(number "N15")
			)
			(pin bidirectional line
				(at 54.61 -137.16 180)
				(length 7.62)
				(name "IO3D7P16")
				(number "P16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC2S50-PQ208"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 40.64 111.76 0)
		)
		(property "Value" "XC2S50-PQ208"
			(at 31.75 -113.03 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC2S50-PQ208_0_1")
		(symbol "XC2S50-PQ208_1_1"
			(pin bidirectional line
				(at -54.61 106.68 0)
				(length 7.62)
				(name "TMS")
				(number "2")
			)
			(pin bidirectional line
				(at -54.61 104.14 0)
				(length 7.62)
				(name "TDO")
				(number "157")
			)
			(pin bidirectional line
				(at -54.61 101.6 0)
				(length 7.62)
				(name "TDI")
				(number "159")
			)
			(pin bidirectional line
				(at -54.61 99.06 0)
				(length 7.62)
				(name "TCK")
				(number "207")
			)
			(pin bidirectional line
				(at -54.61 93.98 0)
				(length 7.62)
				(name "DONE")
				(number "104")
			)
			(pin input line
				(at -54.61 91.44 0)
				(length 7.62)
				(name "/PROG")
				(number "106")
			)
			(pin bidirectional line
				(at -54.61 88.9 0)
				(length 7.62)
				(name "/INIT")
				(number "107")
			)
			(pin bidirectional clock
				(at -54.61 86.36 0)
				(length 7.62)
				(name "CCLK")
				(number "155")
			)
			(pin input line
				(at -54.61 81.28 0)
				(length 7.62)
				(name "M0")
				(number "52")
			)
			(pin input line
				(at -54.61 78.74 0)
				(length 7.62)
				(name "M1")
				(number "50")
			)
			(pin input line
				(at -54.61 76.2 0)
				(length 7.62)
				(name "M2")
				(number "54")
			)
			(pin bidirectional line
				(at -54.61 71.12 0)
				(length 7.62)
				(name "IO7P3")
				(number "3")
			)
			(pin bidirectional line
				(at -54.61 68.58 0)
				(length 7.62)
				(name "IO7P4")
				(number "4")
			)
			(pin bidirectional line
				(at -54.61 66.04 0)
				(length 7.62)
				(name "IO7P5")
				(number "5")
			)
			(pin bidirectional line
				(at -54.61 63.5 0)
				(length 7.62)
				(name "IO7VRP6")
				(number "6")
			)
			(pin bidirectional line
				(at -54.61 60.96 0)
				(length 7.62)
				(name "IO7P7")
				(number "7")
			)
			(pin bidirectional line
				(at -54.61 58.42 0)
				(length 7.62)
				(name "IO7P8")
				(number "8")
			)
			(pin bidirectional line
				(at -54.61 55.88 0)
				(length 7.62)
				(name "IO7P9")
				(number "9")
			)
			(pin bidirectional line
				(at -54.61 53.34 0)
				(length 7.62)
				(name "IO7P10")
				(number "10")
			)
			(pin bidirectional line
				(at -54.61 50.8 0)
				(length 7.62)
				(name "IO7P14")
				(number "14")
			)
			(pin bidirectional line
				(at -54.61 48.26 0)
				(length 7.62)
				(name "IO7P15")
				(number "15")
			)
			(pin bidirectional line
				(at -54.61 45.72 0)
				(length 7.62)
				(name "IO7P16")
				(number "16")
			)
			(pin bidirectional line
				(at -54.61 43.18 0)
				(length 7.62)
				(name "IO7P17")
				(number "17")
			)
			(pin bidirectional line
				(at -54.61 40.64 0)
				(length 7.62)
				(name "IO7P18")
				(number "18")
			)
			(pin bidirectional line
				(at -54.61 38.1 0)
				(length 7.62)
				(name "IO7VRP20")
				(number "20")
			)
			(pin bidirectional line
				(at -54.61 35.56 0)
				(length 7.62)
				(name "IO7P21")
				(number "21")
			)
			(pin bidirectional line
				(at -54.61 33.02 0)
				(length 7.62)
				(name "IO7P22")
				(number "22")
			)
			(pin bidirectional line
				(at -54.61 30.48 0)
				(length 7.62)
				(name "IO7P23")
				(number "23")
			)
			(pin bidirectional line
				(at -54.61 25.4 0)
				(length 7.62)
				(name "IO6P29")
				(number "29")
			)
			(pin bidirectional line
				(at -54.61 22.86 0)
				(length 7.62)
				(name "IO6P30")
				(number "30")
			)
			(pin bidirectional line
				(at -54.61 20.32 0)
				(length 7.62)
				(name "IO6VRP31")
				(number "31")
			)
			(pin bidirectional line
				(at -54.61 17.78 0)
				(length 7.62)
				(name "IO6P33")
				(number "33")
			)
			(pin bidirectional line
				(at -54.61 15.24 0)
				(length 7.62)
				(name "IO6P34")
				(number "34")
			)
			(pin bidirectional line
				(at -54.61 12.7 0)
				(length 7.62)
				(name "IO6P35")
				(number "35")
			)
			(pin bidirectional line
				(at -54.61 10.16 0)
				(length 7.62)
				(name "IO6P36")
				(number "36")
			)
			(pin bidirectional line
				(at -54.61 7.62 0)
				(length 7.62)
				(name "IO6P37")
				(number "37")
			)
			(pin bidirectional line
				(at -54.61 5.08 0)
				(length 7.62)
				(name "IO6P41")
				(number "41")
			)
			(pin bidirectional line
				(at -54.61 2.54 0)
				(length 7.62)
				(name "IO6P42")
				(number "42")
			)
			(pin bidirectional line
				(at -54.61 0 0)
				(length 7.62)
				(name "IO6P43")
				(number "43")
			)
			(pin bidirectional line
				(at -54.61 -2.54 0)
				(length 7.62)
				(name "IO6P44")
				(number "44")
			)
			(pin bidirectional line
				(at -54.61 -5.08 0)
				(length 7.62)
				(name "IO6VRP45")
				(number "45")
			)
			(pin bidirectional line
				(at -54.61 -7.62 0)
				(length 7.62)
				(name "IO6P46")
				(number "46")
			)
			(pin bidirectional line
				(at -54.61 -10.16 0)
				(length 7.62)
				(name "IO6P47")
				(number "47")
			)
			(pin bidirectional line
				(at -54.61 -12.7 0)
				(length 7.62)
				(name "IO6P48")
				(number "48")
			)
			(pin bidirectional line
				(at -54.61 -15.24 0)
				(length 7.62)
				(name "IO6P49")
				(number "49")
			)
			(pin bidirectional line
				(at -54.61 -20.32 0)
				(length 7.62)
				(name "IO5P57")
				(number "57")
			)
			(pin bidirectional line
				(at -54.61 -22.86 0)
				(length 7.62)
				(name "IO5P58")
				(number "58")
			)
			(pin bidirectional line
				(at -54.61 -25.4 0)
				(length 7.62)
				(name "IO5VRP59")
				(number "59")
			)
			(pin bidirectional line
				(at -54.61 -27.94 0)
				(length 7.62)
				(name "IO5P60")
				(number "60")
			)
			(pin bidirectional line
				(at -54.61 -30.48 0)
				(length 7.62)
				(name "IO5P61")
				(number "61")
			)
			(pin bidirectional line
				(at -54.61 -33.02 0)
				(length 7.62)
				(name "IO5P62")
				(number "62")
			)
			(pin bidirectional line
				(at -54.61 -35.56 0)
				(length 7.62)
				(name "IO5P63")
				(number "63")
			)
			(pin bidirectional line
				(at -54.61 -38.1 0)
				(length 7.62)
				(name "IO5P67")
				(number "67")
			)
			(pin bidirectional line
				(at -54.61 -40.64 0)
				(length 7.62)
				(name "IO5P68")
				(number "68")
			)
			(pin bidirectional line
				(at -54.61 -43.18 0)
				(length 7.62)
				(name "IO5P69")
				(number "69")
			)
			(pin bidirectional line
				(at -54.61 -45.72 0)
				(length 7.62)
				(name "IO5P70")
				(number "70")
			)
			(pin bidirectional line
				(at -54.61 -48.26 0)
				(length 7.62)
				(name "IO5P71")
				(number "71")
			)
			(pin bidirectional line
				(at -54.61 -50.8 0)
				(length 7.62)
				(name "IO5VRP73")
				(number "73")
			)
			(pin bidirectional line
				(at -54.61 -53.34 0)
				(length 7.62)
				(name "IO5P74")
				(number "74")
			)
			(pin input clock
				(at -54.61 -55.88 0)
				(length 7.62)
				(name "CGK1")
				(number "77")
			)
			(pin input clock
				(at -54.61 -60.96 0)
				(length 7.62)
				(name "CGK0")
				(number "80")
			)
			(pin bidirectional line
				(at -54.61 -63.5 0)
				(length 7.62)
				(name "IO4P81")
				(number "81")
			)
			(pin bidirectional line
				(at -54.61 -66.04 0)
				(length 7.62)
				(name "IO4P82")
				(number "82")
			)
			(pin bidirectional line
				(at -54.61 -68.58 0)
				(length 7.62)
				(name "IO4P83")
				(number "83")
			)
			(pin bidirectional line
				(at -54.61 -71.12 0)
				(length 7.62)
				(name "IO4VRP84")
				(number "84")
			)
			(pin bidirectional line
				(at -54.61 -73.66 0)
				(length 7.62)
				(name "IO4P86")
				(number "86")
			)
			(pin bidirectional line
				(at -54.61 -76.2 0)
				(length 7.62)
				(name "IO4P87")
				(number "87")
			)
			(pin bidirectional line
				(at -54.61 -78.74 0)
				(length 7.62)
				(name "IO4P88")
				(number "88")
			)
			(pin bidirectional line
				(at -54.61 -81.28 0)
				(length 7.62)
				(name "IO4P89")
				(number "89")
			)
			(pin bidirectional line
				(at -54.61 -83.82 0)
				(length 7.62)
				(name "IO4P90")
				(number "90")
			)
			(pin bidirectional line
				(at -54.61 -86.36 0)
				(length 7.62)
				(name "IO4P94")
				(number "94")
			)
			(pin bidirectional line
				(at -54.61 -88.9 0)
				(length 7.62)
				(name "IO4P95")
				(number "95")
			)
			(pin bidirectional line
				(at -54.61 -91.44 0)
				(length 7.62)
				(name "IO4P96")
				(number "96")
			)
			(pin bidirectional line
				(at -54.61 -93.98 0)
				(length 7.62)
				(name "IO4P97")
				(number "97")
			)
			(pin bidirectional line
				(at -54.61 -96.52 0)
				(length 7.62)
				(name "IO4VRP98")
				(number "98")
			)
			(pin bidirectional line
				(at -54.61 -99.06 0)
				(length 7.62)
				(name "IO4P99")
				(number "99")
			)
			(pin bidirectional line
				(at -54.61 -101.6 0)
				(length 7.62)
				(name "IO4P100")
				(number "100")
			)
			(pin bidirectional line
				(at -54.61 -104.14 0)
				(length 7.62)
				(name "IO4P101")
				(number "101")
			)
			(pin bidirectional line
				(at -54.61 -106.68 0)
				(length 7.62)
				(name "IO4P102")
				(number "102")
			)
			(pin passive line
				(at -36.83 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "12")
			)
			(pin passive line
				(at -34.29 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "26")
			)
			(pin passive line
				(at -31.75 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "39")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "103")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "116")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "124")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "131")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "137")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "145")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "158")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "169")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "177")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "183")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "190")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "198")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "40")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "51")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "64")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "72")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "79")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "85")
			)
			(pin passive line
				(at -31.75 -116.84 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "93")
			)
			(pin passive line
				(at -29.21 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "53")
			)
			(pin passive line
				(at -26.67 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "65")
			)
			(pin passive line
				(at -24.13 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "78")
			)
			(pin passive line
				(at -21.59 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "92")
			)
			(pin passive line
				(at -19.05 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "105")
			)
			(pin passive line
				(at -16.51 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "117")
			)
			(pin passive line
				(at -13.97 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "130")
			)
			(pin passive line
				(at -11.43 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "144")
			)
			(pin passive line
				(at -8.89 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "156")
			)
			(pin passive line
				(at -6.35 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "170")
			)
			(pin passive line
				(at -3.81 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "184")
			)
			(pin passive line
				(at -1.27 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "197")
			)
			(pin passive line
				(at 1.27 116.84 270)
				(length 7.62)
				(name "VCCO")
				(number "208")
			)
			(pin passive line
				(at 8.89 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "13")
			)
			(pin passive line
				(at 11.43 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "28")
			)
			(pin passive line
				(at 13.97 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "38")
			)
			(pin passive line
				(at 16.51 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "66")
			)
			(pin passive line
				(at 19.05 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "76")
			)
			(pin passive line
				(at 21.59 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "91")
			)
			(pin passive line
				(at 24.13 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "118")
			)
			(pin passive line
				(at 26.67 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "128")
			)
			(pin passive line
				(at 29.21 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "143")
			)
			(pin passive line
				(at 31.75 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "171")
			)
			(pin passive line
				(at 34.29 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "186")
			)
			(pin passive line
				(at 36.83 116.84 270)
				(length 7.62)
				(name "VCCINT")
				(number "196")
			)
			(pin bidirectional line
				(at 54.61 96.52 180)
				(length 7.62)
				(name "IRDY2")
				(number "132")
			)
			(pin bidirectional line
				(at 54.61 93.98 180)
				(length 7.62)
				(name "TRDY3")
				(number "129")
			)
			(pin bidirectional line
				(at 54.61 91.44 180)
				(length 7.62)
				(name "TRDY6")
				(number "27")
			)
			(pin bidirectional line
				(at 54.61 88.9 180)
				(length 7.62)
				(name "IRDY7")
				(number "24")
			)
			(pin bidirectional line
				(at 54.61 83.82 180)
				(length 7.62)
				(name "/WR")
				(number "161")
			)
			(pin bidirectional line
				(at 54.61 81.28 180)
				(length 7.62)
				(name "/CS")
				(number "160")
			)
			(pin bidirectional line
				(at 54.61 76.2 180)
				(length 7.62)
				(name "BUSY/DOUT")
				(number "154")
			)
			(pin bidirectional line
				(at 54.61 73.66 180)
				(length 7.62)
				(name "D0/DIN")
				(number "153")
			)
			(pin bidirectional line
				(at 54.61 66.04 180)
				(length 7.62)
				(name "IO0P206")
				(number "206")
			)
			(pin bidirectional line
				(at 54.61 63.5 180)
				(length 7.62)
				(name "IO0P205")
				(number "205")
			)
			(pin bidirectional line
				(at 54.61 60.96 180)
				(length 7.62)
				(name "IO0P204")
				(number "204")
			)
			(pin bidirectional line
				(at 54.61 58.42 180)
				(length 7.62)
				(name "IO0VRP203")
				(number "203")
			)
			(pin bidirectional line
				(at 54.61 55.88 180)
				(length 7.62)
				(name "IO0P202")
				(number "202")
			)
			(pin bidirectional line
				(at 54.61 53.34 180)
				(length 7.62)
				(name "IO0P201")
				(number "201")
			)
			(pin bidirectional line
				(at 54.61 50.8 180)
				(length 7.62)
				(name "IO0P200")
				(number "200")
			)
			(pin bidirectional line
				(at 54.61 48.26 180)
				(length 7.62)
				(name "IO0P199")
				(number "199")
			)
			(pin bidirectional line
				(at 54.61 45.72 180)
				(length 7.62)
				(name "IO0P195")
				(number "195")
			)
			(pin bidirectional line
				(at 54.61 43.18 180)
				(length 7.62)
				(name "IO0P194")
				(number "194")
			)
			(pin bidirectional line
				(at 54.61 40.64 180)
				(length 7.62)
				(name "IO0P193")
				(number "193")
			)
			(pin bidirectional line
				(at 54.61 38.1 180)
				(length 7.62)
				(name "IO0P192")
				(number "192")
			)
			(pin bidirectional line
				(at 54.61 35.56 180)
				(length 7.62)
				(name "IO0P191")
				(number "191")
			)
			(pin bidirectional line
				(at 54.61 33.02 180)
				(length 7.62)
				(name "IO0VRP189")
				(number "189")
			)
			(pin bidirectional line
				(at 54.61 30.48 180)
				(length 7.62)
				(name "IO0P188")
				(number "188")
			)
			(pin bidirectional line
				(at 54.61 27.94 180)
				(length 7.62)
				(name "IO0P187")
				(number "187")
			)
			(pin input clock
				(at 54.61 25.4 180)
				(length 7.62)
				(name "GCK3")
				(number "185")
			)
			(pin input clock
				(at 54.61 20.32 180)
				(length 7.62)
				(name "GCK2")
				(number "182")
			)
			(pin bidirectional line
				(at 54.61 17.78 180)
				(length 7.62)
				(name "IO1P181")
				(number "181")
			)
			(pin bidirectional line
				(at 54.61 15.24 180)
				(length 7.62)
				(name "IO1P180")
				(number "180")
			)
			(pin bidirectional line
				(at 54.61 12.7 180)
				(length 7.62)
				(name "IO1P179")
				(number "179")
			)
			(pin bidirectional line
				(at 54.61 10.16 180)
				(length 7.62)
				(name "IO1VRP178")
				(number "178")
			)
			(pin bidirectional line
				(at 54.61 7.62 180)
				(length 7.62)
				(name "IO1P176")
				(number "176")
			)
			(pin bidirectional line
				(at 54.61 5.08 180)
				(length 7.62)
				(name "IO1P175")
				(number "175")
			)
			(pin bidirectional line
				(at 54.61 2.54 180)
				(length 7.62)
				(name "IO1P174")
				(number "174")
			)
			(pin bidirectional line
				(at 54.61 0 180)
				(length 7.62)
				(name "IO1P173")
				(number "173")
			)
			(pin bidirectional line
				(at 54.61 -2.54 180)
				(length 7.62)
				(name "IO1P172")
				(number "172")
			)
			(pin bidirectional line
				(at 54.61 -5.08 180)
				(length 7.62)
				(name "IO1P168")
				(number "168")
			)
			(pin bidirectional line
				(at 54.61 -7.62 180)
				(length 7.62)
				(name "IO1P167")
				(number "167")
			)
			(pin bidirectional line
				(at 54.61 -10.16 180)
				(length 7.62)
				(name "IO1P166")
				(number "166")
			)
			(pin bidirectional line
				(at 54.61 -12.7 180)
				(length 7.62)
				(name "IO1P165")
				(number "165")
			)
			(pin bidirectional line
				(at 54.61 -15.24 180)
				(length 7.62)
				(name "IO1VRP164")
				(number "164")
			)
			(pin bidirectional line
				(at 54.61 -17.78 180)
				(length 7.62)
				(name "IO1P163")
				(number "163")
			)
			(pin bidirectional line
				(at 54.61 -20.32 180)
				(length 7.62)
				(name "IO1P162")
				(number "162")
			)
			(pin bidirectional line
				(at 54.61 -25.4 180)
				(length 7.62)
				(name "IO2P152")
				(number "152")
			)
			(pin bidirectional line
				(at 54.61 -27.94 180)
				(length 7.62)
				(name "IO2P151")
				(number "151")
			)
			(pin bidirectional line
				(at 54.61 -30.48 180)
				(length 7.62)
				(name "IO2VRP150")
				(number "150")
			)
			(pin bidirectional line
				(at 54.61 -33.02 180)
				(length 7.62)
				(name "IO2P149")
				(number "149")
			)
			(pin bidirectional line
				(at 54.61 -35.56 180)
				(length 7.62)
				(name "IO2P148")
				(number "148")
			)
			(pin bidirectional line
				(at 54.61 -38.1 180)
				(length 7.62)
				(name "IO2P147")
				(number "147")
			)
			(pin bidirectional line
				(at 54.61 -40.64 180)
				(length 7.62)
				(name "IO2/D1P46")
				(number "146")
			)
			(pin bidirectional line
				(at 54.61 -43.18 180)
				(length 7.62)
				(name "IO2/D2P142")
				(number "142")
			)
			(pin bidirectional line
				(at 54.61 -45.72 180)
				(length 7.62)
				(name "IO2P141")
				(number "141")
			)
			(pin bidirectional line
				(at 54.61 -48.26 180)
				(length 7.62)
				(name "IO2P140")
				(number "140")
			)
			(pin bidirectional line
				(at 54.61 -50.8 180)
				(length 7.62)
				(name "IO2P139")
				(number "139")
			)
			(pin bidirectional line
				(at 54.61 -53.34 180)
				(length 7.62)
				(name "IO2P138")
				(number "138")
			)
			(pin bidirectional line
				(at 54.61 -55.88 180)
				(length 7.62)
				(name "IO2VRP136")
				(number "136")
			)
			(pin bidirectional line
				(at 54.61 -58.42 180)
				(length 7.62)
				(name "IO2/D3P135")
				(number "135")
			)
			(pin bidirectional line
				(at 54.61 -60.96 180)
				(length 7.62)
				(name "IO2P134")
				(number "134")
			)
			(pin bidirectional line
				(at 54.61 -63.5 180)
				(length 7.62)
				(name "IO2P133")
				(number "133")
			)
			(pin bidirectional line
				(at 54.61 -68.58 180)
				(length 7.62)
				(name "IO3P127")
				(number "127")
			)
			(pin bidirectional line
				(at 54.61 -71.12 180)
				(length 7.62)
				(name "IO3/D4P126")
				(number "126")
			)
			(pin bidirectional line
				(at 54.61 -73.66 180)
				(length 7.62)
				(name "IO3VRP125")
				(number "125")
			)
			(pin bidirectional line
				(at 54.61 -76.2 180)
				(length 7.62)
				(name "IO3P123")
				(number "123")
			)
			(pin bidirectional line
				(at 54.61 -78.74 180)
				(length 7.62)
				(name "IO3P122")
				(number "122")
			)
			(pin bidirectional line
				(at 54.61 -81.28 180)
				(length 7.62)
				(name "IO3P121")
				(number "121")
			)
			(pin bidirectional line
				(at 54.61 -83.82 180)
				(length 7.62)
				(name "IO3P120")
				(number "120")
			)
			(pin bidirectional line
				(at 54.61 -86.36 180)
				(length 7.62)
				(name "IO3/D5P119")
				(number "119")
			)
			(pin bidirectional line
				(at 54.61 -88.9 180)
				(length 7.62)
				(name "IO3/D6P115")
				(number "115")
			)
			(pin bidirectional line
				(at 54.61 -91.44 180)
				(length 7.62)
				(name "IO3P114")
				(number "114")
			)
			(pin bidirectional line
				(at 54.61 -93.98 180)
				(length 7.62)
				(name "IO3P113")
				(number "113")
			)
			(pin bidirectional line
				(at 54.61 -96.52 180)
				(length 7.62)
				(name "IO3P112")
				(number "112")
			)
			(pin bidirectional line
				(at 54.61 -99.06 180)
				(length 7.62)
				(name "IO3VRP111")
				(number "111")
			)
			(pin bidirectional line
				(at 54.61 -101.6 180)
				(length 7.62)
				(name "IO3P110")
				(number "110")
			)
			(pin bidirectional line
				(at 54.61 -104.14 180)
				(length 7.62)
				(name "IO3P109")
				(number "109")
			)
			(pin bidirectional line
				(at 54.61 -106.68 180)
				(length 7.62)
				(name "IO3/D7P108")
				(number "108")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC2S64A-xQFG48"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 34.29 0)
		)
		(property "Value" "XC2S64A-xQFG48"
			(at 5.08 -34.29 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "xilinx/xc2c64.pdf"
			(at 0 0 0)
		)
		(property "Description" "Xilinx CoolRunner"
			(at 0 0 0)
		)
		(symbol "XC2S64A-xQFG48_0_1")
		(symbol "XC2S64A-xQFG48_1_1"
			(pin output line
				(at -24.13 30.48 0)
				(length 7.62)
				(name "TDO")
				(number "40")
			)
			(pin input line
				(at -24.13 27.94 0)
				(length 7.62)
				(name "TCK")
				(number "23")
			)
			(pin input line
				(at -24.13 25.4 0)
				(length 7.62)
				(name "TDI")
				(number "21")
			)
			(pin input line
				(at -24.13 22.86 0)
				(length 7.62)
				(name "TMS")
				(number "22")
			)
			(pin bidirectional line
				(at -24.13 17.78 0)
				(length 7.62)
				(name "A2")
				(number "5")
			)
			(pin bidirectional line
				(at -24.13 15.24 0)
				(length 7.62)
				(name "A3")
				(number "4")
			)
			(pin bidirectional line
				(at -24.13 12.7 0)
				(length 7.62)
				(name "GTS1")
				(number "2")
			)
			(pin bidirectional line
				(at -24.13 10.16 0)
				(length 7.62)
				(name "GTS0")
				(number "1")
			)
			(pin bidirectional line
				(at -24.13 7.62 0)
				(length 7.62)
				(name "GTS3")
				(number "48")
			)
			(pin bidirectional line
				(at -24.13 5.08 0)
				(length 7.62)
				(name "GTS2")
				(number "47")
			)
			(pin bidirectional line
				(at -24.13 2.54 0)
				(length 7.62)
				(name "GSR")
				(number "46")
			)
			(pin bidirectional line
				(at -24.13 -2.54 0)
				(length 7.62)
				(name "B1")
				(number "6")
			)
			(pin bidirectional line
				(at -24.13 -5.08 0)
				(length 7.62)
				(name "B2")
				(number "7")
			)
			(pin bidirectional line
				(at -24.13 -7.62 0)
				(length 7.62)
				(name "B3")
				(number "8")
			)
			(pin passive line
				(at -24.13 -10.16 0)
				(length 7.62)
				(name "B4")
				(number "9")
			)
			(pin bidirectional line
				(at -24.13 -12.7 0)
				(length 7.62)
				(name "B5")
				(number "10")
			)
			(pin passive line
				(at -24.13 -15.24 0)
				(length 7.62)
				(name "GCK0")
				(number "11")
			)
			(pin bidirectional line
				(at -24.13 -17.78 0)
				(length 7.62)
				(name "GCK1")
				(number "12")
			)
			(pin bidirectional line
				(at -24.13 -20.32 0)
				(length 7.62)
				(name "GCK2")
				(number "13")
			)
			(pin bidirectional line
				(at -24.13 -22.86 0)
				(length 7.62)
				(name "B12")
				(number "14")
			)
			(pin bidirectional line
				(at -24.13 -25.4 0)
				(length 7.62)
				(name "B13")
				(number "15")
			)
			(pin power_in line
				(at -10.16 36.83 270)
				(length 3.81)
				(name "VCCjtag")
				(number "3")
			)
			(pin power_in line
				(at -3.81 36.83 270)
				(length 3.81)
				(name "VCCio1")
				(number "19")
			)
			(pin power_in line
				(at -2.54 -36.83 90)
				(length 3.81)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at -2.54 -36.83 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at -2.54 -36.83 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin power_in line
				(at -1.27 36.83 270)
				(length 3.81)
				(name "VCCio2")
				(number "42")
			)
			(pin power_in line
				(at 3.81 36.83 270)
				(length 3.81)
				(name "VCCint")
				(number "29")
			)
			(pin bidirectional line
				(at 24.13 22.86 180)
				(length 7.62)
				(name "D1")
				(number "17")
			)
			(pin bidirectional line
				(at 24.13 20.32 180)
				(length 7.62)
				(name "D2")
				(number "18")
			)
			(pin bidirectional line
				(at 24.13 17.78 180)
				(length 7.62)
				(name "D7")
				(number "20")
			)
			(pin bidirectional line
				(at 24.13 15.24 180)
				(length 7.62)
				(name "D10")
				(number "24")
			)
			(pin bidirectional line
				(at 24.13 12.7 180)
				(length 7.62)
				(name "D11")
				(number "25")
			)
			(pin bidirectional line
				(at 24.13 10.16 180)
				(length 7.62)
				(name "D12")
				(number "26")
			)
			(pin bidirectional line
				(at 24.13 7.62 180)
				(length 7.62)
				(name "D13")
				(number "27")
			)
			(pin bidirectional line
				(at 24.13 5.08 180)
				(length 7.62)
				(name "D13")
				(number "28")
			)
			(pin bidirectional line
				(at 24.13 2.54 180)
				(length 7.62)
				(name "D16")
				(number "30")
			)
			(pin bidirectional line
				(at 24.13 -2.54 180)
				(length 7.62)
				(name "C1")
				(number "45")
			)
			(pin bidirectional line
				(at 24.13 -5.08 180)
				(length 7.62)
				(name "C2")
				(number "44")
			)
			(pin bidirectional line
				(at 24.13 -7.62 180)
				(length 7.62)
				(name "C3")
				(number "43")
			)
			(pin bidirectional line
				(at 24.13 -10.16 180)
				(length 7.62)
				(name "C5")
				(number "39")
			)
			(pin bidirectional line
				(at 24.13 -12.7 180)
				(length 7.62)
				(name "C6")
				(number "38")
			)
			(pin bidirectional line
				(at 24.13 -15.24 180)
				(length 7.62)
				(name "C9")
				(number "37")
			)
			(pin bidirectional line
				(at 24.13 -17.78 180)
				(length 7.62)
				(name "C10")
				(number "36")
			)
			(pin bidirectional line
				(at 24.13 -20.32 180)
				(length 7.62)
				(name "C11")
				(number "35")
			)
			(pin bidirectional line
				(at 24.13 -22.86 180)
				(length 7.62)
				(name "C12")
				(number "34")
			)
			(pin bidirectional line
				(at 24.13 -25.4 180)
				(length 7.62)
				(name "C14")
				(number "33")
			)
			(pin bidirectional line
				(at 24.13 -27.94 180)
				(length 7.62)
				(name "C15")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC3020-PC68"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XC3020-PC68"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC3020-PC68_0_1")
		(symbol "XC3020-PC68_1_1"
			(pin input line
				(at -24.13 39.37 0)
				(length 7.62)
				(name "~{PWRDWN}")
				(number "10")
			)
			(pin input line
				(at -24.13 36.83 0)
				(length 7.62)
				(name "M0")
				(number "26")
			)
			(pin input line
				(at -24.13 34.29 0)
				(length 7.62)
				(name "M1")
				(number "25")
			)
			(pin bidirectional line
				(at -24.13 31.75 0)
				(length 7.62)
				(name "M2")
				(number "27")
			)
			(pin input line
				(at -24.13 29.21 0)
				(length 7.62)
				(name "~{RESET}")
				(number "44")
			)
			(pin bidirectional line
				(at -24.13 26.67 0)
				(length 7.62)
				(name "D/PROG")
				(number "45")
			)
			(pin bidirectional line
				(at -24.13 24.13 0)
				(length 7.62)
				(name "DIN")
				(number "58")
			)
			(pin bidirectional line
				(at -24.13 21.59 0)
				(length 7.62)
				(name "DOUT")
				(number "59")
			)
			(pin input clock
				(at -24.13 19.05 0)
				(length 7.62)
				(name "CLK")
				(number "60")
			)
			(pin output line
				(at -24.13 16.51 0)
				(length 7.62)
				(name "HDC")
				(number "28")
			)
			(pin output line
				(at -24.13 13.97 0)
				(length 7.62)
				(name "LDC")
				(number "30")
			)
			(pin passive line
				(at -24.13 11.43 0)
				(length 7.62)
				(name "P2")
				(number "2")
			)
			(pin passive line
				(at -24.13 8.89 0)
				(length 7.62)
				(name "P3")
				(number "3")
			)
			(pin passive line
				(at -24.13 6.35 0)
				(length 7.62)
				(name "P4")
				(number "4")
			)
			(pin passive line
				(at -24.13 3.81 0)
				(length 7.62)
				(name "P5")
				(number "5")
			)
			(pin passive line
				(at -24.13 1.27 0)
				(length 7.62)
				(name "P6")
				(number "6")
			)
			(pin passive line
				(at -24.13 -1.27 0)
				(length 7.62)
				(name "P7")
				(number "7")
			)
			(pin passive line
				(at -24.13 -3.81 0)
				(length 7.62)
				(name "P8")
				(number "8")
			)
			(pin passive line
				(at -24.13 -6.35 0)
				(length 7.62)
				(name "P9")
				(number "9")
			)
			(pin passive line
				(at -24.13 -8.89 0)
				(length 7.62)
				(name "P11")
				(number "11")
			)
			(pin passive line
				(at -24.13 -11.43 0)
				(length 7.62)
				(name "P12")
				(number "12")
			)
			(pin passive line
				(at -24.13 -13.97 0)
				(length 7.62)
				(name "P13")
				(number "13")
			)
			(pin passive line
				(at -24.13 -16.51 0)
				(length 7.62)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -24.13 -19.05 0)
				(length 7.62)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -24.13 -21.59 0)
				(length 7.62)
				(name "P16")
				(number "16")
			)
			(pin passive line
				(at -24.13 -24.13 0)
				(length 7.62)
				(name "P17")
				(number "17")
			)
			(pin passive line
				(at -24.13 -26.67 0)
				(length 7.62)
				(name "P19")
				(number "19")
			)
			(pin passive line
				(at -24.13 -29.21 0)
				(length 7.62)
				(name "P20")
				(number "20")
			)
			(pin passive line
				(at -24.13 -31.75 0)
				(length 7.62)
				(name "P21")
				(number "21")
			)
			(pin passive line
				(at -24.13 -34.29 0)
				(length 7.62)
				(name "P22/INIT")
				(number "22")
			)
			(pin passive line
				(at -24.13 -36.83 0)
				(length 7.62)
				(name "P23")
				(number "23")
			)
			(pin passive line
				(at -24.13 -39.37 0)
				(length 7.62)
				(name "P24")
				(number "24")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "18")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 3.81)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 24.13 39.37 180)
				(length 7.62)
				(name "P68")
				(number "68")
			)
			(pin passive line
				(at 24.13 36.83 180)
				(length 7.62)
				(name "P67")
				(number "67")
			)
			(pin passive line
				(at 24.13 34.29 180)
				(length 7.62)
				(name "P66")
				(number "66")
			)
			(pin passive line
				(at 24.13 31.75 180)
				(length 7.62)
				(name "P65")
				(number "65")
			)
			(pin passive line
				(at 24.13 29.21 180)
				(length 7.62)
				(name "P64")
				(number "64")
			)
			(pin passive line
				(at 24.13 26.67 180)
				(length 7.62)
				(name "P63")
				(number "63")
			)
			(pin passive line
				(at 24.13 24.13 180)
				(length 7.62)
				(name "P62")
				(number "62")
			)
			(pin passive line
				(at 24.13 21.59 180)
				(length 7.62)
				(name "P61")
				(number "61")
			)
			(pin passive line
				(at 24.13 19.05 180)
				(length 7.62)
				(name "P57")
				(number "57")
			)
			(pin passive line
				(at 24.13 16.51 180)
				(length 7.62)
				(name "P56")
				(number "56")
			)
			(pin passive line
				(at 24.13 13.97 180)
				(length 7.62)
				(name "P55")
				(number "55")
			)
			(pin passive line
				(at 24.13 11.43 180)
				(length 7.62)
				(name "P54")
				(number "54")
			)
			(pin passive line
				(at 24.13 8.89 180)
				(length 7.62)
				(name "P53")
				(number "53")
			)
			(pin passive line
				(at 24.13 6.35 180)
				(length 7.62)
				(name "P51")
				(number "51")
			)
			(pin passive line
				(at 24.13 3.81 180)
				(length 7.62)
				(name "P50")
				(number "50")
			)
			(pin passive line
				(at 24.13 1.27 180)
				(length 7.62)
				(name "P49")
				(number "49")
			)
			(pin passive line
				(at 24.13 -1.27 180)
				(length 7.62)
				(name "P48")
				(number "48")
			)
			(pin passive line
				(at 24.13 -3.81 180)
				(length 7.62)
				(name "P47-XO")
				(number "47")
			)
			(pin passive line
				(at 24.13 -6.35 180)
				(length 7.62)
				(name "P46")
				(number "46")
			)
			(pin passive line
				(at 24.13 -8.89 180)
				(length 7.62)
				(name "P43-XI")
				(number "43")
			)
			(pin passive line
				(at 24.13 -11.43 180)
				(length 7.62)
				(name "P42")
				(number "42")
			)
			(pin passive line
				(at 24.13 -13.97 180)
				(length 7.62)
				(name "P41")
				(number "41")
			)
			(pin passive line
				(at 24.13 -16.51 180)
				(length 7.62)
				(name "P40")
				(number "40")
			)
			(pin passive line
				(at 24.13 -19.05 180)
				(length 7.62)
				(name "P39")
				(number "39")
			)
			(pin passive line
				(at 24.13 -21.59 180)
				(length 7.62)
				(name "P38")
				(number "38")
			)
			(pin passive line
				(at 24.13 -24.13 180)
				(length 7.62)
				(name "P37")
				(number "37")
			)
			(pin passive line
				(at 24.13 -26.67 180)
				(length 7.62)
				(name "P36")
				(number "36")
			)
			(pin passive line
				(at 24.13 -29.21 180)
				(length 7.62)
				(name "P34")
				(number "34")
			)
			(pin passive line
				(at 24.13 -31.75 180)
				(length 7.62)
				(name "P33")
				(number "33")
			)
			(pin passive line
				(at 24.13 -34.29 180)
				(length 7.62)
				(name "P32")
				(number "32")
			)
			(pin passive line
				(at 24.13 -36.83 180)
				(length 7.62)
				(name "P31")
				(number "31")
			)
			(pin passive line
				(at 24.13 -39.37 180)
				(length 7.62)
				(name "P29")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC3030-PC44"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XC3030-PC44"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC3030-PC44_0_1")
		(symbol "XC3030-PC44_1_1"
			(pin input line
				(at -24.13 24.13 0)
				(length 7.62)
				(name "~{PWRDWN}")
				(number "7")
			)
			(pin input line
				(at -24.13 21.59 0)
				(length 7.62)
				(name "M0")
				(number "17")
			)
			(pin input line
				(at -24.13 19.05 0)
				(length 7.62)
				(name "M1")
				(number "16")
			)
			(pin bidirectional line
				(at -24.13 16.51 0)
				(length 7.62)
				(name "M2")
				(number "18")
			)
			(pin input line
				(at -24.13 13.97 0)
				(length 7.62)
				(name "~{RESET}")
				(number "27")
			)
			(pin bidirectional line
				(at -24.13 11.43 0)
				(length 7.62)
				(name "D/PROG")
				(number "28")
			)
			(pin bidirectional line
				(at -24.13 8.89 0)
				(length 7.62)
				(name "DIN")
				(number "38")
			)
			(pin bidirectional line
				(at -24.13 6.35 0)
				(length 7.62)
				(name "DOUT")
				(number "39")
			)
			(pin input clock
				(at -24.13 3.81 0)
				(length 7.62)
				(name "CLK")
				(number "40")
			)
			(pin output line
				(at -24.13 1.27 0)
				(length 7.62)
				(name "HDC")
				(number "19")
			)
			(pin output line
				(at -24.13 -1.27 0)
				(length 7.62)
				(name "LDC")
				(number "20")
			)
			(pin passive line
				(at -24.13 -3.81 0)
				(length 7.62)
				(name "P2")
				(number "2")
			)
			(pin passive line
				(at -24.13 -6.35 0)
				(length 7.62)
				(name "P3")
				(number "3")
			)
			(pin passive line
				(at -24.13 -8.89 0)
				(length 7.62)
				(name "P4")
				(number "4")
			)
			(pin passive line
				(at -24.13 -11.43 0)
				(length 7.62)
				(name "P5")
				(number "5")
			)
			(pin passive line
				(at -24.13 -13.97 0)
				(length 7.62)
				(name "P6")
				(number "6")
			)
			(pin passive line
				(at -24.13 -16.51 0)
				(length 7.62)
				(name "P8-GCLK")
				(number "8")
			)
			(pin bidirectional line
				(at -24.13 -19.05 0)
				(length 7.62)
				(name "P9")
				(number "9")
			)
			(pin passive line
				(at -24.13 -21.59 0)
				(length 7.62)
				(name "P10")
				(number "10")
			)
			(pin passive line
				(at -24.13 -24.13 0)
				(length 7.62)
				(name "P11")
				(number "11")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 6.35)
				(name "VCC")
				(number "12")
			)
			(pin passive line
				(at 0 33.02 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "34")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 6.35)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 24.13 24.13 180)
				(length 7.62)
				(name "P44")
				(number "44")
			)
			(pin passive line
				(at 24.13 21.59 180)
				(length 7.62)
				(name "P43")
				(number "43")
			)
			(pin passive line
				(at 24.13 19.05 180)
				(length 7.62)
				(name "P42")
				(number "42")
			)
			(pin passive line
				(at 24.13 16.51 180)
				(length 7.62)
				(name "P41")
				(number "41")
			)
			(pin passive line
				(at 24.13 13.97 180)
				(length 7.62)
				(name "P37")
				(number "37")
			)
			(pin passive line
				(at 24.13 11.43 180)
				(length 7.62)
				(name "P36")
				(number "36")
			)
			(pin passive line
				(at 24.13 8.89 180)
				(length 7.62)
				(name "P35")
				(number "35")
			)
			(pin passive line
				(at 24.13 6.35 180)
				(length 7.62)
				(name "P33")
				(number "33")
			)
			(pin passive line
				(at 24.13 3.81 180)
				(length 7.62)
				(name "P32")
				(number "32")
			)
			(pin passive line
				(at 24.13 1.27 180)
				(length 7.62)
				(name "P31")
				(number "31")
			)
			(pin passive line
				(at 24.13 -1.27 180)
				(length 7.62)
				(name "XOUT-P30")
				(number "30")
			)
			(pin passive line
				(at 24.13 -3.81 180)
				(length 7.62)
				(name "P29")
				(number "29")
			)
			(pin passive line
				(at 24.13 -6.35 180)
				(length 7.62)
				(name "XIN-P26")
				(number "26")
			)
			(pin passive line
				(at 24.13 -8.89 180)
				(length 7.62)
				(name "P25")
				(number "25")
			)
			(pin passive line
				(at 24.13 -11.43 180)
				(length 7.62)
				(name "P24")
				(number "24")
			)
			(pin passive line
				(at 24.13 -13.97 180)
				(length 7.62)
				(name "INIT-P22")
				(number "22")
			)
			(pin passive line
				(at 24.13 -16.51 180)
				(length 7.62)
				(name "P21")
				(number "21")
			)
			(pin passive line
				(at 24.13 -19.05 180)
				(length 7.62)
				(name "P15")
				(number "15")
			)
			(pin bidirectional line
				(at 24.13 -21.59 180)
				(length 7.62)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at 24.13 -24.13 180)
				(length 7.62)
				(name "P13")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC3030-PC84"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XC3030-PC84"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC3030-PC84_0_1")
		(symbol "XC3030-PC84_1_1"
			(pin input line
				(at -27.94 49.53 0)
				(length 7.62)
				(name "~{PWRDWN}")
				(number "12")
			)
			(pin input line
				(at -27.94 46.99 0)
				(length 7.62)
				(name "M0")
				(number "32")
			)
			(pin input line
				(at -27.94 44.45 0)
				(length 7.62)
				(name "M1")
				(number "31")
			)
			(pin bidirectional line
				(at -27.94 41.91 0)
				(length 7.62)
				(name "M2")
				(number "33")
			)
			(pin input line
				(at -27.94 39.37 0)
				(length 7.62)
				(name "~{RESET}")
				(number "54")
			)
			(pin bidirectional line
				(at -27.94 36.83 0)
				(length 7.62)
				(name "DONE/PROG")
				(number "55")
			)
			(pin input line
				(at -27.94 34.29 0)
				(length 7.62)
				(name "DIN")
				(number "72")
			)
			(pin passive line
				(at -27.94 31.75 0)
				(length 7.62)
				(name "DOUT")
				(number "73")
			)
			(pin bidirectional clock
				(at -27.94 29.21 0)
				(length 7.62)
				(name "CLK")
				(number "74")
			)
			(pin passive line
				(at -27.94 26.67 0)
				(length 7.62)
				(name "HDC")
				(number "34")
			)
			(pin passive line
				(at -27.94 24.13 0)
				(length 7.62)
				(name "LDC")
				(number "36")
			)
			(pin passive line
				(at -27.94 21.59 0)
				(length 7.62)
				(name "P2")
				(number "2")
			)
			(pin passive line
				(at -27.94 19.05 0)
				(length 7.62)
				(name "P3")
				(number "3")
			)
			(pin passive line
				(at -27.94 16.51 0)
				(length 7.62)
				(name "P4")
				(number "4")
			)
			(pin passive line
				(at -27.94 13.97 0)
				(length 7.62)
				(name "P5")
				(number "5")
			)
			(pin passive line
				(at -27.94 11.43 0)
				(length 7.62)
				(name "P6")
				(number "6")
			)
			(pin passive line
				(at -27.94 8.89 0)
				(length 7.62)
				(name "P7")
				(number "7")
			)
			(pin passive line
				(at -27.94 6.35 0)
				(length 7.62)
				(name "P8")
				(number "8")
			)
			(pin passive line
				(at -27.94 3.81 0)
				(length 7.62)
				(name "P9")
				(number "9")
			)
			(pin passive line
				(at -27.94 1.27 0)
				(length 7.62)
				(name "P10")
				(number "10")
			)
			(pin passive line
				(at -27.94 -1.27 0)
				(length 7.62)
				(name "P11")
				(number "11")
			)
			(pin passive line
				(at -27.94 -3.81 0)
				(length 7.62)
				(name "P13")
				(number "13")
			)
			(pin passive line
				(at -27.94 -6.35 0)
				(length 7.62)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -27.94 -8.89 0)
				(length 7.62)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -27.94 -11.43 0)
				(length 7.62)
				(name "P16")
				(number "16")
			)
			(pin passive line
				(at -27.94 -13.97 0)
				(length 7.62)
				(name "P17")
				(number "17")
			)
			(pin passive line
				(at -27.94 -16.51 0)
				(length 7.62)
				(name "P18")
				(number "18")
			)
			(pin passive line
				(at -27.94 -19.05 0)
				(length 7.62)
				(name "P19")
				(number "19")
			)
			(pin passive line
				(at -27.94 -21.59 0)
				(length 7.62)
				(name "P20")
				(number "20")
			)
			(pin passive line
				(at -27.94 -24.13 0)
				(length 7.62)
				(name "P21")
				(number "21")
			)
			(pin passive line
				(at -27.94 -26.67 0)
				(length 7.62)
				(name "P23")
				(number "23")
			)
			(pin passive line
				(at -27.94 -29.21 0)
				(length 7.62)
				(name "P24")
				(number "24")
			)
			(pin passive line
				(at -27.94 -31.75 0)
				(length 7.62)
				(name "P25")
				(number "25")
			)
			(pin passive line
				(at -27.94 -34.29 0)
				(length 7.62)
				(name "P26")
				(number "26")
			)
			(pin passive line
				(at -27.94 -36.83 0)
				(length 7.62)
				(name "P27")
				(number "27")
			)
			(pin passive line
				(at -27.94 -39.37 0)
				(length 7.62)
				(name "P28")
				(number "28")
			)
			(pin passive line
				(at -27.94 -41.91 0)
				(length 7.62)
				(name "P29")
				(number "29")
			)
			(pin passive line
				(at -27.94 -44.45 0)
				(length 7.62)
				(name "P30")
				(number "30")
			)
			(pin passive line
				(at -27.94 -46.99 0)
				(length 7.62)
				(name "P35")
				(number "35")
			)
			(pin passive line
				(at -27.94 -49.53 0)
				(length 7.62)
				(name "P37")
				(number "37")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 6.35)
				(name "VCC")
				(number "22")
			)
			(pin passive line
				(at 0 58.42 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "64")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 6.35)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at 27.94 49.53 180)
				(length 7.62)
				(name "P84")
				(number "84")
			)
			(pin passive line
				(at 27.94 46.99 180)
				(length 7.62)
				(name "P83")
				(number "83")
			)
			(pin passive line
				(at 27.94 44.45 180)
				(length 7.62)
				(name "P82")
				(number "82")
			)
			(pin passive line
				(at 27.94 41.91 180)
				(length 7.62)
				(name "P81")
				(number "81")
			)
			(pin passive line
				(at 27.94 39.37 180)
				(length 7.62)
				(name "P80")
				(number "80")
			)
			(pin passive line
				(at 27.94 36.83 180)
				(length 7.62)
				(name "P79")
				(number "79")
			)
			(pin passive line
				(at 27.94 34.29 180)
				(length 7.62)
				(name "P78")
				(number "78")
			)
			(pin passive line
				(at 27.94 31.75 180)
				(length 7.62)
				(name "P77")
				(number "77")
			)
			(pin passive line
				(at 27.94 29.21 180)
				(length 7.62)
				(name "CS2/P76")
				(number "76")
			)
			(pin passive line
				(at 27.94 26.67 180)
				(length 7.62)
				(name "WS/P75")
				(number "75")
			)
			(pin passive line
				(at 27.94 24.13 180)
				(length 7.62)
				(name "P71")
				(number "71")
			)
			(pin passive line
				(at 27.94 21.59 180)
				(length 7.62)
				(name "P70")
				(number "70")
			)
			(pin passive line
				(at 27.94 19.05 180)
				(length 7.62)
				(name "P69")
				(number "69")
			)
			(pin passive line
				(at 27.94 16.51 180)
				(length 7.62)
				(name "P68")
				(number "68")
			)
			(pin passive line
				(at 27.94 13.97 180)
				(length 7.62)
				(name "P67")
				(number "67")
			)
			(pin passive line
				(at 27.94 11.43 180)
				(length 7.62)
				(name "CS1/P66")
				(number "66")
			)
			(pin passive line
				(at 27.94 8.89 180)
				(length 7.62)
				(name "P65")
				(number "65")
			)
			(pin passive line
				(at 27.94 6.35 180)
				(length 7.62)
				(name "P63")
				(number "63")
			)
			(pin passive line
				(at 27.94 3.81 180)
				(length 7.62)
				(name "P62")
				(number "62")
			)
			(pin passive line
				(at 27.94 1.27 180)
				(length 7.62)
				(name "CS0/P61")
				(number "61")
			)
			(pin passive line
				(at 27.94 -1.27 180)
				(length 7.62)
				(name "P60")
				(number "60")
			)
			(pin passive line
				(at 27.94 -3.81 180)
				(length 7.62)
				(name "P59")
				(number "59")
			)
			(pin passive line
				(at 27.94 -6.35 180)
				(length 7.62)
				(name "P58")
				(number "58")
			)
			(pin passive line
				(at 27.94 -8.89 180)
				(length 7.62)
				(name "XTL1(O)/P57")
				(number "57")
			)
			(pin passive line
				(at 27.94 -11.43 180)
				(length 7.62)
				(name "P56")
				(number "56")
			)
			(pin passive line
				(at 27.94 -13.97 180)
				(length 7.62)
				(name "XTL2(I)/P53")
				(number "53")
			)
			(pin passive line
				(at 27.94 -16.51 180)
				(length 7.62)
				(name "P52")
				(number "52")
			)
			(pin passive line
				(at 27.94 -19.05 180)
				(length 7.62)
				(name "P51")
				(number "51")
			)
			(pin passive line
				(at 27.94 -21.59 180)
				(length 7.62)
				(name "P50")
				(number "50")
			)
			(pin passive line
				(at 27.94 -24.13 180)
				(length 7.62)
				(name "P49")
				(number "49")
			)
			(pin passive line
				(at 27.94 -26.67 180)
				(length 7.62)
				(name "P48")
				(number "48")
			)
			(pin passive line
				(at 27.94 -29.21 180)
				(length 7.62)
				(name "P47")
				(number "47")
			)
			(pin passive line
				(at 27.94 -31.75 180)
				(length 7.62)
				(name "P46")
				(number "46")
			)
			(pin passive line
				(at 27.94 -34.29 180)
				(length 7.62)
				(name "P45")
				(number "45")
			)
			(pin passive line
				(at 27.94 -36.83 180)
				(length 7.62)
				(name "P44")
				(number "44")
			)
			(pin passive line
				(at 27.94 -39.37 180)
				(length 7.62)
				(name "INIT/P42")
				(number "42")
			)
			(pin passive line
				(at 27.94 -41.91 180)
				(length 7.62)
				(name "P41")
				(number "41")
			)
			(pin passive line
				(at 27.94 -44.45 180)
				(length 7.62)
				(name "P40")
				(number "40")
			)
			(pin passive line
				(at 27.94 -46.99 180)
				(length 7.62)
				(name "P39")
				(number "39")
			)
			(pin passive line
				(at 27.94 -49.53 180)
				(length 7.62)
				(name "P38")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC3030-VQ100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XC3030-VQ100"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC3030-VQ100_0_1")
		(symbol "XC3030-VQ100_1_1"
			(pin input line
				(at -24.13 54.61 0)
				(length 7.62)
				(name "~{PWRDWN}")
				(number "26")
			)
			(pin input line
				(at -24.13 52.07 0)
				(length 7.62)
				(name "M0/RT")
				(number "51")
			)
			(pin input line
				(at -24.13 49.53 0)
				(length 7.62)
				(name "M1/RD")
				(number "49")
			)
			(pin passive line
				(at -24.13 46.99 0)
				(length 7.62)
				(name "M2")
				(number "53")
			)
			(pin input line
				(at -24.13 44.45 0)
				(length 7.62)
				(name "~{RESET}")
				(number "75")
			)
			(pin open_collector line
				(at -24.13 41.91 0)
				(length 7.62)
				(name "DONE/PG")
				(number "77")
			)
			(pin passive line
				(at -24.13 39.37 0)
				(length 7.62)
				(name "P/DIN")
				(number "97")
			)
			(pin passive line
				(at -24.13 36.83 0)
				(length 7.62)
				(name "P/DOUT")
				(number "98")
			)
			(pin bidirectional clock
				(at -24.13 34.29 0)
				(length 7.62)
				(name "CLK")
				(number "99")
			)
			(pin passive line
				(at -24.13 31.75 0)
				(length 7.62)
				(name "P/HDC")
				(number "54")
			)
			(pin passive line
				(at -24.13 29.21 0)
				(length 7.62)
				(name "P/LDC")
				(number "56")
			)
			(pin passive line
				(at -24.13 26.67 0)
				(length 7.62)
				(name "P2")
				(number "2")
			)
			(pin passive line
				(at -24.13 24.13 0)
				(length 7.62)
				(name "P3")
				(number "3")
			)
			(pin passive line
				(at -24.13 19.05 0)
				(length 7.62)
				(name "P5")
				(number "5")
			)
			(pin passive line
				(at -24.13 16.51 0)
				(length 7.62)
				(name "P6")
				(number "6")
			)
			(pin passive line
				(at -24.13 13.97 0)
				(length 7.62)
				(name "P7")
				(number "7")
			)
			(pin passive line
				(at -24.13 11.43 0)
				(length 7.62)
				(name "P8")
				(number "8")
			)
			(pin passive line
				(at -24.13 8.89 0)
				(length 7.62)
				(name "P9")
				(number "9")
			)
			(pin passive line
				(at -24.13 6.35 0)
				(length 7.62)
				(name "P10")
				(number "10")
			)
			(pin passive line
				(at -24.13 3.81 0)
				(length 7.62)
				(name "P11")
				(number "11")
			)
			(pin passive line
				(at -24.13 1.27 0)
				(length 7.62)
				(name "P12")
				(number "12")
			)
			(pin passive line
				(at -24.13 -1.27 0)
				(length 7.62)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -24.13 -3.81 0)
				(length 7.62)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -24.13 -6.35 0)
				(length 7.62)
				(name "P16")
				(number "16")
			)
			(pin passive line
				(at -24.13 -8.89 0)
				(length 7.62)
				(name "P17")
				(number "17")
			)
			(pin passive line
				(at -24.13 -11.43 0)
				(length 7.62)
				(name "P18")
				(number "18")
			)
			(pin passive line
				(at -24.13 -13.97 0)
				(length 7.62)
				(name "P19")
				(number "19")
			)
			(pin passive line
				(at -24.13 -16.51 0)
				(length 7.62)
				(name "P20")
				(number "20")
			)
			(pin passive line
				(at -24.13 -19.05 0)
				(length 7.62)
				(name "P21")
				(number "21")
			)
			(pin passive line
				(at -24.13 -21.59 0)
				(length 7.62)
				(name "P22")
				(number "22")
			)
			(pin passive line
				(at -24.13 -24.13 0)
				(length 7.62)
				(name "P23")
				(number "23")
			)
			(pin passive line
				(at -24.13 -26.67 0)
				(length 7.62)
				(name "P/TCLKIN")
				(number "27")
			)
			(pin passive line
				(at -24.13 -31.75 0)
				(length 7.62)
				(name "P29")
				(number "29")
			)
			(pin passive line
				(at -24.13 -34.29 0)
				(length 7.62)
				(name "P30")
				(number "30")
			)
			(pin passive line
				(at -24.13 -36.83 0)
				(length 7.62)
				(name "P31")
				(number "31")
			)
			(pin passive line
				(at -24.13 -39.37 0)
				(length 7.62)
				(name "P32")
				(number "32")
			)
			(pin passive line
				(at -24.13 -41.91 0)
				(length 7.62)
				(name "P33")
				(number "33")
			)
			(pin passive line
				(at -24.13 -44.45 0)
				(length 7.62)
				(name "P34")
				(number "34")
			)
			(pin passive line
				(at -24.13 -46.99 0)
				(length 7.62)
				(name "P35")
				(number "35")
			)
			(pin passive line
				(at -24.13 -49.53 0)
				(length 7.62)
				(name "P36")
				(number "36")
			)
			(pin passive line
				(at -24.13 -52.07 0)
				(length 7.62)
				(name "P37")
				(number "37")
			)
			(pin passive line
				(at -24.13 -54.61 0)
				(length 7.62)
				(name "P39")
				(number "39")
			)
			(pin passive line
				(at 0 63.5 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "100")
			)
			(pin power_in line
				(at 0 63.5 270)
				(length 6.35)
				(name "VCC")
				(number "24")
			)
			(pin passive line
				(at 0 63.5 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "38")
			)
			(pin passive line
				(at 0 63.5 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin passive line
				(at 0 63.5 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "76")
			)
			(pin passive line
				(at 0 63.5 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "88")
			)
			(pin power_in line
				(at 0 -63.5 90)
				(length 6.35)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "50")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "74")
			)
			(pin passive line
				(at 24.13 54.61 180)
				(length 7.62)
				(name "P/RDY")
				(number "96")
			)
			(pin passive line
				(at 24.13 52.07 180)
				(length 7.62)
				(name "P91")
				(number "95")
			)
			(pin passive line
				(at 24.13 49.53 180)
				(length 7.62)
				(name "P94")
				(number "94")
			)
			(pin passive line
				(at 24.13 46.99 180)
				(length 7.62)
				(name "P93")
				(number "93")
			)
			(pin passive line
				(at 24.13 44.45 180)
				(length 7.62)
				(name "P92")
				(number "92")
			)
			(pin passive line
				(at 24.13 41.91 180)
				(length 7.62)
				(name "P91")
				(number "91")
			)
			(pin passive line
				(at 24.13 39.37 180)
				(length 7.62)
				(name "P90")
				(number "90")
			)
			(pin passive line
				(at 24.13 36.83 180)
				(length 7.62)
				(name "P98")
				(number "89")
			)
			(pin passive line
				(at 24.13 34.29 180)
				(length 7.62)
				(name "P87")
				(number "87")
			)
			(pin passive line
				(at 24.13 31.75 180)
				(length 7.62)
				(name "P86")
				(number "86")
			)
			(pin passive line
				(at 24.13 29.21 180)
				(length 7.62)
				(name "P85")
				(number "85")
			)
			(pin passive line
				(at 24.13 26.67 180)
				(length 7.62)
				(name "P84")
				(number "84")
			)
			(pin passive line
				(at 24.13 24.13 180)
				(length 7.62)
				(name "P83")
				(number "83")
			)
			(pin passive line
				(at 24.13 21.59 180)
				(length 7.62)
				(name "P82")
				(number "82")
			)
			(pin passive line
				(at 24.13 19.05 180)
				(length 7.62)
				(name "P81")
				(number "81")
			)
			(pin passive line
				(at 24.13 16.51 180)
				(length 7.62)
				(name "P80")
				(number "80")
			)
			(pin passive line
				(at 24.13 13.97 180)
				(length 7.62)
				(name "P/XO")
				(number "79")
			)
			(pin passive line
				(at 24.13 11.43 180)
				(length 7.62)
				(name "P78")
				(number "78")
			)
			(pin passive line
				(at 24.13 8.89 180)
				(length 7.62)
				(name "P/XI")
				(number "73")
			)
			(pin passive line
				(at 24.13 6.35 180)
				(length 7.62)
				(name "P72")
				(number "72")
			)
			(pin passive line
				(at 24.13 3.81 180)
				(length 7.62)
				(name "P71")
				(number "71")
			)
			(pin passive line
				(at 24.13 1.27 180)
				(length 7.62)
				(name "P70")
				(number "70")
			)
			(pin passive line
				(at 24.13 -1.27 180)
				(length 7.62)
				(name "P69")
				(number "69")
			)
			(pin passive line
				(at 24.13 -3.81 180)
				(length 7.62)
				(name "P68")
				(number "68")
			)
			(pin passive line
				(at 24.13 -6.35 180)
				(length 7.62)
				(name "P67")
				(number "67")
			)
			(pin passive line
				(at 24.13 -8.89 180)
				(length 7.62)
				(name "P66")
				(number "66")
			)
			(pin passive line
				(at 24.13 -11.43 180)
				(length 7.62)
				(name "P65")
				(number "65")
			)
			(pin passive line
				(at 24.13 -13.97 180)
				(length 7.62)
				(name "P64")
				(number "64")
			)
			(pin passive line
				(at 24.13 -16.51 180)
				(length 7.62)
				(name "P/INIT")
				(number "62")
			)
			(pin passive line
				(at 24.13 -19.05 180)
				(length 7.62)
				(name "P61")
				(number "61")
			)
			(pin passive line
				(at 24.13 -21.59 180)
				(length 7.62)
				(name "P60")
				(number "60")
			)
			(pin passive line
				(at 24.13 -24.13 180)
				(length 7.62)
				(name "P59")
				(number "59")
			)
			(pin passive line
				(at 24.13 -26.67 180)
				(length 7.62)
				(name "P58")
				(number "58")
			)
			(pin passive line
				(at 24.13 -29.21 180)
				(length 7.62)
				(name "P57")
				(number "57")
			)
			(pin passive line
				(at 24.13 -31.75 180)
				(length 7.62)
				(name "P55")
				(number "55")
			)
			(pin passive line
				(at 24.13 -34.29 180)
				(length 7.62)
				(name "P48")
				(number "48")
			)
			(pin passive line
				(at 24.13 -36.83 180)
				(length 7.62)
				(name "P47")
				(number "47")
			)
			(pin passive line
				(at 24.13 -39.37 180)
				(length 7.62)
				(name "P46")
				(number "46")
			)
			(pin passive line
				(at 24.13 -41.91 180)
				(length 7.62)
				(name "P45")
				(number "45")
			)
			(pin passive line
				(at 24.13 -44.45 180)
				(length 7.62)
				(name "P44")
				(number "44")
			)
			(pin passive line
				(at 24.13 -46.99 180)
				(length 7.62)
				(name "P43")
				(number "43")
			)
			(pin passive line
				(at 24.13 -49.53 180)
				(length 7.62)
				(name "P42")
				(number "42")
			)
			(pin passive line
				(at 24.13 -52.07 180)
				(length 7.62)
				(name "P41")
				(number "41")
			)
			(pin passive line
				(at 24.13 -54.61 180)
				(length 7.62)
				(name "P40")
				(number "40")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC3042-VQ100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XC3042-VQ100"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC3042-VQ100_0_1")
		(symbol "XC3042-VQ100_1_1"
			(pin input line
				(at -24.13 54.61 0)
				(length 7.62)
				(name "~{PWRDWN}")
				(number "26")
			)
			(pin input line
				(at -24.13 52.07 0)
				(length 7.62)
				(name "M0")
				(number "51")
			)
			(pin input line
				(at -24.13 49.53 0)
				(length 7.62)
				(name "M1")
				(number "49")
			)
			(pin passive line
				(at -24.13 46.99 0)
				(length 7.62)
				(name "M2")
				(number "53")
			)
			(pin input line
				(at -24.13 44.45 0)
				(length 7.62)
				(name "~{RESET}")
				(number "75")
			)
			(pin open_collector line
				(at -24.13 41.91 0)
				(length 7.62)
				(name "DONE/PG")
				(number "77")
			)
			(pin passive line
				(at -24.13 39.37 0)
				(length 7.62)
				(name "P/DIN")
				(number "97")
			)
			(pin passive line
				(at -24.13 36.83 0)
				(length 7.62)
				(name "P/DOUT")
				(number "98")
			)
			(pin bidirectional clock
				(at -24.13 34.29 0)
				(length 7.62)
				(name "CLK")
				(number "99")
			)
			(pin passive line
				(at -24.13 31.75 0)
				(length 7.62)
				(name "P/HDC")
				(number "54")
			)
			(pin passive line
				(at -24.13 29.21 0)
				(length 7.62)
				(name "P/LDC")
				(number "56")
			)
			(pin passive line
				(at -24.13 26.67 0)
				(length 7.62)
				(name "P2")
				(number "2")
			)
			(pin passive line
				(at -24.13 24.13 0)
				(length 7.62)
				(name "P3")
				(number "3")
			)
			(pin passive line
				(at -24.13 21.59 0)
				(length 7.62)
				(name "P4")
				(number "4")
			)
			(pin passive line
				(at -24.13 19.05 0)
				(length 7.62)
				(name "P5")
				(number "5")
			)
			(pin passive line
				(at -24.13 16.51 0)
				(length 7.62)
				(name "P6")
				(number "6")
			)
			(pin passive line
				(at -24.13 13.97 0)
				(length 7.62)
				(name "P7")
				(number "7")
			)
			(pin passive line
				(at -24.13 11.43 0)
				(length 7.62)
				(name "P8")
				(number "8")
			)
			(pin passive line
				(at -24.13 8.89 0)
				(length 7.62)
				(name "P9")
				(number "9")
			)
			(pin passive line
				(at -24.13 6.35 0)
				(length 7.62)
				(name "P10")
				(number "10")
			)
			(pin passive line
				(at -24.13 3.81 0)
				(length 7.62)
				(name "P11")
				(number "11")
			)
			(pin passive line
				(at -24.13 1.27 0)
				(length 7.62)
				(name "P12")
				(number "12")
			)
			(pin passive line
				(at -24.13 -1.27 0)
				(length 7.62)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -24.13 -3.81 0)
				(length 7.62)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -24.13 -6.35 0)
				(length 7.62)
				(name "P16")
				(number "16")
			)
			(pin passive line
				(at -24.13 -8.89 0)
				(length 7.62)
				(name "P17")
				(number "17")
			)
			(pin passive line
				(at -24.13 -11.43 0)
				(length 7.62)
				(name "P18")
				(number "18")
			)
			(pin passive line
				(at -24.13 -13.97 0)
				(length 7.62)
				(name "P19")
				(number "19")
			)
			(pin passive line
				(at -24.13 -16.51 0)
				(length 7.62)
				(name "P20")
				(number "20")
			)
			(pin passive line
				(at -24.13 -19.05 0)
				(length 7.62)
				(name "P21")
				(number "21")
			)
			(pin passive line
				(at -24.13 -21.59 0)
				(length 7.62)
				(name "P22")
				(number "22")
			)
			(pin passive line
				(at -24.13 -24.13 0)
				(length 7.62)
				(name "P23")
				(number "23")
			)
			(pin passive line
				(at -24.13 -26.67 0)
				(length 7.62)
				(name "P/TCLKIN")
				(number "27")
			)
			(pin passive line
				(at -24.13 -29.21 0)
				(length 7.62)
				(name "P28")
				(number "28")
			)
			(pin passive line
				(at -24.13 -31.75 0)
				(length 7.62)
				(name "P29")
				(number "29")
			)
			(pin passive line
				(at -24.13 -34.29 0)
				(length 7.62)
				(name "P30")
				(number "30")
			)
			(pin passive line
				(at -24.13 -36.83 0)
				(length 7.62)
				(name "P31")
				(number "31")
			)
			(pin passive line
				(at -24.13 -39.37 0)
				(length 7.62)
				(name "P32")
				(number "32")
			)
			(pin passive line
				(at -24.13 -41.91 0)
				(length 7.62)
				(name "P33")
				(number "33")
			)
			(pin passive line
				(at -24.13 -44.45 0)
				(length 7.62)
				(name "P34")
				(number "34")
			)
			(pin passive line
				(at -24.13 -46.99 0)
				(length 7.62)
				(name "P35")
				(number "35")
			)
			(pin passive line
				(at -24.13 -49.53 0)
				(length 7.62)
				(name "P36")
				(number "36")
			)
			(pin passive line
				(at -24.13 -52.07 0)
				(length 7.62)
				(name "P37")
				(number "37")
			)
			(pin passive line
				(at -24.13 -54.61 0)
				(length 7.62)
				(name "P39")
				(number "39")
			)
			(pin passive line
				(at 0 63.5 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "100")
			)
			(pin power_in line
				(at 0 63.5 270)
				(length 6.35)
				(name "VCC")
				(number "24")
			)
			(pin passive line
				(at 0 63.5 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "38")
			)
			(pin passive line
				(at 0 63.5 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin passive line
				(at 0 63.5 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "76")
			)
			(pin passive line
				(at 0 63.5 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "88")
			)
			(pin power_in line
				(at 0 -63.5 90)
				(length 6.35)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "50")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "74")
			)
			(pin passive line
				(at 24.13 54.61 180)
				(length 7.62)
				(name "P/RDY")
				(number "96")
			)
			(pin passive line
				(at 24.13 52.07 180)
				(length 7.62)
				(name "P95")
				(number "95")
			)
			(pin passive line
				(at 24.13 49.53 180)
				(length 7.62)
				(name "P94")
				(number "94")
			)
			(pin passive line
				(at 24.13 46.99 180)
				(length 7.62)
				(name "P93")
				(number "93")
			)
			(pin passive line
				(at 24.13 44.45 180)
				(length 7.62)
				(name "P92")
				(number "92")
			)
			(pin passive line
				(at 24.13 41.91 180)
				(length 7.62)
				(name "P91")
				(number "91")
			)
			(pin passive line
				(at 24.13 39.37 180)
				(length 7.62)
				(name "P90")
				(number "90")
			)
			(pin passive line
				(at 24.13 36.83 180)
				(length 7.62)
				(name "P98")
				(number "89")
			)
			(pin passive line
				(at 24.13 34.29 180)
				(length 7.62)
				(name "P87")
				(number "87")
			)
			(pin passive line
				(at 24.13 31.75 180)
				(length 7.62)
				(name "P86")
				(number "86")
			)
			(pin passive line
				(at 24.13 29.21 180)
				(length 7.62)
				(name "P85")
				(number "85")
			)
			(pin passive line
				(at 24.13 26.67 180)
				(length 7.62)
				(name "P84")
				(number "84")
			)
			(pin passive line
				(at 24.13 24.13 180)
				(length 7.62)
				(name "P83")
				(number "83")
			)
			(pin passive line
				(at 24.13 21.59 180)
				(length 7.62)
				(name "P82")
				(number "82")
			)
			(pin passive line
				(at 24.13 19.05 180)
				(length 7.62)
				(name "P81")
				(number "81")
			)
			(pin passive line
				(at 24.13 16.51 180)
				(length 7.62)
				(name "P80")
				(number "80")
			)
			(pin passive line
				(at 24.13 13.97 180)
				(length 7.62)
				(name "P/XO")
				(number "79")
			)
			(pin passive line
				(at 24.13 11.43 180)
				(length 7.62)
				(name "P78")
				(number "78")
			)
			(pin passive line
				(at 24.13 8.89 180)
				(length 7.62)
				(name "P/XI")
				(number "73")
			)
			(pin passive line
				(at 24.13 6.35 180)
				(length 7.62)
				(name "P72")
				(number "72")
			)
			(pin passive line
				(at 24.13 3.81 180)
				(length 7.62)
				(name "P71")
				(number "71")
			)
			(pin passive line
				(at 24.13 1.27 180)
				(length 7.62)
				(name "P70")
				(number "70")
			)
			(pin passive line
				(at 24.13 -1.27 180)
				(length 7.62)
				(name "P69")
				(number "69")
			)
			(pin passive line
				(at 24.13 -3.81 180)
				(length 7.62)
				(name "P68")
				(number "68")
			)
			(pin passive line
				(at 24.13 -6.35 180)
				(length 7.62)
				(name "P67")
				(number "67")
			)
			(pin passive line
				(at 24.13 -8.89 180)
				(length 7.62)
				(name "P66")
				(number "66")
			)
			(pin passive line
				(at 24.13 -11.43 180)
				(length 7.62)
				(name "P65")
				(number "65")
			)
			(pin passive line
				(at 24.13 -13.97 180)
				(length 7.62)
				(name "P64")
				(number "64")
			)
			(pin passive line
				(at 24.13 -16.51 180)
				(length 7.62)
				(name "P/INIT")
				(number "62")
			)
			(pin passive line
				(at 24.13 -19.05 180)
				(length 7.62)
				(name "P61")
				(number "61")
			)
			(pin passive line
				(at 24.13 -21.59 180)
				(length 7.62)
				(name "P60")
				(number "60")
			)
			(pin passive line
				(at 24.13 -24.13 180)
				(length 7.62)
				(name "P59")
				(number "59")
			)
			(pin passive line
				(at 24.13 -26.67 180)
				(length 7.62)
				(name "P58")
				(number "58")
			)
			(pin passive line
				(at 24.13 -29.21 180)
				(length 7.62)
				(name "P57")
				(number "57")
			)
			(pin passive line
				(at 24.13 -31.75 180)
				(length 7.62)
				(name "P55")
				(number "55")
			)
			(pin passive line
				(at 24.13 -34.29 180)
				(length 7.62)
				(name "P48")
				(number "48")
			)
			(pin passive line
				(at 24.13 -36.83 180)
				(length 7.62)
				(name "P47")
				(number "47")
			)
			(pin passive line
				(at 24.13 -39.37 180)
				(length 7.62)
				(name "P46")
				(number "46")
			)
			(pin passive line
				(at 24.13 -41.91 180)
				(length 7.62)
				(name "P45")
				(number "45")
			)
			(pin passive line
				(at 24.13 -44.45 180)
				(length 7.62)
				(name "P44")
				(number "44")
			)
			(pin passive line
				(at 24.13 -46.99 180)
				(length 7.62)
				(name "P43")
				(number "43")
			)
			(pin passive line
				(at 24.13 -49.53 180)
				(length 7.62)
				(name "P42")
				(number "42")
			)
			(pin passive line
				(at 24.13 -52.07 180)
				(length 7.62)
				(name "P41")
				(number "41")
			)
			(pin passive line
				(at 24.13 -54.61 180)
				(length 7.62)
				(name "P40")
				(number "40")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC3S1400A-FG484"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "XC3S1400A-FG484"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA484"
			(at 0 0 0)
		)
		(symbol "XC3S1400A-FG484_0_1")
		(symbol "XC3S1400A-FG484_1_1"
			(pin input line
				(at -78.74 129.54 0)
				(length 7.62)
				(name "TMS")
				(number "D4")
			)
			(pin output line
				(at -78.74 127 0)
				(length 7.62)
				(name "TDO")
				(number "E19")
			)
			(pin input line
				(at -78.74 124.46 0)
				(length 7.62)
				(name "TDI")
				(number "F5")
			)
			(pin input line
				(at -78.74 121.92 0)
				(length 7.62)
				(name "TCK")
				(number "A21")
			)
			(pin bidirectional line
				(at -78.74 116.84 0)
				(length 7.62)
				(name "DONE")
				(number "Y19")
			)
			(pin bidirectional line
				(at -78.74 114.3 0)
				(length 7.62)
				(name "PROG_B")
				(number "C4")
			)
			(pin bidirectional line
				(at -78.74 109.22 0)
				(length 7.62)
				(name "IO_L01N_0")
				(number "D18")
			)
			(pin bidirectional line
				(at -78.74 106.68 0)
				(length 7.62)
				(name "IO_L01P_0")
				(number "E17")
			)
			(pin bidirectional line
				(at -78.74 104.14 0)
				(length 7.62)
				(name "IO_L02N_0")
				(number "C19")
			)
			(pin bidirectional line
				(at -78.74 101.6 0)
				(length 7.62)
				(name "IO_L02P_0/VREF_0")
				(number "D19")
			)
			(pin bidirectional line
				(at -78.74 99.06 0)
				(length 7.62)
				(name "IO_L03N_0")
				(number "A20")
			)
			(pin bidirectional line
				(at -78.74 96.52 0)
				(length 7.62)
				(name "IO_L03P_0")
				(number "B20")
			)
			(pin bidirectional line
				(at -78.74 93.98 0)
				(length 7.62)
				(name "IO_L04N_0")
				(number "F15")
			)
			(pin bidirectional line
				(at -78.74 91.44 0)
				(length 7.62)
				(name "IO_L04P_0")
				(number "E15")
			)
			(pin bidirectional line
				(at -78.74 88.9 0)
				(length 7.62)
				(name "IO_L05N_0")
				(number "A18")
			)
			(pin bidirectional line
				(at -78.74 86.36 0)
				(length 7.62)
				(name "IO_L05P_0")
				(number "C18")
			)
			(pin bidirectional line
				(at -78.74 83.82 0)
				(length 7.62)
				(name "IO_L06N_0")
				(number "A19")
			)
			(pin bidirectional line
				(at -78.74 81.28 0)
				(length 7.62)
				(name "IO_L06P_0/VREF_0")
				(number "B19")
			)
			(pin bidirectional line
				(at -78.74 78.74 0)
				(length 7.62)
				(name "IO_L07N_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -78.74 76.2 0)
				(length 7.62)
				(name "IO_L07P_0")
				(number "D17")
			)
			(pin bidirectional line
				(at -78.74 73.66 0)
				(length 7.62)
				(name "IO_L08N_0")
				(number "C16")
			)
			(pin bidirectional line
				(at -78.74 71.12 0)
				(length 7.62)
				(name "IO_L08P_0")
				(number "D16")
			)
			(pin bidirectional line
				(at -78.74 68.58 0)
				(length 7.62)
				(name "IO_L09N_0")
				(number "E14")
			)
			(pin bidirectional line
				(at -78.74 66.04 0)
				(length 7.62)
				(name "IO_L09P_0")
				(number "C14")
			)
			(pin bidirectional line
				(at -78.74 63.5 0)
				(length 7.62)
				(name "IO_L10N_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -78.74 60.96 0)
				(length 7.62)
				(name "IO_L10P_0")
				(number "B17")
			)
			(pin bidirectional line
				(at -78.74 58.42 0)
				(length 7.62)
				(name "IO_L11N_0")
				(number "C15")
			)
			(pin bidirectional line
				(at -78.74 55.88 0)
				(length 7.62)
				(name "IO_L11P_0")
				(number "D15")
			)
			(pin bidirectional line
				(at -78.74 53.34 0)
				(length 7.62)
				(name "IO_L12N_0/VREF_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -78.74 50.8 0)
				(length 7.62)
				(name "IO_L12P_0")
				(number "A16")
			)
			(pin bidirectional line
				(at -78.74 48.26 0)
				(length 7.62)
				(name "IO_L13N_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -78.74 45.72 0)
				(length 7.62)
				(name "IO_L13P_0")
				(number "B15")
			)
			(pin bidirectional line
				(at -78.74 43.18 0)
				(length 7.62)
				(name "IO_L14N_0")
				(number "E13")
			)
			(pin bidirectional line
				(at -78.74 40.64 0)
				(length 7.62)
				(name "IO_L14P_0")
				(number "F13")
			)
			(pin bidirectional line
				(at -78.74 38.1 0)
				(length 7.62)
				(name "IO_L15N_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -78.74 35.56 0)
				(length 7.62)
				(name "IO_L15P_0")
				(number "D13")
			)
			(pin bidirectional line
				(at -78.74 33.02 0)
				(length 7.62)
				(name "IO_L16N_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -78.74 30.48 0)
				(length 7.62)
				(name "IO_L16P_0")
				(number "B13")
			)
			(pin bidirectional line
				(at -78.74 27.94 0)
				(length 7.62)
				(name "IO_L17N_0/GCLK5")
				(number "E12")
			)
			(pin bidirectional line
				(at -78.74 25.4 0)
				(length 7.62)
				(name "IO_L17P_0/GCLK4")
				(number "C12")
			)
			(pin bidirectional line
				(at -78.74 22.86 0)
				(length 7.62)
				(name "IO_L18N_0/GCLK7")
				(number "A11")
			)
			(pin bidirectional line
				(at -78.74 20.32 0)
				(length 7.62)
				(name "IO_L18P_0/GCLK6")
				(number "A12")
			)
			(pin bidirectional line
				(at -78.74 17.78 0)
				(length 7.62)
				(name "IO_L19N_0/GCLK9")
				(number "C11")
			)
			(pin bidirectional line
				(at -78.74 15.24 0)
				(length 7.62)
				(name "IO_L19P_0/GCLK8")
				(number "B11")
			)
			(pin bidirectional line
				(at -78.74 12.7 0)
				(length 7.62)
				(name "IO_L20N_0/GCLK11")
				(number "E11")
			)
			(pin bidirectional line
				(at -78.74 10.16 0)
				(length 7.62)
				(name "IO_L20P_0/GCLK10")
				(number "D11")
			)
			(pin bidirectional line
				(at -78.74 7.62 0)
				(length 7.62)
				(name "IO_L21N_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -78.74 5.08 0)
				(length 7.62)
				(name "IO_L21P_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -78.74 2.54 0)
				(length 7.62)
				(name "IO_L22N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -78.74 0 0)
				(length 7.62)
				(name "IO_L22P_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -78.74 -2.54 0)
				(length 7.62)
				(name "IO_L23N_0")
				(number "E10")
			)
			(pin bidirectional line
				(at -78.74 -5.08 0)
				(length 7.62)
				(name "IO_L23P_0")
				(number "D10")
			)
			(pin bidirectional line
				(at -78.74 -7.62 0)
				(length 7.62)
				(name "IO_L24N_0/VREF_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -78.74 -10.16 0)
				(length 7.62)
				(name "IO_L24P_0")
				(number "B9")
			)
			(pin bidirectional line
				(at -78.74 -12.7 0)
				(length 7.62)
				(name "IO_L25N_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -78.74 -15.24 0)
				(length 7.62)
				(name "IO_L25P_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -78.74 -17.78 0)
				(length 7.62)
				(name "IO_L26N_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -78.74 -20.32 0)
				(length 7.62)
				(name "IO_L26P_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -78.74 -22.86 0)
				(length 7.62)
				(name "IO_L27N_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -78.74 -25.4 0)
				(length 7.62)
				(name "IO_L27P_0")
				(number "D7")
			)
			(pin bidirectional line
				(at -78.74 -27.94 0)
				(length 7.62)
				(name "IO_L28N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -78.74 -30.48 0)
				(length 7.62)
				(name "IO_L28P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -78.74 -33.02 0)
				(length 7.62)
				(name "IO_L29N_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -78.74 -35.56 0)
				(length 7.62)
				(name "IO_L29P_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -78.74 -38.1 0)
				(length 7.62)
				(name "IO_L30N_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -78.74 -40.64 0)
				(length 7.62)
				(name "IO_L30P_0")
				(number "E9")
			)
			(pin bidirectional line
				(at -78.74 -43.18 0)
				(length 7.62)
				(name "IO_L31N_0")
				(number "B4")
			)
			(pin bidirectional line
				(at -78.74 -45.72 0)
				(length 7.62)
				(name "IO_L31P_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -78.74 -48.26 0)
				(length 7.62)
				(name "IO_L32N_0")
				(number "D5")
			)
			(pin bidirectional line
				(at -78.74 -50.8 0)
				(length 7.62)
				(name "IO_L32P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -78.74 -53.34 0)
				(length 7.62)
				(name "IO_L33N_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -78.74 -55.88 0)
				(length 7.62)
				(name "IO_L33P_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -78.74 -58.42 0)
				(length 7.62)
				(name "IO-L34N_0")
				(number "F8")
			)
			(pin bidirectional line
				(at -78.74 -60.96 0)
				(length 7.62)
				(name "IO_L34P_0")
				(number "E7")
			)
			(pin bidirectional line
				(at -78.74 -63.5 0)
				(length 7.62)
				(name "IO_L35N_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -78.74 -66.04 0)
				(length 7.62)
				(name "IO_L35P_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -78.74 -68.58 0)
				(length 7.62)
				(name "IO_L36N_0/PUDC_B")
				(number "A2")
			)
			(pin bidirectional line
				(at -78.74 -71.12 0)
				(length 7.62)
				(name "IO_L36P_0/VREF_0")
				(number "B2")
			)
			(pin input line
				(at -78.74 -73.66 0)
				(length 7.62)
				(name "IP_0")
				(number "E16")
			)
			(pin input line
				(at -78.74 -76.2 0)
				(length 7.62)
				(name "IP_0")
				(number "E8")
			)
			(pin input line
				(at -78.74 -78.74 0)
				(length 7.62)
				(name "IP_0")
				(number "F10")
			)
			(pin input line
				(at -78.74 -81.28 0)
				(length 7.62)
				(name "IP_0")
				(number "F12")
			)
			(pin input line
				(at -78.74 -83.82 0)
				(length 7.62)
				(name "IP_0")
				(number "F16")
			)
			(pin input line
				(at -78.74 -86.36 0)
				(length 7.62)
				(name "IP_0")
				(number "G10")
			)
			(pin input line
				(at -78.74 -88.9 0)
				(length 7.62)
				(name "IP_0")
				(number "G11")
			)
			(pin input line
				(at -78.74 -91.44 0)
				(length 7.62)
				(name "IP_0")
				(number "G12")
			)
			(pin input line
				(at -78.74 -93.98 0)
				(length 7.62)
				(name "IP_0")
				(number "G13")
			)
			(pin input line
				(at -78.74 -96.52 0)
				(length 7.62)
				(name "IP_0")
				(number "G14")
			)
			(pin input line
				(at -78.74 -99.06 0)
				(length 7.62)
				(name "IP_0")
				(number "G15")
			)
			(pin input line
				(at -78.74 -101.6 0)
				(length 7.62)
				(name "IP_0")
				(number "G16")
			)
			(pin input line
				(at -78.74 -104.14 0)
				(length 7.62)
				(name "IP_0")
				(number "G7")
			)
			(pin input line
				(at -78.74 -106.68 0)
				(length 7.62)
				(name "IP_0")
				(number "G9")
			)
			(pin input line
				(at -78.74 -109.22 0)
				(length 7.62)
				(name "IP_0")
				(number "H10")
			)
			(pin input line
				(at -78.74 -111.76 0)
				(length 7.62)
				(name "IP_0")
				(number "H13")
			)
			(pin input line
				(at -78.74 -114.3 0)
				(length 7.62)
				(name "IP_0")
				(number "H14")
			)
			(pin input line
				(at -78.74 -116.84 0)
				(length 7.62)
				(name "IP_0/VREF_0")
				(number "G8")
			)
			(pin input line
				(at -78.74 -119.38 0)
				(length 7.62)
				(name "IP_0/VREF_0")
				(number "H12")
			)
			(pin input line
				(at -78.74 -121.92 0)
				(length 7.62)
				(name "IP_0/VREF_0")
				(number "H9")
			)
			(pin power_in line
				(at -66.04 -140.97 90)
				(length 7.62)
				(name "GND")
				(number "A1")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "A22")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "AA11")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "AA16")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "AA7")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "AB1")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "AB22")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "B12")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "B16")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "B7")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "C20")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "C3")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "D14")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "D9")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "F11")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "F17")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "F6")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "G2")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "G21")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "J11")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "J13")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "J14")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "J19")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "J4")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "J9")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "K10")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "K12")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "L11")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "L13")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "L17")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "L2")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "L6")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "L9")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "M10")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "M12")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "M14")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "M21")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "N11")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "N13")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "P10")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "P14")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "P19")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "P4")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "P9")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "T12")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "T2")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "T21")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "U17")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "U6")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "W10")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "W14")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "Y20")
			)
			(pin passive line
				(at -66.04 -140.97 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "Y3")
			)
			(pin power_in line
				(at -60.96 140.97 270)
				(length 7.62)
				(name "VCCO0")
				(number "B10")
			)
			(pin power_in line
				(at -58.42 140.97 270)
				(length 7.62)
				(name "VCCO0")
				(number "B14")
			)
			(pin power_in line
				(at -55.88 140.97 270)
				(length 7.62)
				(name "VCCO0")
				(number "B18")
			)
			(pin power_in line
				(at -53.34 140.97 270)
				(length 7.62)
				(name "VCCO0")
				(number "B5")
			)
			(pin power_in line
				(at -50.8 140.97 270)
				(length 7.62)
				(name "VCCO0")
				(number "F14")
			)
			(pin power_in line
				(at -48.26 140.97 270)
				(length 7.62)
				(name "VCCO0")
				(number "F9")
			)
			(pin power_in line
				(at -34.29 140.97 270)
				(length 7.62)
				(name "VCCAUX")
				(number "D12")
			)
			(pin power_in line
				(at -31.75 140.97 270)
				(length 7.62)
				(name "VCCAUX")
				(number "E18")
			)
			(pin power_in line
				(at -29.21 140.97 270)
				(length 7.62)
				(name "VCCAUX")
				(number "E5")
			)
			(pin power_in line
				(at -26.67 140.97 270)
				(length 7.62)
				(name "VCCAUX")
				(number "H11")
			)
			(pin power_in line
				(at -24.13 140.97 270)
				(length 7.62)
				(name "VCCAUX")
				(number "L4")
			)
			(pin power_in line
				(at -21.59 140.97 270)
				(length 7.62)
				(name "VCCAUX")
				(number "M19")
			)
			(pin power_in line
				(at -19.05 140.97 270)
				(length 7.62)
				(name "VCCAUX")
				(number "P11")
			)
			(pin power_in line
				(at -16.51 140.97 270)
				(length 7.62)
				(name "VCCAUX")
				(number "V18")
			)
			(pin power_in line
				(at -13.97 140.97 270)
				(length 7.62)
				(name "VCCAUX")
				(number "V5")
			)
			(pin power_in line
				(at -11.43 140.97 270)
				(length 7.62)
				(name "VCCAUX")
				(number "W11")
			)
			(pin power_in line
				(at 0 140.97 270)
				(length 7.62)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 2.54 140.97 270)
				(length 7.62)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 5.08 140.97 270)
				(length 7.62)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 7.62 140.97 270)
				(length 7.62)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 10.16 140.97 270)
				(length 7.62)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 12.7 140.97 270)
				(length 7.62)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 15.24 140.97 270)
				(length 7.62)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 17.78 140.97 270)
				(length 7.62)
				(name "VCCINT")
				(number "L14")
			)
			(pin passive line
				(at 20.32 140.97 270)
				(length 7.62)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 22.86 140.97 270)
				(length 7.62)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 140.97 270)
				(length 7.62)
				(name "VCCINT")
				(number "M9")
			)
			(pin power_in line
				(at 27.94 140.97 270)
				(length 7.62)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 30.48 140.97 270)
				(length 7.62)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 33.02 140.97 270)
				(length 7.62)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 35.56 140.97 270)
				(length 7.62)
				(name "VCCINT")
				(number "P13")
			)
			(pin passive line
				(at 48.26 140.97 270)
				(length 7.62)
				(name "VCCO3")
				(number "E2")
			)
			(pin power_in line
				(at 50.8 140.97 270)
				(length 7.62)
				(name "VCCO3")
				(number "J2")
			)
			(pin power_in line
				(at 53.34 140.97 270)
				(length 7.62)
				(name "VCCO3")
				(number "J6")
			)
			(pin power_in line
				(at 55.88 140.97 270)
				(length 7.62)
				(name "VCCO3")
				(number "N2")
			)
			(pin power_in line
				(at 58.42 140.97 270)
				(length 7.62)
				(name "VCCO3")
				(number "P6")
			)
			(pin power_in line
				(at 60.96 140.97 270)
				(length 7.62)
				(name "VCCO3")
				(number "V2")
			)
			(pin input line
				(at 78.74 114.3 180)
				(length 7.62)
				(name "IP_L46P_3")
				(number "R7")
			)
			(pin input line
				(at 78.74 111.76 180)
				(length 7.62)
				(name "IP_L46N_3/VREF_3")
				(number "T6")
			)
			(pin input line
				(at 78.74 109.22 180)
				(length 7.62)
				(name "IP_L39P_3")
				(number "P7")
			)
			(pin input line
				(at 78.74 106.68 180)
				(length 7.62)
				(name "IP_L39N_3")
				(number "R8")
			)
			(pin input line
				(at 78.74 104.14 180)
				(length 7.62)
				(name "IP_L35P_3")
				(number "N7")
			)
			(pin input line
				(at 78.74 101.6 180)
				(length 7.62)
				(name "IP_L35N_3")
				(number "P8")
			)
			(pin input line
				(at 78.74 99.06 180)
				(length 7.62)
				(name "IP_L31P_3")
				(number "N6")
			)
			(pin input line
				(at 78.74 96.52 180)
				(length 7.62)
				(name "IP_L31N_3")
				(number "N5")
			)
			(pin input line
				(at 78.74 93.98 180)
				(length 7.62)
				(name "IP_L27P_3")
				(number "N8")
			)
			(pin input line
				(at 78.74 91.44 180)
				(length 7.62)
				(name "IP_L27N_3")
				(number "N9")
			)
			(pin input line
				(at 78.74 88.9 180)
				(length 7.62)
				(name "IP_L23P_3")
				(number "M7")
			)
			(pin input line
				(at 78.74 86.36 180)
				(length 7.62)
				(name "IP_L23N_3")
				(number "M6")
			)
			(pin input line
				(at 78.74 83.82 180)
				(length 7.62)
				(name "IP_L19P_3")
				(number "L7")
			)
			(pin input line
				(at 78.74 81.28 180)
				(length 7.62)
				(name "IP_L19N_3")
				(number "M8")
			)
			(pin input line
				(at 78.74 78.74 180)
				(length 7.62)
				(name "IP_L15P_3")
				(number "K7")
			)
			(pin input line
				(at 78.74 76.2 180)
				(length 7.62)
				(name "IP_L15N_3/VREF_3")
				(number "L8")
			)
			(pin input line
				(at 78.74 73.66 180)
				(length 7.62)
				(name "IP_L11P_3")
				(number "J7")
			)
			(pin input line
				(at 78.74 71.12 180)
				(length 7.62)
				(name "IP_L11N_3")
				(number "K8")
			)
			(pin input line
				(at 78.74 68.58 180)
				(length 7.62)
				(name "IP_L04P_3")
				(number "H8")
			)
			(pin input line
				(at 78.74 66.04 180)
				(length 7.62)
				(name "IP_L04N_3/VREF_3")
				(number "H7")
			)
			(pin input line
				(at 78.74 63.5 180)
				(length 7.62)
				(name "IP_3/VREF_3")
				(number "R6")
			)
			(pin input line
				(at 78.74 60.96 180)
				(length 7.62)
				(name "IP_3/VREF_3")
				(number "J8")
			)
			(pin bidirectional line
				(at 78.74 58.42 180)
				(length 7.62)
				(name "IO_L45P_3")
				(number "AA1")
			)
			(pin bidirectional line
				(at 78.74 55.88 180)
				(length 7.62)
				(name "IO_L45N_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 78.74 53.34 180)
				(length 7.62)
				(name "IO_L44P_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 78.74 50.8 180)
				(length 7.62)
				(name "IO_L44N_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 78.74 48.26 180)
				(length 7.62)
				(name "IO_L43P_3")
				(number "V4")
			)
			(pin bidirectional line
				(at 78.74 45.72 180)
				(length 7.62)
				(name "IO_L43N_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 78.74 43.18 180)
				(length 7.62)
				(name "IO_L42P_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 78.74 40.64 180)
				(length 7.62)
				(name "IO_L42N_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 78.74 38.1 180)
				(length 7.62)
				(name "IO_L41P_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 78.74 35.56 180)
				(length 7.62)
				(name "IO_L41N_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 78.74 33.02 180)
				(length 7.62)
				(name "IO_L40P_3")
				(number "T5")
			)
			(pin bidirectional line
				(at 78.74 30.48 180)
				(length 7.62)
				(name "IO_L40N_3")
				(number "U5")
			)
			(pin bidirectional line
				(at 78.74 27.94 180)
				(length 7.62)
				(name "IO_L38P_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 78.74 25.4 180)
				(length 7.62)
				(name "IO_L38N_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 78.74 22.86 180)
				(length 7.62)
				(name "IO_L37P_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 78.74 20.32 180)
				(length 7.62)
				(name "IO_L37N_3")
				(number "U2")
			)
			(pin input line
				(at 78.74 17.78 180)
				(length 7.62)
				(name "IO_L36P_3/VREF_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 78.74 15.24 180)
				(length 7.62)
				(name "IO_L36N_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 78.74 12.7 180)
				(length 7.62)
				(name "IO_L34P_3")
				(number "R5")
			)
			(pin bidirectional line
				(at 78.74 10.16 180)
				(length 7.62)
				(name "IO_L34N_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 78.74 7.62 180)
				(length 7.62)
				(name "IO_L33P_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 78.74 5.08 180)
				(length 7.62)
				(name "IO_L33N_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 78.74 2.54 180)
				(length 7.62)
				(name "IO_L32P_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 78.74 0 180)
				(length 7.62)
				(name "IO_L32N_3")
				(number "R2")
			)
			(pin bidirectional line
				(at 78.74 -2.54 180)
				(length 7.62)
				(name "IO_L30P_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 78.74 -5.08 180)
				(length 7.62)
				(name "IO_L30N_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 78.74 -7.62 180)
				(length 7.62)
				(name "IO_L29P_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 78.74 -10.16 180)
				(length 7.62)
				(name "IO_L29N_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 78.74 -12.7 180)
				(length 7.62)
				(name "IO_L28P_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 78.74 -15.24 180)
				(length 7.62)
				(name "IO_L28N_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 78.74 -17.78 180)
				(length 7.62)
				(name "IO_L26P_3/VREF_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 78.74 -20.32 180)
				(length 7.62)
				(name "IO_L26N_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 78.74 -22.86 180)
				(length 7.62)
				(name "IO_L25P_3/TRDY2/LHCLK6")
				(number "M3")
			)
			(pin bidirectional line
				(at 78.74 -25.4 180)
				(length 7.62)
				(name "IO_L25N_3/LHCLK7")
				(number "M4")
			)
			(pin bidirectional line
				(at 78.74 -27.94 180)
				(length 7.62)
				(name "IO_L24P_3/LHCLK4")
				(number "M1")
			)
			(pin bidirectional line
				(at 78.74 -30.48 180)
				(length 7.62)
				(name "IO_L24N_3/LHCLK5")
				(number "M2")
			)
			(pin bidirectional line
				(at 78.74 -33.02 180)
				(length 7.62)
				(name "IO_L22P_3/LHCLK2")
				(number "K1")
			)
			(pin bidirectional line
				(at 78.74 -35.56 180)
				(length 7.62)
				(name "IO_L22N_3/IRDY2/LHCLK3")
				(number "L1")
			)
			(pin bidirectional line
				(at 78.74 -38.1 180)
				(length 7.62)
				(name "IO_L21P_3/LHCLK0")
				(number "L5")
			)
			(pin bidirectional line
				(at 78.74 -40.64 180)
				(length 7.62)
				(name "IO_L21N_3/LHCLK1")
				(number "L3")
			)
			(pin bidirectional line
				(at 78.74 -43.18 180)
				(length 7.62)
				(name "IO_L20P_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 78.74 -45.72 180)
				(length 7.62)
				(name "IO_L20N_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 78.74 -48.26 180)
				(length 7.62)
				(name "IO_L18P_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 78.74 -50.8 180)
				(length 7.62)
				(name "IO_L18N_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 78.74 -53.34 180)
				(length 7.62)
				(name "IO_L17P_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 78.74 -55.88 180)
				(length 7.62)
				(name "IO_L17N_3/VREF_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 78.74 -58.42 180)
				(length 7.62)
				(name "IO_L16P_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 78.74 -60.96 180)
				(length 7.62)
				(name "IO_L16N_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 78.74 -63.5 180)
				(length 7.62)
				(name "IO_L14P_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 78.74 -66.04 180)
				(length 7.62)
				(name "IO_L14N_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 78.74 -68.58 180)
				(length 7.62)
				(name "IO_L13P_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 78.74 -71.12 180)
				(length 7.62)
				(name "IO_L13N_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 78.74 -73.66 180)
				(length 7.62)
				(name "IO_L12P_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 78.74 -76.2 180)
				(length 7.62)
				(name "IO_L12N_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 78.74 -78.74 180)
				(length 7.62)
				(name "IO_L10P_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 78.74 -81.28 180)
				(length 7.62)
				(name "IO_L10N_3")
				(number "J5")
			)
			(pin bidirectional line
				(at 78.74 -83.82 180)
				(length 7.62)
				(name "IO_L09P_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 78.74 -86.36 180)
				(length 7.62)
				(name "IO_L09N_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 78.74 -88.9 180)
				(length 7.62)
				(name "IO_L08P_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 78.74 -91.44 180)
				(length 7.62)
				(name "IO_L08N_3")
				(number "G4")
			)
			(pin bidirectional line
				(at 78.74 -93.98 180)
				(length 7.62)
				(name "IO_L07P_3")
				(number "F4")
			)
			(pin bidirectional line
				(at 78.74 -96.52 180)
				(length 7.62)
				(name "IO_L07N_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 78.74 -99.06 180)
				(length 7.62)
				(name "IO_L06P_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 78.74 -101.6 180)
				(length 7.62)
				(name "IO_L06N_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 78.74 -104.14 180)
				(length 7.62)
				(name "IO_L05P_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 78.74 -106.68 180)
				(length 7.62)
				(name "IO_L05N_3")
				(number "G5")
			)
			(pin bidirectional line
				(at 78.74 -109.22 180)
				(length 7.62)
				(name "IO_L03P_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 78.74 -111.76 180)
				(length 7.62)
				(name "IO_L03N_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 78.74 -114.3 180)
				(length 7.62)
				(name "IO_L02P_3")
				(number "B1")
			)
			(pin bidirectional line
				(at 78.74 -116.84 180)
				(length 7.62)
				(name "IO_L02N_3")
				(number "C2")
			)
			(pin bidirectional line
				(at 78.74 -119.38 180)
				(length 7.62)
				(name "IO_L01P_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 78.74 -121.92 180)
				(length 7.62)
				(name "IO_L01N_3")
				(number "D2")
			)
		)
		(symbol "XC3S1400A-FG484_2_1"
			(pin bidirectional line
				(at -78.74 118.11 0)
				(length 7.62)
				(name "IO_L01N_1/LDC2")
				(number "Y21")
			)
			(pin bidirectional line
				(at -78.74 115.57 0)
				(length 7.62)
				(name "IO_L01P_1/HDC")
				(number "AA22")
			)
			(pin bidirectional line
				(at -78.74 113.03 0)
				(length 7.62)
				(name "IO_L02N_1/LDC0")
				(number "W20")
			)
			(pin bidirectional line
				(at -78.74 110.49 0)
				(length 7.62)
				(name "IO_L02P_1/LDC1")
				(number "W19")
			)
			(pin bidirectional line
				(at -78.74 107.95 0)
				(length 7.62)
				(name "IO_L03N_1/A1")
				(number "T18")
			)
			(pin bidirectional line
				(at -78.74 105.41 0)
				(length 7.62)
				(name "IO_L03P_1/A0")
				(number "T17")
			)
			(pin bidirectional line
				(at -78.74 102.87 0)
				(length 7.62)
				(name "IO_L05N_1")
				(number "W21")
			)
			(pin bidirectional line
				(at -78.74 100.33 0)
				(length 7.62)
				(name "IO_L05P_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at -78.74 97.79 0)
				(length 7.62)
				(name "IO_L06N_1")
				(number "V20")
			)
			(pin bidirectional line
				(at -78.74 95.25 0)
				(length 7.62)
				(name "IO_L06P_1")
				(number "V19")
			)
			(pin bidirectional line
				(at -78.74 92.71 0)
				(length 7.62)
				(name "IO_L07N_1")
				(number "V22")
			)
			(pin bidirectional line
				(at -78.74 90.17 0)
				(length 7.62)
				(name "IO_L07P_1")
				(number "W22")
			)
			(pin bidirectional line
				(at -78.74 87.63 0)
				(length 7.62)
				(name "IO_L09N_1")
				(number "U21")
			)
			(pin bidirectional line
				(at -78.74 85.09 0)
				(length 7.62)
				(name "IO_L09P_1")
				(number "U22")
			)
			(pin bidirectional line
				(at -78.74 82.55 0)
				(length 7.62)
				(name "IO_L10N_1")
				(number "U19")
			)
			(pin bidirectional line
				(at -78.74 80.01 0)
				(length 7.62)
				(name "IO_L10P_1")
				(number "U20")
			)
			(pin bidirectional line
				(at -78.74 77.47 0)
				(length 7.62)
				(name "IO_L11N_1")
				(number "T22")
			)
			(pin bidirectional line
				(at -78.74 74.93 0)
				(length 7.62)
				(name "IO_L11P_1")
				(number "T20")
			)
			(pin bidirectional line
				(at -78.74 72.39 0)
				(length 7.62)
				(name "IO_L13N_1")
				(number "T19")
			)
			(pin bidirectional line
				(at -78.74 69.85 0)
				(length 7.62)
				(name "IO_L13P_1")
				(number "R20")
			)
			(pin bidirectional line
				(at -78.74 67.31 0)
				(length 7.62)
				(name "IO_L14N_1")
				(number "R22")
			)
			(pin bidirectional line
				(at -78.74 64.77 0)
				(length 7.62)
				(name "IO_L14P_1")
				(number "R21")
			)
			(pin bidirectional line
				(at -78.74 62.23 0)
				(length 7.62)
				(name "IO_L15N_1/VREF_1")
				(number "P22")
			)
			(pin bidirectional line
				(at -78.74 59.69 0)
				(length 7.62)
				(name "IO_L15P_1")
				(number "P20")
			)
			(pin bidirectional line
				(at -78.74 57.15 0)
				(length 7.62)
				(name "IO_L17N_1/A3")
				(number "P18")
			)
			(pin bidirectional line
				(at -78.74 54.61 0)
				(length 7.62)
				(name "IO_L17P_1/A2")
				(number "R19")
			)
			(pin bidirectional line
				(at -78.74 52.07 0)
				(length 7.62)
				(name "IO_L18N_1/A5")
				(number "N21")
			)
			(pin bidirectional line
				(at -78.74 49.53 0)
				(length 7.62)
				(name "IO_L18P_1/A4")
				(number "N22")
			)
			(pin bidirectional line
				(at -78.74 46.99 0)
				(length 7.62)
				(name "IO_L19N_1/A7")
				(number "N19")
			)
			(pin bidirectional line
				(at -78.74 44.45 0)
				(length 7.62)
				(name "IO_L19P_1/A6")
				(number "N20")
			)
			(pin bidirectional line
				(at -78.74 41.91 0)
				(length 7.62)
				(name "IO_L20N_1/A9")
				(number "N17")
			)
			(pin bidirectional line
				(at -78.74 39.37 0)
				(length 7.62)
				(name "IO_L20P_1/A8")
				(number "N18")
			)
			(pin bidirectional line
				(at -78.74 36.83 0)
				(length 7.62)
				(name "IO_L21N_1/RHCLK1")
				(number "L22")
			)
			(pin bidirectional line
				(at -78.74 34.29 0)
				(length 7.62)
				(name "IO_L21P_1/RHCLK0")
				(number "M22")
			)
			(pin bidirectional line
				(at -78.74 31.75 0)
				(length 7.62)
				(name "IO_L22N_1/TRDY1/RHCLK3")
				(number "L20")
			)
			(pin bidirectional line
				(at -78.74 29.21 0)
				(length 7.62)
				(name "IO_L22P_1/RHCLK2")
				(number "L21")
			)
			(pin bidirectional line
				(at -78.74 26.67 0)
				(length 7.62)
				(name "IO_L24N_1/RHCLK5")
				(number "M20")
			)
			(pin bidirectional line
				(at -78.74 24.13 0)
				(length 7.62)
				(name "IO_L24P_1/RHCLK4")
				(number "M18")
			)
			(pin bidirectional line
				(at -78.74 21.59 0)
				(length 7.62)
				(name "IO_L25N_1/RHCLK7")
				(number "K19")
			)
			(pin bidirectional line
				(at -78.74 19.05 0)
				(length 7.62)
				(name "IO_L25P_1/IRDY1/RHCLK6")
				(number "K20")
			)
			(pin bidirectional line
				(at -78.74 16.51 0)
				(length 7.62)
				(name "IO_L26N_1/A11")
				(number "J22")
			)
			(pin bidirectional line
				(at -78.74 13.97 0)
				(length 7.62)
				(name "IO_L26P_1/A10")
				(number "K22")
			)
			(pin bidirectional line
				(at -78.74 11.43 0)
				(length 7.62)
				(name "IO_L28N_1")
				(number "L19")
			)
			(pin bidirectional line
				(at -78.74 8.89 0)
				(length 7.62)
				(name "IO_L28P_1")
				(number "L18")
			)
			(pin bidirectional line
				(at -78.74 6.35 0)
				(length 7.62)
				(name "IO_L29N_1/A13")
				(number "J20")
			)
			(pin bidirectional line
				(at -78.74 3.81 0)
				(length 7.62)
				(name "IO_L29P_1/A12")
				(number "J21")
			)
			(pin bidirectional line
				(at -78.74 1.27 0)
				(length 7.62)
				(name "IO_L30N_1/A15")
				(number "G22")
			)
			(pin bidirectional line
				(at -78.74 -1.27 0)
				(length 7.62)
				(name "IO_L30P_1/A14")
				(number "H22")
			)
			(pin bidirectional line
				(at -78.74 -3.81 0)
				(length 7.62)
				(name "IO_L32N_1")
				(number "K18")
			)
			(pin bidirectional line
				(at -78.74 -6.35 0)
				(length 7.62)
				(name "IO_L32P_1")
				(number "K17")
			)
			(pin bidirectional line
				(at -78.74 -8.89 0)
				(length 7.62)
				(name "IO_L33N_1/A17")
				(number "H20")
			)
			(pin bidirectional line
				(at -78.74 -11.43 0)
				(length 7.62)
				(name "IO_L33P_1/A16")
				(number "H21")
			)
			(pin bidirectional line
				(at -78.74 -13.97 0)
				(length 7.62)
				(name "IO_L34N_1/A19")
				(number "F21")
			)
			(pin bidirectional line
				(at -78.74 -16.51 0)
				(length 7.62)
				(name "IO_L34P_1/A18")
				(number "F22")
			)
			(pin bidirectional line
				(at -78.74 -19.05 0)
				(length 7.62)
				(name "IO_L36N_1")
				(number "G20")
			)
			(pin bidirectional line
				(at -78.74 -21.59 0)
				(length 7.62)
				(name "IO_L36P_1")
				(number "G19")
			)
			(pin bidirectional line
				(at -78.74 -24.13 0)
				(length 7.62)
				(name "IO_L37N_1")
				(number "H19")
			)
			(pin bidirectional line
				(at -78.74 -26.67 0)
				(length 7.62)
				(name "IO_L37P_1")
				(number "J18")
			)
			(pin bidirectional line
				(at -78.74 -29.21 0)
				(length 7.62)
				(name "IO_L38N_1")
				(number "F20")
			)
			(pin bidirectional line
				(at -78.74 -31.75 0)
				(length 7.62)
				(name "IO_L38P_1")
				(number "E20")
			)
			(pin bidirectional line
				(at -78.74 -34.29 0)
				(length 7.62)
				(name "IO_L40N_1")
				(number "F18")
			)
			(pin bidirectional line
				(at -78.74 -36.83 0)
				(length 7.62)
				(name "IO_L40P_1")
				(number "F19")
			)
			(pin bidirectional line
				(at -78.74 -39.37 0)
				(length 7.62)
				(name "IO_L41N_1")
				(number "D22")
			)
			(pin bidirectional line
				(at -78.74 -41.91 0)
				(length 7.62)
				(name "IO_L41P_1")
				(number "E22")
			)
			(pin bidirectional line
				(at -78.74 -44.45 0)
				(length 7.62)
				(name "IO_L42N_1")
				(number "D20")
			)
			(pin bidirectional line
				(at -78.74 -46.99 0)
				(length 7.62)
				(name "IO_L42P_1")
				(number "D21")
			)
			(pin bidirectional line
				(at -78.74 -49.53 0)
				(length 7.62)
				(name "IO_L44N_1/A21")
				(number "C21")
			)
			(pin bidirectional line
				(at -78.74 -52.07 0)
				(length 7.62)
				(name "IO_L44P_1/A20")
				(number "C22")
			)
			(pin bidirectional line
				(at -78.74 -54.61 0)
				(length 7.62)
				(name "IO_L45N_1/A23")
				(number "B21")
			)
			(pin bidirectional line
				(at -78.74 -57.15 0)
				(length 7.62)
				(name "IO_L45P_1/A22")
				(number "B22")
			)
			(pin bidirectional line
				(at -78.74 -59.69 0)
				(length 7.62)
				(name "IO_L46N_1/A25")
				(number "G17")
			)
			(pin bidirectional line
				(at -78.74 -62.23 0)
				(length 7.62)
				(name "IO_L46P_1/A24")
				(number "G18")
			)
			(pin input line
				(at -78.74 -64.77 0)
				(length 7.62)
				(name "IP_L04N_1/VREF_1")
				(number "R16")
			)
			(pin input line
				(at -78.74 -67.31 0)
				(length 7.62)
				(name "IP_L04P_1")
				(number "R15")
			)
			(pin input line
				(at -78.74 -69.85 0)
				(length 7.62)
				(name "IP_L08N_1")
				(number "P16")
			)
			(pin input line
				(at -78.74 -72.39 0)
				(length 7.62)
				(name "IP_L08P_1")
				(number "P15")
			)
			(pin input line
				(at -78.74 -74.93 0)
				(length 7.62)
				(name "IP_L12N_1/VREF_1")
				(number "R18")
			)
			(pin input line
				(at -78.74 -77.47 0)
				(length 7.62)
				(name "IP_L12P_1")
				(number "R17")
			)
			(pin input line
				(at -78.74 -80.01 0)
				(length 7.62)
				(name "IP_L16N_1/VREF_1")
				(number "N16")
			)
			(pin input line
				(at -78.74 -82.55 0)
				(length 7.62)
				(name "IP_L16P_1")
				(number "N15")
			)
			(pin input line
				(at -78.74 -85.09 0)
				(length 7.62)
				(name "IP_L23N_1")
				(number "M16")
			)
			(pin input line
				(at -78.74 -87.63 0)
				(length 7.62)
				(name "IP_L23P_1")
				(number "M17")
			)
			(pin input line
				(at -78.74 -90.17 0)
				(length 7.62)
				(name "IP_L27N_1")
				(number "L16")
			)
			(pin input line
				(at -78.74 -92.71 0)
				(length 7.62)
				(name "IP_L27P_1/VREF_1")
				(number "M15")
			)
			(pin input line
				(at -78.74 -95.25 0)
				(length 7.62)
				(name "IP_L31N_1")
				(number "K16")
			)
			(pin input line
				(at -78.74 -97.79 0)
				(length 7.62)
				(name "IP_L31P_1")
				(number "L15")
			)
			(pin input line
				(at -78.74 -100.33 0)
				(length 7.62)
				(name "IP_L35N_1")
				(number "K15")
			)
			(pin input line
				(at -78.74 -102.87 0)
				(length 7.62)
				(name "IP_L35P_1/VREF_1")
				(number "K14")
			)
			(pin input line
				(at -78.74 -105.41 0)
				(length 7.62)
				(name "IP_L39N_1")
				(number "H18")
			)
			(pin input line
				(at -78.74 -107.95 0)
				(length 7.62)
				(name "IP_L39P_1")
				(number "H17")
			)
			(pin input line
				(at -78.74 -110.49 0)
				(length 7.62)
				(name "IP_L43N_1/VREF_1")
				(number "J15")
			)
			(pin input line
				(at -78.74 -113.03 0)
				(length 7.62)
				(name "IP_L43P_1")
				(number "J16")
			)
			(pin input line
				(at -78.74 -115.57 0)
				(length 7.62)
				(name "IP_L47N_1")
				(number "H15")
			)
			(pin input line
				(at -78.74 -118.11 0)
				(length 7.62)
				(name "IP_L47P_1/VREF_1")
				(number "H16")
			)
			(pin input line
				(at -78.74 -120.65 0)
				(length 7.62)
				(name "SUSPEND")
				(number "U18")
			)
			(pin power_in line
				(at -57.15 140.97 270)
				(length 7.62)
				(name "VCCO1")
				(number "E21")
			)
			(pin power_in line
				(at -54.61 140.97 270)
				(length 7.62)
				(name "VCCO1")
				(number "J17")
			)
			(pin power_in line
				(at -52.07 140.97 270)
				(length 7.62)
				(name "VCCO1")
				(number "K21")
			)
			(pin power_in line
				(at -49.53 140.97 270)
				(length 7.62)
				(name "VCCO1")
				(number "P17")
			)
			(pin power_in line
				(at -46.99 140.97 270)
				(length 7.62)
				(name "VCCO1")
				(number "P21")
			)
			(pin power_in line
				(at -44.45 140.97 270)
				(length 7.62)
				(name "VCCO1")
				(number "V21")
			)
			(pin power_in line
				(at 44.45 140.97 270)
				(length 7.62)
				(name "VCCO2")
				(number "AA13")
			)
			(pin power_in line
				(at 46.99 140.97 270)
				(length 7.62)
				(name "VCCO2")
				(number "AA18")
			)
			(pin power_in line
				(at 49.53 140.97 270)
				(length 7.62)
				(name "VCCO2")
				(number "AA5")
			)
			(pin power_in line
				(at 52.07 140.97 270)
				(length 7.62)
				(name "VCCO2")
				(number "AA9")
			)
			(pin passive line
				(at 54.61 140.97 270)
				(length 7.62)
				(name "VCCO2")
				(number "U14")
			)
			(pin power_in line
				(at 57.15 140.97 270)
				(length 7.62)
				(name "VCCO2")
				(number "U9")
			)
			(pin input line
				(at 78.74 118.11 180)
				(length 7.62)
				(name "IP_2/VREF_2")
				(number "V8")
			)
			(pin input line
				(at 78.74 115.57 180)
				(length 7.62)
				(name "IP_2/VREF_2")
				(number "T8")
			)
			(pin input line
				(at 78.74 113.03 180)
				(length 7.62)
				(name "IP_2/VREF_2")
				(number "T7")
			)
			(pin input line
				(at 78.74 110.49 180)
				(length 7.62)
				(name "IP_2/VREF_2")
				(number "T16")
			)
			(pin input line
				(at 78.74 107.95 180)
				(length 7.62)
				(name "IP_2/VREF_2")
				(number "T15")
			)
			(pin input line
				(at 78.74 105.41 180)
				(length 7.62)
				(name "IP_2/VREF_2")
				(number "T11")
			)
			(pin input line
				(at 78.74 102.87 180)
				(length 7.62)
				(name "IP_2/VREF_2")
				(number "T10")
			)
			(pin input line
				(at 78.74 100.33 180)
				(length 7.62)
				(name "IP_2/VREF_2")
				(number "R14")
			)
			(pin input line
				(at 78.74 97.79 180)
				(length 7.62)
				(name "IP_2/VREF_2")
				(number "R13")
			)
			(pin input line
				(at 78.74 95.25 180)
				(length 7.62)
				(name "IP_2/VREF_2")
				(number "R12")
			)
			(pin input line
				(at 78.74 92.71 180)
				(length 7.62)
				(name "IP_2")
				(number "V7")
			)
			(pin input line
				(at 78.74 90.17 180)
				(length 7.62)
				(name "IP_2")
				(number "U8")
			)
			(pin input line
				(at 78.74 87.63 180)
				(length 7.62)
				(name "IP_2")
				(number "U7")
			)
			(pin input line
				(at 78.74 85.09 180)
				(length 7.62)
				(name "IP_2")
				(number "U16")
			)
			(pin input line
				(at 78.74 82.55 180)
				(length 7.62)
				(name "IP_2")
				(number "U15")
			)
			(pin input line
				(at 78.74 80.01 180)
				(length 7.62)
				(name "IP_2")
				(number "U10")
			)
			(pin input line
				(at 78.74 77.47 180)
				(length 7.62)
				(name "IP_2")
				(number "T9")
			)
			(pin input line
				(at 78.74 74.93 180)
				(length 7.62)
				(name "IP_2")
				(number "T14")
			)
			(pin input line
				(at 78.74 72.39 180)
				(length 7.62)
				(name "IP_2")
				(number "T13")
			)
			(pin input line
				(at 78.74 69.85 180)
				(length 7.62)
				(name "IP_2")
				(number "R9")
			)
			(pin input line
				(at 78.74 67.31 180)
				(length 7.62)
				(name "IP_2")
				(number "R11")
			)
			(pin input line
				(at 78.74 64.77 180)
				(length 7.62)
				(name "IP_2")
				(number "R10")
			)
			(pin input line
				(at 78.74 62.23 180)
				(length 7.62)
				(name "IP_2")
				(number "P12")
			)
			(pin bidirectional line
				(at 78.74 59.69 180)
				(length 7.62)
				(name "IO_L36P_2/D0/DIN/MISO")
				(number "AB20")
			)
			(pin bidirectional line
				(at 78.74 57.15 180)
				(length 7.62)
				(name "IO_L36N_2/CCLK")
				(number "AA20")
			)
			(pin bidirectional line
				(at 78.74 54.61 180)
				(length 7.62)
				(name "IO_L35P_2")
				(number "AB21")
			)
			(pin bidirectional line
				(at 78.74 52.07 180)
				(length 7.62)
				(name "IO_L35N_2")
				(number "AA21")
			)
			(pin bidirectional line
				(at 78.74 49.53 180)
				(length 7.62)
				(name "IO_L34P_2")
				(number "Y18")
			)
			(pin bidirectional line
				(at 78.74 46.99 180)
				(length 7.62)
				(name "IO_L34N_2")
				(number "W17")
			)
			(pin bidirectional line
				(at 78.74 44.45 180)
				(length 7.62)
				(name "IO_L33P_2")
				(number "W18")
			)
			(pin bidirectional line
				(at 78.74 41.91 180)
				(length 7.62)
				(name "IO_L33N_2")
				(number "V17")
			)
			(pin bidirectional line
				(at 78.74 39.37 180)
				(length 7.62)
				(name "IO_L32P_2")
				(number "AB19")
			)
			(pin bidirectional line
				(at 78.74 36.83 180)
				(length 7.62)
				(name "IO_L32N_2")
				(number "AA19")
			)
			(pin bidirectional line
				(at 78.74 34.29 180)
				(length 7.62)
				(name "IO_L31P_2")
				(number "W16")
			)
			(pin bidirectional line
				(at 78.74 31.75 180)
				(length 7.62)
				(name "IO_L31N_2")
				(number "V16")
			)
			(pin bidirectional line
				(at 78.74 29.21 180)
				(length 7.62)
				(name "IO_L30P_2")
				(number "V14")
			)
			(pin bidirectional line
				(at 78.74 26.67 180)
				(length 7.62)
				(name "IO_L30N_2")
				(number "V15")
			)
			(pin bidirectional line
				(at 78.74 24.13 180)
				(length 7.62)
				(name "IO_L29P_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at 78.74 21.59 180)
				(length 7.62)
				(name "IO_L29N_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at 78.74 19.05 180)
				(length 7.62)
				(name "IO_L28P_2/D2")
				(number "AA17")
			)
			(pin bidirectional line
				(at 78.74 16.51 180)
				(length 7.62)
				(name "IO_L28N_2/D1")
				(number "Y17")
			)
			(pin bidirectional line
				(at 78.74 13.97 180)
				(length 7.62)
				(name "IO_L27P_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at 78.74 11.43 180)
				(length 7.62)
				(name "IO_L27N_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at 78.74 8.89 180)
				(length 7.62)
				(name "IO_L26P_2/INIT_B")
				(number "V13")
			)
			(pin bidirectional line
				(at 78.74 6.35 180)
				(length 7.62)
				(name "IO_L26N_2/D3")
				(number "U13")
			)
			(pin bidirectional line
				(at 78.74 3.81 180)
				(length 7.62)
				(name "IO_L25P_2")
				(number "W15")
			)
			(pin bidirectional line
				(at 78.74 1.27 180)
				(length 7.62)
				(name "IO_L25N_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at 78.74 -1.27 180)
				(length 7.62)
				(name "IO_L24P_2/AWAKE")
				(number "AB15")
			)
			(pin bidirectional line
				(at 78.74 -3.81 180)
				(length 7.62)
				(name "IO_L24N_2/DOUT")
				(number "AA15")
			)
			(pin bidirectional line
				(at 78.74 -6.35 180)
				(length 7.62)
				(name "IO_L23P_2")
				(number "W13")
			)
			(pin bidirectional line
				(at 78.74 -8.89 180)
				(length 7.62)
				(name "IO_L23N_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at 78.74 -11.43 180)
				(length 7.62)
				(name "IO_L22P_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at 78.74 -13.97 180)
				(length 7.62)
				(name "IO_L22N_2/MOSI/CSI_B")
				(number "AB14")
			)
			(pin bidirectional line
				(at 78.74 -16.51 180)
				(length 7.62)
				(name "IO_L21P_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at 78.74 -19.05 180)
				(length 7.62)
				(name "IO_L21N_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at 78.74 -21.59 180)
				(length 7.62)
				(name "IO_L20P_2/GCLK2")
				(number "V12")
			)
			(pin bidirectional line
				(at 78.74 -24.13 180)
				(length 7.62)
				(name "IO_L20N_2/GCLK3")
				(number "U12")
			)
			(pin bidirectional line
				(at 78.74 -26.67 180)
				(length 7.62)
				(name "IO_L19P_2/GCLK0")
				(number "AA12")
			)
			(pin bidirectional line
				(at 78.74 -29.21 180)
				(length 7.62)
				(name "IO_L19N_2/GCLK1")
				(number "AB12")
			)
			(pin bidirectional line
				(at 78.74 -31.75 180)
				(length 7.62)
				(name "IO_L18P_2/GCLK14")
				(number "W12")
			)
			(pin bidirectional line
				(at 78.74 -34.29 180)
				(length 7.62)
				(name "IO_L18N_2/GCLK15")
				(number "Y12")
			)
			(pin bidirectional line
				(at 78.74 -36.83 180)
				(length 7.62)
				(name "IO_L17P_2/GCLK12")
				(number "U11")
			)
			(pin bidirectional line
				(at 78.74 -39.37 180)
				(length 7.62)
				(name "IO_L17N_2/GCLK13")
				(number "V11")
			)
			(pin bidirectional line
				(at 78.74 -41.91 180)
				(length 7.62)
				(name "IO_L16P_2/D5")
				(number "Y11")
			)
			(pin bidirectional line
				(at 78.74 -44.45 180)
				(length 7.62)
				(name "IO_L16N_2/D4")
				(number "AB11")
			)
			(pin bidirectional line
				(at 78.74 -46.99 180)
				(length 7.62)
				(name "IO_L15P_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at 78.74 -49.53 180)
				(length 7.62)
				(name "IO_L15N_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at 78.74 -52.07 180)
				(length 7.62)
				(name "IO_L14P_2/D7")
				(number "Y9")
			)
			(pin bidirectional line
				(at 78.74 -54.61 180)
				(length 7.62)
				(name "IO_L14N_2/D6")
				(number "AB9")
			)
			(pin bidirectional line
				(at 78.74 -57.15 180)
				(length 7.62)
				(name "IO_L13P_2")
				(number "V10")
			)
			(pin bidirectional line
				(at 78.74 -59.69 180)
				(length 7.62)
				(name "IO_L13N_2")
				(number "Y10")
			)
			(pin bidirectional line
				(at 78.74 -62.23 180)
				(length 7.62)
				(name "IO_L12P_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at 78.74 -64.77 180)
				(length 7.62)
				(name "IO_L12N_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at 78.74 -67.31 180)
				(length 7.62)
				(name "IO_L11P_2/VS1")
				(number "W8")
			)
			(pin bidirectional line
				(at 78.74 -69.85 180)
				(length 7.62)
				(name "IO_L11N_2/VS0")
				(number "Y8")
			)
			(pin bidirectional line
				(at 78.74 -72.39 180)
				(length 7.62)
				(name "IO_L10P_2")
				(number "Y7")
			)
			(pin bidirectional line
				(at 78.74 -74.93 180)
				(length 7.62)
				(name "IO_L10N_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at 78.74 -77.47 180)
				(length 7.62)
				(name "IO_L09P_2/RDWR_B")
				(number "V9")
			)
			(pin bidirectional line
				(at 78.74 -80.01 180)
				(length 7.62)
				(name "IO_L09N_2/VS2")
				(number "W9")
			)
			(pin bidirectional line
				(at 78.74 -82.55 180)
				(length 7.62)
				(name "IO_L08P_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at 78.74 -85.09 180)
				(length 7.62)
				(name "IO_L08N_2")
				(number "AB6")
			)
			(pin bidirectional line
				(at 78.74 -87.63 180)
				(length 7.62)
				(name "IO_L07P_2")
				(number "W7")
			)
			(pin bidirectional line
				(at 78.74 -90.17 180)
				(length 7.62)
				(name "IO_L07N_2")
				(number "Y6")
			)
			(pin bidirectional line
				(at 78.74 -92.71 180)
				(length 7.62)
				(name "IO_L06P_2")
				(number "AB4")
			)
			(pin bidirectional line
				(at 78.74 -95.25 180)
				(length 7.62)
				(name "IO_L06N_2")
				(number "AB5")
			)
			(pin bidirectional line
				(at 78.74 -97.79 180)
				(length 7.62)
				(name "IO_L05P_2")
				(number "W6")
			)
			(pin bidirectional line
				(at 78.74 -100.33 180)
				(length 7.62)
				(name "IO_L05N_2")
				(number "Y5")
			)
			(pin bidirectional line
				(at 78.74 -102.87 180)
				(length 7.62)
				(name "IO_L04P_2")
				(number "AB3")
			)
			(pin bidirectional line
				(at 78.74 -105.41 180)
				(length 7.62)
				(name "IO_L04N_2")
				(number "AA4")
			)
			(pin bidirectional line
				(at 78.74 -107.95 180)
				(length 7.62)
				(name "IO_L03P_2")
				(number "AB2")
			)
			(pin bidirectional line
				(at 78.74 -110.49 180)
				(length 7.62)
				(name "IO_L03N_2")
				(number "AA3")
			)
			(pin bidirectional line
				(at 78.74 -113.03 180)
				(length 7.62)
				(name "IO_L02P_2/M2")
				(number "W4")
			)
			(pin bidirectional line
				(at 78.74 -115.57 180)
				(length 7.62)
				(name "IO_L02N_2/CSO_B")
				(number "Y4")
			)
			(pin bidirectional line
				(at 78.74 -118.11 180)
				(length 7.62)
				(name "IO_L01P_2/M1")
				(number "V6")
			)
			(pin bidirectional line
				(at 78.74 -120.65 180)
				(length 7.62)
				(name "IO_L01N_2/M0")
				(number "W5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC3S200AN-FT256"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "XC3S200AN-FT256"
			(at -15.24 128.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "BGA256/1mm"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA256"
			(at 0 0 0)
		)
		(symbol "XC3S200AN-FT256_0_0"
			(text "0"
				(at -12.7 58.42 0)
			)
			(text "1"
				(at -5.08 -66.04 0)
			)
			(text "3"
				(at 2.54 64.77 0)
			)
			(text "2"
				(at 2.54 -55.88 0)
			)
		)
		(symbol "XC3S200AN-FT256_0_1")
		(symbol "XC3S200AN-FT256_1_1"
			(pin input line
				(at -54.61 138.43 0)
				(length 7.62)
				(name "TMS")
				(number "B2")
			)
			(pin output line
				(at -54.61 135.89 0)
				(length 7.62)
				(name "TDO")
				(number "B16")
			)
			(pin input line
				(at -54.61 133.35 0)
				(length 7.62)
				(name "TDI")
				(number "B1")
			)
			(pin input line
				(at -54.61 130.81 0)
				(length 7.62)
				(name "TCK")
				(number "A15")
			)
			(pin bidirectional line
				(at -54.61 125.73 0)
				(length 7.62)
				(name "DONE")
				(number "T15")
			)
			(pin bidirectional line
				(at -54.61 123.19 0)
				(length 7.62)
				(name "/PROG")
				(number "A2")
			)
			(pin bidirectional line
				(at -54.61 118.11 0)
				(length 7.62)
				(name "IO_L01N_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -54.61 115.57 0)
				(length 7.62)
				(name "IO_L01P_0")
				(number "D13")
			)
			(pin bidirectional line
				(at -54.61 113.03 0)
				(length 7.62)
				(name "IO_L02N_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -54.61 110.49 0)
				(length 7.62)
				(name "IO_L02P_0/VREF_0")
				(number "B15")
			)
			(pin bidirectional line
				(at -54.61 107.95 0)
				(length 7.62)
				(name "IO_L03N_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -54.61 105.41 0)
				(length 7.62)
				(name "IO_L03P_0")
				(number "C12")
			)
			(pin bidirectional line
				(at -54.61 102.87 0)
				(length 7.62)
				(name "IO_L04N_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -54.61 100.33 0)
				(length 7.62)
				(name "IO_L04P_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -54.61 97.79 0)
				(length 7.62)
				(name "IO_L05N_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -54.61 95.25 0)
				(length 7.62)
				(name "IO_L05P_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -54.61 92.71 0)
				(length 7.62)
				(name "IO_L06N_0/VREF_0")
				(number "E10")
			)
			(pin bidirectional line
				(at -54.61 90.17 0)
				(length 7.62)
				(name "IO_L06P_0")
				(number "D10")
			)
			(pin bidirectional line
				(at -54.61 87.63 0)
				(length 7.62)
				(name "IO_L07N_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -54.61 85.09 0)
				(length 7.62)
				(name "IO_L07P_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -54.61 82.55 0)
				(length 7.62)
				(name "IO_L08N_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -54.61 80.01 0)
				(length 7.62)
				(name "IO_L08P_0")
				(number "B10")
			)
			(pin bidirectional line
				(at -54.61 77.47 0)
				(length 7.62)
				(name "IO_L09N_0/GCLK5")
				(number "D9")
			)
			(pin bidirectional line
				(at -54.61 74.93 0)
				(length 7.62)
				(name "IO_L09P_0/GCLK4")
				(number "C10")
			)
			(pin bidirectional line
				(at -54.61 72.39 0)
				(length 7.62)
				(name "IO_L10N_0/GCLK7")
				(number "A9")
			)
			(pin bidirectional line
				(at -54.61 69.85 0)
				(length 7.62)
				(name "IO_L10P_0/GCLK6")
				(number "C9")
			)
			(pin bidirectional line
				(at -54.61 67.31 0)
				(length 7.62)
				(name "IO_L11N_0/GCLK9")
				(number "D8")
			)
			(pin bidirectional line
				(at -54.61 64.77 0)
				(length 7.62)
				(name "IO_L11P_0/GCLK8")
				(number "C8")
			)
			(pin bidirectional line
				(at -54.61 62.23 0)
				(length 7.62)
				(name "IO_L12N_0/GCLK11")
				(number "B8")
			)
			(pin bidirectional line
				(at -54.61 59.69 0)
				(length 7.62)
				(name "IO_L12P_0/GCLK10")
				(number "A8")
			)
			(pin bidirectional line
				(at -54.61 57.15 0)
				(length 7.62)
				(name "IO_L13N_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -54.61 54.61 0)
				(length 7.62)
				(name "IO_L13P_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -54.61 52.07 0)
				(length 7.62)
				(name "IO_L14N_0/VREF_0")
				(number "E7")
			)
			(pin bidirectional line
				(at -54.61 49.53 0)
				(length 7.62)
				(name "IO_L14P_0")
				(number "F8")
			)
			(pin bidirectional line
				(at -54.61 46.99 0)
				(length 7.62)
				(name "IO_L15N_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -54.61 44.45 0)
				(length 7.62)
				(name "IO_L15P_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -54.61 41.91 0)
				(length 7.62)
				(name "IO_L16N_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -54.61 39.37 0)
				(length 7.62)
				(name "IO_L16P_0")
				(number "D7")
			)
			(pin bidirectional line
				(at -54.61 36.83 0)
				(length 7.62)
				(name "IO_L17N_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -54.61 34.29 0)
				(length 7.62)
				(name "IO_L17P_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -54.61 31.75 0)
				(length 7.62)
				(name "IO_L18N_0")
				(number "B4")
			)
			(pin bidirectional line
				(at -54.61 29.21 0)
				(length 7.62)
				(name "IO_L18P_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -54.61 26.67 0)
				(length 7.62)
				(name "IO_L19N_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -54.61 24.13 0)
				(length 7.62)
				(name "IO_L19P_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -54.61 21.59 0)
				(length 7.62)
				(name "IO_L20N_0/PUDC_B")
				(number "D5")
			)
			(pin bidirectional line
				(at -54.61 19.05 0)
				(length 7.62)
				(name "IO_L20P_0/VREF_0")
				(number "C4")
			)
			(pin input line
				(at -54.61 16.51 0)
				(length 7.62)
				(name "IP_0")
				(number "D6")
			)
			(pin input line
				(at -54.61 13.97 0)
				(length 7.62)
				(name "IP_0")
				(number "D12")
			)
			(pin input line
				(at -54.61 11.43 0)
				(length 7.62)
				(name "IP_0")
				(number "E6")
			)
			(pin input line
				(at -54.61 8.89 0)
				(length 7.62)
				(name "IP_0")
				(number "F7")
			)
			(pin input line
				(at -54.61 6.35 0)
				(length 7.62)
				(name "IP_0")
				(number "F9")
			)
			(pin input line
				(at -54.61 3.81 0)
				(length 7.62)
				(name "IP_0")
				(number "F10")
			)
			(pin input line
				(at -54.61 1.27 0)
				(length 7.62)
				(name "IP_0/VREF_0")
				(number "E9")
			)
			(pin bidirectional line
				(at -54.61 -5.08 0)
				(length 7.62)
				(name "IO_L01N_1/LDC2")
				(number "N14")
			)
			(pin bidirectional line
				(at -54.61 -7.62 0)
				(length 7.62)
				(name "IO_L01P_1/HDC")
				(number "N13")
			)
			(pin bidirectional line
				(at -54.61 -10.16 0)
				(length 7.62)
				(name "IO_L02N_1/LDC0")
				(number "P15")
			)
			(pin bidirectional line
				(at -54.61 -12.7 0)
				(length 7.62)
				(name "IO_L02P_1/LDC1")
				(number "R15")
			)
			(pin bidirectional line
				(at -54.61 -15.24 0)
				(length 7.62)
				(name "IO_L03N_1/A1")
				(number "N16")
			)
			(pin bidirectional line
				(at -54.61 -17.78 0)
				(length 7.62)
				(name "IO_L03P_1/A0")
				(number "P16")
			)
			(pin bidirectional line
				(at -54.61 -20.32 0)
				(length 7.62)
				(name "IO_L05N_1/VREF_1")
				(number "M14")
			)
			(pin bidirectional line
				(at -54.61 -22.86 0)
				(length 7.62)
				(name "IO_L05P_1")
				(number "M13")
			)
			(pin bidirectional line
				(at -54.61 -25.4 0)
				(length 7.62)
				(name "IO_L06N_1/A3")
				(number "K13")
			)
			(pin bidirectional line
				(at -54.61 -27.94 0)
				(length 7.62)
				(name "IO_L06P_1/A2")
				(number "L13")
			)
			(pin bidirectional line
				(at -54.61 -30.48 0)
				(length 7.62)
				(name "IO_L07N_1/A5")
				(number "M16")
			)
			(pin bidirectional line
				(at -54.61 -33.02 0)
				(length 7.62)
				(name "IO_L07P_1/A4")
				(number "M15")
			)
			(pin bidirectional line
				(at -54.61 -35.56 0)
				(length 7.62)
				(name "IO_L08N_1/A7")
				(number "L16")
			)
			(pin bidirectional line
				(at -54.61 -38.1 0)
				(length 7.62)
				(name "IO_L08P_1/A6")
				(number "L14")
			)
			(pin bidirectional line
				(at -54.61 -40.64 0)
				(length 7.62)
				(name "IO_L10N_1/A9")
				(number "J13")
			)
			(pin bidirectional line
				(at -54.61 -43.18 0)
				(length 7.62)
				(name "IO_L10P_1/A8")
				(number "J12")
			)
			(pin bidirectional line
				(at -54.61 -45.72 0)
				(length 7.62)
				(name "IO_L11N_1/RHCLK1")
				(number "K14")
			)
			(pin bidirectional line
				(at -54.61 -48.26 0)
				(length 7.62)
				(name "IO_L11P_1/RHCLK0")
				(number "K15")
			)
			(pin bidirectional line
				(at -54.61 -50.8 0)
				(length 7.62)
				(name "IO_L12N_1/TRDY1/RHCLK3")
				(number "J16")
			)
			(pin bidirectional line
				(at -54.61 -53.34 0)
				(length 7.62)
				(name "IO_L12P_1/RHCLK2")
				(number "K16")
			)
			(pin bidirectional line
				(at -54.61 -55.88 0)
				(length 7.62)
				(name "IO_L14N_1/RHCLK5")
				(number "H14")
			)
			(pin bidirectional line
				(at -54.61 -58.42 0)
				(length 7.62)
				(name "IO_L14P_1/RHCLK4")
				(number "J14")
			)
			(pin bidirectional line
				(at -54.61 -60.96 0)
				(length 7.62)
				(name "IO_L15N_1/RHCLK7")
				(number "H16")
			)
			(pin bidirectional line
				(at -54.61 -63.5 0)
				(length 7.62)
				(name "IO_L15P_1/IRDY1/RHCLK6")
				(number "H15")
			)
			(pin bidirectional line
				(at -54.61 -66.04 0)
				(length 7.62)
				(name "IO_L16N_1/A11")
				(number "F16")
			)
			(pin bidirectional line
				(at -54.61 -68.58 0)
				(length 7.62)
				(name "IO_L16P_1/A10")
				(number "G16")
			)
			(pin bidirectional line
				(at -54.61 -71.12 0)
				(length 7.62)
				(name "IO_L17N_1/A13")
				(number "G14")
			)
			(pin bidirectional line
				(at -54.61 -73.66 0)
				(length 7.62)
				(name "IO_L17P_1/A12")
				(number "H13")
			)
			(pin bidirectional line
				(at -54.61 -76.2 0)
				(length 7.62)
				(name "IO_L18N_1/A15")
				(number "F15")
			)
			(pin bidirectional line
				(at -54.61 -78.74 0)
				(length 7.62)
				(name "IO_L18P_1/A14")
				(number "E16")
			)
			(pin bidirectional line
				(at -54.61 -81.28 0)
				(length 7.62)
				(name "IO_L19N_1/A17")
				(number "F14")
			)
			(pin bidirectional line
				(at -54.61 -83.82 0)
				(length 7.62)
				(name "IO_L19P_1/A16")
				(number "G13")
			)
			(pin bidirectional line
				(at -54.61 -86.36 0)
				(length 7.62)
				(name "IO_L20N_1/A19")
				(number "F13")
			)
			(pin bidirectional line
				(at -54.61 -88.9 0)
				(length 7.62)
				(name "IO_L20P_1/A18")
				(number "E14")
			)
			(pin bidirectional line
				(at -54.61 -91.44 0)
				(length 7.62)
				(name "IO_L22N_1/A21")
				(number "D15")
			)
			(pin bidirectional line
				(at -54.61 -93.98 0)
				(length 7.62)
				(name "IO_L22P_1/A20")
				(number "D16")
			)
			(pin bidirectional line
				(at -54.61 -96.52 0)
				(length 7.62)
				(name "IO_L23N_1/A23")
				(number "D14")
			)
			(pin bidirectional line
				(at -54.61 -99.06 0)
				(length 7.62)
				(name "IO_L23P_1/A22")
				(number "E13")
			)
			(pin bidirectional line
				(at -54.61 -101.6 0)
				(length 7.62)
				(name "IO_L24N_1/A25")
				(number "C15")
			)
			(pin bidirectional line
				(at -54.61 -104.14 0)
				(length 7.62)
				(name "IO_L24P_1/A24")
				(number "C16")
			)
			(pin input line
				(at -54.61 -106.68 0)
				(length 7.62)
				(name "IP_L04N_1/VREF_1")
				(number "K12")
			)
			(pin input line
				(at -54.61 -109.22 0)
				(length 7.62)
				(name "IP_L04P_1")
				(number "K11")
			)
			(pin input line
				(at -54.61 -111.76 0)
				(length 7.62)
				(name "IP_L09N_1")
				(number "J11")
			)
			(pin input line
				(at -54.61 -114.3 0)
				(length 7.62)
				(name "IP_L09P_1/VREF_1")
				(number "J10")
			)
			(pin input line
				(at -54.61 -116.84 0)
				(length 7.62)
				(name "IP_L13N_1")
				(number "H11")
			)
			(pin input line
				(at -54.61 -119.38 0)
				(length 7.62)
				(name "IP_L13P_1")
				(number "H10")
			)
			(pin input line
				(at -54.61 -121.92 0)
				(length 7.62)
				(name "IP_L21N_1")
				(number "G11")
			)
			(pin input line
				(at -54.61 -124.46 0)
				(length 7.62)
				(name "IP_L21P_1/VREF_1")
				(number "G12")
			)
			(pin input line
				(at -54.61 -127 0)
				(length 7.62)
				(name "IP_L25N_1")
				(number "F11")
			)
			(pin input line
				(at -54.61 -129.54 0)
				(length 7.62)
				(name "IP_L25P_1/VREF_1")
				(number "F12")
			)
			(pin input line
				(at -54.61 -132.08 0)
				(length 7.62)
				(name "SUSPEND")
				(number "R16")
			)
			(pin power_in line
				(at -34.29 149.86 270)
				(length 7.62)
				(name "VCCO0")
				(number "B5")
			)
			(pin power_in line
				(at -34.29 -149.86 90)
				(length 7.62)
				(name "GND")
				(number "A1")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "A16")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "B11")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "B7")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "C14")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "C3")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "E12")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "E5")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "F2")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "F6")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "G10")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "G15")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "G8")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "H9")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "J8")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "K2")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "K7")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "K9")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "L11")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "L15")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "M12")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "M5")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "P14")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "P3")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "R10")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "R6")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "T1")
			)
			(pin passive line
				(at -34.29 -149.86 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at -31.75 149.86 270)
				(length 7.62)
				(name "VCCO0")
				(number "B9")
			)
			(pin power_in line
				(at -29.21 149.86 270)
				(length 7.62)
				(name "VCCO0")
				(number "B13")
			)
			(pin power_in line
				(at -26.67 149.86 270)
				(length 7.62)
				(name "VCCO0")
				(number "E8")
			)
			(pin power_in line
				(at -24.13 149.86 270)
				(length 7.62)
				(name "VCCO1")
				(number "E15")
			)
			(pin power_in line
				(at -21.59 149.86 270)
				(length 7.62)
				(name "VCCO1")
				(number "H12")
			)
			(pin power_in line
				(at -19.05 149.86 270)
				(length 7.62)
				(name "VCCO1")
				(number "J15")
			)
			(pin power_in line
				(at -16.51 149.86 270)
				(length 7.62)
				(name "VCCO1")
				(number "N15")
			)
			(pin power_in line
				(at -13.97 149.86 270)
				(length 7.62)
				(name "VCCO2")
				(number "M9")
			)
			(pin power_in line
				(at -11.43 149.86 270)
				(length 7.62)
				(name "VCCO2")
				(number "R4")
			)
			(pin power_in line
				(at -8.89 149.86 270)
				(length 7.62)
				(name "VCCO2")
				(number "R8")
			)
			(pin power_in line
				(at -6.35 149.86 270)
				(length 7.62)
				(name "VCCO2")
				(number "R12")
			)
			(pin passive line
				(at -3.81 149.86 270)
				(length 7.62)
				(name "VCCO3")
				(number "D2")
			)
			(pin power_in line
				(at -1.27 149.86 270)
				(length 7.62)
				(name "VCCO3")
				(number "H2")
			)
			(pin power_in line
				(at 1.27 149.86 270)
				(length 7.62)
				(name "VCCO3")
				(number "J5")
			)
			(pin power_in line
				(at 3.81 149.86 270)
				(length 7.62)
				(name "VCCO3")
				(number "M2")
			)
			(pin power_in line
				(at 11.43 149.86 270)
				(length 7.62)
				(name "VCCAUX")
				(number "E11")
			)
			(pin power_in line
				(at 13.97 149.86 270)
				(length 7.62)
				(name "VCCAUX")
				(number "F5")
			)
			(pin power_in line
				(at 16.51 149.86 270)
				(length 7.62)
				(name "VCCAUX")
				(number "L12")
			)
			(pin power_in line
				(at 19.05 149.86 270)
				(length 7.62)
				(name "VCCAUX")
				(number "M6")
			)
			(pin power_in line
				(at 26.67 149.86 270)
				(length 7.62)
				(name "VCCINT")
				(number "G7")
			)
			(pin power_in line
				(at 29.21 149.86 270)
				(length 7.62)
				(name "VCCINT")
				(number "G9")
			)
			(pin power_in line
				(at 31.75 149.86 270)
				(length 7.62)
				(name "VCCINT")
				(number "H8")
			)
			(pin power_in line
				(at 34.29 149.86 270)
				(length 7.62)
				(name "VCCINT")
				(number "J9")
			)
			(pin power_in line
				(at 36.83 149.86 270)
				(length 7.62)
				(name "VCCINT")
				(number "K8")
			)
			(pin power_in line
				(at 39.37 149.86 270)
				(length 7.62)
				(name "VCCINT")
				(number "K10")
			)
			(pin input line
				(at 54.61 125.73 180)
				(length 7.62)
				(name "IP_L25P_3")
				(number "L5")
			)
			(pin input line
				(at 54.61 123.19 180)
				(length 7.62)
				(name "IP_L25N_3/VREF_3")
				(number "L6")
			)
			(pin input line
				(at 54.61 120.65 180)
				(length 7.62)
				(name "IP_L21P_3")
				(number "K5")
			)
			(pin input line
				(at 54.61 118.11 180)
				(length 7.62)
				(name "IP_L21N_3")
				(number "K6")
			)
			(pin input line
				(at 54.61 115.57 180)
				(length 7.62)
				(name "IP_L13P_3")
				(number "H7")
			)
			(pin input line
				(at 54.61 113.03 180)
				(length 7.62)
				(name "IP_L13N_3")
				(number "J7")
			)
			(pin input line
				(at 54.61 110.49 180)
				(length 7.62)
				(name "IP_L06P_3")
				(number "G6")
			)
			(pin input line
				(at 54.61 107.95 180)
				(length 7.62)
				(name "IP_L06N_3/VREF_3")
				(number "G5")
			)
			(pin input line
				(at 54.61 105.41 180)
				(length 7.62)
				(name "IP_L04P_3")
				(number "E4")
			)
			(pin input line
				(at 54.61 102.87 180)
				(length 7.62)
				(name "IP_L04N_3/VREF_3")
				(number "F4")
			)
			(pin bidirectional line
				(at 54.61 100.33 180)
				(length 7.62)
				(name "IO_L24P_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 54.61 97.79 180)
				(length 7.62)
				(name "IO_L24N_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 54.61 95.25 180)
				(length 7.62)
				(name "IO_L23P_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 54.61 92.71 180)
				(length 7.62)
				(name "IO_L23N_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 54.61 90.17 180)
				(length 7.62)
				(name "IO_L22P_3")
				(number "N2")
			)
			(pin bidirectional line
				(at 54.61 87.63 180)
				(length 7.62)
				(name "IO_L22N_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 54.61 85.09 180)
				(length 7.62)
				(name "IO_L20P_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 54.61 82.55 180)
				(length 7.62)
				(name "IO_L20N_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 54.61 80.01 180)
				(length 7.62)
				(name "IO_L19P_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 54.61 77.47 180)
				(length 7.62)
				(name "IO_L19N_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 54.61 74.93 180)
				(length 7.62)
				(name "IO_L18P_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 54.61 72.39 180)
				(length 7.62)
				(name "IO_L18N_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 54.61 69.85 180)
				(length 7.62)
				(name "IO_L17P_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 54.61 67.31 180)
				(length 7.62)
				(name "IO_L17N_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 54.61 64.77 180)
				(length 7.62)
				(name "IO_L16P_3/VREF_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 54.61 62.23 180)
				(length 7.62)
				(name "IO_L16N_3")
				(number "L2")
			)
			(pin bidirectional line
				(at 54.61 59.69 180)
				(length 7.62)
				(name "IO_L15P_3/TRDY2/LHCLK6")
				(number "K3")
			)
			(pin bidirectional line
				(at 54.61 57.15 180)
				(length 7.62)
				(name "IO_L15N_3/LHCLK7")
				(number "K1")
			)
			(pin bidirectional line
				(at 54.61 54.61 180)
				(length 7.62)
				(name "IO_L14P_3/LHCLK4")
				(number "J2")
			)
			(pin bidirectional line
				(at 54.61 52.07 180)
				(length 7.62)
				(name "IO_L14N_3/LHCLK5")
				(number "J1")
			)
			(pin bidirectional line
				(at 54.61 49.53 180)
				(length 7.62)
				(name "IO_L12P_3/LHCLK2")
				(number "H3")
			)
			(pin bidirectional line
				(at 54.61 46.99 180)
				(length 7.62)
				(name "IO_L12N_3/IRDY2/LHCLK3")
				(number "J3")
			)
			(pin bidirectional line
				(at 54.61 44.45 180)
				(length 7.62)
				(name "IO_L11P_3/LHCLK0")
				(number "G2")
			)
			(pin bidirectional line
				(at 54.61 41.91 180)
				(length 7.62)
				(name "IO_L11N_3/LHCLK1")
				(number "H1")
			)
			(pin bidirectional line
				(at 54.61 39.37 180)
				(length 7.62)
				(name "IO_L10P_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 54.61 36.83 180)
				(length 7.62)
				(name "IO_L10N_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 54.61 34.29 180)
				(length 7.62)
				(name "IO_L09P_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 54.61 31.75 180)
				(length 7.62)
				(name "IO_L09N_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 54.61 29.21 180)
				(length 7.62)
				(name "IO_L08P_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 54.61 26.67 180)
				(length 7.62)
				(name "IO_L08N_3/VREF_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 54.61 24.13 180)
				(length 7.62)
				(name "IO_L07P_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 54.61 21.59 180)
				(length 7.62)
				(name "IO_L07N_3")
				(number "G4")
			)
			(pin bidirectional line
				(at 54.61 19.05 180)
				(length 7.62)
				(name "IO_L05P_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 54.61 16.51 180)
				(length 7.62)
				(name "IO_L05N_3")
				(number "E2")
			)
			(pin bidirectional line
				(at 54.61 13.97 180)
				(length 7.62)
				(name "IO_L03P_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 54.61 11.43 180)
				(length 7.62)
				(name "IO_L03N_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 54.61 8.89 180)
				(length 7.62)
				(name "IO_L02P_3")
				(number "D4")
			)
			(pin bidirectional line
				(at 54.61 6.35 180)
				(length 7.62)
				(name "IO_L02N_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 54.61 3.81 180)
				(length 7.62)
				(name "IO_L01P_3")
				(number "C2")
			)
			(pin bidirectional line
				(at 54.61 1.27 180)
				(length 7.62)
				(name "IO_L01N_3")
				(number "C1")
			)
			(pin input line
				(at 54.61 -5.08 180)
				(length 7.62)
				(name "IP_2/VREF_2")
				(number "N5")
			)
			(pin input line
				(at 54.61 -7.62 180)
				(length 7.62)
				(name "IP_2/VREF_2")
				(number "M11")
			)
			(pin input line
				(at 54.61 -10.16 180)
				(length 7.62)
				(name "IP_2/VREF_2")
				(number "M8")
			)
			(pin input line
				(at 54.61 -12.7 180)
				(length 7.62)
				(name "IP_2/VREF_2")
				(number "M7")
			)
			(pin input line
				(at 54.61 -15.24 180)
				(length 7.62)
				(name "IP_2/VREF_2")
				(number "L10")
			)
			(pin input line
				(at 54.61 -17.78 180)
				(length 7.62)
				(name "IP_2/VREF_2")
				(number "L9")
			)
			(pin input line
				(at 54.61 -20.32 180)
				(length 7.62)
				(name "IP_2")
				(number "L8")
			)
			(pin input line
				(at 54.61 -22.86 180)
				(length 7.62)
				(name "IP_2")
				(number "L7")
			)
			(pin bidirectional line
				(at 54.61 -25.4 180)
				(length 7.62)
				(name "IO_L20P_2/D0/DIN/MISO")
				(number "T14")
			)
			(pin bidirectional line
				(at 54.61 -27.94 180)
				(length 7.62)
				(name "IO_L20N_2/CCLK")
				(number "R14")
			)
			(pin bidirectional line
				(at 54.61 -30.48 180)
				(length 7.62)
				(name "IO_L19P_2")
				(number "N12")
			)
			(pin bidirectional line
				(at 54.61 -33.02 180)
				(length 7.62)
				(name "IO_L19N_2")
				(number "P13")
			)
			(pin bidirectional line
				(at 54.61 -35.56 180)
				(length 7.62)
				(name "IO_L18P_2/D2")
				(number "T13")
			)
			(pin bidirectional line
				(at 54.61 -38.1 180)
				(length 7.62)
				(name "IO_L18N_2/D1")
				(number "R13")
			)
			(pin bidirectional line
				(at 54.61 -40.64 180)
				(length 7.62)
				(name "IO_L17P_2/INIT_B")
				(number "T12")
			)
			(pin bidirectional line
				(at 54.61 -43.18 180)
				(length 7.62)
				(name "IO_L17N_2/D3")
				(number "P12")
			)
			(pin bidirectional line
				(at 54.61 -45.72 180)
				(length 7.62)
				(name "IO_L16P_2")
				(number "P11")
			)
			(pin bidirectional line
				(at 54.61 -48.26 180)
				(length 7.62)
				(name "IO_L16N_2")
				(number "N11")
			)
			(pin bidirectional line
				(at 54.61 -50.8 180)
				(length 7.62)
				(name "IO_L15P_2/AWAKE")
				(number "T11")
			)
			(pin bidirectional line
				(at 54.61 -53.34 180)
				(length 7.62)
				(name "IO_L15N_2/DOUT")
				(number "R11")
			)
			(pin bidirectional line
				(at 54.61 -55.88 180)
				(length 7.62)
				(name "IO_L14P_2")
				(number "T10")
			)
			(pin bidirectional line
				(at 54.61 -58.42 180)
				(length 7.62)
				(name "IO_L14N_2/MOSI/CSI_B")
				(number "P10")
			)
			(pin bidirectional line
				(at 54.61 -60.96 180)
				(length 7.62)
				(name "IO_L13P_2")
				(number "N10")
			)
			(pin bidirectional line
				(at 54.61 -63.5 180)
				(length 7.62)
				(name "IO_L13N_2")
				(number "M10")
			)
			(pin bidirectional line
				(at 54.61 -66.04 180)
				(length 7.62)
				(name "IO_L12P_2/GCLK2")
				(number "R9")
			)
			(pin bidirectional line
				(at 54.61 -68.58 180)
				(length 7.62)
				(name "IO_L12N_2/GCLK3")
				(number "T9")
			)
			(pin bidirectional line
				(at 54.61 -71.12 180)
				(length 7.62)
				(name "IO_L11P_2/GCLK0")
				(number "N9")
			)
			(pin bidirectional line
				(at 54.61 -73.66 180)
				(length 7.62)
				(name "IO_L11N_2/GCLK1")
				(number "P9")
			)
			(pin bidirectional line
				(at 54.61 -76.2 180)
				(length 7.62)
				(name "IO_L10P_2/GCLK14")
				(number "P8")
			)
			(pin bidirectional line
				(at 54.61 -78.74 180)
				(length 7.62)
				(name "IO_L10N_2/GCLK15")
				(number "T8")
			)
			(pin bidirectional line
				(at 54.61 -81.28 180)
				(length 7.62)
				(name "IO_L09P_2/GCLK12")
				(number "R7")
			)
			(pin bidirectional line
				(at 54.61 -83.82 180)
				(length 7.62)
				(name "IO_L09N_2/GCLK13")
				(number "T7")
			)
			(pin bidirectional line
				(at 54.61 -86.36 180)
				(length 7.62)
				(name "IO_L08P_2/D5")
				(number "P7")
			)
			(pin bidirectional line
				(at 54.61 -88.9 180)
				(length 7.62)
				(name "IO_L08N_2/D4")
				(number "N8")
			)
			(pin bidirectional line
				(at 54.61 -91.44 180)
				(length 7.62)
				(name "IO_L07P_2")
				(number "N7")
			)
			(pin bidirectional line
				(at 54.61 -93.98 180)
				(length 7.62)
				(name "IO_L07N_2")
				(number "P6")
			)
			(pin bidirectional line
				(at 54.61 -96.52 180)
				(length 7.62)
				(name "IO_L06P_2/D7")
				(number "T5")
			)
			(pin bidirectional line
				(at 54.61 -99.06 180)
				(length 7.62)
				(name "IO_L06N_2/D6")
				(number "T6")
			)
			(pin bidirectional line
				(at 54.61 -101.6 180)
				(length 7.62)
				(name "IO_L05P_2")
				(number "T4")
			)
			(pin bidirectional line
				(at 54.61 -104.14 180)
				(length 7.62)
				(name "IO_L05N_2")
				(number "R5")
			)
			(pin bidirectional line
				(at 54.61 -106.68 180)
				(length 7.62)
				(name "IO_L04P_2/VS1")
				(number "N6")
			)
			(pin bidirectional line
				(at 54.61 -109.22 180)
				(length 7.62)
				(name "IO_L04N_2/VS0")
				(number "P5")
			)
			(pin bidirectional line
				(at 54.61 -111.76 180)
				(length 7.62)
				(name "IO_L03P_2/RDWR_B")
				(number "R3")
			)
			(pin bidirectional line
				(at 54.61 -114.3 180)
				(length 7.62)
				(name "IO_L03N_2/VS2")
				(number "T3")
			)
			(pin bidirectional line
				(at 54.61 -116.84 180)
				(length 7.62)
				(name "IO_L02P_2/M2")
				(number "R2")
			)
			(pin bidirectional line
				(at 54.61 -119.38 180)
				(length 7.62)
				(name "IO_L02N_2/CSO_B")
				(number "T2")
			)
			(pin bidirectional line
				(at 54.61 -121.92 180)
				(length 7.62)
				(name "IO_L01P_2/M1")
				(number "N4")
			)
			(pin bidirectional line
				(at 54.61 -124.46 180)
				(length 7.62)
				(name "IO_L01N_2/M0")
				(number "P4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC3S400-FG320"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XC3S400-FG320"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC3S400-FG320_0_1")
		(symbol "XC3S400-FG320_1_1"
			(pin input line
				(at -58.42 80.01 0)
				(length 7.62)
				(name "TMS")
				(number "B16")
			)
			(pin output line
				(at -58.42 78.74 0)
				(length 7.62)
				(name "TDO")
				(number "D15")
			)
			(pin input line
				(at -58.42 77.47 0)
				(length 7.62)
				(name "TDI")
				(number "D4")
			)
			(pin input line
				(at -58.42 76.2 0)
				(length 7.62)
				(name "TCK")
				(number "E14")
			)
			(pin input line
				(at -58.42 74.93 0)
				(length 7.62)
				(name "INIT")
				(number "U10")
			)
			(pin output line
				(at -58.42 73.66 0)
				(length 7.62)
				(name "DONE")
				(number "R15")
			)
			(pin input line
				(at -58.42 72.39 0)
				(length 7.62)
				(name "PROG/B")
				(number "E5")
			)
			(pin input clock
				(at -58.42 69.85 0)
				(length 7.62)
				(name "CCLK")
				(number "T15")
			)
			(pin input line
				(at -58.42 67.31 0)
				(length 7.62)
				(name "M0")
				(number "P5")
			)
			(pin input line
				(at -58.42 66.04 0)
				(length 7.62)
				(name "M1")
				(number "U3")
			)
			(pin input line
				(at -58.42 64.77 0)
				(length 7.62)
				(name "M2")
				(number "R4")
			)
			(pin bidirectional line
				(at -58.42 62.23 0)
				(length 7.62)
				(name "IO0/D9")
				(number "D9")
			)
			(pin bidirectional line
				(at -58.42 60.96 0)
				(length 7.62)
				(name "IO0/E7")
				(number "E7")
			)
			(pin bidirectional line
				(at -58.42 59.69 0)
				(length 7.62)
				(name "IO0VREF/B3")
				(number "B3")
			)
			(pin bidirectional line
				(at -58.42 58.42 0)
				(length 7.62)
				(name "IO0VREF/D6")
				(number "D6")
			)
			(pin bidirectional line
				(at -58.42 57.15 0)
				(length 7.62)
				(name "IO0VRP/A2")
				(number "A2")
			)
			(pin bidirectional line
				(at -58.42 55.88 0)
				(length 7.62)
				(name "IO0VRN/A3")
				(number "A3")
			)
			(pin bidirectional line
				(at -58.42 54.61 0)
				(length 7.62)
				(name "IO0/B4")
				(number "B4")
			)
			(pin bidirectional line
				(at -58.42 53.34 0)
				(length 7.62)
				(name "IO0/C4")
				(number "C4")
			)
			(pin bidirectional line
				(at -58.42 52.07 0)
				(length 7.62)
				(name "IO0/C5")
				(number "C5")
			)
			(pin bidirectional line
				(at -58.42 50.8 0)
				(length 7.62)
				(name "IO0/D5")
				(number "D5")
			)
			(pin bidirectional line
				(at -58.42 49.53 0)
				(length 7.62)
				(name "IO0/A4")
				(number "A4")
			)
			(pin bidirectional line
				(at -58.42 48.26 0)
				(length 7.62)
				(name "IO0/A5")
				(number "A5")
			)
			(pin bidirectional line
				(at -58.42 46.99 0)
				(length 7.62)
				(name "IO0/B5")
				(number "B5")
			)
			(pin bidirectional line
				(at -58.42 45.72 0)
				(length 7.62)
				(name "IO0/B6")
				(number "B6")
			)
			(pin bidirectional line
				(at -58.42 44.45 0)
				(length 7.62)
				(name "IO0/C7")
				(number "C7")
			)
			(pin bidirectional line
				(at -58.42 43.18 0)
				(length 7.62)
				(name "IO0/D7")
				(number "D7")
			)
			(pin bidirectional line
				(at -58.42 41.91 0)
				(length 7.62)
				(name "IO0/C8")
				(number "C8")
			)
			(pin bidirectional line
				(at -58.42 40.64 0)
				(length 7.62)
				(name "IO0/D8")
				(number "D8")
			)
			(pin bidirectional line
				(at -58.42 39.37 0)
				(length 7.62)
				(name "IO0/E8")
				(number "E8")
			)
			(pin bidirectional line
				(at -58.42 38.1 0)
				(length 7.62)
				(name "IO0/F8")
				(number "F8")
			)
			(pin bidirectional line
				(at -58.42 36.83 0)
				(length 7.62)
				(name "IO0/A7")
				(number "A7")
			)
			(pin bidirectional line
				(at -58.42 35.56 0)
				(length 7.62)
				(name "IO0/A8")
				(number "A8")
			)
			(pin bidirectional line
				(at -58.42 34.29 0)
				(length 7.62)
				(name "IO0/B9")
				(number "B9")
			)
			(pin bidirectional line
				(at -58.42 33.02 0)
				(length 7.62)
				(name "IO0VREF/A9")
				(number "A9")
			)
			(pin input clock
				(at -58.42 31.75 0)
				(length 7.62)
				(name "GCLK7/E9")
				(number "E9")
			)
			(pin input clock
				(at -58.42 30.48 0)
				(length 7.62)
				(name "GCLK6/F9")
				(number "F9")
			)
			(pin bidirectional line
				(at -58.42 27.94 0)
				(length 7.62)
				(name "IO1/A11")
				(number "A11")
			)
			(pin bidirectional line
				(at -58.42 26.67 0)
				(length 7.62)
				(name "IO1/B13")
				(number "B13")
			)
			(pin bidirectional line
				(at -58.42 25.4 0)
				(length 7.62)
				(name "IO1/D10")
				(number "D10")
			)
			(pin bidirectional line
				(at -58.42 24.13 0)
				(length 7.62)
				(name "IO1VREF/A12")
				(number "A12")
			)
			(pin bidirectional line
				(at -58.42 22.86 0)
				(length 7.62)
				(name "IO1VRP/A16")
				(number "A16")
			)
			(pin bidirectional line
				(at -58.42 21.59 0)
				(length 7.62)
				(name "IO1VRN/A17")
				(number "A17")
			)
			(pin bidirectional line
				(at -58.42 20.32 0)
				(length 7.62)
				(name "IO1VREF/A15")
				(number "A15")
			)
			(pin bidirectional line
				(at -58.42 19.05 0)
				(length 7.62)
				(name "IO1/B15")
				(number "B15")
			)
			(pin bidirectional line
				(at -58.42 17.78 0)
				(length 7.62)
				(name "IO1/C14")
				(number "C14")
			)
			(pin bidirectional line
				(at -58.42 16.51 0)
				(length 7.62)
				(name "IO1/C15")
				(number "C15")
			)
			(pin bidirectional line
				(at -58.42 15.24 0)
				(length 7.62)
				(name "IO1/A14")
				(number "A14")
			)
			(pin bidirectional line
				(at -58.42 13.97 0)
				(length 7.62)
				(name "IO1/B14")
				(number "B14")
			)
			(pin bidirectional line
				(at -58.42 12.7 0)
				(length 7.62)
				(name "IO1/D14")
				(number "D14")
			)
			(pin bidirectional line
				(at -58.42 11.43 0)
				(length 7.62)
				(name "IO1/D13")
				(number "D13")
			)
			(pin bidirectional line
				(at -58.42 10.16 0)
				(length 7.62)
				(name "IO1/E13")
				(number "E13")
			)
			(pin bidirectional line
				(at -58.42 8.89 0)
				(length 7.62)
				(name "IO1/E12")
				(number "E12")
			)
			(pin bidirectional line
				(at -58.42 7.62 0)
				(length 7.62)
				(name "IO1/C12")
				(number "C12")
			)
			(pin bidirectional line
				(at -58.42 6.35 0)
				(length 7.62)
				(name "IO1/D12")
				(number "D12")
			)
			(pin bidirectional line
				(at -58.42 5.08 0)
				(length 7.62)
				(name "IO1/F11")
				(number "F11")
			)
			(pin bidirectional line
				(at -58.42 3.81 0)
				(length 7.62)
				(name "IO1/E11")
				(number "E11")
			)
			(pin bidirectional line
				(at -58.42 2.54 0)
				(length 7.62)
				(name "IO1/C11")
				(number "C11")
			)
			(pin bidirectional line
				(at -58.42 1.27 0)
				(length 7.62)
				(name "IO1/D11")
				(number "D11")
			)
			(pin bidirectional line
				(at -58.42 0 0)
				(length 7.62)
				(name "IO1VREF/A10")
				(number "A10")
			)
			(pin bidirectional line
				(at -58.42 -1.27 0)
				(length 7.62)
				(name "IO1/B10")
				(number "B10")
			)
			(pin input clock
				(at -58.42 -2.54 0)
				(length 7.62)
				(name "GCLK5/E10")
				(number "E10")
			)
			(pin input clock
				(at -58.42 -3.81 0)
				(length 7.62)
				(name "GCLK4/F10")
				(number "F10")
			)
			(pin bidirectional line
				(at -58.42 -6.35 0)
				(length 7.62)
				(name "IO2/J13")
				(number "J13")
			)
			(pin bidirectional line
				(at -58.42 -7.62 0)
				(length 7.62)
				(name "IO2VRP/C16")
				(number "C16")
			)
			(pin bidirectional line
				(at -58.42 -8.89 0)
				(length 7.62)
				(name "IO2VRN/C17")
				(number "C17")
			)
			(pin bidirectional line
				(at -58.42 -10.16 0)
				(length 7.62)
				(name "IO2/B18")
				(number "B18")
			)
			(pin bidirectional line
				(at -58.42 -11.43 0)
				(length 7.62)
				(name "IO2/C18")
				(number "C18")
			)
			(pin bidirectional line
				(at -58.42 -12.7 0)
				(length 7.62)
				(name "IO2/D17")
				(number "D17")
			)
			(pin bidirectional line
				(at -58.42 -13.97 0)
				(length 7.62)
				(name "IO2VREF/D18")
				(number "D18")
			)
			(pin bidirectional line
				(at -58.42 -15.24 0)
				(length 7.62)
				(name "IO2/D16")
				(number "D16")
			)
			(pin bidirectional line
				(at -58.42 -16.51 0)
				(length 7.62)
				(name "IO2/E16")
				(number "E16")
			)
			(pin bidirectional line
				(at -58.42 -17.78 0)
				(length 7.62)
				(name "IO2/E17")
				(number "E17")
			)
			(pin bidirectional line
				(at -58.42 -19.05 0)
				(length 7.62)
				(name "IO2/E18")
				(number "E18")
			)
			(pin bidirectional line
				(at -58.42 -20.32 0)
				(length 7.62)
				(name "IO2/F15")
				(number "F15")
			)
			(pin bidirectional line
				(at -58.42 -21.59 0)
				(length 7.62)
				(name "IO2/E15")
				(number "E15")
			)
			(pin bidirectional line
				(at -58.42 -22.86 0)
				(length 7.62)
				(name "IO2/F14")
				(number "F14")
			)
			(pin bidirectional line
				(at -58.42 -24.13 0)
				(length 7.62)
				(name "IO2/G14")
				(number "G14")
			)
			(pin bidirectional line
				(at -58.42 -25.4 0)
				(length 7.62)
				(name "IO2VREF/G18")
				(number "G18")
			)
			(pin bidirectional line
				(at -58.42 -26.67 0)
				(length 7.62)
				(name "IO2/F17")
				(number "F17")
			)
			(pin bidirectional line
				(at -58.42 -27.94 0)
				(length 7.62)
				(name "IO2/G15")
				(number "G15")
			)
			(pin bidirectional line
				(at -58.42 -29.21 0)
				(length 7.62)
				(name "IO2/G16")
				(number "G16")
			)
			(pin bidirectional line
				(at -58.42 -30.48 0)
				(length 7.62)
				(name "IO2/H13")
				(number "H13")
			)
			(pin bidirectional line
				(at -58.42 -31.75 0)
				(length 7.62)
				(name "IO2/H14")
				(number "H14")
			)
			(pin bidirectional line
				(at -58.42 -33.02 0)
				(length 7.62)
				(name "IO2VREF/H16")
				(number "H16")
			)
			(pin bidirectional line
				(at -58.42 -34.29 0)
				(length 7.62)
				(name "IO2/H15")
				(number "H15")
			)
			(pin bidirectional line
				(at -58.42 -35.56 0)
				(length 7.62)
				(name "IO2/H17")
				(number "H17")
			)
			(pin bidirectional line
				(at -58.42 -36.83 0)
				(length 7.62)
				(name "IO2/H18")
				(number "H18")
			)
			(pin bidirectional line
				(at -58.42 -38.1 0)
				(length 7.62)
				(name "IO2/J18")
				(number "J18")
			)
			(pin bidirectional line
				(at -58.42 -39.37 0)
				(length 7.62)
				(name "IO2/J17")
				(number "J17")
			)
			(pin bidirectional line
				(at -58.42 -40.64 0)
				(length 7.62)
				(name "IO2/J15")
				(number "J15")
			)
			(pin bidirectional line
				(at -58.42 -41.91 0)
				(length 7.62)
				(name "IO2VREF/J14")
				(number "J14")
			)
			(pin bidirectional line
				(at -58.42 -44.45 0)
				(length 7.62)
				(name "IO3/K15")
				(number "K15")
			)
			(pin bidirectional line
				(at -58.42 -45.72 0)
				(length 7.62)
				(name "IO3VRP/T17")
				(number "T17")
			)
			(pin bidirectional line
				(at -58.42 -46.99 0)
				(length 7.62)
				(name "IO3VRN/T16")
				(number "T16")
			)
			(pin bidirectional line
				(at -58.42 -48.26 0)
				(length 7.62)
				(name "IO3/T18")
				(number "T18")
			)
			(pin bidirectional line
				(at -58.42 -49.53 0)
				(length 7.62)
				(name "IO3/U18")
				(number "U18")
			)
			(pin bidirectional line
				(at -58.42 -50.8 0)
				(length 7.62)
				(name "IO3/P16")
				(number "P16")
			)
			(pin bidirectional line
				(at -58.42 -52.07 0)
				(length 7.62)
				(name "IO3VREF/R16")
				(number "R16")
			)
			(pin bidirectional line
				(at -58.42 -53.34 0)
				(length 7.62)
				(name "IO3/R17")
				(number "R17")
			)
			(pin bidirectional line
				(at -58.42 -54.61 0)
				(length 7.62)
				(name "IO3/R18")
				(number "R18")
			)
			(pin bidirectional line
				(at -58.42 -55.88 0)
				(length 7.62)
				(name "IO3/P18")
				(number "P18")
			)
			(pin bidirectional line
				(at -58.42 -57.15 0)
				(length 7.62)
				(name "IO3/P17")
				(number "P17")
			)
			(pin bidirectional line
				(at -58.42 -58.42 0)
				(length 7.62)
				(name "IO3/P15")
				(number "P15")
			)
			(pin bidirectional line
				(at -58.42 -59.69 0)
				(length 7.62)
				(name "IO3/N15")
				(number "N15")
			)
			(pin bidirectional line
				(at -58.42 -60.96 0)
				(length 7.62)
				(name "IO3/M14")
				(number "M14")
			)
			(pin bidirectional line
				(at -58.42 -62.23 0)
				(length 7.62)
				(name "IO3/N14")
				(number "N14")
			)
			(pin bidirectional line
				(at -58.42 -63.5 0)
				(length 7.62)
				(name "IO3/M15")
				(number "M15")
			)
			(pin bidirectional line
				(at -58.42 -64.77 0)
				(length 7.62)
				(name "IO3VREF/M16")
				(number "M16")
			)
			(pin bidirectional line
				(at -58.42 -66.04 0)
				(length 7.62)
				(name "IO3/M18")
				(number "M18")
			)
			(pin bidirectional line
				(at -58.42 -67.31 0)
				(length 7.62)
				(name "IO3/N17")
				(number "N17")
			)
			(pin bidirectional line
				(at -58.42 -68.58 0)
				(length 7.62)
				(name "IO3/L14")
				(number "L14")
			)
			(pin bidirectional line
				(at -58.42 -69.85 0)
				(length 7.62)
				(name "IO3/L13")
				(number "L13")
			)
			(pin bidirectional line
				(at -58.42 -71.12 0)
				(length 7.62)
				(name "IO3/L15")
				(number "L15")
			)
			(pin bidirectional line
				(at -58.42 -72.39 0)
				(length 7.62)
				(name "IO3VREF/L16")
				(number "L16")
			)
			(pin bidirectional line
				(at -58.42 -73.66 0)
				(length 7.62)
				(name "IO3/L18")
				(number "L18")
			)
			(pin bidirectional line
				(at -58.42 -74.93 0)
				(length 7.62)
				(name "IO3/L17")
				(number "L17")
			)
			(pin bidirectional line
				(at -58.42 -76.2 0)
				(length 7.62)
				(name "IO3/K13")
				(number "K13")
			)
			(pin bidirectional line
				(at -58.42 -77.47 0)
				(length 7.62)
				(name "IO3/K14")
				(number "K14")
			)
			(pin bidirectional line
				(at -58.42 -78.74 0)
				(length 7.62)
				(name "IO3VREF/K17")
				(number "K17")
			)
			(pin bidirectional line
				(at -58.42 -80.01 0)
				(length 7.62)
				(name "IO3/K18")
				(number "K18")
			)
			(pin power_in line
				(at -36.83 90.17 270)
				(length 7.62)
				(name "VCCO0")
				(number "B8")
			)
			(pin power_in line
				(at -35.56 90.17 270)
				(length 7.62)
				(name "VCCO0")
				(number "C6")
			)
			(pin power_in line
				(at -34.29 90.17 270)
				(length 7.62)
				(name "VCCO0")
				(number "G8")
			)
			(pin power_in line
				(at -33.02 90.17 270)
				(length 7.62)
				(name "VCCO0")
				(number "G9")
			)
			(pin power_in line
				(at -30.48 90.17 270)
				(length 7.62)
				(name "VCCO1")
				(number "B11")
			)
			(pin power_in line
				(at -29.21 90.17 270)
				(length 7.62)
				(name "VCCO1")
				(number "C13")
			)
			(pin power_in line
				(at -27.94 90.17 270)
				(length 7.62)
				(name "VCCO1")
				(number "G10")
			)
			(pin power_in line
				(at -26.67 90.17 270)
				(length 7.62)
				(name "VCCO1")
				(number "G11")
			)
			(pin power_in line
				(at -25.4 -90.17 90)
				(length 7.62)
				(name "GND")
				(number "A1")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "A13")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "A18")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "A6")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "B17")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "B2")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "C10")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "C9")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "F1")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "F18")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "G12")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "G7")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "H10")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "H11")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "H8")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "H9")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "J11")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "J16")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "J3")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "J8")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "K11")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "K16")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "K3")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "K8")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "L10")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "L11")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "L8")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "L9")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "M12")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "M7")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "N1")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "N18")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "T10")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "T9")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "U17")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "U2")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "V1")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "V13")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "V18")
			)
			(pin passive line
				(at -25.4 -90.17 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "V6")
			)
			(pin power_in line
				(at -24.13 90.17 270)
				(length 7.62)
				(name "VCCO2")
				(number "F16")
			)
			(pin power_in line
				(at -22.86 90.17 270)
				(length 7.62)
				(name "VCCO2")
				(number "H12")
			)
			(pin power_in line
				(at -21.59 90.17 270)
				(length 7.62)
				(name "VCCO2")
				(number "J12")
			)
			(pin power_in line
				(at -19.05 90.17 270)
				(length 7.62)
				(name "VCCO3")
				(number "K12")
			)
			(pin power_in line
				(at -17.78 90.17 270)
				(length 7.62)
				(name "VCCO3")
				(number "L12")
			)
			(pin power_in line
				(at -16.51 90.17 270)
				(length 7.62)
				(name "VCCO3")
				(number "N16")
			)
			(pin power_in line
				(at -13.97 90.17 270)
				(length 7.62)
				(name "VCCO4")
				(number "M10")
			)
			(pin power_in line
				(at -12.7 90.17 270)
				(length 7.62)
				(name "VCCO4")
				(number "M11")
			)
			(pin power_in line
				(at -11.43 90.17 270)
				(length 7.62)
				(name "VCCO4")
				(number "T13")
			)
			(pin power_in line
				(at -10.16 90.17 270)
				(length 7.62)
				(name "VCCO4")
				(number "U11")
			)
			(pin power_in line
				(at -7.62 90.17 270)
				(length 7.62)
				(name "VCCO5")
				(number "M8")
			)
			(pin power_in line
				(at -6.35 90.17 270)
				(length 7.62)
				(name "VCCO5")
				(number "M9")
			)
			(pin power_in line
				(at -5.08 90.17 270)
				(length 7.62)
				(name "VCCO5")
				(number "T6")
			)
			(pin power_in line
				(at -3.81 90.17 270)
				(length 7.62)
				(name "VCCO5")
				(number "U8")
			)
			(pin power_in line
				(at -1.27 90.17 270)
				(length 7.62)
				(name "VCCO6")
				(number "K7")
			)
			(pin power_in line
				(at 0 90.17 270)
				(length 7.62)
				(name "VCCO6")
				(number "L7")
			)
			(pin power_in line
				(at 1.27 90.17 270)
				(length 7.62)
				(name "VCCO6")
				(number "N3")
			)
			(pin power_in line
				(at 3.81 90.17 270)
				(length 7.62)
				(name "VCCO7")
				(number "F3")
			)
			(pin power_in line
				(at 5.08 90.17 270)
				(length 7.62)
				(name "VCCO7")
				(number "H7")
			)
			(pin power_in line
				(at 6.35 90.17 270)
				(length 7.62)
				(name "VCCO7")
				(number "J7")
			)
			(pin power_in line
				(at 11.43 90.17 270)
				(length 7.62)
				(name "VCCAUX")
				(number "B12")
			)
			(pin power_in line
				(at 12.7 90.17 270)
				(length 7.62)
				(name "VCCAUX")
				(number "B7")
			)
			(pin power_in line
				(at 13.97 90.17 270)
				(length 7.62)
				(name "VCCAUX")
				(number "G17")
			)
			(pin power_in line
				(at 15.24 90.17 270)
				(length 7.62)
				(name "VCCAUX")
				(number "G2")
			)
			(pin power_in line
				(at 16.51 90.17 270)
				(length 7.62)
				(name "VCCAUX")
				(number "M17")
			)
			(pin power_in line
				(at 17.78 90.17 270)
				(length 7.62)
				(name "VCCAUX")
				(number "M2")
			)
			(pin power_in line
				(at 19.05 90.17 270)
				(length 7.62)
				(name "VCCAUX")
				(number "U12")
			)
			(pin power_in line
				(at 20.32 90.17 270)
				(length 7.62)
				(name "VCCAUX")
				(number "U7")
			)
			(pin power_in line
				(at 22.86 90.17 270)
				(length 7.62)
				(name "VCCINT")
				(number "F12")
			)
			(pin power_in line
				(at 24.13 90.17 270)
				(length 7.62)
				(name "VCCINT")
				(number "F13")
			)
			(pin power_in line
				(at 25.4 90.17 270)
				(length 7.62)
				(name "VCCINT")
				(number "F6")
			)
			(pin power_in line
				(at 26.67 90.17 270)
				(length 7.62)
				(name "VCCINT")
				(number "F7")
			)
			(pin power_in line
				(at 27.94 90.17 270)
				(length 7.62)
				(name "VCCINT")
				(number "G13")
			)
			(pin power_in line
				(at 29.21 90.17 270)
				(length 7.62)
				(name "VCCINT")
				(number "G6")
			)
			(pin power_in line
				(at 30.48 90.17 270)
				(length 7.62)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 31.75 90.17 270)
				(length 7.62)
				(name "VCCINT")
				(number "M6")
			)
			(pin power_in line
				(at 33.02 90.17 270)
				(length 7.62)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 34.29 90.17 270)
				(length 7.62)
				(name "VCCINT")
				(number "N13")
			)
			(pin power_in line
				(at 35.56 90.17 270)
				(length 7.62)
				(name "VCCINT")
				(number "N6")
			)
			(pin power_in line
				(at 36.83 90.17 270)
				(length 7.62)
				(name "VCCINT")
				(number "N7")
			)
			(pin input line
				(at 58.42 73.66 180)
				(length 7.62)
				(name "HSWAP/EN")
				(number "E6")
			)
			(pin bidirectional line
				(at 58.42 69.85 180)
				(length 7.62)
				(name "CS")
				(number "V2")
			)
			(pin bidirectional line
				(at 58.42 68.58 180)
				(length 7.62)
				(name "RDWR")
				(number "V3")
			)
			(pin output line
				(at 58.42 64.77 180)
				(length 7.62)
				(name "DOUT/BUSY")
				(number "V10")
			)
			(pin input line
				(at 58.42 63.5 180)
				(length 7.62)
				(name "DIN/D0")
				(number "T12")
			)
			(pin bidirectional line
				(at 58.42 58.42 180)
				(length 7.62)
				(name "IO7/J4")
				(number "J4")
			)
			(pin bidirectional line
				(at 58.42 57.15 180)
				(length 7.62)
				(name "IO7VREF/J5")
				(number "J5")
			)
			(pin bidirectional line
				(at 58.42 55.88 180)
				(length 7.62)
				(name "IO7/J2")
				(number "J2")
			)
			(pin bidirectional line
				(at 58.42 54.61 180)
				(length 7.62)
				(name "IO7/J1")
				(number "J1")
			)
			(pin bidirectional line
				(at 58.42 53.34 180)
				(length 7.62)
				(name "IO7/H2")
				(number "H2")
			)
			(pin bidirectional line
				(at 58.42 52.07 180)
				(length 7.62)
				(name "IO7/H1")
				(number "H1")
			)
			(pin bidirectional line
				(at 58.42 50.8 180)
				(length 7.62)
				(name "IO7/H3")
				(number "H3")
			)
			(pin bidirectional line
				(at 58.42 49.53 180)
				(length 7.62)
				(name "IO7/H4")
				(number "H4")
			)
			(pin bidirectional line
				(at 58.42 48.26 180)
				(length 7.62)
				(name "IO7VREF/H6")
				(number "H6")
			)
			(pin bidirectional line
				(at 58.42 46.99 180)
				(length 7.62)
				(name "IO7/H5")
				(number "H5")
			)
			(pin bidirectional line
				(at 58.42 45.72 180)
				(length 7.62)
				(name "IO7/G3")
				(number "G3")
			)
			(pin bidirectional line
				(at 58.42 44.45 180)
				(length 7.62)
				(name "IO7/G4")
				(number "G4")
			)
			(pin bidirectional line
				(at 58.42 43.18 180)
				(length 7.62)
				(name "IO7/F2")
				(number "F2")
			)
			(pin bidirectional line
				(at 58.42 41.91 180)
				(length 7.62)
				(name "IO7/G1")
				(number "G1")
			)
			(pin bidirectional line
				(at 58.42 40.64 180)
				(length 7.62)
				(name "IO7/F5")
				(number "F5")
			)
			(pin bidirectional line
				(at 58.42 39.37 180)
				(length 7.62)
				(name "IO7/G5")
				(number "G5")
			)
			(pin bidirectional line
				(at 58.42 38.1 180)
				(length 7.62)
				(name "IO7/F4")
				(number "F4")
			)
			(pin bidirectional line
				(at 58.42 36.83 180)
				(length 7.62)
				(name "IO7/E4")
				(number "E4")
			)
			(pin bidirectional line
				(at 58.42 35.56 180)
				(length 7.62)
				(name "IO7/E1")
				(number "E1")
			)
			(pin bidirectional line
				(at 58.42 34.29 180)
				(length 7.62)
				(name "IO7/E2")
				(number "E2")
			)
			(pin bidirectional line
				(at 58.42 33.02 180)
				(length 7.62)
				(name "IO7/D3")
				(number "D3")
			)
			(pin bidirectional line
				(at 58.42 31.75 180)
				(length 7.62)
				(name "IO7VREF/E3")
				(number "E3")
			)
			(pin bidirectional line
				(at 58.42 30.48 180)
				(length 7.62)
				(name "IO7/D2")
				(number "D2")
			)
			(pin bidirectional line
				(at 58.42 29.21 180)
				(length 7.62)
				(name "IO7/D1")
				(number "D1")
			)
			(pin bidirectional line
				(at 58.42 27.94 180)
				(length 7.62)
				(name "IO7VREF/B1")
				(number "B1")
			)
			(pin bidirectional line
				(at 58.42 26.67 180)
				(length 7.62)
				(name "IO7/C1")
				(number "C1")
			)
			(pin bidirectional line
				(at 58.42 25.4 180)
				(length 7.62)
				(name "IO7VRN/C2")
				(number "C2")
			)
			(pin bidirectional line
				(at 58.42 24.13 180)
				(length 7.62)
				(name "IO7VRP/C3")
				(number "C3")
			)
			(pin bidirectional line
				(at 58.42 22.86 180)
				(length 7.62)
				(name "IO7/J6")
				(number "J6")
			)
			(pin bidirectional line
				(at 58.42 20.32 180)
				(length 7.62)
				(name "IO6VREF/K2")
				(number "K2")
			)
			(pin bidirectional line
				(at 58.42 19.05 180)
				(length 7.62)
				(name "IO6/K1")
				(number "K1")
			)
			(pin bidirectional line
				(at 58.42 17.78 180)
				(length 7.62)
				(name "IO6/K4")
				(number "K4")
			)
			(pin bidirectional line
				(at 58.42 16.51 180)
				(length 7.62)
				(name "IO6/K5")
				(number "K5")
			)
			(pin bidirectional line
				(at 58.42 15.24 180)
				(length 7.62)
				(name "IO6/L1")
				(number "L1")
			)
			(pin bidirectional line
				(at 58.42 13.97 180)
				(length 7.62)
				(name "IO6/L2")
				(number "L2")
			)
			(pin bidirectional line
				(at 58.42 12.7 180)
				(length 7.62)
				(name "IO6/L4")
				(number "L4")
			)
			(pin bidirectional line
				(at 58.42 11.43 180)
				(length 7.62)
				(name "IO6VREF/L3")
				(number "L3")
			)
			(pin bidirectional line
				(at 58.42 10.16 180)
				(length 7.62)
				(name "IO6/L5")
				(number "L5")
			)
			(pin bidirectional line
				(at 58.42 8.89 180)
				(length 7.62)
				(name "IO6/L6")
				(number "L6")
			)
			(pin bidirectional line
				(at 58.42 7.62 180)
				(length 7.62)
				(name "IO6/M1")
				(number "M1")
			)
			(pin bidirectional line
				(at 58.42 6.35 180)
				(length 7.62)
				(name "IO6VREF/N2")
				(number "N2")
			)
			(pin bidirectional line
				(at 58.42 5.08 180)
				(length 7.62)
				(name "IO6/M4")
				(number "M4")
			)
			(pin bidirectional line
				(at 58.42 3.81 180)
				(length 7.62)
				(name "IO6/M3")
				(number "M3")
			)
			(pin bidirectional line
				(at 58.42 2.54 180)
				(length 7.62)
				(name "IO6/M5")
				(number "M5")
			)
			(pin bidirectional line
				(at 58.42 1.27 180)
				(length 7.62)
				(name "IO6/N5")
				(number "N5")
			)
			(pin bidirectional line
				(at 58.42 0 180)
				(length 7.62)
				(name "IO6/P4")
				(number "P4")
			)
			(pin bidirectional line
				(at 58.42 -1.27 180)
				(length 7.62)
				(name "IO6/N4")
				(number "N4")
			)
			(pin bidirectional line
				(at 58.42 -2.54 180)
				(length 7.62)
				(name "IO6/P1")
				(number "P1")
			)
			(pin bidirectional line
				(at 58.42 -3.81 180)
				(length 7.62)
				(name "IO6/P2")
				(number "P2")
			)
			(pin bidirectional line
				(at 58.42 -5.08 180)
				(length 7.62)
				(name "IO6/P3")
				(number "P3")
			)
			(pin bidirectional line
				(at 58.42 -6.35 180)
				(length 7.62)
				(name "IO6/R3")
				(number "R3")
			)
			(pin bidirectional line
				(at 58.42 -7.62 180)
				(length 7.62)
				(name "IO6VREF/R1")
				(number "R1")
			)
			(pin bidirectional line
				(at 58.42 -8.89 180)
				(length 7.62)
				(name "IO6/R2")
				(number "R2")
			)
			(pin bidirectional line
				(at 58.42 -10.16 180)
				(length 7.62)
				(name "IO6/T1")
				(number "T1")
			)
			(pin bidirectional line
				(at 58.42 -11.43 180)
				(length 7.62)
				(name "IO6/U1")
				(number "U1")
			)
			(pin bidirectional line
				(at 58.42 -12.7 180)
				(length 7.62)
				(name "IO6VRN/T2")
				(number "T2")
			)
			(pin bidirectional line
				(at 58.42 -13.97 180)
				(length 7.62)
				(name "IO6VRP/T3")
				(number "T3")
			)
			(pin bidirectional line
				(at 58.42 -15.24 180)
				(length 7.62)
				(name "IO6/K6")
				(number "K6")
			)
			(pin input clock
				(at 58.42 -17.78 180)
				(length 7.62)
				(name "GCLK2/P9")
				(number "P9")
			)
			(pin input clock
				(at 58.42 -19.05 180)
				(length 7.62)
				(name "GCLK3/N9")
				(number "N9")
			)
			(pin bidirectional line
				(at 58.42 -20.32 180)
				(length 7.62)
				(name "IO5D5/V9")
				(number "V9")
			)
			(pin bidirectional line
				(at 58.42 -21.59 180)
				(length 7.62)
				(name "IO5D4/U9")
				(number "U9")
			)
			(pin bidirectional line
				(at 58.42 -22.86 180)
				(length 7.62)
				(name "IO5/T8")
				(number "T8")
			)
			(pin bidirectional line
				(at 58.42 -24.13 180)
				(length 7.62)
				(name "IO5/R8")
				(number "R8")
			)
			(pin bidirectional line
				(at 58.42 -25.4 180)
				(length 7.62)
				(name "IO5VREF/V7")
				(number "V7")
			)
			(pin bidirectional line
				(at 58.42 -26.67 180)
				(length 7.62)
				(name "IO5/V8")
				(number "V8")
			)
			(pin bidirectional line
				(at 58.42 -27.94 180)
				(length 7.62)
				(name "IO5D7/T7")
				(number "T7")
			)
			(pin bidirectional line
				(at 58.42 -29.21 180)
				(length 7.62)
				(name "IO5D6/R7")
				(number "R7")
			)
			(pin bidirectional line
				(at 58.42 -30.48 180)
				(length 7.62)
				(name "IO5/P7")
				(number "P7")
			)
			(pin bidirectional line
				(at 58.42 -31.75 180)
				(length 7.62)
				(name "IO5VREF/P6")
				(number "P6")
			)
			(pin bidirectional line
				(at 58.42 -33.02 180)
				(length 7.62)
				(name "IO5/U5")
				(number "U5")
			)
			(pin bidirectional line
				(at 58.42 -34.29 180)
				(length 7.62)
				(name "IO5/V5")
				(number "V5")
			)
			(pin bidirectional line
				(at 58.42 -35.56 180)
				(length 7.62)
				(name "IO5/R5")
				(number "R5")
			)
			(pin bidirectional line
				(at 58.42 -36.83 180)
				(length 7.62)
				(name "IO5/R6")
				(number "R6")
			)
			(pin bidirectional line
				(at 58.42 -38.1 180)
				(length 7.62)
				(name "IO5VRN/U4")
				(number "U4")
			)
			(pin bidirectional line
				(at 58.42 -39.37 180)
				(length 7.62)
				(name "IO5VRP/V4")
				(number "V4")
			)
			(pin bidirectional line
				(at 58.42 -40.64 180)
				(length 7.62)
				(name "IO5/T4")
				(number "T4")
			)
			(pin bidirectional line
				(at 58.42 -41.91 180)
				(length 7.62)
				(name "IO5/T5")
				(number "T5")
			)
			(pin bidirectional line
				(at 58.42 -43.18 180)
				(length 7.62)
				(name "IO5VREF/R9")
				(number "R9")
			)
			(pin bidirectional line
				(at 58.42 -44.45 180)
				(length 7.62)
				(name "IO5/U6")
				(number "U6")
			)
			(pin bidirectional line
				(at 58.42 -45.72 180)
				(length 7.62)
				(name "IO5/P8")
				(number "P8")
			)
			(pin bidirectional line
				(at 58.42 -46.99 180)
				(length 7.62)
				(name "IO5/N8")
				(number "N8")
			)
			(pin input clock
				(at 58.42 -49.53 180)
				(length 7.62)
				(name "GCLK0/P10")
				(number "P10")
			)
			(pin input clock
				(at 58.42 -50.8 180)
				(length 7.62)
				(name "GCLK1/N10")
				(number "N10")
			)
			(pin bidirectional line
				(at 58.42 -52.07 180)
				(length 7.62)
				(name "IO4D3/P11")
				(number "P11")
			)
			(pin bidirectional line
				(at 58.42 -53.34 180)
				(length 7.62)
				(name "IO4D2/N11")
				(number "N11")
			)
			(pin bidirectional line
				(at 58.42 -54.61 180)
				(length 7.62)
				(name "IO4/T11")
				(number "T11")
			)
			(pin bidirectional line
				(at 58.42 -55.88 180)
				(length 7.62)
				(name "IO4/R11")
				(number "R11")
			)
			(pin bidirectional line
				(at 58.42 -57.15 180)
				(length 7.62)
				(name "IO4/V11")
				(number "V11")
			)
			(pin bidirectional line
				(at 58.42 -58.42 180)
				(length 7.62)
				(name "IO4/V12")
				(number "V12")
			)
			(pin bidirectional line
				(at 58.42 -59.69 180)
				(length 7.62)
				(name "IO4D1/R12")
				(number "R12")
			)
			(pin bidirectional line
				(at 58.42 -60.96 180)
				(length 7.62)
				(name "IO4/P13")
				(number "P13")
			)
			(pin bidirectional line
				(at 58.42 -62.23 180)
				(length 7.62)
				(name "IO4/R13")
				(number "R13")
			)
			(pin bidirectional line
				(at 58.42 -63.5 180)
				(length 7.62)
				(name "IO4/U14")
				(number "U14")
			)
			(pin bidirectional line
				(at 58.42 -64.77 180)
				(length 7.62)
				(name "IO4/T14")
				(number "T14")
			)
			(pin bidirectional line
				(at 58.42 -66.04 180)
				(length 7.62)
				(name "IO4/V15")
				(number "V15")
			)
			(pin bidirectional line
				(at 58.42 -67.31 180)
				(length 7.62)
				(name "IO4/U15")
				(number "U15")
			)
			(pin bidirectional line
				(at 58.42 -68.58 180)
				(length 7.62)
				(name "IO4/R14")
				(number "R14")
			)
			(pin bidirectional line
				(at 58.42 -69.85 180)
				(length 7.62)
				(name "IO4VREF/P14")
				(number "P14")
			)
			(pin bidirectional line
				(at 58.42 -71.12 180)
				(length 7.62)
				(name "IO4VRN/V16")
				(number "V16")
			)
			(pin bidirectional line
				(at 58.42 -72.39 180)
				(length 7.62)
				(name "IO4VRP/U16")
				(number "U16")
			)
			(pin bidirectional line
				(at 58.42 -73.66 180)
				(length 7.62)
				(name "IO4VREF/V17")
				(number "V17")
			)
			(pin bidirectional line
				(at 58.42 -74.93 180)
				(length 7.62)
				(name "IO4VREF/U13")
				(number "U13")
			)
			(pin bidirectional line
				(at 58.42 -76.2 180)
				(length 7.62)
				(name "IO4VREF/R10")
				(number "R10")
			)
			(pin bidirectional line
				(at 58.42 -77.47 180)
				(length 7.62)
				(name "IO4/V14")
				(number "V14")
			)
			(pin bidirectional line
				(at 58.42 -78.74 180)
				(length 7.62)
				(name "IO4/P12")
				(number "P12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC3S400-PQ208"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 41.91 116.84 0)
		)
		(property "Value" "XC3S400-PQ208"
			(at 43.18 -118.11 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC3S400-PQ208_0_0"
			(text "7"
				(at -10.16 58.42 0)
			)
			(text "6"
				(at -10.16 5.08 0)
			)
			(text "5"
				(at -10.16 -41.91 0)
			)
			(text "4"
				(at -10.16 -82.55 0)
			)
			(text "0"
				(at 13.97 62.23 0)
			)
			(text "1"
				(at 13.97 21.59 0)
			)
			(text "2"
				(at 13.97 -25.4 0)
			)
			(text "3"
				(at 13.97 -77.47 0)
			)
		)
		(symbol "XC3S400-PQ208_0_1")
		(symbol "XC3S400-PQ208_1_1"
			(pin bidirectional line
				(at -54.61 111.76 0)
				(length 7.62)
				(name "TMS")
				(number "160")
			)
			(pin bidirectional line
				(at -54.61 109.22 0)
				(length 7.62)
				(name "TDO")
				(number "158")
			)
			(pin bidirectional line
				(at -54.61 106.68 0)
				(length 7.62)
				(name "TDI")
				(number "208")
			)
			(pin bidirectional line
				(at -54.61 104.14 0)
				(length 7.62)
				(name "TCK")
				(number "159")
			)
			(pin input line
				(at -54.61 100.33 0)
				(length 7.62)
				(name "PROG_B")
				(number "207")
			)
			(pin input line
				(at -54.61 97.79 0)
				(length 7.62)
				(name "HSWAP_EN")
				(number "206")
			)
			(pin bidirectional line
				(at -54.61 95.25 0)
				(length 7.62)
				(name "DONE")
				(number "103")
			)
			(pin bidirectional clock
				(at -54.61 92.71 0)
				(length 7.62)
				(name "CCLK")
				(number "104")
			)
			(pin input line
				(at -54.61 88.9 0)
				(length 7.62)
				(name "M0")
				(number "55")
			)
			(pin input line
				(at -54.61 86.36 0)
				(length 7.62)
				(name "M1")
				(number "54")
			)
			(pin input line
				(at -54.61 83.82 0)
				(length 7.62)
				(name "M2")
				(number "56")
			)
			(pin bidirectional line
				(at -54.61 80.01 0)
				(length 7.62)
				(name "IO_L01P_7/VRN_7")
				(number "2")
			)
			(pin bidirectional line
				(at -54.61 77.47 0)
				(length 7.62)
				(name "IO_L01N_7/VRP_7")
				(number "3")
			)
			(pin bidirectional line
				(at -54.61 74.93 0)
				(length 7.62)
				(name "IO_L16P_7/VREF_7")
				(number "4")
			)
			(pin bidirectional line
				(at -54.61 72.39 0)
				(length 7.62)
				(name "IO_L16N_7")
				(number "5")
			)
			(pin bidirectional line
				(at -54.61 69.85 0)
				(length 7.62)
				(name "IO_L19P_7")
				(number "7")
			)
			(pin bidirectional line
				(at -54.61 67.31 0)
				(length 7.62)
				(name "IO_L19N_7/VREF_7")
				(number "9")
			)
			(pin bidirectional line
				(at -54.61 64.77 0)
				(length 7.62)
				(name "IO_L20P_7")
				(number "10")
			)
			(pin bidirectional line
				(at -54.61 62.23 0)
				(length 7.62)
				(name "IO_L20N_7")
				(number "11")
			)
			(pin bidirectional line
				(at -54.61 59.69 0)
				(length 7.62)
				(name "IO_L21P_7")
				(number "12")
			)
			(pin bidirectional line
				(at -54.61 57.15 0)
				(length 7.62)
				(name "IO_L21N_7")
				(number "13")
			)
			(pin bidirectional line
				(at -54.61 54.61 0)
				(length 7.62)
				(name "IO_L22P_7")
				(number "15")
			)
			(pin bidirectional line
				(at -54.61 52.07 0)
				(length 7.62)
				(name "IO_L22N_7")
				(number "16")
			)
			(pin bidirectional line
				(at -54.61 49.53 0)
				(length 7.62)
				(name "IO_L23P_7")
				(number "18")
			)
			(pin bidirectional line
				(at -54.61 46.99 0)
				(length 7.62)
				(name "IO_L23N_7")
				(number "19")
			)
			(pin bidirectional line
				(at -54.61 44.45 0)
				(length 7.62)
				(name "IO_L24P_7")
				(number "20")
			)
			(pin bidirectional line
				(at -54.61 41.91 0)
				(length 7.62)
				(name "IO_L24N_7")
				(number "21")
			)
			(pin bidirectional line
				(at -54.61 39.37 0)
				(length 7.62)
				(name "IO_L39P_7")
				(number "22")
			)
			(pin bidirectional line
				(at -54.61 36.83 0)
				(length 7.62)
				(name "IO_L39N_7")
				(number "24")
			)
			(pin bidirectional line
				(at -54.61 34.29 0)
				(length 7.62)
				(name "IO_L40P_7")
				(number "26")
			)
			(pin bidirectional line
				(at -54.61 31.75 0)
				(length 7.62)
				(name "IO_L40N_7/VREF_7")
				(number "27")
			)
			(pin bidirectional line
				(at -54.61 26.67 0)
				(length 7.62)
				(name "IO_L40P_6/VREF_6")
				(number "28")
			)
			(pin bidirectional line
				(at -54.61 24.13 0)
				(length 7.62)
				(name "IO_L40N_6")
				(number "29")
			)
			(pin bidirectional line
				(at -54.61 21.59 0)
				(length 7.62)
				(name "IO_L39P_6")
				(number "31")
			)
			(pin bidirectional line
				(at -54.61 19.05 0)
				(length 7.62)
				(name "IO_L39N_6")
				(number "33")
			)
			(pin bidirectional line
				(at -54.61 16.51 0)
				(length 7.62)
				(name "IO_L24P_6")
				(number "34")
			)
			(pin bidirectional line
				(at -54.61 13.97 0)
				(length 7.62)
				(name "IO_L24N_6/VREF_6")
				(number "35")
			)
			(pin bidirectional line
				(at -54.61 11.43 0)
				(length 7.62)
				(name "IO_L23P_6")
				(number "36")
			)
			(pin bidirectional line
				(at -54.61 8.89 0)
				(length 7.62)
				(name "IO_L23N_6")
				(number "37")
			)
			(pin bidirectional line
				(at -54.61 6.35 0)
				(length 7.62)
				(name "IO_L22P_6")
				(number "39")
			)
			(pin bidirectional line
				(at -54.61 3.81 0)
				(length 7.62)
				(name "IO_L22N_6")
				(number "40")
			)
			(pin bidirectional line
				(at -54.61 1.27 0)
				(length 7.62)
				(name "IO_L21P_6")
				(number "42")
			)
			(pin bidirectional line
				(at -54.61 -1.27 0)
				(length 7.62)
				(name "IO_L21N_6")
				(number "43")
			)
			(pin bidirectional line
				(at -54.61 -3.81 0)
				(length 7.62)
				(name "IO_L20P_6")
				(number "44")
			)
			(pin bidirectional line
				(at -54.61 -6.35 0)
				(length 7.62)
				(name "IO_L20N_6")
				(number "45")
			)
			(pin bidirectional line
				(at -54.61 -8.89 0)
				(length 7.62)
				(name "IO_L19P_6")
				(number "46")
			)
			(pin bidirectional line
				(at -54.61 -11.43 0)
				(length 7.62)
				(name "IO_L19N_6")
				(number "48")
			)
			(pin bidirectional line
				(at -54.61 -13.97 0)
				(length 7.62)
				(name "IO/VREF_6")
				(number "50")
			)
			(pin bidirectional line
				(at -54.61 -16.51 0)
				(length 7.62)
				(name "IO_L01P_6/VRN_6")
				(number "51")
			)
			(pin bidirectional line
				(at -54.61 -19.05 0)
				(length 7.62)
				(name "IO_L01N_6/VRP_6")
				(number "52")
			)
			(pin bidirectional line
				(at -54.61 -24.13 0)
				(length 7.62)
				(name "IO_L01P_5/CS_B")
				(number "57")
			)
			(pin bidirectional line
				(at -54.61 -26.67 0)
				(length 7.62)
				(name "IO_L01N_5/RDWR_B")
				(number "58")
			)
			(pin bidirectional line
				(at -54.61 -29.21 0)
				(length 7.62)
				(name "IO_L10P_5/VRN_5")
				(number "61")
			)
			(pin bidirectional line
				(at -54.61 -31.75 0)
				(length 7.62)
				(name "IO_L10N_5/VRP_5")
				(number "62")
			)
			(pin bidirectional line
				(at -54.61 -34.29 0)
				(length 7.62)
				(name "IO")
				(number "63")
			)
			(pin bidirectional line
				(at -54.61 -36.83 0)
				(length 7.62)
				(name "IO_L27P_5")
				(number "64")
			)
			(pin bidirectional line
				(at -54.61 -39.37 0)
				(length 7.62)
				(name "IO_L27N_5/VREF_5")
				(number "65")
			)
			(pin bidirectional line
				(at -54.61 -41.91 0)
				(length 7.62)
				(name "IO_L28P_5/D7")
				(number "67")
			)
			(pin bidirectional line
				(at -54.61 -44.45 0)
				(length 7.62)
				(name "IO_L28N_5/D6")
				(number "68")
			)
			(pin bidirectional line
				(at -54.61 -46.99 0)
				(length 7.62)
				(name "IO")
				(number "71")
			)
			(pin bidirectional line
				(at -54.61 -49.53 0)
				(length 7.62)
				(name "IO_L31P_5/D5")
				(number "72")
			)
			(pin bidirectional line
				(at -54.61 -52.07 0)
				(length 7.62)
				(name "IO_L31N_5/D4")
				(number "74")
			)
			(pin bidirectional clock
				(at -54.61 -54.61 0)
				(length 7.62)
				(name "IO_L32P_5/GCLK2")
				(number "76")
			)
			(pin bidirectional clock
				(at -54.61 -57.15 0)
				(length 7.62)
				(name "IO_L32N_5/GCLK3")
				(number "77")
			)
			(pin bidirectional line
				(at -54.61 -59.69 0)
				(length 7.62)
				(name "IO/VREF_5")
				(number "78")
			)
			(pin bidirectional clock
				(at -54.61 -64.77 0)
				(length 7.62)
				(name "IO_L32P_4/GCLK0")
				(number "79")
			)
			(pin bidirectional clock
				(at -54.61 -67.31 0)
				(length 7.62)
				(name "IO_L32N_4/GCLK1")
				(number "80")
			)
			(pin bidirectional line
				(at -54.61 -69.85 0)
				(length 7.62)
				(name "IO_L31P_4/DOUT/BUSY")
				(number "81")
			)
			(pin bidirectional line
				(at -54.61 -72.39 0)
				(length 7.62)
				(name "IO_L31N_4/INIT_B")
				(number "83")
			)
			(pin bidirectional line
				(at -54.61 -74.93 0)
				(length 7.62)
				(name "IO/VREF_4")
				(number "85")
			)
			(pin bidirectional line
				(at -54.61 -77.47 0)
				(length 7.62)
				(name "IO_L30P_4/D3")
				(number "86")
			)
			(pin bidirectional line
				(at -54.61 -80.01 0)
				(length 7.62)
				(name "IO_L30N_4/D2")
				(number "87")
			)
			(pin bidirectional line
				(at -54.61 -82.55 0)
				(length 7.62)
				(name "IO_L27P_4/D1")
				(number "90")
			)
			(pin bidirectional line
				(at -54.61 -85.09 0)
				(length 7.62)
				(name "IO_L27N_4/DIN/D0")
				(number "92")
			)
			(pin bidirectional line
				(at -54.61 -87.63 0)
				(length 7.62)
				(name "IO")
				(number "93")
			)
			(pin bidirectional line
				(at -54.61 -90.17 0)
				(length 7.62)
				(name "IO_L25P_4")
				(number "94")
			)
			(pin bidirectional line
				(at -54.61 -92.71 0)
				(length 7.62)
				(name "IO_L25N_4")
				(number "95")
			)
			(pin bidirectional line
				(at -54.61 -95.25 0)
				(length 7.62)
				(name "IO/VREF_4")
				(number "96")
			)
			(pin bidirectional line
				(at -54.61 -97.79 0)
				(length 7.62)
				(name "IO")
				(number "97")
			)
			(pin bidirectional line
				(at -54.61 -100.33 0)
				(length 7.62)
				(name "IO_L01P_4/VRN_4")
				(number "100")
			)
			(pin bidirectional line
				(at -54.61 -102.87 0)
				(length 7.62)
				(name "IO_L01N_4/VRP_4")
				(number "101")
			)
			(pin bidirectional line
				(at -54.61 -105.41 0)
				(length 7.62)
				(name "IO/VREF_4")
				(number "102")
			)
			(pin power_in line
				(at -36.83 121.92 270)
				(length 7.62)
				(name "VCCO_0")
				(number "201")
			)
			(pin power_in line
				(at -34.29 121.92 270)
				(length 7.62)
				(name "VCCO_0")
				(number "188")
			)
			(pin power_in line
				(at -31.75 121.92 270)
				(length 7.62)
				(name "VCCO_1")
				(number "177")
			)
			(pin power_in line
				(at -31.75 -121.92 90)
				(length 7.62)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "105")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "112")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "118")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "129")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "134")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "145")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "151")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "157")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "163")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "170")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "179")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "186")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "195")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "202")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "47")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "59")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "66")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "75")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "82")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "91")
			)
			(pin passive line
				(at -31.75 -121.92 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "99")
			)
			(pin power_in line
				(at -29.21 121.92 270)
				(length 7.62)
				(name "VCCO_1")
				(number "164")
			)
			(pin power_in line
				(at -26.67 121.92 270)
				(length 7.62)
				(name "VCCO_2")
				(number "153")
			)
			(pin power_in line
				(at -24.13 121.92 270)
				(length 7.62)
				(name "VCCO_2")
				(number "136")
			)
			(pin power_in line
				(at -21.59 121.92 270)
				(length 7.62)
				(name "VCCO_3")
				(number "127")
			)
			(pin power_in line
				(at -19.05 121.92 270)
				(length 7.62)
				(name "VCCO_3")
				(number "110")
			)
			(pin power_in line
				(at -16.51 121.92 270)
				(length 7.62)
				(name "VCCO_4")
				(number "98")
			)
			(pin power_in line
				(at -13.97 121.92 270)
				(length 7.62)
				(name "VCCO_4")
				(number "84")
			)
			(pin power_in line
				(at -11.43 121.92 270)
				(length 7.62)
				(name "VCCO_5")
				(number "73")
			)
			(pin power_in line
				(at -8.89 121.92 270)
				(length 7.62)
				(name "VCCO_5")
				(number "60")
			)
			(pin passive line
				(at -6.35 121.92 270)
				(length 7.62)
				(name "VCCO_6")
				(number "49")
			)
			(pin power_in line
				(at -3.81 121.92 270)
				(length 7.62)
				(name "VCCO_6")
				(number "32")
			)
			(pin power_in line
				(at -1.27 121.92 270)
				(length 7.62)
				(name "VCCO_7")
				(number "23")
			)
			(pin power_in line
				(at 1.27 121.92 270)
				(length 7.62)
				(name "VCCO_7")
				(number "6")
			)
			(pin power_in line
				(at 8.89 121.92 270)
				(length 7.62)
				(name "VCCAUX")
				(number "193")
			)
			(pin power_in line
				(at 11.43 121.92 270)
				(length 7.62)
				(name "VCCAUX")
				(number "173")
			)
			(pin power_in line
				(at 13.97 121.92 270)
				(length 7.62)
				(name "VCCAUX")
				(number "142")
			)
			(pin power_in line
				(at 16.51 121.92 270)
				(length 7.62)
				(name "VCCAUX")
				(number "121")
			)
			(pin power_in line
				(at 19.05 121.92 270)
				(length 7.62)
				(name "VCCAUX")
				(number "89")
			)
			(pin power_in line
				(at 21.59 121.92 270)
				(length 7.62)
				(name "VCCAUX")
				(number "69")
			)
			(pin power_in line
				(at 24.13 121.92 270)
				(length 7.62)
				(name "VCCAUX")
				(number "38")
			)
			(pin power_in line
				(at 26.67 121.92 270)
				(length 7.62)
				(name "VCCAUX")
				(number "17")
			)
			(pin power_in line
				(at 29.21 121.92 270)
				(length 7.62)
				(name "VCCINT")
				(number "192")
			)
			(pin power_in line
				(at 31.75 121.92 270)
				(length 7.62)
				(name "VCCINT")
				(number "174")
			)
			(pin power_in line
				(at 34.29 121.92 270)
				(length 7.62)
				(name "VCCINT")
				(number "88")
			)
			(pin power_in line
				(at 36.83 121.92 270)
				(length 7.62)
				(name "VCCINT")
				(number "70")
			)
			(pin bidirectional line
				(at 54.61 81.28 180)
				(length 7.62)
				(name "IO/VREF_0")
				(number "205")
			)
			(pin bidirectional line
				(at 54.61 78.74 180)
				(length 7.62)
				(name "IO_L01N_0/VRP_0")
				(number "204")
			)
			(pin bidirectional line
				(at 54.61 76.2 180)
				(length 7.62)
				(name "IO_L01P_0/VRN_0")
				(number "203")
			)
			(pin bidirectional line
				(at 54.61 73.66 180)
				(length 7.62)
				(name "IO/VREF_0")
				(number "200")
			)
			(pin bidirectional line
				(at 54.61 71.12 180)
				(length 7.62)
				(name "IO_L25N_0")
				(number "199")
			)
			(pin bidirectional line
				(at 54.61 68.58 180)
				(length 7.62)
				(name "IO_L25P_0")
				(number "198")
			)
			(pin bidirectional line
				(at 54.61 66.04 180)
				(length 7.62)
				(name "IO")
				(number "197")
			)
			(pin bidirectional line
				(at 54.61 63.5 180)
				(length 7.62)
				(name "IO_L27N_0")
				(number "196")
			)
			(pin bidirectional line
				(at 54.61 60.96 180)
				(length 7.62)
				(name "IO_L27P_0")
				(number "194")
			)
			(pin bidirectional line
				(at 54.61 58.42 180)
				(length 7.62)
				(name "IO_L30N_0")
				(number "191")
			)
			(pin bidirectional line
				(at 54.61 55.88 180)
				(length 7.62)
				(name "IO_L30P_0")
				(number "190")
			)
			(pin bidirectional line
				(at 54.61 53.34 180)
				(length 7.62)
				(name "IO")
				(number "189")
			)
			(pin bidirectional line
				(at 54.61 50.8 180)
				(length 7.62)
				(name "IO_L31N_0")
				(number "187")
			)
			(pin bidirectional line
				(at 54.61 48.26 180)
				(length 7.62)
				(name "IO_L31P_0/VREF_0")
				(number "185")
			)
			(pin bidirectional clock
				(at 54.61 45.72 180)
				(length 7.62)
				(name "IO_L32N_0/GCLK7")
				(number "184")
			)
			(pin bidirectional clock
				(at 54.61 43.18 180)
				(length 7.62)
				(name "IO_L32P_0/GCLK6")
				(number "183")
			)
			(pin bidirectional line
				(at 54.61 38.1 180)
				(length 7.62)
				(name "IO")
				(number "182")
			)
			(pin bidirectional clock
				(at 54.61 35.56 180)
				(length 7.62)
				(name "IO_L32N_1GCLK5")
				(number "181")
			)
			(pin bidirectional clock
				(at 54.61 33.02 180)
				(length 7.62)
				(name "IO_L32P_1/GCLK4")
				(number "180")
			)
			(pin bidirectional line
				(at 54.61 30.48 180)
				(length 7.62)
				(name "IO_L31N_1/VREF_1")
				(number "178")
			)
			(pin bidirectional line
				(at 54.61 27.94 180)
				(length 7.62)
				(name "IO_L31P_1")
				(number "176")
			)
			(pin bidirectional line
				(at 54.61 25.4 180)
				(length 7.62)
				(name "IO")
				(number "175")
			)
			(pin bidirectional line
				(at 54.61 22.86 180)
				(length 7.62)
				(name "IO_L28N_1")
				(number "172")
			)
			(pin bidirectional line
				(at 54.61 20.32 180)
				(length 7.62)
				(name "IO_L28P_1")
				(number "171")
			)
			(pin bidirectional line
				(at 54.61 17.78 180)
				(length 7.62)
				(name "IO_L27N_1")
				(number "169")
			)
			(pin bidirectional line
				(at 54.61 15.24 180)
				(length 7.62)
				(name "IO_L27P_1")
				(number "168")
			)
			(pin bidirectional line
				(at 54.61 12.7 180)
				(length 7.62)
				(name "IO")
				(number "167")
			)
			(pin bidirectional line
				(at 54.61 10.16 180)
				(length 7.62)
				(name "IO_L10N_1/VREF_1")
				(number "166")
			)
			(pin bidirectional line
				(at 54.61 7.62 180)
				(length 7.62)
				(name "IO_L10P_1")
				(number "165")
			)
			(pin bidirectional line
				(at 54.61 5.08 180)
				(length 7.62)
				(name "IO_L01N_1/VRP_1")
				(number "162")
			)
			(pin bidirectional line
				(at 54.61 2.54 180)
				(length 7.62)
				(name "IO_L01P_1/VRN_1")
				(number "161")
			)
			(pin bidirectional line
				(at 54.61 -2.54 180)
				(length 7.62)
				(name "IO_L01N_2/VRP_2")
				(number "156")
			)
			(pin bidirectional line
				(at 54.61 -5.08 180)
				(length 7.62)
				(name "IO_L01P_2/VRN_2")
				(number "155")
			)
			(pin bidirectional line
				(at 54.61 -7.62 180)
				(length 7.62)
				(name "IO/VREF_2")
				(number "154")
			)
			(pin bidirectional line
				(at 54.61 -10.16 180)
				(length 7.62)
				(name "IO_L19N_2")
				(number "152")
			)
			(pin bidirectional line
				(at 54.61 -12.7 180)
				(length 7.62)
				(name "IO_L19P_2")
				(number "150")
			)
			(pin bidirectional line
				(at 54.61 -15.24 180)
				(length 7.62)
				(name "IO_L20N_2")
				(number "149")
			)
			(pin bidirectional line
				(at 54.61 -17.78 180)
				(length 7.62)
				(name "IO_L20P_2")
				(number "148")
			)
			(pin bidirectional line
				(at 54.61 -20.32 180)
				(length 7.62)
				(name "IO-L21N_2")
				(number "147")
			)
			(pin bidirectional line
				(at 54.61 -22.86 180)
				(length 7.62)
				(name "IO_L21P_2")
				(number "146")
			)
			(pin bidirectional line
				(at 54.61 -25.4 180)
				(length 7.62)
				(name "IO_L22N_2")
				(number "144")
			)
			(pin bidirectional line
				(at 54.61 -27.94 180)
				(length 7.62)
				(name "IO_L22P_2")
				(number "143")
			)
			(pin bidirectional line
				(at 54.61 -30.48 180)
				(length 7.62)
				(name "IO_L23N_2/VREF_2")
				(number "141")
			)
			(pin bidirectional line
				(at 54.61 -33.02 180)
				(length 7.62)
				(name "IO_L23P_2")
				(number "140")
			)
			(pin bidirectional line
				(at 54.61 -35.56 180)
				(length 7.62)
				(name "IO_L24N_2")
				(number "139")
			)
			(pin bidirectional line
				(at 54.61 -38.1 180)
				(length 7.62)
				(name "IO_L24P_2")
				(number "138")
			)
			(pin bidirectional line
				(at 54.61 -40.64 180)
				(length 7.62)
				(name "IO_L39N_2")
				(number "137")
			)
			(pin bidirectional line
				(at 54.61 -43.18 180)
				(length 7.62)
				(name "IO_L39P_2")
				(number "135")
			)
			(pin bidirectional line
				(at 54.61 -45.72 180)
				(length 7.62)
				(name "IO_L40N_2")
				(number "133")
			)
			(pin bidirectional line
				(at 54.61 -48.26 180)
				(length 7.62)
				(name "IO_L40P_2/VREF_2")
				(number "132")
			)
			(pin bidirectional line
				(at 54.61 -53.34 180)
				(length 7.62)
				(name "IO_L40N_3/VREF_3")
				(number "131")
			)
			(pin bidirectional line
				(at 54.61 -55.88 180)
				(length 7.62)
				(name "IO_L40P_3")
				(number "130")
			)
			(pin bidirectional line
				(at 54.61 -58.42 180)
				(length 7.62)
				(name "IO_L39N_3")
				(number "128")
			)
			(pin bidirectional line
				(at 54.61 -60.96 180)
				(length 7.62)
				(name "IO_L39P_3")
				(number "126")
			)
			(pin bidirectional line
				(at 54.61 -63.5 180)
				(length 7.62)
				(name "IO_L24N_3")
				(number "125")
			)
			(pin bidirectional line
				(at 54.61 -66.04 180)
				(length 7.62)
				(name "IO_L24P_3")
				(number "124")
			)
			(pin bidirectional line
				(at 54.61 -68.58 180)
				(length 7.62)
				(name "IO_L23N_3")
				(number "123")
			)
			(pin bidirectional line
				(at 54.61 -71.12 180)
				(length 7.62)
				(name "IO_L23P_3/VREF_3")
				(number "122")
			)
			(pin bidirectional line
				(at 54.61 -73.66 180)
				(length 7.62)
				(name "IO_L22N_3")
				(number "120")
			)
			(pin bidirectional line
				(at 54.61 -76.2 180)
				(length 7.62)
				(name "IO_L22P_3")
				(number "119")
			)
			(pin bidirectional line
				(at 54.61 -78.74 180)
				(length 7.62)
				(name "IO_L21N_3")
				(number "117")
			)
			(pin bidirectional line
				(at 54.61 -81.28 180)
				(length 7.62)
				(name "IO_L21P_3")
				(number "116")
			)
			(pin bidirectional line
				(at 54.61 -83.82 180)
				(length 7.62)
				(name "IO_L20N_3")
				(number "115")
			)
			(pin bidirectional line
				(at 54.61 -86.36 180)
				(length 7.62)
				(name "IO_L20P_3")
				(number "114")
			)
			(pin bidirectional line
				(at 54.61 -88.9 180)
				(length 7.62)
				(name "IO_L19N_3")
				(number "113")
			)
			(pin bidirectional line
				(at 54.61 -91.44 180)
				(length 7.62)
				(name "IO_L19P_3")
				(number "111")
			)
			(pin bidirectional line
				(at 54.61 -93.98 180)
				(length 7.62)
				(name "IO_L17N_3")
				(number "109")
			)
			(pin bidirectional line
				(at 54.61 -96.52 180)
				(length 7.62)
				(name "IO_L17P_3/VREF_3")
				(number "108")
			)
			(pin bidirectional line
				(at 54.61 -99.06 180)
				(length 7.62)
				(name "IO_L01N_3/VRP_3")
				(number "107")
			)
			(pin bidirectional line
				(at 54.61 -101.6 180)
				(length 7.62)
				(name "IO_L01P_3/VRN_3")
				(number "106")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC3S50-VQ100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 26.67 66.04 0)
		)
		(property "Value" "XC3S50-VQ100"
			(at 24.13 -68.58 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "xilinx/spartan2e/spartan2e.pdf"
			(at 0 0 0)
		)
		(property "Description" "spartan 2"
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC3S50-VQ100_0_0"
			(text "Bank7"
				(at -17.78 17.78 900)
			)
			(text "Bank6"
				(at -17.78 -6.35 900)
			)
			(text "Bank5"
				(at -17.78 -29.21 900)
			)
			(text "Bank4"
				(at -17.78 -52.07 900)
			)
			(text "Bank0"
				(at 15.24 16.51 900)
			)
			(text "Bank1"
				(at 15.24 -6.35 900)
			)
			(text "Bank2"
				(at 15.24 -29.21 900)
			)
			(text "Bank3"
				(at 15.24 -52.07 900)
			)
		)
		(symbol "XC3S50-VQ100_0_1")
		(symbol "XC3S50-VQ100_1_1"
			(pin input line
				(at -41.91 60.96 0)
				(length 7.62)
				(name "TMS")
				(number "78")
			)
			(pin output line
				(at -41.91 58.42 0)
				(length 7.62)
				(name "TDO")
				(number "76")
			)
			(pin input line
				(at -41.91 55.88 0)
				(length 7.62)
				(name "TDI")
				(number "100")
			)
			(pin input line
				(at -41.91 53.34 0)
				(length 7.62)
				(name "TCK")
				(number "77")
			)
			(pin open_collector line
				(at -41.91 48.26 0)
				(length 7.62)
				(name "DONE")
				(number "51")
			)
			(pin input line
				(at -41.91 45.72 0)
				(length 7.62)
				(name "~{PROG}")
				(number "99")
			)
			(pin bidirectional line
				(at -41.91 43.18 0)
				(length 7.62)
				(name "HSWAP_EN")
				(number "98")
			)
			(pin input clock
				(at -41.91 40.64 0)
				(length 7.62)
				(name "CCLK")
				(number "52")
			)
			(pin input line
				(at -41.91 35.56 0)
				(length 7.62)
				(name "M0")
				(number "25")
			)
			(pin input line
				(at -41.91 33.02 0)
				(length 7.62)
				(name "M1")
				(number "24")
			)
			(pin input line
				(at -41.91 30.48 0)
				(length 7.62)
				(name "M2")
				(number "26")
			)
			(pin bidirectional line
				(at -41.91 25.4 0)
				(length 7.62)
				(name "IO-VRN")
				(number "1")
			)
			(pin bidirectional line
				(at -41.91 22.86 0)
				(length 7.62)
				(name "IO-VRP")
				(number "2")
			)
			(pin bidirectional line
				(at -41.91 20.32 0)
				(length 7.62)
				(name "IO")
				(number "4")
			)
			(pin bidirectional line
				(at -41.91 17.78 0)
				(length 7.62)
				(name "IO")
				(number "5")
			)
			(pin bidirectional line
				(at -41.91 15.24 0)
				(length 7.62)
				(name "IO")
				(number "8")
			)
			(pin bidirectional line
				(at -41.91 12.7 0)
				(length 7.62)
				(name "IO")
				(number "9")
			)
			(pin bidirectional line
				(at -41.91 10.16 0)
				(length 7.62)
				(name "IO")
				(number "11")
			)
			(pin bidirectional line
				(at -41.91 7.62 0)
				(length 7.62)
				(name "IO/VREF")
				(number "12")
			)
			(pin input line
				(at -41.91 2.54 0)
				(length 7.62)
				(name "IO-VREF")
				(number "13")
			)
			(pin bidirectional line
				(at -41.91 0 0)
				(length 7.62)
				(name "IO")
				(number "14")
			)
			(pin bidirectional line
				(at -41.91 -2.54 0)
				(length 7.62)
				(name "IO")
				(number "15")
			)
			(pin bidirectional line
				(at -41.91 -5.08 0)
				(length 7.62)
				(name "IO/VREF")
				(number "16")
			)
			(pin bidirectional line
				(at -41.91 -7.62 0)
				(length 7.62)
				(name "IO")
				(number "17")
			)
			(pin bidirectional line
				(at -41.91 -10.16 0)
				(length 7.62)
				(name "IO")
				(number "21")
			)
			(pin bidirectional line
				(at -41.91 -12.7 0)
				(length 7.62)
				(name "IO-VRN")
				(number "22")
			)
			(pin bidirectional line
				(at -41.91 -15.24 0)
				(length 7.62)
				(name "IO-VRP")
				(number "23")
			)
			(pin bidirectional line
				(at -41.91 -20.32 0)
				(length 7.62)
				(name "IO/CS")
				(number "27")
			)
			(pin bidirectional line
				(at -41.91 -22.86 0)
				(length 7.62)
				(name "IO/RDWR")
				(number "28")
			)
			(pin bidirectional line
				(at -41.91 -25.4 0)
				(length 7.62)
				(name "IO/D7")
				(number "30")
			)
			(pin bidirectional line
				(at -41.91 -27.94 0)
				(length 7.62)
				(name "IO/D6")
				(number "32")
			)
			(pin bidirectional line
				(at -41.91 -30.48 0)
				(length 7.62)
				(name "IO/D5")
				(number "34")
			)
			(pin bidirectional line
				(at -41.91 -33.02 0)
				(length 7.62)
				(name "IO/D4")
				(number "35")
			)
			(pin bidirectional line
				(at -41.91 -35.56 0)
				(length 7.62)
				(name "IO/GCK2")
				(number "36")
			)
			(pin bidirectional line
				(at -41.91 -38.1 0)
				(length 7.62)
				(name "IO/GCK3")
				(number "37")
			)
			(pin bidirectional line
				(at -41.91 -43.18 0)
				(length 7.62)
				(name "IO/GCK0")
				(number "38")
			)
			(pin bidirectional line
				(at -41.91 -45.72 0)
				(length 7.62)
				(name "IO/GCK1")
				(number "39")
			)
			(pin bidirectional line
				(at -41.91 -48.26 0)
				(length 7.62)
				(name "IO/DOUT/BUSY")
				(number "40")
			)
			(pin bidirectional line
				(at -41.91 -50.8 0)
				(length 7.62)
				(name "IO/INIT")
				(number "42")
			)
			(pin bidirectional line
				(at -41.91 -53.34 0)
				(length 7.62)
				(name "IO/D3")
				(number "43")
			)
			(pin bidirectional line
				(at -41.91 -55.88 0)
				(length 7.62)
				(name "IO/D2")
				(number "44")
			)
			(pin bidirectional line
				(at -41.91 -58.42 0)
				(length 7.62)
				(name "IO/D1")
				(number "47")
			)
			(pin bidirectional line
				(at -41.91 -60.96 0)
				(length 7.62)
				(name "IO/D0/DIN")
				(number "48")
			)
			(pin power_in line
				(at -22.86 71.12 270)
				(length 7.62)
				(name "VCCAUX(2.5V)")
				(number "7")
			)
			(pin power_in line
				(at -20.32 71.12 270)
				(length 7.62)
				(name "VCCAUX(2.5V)")
				(number "33")
			)
			(pin power_in line
				(at -17.78 71.12 270)
				(length 7.62)
				(name "VCCAUX(2.5V)")
				(number "58")
			)
			(pin power_in line
				(at -15.24 71.12 270)
				(length 7.62)
				(name "VCCAUX(2.5V)")
				(number "84")
			)
			(pin power_in line
				(at -10.16 71.12 270)
				(length 7.62)
				(name "VCCO_7")
				(number "6")
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 7.62)
				(name "VCCO_6")
				(number "19")
			)
			(pin power_in line
				(at -7.62 -71.12 90)
				(length 7.62)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at -7.62 -71.12 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at -7.62 -71.12 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at -7.62 -71.12 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at -7.62 -71.12 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin passive line
				(at -7.62 -71.12 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "66")
			)
			(pin passive line
				(at -7.62 -71.12 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "73")
			)
			(pin passive line
				(at -7.62 -71.12 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "82")
			)
			(pin passive line
				(at -7.62 -71.12 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "95")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 7.62)
				(name "VCCO_5")
				(number "31")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 7.62)
				(name "VCCO_4")
				(number "46")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 7.62)
				(name "VCCO_3")
				(number "57")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 7.62)
				(name "VCCO_2")
				(number "70")
			)
			(pin passive line
				(at 5.08 71.12 270)
				(length 7.62)
				(name "VCCO_1")
				(number "83")
			)
			(pin passive line
				(at 7.62 71.12 270)
				(length 7.62)
				(name "VCCO_0")
				(number "94")
			)
			(pin power_in line
				(at 12.7 71.12 270)
				(length 7.62)
				(name "VCCINT(1.2V)")
				(number "18")
			)
			(pin power_in line
				(at 15.24 71.12 270)
				(length 7.62)
				(name "VCCINT(1.2V)")
				(number "45")
			)
			(pin power_in line
				(at 17.78 71.12 270)
				(length 7.62)
				(name "VCCINT(1.2V)")
				(number "69")
			)
			(pin power_in line
				(at 20.32 71.12 270)
				(length 7.62)
				(name "VCCINT(1.2V)")
				(number "93")
			)
			(pin bidirectional line
				(at 39.37 25.4 180)
				(length 7.62)
				(name "IO/GCK6")
				(number "89")
			)
			(pin bidirectional line
				(at 39.37 22.86 180)
				(length 7.62)
				(name "IO/GCK7")
				(number "90")
			)
			(pin bidirectional line
				(at 39.37 20.32 180)
				(length 7.62)
				(name "IO/VREF")
				(number "91")
			)
			(pin bidirectional line
				(at 39.37 17.78 180)
				(length 7.62)
				(name "IO")
				(number "92")
			)
			(pin bidirectional line
				(at 39.37 15.24 180)
				(length 7.62)
				(name "IO-VRN")
				(number "96")
			)
			(pin bidirectional line
				(at 39.37 12.7 180)
				(length 7.62)
				(name "IO-VRP")
				(number "97")
			)
			(pin bidirectional line
				(at 39.37 2.54 180)
				(length 7.62)
				(name "IO-VRN")
				(number "79")
			)
			(pin bidirectional line
				(at 39.37 0 180)
				(length 7.62)
				(name "IO-VRP")
				(number "80")
			)
			(pin bidirectional line
				(at 39.37 -2.54 180)
				(length 7.62)
				(name "IO")
				(number "81")
			)
			(pin bidirectional line
				(at 39.37 -5.08 180)
				(length 7.62)
				(name "IO")
				(number "85")
			)
			(pin bidirectional line
				(at 39.37 -7.62 180)
				(length 7.62)
				(name "IO/VREF")
				(number "86")
			)
			(pin bidirectional line
				(at 39.37 -10.16 180)
				(length 7.62)
				(name "IO/GCLK4")
				(number "87")
			)
			(pin bidirectional line
				(at 39.37 -12.7 180)
				(length 7.62)
				(name "IO/GCLK5")
				(number "88")
			)
			(pin bidirectional line
				(at 39.37 -20.32 180)
				(length 7.62)
				(name "IO/VREF")
				(number "64")
			)
			(pin bidirectional line
				(at 39.37 -22.86 180)
				(length 7.62)
				(name "IO")
				(number "65")
			)
			(pin bidirectional line
				(at 39.37 -25.4 180)
				(length 7.62)
				(name "IO")
				(number "67")
			)
			(pin bidirectional line
				(at 39.37 -27.94 180)
				(length 7.62)
				(name "IO")
				(number "68")
			)
			(pin bidirectional line
				(at 39.37 -30.48 180)
				(length 7.62)
				(name "IO")
				(number "71")
			)
			(pin bidirectional line
				(at 39.37 -33.02 180)
				(length 7.62)
				(name "IO")
				(number "72")
			)
			(pin bidirectional line
				(at 39.37 -35.56 180)
				(length 7.62)
				(name "IO-VRN")
				(number "74")
			)
			(pin bidirectional line
				(at 39.37 -38.1 180)
				(length 7.62)
				(name "IO-VRP")
				(number "75")
			)
			(pin bidirectional line
				(at 39.37 -43.18 180)
				(length 7.62)
				(name "IO-VRN")
				(number "53")
			)
			(pin bidirectional line
				(at 39.37 -45.72 180)
				(length 7.62)
				(name "IO-VRP")
				(number "54")
			)
			(pin bidirectional line
				(at 39.37 -48.26 180)
				(length 7.62)
				(name "IO")
				(number "55")
			)
			(pin bidirectional line
				(at 39.37 -50.8 180)
				(length 7.62)
				(name "IO")
				(number "59")
			)
			(pin bidirectional line
				(at 39.37 -53.34 180)
				(length 7.62)
				(name "IO")
				(number "60")
			)
			(pin bidirectional line
				(at 39.37 -55.88 180)
				(length 7.62)
				(name "IO")
				(number "61")
			)
			(pin bidirectional line
				(at 39.37 -58.42 180)
				(length 7.62)
				(name "IO")
				(number "62")
			)
			(pin bidirectional line
				(at 39.37 -60.96 180)
				(length 7.62)
				(name "IO/VREF")
				(number "63")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC3S50AN-TQG144"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "XC3S50AN-TQG144"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP144"
			(at 0 0 0)
		)
		(symbol "XC3S50AN-TQG144_0_0"
			(text "0"
				(at -12.7 25.4 0)
			)
			(text "1"
				(at -12.7 -45.72 0)
			)
			(text "3"
				(at 11.43 36.83 0)
			)
			(text "2"
				(at 11.43 -34.29 0)
			)
		)
		(symbol "XC3S50AN-TQG144_0_1")
		(symbol "XC3S50AN-TQG144_1_1"
			(pin input line
				(at -54.61 78.74 0)
				(length 7.62)
				(name "TMS")
				(number "1")
			)
			(pin output line
				(at -54.61 76.2 0)
				(length 7.62)
				(name "TDO")
				(number "107")
			)
			(pin input line
				(at -54.61 73.66 0)
				(length 7.62)
				(name "TDI")
				(number "2")
			)
			(pin input line
				(at -54.61 71.12 0)
				(length 7.62)
				(name "TCK")
				(number "109")
			)
			(pin bidirectional line
				(at -54.61 66.04 0)
				(length 7.62)
				(name "DONE")
				(number "73")
			)
			(pin bidirectional line
				(at -54.61 63.5 0)
				(length 7.62)
				(name "PROG_B")
				(number "144")
			)
			(pin input line
				(at -54.61 60.96 0)
				(length 7.62)
				(name "SUSPEND")
				(number "74")
			)
			(pin bidirectional line
				(at -54.61 55.88 0)
				(length 7.62)
				(name "IO_0")
				(number "142")
			)
			(pin bidirectional line
				(at -54.61 53.34 0)
				(length 7.62)
				(name "IO_L01N_0")
				(number "111")
			)
			(pin bidirectional line
				(at -54.61 50.8 0)
				(length 7.62)
				(name "IO_L01P_0")
				(number "110")
			)
			(pin bidirectional line
				(at -54.61 48.26 0)
				(length 7.62)
				(name "IO_L02N_0")
				(number "113")
			)
			(pin bidirectional line
				(at -54.61 45.72 0)
				(length 7.62)
				(name "IO_L02P_0/VREF_0")
				(number "112")
			)
			(pin bidirectional line
				(at -54.61 43.18 0)
				(length 7.62)
				(name "IO_L03N_0")
				(number "117")
			)
			(pin bidirectional line
				(at -54.61 40.64 0)
				(length 7.62)
				(name "IO_L03P_0")
				(number "115")
			)
			(pin bidirectional line
				(at -54.61 38.1 0)
				(length 7.62)
				(name "IO_L04N_0")
				(number "116")
			)
			(pin bidirectional line
				(at -54.61 35.56 0)
				(length 7.62)
				(name "IO_L04P_0")
				(number "114")
			)
			(pin bidirectional line
				(at -54.61 33.02 0)
				(length 7.62)
				(name "IO_L05N_0")
				(number "121")
			)
			(pin bidirectional line
				(at -54.61 30.48 0)
				(length 7.62)
				(name "IO_L05P_0")
				(number "120")
			)
			(pin bidirectional line
				(at -54.61 27.94 0)
				(length 7.62)
				(name "IO_L06N_0/GCLK5")
				(number "126")
			)
			(pin bidirectional line
				(at -54.61 25.4 0)
				(length 7.62)
				(name "IO_L06P_0/GCLK4")
				(number "124")
			)
			(pin bidirectional line
				(at -54.61 22.86 0)
				(length 7.62)
				(name "IO_L07N_0/GCLK7")
				(number "127")
			)
			(pin bidirectional line
				(at -54.61 20.32 0)
				(length 7.62)
				(name "IO_L07P_0/GCLK6")
				(number "125")
			)
			(pin bidirectional line
				(at -54.61 17.78 0)
				(length 7.62)
				(name "IO_L08N_0/GCLK9")
				(number "131")
			)
			(pin bidirectional line
				(at -54.61 15.24 0)
				(length 7.62)
				(name "IO_L08P_0/GCLK8")
				(number "129")
			)
			(pin bidirectional line
				(at -54.61 12.7 0)
				(length 7.62)
				(name "IO_L09N_0/GCLK11")
				(number "132")
			)
			(pin bidirectional line
				(at -54.61 10.16 0)
				(length 7.62)
				(name "IO_L09P_0/GCLK10")
				(number "130")
			)
			(pin bidirectional line
				(at -54.61 7.62 0)
				(length 7.62)
				(name "IO_L10N_0")
				(number "135")
			)
			(pin bidirectional line
				(at -54.61 5.08 0)
				(length 7.62)
				(name "IO_L10P_0")
				(number "134")
			)
			(pin bidirectional line
				(at -54.61 2.54 0)
				(length 7.62)
				(name "IO_L11N_0")
				(number "139")
			)
			(pin bidirectional line
				(at -54.61 0 0)
				(length 7.62)
				(name "IO_L11P_0")
				(number "138")
			)
			(pin bidirectional line
				(at -54.61 -2.54 0)
				(length 7.62)
				(name "IO_L12N_0/PUDC_B")
				(number "143")
			)
			(pin bidirectional line
				(at -54.61 -5.08 0)
				(length 7.62)
				(name "IO_L12P_0/VREF_0")
				(number "141")
			)
			(pin input line
				(at -54.61 -7.62 0)
				(length 7.62)
				(name "IP_0")
				(number "140")
			)
			(pin input line
				(at -54.61 -10.16 0)
				(length 7.62)
				(name "IP_0/VREF_0")
				(number "123")
			)
			(pin bidirectional line
				(at -54.61 -15.24 0)
				(length 7.62)
				(name "IO_1")
				(number "79")
			)
			(pin bidirectional line
				(at -54.61 -17.78 0)
				(length 7.62)
				(name "IO_L01N_1/LDC2")
				(number "78")
			)
			(pin bidirectional line
				(at -54.61 -20.32 0)
				(length 7.62)
				(name "IO_L01P_1/HDC")
				(number "76")
			)
			(pin bidirectional line
				(at -54.61 -22.86 0)
				(length 7.62)
				(name "IO_L02N_1/LDC0")
				(number "77")
			)
			(pin bidirectional line
				(at -54.61 -25.4 0)
				(length 7.62)
				(name "IO_L02P_1/LDC1")
				(number "75")
			)
			(pin bidirectional line
				(at -54.61 -27.94 0)
				(length 7.62)
				(name "IO_L03N_1")
				(number "84")
			)
			(pin bidirectional line
				(at -54.61 -30.48 0)
				(length 7.62)
				(name "IO_L03P_1")
				(number "82")
			)
			(pin bidirectional line
				(at -54.61 -33.02 0)
				(length 7.62)
				(name "IO_L04N_1/RHCLK1")
				(number "85")
			)
			(pin bidirectional line
				(at -54.61 -35.56 0)
				(length 7.62)
				(name "IO_L04P_1/RHCLK0")
				(number "83")
			)
			(pin bidirectional line
				(at -54.61 -38.1 0)
				(length 7.62)
				(name "IO_L05N_1/TRDY1/RHCLK3")
				(number "88")
			)
			(pin bidirectional line
				(at -54.61 -40.64 0)
				(length 7.62)
				(name "IO_L05P_1/RHCLK2")
				(number "87")
			)
			(pin bidirectional line
				(at -54.61 -43.18 0)
				(length 7.62)
				(name "IO_L06N_1/RHCLK5")
				(number "92")
			)
			(pin bidirectional line
				(at -54.61 -45.72 0)
				(length 7.62)
				(name "IO_L06P_1/RHCLK4")
				(number "90")
			)
			(pin bidirectional line
				(at -54.61 -48.26 0)
				(length 7.62)
				(name "IO_L07N_1/RHCLK7")
				(number "93")
			)
			(pin bidirectional line
				(at -54.61 -50.8 0)
				(length 7.62)
				(name "IO_L07P_1/IRDY1/RHCLK6")
				(number "91")
			)
			(pin bidirectional line
				(at -54.61 -53.34 0)
				(length 7.62)
				(name "IO_L08N_1")
				(number "98")
			)
			(pin bidirectional line
				(at -54.61 -55.88 0)
				(length 7.62)
				(name "IO_L08P_1")
				(number "96")
			)
			(pin bidirectional line
				(at -54.61 -58.42 0)
				(length 7.62)
				(name "IO_L09N_1")
				(number "101")
			)
			(pin bidirectional line
				(at -54.61 -60.96 0)
				(length 7.62)
				(name "IO_L09P_1")
				(number "99")
			)
			(pin bidirectional line
				(at -54.61 -63.5 0)
				(length 7.62)
				(name "IO_L10N_1")
				(number "104")
			)
			(pin bidirectional line
				(at -54.61 -66.04 0)
				(length 7.62)
				(name "IO_L10P_1")
				(number "102")
			)
			(pin bidirectional line
				(at -54.61 -68.58 0)
				(length 7.62)
				(name "IO_L11N_1")
				(number "105")
			)
			(pin bidirectional line
				(at -54.61 -71.12 0)
				(length 7.62)
				(name "IO_L11P_1")
				(number "103")
			)
			(pin input line
				(at -54.61 -73.66 0)
				(length 7.62)
				(name "IP_1/VREF_1")
				(number "80")
			)
			(pin input line
				(at -54.61 -76.2 0)
				(length 7.62)
				(name "IP_1/VREF_1")
				(number "97")
			)
			(pin power_in line
				(at -25.4 88.9 270)
				(length 7.62)
				(name "VCCO0")
				(number "119")
			)
			(pin power_in line
				(at -22.86 88.9 270)
				(length 7.62)
				(name "VCCO0")
				(number "136")
			)
			(pin power_in line
				(at -17.78 88.9 270)
				(length 7.62)
				(name "VCCO1")
				(number "86")
			)
			(pin power_in line
				(at -15.24 88.9 270)
				(length 7.62)
				(name "VCCO1")
				(number "95")
			)
			(pin power_in line
				(at -10.16 88.9 270)
				(length 7.62)
				(name "VCCO2")
				(number "40")
			)
			(pin power_in line
				(at -7.62 88.9 270)
				(length 7.62)
				(name "VCCO2")
				(number "61")
			)
			(pin passive line
				(at -2.54 88.9 270)
				(length 7.62)
				(name "VCCO3")
				(number "14")
			)
			(pin power_in line
				(at 0 88.9 270)
				(length 7.62)
				(name "VCCO3")
				(number "23")
			)
			(pin power_in line
				(at 5.08 88.9 270)
				(length 7.62)
				(name "VCCAUX")
				(number "36")
			)
			(pin power_in line
				(at 7.62 88.9 270)
				(length 7.62)
				(name "VCCAUX")
				(number "66")
			)
			(pin power_in line
				(at 10.16 88.9 270)
				(length 7.62)
				(name "VCCAUX")
				(number "108")
			)
			(pin power_in line
				(at 12.7 88.9 270)
				(length 7.62)
				(name "VCCAUX")
				(number "133")
			)
			(pin power_in line
				(at 13.97 -86.36 90)
				(length 7.62)
				(name "GND")
				(number "100")
			)
			(pin passive line
				(at 13.97 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "106")
			)
			(pin passive line
				(at 13.97 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "118")
			)
			(pin passive line
				(at 13.97 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "128")
			)
			(pin passive line
				(at 13.97 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "137")
			)
			(pin passive line
				(at 13.97 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 13.97 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin passive line
				(at 13.97 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 13.97 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "56")
			)
			(pin passive line
				(at 13.97 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin passive line
				(at 13.97 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "81")
			)
			(pin passive line
				(at 13.97 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "89")
			)
			(pin passive line
				(at 13.97 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 17.78 88.9 270)
				(length 7.62)
				(name "VCCINT")
				(number "22")
			)
			(pin power_in line
				(at 20.32 88.9 270)
				(length 7.62)
				(name "VCCINT")
				(number "52")
			)
			(pin power_in line
				(at 22.86 88.9 270)
				(length 7.62)
				(name "VCCINT")
				(number "94")
			)
			(pin power_in line
				(at 25.4 88.9 270)
				(length 7.62)
				(name "VCCINT")
				(number "122")
			)
			(pin input line
				(at 54.61 69.85 180)
				(length 7.62)
				(name "IN_L13P_3")
				(number "33")
			)
			(pin input line
				(at 54.61 67.31 180)
				(length 7.62)
				(name "IN_L13N_3/VREF_3")
				(number "35")
			)
			(pin bidirectional line
				(at 54.61 64.77 180)
				(length 7.62)
				(name "IO_L12P_3")
				(number "31")
			)
			(pin bidirectional line
				(at 54.61 62.23 180)
				(length 7.62)
				(name "IO_L12N_3")
				(number "32")
			)
			(pin bidirectional line
				(at 54.61 59.69 180)
				(length 7.62)
				(name "IO_L11P_3")
				(number "28")
			)
			(pin bidirectional line
				(at 54.61 57.15 180)
				(length 7.62)
				(name "IO_L11N_3")
				(number "30")
			)
			(pin bidirectional line
				(at 54.61 54.61 180)
				(length 7.62)
				(name "IO_L10P_3")
				(number "27")
			)
			(pin bidirectional line
				(at 54.61 52.07 180)
				(length 7.62)
				(name "IO_L10N_3")
				(number "29")
			)
			(pin bidirectional line
				(at 54.61 49.53 180)
				(length 7.62)
				(name "IO_L09P_3")
				(number "24")
			)
			(pin bidirectional line
				(at 54.61 46.99 180)
				(length 7.62)
				(name "IO_L09N_3")
				(number "25")
			)
			(pin bidirectional line
				(at 54.61 44.45 180)
				(length 7.62)
				(name "IO_L08P_3/TRDY2/LHCLK6")
				(number "19")
			)
			(pin bidirectional line
				(at 54.61 41.91 180)
				(length 7.62)
				(name "IO_L08N_3/LHCLK7")
				(number "21")
			)
			(pin bidirectional line
				(at 54.61 39.37 180)
				(length 7.62)
				(name "IO_L07P_3/LHCLK4")
				(number "18")
			)
			(pin bidirectional line
				(at 54.61 36.83 180)
				(length 7.62)
				(name "IO_L07N_3/LHCLK5")
				(number "20")
			)
			(pin bidirectional line
				(at 54.61 34.29 180)
				(length 7.62)
				(name "IO_L06P_3/LHCLK2")
				(number "15")
			)
			(pin bidirectional line
				(at 54.61 31.75 180)
				(length 7.62)
				(name "IO_L06N_3/IRDY2/LHCLK3")
				(number "16")
			)
			(pin bidirectional line
				(at 54.61 29.21 180)
				(length 7.62)
				(name "IO_L05P_3/LHCLK0")
				(number "12")
			)
			(pin bidirectional line
				(at 54.61 26.67 180)
				(length 7.62)
				(name "IO_L05N_3/LHCLK1")
				(number "13")
			)
			(pin bidirectional line
				(at 54.61 24.13 180)
				(length 7.62)
				(name "IO_L04P_3")
				(number "10")
			)
			(pin bidirectional line
				(at 54.61 21.59 180)
				(length 7.62)
				(name "IO_L04N_3/VREF_3")
				(number "11")
			)
			(pin bidirectional line
				(at 54.61 19.05 180)
				(length 7.62)
				(name "IO_L03P_3")
				(number "7")
			)
			(pin bidirectional line
				(at 54.61 16.51 180)
				(length 7.62)
				(name "IO_L03N_3")
				(number "8")
			)
			(pin bidirectional line
				(at 54.61 13.97 180)
				(length 7.62)
				(name "IO_L02P_3")
				(number "3")
			)
			(pin bidirectional line
				(at 54.61 11.43 180)
				(length 7.62)
				(name "IO_L02N_3")
				(number "5")
			)
			(pin bidirectional line
				(at 54.61 8.89 180)
				(length 7.62)
				(name "IO_L01P_3")
				(number "4")
			)
			(pin bidirectional line
				(at 54.61 6.35 180)
				(length 7.62)
				(name "IO_L01N_3")
				(number "6")
			)
			(pin input line
				(at 54.61 1.27 180)
				(length 7.62)
				(name "IP_2/VREF_2")
				(number "53")
			)
			(pin bidirectional line
				(at 54.61 -1.27 180)
				(length 7.62)
				(name "IO_L14P_2/D1")
				(number "70")
			)
			(pin bidirectional line
				(at 54.61 -3.81 180)
				(length 7.62)
				(name "IO_L14N_2/CCLK")
				(number "72")
			)
			(pin bidirectional line
				(at 54.61 -6.35 180)
				(length 7.62)
				(name "IO_L13P_2/D2")
				(number "69")
			)
			(pin bidirectional line
				(at 54.61 -8.89 180)
				(length 7.62)
				(name "IO_L13N_2/D0/DIN/MISO")
				(number "71")
			)
			(pin bidirectional line
				(at 54.61 -11.43 180)
				(length 7.62)
				(name "IO_L12P_2/INIT_B")
				(number "67")
			)
			(pin bidirectional line
				(at 54.61 -13.97 180)
				(length 7.62)
				(name "IO_L12N_2/D3")
				(number "68")
			)
			(pin bidirectional line
				(at 54.61 -16.51 180)
				(length 7.62)
				(name "IO_L11P_2/AWAKE")
				(number "63")
			)
			(pin bidirectional line
				(at 54.61 -19.05 180)
				(length 7.62)
				(name "IO_L11N_2/DOUT")
				(number "64")
			)
			(pin bidirectional line
				(at 54.61 -21.59 180)
				(length 7.62)
				(name "IO_L10P_2/GCLK2")
				(number "58")
			)
			(pin bidirectional line
				(at 54.61 -24.13 180)
				(length 7.62)
				(name "IO_L10N_2/GCLK3")
				(number "60")
			)
			(pin bidirectional line
				(at 54.61 -26.67 180)
				(length 7.62)
				(name "IO_L09P_2/GCLK0")
				(number "57")
			)
			(pin bidirectional line
				(at 54.61 -29.21 180)
				(length 7.62)
				(name "IO_L09N_2/GCLK1")
				(number "59")
			)
			(pin bidirectional line
				(at 54.61 -31.75 180)
				(length 7.62)
				(name "IO_L08P_2/GCLK14")
				(number "54")
			)
			(pin bidirectional line
				(at 54.61 -34.29 180)
				(length 7.62)
				(name "IO_L08N_2/GCLK15")
				(number "55")
			)
			(pin bidirectional line
				(at 54.61 -36.83 180)
				(length 7.62)
				(name "IO_L07P_2/D5")
				(number "50")
			)
			(pin bidirectional line
				(at 54.61 -39.37 180)
				(length 7.62)
				(name "IO_L07N_2/D4")
				(number "51")
			)
			(pin bidirectional line
				(at 54.61 -41.91 180)
				(length 7.62)
				(name "IO_L06P_2")
				(number "47")
			)
			(pin bidirectional line
				(at 54.61 -44.45 180)
				(length 7.62)
				(name "IO_L06N_2/D6")
				(number "49")
			)
			(pin bidirectional line
				(at 54.61 -46.99 180)
				(length 7.62)
				(name "IO_L05P_2")
				(number "46")
			)
			(pin bidirectional line
				(at 54.61 -49.53 180)
				(length 7.62)
				(name "IO_L05N_2/D7")
				(number "48")
			)
			(pin bidirectional line
				(at 54.61 -52.07 180)
				(length 7.62)
				(name "IO_L04P_2/VS2")
				(number "43")
			)
			(pin bidirectional line
				(at 54.61 -54.61 180)
				(length 7.62)
				(name "IO_L04N_2/VS0")
				(number "45")
			)
			(pin bidirectional line
				(at 54.61 -57.15 180)
				(length 7.62)
				(name "IO_L03P_2/RDWR_B")
				(number "42")
			)
			(pin bidirectional line
				(at 54.61 -59.69 180)
				(length 7.62)
				(name "IO_L03N_2/VS1")
				(number "44")
			)
			(pin bidirectional line
				(at 54.61 -62.23 180)
				(length 7.62)
				(name "IO_L02P_2/M2")
				(number "39")
			)
			(pin bidirectional line
				(at 54.61 -64.77 180)
				(length 7.62)
				(name "IO_L02N_2/CSO_B")
				(number "41")
			)
			(pin bidirectional line
				(at 54.61 -67.31 180)
				(length 7.62)
				(name "IO_L01P_2/M1")
				(number "37")
			)
			(pin bidirectional line
				(at 54.61 -69.85 180)
				(length 7.62)
				(name "IO_L01N_2/M0")
				(number "38")
			)
			(pin bidirectional line
				(at 54.61 -72.39 180)
				(length 7.62)
				(name "IO_2/MOSI/CSI_B")
				(number "62")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC4003-PC84"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XC4003-PC84"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC4003-PC84_0_1")
		(symbol "XC4003-PC84_1_1"
			(pin input line
				(at -27.94 49.53 0)
				(length 7.62)
				(name "M0")
				(number "32")
			)
			(pin input line
				(at -27.94 46.99 0)
				(length 7.62)
				(name "M1")
				(number "30")
			)
			(pin input line
				(at -27.94 44.45 0)
				(length 7.62)
				(name "M2")
				(number "34")
			)
			(pin input line
				(at -27.94 39.37 0)
				(length 7.62)
				(name "~{PROG}")
				(number "55")
			)
			(pin bidirectional line
				(at -27.94 36.83 0)
				(length 7.62)
				(name "DONE")
				(number "53")
			)
			(pin input line
				(at -27.94 34.29 0)
				(length 7.62)
				(name "DIN/P71")
				(number "71")
			)
			(pin passive line
				(at -27.94 31.75 0)
				(length 7.62)
				(name "DOUT-SGI3")
				(number "72")
			)
			(pin passive clock
				(at -27.94 29.21 0)
				(length 7.62)
				(name "CCLK")
				(number "73")
			)
			(pin bidirectional line
				(at -27.94 26.67 0)
				(length 7.62)
				(name "INIT-P41")
				(number "41")
			)
			(pin passive line
				(at -27.94 24.13 0)
				(length 7.62)
				(name "HDC")
				(number "35")
			)
			(pin passive line
				(at -27.94 21.59 0)
				(length 7.62)
				(name "LDC")
				(number "37")
			)
			(pin passive line
				(at -27.94 19.05 0)
				(length 7.62)
				(name "P3")
				(number "3")
			)
			(pin passive line
				(at -27.94 16.51 0)
				(length 7.62)
				(name "P4")
				(number "4")
			)
			(pin passive line
				(at -27.94 13.97 0)
				(length 7.62)
				(name "P5")
				(number "5")
			)
			(pin passive line
				(at -27.94 11.43 0)
				(length 7.62)
				(name "P6")
				(number "6")
			)
			(pin passive line
				(at -27.94 8.89 0)
				(length 7.62)
				(name "P7")
				(number "7")
			)
			(pin passive line
				(at -27.94 6.35 0)
				(length 7.62)
				(name "P8")
				(number "8")
			)
			(pin passive line
				(at -27.94 3.81 0)
				(length 7.62)
				(name "P9")
				(number "9")
			)
			(pin passive line
				(at -27.94 1.27 0)
				(length 7.62)
				(name "P10-SGI4")
				(number "10")
			)
			(pin passive line
				(at -27.94 -3.81 0)
				(length 7.62)
				(name "P13-PGI1")
				(number "13")
			)
			(pin passive line
				(at -27.94 -6.35 0)
				(length 7.62)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -27.94 -8.89 0)
				(length 7.62)
				(name "TDI")
				(number "15")
			)
			(pin passive line
				(at -27.94 -11.43 0)
				(length 7.62)
				(name "TCK")
				(number "16")
			)
			(pin passive line
				(at -27.94 -13.97 0)
				(length 7.62)
				(name "TMS")
				(number "17")
			)
			(pin passive line
				(at -27.94 -16.51 0)
				(length 7.62)
				(name "P18")
				(number "18")
			)
			(pin passive line
				(at -27.94 -19.05 0)
				(length 7.62)
				(name "P19")
				(number "19")
			)
			(pin passive line
				(at -27.94 -21.59 0)
				(length 7.62)
				(name "P20")
				(number "20")
			)
			(pin passive line
				(at -27.94 -26.67 0)
				(length 7.62)
				(name "P23")
				(number "23")
			)
			(pin passive line
				(at -27.94 -29.21 0)
				(length 7.62)
				(name "P24")
				(number "24")
			)
			(pin passive line
				(at -27.94 -31.75 0)
				(length 7.62)
				(name "P25")
				(number "25")
			)
			(pin passive line
				(at -27.94 -34.29 0)
				(length 7.62)
				(name "P26")
				(number "26")
			)
			(pin passive line
				(at -27.94 -36.83 0)
				(length 7.62)
				(name "P27")
				(number "27")
			)
			(pin passive line
				(at -27.94 -39.37 0)
				(length 7.62)
				(name "P28")
				(number "28")
			)
			(pin passive line
				(at -27.94 -41.91 0)
				(length 7.62)
				(name "P29-SGI1")
				(number "29")
			)
			(pin bidirectional line
				(at -27.94 -46.99 0)
				(length 7.62)
				(name "P36")
				(number "36")
			)
			(pin passive line
				(at 0 58.42 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "11")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 6.35)
				(name "VCC")
				(number "2")
			)
			(pin passive line
				(at 0 58.42 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "33")
			)
			(pin passive line
				(at 0 58.42 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "42")
			)
			(pin passive line
				(at 0 58.42 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "54")
			)
			(pin passive line
				(at 0 58.42 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "74")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 6.35)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "52")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "64")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "76")
			)
			(pin passive line
				(at 27.94 49.53 180)
				(length 7.62)
				(name "P84")
				(number "84")
			)
			(pin passive line
				(at 27.94 46.99 180)
				(length 7.62)
				(name "P83")
				(number "83")
			)
			(pin passive line
				(at 27.94 44.45 180)
				(length 7.62)
				(name "P82")
				(number "82")
			)
			(pin passive line
				(at 27.94 41.91 180)
				(length 7.62)
				(name "P81")
				(number "81")
			)
			(pin passive line
				(at 27.94 39.37 180)
				(length 7.62)
				(name "P80")
				(number "80")
			)
			(pin passive line
				(at 27.94 36.83 180)
				(length 7.62)
				(name "P79")
				(number "79")
			)
			(pin passive line
				(at 27.94 34.29 180)
				(length 7.62)
				(name "PGI4-P78")
				(number "78")
			)
			(pin passive line
				(at 27.94 31.75 180)
				(length 7.62)
				(name "P77")
				(number "77")
			)
			(pin passive line
				(at 27.94 26.67 180)
				(length 7.62)
				(name "TD0")
				(number "75")
			)
			(pin passive line
				(at 27.94 21.59 180)
				(length 7.62)
				(name "RCLK-RDY-P70")
				(number "70")
			)
			(pin passive line
				(at 27.94 19.05 180)
				(length 7.62)
				(name "P69")
				(number "69")
			)
			(pin passive line
				(at 27.94 16.51 180)
				(length 7.62)
				(name "P68")
				(number "68")
			)
			(pin passive line
				(at 27.94 13.97 180)
				(length 7.62)
				(name "P67")
				(number "67")
			)
			(pin passive line
				(at 27.94 11.43 180)
				(length 7.62)
				(name "P66")
				(number "66")
			)
			(pin passive line
				(at 27.94 8.89 180)
				(length 7.62)
				(name "P65")
				(number "65")
			)
			(pin passive line
				(at 27.94 3.81 180)
				(length 7.62)
				(name "P62")
				(number "62")
			)
			(pin passive line
				(at 27.94 1.27 180)
				(length 7.62)
				(name "P61")
				(number "61")
			)
			(pin passive line
				(at 27.94 -1.27 180)
				(length 7.62)
				(name "P60")
				(number "60")
			)
			(pin passive line
				(at 27.94 -3.81 180)
				(length 7.62)
				(name "P59")
				(number "59")
			)
			(pin passive line
				(at 27.94 -6.35 180)
				(length 7.62)
				(name "P58")
				(number "58")
			)
			(pin passive line
				(at 27.94 -8.89 180)
				(length 7.62)
				(name "PGI3-P57")
				(number "57")
			)
			(pin passive line
				(at 27.94 -11.43 180)
				(length 7.62)
				(name "P56")
				(number "56")
			)
			(pin passive line
				(at 27.94 -19.05 180)
				(length 7.62)
				(name "SGI2-P51")
				(number "51")
			)
			(pin passive line
				(at 27.94 -21.59 180)
				(length 7.62)
				(name "P50")
				(number "50")
			)
			(pin passive line
				(at 27.94 -24.13 180)
				(length 7.62)
				(name "P49")
				(number "49")
			)
			(pin passive line
				(at 27.94 -26.67 180)
				(length 7.62)
				(name "P48")
				(number "48")
			)
			(pin passive line
				(at 27.94 -29.21 180)
				(length 7.62)
				(name "P47")
				(number "47")
			)
			(pin passive line
				(at 27.94 -31.75 180)
				(length 7.62)
				(name "P46")
				(number "46")
			)
			(pin passive line
				(at 27.94 -34.29 180)
				(length 7.62)
				(name "P45")
				(number "45")
			)
			(pin passive line
				(at 27.94 -36.83 180)
				(length 7.62)
				(name "P44")
				(number "44")
			)
			(pin passive line
				(at 27.94 -44.45 180)
				(length 7.62)
				(name "P40")
				(number "40")
			)
			(pin passive line
				(at 27.94 -46.99 180)
				(length 7.62)
				(name "P39")
				(number "39")
			)
			(pin passive line
				(at 27.94 -49.53 180)
				(length 7.62)
				(name "P38")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC4003-VQ100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XC4003-VQ100"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "xilinx/xc400x-pinout.pdf"
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC4003-VQ100_0_1")
		(symbol "XC4003-VQ100_1_1"
			(pin input line
				(at -24.13 57.15 0)
				(length 7.62)
				(name "M0/RT")
				(number "24")
			)
			(pin input line
				(at -24.13 54.61 0)
				(length 7.62)
				(name "M1/RD")
				(number "22")
			)
			(pin passive line
				(at -24.13 52.07 0)
				(length 7.62)
				(name "M2")
				(number "26")
			)
			(pin input line
				(at -24.13 46.99 0)
				(length 7.62)
				(name "~{PROG}")
				(number "52")
			)
			(pin open_collector line
				(at -24.13 44.45 0)
				(length 7.62)
				(name "DONE")
				(number "50")
			)
			(pin passive line
				(at -24.13 41.91 0)
				(length 7.62)
				(name "DIN")
				(number "72")
			)
			(pin passive line
				(at -24.13 39.37 0)
				(length 7.62)
				(name "DOUT/SGCK4")
				(number "73")
			)
			(pin input clock
				(at -24.13 36.83 0)
				(length 7.62)
				(name "CCLK")
				(number "74")
			)
			(pin passive line
				(at -24.13 34.29 0)
				(length 7.62)
				(name "P/HDC")
				(number "28")
			)
			(pin passive line
				(at -24.13 31.75 0)
				(length 7.62)
				(name "P/LDC")
				(number "30")
			)
			(pin passive line
				(at -24.13 29.21 0)
				(length 7.62)
				(name "PGCK1")
				(number "2")
			)
			(pin passive line
				(at -24.13 26.67 0)
				(length 7.62)
				(name "P/A17")
				(number "3")
			)
			(pin passive line
				(at -24.13 24.13 0)
				(length 7.62)
				(name "P/TDI")
				(number "4")
			)
			(pin passive line
				(at -24.13 21.59 0)
				(length 7.62)
				(name "P/TCK")
				(number "5")
			)
			(pin passive line
				(at -24.13 19.05 0)
				(length 7.62)
				(name "P/A3")
				(number "6")
			)
			(pin passive line
				(at -24.13 16.51 0)
				(length 7.62)
				(name "P7")
				(number "7")
			)
			(pin passive line
				(at -24.13 13.97 0)
				(length 7.62)
				(name "P8")
				(number "8")
			)
			(pin passive line
				(at -24.13 11.43 0)
				(length 7.62)
				(name "P/A15")
				(number "9")
			)
			(pin passive line
				(at -24.13 8.89 0)
				(length 7.62)
				(name "P/A4")
				(number "10")
			)
			(pin bidirectional line
				(at -24.13 3.81 0)
				(length 7.62)
				(name "P13")
				(number "13")
			)
			(pin passive line
				(at -24.13 1.27 0)
				(length 7.62)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -24.13 -1.27 0)
				(length 7.62)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -24.13 -3.81 0)
				(length 7.62)
				(name "P16")
				(number "16")
			)
			(pin passive line
				(at -24.13 -6.35 0)
				(length 7.62)
				(name "P17")
				(number "17")
			)
			(pin passive line
				(at -24.13 -8.89 0)
				(length 7.62)
				(name "P18")
				(number "18")
			)
			(pin passive line
				(at -24.13 -11.43 0)
				(length 7.62)
				(name "P19")
				(number "19")
			)
			(pin passive line
				(at -24.13 -13.97 0)
				(length 7.62)
				(name "P20")
				(number "20")
			)
			(pin passive line
				(at -24.13 -16.51 0)
				(length 7.62)
				(name "SGCK2")
				(number "21")
			)
			(pin passive line
				(at -24.13 -24.13 0)
				(length 7.62)
				(name "PGCK2")
				(number "27")
			)
			(pin passive line
				(at -24.13 -29.21 0)
				(length 7.62)
				(name "P29")
				(number "29")
			)
			(pin passive line
				(at -24.13 -34.29 0)
				(length 7.62)
				(name "P31")
				(number "31")
			)
			(pin passive line
				(at -24.13 -36.83 0)
				(length 7.62)
				(name "P32")
				(number "32")
			)
			(pin passive line
				(at -24.13 -39.37 0)
				(length 7.62)
				(name "P33")
				(number "33")
			)
			(pin passive line
				(at -24.13 -41.91 0)
				(length 7.62)
				(name "P34")
				(number "34")
			)
			(pin passive line
				(at -24.13 -44.45 0)
				(length 7.62)
				(name "P35")
				(number "35")
			)
			(pin passive line
				(at -24.13 -46.99 0)
				(length 7.62)
				(name "P36/INIT")
				(number "36")
			)
			(pin passive line
				(at -24.13 -52.07 0)
				(length 7.62)
				(name "P39")
				(number "39")
			)
			(pin passive line
				(at -24.13 -54.61 0)
				(length 7.62)
				(name "P40")
				(number "40")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "100")
			)
			(pin power_in line
				(at 0 66.04 270)
				(length 6.35)
				(name "VCC")
				(number "12")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "25")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "37")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "51")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "63")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "75")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 6.35)
				(hide yes)
				(name "VCC")
				(number "89")
			)
			(pin power_in line
				(at 0 -66.04 90)
				(length 6.35)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "49")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "64")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "77")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 6.35)
				(hide yes)
				(name "GND")
				(number "88")
			)
			(pin bidirectional line
				(at 24.13 57.15 180)
				(length 7.62)
				(name "SGCK1")
				(number "99")
			)
			(pin bidirectional line
				(at 24.13 54.61 180)
				(length 7.62)
				(name "P98")
				(number "98")
			)
			(pin passive line
				(at 24.13 52.07 180)
				(length 7.62)
				(name "P97")
				(number "97")
			)
			(pin passive line
				(at 24.13 49.53 180)
				(length 7.62)
				(name "P96")
				(number "96")
			)
			(pin passive line
				(at 24.13 46.99 180)
				(length 7.62)
				(name "P91")
				(number "95")
			)
			(pin passive line
				(at 24.13 44.45 180)
				(length 7.62)
				(name "P94")
				(number "94")
			)
			(pin passive line
				(at 24.13 41.91 180)
				(length 7.62)
				(name "P93")
				(number "93")
			)
			(pin passive line
				(at 24.13 39.37 180)
				(length 7.62)
				(name "P92")
				(number "92")
			)
			(pin passive line
				(at 24.13 36.83 180)
				(length 7.62)
				(name "P91")
				(number "91")
			)
			(pin bidirectional line
				(at 24.13 34.29 180)
				(length 7.62)
				(name "P90")
				(number "90")
			)
			(pin passive line
				(at 24.13 31.75 180)
				(length 7.62)
				(name "P87")
				(number "87")
			)
			(pin passive line
				(at 24.13 29.21 180)
				(length 7.62)
				(name "P86")
				(number "86")
			)
			(pin passive line
				(at 24.13 26.67 180)
				(length 7.62)
				(name "P85")
				(number "85")
			)
			(pin passive line
				(at 24.13 24.13 180)
				(length 7.62)
				(name "P84")
				(number "84")
			)
			(pin passive line
				(at 24.13 21.59 180)
				(length 7.62)
				(name "P83")
				(number "83")
			)
			(pin passive line
				(at 24.13 19.05 180)
				(length 7.62)
				(name "P82")
				(number "82")
			)
			(pin passive line
				(at 24.13 16.51 180)
				(length 7.62)
				(name "P81")
				(number "81")
			)
			(pin passive line
				(at 24.13 13.97 180)
				(length 7.62)
				(name "P80")
				(number "80")
			)
			(pin passive line
				(at 24.13 11.43 180)
				(length 7.62)
				(name "PGCK4")
				(number "79")
			)
			(pin passive line
				(at 24.13 8.89 180)
				(length 7.62)
				(name "P78")
				(number "78")
			)
			(pin output line
				(at 24.13 6.35 180)
				(length 7.62)
				(name "TDO")
				(number "76")
			)
			(pin passive line
				(at 24.13 3.81 180)
				(length 7.62)
				(name "P71/RDY")
				(number "71")
			)
			(pin passive line
				(at 24.13 1.27 180)
				(length 7.62)
				(name "P70")
				(number "70")
			)
			(pin passive line
				(at 24.13 -1.27 180)
				(length 7.62)
				(name "P69")
				(number "69")
			)
			(pin passive line
				(at 24.13 -3.81 180)
				(length 7.62)
				(name "P68")
				(number "68")
			)
			(pin passive line
				(at 24.13 -6.35 180)
				(length 7.62)
				(name "P67")
				(number "67")
			)
			(pin passive line
				(at 24.13 -8.89 180)
				(length 7.62)
				(name "P66")
				(number "66")
			)
			(pin passive line
				(at 24.13 -11.43 180)
				(length 7.62)
				(name "P65")
				(number "65")
			)
			(pin passive line
				(at 24.13 -13.97 180)
				(length 7.62)
				(name "P62")
				(number "62")
			)
			(pin passive line
				(at 24.13 -16.51 180)
				(length 7.62)
				(name "P61")
				(number "61")
			)
			(pin passive line
				(at 24.13 -19.05 180)
				(length 7.62)
				(name "P60")
				(number "60")
			)
			(pin passive line
				(at 24.13 -21.59 180)
				(length 7.62)
				(name "P59")
				(number "59")
			)
			(pin passive line
				(at 24.13 -24.13 180)
				(length 7.62)
				(name "P58")
				(number "58")
			)
			(pin passive line
				(at 24.13 -26.67 180)
				(length 7.62)
				(name "P57")
				(number "57")
			)
			(pin bidirectional line
				(at 24.13 -29.21 180)
				(length 7.62)
				(name "P56")
				(number "56")
			)
			(pin passive line
				(at 24.13 -31.75 180)
				(length 7.62)
				(name "P55")
				(number "55")
			)
			(pin bidirectional line
				(at 24.13 -34.29 180)
				(length 7.62)
				(name "PGCK3")
				(number "54")
			)
			(pin bidirectional line
				(at 24.13 -36.83 180)
				(length 7.62)
				(name "P53")
				(number "53")
			)
			(pin passive line
				(at 24.13 -39.37 180)
				(length 7.62)
				(name "SGCK3")
				(number "48")
			)
			(pin passive line
				(at 24.13 -41.91 180)
				(length 7.62)
				(name "P47")
				(number "47")
			)
			(pin passive line
				(at 24.13 -44.45 180)
				(length 7.62)
				(name "P46")
				(number "46")
			)
			(pin passive line
				(at 24.13 -46.99 180)
				(length 7.62)
				(name "P45")
				(number "45")
			)
			(pin passive line
				(at 24.13 -49.53 180)
				(length 7.62)
				(name "P44")
				(number "44")
			)
			(pin passive line
				(at 24.13 -52.07 180)
				(length 7.62)
				(name "P43")
				(number "43")
			)
			(pin passive line
				(at 24.13 -54.61 180)
				(length 7.62)
				(name "P42")
				(number "42")
			)
			(pin passive line
				(at 24.13 -57.15 180)
				(length 7.62)
				(name "P41")
				(number "41")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC4004-PQ160"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XC4004-PQ160"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC4004-PQ160_0_1")
		(symbol "XC4004-PQ160_1_1"
			(pin input line
				(at -29.21 66.04 0)
				(length 7.62)
				(name "M0")
				(number "40")
			)
			(pin input line
				(at -29.21 63.5 0)
				(length 7.62)
				(name "M1")
				(number "38")
			)
			(pin input line
				(at -29.21 60.96 0)
				(length 7.62)
				(name "M2")
				(number "42")
			)
			(pin input line
				(at -29.21 58.42 0)
				(length 7.62)
				(name "~{PROG}")
				(number "82")
			)
			(pin input line
				(at -29.21 55.88 0)
				(length 7.62)
				(name "DONE")
				(number "80")
			)
			(pin bidirectional line
				(at -29.21 53.34 0)
				(length 7.62)
				(name "DIN/D0")
				(number "117")
			)
			(pin bidirectional line
				(at -29.21 50.8 0)
				(length 7.62)
				(name "DOUT/SGCK4")
				(number "118")
			)
			(pin input clock
				(at -29.21 48.26 0)
				(length 7.62)
				(name "CCLK")
				(number "119")
			)
			(pin bidirectional line
				(at -29.21 43.18 0)
				(length 7.62)
				(name "P44/HDC")
				(number "44")
			)
			(pin bidirectional line
				(at -29.21 40.64 0)
				(length 7.62)
				(name "P48/LDC")
				(number "48")
			)
			(pin bidirectional line
				(at -29.21 35.56 0)
				(length 7.62)
				(name "PGCK1")
				(number "2")
			)
			(pin bidirectional line
				(at -29.21 33.02 0)
				(length 7.62)
				(name "P3")
				(number "3")
			)
			(pin bidirectional line
				(at -29.21 30.48 0)
				(length 7.62)
				(name "P4")
				(number "4")
			)
			(pin bidirectional line
				(at -29.21 27.94 0)
				(length 7.62)
				(name "P5")
				(number "5")
			)
			(pin bidirectional line
				(at -29.21 25.4 0)
				(length 7.62)
				(name "P6/TDI")
				(number "6")
			)
			(pin bidirectional line
				(at -29.21 22.86 0)
				(length 7.62)
				(name "P7/TCK")
				(number "7")
			)
			(pin bidirectional line
				(at -29.21 20.32 0)
				(length 7.62)
				(name "P13/TMS")
				(number "13")
			)
			(pin bidirectional line
				(at -29.21 17.78 0)
				(length 7.62)
				(name "P14")
				(number "14")
			)
			(pin bidirectional line
				(at -29.21 15.24 0)
				(length 7.62)
				(name "P15")
				(number "15")
			)
			(pin bidirectional line
				(at -29.21 12.7 0)
				(length 7.62)
				(name "P16")
				(number "16")
			)
			(pin bidirectional line
				(at -29.21 10.16 0)
				(length 7.62)
				(name "P17")
				(number "17")
			)
			(pin bidirectional line
				(at -29.21 7.62 0)
				(length 7.62)
				(name "P18")
				(number "18")
			)
			(pin bidirectional line
				(at -29.21 5.08 0)
				(length 7.62)
				(name "P21")
				(number "21")
			)
			(pin bidirectional line
				(at -29.21 2.54 0)
				(length 7.62)
				(name "P22")
				(number "22")
			)
			(pin bidirectional line
				(at -29.21 0 0)
				(length 7.62)
				(name "P23")
				(number "23")
			)
			(pin bidirectional line
				(at -29.21 -2.54 0)
				(length 7.62)
				(name "P24")
				(number "24")
			)
			(pin bidirectional line
				(at -29.21 -5.08 0)
				(length 7.62)
				(name "P25")
				(number "25")
			)
			(pin bidirectional line
				(at -29.21 -7.62 0)
				(length 7.62)
				(name "P26")
				(number "26")
			)
			(pin bidirectional line
				(at -29.21 -10.16 0)
				(length 7.62)
				(name "P32")
				(number "32")
			)
			(pin bidirectional line
				(at -29.21 -12.7 0)
				(length 7.62)
				(name "P33")
				(number "33")
			)
			(pin bidirectional line
				(at -29.21 -15.24 0)
				(length 7.62)
				(name "P34")
				(number "34")
			)
			(pin bidirectional line
				(at -29.21 -17.78 0)
				(length 7.62)
				(name "P35")
				(number "35")
			)
			(pin bidirectional line
				(at -29.21 -20.32 0)
				(length 7.62)
				(name "P36")
				(number "36")
			)
			(pin bidirectional line
				(at -29.21 -22.86 0)
				(length 7.62)
				(name "SGCK2")
				(number "37")
			)
			(pin bidirectional line
				(at -29.21 -25.4 0)
				(length 7.62)
				(name "PGCK2")
				(number "43")
			)
			(pin bidirectional line
				(at -29.21 -27.94 0)
				(length 7.62)
				(name "P45")
				(number "45")
			)
			(pin bidirectional line
				(at -29.21 -30.48 0)
				(length 7.62)
				(name "P46")
				(number "46")
			)
			(pin bidirectional line
				(at -29.21 -33.02 0)
				(length 7.62)
				(name "P47")
				(number "47")
			)
			(pin bidirectional line
				(at -29.21 -35.56 0)
				(length 7.62)
				(name "P54")
				(number "54")
			)
			(pin bidirectional line
				(at -29.21 -38.1 0)
				(length 7.62)
				(name "P55")
				(number "55")
			)
			(pin bidirectional line
				(at -29.21 -40.64 0)
				(length 7.62)
				(name "P56")
				(number "56")
			)
			(pin bidirectional line
				(at -29.21 -43.18 0)
				(length 7.62)
				(name "P57")
				(number "57")
			)
			(pin bidirectional line
				(at -29.21 -45.72 0)
				(length 7.62)
				(name "P58")
				(number "58")
			)
			(pin bidirectional line
				(at -29.21 -48.26 0)
				(length 7.62)
				(name "P59/INIT")
				(number "59")
			)
			(pin bidirectional line
				(at -29.21 -50.8 0)
				(length 7.62)
				(name "P62")
				(number "62")
			)
			(pin bidirectional line
				(at -29.21 -53.34 0)
				(length 7.62)
				(name "P63")
				(number "63")
			)
			(pin bidirectional line
				(at -29.21 -55.88 0)
				(length 7.62)
				(name "P64")
				(number "64")
			)
			(pin bidirectional line
				(at -29.21 -58.42 0)
				(length 7.62)
				(name "P65")
				(number "65")
			)
			(pin bidirectional line
				(at -29.21 -60.96 0)
				(length 7.62)
				(name "P66")
				(number "66")
			)
			(pin bidirectional line
				(at -29.21 -63.5 0)
				(length 7.62)
				(name "P67")
				(number "67")
			)
			(pin passive line
				(at 0 76.2 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "100")
			)
			(pin passive line
				(at 0 76.2 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "120")
			)
			(pin passive line
				(at 0 76.2 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "142")
			)
			(pin passive line
				(at 0 76.2 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "160")
			)
			(pin power_in line
				(at 0 76.2 270)
				(length 7.62)
				(name "VCC")
				(number "20")
			)
			(pin passive line
				(at 0 76.2 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "41")
			)
			(pin passive line
				(at 0 76.2 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "60")
			)
			(pin passive line
				(at 0 76.2 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "81")
			)
			(pin power_in line
				(at 0 -76.2 90)
				(length 7.62)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -76.2 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -76.2 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "101")
			)
			(pin passive line
				(at 0 -76.2 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "110")
			)
			(pin passive line
				(at 0 -76.2 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "122")
			)
			(pin passive line
				(at 0 -76.2 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "131")
			)
			(pin passive line
				(at 0 -76.2 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "141")
			)
			(pin passive line
				(at 0 -76.2 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "151")
			)
			(pin passive line
				(at 0 -76.2 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -76.2 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -76.2 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin passive line
				(at 0 -76.2 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "51")
			)
			(pin passive line
				(at 0 -76.2 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "61")
			)
			(pin passive line
				(at 0 -76.2 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "70")
			)
			(pin passive line
				(at 0 -76.2 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "79")
			)
			(pin passive line
				(at 0 -76.2 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "91")
			)
			(pin bidirectional line
				(at 29.21 66.04 180)
				(length 7.62)
				(name "SGCK1")
				(number "159")
			)
			(pin bidirectional line
				(at 29.21 63.5 180)
				(length 7.62)
				(name "P158")
				(number "158")
			)
			(pin bidirectional line
				(at 29.21 60.96 180)
				(length 7.62)
				(name "P157")
				(number "157")
			)
			(pin bidirectional line
				(at 29.21 58.42 180)
				(length 7.62)
				(name "P156")
				(number "156")
			)
			(pin bidirectional line
				(at 29.21 55.88 180)
				(length 7.62)
				(name "P155")
				(number "155")
			)
			(pin bidirectional line
				(at 29.21 53.34 180)
				(length 7.62)
				(name "P154")
				(number "154")
			)
			(pin bidirectional line
				(at 29.21 50.8 180)
				(length 7.62)
				(name "P148")
				(number "148")
			)
			(pin bidirectional line
				(at 29.21 48.26 180)
				(length 7.62)
				(name "P147")
				(number "147")
			)
			(pin bidirectional line
				(at 29.21 45.72 180)
				(length 7.62)
				(name "P146")
				(number "146")
			)
			(pin bidirectional line
				(at 29.21 43.18 180)
				(length 7.62)
				(name "P145")
				(number "145")
			)
			(pin bidirectional line
				(at 29.21 40.64 180)
				(length 7.62)
				(name "P144")
				(number "144")
			)
			(pin bidirectional line
				(at 29.21 38.1 180)
				(length 7.62)
				(name "P143")
				(number "143")
			)
			(pin bidirectional line
				(at 29.21 35.56 180)
				(length 7.62)
				(name "P140")
				(number "140")
			)
			(pin bidirectional line
				(at 29.21 33.02 180)
				(length 7.62)
				(name "P139")
				(number "139")
			)
			(pin bidirectional line
				(at 29.21 30.48 180)
				(length 7.62)
				(name "P138")
				(number "138")
			)
			(pin bidirectional line
				(at 29.21 27.94 180)
				(length 7.62)
				(name "P137")
				(number "137")
			)
			(pin bidirectional line
				(at 29.21 25.4 180)
				(length 7.62)
				(name "P135")
				(number "135")
			)
			(pin bidirectional line
				(at 29.21 22.86 180)
				(length 7.62)
				(name "P134")
				(number "134")
			)
			(pin bidirectional line
				(at 29.21 20.32 180)
				(length 7.62)
				(name "P128")
				(number "128")
			)
			(pin bidirectional line
				(at 29.21 17.78 180)
				(length 7.62)
				(name "P127")
				(number "127")
			)
			(pin bidirectional line
				(at 29.21 15.24 180)
				(length 7.62)
				(name "P126")
				(number "126")
			)
			(pin bidirectional line
				(at 29.21 12.7 180)
				(length 7.62)
				(name "P125")
				(number "125")
			)
			(pin bidirectional line
				(at 29.21 10.16 180)
				(length 7.62)
				(name "PGCK4")
				(number "124")
			)
			(pin bidirectional line
				(at 29.21 7.62 180)
				(length 7.62)
				(name "P123")
				(number "123")
			)
			(pin output line
				(at 29.21 5.08 180)
				(length 7.62)
				(name "TDO")
				(number "121")
			)
			(pin bidirectional line
				(at 29.21 2.54 180)
				(length 7.62)
				(name "P116")
				(number "116")
			)
			(pin bidirectional line
				(at 29.21 0 180)
				(length 7.62)
				(name "P115")
				(number "115")
			)
			(pin bidirectional line
				(at 29.21 -2.54 180)
				(length 7.62)
				(name "P114/BUSY")
				(number "114")
			)
			(pin bidirectional line
				(at 29.21 -5.08 180)
				(length 7.62)
				(name "P113")
				(number "113")
			)
			(pin bidirectional line
				(at 29.21 -7.62 180)
				(length 7.62)
				(name "P107")
				(number "107")
			)
			(pin bidirectional line
				(at 29.21 -10.16 180)
				(length 7.62)
				(name "P106")
				(number "106")
			)
			(pin bidirectional line
				(at 29.21 -12.7 180)
				(length 7.62)
				(name "P105")
				(number "105")
			)
			(pin bidirectional line
				(at 29.21 -15.24 180)
				(length 7.62)
				(name "P104")
				(number "104")
			)
			(pin bidirectional line
				(at 29.21 -17.78 180)
				(length 7.62)
				(name "P103")
				(number "103")
			)
			(pin bidirectional line
				(at 29.21 -20.32 180)
				(length 7.62)
				(name "P102")
				(number "102")
			)
			(pin bidirectional line
				(at 29.21 -22.86 180)
				(length 7.62)
				(name "P99")
				(number "99")
			)
			(pin bidirectional line
				(at 29.21 -25.4 180)
				(length 7.62)
				(name "P98")
				(number "98")
			)
			(pin bidirectional line
				(at 29.21 -27.94 180)
				(length 7.62)
				(name "P97")
				(number "97")
			)
			(pin bidirectional line
				(at 29.21 -30.48 180)
				(length 7.62)
				(name "P96")
				(number "96")
			)
			(pin bidirectional line
				(at 29.21 -33.02 180)
				(length 7.62)
				(name "P95")
				(number "95")
			)
			(pin bidirectional line
				(at 29.21 -35.56 180)
				(length 7.62)
				(name "P94")
				(number "94")
			)
			(pin bidirectional line
				(at 29.21 -38.1 180)
				(length 7.62)
				(name "P88")
				(number "88")
			)
			(pin bidirectional line
				(at 29.21 -40.64 180)
				(length 7.62)
				(name "P87")
				(number "87")
			)
			(pin bidirectional line
				(at 29.21 -43.18 180)
				(length 7.62)
				(name "P86")
				(number "86")
			)
			(pin bidirectional line
				(at 29.21 -45.72 180)
				(length 7.62)
				(name "P85")
				(number "85")
			)
			(pin bidirectional line
				(at 29.21 -48.26 180)
				(length 7.62)
				(name "PGCK3")
				(number "84")
			)
			(pin bidirectional line
				(at 29.21 -50.8 180)
				(length 7.62)
				(name "P83")
				(number "83")
			)
			(pin bidirectional line
				(at 29.21 -53.34 180)
				(length 7.62)
				(name "SGCK3")
				(number "78")
			)
			(pin bidirectional line
				(at 29.21 -55.88 180)
				(length 7.62)
				(name "P77")
				(number "77")
			)
			(pin bidirectional line
				(at 29.21 -58.42 180)
				(length 7.62)
				(name "P76")
				(number "76")
			)
			(pin bidirectional line
				(at 29.21 -60.96 180)
				(length 7.62)
				(name "P75")
				(number "75")
			)
			(pin bidirectional line
				(at 29.21 -63.5 180)
				(length 7.62)
				(name "P74")
				(number "74")
			)
			(pin bidirectional line
				(at 29.21 -66.04 180)
				(length 7.62)
				(name "P73")
				(number "73")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC4005-PG156"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XC4005-PG156"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC4005-PG156_0_1")
		(symbol "XC4005-PG156_1_1"
			(pin input line
				(at -27.94 76.2 0)
				(length 7.62)
				(name "M0")
				(number "A16")
			)
			(pin input line
				(at -27.94 73.66 0)
				(length 7.62)
				(name "M1")
				(number "A15")
			)
			(pin input line
				(at -27.94 71.12 0)
				(length 7.62)
				(name "M2")
				(number "B15")
			)
			(pin input line
				(at -27.94 66.04 0)
				(length 7.62)
				(name "~{PROG}")
				(number "R14")
			)
			(pin bidirectional line
				(at -27.94 63.5 0)
				(length 7.62)
				(name "DONE")
				(number "R15")
			)
			(pin input line
				(at -27.94 60.96 0)
				(length 7.62)
				(name "DIN")
				(number "P4")
			)
			(pin passive line
				(at -27.94 58.42 0)
				(length 7.62)
				(name "DOUT-SGCK4")
				(number "T2")
			)
			(pin passive clock
				(at -27.94 55.88 0)
				(length 7.62)
				(name "CCLK")
				(number "R2")
			)
			(pin passive line
				(at -27.94 50.8 0)
				(length 7.62)
				(name "HDC")
				(number "D14")
			)
			(pin passive line
				(at -27.94 48.26 0)
				(length 7.62)
				(name "LDC")
				(number "C16")
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 7.62)
				(name "P41-INIT")
				(number "H15")
			)
			(pin passive line
				(at -27.94 40.64 0)
				(length 7.62)
				(name "P3")
				(number "H1")
			)
			(pin passive line
				(at -27.94 38.1 0)
				(length 7.62)
				(name "P4")
				(number "G1")
			)
			(pin passive line
				(at -27.94 35.56 0)
				(length 7.62)
				(name "P")
				(number "G2")
			)
			(pin passive line
				(at -27.94 33.02 0)
				(length 7.62)
				(name "P")
				(number "G3")
			)
			(pin passive line
				(at -27.94 30.48 0)
				(length 7.62)
				(name "P5")
				(number "F1")
			)
			(pin passive line
				(at -27.94 27.94 0)
				(length 7.62)
				(name "P6")
				(number "F2")
			)
			(pin passive line
				(at -27.94 25.4 0)
				(length 7.62)
				(name "P")
				(number "E1")
			)
			(pin passive line
				(at -27.94 22.86 0)
				(length 7.62)
				(name "P")
				(number "E2")
			)
			(pin passive line
				(at -27.94 20.32 0)
				(length 7.62)
				(name "P7")
				(number "E3")
			)
			(pin passive line
				(at -27.94 17.78 0)
				(length 7.62)
				(name "P8")
				(number "C1")
			)
			(pin passive line
				(at -27.94 15.24 0)
				(length 7.62)
				(name "P9")
				(number "B1")
			)
			(pin passive line
				(at -27.94 12.7 0)
				(length 7.62)
				(name "P")
				(number "C2")
			)
			(pin passive line
				(at -27.94 10.16 0)
				(length 7.62)
				(name "P")
				(number "D3")
			)
			(pin passive line
				(at -27.94 7.62 0)
				(length 7.62)
				(name "P10-SGCK1")
				(number "B2")
			)
			(pin passive line
				(at -27.94 5.08 0)
				(length 7.62)
				(name "P13-PGCK1")
				(number "B3")
			)
			(pin passive line
				(at -27.94 2.54 0)
				(length 7.62)
				(name "P14")
				(number "A1")
			)
			(pin passive line
				(at -27.94 0 0)
				(length 7.62)
				(name "P")
				(number "A2")
			)
			(pin passive line
				(at -27.94 -2.54 0)
				(length 7.62)
				(name "P")
				(number "C5")
			)
			(pin passive line
				(at -27.94 -5.08 0)
				(length 7.62)
				(name "TDI")
				(number "B4")
			)
			(pin passive line
				(at -27.94 -7.62 0)
				(length 7.62)
				(name "TCK")
				(number "A3")
			)
			(pin passive line
				(at -27.94 -10.16 0)
				(length 7.62)
				(name "P")
				(number "B5")
			)
			(pin passive line
				(at -27.94 -12.7 0)
				(length 7.62)
				(name "P")
				(number "B6")
			)
			(pin passive line
				(at -27.94 -15.24 0)
				(length 7.62)
				(name "TMS")
				(number "A5")
			)
			(pin passive line
				(at -27.94 -17.78 0)
				(length 7.62)
				(name "P18")
				(number "C7")
			)
			(pin passive line
				(at -27.94 -20.32 0)
				(length 7.62)
				(name "P")
				(number "B7")
			)
			(pin passive line
				(at -27.94 -22.86 0)
				(length 7.62)
				(name "P")
				(number "A6")
			)
			(pin passive line
				(at -27.94 -25.4 0)
				(length 7.62)
				(name "P19")
				(number "A7")
			)
			(pin passive line
				(at -27.94 -27.94 0)
				(length 7.62)
				(name "P20")
				(number "A8")
			)
			(pin passive line
				(at -27.94 -30.48 0)
				(length 7.62)
				(name "P23")
				(number "C9")
			)
			(pin passive line
				(at -27.94 -33.02 0)
				(length 7.62)
				(name "P24")
				(number "B9")
			)
			(pin passive line
				(at -27.94 -35.56 0)
				(length 7.62)
				(name "P")
				(number "A9")
			)
			(pin passive line
				(at -27.94 -38.1 0)
				(length 7.62)
				(name "P")
				(number "B10")
			)
			(pin passive line
				(at -27.94 -40.64 0)
				(length 7.62)
				(name "P25")
				(number "C10")
			)
			(pin passive line
				(at -27.94 -43.18 0)
				(length 7.62)
				(name "P26")
				(number "A10")
			)
			(pin passive line
				(at -27.94 -45.72 0)
				(length 7.62)
				(name "P")
				(number "A11")
			)
			(pin passive line
				(at -27.94 -48.26 0)
				(length 7.62)
				(name "P")
				(number "B11")
			)
			(pin passive line
				(at -27.94 -50.8 0)
				(length 7.62)
				(name "P27")
				(number "B12")
			)
			(pin passive line
				(at -27.94 -53.34 0)
				(length 7.62)
				(name "P")
				(number "A13")
			)
			(pin passive line
				(at -27.94 -55.88 0)
				(length 7.62)
				(name "P")
				(number "A14")
			)
			(pin passive line
				(at -27.94 -58.42 0)
				(length 7.62)
				(name "P")
				(number "C12")
			)
			(pin passive line
				(at -27.94 -60.96 0)
				(length 7.62)
				(name "P28")
				(number "B13")
			)
			(pin passive line
				(at -27.94 -63.5 0)
				(length 7.62)
				(name "P29-SGCK2")
				(number "B14")
			)
			(pin passive line
				(at -27.94 -66.04 0)
				(length 7.62)
				(name "P-PGCK2")
				(number "B16")
			)
			(pin passive line
				(at -27.94 -68.58 0)
				(length 7.62)
				(name "P")
				(number "C15")
			)
			(pin passive line
				(at -27.94 -71.12 0)
				(length 7.62)
				(name "P")
				(number "D15")
			)
			(pin bidirectional line
				(at -27.94 -73.66 0)
				(length 7.62)
				(name "P36")
				(number "E14")
			)
			(pin passive line
				(at -27.94 -76.2 0)
				(length 7.62)
				(name "P")
				(number "F15")
			)
			(pin power_in line
				(at 0 86.36 270)
				(length 7.62)
				(name "VCC")
				(number "B8")
			)
			(pin passive line
				(at 0 86.36 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "C14")
			)
			(pin passive line
				(at 0 86.36 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "C3")
			)
			(pin passive line
				(at 0 86.36 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "H14")
			)
			(pin passive line
				(at 0 86.36 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "H3")
			)
			(pin passive line
				(at 0 86.36 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "P13")
			)
			(pin passive line
				(at 0 86.36 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "P3")
			)
			(pin passive line
				(at 0 86.36 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "R8")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "C11")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "C13")
			)
			(pin power_in line
				(at 0 -86.36 90)
				(length 7.62)
				(name "GND")
				(number "C4")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "C6")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "C8")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "F14")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "F3")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "H2")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "J14")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "L14")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "L3")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "N3")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "P11")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "P14")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "P6")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "P8")
			)
			(pin passive line
				(at 27.94 76.2 180)
				(length 7.62)
				(name "P84")
				(number "J3")
			)
			(pin passive line
				(at 27.94 73.66 180)
				(length 7.62)
				(name "P83")
				(number "J2")
			)
			(pin passive line
				(at 27.94 71.12 180)
				(length 7.62)
				(name "P")
				(number "J1")
			)
			(pin passive line
				(at 27.94 68.58 180)
				(length 7.62)
				(name "P")
				(number "K1")
			)
			(pin passive line
				(at 27.94 66.04 180)
				(length 7.62)
				(name "P82")
				(number "K2")
			)
			(pin passive line
				(at 27.94 63.5 180)
				(length 7.62)
				(name "P81")
				(number "K3")
			)
			(pin passive line
				(at 27.94 60.96 180)
				(length 7.62)
				(name "P")
				(number "L1")
			)
			(pin passive line
				(at 27.94 58.42 180)
				(length 7.62)
				(name "P")
				(number "L2")
			)
			(pin passive line
				(at 27.94 55.88 180)
				(length 7.62)
				(name "P80")
				(number "N1")
			)
			(pin passive line
				(at 27.94 53.34 180)
				(length 7.62)
				(name "P79")
				(number "P1")
			)
			(pin passive line
				(at 27.94 50.8 180)
				(length 7.62)
				(name "P")
				(number "M3")
			)
			(pin passive line
				(at 27.94 48.26 180)
				(length 7.62)
				(name "P")
				(number "N2")
			)
			(pin passive line
				(at 27.94 45.72 180)
				(length 7.62)
				(name "P78-PGCK4")
				(number "P2")
			)
			(pin passive line
				(at 27.94 43.18 180)
				(length 7.62)
				(name "P77")
				(number "R1")
			)
			(pin output line
				(at 27.94 40.64 180)
				(length 7.62)
				(name "TD0")
				(number "T1")
			)
			(pin passive line
				(at 27.94 38.1 180)
				(length 7.62)
				(name "P")
				(number "R3")
			)
			(pin passive line
				(at 27.94 35.56 180)
				(length 7.62)
				(name "P")
				(number "R4")
			)
			(pin passive line
				(at 27.94 33.02 180)
				(length 7.62)
				(name "RCLK-RDY-P70")
				(number "P5")
			)
			(pin passive line
				(at 27.94 30.48 180)
				(length 7.62)
				(name "P69")
				(number "T3")
			)
			(pin passive line
				(at 27.94 27.94 180)
				(length 7.62)
				(name "P")
				(number "T4")
			)
			(pin passive line
				(at 27.94 25.4 180)
				(length 7.62)
				(name "P")
				(number "R6")
			)
			(pin passive line
				(at 27.94 22.86 180)
				(length 7.62)
				(name "P68")
				(number "T5")
			)
			(pin passive line
				(at 27.94 20.32 180)
				(length 7.62)
				(name "P67")
				(number "P7")
			)
			(pin passive line
				(at 27.94 17.78 180)
				(length 7.62)
				(name "P")
				(number "R7")
			)
			(pin passive line
				(at 27.94 15.24 180)
				(length 7.62)
				(name "P")
				(number "T6")
			)
			(pin passive line
				(at 27.94 12.7 180)
				(length 7.62)
				(name "P66")
				(number "T7")
			)
			(pin passive line
				(at 27.94 10.16 180)
				(length 7.62)
				(name "P65")
				(number "T8")
			)
			(pin passive line
				(at 27.94 7.62 180)
				(length 7.62)
				(name "P62")
				(number "P9")
			)
			(pin passive line
				(at 27.94 5.08 180)
				(length 7.62)
				(name "P61")
				(number "R9")
			)
			(pin passive line
				(at 27.94 2.54 180)
				(length 7.62)
				(name "P")
				(number "T9")
			)
			(pin passive line
				(at 27.94 0 180)
				(length 7.62)
				(name "P")
				(number "R10")
			)
			(pin passive line
				(at 27.94 -2.54 180)
				(length 7.62)
				(name "P60")
				(number "P10")
			)
			(pin passive line
				(at 27.94 -5.08 180)
				(length 7.62)
				(name "P59")
				(number "T10")
			)
			(pin passive line
				(at 27.94 -7.62 180)
				(length 7.62)
				(name "P")
				(number "T11")
			)
			(pin passive line
				(at 27.94 -10.16 180)
				(length 7.62)
				(name "P")
				(number "R11")
			)
			(pin passive line
				(at 27.94 -12.7 180)
				(length 7.62)
				(name "P")
				(number "T13")
			)
			(pin passive line
				(at 27.94 -15.24 180)
				(length 7.62)
				(name "P58")
				(number "T14")
			)
			(pin passive line
				(at 27.94 -17.78 180)
				(length 7.62)
				(name "P")
				(number "P12")
			)
			(pin passive line
				(at 27.94 -20.32 180)
				(length 7.62)
				(name "P")
				(number "R13")
			)
			(pin passive line
				(at 27.94 -22.86 180)
				(length 7.62)
				(name "P57-PGCK3")
				(number "T15")
			)
			(pin passive line
				(at 27.94 -25.4 180)
				(length 7.62)
				(name "P56")
				(number "T16")
			)
			(pin passive line
				(at 27.94 -27.94 180)
				(length 7.62)
				(name "P51-SGCK3")
				(number "R16")
			)
			(pin passive line
				(at 27.94 -30.48 180)
				(length 7.62)
				(name "P50")
				(number "N14")
			)
			(pin passive line
				(at 27.94 -33.02 180)
				(length 7.62)
				(name "P")
				(number "P15")
			)
			(pin passive line
				(at 27.94 -35.56 180)
				(length 7.62)
				(name "P")
				(number "N15")
			)
			(pin passive line
				(at 27.94 -38.1 180)
				(length 7.62)
				(name "P49")
				(number "M14")
			)
			(pin passive line
				(at 27.94 -40.64 180)
				(length 7.62)
				(name "P48")
				(number "P16")
			)
			(pin passive line
				(at 27.94 -43.18 180)
				(length 7.62)
				(name "P")
				(number "L15")
			)
			(pin passive line
				(at 27.94 -45.72 180)
				(length 7.62)
				(name "P")
				(number "M16")
			)
			(pin passive line
				(at 27.94 -48.26 180)
				(length 7.62)
				(name "P47")
				(number "L16")
			)
			(pin passive line
				(at 27.94 -50.8 180)
				(length 7.62)
				(name "P46")
				(number "K14")
			)
			(pin passive line
				(at 27.94 -53.34 180)
				(length 7.62)
				(name "P")
				(number "K15")
			)
			(pin passive line
				(at 27.94 -55.88 180)
				(length 7.62)
				(name "P")
				(number "K16")
			)
			(pin passive line
				(at 27.94 -58.42 180)
				(length 7.62)
				(name "P45")
				(number "J16")
			)
			(pin passive line
				(at 27.94 -60.96 180)
				(length 7.62)
				(name "P44")
				(number "J15")
			)
			(pin passive line
				(at 27.94 -63.5 180)
				(length 7.62)
				(name "P40")
				(number "H16")
			)
			(pin passive line
				(at 27.94 -66.04 180)
				(length 7.62)
				(name "P")
				(number "G16")
			)
			(pin passive line
				(at 27.94 -68.58 180)
				(length 7.62)
				(name "P")
				(number "G15")
			)
			(pin passive line
				(at 27.94 -71.12 180)
				(length 7.62)
				(name "P39")
				(number "G14")
			)
			(pin passive line
				(at 27.94 -73.66 180)
				(length 7.62)
				(name "P38")
				(number "F16")
			)
			(pin passive line
				(at 27.94 -76.2 180)
				(length 7.62)
				(name "P")
				(number "E16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC4005-PQ100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XC4005-PQ100"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC4005-PQ100_0_1")
		(symbol "XC4005-PQ100_1_1"
			(pin input line
				(at -26.67 55.88 0)
				(length 7.62)
				(name "M0")
				(number "27")
			)
			(pin passive line
				(at -26.67 53.34 0)
				(length 7.62)
				(name "M1")
				(number "25")
			)
			(pin input line
				(at -26.67 50.8 0)
				(length 7.62)
				(name "M2")
				(number "29")
			)
			(pin input line
				(at -26.67 48.26 0)
				(length 7.62)
				(name "~{PROG}")
				(number "55")
			)
			(pin open_collector line
				(at -26.67 45.72 0)
				(length 7.62)
				(name "DONE")
				(number "53")
			)
			(pin passive line
				(at -26.67 43.18 0)
				(length 7.62)
				(name "DIN/D0")
				(number "75")
			)
			(pin passive line
				(at -26.67 40.64 0)
				(length 7.62)
				(name "DOUT/SGCK4")
				(number "76")
			)
			(pin input clock
				(at -26.67 38.1 0)
				(length 7.62)
				(name "CCLK")
				(number "77")
			)
			(pin passive line
				(at -26.67 33.02 0)
				(length 7.62)
				(name "P31/HDC")
				(number "31")
			)
			(pin passive line
				(at -26.67 30.48 0)
				(length 7.62)
				(name "P33/LDC")
				(number "33")
			)
			(pin passive line
				(at -26.67 25.4 0)
				(length 7.62)
				(name "PGCK1")
				(number "5")
			)
			(pin passive line
				(at -26.67 22.86 0)
				(length 7.62)
				(name "P6")
				(number "6")
			)
			(pin passive line
				(at -26.67 20.32 0)
				(length 7.62)
				(name "P7/TDI")
				(number "7")
			)
			(pin passive line
				(at -26.67 17.78 0)
				(length 7.62)
				(name "P8/TCK")
				(number "8")
			)
			(pin passive line
				(at -26.67 15.24 0)
				(length 7.62)
				(name "P9/TMS")
				(number "9")
			)
			(pin passive line
				(at -26.67 12.7 0)
				(length 7.62)
				(name "P11")
				(number "11")
			)
			(pin passive line
				(at -26.67 10.16 0)
				(length 7.62)
				(name "P12")
				(number "12")
			)
			(pin passive line
				(at -26.67 7.62 0)
				(length 7.62)
				(name "P13")
				(number "13")
			)
			(pin passive line
				(at -26.67 5.08 0)
				(length 7.62)
				(name "P16")
				(number "16")
			)
			(pin passive line
				(at -26.67 2.54 0)
				(length 7.62)
				(name "P17")
				(number "17")
			)
			(pin passive line
				(at -26.67 0 0)
				(length 7.62)
				(name "P18")
				(number "18")
			)
			(pin passive line
				(at -26.67 -2.54 0)
				(length 7.62)
				(name "P19")
				(number "19")
			)
			(pin passive line
				(at -26.67 -5.08 0)
				(length 7.62)
				(name "P20")
				(number "20")
			)
			(pin passive line
				(at -26.67 -7.62 0)
				(length 7.62)
				(name "P21")
				(number "21")
			)
			(pin passive line
				(at -26.67 -10.16 0)
				(length 7.62)
				(name "P22")
				(number "22")
			)
			(pin passive line
				(at -26.67 -12.7 0)
				(length 7.62)
				(name "P23")
				(number "23")
			)
			(pin passive line
				(at -26.67 -17.78 0)
				(length 7.62)
				(name "SGCK2")
				(number "24")
			)
			(pin passive line
				(at -26.67 -20.32 0)
				(length 7.62)
				(name "PGCK2")
				(number "30")
			)
			(pin passive line
				(at -26.67 -25.4 0)
				(length 7.62)
				(name "P32")
				(number "32")
			)
			(pin passive line
				(at -26.67 -27.94 0)
				(length 7.62)
				(name "P34")
				(number "34")
			)
			(pin passive line
				(at -26.67 -30.48 0)
				(length 7.62)
				(name "P35")
				(number "35")
			)
			(pin passive line
				(at -26.67 -33.02 0)
				(length 7.62)
				(name "P36")
				(number "36")
			)
			(pin passive line
				(at -26.67 -35.56 0)
				(length 7.62)
				(name "P37")
				(number "37")
			)
			(pin passive line
				(at -26.67 -38.1 0)
				(length 7.62)
				(name "P38")
				(number "38")
			)
			(pin passive line
				(at -26.67 -40.64 0)
				(length 7.62)
				(name "P39/INIT")
				(number "39")
			)
			(pin passive line
				(at -26.67 -43.18 0)
				(length 7.62)
				(name "P42")
				(number "42")
			)
			(pin passive line
				(at -26.67 -45.72 0)
				(length 7.62)
				(name "P43")
				(number "43")
			)
			(pin passive line
				(at -26.67 -48.26 0)
				(length 7.62)
				(name "P44")
				(number "44")
			)
			(pin passive line
				(at -26.67 -50.8 0)
				(length 7.62)
				(name "P45")
				(number "45")
			)
			(pin passive line
				(at -26.67 -53.34 0)
				(length 7.62)
				(name "P46")
				(number "46")
			)
			(pin passive line
				(at -26.67 -55.88 0)
				(length 7.62)
				(name "P47")
				(number "47")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "15")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at 0 66.04 270)
				(length 7.62)
				(name "VCC")
				(number "3")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "40")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "54")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "66")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "78")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "92")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin power_in line
				(at 0 -66.04 90)
				(length 7.62)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "52")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "67")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "80")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "91")
			)
			(pin passive line
				(at 26.67 55.88 180)
				(length 7.62)
				(name "SGCK1")
				(number "2")
			)
			(pin passive line
				(at 26.67 53.34 180)
				(length 7.62)
				(name "P1")
				(number "1")
			)
			(pin passive line
				(at 26.67 50.8 180)
				(length 7.62)
				(name "P100")
				(number "100")
			)
			(pin passive line
				(at 26.67 48.26 180)
				(length 7.62)
				(name "P99")
				(number "99")
			)
			(pin passive line
				(at 26.67 45.72 180)
				(length 7.62)
				(name "P98")
				(number "98")
			)
			(pin passive line
				(at 26.67 43.18 180)
				(length 7.62)
				(name "P97")
				(number "97")
			)
			(pin passive line
				(at 26.67 40.64 180)
				(length 7.62)
				(name "P96")
				(number "96")
			)
			(pin passive line
				(at 26.67 38.1 180)
				(length 7.62)
				(name "P95")
				(number "95")
			)
			(pin passive line
				(at 26.67 35.56 180)
				(length 7.62)
				(name "P94")
				(number "94")
			)
			(pin passive line
				(at 26.67 33.02 180)
				(length 7.62)
				(name "P93")
				(number "93")
			)
			(pin passive line
				(at 26.67 30.48 180)
				(length 7.62)
				(name "P90")
				(number "90")
			)
			(pin passive line
				(at 26.67 27.94 180)
				(length 7.62)
				(name "P89")
				(number "89")
			)
			(pin passive line
				(at 26.67 25.4 180)
				(length 7.62)
				(name "P88")
				(number "88")
			)
			(pin passive line
				(at 26.67 22.86 180)
				(length 7.62)
				(name "P87")
				(number "87")
			)
			(pin passive line
				(at 26.67 20.32 180)
				(length 7.62)
				(name "P86")
				(number "86")
			)
			(pin passive line
				(at 26.67 17.78 180)
				(length 7.62)
				(name "P85")
				(number "85")
			)
			(pin passive line
				(at 26.67 15.24 180)
				(length 7.62)
				(name "P84")
				(number "84")
			)
			(pin passive line
				(at 26.67 12.7 180)
				(length 7.62)
				(name "P83")
				(number "83")
			)
			(pin passive line
				(at 26.67 7.62 180)
				(length 7.62)
				(name "PGCK4")
				(number "82")
			)
			(pin passive line
				(at 26.67 5.08 180)
				(length 7.62)
				(name "P81")
				(number "81")
			)
			(pin output line
				(at 26.67 2.54 180)
				(length 7.62)
				(name "TDO")
				(number "79")
			)
			(pin passive line
				(at 26.67 0 180)
				(length 7.62)
				(name "P74/BUSY")
				(number "74")
			)
			(pin passive line
				(at 26.67 -2.54 180)
				(length 7.62)
				(name "P73")
				(number "73")
			)
			(pin passive line
				(at 26.67 -5.08 180)
				(length 7.62)
				(name "P72")
				(number "72")
			)
			(pin passive line
				(at 26.67 -7.62 180)
				(length 7.62)
				(name "P71")
				(number "71")
			)
			(pin passive line
				(at 26.67 -10.16 180)
				(length 7.62)
				(name "P70")
				(number "70")
			)
			(pin passive line
				(at 26.67 -12.7 180)
				(length 7.62)
				(name "P69")
				(number "69")
			)
			(pin passive line
				(at 26.67 -15.24 180)
				(length 7.62)
				(name "P68")
				(number "68")
			)
			(pin passive line
				(at 26.67 -17.78 180)
				(length 7.62)
				(name "P65")
				(number "65")
			)
			(pin passive line
				(at 26.67 -20.32 180)
				(length 7.62)
				(name "P64")
				(number "64")
			)
			(pin passive line
				(at 26.67 -22.86 180)
				(length 7.62)
				(name "P63")
				(number "63")
			)
			(pin passive line
				(at 26.67 -25.4 180)
				(length 7.62)
				(name "P62")
				(number "62")
			)
			(pin passive line
				(at 26.67 -27.94 180)
				(length 7.62)
				(name "P61")
				(number "61")
			)
			(pin passive line
				(at 26.67 -30.48 180)
				(length 7.62)
				(name "P60")
				(number "60")
			)
			(pin passive line
				(at 26.67 -33.02 180)
				(length 7.62)
				(name "P59")
				(number "59")
			)
			(pin passive line
				(at 26.67 -35.56 180)
				(length 7.62)
				(name "P58")
				(number "58")
			)
			(pin passive line
				(at 26.67 -40.64 180)
				(length 7.62)
				(name "PGCK3")
				(number "57")
			)
			(pin passive line
				(at 26.67 -43.18 180)
				(length 7.62)
				(name "P56")
				(number "56")
			)
			(pin passive line
				(at 26.67 -45.72 180)
				(length 7.62)
				(name "SGCK3")
				(number "51")
			)
			(pin passive line
				(at 26.67 -50.8 180)
				(length 7.62)
				(name "P50")
				(number "50")
			)
			(pin passive line
				(at 26.67 -53.34 180)
				(length 7.62)
				(name "P49")
				(number "49")
			)
			(pin passive line
				(at 26.67 -55.88 180)
				(length 7.62)
				(name "P48")
				(number "48")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC4005-PQ160"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XC4005-PQ160"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC4005-PQ160_0_1")
		(symbol "XC4005-PQ160_1_1"
			(pin input line
				(at -27.94 76.2 0)
				(length 7.62)
				(name "M0")
				(number "40")
			)
			(pin input line
				(at -27.94 73.66 0)
				(length 7.62)
				(name "M1")
				(number "38")
			)
			(pin input line
				(at -27.94 71.12 0)
				(length 7.62)
				(name "M2")
				(number "42")
			)
			(pin input line
				(at -27.94 66.04 0)
				(length 7.62)
				(name "~{PROG}")
				(number "82")
			)
			(pin bidirectional line
				(at -27.94 63.5 0)
				(length 7.62)
				(name "DONE")
				(number "80")
			)
			(pin input line
				(at -27.94 60.96 0)
				(length 7.62)
				(name "DIN")
				(number "117")
			)
			(pin passive line
				(at -27.94 58.42 0)
				(length 7.62)
				(name "DOUT-SGI4")
				(number "118")
			)
			(pin passive clock
				(at -27.94 55.88 0)
				(length 7.62)
				(name "CCLK")
				(number "119")
			)
			(pin passive line
				(at -27.94 50.8 0)
				(length 7.62)
				(name "HDC")
				(number "44")
			)
			(pin passive line
				(at -27.94 48.26 0)
				(length 7.62)
				(name "LDC")
				(number "48")
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 7.62)
				(name "PGCK1")
				(number "2")
			)
			(pin passive line
				(at -27.94 40.64 0)
				(length 7.62)
				(name "P3")
				(number "3")
			)
			(pin passive line
				(at -27.94 38.1 0)
				(length 7.62)
				(name "P4")
				(number "4")
			)
			(pin passive line
				(at -27.94 35.56 0)
				(length 7.62)
				(name "P5")
				(number "5")
			)
			(pin passive line
				(at -27.94 33.02 0)
				(length 7.62)
				(name "TDI")
				(number "6")
			)
			(pin passive line
				(at -27.94 30.48 0)
				(length 7.62)
				(name "TCK")
				(number "7")
			)
			(pin passive line
				(at -27.94 27.94 0)
				(length 7.62)
				(name "P11")
				(number "11")
			)
			(pin passive line
				(at -27.94 25.4 0)
				(length 7.62)
				(name "P12")
				(number "12")
			)
			(pin passive line
				(at -27.94 22.86 0)
				(length 7.62)
				(name "TMS")
				(number "13")
			)
			(pin passive line
				(at -27.94 20.32 0)
				(length 7.62)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -27.94 17.78 0)
				(length 7.62)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -27.94 15.24 0)
				(length 7.62)
				(name "P16")
				(number "16")
			)
			(pin passive line
				(at -27.94 12.7 0)
				(length 7.62)
				(name "P17")
				(number "17")
			)
			(pin passive line
				(at -27.94 10.16 0)
				(length 7.62)
				(name "P18")
				(number "18")
			)
			(pin passive line
				(at -27.94 7.62 0)
				(length 7.62)
				(name "P21")
				(number "21")
			)
			(pin passive line
				(at -27.94 5.08 0)
				(length 7.62)
				(name "P22")
				(number "22")
			)
			(pin passive line
				(at -27.94 2.54 0)
				(length 7.62)
				(name "P23")
				(number "23")
			)
			(pin passive line
				(at -27.94 0 0)
				(length 7.62)
				(name "P24")
				(number "24")
			)
			(pin passive line
				(at -27.94 -2.54 0)
				(length 7.62)
				(name "P25")
				(number "25")
			)
			(pin passive line
				(at -27.94 -5.08 0)
				(length 7.62)
				(name "P26")
				(number "26")
			)
			(pin passive line
				(at -27.94 -7.62 0)
				(length 7.62)
				(name "P27")
				(number "27")
			)
			(pin passive line
				(at -27.94 -10.16 0)
				(length 7.62)
				(name "P28")
				(number "28")
			)
			(pin passive line
				(at -27.94 -12.7 0)
				(length 7.62)
				(name "P32")
				(number "32")
			)
			(pin passive line
				(at -27.94 -15.24 0)
				(length 7.62)
				(name "P33")
				(number "33")
			)
			(pin passive line
				(at -27.94 -17.78 0)
				(length 7.62)
				(name "P34")
				(number "34")
			)
			(pin passive line
				(at -27.94 -20.32 0)
				(length 7.62)
				(name "P35")
				(number "35")
			)
			(pin passive line
				(at -27.94 -22.86 0)
				(length 7.62)
				(name "P36")
				(number "36")
			)
			(pin passive line
				(at -27.94 -25.4 0)
				(length 7.62)
				(name "SGCK2")
				(number "37")
			)
			(pin passive line
				(at -27.94 -27.94 0)
				(length 7.62)
				(name "PGCK2")
				(number "43")
			)
			(pin passive line
				(at -27.94 -30.48 0)
				(length 7.62)
				(name "P45")
				(number "45")
			)
			(pin passive line
				(at -27.94 -33.02 0)
				(length 7.62)
				(name "P46")
				(number "46")
			)
			(pin passive line
				(at -27.94 -35.56 0)
				(length 7.62)
				(name "P47")
				(number "47")
			)
			(pin passive line
				(at -27.94 -38.1 0)
				(length 7.62)
				(name "P52")
				(number "52")
			)
			(pin passive line
				(at -27.94 -40.64 0)
				(length 7.62)
				(name "P53")
				(number "53")
			)
			(pin passive line
				(at -27.94 -43.18 0)
				(length 7.62)
				(name "P54")
				(number "54")
			)
			(pin passive line
				(at -27.94 -45.72 0)
				(length 7.62)
				(name "P55")
				(number "55")
			)
			(pin passive line
				(at -27.94 -48.26 0)
				(length 7.62)
				(name "P56")
				(number "56")
			)
			(pin passive line
				(at -27.94 -50.8 0)
				(length 7.62)
				(name "P57")
				(number "57")
			)
			(pin passive line
				(at -27.94 -53.34 0)
				(length 7.62)
				(name "P58")
				(number "58")
			)
			(pin passive line
				(at -27.94 -55.88 0)
				(length 7.62)
				(name "P59-INIT")
				(number "59")
			)
			(pin passive line
				(at -27.94 -58.42 0)
				(length 7.62)
				(name "P62")
				(number "62")
			)
			(pin passive line
				(at -27.94 -60.96 0)
				(length 7.62)
				(name "P63")
				(number "63")
			)
			(pin passive line
				(at -27.94 -63.5 0)
				(length 7.62)
				(name "P64")
				(number "64")
			)
			(pin passive line
				(at -27.94 -66.04 0)
				(length 7.62)
				(name "P65")
				(number "65")
			)
			(pin passive line
				(at -27.94 -68.58 0)
				(length 7.62)
				(name "P66")
				(number "66")
			)
			(pin passive line
				(at -27.94 -71.12 0)
				(length 7.62)
				(name "P67")
				(number "67")
			)
			(pin bidirectional line
				(at -27.94 -73.66 0)
				(length 7.62)
				(name "P68")
				(number "68")
			)
			(pin passive line
				(at -27.94 -76.2 0)
				(length 7.62)
				(name "P69")
				(number "69")
			)
			(pin passive line
				(at 0 86.36 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "100")
			)
			(pin passive line
				(at 0 86.36 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "120")
			)
			(pin passive line
				(at 0 86.36 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "142")
			)
			(pin passive line
				(at 0 86.36 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "160")
			)
			(pin power_in line
				(at 0 86.36 270)
				(length 7.62)
				(name "VCC")
				(number "20")
			)
			(pin passive line
				(at 0 86.36 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "41")
			)
			(pin passive line
				(at 0 86.36 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "60")
			)
			(pin passive line
				(at 0 86.36 270)
				(length 7.62)
				(hide yes)
				(name "VCC")
				(number "81")
			)
			(pin power_in line
				(at 0 -86.36 90)
				(length 7.62)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "101")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "110")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "122")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "131")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "141")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "151")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "51")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "61")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "70")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "79")
			)
			(pin passive line
				(at 0 -86.36 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "91")
			)
			(pin passive line
				(at 27.94 76.2 180)
				(length 7.62)
				(name "SGCK1")
				(number "159")
			)
			(pin passive line
				(at 27.94 73.66 180)
				(length 7.62)
				(name "P158")
				(number "158")
			)
			(pin passive line
				(at 27.94 71.12 180)
				(length 7.62)
				(name "P157")
				(number "157")
			)
			(pin passive line
				(at 27.94 68.58 180)
				(length 7.62)
				(name "P156")
				(number "156")
			)
			(pin passive line
				(at 27.94 66.04 180)
				(length 7.62)
				(name "P155")
				(number "155")
			)
			(pin passive line
				(at 27.94 63.5 180)
				(length 7.62)
				(name "P154")
				(number "154")
			)
			(pin passive line
				(at 27.94 60.96 180)
				(length 7.62)
				(name "P150")
				(number "150")
			)
			(pin passive line
				(at 27.94 58.42 180)
				(length 7.62)
				(name "P149")
				(number "149")
			)
			(pin passive line
				(at 27.94 55.88 180)
				(length 7.62)
				(name "P148")
				(number "148")
			)
			(pin passive line
				(at 27.94 53.34 180)
				(length 7.62)
				(name "P147")
				(number "147")
			)
			(pin passive line
				(at 27.94 50.8 180)
				(length 7.62)
				(name "P146")
				(number "146")
			)
			(pin passive line
				(at 27.94 48.26 180)
				(length 7.62)
				(name "P145")
				(number "145")
			)
			(pin passive line
				(at 27.94 45.72 180)
				(length 7.62)
				(name "P144")
				(number "144")
			)
			(pin passive line
				(at 27.94 43.18 180)
				(length 7.62)
				(name "P143")
				(number "143")
			)
			(pin passive line
				(at 27.94 40.64 180)
				(length 7.62)
				(name "P140")
				(number "140")
			)
			(pin passive line
				(at 27.94 38.1 180)
				(length 7.62)
				(name "P139")
				(number "139")
			)
			(pin passive line
				(at 27.94 35.56 180)
				(length 7.62)
				(name "P138")
				(number "138")
			)
			(pin passive line
				(at 27.94 33.02 180)
				(length 7.62)
				(name "P137")
				(number "137")
			)
			(pin passive line
				(at 27.94 30.48 180)
				(length 7.62)
				(name "P135")
				(number "135")
			)
			(pin passive line
				(at 27.94 27.94 180)
				(length 7.62)
				(name "P134")
				(number "134")
			)
			(pin passive line
				(at 27.94 25.4 180)
				(length 7.62)
				(name "P133")
				(number "133")
			)
			(pin passive line
				(at 27.94 22.86 180)
				(length 7.62)
				(name "P132")
				(number "132")
			)
			(pin passive line
				(at 27.94 20.32 180)
				(length 7.62)
				(name "P128")
				(number "128")
			)
			(pin passive line
				(at 27.94 17.78 180)
				(length 7.62)
				(name "P127")
				(number "127")
			)
			(pin passive line
				(at 27.94 15.24 180)
				(length 7.62)
				(name "P126")
				(number "126")
			)
			(pin passive line
				(at 27.94 12.7 180)
				(length 7.62)
				(name "P125")
				(number "125")
			)
			(pin passive line
				(at 27.94 10.16 180)
				(length 7.62)
				(name "P124")
				(number "124")
			)
			(pin passive line
				(at 27.94 7.62 180)
				(length 7.62)
				(name "P123")
				(number "123")
			)
			(pin output line
				(at 27.94 5.08 180)
				(length 7.62)
				(name "TDO")
				(number "121")
			)
			(pin passive line
				(at 27.94 2.54 180)
				(length 7.62)
				(name "P116")
				(number "116")
			)
			(pin passive line
				(at 27.94 0 180)
				(length 7.62)
				(name "P115")
				(number "115")
			)
			(pin passive line
				(at 27.94 -2.54 180)
				(length 7.62)
				(name "P114-RDY")
				(number "114")
			)
			(pin passive line
				(at 27.94 -5.08 180)
				(length 7.62)
				(name "P113")
				(number "113")
			)
			(pin passive line
				(at 27.94 -7.62 180)
				(length 7.62)
				(name "P109")
				(number "109")
			)
			(pin passive line
				(at 27.94 -10.16 180)
				(length 7.62)
				(name "P108")
				(number "108")
			)
			(pin passive line
				(at 27.94 -12.7 180)
				(length 7.62)
				(name "P107")
				(number "107")
			)
			(pin passive line
				(at 27.94 -15.24 180)
				(length 7.62)
				(name "P106")
				(number "106")
			)
			(pin passive line
				(at 27.94 -17.78 180)
				(length 7.62)
				(name "P105")
				(number "105")
			)
			(pin passive line
				(at 27.94 -20.32 180)
				(length 7.62)
				(name "P104")
				(number "104")
			)
			(pin passive line
				(at 27.94 -22.86 180)
				(length 7.62)
				(name "P103")
				(number "103")
			)
			(pin passive line
				(at 27.94 -25.4 180)
				(length 7.62)
				(name "P102")
				(number "102")
			)
			(pin passive line
				(at 27.94 -27.94 180)
				(length 7.62)
				(name "P90")
				(number "99")
			)
			(pin passive line
				(at 27.94 -30.48 180)
				(length 7.62)
				(name "P98")
				(number "98")
			)
			(pin passive line
				(at 27.94 -33.02 180)
				(length 7.62)
				(name "P97")
				(number "97")
			)
			(pin passive line
				(at 27.94 -35.56 180)
				(length 7.62)
				(name "P96")
				(number "96")
			)
			(pin passive line
				(at 27.94 -38.1 180)
				(length 7.62)
				(name "P95")
				(number "95")
			)
			(pin passive line
				(at 27.94 -40.64 180)
				(length 7.62)
				(name "P93")
				(number "94")
			)
			(pin passive line
				(at 27.94 -43.18 180)
				(length 7.62)
				(name "P93")
				(number "93")
			)
			(pin passive line
				(at 27.94 -45.72 180)
				(length 7.62)
				(name "P92")
				(number "92")
			)
			(pin passive line
				(at 27.94 -48.26 180)
				(length 7.62)
				(name "P88")
				(number "88")
			)
			(pin passive line
				(at 27.94 -50.8 180)
				(length 7.62)
				(name "P87")
				(number "87")
			)
			(pin passive line
				(at 27.94 -53.34 180)
				(length 7.62)
				(name "P86")
				(number "86")
			)
			(pin passive line
				(at 27.94 -55.88 180)
				(length 7.62)
				(name "P85")
				(number "85")
			)
			(pin passive line
				(at 27.94 -58.42 180)
				(length 7.62)
				(name "PGCK3")
				(number "84")
			)
			(pin passive line
				(at 27.94 -60.96 180)
				(length 7.62)
				(name "P83")
				(number "83")
			)
			(pin passive line
				(at 27.94 -63.5 180)
				(length 7.62)
				(name "SGCK3")
				(number "78")
			)
			(pin passive line
				(at 27.94 -66.04 180)
				(length 7.62)
				(name "P77")
				(number "77")
			)
			(pin passive line
				(at 27.94 -68.58 180)
				(length 7.62)
				(name "P76")
				(number "76")
			)
			(pin passive line
				(at 27.94 -71.12 180)
				(length 7.62)
				(name "P75")
				(number "75")
			)
			(pin passive line
				(at 27.94 -73.66 180)
				(length 7.62)
				(name "P74")
				(number "74")
			)
			(pin passive line
				(at 27.94 -76.2 180)
				(length 7.62)
				(name "P73")
				(number "73")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX25T-BG484"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 76.2 0)
		)
		(property "Value" "XC6SLX25T-BG484"
			(at 0 78.74 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "SPARTAN-6  FG484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(symbol "XC6SLX25T-BG484_1_1"
			(pin input line
				(at -35.56 87.63 0)
				(length 7.62)
				(name "TCK")
				(number "A21")
			)
			(pin input line
				(at -35.56 85.09 0)
				(length 7.62)
				(name "TDI")
				(number "E18")
			)
			(pin input line
				(at -35.56 82.55 0)
				(length 7.62)
				(name "TMS")
				(number "D20")
			)
			(pin output line
				(at -35.56 80.01 0)
				(length 7.62)
				(name "TDO")
				(number "G17")
			)
			(pin bidirectional line
				(at -35.56 72.39 0)
				(length 7.62)
				(name "IO_L1P_HSWAPEN_0")
				(number "C3")
			)
			(pin bidirectional line
				(at -35.56 69.85 0)
				(length 7.62)
				(name "IO_L1N_VREF_0")
				(number "D3")
			)
			(pin bidirectional line
				(at -35.56 67.31 0)
				(length 7.62)
				(name "IO_L2P_0")
				(number "D4")
			)
			(pin bidirectional line
				(at -35.56 64.77 0)
				(length 7.62)
				(name "IO_L2N_0")
				(number "D5")
			)
			(pin bidirectional line
				(at -35.56 62.23 0)
				(length 7.62)
				(name "IO_L3P_0")
				(number "B2")
			)
			(pin bidirectional line
				(at -35.56 59.69 0)
				(length 7.62)
				(name "IO_L3N_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -35.56 57.15 0)
				(length 7.62)
				(name "IO_L4P_0")
				(number "E5")
			)
			(pin bidirectional line
				(at -35.56 54.61 0)
				(length 7.62)
				(name "IO_L4N_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -35.56 52.07 0)
				(length 7.62)
				(name "IO_L5P_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -35.56 49.53 0)
				(length 7.62)
				(name "IO_L5N_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -35.56 46.99 0)
				(length 7.62)
				(name "IO_L6P_0")
				(number "C4")
			)
			(pin bidirectional line
				(at -35.56 44.45 0)
				(length 7.62)
				(name "IO_L6N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -35.56 41.91 0)
				(length 7.62)
				(name "IO_L7P_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -35.56 39.37 0)
				(length 7.62)
				(name "IO_L7N_0")
				(number "F8")
			)
			(pin bidirectional line
				(at -35.56 36.83 0)
				(length 7.62)
				(name "IO_L8P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -35.56 34.29 0)
				(length 7.62)
				(name "IO_L8N_VREF_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -35.56 31.75 0)
				(length 7.62)
				(name "IO_L32P_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -35.56 29.21 0)
				(length 7.62)
				(name "IO_L32N_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -35.56 26.67 0)
				(length 7.62)
				(name "IO_L33P_0")
				(number "H10")
			)
			(pin bidirectional line
				(at -35.56 24.13 0)
				(length 7.62)
				(name "IO_L33N_0")
				(number "H11")
			)
			(pin bidirectional line
				(at -35.56 21.59 0)
				(length 7.62)
				(name "IO_L34P_GCLK19_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -35.56 19.05 0)
				(length 7.62)
				(name "IO_L34N_GCLK18_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -35.56 16.51 0)
				(length 7.62)
				(name "IO_L35P_GCLK17_0")
				(number "H12")
			)
			(pin bidirectional line
				(at -35.56 13.97 0)
				(length 7.62)
				(name "IO_L35N_GCLK16_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -35.56 11.43 0)
				(length 7.62)
				(name "IO_L36P_GCLK15_0")
				(number "F14")
			)
			(pin bidirectional line
				(at -35.56 8.89 0)
				(length 7.62)
				(name "IO_L36N_GCLK14_0")
				(number "F15")
			)
			(pin bidirectional line
				(at -35.56 6.35 0)
				(length 7.62)
				(name "IO_L37P_GCLK13_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -35.56 3.81 0)
				(length 7.62)
				(name "IO_L37N_GCLK12_0")
				(number "F16")
			)
			(pin bidirectional line
				(at -35.56 1.27 0)
				(length 7.62)
				(name "IO_L38P_0")
				(number "H13")
			)
			(pin bidirectional line
				(at -35.56 -1.27 0)
				(length 7.62)
				(name "IO_L38N_VREF_0")
				(number "G13")
			)
			(pin bidirectional line
				(at -35.56 -3.81 0)
				(length 7.62)
				(name "IO_L49P_0")
				(number "H14")
			)
			(pin bidirectional line
				(at -35.56 -6.35 0)
				(length 7.62)
				(name "IO_L49N_0")
				(number "G15")
			)
			(pin bidirectional line
				(at -35.56 -8.89 0)
				(length 7.62)
				(name "IO_L50P_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -35.56 -11.43 0)
				(length 7.62)
				(name "IO_L50N_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -35.56 -13.97 0)
				(length 7.62)
				(name "IO_L51P_0")
				(number "G16")
			)
			(pin bidirectional line
				(at -35.56 -16.51 0)
				(length 7.62)
				(name "IO_L51N_0")
				(number "F17")
			)
			(pin bidirectional line
				(at -35.56 -19.05 0)
				(length 7.62)
				(name "IO_L62P_0")
				(number "D18")
			)
			(pin bidirectional line
				(at -35.56 -21.59 0)
				(length 7.62)
				(name "IO_L62N_VREF_0")
				(number "D19")
			)
			(pin bidirectional line
				(at -35.56 -24.13 0)
				(length 7.62)
				(name "IO_L63P_SCP7_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -35.56 -26.67 0)
				(length 7.62)
				(name "IO_L63N_SCP6_0")
				(number "A18")
			)
			(pin bidirectional line
				(at -35.56 -29.21 0)
				(length 7.62)
				(name "IO_L64P_SCP5_0")
				(number "C19")
			)
			(pin bidirectional line
				(at -35.56 -31.75 0)
				(length 7.62)
				(name "IO_L46N_SCP4_0")
				(number "A19")
			)
			(pin bidirectional line
				(at -35.56 -34.29 0)
				(length 7.62)
				(name "IO_L65P_SCP3_0")
				(number "B20")
			)
			(pin bidirectional line
				(at -35.56 -36.83 0)
				(length 7.62)
				(name "IO_L65N_SCP2_0")
				(number "A20")
			)
			(pin bidirectional line
				(at -35.56 -39.37 0)
				(length 7.62)
				(name "IO_L66P_SCP1_0")
				(number "D17")
			)
			(pin bidirectional line
				(at -35.56 -41.91 0)
				(length 7.62)
				(name "IO_L66N_SCP0_0")
				(number "C18")
			)
			(pin output line
				(at -35.56 -46.99 0)
				(length 7.62)
				(name "MGTTXN0_101")
				(number "A6")
			)
			(pin output line
				(at -35.56 -49.53 0)
				(length 7.62)
				(name "MGTTXP0_101")
				(number "B6")
			)
			(pin passive line
				(at -35.56 -52.07 0)
				(length 7.62)
				(name "MGTAVCCPLL0_101")
				(number "B9")
			)
			(pin input line
				(at -35.56 -54.61 0)
				(length 7.62)
				(name "MGTREFCLK0N_101")
				(number "B10")
			)
			(pin input line
				(at -35.56 -57.15 0)
				(length 7.62)
				(name "MGTREFCLK0P_101")
				(number "A10")
			)
			(pin input line
				(at -35.56 -59.69 0)
				(length 7.62)
				(name "MGTRXN0_101")
				(number "C7")
			)
			(pin input line
				(at -35.56 -62.23 0)
				(length 7.62)
				(name "MGTRXP0_101")
				(number "D7")
			)
			(pin input line
				(at -35.56 -64.77 0)
				(length 7.62)
				(name "MGTRREF_101")
				(number "E9")
			)
			(pin input line
				(at -35.56 -67.31 0)
				(length 7.62)
				(name "MGTRXN1_101")
				(number "C9")
			)
			(pin passive line
				(at -35.56 -69.85 0)
				(length 7.62)
				(name "MGTAVTTRCAL_101")
				(number "E8")
			)
			(pin input line
				(at -35.56 -72.39 0)
				(length 7.62)
				(name "MGTRXP1_101")
				(number "D9")
			)
			(pin passive line
				(at -35.56 -74.93 0)
				(length 7.62)
				(name "MGTAVCCPLL1_101")
				(number "D12")
			)
			(pin input line
				(at -35.56 -77.47 0)
				(length 7.62)
				(name "MGTREFCLK1N_101")
				(number "D11")
			)
			(pin input line
				(at -35.56 -80.01 0)
				(length 7.62)
				(name "MGTREFCLK1P_101")
				(number "C11")
			)
			(pin output line
				(at -35.56 -82.55 0)
				(length 7.62)
				(name "MGTTXN1_101")
				(number "A8")
			)
			(pin output line
				(at -35.56 -85.09 0)
				(length 7.62)
				(name "MGTTXP1_101")
				(number "B8")
			)
			(pin passive line
				(at -35.56 -87.63 0)
				(length 7.62)
				(name "MGTAVCC_101")
				(number "C10")
			)
			(pin passive line
				(at -35.56 -90.17 0)
				(length 7.62)
				(name "MGTAVTTRX_101")
				(number "D8")
			)
			(pin passive line
				(at -35.56 -92.71 0)
				(length 7.62)
				(name "MGTAVTTTX_101")
				(number "A7")
			)
			(pin power_in line
				(at -17.78 100.33 270)
				(length 5.08)
				(name "VCCO_0")
				(number "B19")
			)
			(pin power_in line
				(at -15.24 100.33 270)
				(length 5.08)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -12.7 100.33 270)
				(length 5.08)
				(name "VCCO_0")
				(number "E17")
			)
			(pin power_in line
				(at -10.16 100.33 270)
				(length 5.08)
				(name "VCCO_0")
				(number "F6")
			)
			(pin power_in line
				(at -7.62 100.33 270)
				(length 5.08)
				(name "VCCO_0")
				(number "G10")
			)
			(pin power_in line
				(at -5.08 100.33 270)
				(length 5.08)
				(name "VCCO_0")
				(number "G14")
			)
			(pin power_in line
				(at 2.54 100.33 270)
				(length 5.08)
				(name "VCCO_1")
				(number "C21")
			)
			(pin power_in line
				(at 5.08 100.33 270)
				(length 5.08)
				(name "VCCO_1")
				(number "E19")
			)
			(pin power_in line
				(at 7.62 100.33 270)
				(length 5.08)
				(name "VCCO_1")
				(number "G21")
			)
			(pin power_in line
				(at 10.16 100.33 270)
				(length 5.08)
				(name "VCCO_1")
				(number "J18")
			)
			(pin power_in line
				(at 12.7 100.33 270)
				(length 5.08)
				(name "VCCO_1")
				(number "L16")
			)
			(pin power_in line
				(at 15.24 100.33 270)
				(length 5.08)
				(name "VCCO_1")
				(number "L21")
			)
			(pin power_in line
				(at 17.78 100.33 270)
				(length 5.08)
				(name "VCCO_1")
				(number "N18")
			)
			(pin power_in line
				(at 20.32 100.33 270)
				(length 5.08)
				(name "VCCO_1")
				(number "R21")
			)
			(pin power_in line
				(at 22.86 100.33 270)
				(length 5.08)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 25.4 100.33 270)
				(length 5.08)
				(name "VCCO_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 35.56 74.93 180)
				(length 7.62)
				(name "IO_L1P_A25_1")
				(number "F18")
			)
			(pin bidirectional line
				(at 35.56 72.39 180)
				(length 7.62)
				(name "IO_L1N_A24_VREF_1")
				(number "F19")
			)
			(pin bidirectional line
				(at 35.56 69.85 180)
				(length 7.62)
				(name "IO_L19P_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 35.56 67.31 180)
				(length 7.62)
				(name "IO_L19N_1")
				(number "J17")
			)
			(pin bidirectional line
				(at 35.56 64.77 180)
				(length 7.62)
				(name "IO_L20P_1")
				(number "C20")
			)
			(pin bidirectional line
				(at 35.56 62.23 180)
				(length 7.62)
				(name "IO_L20N_1")
				(number "C22")
			)
			(pin bidirectional line
				(at 35.56 59.69 180)
				(length 7.62)
				(name "IO_L29P_A23_M1A13_1")
				(number "G19")
			)
			(pin bidirectional line
				(at 35.56 57.15 180)
				(length 7.62)
				(name "IO_L29N_A22_M1A14_1")
				(number "F20")
			)
			(pin bidirectional line
				(at 35.56 54.61 180)
				(length 7.62)
				(name "IO_L30P_A21_M1RESET_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 35.56 52.07 180)
				(length 7.62)
				(name "IO_L30N_A20_M1A11_1")
				(number "H19")
			)
			(pin bidirectional line
				(at 35.56 49.53 180)
				(length 7.62)
				(name "IO_L31P_A19_M1CKE_1")
				(number "F21")
			)
			(pin bidirectional line
				(at 35.56 46.99 180)
				(length 7.62)
				(name "IO_L31N_A18_M1A12_1")
				(number "F22")
			)
			(pin bidirectional line
				(at 35.56 44.45 180)
				(length 7.62)
				(name "IO_L32P_A17_M1A8_1")
				(number "E20")
			)
			(pin bidirectional line
				(at 35.56 41.91 180)
				(length 7.62)
				(name "IO_L32N_A16_M1A9_1")
				(number "E22")
			)
			(pin bidirectional line
				(at 35.56 39.37 180)
				(length 7.62)
				(name "IO_L33P_A15_M1A10_1")
				(number "J19")
			)
			(pin bidirectional line
				(at 35.56 36.83 180)
				(length 7.62)
				(name "IO_L33N_A14_M1A4_1")
				(number "H20")
			)
			(pin bidirectional line
				(at 35.56 34.29 180)
				(length 7.62)
				(name "IO_L34P_A13_M1WE_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 35.56 31.75 180)
				(length 7.62)
				(name "IO_L34N_A12_M1BA2_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 35.56 29.21 180)
				(length 7.62)
				(name "IO_L35P_A11_M1A7_1")
				(number "G20")
			)
			(pin bidirectional line
				(at 35.56 26.67 180)
				(length 7.62)
				(name "IO_L35N_A10_M1A2_1")
				(number "G22")
			)
			(pin input line
				(at 35.56 24.13 180)
				(length 7.62)
				(name "IO_L36P_A9_M1BA0_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 35.56 21.59 180)
				(length 7.62)
				(name "IO_L36N_A8_M1BA1_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 35.56 19.05 180)
				(length 7.62)
				(name "IO_L37P_A7_M1A0_1")
				(number "H21")
			)
			(pin bidirectional line
				(at 35.56 16.51 180)
				(length 7.62)
				(name "IO_L37N_A6_M1A1_1")
				(number "H22")
			)
			(pin bidirectional line
				(at 35.56 13.97 180)
				(length 7.62)
				(name "IO_L38P_A5_M1CLK_1")
				(number "K20")
			)
			(pin bidirectional line
				(at 35.56 11.43 180)
				(length 7.62)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 35.56 8.89 180)
				(length 7.62)
				(name "IO_L39P_M1A3_1")
				(number "J20")
			)
			(pin bidirectional line
				(at 35.56 6.35 180)
				(length 7.62)
				(name "IO_L39N_M1ODT_1")
				(number "J22")
			)
			(pin bidirectional line
				(at 35.56 3.81 180)
				(length 7.62)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "M20")
			)
			(pin bidirectional line
				(at 35.56 1.27 180)
				(length 7.62)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 35.56 -1.27 180)
				(length 7.62)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "K21")
			)
			(pin bidirectional line
				(at 35.56 -3.81 180)
				(length 7.62)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "K22")
			)
			(pin bidirectional line
				(at 35.56 -6.35 180)
				(length 7.62)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 35.56 -8.89 180)
				(length 7.62)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 35.56 -11.43 180)
				(length 7.62)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "L20")
			)
			(pin bidirectional line
				(at 35.56 -13.97 180)
				(length 7.62)
				(name "IO_L43N_CLK4_M1DQ5_1")
				(number "L22")
			)
			(pin bidirectional line
				(at 35.56 -16.51 180)
				(length 7.62)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 35.56 -19.05 180)
				(length 7.62)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "M22")
			)
			(pin bidirectional line
				(at 35.56 -21.59 180)
				(length 7.62)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 35.56 -24.13 180)
				(length 7.62)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 35.56 -26.67 180)
				(length 7.62)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 35.56 -29.21 180)
				(length 7.62)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 35.56 -31.75 180)
				(length 7.62)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 35.56 -34.29 180)
				(length 7.62)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 35.56 -36.83 180)
				(length 7.62)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "T21")
			)
			(pin bidirectional line
				(at 35.56 -39.37 180)
				(length 7.62)
				(name "IO_L48N_M1DQ9_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 35.56 -41.91 180)
				(length 7.62)
				(name "IO_L49P_M1DQ10_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 35.56 -44.45 180)
				(length 7.62)
				(name "IO_L49N_M1DQ11_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 35.56 -46.99 180)
				(length 7.62)
				(name "IO_L50P_M1UDQS_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 35.56 -49.53 180)
				(length 7.62)
				(name "IO_L50N_M1UDQSN_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 35.56 -52.07 180)
				(length 7.62)
				(name "IO_L51P_M1DQ12_1")
				(number "W20")
			)
			(pin bidirectional line
				(at 35.56 -54.61 180)
				(length 7.62)
				(name "IO_L51N_M1DQ13_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 35.56 -57.15 180)
				(length 7.62)
				(name "IO_L52P_M1DQ14_1")
				(number "Y21")
			)
			(pin bidirectional line
				(at 35.56 -59.69 180)
				(length 7.62)
				(name "IO_L52N_M1DQ15_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at 35.56 -62.23 180)
				(length 7.62)
				(name "IO_L53P_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 35.56 -64.77 180)
				(length 7.62)
				(name "IO_L53N_VREF_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 35.56 -67.31 180)
				(length 7.62)
				(name "IO_L59P_1")
				(number "U19")
			)
			(pin bidirectional line
				(at 35.56 -69.85 180)
				(length 7.62)
				(name "IO_L59N_1")
				(number "T20")
			)
			(pin bidirectional line
				(at 35.56 -72.39 180)
				(length 7.62)
				(name "IO_L60P_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 35.56 -74.93 180)
				(length 7.62)
				(name "IO_L60N_1")
				(number "P16")
			)
			(pin bidirectional line
				(at 35.56 -77.47 180)
				(length 7.62)
				(name "IO_L61P_1")
				(number "M17")
			)
			(pin bidirectional line
				(at 35.56 -80.01 180)
				(length 7.62)
				(name "IO_L61N_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 35.56 -82.55 180)
				(length 7.62)
				(name "IO_L74P_AWAKE_1")
				(number "V19")
			)
			(pin bidirectional line
				(at 35.56 -85.09 180)
				(length 7.62)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "V20")
			)
		)
		(symbol "XC6SLX25T-BG484_2_1"
			(pin input line
				(at -38.1 99.06 0)
				(length 7.62)
				(name "SUSPEND")
				(number "AA22")
			)
			(pin input line
				(at -38.1 96.52 0)
				(length 7.62)
				(name "CMPCS_B_2")
				(number "V18")
			)
			(pin bidirectional line
				(at -38.1 93.98 0)
				(length 7.62)
				(name "DONE_2")
				(number "AB21")
			)
			(pin input line
				(at -38.1 88.9 0)
				(length 7.62)
				(name "PROGRAM_B_2")
				(number "AB2")
			)
			(pin bidirectional line
				(at -38.1 83.82 0)
				(length 7.62)
				(name "IO_L1P_CCLK_2")
				(number "Y20")
			)
			(pin bidirectional line
				(at -38.1 81.28 0)
				(length 7.62)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "AA21")
			)
			(pin bidirectional line
				(at -38.1 78.74 0)
				(length 7.62)
				(name "IO_L2P_CMPCLK_2")
				(number "V17")
			)
			(pin bidirectional line
				(at -38.1 76.2 0)
				(length 7.62)
				(name "IO_L2N_CMPMOSI_2")
				(number "W18")
			)
			(pin bidirectional line
				(at -38.1 73.66 0)
				(length 7.62)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "AA20")
			)
			(pin bidirectional line
				(at -38.1 71.12 0)
				(length 7.62)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AB20")
			)
			(pin bidirectional line
				(at -38.1 68.58 0)
				(length 7.62)
				(name "IO_L5P_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -38.1 66.04 0)
				(length 7.62)
				(name "IO_L5N_2")
				(number "Y18")
			)
			(pin bidirectional line
				(at -38.1 63.5 0)
				(length 7.62)
				(name "IO_L6P_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -38.1 60.96 0)
				(length 7.62)
				(name "IO_L6N_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -38.1 58.42 0)
				(length 7.62)
				(name "IO_L12P_D1_MISO2_2")
				(number "R13")
			)
			(pin bidirectional line
				(at -38.1 55.88 0)
				(length 7.62)
				(name "IO_L12N_D2_MISO3_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -38.1 53.34 0)
				(length 7.62)
				(name "IO_L13P_M1_2")
				(number "Y19")
			)
			(pin bidirectional line
				(at -38.1 50.8 0)
				(length 7.62)
				(name "IO_L13N_D10_2")
				(number "AB19")
			)
			(pin bidirectional line
				(at -38.1 48.26 0)
				(length 7.62)
				(name "IO_L14P_D11_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -38.1 45.72 0)
				(length 7.62)
				(name "IO_L14N_D12_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -38.1 43.18 0)
				(length 7.62)
				(name "IO_L15P_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -38.1 40.64 0)
				(length 7.62)
				(name "IO_L15N_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -38.1 38.1 0)
				(length 7.62)
				(name "IO_L16P_2")
				(number "U14")
			)
			(pin bidirectional line
				(at -38.1 35.56 0)
				(length 7.62)
				(name "IO_L16N_VREF_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -38.1 33.02 0)
				(length 7.62)
				(name "IO_L17P_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -38.1 30.48 0)
				(length 7.62)
				(name "IO_L17N_2")
				(number "W15")
			)
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 7.62)
				(name "IO_L18P_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 7.62)
				(name "IO_L18N_2")
				(number "W13")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 7.62)
				(name "IO_L19P_2")
				(number "AA16")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 7.62)
				(name "IO_L19N_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 7.62)
				(name "IO_L20P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 7.62)
				(name "IO_L20N_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 7.62)
				(name "IO_L21P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 7.62)
				(name "IO_L21N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -38.1 7.62 0)
				(length 7.62)
				(name "IO_L29P_GCLK3_2")
				(number "T12")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 7.62)
				(name "IO_L29N_GCLK2_2")
				(number "U12")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 7.62)
				(name "IO_L30P_GCLK1_D13_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 7.62)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 7.62)
				(name "IO_L31P_GCLK31_D14_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 7.62)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AB12")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 7.62)
				(name "IO_L32P_GCLK29_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 7.62)
				(name "IO_L32N_GCLK28_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 7.62)
				(name "IO_L40P_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 7.62)
				(name "IO_L40N_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 7.62)
				(name "IO_L41P_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 7.62)
				(name "IO_L41N_VREF_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 7.62)
				(name "IO_L42P_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 7.62)
				(name "IO_L42N_2")
				(number "W11")
			)
			(pin bidirectional line
				(at -38.1 -27.94 0)
				(length 7.62)
				(name "IO_L43P_2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -38.1 -30.48 0)
				(length 7.62)
				(name "IO_L43N_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -38.1 -33.02 0)
				(length 7.62)
				(name "IO_L44P_2")
				(number "W10")
			)
			(pin bidirectional line
				(at -38.1 -35.56 0)
				(length 7.62)
				(name "IO_L44N_2")
				(number "Y10")
			)
			(pin bidirectional line
				(at -38.1 -38.1 0)
				(length 7.62)
				(name "IO_L45P_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at -38.1 -40.64 0)
				(length 7.62)
				(name "IO_L45N_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at -38.1 -43.18 0)
				(length 7.62)
				(name "IO_L46P_2")
				(number "T10")
			)
			(pin bidirectional line
				(at -38.1 -45.72 0)
				(length 7.62)
				(name "IO_L46N_2")
				(number "U10")
			)
			(pin bidirectional line
				(at -38.1 -48.26 0)
				(length 7.62)
				(name "IO_L47P_2")
				(number "Y7")
			)
			(pin bidirectional line
				(at -38.1 -50.8 0)
				(length 7.62)
				(name "IO_L47N_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at -38.1 -53.34 0)
				(length 7.62)
				(name "IO_L48P_D7_2")
				(number "W9")
			)
			(pin bidirectional line
				(at -38.1 -55.88 0)
				(length 7.62)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "Y8")
			)
			(pin bidirectional line
				(at -38.1 -58.42 0)
				(length 7.62)
				(name "IO_L49P_D3_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -38.1 -60.96 0)
				(length 7.62)
				(name "IO_L49N_D4_2")
				(number "AB6")
			)
			(pin bidirectional line
				(at -38.1 -63.5 0)
				(length 7.62)
				(name "IO_L50P_2")
				(number "U9")
			)
			(pin bidirectional line
				(at -38.1 -66.04 0)
				(length 7.62)
				(name "IO_L50N_2")
				(number "V9")
			)
			(pin bidirectional line
				(at -38.1 -68.58 0)
				(length 7.62)
				(name "IO_L57P_2")
				(number "T8")
			)
			(pin bidirectional line
				(at -38.1 -71.12 0)
				(length 7.62)
				(name "IO_L57N_2")
				(number "U8")
			)
			(pin bidirectional line
				(at -38.1 -73.66 0)
				(length 7.62)
				(name "IO_L58P_2")
				(number "V7")
			)
			(pin bidirectional line
				(at -38.1 -76.2 0)
				(length 7.62)
				(name "IO_L58N_2")
				(number "W8")
			)
			(pin bidirectional line
				(at -38.1 -78.74 0)
				(length 7.62)
				(name "IO_L59P_2")
				(number "R9")
			)
			(pin bidirectional line
				(at -38.1 -81.28 0)
				(length 7.62)
				(name "IO_L59N_2")
				(number "R8")
			)
			(pin bidirectional line
				(at -38.1 -83.82 0)
				(length 7.62)
				(name "IO_L60P_2")
				(number "W6")
			)
			(pin bidirectional line
				(at -38.1 -86.36 0)
				(length 7.62)
				(name "IO_L60N_2")
				(number "Y6")
			)
			(pin bidirectional line
				(at -38.1 -88.9 0)
				(length 7.62)
				(name "IO_L62P_D5_2")
				(number "Y5")
			)
			(pin bidirectional line
				(at -38.1 -91.44 0)
				(length 7.62)
				(name "IO_L62N_D6_2")
				(number "AB5")
			)
			(pin bidirectional line
				(at -38.1 -93.98 0)
				(length 7.62)
				(name "IO_L63P_2")
				(number "AA4")
			)
			(pin bidirectional line
				(at -38.1 -96.52 0)
				(length 7.62)
				(name "IO_L63N_2")
				(number "AB4")
			)
			(pin bidirectional line
				(at -38.1 -99.06 0)
				(length 7.62)
				(name "IO_L64P_D8_2")
				(number "T7")
			)
			(pin bidirectional line
				(at -38.1 -101.6 0)
				(length 7.62)
				(name "IO_L64N_D9_2")
				(number "U6")
			)
			(pin bidirectional line
				(at -38.1 -104.14 0)
				(length 7.62)
				(name "IO_L65P_INIT_B_2")
				(number "Y4")
			)
			(pin bidirectional line
				(at -38.1 -106.68 0)
				(length 7.62)
				(name "IO_L65N_CSO_B_2")
				(number "AA3")
			)
			(pin power_in line
				(at -27.94 115.57 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA11")
			)
			(pin power_in line
				(at -25.4 115.57 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA15")
			)
			(pin power_in line
				(at -22.86 115.57 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA19")
			)
			(pin power_in line
				(at -20.32 115.57 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA7")
			)
			(pin power_in line
				(at -17.78 115.57 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AB3")
			)
			(pin power_in line
				(at -15.24 115.57 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T13")
			)
			(pin power_in line
				(at -12.7 115.57 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T9")
			)
			(pin power_in line
				(at -10.16 115.57 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V12")
			)
			(pin power_in line
				(at -7.62 115.57 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V16")
			)
			(pin power_in line
				(at -5.08 115.57 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V8")
			)
			(pin power_in line
				(at -2.54 115.57 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W5")
			)
			(pin power_in line
				(at 5.08 115.57 270)
				(length 6.35)
				(name "VCCO_3")
				(number "C2")
			)
			(pin power_in line
				(at 7.62 115.57 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F4")
			)
			(pin power_in line
				(at 10.16 115.57 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G2")
			)
			(pin power_in line
				(at 12.7 115.57 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 15.24 115.57 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L2")
			)
			(pin power_in line
				(at 17.78 115.57 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L7")
			)
			(pin power_in line
				(at 20.32 115.57 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N5")
			)
			(pin power_in line
				(at 22.86 115.57 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 25.4 115.57 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U5")
			)
			(pin power_in line
				(at 27.94 115.57 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 38.1 63.5 180)
				(length 7.62)
				(name "IO_L1P_3")
				(number "R7")
			)
			(pin bidirectional line
				(at 38.1 60.96 180)
				(length 7.62)
				(name "IO_L1N_VREF_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 38.1 58.42 180)
				(length 7.62)
				(name "IO_L2P_3")
				(number "W4")
			)
			(pin bidirectional line
				(at 38.1 55.88 180)
				(length 7.62)
				(name "IO_L2N_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 38.1 53.34 180)
				(length 7.62)
				(name "IO_L9P_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 38.1 50.8 180)
				(length 7.62)
				(name "IO_L9N_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 38.1 48.26 180)
				(length 7.62)
				(name "IO_L10P_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 38.1 45.72 180)
				(length 7.62)
				(name "IO_L10N_3")
				(number "AA1")
			)
			(pin bidirectional line
				(at 38.1 43.18 180)
				(length 7.62)
				(name "IO_L31P_3")
				(number "M7")
			)
			(pin bidirectional line
				(at 38.1 40.64 180)
				(length 7.62)
				(name "IO_L31N_VREF_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 38.1 38.1 180)
				(length 7.62)
				(name "IO_L32P_M3DQ14_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 38.1 35.56 180)
				(length 7.62)
				(name "IO_L32N_M3DQ15_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 38.1 33.02 180)
				(length 7.62)
				(name "IO_L33P_M3DQ12_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 38.1 30.48 180)
				(length 7.62)
				(name "IO_L33N_M3DQ13_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 7.62)
				(name "IO_L34P_M3UDQS_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 7.62)
				(name "IO_L34N_M3UDQSN_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 7.62)
				(name "IO_L35P_M3DQ10_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 7.62)
				(name "IO_L35N_M3DQ11_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 7.62)
				(name "IO_L36P_M3DQ8_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 7.62)
				(name "IO_L36N_M3DQ9_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 7.62)
				(name "IO_L37P_M3DQ0_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 7.62)
				(name "IO_L37N_M3DQ1_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 7.62)
				(name "IO_L38P_M3DQ2_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 7.62)
				(name "IO_L38N_M3DQ3_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 7.62)
				(name "IO_L39P_M3LDQS_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 7.62)
				(name "IO_L39N_M3LDQSN_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 7.62)
				(name "IO_L40P_M3DQ6_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 7.62)
				(name "IO_L40N_M3DQ7_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 7.62)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 7.62)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 7.62)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 7.62)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 7.62)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 7.62)
				(name "IO_L43N_GCLK22_TRDY2_M3CASN_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 7.62)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 7.62)
				(name "IO_L44N_GCLK207_M3A6_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 7.62)
				(name "IO_L45P_M3A3_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 7.62)
				(name "IO_L45N_M3ODT_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 38.1 -33.02 180)
				(length 7.62)
				(name "IO_L46P_M3CLK_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 38.1 -35.56 180)
				(length 7.62)
				(name "IO_L46N_M3CLKN_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 38.1 -38.1 180)
				(length 7.62)
				(name "IO_L47P_M3A0_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 38.1 -40.64 180)
				(length 7.62)
				(name "IO_L47N_M3A1_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 38.1 -43.18 180)
				(length 7.62)
				(name "IO_L48P_M3BA0_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 38.1 -45.72 180)
				(length 7.62)
				(name "IO_L48N_M3BA1_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 38.1 -48.26 180)
				(length 7.62)
				(name "IO_L49P_M3A7_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 38.1 -50.8 180)
				(length 7.62)
				(name "IO_L49N_M3A2_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 38.1 -53.34 180)
				(length 7.62)
				(name "IO_L50P_M3WE_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 38.1 -55.88 180)
				(length 7.62)
				(name "IO_L50N_M3BA2_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 38.1 -58.42 180)
				(length 7.62)
				(name "IO_L51P_M3A10_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 38.1 -60.96 180)
				(length 7.62)
				(name "IO_L51N_M3A4_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 38.1 -63.5 180)
				(length 7.62)
				(name "IO_L52P_M3A8_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 38.1 -66.04 180)
				(length 7.62)
				(name "IO_L52N_M3A9_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 38.1 -68.58 180)
				(length 7.62)
				(name "IO_L53P_M3CKE_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 38.1 -71.12 180)
				(length 7.62)
				(name "IO_L53N_M3A12_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 38.1 -73.66 180)
				(length 7.62)
				(name "IO_L54P_M3RESET_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 38.1 -76.2 180)
				(length 7.62)
				(name "IO_L54N_M3A11_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 38.1 -78.74 180)
				(length 7.62)
				(name "IO_L55P_M3A13_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 38.1 -81.28 180)
				(length 7.62)
				(name "IO_L55N_M3A14_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 38.1 -83.82 180)
				(length 7.62)
				(name "IO_L59P_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 38.1 -86.36 180)
				(length 7.62)
				(name "IO_L59N_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 38.1 -88.9 180)
				(length 7.62)
				(name "IO_L60P_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 38.1 -91.44 180)
				(length 7.62)
				(name "IO_L60N_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 38.1 -93.98 180)
				(length 7.62)
				(name "IO_L83P_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 38.1 -96.52 180)
				(length 7.62)
				(name "IO_L83N_VREF_3")
				(number "B1")
			)
		)
		(symbol "XC6SLX25T-BG484_3_1"
			(pin power_in line
				(at -16.51 72.39 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F11")
			)
			(pin power_in line
				(at -16.51 69.85 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G12")
			)
			(pin power_in line
				(at -16.51 67.31 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H15")
			)
			(pin power_in line
				(at -16.51 64.77 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H9")
			)
			(pin power_in line
				(at -16.51 62.23 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -16.51 59.69 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L8")
			)
			(pin power_in line
				(at -16.51 57.15 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M15")
			)
			(pin power_in line
				(at -16.51 54.61 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N8")
			)
			(pin power_in line
				(at -16.51 52.07 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R10")
			)
			(pin power_in line
				(at -16.51 49.53 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R12")
			)
			(pin power_in line
				(at -16.51 46.99 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R6")
			)
			(pin power_in line
				(at -16.51 44.45 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -16.51 41.91 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -16.51 19.05 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -16.51 16.51 0)
				(length 6.35)
				(name "GND")
				(number "J13")
			)
			(pin power_in line
				(at -16.51 13.97 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at -16.51 11.43 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -16.51 8.89 0)
				(length 6.35)
				(name "GND")
				(number "J21")
			)
			(pin power_in line
				(at -16.51 6.35 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -16.51 3.81 0)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at -16.51 1.27 0)
				(length 6.35)
				(name "GND")
				(number "K12")
			)
			(pin power_in line
				(at -16.51 -1.27 0)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at -16.51 -3.81 0)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at -16.51 -6.35 0)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at -16.51 -8.89 0)
				(length 6.35)
				(name "GND")
				(number "L18")
			)
			(pin power_in line
				(at -16.51 -11.43 0)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at -16.51 -13.97 0)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at -16.51 -16.51 0)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at -16.51 -19.05 0)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at -16.51 -21.59 0)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at -16.51 -24.13 0)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at -16.51 -26.67 0)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at -16.51 -29.21 0)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at -16.51 -31.75 0)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at -16.51 -34.29 0)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at -16.51 -36.83 0)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at -16.51 -39.37 0)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at -16.51 -41.91 0)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at -16.51 -44.45 0)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at -16.51 -46.99 0)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at -16.51 -49.53 0)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at -16.51 -52.07 0)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at -16.51 -54.61 0)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at -16.51 -57.15 0)
				(length 6.35)
				(name "GND")
				(number "U7")
			)
			(pin power_in line
				(at -16.51 -59.69 0)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at -16.51 -62.23 0)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at -16.51 -64.77 0)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at -16.51 -67.31 0)
				(length 6.35)
				(name "GND")
				(number "W16")
			)
			(pin power_in line
				(at -16.51 -69.85 0)
				(length 6.35)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at -16.51 -72.39 0)
				(length 6.35)
				(name "GND")
				(number "W7")
			)
			(pin power_in line
				(at 16.51 72.39 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 16.51 69.85 180)
				(length 6.35)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 16.51 67.31 180)
				(length 6.35)
				(name "VCCINT")
				(number "J14")
			)
			(pin power_in line
				(at 16.51 64.77 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 16.51 62.23 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 16.51 59.69 180)
				(length 6.35)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 16.51 57.15 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 16.51 54.61 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 16.51 52.07 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 16.51 49.53 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 16.51 46.99 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 16.51 44.45 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 16.51 41.91 180)
				(length 6.35)
				(name "VCCINT")
				(number "M9")
			)
			(pin power_in line
				(at 16.51 39.37 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 16.51 36.83 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 16.51 34.29 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 16.51 31.75 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 16.51 29.21 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 16.51 26.67 180)
				(length 6.35)
				(name "VCCINT")
				(number "P9")
			)
			(pin power_in line
				(at 16.51 24.13 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 16.51 11.43 180)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at 16.51 8.89 180)
				(length 6.35)
				(name "GND")
				(number "A11")
			)
			(pin power_in line
				(at 16.51 6.35 180)
				(length 6.35)
				(name "GND")
				(number "A13")
			)
			(pin power_in line
				(at 16.51 3.81 180)
				(length 6.35)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at 16.51 1.27 180)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at 16.51 -1.27 180)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 16.51 -3.81 180)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at 16.51 -6.35 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 16.51 -8.89 180)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at 16.51 -11.43 180)
				(length 6.35)
				(name "GND")
				(number "AB1")
			)
			(pin power_in line
				(at 16.51 -13.97 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
			(pin power_in line
				(at 16.51 -16.51 180)
				(length 6.35)
				(name "GND")
				(number "B11")
			)
			(pin power_in line
				(at 16.51 -19.05 180)
				(length 6.35)
				(name "GND")
				(number "B15")
			)
			(pin power_in line
				(at 16.51 -21.59 180)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at 16.51 -24.13 180)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at 16.51 -26.67 180)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at 16.51 -29.21 180)
				(length 6.35)
				(name "GND")
				(number "C12")
			)
			(pin power_in line
				(at 16.51 -31.75 180)
				(length 6.35)
				(name "GND")
				(number "C14")
			)
			(pin power_in line
				(at 16.51 -34.29 180)
				(length 6.35)
				(name "GND")
				(number "C16")
			)
			(pin power_in line
				(at 16.51 -36.83 180)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at 16.51 -39.37 180)
				(length 6.35)
				(name "GND")
				(number "C8")
			)
			(pin power_in line
				(at 16.51 -41.91 180)
				(length 6.35)
				(name "GND")
				(number "D10")
			)
			(pin power_in line
				(at 16.51 -44.45 180)
				(length 6.35)
				(name "GND")
				(number "D16")
			)
			(pin power_in line
				(at 16.51 -46.99 180)
				(length 6.35)
				(name "GND")
				(number "D6")
			)
			(pin power_in line
				(at 16.51 -49.53 180)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at 16.51 -52.07 180)
				(length 6.35)
				(name "GND")
				(number "E14")
			)
			(pin power_in line
				(at 16.51 -54.61 180)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at 16.51 -57.15 180)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at 16.51 -59.69 180)
				(length 6.35)
				(name "GND")
				(number "E21")
			)
			(pin power_in line
				(at 16.51 -62.23 180)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at 16.51 -64.77 180)
				(length 6.35)
				(name "GND")
				(number "F13")
			)
			(pin power_in line
				(at 16.51 -67.31 180)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at 16.51 -69.85 180)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at 16.51 -72.39 180)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XCV150_BG352"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XCV150_BG352"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.xilinx.com/support/documentation/data_sheets/ds003.pdf"
			(at 0 0 0)
		)
		(property "Description" "Virtex FPGA"
			(at 0 0 0)
		)
		(property "ki_keywords" "field programmable gate array"
			(at 0 0 0)
		)
		(symbol "XCV150_BG352_0_1")
		(symbol "XCV150_BG352_1_1"
			(pin passive line
				(at -35.56 99.06 0)
				(length 7.62)
				(name "TMS")
				(number "D23")
			)
			(pin passive line
				(at -35.56 97.79 0)
				(length 7.62)
				(name "TDI")
				(number "B3")
			)
			(pin passive line
				(at -35.56 96.52 0)
				(length 7.62)
				(name "TCK")
				(number "C24")
			)
			(pin passive line
				(at -35.56 95.25 0)
				(length 7.62)
				(name "TDO")
				(number "D4")
			)
			(pin input line
				(at -35.56 92.71 0)
				(length 7.62)
				(name "M0")
				(number "AD24")
			)
			(pin input line
				(at -35.56 91.44 0)
				(length 7.62)
				(name "M1")
				(number "AB23")
			)
			(pin input line
				(at -35.56 90.17 0)
				(length 7.62)
				(name "M2")
				(number "AC23")
			)
			(pin input line
				(at -35.56 86.36 0)
				(length 7.62)
				(name "~{PROGRAM}")
				(number "AC4")
			)
			(pin bidirectional line
				(at -35.56 85.09 0)
				(length 7.62)
				(name "DONE")
				(number "AD3")
			)
			(pin bidirectional line
				(at -35.56 83.82 0)
				(length 7.62)
				(name "~{INIT}")
				(number "AD2")
			)
			(pin output line
				(at -35.56 82.55 0)
				(length 7.62)
				(name "BUSY/DOUT")
				(number "E4")
			)
			(pin bidirectional clock
				(at -35.56 81.28 0)
				(length 7.62)
				(name "CCLK")
				(number "C3")
			)
			(pin input line
				(at -35.56 77.47 0)
				(length 7.62)
				(name "~{WRITE}")
				(number "D5")
			)
			(pin input line
				(at -35.56 74.93 0)
				(length 7.62)
				(name "~{CS}")
				(number "C4")
			)
			(pin power_in line
				(at -35.56 71.12 0)
				(length 7.62)
				(name "VCCO")
				(number "A17")
			)
			(pin power_in line
				(at -35.56 69.85 0)
				(length 7.62)
				(name "VCCO")
				(number "B25")
			)
			(pin power_in line
				(at -35.56 68.58 0)
				(length 7.62)
				(name "VCCO")
				(number "D19")
			)
			(pin bidirectional line
				(at -35.56 67.31 0)
				(length 7.62)
				(name "IO0A15")
				(number "A15")
			)
			(pin bidirectional line
				(at -35.56 66.04 0)
				(length 7.62)
				(name "IOR0A16")
				(number "A16")
			)
			(pin bidirectional line
				(at -35.56 64.77 0)
				(length 7.62)
				(name "IO0A18")
				(number "A18")
			)
			(pin bidirectional line
				(at -35.56 63.5 0)
				(length 7.62)
				(name "IO0A21")
				(number "A21")
			)
			(pin bidirectional line
				(at -35.56 62.23 0)
				(length 7.62)
				(name "IO0A23")
				(number "A23")
			)
			(pin bidirectional line
				(at -35.56 60.96 0)
				(length 7.62)
				(name "IO0A24")
				(number "A24")
			)
			(pin bidirectional line
				(at -35.56 59.69 0)
				(length 7.62)
				(name "IO0B15")
				(number "B15")
			)
			(pin bidirectional line
				(at -35.56 58.42 0)
				(length 7.62)
				(name "IO0B17")
				(number "B17")
			)
			(pin bidirectional line
				(at -35.56 57.15 0)
				(length 7.62)
				(name "IO0B18")
				(number "B18")
			)
			(pin bidirectional line
				(at -35.56 55.88 0)
				(length 7.62)
				(name "IO0B19")
				(number "B19")
			)
			(pin bidirectional line
				(at -35.56 54.61 0)
				(length 7.62)
				(name "IO0B20")
				(number "B20")
			)
			(pin bidirectional line
				(at -35.56 53.34 0)
				(length 7.62)
				(name "IO0B21")
				(number "B21")
			)
			(pin bidirectional line
				(at -35.56 52.07 0)
				(length 7.62)
				(name "IO0B22")
				(number "B22")
			)
			(pin bidirectional line
				(at -35.56 50.8 0)
				(length 7.62)
				(name "IO0B23")
				(number "B23")
			)
			(pin bidirectional line
				(at -35.56 49.53 0)
				(length 7.62)
				(name "IO0B24")
				(number "B24")
			)
			(pin bidirectional line
				(at -35.56 48.26 0)
				(length 7.62)
				(name "IO0C15")
				(number "C15")
			)
			(pin bidirectional line
				(at -35.56 46.99 0)
				(length 7.62)
				(name "IO0C16")
				(number "C16")
			)
			(pin bidirectional line
				(at -35.56 45.72 0)
				(length 7.62)
				(name "IO0C17")
				(number "C17")
			)
			(pin bidirectional line
				(at -35.56 44.45 0)
				(length 7.62)
				(name "IO0C18")
				(number "C18")
			)
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 7.62)
				(name "IOR0C19")
				(number "C19")
			)
			(pin bidirectional line
				(at -35.56 41.91 0)
				(length 7.62)
				(name "IO0C20")
				(number "C20")
			)
			(pin bidirectional line
				(at -35.56 40.64 0)
				(length 7.62)
				(name "IOR0C21")
				(number "C21")
			)
			(pin bidirectional line
				(at -35.56 39.37 0)
				(length 7.62)
				(name "IO0C22")
				(number "C22")
			)
			(pin bidirectional line
				(at -35.56 38.1 0)
				(length 7.62)
				(name "IO0C23")
				(number "C23")
			)
			(pin input line
				(at -35.56 36.83 0)
				(length 7.62)
				(name "GCK3")
				(number "D14")
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 7.62)
				(name "IO0D15")
				(number "D15")
			)
			(pin bidirectional line
				(at -35.56 34.29 0)
				(length 7.62)
				(name "IO0D16")
				(number "D16")
			)
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 7.62)
				(name "IO0D17")
				(number "D17")
			)
			(pin bidirectional line
				(at -35.56 31.75 0)
				(length 7.62)
				(name "IO0D18")
				(number "D18")
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 7.62)
				(name "IO0D20")
				(number "D20")
			)
			(pin bidirectional line
				(at -35.56 29.21 0)
				(length 7.62)
				(name "IO0D21")
				(number "D21")
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 7.62)
				(name "IO0D22")
				(number "D22")
			)
			(pin power_in line
				(at -35.56 25.4 0)
				(length 7.62)
				(name "VCCO")
				(number "A10")
			)
			(pin power_in line
				(at -35.56 24.13 0)
				(length 7.62)
				(name "VCCO")
				(number "D7")
			)
			(pin power_in line
				(at -35.56 22.86 0)
				(length 7.62)
				(name "VCCO")
				(number "D13")
			)
			(pin bidirectional line
				(at -35.56 21.59 0)
				(length 7.62)
				(name "IO1A3")
				(number "A3")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 7.62)
				(name "IO1A4")
				(number "A4")
			)
			(pin bidirectional line
				(at -35.56 19.05 0)
				(length 7.62)
				(name "IO1A6")
				(number "A6")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 7.62)
				(name "IO1A7")
				(number "A7")
			)
			(pin bidirectional line
				(at -35.56 16.51 0)
				(length 7.62)
				(name "IO1A9")
				(number "A9")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 7.62)
				(name "IO1A11")
				(number "A11")
			)
			(pin bidirectional line
				(at -35.56 13.97 0)
				(length 7.62)
				(name "IO1A12")
				(number "A12")
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 7.62)
				(name "IO1A13")
				(number "A13")
			)
			(pin bidirectional line
				(at -35.56 11.43 0)
				(length 7.62)
				(name "IO1B4")
				(number "B4")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 7.62)
				(name "IO1B5")
				(number "B5")
			)
			(pin bidirectional line
				(at -35.56 8.89 0)
				(length 7.62)
				(name "IOR1B6")
				(number "B6")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 7.62)
				(name "IO1B7")
				(number "B7")
			)
			(pin bidirectional line
				(at -35.56 6.35 0)
				(length 7.62)
				(name "IO1B8")
				(number "B8")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 7.62)
				(name "IO1B9")
				(number "B9")
			)
			(pin bidirectional line
				(at -35.56 3.81 0)
				(length 7.62)
				(name "IO1B10")
				(number "B10")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 7.62)
				(name "IO1B11")
				(number "B11")
			)
			(pin bidirectional line
				(at -35.56 1.27 0)
				(length 7.62)
				(name "IO1B12")
				(number "B12")
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 7.62)
				(name "IO1B13")
				(number "B13")
			)
			(pin input line
				(at -35.56 -1.27 0)
				(length 7.62)
				(name "GCK2")
				(number "B14")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 7.62)
				(name "IO1C5")
				(number "C5")
			)
			(pin bidirectional line
				(at -35.56 -3.81 0)
				(length 7.62)
				(name "IO1C6")
				(number "C6")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 7.62)
				(name "IO1C7")
				(number "C7")
			)
			(pin bidirectional line
				(at -35.56 -6.35 0)
				(length 7.62)
				(name "IO1C8")
				(number "C8")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 7.62)
				(name "IOR1C9")
				(number "C9")
			)
			(pin bidirectional line
				(at -35.56 -8.89 0)
				(length 7.62)
				(name "IO1C10")
				(number "C10")
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 7.62)
				(name "IO1C11")
				(number "C11")
			)
			(pin bidirectional line
				(at -35.56 -11.43 0)
				(length 7.62)
				(name "IOR1C12")
				(number "C12")
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 7.62)
				(name "IO1C13")
				(number "C13")
			)
			(pin bidirectional line
				(at -35.56 -13.97 0)
				(length 7.62)
				(name "IO1D6")
				(number "D6")
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 7.62)
				(name "IO1D8")
				(number "D8")
			)
			(pin bidirectional line
				(at -35.56 -16.51 0)
				(length 7.62)
				(name "IO1D9")
				(number "D9")
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 7.62)
				(name "IO1D11")
				(number "D11")
			)
			(pin power_in line
				(at -35.56 -20.32 0)
				(length 7.62)
				(name "VCCO")
				(number "B2")
			)
			(pin power_in line
				(at -35.56 -21.59 0)
				(length 7.62)
				(name "VCCO")
				(number "H4")
			)
			(pin power_in line
				(at -35.56 -22.86 0)
				(length 7.62)
				(name "VCCO")
				(number "K1")
			)
			(pin bidirectional line
				(at -35.56 -24.13 0)
				(length 7.62)
				(name "IO2C1")
				(number "C1")
			)
			(pin bidirectional line
				(at -35.56 -25.4 0)
				(length 7.62)
				(name "IO2C2")
				(number "C2")
			)
			(pin bidirectional line
				(at -35.56 -26.67 0)
				(length 7.62)
				(name "IO2D1")
				(number "D1")
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 7.62)
				(name "IO2D2")
				(number "D2")
			)
			(pin bidirectional line
				(at -35.56 -29.21 0)
				(length 7.62)
				(name "IOR2E2")
				(number "E2")
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 7.62)
				(name "IO2E3")
				(number "E3")
			)
			(pin bidirectional line
				(at -35.56 -31.75 0)
				(length 7.62)
				(name "IO2F1")
				(number "F1")
			)
			(pin bidirectional line
				(at -35.56 -33.02 0)
				(length 7.62)
				(name "IO2F2")
				(number "F2")
			)
			(pin bidirectional line
				(at -35.56 -34.29 0)
				(length 7.62)
				(name "IO2F3")
				(number "F3")
			)
			(pin bidirectional line
				(at -35.56 -35.56 0)
				(length 7.62)
				(name "IO2F4")
				(number "F4")
			)
			(pin bidirectional line
				(at -35.56 -36.83 0)
				(length 7.62)
				(name "IO2G2")
				(number "G2")
			)
			(pin bidirectional line
				(at -35.56 -38.1 0)
				(length 7.62)
				(name "IO2G3")
				(number "G3")
			)
			(pin bidirectional line
				(at -35.56 -39.37 0)
				(length 7.62)
				(name "IO2G4")
				(number "G4")
			)
			(pin bidirectional line
				(at -35.56 -40.64 0)
				(length 7.62)
				(name "IOR2H2")
				(number "H2")
			)
			(pin bidirectional line
				(at -35.56 -41.91 0)
				(length 7.62)
				(name "IO2H3")
				(number "H3")
			)
			(pin bidirectional line
				(at -35.56 -43.18 0)
				(length 7.62)
				(name "IO2J1")
				(number "J1")
			)
			(pin bidirectional line
				(at -35.56 -44.45 0)
				(length 7.62)
				(name "IO2J2")
				(number "J2")
			)
			(pin bidirectional line
				(at -35.56 -45.72 0)
				(length 7.62)
				(name "IO2J4")
				(number "J4")
			)
			(pin bidirectional line
				(at -35.56 -46.99 0)
				(length 7.62)
				(name "IO2K2")
				(number "K2")
			)
			(pin bidirectional line
				(at -35.56 -48.26 0)
				(length 7.62)
				(name "IO2K3")
				(number "K3")
			)
			(pin bidirectional line
				(at -35.56 -49.53 0)
				(length 7.62)
				(name "IO2L2")
				(number "L2")
			)
			(pin bidirectional line
				(at -35.56 -50.8 0)
				(length 7.62)
				(name "IO2L3")
				(number "L3")
			)
			(pin bidirectional line
				(at -35.56 -52.07 0)
				(length 7.62)
				(name "IO2L4")
				(number "L4")
			)
			(pin bidirectional line
				(at -35.56 -53.34 0)
				(length 7.62)
				(name "IO2M1")
				(number "M1")
			)
			(pin bidirectional line
				(at -35.56 -54.61 0)
				(length 7.62)
				(name "IO2M2")
				(number "M2")
			)
			(pin bidirectional line
				(at -35.56 -55.88 0)
				(length 7.62)
				(name "IOR2M4")
				(number "M4")
			)
			(pin bidirectional line
				(at -35.56 -57.15 0)
				(length 7.62)
				(name "IO2N2")
				(number "N2")
			)
			(pin bidirectional line
				(at -35.56 -58.42 0)
				(length 7.62)
				(name "IO2N3")
				(number "N3")
			)
			(pin bidirectional line
				(at -35.56 -59.69 0)
				(length 7.62)
				(name "IO2N4")
				(number "N4")
			)
			(pin power_in line
				(at -35.56 -62.23 0)
				(length 7.62)
				(name "VCCO")
				(number "P4")
			)
			(pin power_in line
				(at -35.56 -63.5 0)
				(length 7.62)
				(name "VCCO")
				(number "U1")
			)
			(pin power_in line
				(at -35.56 -64.77 0)
				(length 7.62)
				(name "VCCO")
				(number "Y4")
			)
			(pin bidirectional line
				(at -35.56 -66.04 0)
				(length 7.62)
				(name "IO3P1")
				(number "P1")
			)
			(pin bidirectional line
				(at -35.56 -67.31 0)
				(length 7.62)
				(name "IO3P3")
				(number "P3")
			)
			(pin bidirectional line
				(at -35.56 -68.58 0)
				(length 7.62)
				(name "IO3R1")
				(number "R1")
			)
			(pin bidirectional line
				(at -35.56 -69.85 0)
				(length 7.62)
				(name "IO3R2")
				(number "R2")
			)
			(pin bidirectional line
				(at -35.56 -71.12 0)
				(length 7.62)
				(name "IOR3R4")
				(number "R4")
			)
			(pin bidirectional line
				(at -35.56 -72.39 0)
				(length 7.62)
				(name "IO3T2")
				(number "T2")
			)
			(pin bidirectional line
				(at -35.56 -73.66 0)
				(length 7.62)
				(name "IO3T3")
				(number "T3")
			)
			(pin bidirectional line
				(at -35.56 -74.93 0)
				(length 7.62)
				(name "IO3T4")
				(number "T4")
			)
			(pin bidirectional line
				(at -35.56 -76.2 0)
				(length 7.62)
				(name "IO3U2")
				(number "U2")
			)
			(pin bidirectional line
				(at -35.56 -77.47 0)
				(length 7.62)
				(name "IO3U3")
				(number "U3")
			)
			(pin bidirectional line
				(at -35.56 -78.74 0)
				(length 7.62)
				(name "IO3V1")
				(number "V1")
			)
			(pin bidirectional line
				(at -35.56 -80.01 0)
				(length 7.62)
				(name "IO3V2")
				(number "V2")
			)
			(pin bidirectional line
				(at -35.56 -81.28 0)
				(length 7.62)
				(name "IOR3V4")
				(number "V4")
			)
			(pin bidirectional line
				(at -35.56 -82.55 0)
				(length 7.62)
				(name "IO3W3")
				(number "W3")
			)
			(pin bidirectional line
				(at -35.56 -83.82 0)
				(length 7.62)
				(name "IO3W4")
				(number "W4")
			)
			(pin bidirectional line
				(at -35.56 -85.09 0)
				(length 7.62)
				(name "IO3Y1")
				(number "Y1")
			)
			(pin bidirectional line
				(at -35.56 -86.36 0)
				(length 7.62)
				(name "IO3Y2")
				(number "Y2")
			)
			(pin bidirectional line
				(at -35.56 -87.63 0)
				(length 7.62)
				(name "IOR3Y3")
				(number "Y3")
			)
			(pin bidirectional line
				(at -35.56 -88.9 0)
				(length 7.62)
				(name "IO3AA1")
				(number "AA1")
			)
			(pin bidirectional line
				(at -35.56 -90.17 0)
				(length 7.62)
				(name "IO3AA2")
				(number "AA2")
			)
			(pin bidirectional line
				(at -35.56 -91.44 0)
				(length 7.62)
				(name "IO3AA3")
				(number "AA3")
			)
			(pin bidirectional line
				(at -35.56 -92.71 0)
				(length 7.62)
				(name "IO3AA4")
				(number "AA4")
			)
			(pin bidirectional line
				(at -35.56 -93.98 0)
				(length 7.62)
				(name "IO3AB2")
				(number "AB2")
			)
			(pin bidirectional line
				(at -35.56 -95.25 0)
				(length 7.62)
				(name "IO3AB3")
				(number "AB3")
			)
			(pin bidirectional line
				(at -35.56 -96.52 0)
				(length 7.62)
				(name "IO3AB4")
				(number "AB4")
			)
			(pin bidirectional line
				(at -35.56 -97.79 0)
				(length 7.62)
				(name "IO3AC1")
				(number "AC1")
			)
			(pin bidirectional line
				(at -35.56 -99.06 0)
				(length 7.62)
				(name "IO3AC2")
				(number "AC2")
			)
			(pin bidirectional line
				(at -35.56 -100.33 0)
				(length 7.62)
				(name "IO3AD1")
				(number "AD1")
			)
			(pin passive line
				(at -20.32 109.22 270)
				(length 7.62)
				(name "v")
				(number "B16")
			)
			(pin passive line
				(at -19.05 109.22 270)
				(length 7.62)
				(name "v")
				(number "D12")
			)
			(pin power_in line
				(at -19.05 -110.49 90)
				(length 7.62)
				(name "GND")
				(number "A1")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "A14")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "A19")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "A2")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "A22")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "A25")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "A26")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "A5")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "A8")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "AB1")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "AB26")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "AE1")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "AE26")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "AF1")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "AF13")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "AF19")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "AF2")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "AF22")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "AF25")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "AF26")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "AF5")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "AF8")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "B1")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "B26")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "E1")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "E26")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "H1")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "H26")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "N1")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "P26")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "W1")
			)
			(pin passive line
				(at -19.05 -110.49 90)
				(length 7.62)
				(hide yes)
				(name "GND")
				(number "W26")
			)
			(pin passive line
				(at -17.78 109.22 270)
				(length 7.62)
				(name "v")
				(number "L1")
			)
			(pin passive line
				(at -16.51 109.22 270)
				(length 7.62)
				(name "v")
				(number "L25")
			)
			(pin passive line
				(at -15.24 109.22 270)
				(length 7.62)
				(name "v")
				(number "R23")
			)
			(pin passive line
				(at -13.97 109.22 270)
				(length 7.62)
				(name "v")
				(number "T1")
			)
			(pin passive line
				(at -12.7 109.22 270)
				(length 7.62)
				(name "v")
				(number "AF11")
			)
			(pin passive line
				(at -11.43 109.22 270)
				(length 7.62)
				(name "v")
				(number "AF16")
			)
			(pin power_in line
				(at -6.35 109.22 270)
				(length 7.62)
				(name "VCCINT")
				(number "A20")
			)
			(pin power_in line
				(at -5.08 109.22 270)
				(length 7.62)
				(name "VCCINT")
				(number "C14")
			)
			(pin power_in line
				(at -3.81 109.22 270)
				(length 7.62)
				(name "VCCINT")
				(number "D10")
			)
			(pin power_in line
				(at -2.54 109.22 270)
				(length 7.62)
				(name "VCCINT")
				(number "J24")
			)
			(pin power_in line
				(at -1.27 109.22 270)
				(length 7.62)
				(name "VCCINT")
				(number "K4")
			)
			(pin power_in line
				(at 0 109.22 270)
				(length 7.62)
				(name "VCCINT")
				(number "P2")
			)
			(pin power_in line
				(at 1.27 109.22 270)
				(length 7.62)
				(name "VCCINT")
				(number "P25")
			)
			(pin power_in line
				(at 2.54 109.22 270)
				(length 7.62)
				(name "VCCINT")
				(number "V24")
			)
			(pin power_in line
				(at 3.81 109.22 270)
				(length 7.62)
				(name "VCCINT")
				(number "W2")
			)
			(pin power_in line
				(at 5.08 109.22 270)
				(length 7.62)
				(name "VCCINT")
				(number "AC10")
			)
			(pin power_in line
				(at 6.35 109.22 270)
				(length 7.62)
				(name "VCCINT")
				(number "AE14")
			)
			(pin power_in line
				(at 7.62 109.22 270)
				(length 7.62)
				(name "VCCINT")
				(number "AE19")
			)
			(pin bidirectional line
				(at 36.83 99.06 180)
				(length 7.62)
				(name "D0/DIN")
				(number "D3")
			)
			(pin bidirectional line
				(at 36.83 97.79 180)
				(length 7.62)
				(name "D1")
				(number "G1")
			)
			(pin bidirectional line
				(at 36.83 96.52 180)
				(length 7.62)
				(name "D2")
				(number "J3")
			)
			(pin bidirectional line
				(at 36.83 95.25 180)
				(length 7.62)
				(name "D3")
				(number "M3")
			)
			(pin bidirectional line
				(at 36.83 93.98 180)
				(length 7.62)
				(name "D4")
				(number "R3")
			)
			(pin bidirectional line
				(at 36.83 92.71 180)
				(length 7.62)
				(name "D5")
				(number "U4")
			)
			(pin bidirectional line
				(at 36.83 91.44 180)
				(length 7.62)
				(name "D6")
				(number "V3")
			)
			(pin bidirectional line
				(at 36.83 90.17 180)
				(length 7.62)
				(name "D7")
				(number "AC3")
			)
			(pin passive line
				(at 36.83 87.63 180)
				(length 7.62)
				(name "DXP")
				(number "AE24")
			)
			(pin passive line
				(at 36.83 86.36 180)
				(length 7.62)
				(name "DXN")
				(number "AD23")
			)
			(pin power_in line
				(at 36.83 83.82 180)
				(length 7.62)
				(name "VCCO")
				(number "G23")
			)
			(pin power_in line
				(at 36.83 82.55 180)
				(length 7.62)
				(name "VCCO")
				(number "K26")
			)
			(pin power_in line
				(at 36.83 81.28 180)
				(length 7.62)
				(name "VCCO")
				(number "N23")
			)
			(pin bidirectional line
				(at 36.83 80.01 180)
				(length 7.62)
				(name "IO7C25")
				(number "C25")
			)
			(pin bidirectional line
				(at 36.83 78.74 180)
				(length 7.62)
				(name "IO7C26")
				(number "C26")
			)
			(pin bidirectional line
				(at 36.83 77.47 180)
				(length 7.62)
				(name "IO7D24")
				(number "D24")
			)
			(pin bidirectional line
				(at 36.83 76.2 180)
				(length 7.62)
				(name "IO7D25")
				(number "D25")
			)
			(pin bidirectional line
				(at 36.83 74.93 180)
				(length 7.62)
				(name "IOR7D26")
				(number "D26")
			)
			(pin bidirectional line
				(at 36.83 73.66 180)
				(length 7.62)
				(name "IO7E23")
				(number "E23")
			)
			(pin bidirectional line
				(at 36.83 72.39 180)
				(length 7.62)
				(name "IO7E24")
				(number "E24")
			)
			(pin bidirectional line
				(at 36.83 71.12 180)
				(length 7.62)
				(name "IO7E25")
				(number "E25")
			)
			(pin bidirectional line
				(at 36.83 69.85 180)
				(length 7.62)
				(name "IO7F23")
				(number "F23")
			)
			(pin bidirectional line
				(at 36.83 68.58 180)
				(length 7.62)
				(name "IO7F24")
				(number "F24")
			)
			(pin bidirectional line
				(at 36.83 67.31 180)
				(length 7.62)
				(name "IO7F25")
				(number "F25")
			)
			(pin bidirectional line
				(at 36.83 66.04 180)
				(length 7.62)
				(name "IO7F26")
				(number "F26")
			)
			(pin bidirectional line
				(at 36.83 64.77 180)
				(length 7.62)
				(name "IO7G24")
				(number "G24")
			)
			(pin bidirectional line
				(at 36.83 63.5 180)
				(length 7.62)
				(name "IO7G25")
				(number "G25")
			)
			(pin bidirectional line
				(at 36.83 62.23 180)
				(length 7.62)
				(name "IOR7G26")
				(number "G26")
			)
			(pin bidirectional line
				(at 36.83 60.96 180)
				(length 7.62)
				(name "IO7H23")
				(number "H23")
			)
			(pin bidirectional line
				(at 36.83 59.69 180)
				(length 7.62)
				(name "IO7H24")
				(number "H24")
			)
			(pin bidirectional line
				(at 36.83 58.42 180)
				(length 7.62)
				(name "IO7H25")
				(number "H25")
			)
			(pin bidirectional line
				(at 36.83 57.15 180)
				(length 7.62)
				(name "IO7J23")
				(number "J23")
			)
			(pin bidirectional line
				(at 36.83 55.88 180)
				(length 7.62)
				(name "IO7J25")
				(number "J25")
			)
			(pin bidirectional line
				(at 36.83 54.61 180)
				(length 7.62)
				(name "IO7J26")
				(number "J26")
			)
			(pin bidirectional line
				(at 36.83 53.34 180)
				(length 7.62)
				(name "IO7K23")
				(number "K23")
			)
			(pin bidirectional line
				(at 36.83 52.07 180)
				(length 7.62)
				(name "IO7K24")
				(number "K24")
			)
			(pin bidirectional line
				(at 36.83 50.8 180)
				(length 7.62)
				(name "IO7K25")
				(number "K25")
			)
			(pin bidirectional line
				(at 36.83 49.53 180)
				(length 7.62)
				(name "IO7L23")
				(number "L23")
			)
			(pin bidirectional line
				(at 36.83 48.26 180)
				(length 7.62)
				(name "IO7L24")
				(number "L24")
			)
			(pin bidirectional line
				(at 36.83 46.99 180)
				(length 7.62)
				(name "IOR7L26")
				(number "L26")
			)
			(pin bidirectional line
				(at 36.83 45.72 180)
				(length 7.62)
				(name "IO7M23")
				(number "M23")
			)
			(pin bidirectional line
				(at 36.83 44.45 180)
				(length 7.62)
				(name "IO7M24")
				(number "M24")
			)
			(pin bidirectional line
				(at 36.83 43.18 180)
				(length 7.62)
				(name "IO7M25")
				(number "M25")
			)
			(pin bidirectional line
				(at 36.83 41.91 180)
				(length 7.62)
				(name "IO7M26")
				(number "M26")
			)
			(pin bidirectional line
				(at 36.83 40.64 180)
				(length 7.62)
				(name "IO7N24")
				(number "N24")
			)
			(pin bidirectional line
				(at 36.83 39.37 180)
				(length 7.62)
				(name "IO7N25")
				(number "N25")
			)
			(pin power_in line
				(at 36.83 36.83 180)
				(length 7.62)
				(name "VCCO")
				(number "U26")
			)
			(pin power_in line
				(at 36.83 35.56 180)
				(length 7.62)
				(name "VCCO")
				(number "W23")
			)
			(pin power_in line
				(at 36.83 34.29 180)
				(length 7.62)
				(name "VCCO")
				(number "AE25")
			)
			(pin bidirectional line
				(at 36.83 33.02 180)
				(length 7.62)
				(name "IO6N26")
				(number "N26")
			)
			(pin bidirectional line
				(at 36.83 31.75 180)
				(length 7.62)
				(name "IO6P23")
				(number "P23")
			)
			(pin bidirectional line
				(at 36.83 30.48 180)
				(length 7.62)
				(name "IO6P24")
				(number "P24")
			)
			(pin bidirectional line
				(at 36.83 29.21 180)
				(length 7.62)
				(name "IOR6R24")
				(number "R24")
			)
			(pin bidirectional line
				(at 36.83 27.94 180)
				(length 7.62)
				(name "IO6R25")
				(number "R25")
			)
			(pin bidirectional line
				(at 36.83 26.67 180)
				(length 7.62)
				(name "IO6R26")
				(number "R26")
			)
			(pin bidirectional line
				(at 36.83 25.4 180)
				(length 7.62)
				(name "IO6T23")
				(number "T23")
			)
			(pin bidirectional line
				(at 36.83 24.13 180)
				(length 7.62)
				(name "IO6T24")
				(number "T24")
			)
			(pin bidirectional line
				(at 36.83 22.86 180)
				(length 7.62)
				(name "IO6T25")
				(number "T25")
			)
			(pin bidirectional line
				(at 36.83 21.59 180)
				(length 7.62)
				(name "IO6T26")
				(number "T26")
			)
			(pin bidirectional line
				(at 36.83 20.32 180)
				(length 7.62)
				(name "IO6U23")
				(number "U23")
			)
			(pin bidirectional line
				(at 36.83 19.05 180)
				(length 7.62)
				(name "IO6U24")
				(number "U24")
			)
			(pin bidirectional line
				(at 36.83 17.78 180)
				(length 7.62)
				(name "IO6U25")
				(number "U25")
			)
			(pin bidirectional line
				(at 36.83 16.51 180)
				(length 7.62)
				(name "IO6V23")
				(number "V23")
			)
			(pin bidirectional line
				(at 36.83 15.24 180)
				(length 7.62)
				(name "IO6V25")
				(number "V25")
			)
			(pin bidirectional line
				(at 36.83 13.97 180)
				(length 7.62)
				(name "IO6V26")
				(number "V26")
			)
			(pin bidirectional line
				(at 36.83 12.7 180)
				(length 7.62)
				(name "IO6W24")
				(number "W24")
			)
			(pin bidirectional line
				(at 36.83 11.43 180)
				(length 7.62)
				(name "IO6W25")
				(number "W25")
			)
			(pin bidirectional line
				(at 36.83 10.16 180)
				(length 7.62)
				(name "IO6Y23")
				(number "Y23")
			)
			(pin bidirectional line
				(at 36.83 8.89 180)
				(length 7.62)
				(name "IO6Y24")
				(number "Y24")
			)
			(pin bidirectional line
				(at 36.83 7.62 180)
				(length 7.62)
				(name "IO6Y25")
				(number "Y25")
			)
			(pin bidirectional line
				(at 36.83 6.35 180)
				(length 7.62)
				(name "IOR6Y26")
				(number "Y26")
			)
			(pin bidirectional line
				(at 36.83 5.08 180)
				(length 7.62)
				(name "IO6AA23")
				(number "AA23")
			)
			(pin bidirectional line
				(at 36.83 3.81 180)
				(length 7.62)
				(name "IO6AA24")
				(number "AA24")
			)
			(pin bidirectional line
				(at 36.83 2.54 180)
				(length 7.62)
				(name "IOR6AA25")
				(number "AA25")
			)
			(pin bidirectional line
				(at 36.83 1.27 180)
				(length 7.62)
				(name "IO6AA26")
				(number "AA26")
			)
			(pin bidirectional line
				(at 36.83 0 180)
				(length 7.62)
				(name "IO6AB24")
				(number "AB24")
			)
			(pin bidirectional line
				(at 36.83 -1.27 180)
				(length 7.62)
				(name "IO6AB25")
				(number "AB25")
			)
			(pin bidirectional line
				(at 36.83 -2.54 180)
				(length 7.62)
				(name "IO6AC24")
				(number "AC24")
			)
			(pin bidirectional line
				(at 36.83 -3.81 180)
				(length 7.62)
				(name "IO6AC25")
				(number "AC25")
			)
			(pin bidirectional line
				(at 36.83 -5.08 180)
				(length 7.62)
				(name "IO6AC26")
				(number "AC26")
			)
			(pin bidirectional line
				(at 36.83 -6.35 180)
				(length 7.62)
				(name "IO6AD25")
				(number "AD25")
			)
			(pin bidirectional line
				(at 36.83 -7.62 180)
				(length 7.62)
				(name "IO6AD26")
				(number "AD26")
			)
			(pin power_in line
				(at 36.83 -10.16 180)
				(length 7.62)
				(name "VCCO")
				(number "AC14")
			)
			(pin power_in line
				(at 36.83 -11.43 180)
				(length 7.62)
				(name "VCCO")
				(number "AC20")
			)
			(pin power_in line
				(at 36.83 -12.7 180)
				(length 7.62)
				(name "VCCO")
				(number "AF17")
			)
			(pin bidirectional line
				(at 36.83 -13.97 180)
				(length 7.62)
				(name "IOR5AC15")
				(number "AC15")
			)
			(pin bidirectional line
				(at 36.83 -15.24 180)
				(length 7.62)
				(name "IO5AC16")
				(number "AC16")
			)
			(pin bidirectional line
				(at 36.83 -16.51 180)
				(length 7.62)
				(name "IO5AC17")
				(number "AC17")
			)
			(pin bidirectional line
				(at 36.83 -17.78 180)
				(length 7.62)
				(name "IOR5AC18")
				(number "AC18")
			)
			(pin bidirectional line
				(at 36.83 -19.05 180)
				(length 7.62)
				(name "IO5AC19")
				(number "AC19")
			)
			(pin bidirectional line
				(at 36.83 -20.32 180)
				(length 7.62)
				(name "IO5AC21")
				(number "AC21")
			)
			(pin bidirectional line
				(at 36.83 -21.59 180)
				(length 7.62)
				(name "IO5AC22")
				(number "AC22")
			)
			(pin bidirectional line
				(at 36.83 -22.86 180)
				(length 7.62)
				(name "IO5AD14")
				(number "AD14")
			)
			(pin bidirectional line
				(at 36.83 -24.13 180)
				(length 7.62)
				(name "IO5AD15")
				(number "AD15")
			)
			(pin bidirectional line
				(at 36.83 -25.4 180)
				(length 7.62)
				(name "IO5AD16")
				(number "AD16")
			)
			(pin bidirectional line
				(at 36.83 -26.67 180)
				(length 7.62)
				(name "IO5AD17")
				(number "AD17")
			)
			(pin bidirectional line
				(at 36.83 -27.94 180)
				(length 7.62)
				(name "IO5AD18")
				(number "AD18")
			)
			(pin bidirectional line
				(at 36.83 -29.21 180)
				(length 7.62)
				(name "IO5AD19")
				(number "AD19")
			)
			(pin bidirectional line
				(at 36.83 -30.48 180)
				(length 7.62)
				(name "IOR5AD20")
				(number "AD20")
			)
			(pin bidirectional line
				(at 36.83 -31.75 180)
				(length 7.62)
				(name "IO5AD21")
				(number "AD21")
			)
			(pin bidirectional line
				(at 36.83 -33.02 180)
				(length 7.62)
				(name "IO5AD22")
				(number "AD22")
			)
			(pin bidirectional line
				(at 36.83 -34.29 180)
				(length 7.62)
				(name "IO5AE15")
				(number "AE15")
			)
			(pin bidirectional line
				(at 36.83 -35.56 180)
				(length 7.62)
				(name "IO5AE16")
				(number "AE16")
			)
			(pin bidirectional line
				(at 36.83 -36.83 180)
				(length 7.62)
				(name "IO5AE17")
				(number "AE17")
			)
			(pin bidirectional line
				(at 36.83 -38.1 180)
				(length 7.62)
				(name "IO5AE18")
				(number "AE18")
			)
			(pin bidirectional line
				(at 36.83 -39.37 180)
				(length 7.62)
				(name "IO5AE20")
				(number "AE20")
			)
			(pin bidirectional line
				(at 36.83 -40.64 180)
				(length 7.62)
				(name "IO5AE21")
				(number "AE21")
			)
			(pin bidirectional line
				(at 36.83 -41.91 180)
				(length 7.62)
				(name "IO5AE22")
				(number "AE22")
			)
			(pin bidirectional line
				(at 36.83 -43.18 180)
				(length 7.62)
				(name "IO5AE23")
				(number "AE23")
			)
			(pin input line
				(at 36.83 -44.45 180)
				(length 7.62)
				(name "GCK1")
				(number "AF14")
			)
			(pin bidirectional line
				(at 36.83 -45.72 180)
				(length 7.62)
				(name "IO5AF15")
				(number "AF15")
			)
			(pin bidirectional line
				(at 36.83 -46.99 180)
				(length 7.62)
				(name "IO5AF18")
				(number "AF18")
			)
			(pin bidirectional line
				(at 36.83 -48.26 180)
				(length 7.62)
				(name "IO5AF20")
				(number "AF20")
			)
			(pin bidirectional line
				(at 36.83 -49.53 180)
				(length 7.62)
				(name "IO5AF21")
				(number "AF21")
			)
			(pin bidirectional line
				(at 36.83 -50.8 180)
				(length 7.62)
				(name "IO5AF23")
				(number "AF23")
			)
			(pin bidirectional line
				(at 36.83 -52.07 180)
				(length 7.62)
				(name "IO5AF24")
				(number "AF24")
			)
			(pin power_in line
				(at 36.83 -54.61 180)
				(length 7.62)
				(name "VCCO")
				(number "AC8")
			)
			(pin power_in line
				(at 36.83 -55.88 180)
				(length 7.62)
				(name "VCCO")
				(number "AE2")
			)
			(pin power_in line
				(at 36.83 -57.15 180)
				(length 7.62)
				(name "VCCO")
				(number "AF10")
			)
			(pin bidirectional line
				(at 36.83 -58.42 180)
				(length 7.62)
				(name "IO4AC5")
				(number "AC5")
			)
			(pin bidirectional line
				(at 36.83 -59.69 180)
				(length 7.62)
				(name "IO4AC6")
				(number "AC6")
			)
			(pin bidirectional line
				(at 36.83 -60.96 180)
				(length 7.62)
				(name "IO4AC7")
				(number "AC7")
			)
			(pin bidirectional line
				(at 36.83 -62.23 180)
				(length 7.62)
				(name "IO4AC9")
				(number "AC9")
			)
			(pin bidirectional line
				(at 36.83 -63.5 180)
				(length 7.62)
				(name "IO4AC11")
				(number "AC11")
			)
			(pin bidirectional line
				(at 36.83 -64.77 180)
				(length 7.62)
				(name "IOR4AC12")
				(number "AC12")
			)
			(pin bidirectional line
				(at 36.83 -66.04 180)
				(length 7.62)
				(name "IO4AC13")
				(number "AC13")
			)
			(pin bidirectional line
				(at 36.83 -67.31 180)
				(length 7.62)
				(name "IO4AD4")
				(number "AD4")
			)
			(pin bidirectional line
				(at 36.83 -68.58 180)
				(length 7.62)
				(name "IO4AD5")
				(number "AD5")
			)
			(pin bidirectional line
				(at 36.83 -69.85 180)
				(length 7.62)
				(name "IO4AD6")
				(number "AD6")
			)
			(pin bidirectional line
				(at 36.83 -71.12 180)
				(length 7.62)
				(name "IO4AD7")
				(number "AD7")
			)
			(pin bidirectional line
				(at 36.83 -72.39 180)
				(length 7.62)
				(name "IO4AD8")
				(number "AD8")
			)
			(pin bidirectional line
				(at 36.83 -73.66 180)
				(length 7.62)
				(name "IO4AD9")
				(number "AD9")
			)
			(pin bidirectional line
				(at 36.83 -74.93 180)
				(length 7.62)
				(name "IO4AD10")
				(number "AD10")
			)
			(pin bidirectional line
				(at 36.83 -76.2 180)
				(length 7.62)
				(name "IO4AD11")
				(number "AD11")
			)
			(pin bidirectional line
				(at 36.83 -77.47 180)
				(length 7.62)
				(name "IO4AD12")
				(number "AD12")
			)
			(pin bidirectional line
				(at 36.83 -78.74 180)
				(length 7.62)
				(name "IO4AD13")
				(number "AD13")
			)
			(pin bidirectional line
				(at 36.83 -80.01 180)
				(length 7.62)
				(name "IO4AE3")
				(number "AE3")
			)
			(pin bidirectional line
				(at 36.83 -81.28 180)
				(length 7.62)
				(name "IO4AE4")
				(number "AE4")
			)
			(pin bidirectional line
				(at 36.83 -82.55 180)
				(length 7.62)
				(name "IOR4AE5")
				(number "AE5")
			)
			(pin bidirectional line
				(at 36.83 -83.82 180)
				(length 7.62)
				(name "IO4AE6")
				(number "AE6")
			)
			(pin bidirectional line
				(at 36.83 -85.09 180)
				(length 7.62)
				(name "IO4AE7")
				(number "AE7")
			)
			(pin bidirectional line
				(at 36.83 -86.36 180)
				(length 7.62)
				(name "IOR4AE8")
				(number "AE8")
			)
			(pin bidirectional line
				(at 36.83 -87.63 180)
				(length 7.62)
				(name "IO4AE9")
				(number "AE9")
			)
			(pin bidirectional line
				(at 36.83 -88.9 180)
				(length 7.62)
				(name "IO4AE10")
				(number "AE10")
			)
			(pin bidirectional line
				(at 36.83 -90.17 180)
				(length 7.62)
				(name "IO4AE11")
				(number "AE11")
			)
			(pin bidirectional line
				(at 36.83 -91.44 180)
				(length 7.62)
				(name "IO4AE12")
				(number "AE12")
			)
			(pin input line
				(at 36.83 -92.71 180)
				(length 7.62)
				(name "GCK0")
				(number "AE13")
			)
			(pin bidirectional line
				(at 36.83 -93.98 180)
				(length 7.62)
				(name "IO4AF3")
				(number "AF3")
			)
			(pin bidirectional line
				(at 36.83 -95.25 180)
				(length 7.62)
				(name "IO4AF4")
				(number "AF4")
			)
			(pin bidirectional line
				(at 36.83 -96.52 180)
				(length 7.62)
				(name "IO4AF6")
				(number "AF6")
			)
			(pin bidirectional line
				(at 36.83 -97.79 180)
				(length 7.62)
				(name "IO4AF7")
				(number "AF7")
			)
			(pin bidirectional line
				(at 36.83 -99.06 180)
				(length 7.62)
				(name "IO4AF9")
				(number "AF9")
			)
			(pin bidirectional line
				(at 36.83 -100.33 180)
				(length 7.62)
				(name "IO4AF12")
				(number "AF12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC2064-PC68"
		(extends "XC2018-PC68")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XC2064-PC68"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "XC3030-PC68"
		(extends "XC3020-PC68")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XC3030-PC68"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "XC3042-PC84"
		(extends "XC3030-PC84")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XC3042-PC84"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "XC4005-PC84"
		(extends "XC4003-PC84")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XC4005-PC84"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
)
