(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "XC7K160T-FBG484"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC7K160T-FBG484"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Kintex 7 T 160 XC7K160T-FBG484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC7K160T-FBG484_1_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_13")
				(number "T19")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_13")
				(number "T21")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_13")
				(number "U21")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_13")
				(number "U22")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_13")
				(number "V22")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_13")
				(number "T18")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_13")
				(number "U18")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_13")
				(number "W21")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_13")
				(number "W22")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_13")
				(number "U17")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_13")
				(number "V18")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_13")
				(number "T20")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_13")
				(number "U20")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_13")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_13")
				(number "Y22")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_13")
				(number "AA20")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_13")
				(number "AB21")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_13")
				(number "AA21")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_13")
				(number "AB22")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_13")
				(number "AA19")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_13")
				(number "AB20")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_13")
				(number "V20")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_13")
				(number "W20")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_13")
				(number "V19")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_13")
				(number "W19")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_13")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_13")
				(number "Y19")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_13")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_13")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_13")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_13")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_13")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_13")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_13")
				(number "AA16")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_13")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_13")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_13")
				(number "AA15")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_13")
				(number "U16")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_13")
				(number "V17")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_13")
				(number "R16")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_13")
				(number "T16")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_13")
				(number "W16")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_13")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_13")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_13")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_13")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_13")
				(number "W15")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_13")
				(number "T15")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_13")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_13")
				(number "V14")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AA17")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AB14")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "T22")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "U19")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "V16")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "Y20")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "F22")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "G19")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "K20")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "L17")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "N21")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_14")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_D00_MOSI_14")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_D01_DIN_14")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_D02_14")
				(number "G18")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_D03_14")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_PUDC_B_14")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_EMCCLK_14")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_D04_14")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_D05_14")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_D06_14")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_D07_14")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_FCS_B_14")
				(number "L16")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_D08_VREF_14")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_D09_14")
				(number "E21")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_D10_14")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_D11_14")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_D12_14")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_14")
				(number "G21")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_D13_14")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_D14_14")
				(number "J21")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_D15_14")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_14")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_14")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_14")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_14")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_14")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_14")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_14")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_14")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_RDWR_B_14")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_DOUT_CSO_B_14")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_CSI_B_14")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_A15_D31_14")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_A14_D30_14")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_A13_D29_14")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_A12_D28_14")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_A11_D27_14")
				(number "L21")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_A10_D26_14")
				(number "R18")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_A09_D25_VREF_14")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_A08_D24_14")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_A07_D23_14")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_14")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A06_D22_14")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_A05_D21_14")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_A04_D20_14")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_A03_D19_14")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_A02_D18_14")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_A01_D17_14")
				(number "R21")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_A00_D16_14")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_14")
				(number "M16")
			)
		)
		(symbol "XC7K160T-FBG484_2_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_15")
				(number "D12")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_AD0P_15")
				(number "G15")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_AD0N_15")
				(number "G16")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_AD8P_15")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_AD8N_15")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_AD1P_15")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_AD1N_15")
				(number "F16")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_AD9P_15")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_AD9N_15")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_AD2P_15")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_AD2N_15")
				(number "B13")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_15")
				(number "E14")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_15")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_AD10P_15")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_AD10N_15")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_AD3P_15")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_AD3N_15")
				(number "A16")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_AD11P_15")
				(number "B15")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_AD11N_15")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_AD4P_15")
				(number "B17")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_AD4N_15")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_AD12P_15")
				(number "D15")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_AD12N_15")
				(number "D16")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_AD5P_15")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_AD5N_15")
				(number "C18")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_15")
				(number "E17")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_15")
				(number "E18")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_15")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_15")
				(number "D17")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_15")
				(number "H17")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_ADV_B_15")
				(number "G17")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_A28_15")
				(number "J16")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_A27_15")
				(number "J17")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_A26_15")
				(number "F18")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_A25_15")
				(number "E19")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_A24_15")
				(number "D19")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_A23_15")
				(number "D20")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_A22_15")
				(number "C19")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_A21_VREF_15")
				(number "C20")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_A20_15")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_A19_15")
				(number "A19")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_15")
				(number "C22")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A18_15")
				(number "B22")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_A17_15")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_A16_15")
				(number "A21")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_FOE_B_15")
				(number "D21")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_FWE_B_15")
				(number "D22")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_RS1_15")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_RS0_15")
				(number "B21")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_15")
				(number "H15")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "A17")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "B14")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "C21")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "D18")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "E15")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "H16")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "C11")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "D8")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "F12")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "G9")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_6_T0_VREF_16")
				(number "F14")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L7P_T1_16")
				(number "D10")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L7N_T1_16")
				(number "C10")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L8P_T1_16")
				(number "G13")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L8N_T1_16")
				(number "F13")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_16")
				(number "H14")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_16")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L10P_T1_16")
				(number "E13")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L10N_T1_16")
				(number "E12")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_16")
				(number "F11")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_16")
				(number "F10")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_16")
				(number "E11")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_16")
				(number "D11")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_16")
				(number "G11")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_16")
				(number "G10")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_16")
				(number "H12")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_16")
				(number "G12")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_16")
				(number "F9")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_16")
				(number "E9")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L16P_T2_16")
				(number "H9")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L16N_T2_16")
				(number "H8")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L17P_T2_16")
				(number "G8")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L17N_T2_16")
				(number "F8")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_18_T2_16")
				(number "H10")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L19P_T3_16")
				(number "D9")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_16")
				(number "C9")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L20P_T3_16")
				(number "B11")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L20N_T3_16")
				(number "B10")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_16")
				(number "A9")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_16")
				(number "A8")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L22P_T3_16")
				(number "C8")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L22N_T3_16")
				(number "B8")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L23P_T3_16")
				(number "A11")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L23N_T3_16")
				(number "A10")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_24_T3_16")
				(number "E8")
			)
		)
		(symbol "XC7K160T-FBG484_3_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_VRN_33")
				(number "T6")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_33")
				(number "AA5")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_33")
				(number "AB5")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_33")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_33")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_33")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_33")
				(number "AB6")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_33")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_33")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_33")
				(number "AA9")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_33")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_33")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_33")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_33")
				(number "W6")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_33")
				(number "Y6")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_33")
				(number "R7")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_33")
				(number "R6")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_33")
				(number "U8")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_33")
				(number "V8")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_33")
				(number "U7")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_33")
				(number "U6")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_33")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_33")
				(number "W7")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_33")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_33")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_33")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_33")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_33")
				(number "U10")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_33")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_33")
				(number "V10")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_33")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_33")
				(number "T11")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_33")
				(number "T10")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_33")
				(number "U12")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_33")
				(number "U11")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_33")
				(number "T9")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_33")
				(number "T8")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_33")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_33")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_33")
				(number "AA11")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_33")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_33")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_33")
				(number "AA13")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_33")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_33")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_33")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_33")
				(number "V12")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_33")
				(number "T13")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_33")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_VRP_33")
				(number "T14")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AA7")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "T12")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "U9")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "V6")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "W13")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "Y10")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AB4")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "M4")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "N1")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "R5")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "T2")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_34")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_34")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_34")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_34")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_34")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_34")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_34")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_34")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_34")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_34")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_34")
				(number "N2")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_34")
				(number "L5")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_34")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_34")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_34")
				(number "R2")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_34")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_34")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_34")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_34")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_34")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_34")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_34")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_34")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_34")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_34")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_34")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_34")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_34")
				(number "V4")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_34")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_34")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_34")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_34")
				(number "T5")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_34")
				(number "U5")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_34")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_34")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_34")
				(number "N5")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_34")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_34")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_34")
				(number "Y4")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_34")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_34")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_34")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_34")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_34")
				(number "AA1")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_34")
				(number "AB1")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_34")
				(number "AA3")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_34")
				(number "AB2")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_34")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_34")
				(number "AB3")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_34")
				(number "V5")
			)
		)
		(symbol "XC7K160T-FBG484_4_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_115")
				(number "F2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_115")
				(number "F1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_115")
				(number "D2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_115")
				(number "D1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_115")
				(number "B2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_115")
				(number "B1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_115")
				(number "A4")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_115")
				(number "A3")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_115")
				(number "G4")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_115")
				(number "G3")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_115")
				(number "E4")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_115")
				(number "E3")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_115")
				(number "C4")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_115")
				(number "C3")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_115")
				(number "B6")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_115")
				(number "B5")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_115")
				(number "D6")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_115")
				(number "D5")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_115")
				(number "F6")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_115")
				(number "F5")
			)
		)
		(symbol "XC7K160T-FBG484_5_1"
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "A6")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "C6")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "E6")
			)
			(pin power_in line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "G6")
			)
			(pin power_in line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTVCCAUX")
				(number "J4")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "A2")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "C2")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "E2")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "G2")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTTRCAL_115")
				(number "H1")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTRREF_115")
				(number "H2")
			)
		)
		(symbol "XC7K160T-FBG484_6_1"
			(pin power_in line
				(at 25.4 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "J7")
			)
			(pin power_in line
				(at 27.94 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "N7")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "TDI_0")
				(number "K6")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "TDO_0")
				(number "J6")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "TMS_0")
				(number "L6")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TCK_0")
				(number "K7")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "CCLK_0")
				(number "G7")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "M0_0")
				(number "H7")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "M1_0")
				(number "H6")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "M2_0")
				(number "J5")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "DONE_0")
				(number "P6")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "INIT_B_0")
				(number "L7")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "PROGRAM_B_0")
				(number "M6")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "CFGBVS_0")
				(number "M7")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "VP_0")
				(number "L12")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "VN_0")
				(number "M11")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 6.35)
				(name "VREFP_0")
				(number "M12")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "VREFN_0")
				(number "L11")
			)
			(pin bidirectional line
				(at 38.1 -35.56 180)
				(length 6.35)
				(name "DXP_0")
				(number "N12")
			)
			(pin bidirectional line
				(at 38.1 -38.1 180)
				(length 6.35)
				(name "DXN_0")
				(number "N11")
			)
		)
		(symbol "XC7K160T-FBG484_7_1"
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M10")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P8")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P10")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P12")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R9")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R11")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "GNDADC_0")
				(number "K11")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCADC_0")
				(number "K12")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCBATT_0")
				(number "P7")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "L13")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "N13")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "R13")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "A5")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "A7")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "A12")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "B3")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "B4")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "B19")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "C1")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "C5")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "C7")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "C16")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "D3")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "D7")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "D13")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E1")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "E10")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "E20")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "F3")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "F17")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "G1")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "G14")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "H3")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "H5")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "H11")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "H21")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "J1")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "J3")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "J8")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "J10")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "J12")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "J14")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "J18")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "K5")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "J11")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "J13")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "J15")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "L15")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "M8")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "R15")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "K15")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "L2")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "L8")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "L22")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "M19")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "N6")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "N8")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "N16")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "P3")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "P15")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "R8")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "R10")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "R12")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "R20")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "T7")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "T17")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "U4")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "U14")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "V1")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "V11")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "V21")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "W8")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "W18")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "Y5")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "Y15")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AA2")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AA12")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AA22")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AB9")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AB19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC7K160T-FBG676"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC7K160T-FBG676"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Kintex 7 T 160 XC7K160T-FBG676"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC7K160T-FBG676_1_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_12")
				(number "U21")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_12")
				(number "U22")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_12")
				(number "V22")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_12")
				(number "U24")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_12")
				(number "U25")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_12")
				(number "V23")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_12")
				(number "V24")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_12")
				(number "U26")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_12")
				(number "V26")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_12")
				(number "W25")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_12")
				(number "W26")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_12")
				(number "V21")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_12")
				(number "W21")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_12")
				(number "AA25")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_12")
				(number "AB25")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_12")
				(number "W23")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_12")
				(number "W24")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_12")
				(number "AB26")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_12")
				(number "AC26")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_12")
				(number "Y25")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_12")
				(number "Y26")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_12")
				(number "AA23")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_12")
				(number "AB24")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_12")
				(number "Y23")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_12")
				(number "AA24")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_12")
				(number "Y22")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_12")
				(number "AA22")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_12")
				(number "AC23")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_12")
				(number "AC24")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_12")
				(number "W20")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_12")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_12")
				(number "AD23")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_12")
				(number "AD24")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_12")
				(number "AB22")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_12")
				(number "AC22")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_12")
				(number "AB21")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_12")
				(number "AC21")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_12")
				(number "AD21")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_12")
				(number "AE21")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_12")
				(number "AF24")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_12")
				(number "AF25")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_12")
				(number "AD26")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_12")
				(number "AE26")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_12")
				(number "AE23")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_12")
				(number "AF23")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_12")
				(number "AD25")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_12")
				(number "AE25")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_12")
				(number "AE22")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_12")
				(number "AF22")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_12")
				(number "Y20")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AA21")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AC25")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AD22")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AF26")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "U23")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "V20")
			)
			(pin power_in line
				(at -25.4 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "Y24")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "K24")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "N25")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "P22")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "R19")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "T16")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "T26")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_13")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_13")
				(number "K25")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_13")
				(number "K26")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_13")
				(number "R26")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_13")
				(number "P26")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_13")
				(number "M25")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_13")
				(number "L25")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_13")
				(number "P24")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_13")
				(number "N24")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_13")
				(number "N26")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_13")
				(number "M26")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_13")
				(number "R25")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_13")
				(number "P25")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_13")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_13")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_13")
				(number "M24")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_13")
				(number "L24")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_13")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_13")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_13")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_13")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_13")
				(number "P23")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_13")
				(number "N23")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_13")
				(number "N21")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_13")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_13")
				(number "R21")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_13")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_13")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_13")
				(number "R23")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_13")
				(number "T24")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_13")
				(number "T25")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_13")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_13")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_13")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_13")
				(number "T23")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_13")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_13")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_13")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_13")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_13")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_13")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_13")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_13")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_13")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_13")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_13")
				(number "U17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_13")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_13")
				(number "R18")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_13")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_13")
				(number "U16")
			)
		)
		(symbol "XC7K160T-FBG676_2_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_14")
				(number "K21")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_D00_MOSI_14")
				(number "B24")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_D01_DIN_14")
				(number "A25")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_D02_14")
				(number "B22")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_D03_14")
				(number "A22")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_PUDC_B_14")
				(number "B25")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_EMCCLK_14")
				(number "B26")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_D04_14")
				(number "A23")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_D05_14")
				(number "A24")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_D06_14")
				(number "D26")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_D07_14")
				(number "C26")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_FCS_B_14")
				(number "C23")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_D08_VREF_14")
				(number "C24")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_D09_14")
				(number "D21")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_D10_14")
				(number "C22")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_D11_14")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_D12_14")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_14")
				(number "E21")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_D13_14")
				(number "E22")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_D14_14")
				(number "C21")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_D15_14")
				(number "B21")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_14")
				(number "D23")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_14")
				(number "D24")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_14")
				(number "F22")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_14")
				(number "E23")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_14")
				(number "G22")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_14")
				(number "F23")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_14")
				(number "G24")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_14")
				(number "F24")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_RDWR_B_14")
				(number "E25")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_DOUT_CSO_B_14")
				(number "D25")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_CSI_B_14")
				(number "G25")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_A15_D31_14")
				(number "G26")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_A14_D30_14")
				(number "F25")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_A13_D29_14")
				(number "E26")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_A12_D28_14")
				(number "J26")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_A11_D27_14")
				(number "H26")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_A10_D26_14")
				(number "H21")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_A09_D25_VREF_14")
				(number "G21")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_A08_D24_14")
				(number "H23")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_A07_D23_14")
				(number "H24")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_14")
				(number "J21")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A06_D22_14")
				(number "H22")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_A05_D21_14")
				(number "J24")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_A04_D20_14")
				(number "J25")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_A03_D19_14")
				(number "L22")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_A02_D18_14")
				(number "K22")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_A01_D17_14")
				(number "K23")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_A00_D16_14")
				(number "J23")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_14")
				(number "L23")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "A21")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "C25")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "D22")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "F26")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "G23")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "L21")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "B18")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "E19")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "F16")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "H20")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "J17")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_15")
				(number "K15")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_AD0P_15")
				(number "C16")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_AD0N_15")
				(number "B16")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_AD8P_15")
				(number "A18")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_AD8N_15")
				(number "A19")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_AD1P_15")
				(number "B17")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_AD1N_15")
				(number "A17")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_AD9P_15")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_AD9N_15")
				(number "B19")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_AD2P_15")
				(number "C17")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_AD2N_15")
				(number "C18")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_15")
				(number "D15")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_15")
				(number "D16")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_AD10P_15")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_AD10N_15")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_AD3P_15")
				(number "G15")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_AD3N_15")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_AD11P_15")
				(number "J15")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_AD11N_15")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_AD4P_15")
				(number "E15")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_AD4N_15")
				(number "E16")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_AD12P_15")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_AD12N_15")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_AD5P_15")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_AD5N_15")
				(number "E17")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_15")
				(number "E18")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_15")
				(number "D18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_15")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_15")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_15")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_ADV_B_15")
				(number "D20")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_A28_15")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_A27_15")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_A26_15")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_A25_15")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_A24_15")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_A23_15")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_A22_15")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_A21_VREF_15")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_A20_15")
				(number "J18")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_A19_15")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_15")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A18_15")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_A17_15")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_A16_15")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_FOE_B_15")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_FWE_B_15")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_RS1_15")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_RS0_15")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_15")
				(number "M16")
			)
		)
		(symbol "XC7K160T-FBG676_3_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_16")
				(number "J8")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_16")
				(number "H9")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_16")
				(number "H8")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_16")
				(number "G10")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_16")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_16")
				(number "J13")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_16")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_16")
				(number "J11")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_16")
				(number "J10")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_16")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_16")
				(number "G14")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_16")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_16")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_16")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_16")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_16")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_16")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_16")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_16")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_16")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_16")
				(number "B9")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_16")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_16")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_16")
				(number "E10")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_16")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_16")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_16")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_16")
				(number "E11")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_16")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_16")
				(number "F14")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_16")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_16")
				(number "G12")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_16")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_16")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_16")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_16")
				(number "E13")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_16")
				(number "E12")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_16")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_16")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_16")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_16")
				(number "B11")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_16")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_16")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_16")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_16")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_16")
				(number "B15")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_16")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_16")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_16")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_16")
				(number "J14")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "A11")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "B8")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "C15")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "D12")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "E9")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "G13")
			)
			(pin power_in line
				(at -25.4 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "H10")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AB18")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AC15")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AE19")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AF16")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "W17")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "Y14")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_32")
				(number "V13")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_32")
				(number "AE17")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_32")
				(number "AF17")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_32")
				(number "AF14")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_32")
				(number "AF15")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_32")
				(number "AE18")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_32")
				(number "AF18")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_32")
				(number "AD15")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_32")
				(number "AE15")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_32")
				(number "AF19")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_32")
				(number "AF20")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_32")
				(number "AD16")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_32")
				(number "AE16")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_32")
				(number "AA14")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_32")
				(number "AA15")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_32")
				(number "AC14")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_32")
				(number "AD14")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_32")
				(number "Y15")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_32")
				(number "Y16")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_32")
				(number "AB14")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_32")
				(number "AB15")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_32")
				(number "AA17")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_32")
				(number "AA18")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_32")
				(number "AB16")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_32")
				(number "AC16")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_32")
				(number "AC18")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_32")
				(number "AD18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_32")
				(number "AB17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_32")
				(number "AC17")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_32")
				(number "AD20")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_32")
				(number "AE20")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_32")
				(number "AA19")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_32")
				(number "AA20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_32")
				(number "AC19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_32")
				(number "AD19")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_32")
				(number "AB19")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_32")
				(number "AB20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_32")
				(number "Y17")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_32")
				(number "Y18")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_32")
				(number "V16")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_32")
				(number "V17")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_32")
				(number "W18")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_32")
				(number "W19")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_32")
				(number "W15")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_32")
				(number "W16")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_32")
				(number "V18")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_32")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_32")
				(number "V14")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_32")
				(number "W14")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_32")
				(number "W13")
			)
		)
		(symbol "XC7K160T-FBG676_4_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_VRN_33")
				(number "U9")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_33")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_33")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_33")
				(number "V8")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_33")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_33")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_33")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_33")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_33")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_33")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_33")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_33")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_33")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_33")
				(number "AE7")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_33")
				(number "AF7")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_33")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_33")
				(number "AA7")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_33")
				(number "AC8")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_33")
				(number "AD8")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_33")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_33")
				(number "AC7")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_33")
				(number "AA9")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_33")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_33")
				(number "AC9")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_33")
				(number "AD9")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_33")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_33")
				(number "AC11")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_33")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_33")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_33")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_33")
				(number "AC12")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_33")
				(number "AA13")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_33")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_33")
				(number "AC13")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_33")
				(number "AD13")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_33")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_33")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_33")
				(number "AD11")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_33")
				(number "AE11")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_33")
				(number "AD10")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_33")
				(number "AE10")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_33")
				(number "AE12")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_33")
				(number "AF12")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_33")
				(number "AE8")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_33")
				(number "AF8")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_33")
				(number "AE13")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_33")
				(number "AF13")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_33")
				(number "AF10")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_33")
				(number "AF9")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_VRP_33")
				(number "V12")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AA11")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AB8")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AD12")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AE9")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "V10")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "W7")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AA1")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AC5")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AD2")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AF6")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "U3")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "Y4")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_34")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_34")
				(number "U6")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_34")
				(number "U5")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_34")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_34")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_34")
				(number "W6")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_34")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_34")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_34")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_34")
				(number "U7")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_34")
				(number "V6")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_34")
				(number "V4")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_34")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_34")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_34")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_34")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_34")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_34")
				(number "AB1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_34")
				(number "AC1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_34")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_34")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_34")
				(number "AB2")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_34")
				(number "AC2")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_34")
				(number "AA3")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_34")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_34")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_34")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_34")
				(number "AC4")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_34")
				(number "AC3")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_34")
				(number "AA5")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_34")
				(number "AB5")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_34")
				(number "AB6")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_34")
				(number "AC6")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_34")
				(number "Y6")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_34")
				(number "Y5")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_34")
				(number "AD6")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_34")
				(number "AD5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_34")
				(number "AD4")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_34")
				(number "AD3")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_34")
				(number "AD1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_34")
				(number "AE1")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_34")
				(number "AF5")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_34")
				(number "AF4")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_34")
				(number "AE3")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_34")
				(number "AE2")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_34")
				(number "AE6")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_34")
				(number "AE5")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_34")
				(number "AF3")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_34")
				(number "AF2")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_34")
				(number "T7")
			)
		)
		(symbol "XC7K160T-FBG676_5_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_115")
				(number "P2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_115")
				(number "P1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_115")
				(number "M2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_115")
				(number "M1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_115")
				(number "K2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_115")
				(number "K1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_115")
				(number "H2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_115")
				(number "H1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_115")
				(number "R4")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_115")
				(number "R3")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_115")
				(number "N4")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_115")
				(number "N3")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_115")
				(number "L4")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_115")
				(number "L3")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_115")
				(number "J4")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_115")
				(number "J3")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_115")
				(number "H6")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_115")
				(number "H5")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_115")
				(number "K6")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_115")
				(number "K5")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_116")
				(number "F2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_116")
				(number "F1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_116")
				(number "D2")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_116")
				(number "D1")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_116")
				(number "B2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_116")
				(number "B1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_116")
				(number "A4")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_116")
				(number "A3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_116")
				(number "G4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_116")
				(number "G3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_116")
				(number "E4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_116")
				(number "E3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_116")
				(number "C4")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_116")
				(number "C3")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_116")
				(number "B6")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_116")
				(number "B5")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_116")
				(number "D6")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_116")
				(number "D5")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_116")
				(number "F6")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_116")
				(number "F5")
			)
		)
		(symbol "XC7K160T-FBG676_6_1"
			(pin power_in line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "C6")
			)
			(pin power_in line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "E6")
			)
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "G6")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "J6")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "L6")
			)
			(pin power_in line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTVCCAUX")
				(number "N6")
			)
			(pin power_in line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "B3")
			)
			(pin power_in line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "C2")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "D3")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "G2")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "H3")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "L2")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "M3")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTTRCAL_115")
				(number "M5")
			)
			(pin power_in line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTRREF_115")
				(number "M6")
			)
		)
		(symbol "XC7K160T-FBG676_7_1"
			(pin power_in line
				(at 25.4 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "L7")
			)
			(pin power_in line
				(at 27.94 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "T6")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "TDI_0")
				(number "R6")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "TDO_0")
				(number "R7")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "TMS_0")
				(number "N8")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TCK_0")
				(number "L8")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "CCLK_0")
				(number "C8")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "M0_0")
				(number "T5")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "M1_0")
				(number "T2")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "M2_0")
				(number "P5")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "DONE_0")
				(number "J7")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "INIT_B_0")
				(number "G7")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "PROGRAM_B_0")
				(number "P6")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "CFGBVS_0")
				(number "P7")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "VP_0")
				(number "N12")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "VN_0")
				(number "P11")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 6.35)
				(name "VREFP_0")
				(number "P12")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "VREFN_0")
				(number "N11")
			)
			(pin bidirectional line
				(at 38.1 -35.56 180)
				(length 6.35)
				(name "DXP_0")
				(number "R12")
			)
			(pin bidirectional line
				(at 38.1 -38.1 180)
				(length 6.35)
				(name "DXN_0")
				(number "R11")
			)
		)
		(symbol "XC7K160T-FBG676_8_1"
			(pin power_in line
				(at -25.4 99.06 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 96.52 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M10")
			)
			(pin power_in line
				(at -25.4 93.98 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P10")
			)
			(pin power_in line
				(at -25.4 91.44 0)
				(length 6.35)
				(name "VCCAUX")
				(number "T10")
			)
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "T8")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "R9")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "P8")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "GNDADC_0")
				(number "M11")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCADC_0")
				(number "M12")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCBATT_0")
				(number "E8")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "N13")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "R13")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "T12")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "U13")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "GND")
				(number "A2")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "GND")
				(number "A5")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "GND")
				(number "A6")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "GND")
				(number "A7")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "GND")
				(number "A16")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "A26")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "B4")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "B23")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "C1")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "C5")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "C7")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "C10")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "C20")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "D7")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "D17")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "E1")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "E14")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E24")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "F3")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "F21")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G1")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "H25")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "J1")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "J5")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "J12")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "J22")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "K3")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "K4")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "K7")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "K11")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "K13")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "K19")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "L1")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "L10")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "L12")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "L14")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "L16")
			)
			(pin power_in line
				(at -25.4 -91.44 0)
				(length 6.35)
				(name "GND")
				(number "L26")
			)
			(pin power_in line
				(at -25.4 -93.98 0)
				(length 6.35)
				(name "GND")
				(number "M4")
			)
			(pin power_in line
				(at -25.4 -96.52 0)
				(length 6.35)
				(name "GND")
				(number "M7")
			)
			(pin power_in line
				(at -25.4 -99.06 0)
				(length 6.35)
				(name "GND")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 99.06 180)
				(length 6.35)
				(name "VCCINT")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 96.52 180)
				(length 6.35)
				(name "VCCINT")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 93.98 180)
				(length 6.35)
				(name "VCCINT")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 91.44 180)
				(length 6.35)
				(name "VCCINT")
				(number "K12")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "L13")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "L15")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "M8")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "R15")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "T14")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "U15")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "GND")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "GND")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "GND")
				(number "M23")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "GND")
				(number "N1")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "GND")
				(number "N5")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "N7")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "N20")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "P3")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "P4")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "P15")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "P17")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "R2")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "R8")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "R10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "R24")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "T1")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "T3")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "T4")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "T9")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "T11")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "T13")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "T15")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "T21")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "U8")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "U10")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U14")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "U18")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V5")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "V15")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "V25")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "W2")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "W12")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "W22")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "Y9")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "Y19")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AA6")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AA16")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AA26")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AB3")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AB13")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AB23")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "AC10")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "AC20")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "AD7")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "AD17")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "AE4")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "AE14")
			)
			(pin power_in line
				(at 25.4 -91.44 180)
				(length 6.35)
				(name "GND")
				(number "AE24")
			)
			(pin power_in line
				(at 25.4 -93.98 180)
				(length 6.35)
				(name "GND")
				(number "AF1")
			)
			(pin power_in line
				(at 25.4 -96.52 180)
				(length 6.35)
				(name "GND")
				(number "AF11")
			)
			(pin power_in line
				(at 25.4 -99.06 180)
				(length 6.35)
				(name "GND")
				(number "AF21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC7K160T-FFG676"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC7K160T-FFG676"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Kintex 7 T 160 XC7K160T-FFG676"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC7K160T-FFG676_1_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_12")
				(number "U21")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_12")
				(number "U22")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_12")
				(number "V22")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_12")
				(number "U24")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_12")
				(number "U25")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_12")
				(number "V23")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_12")
				(number "V24")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_12")
				(number "U26")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_12")
				(number "V26")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_12")
				(number "W25")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_12")
				(number "W26")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_12")
				(number "V21")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_12")
				(number "W21")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_12")
				(number "AA25")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_12")
				(number "AB25")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_12")
				(number "W23")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_12")
				(number "W24")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_12")
				(number "AB26")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_12")
				(number "AC26")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_12")
				(number "Y25")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_12")
				(number "Y26")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_12")
				(number "AA23")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_12")
				(number "AB24")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_12")
				(number "Y23")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_12")
				(number "AA24")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_12")
				(number "Y22")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_12")
				(number "AA22")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_12")
				(number "AC23")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_12")
				(number "AC24")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_12")
				(number "W20")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_12")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_12")
				(number "AD23")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_12")
				(number "AD24")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_12")
				(number "AB22")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_12")
				(number "AC22")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_12")
				(number "AB21")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_12")
				(number "AC21")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_12")
				(number "AD21")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_12")
				(number "AE21")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_12")
				(number "AF24")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_12")
				(number "AF25")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_12")
				(number "AD26")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_12")
				(number "AE26")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_12")
				(number "AE23")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_12")
				(number "AF23")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_12")
				(number "AD25")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_12")
				(number "AE25")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_12")
				(number "AE22")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_12")
				(number "AF22")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_12")
				(number "Y20")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AA21")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AC25")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AD22")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AF26")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "U23")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "V20")
			)
			(pin power_in line
				(at -25.4 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "Y24")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "K24")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "N25")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "P22")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "R19")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "T16")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "T26")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_13")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_13")
				(number "K25")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_13")
				(number "K26")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_13")
				(number "R26")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_13")
				(number "P26")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_13")
				(number "M25")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_13")
				(number "L25")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_13")
				(number "P24")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_13")
				(number "N24")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_13")
				(number "N26")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_13")
				(number "M26")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_13")
				(number "R25")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_13")
				(number "P25")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_13")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_13")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_13")
				(number "M24")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_13")
				(number "L24")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_13")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_13")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_13")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_13")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_13")
				(number "P23")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_13")
				(number "N23")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_13")
				(number "N21")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_13")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_13")
				(number "R21")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_13")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_13")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_13")
				(number "R23")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_13")
				(number "T24")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_13")
				(number "T25")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_13")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_13")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_13")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_13")
				(number "T23")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_13")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_13")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_13")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_13")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_13")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_13")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_13")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_13")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_13")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_13")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_13")
				(number "U17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_13")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_13")
				(number "R18")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_13")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_13")
				(number "U16")
			)
		)
		(symbol "XC7K160T-FFG676_2_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_14")
				(number "K21")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_D00_MOSI_14")
				(number "B24")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_D01_DIN_14")
				(number "A25")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_D02_14")
				(number "B22")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_D03_14")
				(number "A22")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_PUDC_B_14")
				(number "B25")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_EMCCLK_14")
				(number "B26")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_D04_14")
				(number "A23")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_D05_14")
				(number "A24")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_D06_14")
				(number "D26")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_D07_14")
				(number "C26")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_FCS_B_14")
				(number "C23")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_D08_VREF_14")
				(number "C24")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_D09_14")
				(number "D21")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_D10_14")
				(number "C22")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_D11_14")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_D12_14")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_14")
				(number "E21")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_D13_14")
				(number "E22")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_D14_14")
				(number "C21")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_D15_14")
				(number "B21")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_14")
				(number "D23")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_14")
				(number "D24")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_14")
				(number "F22")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_14")
				(number "E23")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_14")
				(number "G22")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_14")
				(number "F23")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_14")
				(number "G24")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_14")
				(number "F24")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_RDWR_B_14")
				(number "E25")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_DOUT_CSO_B_14")
				(number "D25")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_CSI_B_14")
				(number "G25")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_A15_D31_14")
				(number "G26")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_A14_D30_14")
				(number "F25")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_A13_D29_14")
				(number "E26")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_A12_D28_14")
				(number "J26")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_A11_D27_14")
				(number "H26")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_A10_D26_14")
				(number "H21")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_A09_D25_VREF_14")
				(number "G21")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_A08_D24_14")
				(number "H23")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_A07_D23_14")
				(number "H24")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_14")
				(number "J21")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A06_D22_14")
				(number "H22")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_A05_D21_14")
				(number "J24")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_A04_D20_14")
				(number "J25")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_A03_D19_14")
				(number "L22")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_A02_D18_14")
				(number "K22")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_A01_D17_14")
				(number "K23")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_A00_D16_14")
				(number "J23")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_14")
				(number "L23")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "A21")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "C25")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "D22")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "F26")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "G23")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "L21")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "B18")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "E19")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "F16")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "H20")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "J17")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_15")
				(number "K15")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_AD0P_15")
				(number "C16")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_AD0N_15")
				(number "B16")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_AD8P_15")
				(number "A18")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_AD8N_15")
				(number "A19")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_AD1P_15")
				(number "B17")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_AD1N_15")
				(number "A17")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_AD9P_15")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_AD9N_15")
				(number "B19")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_AD2P_15")
				(number "C17")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_AD2N_15")
				(number "C18")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_15")
				(number "D15")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_15")
				(number "D16")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_AD10P_15")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_AD10N_15")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_AD3P_15")
				(number "G15")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_AD3N_15")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_AD11P_15")
				(number "J15")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_AD11N_15")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_AD4P_15")
				(number "E15")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_AD4N_15")
				(number "E16")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_AD12P_15")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_AD12N_15")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_AD5P_15")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_AD5N_15")
				(number "E17")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_15")
				(number "E18")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_15")
				(number "D18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_15")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_15")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_15")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_ADV_B_15")
				(number "D20")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_A28_15")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_A27_15")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_A26_15")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_A25_15")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_A24_15")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_A23_15")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_A22_15")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_A21_VREF_15")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_A20_15")
				(number "J18")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_A19_15")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_15")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A18_15")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_A17_15")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_A16_15")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_FOE_B_15")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_FWE_B_15")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_RS1_15")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_RS0_15")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_15")
				(number "M16")
			)
		)
		(symbol "XC7K160T-FFG676_3_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_16")
				(number "J8")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_16")
				(number "H9")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_16")
				(number "H8")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_16")
				(number "G10")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_16")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_16")
				(number "J13")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_16")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_16")
				(number "J11")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_16")
				(number "J10")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_16")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_16")
				(number "G14")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_16")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_16")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_16")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_16")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_16")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_16")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_16")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_16")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_16")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_16")
				(number "B9")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_16")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_16")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_16")
				(number "E10")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_16")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_16")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_16")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_16")
				(number "E11")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_16")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_16")
				(number "F14")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_16")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_16")
				(number "G12")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_16")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_16")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_16")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_16")
				(number "E13")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_16")
				(number "E12")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_16")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_16")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_16")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_16")
				(number "B11")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_16")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_16")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_16")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_16")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_16")
				(number "B15")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_16")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_16")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_16")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_16")
				(number "J14")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "A11")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "B8")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "C15")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "D12")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "E9")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "G13")
			)
			(pin power_in line
				(at -25.4 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "H10")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AB18")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AC15")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AE19")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AF16")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "W17")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "Y14")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_32")
				(number "V13")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_32")
				(number "AE17")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_32")
				(number "AF17")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_32")
				(number "AF14")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_32")
				(number "AF15")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_32")
				(number "AE18")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_32")
				(number "AF18")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_32")
				(number "AD15")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_32")
				(number "AE15")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_32")
				(number "AF19")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_32")
				(number "AF20")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_32")
				(number "AD16")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_32")
				(number "AE16")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_32")
				(number "AA14")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_32")
				(number "AA15")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_32")
				(number "AC14")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_32")
				(number "AD14")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_32")
				(number "Y15")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_32")
				(number "Y16")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_32")
				(number "AB14")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_32")
				(number "AB15")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_32")
				(number "AA17")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_32")
				(number "AA18")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_32")
				(number "AB16")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_32")
				(number "AC16")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_32")
				(number "AC18")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_32")
				(number "AD18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_32")
				(number "AB17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_32")
				(number "AC17")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_32")
				(number "AD20")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_32")
				(number "AE20")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_32")
				(number "AA19")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_32")
				(number "AA20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_32")
				(number "AC19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_32")
				(number "AD19")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_32")
				(number "AB19")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_32")
				(number "AB20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_32")
				(number "Y17")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_32")
				(number "Y18")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_32")
				(number "V16")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_32")
				(number "V17")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_32")
				(number "W18")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_32")
				(number "W19")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_32")
				(number "W15")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_32")
				(number "W16")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_32")
				(number "V18")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_32")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_32")
				(number "V14")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_32")
				(number "W14")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_32")
				(number "W13")
			)
		)
		(symbol "XC7K160T-FFG676_4_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_VRN_33")
				(number "U9")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_33")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_33")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_33")
				(number "V8")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_33")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_33")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_33")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_33")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_33")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_33")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_33")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_33")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_33")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_33")
				(number "AE7")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_33")
				(number "AF7")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_33")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_33")
				(number "AA7")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_33")
				(number "AC8")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_33")
				(number "AD8")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_33")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_33")
				(number "AC7")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_33")
				(number "AA9")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_33")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_33")
				(number "AC9")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_33")
				(number "AD9")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_33")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_33")
				(number "AC11")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_33")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_33")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_33")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_33")
				(number "AC12")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_33")
				(number "AA13")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_33")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_33")
				(number "AC13")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_33")
				(number "AD13")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_33")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_33")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_33")
				(number "AD11")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_33")
				(number "AE11")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_33")
				(number "AD10")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_33")
				(number "AE10")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_33")
				(number "AE12")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_33")
				(number "AF12")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_33")
				(number "AE8")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_33")
				(number "AF8")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_33")
				(number "AE13")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_33")
				(number "AF13")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_33")
				(number "AF10")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_33")
				(number "AF9")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_VRP_33")
				(number "V12")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AA11")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AB8")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AD12")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AE9")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "V10")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "W7")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AA1")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AC5")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AD2")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AF6")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "U3")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "Y4")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_34")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_34")
				(number "U6")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_34")
				(number "U5")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_34")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_34")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_34")
				(number "W6")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_34")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_34")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_34")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_34")
				(number "U7")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_34")
				(number "V6")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_34")
				(number "V4")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_34")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_34")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_34")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_34")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_34")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_34")
				(number "AB1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_34")
				(number "AC1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_34")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_34")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_34")
				(number "AB2")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_34")
				(number "AC2")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_34")
				(number "AA3")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_34")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_34")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_34")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_34")
				(number "AC4")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_34")
				(number "AC3")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_34")
				(number "AA5")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_34")
				(number "AB5")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_34")
				(number "AB6")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_34")
				(number "AC6")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_34")
				(number "Y6")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_34")
				(number "Y5")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_34")
				(number "AD6")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_34")
				(number "AD5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_34")
				(number "AD4")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_34")
				(number "AD3")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_34")
				(number "AD1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_34")
				(number "AE1")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_34")
				(number "AF5")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_34")
				(number "AF4")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_34")
				(number "AE3")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_34")
				(number "AE2")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_34")
				(number "AE6")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_34")
				(number "AE5")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_34")
				(number "AF3")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_34")
				(number "AF2")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_34")
				(number "T7")
			)
		)
		(symbol "XC7K160T-FFG676_5_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_115")
				(number "P2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_115")
				(number "P1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_115")
				(number "M2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_115")
				(number "M1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_115")
				(number "K2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_115")
				(number "K1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_115")
				(number "H2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_115")
				(number "H1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_115")
				(number "R4")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_115")
				(number "R3")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_115")
				(number "N4")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_115")
				(number "N3")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_115")
				(number "L4")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_115")
				(number "L3")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_115")
				(number "J4")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_115")
				(number "J3")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_115")
				(number "H6")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_115")
				(number "H5")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_115")
				(number "K6")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_115")
				(number "K5")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_116")
				(number "F2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_116")
				(number "F1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_116")
				(number "D2")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_116")
				(number "D1")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_116")
				(number "B2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_116")
				(number "B1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_116")
				(number "A4")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_116")
				(number "A3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_116")
				(number "G4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_116")
				(number "G3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_116")
				(number "E4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_116")
				(number "E3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_116")
				(number "C4")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_116")
				(number "C3")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_116")
				(number "B6")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_116")
				(number "B5")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_116")
				(number "D6")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_116")
				(number "D5")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_116")
				(number "F6")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_116")
				(number "F5")
			)
		)
		(symbol "XC7K160T-FFG676_6_1"
			(pin power_in line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "C6")
			)
			(pin power_in line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "E6")
			)
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "G6")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "J6")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "L6")
			)
			(pin power_in line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTVCCAUX")
				(number "N6")
			)
			(pin power_in line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "B3")
			)
			(pin power_in line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "C2")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "D3")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "G2")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "H3")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "L2")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "M3")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTTRCAL_115")
				(number "M5")
			)
			(pin power_in line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTRREF_115")
				(number "M6")
			)
		)
		(symbol "XC7K160T-FFG676_7_1"
			(pin power_in line
				(at 25.4 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "L7")
			)
			(pin power_in line
				(at 27.94 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "T6")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "TDI_0")
				(number "R6")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "TDO_0")
				(number "R7")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "TMS_0")
				(number "N8")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TCK_0")
				(number "L8")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "CCLK_0")
				(number "C8")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "M0_0")
				(number "T5")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "M1_0")
				(number "T2")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "M2_0")
				(number "P5")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "DONE_0")
				(number "J7")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "INIT_B_0")
				(number "G7")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "PROGRAM_B_0")
				(number "P6")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "CFGBVS_0")
				(number "P7")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "VP_0")
				(number "N12")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "VN_0")
				(number "P11")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 6.35)
				(name "VREFP_0")
				(number "P12")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "VREFN_0")
				(number "N11")
			)
			(pin bidirectional line
				(at 38.1 -35.56 180)
				(length 6.35)
				(name "DXP_0")
				(number "R12")
			)
			(pin bidirectional line
				(at 38.1 -38.1 180)
				(length 6.35)
				(name "DXN_0")
				(number "R11")
			)
		)
		(symbol "XC7K160T-FFG676_8_1"
			(pin power_in line
				(at -25.4 99.06 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 96.52 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M10")
			)
			(pin power_in line
				(at -25.4 93.98 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P10")
			)
			(pin power_in line
				(at -25.4 91.44 0)
				(length 6.35)
				(name "VCCAUX")
				(number "T10")
			)
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "T8")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "R9")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "P8")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "GNDADC_0")
				(number "M11")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCADC_0")
				(number "M12")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCBATT_0")
				(number "E8")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "N13")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "R13")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "T12")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "U13")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "GND")
				(number "A2")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "GND")
				(number "A5")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "GND")
				(number "A6")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "GND")
				(number "A7")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "GND")
				(number "A16")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "A26")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "B4")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "B23")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "C1")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "C5")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "C7")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "C10")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "C20")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "D7")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "D17")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "E1")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "E14")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E24")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "F3")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "F21")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G1")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "H25")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "J1")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "J5")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "J12")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "J22")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "K3")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "K4")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "K7")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "K11")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "K13")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "K19")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "L1")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "L10")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "L12")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "L14")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "L16")
			)
			(pin power_in line
				(at -25.4 -91.44 0)
				(length 6.35)
				(name "GND")
				(number "L26")
			)
			(pin power_in line
				(at -25.4 -93.98 0)
				(length 6.35)
				(name "GND")
				(number "M4")
			)
			(pin power_in line
				(at -25.4 -96.52 0)
				(length 6.35)
				(name "GND")
				(number "M7")
			)
			(pin power_in line
				(at -25.4 -99.06 0)
				(length 6.35)
				(name "GND")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 99.06 180)
				(length 6.35)
				(name "VCCINT")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 96.52 180)
				(length 6.35)
				(name "VCCINT")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 93.98 180)
				(length 6.35)
				(name "VCCINT")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 91.44 180)
				(length 6.35)
				(name "VCCINT")
				(number "K12")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "L13")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "L15")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "M8")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "R15")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "T14")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "U15")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "GND")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "GND")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "GND")
				(number "M23")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "GND")
				(number "N1")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "GND")
				(number "N5")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "N7")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "N20")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "P3")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "P4")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "P15")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "P17")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "R2")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "R8")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "R10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "R24")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "T1")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "T3")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "T4")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "T9")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "T11")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "T13")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "T15")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "T21")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "U8")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "U10")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U14")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "U18")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V5")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "V15")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "V25")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "W2")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "W12")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "W22")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "Y9")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "Y19")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AA6")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AA16")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AA26")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AB3")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AB13")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AB23")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "AC10")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "AC20")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "AD7")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "AD17")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "AE4")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "AE14")
			)
			(pin power_in line
				(at 25.4 -91.44 180)
				(length 6.35)
				(name "GND")
				(number "AE24")
			)
			(pin power_in line
				(at 25.4 -93.98 180)
				(length 6.35)
				(name "GND")
				(number "AF1")
			)
			(pin power_in line
				(at 25.4 -96.52 180)
				(length 6.35)
				(name "GND")
				(number "AF11")
			)
			(pin power_in line
				(at 25.4 -99.06 180)
				(length 6.35)
				(name "GND")
				(number "AF21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC7K325T-FBG676"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC7K325T-FBG676"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Kintex 7 T 325 XC7K325T-FBG676"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC7K325T-FBG676_1_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_12")
				(number "U21")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_12")
				(number "U22")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_12")
				(number "V22")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_12")
				(number "U24")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_12")
				(number "U25")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_12")
				(number "V23")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_12")
				(number "V24")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_12")
				(number "U26")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_12")
				(number "V26")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_12")
				(number "W25")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_12")
				(number "W26")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_12")
				(number "V21")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_12")
				(number "W21")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_12")
				(number "AA25")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_12")
				(number "AB25")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_12")
				(number "W23")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_12")
				(number "W24")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_12")
				(number "AB26")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_12")
				(number "AC26")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_12")
				(number "Y25")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_12")
				(number "Y26")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_12")
				(number "AA23")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_12")
				(number "AB24")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_12")
				(number "Y23")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_12")
				(number "AA24")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_12")
				(number "Y22")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_12")
				(number "AA22")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_12")
				(number "AC23")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_12")
				(number "AC24")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_12")
				(number "W20")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_12")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_12")
				(number "AD23")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_12")
				(number "AD24")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_12")
				(number "AB22")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_12")
				(number "AC22")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_12")
				(number "AB21")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_12")
				(number "AC21")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_12")
				(number "AD21")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_12")
				(number "AE21")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_12")
				(number "AF24")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_12")
				(number "AF25")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_12")
				(number "AD26")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_12")
				(number "AE26")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_12")
				(number "AE23")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_12")
				(number "AF23")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_12")
				(number "AD25")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_12")
				(number "AE25")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_12")
				(number "AE22")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_12")
				(number "AF22")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_12")
				(number "Y20")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AA21")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AC25")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AD22")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AF26")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "U23")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "V20")
			)
			(pin power_in line
				(at -25.4 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "Y24")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "K24")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "N25")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "P22")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "R19")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "T16")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "T26")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_13")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_13")
				(number "K25")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_13")
				(number "K26")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_13")
				(number "R26")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_13")
				(number "P26")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_13")
				(number "M25")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_13")
				(number "L25")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_13")
				(number "P24")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_13")
				(number "N24")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_13")
				(number "N26")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_13")
				(number "M26")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_13")
				(number "R25")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_13")
				(number "P25")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_13")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_13")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_13")
				(number "M24")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_13")
				(number "L24")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_13")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_13")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_13")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_13")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_13")
				(number "P23")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_13")
				(number "N23")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_13")
				(number "N21")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_13")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_13")
				(number "R21")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_13")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_13")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_13")
				(number "R23")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_13")
				(number "T24")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_13")
				(number "T25")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_13")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_13")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_13")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_13")
				(number "T23")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_13")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_13")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_13")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_13")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_13")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_13")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_13")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_13")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_13")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_13")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_13")
				(number "U17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_13")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_13")
				(number "R18")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_13")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_13")
				(number "U16")
			)
		)
		(symbol "XC7K325T-FBG676_2_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_14")
				(number "K21")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_D00_MOSI_14")
				(number "B24")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_D01_DIN_14")
				(number "A25")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_D02_14")
				(number "B22")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_D03_14")
				(number "A22")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_PUDC_B_14")
				(number "B25")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_EMCCLK_14")
				(number "B26")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_D04_14")
				(number "A23")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_D05_14")
				(number "A24")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_D06_14")
				(number "D26")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_D07_14")
				(number "C26")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_FCS_B_14")
				(number "C23")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_D08_VREF_14")
				(number "C24")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_D09_14")
				(number "D21")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_D10_14")
				(number "C22")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_D11_14")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_D12_14")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_14")
				(number "E21")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_D13_14")
				(number "E22")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_D14_14")
				(number "C21")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_D15_14")
				(number "B21")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_14")
				(number "D23")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_14")
				(number "D24")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_14")
				(number "F22")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_14")
				(number "E23")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_14")
				(number "G22")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_14")
				(number "F23")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_14")
				(number "G24")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_14")
				(number "F24")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_RDWR_B_14")
				(number "E25")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_DOUT_CSO_B_14")
				(number "D25")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_CSI_B_14")
				(number "G25")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_A15_D31_14")
				(number "G26")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_A14_D30_14")
				(number "F25")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_A13_D29_14")
				(number "E26")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_A12_D28_14")
				(number "J26")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_A11_D27_14")
				(number "H26")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_A10_D26_14")
				(number "H21")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_A09_D25_VREF_14")
				(number "G21")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_A08_D24_14")
				(number "H23")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_A07_D23_14")
				(number "H24")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_14")
				(number "J21")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A06_D22_14")
				(number "H22")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_A05_D21_14")
				(number "J24")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_A04_D20_14")
				(number "J25")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_A03_D19_14")
				(number "L22")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_A02_D18_14")
				(number "K22")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_A01_D17_14")
				(number "K23")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_A00_D16_14")
				(number "J23")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_14")
				(number "L23")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "A21")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "C25")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "D22")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "F26")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "G23")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "L21")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "B18")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "E19")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "F16")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "H20")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "J17")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_15")
				(number "K15")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_AD0P_15")
				(number "C16")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_AD0N_15")
				(number "B16")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_AD8P_15")
				(number "A18")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_AD8N_15")
				(number "A19")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_AD1P_15")
				(number "B17")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_AD1N_15")
				(number "A17")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_AD9P_15")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_AD9N_15")
				(number "B19")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_AD2P_15")
				(number "C17")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_AD2N_15")
				(number "C18")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_15")
				(number "D15")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_15")
				(number "D16")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_AD10P_15")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_AD10N_15")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_AD3P_15")
				(number "G15")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_AD3N_15")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_AD11P_15")
				(number "J15")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_AD11N_15")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_AD4P_15")
				(number "E15")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_AD4N_15")
				(number "E16")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_AD12P_15")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_AD12N_15")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_AD5P_15")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_AD5N_15")
				(number "E17")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_15")
				(number "E18")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_15")
				(number "D18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_15")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_15")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_15")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_ADV_B_15")
				(number "D20")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_A28_15")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_A27_15")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_A26_15")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_A25_15")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_A24_15")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_A23_15")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_A22_15")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_A21_VREF_15")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_A20_15")
				(number "J18")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_A19_15")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_15")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A18_15")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_A17_15")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_A16_15")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_FOE_B_15")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_FWE_B_15")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_RS1_15")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_RS0_15")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_15")
				(number "M16")
			)
		)
		(symbol "XC7K325T-FBG676_3_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_16")
				(number "J8")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_16")
				(number "H9")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_16")
				(number "H8")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_16")
				(number "G10")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_16")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_16")
				(number "J13")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_16")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_16")
				(number "J11")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_16")
				(number "J10")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_16")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_16")
				(number "G14")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_16")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_16")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_16")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_16")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_16")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_16")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_16")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_16")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_16")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_16")
				(number "B9")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_16")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_16")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_16")
				(number "E10")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_16")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_16")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_16")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_16")
				(number "E11")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_16")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_16")
				(number "F14")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_16")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_16")
				(number "G12")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_16")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_16")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_16")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_16")
				(number "E13")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_16")
				(number "E12")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_16")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_16")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_16")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_16")
				(number "B11")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_16")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_16")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_16")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_16")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_16")
				(number "B15")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_16")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_16")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_16")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_16")
				(number "J14")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "A11")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "B8")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "C15")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "D12")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "E9")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "G13")
			)
			(pin power_in line
				(at -25.4 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "H10")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AB18")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AC15")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AE19")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AF16")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "W17")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "Y14")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_32")
				(number "V13")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_32")
				(number "AE17")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_32")
				(number "AF17")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_32")
				(number "AF14")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_32")
				(number "AF15")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_32")
				(number "AE18")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_32")
				(number "AF18")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_32")
				(number "AD15")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_32")
				(number "AE15")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_32")
				(number "AF19")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_32")
				(number "AF20")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_32")
				(number "AD16")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_32")
				(number "AE16")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_32")
				(number "AA14")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_32")
				(number "AA15")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_32")
				(number "AC14")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_32")
				(number "AD14")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_32")
				(number "Y15")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_32")
				(number "Y16")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_32")
				(number "AB14")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_32")
				(number "AB15")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_32")
				(number "AA17")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_32")
				(number "AA18")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_32")
				(number "AB16")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_32")
				(number "AC16")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_32")
				(number "AC18")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_32")
				(number "AD18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_32")
				(number "AB17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_32")
				(number "AC17")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_32")
				(number "AD20")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_32")
				(number "AE20")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_32")
				(number "AA19")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_32")
				(number "AA20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_32")
				(number "AC19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_32")
				(number "AD19")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_32")
				(number "AB19")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_32")
				(number "AB20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_32")
				(number "Y17")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_32")
				(number "Y18")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_32")
				(number "V16")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_32")
				(number "V17")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_32")
				(number "W18")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_32")
				(number "W19")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_32")
				(number "W15")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_32")
				(number "W16")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_32")
				(number "V18")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_32")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_32")
				(number "V14")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_32")
				(number "W14")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_32")
				(number "W13")
			)
		)
		(symbol "XC7K325T-FBG676_4_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_VRN_33")
				(number "U9")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_33")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_33")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_33")
				(number "V8")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_33")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_33")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_33")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_33")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_33")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_33")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_33")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_33")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_33")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_33")
				(number "AE7")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_33")
				(number "AF7")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_33")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_33")
				(number "AA7")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_33")
				(number "AC8")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_33")
				(number "AD8")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_33")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_33")
				(number "AC7")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_33")
				(number "AA9")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_33")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_33")
				(number "AC9")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_33")
				(number "AD9")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_33")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_33")
				(number "AC11")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_33")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_33")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_33")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_33")
				(number "AC12")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_33")
				(number "AA13")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_33")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_33")
				(number "AC13")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_33")
				(number "AD13")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_33")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_33")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_33")
				(number "AD11")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_33")
				(number "AE11")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_33")
				(number "AD10")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_33")
				(number "AE10")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_33")
				(number "AE12")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_33")
				(number "AF12")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_33")
				(number "AE8")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_33")
				(number "AF8")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_33")
				(number "AE13")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_33")
				(number "AF13")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_33")
				(number "AF10")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_33")
				(number "AF9")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_VRP_33")
				(number "V12")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AA11")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AB8")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AD12")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AE9")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "V10")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "W7")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AA1")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AC5")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AD2")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AF6")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "U3")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "Y4")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_34")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_34")
				(number "U6")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_34")
				(number "U5")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_34")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_34")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_34")
				(number "W6")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_34")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_34")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_34")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_34")
				(number "U7")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_34")
				(number "V6")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_34")
				(number "V4")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_34")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_34")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_34")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_34")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_34")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_34")
				(number "AB1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_34")
				(number "AC1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_34")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_34")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_34")
				(number "AB2")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_34")
				(number "AC2")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_34")
				(number "AA3")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_34")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_34")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_34")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_34")
				(number "AC4")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_34")
				(number "AC3")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_34")
				(number "AA5")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_34")
				(number "AB5")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_34")
				(number "AB6")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_34")
				(number "AC6")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_34")
				(number "Y6")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_34")
				(number "Y5")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_34")
				(number "AD6")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_34")
				(number "AD5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_34")
				(number "AD4")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_34")
				(number "AD3")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_34")
				(number "AD1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_34")
				(number "AE1")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_34")
				(number "AF5")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_34")
				(number "AF4")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_34")
				(number "AE3")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_34")
				(number "AE2")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_34")
				(number "AE6")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_34")
				(number "AE5")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_34")
				(number "AF3")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_34")
				(number "AF2")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_34")
				(number "T7")
			)
		)
		(symbol "XC7K325T-FBG676_5_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_115")
				(number "P2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_115")
				(number "P1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_115")
				(number "M2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_115")
				(number "M1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_115")
				(number "K2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_115")
				(number "K1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_115")
				(number "H2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_115")
				(number "H1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_115")
				(number "R4")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_115")
				(number "R3")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_115")
				(number "N4")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_115")
				(number "N3")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_115")
				(number "L4")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_115")
				(number "L3")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_115")
				(number "J4")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_115")
				(number "J3")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_115")
				(number "H6")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_115")
				(number "H5")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_115")
				(number "K6")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_115")
				(number "K5")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_116")
				(number "F2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_116")
				(number "F1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_116")
				(number "D2")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_116")
				(number "D1")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_116")
				(number "B2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_116")
				(number "B1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_116")
				(number "A4")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_116")
				(number "A3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_116")
				(number "G4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_116")
				(number "G3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_116")
				(number "E4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_116")
				(number "E3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_116")
				(number "C4")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_116")
				(number "C3")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_116")
				(number "B6")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_116")
				(number "B5")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_116")
				(number "D6")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_116")
				(number "D5")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_116")
				(number "F6")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_116")
				(number "F5")
			)
		)
		(symbol "XC7K325T-FBG676_6_1"
			(pin power_in line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "C6")
			)
			(pin power_in line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "E6")
			)
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "G6")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "J6")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "L6")
			)
			(pin power_in line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTVCCAUX")
				(number "N6")
			)
			(pin power_in line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "B3")
			)
			(pin power_in line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "C2")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "D3")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "G2")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "H3")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "L2")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "M3")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTTRCAL_115")
				(number "M5")
			)
			(pin power_in line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTRREF_115")
				(number "M6")
			)
		)
		(symbol "XC7K325T-FBG676_7_1"
			(pin power_in line
				(at 25.4 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "L7")
			)
			(pin power_in line
				(at 27.94 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "T6")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "TDI_0")
				(number "R6")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "TDO_0")
				(number "R7")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "TMS_0")
				(number "N8")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TCK_0")
				(number "L8")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "CCLK_0")
				(number "C8")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "M0_0")
				(number "T5")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "M1_0")
				(number "T2")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "M2_0")
				(number "P5")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "DONE_0")
				(number "J7")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "INIT_B_0")
				(number "G7")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "PROGRAM_B_0")
				(number "P6")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "CFGBVS_0")
				(number "P7")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "VP_0")
				(number "N12")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "VN_0")
				(number "P11")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 6.35)
				(name "VREFP_0")
				(number "P12")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "VREFN_0")
				(number "N11")
			)
			(pin bidirectional line
				(at 38.1 -35.56 180)
				(length 6.35)
				(name "DXP_0")
				(number "R12")
			)
			(pin bidirectional line
				(at 38.1 -38.1 180)
				(length 6.35)
				(name "DXN_0")
				(number "R11")
			)
		)
		(symbol "XC7K325T-FBG676_8_1"
			(pin power_in line
				(at -25.4 99.06 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 96.52 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M10")
			)
			(pin power_in line
				(at -25.4 93.98 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P10")
			)
			(pin power_in line
				(at -25.4 91.44 0)
				(length 6.35)
				(name "VCCAUX")
				(number "T10")
			)
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "T8")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "R9")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "P8")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "GNDADC_0")
				(number "M11")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCADC_0")
				(number "M12")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCBATT_0")
				(number "E8")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "N13")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "R13")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "T12")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "U13")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "GND")
				(number "A2")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "GND")
				(number "A5")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "GND")
				(number "A6")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "GND")
				(number "A7")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "GND")
				(number "A16")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "A26")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "B4")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "B23")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "C1")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "C5")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "C7")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "C10")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "C20")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "D7")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "D17")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "E1")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "E14")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E24")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "F3")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "F21")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G1")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "H25")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "J1")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "J5")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "J12")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "J22")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "K3")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "K4")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "K7")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "K11")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "K13")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "K19")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "L1")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "L10")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "L12")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "L14")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "L16")
			)
			(pin power_in line
				(at -25.4 -91.44 0)
				(length 6.35)
				(name "GND")
				(number "L26")
			)
			(pin power_in line
				(at -25.4 -93.98 0)
				(length 6.35)
				(name "GND")
				(number "M4")
			)
			(pin power_in line
				(at -25.4 -96.52 0)
				(length 6.35)
				(name "GND")
				(number "M7")
			)
			(pin power_in line
				(at -25.4 -99.06 0)
				(length 6.35)
				(name "GND")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 99.06 180)
				(length 6.35)
				(name "VCCINT")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 96.52 180)
				(length 6.35)
				(name "VCCINT")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 93.98 180)
				(length 6.35)
				(name "VCCINT")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 91.44 180)
				(length 6.35)
				(name "VCCINT")
				(number "K12")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "L13")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "L15")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "M8")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "R15")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "T14")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "U15")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "GND")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "GND")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "GND")
				(number "M23")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "GND")
				(number "N1")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "GND")
				(number "N5")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "N7")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "N20")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "P3")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "P4")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "P15")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "P17")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "R2")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "R8")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "R10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "R24")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "T1")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "T3")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "T4")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "T9")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "T11")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "T13")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "T15")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "T21")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "U8")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "U10")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U14")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "U18")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V5")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "V15")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "V25")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "W2")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "W12")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "W22")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "Y9")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "Y19")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AA6")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AA16")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AA26")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AB3")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AB13")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AB23")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "AC10")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "AC20")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "AD7")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "AD17")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "AE4")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "AE14")
			)
			(pin power_in line
				(at 25.4 -91.44 180)
				(length 6.35)
				(name "GND")
				(number "AE24")
			)
			(pin power_in line
				(at 25.4 -93.98 180)
				(length 6.35)
				(name "GND")
				(number "AF1")
			)
			(pin power_in line
				(at 25.4 -96.52 180)
				(length 6.35)
				(name "GND")
				(number "AF11")
			)
			(pin power_in line
				(at 25.4 -99.06 180)
				(length 6.35)
				(name "GND")
				(number "AF21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC7K325T-FBG900"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC7K325T-FBG900"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Kintex 7 T 325 XC7K325T-FBG900"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC7K325T-FBG900_1_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_12")
				(number "Y20")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_12")
				(number "Y23")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_12")
				(number "Y24")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_12")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_12")
				(number "AA21")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_12")
				(number "AB22")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_12")
				(number "AB23")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_12")
				(number "AA22")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_12")
				(number "AA23")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_12")
				(number "AC20")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_12")
				(number "AC21")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_12")
				(number "AA20")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_12")
				(number "AB20")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_12")
				(number "AB24")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_12")
				(number "AC25")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_12")
				(number "AC22")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_12")
				(number "AD22")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_12")
				(number "AC24")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_12")
				(number "AD24")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_12")
				(number "AD21")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_12")
				(number "AE21")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_12")
				(number "AE23")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_12")
				(number "AF23")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_12")
				(number "AD23")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_12")
				(number "AE24")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_12")
				(number "AF22")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_12")
				(number "AG23")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_12")
				(number "AG24")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_12")
				(number "AH24")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_12")
				(number "AJ24")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_12")
				(number "AK25")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_12")
				(number "AE25")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_12")
				(number "AF25")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_12")
				(number "AK23")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_12")
				(number "AK24")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_12")
				(number "AG25")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_12")
				(number "AH25")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_12")
				(number "AF20")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_12")
				(number "AF21")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_12")
				(number "AG22")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_12")
				(number "AH22")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_12")
				(number "AJ22")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_12")
				(number "AJ23")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_12")
				(number "AG20")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_12")
				(number "AH20")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_12")
				(number "AH21")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_12")
				(number "AJ21")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_12")
				(number "AK20")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_12")
				(number "AK21")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_12")
				(number "AE20")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AC23")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AD20")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AF24")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AG21")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AK22")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "Y22")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AA29")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AB26")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AD30")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AE27")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AH28")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AJ25")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_13")
				(number "Y25")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_13")
				(number "Y26")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_13")
				(number "AA26")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_13")
				(number "W27")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_13")
				(number "W28")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_13")
				(number "Y28")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_13")
				(number "AA28")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_13")
				(number "W29")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_13")
				(number "Y29")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_13")
				(number "AA27")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_13")
				(number "AB28")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_13")
				(number "AA25")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_13")
				(number "AB25")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_13")
				(number "AC29")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_13")
				(number "AC30")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_13")
				(number "Y30")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_13")
				(number "AA30")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_13")
				(number "AD29")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_13")
				(number "AE29")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_13")
				(number "AB29")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_13")
				(number "AB30")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_13")
				(number "AD27")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_13")
				(number "AD28")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_13")
				(number "AB27")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_13")
				(number "AC27")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_13")
				(number "AG29")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_13")
				(number "AH29")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_13")
				(number "AE28")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_13")
				(number "AF28")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_13")
				(number "AK29")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_13")
				(number "AK30")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_13")
				(number "AE30")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_13")
				(number "AF30")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_13")
				(number "AJ28")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_13")
				(number "AJ29")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_13")
				(number "AG30")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_13")
				(number "AH30")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_13")
				(number "AC26")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_13")
				(number "AD26")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_13")
				(number "AJ27")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_13")
				(number "AK28")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_13")
				(number "AG27")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_13")
				(number "AG28")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_13")
				(number "AH26")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_13")
				(number "AH27")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_13")
				(number "AF26")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_13")
				(number "AF27")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_13")
				(number "AJ26")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_13")
				(number "AK26")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_13")
				(number "AE26")
			)
		)
		(symbol "XC7K325T-FBG900_2_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_14")
				(number "R19")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_D00_MOSI_14")
				(number "P24")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_D01_DIN_14")
				(number "R25")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_D02_14")
				(number "R20")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_D03_14")
				(number "R21")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_PUDC_B_14")
				(number "R23")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_EMCCLK_14")
				(number "R24")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_D04_14")
				(number "T20")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_D05_14")
				(number "T21")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_D06_14")
				(number "T22")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_D07_14")
				(number "T23")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_FCS_B_14")
				(number "U19")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_D08_VREF_14")
				(number "U20")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_D09_14")
				(number "P29")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_D10_14")
				(number "R29")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_D11_14")
				(number "P27")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_D12_14")
				(number "P28")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_14")
				(number "R30")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_D13_14")
				(number "T30")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_D14_14")
				(number "P26")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_D15_14")
				(number "R26")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_14")
				(number "R28")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_14")
				(number "T28")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_14")
				(number "T26")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_14")
				(number "T27")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_14")
				(number "U27")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_14")
				(number "U28")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_14")
				(number "T25")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_14")
				(number "U25")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_RDWR_B_14")
				(number "U29")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_DOUT_CSO_B_14")
				(number "U30")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_CSI_B_14")
				(number "V26")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_A15_D31_14")
				(number "V27")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_A14_D30_14")
				(number "V29")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_A13_D29_14")
				(number "V30")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_A12_D28_14")
				(number "V25")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_A11_D27_14")
				(number "W26")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_A10_D26_14")
				(number "V19")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_A09_D25_VREF_14")
				(number "V20")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_A08_D24_14")
				(number "W23")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_A07_D23_14")
				(number "W24")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_14")
				(number "U22")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A06_D22_14")
				(number "U23")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_A05_D21_14")
				(number "V21")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_A04_D20_14")
				(number "V22")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_A03_D19_14")
				(number "U24")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_A02_D18_14")
				(number "V24")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_A01_D17_14")
				(number "W21")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_A00_D16_14")
				(number "W22")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_14")
				(number "W19")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "P30")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "R27")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "T24")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "U21")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "V28")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "W25")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "J25")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "K22")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "L29")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "M26")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "N23")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_15")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_AD0P_15")
				(number "J23")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_AD0N_15")
				(number "J24")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_AD8P_15")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_AD8N_15")
				(number "L23")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_AD1P_15")
				(number "K23")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_AD1N_15")
				(number "K24")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_AD9P_15")
				(number "L21")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_AD9N_15")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_AD2P_15")
				(number "J21")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_AD2N_15")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_15")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_15")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_AD10P_15")
				(number "J29")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_AD10N_15")
				(number "H29")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_AD3P_15")
				(number "J27")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_AD3N_15")
				(number "J28")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_AD11P_15")
				(number "L30")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_AD11N_15")
				(number "K30")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_AD4P_15")
				(number "K26")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_AD4N_15")
				(number "J26")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_AD12P_15")
				(number "L26")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_AD12N_15")
				(number "L27")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_AD5P_15")
				(number "L25")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_AD5N_15")
				(number "K25")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_15")
				(number "K28")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_15")
				(number "K29")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_15")
				(number "M28")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_15")
				(number "L28")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_15")
				(number "M29")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_ADV_B_15")
				(number "M30")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_A28_15")
				(number "N27")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_A27_15")
				(number "M27")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_A26_15")
				(number "N29")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_A25_15")
				(number "N30")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_A24_15")
				(number "N25")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_A23_15")
				(number "N26")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_A22_15")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_A21_VREF_15")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_A20_15")
				(number "N21")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_A19_15")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_15")
				(number "P23")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A18_15")
				(number "N24")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_A17_15")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_A16_15")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_FOE_B_15")
				(number "M24")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_FWE_B_15")
				(number "M25")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_RS1_15")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_RS0_15")
				(number "M23")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_15")
				(number "P19")
			)
		)
		(symbol "XC7K325T-FBG900_3_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_16")
				(number "F23")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_16")
				(number "B23")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_16")
				(number "A23")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_16")
				(number "E23")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_16")
				(number "D23")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_16")
				(number "F25")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_16")
				(number "E25")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_16")
				(number "E24")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_16")
				(number "D24")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_16")
				(number "F26")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_16")
				(number "E26")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_16")
				(number "G23")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_16")
				(number "G24")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_16")
				(number "B27")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_16")
				(number "A27")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_16")
				(number "C24")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_16")
				(number "B24")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_16")
				(number "B28")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_16")
				(number "A28")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_16")
				(number "A25")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_16")
				(number "A26")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_16")
				(number "D26")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_16")
				(number "C26")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_16")
				(number "C25")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_16")
				(number "B25")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_16")
				(number "D27")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_16")
				(number "C27")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_16")
				(number "E28")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_16")
				(number "D28")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_16")
				(number "C29")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_16")
				(number "B29")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_16")
				(number "D29")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_16")
				(number "C30")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_16")
				(number "B30")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_16")
				(number "A30")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_16")
				(number "E29")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_16")
				(number "E30")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_16")
				(number "H24")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_16")
				(number "H25")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_16")
				(number "G28")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_16")
				(number "F28")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_16")
				(number "G27")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_16")
				(number "F27")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_16")
				(number "G29")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_16")
				(number "F30")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_16")
				(number "H26")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_16")
				(number "H27")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_16")
				(number "H30")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_16")
				(number "G30")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_16")
				(number "G25")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "A29")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "B26")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "C23")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "D30")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "E27")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "F24")
			)
			(pin power_in line
				(at -25.4 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "H28")
			)
			(pin power_in line
				(at 25.4 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "A19")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "B16")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "D20")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "E17")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "G21")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "H18")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_17")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_17")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_17")
				(number "J18")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_17")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_17")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_17")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_17")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_17")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_17")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_17")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_17")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_17")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_17")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_17")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_17")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_17")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_17")
				(number "C21")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_17")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_17")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_17")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_17")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_17")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_17")
				(number "E21")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_17")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_17")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_17")
				(number "D17")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_17")
				(number "D18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_17")
				(number "E19")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_17")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_17")
				(number "D16")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_17")
				(number "C16")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_17")
				(number "G18")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_17")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_17")
				(number "C17")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_17")
				(number "B17")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_17")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_17")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_17")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_17")
				(number "B20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_17")
				(number "A16")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_17")
				(number "A17")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_17")
				(number "A20")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_17")
				(number "A21")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_17")
				(number "B18")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_17")
				(number "A18")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_17")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_17")
				(number "A22")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_17")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_17")
				(number "B19")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_17")
				(number "E18")
			)
		)
		(symbol "XC7K325T-FBG900_4_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_18")
				(number "G12")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_18")
				(number "L16")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_18")
				(number "K16")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_18")
				(number "L15")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_18")
				(number "K15")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_18")
				(number "L12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_18")
				(number "L13")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_18")
				(number "K13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_18")
				(number "J13")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_18")
				(number "K14")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_18")
				(number "J14")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_18")
				(number "L11")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_18")
				(number "K11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_18")
				(number "H15")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_18")
				(number "G15")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_18")
				(number "J11")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_18")
				(number "J12")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_18")
				(number "J16")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_18")
				(number "H16")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_18")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_18")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_18")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_18")
				(number "G14")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_18")
				(number "G13")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_18")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_18")
				(number "D12")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_18")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_18")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_18")
				(number "E13")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_18")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_18")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_18")
				(number "F11")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_18")
				(number "E11")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_18")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_18")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_18")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_18")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_18")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_18")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_18")
				(number "E14")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_18")
				(number "E15")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_18")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_18")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_18")
				(number "B13")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_18")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_18")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_18")
				(number "B15")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_18")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_18")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_18")
				(number "F16")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "C13")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "D10")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "F14")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "G11")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "J15")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "K12")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AA19")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AB16")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AE17")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AF14")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AH18")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AJ15")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_32")
				(number "Y14")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_32")
				(number "AK16")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_32")
				(number "AK15")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_32")
				(number "AG15")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_32")
				(number "AH15")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_32")
				(number "AH16")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_32")
				(number "AJ16")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_32")
				(number "AF15")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_32")
				(number "AG14")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_32")
				(number "AH17")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_32")
				(number "AJ17")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_32")
				(number "AE16")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_32")
				(number "AF16")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_32")
				(number "AJ19")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_32")
				(number "AK19")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_32")
				(number "AG19")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_32")
				(number "AH19")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_32")
				(number "AJ18")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_32")
				(number "AK18")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_32")
				(number "AD19")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_32")
				(number "AE19")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_32")
				(number "AF18")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_32")
				(number "AG18")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_32")
				(number "AF17")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_32")
				(number "AG17")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_32")
				(number "AD18")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_32")
				(number "AE18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_32")
				(number "AD17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_32")
				(number "AD16")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_32")
				(number "Y19")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_32")
				(number "Y18")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_32")
				(number "AA18")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_32")
				(number "AB18")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_32")
				(number "AB19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_32")
				(number "AC19")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_32")
				(number "AB17")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_32")
				(number "AC17")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_32")
				(number "AE15")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_32")
				(number "AE14")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_32")
				(number "AA15")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_32")
				(number "AB15")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_32")
				(number "AC16")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_32")
				(number "AC15")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_32")
				(number "AC14")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_32")
				(number "AD14")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_32")
				(number "AA17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_32")
				(number "AA16")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_32")
				(number "Y16")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_32")
				(number "Y15")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_32")
				(number "AB14")
			)
		)
		(symbol "XC7K325T-FBG900_5_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_VRN_33")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_33")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_33")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_33")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_33")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_33")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_33")
				(number "AC9")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_33")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_33")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_33")
				(number "AA11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_33")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_33")
				(number "AA13")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_33")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_33")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_33")
				(number "AC10")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_33")
				(number "AD8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_33")
				(number "AE8")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_33")
				(number "AC12")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_33")
				(number "AC11")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_33")
				(number "AD9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_33")
				(number "AE9")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_33")
				(number "AE11")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_33")
				(number "AF11")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_33")
				(number "AD12")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_33")
				(number "AD11")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_33")
				(number "AG10")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_33")
				(number "AH10")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_33")
				(number "AE10")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_33")
				(number "AF10")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_33")
				(number "AJ9")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_33")
				(number "AK9")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_33")
				(number "AG9")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_33")
				(number "AH9")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_33")
				(number "AK11")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_33")
				(number "AK10")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_33")
				(number "AH11")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_33")
				(number "AJ11")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_33")
				(number "AE13")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_33")
				(number "AF13")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_33")
				(number "AK14")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_33")
				(number "AK13")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_33")
				(number "AH14")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_33")
				(number "AJ14")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_33")
				(number "AJ13")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_33")
				(number "AJ12")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_33")
				(number "AF12")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_33")
				(number "AG12")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_33")
				(number "AG13")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_33")
				(number "AH12")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_VRP_33")
				(number "AD13")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AA9")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AC13")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AD10")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AG11")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AK12")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "Y12")
			)
			(pin power_in line
				(at 25.4 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AC3")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AE7")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AF4")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AG1")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AH8")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AJ5")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AK2")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_34")
				(number "AC6")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_34")
				(number "AD4")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_34")
				(number "AD3")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_34")
				(number "AC2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_34")
				(number "AC1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_34")
				(number "AD2")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_34")
				(number "AD1")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_34")
				(number "AC5")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_34")
				(number "AC4")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_34")
				(number "AD6")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_34")
				(number "AE6")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_34")
				(number "AC7")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_34")
				(number "AD7")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_34")
				(number "AF3")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_34")
				(number "AF2")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_34")
				(number "AE1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_34")
				(number "AF1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_34")
				(number "AG4")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_34")
				(number "AG3")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_34")
				(number "AE4")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_34")
				(number "AE3")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_34")
				(number "AE5")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_34")
				(number "AF5")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_34")
				(number "AF6")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_34")
				(number "AG5")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_34")
				(number "AH4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_34")
				(number "AJ4")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_34")
				(number "AH6")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_34")
				(number "AH5")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_34")
				(number "AG2")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_34")
				(number "AH1")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_34")
				(number "AH2")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_34")
				(number "AJ2")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_34")
				(number "AJ1")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_34")
				(number "AK1")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_34")
				(number "AJ3")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_34")
				(number "AK3")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_34")
				(number "AF8")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_34")
				(number "AG8")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_34")
				(number "AF7")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_34")
				(number "AG7")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_34")
				(number "AH7")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_34")
				(number "AJ7")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_34")
				(number "AJ6")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_34")
				(number "AK6")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_34")
				(number "AJ8")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_34")
				(number "AK8")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_34")
				(number "AK5")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_34")
				(number "AK4")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_34")
				(number "AB7")
			)
		)
		(symbol "XC7K325T-FBG900_6_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_115")
				(number "Y2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_115")
				(number "Y1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_115")
				(number "V2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_115")
				(number "V1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_115")
				(number "U4")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_115")
				(number "U3")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_115")
				(number "T2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_115")
				(number "T1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_115")
				(number "AA4")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_115")
				(number "AA3")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_115")
				(number "Y6")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_115")
				(number "Y5")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_115")
				(number "W4")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_115")
				(number "W3")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_115")
				(number "V6")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_115")
				(number "V5")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_115")
				(number "R8")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_115")
				(number "R7")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_115")
				(number "U8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_115")
				(number "U7")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_116")
				(number "P2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_116")
				(number "P1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_116")
				(number "N4")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_116")
				(number "N3")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_116")
				(number "M2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_116")
				(number "M1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_116")
				(number "L4")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_116")
				(number "L3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_116")
				(number "T6")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_116")
				(number "T5")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_116")
				(number "R4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_116")
				(number "R3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_116")
				(number "P6")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_116")
				(number "P5")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_116")
				(number "M6")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_116")
				(number "M5")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_116")
				(number "L8")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_116")
				(number "L7")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_116")
				(number "N8")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_116")
				(number "N7")
			)
		)
		(symbol "XC7K325T-FBG900_7_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_117")
				(number "K2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_117")
				(number "K1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_117")
				(number "J4")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_117")
				(number "J3")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_117")
				(number "H2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_117")
				(number "H1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_117")
				(number "F2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_117")
				(number "F1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_117")
				(number "K6")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_117")
				(number "K5")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_117")
				(number "H6")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_117")
				(number "H5")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_117")
				(number "G4")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_117")
				(number "G3")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_117")
				(number "F6")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_117")
				(number "F5")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_117")
				(number "G8")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_117")
				(number "G7")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_117")
				(number "J8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_117")
				(number "J7")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_118")
				(number "D2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_118")
				(number "D1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_118")
				(number "C4")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_118")
				(number "C3")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_118")
				(number "B2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_118")
				(number "B1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_118")
				(number "A4")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_118")
				(number "A3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_118")
				(number "E4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_118")
				(number "E3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_118")
				(number "D6")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_118")
				(number "D5")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_118")
				(number "B6")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_118")
				(number "B5")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_118")
				(number "A8")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_118")
				(number "A7")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_118")
				(number "C8")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_118")
				(number "C7")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_118")
				(number "E8")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_118")
				(number "E7")
			)
		)
		(symbol "XC7K325T-FBG900_8_1"
			(pin power_in line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "B7")
			)
			(pin power_in line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "D7")
			)
			(pin power_in line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "F7")
			)
			(pin power_in line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "H7")
			)
			(pin power_in line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "K7")
			)
			(pin power_in line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "M7")
			)
			(pin power_in line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "P7")
			)
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTVCCAUX")
				(number "T7")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTVCCAUX")
				(number "V7")
			)
			(pin power_in line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "B3")
			)
			(pin power_in line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "C5")
			)
			(pin power_in line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "D3")
			)
			(pin power_in line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "E5")
			)
			(pin power_in line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "F3")
			)
			(pin power_in line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "G5")
			)
			(pin power_in line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "H3")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "J5")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "K3")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "L5")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "M3")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "N5")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "P3")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "R5")
			)
			(pin power_in line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "T3")
			)
			(pin power_in line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "U5")
			)
			(pin power_in line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "V3")
			)
			(pin power_in line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "W5")
			)
			(pin power_in line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTAVTTRCAL_115")
				(number "W7")
			)
			(pin power_in line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTRREF_115")
				(number "W8")
			)
		)
		(symbol "XC7K325T-FBG900_9_1"
			(pin power_in line
				(at 25.4 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "AB6")
			)
			(pin power_in line
				(at 27.94 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "T9")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "TDI_0")
				(number "H10")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "TDO_0")
				(number "G10")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "TMS_0")
				(number "F10")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TCK_0")
				(number "E10")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "CCLK_0")
				(number "B10")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "M0_0")
				(number "AB5")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "M1_0")
				(number "AB2")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "M2_0")
				(number "AB1")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "DONE_0")
				(number "M10")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "INIT_B_0")
				(number "A10")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "PROGRAM_B_0")
				(number "K10")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "CFGBVS_0")
				(number "L10")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "VP_0")
				(number "R15")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "VN_0")
				(number "T14")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 6.35)
				(name "VREFP_0")
				(number "T15")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "VREFN_0")
				(number "R14")
			)
			(pin bidirectional line
				(at 38.1 -35.56 180)
				(length 6.35)
				(name "DXP_0")
				(number "U15")
			)
			(pin bidirectional line
				(at 38.1 -38.1 180)
				(length 6.35)
				(name "DXN_0")
				(number "U14")
			)
		)
		(symbol "XC7K325T-FBG900_10_1"
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P13")
			)
			(pin power_in line
				(at -25.4 86.36 0)
				(length 6.35)
				(name "VCCAUX")
				(number "T13")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V13")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V15")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "VCCAUX")
				(number "W14")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "W12")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "V11")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "W10")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "GNDADC_0")
				(number "P14")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCADC_0")
				(number "P15")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCBATT_0")
				(number "C10")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "N16")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "R16")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "U16")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "W16")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "A2")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "A5")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "A6")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "A14")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "A24")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "B4")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "B8")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "B21")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "C1")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "C2")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "C9")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "C18")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C28")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "D8")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "D9")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "D15")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "D25")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "E1")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "E6")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "E9")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "E12")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "E22")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "F8")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "F9")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "F19")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "F29")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "G1")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "G2")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "G6")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "G9")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "G16")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "G26")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "H13")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "H23")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "J1")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "J6")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "M17")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "N18")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "P17")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "R10")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "R12")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "T11")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "T17")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "U10")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "U18")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "V17")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "W18")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "J20")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "J30")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "K4")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "K17")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "K27")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "L1")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "L2")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "L6")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "L24")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "M4")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "M8")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "M16")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "M18")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "M21")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "N1")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "N6")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "N28")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "P4")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "P8")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "P16")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "P18")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "P25")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "R2")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "R6")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "R9")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "R11")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "R13")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "R17")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "R22")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "T4")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "T8")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "T10")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "T12")
			)
		)
		(symbol "XC7K325T-FBG900_11_1"
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "GND")
				(number "T18")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "GND")
				(number "T19")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "GND")
				(number "T29")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "U1")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "U6")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "U9")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "U13")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "U17")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "U26")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "V8")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "V9")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "V12")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "V16")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "V18")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "V23")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "W1")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "W2")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "W6")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "W9")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "W11")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "W13")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "W15")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "W17")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "W20")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "W30")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "Y3")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "Y4")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "Y7")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "Y8")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "Y9")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "Y17")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "GND")
				(number "Y27")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "GND")
				(number "AA1")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "GND")
				(number "AA2")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "AA6")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "AA7")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "AA14")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "AA24")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "AB3")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "AB4")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "AB11")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "AB21")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "AC8")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "AC18")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "AC28")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "AD5")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "AD15")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "AD25")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "AE2")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "AE12")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "AE22")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "AF9")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "AF19")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "AF29")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "AG6")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "AG16")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "AG26")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "AH3")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "AH13")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "AH23")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "AJ10")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "AJ20")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "AJ30")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "AK7")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "AK17")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "AK27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC7K325T-FFG676"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC7K325T-FFG676"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Kintex 7 T 325 XC7K325T-FFG676"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC7K325T-FFG676_1_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_12")
				(number "U21")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_12")
				(number "U22")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_12")
				(number "V22")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_12")
				(number "U24")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_12")
				(number "U25")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_12")
				(number "V23")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_12")
				(number "V24")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_12")
				(number "U26")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_12")
				(number "V26")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_12")
				(number "W25")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_12")
				(number "W26")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_12")
				(number "V21")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_12")
				(number "W21")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_12")
				(number "AA25")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_12")
				(number "AB25")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_12")
				(number "W23")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_12")
				(number "W24")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_12")
				(number "AB26")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_12")
				(number "AC26")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_12")
				(number "Y25")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_12")
				(number "Y26")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_12")
				(number "AA23")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_12")
				(number "AB24")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_12")
				(number "Y23")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_12")
				(number "AA24")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_12")
				(number "Y22")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_12")
				(number "AA22")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_12")
				(number "AC23")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_12")
				(number "AC24")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_12")
				(number "W20")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_12")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_12")
				(number "AD23")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_12")
				(number "AD24")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_12")
				(number "AB22")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_12")
				(number "AC22")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_12")
				(number "AB21")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_12")
				(number "AC21")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_12")
				(number "AD21")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_12")
				(number "AE21")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_12")
				(number "AF24")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_12")
				(number "AF25")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_12")
				(number "AD26")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_12")
				(number "AE26")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_12")
				(number "AE23")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_12")
				(number "AF23")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_12")
				(number "AD25")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_12")
				(number "AE25")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_12")
				(number "AE22")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_12")
				(number "AF22")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_12")
				(number "Y20")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AA21")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AC25")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AD22")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AF26")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "U23")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "V20")
			)
			(pin power_in line
				(at -25.4 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "Y24")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "K24")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "N25")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "P22")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "R19")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "T16")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "T26")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_13")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_13")
				(number "K25")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_13")
				(number "K26")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_13")
				(number "R26")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_13")
				(number "P26")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_13")
				(number "M25")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_13")
				(number "L25")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_13")
				(number "P24")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_13")
				(number "N24")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_13")
				(number "N26")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_13")
				(number "M26")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_13")
				(number "R25")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_13")
				(number "P25")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_13")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_13")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_13")
				(number "M24")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_13")
				(number "L24")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_13")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_13")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_13")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_13")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_13")
				(number "P23")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_13")
				(number "N23")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_13")
				(number "N21")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_13")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_13")
				(number "R21")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_13")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_13")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_13")
				(number "R23")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_13")
				(number "T24")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_13")
				(number "T25")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_13")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_13")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_13")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_13")
				(number "T23")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_13")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_13")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_13")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_13")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_13")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_13")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_13")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_13")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_13")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_13")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_13")
				(number "U17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_13")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_13")
				(number "R18")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_13")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_13")
				(number "U16")
			)
		)
		(symbol "XC7K325T-FFG676_2_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_14")
				(number "K21")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_D00_MOSI_14")
				(number "B24")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_D01_DIN_14")
				(number "A25")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_D02_14")
				(number "B22")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_D03_14")
				(number "A22")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_PUDC_B_14")
				(number "B25")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_EMCCLK_14")
				(number "B26")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_D04_14")
				(number "A23")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_D05_14")
				(number "A24")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_D06_14")
				(number "D26")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_D07_14")
				(number "C26")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_FCS_B_14")
				(number "C23")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_D08_VREF_14")
				(number "C24")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_D09_14")
				(number "D21")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_D10_14")
				(number "C22")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_D11_14")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_D12_14")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_14")
				(number "E21")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_D13_14")
				(number "E22")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_D14_14")
				(number "C21")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_D15_14")
				(number "B21")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_14")
				(number "D23")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_14")
				(number "D24")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_14")
				(number "F22")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_14")
				(number "E23")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_14")
				(number "G22")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_14")
				(number "F23")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_14")
				(number "G24")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_14")
				(number "F24")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_RDWR_B_14")
				(number "E25")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_DOUT_CSO_B_14")
				(number "D25")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_CSI_B_14")
				(number "G25")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_A15_D31_14")
				(number "G26")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_A14_D30_14")
				(number "F25")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_A13_D29_14")
				(number "E26")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_A12_D28_14")
				(number "J26")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_A11_D27_14")
				(number "H26")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_A10_D26_14")
				(number "H21")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_A09_D25_VREF_14")
				(number "G21")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_A08_D24_14")
				(number "H23")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_A07_D23_14")
				(number "H24")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_14")
				(number "J21")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A06_D22_14")
				(number "H22")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_A05_D21_14")
				(number "J24")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_A04_D20_14")
				(number "J25")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_A03_D19_14")
				(number "L22")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_A02_D18_14")
				(number "K22")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_A01_D17_14")
				(number "K23")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_A00_D16_14")
				(number "J23")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_14")
				(number "L23")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "A21")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "C25")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "D22")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "F26")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "G23")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "L21")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "B18")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "E19")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "F16")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "H20")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "J17")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_15")
				(number "K15")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_AD0P_15")
				(number "C16")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_AD0N_15")
				(number "B16")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_AD8P_15")
				(number "A18")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_AD8N_15")
				(number "A19")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_AD1P_15")
				(number "B17")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_AD1N_15")
				(number "A17")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_AD9P_15")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_AD9N_15")
				(number "B19")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_AD2P_15")
				(number "C17")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_AD2N_15")
				(number "C18")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_15")
				(number "D15")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_15")
				(number "D16")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_AD10P_15")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_AD10N_15")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_AD3P_15")
				(number "G15")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_AD3N_15")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_AD11P_15")
				(number "J15")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_AD11N_15")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_AD4P_15")
				(number "E15")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_AD4N_15")
				(number "E16")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_AD12P_15")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_AD12N_15")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_AD5P_15")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_AD5N_15")
				(number "E17")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_15")
				(number "E18")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_15")
				(number "D18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_15")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_15")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_15")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_ADV_B_15")
				(number "D20")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_A28_15")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_A27_15")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_A26_15")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_A25_15")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_A24_15")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_A23_15")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_A22_15")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_A21_VREF_15")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_A20_15")
				(number "J18")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_A19_15")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_15")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A18_15")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_A17_15")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_A16_15")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_FOE_B_15")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_FWE_B_15")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_RS1_15")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_RS0_15")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_15")
				(number "M16")
			)
		)
		(symbol "XC7K325T-FFG676_3_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_16")
				(number "J8")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_16")
				(number "H9")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_16")
				(number "H8")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_16")
				(number "G10")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_16")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_16")
				(number "J13")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_16")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_16")
				(number "J11")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_16")
				(number "J10")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_16")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_16")
				(number "G14")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_16")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_16")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_16")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_16")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_16")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_16")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_16")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_16")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_16")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_16")
				(number "B9")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_16")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_16")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_16")
				(number "E10")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_16")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_16")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_16")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_16")
				(number "E11")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_16")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_16")
				(number "F14")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_16")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_16")
				(number "G12")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_16")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_16")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_16")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_16")
				(number "E13")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_16")
				(number "E12")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_16")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_16")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_16")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_16")
				(number "B11")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_16")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_16")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_16")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_16")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_16")
				(number "B15")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_16")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_16")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_16")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_16")
				(number "J14")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "A11")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "B8")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "C15")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "D12")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "E9")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "G13")
			)
			(pin power_in line
				(at -25.4 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "H10")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AB18")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AC15")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AE19")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AF16")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "W17")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "Y14")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_32")
				(number "V13")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_32")
				(number "AE17")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_32")
				(number "AF17")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_32")
				(number "AF14")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_32")
				(number "AF15")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_32")
				(number "AE18")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_32")
				(number "AF18")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_32")
				(number "AD15")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_32")
				(number "AE15")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_32")
				(number "AF19")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_32")
				(number "AF20")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_32")
				(number "AD16")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_32")
				(number "AE16")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_32")
				(number "AA14")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_32")
				(number "AA15")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_32")
				(number "AC14")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_32")
				(number "AD14")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_32")
				(number "Y15")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_32")
				(number "Y16")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_32")
				(number "AB14")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_32")
				(number "AB15")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_32")
				(number "AA17")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_32")
				(number "AA18")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_32")
				(number "AB16")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_32")
				(number "AC16")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_32")
				(number "AC18")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_32")
				(number "AD18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_32")
				(number "AB17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_32")
				(number "AC17")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_32")
				(number "AD20")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_32")
				(number "AE20")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_32")
				(number "AA19")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_32")
				(number "AA20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_32")
				(number "AC19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_32")
				(number "AD19")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_32")
				(number "AB19")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_32")
				(number "AB20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_32")
				(number "Y17")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_32")
				(number "Y18")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_32")
				(number "V16")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_32")
				(number "V17")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_32")
				(number "W18")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_32")
				(number "W19")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_32")
				(number "W15")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_32")
				(number "W16")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_32")
				(number "V18")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_32")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_32")
				(number "V14")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_32")
				(number "W14")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_32")
				(number "W13")
			)
		)
		(symbol "XC7K325T-FFG676_4_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_VRN_33")
				(number "U9")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_33")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_33")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_33")
				(number "V8")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_33")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_33")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_33")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_33")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_33")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_33")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_33")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_33")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_33")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_33")
				(number "AE7")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_33")
				(number "AF7")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_33")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_33")
				(number "AA7")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_33")
				(number "AC8")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_33")
				(number "AD8")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_33")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_33")
				(number "AC7")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_33")
				(number "AA9")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_33")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_33")
				(number "AC9")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_33")
				(number "AD9")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_33")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_33")
				(number "AC11")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_33")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_33")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_33")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_33")
				(number "AC12")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_33")
				(number "AA13")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_33")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_33")
				(number "AC13")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_33")
				(number "AD13")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_33")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_33")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_33")
				(number "AD11")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_33")
				(number "AE11")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_33")
				(number "AD10")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_33")
				(number "AE10")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_33")
				(number "AE12")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_33")
				(number "AF12")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_33")
				(number "AE8")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_33")
				(number "AF8")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_33")
				(number "AE13")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_33")
				(number "AF13")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_33")
				(number "AF10")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_33")
				(number "AF9")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_VRP_33")
				(number "V12")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AA11")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AB8")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AD12")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AE9")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "V10")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "W7")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AA1")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AC5")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AD2")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AF6")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "U3")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "Y4")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_34")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_34")
				(number "U6")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_34")
				(number "U5")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_34")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_34")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_34")
				(number "W6")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_34")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_34")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_34")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_34")
				(number "U7")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_34")
				(number "V6")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_34")
				(number "V4")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_34")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_34")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_34")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_34")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_34")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_34")
				(number "AB1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_34")
				(number "AC1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_34")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_34")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_34")
				(number "AB2")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_34")
				(number "AC2")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_34")
				(number "AA3")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_34")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_34")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_34")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_34")
				(number "AC4")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_34")
				(number "AC3")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_34")
				(number "AA5")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_34")
				(number "AB5")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_34")
				(number "AB6")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_34")
				(number "AC6")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_34")
				(number "Y6")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_34")
				(number "Y5")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_34")
				(number "AD6")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_34")
				(number "AD5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_34")
				(number "AD4")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_34")
				(number "AD3")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_34")
				(number "AD1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_34")
				(number "AE1")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_34")
				(number "AF5")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_34")
				(number "AF4")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_34")
				(number "AE3")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_34")
				(number "AE2")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_34")
				(number "AE6")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_34")
				(number "AE5")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_34")
				(number "AF3")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_34")
				(number "AF2")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_34")
				(number "T7")
			)
		)
		(symbol "XC7K325T-FFG676_5_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_115")
				(number "P2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_115")
				(number "P1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_115")
				(number "M2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_115")
				(number "M1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_115")
				(number "K2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_115")
				(number "K1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_115")
				(number "H2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_115")
				(number "H1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_115")
				(number "R4")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_115")
				(number "R3")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_115")
				(number "N4")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_115")
				(number "N3")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_115")
				(number "L4")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_115")
				(number "L3")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_115")
				(number "J4")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_115")
				(number "J3")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_115")
				(number "H6")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_115")
				(number "H5")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_115")
				(number "K6")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_115")
				(number "K5")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_116")
				(number "F2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_116")
				(number "F1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_116")
				(number "D2")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_116")
				(number "D1")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_116")
				(number "B2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_116")
				(number "B1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_116")
				(number "A4")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_116")
				(number "A3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_116")
				(number "G4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_116")
				(number "G3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_116")
				(number "E4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_116")
				(number "E3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_116")
				(number "C4")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_116")
				(number "C3")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_116")
				(number "B6")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_116")
				(number "B5")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_116")
				(number "D6")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_116")
				(number "D5")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_116")
				(number "F6")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_116")
				(number "F5")
			)
		)
		(symbol "XC7K325T-FFG676_6_1"
			(pin power_in line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "C6")
			)
			(pin power_in line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "E6")
			)
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "G6")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "J6")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "L6")
			)
			(pin power_in line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTVCCAUX")
				(number "N6")
			)
			(pin power_in line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "B3")
			)
			(pin power_in line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "C2")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "D3")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "G2")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "H3")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "L2")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "M3")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTTRCAL_115")
				(number "M5")
			)
			(pin power_in line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTRREF_115")
				(number "M6")
			)
		)
		(symbol "XC7K325T-FFG676_7_1"
			(pin power_in line
				(at 25.4 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "L7")
			)
			(pin power_in line
				(at 27.94 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "T6")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "TDI_0")
				(number "R6")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "TDO_0")
				(number "R7")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "TMS_0")
				(number "N8")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TCK_0")
				(number "L8")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "CCLK_0")
				(number "C8")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "M0_0")
				(number "T5")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "M1_0")
				(number "T2")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "M2_0")
				(number "P5")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "DONE_0")
				(number "J7")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "INIT_B_0")
				(number "G7")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "PROGRAM_B_0")
				(number "P6")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "CFGBVS_0")
				(number "P7")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "VP_0")
				(number "N12")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "VN_0")
				(number "P11")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 6.35)
				(name "VREFP_0")
				(number "P12")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "VREFN_0")
				(number "N11")
			)
			(pin bidirectional line
				(at 38.1 -35.56 180)
				(length 6.35)
				(name "DXP_0")
				(number "R12")
			)
			(pin bidirectional line
				(at 38.1 -38.1 180)
				(length 6.35)
				(name "DXN_0")
				(number "R11")
			)
		)
		(symbol "XC7K325T-FFG676_8_1"
			(pin power_in line
				(at -25.4 99.06 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 96.52 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M10")
			)
			(pin power_in line
				(at -25.4 93.98 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P10")
			)
			(pin power_in line
				(at -25.4 91.44 0)
				(length 6.35)
				(name "VCCAUX")
				(number "T10")
			)
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "T8")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "R9")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "P8")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "GNDADC_0")
				(number "M11")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCADC_0")
				(number "M12")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCBATT_0")
				(number "E8")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "N13")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "R13")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "T12")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "U13")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "GND")
				(number "A2")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "GND")
				(number "A5")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "GND")
				(number "A6")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "GND")
				(number "A7")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "GND")
				(number "A16")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "A26")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "B4")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "B23")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "C1")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "C5")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "C7")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "C10")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "C20")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "D7")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "D17")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "E1")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "E14")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E24")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "F3")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "F21")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G1")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "H25")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "J1")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "J5")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "J12")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "J22")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "K3")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "K4")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "K7")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "K11")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "K13")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "K19")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "L1")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "L10")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "L12")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "L14")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "L16")
			)
			(pin power_in line
				(at -25.4 -91.44 0)
				(length 6.35)
				(name "GND")
				(number "L26")
			)
			(pin power_in line
				(at -25.4 -93.98 0)
				(length 6.35)
				(name "GND")
				(number "M4")
			)
			(pin power_in line
				(at -25.4 -96.52 0)
				(length 6.35)
				(name "GND")
				(number "M7")
			)
			(pin power_in line
				(at -25.4 -99.06 0)
				(length 6.35)
				(name "GND")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 99.06 180)
				(length 6.35)
				(name "VCCINT")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 96.52 180)
				(length 6.35)
				(name "VCCINT")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 93.98 180)
				(length 6.35)
				(name "VCCINT")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 91.44 180)
				(length 6.35)
				(name "VCCINT")
				(number "K12")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "L13")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "L15")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "M8")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "R15")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "T14")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "U15")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "GND")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "GND")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "GND")
				(number "M23")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "GND")
				(number "N1")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "GND")
				(number "N5")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "N7")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "N20")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "P3")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "P4")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "P15")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "P17")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "R2")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "R8")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "R10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "R24")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "T1")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "T3")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "T4")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "T9")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "T11")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "T13")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "T15")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "T21")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "U8")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "U10")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U14")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "U18")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V5")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "V15")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "V25")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "W2")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "W12")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "W22")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "Y9")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "Y19")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AA6")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AA16")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AA26")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AB3")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AB13")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AB23")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "AC10")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "AC20")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "AD7")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "AD17")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "AE4")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "AE14")
			)
			(pin power_in line
				(at 25.4 -91.44 180)
				(length 6.35)
				(name "GND")
				(number "AE24")
			)
			(pin power_in line
				(at 25.4 -93.98 180)
				(length 6.35)
				(name "GND")
				(number "AF1")
			)
			(pin power_in line
				(at 25.4 -96.52 180)
				(length 6.35)
				(name "GND")
				(number "AF11")
			)
			(pin power_in line
				(at 25.4 -99.06 180)
				(length 6.35)
				(name "GND")
				(number "AF21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC7K325T-FFG900"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC7K325T-FFG900"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Kintex 7 T 325 XC7K325T-FFG900"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC7K325T-FFG900_1_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_12")
				(number "Y20")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_12")
				(number "Y23")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_12")
				(number "Y24")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_12")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_12")
				(number "AA21")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_12")
				(number "AB22")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_12")
				(number "AB23")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_12")
				(number "AA22")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_12")
				(number "AA23")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_12")
				(number "AC20")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_12")
				(number "AC21")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_12")
				(number "AA20")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_12")
				(number "AB20")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_12")
				(number "AB24")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_12")
				(number "AC25")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_12")
				(number "AC22")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_12")
				(number "AD22")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_12")
				(number "AC24")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_12")
				(number "AD24")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_12")
				(number "AD21")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_12")
				(number "AE21")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_12")
				(number "AE23")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_12")
				(number "AF23")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_12")
				(number "AD23")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_12")
				(number "AE24")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_12")
				(number "AF22")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_12")
				(number "AG23")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_12")
				(number "AG24")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_12")
				(number "AH24")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_12")
				(number "AJ24")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_12")
				(number "AK25")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_12")
				(number "AE25")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_12")
				(number "AF25")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_12")
				(number "AK23")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_12")
				(number "AK24")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_12")
				(number "AG25")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_12")
				(number "AH25")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_12")
				(number "AF20")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_12")
				(number "AF21")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_12")
				(number "AG22")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_12")
				(number "AH22")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_12")
				(number "AJ22")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_12")
				(number "AJ23")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_12")
				(number "AG20")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_12")
				(number "AH20")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_12")
				(number "AH21")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_12")
				(number "AJ21")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_12")
				(number "AK20")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_12")
				(number "AK21")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_12")
				(number "AE20")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AC23")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AD20")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AF24")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AG21")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AK22")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "Y22")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AA29")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AB26")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AD30")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AE27")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AH28")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AJ25")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_13")
				(number "Y25")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_13")
				(number "Y26")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_13")
				(number "AA26")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_13")
				(number "W27")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_13")
				(number "W28")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_13")
				(number "Y28")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_13")
				(number "AA28")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_13")
				(number "W29")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_13")
				(number "Y29")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_13")
				(number "AA27")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_13")
				(number "AB28")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_13")
				(number "AA25")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_13")
				(number "AB25")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_13")
				(number "AC29")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_13")
				(number "AC30")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_13")
				(number "Y30")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_13")
				(number "AA30")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_13")
				(number "AD29")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_13")
				(number "AE29")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_13")
				(number "AB29")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_13")
				(number "AB30")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_13")
				(number "AD27")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_13")
				(number "AD28")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_13")
				(number "AB27")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_13")
				(number "AC27")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_13")
				(number "AG29")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_13")
				(number "AH29")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_13")
				(number "AE28")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_13")
				(number "AF28")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_13")
				(number "AK29")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_13")
				(number "AK30")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_13")
				(number "AE30")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_13")
				(number "AF30")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_13")
				(number "AJ28")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_13")
				(number "AJ29")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_13")
				(number "AG30")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_13")
				(number "AH30")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_13")
				(number "AC26")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_13")
				(number "AD26")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_13")
				(number "AJ27")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_13")
				(number "AK28")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_13")
				(number "AG27")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_13")
				(number "AG28")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_13")
				(number "AH26")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_13")
				(number "AH27")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_13")
				(number "AF26")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_13")
				(number "AF27")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_13")
				(number "AJ26")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_13")
				(number "AK26")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_13")
				(number "AE26")
			)
		)
		(symbol "XC7K325T-FFG900_2_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_14")
				(number "R19")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_D00_MOSI_14")
				(number "P24")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_D01_DIN_14")
				(number "R25")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_D02_14")
				(number "R20")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_D03_14")
				(number "R21")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_PUDC_B_14")
				(number "R23")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_EMCCLK_14")
				(number "R24")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_D04_14")
				(number "T20")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_D05_14")
				(number "T21")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_D06_14")
				(number "T22")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_D07_14")
				(number "T23")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_FCS_B_14")
				(number "U19")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_D08_VREF_14")
				(number "U20")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_D09_14")
				(number "P29")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_D10_14")
				(number "R29")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_D11_14")
				(number "P27")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_D12_14")
				(number "P28")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_14")
				(number "R30")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_D13_14")
				(number "T30")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_D14_14")
				(number "P26")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_D15_14")
				(number "R26")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_14")
				(number "R28")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_14")
				(number "T28")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_14")
				(number "T26")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_14")
				(number "T27")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_14")
				(number "U27")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_14")
				(number "U28")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_14")
				(number "T25")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_14")
				(number "U25")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_RDWR_B_14")
				(number "U29")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_DOUT_CSO_B_14")
				(number "U30")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_CSI_B_14")
				(number "V26")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_A15_D31_14")
				(number "V27")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_A14_D30_14")
				(number "V29")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_A13_D29_14")
				(number "V30")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_A12_D28_14")
				(number "V25")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_A11_D27_14")
				(number "W26")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_A10_D26_14")
				(number "V19")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_A09_D25_VREF_14")
				(number "V20")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_A08_D24_14")
				(number "W23")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_A07_D23_14")
				(number "W24")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_14")
				(number "U22")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A06_D22_14")
				(number "U23")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_A05_D21_14")
				(number "V21")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_A04_D20_14")
				(number "V22")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_A03_D19_14")
				(number "U24")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_A02_D18_14")
				(number "V24")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_A01_D17_14")
				(number "W21")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_A00_D16_14")
				(number "W22")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_14")
				(number "W19")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "P30")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "R27")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "T24")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "U21")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "V28")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "W25")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "J25")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "K22")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "L29")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "M26")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "N23")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_15")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_AD0P_15")
				(number "J23")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_AD0N_15")
				(number "J24")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_AD8P_15")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_AD8N_15")
				(number "L23")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_AD1P_15")
				(number "K23")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_AD1N_15")
				(number "K24")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_AD9P_15")
				(number "L21")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_AD9N_15")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_AD2P_15")
				(number "J21")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_AD2N_15")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_15")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_15")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_AD10P_15")
				(number "J29")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_AD10N_15")
				(number "H29")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_AD3P_15")
				(number "J27")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_AD3N_15")
				(number "J28")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_AD11P_15")
				(number "L30")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_AD11N_15")
				(number "K30")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_AD4P_15")
				(number "K26")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_AD4N_15")
				(number "J26")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_AD12P_15")
				(number "L26")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_AD12N_15")
				(number "L27")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_AD5P_15")
				(number "L25")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_AD5N_15")
				(number "K25")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_15")
				(number "K28")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_15")
				(number "K29")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_15")
				(number "M28")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_15")
				(number "L28")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_15")
				(number "M29")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_ADV_B_15")
				(number "M30")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_A28_15")
				(number "N27")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_A27_15")
				(number "M27")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_A26_15")
				(number "N29")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_A25_15")
				(number "N30")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_A24_15")
				(number "N25")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_A23_15")
				(number "N26")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_A22_15")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_A21_VREF_15")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_A20_15")
				(number "N21")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_A19_15")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_15")
				(number "P23")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A18_15")
				(number "N24")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_A17_15")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_A16_15")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_FOE_B_15")
				(number "M24")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_FWE_B_15")
				(number "M25")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_RS1_15")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_RS0_15")
				(number "M23")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_15")
				(number "P19")
			)
		)
		(symbol "XC7K325T-FFG900_3_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_16")
				(number "F23")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_16")
				(number "B23")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_16")
				(number "A23")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_16")
				(number "E23")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_16")
				(number "D23")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_16")
				(number "F25")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_16")
				(number "E25")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_16")
				(number "E24")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_16")
				(number "D24")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_16")
				(number "F26")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_16")
				(number "E26")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_16")
				(number "G23")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_16")
				(number "G24")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_16")
				(number "B27")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_16")
				(number "A27")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_16")
				(number "C24")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_16")
				(number "B24")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_16")
				(number "B28")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_16")
				(number "A28")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_16")
				(number "A25")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_16")
				(number "A26")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_16")
				(number "D26")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_16")
				(number "C26")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_16")
				(number "C25")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_16")
				(number "B25")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_16")
				(number "D27")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_16")
				(number "C27")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_16")
				(number "E28")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_16")
				(number "D28")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_16")
				(number "C29")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_16")
				(number "B29")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_16")
				(number "D29")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_16")
				(number "C30")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_16")
				(number "B30")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_16")
				(number "A30")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_16")
				(number "E29")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_16")
				(number "E30")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_16")
				(number "H24")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_16")
				(number "H25")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_16")
				(number "G28")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_16")
				(number "F28")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_16")
				(number "G27")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_16")
				(number "F27")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_16")
				(number "G29")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_16")
				(number "F30")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_16")
				(number "H26")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_16")
				(number "H27")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_16")
				(number "H30")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_16")
				(number "G30")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_16")
				(number "G25")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "A29")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "B26")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "C23")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "D30")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "E27")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "F24")
			)
			(pin power_in line
				(at -25.4 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "H28")
			)
			(pin power_in line
				(at 25.4 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "A19")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "B16")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "D20")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "E17")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "G21")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "H18")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_17")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_17")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_17")
				(number "J18")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_17")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_17")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_17")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_17")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_17")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_17")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_17")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_17")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_17")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_17")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_17")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_17")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_17")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_17")
				(number "C21")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_17")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_17")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_17")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_17")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_17")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_17")
				(number "E21")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_17")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_17")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_17")
				(number "D17")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_17")
				(number "D18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_17")
				(number "E19")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_17")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_17")
				(number "D16")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_17")
				(number "C16")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_17")
				(number "G18")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_17")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_17")
				(number "C17")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_17")
				(number "B17")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_17")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_17")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_17")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_17")
				(number "B20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_17")
				(number "A16")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_17")
				(number "A17")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_17")
				(number "A20")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_17")
				(number "A21")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_17")
				(number "B18")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_17")
				(number "A18")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_17")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_17")
				(number "A22")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_17")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_17")
				(number "B19")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_17")
				(number "E18")
			)
		)
		(symbol "XC7K325T-FFG900_4_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_18")
				(number "G12")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_18")
				(number "L16")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_18")
				(number "K16")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_18")
				(number "L15")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_18")
				(number "K15")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_18")
				(number "L12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_18")
				(number "L13")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_18")
				(number "K13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_18")
				(number "J13")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_18")
				(number "K14")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_18")
				(number "J14")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_18")
				(number "L11")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_18")
				(number "K11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_18")
				(number "H15")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_18")
				(number "G15")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_18")
				(number "J11")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_18")
				(number "J12")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_18")
				(number "J16")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_18")
				(number "H16")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_18")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_18")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_18")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_18")
				(number "G14")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_18")
				(number "G13")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_18")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_18")
				(number "D12")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_18")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_18")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_18")
				(number "E13")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_18")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_18")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_18")
				(number "F11")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_18")
				(number "E11")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_18")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_18")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_18")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_18")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_18")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_18")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_18")
				(number "E14")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_18")
				(number "E15")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_18")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_18")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_18")
				(number "B13")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_18")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_18")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_18")
				(number "B15")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_18")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_18")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_18")
				(number "F16")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "C13")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "D10")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "F14")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "G11")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "J15")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "K12")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AA19")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AB16")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AE17")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AF14")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AH18")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AJ15")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_32")
				(number "Y14")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_32")
				(number "AK16")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_32")
				(number "AK15")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_32")
				(number "AG15")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_32")
				(number "AH15")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_32")
				(number "AH16")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_32")
				(number "AJ16")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_32")
				(number "AF15")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_32")
				(number "AG14")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_32")
				(number "AH17")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_32")
				(number "AJ17")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_32")
				(number "AE16")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_32")
				(number "AF16")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_32")
				(number "AJ19")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_32")
				(number "AK19")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_32")
				(number "AG19")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_32")
				(number "AH19")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_32")
				(number "AJ18")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_32")
				(number "AK18")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_32")
				(number "AD19")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_32")
				(number "AE19")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_32")
				(number "AF18")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_32")
				(number "AG18")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_32")
				(number "AF17")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_32")
				(number "AG17")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_32")
				(number "AD18")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_32")
				(number "AE18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_32")
				(number "AD17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_32")
				(number "AD16")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_32")
				(number "Y19")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_32")
				(number "Y18")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_32")
				(number "AA18")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_32")
				(number "AB18")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_32")
				(number "AB19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_32")
				(number "AC19")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_32")
				(number "AB17")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_32")
				(number "AC17")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_32")
				(number "AE15")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_32")
				(number "AE14")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_32")
				(number "AA15")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_32")
				(number "AB15")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_32")
				(number "AC16")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_32")
				(number "AC15")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_32")
				(number "AC14")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_32")
				(number "AD14")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_32")
				(number "AA17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_32")
				(number "AA16")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_32")
				(number "Y16")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_32")
				(number "Y15")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_32")
				(number "AB14")
			)
		)
		(symbol "XC7K325T-FFG900_5_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_VRN_33")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_33")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_33")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_33")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_33")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_33")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_33")
				(number "AC9")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_33")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_33")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_33")
				(number "AA11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_33")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_33")
				(number "AA13")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_33")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_33")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_33")
				(number "AC10")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_33")
				(number "AD8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_33")
				(number "AE8")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_33")
				(number "AC12")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_33")
				(number "AC11")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_33")
				(number "AD9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_33")
				(number "AE9")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_33")
				(number "AE11")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_33")
				(number "AF11")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_33")
				(number "AD12")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_33")
				(number "AD11")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_33")
				(number "AG10")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_33")
				(number "AH10")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_33")
				(number "AE10")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_33")
				(number "AF10")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_33")
				(number "AJ9")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_33")
				(number "AK9")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_33")
				(number "AG9")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_33")
				(number "AH9")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_33")
				(number "AK11")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_33")
				(number "AK10")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_33")
				(number "AH11")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_33")
				(number "AJ11")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_33")
				(number "AE13")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_33")
				(number "AF13")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_33")
				(number "AK14")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_33")
				(number "AK13")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_33")
				(number "AH14")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_33")
				(number "AJ14")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_33")
				(number "AJ13")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_33")
				(number "AJ12")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_33")
				(number "AF12")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_33")
				(number "AG12")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_33")
				(number "AG13")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_33")
				(number "AH12")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_VRP_33")
				(number "AD13")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AA9")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AC13")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AD10")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AG11")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AK12")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "Y12")
			)
			(pin power_in line
				(at 25.4 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AC3")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AE7")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AF4")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AG1")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AH8")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AJ5")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AK2")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_34")
				(number "AC6")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_34")
				(number "AD4")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_34")
				(number "AD3")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_34")
				(number "AC2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_34")
				(number "AC1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_34")
				(number "AD2")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_34")
				(number "AD1")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_34")
				(number "AC5")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_34")
				(number "AC4")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_34")
				(number "AD6")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_34")
				(number "AE6")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_34")
				(number "AC7")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_34")
				(number "AD7")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_34")
				(number "AF3")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_34")
				(number "AF2")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_34")
				(number "AE1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_34")
				(number "AF1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_34")
				(number "AG4")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_34")
				(number "AG3")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_34")
				(number "AE4")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_34")
				(number "AE3")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_34")
				(number "AE5")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_34")
				(number "AF5")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_34")
				(number "AF6")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_34")
				(number "AG5")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_34")
				(number "AH4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_34")
				(number "AJ4")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_34")
				(number "AH6")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_34")
				(number "AH5")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_34")
				(number "AG2")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_34")
				(number "AH1")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_34")
				(number "AH2")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_34")
				(number "AJ2")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_34")
				(number "AJ1")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_34")
				(number "AK1")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_34")
				(number "AJ3")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_34")
				(number "AK3")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_34")
				(number "AF8")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_34")
				(number "AG8")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_34")
				(number "AF7")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_34")
				(number "AG7")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_34")
				(number "AH7")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_34")
				(number "AJ7")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_34")
				(number "AJ6")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_34")
				(number "AK6")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_34")
				(number "AJ8")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_34")
				(number "AK8")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_34")
				(number "AK5")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_34")
				(number "AK4")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_34")
				(number "AB7")
			)
		)
		(symbol "XC7K325T-FFG900_6_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_115")
				(number "Y2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_115")
				(number "Y1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_115")
				(number "V2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_115")
				(number "V1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_115")
				(number "U4")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_115")
				(number "U3")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_115")
				(number "T2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_115")
				(number "T1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_115")
				(number "AA4")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_115")
				(number "AA3")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_115")
				(number "Y6")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_115")
				(number "Y5")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_115")
				(number "W4")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_115")
				(number "W3")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_115")
				(number "V6")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_115")
				(number "V5")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_115")
				(number "R8")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_115")
				(number "R7")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_115")
				(number "U8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_115")
				(number "U7")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_116")
				(number "P2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_116")
				(number "P1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_116")
				(number "N4")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_116")
				(number "N3")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_116")
				(number "M2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_116")
				(number "M1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_116")
				(number "L4")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_116")
				(number "L3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_116")
				(number "T6")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_116")
				(number "T5")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_116")
				(number "R4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_116")
				(number "R3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_116")
				(number "P6")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_116")
				(number "P5")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_116")
				(number "M6")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_116")
				(number "M5")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_116")
				(number "L8")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_116")
				(number "L7")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_116")
				(number "N8")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_116")
				(number "N7")
			)
		)
		(symbol "XC7K325T-FFG900_7_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_117")
				(number "K2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_117")
				(number "K1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_117")
				(number "J4")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_117")
				(number "J3")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_117")
				(number "H2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_117")
				(number "H1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_117")
				(number "F2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_117")
				(number "F1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_117")
				(number "K6")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_117")
				(number "K5")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_117")
				(number "H6")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_117")
				(number "H5")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_117")
				(number "G4")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_117")
				(number "G3")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_117")
				(number "F6")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_117")
				(number "F5")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_117")
				(number "G8")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_117")
				(number "G7")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_117")
				(number "J8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_117")
				(number "J7")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_118")
				(number "D2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_118")
				(number "D1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_118")
				(number "C4")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_118")
				(number "C3")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_118")
				(number "B2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_118")
				(number "B1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_118")
				(number "A4")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_118")
				(number "A3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_118")
				(number "E4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_118")
				(number "E3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_118")
				(number "D6")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_118")
				(number "D5")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_118")
				(number "B6")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_118")
				(number "B5")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_118")
				(number "A8")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_118")
				(number "A7")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_118")
				(number "C8")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_118")
				(number "C7")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_118")
				(number "E8")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_118")
				(number "E7")
			)
		)
		(symbol "XC7K325T-FFG900_8_1"
			(pin power_in line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "B7")
			)
			(pin power_in line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "D7")
			)
			(pin power_in line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "F7")
			)
			(pin power_in line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "H7")
			)
			(pin power_in line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "K7")
			)
			(pin power_in line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "M7")
			)
			(pin power_in line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "P7")
			)
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTVCCAUX")
				(number "T7")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTVCCAUX")
				(number "V7")
			)
			(pin power_in line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "B3")
			)
			(pin power_in line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "C5")
			)
			(pin power_in line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "D3")
			)
			(pin power_in line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "E5")
			)
			(pin power_in line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "F3")
			)
			(pin power_in line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "G5")
			)
			(pin power_in line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "H3")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "J5")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "K3")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "L5")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "M3")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "N5")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "P3")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "R5")
			)
			(pin power_in line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "T3")
			)
			(pin power_in line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "U5")
			)
			(pin power_in line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "V3")
			)
			(pin power_in line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "W5")
			)
			(pin power_in line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTAVTTRCAL_115")
				(number "W7")
			)
			(pin power_in line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTRREF_115")
				(number "W8")
			)
		)
		(symbol "XC7K325T-FFG900_9_1"
			(pin power_in line
				(at 25.4 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "AB6")
			)
			(pin power_in line
				(at 27.94 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "T9")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "TDI_0")
				(number "H10")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "TDO_0")
				(number "G10")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "TMS_0")
				(number "F10")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TCK_0")
				(number "E10")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "CCLK_0")
				(number "B10")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "M0_0")
				(number "AB5")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "M1_0")
				(number "AB2")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "M2_0")
				(number "AB1")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "DONE_0")
				(number "M10")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "INIT_B_0")
				(number "A10")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "PROGRAM_B_0")
				(number "K10")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "CFGBVS_0")
				(number "L10")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "VP_0")
				(number "R15")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "VN_0")
				(number "T14")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 6.35)
				(name "VREFP_0")
				(number "T15")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "VREFN_0")
				(number "R14")
			)
			(pin bidirectional line
				(at 38.1 -35.56 180)
				(length 6.35)
				(name "DXP_0")
				(number "U15")
			)
			(pin bidirectional line
				(at 38.1 -38.1 180)
				(length 6.35)
				(name "DXN_0")
				(number "U14")
			)
		)
		(symbol "XC7K325T-FFG900_10_1"
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P13")
			)
			(pin power_in line
				(at -25.4 86.36 0)
				(length 6.35)
				(name "VCCAUX")
				(number "T13")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V13")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V15")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "VCCAUX")
				(number "W14")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "W12")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "V11")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "W10")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "GNDADC_0")
				(number "P14")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCADC_0")
				(number "P15")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCBATT_0")
				(number "C10")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "N16")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "R16")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "U16")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "W16")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "A2")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "A5")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "A6")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "A14")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "A24")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "B4")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "B8")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "B21")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "C1")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "C2")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "C9")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "C18")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C28")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "D8")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "D9")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "D15")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "D25")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "E1")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "E6")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "E9")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "E12")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "E22")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "F8")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "F9")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "F19")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "F29")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "G1")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "G2")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "G6")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "G9")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "G16")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "G26")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "H13")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "H23")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "J1")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "J6")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "M17")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "N18")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "P17")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "R10")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "R12")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "T11")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "T17")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "U10")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "U18")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "V17")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "W18")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "J20")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "J30")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "K4")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "K17")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "K27")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "L1")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "L2")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "L6")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "L24")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "M4")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "M8")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "M16")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "M18")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "M21")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "N1")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "N6")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "N28")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "P4")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "P8")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "P16")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "P18")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "P25")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "R2")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "R6")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "R9")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "R11")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "R13")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "R17")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "R22")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "T4")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "T8")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "T10")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "T12")
			)
		)
		(symbol "XC7K325T-FFG900_11_1"
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "GND")
				(number "T18")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "GND")
				(number "T19")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "GND")
				(number "T29")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "U1")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "U6")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "U9")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "U13")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "U17")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "U26")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "V8")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "V9")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "V12")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "V16")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "V18")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "V23")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "W1")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "W2")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "W6")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "W9")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "W11")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "W13")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "W15")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "W17")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "W20")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "W30")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "Y3")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "Y4")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "Y7")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "Y8")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "Y9")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "Y17")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "GND")
				(number "Y27")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "GND")
				(number "AA1")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "GND")
				(number "AA2")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "AA6")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "AA7")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "AA14")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "AA24")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "AB3")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "AB4")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "AB11")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "AB21")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "AC8")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "AC18")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "AC28")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "AD5")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "AD15")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "AD25")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "AE2")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "AE12")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "AE22")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "AF9")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "AF19")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "AF29")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "AG6")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "AG16")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "AG26")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "AH3")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "AH13")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "AH23")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "AJ10")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "AJ20")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "AJ30")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "AK7")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "AK17")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "AK27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC7K355T-FFG901"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC7K355T-FFG901"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Kintex 7 T 355 XC7K355T-FFG901"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC7K355T-FFG901_1_1"
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AA19")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AB16")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AE17")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AF14")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AH18")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AJ15")
			)
			(pin power_in line
				(at 25.4 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AC23")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AD20")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AF24")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AG21")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AJ25")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AK22")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_12")
				(number "Y23")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_12")
				(number "Y20")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_12")
				(number "Y21")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_12")
				(number "AA20")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_12")
				(number "AA21")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_12")
				(number "AA22")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_12")
				(number "AA23")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_12")
				(number "AB20")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_12")
				(number "AC20")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_12")
				(number "AB22")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_12")
				(number "AB23")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_12")
				(number "AC21")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_12")
				(number "AC22")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_12")
				(number "AD26")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_12")
				(number "AE26")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_12")
				(number "AH25")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_12")
				(number "AH26")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_12")
				(number "AE25")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_12")
				(number "AF26")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_12")
				(number "AD24")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_12")
				(number "AE24")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_12")
				(number "AF25")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_12")
				(number "AG25")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_12")
				(number "AG24")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_12")
				(number "AH24")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_12")
				(number "AG22")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_12")
				(number "AG23")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_12")
				(number "AF22")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_12")
				(number "AF23")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_12")
				(number "AD23")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_12")
				(number "AE23")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_12")
				(number "AD21")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_12")
				(number "AD22")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_12")
				(number "AE21")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_12")
				(number "AF21")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_12")
				(number "AF20")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_12")
				(number "AG20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_12")
				(number "AH21")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_12")
				(number "AH22")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_12")
				(number "AJ21")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_12")
				(number "AK21")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_12")
				(number "AJ22")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_12")
				(number "AK23")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_12")
				(number "AJ23")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_12")
				(number "AJ24")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_12")
				(number "AK24")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_12")
				(number "AK25")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_12")
				(number "AJ26")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_12")
				(number "AK26")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_12")
				(number "AE20")
			)
		)
		(symbol "XC7K355T-FFG901_2_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_13")
				(number "W24")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_13")
				(number "AA28")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_13")
				(number "AB28")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_13")
				(number "AB29")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_13")
				(number "AB30")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_13")
				(number "Y30")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_13")
				(number "AA30")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_13")
				(number "Y28")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_13")
				(number "Y29")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_13")
				(number "W28")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_13")
				(number "W29")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_13")
				(number "W26")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_13")
				(number "W27")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_13")
				(number "AC26")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_13")
				(number "AD27")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_13")
				(number "Y25")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_13")
				(number "AA25")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_13")
				(number "AB25")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_13")
				(number "AC25")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_13")
				(number "AB24")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_13")
				(number "AC24")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_13")
				(number "Y26")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_13")
				(number "AA26")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_13")
				(number "AA27")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_13")
				(number "AB27")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_13")
				(number "AC27")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_13")
				(number "AD28")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_13")
				(number "AE28")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_13")
				(number "AF28")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_13")
				(number "AC29")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_13")
				(number "AC30")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_13")
				(number "AD29")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_13")
				(number "AE29")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_13")
				(number "AE30")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_13")
				(number "AF30")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_13")
				(number "AF27")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_13")
				(number "AG28")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_13")
				(number "AG27")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_13")
				(number "AH27")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_13")
				(number "AG29")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_13")
				(number "AH29")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_13")
				(number "AJ27")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_13")
				(number "AJ28")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_13")
				(number "AG30")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_13")
				(number "AH30")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_13")
				(number "AJ29")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_13")
				(number "AK30")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_13")
				(number "AK28")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_13")
				(number "AK29")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_13")
				(number "Y24")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AA29")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AB26")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AD30")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AE27")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AH28")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "W25")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "R17")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "R27")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "T24")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "U21")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "V18")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "V28")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_14")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_D00_MOSI_14")
				(number "R30")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_D01_DIN_14")
				(number "T30")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_D02_14")
				(number "R28")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_D03_14")
				(number "T28")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_PUDC_B_14")
				(number "V29")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_EMCCLK_14")
				(number "V30")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_D04_14")
				(number "U29")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_D05_14")
				(number "U30")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_D06_14")
				(number "U27")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_D07_14")
				(number "U28")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_FCS_B_14")
				(number "V26")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_D08_VREF_14")
				(number "V27")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_D09_14")
				(number "R24")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_D10_14")
				(number "R25")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_D11_14")
				(number "R23")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_D12_14")
				(number "T23")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_14")
				(number "V24")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_D13_14")
				(number "V25")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_D14_14")
				(number "R26")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_D15_14")
				(number "T27")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_14")
				(number "T25")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_14")
				(number "T26")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_14")
				(number "U24")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_14")
				(number "U25")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_14")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_14")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_14")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_14")
				(number "U23")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_RDWR_B_14")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_DOUT_CSO_B_14")
				(number "R21")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_CSI_B_14")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_A15_D31_14")
				(number "T21")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_A14_D30_14")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_A13_D29_14")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_A12_D28_14")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_A11_D27_14")
				(number "W23")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_A10_D26_14")
				(number "R18")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_A09_D25_VREF_14")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_A08_D24_14")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_A07_D23_14")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_14")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A06_D22_14")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_A05_D21_14")
				(number "U17")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_A04_D20_14")
				(number "U18")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_A03_D19_14")
				(number "V17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_A02_D18_14")
				(number "W17")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_A01_D17_14")
				(number "W18")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_A00_D16_14")
				(number "W19")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_14")
				(number "W21")
			)
		)
		(symbol "XC7K355T-FFG901_3_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_15")
				(number "L22")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_AD0P_15")
				(number "K28")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_AD0N_15")
				(number "K29")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_AD8P_15")
				(number "L30")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_AD8N_15")
				(number "K30")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_AD1P_15")
				(number "N30")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_AD1N_15")
				(number "M30")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_AD9P_15")
				(number "N29")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_AD9N_15")
				(number "M29")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_AD2P_15")
				(number "R29")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_AD2N_15")
				(number "P29")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_15")
				(number "M28")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_15")
				(number "L28")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_AD10P_15")
				(number "K25")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_AD10N_15")
				(number "K26")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_AD3P_15")
				(number "P26")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_AD3N_15")
				(number "N26")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_AD11P_15")
				(number "N27")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_AD11N_15")
				(number "M27")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_AD4P_15")
				(number "P27")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_AD4N_15")
				(number "P28")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_AD12P_15")
				(number "M25")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_AD12N_15")
				(number "L25")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_AD5P_15")
				(number "L26")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_AD5N_15")
				(number "L27")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_15")
				(number "M23")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_15")
				(number "M24")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_15")
				(number "N24")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_15")
				(number "N25")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_15")
				(number "L23")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_ADV_B_15")
				(number "K24")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_A28_15")
				(number "N22")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_A27_15")
				(number "M22")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_A26_15")
				(number "P23")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_A25_15")
				(number "P24")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_A24_15")
				(number "L20")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_A23_15")
				(number "L21")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_A22_15")
				(number "N20")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_A21_VREF_15")
				(number "M20")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_A20_15")
				(number "P21")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_A19_15")
				(number "N21")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_15")
				(number "M18")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A18_15")
				(number "M19")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_A17_15")
				(number "P19")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_A16_15")
				(number "N19")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_FOE_B_15")
				(number "N17")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_FWE_B_15")
				(number "M17")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_RS1_15")
				(number "P17")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_RS0_15")
				(number "P18")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_15")
				(number "P22")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "L19")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "L29")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "M26")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "N23")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "P20")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "P30")
			)
			(pin power_in line
				(at 25.4 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "A29")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "B26")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "D30")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "E27")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "F24")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "H28")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "J25")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_16")
				(number "E24")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_16")
				(number "D24")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_16")
				(number "C24")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_16")
				(number "B24")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_16")
				(number "B25")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_16")
				(number "C25")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_16")
				(number "C26")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_16")
				(number "A25")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_16")
				(number "A26")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_16")
				(number "C27")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_16")
				(number "B27")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_16")
				(number "D26")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_16")
				(number "D27")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_16")
				(number "H24")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_16")
				(number "G24")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_16")
				(number "H25")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_16")
				(number "G25")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_16")
				(number "J26")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_16")
				(number "J27")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_16")
				(number "H26")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_16")
				(number "H27")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_16")
				(number "F25")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_16")
				(number "F26")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_16")
				(number "E25")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_16")
				(number "E26")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_16")
				(number "G27")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_16")
				(number "F27")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_16")
				(number "G28")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_16")
				(number "F28")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_16")
				(number "H29")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_16")
				(number "G29")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_16")
				(number "F30")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_16")
				(number "E30")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_16")
				(number "H30")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_16")
				(number "G30")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_16")
				(number "J28")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_16")
				(number "J29")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_16")
				(number "E28")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_16")
				(number "D28")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_16")
				(number "E29")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_16")
				(number "D29")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_16")
				(number "C29")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_16")
				(number "C30")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_16")
				(number "B28")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_16")
				(number "B29")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_16")
				(number "B30")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_16")
				(number "A30")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_16")
				(number "A27")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_16")
				(number "A28")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_16")
				(number "J24")
			)
		)
		(symbol "XC7K355T-FFG901_4_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_17")
				(number "H21")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_17")
				(number "K23")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_17")
				(number "J23")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_17")
				(number "J22")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_17")
				(number "H22")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_17")
				(number "K21")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_17")
				(number "J21")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_17")
				(number "K19")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_17")
				(number "K20")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_17")
				(number "J18")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_17")
				(number "J19")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_17")
				(number "L18")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_17")
				(number "K18")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_17")
				(number "G23")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_17")
				(number "F23")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_17")
				(number "H20")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_17")
				(number "G20")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_17")
				(number "H19")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_17")
				(number "G19")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_17")
				(number "G18")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_17")
				(number "F18")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_17")
				(number "G22")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_17")
				(number "F22")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_17")
				(number "F20")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_17")
				(number "F21")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_17")
				(number "E20")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_17")
				(number "E21")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_17")
				(number "D21")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_17")
				(number "D22")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_17")
				(number "E23")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_17")
				(number "D23")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_17")
				(number "C21")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_17")
				(number "C22")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_17")
				(number "E18")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_17")
				(number "E19")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_17")
				(number "D18")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_17")
				(number "D19")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_17")
				(number "C19")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_17")
				(number "C20")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_17")
				(number "B19")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_17")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_17")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_17")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_17")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_17")
				(number "A21")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_17")
				(number "B22")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_17")
				(number "B23")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_17")
				(number "A22")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_17")
				(number "A23")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_17")
				(number "L17")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "A19")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "C23")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "D20")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "G21")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "H18")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "K22")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "B16")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "E17")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "F14")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "J15")
			)
		)
		(symbol "XC7K355T-FFG901_5_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_112")
				(number "AK6")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_112")
				(number "AK5")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_112")
				(number "AJ4")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_112")
				(number "AJ3")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_112")
				(number "AK2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_112")
				(number "AK1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_112")
				(number "AH2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_112")
				(number "AH1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_112")
				(number "AH6")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_112")
				(number "AH5")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_112")
				(number "AG4")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_112")
				(number "AG3")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_112")
				(number "AE4")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_112")
				(number "AE3")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_112")
				(number "AC4")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_112")
				(number "AC3")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_112")
				(number "AD6")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_112")
				(number "AD5")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_112")
				(number "AF6")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_112")
				(number "AF5")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_113")
				(number "AF2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_113")
				(number "AF1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_113")
				(number "AD2")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_113")
				(number "AD1")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_113")
				(number "AB2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_113")
				(number "AB1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_113")
				(number "Y2")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_113")
				(number "Y1")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_113")
				(number "AB6")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_113")
				(number "AB5")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_113")
				(number "AA4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_113")
				(number "AA3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_113")
				(number "Y6")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_113")
				(number "Y5")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_113")
				(number "W4")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_113")
				(number "W3")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_113")
				(number "U8")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_113")
				(number "U7")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_113")
				(number "W8")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_113")
				(number "W7")
			)
		)
		(symbol "XC7K355T-FFG901_6_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_114")
				(number "V2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_114")
				(number "V1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_114")
				(number "T2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_114")
				(number "T1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_114")
				(number "P2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_114")
				(number "P1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_114")
				(number "N4")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_114")
				(number "N3")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_114")
				(number "V6")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_114")
				(number "V5")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_114")
				(number "U4")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_114")
				(number "U3")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_114")
				(number "R4")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_114")
				(number "R3")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_114")
				(number "P6")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_114")
				(number "P5")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_114")
				(number "R8")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_114")
				(number "R7")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_114")
				(number "T6")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_114")
				(number "T5")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_115")
				(number "M2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_115")
				(number "M1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_115")
				(number "K2")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_115")
				(number "K1")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_115")
				(number "H2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_115")
				(number "H1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_115")
				(number "F2")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_115")
				(number "F1")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_115")
				(number "M6")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_115")
				(number "M5")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_115")
				(number "L4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_115")
				(number "L3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_115")
				(number "K6")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_115")
				(number "K5")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_115")
				(number "J4")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_115")
				(number "J3")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_115")
				(number "J8")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_115")
				(number "J7")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_115")
				(number "L8")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_115")
				(number "L7")
			)
		)
		(symbol "XC7K355T-FFG901_7_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_116")
				(number "D2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_116")
				(number "D1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_116")
				(number "B2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_116")
				(number "B1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_116")
				(number "A4")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_116")
				(number "A3")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_116")
				(number "B6")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_116")
				(number "B5")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_116")
				(number "G4")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_116")
				(number "G3")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_116")
				(number "E4")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_116")
				(number "E3")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_116")
				(number "D6")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_116")
				(number "D5")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_116")
				(number "C4")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_116")
				(number "C3")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_116")
				(number "F6")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_116")
				(number "F5")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_116")
				(number "H6")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_116")
				(number "H5")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_117")
				(number "C8")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_117")
				(number "C7")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_117")
				(number "A8")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_117")
				(number "A7")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_117")
				(number "B10")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_117")
				(number "B9")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_117")
				(number "A12")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_117")
				(number "A11")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_117")
				(number "F10")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_117")
				(number "F9")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_117")
				(number "D10")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_117")
				(number "D9")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_117")
				(number "E12")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_117")
				(number "E11")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_117")
				(number "C12")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_117")
				(number "C11")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_117")
				(number "E8")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_117")
				(number "E7")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_117")
				(number "G8")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_117")
				(number "G7")
			)
		)
		(symbol "XC7K355T-FFG901_8_1"
			(pin power_in line
				(at -38.1 33.02 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AA6")
			)
			(pin power_in line
				(at -38.1 30.48 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AC6")
			)
			(pin power_in line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AE6")
			)
			(pin power_in line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AG6")
			)
			(pin power_in line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AH7")
			)
			(pin power_in line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AH11")
			)
			(pin power_in line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AK11")
			)
			(pin power_in line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "N6")
			)
			(pin power_in line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "R6")
			)
			(pin power_in line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "U6")
			)
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "W6")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTVCCAUX_G10")
				(number "AA8")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTVCCAUX_G10")
				(number "Y7")
			)
			(pin power_in line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "B11")
			)
			(pin power_in line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "D7")
			)
			(pin power_in line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "D11")
			)
			(pin power_in line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "E6")
			)
			(pin power_in line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "G6")
			)
			(pin power_in line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "J6")
			)
			(pin power_in line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "L6")
			)
			(pin power_in line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTVCCAUX_G11")
				(number "K8")
			)
			(pin power_in line
				(at 38.1 33.02 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AB3")
			)
			(pin power_in line
				(at 38.1 30.48 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AC2")
			)
			(pin power_in line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AF3")
			)
			(pin power_in line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AG2")
			)
			(pin power_in line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AG9")
			)
			(pin power_in line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AJ6")
			)
			(pin power_in line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AJ9")
			)
			(pin power_in line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AK3")
			)
			(pin power_in line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AK7")
			)
			(pin power_in line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "P3")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "R2")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "V3")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "W2")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "B3")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "B7")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "C2")
			)
			(pin power_in line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "C6")
			)
			(pin power_in line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "C9")
			)
			(pin power_in line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "E9")
			)
			(pin power_in line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "F3")
			)
			(pin power_in line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "G2")
			)
			(pin power_in line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "K3")
			)
			(pin power_in line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "L2")
			)
			(pin power_in line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "MGTAVTTRCAL_115")
				(number "N8")
			)
			(pin power_in line
				(at 38.1 -33.02 180)
				(length 6.35)
				(name "MGTRREF_115")
				(number "N7")
			)
		)
		(symbol "XC7K355T-FFG901_9_1"
			(pin power_in line
				(at 25.4 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "J10")
			)
			(pin power_in line
				(at 27.94 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "K11")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "TDI_0")
				(number "H11")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "TDO_0")
				(number "J13")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "TMS_0")
				(number "J11")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TCK_0")
				(number "H12")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "CCLK_0")
				(number "H13")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "M0_0")
				(number "AC13")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "M1_0")
				(number "AC12")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "M2_0")
				(number "AB12")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "DONE_0")
				(number "AC10")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "INIT_B_0")
				(number "H10")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "PROGRAM_B_0")
				(number "AB11")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "CFGBVS_0")
				(number "AC11")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "VP_0")
				(number "R13")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "VN_0")
				(number "T12")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 6.35)
				(name "VREFP_0")
				(number "T13")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "VREFN_0")
				(number "R12")
			)
			(pin bidirectional line
				(at 38.1 -35.56 180)
				(length 6.35)
				(name "DXP_0")
				(number "U13")
			)
			(pin bidirectional line
				(at 38.1 -38.1 180)
				(length 6.35)
				(name "DXN_0")
				(number "U12")
			)
		)
		(symbol "XC7K355T-FFG901_10_1"
			(pin power_in line
				(at -25.4 99.06 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M16")
			)
			(pin power_in line
				(at -25.4 96.52 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P16")
			)
			(pin power_in line
				(at -25.4 93.98 0)
				(length 6.35)
				(name "VCCAUX")
				(number "T16")
			)
			(pin power_in line
				(at -25.4 91.44 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V16")
			)
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "VCCAUX")
				(number "Y16")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "GNDADC_0")
				(number "P12")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "VCCADC_0")
				(number "P13")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "VCCBATT_0")
				(number "G13")
			)
			(pin power_in line
				(at -25.4 76.2 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "AA15")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "R15")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "U15")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "W15")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "A2")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "A5")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "A6")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "A10")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A13")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A24")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "B4")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B8")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B12")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B21")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C1")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "C5")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "C10")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "C13")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "C18")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "C28")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "D3")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "D8")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "D12")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "D13")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "D15")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "D25")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "E1")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "E10")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "E13")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "E22")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "F8")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "F12")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "F13")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "F19")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "F29")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "G1")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "G9")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "G10")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "G11")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 -91.44 0)
				(length 6.35)
				(name "GND")
				(number "G16")
			)
			(pin power_in line
				(at -25.4 -93.98 0)
				(length 6.35)
				(name "GND")
				(number "G26")
			)
			(pin power_in line
				(at -25.4 -96.52 0)
				(length 6.35)
				(name "GND")
				(number "H3")
			)
			(pin power_in line
				(at -25.4 -99.06 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at 25.4 99.06 180)
				(length 6.35)
				(name "VCCINT")
				(number "K12")
			)
			(pin power_in line
				(at 25.4 96.52 180)
				(length 6.35)
				(name "VCCINT")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 93.98 180)
				(length 6.35)
				(name "VCCINT")
				(number "K16")
			)
			(pin power_in line
				(at 25.4 91.44 180)
				(length 6.35)
				(name "VCCINT")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "L13")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "L15")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "R11")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "T10")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "T14")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "U11")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "V10")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "V12")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "W11")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "W13")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y10")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y12")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y14")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "AA11")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "H9")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "H23")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "J1")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "J5")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "J20")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "J30")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "K4")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "K7")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "K15")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "K17")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "K27")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "L1")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "L16")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "L24")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "M3")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "M4")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "M7")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "M8")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "M21")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "N1")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "N5")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "N16")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "N18")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "N28")
			)
			(pin power_in line
				(at 25.4 -91.44 180)
				(length 6.35)
				(name "GND")
				(number "P4")
			)
			(pin power_in line
				(at 25.4 -93.98 180)
				(length 6.35)
				(name "GND")
				(number "P7")
			)
			(pin power_in line
				(at 25.4 -96.52 180)
				(length 6.35)
				(name "GND")
				(number "P8")
			)
			(pin power_in line
				(at 25.4 -99.06 180)
				(length 6.35)
				(name "GND")
				(number "P9")
			)
		)
		(symbol "XC7K355T-FFG901_11_1"
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "GND")
				(number "P11")
			)
			(pin power_in line
				(at -25.4 76.2 0)
				(length 6.35)
				(name "GND")
				(number "P15")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "GND")
				(number "P25")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "GND")
				(number "R9")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "GND")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "GND")
				(number "R14")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "GND")
				(number "R16")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "GND")
				(number "R22")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "GND")
				(number "T3")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "GND")
				(number "T4")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "GND")
				(number "T7")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "GND")
				(number "T8")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "GND")
				(number "T9")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "GND")
				(number "T11")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "GND")
				(number "T15")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "T19")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "T29")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "U1")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "U5")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "U9")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "U10")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "U14")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "U16")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "U26")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "V7")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "V8")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "V9")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "V11")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "V13")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "V15")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "V23")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "W1")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "W5")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "W9")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "W10")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "W12")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "W14")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "W16")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "W20")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "W30")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "Y3")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "Y4")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "Y8")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "Y9")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "Y11")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "Y13")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "Y15")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "Y17")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "Y27")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "AA1")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "AA2")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "AA7")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "AA10")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "AA12")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "AA14")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "AA16")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "AA24")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "GND")
				(number "AB4")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "GND")
				(number "AB7")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "GND")
				(number "AB8")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "GND")
				(number "AB9")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "GND")
				(number "AB10")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "GND")
				(number "AB13")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "GND")
				(number "AB21")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "GND")
				(number "AC1")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "GND")
				(number "AC5")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "GND")
				(number "AC9")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "GND")
				(number "AC18")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "GND")
				(number "AC28")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "GND")
				(number "AD3")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "GND")
				(number "AD4")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "GND")
				(number "AD7")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "GND")
				(number "AD8")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "GND")
				(number "AD9")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "AD10")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "AD11")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "AD12")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "AD13")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "AD15")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "AD25")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "AE1")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "AE2")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "AE5")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "AE9")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "AE10")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "AE13")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "AE22")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "AF4")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "AF7")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "AF8")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "AF11")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "AF12")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "AF13")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "AF19")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "AF29")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "AG1")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "AG5")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "AG10")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "AG13")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "AG16")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "AG26")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "AH3")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "AH4")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "AH8")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "AH12")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "AH13")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "AH23")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "AJ1")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AJ2")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AJ5")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AJ10")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AJ13")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AJ20")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AJ30")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AK4")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AK8")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AK12")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AK13")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "AK17")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "AK27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC7K410T-FBG676"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC7K410T-FBG676"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Kintex 7 T 410 XC7K410T-FBG676"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC7K410T-FBG676_1_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_12")
				(number "U21")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_12")
				(number "U22")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_12")
				(number "V22")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_12")
				(number "U24")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_12")
				(number "U25")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_12")
				(number "V23")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_12")
				(number "V24")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_12")
				(number "U26")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_12")
				(number "V26")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_12")
				(number "W25")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_12")
				(number "W26")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_12")
				(number "V21")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_12")
				(number "W21")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_12")
				(number "AA25")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_12")
				(number "AB25")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_12")
				(number "W23")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_12")
				(number "W24")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_12")
				(number "AB26")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_12")
				(number "AC26")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_12")
				(number "Y25")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_12")
				(number "Y26")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_12")
				(number "AA23")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_12")
				(number "AB24")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_12")
				(number "Y23")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_12")
				(number "AA24")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_12")
				(number "Y22")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_12")
				(number "AA22")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_12")
				(number "AC23")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_12")
				(number "AC24")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_12")
				(number "W20")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_12")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_12")
				(number "AD23")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_12")
				(number "AD24")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_12")
				(number "AB22")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_12")
				(number "AC22")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_12")
				(number "AB21")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_12")
				(number "AC21")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_12")
				(number "AD21")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_12")
				(number "AE21")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_12")
				(number "AF24")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_12")
				(number "AF25")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_12")
				(number "AD26")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_12")
				(number "AE26")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_12")
				(number "AE23")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_12")
				(number "AF23")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_12")
				(number "AD25")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_12")
				(number "AE25")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_12")
				(number "AE22")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_12")
				(number "AF22")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_12")
				(number "Y20")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AA21")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AC25")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AD22")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AF26")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "U23")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "V20")
			)
			(pin power_in line
				(at -25.4 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "Y24")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "K24")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "N25")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "P22")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "R19")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "T16")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "T26")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_13")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_13")
				(number "K25")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_13")
				(number "K26")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_13")
				(number "R26")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_13")
				(number "P26")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_13")
				(number "M25")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_13")
				(number "L25")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_13")
				(number "P24")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_13")
				(number "N24")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_13")
				(number "N26")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_13")
				(number "M26")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_13")
				(number "R25")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_13")
				(number "P25")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_13")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_13")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_13")
				(number "M24")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_13")
				(number "L24")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_13")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_13")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_13")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_13")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_13")
				(number "P23")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_13")
				(number "N23")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_13")
				(number "N21")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_13")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_13")
				(number "R21")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_13")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_13")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_13")
				(number "R23")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_13")
				(number "T24")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_13")
				(number "T25")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_13")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_13")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_13")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_13")
				(number "T23")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_13")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_13")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_13")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_13")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_13")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_13")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_13")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_13")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_13")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_13")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_13")
				(number "U17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_13")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_13")
				(number "R18")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_13")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_13")
				(number "U16")
			)
		)
		(symbol "XC7K410T-FBG676_2_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_14")
				(number "K21")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_D00_MOSI_14")
				(number "B24")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_D01_DIN_14")
				(number "A25")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_D02_14")
				(number "B22")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_D03_14")
				(number "A22")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_PUDC_B_14")
				(number "B25")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_EMCCLK_14")
				(number "B26")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_D04_14")
				(number "A23")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_D05_14")
				(number "A24")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_D06_14")
				(number "D26")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_D07_14")
				(number "C26")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_FCS_B_14")
				(number "C23")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_D08_VREF_14")
				(number "C24")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_D09_14")
				(number "D21")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_D10_14")
				(number "C22")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_D11_14")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_D12_14")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_14")
				(number "E21")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_D13_14")
				(number "E22")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_D14_14")
				(number "C21")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_D15_14")
				(number "B21")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_14")
				(number "D23")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_14")
				(number "D24")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_14")
				(number "F22")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_14")
				(number "E23")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_14")
				(number "G22")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_14")
				(number "F23")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_14")
				(number "G24")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_14")
				(number "F24")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_RDWR_B_14")
				(number "E25")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_DOUT_CSO_B_14")
				(number "D25")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_CSI_B_14")
				(number "G25")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_A15_D31_14")
				(number "G26")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_A14_D30_14")
				(number "F25")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_A13_D29_14")
				(number "E26")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_A12_D28_14")
				(number "J26")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_A11_D27_14")
				(number "H26")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_A10_D26_14")
				(number "H21")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_A09_D25_VREF_14")
				(number "G21")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_A08_D24_14")
				(number "H23")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_A07_D23_14")
				(number "H24")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_14")
				(number "J21")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A06_D22_14")
				(number "H22")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_A05_D21_14")
				(number "J24")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_A04_D20_14")
				(number "J25")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_A03_D19_14")
				(number "L22")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_A02_D18_14")
				(number "K22")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_A01_D17_14")
				(number "K23")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_A00_D16_14")
				(number "J23")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_14")
				(number "L23")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "A21")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "C25")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "D22")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "F26")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "G23")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "L21")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "B18")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "E19")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "F16")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "H20")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "J17")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_15")
				(number "K15")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_AD0P_15")
				(number "C16")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_AD0N_15")
				(number "B16")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_AD8P_15")
				(number "A18")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_AD8N_15")
				(number "A19")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_AD1P_15")
				(number "B17")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_AD1N_15")
				(number "A17")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_AD9P_15")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_AD9N_15")
				(number "B19")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_AD2P_15")
				(number "C17")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_AD2N_15")
				(number "C18")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_15")
				(number "D15")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_15")
				(number "D16")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_AD10P_15")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_AD10N_15")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_AD3P_15")
				(number "G15")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_AD3N_15")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_AD11P_15")
				(number "J15")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_AD11N_15")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_AD4P_15")
				(number "E15")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_AD4N_15")
				(number "E16")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_AD12P_15")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_AD12N_15")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_AD5P_15")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_AD5N_15")
				(number "E17")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_15")
				(number "E18")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_15")
				(number "D18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_15")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_15")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_15")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_ADV_B_15")
				(number "D20")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_A28_15")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_A27_15")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_A26_15")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_A25_15")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_A24_15")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_A23_15")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_A22_15")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_A21_VREF_15")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_A20_15")
				(number "J18")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_A19_15")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_15")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A18_15")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_A17_15")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_A16_15")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_FOE_B_15")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_FWE_B_15")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_RS1_15")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_RS0_15")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_15")
				(number "M16")
			)
		)
		(symbol "XC7K410T-FBG676_3_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_16")
				(number "J8")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_16")
				(number "H9")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_16")
				(number "H8")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_16")
				(number "G10")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_16")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_16")
				(number "J13")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_16")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_16")
				(number "J11")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_16")
				(number "J10")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_16")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_16")
				(number "G14")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_16")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_16")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_16")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_16")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_16")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_16")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_16")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_16")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_16")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_16")
				(number "B9")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_16")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_16")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_16")
				(number "E10")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_16")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_16")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_16")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_16")
				(number "E11")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_16")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_16")
				(number "F14")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_16")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_16")
				(number "G12")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_16")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_16")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_16")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_16")
				(number "E13")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_16")
				(number "E12")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_16")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_16")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_16")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_16")
				(number "B11")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_16")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_16")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_16")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_16")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_16")
				(number "B15")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_16")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_16")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_16")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_16")
				(number "J14")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "A11")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "B8")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "C15")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "D12")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "E9")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "G13")
			)
			(pin power_in line
				(at -25.4 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "H10")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AB18")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AC15")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AE19")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AF16")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "W17")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "Y14")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_32")
				(number "V13")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_32")
				(number "AE17")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_32")
				(number "AF17")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_32")
				(number "AF14")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_32")
				(number "AF15")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_32")
				(number "AE18")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_32")
				(number "AF18")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_32")
				(number "AD15")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_32")
				(number "AE15")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_32")
				(number "AF19")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_32")
				(number "AF20")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_32")
				(number "AD16")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_32")
				(number "AE16")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_32")
				(number "AA14")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_32")
				(number "AA15")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_32")
				(number "AC14")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_32")
				(number "AD14")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_32")
				(number "Y15")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_32")
				(number "Y16")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_32")
				(number "AB14")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_32")
				(number "AB15")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_32")
				(number "AA17")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_32")
				(number "AA18")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_32")
				(number "AB16")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_32")
				(number "AC16")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_32")
				(number "AC18")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_32")
				(number "AD18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_32")
				(number "AB17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_32")
				(number "AC17")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_32")
				(number "AD20")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_32")
				(number "AE20")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_32")
				(number "AA19")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_32")
				(number "AA20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_32")
				(number "AC19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_32")
				(number "AD19")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_32")
				(number "AB19")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_32")
				(number "AB20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_32")
				(number "Y17")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_32")
				(number "Y18")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_32")
				(number "V16")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_32")
				(number "V17")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_32")
				(number "W18")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_32")
				(number "W19")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_32")
				(number "W15")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_32")
				(number "W16")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_32")
				(number "V18")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_32")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_32")
				(number "V14")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_32")
				(number "W14")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_32")
				(number "W13")
			)
		)
		(symbol "XC7K410T-FBG676_4_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_VRN_33")
				(number "U9")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_33")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_33")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_33")
				(number "V8")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_33")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_33")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_33")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_33")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_33")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_33")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_33")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_33")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_33")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_33")
				(number "AE7")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_33")
				(number "AF7")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_33")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_33")
				(number "AA7")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_33")
				(number "AC8")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_33")
				(number "AD8")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_33")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_33")
				(number "AC7")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_33")
				(number "AA9")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_33")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_33")
				(number "AC9")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_33")
				(number "AD9")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_33")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_33")
				(number "AC11")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_33")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_33")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_33")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_33")
				(number "AC12")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_33")
				(number "AA13")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_33")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_33")
				(number "AC13")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_33")
				(number "AD13")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_33")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_33")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_33")
				(number "AD11")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_33")
				(number "AE11")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_33")
				(number "AD10")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_33")
				(number "AE10")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_33")
				(number "AE12")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_33")
				(number "AF12")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_33")
				(number "AE8")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_33")
				(number "AF8")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_33")
				(number "AE13")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_33")
				(number "AF13")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_33")
				(number "AF10")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_33")
				(number "AF9")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_VRP_33")
				(number "V12")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AA11")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AB8")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AD12")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AE9")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "V10")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "W7")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AA1")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AC5")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AD2")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AF6")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "U3")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "Y4")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_34")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_34")
				(number "U6")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_34")
				(number "U5")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_34")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_34")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_34")
				(number "W6")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_34")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_34")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_34")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_34")
				(number "U7")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_34")
				(number "V6")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_34")
				(number "V4")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_34")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_34")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_34")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_34")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_34")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_34")
				(number "AB1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_34")
				(number "AC1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_34")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_34")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_34")
				(number "AB2")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_34")
				(number "AC2")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_34")
				(number "AA3")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_34")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_34")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_34")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_34")
				(number "AC4")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_34")
				(number "AC3")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_34")
				(number "AA5")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_34")
				(number "AB5")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_34")
				(number "AB6")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_34")
				(number "AC6")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_34")
				(number "Y6")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_34")
				(number "Y5")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_34")
				(number "AD6")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_34")
				(number "AD5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_34")
				(number "AD4")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_34")
				(number "AD3")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_34")
				(number "AD1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_34")
				(number "AE1")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_34")
				(number "AF5")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_34")
				(number "AF4")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_34")
				(number "AE3")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_34")
				(number "AE2")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_34")
				(number "AE6")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_34")
				(number "AE5")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_34")
				(number "AF3")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_34")
				(number "AF2")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_34")
				(number "T7")
			)
		)
		(symbol "XC7K410T-FBG676_5_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_115")
				(number "P2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_115")
				(number "P1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_115")
				(number "M2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_115")
				(number "M1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_115")
				(number "K2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_115")
				(number "K1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_115")
				(number "H2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_115")
				(number "H1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_115")
				(number "R4")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_115")
				(number "R3")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_115")
				(number "N4")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_115")
				(number "N3")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_115")
				(number "L4")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_115")
				(number "L3")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_115")
				(number "J4")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_115")
				(number "J3")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_115")
				(number "H6")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_115")
				(number "H5")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_115")
				(number "K6")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_115")
				(number "K5")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_116")
				(number "F2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_116")
				(number "F1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_116")
				(number "D2")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_116")
				(number "D1")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_116")
				(number "B2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_116")
				(number "B1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_116")
				(number "A4")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_116")
				(number "A3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_116")
				(number "G4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_116")
				(number "G3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_116")
				(number "E4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_116")
				(number "E3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_116")
				(number "C4")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_116")
				(number "C3")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_116")
				(number "B6")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_116")
				(number "B5")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_116")
				(number "D6")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_116")
				(number "D5")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_116")
				(number "F6")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_116")
				(number "F5")
			)
		)
		(symbol "XC7K410T-FBG676_6_1"
			(pin power_in line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "C6")
			)
			(pin power_in line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "E6")
			)
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "G6")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "J6")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "L6")
			)
			(pin power_in line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTVCCAUX")
				(number "N6")
			)
			(pin power_in line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "B3")
			)
			(pin power_in line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "C2")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "D3")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "G2")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "H3")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "L2")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "M3")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTTRCAL_115")
				(number "M5")
			)
			(pin power_in line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTRREF_115")
				(number "M6")
			)
		)
		(symbol "XC7K410T-FBG676_7_1"
			(pin power_in line
				(at 25.4 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "L7")
			)
			(pin power_in line
				(at 27.94 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "T6")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "TDI_0")
				(number "R6")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "TDO_0")
				(number "R7")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "TMS_0")
				(number "N8")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TCK_0")
				(number "L8")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "CCLK_0")
				(number "C8")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "M0_0")
				(number "T5")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "M1_0")
				(number "T2")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "M2_0")
				(number "P5")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "DONE_0")
				(number "J7")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "INIT_B_0")
				(number "G7")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "PROGRAM_B_0")
				(number "P6")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "CFGBVS_0")
				(number "P7")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "VP_0")
				(number "N12")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "VN_0")
				(number "P11")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 6.35)
				(name "VREFP_0")
				(number "P12")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "VREFN_0")
				(number "N11")
			)
			(pin bidirectional line
				(at 38.1 -35.56 180)
				(length 6.35)
				(name "DXP_0")
				(number "R12")
			)
			(pin bidirectional line
				(at 38.1 -38.1 180)
				(length 6.35)
				(name "DXN_0")
				(number "R11")
			)
		)
		(symbol "XC7K410T-FBG676_8_1"
			(pin power_in line
				(at -25.4 99.06 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 96.52 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M10")
			)
			(pin power_in line
				(at -25.4 93.98 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P10")
			)
			(pin power_in line
				(at -25.4 91.44 0)
				(length 6.35)
				(name "VCCAUX")
				(number "T10")
			)
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "T8")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "R9")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "P8")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "GNDADC_0")
				(number "M11")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCADC_0")
				(number "M12")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCBATT_0")
				(number "E8")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "N13")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "R13")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "T12")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "U13")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "GND")
				(number "A2")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "GND")
				(number "A5")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "GND")
				(number "A6")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "GND")
				(number "A7")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "GND")
				(number "A16")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "A26")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "B4")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "B23")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "C1")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "C5")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "C7")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "C10")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "C20")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "D7")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "D17")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "E1")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "E14")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E24")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "F3")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "F21")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G1")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "H25")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "J1")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "J5")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "J12")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "J22")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "K3")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "K4")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "K7")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "K11")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "K13")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "K19")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "L1")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "L10")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "L12")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "L14")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "L16")
			)
			(pin power_in line
				(at -25.4 -91.44 0)
				(length 6.35)
				(name "GND")
				(number "L26")
			)
			(pin power_in line
				(at -25.4 -93.98 0)
				(length 6.35)
				(name "GND")
				(number "M4")
			)
			(pin power_in line
				(at -25.4 -96.52 0)
				(length 6.35)
				(name "GND")
				(number "M7")
			)
			(pin power_in line
				(at -25.4 -99.06 0)
				(length 6.35)
				(name "GND")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 99.06 180)
				(length 6.35)
				(name "VCCINT")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 96.52 180)
				(length 6.35)
				(name "VCCINT")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 93.98 180)
				(length 6.35)
				(name "VCCINT")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 91.44 180)
				(length 6.35)
				(name "VCCINT")
				(number "K12")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "L13")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "L15")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "M8")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "R15")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "T14")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "U15")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "GND")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "GND")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "GND")
				(number "M23")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "GND")
				(number "N1")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "GND")
				(number "N5")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "N7")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "N20")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "P3")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "P4")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "P15")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "P17")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "R2")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "R8")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "R10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "R24")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "T1")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "T3")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "T4")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "T9")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "T11")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "T13")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "T15")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "T21")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "U8")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "U10")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U14")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "U18")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V5")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "V15")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "V25")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "W2")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "W12")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "W22")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "Y9")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "Y19")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AA6")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AA16")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AA26")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AB3")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AB13")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AB23")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "AC10")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "AC20")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "AD7")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "AD17")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "AE4")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "AE14")
			)
			(pin power_in line
				(at 25.4 -91.44 180)
				(length 6.35)
				(name "GND")
				(number "AE24")
			)
			(pin power_in line
				(at 25.4 -93.98 180)
				(length 6.35)
				(name "GND")
				(number "AF1")
			)
			(pin power_in line
				(at 25.4 -96.52 180)
				(length 6.35)
				(name "GND")
				(number "AF11")
			)
			(pin power_in line
				(at 25.4 -99.06 180)
				(length 6.35)
				(name "GND")
				(number "AF21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC7K410T-FBG900"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC7K410T-FBG900"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Kintex 7 T 410 XC7K410T-FBG900"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC7K410T-FBG900_1_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_12")
				(number "Y20")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_12")
				(number "Y23")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_12")
				(number "Y24")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_12")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_12")
				(number "AA21")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_12")
				(number "AB22")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_12")
				(number "AB23")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_12")
				(number "AA22")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_12")
				(number "AA23")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_12")
				(number "AC20")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_12")
				(number "AC21")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_12")
				(number "AA20")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_12")
				(number "AB20")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_12")
				(number "AB24")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_12")
				(number "AC25")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_12")
				(number "AC22")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_12")
				(number "AD22")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_12")
				(number "AC24")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_12")
				(number "AD24")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_12")
				(number "AD21")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_12")
				(number "AE21")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_12")
				(number "AE23")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_12")
				(number "AF23")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_12")
				(number "AD23")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_12")
				(number "AE24")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_12")
				(number "AF22")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_12")
				(number "AG23")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_12")
				(number "AG24")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_12")
				(number "AH24")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_12")
				(number "AJ24")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_12")
				(number "AK25")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_12")
				(number "AE25")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_12")
				(number "AF25")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_12")
				(number "AK23")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_12")
				(number "AK24")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_12")
				(number "AG25")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_12")
				(number "AH25")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_12")
				(number "AF20")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_12")
				(number "AF21")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_12")
				(number "AG22")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_12")
				(number "AH22")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_12")
				(number "AJ22")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_12")
				(number "AJ23")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_12")
				(number "AG20")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_12")
				(number "AH20")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_12")
				(number "AH21")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_12")
				(number "AJ21")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_12")
				(number "AK20")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_12")
				(number "AK21")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_12")
				(number "AE20")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AC23")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AD20")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AF24")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AG21")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AK22")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "Y22")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AA29")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AB26")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AD30")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AE27")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AH28")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AJ25")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_13")
				(number "Y25")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_13")
				(number "Y26")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_13")
				(number "AA26")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_13")
				(number "W27")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_13")
				(number "W28")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_13")
				(number "Y28")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_13")
				(number "AA28")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_13")
				(number "W29")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_13")
				(number "Y29")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_13")
				(number "AA27")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_13")
				(number "AB28")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_13")
				(number "AA25")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_13")
				(number "AB25")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_13")
				(number "AC29")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_13")
				(number "AC30")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_13")
				(number "Y30")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_13")
				(number "AA30")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_13")
				(number "AD29")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_13")
				(number "AE29")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_13")
				(number "AB29")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_13")
				(number "AB30")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_13")
				(number "AD27")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_13")
				(number "AD28")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_13")
				(number "AB27")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_13")
				(number "AC27")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_13")
				(number "AG29")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_13")
				(number "AH29")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_13")
				(number "AE28")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_13")
				(number "AF28")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_13")
				(number "AK29")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_13")
				(number "AK30")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_13")
				(number "AE30")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_13")
				(number "AF30")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_13")
				(number "AJ28")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_13")
				(number "AJ29")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_13")
				(number "AG30")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_13")
				(number "AH30")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_13")
				(number "AC26")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_13")
				(number "AD26")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_13")
				(number "AJ27")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_13")
				(number "AK28")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_13")
				(number "AG27")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_13")
				(number "AG28")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_13")
				(number "AH26")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_13")
				(number "AH27")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_13")
				(number "AF26")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_13")
				(number "AF27")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_13")
				(number "AJ26")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_13")
				(number "AK26")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_13")
				(number "AE26")
			)
		)
		(symbol "XC7K410T-FBG900_2_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_14")
				(number "R19")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_D00_MOSI_14")
				(number "P24")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_D01_DIN_14")
				(number "R25")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_D02_14")
				(number "R20")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_D03_14")
				(number "R21")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_PUDC_B_14")
				(number "R23")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_EMCCLK_14")
				(number "R24")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_D04_14")
				(number "T20")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_D05_14")
				(number "T21")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_D06_14")
				(number "T22")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_D07_14")
				(number "T23")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_FCS_B_14")
				(number "U19")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_D08_VREF_14")
				(number "U20")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_D09_14")
				(number "P29")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_D10_14")
				(number "R29")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_D11_14")
				(number "P27")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_D12_14")
				(number "P28")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_14")
				(number "R30")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_D13_14")
				(number "T30")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_D14_14")
				(number "P26")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_D15_14")
				(number "R26")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_14")
				(number "R28")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_14")
				(number "T28")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_14")
				(number "T26")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_14")
				(number "T27")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_14")
				(number "U27")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_14")
				(number "U28")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_14")
				(number "T25")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_14")
				(number "U25")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_RDWR_B_14")
				(number "U29")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_DOUT_CSO_B_14")
				(number "U30")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_CSI_B_14")
				(number "V26")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_A15_D31_14")
				(number "V27")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_A14_D30_14")
				(number "V29")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_A13_D29_14")
				(number "V30")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_A12_D28_14")
				(number "V25")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_A11_D27_14")
				(number "W26")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_A10_D26_14")
				(number "V19")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_A09_D25_VREF_14")
				(number "V20")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_A08_D24_14")
				(number "W23")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_A07_D23_14")
				(number "W24")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_14")
				(number "U22")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A06_D22_14")
				(number "U23")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_A05_D21_14")
				(number "V21")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_A04_D20_14")
				(number "V22")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_A03_D19_14")
				(number "U24")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_A02_D18_14")
				(number "V24")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_A01_D17_14")
				(number "W21")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_A00_D16_14")
				(number "W22")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_14")
				(number "W19")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "P30")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "R27")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "T24")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "U21")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "V28")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "W25")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "J25")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "K22")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "L29")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "M26")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "N23")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_15")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_AD0P_15")
				(number "J23")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_AD0N_15")
				(number "J24")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_AD8P_15")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_AD8N_15")
				(number "L23")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_AD1P_15")
				(number "K23")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_AD1N_15")
				(number "K24")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_AD9P_15")
				(number "L21")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_AD9N_15")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_AD2P_15")
				(number "J21")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_AD2N_15")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_15")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_15")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_AD10P_15")
				(number "J29")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_AD10N_15")
				(number "H29")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_AD3P_15")
				(number "J27")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_AD3N_15")
				(number "J28")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_AD11P_15")
				(number "L30")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_AD11N_15")
				(number "K30")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_AD4P_15")
				(number "K26")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_AD4N_15")
				(number "J26")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_AD12P_15")
				(number "L26")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_AD12N_15")
				(number "L27")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_AD5P_15")
				(number "L25")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_AD5N_15")
				(number "K25")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_15")
				(number "K28")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_15")
				(number "K29")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_15")
				(number "M28")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_15")
				(number "L28")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_15")
				(number "M29")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_ADV_B_15")
				(number "M30")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_A28_15")
				(number "N27")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_A27_15")
				(number "M27")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_A26_15")
				(number "N29")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_A25_15")
				(number "N30")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_A24_15")
				(number "N25")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_A23_15")
				(number "N26")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_A22_15")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_A21_VREF_15")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_A20_15")
				(number "N21")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_A19_15")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_15")
				(number "P23")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A18_15")
				(number "N24")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_A17_15")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_A16_15")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_FOE_B_15")
				(number "M24")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_FWE_B_15")
				(number "M25")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_RS1_15")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_RS0_15")
				(number "M23")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_15")
				(number "P19")
			)
		)
		(symbol "XC7K410T-FBG900_3_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_16")
				(number "F23")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_16")
				(number "B23")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_16")
				(number "A23")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_16")
				(number "E23")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_16")
				(number "D23")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_16")
				(number "F25")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_16")
				(number "E25")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_16")
				(number "E24")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_16")
				(number "D24")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_16")
				(number "F26")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_16")
				(number "E26")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_16")
				(number "G23")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_16")
				(number "G24")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_16")
				(number "B27")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_16")
				(number "A27")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_16")
				(number "C24")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_16")
				(number "B24")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_16")
				(number "B28")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_16")
				(number "A28")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_16")
				(number "A25")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_16")
				(number "A26")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_16")
				(number "D26")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_16")
				(number "C26")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_16")
				(number "C25")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_16")
				(number "B25")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_16")
				(number "D27")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_16")
				(number "C27")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_16")
				(number "E28")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_16")
				(number "D28")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_16")
				(number "C29")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_16")
				(number "B29")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_16")
				(number "D29")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_16")
				(number "C30")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_16")
				(number "B30")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_16")
				(number "A30")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_16")
				(number "E29")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_16")
				(number "E30")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_16")
				(number "H24")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_16")
				(number "H25")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_16")
				(number "G28")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_16")
				(number "F28")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_16")
				(number "G27")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_16")
				(number "F27")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_16")
				(number "G29")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_16")
				(number "F30")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_16")
				(number "H26")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_16")
				(number "H27")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_16")
				(number "H30")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_16")
				(number "G30")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_16")
				(number "G25")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "A29")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "B26")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "C23")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "D30")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "E27")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "F24")
			)
			(pin power_in line
				(at -25.4 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "H28")
			)
			(pin power_in line
				(at 25.4 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "A19")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "B16")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "D20")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "E17")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "G21")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "H18")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_17")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_17")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_17")
				(number "J18")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_17")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_17")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_17")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_17")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_17")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_17")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_17")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_17")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_17")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_17")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_17")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_17")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_17")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_17")
				(number "C21")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_17")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_17")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_17")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_17")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_17")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_17")
				(number "E21")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_17")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_17")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_17")
				(number "D17")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_17")
				(number "D18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_17")
				(number "E19")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_17")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_17")
				(number "D16")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_17")
				(number "C16")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_17")
				(number "G18")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_17")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_17")
				(number "C17")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_17")
				(number "B17")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_17")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_17")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_17")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_17")
				(number "B20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_17")
				(number "A16")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_17")
				(number "A17")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_17")
				(number "A20")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_17")
				(number "A21")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_17")
				(number "B18")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_17")
				(number "A18")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_17")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_17")
				(number "A22")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_17")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_17")
				(number "B19")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_17")
				(number "E18")
			)
		)
		(symbol "XC7K410T-FBG900_4_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_18")
				(number "G12")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_18")
				(number "L16")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_18")
				(number "K16")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_18")
				(number "L15")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_18")
				(number "K15")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_18")
				(number "L12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_18")
				(number "L13")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_18")
				(number "K13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_18")
				(number "J13")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_18")
				(number "K14")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_18")
				(number "J14")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_18")
				(number "L11")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_18")
				(number "K11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_18")
				(number "H15")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_18")
				(number "G15")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_18")
				(number "J11")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_18")
				(number "J12")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_18")
				(number "J16")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_18")
				(number "H16")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_18")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_18")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_18")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_18")
				(number "G14")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_18")
				(number "G13")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_18")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_18")
				(number "D12")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_18")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_18")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_18")
				(number "E13")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_18")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_18")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_18")
				(number "F11")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_18")
				(number "E11")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_18")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_18")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_18")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_18")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_18")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_18")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_18")
				(number "E14")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_18")
				(number "E15")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_18")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_18")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_18")
				(number "B13")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_18")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_18")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_18")
				(number "B15")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_18")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_18")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_18")
				(number "F16")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "C13")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "D10")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "F14")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "G11")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "J15")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "K12")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AA19")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AB16")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AE17")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AF14")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AH18")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AJ15")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_32")
				(number "Y14")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_32")
				(number "AK16")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_32")
				(number "AK15")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_32")
				(number "AG15")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_32")
				(number "AH15")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_32")
				(number "AH16")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_32")
				(number "AJ16")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_32")
				(number "AF15")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_32")
				(number "AG14")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_32")
				(number "AH17")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_32")
				(number "AJ17")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_32")
				(number "AE16")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_32")
				(number "AF16")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_32")
				(number "AJ19")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_32")
				(number "AK19")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_32")
				(number "AG19")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_32")
				(number "AH19")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_32")
				(number "AJ18")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_32")
				(number "AK18")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_32")
				(number "AD19")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_32")
				(number "AE19")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_32")
				(number "AF18")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_32")
				(number "AG18")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_32")
				(number "AF17")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_32")
				(number "AG17")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_32")
				(number "AD18")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_32")
				(number "AE18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_32")
				(number "AD17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_32")
				(number "AD16")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_32")
				(number "Y19")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_32")
				(number "Y18")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_32")
				(number "AA18")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_32")
				(number "AB18")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_32")
				(number "AB19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_32")
				(number "AC19")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_32")
				(number "AB17")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_32")
				(number "AC17")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_32")
				(number "AE15")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_32")
				(number "AE14")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_32")
				(number "AA15")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_32")
				(number "AB15")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_32")
				(number "AC16")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_32")
				(number "AC15")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_32")
				(number "AC14")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_32")
				(number "AD14")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_32")
				(number "AA17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_32")
				(number "AA16")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_32")
				(number "Y16")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_32")
				(number "Y15")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_32")
				(number "AB14")
			)
		)
		(symbol "XC7K410T-FBG900_5_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_VRN_33")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_33")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_33")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_33")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_33")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_33")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_33")
				(number "AC9")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_33")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_33")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_33")
				(number "AA11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_33")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_33")
				(number "AA13")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_33")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_33")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_33")
				(number "AC10")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_33")
				(number "AD8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_33")
				(number "AE8")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_33")
				(number "AC12")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_33")
				(number "AC11")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_33")
				(number "AD9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_33")
				(number "AE9")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_33")
				(number "AE11")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_33")
				(number "AF11")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_33")
				(number "AD12")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_33")
				(number "AD11")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_33")
				(number "AG10")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_33")
				(number "AH10")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_33")
				(number "AE10")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_33")
				(number "AF10")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_33")
				(number "AJ9")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_33")
				(number "AK9")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_33")
				(number "AG9")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_33")
				(number "AH9")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_33")
				(number "AK11")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_33")
				(number "AK10")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_33")
				(number "AH11")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_33")
				(number "AJ11")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_33")
				(number "AE13")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_33")
				(number "AF13")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_33")
				(number "AK14")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_33")
				(number "AK13")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_33")
				(number "AH14")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_33")
				(number "AJ14")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_33")
				(number "AJ13")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_33")
				(number "AJ12")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_33")
				(number "AF12")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_33")
				(number "AG12")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_33")
				(number "AG13")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_33")
				(number "AH12")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_VRP_33")
				(number "AD13")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AA9")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AC13")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AD10")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AG11")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AK12")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "Y12")
			)
			(pin power_in line
				(at 25.4 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AC3")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AE7")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AF4")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AG1")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AH8")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AJ5")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AK2")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_34")
				(number "AC6")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_34")
				(number "AD4")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_34")
				(number "AD3")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_34")
				(number "AC2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_34")
				(number "AC1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_34")
				(number "AD2")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_34")
				(number "AD1")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_34")
				(number "AC5")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_34")
				(number "AC4")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_34")
				(number "AD6")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_34")
				(number "AE6")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_34")
				(number "AC7")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_34")
				(number "AD7")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_34")
				(number "AF3")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_34")
				(number "AF2")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_34")
				(number "AE1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_34")
				(number "AF1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_34")
				(number "AG4")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_34")
				(number "AG3")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_34")
				(number "AE4")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_34")
				(number "AE3")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_34")
				(number "AE5")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_34")
				(number "AF5")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_34")
				(number "AF6")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_34")
				(number "AG5")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_34")
				(number "AH4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_34")
				(number "AJ4")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_34")
				(number "AH6")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_34")
				(number "AH5")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_34")
				(number "AG2")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_34")
				(number "AH1")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_34")
				(number "AH2")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_34")
				(number "AJ2")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_34")
				(number "AJ1")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_34")
				(number "AK1")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_34")
				(number "AJ3")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_34")
				(number "AK3")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_34")
				(number "AF8")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_34")
				(number "AG8")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_34")
				(number "AF7")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_34")
				(number "AG7")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_34")
				(number "AH7")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_34")
				(number "AJ7")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_34")
				(number "AJ6")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_34")
				(number "AK6")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_34")
				(number "AJ8")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_34")
				(number "AK8")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_34")
				(number "AK5")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_34")
				(number "AK4")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_34")
				(number "AB7")
			)
		)
		(symbol "XC7K410T-FBG900_6_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_115")
				(number "Y2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_115")
				(number "Y1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_115")
				(number "V2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_115")
				(number "V1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_115")
				(number "U4")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_115")
				(number "U3")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_115")
				(number "T2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_115")
				(number "T1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_115")
				(number "AA4")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_115")
				(number "AA3")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_115")
				(number "Y6")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_115")
				(number "Y5")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_115")
				(number "W4")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_115")
				(number "W3")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_115")
				(number "V6")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_115")
				(number "V5")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_115")
				(number "R8")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_115")
				(number "R7")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_115")
				(number "U8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_115")
				(number "U7")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_116")
				(number "P2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_116")
				(number "P1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_116")
				(number "N4")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_116")
				(number "N3")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_116")
				(number "M2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_116")
				(number "M1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_116")
				(number "L4")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_116")
				(number "L3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_116")
				(number "T6")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_116")
				(number "T5")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_116")
				(number "R4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_116")
				(number "R3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_116")
				(number "P6")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_116")
				(number "P5")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_116")
				(number "M6")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_116")
				(number "M5")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_116")
				(number "L8")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_116")
				(number "L7")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_116")
				(number "N8")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_116")
				(number "N7")
			)
		)
		(symbol "XC7K410T-FBG900_7_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_117")
				(number "K2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_117")
				(number "K1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_117")
				(number "J4")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_117")
				(number "J3")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_117")
				(number "H2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_117")
				(number "H1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_117")
				(number "F2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_117")
				(number "F1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_117")
				(number "K6")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_117")
				(number "K5")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_117")
				(number "H6")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_117")
				(number "H5")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_117")
				(number "G4")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_117")
				(number "G3")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_117")
				(number "F6")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_117")
				(number "F5")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_117")
				(number "G8")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_117")
				(number "G7")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_117")
				(number "J8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_117")
				(number "J7")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_118")
				(number "D2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_118")
				(number "D1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_118")
				(number "C4")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_118")
				(number "C3")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_118")
				(number "B2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_118")
				(number "B1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_118")
				(number "A4")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_118")
				(number "A3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_118")
				(number "E4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_118")
				(number "E3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_118")
				(number "D6")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_118")
				(number "D5")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_118")
				(number "B6")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_118")
				(number "B5")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_118")
				(number "A8")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_118")
				(number "A7")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_118")
				(number "C8")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_118")
				(number "C7")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_118")
				(number "E8")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_118")
				(number "E7")
			)
		)
		(symbol "XC7K410T-FBG900_8_1"
			(pin power_in line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "B7")
			)
			(pin power_in line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "D7")
			)
			(pin power_in line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "F7")
			)
			(pin power_in line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "H7")
			)
			(pin power_in line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "K7")
			)
			(pin power_in line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "M7")
			)
			(pin power_in line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "P7")
			)
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTVCCAUX")
				(number "T7")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTVCCAUX")
				(number "V7")
			)
			(pin power_in line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "B3")
			)
			(pin power_in line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "C5")
			)
			(pin power_in line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "D3")
			)
			(pin power_in line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "E5")
			)
			(pin power_in line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "F3")
			)
			(pin power_in line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "G5")
			)
			(pin power_in line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "H3")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "J5")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "K3")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "L5")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "M3")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "N5")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "P3")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "R5")
			)
			(pin power_in line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "T3")
			)
			(pin power_in line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "U5")
			)
			(pin power_in line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "V3")
			)
			(pin power_in line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "W5")
			)
			(pin power_in line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTAVTTRCAL_115")
				(number "W7")
			)
			(pin power_in line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTRREF_115")
				(number "W8")
			)
		)
		(symbol "XC7K410T-FBG900_9_1"
			(pin power_in line
				(at 25.4 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "AB6")
			)
			(pin power_in line
				(at 27.94 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "T9")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "TDI_0")
				(number "H10")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "TDO_0")
				(number "G10")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "TMS_0")
				(number "F10")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TCK_0")
				(number "E10")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "CCLK_0")
				(number "B10")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "M0_0")
				(number "AB5")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "M1_0")
				(number "AB2")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "M2_0")
				(number "AB1")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "DONE_0")
				(number "M10")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "INIT_B_0")
				(number "A10")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "PROGRAM_B_0")
				(number "K10")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "CFGBVS_0")
				(number "L10")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "VP_0")
				(number "R15")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "VN_0")
				(number "T14")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 6.35)
				(name "VREFP_0")
				(number "T15")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "VREFN_0")
				(number "R14")
			)
			(pin bidirectional line
				(at 38.1 -35.56 180)
				(length 6.35)
				(name "DXP_0")
				(number "U15")
			)
			(pin bidirectional line
				(at 38.1 -38.1 180)
				(length 6.35)
				(name "DXN_0")
				(number "U14")
			)
		)
		(symbol "XC7K410T-FBG900_10_1"
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P13")
			)
			(pin power_in line
				(at -25.4 86.36 0)
				(length 6.35)
				(name "VCCAUX")
				(number "T13")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V13")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V15")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "VCCAUX")
				(number "W14")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "W12")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "V11")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "W10")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "GNDADC_0")
				(number "P14")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCADC_0")
				(number "P15")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCBATT_0")
				(number "C10")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "N16")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "R16")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "U16")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "W16")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "A2")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "A5")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "A6")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "A14")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "A24")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "B4")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "B8")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "B21")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "C1")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "C2")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "C9")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "C18")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C28")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "D8")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "D9")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "D15")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "D25")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "E1")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "E6")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "E9")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "E12")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "E22")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "F8")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "F9")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "F19")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "F29")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "G1")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "G2")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "G6")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "G9")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "G16")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "G26")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "H13")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "H23")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "J1")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "J6")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "M17")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "N18")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "P17")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "R10")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "R12")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "T11")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "T17")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "U10")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "U18")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "V17")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "W18")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "J20")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "J30")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "K4")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "K17")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "K27")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "L1")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "L2")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "L6")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "L24")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "M4")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "M8")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "M16")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "M18")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "M21")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "N1")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "N6")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "N28")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "P4")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "P8")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "P16")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "P18")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "P25")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "R2")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "R6")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "R9")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "R11")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "R13")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "R17")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "R22")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "T4")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "T8")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "T10")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "T12")
			)
		)
		(symbol "XC7K410T-FBG900_11_1"
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "GND")
				(number "T18")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "GND")
				(number "T19")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "GND")
				(number "T29")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "U1")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "U6")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "U9")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "U13")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "U17")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "U26")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "V8")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "V9")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "V12")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "V16")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "V18")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "V23")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "W1")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "W2")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "W6")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "W9")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "W11")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "W13")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "W15")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "W17")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "W20")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "W30")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "Y3")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "Y4")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "Y7")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "Y8")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "Y9")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "Y17")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "GND")
				(number "Y27")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "GND")
				(number "AA1")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "GND")
				(number "AA2")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "AA6")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "AA7")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "AA14")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "AA24")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "AB3")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "AB4")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "AB11")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "AB21")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "AC8")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "AC18")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "AC28")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "AD5")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "AD15")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "AD25")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "AE2")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "AE12")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "AE22")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "AF9")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "AF19")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "AF29")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "AG6")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "AG16")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "AG26")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "AH3")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "AH13")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "AH23")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "AJ10")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "AJ20")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "AJ30")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "AK7")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "AK17")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "AK27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC7K410T-FFG676"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC7K410T-FFG676"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Kintex 7 T 410 XC7K410T-FFG676"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC7K410T-FFG676_1_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_12")
				(number "U21")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_12")
				(number "U22")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_12")
				(number "V22")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_12")
				(number "U24")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_12")
				(number "U25")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_12")
				(number "V23")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_12")
				(number "V24")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_12")
				(number "U26")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_12")
				(number "V26")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_12")
				(number "W25")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_12")
				(number "W26")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_12")
				(number "V21")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_12")
				(number "W21")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_12")
				(number "AA25")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_12")
				(number "AB25")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_12")
				(number "W23")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_12")
				(number "W24")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_12")
				(number "AB26")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_12")
				(number "AC26")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_12")
				(number "Y25")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_12")
				(number "Y26")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_12")
				(number "AA23")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_12")
				(number "AB24")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_12")
				(number "Y23")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_12")
				(number "AA24")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_12")
				(number "Y22")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_12")
				(number "AA22")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_12")
				(number "AC23")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_12")
				(number "AC24")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_12")
				(number "W20")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_12")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_12")
				(number "AD23")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_12")
				(number "AD24")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_12")
				(number "AB22")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_12")
				(number "AC22")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_12")
				(number "AB21")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_12")
				(number "AC21")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_12")
				(number "AD21")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_12")
				(number "AE21")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_12")
				(number "AF24")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_12")
				(number "AF25")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_12")
				(number "AD26")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_12")
				(number "AE26")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_12")
				(number "AE23")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_12")
				(number "AF23")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_12")
				(number "AD25")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_12")
				(number "AE25")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_12")
				(number "AE22")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_12")
				(number "AF22")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_12")
				(number "Y20")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AA21")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AC25")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AD22")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AF26")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "U23")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "V20")
			)
			(pin power_in line
				(at -25.4 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "Y24")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "K24")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "N25")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "P22")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "R19")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "T16")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "T26")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_13")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_13")
				(number "K25")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_13")
				(number "K26")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_13")
				(number "R26")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_13")
				(number "P26")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_13")
				(number "M25")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_13")
				(number "L25")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_13")
				(number "P24")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_13")
				(number "N24")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_13")
				(number "N26")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_13")
				(number "M26")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_13")
				(number "R25")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_13")
				(number "P25")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_13")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_13")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_13")
				(number "M24")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_13")
				(number "L24")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_13")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_13")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_13")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_13")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_13")
				(number "P23")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_13")
				(number "N23")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_13")
				(number "N21")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_13")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_13")
				(number "R21")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_13")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_13")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_13")
				(number "R23")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_13")
				(number "T24")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_13")
				(number "T25")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_13")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_13")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_13")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_13")
				(number "T23")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_13")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_13")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_13")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_13")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_13")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_13")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_13")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_13")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_13")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_13")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_13")
				(number "U17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_13")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_13")
				(number "R18")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_13")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_13")
				(number "U16")
			)
		)
		(symbol "XC7K410T-FFG676_2_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_14")
				(number "K21")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_D00_MOSI_14")
				(number "B24")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_D01_DIN_14")
				(number "A25")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_D02_14")
				(number "B22")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_D03_14")
				(number "A22")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_PUDC_B_14")
				(number "B25")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_EMCCLK_14")
				(number "B26")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_D04_14")
				(number "A23")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_D05_14")
				(number "A24")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_D06_14")
				(number "D26")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_D07_14")
				(number "C26")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_FCS_B_14")
				(number "C23")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_D08_VREF_14")
				(number "C24")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_D09_14")
				(number "D21")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_D10_14")
				(number "C22")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_D11_14")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_D12_14")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_14")
				(number "E21")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_D13_14")
				(number "E22")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_D14_14")
				(number "C21")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_D15_14")
				(number "B21")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_14")
				(number "D23")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_14")
				(number "D24")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_14")
				(number "F22")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_14")
				(number "E23")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_14")
				(number "G22")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_14")
				(number "F23")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_14")
				(number "G24")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_14")
				(number "F24")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_RDWR_B_14")
				(number "E25")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_DOUT_CSO_B_14")
				(number "D25")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_CSI_B_14")
				(number "G25")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_A15_D31_14")
				(number "G26")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_A14_D30_14")
				(number "F25")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_A13_D29_14")
				(number "E26")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_A12_D28_14")
				(number "J26")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_A11_D27_14")
				(number "H26")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_A10_D26_14")
				(number "H21")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_A09_D25_VREF_14")
				(number "G21")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_A08_D24_14")
				(number "H23")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_A07_D23_14")
				(number "H24")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_14")
				(number "J21")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A06_D22_14")
				(number "H22")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_A05_D21_14")
				(number "J24")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_A04_D20_14")
				(number "J25")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_A03_D19_14")
				(number "L22")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_A02_D18_14")
				(number "K22")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_A01_D17_14")
				(number "K23")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_A00_D16_14")
				(number "J23")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_14")
				(number "L23")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "A21")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "C25")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "D22")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "F26")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "G23")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "L21")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "B18")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "E19")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "F16")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "H20")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "J17")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_15")
				(number "K15")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_AD0P_15")
				(number "C16")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_AD0N_15")
				(number "B16")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_AD8P_15")
				(number "A18")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_AD8N_15")
				(number "A19")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_AD1P_15")
				(number "B17")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_AD1N_15")
				(number "A17")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_AD9P_15")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_AD9N_15")
				(number "B19")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_AD2P_15")
				(number "C17")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_AD2N_15")
				(number "C18")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_15")
				(number "D15")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_15")
				(number "D16")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_AD10P_15")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_AD10N_15")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_AD3P_15")
				(number "G15")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_AD3N_15")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_AD11P_15")
				(number "J15")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_AD11N_15")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_AD4P_15")
				(number "E15")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_AD4N_15")
				(number "E16")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_AD12P_15")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_AD12N_15")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_AD5P_15")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_AD5N_15")
				(number "E17")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_15")
				(number "E18")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_15")
				(number "D18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_15")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_15")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_15")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_ADV_B_15")
				(number "D20")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_A28_15")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_A27_15")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_A26_15")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_A25_15")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_A24_15")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_A23_15")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_A22_15")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_A21_VREF_15")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_A20_15")
				(number "J18")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_A19_15")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_15")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A18_15")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_A17_15")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_A16_15")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_FOE_B_15")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_FWE_B_15")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_RS1_15")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_RS0_15")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_15")
				(number "M16")
			)
		)
		(symbol "XC7K410T-FFG676_3_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_16")
				(number "J8")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_16")
				(number "H9")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_16")
				(number "H8")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_16")
				(number "G10")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_16")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_16")
				(number "J13")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_16")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_16")
				(number "J11")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_16")
				(number "J10")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_16")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_16")
				(number "G14")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_16")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_16")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_16")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_16")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_16")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_16")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_16")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_16")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_16")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_16")
				(number "B9")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_16")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_16")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_16")
				(number "E10")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_16")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_16")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_16")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_16")
				(number "E11")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_16")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_16")
				(number "F14")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_16")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_16")
				(number "G12")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_16")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_16")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_16")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_16")
				(number "E13")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_16")
				(number "E12")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_16")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_16")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_16")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_16")
				(number "B11")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_16")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_16")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_16")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_16")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_16")
				(number "B15")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_16")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_16")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_16")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_16")
				(number "J14")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "A11")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "B8")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "C15")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "D12")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "E9")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "G13")
			)
			(pin power_in line
				(at -25.4 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "H10")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AB18")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AC15")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AE19")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AF16")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "W17")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "Y14")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_32")
				(number "V13")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_32")
				(number "AE17")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_32")
				(number "AF17")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_32")
				(number "AF14")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_32")
				(number "AF15")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_32")
				(number "AE18")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_32")
				(number "AF18")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_32")
				(number "AD15")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_32")
				(number "AE15")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_32")
				(number "AF19")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_32")
				(number "AF20")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_32")
				(number "AD16")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_32")
				(number "AE16")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_32")
				(number "AA14")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_32")
				(number "AA15")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_32")
				(number "AC14")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_32")
				(number "AD14")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_32")
				(number "Y15")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_32")
				(number "Y16")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_32")
				(number "AB14")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_32")
				(number "AB15")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_32")
				(number "AA17")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_32")
				(number "AA18")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_32")
				(number "AB16")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_32")
				(number "AC16")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_32")
				(number "AC18")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_32")
				(number "AD18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_32")
				(number "AB17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_32")
				(number "AC17")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_32")
				(number "AD20")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_32")
				(number "AE20")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_32")
				(number "AA19")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_32")
				(number "AA20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_32")
				(number "AC19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_32")
				(number "AD19")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_32")
				(number "AB19")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_32")
				(number "AB20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_32")
				(number "Y17")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_32")
				(number "Y18")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_32")
				(number "V16")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_32")
				(number "V17")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_32")
				(number "W18")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_32")
				(number "W19")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_32")
				(number "W15")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_32")
				(number "W16")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_32")
				(number "V18")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_32")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_32")
				(number "V14")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_32")
				(number "W14")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_32")
				(number "W13")
			)
		)
		(symbol "XC7K410T-FFG676_4_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_VRN_33")
				(number "U9")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_33")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_33")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_33")
				(number "V8")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_33")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_33")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_33")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_33")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_33")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_33")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_33")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_33")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_33")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_33")
				(number "AE7")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_33")
				(number "AF7")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_33")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_33")
				(number "AA7")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_33")
				(number "AC8")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_33")
				(number "AD8")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_33")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_33")
				(number "AC7")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_33")
				(number "AA9")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_33")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_33")
				(number "AC9")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_33")
				(number "AD9")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_33")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_33")
				(number "AC11")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_33")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_33")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_33")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_33")
				(number "AC12")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_33")
				(number "AA13")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_33")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_33")
				(number "AC13")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_33")
				(number "AD13")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_33")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_33")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_33")
				(number "AD11")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_33")
				(number "AE11")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_33")
				(number "AD10")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_33")
				(number "AE10")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_33")
				(number "AE12")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_33")
				(number "AF12")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_33")
				(number "AE8")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_33")
				(number "AF8")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_33")
				(number "AE13")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_33")
				(number "AF13")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_33")
				(number "AF10")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_33")
				(number "AF9")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_VRP_33")
				(number "V12")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AA11")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AB8")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AD12")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AE9")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "V10")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "W7")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AA1")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AC5")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AD2")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AF6")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "U3")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "Y4")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_34")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_34")
				(number "U6")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_34")
				(number "U5")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_34")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_34")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_34")
				(number "W6")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_34")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_34")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_34")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_34")
				(number "U7")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_34")
				(number "V6")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_34")
				(number "V4")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_34")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_34")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_34")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_34")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_34")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_34")
				(number "AB1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_34")
				(number "AC1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_34")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_34")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_34")
				(number "AB2")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_34")
				(number "AC2")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_34")
				(number "AA3")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_34")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_34")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_34")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_34")
				(number "AC4")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_34")
				(number "AC3")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_34")
				(number "AA5")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_34")
				(number "AB5")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_34")
				(number "AB6")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_34")
				(number "AC6")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_34")
				(number "Y6")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_34")
				(number "Y5")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_34")
				(number "AD6")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_34")
				(number "AD5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_34")
				(number "AD4")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_34")
				(number "AD3")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_34")
				(number "AD1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_34")
				(number "AE1")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_34")
				(number "AF5")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_34")
				(number "AF4")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_34")
				(number "AE3")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_34")
				(number "AE2")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_34")
				(number "AE6")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_34")
				(number "AE5")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_34")
				(number "AF3")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_34")
				(number "AF2")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_34")
				(number "T7")
			)
		)
		(symbol "XC7K410T-FFG676_5_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_115")
				(number "P2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_115")
				(number "P1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_115")
				(number "M2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_115")
				(number "M1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_115")
				(number "K2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_115")
				(number "K1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_115")
				(number "H2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_115")
				(number "H1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_115")
				(number "R4")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_115")
				(number "R3")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_115")
				(number "N4")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_115")
				(number "N3")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_115")
				(number "L4")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_115")
				(number "L3")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_115")
				(number "J4")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_115")
				(number "J3")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_115")
				(number "H6")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_115")
				(number "H5")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_115")
				(number "K6")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_115")
				(number "K5")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_116")
				(number "F2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_116")
				(number "F1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_116")
				(number "D2")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_116")
				(number "D1")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_116")
				(number "B2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_116")
				(number "B1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_116")
				(number "A4")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_116")
				(number "A3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_116")
				(number "G4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_116")
				(number "G3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_116")
				(number "E4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_116")
				(number "E3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_116")
				(number "C4")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_116")
				(number "C3")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_116")
				(number "B6")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_116")
				(number "B5")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_116")
				(number "D6")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_116")
				(number "D5")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_116")
				(number "F6")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_116")
				(number "F5")
			)
		)
		(symbol "XC7K410T-FFG676_6_1"
			(pin power_in line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "C6")
			)
			(pin power_in line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "E6")
			)
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "G6")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "J6")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "L6")
			)
			(pin power_in line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTVCCAUX")
				(number "N6")
			)
			(pin power_in line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "B3")
			)
			(pin power_in line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "C2")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "D3")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "G2")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "H3")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "L2")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "M3")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTTRCAL_115")
				(number "M5")
			)
			(pin power_in line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTRREF_115")
				(number "M6")
			)
		)
		(symbol "XC7K410T-FFG676_7_1"
			(pin power_in line
				(at 25.4 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "L7")
			)
			(pin power_in line
				(at 27.94 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "T6")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "TDI_0")
				(number "R6")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "TDO_0")
				(number "R7")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "TMS_0")
				(number "N8")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TCK_0")
				(number "L8")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "CCLK_0")
				(number "C8")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "M0_0")
				(number "T5")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "M1_0")
				(number "T2")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "M2_0")
				(number "P5")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "DONE_0")
				(number "J7")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "INIT_B_0")
				(number "G7")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "PROGRAM_B_0")
				(number "P6")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "CFGBVS_0")
				(number "P7")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "VP_0")
				(number "N12")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "VN_0")
				(number "P11")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 6.35)
				(name "VREFP_0")
				(number "P12")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "VREFN_0")
				(number "N11")
			)
			(pin bidirectional line
				(at 38.1 -35.56 180)
				(length 6.35)
				(name "DXP_0")
				(number "R12")
			)
			(pin bidirectional line
				(at 38.1 -38.1 180)
				(length 6.35)
				(name "DXN_0")
				(number "R11")
			)
		)
		(symbol "XC7K410T-FFG676_8_1"
			(pin power_in line
				(at -25.4 99.06 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 96.52 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M10")
			)
			(pin power_in line
				(at -25.4 93.98 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P10")
			)
			(pin power_in line
				(at -25.4 91.44 0)
				(length 6.35)
				(name "VCCAUX")
				(number "T10")
			)
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "T8")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "R9")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "P8")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "GNDADC_0")
				(number "M11")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCADC_0")
				(number "M12")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCBATT_0")
				(number "E8")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "N13")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "R13")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "T12")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "U13")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "GND")
				(number "A2")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "GND")
				(number "A5")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "GND")
				(number "A6")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "GND")
				(number "A7")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "GND")
				(number "A16")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "A26")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "B4")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "B23")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "C1")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "C5")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "C7")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "C10")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "C20")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "D7")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "D17")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "E1")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "E14")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E24")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "F3")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "F21")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G1")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "H25")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "J1")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "J5")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "J12")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "J22")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "K3")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "K4")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "K7")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "K11")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "K13")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "K19")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "L1")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "L10")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "L12")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "L14")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "L16")
			)
			(pin power_in line
				(at -25.4 -91.44 0)
				(length 6.35)
				(name "GND")
				(number "L26")
			)
			(pin power_in line
				(at -25.4 -93.98 0)
				(length 6.35)
				(name "GND")
				(number "M4")
			)
			(pin power_in line
				(at -25.4 -96.52 0)
				(length 6.35)
				(name "GND")
				(number "M7")
			)
			(pin power_in line
				(at -25.4 -99.06 0)
				(length 6.35)
				(name "GND")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 99.06 180)
				(length 6.35)
				(name "VCCINT")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 96.52 180)
				(length 6.35)
				(name "VCCINT")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 93.98 180)
				(length 6.35)
				(name "VCCINT")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 91.44 180)
				(length 6.35)
				(name "VCCINT")
				(number "K12")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "L13")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "L15")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "M8")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "R15")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "T14")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "U15")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "GND")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "GND")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "GND")
				(number "M23")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "GND")
				(number "N1")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "GND")
				(number "N5")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "N7")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "N20")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "P3")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "P4")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "P15")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "P17")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "R2")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "R8")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "R10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "R24")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "T1")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "T3")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "T4")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "T9")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "T11")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "T13")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "T15")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "T21")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "U8")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "U10")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U14")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "U18")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V5")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "V15")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "V25")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "W2")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "W12")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "W22")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "Y9")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "Y19")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AA6")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AA16")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AA26")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AB3")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AB13")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AB23")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "AC10")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "AC20")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "AD7")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "AD17")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "AE4")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "AE14")
			)
			(pin power_in line
				(at 25.4 -91.44 180)
				(length 6.35)
				(name "GND")
				(number "AE24")
			)
			(pin power_in line
				(at 25.4 -93.98 180)
				(length 6.35)
				(name "GND")
				(number "AF1")
			)
			(pin power_in line
				(at 25.4 -96.52 180)
				(length 6.35)
				(name "GND")
				(number "AF11")
			)
			(pin power_in line
				(at 25.4 -99.06 180)
				(length 6.35)
				(name "GND")
				(number "AF21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC7K410T-FFG900"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC7K410T-FFG900"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Kintex 7 T 410 XC7K410T-FFG900"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC7K410T-FFG900_1_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_12")
				(number "Y20")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_12")
				(number "Y23")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_12")
				(number "Y24")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_12")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_12")
				(number "AA21")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_12")
				(number "AB22")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_12")
				(number "AB23")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_12")
				(number "AA22")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_12")
				(number "AA23")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_12")
				(number "AC20")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_12")
				(number "AC21")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_12")
				(number "AA20")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_12")
				(number "AB20")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_12")
				(number "AB24")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_12")
				(number "AC25")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_12")
				(number "AC22")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_12")
				(number "AD22")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_12")
				(number "AC24")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_12")
				(number "AD24")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_12")
				(number "AD21")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_12")
				(number "AE21")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_12")
				(number "AE23")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_12")
				(number "AF23")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_12")
				(number "AD23")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_12")
				(number "AE24")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_12")
				(number "AF22")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_12")
				(number "AG23")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_12")
				(number "AG24")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_12")
				(number "AH24")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_12")
				(number "AJ24")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_12")
				(number "AK25")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_12")
				(number "AE25")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_12")
				(number "AF25")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_12")
				(number "AK23")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_12")
				(number "AK24")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_12")
				(number "AG25")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_12")
				(number "AH25")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_12")
				(number "AF20")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_12")
				(number "AF21")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_12")
				(number "AG22")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_12")
				(number "AH22")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_12")
				(number "AJ22")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_12")
				(number "AJ23")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_12")
				(number "AG20")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_12")
				(number "AH20")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_12")
				(number "AH21")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_12")
				(number "AJ21")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_12")
				(number "AK20")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_12")
				(number "AK21")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_12")
				(number "AE20")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AC23")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AD20")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AF24")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AG21")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AK22")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "Y22")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AA29")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AB26")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AD30")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AE27")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AH28")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AJ25")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_13")
				(number "Y25")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_13")
				(number "Y26")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_13")
				(number "AA26")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_13")
				(number "W27")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_13")
				(number "W28")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_13")
				(number "Y28")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_13")
				(number "AA28")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_13")
				(number "W29")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_13")
				(number "Y29")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_13")
				(number "AA27")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_13")
				(number "AB28")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_13")
				(number "AA25")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_13")
				(number "AB25")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_13")
				(number "AC29")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_13")
				(number "AC30")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_13")
				(number "Y30")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_13")
				(number "AA30")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_13")
				(number "AD29")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_13")
				(number "AE29")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_13")
				(number "AB29")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_13")
				(number "AB30")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_13")
				(number "AD27")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_13")
				(number "AD28")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_13")
				(number "AB27")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_13")
				(number "AC27")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_13")
				(number "AG29")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_13")
				(number "AH29")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_13")
				(number "AE28")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_13")
				(number "AF28")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_13")
				(number "AK29")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_13")
				(number "AK30")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_13")
				(number "AE30")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_13")
				(number "AF30")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_13")
				(number "AJ28")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_13")
				(number "AJ29")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_13")
				(number "AG30")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_13")
				(number "AH30")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_13")
				(number "AC26")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_13")
				(number "AD26")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_13")
				(number "AJ27")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_13")
				(number "AK28")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_13")
				(number "AG27")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_13")
				(number "AG28")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_13")
				(number "AH26")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_13")
				(number "AH27")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_13")
				(number "AF26")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_13")
				(number "AF27")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_13")
				(number "AJ26")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_13")
				(number "AK26")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_13")
				(number "AE26")
			)
		)
		(symbol "XC7K410T-FFG900_2_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_14")
				(number "R19")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_D00_MOSI_14")
				(number "P24")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_D01_DIN_14")
				(number "R25")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_D02_14")
				(number "R20")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_D03_14")
				(number "R21")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_PUDC_B_14")
				(number "R23")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_EMCCLK_14")
				(number "R24")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_D04_14")
				(number "T20")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_D05_14")
				(number "T21")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_D06_14")
				(number "T22")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_D07_14")
				(number "T23")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_FCS_B_14")
				(number "U19")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_D08_VREF_14")
				(number "U20")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_D09_14")
				(number "P29")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_D10_14")
				(number "R29")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_D11_14")
				(number "P27")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_D12_14")
				(number "P28")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_14")
				(number "R30")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_D13_14")
				(number "T30")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_D14_14")
				(number "P26")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_D15_14")
				(number "R26")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_14")
				(number "R28")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_14")
				(number "T28")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_14")
				(number "T26")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_14")
				(number "T27")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_14")
				(number "U27")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_14")
				(number "U28")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_14")
				(number "T25")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_14")
				(number "U25")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_RDWR_B_14")
				(number "U29")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_DOUT_CSO_B_14")
				(number "U30")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_CSI_B_14")
				(number "V26")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_A15_D31_14")
				(number "V27")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_A14_D30_14")
				(number "V29")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_A13_D29_14")
				(number "V30")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_A12_D28_14")
				(number "V25")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_A11_D27_14")
				(number "W26")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_A10_D26_14")
				(number "V19")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_A09_D25_VREF_14")
				(number "V20")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_A08_D24_14")
				(number "W23")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_A07_D23_14")
				(number "W24")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_14")
				(number "U22")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A06_D22_14")
				(number "U23")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_A05_D21_14")
				(number "V21")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_A04_D20_14")
				(number "V22")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_A03_D19_14")
				(number "U24")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_A02_D18_14")
				(number "V24")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_A01_D17_14")
				(number "W21")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_A00_D16_14")
				(number "W22")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_14")
				(number "W19")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "P30")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "R27")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "T24")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "U21")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "V28")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "W25")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "J25")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "K22")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "L29")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "M26")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "N23")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_15")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_AD0P_15")
				(number "J23")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_AD0N_15")
				(number "J24")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_AD8P_15")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_AD8N_15")
				(number "L23")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_AD1P_15")
				(number "K23")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_AD1N_15")
				(number "K24")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_AD9P_15")
				(number "L21")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_AD9N_15")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_AD2P_15")
				(number "J21")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_AD2N_15")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_15")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_15")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_AD10P_15")
				(number "J29")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_AD10N_15")
				(number "H29")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_AD3P_15")
				(number "J27")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_AD3N_15")
				(number "J28")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_AD11P_15")
				(number "L30")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_AD11N_15")
				(number "K30")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_AD4P_15")
				(number "K26")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_AD4N_15")
				(number "J26")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_AD12P_15")
				(number "L26")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_AD12N_15")
				(number "L27")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_AD5P_15")
				(number "L25")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_AD5N_15")
				(number "K25")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_15")
				(number "K28")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_15")
				(number "K29")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_15")
				(number "M28")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_15")
				(number "L28")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_15")
				(number "M29")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_ADV_B_15")
				(number "M30")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_A28_15")
				(number "N27")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_A27_15")
				(number "M27")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_A26_15")
				(number "N29")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_A25_15")
				(number "N30")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_A24_15")
				(number "N25")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_A23_15")
				(number "N26")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_A22_15")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_A21_VREF_15")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_A20_15")
				(number "N21")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_A19_15")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_15")
				(number "P23")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A18_15")
				(number "N24")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_A17_15")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_A16_15")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_FOE_B_15")
				(number "M24")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_FWE_B_15")
				(number "M25")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_RS1_15")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_RS0_15")
				(number "M23")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_15")
				(number "P19")
			)
		)
		(symbol "XC7K410T-FFG900_3_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_16")
				(number "F23")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_16")
				(number "B23")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_16")
				(number "A23")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_16")
				(number "E23")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_16")
				(number "D23")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_16")
				(number "F25")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_16")
				(number "E25")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_16")
				(number "E24")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_16")
				(number "D24")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_16")
				(number "F26")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_16")
				(number "E26")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_16")
				(number "G23")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_16")
				(number "G24")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_16")
				(number "B27")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_16")
				(number "A27")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_16")
				(number "C24")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_16")
				(number "B24")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_16")
				(number "B28")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_16")
				(number "A28")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_16")
				(number "A25")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_16")
				(number "A26")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_16")
				(number "D26")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_16")
				(number "C26")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_16")
				(number "C25")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_16")
				(number "B25")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_16")
				(number "D27")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_16")
				(number "C27")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_16")
				(number "E28")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_16")
				(number "D28")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_16")
				(number "C29")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_16")
				(number "B29")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_16")
				(number "D29")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_16")
				(number "C30")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_16")
				(number "B30")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_16")
				(number "A30")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_16")
				(number "E29")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_16")
				(number "E30")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_16")
				(number "H24")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_16")
				(number "H25")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_16")
				(number "G28")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_16")
				(number "F28")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_16")
				(number "G27")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_16")
				(number "F27")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_16")
				(number "G29")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_16")
				(number "F30")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_16")
				(number "H26")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_16")
				(number "H27")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_16")
				(number "H30")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_16")
				(number "G30")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_16")
				(number "G25")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "A29")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "B26")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "C23")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "D30")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "E27")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "F24")
			)
			(pin power_in line
				(at -25.4 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "H28")
			)
			(pin power_in line
				(at 25.4 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "A19")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "B16")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "D20")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "E17")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "G21")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "H18")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_17")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_17")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_17")
				(number "J18")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_17")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_17")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_17")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_17")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_17")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_17")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_17")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_17")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_17")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_17")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_17")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_17")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_17")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_17")
				(number "C21")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_17")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_17")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_17")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_17")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_17")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_17")
				(number "E21")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_17")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_17")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_17")
				(number "D17")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_17")
				(number "D18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_17")
				(number "E19")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_17")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_17")
				(number "D16")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_17")
				(number "C16")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_17")
				(number "G18")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_17")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_17")
				(number "C17")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_17")
				(number "B17")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_17")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_17")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_17")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_17")
				(number "B20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_17")
				(number "A16")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_17")
				(number "A17")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_17")
				(number "A20")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_17")
				(number "A21")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_17")
				(number "B18")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_17")
				(number "A18")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_17")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_17")
				(number "A22")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_17")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_17")
				(number "B19")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_17")
				(number "E18")
			)
		)
		(symbol "XC7K410T-FFG900_4_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_18")
				(number "G12")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_18")
				(number "L16")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_18")
				(number "K16")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_18")
				(number "L15")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_18")
				(number "K15")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_18")
				(number "L12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_18")
				(number "L13")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_18")
				(number "K13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_18")
				(number "J13")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_18")
				(number "K14")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_18")
				(number "J14")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_18")
				(number "L11")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_18")
				(number "K11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_18")
				(number "H15")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_18")
				(number "G15")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_18")
				(number "J11")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_18")
				(number "J12")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_18")
				(number "J16")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_18")
				(number "H16")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_18")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_18")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_18")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_18")
				(number "G14")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_18")
				(number "G13")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_18")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_18")
				(number "D12")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_18")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_18")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_18")
				(number "E13")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_18")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_18")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_18")
				(number "F11")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_18")
				(number "E11")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_18")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_18")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_18")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_18")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_18")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_18")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_18")
				(number "E14")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_18")
				(number "E15")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_18")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_18")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_18")
				(number "B13")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_18")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_18")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_18")
				(number "B15")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_18")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_18")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_18")
				(number "F16")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "C13")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "D10")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "F14")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "G11")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "J15")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "K12")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AA19")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AB16")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AE17")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AF14")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AH18")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AJ15")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_32")
				(number "Y14")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_32")
				(number "AK16")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_32")
				(number "AK15")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_32")
				(number "AG15")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_32")
				(number "AH15")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_32")
				(number "AH16")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_32")
				(number "AJ16")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_32")
				(number "AF15")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_32")
				(number "AG14")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_32")
				(number "AH17")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_32")
				(number "AJ17")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_32")
				(number "AE16")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_32")
				(number "AF16")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_32")
				(number "AJ19")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_32")
				(number "AK19")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_32")
				(number "AG19")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_32")
				(number "AH19")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_32")
				(number "AJ18")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_32")
				(number "AK18")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_32")
				(number "AD19")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_32")
				(number "AE19")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_32")
				(number "AF18")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_32")
				(number "AG18")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_32")
				(number "AF17")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_32")
				(number "AG17")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_32")
				(number "AD18")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_32")
				(number "AE18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_32")
				(number "AD17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_32")
				(number "AD16")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_32")
				(number "Y19")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_32")
				(number "Y18")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_32")
				(number "AA18")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_32")
				(number "AB18")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_32")
				(number "AB19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_32")
				(number "AC19")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_32")
				(number "AB17")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_32")
				(number "AC17")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_32")
				(number "AE15")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_32")
				(number "AE14")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_32")
				(number "AA15")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_32")
				(number "AB15")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_32")
				(number "AC16")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_32")
				(number "AC15")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_32")
				(number "AC14")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_32")
				(number "AD14")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_32")
				(number "AA17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_32")
				(number "AA16")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_32")
				(number "Y16")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_32")
				(number "Y15")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_32")
				(number "AB14")
			)
		)
		(symbol "XC7K410T-FFG900_5_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_VRN_33")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_33")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_33")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_33")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_33")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_33")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_33")
				(number "AC9")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_33")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_33")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_33")
				(number "AA11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_33")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_33")
				(number "AA13")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_33")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_33")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_33")
				(number "AC10")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_33")
				(number "AD8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_33")
				(number "AE8")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_33")
				(number "AC12")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_33")
				(number "AC11")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_33")
				(number "AD9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_33")
				(number "AE9")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_33")
				(number "AE11")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_33")
				(number "AF11")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_33")
				(number "AD12")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_33")
				(number "AD11")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_33")
				(number "AG10")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_33")
				(number "AH10")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_33")
				(number "AE10")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_33")
				(number "AF10")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_33")
				(number "AJ9")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_33")
				(number "AK9")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_33")
				(number "AG9")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_33")
				(number "AH9")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_33")
				(number "AK11")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_33")
				(number "AK10")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_33")
				(number "AH11")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_33")
				(number "AJ11")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_33")
				(number "AE13")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_33")
				(number "AF13")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_33")
				(number "AK14")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_33")
				(number "AK13")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_33")
				(number "AH14")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_33")
				(number "AJ14")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_33")
				(number "AJ13")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_33")
				(number "AJ12")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_33")
				(number "AF12")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_33")
				(number "AG12")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_33")
				(number "AG13")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_33")
				(number "AH12")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_VRP_33")
				(number "AD13")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AA9")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AC13")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AD10")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AG11")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AK12")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "Y12")
			)
			(pin power_in line
				(at 25.4 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AC3")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AE7")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AF4")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AG1")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AH8")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AJ5")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AK2")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_34")
				(number "AC6")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_34")
				(number "AD4")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_34")
				(number "AD3")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_34")
				(number "AC2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_34")
				(number "AC1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_34")
				(number "AD2")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_34")
				(number "AD1")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_34")
				(number "AC5")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_34")
				(number "AC4")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_34")
				(number "AD6")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_34")
				(number "AE6")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_34")
				(number "AC7")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_34")
				(number "AD7")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_34")
				(number "AF3")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_34")
				(number "AF2")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_34")
				(number "AE1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_34")
				(number "AF1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_34")
				(number "AG4")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_34")
				(number "AG3")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_34")
				(number "AE4")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_34")
				(number "AE3")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_34")
				(number "AE5")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_34")
				(number "AF5")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_34")
				(number "AF6")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_34")
				(number "AG5")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_34")
				(number "AH4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_34")
				(number "AJ4")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_34")
				(number "AH6")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_34")
				(number "AH5")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_34")
				(number "AG2")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_34")
				(number "AH1")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_34")
				(number "AH2")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_34")
				(number "AJ2")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_34")
				(number "AJ1")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_34")
				(number "AK1")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_34")
				(number "AJ3")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_34")
				(number "AK3")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_34")
				(number "AF8")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_34")
				(number "AG8")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_34")
				(number "AF7")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_34")
				(number "AG7")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_34")
				(number "AH7")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_34")
				(number "AJ7")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_34")
				(number "AJ6")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_34")
				(number "AK6")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_34")
				(number "AJ8")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_34")
				(number "AK8")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_34")
				(number "AK5")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_34")
				(number "AK4")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_34")
				(number "AB7")
			)
		)
		(symbol "XC7K410T-FFG900_6_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_115")
				(number "Y2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_115")
				(number "Y1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_115")
				(number "V2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_115")
				(number "V1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_115")
				(number "U4")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_115")
				(number "U3")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_115")
				(number "T2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_115")
				(number "T1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_115")
				(number "AA4")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_115")
				(number "AA3")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_115")
				(number "Y6")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_115")
				(number "Y5")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_115")
				(number "W4")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_115")
				(number "W3")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_115")
				(number "V6")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_115")
				(number "V5")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_115")
				(number "R8")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_115")
				(number "R7")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_115")
				(number "U8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_115")
				(number "U7")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_116")
				(number "P2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_116")
				(number "P1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_116")
				(number "N4")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_116")
				(number "N3")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_116")
				(number "M2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_116")
				(number "M1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_116")
				(number "L4")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_116")
				(number "L3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_116")
				(number "T6")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_116")
				(number "T5")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_116")
				(number "R4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_116")
				(number "R3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_116")
				(number "P6")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_116")
				(number "P5")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_116")
				(number "M6")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_116")
				(number "M5")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_116")
				(number "L8")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_116")
				(number "L7")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_116")
				(number "N8")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_116")
				(number "N7")
			)
		)
		(symbol "XC7K410T-FFG900_7_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_117")
				(number "K2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_117")
				(number "K1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_117")
				(number "J4")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_117")
				(number "J3")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_117")
				(number "H2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_117")
				(number "H1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_117")
				(number "F2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_117")
				(number "F1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_117")
				(number "K6")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_117")
				(number "K5")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_117")
				(number "H6")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_117")
				(number "H5")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_117")
				(number "G4")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_117")
				(number "G3")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_117")
				(number "F6")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_117")
				(number "F5")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_117")
				(number "G8")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_117")
				(number "G7")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_117")
				(number "J8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_117")
				(number "J7")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_118")
				(number "D2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_118")
				(number "D1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_118")
				(number "C4")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_118")
				(number "C3")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_118")
				(number "B2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_118")
				(number "B1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_118")
				(number "A4")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_118")
				(number "A3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_118")
				(number "E4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_118")
				(number "E3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_118")
				(number "D6")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_118")
				(number "D5")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_118")
				(number "B6")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_118")
				(number "B5")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_118")
				(number "A8")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_118")
				(number "A7")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_118")
				(number "C8")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_118")
				(number "C7")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_118")
				(number "E8")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_118")
				(number "E7")
			)
		)
		(symbol "XC7K410T-FFG900_8_1"
			(pin power_in line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "B7")
			)
			(pin power_in line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "D7")
			)
			(pin power_in line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "F7")
			)
			(pin power_in line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "H7")
			)
			(pin power_in line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "K7")
			)
			(pin power_in line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "M7")
			)
			(pin power_in line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "P7")
			)
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTVCCAUX")
				(number "T7")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTVCCAUX")
				(number "V7")
			)
			(pin power_in line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "B3")
			)
			(pin power_in line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "C5")
			)
			(pin power_in line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "D3")
			)
			(pin power_in line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "E5")
			)
			(pin power_in line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "F3")
			)
			(pin power_in line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "G5")
			)
			(pin power_in line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "H3")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "J5")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "K3")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "L5")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "M3")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "N5")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "P3")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "R5")
			)
			(pin power_in line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "T3")
			)
			(pin power_in line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "U5")
			)
			(pin power_in line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "V3")
			)
			(pin power_in line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "W5")
			)
			(pin power_in line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTAVTTRCAL_115")
				(number "W7")
			)
			(pin power_in line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTRREF_115")
				(number "W8")
			)
		)
		(symbol "XC7K410T-FFG900_9_1"
			(pin power_in line
				(at 25.4 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "AB6")
			)
			(pin power_in line
				(at 27.94 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "T9")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "TDI_0")
				(number "H10")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "TDO_0")
				(number "G10")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "TMS_0")
				(number "F10")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TCK_0")
				(number "E10")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "CCLK_0")
				(number "B10")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "M0_0")
				(number "AB5")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "M1_0")
				(number "AB2")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "M2_0")
				(number "AB1")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "DONE_0")
				(number "M10")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "INIT_B_0")
				(number "A10")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "PROGRAM_B_0")
				(number "K10")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "CFGBVS_0")
				(number "L10")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "VP_0")
				(number "R15")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "VN_0")
				(number "T14")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 6.35)
				(name "VREFP_0")
				(number "T15")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "VREFN_0")
				(number "R14")
			)
			(pin bidirectional line
				(at 38.1 -35.56 180)
				(length 6.35)
				(name "DXP_0")
				(number "U15")
			)
			(pin bidirectional line
				(at 38.1 -38.1 180)
				(length 6.35)
				(name "DXN_0")
				(number "U14")
			)
		)
		(symbol "XC7K410T-FFG900_10_1"
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P13")
			)
			(pin power_in line
				(at -25.4 86.36 0)
				(length 6.35)
				(name "VCCAUX")
				(number "T13")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V13")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V15")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "VCCAUX")
				(number "W14")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "W12")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "V11")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "W10")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "GNDADC_0")
				(number "P14")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCADC_0")
				(number "P15")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCBATT_0")
				(number "C10")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "N16")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "R16")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "U16")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "W16")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "A2")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "A5")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "A6")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "A14")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "A24")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "B4")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "B8")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "B21")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "C1")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "C2")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "C9")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "C18")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C28")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "D8")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "D9")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "D15")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "D25")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "E1")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "E6")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "E9")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "E12")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "E22")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "F8")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "F9")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "F19")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "F29")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "G1")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "G2")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "G6")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "G9")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "G16")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "G26")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "H13")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "H23")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "J1")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "J6")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "M17")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "N18")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "P17")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "R10")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "R12")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "T11")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "T17")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "U10")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "U18")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "V17")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "W18")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "J20")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "J30")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "K4")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "K17")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "K27")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "L1")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "L2")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "L6")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "L24")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "M4")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "M8")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "M16")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "M18")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "M21")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "N1")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "N6")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "N28")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "P4")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "P8")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "P16")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "P18")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "P25")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "R2")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "R6")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "R9")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "R11")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "R13")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "R17")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "R22")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "T4")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "T8")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "T10")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "T12")
			)
		)
		(symbol "XC7K410T-FFG900_11_1"
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "GND")
				(number "T18")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "GND")
				(number "T19")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "GND")
				(number "T29")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "U1")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "U6")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "U9")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "U13")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "U17")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "U26")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "V8")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "V9")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "V12")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "V16")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "V18")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "V23")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "W1")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "W2")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "W6")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "W9")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "W11")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "W13")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "W15")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "W17")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "W20")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "W30")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "Y3")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "Y4")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "Y7")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "Y8")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "Y9")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "Y17")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "GND")
				(number "Y27")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "GND")
				(number "AA1")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "GND")
				(number "AA2")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "AA6")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "AA7")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "AA14")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "AA24")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "AB3")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "AB4")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "AB11")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "AB21")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "AC8")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "AC18")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "AC28")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "AD5")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "AD15")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "AD25")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "AE2")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "AE12")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "AE22")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "AF9")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "AF19")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "AF29")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "AG6")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "AG16")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "AG26")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "AH3")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "AH13")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "AH23")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "AJ10")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "AJ20")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "AJ30")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "AK7")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "AK17")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "AK27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC7K420T-FFG1156"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC7K420T-FFG1156"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Kintex 7 T 420 XC7K420T-FFG1156"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC7K420T-FFG1156_1_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_11")
				(number "AG18")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_11")
				(number "AK23")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_11")
				(number "AL23")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_11")
				(number "AM22")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_11")
				(number "AN22")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_11")
				(number "AP21")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_11")
				(number "AP22")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_11")
				(number "AN20")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_11")
				(number "AP20")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_11")
				(number "AN19")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_11")
				(number "AP19")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_11")
				(number "AL21")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_11")
				(number "AM21")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_11")
				(number "AN17")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_11")
				(number "AN18")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_11")
				(number "AP16")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_11")
				(number "AP17")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_11")
				(number "AM17")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_11")
				(number "AM18")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_11")
				(number "AL16")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_11")
				(number "AM16")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_11")
				(number "AL20")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_11")
				(number "AM20")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_11")
				(number "AL18")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_11")
				(number "AL19")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_11")
				(number "AK18")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_11")
				(number "AK19")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_11")
				(number "AH19")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_11")
				(number "AJ19")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_11")
				(number "AK16")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_11")
				(number "AK17")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_11")
				(number "AJ16")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_11")
				(number "AJ17")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_11")
				(number "AH17")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_11")
				(number "AH18")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_11")
				(number "AG16")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_11")
				(number "AG17")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_11")
				(number "AJ22")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_11")
				(number "AK22")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_11")
				(number "AJ21")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_11")
				(number "AK21")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_11")
				(number "AH20")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_11")
				(number "AJ20")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_11")
				(number "AG20")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_11")
				(number "AG21")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_11")
				(number "AG22")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_11")
				(number "AH22")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_11")
				(number "AG23")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_11")
				(number "AH23")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_11")
				(number "AG15")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AH21")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AJ18")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AK15")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AL22")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AM19")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AN16")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AF27")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AG24")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AJ28")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AK25")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AN26")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AP23")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_12")
				(number "AD25")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_12")
				(number "AM23")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_12")
				(number "AN23")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_12")
				(number "AN24")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_12")
				(number "AP24")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_12")
				(number "AN25")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_12")
				(number "AP25")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_12")
				(number "AP26")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_12")
				(number "AP27")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_12")
				(number "AN27")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_12")
				(number "AN28")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_12")
				(number "AM27")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_12")
				(number "AM28")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_12")
				(number "AM25")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_12")
				(number "AM26")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_12")
				(number "AJ29")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_12")
				(number "AK29")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_12")
				(number "AK24")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_12")
				(number "AL24")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_12")
				(number "AK28")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_12")
				(number "AL28")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_12")
				(number "AL25")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_12")
				(number "AL26")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_12")
				(number "AK26")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_12")
				(number "AK27")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_12")
				(number "AJ26")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_12")
				(number "AJ27")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_12")
				(number "AH27")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_12")
				(number "AH28")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_12")
				(number "AH25")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_12")
				(number "AJ25")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_12")
				(number "AH24")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_12")
				(number "AJ24")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_12")
				(number "AG26")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_12")
				(number "AG27")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_12")
				(number "AG28")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_12")
				(number "AH29")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_12")
				(number "AD29")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_12")
				(number "AE29")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_12")
				(number "AF28")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_12")
				(number "AF29")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_12")
				(number "AE27")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_12")
				(number "AE28")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_12")
				(number "AE26")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_12")
				(number "AF26")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_12")
				(number "AE24")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_12")
				(number "AF24")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_12")
				(number "AF25")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_12")
				(number "AG25")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_12")
				(number "AD24")
			)
		)
		(symbol "XC7K420T-FFG1156_2_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_13")
				(number "AC30")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_13")
				(number "AC32")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_13")
				(number "AC33")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_13")
				(number "AC34")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_13")
				(number "AD34")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_13")
				(number "AE34")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_13")
				(number "AF34")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_13")
				(number "AE33")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_13")
				(number "AF33")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_13")
				(number "AE31")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_13")
				(number "AE32")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_13")
				(number "AD31")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_13")
				(number "AD32")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_13")
				(number "AH34")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_13")
				(number "AJ34")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_13")
				(number "AF30")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_13")
				(number "AG30")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_13")
				(number "AG33")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_13")
				(number "AH33")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_13")
				(number "AH30")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_13")
				(number "AJ30")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_13")
				(number "AG32")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_13")
				(number "AH32")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_13")
				(number "AF31")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_13")
				(number "AG31")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_13")
				(number "AJ31")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_13")
				(number "AK31")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_13")
				(number "AJ32")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_13")
				(number "AK32")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_13")
				(number "AK33")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_13")
				(number "AL33")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_13")
				(number "AK34")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_13")
				(number "AL34")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_13")
				(number "AL30")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_13")
				(number "AL31")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_13")
				(number "AL29")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_13")
				(number "AM30")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_13")
				(number "AM31")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_13")
				(number "AM32")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_13")
				(number "AM33")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_13")
				(number "AN34")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_13")
				(number "AN32")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_13")
				(number "AP33")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_13")
				(number "AP31")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_13")
				(number "AP32")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_13")
				(number "AP29")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_13")
				(number "AP30")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_13")
				(number "AN29")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_13")
				(number "AN30")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_13")
				(number "AD30")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AD33")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AE30")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AG34")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AH31")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AL32")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AM29")
			)
			(pin power_in line
				(at -25.4 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AN33")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "AA32")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "AB29")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "AC26")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "V31")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "W28")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "Y25")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_14")
				(number "AA24")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_D00_MOSI_14")
				(number "AA33")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_D01_DIN_14")
				(number "AA34")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_D02_14")
				(number "Y33")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_D03_14")
				(number "Y34")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_PUDC_B_14")
				(number "V34")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_EMCCLK_14")
				(number "W34")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_D04_14")
				(number "V32")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_D05_14")
				(number "V33")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_D06_14")
				(number "W31")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_D07_14")
				(number "W32")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_FCS_B_14")
				(number "V30")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_D08_VREF_14")
				(number "W30")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_D09_14")
				(number "V25")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_D10_14")
				(number "W25")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_D11_14")
				(number "V29")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_D12_14")
				(number "W29")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_14")
				(number "V27")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_D13_14")
				(number "V28")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_D14_14")
				(number "W24")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_D15_14")
				(number "Y24")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_14")
				(number "W26")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_14")
				(number "W27")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_14")
				(number "Y26")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_14")
				(number "Y27")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_14")
				(number "AA28")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_14")
				(number "AA29")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_14")
				(number "Y28")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_14")
				(number "Y29")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_RDWR_B_14")
				(number "AB30")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_DOUT_CSO_B_14")
				(number "AB31")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_CSI_B_14")
				(number "Y31")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_A15_D31_14")
				(number "Y32")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_A14_D30_14")
				(number "AB32")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_A13_D29_14")
				(number "AB33")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_A12_D28_14")
				(number "AA30")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_A11_D27_14")
				(number "AA31")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_A10_D26_14")
				(number "AA26")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_A09_D25_VREF_14")
				(number "AB26")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_A08_D24_14")
				(number "AB27")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_A07_D23_14")
				(number "AB28")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_14")
				(number "AA25")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A06_D22_14")
				(number "AB25")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_A05_D21_14")
				(number "AC27")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_A04_D20_14")
				(number "AD27")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_A03_D19_14")
				(number "AC28")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_A02_D18_14")
				(number "AC29")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_A01_D17_14")
				(number "AC25")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_A00_D16_14")
				(number "AD26")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_14")
				(number "AC24")
			)
		)
		(symbol "XC7K420T-FFG1156_3_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_15")
				(number "T24")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_AD0P_15")
				(number "N28")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_AD0N_15")
				(number "M28")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_AD8P_15")
				(number "P29")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_AD8N_15")
				(number "N29")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_AD1P_15")
				(number "P27")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_AD1N_15")
				(number "N27")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_AD9P_15")
				(number "N24")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_AD9N_15")
				(number "N25")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_AD2P_15")
				(number "P25")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_AD2N_15")
				(number "P26")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_15")
				(number "R24")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_15")
				(number "P24")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_AD10P_15")
				(number "R26")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_AD10N_15")
				(number "R27")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_AD3P_15")
				(number "T25")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_AD3N_15")
				(number "T26")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_AD11P_15")
				(number "U25")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_AD11N_15")
				(number "U26")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_AD4P_15")
				(number "U27")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_AD4N_15")
				(number "U28")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_AD12P_15")
				(number "T28")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_AD12N_15")
				(number "T29")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_AD5P_15")
				(number "R28")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_AD5N_15")
				(number "R29")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_15")
				(number "R31")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_15")
				(number "P31")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_15")
				(number "P30")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_15")
				(number "N30")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_15")
				(number "M30")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_ADV_B_15")
				(number "M31")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_A28_15")
				(number "N32")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_A27_15")
				(number "M32")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_A26_15")
				(number "N33")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_A25_15")
				(number "M33")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_A24_15")
				(number "P34")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_A23_15")
				(number "N34")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_A22_15")
				(number "U30")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_A21_VREF_15")
				(number "U31")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_A20_15")
				(number "T30")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_A19_15")
				(number "T31")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_15")
				(number "U32")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A18_15")
				(number "U33")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_A17_15")
				(number "R32")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_A16_15")
				(number "P32")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_FOE_B_15")
				(number "T33")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_FWE_B_15")
				(number "T34")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_RS1_15")
				(number "R33")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_RS0_15")
				(number "R34")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_15")
				(number "V24")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "N26")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "P33")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "R30")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "T27")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "U24")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "U34")
			)
			(pin power_in line
				(at 25.4 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "A32")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "B29")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "D33")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "E30")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "G34")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "H31")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "L32")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_16")
				(number "J29")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_16")
				(number "A29")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_16")
				(number "A30")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_16")
				(number "B30")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_16")
				(number "A31")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_16")
				(number "B31")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_16")
				(number "B32")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_16")
				(number "B33")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_16")
				(number "A33")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_16")
				(number "C32")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_16")
				(number "C33")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_16")
				(number "C29")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_16")
				(number "C30")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_16")
				(number "D29")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_16")
				(number "D30")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_16")
				(number "F34")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_16")
				(number "E34")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_16")
				(number "D34")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_16")
				(number "C34")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_16")
				(number "F33")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_16")
				(number "E33")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_16")
				(number "E31")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_16")
				(number "D31")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_16")
				(number "E32")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_16")
				(number "D32")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_16")
				(number "G30")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_16")
				(number "F30")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_16")
				(number "G31")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_16")
				(number "F31")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_16")
				(number "H29")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_16")
				(number "H30")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_16")
				(number "F29")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_16")
				(number "E29")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_16")
				(number "H32")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_16")
				(number "G32")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_16")
				(number "H33")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_16")
				(number "G33")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_16")
				(number "J30")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_16")
				(number "J31")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_16")
				(number "L31")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_16")
				(number "K31")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_16")
				(number "K32")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_16")
				(number "J32")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_16")
				(number "L33")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_16")
				(number "K33")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_16")
				(number "L34")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_16")
				(number "K34")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_16")
				(number "J34")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_16")
				(number "H34")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_16")
				(number "L30")
			)
		)
		(symbol "XC7K420T-FFG1156_4_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_17")
				(number "H23")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_17")
				(number "C24")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_17")
				(number "C25")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_17")
				(number "A24")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_17")
				(number "A25")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_17")
				(number "B25")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_17")
				(number "A26")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_17")
				(number "B26")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_17")
				(number "B27")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_17")
				(number "B28")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_17")
				(number "A28")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_17")
				(number "C27")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_17")
				(number "C28")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_17")
				(number "F24")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_17")
				(number "E24")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_17")
				(number "D26")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_17")
				(number "D27")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_17")
				(number "D24")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_17")
				(number "D25")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_17")
				(number "F28")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_17")
				(number "E28")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_17")
				(number "F25")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_17")
				(number "F26")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_17")
				(number "E26")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_17")
				(number "E27")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_17")
				(number "H27")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_17")
				(number "G27")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_17")
				(number "G25")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_17")
				(number "G26")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_17")
				(number "J24")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_17")
				(number "J25")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_17")
				(number "H24")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_17")
				(number "H25")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_17")
				(number "H28")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_17")
				(number "G28")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_17")
				(number "J26")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_17")
				(number "J27")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_17")
				(number "L25")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_17")
				(number "L26")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_17")
				(number "L24")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_17")
				(number "K24")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_17")
				(number "K28")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_17")
				(number "K29")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_17")
				(number "K26")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_17")
				(number "K27")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_17")
				(number "M26")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_17")
				(number "M27")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_17")
				(number "L28")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_17")
				(number "L29")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_17")
				(number "M25")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "C26")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "F27")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "G24")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "J28")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "K25")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "M29")
			)
			(pin power_in line
				(at 25.4 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "A22")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "B19")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "C16")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "D23")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "E20")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "F17")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_18")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_18")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_18")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_18")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_18")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_18")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_18")
				(number "G18")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_18")
				(number "F16")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_18")
				(number "E16")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_18")
				(number "E17")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_18")
				(number "E18")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_18")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_18")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_18")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_18")
				(number "G21")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_18")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_18")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_18")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_18")
				(number "G23")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_18")
				(number "F23")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_18")
				(number "E23")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_18")
				(number "D20")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_18")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_18")
				(number "E21")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_18")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_18")
				(number "E19")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_18")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_18")
				(number "C18")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_18")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_18")
				(number "D16")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_18")
				(number "D17")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_18")
				(number "C17")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_18")
				(number "B17")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_18")
				(number "B16")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_18")
				(number "A16")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_18")
				(number "B18")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_18")
				(number "A18")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_18")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_18")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_18")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_18")
				(number "B20")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_18")
				(number "A19")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_18")
				(number "A20")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_18")
				(number "B21")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_18")
				(number "A21")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_18")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_18")
				(number "A23")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_18")
				(number "C23")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_18")
				(number "B23")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_18")
				(number "H22")
			)
		)
		(symbol "XC7K420T-FFG1156_5_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_111")
				(number "AN12")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_111")
				(number "AN11")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_111")
				(number "AP10")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_111")
				(number "AP9")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_111")
				(number "AN8")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_111")
				(number "AN7")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_111")
				(number "AL8")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_111")
				(number "AL7")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_111")
				(number "AM10")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_111")
				(number "AM9")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_111")
				(number "AL12")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_111")
				(number "AL11")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_111")
				(number "AJ12")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_111")
				(number "AJ11")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_111")
				(number "AK10")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_111")
				(number "AK9")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_111")
				(number "AH10")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_111")
				(number "AH9")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_111")
				(number "AJ8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_111")
				(number "AJ7")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_112")
				(number "AP6")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_112")
				(number "AP5")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_112")
				(number "AN4")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_112")
				(number "AN3")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_112")
				(number "AP2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_112")
				(number "AP1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_112")
				(number "AM2")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_112")
				(number "AM1")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_112")
				(number "AM6")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_112")
				(number "AM5")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_112")
				(number "AL4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_112")
				(number "AL3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_112")
				(number "AK6")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_112")
				(number "AK5")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_112")
				(number "AJ4")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_112")
				(number "AJ3")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_112")
				(number "AG8")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_112")
				(number "AG7")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_112")
				(number "AH6")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_112")
				(number "AH5")
			)
		)
		(symbol "XC7K420T-FFG1156_6_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_113")
				(number "AK2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_113")
				(number "AK1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_113")
				(number "AH2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_113")
				(number "AH1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_113")
				(number "AF2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_113")
				(number "AF1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_113")
				(number "AD2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_113")
				(number "AD1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_113")
				(number "AG4")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_113")
				(number "AG3")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_113")
				(number "AF6")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_113")
				(number "AF5")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_113")
				(number "AE4")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_113")
				(number "AE3")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_113")
				(number "AC4")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_113")
				(number "AC3")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_113")
				(number "AC8")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_113")
				(number "AC7")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_113")
				(number "AD6")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_113")
				(number "AD5")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_114")
				(number "AB2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_114")
				(number "AB1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_114")
				(number "Y2")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_114")
				(number "Y1")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_114")
				(number "W4")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_114")
				(number "W3")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_114")
				(number "V2")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_114")
				(number "V1")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_114")
				(number "AB6")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_114")
				(number "AB5")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_114")
				(number "AA4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_114")
				(number "AA3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_114")
				(number "Y6")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_114")
				(number "Y5")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_114")
				(number "V6")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_114")
				(number "V5")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_114")
				(number "W8")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_114")
				(number "W7")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_114")
				(number "AA8")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_114")
				(number "AA7")
			)
		)
		(symbol "XC7K420T-FFG1156_7_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_115")
				(number "U4")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_115")
				(number "U3")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_115")
				(number "T2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_115")
				(number "T1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_115")
				(number "P2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_115")
				(number "P1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_115")
				(number "N4")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_115")
				(number "N3")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_115")
				(number "T6")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_115")
				(number "T5")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_115")
				(number "R4")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_115")
				(number "R3")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_115")
				(number "P6")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_115")
				(number "P5")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_115")
				(number "M6")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_115")
				(number "M5")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_115")
				(number "R8")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_115")
				(number "R7")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_115")
				(number "U8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_115")
				(number "U7")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_116")
				(number "M2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_116")
				(number "M1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_116")
				(number "K2")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_116")
				(number "K1")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_116")
				(number "H2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_116")
				(number "H1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_116")
				(number "F2")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_116")
				(number "F1")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_116")
				(number "L4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_116")
				(number "L3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_116")
				(number "K6")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_116")
				(number "K5")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_116")
				(number "J4")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_116")
				(number "J3")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_116")
				(number "H6")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_116")
				(number "H5")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_116")
				(number "J8")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_116")
				(number "J7")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_116")
				(number "L8")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_116")
				(number "L7")
			)
		)
		(symbol "XC7K420T-FFG1156_8_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_117")
				(number "D2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_117")
				(number "D1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_117")
				(number "B2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_117")
				(number "B1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_117")
				(number "A4")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_117")
				(number "A3")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_117")
				(number "B6")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_117")
				(number "B5")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_117")
				(number "G4")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_117")
				(number "G3")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_117")
				(number "E4")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_117")
				(number "E3")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_117")
				(number "D6")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_117")
				(number "D5")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_117")
				(number "C4")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_117")
				(number "C3")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_117")
				(number "F6")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_117")
				(number "F5")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_117")
				(number "G8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_117")
				(number "G7")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_118")
				(number "C8")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_118")
				(number "C7")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_118")
				(number "A8")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_118")
				(number "A7")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_118")
				(number "B10")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_118")
				(number "B9")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_118")
				(number "A12")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_118")
				(number "A11")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_118")
				(number "F10")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_118")
				(number "F9")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_118")
				(number "E12")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_118")
				(number "E11")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_118")
				(number "D10")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_118")
				(number "D9")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_118")
				(number "C12")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_118")
				(number "C11")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_118")
				(number "E8")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_118")
				(number "E7")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_118")
				(number "H10")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_118")
				(number "H9")
			)
		)
		(symbol "XC7K420T-FFG1156_9_1"
			(pin power_in line
				(at -38.1 35.56 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AA6")
			)
			(pin power_in line
				(at -38.1 33.02 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AC6")
			)
			(pin power_in line
				(at -38.1 30.48 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AE6")
			)
			(pin power_in line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AG6")
			)
			(pin power_in line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AJ6")
			)
			(pin power_in line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AJ9")
			)
			(pin power_in line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AK12")
			)
			(pin power_in line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AM12")
			)
			(pin power_in line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AP12")
			)
			(pin power_in line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "W6")
			)
			(pin power_in line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTVCCAUX_G10")
				(number "AD9")
			)
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTVCCAUX_G10")
				(number "AE8")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "B12")
			)
			(pin power_in line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "D12")
			)
			(pin power_in line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "F12")
			)
			(pin power_in line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "G6")
			)
			(pin power_in line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "G9")
			)
			(pin power_in line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "J6")
			)
			(pin power_in line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "L6")
			)
			(pin power_in line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "N6")
			)
			(pin power_in line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "R6")
			)
			(pin power_in line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "U6")
			)
			(pin power_in line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTVCCAUX_G11")
				(number "M9")
			)
			(pin power_in line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTVCCAUX_G11")
				(number "N8")
			)
			(pin power_in line
				(at 38.1 35.56 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AC2")
			)
			(pin power_in line
				(at 38.1 33.02 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AD3")
			)
			(pin power_in line
				(at 38.1 30.48 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AG2")
			)
			(pin power_in line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AH3")
			)
			(pin power_in line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AL2")
			)
			(pin power_in line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AL6")
			)
			(pin power_in line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AL9")
			)
			(pin power_in line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AM3")
			)
			(pin power_in line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AN6")
			)
			(pin power_in line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AN9")
			)
			(pin power_in line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "W2")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "Y3")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "C2")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "C6")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "C9")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "D3")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "E6")
			)
			(pin power_in line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "E9")
			)
			(pin power_in line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "G2")
			)
			(pin power_in line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "H3")
			)
			(pin power_in line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "L2")
			)
			(pin power_in line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "M3")
			)
			(pin power_in line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "R2")
			)
			(pin power_in line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "T3")
			)
			(pin power_in line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "MGTAVTTRCAL_115")
				(number "T10")
			)
			(pin power_in line
				(at 38.1 -33.02 180)
				(length 6.35)
				(name "MGTRREF_115")
				(number "T9")
			)
		)
		(symbol "XC7K420T-FFG1156_10_1"
			(pin power_in line
				(at 25.4 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G14")
			)
			(pin power_in line
				(at 27.94 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H13")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "TDI_0")
				(number "G15")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "TDO_0")
				(number "F14")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "TMS_0")
				(number "H15")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TCK_0")
				(number "F15")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "CCLK_0")
				(number "D15")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "M0_0")
				(number "AJ15")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "M1_0")
				(number "AH15")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "M2_0")
				(number "AJ14")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "DONE_0")
				(number "AH14")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "INIT_B_0")
				(number "AG14")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "PROGRAM_B_0")
				(number "AM15")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "CFGBVS_0")
				(number "AL15")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "VP_0")
				(number "U17")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "VN_0")
				(number "V16")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 6.35)
				(name "VREFP_0")
				(number "V17")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "VREFN_0")
				(number "U16")
			)
			(pin bidirectional line
				(at 38.1 -35.56 180)
				(length 6.35)
				(name "DXP_0")
				(number "W17")
			)
			(pin bidirectional line
				(at 38.1 -38.1 180)
				(length 6.35)
				(name "DXN_0")
				(number "W16")
			)
		)
		(symbol "XC7K420T-FFG1156_11_1"
			(pin power_in line
				(at -25.4 175.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "Y15")
			)
			(pin power_in line
				(at -25.4 172.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "Y17")
			)
			(pin power_in line
				(at -25.4 170.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA16")
			)
			(pin power_in line
				(at -25.4 167.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA18")
			)
			(pin power_in line
				(at -25.4 165.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AB15")
			)
			(pin power_in line
				(at -25.4 162.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AB17")
			)
			(pin power_in line
				(at -25.4 160.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AC16")
			)
			(pin power_in line
				(at -25.4 157.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AC18")
			)
			(pin power_in line
				(at -25.4 154.94 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AD15")
			)
			(pin power_in line
				(at -25.4 152.4 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AD17")
			)
			(pin power_in line
				(at -25.4 149.86 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AE16")
			)
			(pin power_in line
				(at -25.4 147.32 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AE18")
			)
			(pin power_in line
				(at -25.4 144.78 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AF15")
			)
			(pin power_in line
				(at -25.4 142.24 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AF17")
			)
			(pin power_in line
				(at -25.4 137.16 0)
				(length 6.35)
				(name "GNDADC_0")
				(number "T16")
			)
			(pin power_in line
				(at -25.4 134.62 0)
				(length 6.35)
				(name "VCCADC_0")
				(number "T17")
			)
			(pin power_in line
				(at -25.4 132.08 0)
				(length 6.35)
				(name "VCCBATT_0")
				(number "C15")
			)
			(pin power_in line
				(at -25.4 129.54 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "AA20")
			)
			(pin power_in line
				(at -25.4 127 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "AB19")
			)
			(pin power_in line
				(at -25.4 124.46 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "AC20")
			)
			(pin power_in line
				(at -25.4 121.92 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "AD19")
			)
			(pin power_in line
				(at -25.4 119.38 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "AE20")
			)
			(pin power_in line
				(at -25.4 116.84 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "AF19")
			)
			(pin power_in line
				(at -25.4 114.3 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "R20")
			)
			(pin power_in line
				(at -25.4 111.76 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "T19")
			)
			(pin power_in line
				(at -25.4 109.22 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "U20")
			)
			(pin power_in line
				(at -25.4 106.68 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "V19")
			)
			(pin power_in line
				(at -25.4 104.14 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "W20")
			)
			(pin power_in line
				(at -25.4 101.6 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "Y19")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "A2")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "A5")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "A6")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "A10")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "A13")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "A14")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "A15")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "A17")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "A27")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "A34")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "B3")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "B4")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "B8")
			)
			(pin power_in line
				(at -25.4 -91.44 0)
				(length 6.35)
				(name "GND")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 -93.98 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 -96.52 0)
				(length 6.35)
				(name "GND")
				(number "B14")
			)
			(pin power_in line
				(at -25.4 -99.06 0)
				(length 6.35)
				(name "GND")
				(number "B15")
			)
			(pin power_in line
				(at -25.4 -101.6 0)
				(length 6.35)
				(name "GND")
				(number "B24")
			)
			(pin power_in line
				(at -25.4 -104.14 0)
				(length 6.35)
				(name "GND")
				(number "B34")
			)
			(pin power_in line
				(at -25.4 -106.68 0)
				(length 6.35)
				(name "GND")
				(number "C1")
			)
			(pin power_in line
				(at -25.4 -109.22 0)
				(length 6.35)
				(name "GND")
				(number "C5")
			)
			(pin power_in line
				(at -25.4 -111.76 0)
				(length 6.35)
				(name "GND")
				(number "C10")
			)
			(pin power_in line
				(at -25.4 -114.3 0)
				(length 6.35)
				(name "GND")
				(number "C13")
			)
			(pin power_in line
				(at -25.4 -116.84 0)
				(length 6.35)
				(name "GND")
				(number "C14")
			)
			(pin power_in line
				(at -25.4 -119.38 0)
				(length 6.35)
				(name "GND")
				(number "C21")
			)
			(pin power_in line
				(at -25.4 -121.92 0)
				(length 6.35)
				(name "GND")
				(number "C31")
			)
			(pin power_in line
				(at -25.4 -124.46 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -127 0)
				(length 6.35)
				(name "GND")
				(number "D7")
			)
			(pin power_in line
				(at -25.4 -129.54 0)
				(length 6.35)
				(name "GND")
				(number "D8")
			)
			(pin power_in line
				(at -25.4 -132.08 0)
				(length 6.35)
				(name "GND")
				(number "D11")
			)
			(pin power_in line
				(at -25.4 -134.62 0)
				(length 6.35)
				(name "GND")
				(number "D13")
			)
			(pin power_in line
				(at -25.4 -137.16 0)
				(length 6.35)
				(name "GND")
				(number "D14")
			)
			(pin power_in line
				(at -25.4 -139.7 0)
				(length 6.35)
				(name "GND")
				(number "D18")
			)
			(pin power_in line
				(at -25.4 -142.24 0)
				(length 6.35)
				(name "GND")
				(number "D28")
			)
			(pin power_in line
				(at -25.4 -144.78 0)
				(length 6.35)
				(name "GND")
				(number "E1")
			)
			(pin power_in line
				(at -25.4 -147.32 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -149.86 0)
				(length 6.35)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 -152.4 0)
				(length 6.35)
				(name "GND")
				(number "E10")
			)
			(pin power_in line
				(at -25.4 -154.94 0)
				(length 6.35)
				(name "GND")
				(number "E13")
			)
			(pin power_in line
				(at -25.4 -157.48 0)
				(length 6.35)
				(name "GND")
				(number "E14")
			)
			(pin power_in line
				(at -25.4 -160.02 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -162.56 0)
				(length 6.35)
				(name "GND")
				(number "E25")
			)
			(pin power_in line
				(at -25.4 -165.1 0)
				(length 6.35)
				(name "GND")
				(number "F3")
			)
			(pin power_in line
				(at -25.4 -167.64 0)
				(length 6.35)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at -25.4 -170.18 0)
				(length 6.35)
				(name "GND")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 -172.72 0)
				(length 6.35)
				(name "GND")
				(number "F8")
			)
			(pin power_in line
				(at -25.4 -175.26 0)
				(length 6.35)
				(name "GND")
				(number "F11")
			)
			(pin power_in line
				(at 25.4 175.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 172.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "J14")
			)
			(pin power_in line
				(at 25.4 170.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "J16")
			)
			(pin power_in line
				(at 25.4 167.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "J18")
			)
			(pin power_in line
				(at 25.4 165.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "J20")
			)
			(pin power_in line
				(at 25.4 162.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "J22")
			)
			(pin power_in line
				(at 25.4 160.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 157.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 154.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "K15")
			)
			(pin power_in line
				(at 25.4 152.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "K17")
			)
			(pin power_in line
				(at 25.4 149.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "K19")
			)
			(pin power_in line
				(at 25.4 147.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "K21")
			)
			(pin power_in line
				(at 25.4 144.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "K23")
			)
			(pin power_in line
				(at 25.4 142.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 139.7 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 137.16 180)
				(length 6.35)
				(name "VCCINT")
				(number "L16")
			)
			(pin power_in line
				(at 25.4 134.62 180)
				(length 6.35)
				(name "VCCINT")
				(number "L18")
			)
			(pin power_in line
				(at 25.4 132.08 180)
				(length 6.35)
				(name "VCCINT")
				(number "L20")
			)
			(pin power_in line
				(at 25.4 129.54 180)
				(length 6.35)
				(name "VCCINT")
				(number "L22")
			)
			(pin power_in line
				(at 25.4 127 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 124.46 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 121.92 180)
				(length 6.35)
				(name "VCCINT")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 119.38 180)
				(length 6.35)
				(name "VCCINT")
				(number "M17")
			)
			(pin power_in line
				(at 25.4 116.84 180)
				(length 6.35)
				(name "VCCINT")
				(number "M19")
			)
			(pin power_in line
				(at 25.4 114.3 180)
				(length 6.35)
				(name "VCCINT")
				(number "M21")
			)
			(pin power_in line
				(at 25.4 111.76 180)
				(length 6.35)
				(name "VCCINT")
				(number "M23")
			)
			(pin power_in line
				(at 25.4 109.22 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 106.68 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 104.14 180)
				(length 6.35)
				(name "VCCINT")
				(number "N16")
			)
			(pin power_in line
				(at 25.4 101.6 180)
				(length 6.35)
				(name "VCCINT")
				(number "N18")
			)
			(pin power_in line
				(at 25.4 99.06 180)
				(length 6.35)
				(name "VCCINT")
				(number "N20")
			)
			(pin power_in line
				(at 25.4 96.52 180)
				(length 6.35)
				(name "VCCINT")
				(number "N22")
			)
			(pin power_in line
				(at 25.4 93.98 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 91.44 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "P15")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "P17")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "P19")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "P21")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "P23")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "R12")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "R16")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "R22")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "T13")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "T15")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "T21")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "T23")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "U14")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "U18")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "U22")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "V11")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "V13")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "V15")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "V21")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "V23")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "W10")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "W12")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "W14")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "W18")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "W22")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y11")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y13")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y21")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y23")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "VCCINT")
				(number "AA10")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "VCCINT")
				(number "AA12")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "VCCINT")
				(number "AA14")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "VCCINT")
				(number "AA22")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "VCCINT")
				(number "AB11")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "VCCINT")
				(number "AB13")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "VCCINT")
				(number "AB21")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "VCCINT")
				(number "AB23")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "VCCINT")
				(number "AC12")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "AC14")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "AC22")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "AD11")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "AD13")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "AD21")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "AD23")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "AE12")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "AE14")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "AE22")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "AF11")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "AF13")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "AF21")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "AF23")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "F13")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "F22")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "F32")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "G1")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "G10")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "G11")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "G12")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "G13")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "G19")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "G29")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "H11")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "H12")
			)
			(pin power_in line
				(at 25.4 -91.44 180)
				(length 6.35)
				(name "GND")
				(number "H14")
			)
			(pin power_in line
				(at 25.4 -93.98 180)
				(length 6.35)
				(name "GND")
				(number "H16")
			)
			(pin power_in line
				(at 25.4 -96.52 180)
				(length 6.35)
				(name "GND")
				(number "H26")
			)
			(pin power_in line
				(at 25.4 -99.06 180)
				(length 6.35)
				(name "GND")
				(number "J1")
			)
			(pin power_in line
				(at 25.4 -101.6 180)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at 25.4 -104.14 180)
				(length 6.35)
				(name "GND")
				(number "J5")
			)
			(pin power_in line
				(at 25.4 -106.68 180)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 -109.22 180)
				(length 6.35)
				(name "GND")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 -111.76 180)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at 25.4 -114.3 180)
				(length 6.35)
				(name "GND")
				(number "J13")
			)
			(pin power_in line
				(at 25.4 -116.84 180)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at 25.4 -119.38 180)
				(length 6.35)
				(name "GND")
				(number "J17")
			)
			(pin power_in line
				(at 25.4 -121.92 180)
				(length 6.35)
				(name "GND")
				(number "J19")
			)
			(pin power_in line
				(at 25.4 -124.46 180)
				(length 6.35)
				(name "GND")
				(number "J21")
			)
			(pin power_in line
				(at 25.4 -127 180)
				(length 6.35)
				(name "GND")
				(number "J23")
			)
			(pin power_in line
				(at 25.4 -129.54 180)
				(length 6.35)
				(name "GND")
				(number "J33")
			)
			(pin power_in line
				(at 25.4 -132.08 180)
				(length 6.35)
				(name "GND")
				(number "K3")
			)
			(pin power_in line
				(at 25.4 -134.62 180)
				(length 6.35)
				(name "GND")
				(number "K4")
			)
			(pin power_in line
				(at 25.4 -137.16 180)
				(length 6.35)
				(name "GND")
				(number "K7")
			)
			(pin power_in line
				(at 25.4 -139.7 180)
				(length 6.35)
				(name "GND")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 -142.24 180)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 -144.78 180)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 -147.32 180)
				(length 6.35)
				(name "GND")
				(number "K12")
			)
			(pin power_in line
				(at 25.4 -149.86 180)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 -152.4 180)
				(length 6.35)
				(name "GND")
				(number "K16")
			)
			(pin power_in line
				(at 25.4 -154.94 180)
				(length 6.35)
				(name "GND")
				(number "K18")
			)
			(pin power_in line
				(at 25.4 -157.48 180)
				(length 6.35)
				(name "GND")
				(number "K20")
			)
			(pin power_in line
				(at 25.4 -160.02 180)
				(length 6.35)
				(name "GND")
				(number "K22")
			)
			(pin power_in line
				(at 25.4 -162.56 180)
				(length 6.35)
				(name "GND")
				(number "K30")
			)
			(pin power_in line
				(at 25.4 -165.1 180)
				(length 6.35)
				(name "GND")
				(number "L1")
			)
			(pin power_in line
				(at 25.4 -167.64 180)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at 25.4 -170.18 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 -172.72 180)
				(length 6.35)
				(name "GND")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 -175.26 180)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
		)
		(symbol "XC7K420T-FFG1156_12_1"
			(pin power_in line
				(at -25.4 162.56 0)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at -25.4 160.02 0)
				(length 6.35)
				(name "GND")
				(number "L15")
			)
			(pin power_in line
				(at -25.4 157.48 0)
				(length 6.35)
				(name "GND")
				(number "L17")
			)
			(pin power_in line
				(at -25.4 154.94 0)
				(length 6.35)
				(name "GND")
				(number "L19")
			)
			(pin power_in line
				(at -25.4 152.4 0)
				(length 6.35)
				(name "GND")
				(number "L21")
			)
			(pin power_in line
				(at -25.4 149.86 0)
				(length 6.35)
				(name "GND")
				(number "L23")
			)
			(pin power_in line
				(at -25.4 147.32 0)
				(length 6.35)
				(name "GND")
				(number "L27")
			)
			(pin power_in line
				(at -25.4 144.78 0)
				(length 6.35)
				(name "GND")
				(number "M4")
			)
			(pin power_in line
				(at -25.4 142.24 0)
				(length 6.35)
				(name "GND")
				(number "M7")
			)
			(pin power_in line
				(at -25.4 139.7 0)
				(length 6.35)
				(name "GND")
				(number "M8")
			)
			(pin power_in line
				(at -25.4 137.16 0)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at -25.4 134.62 0)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at -25.4 132.08 0)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at -25.4 129.54 0)
				(length 6.35)
				(name "GND")
				(number "M16")
			)
			(pin power_in line
				(at -25.4 127 0)
				(length 6.35)
				(name "GND")
				(number "M18")
			)
			(pin power_in line
				(at -25.4 124.46 0)
				(length 6.35)
				(name "GND")
				(number "M20")
			)
			(pin power_in line
				(at -25.4 121.92 0)
				(length 6.35)
				(name "GND")
				(number "M22")
			)
			(pin power_in line
				(at -25.4 119.38 0)
				(length 6.35)
				(name "GND")
				(number "M24")
			)
			(pin power_in line
				(at -25.4 116.84 0)
				(length 6.35)
				(name "GND")
				(number "M34")
			)
			(pin power_in line
				(at -25.4 114.3 0)
				(length 6.35)
				(name "GND")
				(number "N1")
			)
			(pin power_in line
				(at -25.4 111.76 0)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at -25.4 109.22 0)
				(length 6.35)
				(name "GND")
				(number "N5")
			)
			(pin power_in line
				(at -25.4 106.68 0)
				(length 6.35)
				(name "GND")
				(number "N7")
			)
			(pin power_in line
				(at -25.4 104.14 0)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at -25.4 101.6 0)
				(length 6.35)
				(name "GND")
				(number "N10")
			)
			(pin power_in line
				(at -25.4 99.06 0)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at -25.4 96.52 0)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at -25.4 93.98 0)
				(length 6.35)
				(name "GND")
				(number "N15")
			)
			(pin power_in line
				(at -25.4 91.44 0)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "GND")
				(number "N19")
			)
			(pin power_in line
				(at -25.4 86.36 0)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "GND")
				(number "N23")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "GND")
				(number "N31")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "GND")
				(number "P3")
			)
			(pin power_in line
				(at -25.4 76.2 0)
				(length 6.35)
				(name "GND")
				(number "P4")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "GND")
				(number "P7")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "GND")
				(number "P8")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "GND")
				(number "P9")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "GND")
				(number "P16")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "GND")
				(number "P18")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "GND")
				(number "P20")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "GND")
				(number "P22")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "GND")
				(number "P28")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "GND")
				(number "R9")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "GND")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "R11")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "R13")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "R15")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "R17")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "R19")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "R21")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "R23")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "R25")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "T4")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "T7")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "T8")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "T11")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "T12")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "T14")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "T18")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "T20")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "T22")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "T32")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "U1")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "U5")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "U9")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "U10")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "U13")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "U15")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "U19")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "U23")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "U29")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "V3")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "V7")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "V8")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "V9")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "V12")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "V18")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "V20")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "V22")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "V26")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "W1")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "W5")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "W9")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "W11")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "W13")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "W15")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "W21")
			)
			(pin power_in line
				(at -25.4 -91.44 0)
				(length 6.35)
				(name "GND")
				(number "W23")
			)
			(pin power_in line
				(at -25.4 -93.98 0)
				(length 6.35)
				(name "GND")
				(number "W33")
			)
			(pin power_in line
				(at -25.4 -96.52 0)
				(length 6.35)
				(name "GND")
				(number "Y4")
			)
			(pin power_in line
				(at -25.4 -99.06 0)
				(length 6.35)
				(name "GND")
				(number "Y7")
			)
			(pin power_in line
				(at -25.4 -101.6 0)
				(length 6.35)
				(name "GND")
				(number "Y8")
			)
			(pin power_in line
				(at -25.4 -104.14 0)
				(length 6.35)
				(name "GND")
				(number "Y9")
			)
			(pin power_in line
				(at -25.4 -106.68 0)
				(length 6.35)
				(name "GND")
				(number "Y10")
			)
			(pin power_in line
				(at -25.4 -109.22 0)
				(length 6.35)
				(name "GND")
				(number "Y12")
			)
			(pin power_in line
				(at -25.4 -111.76 0)
				(length 6.35)
				(name "GND")
				(number "Y14")
			)
			(pin power_in line
				(at -25.4 -114.3 0)
				(length 6.35)
				(name "GND")
				(number "Y16")
			)
			(pin power_in line
				(at -25.4 -116.84 0)
				(length 6.35)
				(name "GND")
				(number "Y18")
			)
			(pin power_in line
				(at -25.4 -119.38 0)
				(length 6.35)
				(name "GND")
				(number "Y20")
			)
			(pin power_in line
				(at -25.4 -121.92 0)
				(length 6.35)
				(name "GND")
				(number "Y22")
			)
			(pin power_in line
				(at -25.4 -124.46 0)
				(length 6.35)
				(name "GND")
				(number "Y30")
			)
			(pin power_in line
				(at -25.4 -127 0)
				(length 6.35)
				(name "GND")
				(number "AA1")
			)
			(pin power_in line
				(at -25.4 -129.54 0)
				(length 6.35)
				(name "GND")
				(number "AA2")
			)
			(pin power_in line
				(at -25.4 -132.08 0)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at -25.4 -134.62 0)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at -25.4 -137.16 0)
				(length 6.35)
				(name "GND")
				(number "AA11")
			)
			(pin power_in line
				(at -25.4 -139.7 0)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at -25.4 -142.24 0)
				(length 6.35)
				(name "GND")
				(number "AA15")
			)
			(pin power_in line
				(at -25.4 -144.78 0)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at -25.4 -147.32 0)
				(length 6.35)
				(name "GND")
				(number "AA19")
			)
			(pin power_in line
				(at -25.4 -149.86 0)
				(length 6.35)
				(name "GND")
				(number "AA21")
			)
			(pin power_in line
				(at -25.4 -152.4 0)
				(length 6.35)
				(name "GND")
				(number "AA23")
			)
			(pin power_in line
				(at -25.4 -154.94 0)
				(length 6.35)
				(name "GND")
				(number "AA27")
			)
			(pin power_in line
				(at -25.4 -157.48 0)
				(length 6.35)
				(name "GND")
				(number "AB3")
			)
			(pin power_in line
				(at -25.4 -160.02 0)
				(length 6.35)
				(name "GND")
				(number "AB4")
			)
			(pin power_in line
				(at -25.4 -162.56 0)
				(length 6.35)
				(name "GND")
				(number "AB7")
			)
			(pin power_in line
				(at 25.4 162.56 180)
				(length 6.35)
				(name "GND")
				(number "AB8")
			)
			(pin power_in line
				(at 25.4 160.02 180)
				(length 6.35)
				(name "GND")
				(number "AB9")
			)
			(pin power_in line
				(at 25.4 157.48 180)
				(length 6.35)
				(name "GND")
				(number "AB10")
			)
			(pin power_in line
				(at 25.4 154.94 180)
				(length 6.35)
				(name "GND")
				(number "AB12")
			)
			(pin power_in line
				(at 25.4 152.4 180)
				(length 6.35)
				(name "GND")
				(number "AB14")
			)
			(pin power_in line
				(at 25.4 149.86 180)
				(length 6.35)
				(name "GND")
				(number "AB16")
			)
			(pin power_in line
				(at 25.4 147.32 180)
				(length 6.35)
				(name "GND")
				(number "AB18")
			)
			(pin power_in line
				(at 25.4 144.78 180)
				(length 6.35)
				(name "GND")
				(number "AB20")
			)
			(pin power_in line
				(at 25.4 142.24 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
			(pin power_in line
				(at 25.4 139.7 180)
				(length 6.35)
				(name "GND")
				(number "AB24")
			)
			(pin power_in line
				(at 25.4 137.16 180)
				(length 6.35)
				(name "GND")
				(number "AB34")
			)
			(pin power_in line
				(at 25.4 134.62 180)
				(length 6.35)
				(name "GND")
				(number "AC1")
			)
			(pin power_in line
				(at 25.4 132.08 180)
				(length 6.35)
				(name "GND")
				(number "AC5")
			)
			(pin power_in line
				(at 25.4 129.54 180)
				(length 6.35)
				(name "GND")
				(number "AC9")
			)
			(pin power_in line
				(at 25.4 127 180)
				(length 6.35)
				(name "GND")
				(number "AC10")
			)
			(pin power_in line
				(at 25.4 124.46 180)
				(length 6.35)
				(name "GND")
				(number "AC11")
			)
			(pin power_in line
				(at 25.4 121.92 180)
				(length 6.35)
				(name "GND")
				(number "AC13")
			)
			(pin power_in line
				(at 25.4 119.38 180)
				(length 6.35)
				(name "GND")
				(number "AC15")
			)
			(pin power_in line
				(at 25.4 116.84 180)
				(length 6.35)
				(name "GND")
				(number "AC17")
			)
			(pin power_in line
				(at 25.4 114.3 180)
				(length 6.35)
				(name "GND")
				(number "AC19")
			)
			(pin power_in line
				(at 25.4 111.76 180)
				(length 6.35)
				(name "GND")
				(number "AC21")
			)
			(pin power_in line
				(at 25.4 109.22 180)
				(length 6.35)
				(name "GND")
				(number "AC23")
			)
			(pin power_in line
				(at 25.4 106.68 180)
				(length 6.35)
				(name "GND")
				(number "AC31")
			)
			(pin power_in line
				(at 25.4 104.14 180)
				(length 6.35)
				(name "GND")
				(number "AD4")
			)
			(pin power_in line
				(at 25.4 101.6 180)
				(length 6.35)
				(name "GND")
				(number "AD7")
			)
			(pin power_in line
				(at 25.4 99.06 180)
				(length 6.35)
				(name "GND")
				(number "AD8")
			)
			(pin power_in line
				(at 25.4 96.52 180)
				(length 6.35)
				(name "GND")
				(number "AD10")
			)
			(pin power_in line
				(at 25.4 93.98 180)
				(length 6.35)
				(name "GND")
				(number "AD12")
			)
			(pin power_in line
				(at 25.4 91.44 180)
				(length 6.35)
				(name "GND")
				(number "AD14")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "GND")
				(number "AD16")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "GND")
				(number "AD18")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "GND")
				(number "AD20")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "GND")
				(number "AD22")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "GND")
				(number "AD28")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "GND")
				(number "AE1")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "GND")
				(number "AE2")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "GND")
				(number "AE5")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "GND")
				(number "AE7")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "GND")
				(number "AE9")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "GND")
				(number "AE10")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "GND")
				(number "AE11")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "GND")
				(number "AE13")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "GND")
				(number "AE15")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "GND")
				(number "AE17")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "GND")
				(number "AE19")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "GND")
				(number "AE21")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "GND")
				(number "AE23")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "GND")
				(number "AE25")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "GND")
				(number "AF3")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "GND")
				(number "AF4")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "AF7")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "AF8")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "AF9")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "AF10")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "AF12")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "AF14")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "AF16")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "AF18")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "AF20")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "AF22")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "AF32")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "AG1")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "AG5")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "AG9")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "AG10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "AG11")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "AG12")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "AG13")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "AG19")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "AG29")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "AH4")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "AH7")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "AH8")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "AH11")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "AH12")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "AH13")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "AH16")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "AH26")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "AJ1")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "AJ2")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "AJ5")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "AJ10")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "AJ13")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "AJ23")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AJ33")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AK3")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AK4")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AK7")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AK8")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AK11")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AK13")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AK14")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AK20")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AK30")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "AL1")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "AL5")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "AL10")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "AL13")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "AL14")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "AL17")
			)
			(pin power_in line
				(at 25.4 -91.44 180)
				(length 6.35)
				(name "GND")
				(number "AL27")
			)
			(pin power_in line
				(at 25.4 -93.98 180)
				(length 6.35)
				(name "GND")
				(number "AM4")
			)
			(pin power_in line
				(at 25.4 -96.52 180)
				(length 6.35)
				(name "GND")
				(number "AM7")
			)
			(pin power_in line
				(at 25.4 -99.06 180)
				(length 6.35)
				(name "GND")
				(number "AM8")
			)
			(pin power_in line
				(at 25.4 -101.6 180)
				(length 6.35)
				(name "GND")
				(number "AM11")
			)
			(pin power_in line
				(at 25.4 -104.14 180)
				(length 6.35)
				(name "GND")
				(number "AM13")
			)
			(pin power_in line
				(at 25.4 -106.68 180)
				(length 6.35)
				(name "GND")
				(number "AM14")
			)
			(pin power_in line
				(at 25.4 -109.22 180)
				(length 6.35)
				(name "GND")
				(number "AM24")
			)
			(pin power_in line
				(at 25.4 -111.76 180)
				(length 6.35)
				(name "GND")
				(number "AM34")
			)
			(pin power_in line
				(at 25.4 -114.3 180)
				(length 6.35)
				(name "GND")
				(number "AN1")
			)
			(pin power_in line
				(at 25.4 -116.84 180)
				(length 6.35)
				(name "GND")
				(number "AN2")
			)
			(pin power_in line
				(at 25.4 -119.38 180)
				(length 6.35)
				(name "GND")
				(number "AN5")
			)
			(pin power_in line
				(at 25.4 -121.92 180)
				(length 6.35)
				(name "GND")
				(number "AN10")
			)
			(pin power_in line
				(at 25.4 -124.46 180)
				(length 6.35)
				(name "GND")
				(number "AN13")
			)
			(pin power_in line
				(at 25.4 -127 180)
				(length 6.35)
				(name "GND")
				(number "AN14")
			)
			(pin power_in line
				(at 25.4 -129.54 180)
				(length 6.35)
				(name "GND")
				(number "AN15")
			)
			(pin power_in line
				(at 25.4 -132.08 180)
				(length 6.35)
				(name "GND")
				(number "AN21")
			)
			(pin power_in line
				(at 25.4 -134.62 180)
				(length 6.35)
				(name "GND")
				(number "AN31")
			)
			(pin power_in line
				(at 25.4 -137.16 180)
				(length 6.35)
				(name "GND")
				(number "AP3")
			)
			(pin power_in line
				(at 25.4 -139.7 180)
				(length 6.35)
				(name "GND")
				(number "AP4")
			)
			(pin power_in line
				(at 25.4 -142.24 180)
				(length 6.35)
				(name "GND")
				(number "AP7")
			)
			(pin power_in line
				(at 25.4 -144.78 180)
				(length 6.35)
				(name "GND")
				(number "AP8")
			)
			(pin power_in line
				(at 25.4 -147.32 180)
				(length 6.35)
				(name "GND")
				(number "AP11")
			)
			(pin power_in line
				(at 25.4 -149.86 180)
				(length 6.35)
				(name "GND")
				(number "AP13")
			)
			(pin power_in line
				(at 25.4 -152.4 180)
				(length 6.35)
				(name "GND")
				(number "AP14")
			)
			(pin power_in line
				(at 25.4 -154.94 180)
				(length 6.35)
				(name "GND")
				(number "AP15")
			)
			(pin power_in line
				(at 25.4 -157.48 180)
				(length 6.35)
				(name "GND")
				(number "AP18")
			)
			(pin power_in line
				(at 25.4 -160.02 180)
				(length 6.35)
				(name "GND")
				(number "AP28")
			)
			(pin power_in line
				(at 25.4 -162.56 180)
				(length 6.35)
				(name "GND")
				(number "AP34")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC7K420T-FFG901"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC7K420T-FFG901"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Kintex 7 T 420 XC7K420T-FFG901"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC7K420T-FFG901_1_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_11")
				(number "AC19")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_11")
				(number "AG19")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_11")
				(number "AH20")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_11")
				(number "AH19")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_11")
				(number "AJ19")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_11")
				(number "AK19")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_11")
				(number "AK20")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_11")
				(number "AJ18")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_11")
				(number "AK18")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_11")
				(number "AJ16")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_11")
				(number "AJ17")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_11")
				(number "AF18")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_11")
				(number "AG18")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_11")
				(number "AK15")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_11")
				(number "AK16")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_11")
				(number "AH14")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_11")
				(number "AH15")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_11")
				(number "AG14")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_11")
				(number "AG15")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_11")
				(number "AJ14")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_11")
				(number "AK14")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_11")
				(number "AH16")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_11")
				(number "AH17")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_11")
				(number "AF17")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_11")
				(number "AG17")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_11")
				(number "AF15")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_11")
				(number "AF16")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_11")
				(number "AE15")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_11")
				(number "AE16")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_11")
				(number "AC16")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_11")
				(number "AD16")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_11")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_11")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_11")
				(number "AC14")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_11")
				(number "AC15")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_11")
				(number "AD14")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_11")
				(number "AE14")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_11")
				(number "AE18")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_11")
				(number "AE19")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_11")
				(number "AD18")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_11")
				(number "AD19")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_11")
				(number "AC17")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_11")
				(number "AD17")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_11")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_11")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_11")
				(number "AA17")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_11")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_11")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_11")
				(number "Y19")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_11")
				(number "AB19")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AA19")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AB16")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AE17")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AF14")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AH18")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AJ15")
			)
			(pin power_in line
				(at 25.4 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AC23")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AD20")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AF24")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AG21")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AJ25")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AK22")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_12")
				(number "Y23")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_12")
				(number "Y20")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_12")
				(number "Y21")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_12")
				(number "AA20")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_12")
				(number "AA21")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_12")
				(number "AA22")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_12")
				(number "AA23")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_12")
				(number "AB20")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_12")
				(number "AC20")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_12")
				(number "AB22")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_12")
				(number "AB23")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_12")
				(number "AC21")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_12")
				(number "AC22")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_12")
				(number "AD26")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_12")
				(number "AE26")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_12")
				(number "AH25")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_12")
				(number "AH26")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_12")
				(number "AE25")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_12")
				(number "AF26")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_12")
				(number "AD24")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_12")
				(number "AE24")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_12")
				(number "AF25")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_12")
				(number "AG25")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_12")
				(number "AG24")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_12")
				(number "AH24")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_12")
				(number "AG22")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_12")
				(number "AG23")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_12")
				(number "AF22")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_12")
				(number "AF23")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_12")
				(number "AD23")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_12")
				(number "AE23")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_12")
				(number "AD21")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_12")
				(number "AD22")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_12")
				(number "AE21")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_12")
				(number "AF21")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_12")
				(number "AF20")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_12")
				(number "AG20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_12")
				(number "AH21")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_12")
				(number "AH22")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_12")
				(number "AJ21")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_12")
				(number "AK21")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_12")
				(number "AJ22")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_12")
				(number "AK23")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_12")
				(number "AJ23")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_12")
				(number "AJ24")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_12")
				(number "AK24")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_12")
				(number "AK25")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_12")
				(number "AJ26")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_12")
				(number "AK26")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_12")
				(number "AE20")
			)
		)
		(symbol "XC7K420T-FFG901_2_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_13")
				(number "W24")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_13")
				(number "AA28")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_13")
				(number "AB28")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_13")
				(number "AB29")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_13")
				(number "AB30")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_13")
				(number "Y30")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_13")
				(number "AA30")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_13")
				(number "Y28")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_13")
				(number "Y29")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_13")
				(number "W28")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_13")
				(number "W29")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_13")
				(number "W26")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_13")
				(number "W27")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_13")
				(number "AC26")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_13")
				(number "AD27")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_13")
				(number "Y25")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_13")
				(number "AA25")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_13")
				(number "AB25")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_13")
				(number "AC25")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_13")
				(number "AB24")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_13")
				(number "AC24")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_13")
				(number "Y26")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_13")
				(number "AA26")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_13")
				(number "AA27")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_13")
				(number "AB27")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_13")
				(number "AC27")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_13")
				(number "AD28")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_13")
				(number "AE28")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_13")
				(number "AF28")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_13")
				(number "AC29")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_13")
				(number "AC30")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_13")
				(number "AD29")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_13")
				(number "AE29")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_13")
				(number "AE30")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_13")
				(number "AF30")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_13")
				(number "AF27")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_13")
				(number "AG28")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_13")
				(number "AG27")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_13")
				(number "AH27")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_13")
				(number "AG29")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_13")
				(number "AH29")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_13")
				(number "AJ27")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_13")
				(number "AJ28")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_13")
				(number "AG30")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_13")
				(number "AH30")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_13")
				(number "AJ29")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_13")
				(number "AK30")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_13")
				(number "AK28")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_13")
				(number "AK29")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_13")
				(number "Y24")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AA29")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AB26")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AD30")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AE27")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AH28")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "W25")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "R17")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "R27")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "T24")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "U21")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "V18")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "V28")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_14")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_D00_MOSI_14")
				(number "R30")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_D01_DIN_14")
				(number "T30")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_D02_14")
				(number "R28")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_D03_14")
				(number "T28")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_PUDC_B_14")
				(number "V29")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_EMCCLK_14")
				(number "V30")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_D04_14")
				(number "U29")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_D05_14")
				(number "U30")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_D06_14")
				(number "U27")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_D07_14")
				(number "U28")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_FCS_B_14")
				(number "V26")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_D08_VREF_14")
				(number "V27")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_D09_14")
				(number "R24")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_D10_14")
				(number "R25")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_D11_14")
				(number "R23")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_D12_14")
				(number "T23")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_14")
				(number "V24")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_D13_14")
				(number "V25")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_D14_14")
				(number "R26")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_D15_14")
				(number "T27")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_14")
				(number "T25")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_14")
				(number "T26")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_14")
				(number "U24")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_14")
				(number "U25")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_14")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_14")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_14")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_14")
				(number "U23")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_RDWR_B_14")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_DOUT_CSO_B_14")
				(number "R21")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_CSI_B_14")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_A15_D31_14")
				(number "T21")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_A14_D30_14")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_A13_D29_14")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_A12_D28_14")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_A11_D27_14")
				(number "W23")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_A10_D26_14")
				(number "R18")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_A09_D25_VREF_14")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_A08_D24_14")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_A07_D23_14")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_14")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A06_D22_14")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_A05_D21_14")
				(number "U17")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_A04_D20_14")
				(number "U18")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_A03_D19_14")
				(number "V17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_A02_D18_14")
				(number "W17")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_A01_D17_14")
				(number "W18")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_A00_D16_14")
				(number "W19")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_14")
				(number "W21")
			)
		)
		(symbol "XC7K420T-FFG901_3_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_15")
				(number "L22")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_AD0P_15")
				(number "K28")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_AD0N_15")
				(number "K29")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_AD8P_15")
				(number "L30")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_AD8N_15")
				(number "K30")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_AD1P_15")
				(number "N30")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_AD1N_15")
				(number "M30")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_AD9P_15")
				(number "N29")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_AD9N_15")
				(number "M29")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_AD2P_15")
				(number "R29")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_AD2N_15")
				(number "P29")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_15")
				(number "M28")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_15")
				(number "L28")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_AD10P_15")
				(number "K25")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_AD10N_15")
				(number "K26")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_AD3P_15")
				(number "P26")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_AD3N_15")
				(number "N26")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_AD11P_15")
				(number "N27")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_AD11N_15")
				(number "M27")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_AD4P_15")
				(number "P27")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_AD4N_15")
				(number "P28")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_AD12P_15")
				(number "M25")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_AD12N_15")
				(number "L25")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_AD5P_15")
				(number "L26")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_AD5N_15")
				(number "L27")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_15")
				(number "M23")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_15")
				(number "M24")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_15")
				(number "N24")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_15")
				(number "N25")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_15")
				(number "L23")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_ADV_B_15")
				(number "K24")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_A28_15")
				(number "N22")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_A27_15")
				(number "M22")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_A26_15")
				(number "P23")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_A25_15")
				(number "P24")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_A24_15")
				(number "L20")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_A23_15")
				(number "L21")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_A22_15")
				(number "N20")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_A21_VREF_15")
				(number "M20")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_A20_15")
				(number "P21")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_A19_15")
				(number "N21")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_15")
				(number "M18")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A18_15")
				(number "M19")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_A17_15")
				(number "P19")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_A16_15")
				(number "N19")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_FOE_B_15")
				(number "N17")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_FWE_B_15")
				(number "M17")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_RS1_15")
				(number "P17")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_RS0_15")
				(number "P18")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_15")
				(number "P22")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "L19")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "L29")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "M26")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "N23")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "P20")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "P30")
			)
			(pin power_in line
				(at 25.4 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "A29")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "B26")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "D30")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "E27")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "F24")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "H28")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "J25")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_16")
				(number "E24")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_16")
				(number "D24")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_16")
				(number "C24")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_16")
				(number "B24")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_16")
				(number "B25")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_16")
				(number "C25")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_16")
				(number "C26")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_16")
				(number "A25")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_16")
				(number "A26")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_16")
				(number "C27")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_16")
				(number "B27")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_16")
				(number "D26")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_16")
				(number "D27")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_16")
				(number "H24")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_16")
				(number "G24")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_16")
				(number "H25")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_16")
				(number "G25")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_16")
				(number "J26")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_16")
				(number "J27")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_16")
				(number "H26")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_16")
				(number "H27")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_16")
				(number "F25")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_16")
				(number "F26")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_16")
				(number "E25")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_16")
				(number "E26")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_16")
				(number "G27")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_16")
				(number "F27")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_16")
				(number "G28")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_16")
				(number "F28")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_16")
				(number "H29")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_16")
				(number "G29")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_16")
				(number "F30")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_16")
				(number "E30")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_16")
				(number "H30")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_16")
				(number "G30")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_16")
				(number "J28")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_16")
				(number "J29")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_16")
				(number "E28")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_16")
				(number "D28")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_16")
				(number "E29")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_16")
				(number "D29")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_16")
				(number "C29")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_16")
				(number "C30")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_16")
				(number "B28")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_16")
				(number "B29")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_16")
				(number "B30")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_16")
				(number "A30")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_16")
				(number "A27")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_16")
				(number "A28")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_16")
				(number "J24")
			)
		)
		(symbol "XC7K420T-FFG901_4_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_17")
				(number "H21")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_17")
				(number "K23")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_17")
				(number "J23")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_17")
				(number "J22")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_17")
				(number "H22")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_17")
				(number "K21")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_17")
				(number "J21")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_17")
				(number "K19")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_17")
				(number "K20")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_17")
				(number "J18")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_17")
				(number "J19")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_17")
				(number "L18")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_17")
				(number "K18")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_17")
				(number "G23")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_17")
				(number "F23")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_17")
				(number "H20")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_17")
				(number "G20")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_17")
				(number "H19")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_17")
				(number "G19")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_17")
				(number "G18")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_17")
				(number "F18")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_17")
				(number "G22")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_17")
				(number "F22")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_17")
				(number "F20")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_17")
				(number "F21")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_17")
				(number "E20")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_17")
				(number "E21")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_17")
				(number "D21")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_17")
				(number "D22")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_17")
				(number "E23")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_17")
				(number "D23")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_17")
				(number "C21")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_17")
				(number "C22")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_17")
				(number "E18")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_17")
				(number "E19")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_17")
				(number "D18")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_17")
				(number "D19")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_17")
				(number "C19")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_17")
				(number "C20")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_17")
				(number "B19")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_17")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_17")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_17")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_17")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_17")
				(number "A21")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_17")
				(number "B22")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_17")
				(number "B23")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_17")
				(number "A22")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_17")
				(number "A23")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_17")
				(number "L17")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "A19")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "C23")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "D20")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "G21")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "H18")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "K22")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "B16")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "E17")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "F14")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "J15")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L6P_T0_18")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_18")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L7P_T1_18")
				(number "J14")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L7N_T1_18")
				(number "H15")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L8P_T1_18")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L8N_T1_18")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_18")
				(number "H14")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_18")
				(number "G14")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L10P_T1_18")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L10N_T1_18")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_18")
				(number "F16")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_18")
				(number "E16")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_18")
				(number "G15")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_18")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_18")
				(number "C15")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_18")
				(number "C16")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_18")
				(number "E15")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_18")
				(number "D16")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_18")
				(number "E14")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_18")
				(number "D14")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L16P_T2_18")
				(number "C14")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L16N_T2_18")
				(number "B15")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L17P_T2_18")
				(number "B14")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L17N_T2_18")
				(number "A14")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L18P_T2_18")
				(number "A15")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L18N_T2_18")
				(number "A16")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L19P_T3_18")
				(number "D17")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_18")
				(number "C17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L20P_T3_18")
				(number "B17")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L20N_T3_18")
				(number "A17")
			)
		)
		(symbol "XC7K420T-FFG901_5_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_111")
				(number "AJ12")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_111")
				(number "AJ11")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_111")
				(number "AK10")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_111")
				(number "AK9")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_111")
				(number "AJ8")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_111")
				(number "AJ7")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_111")
				(number "AG8")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_111")
				(number "AG7")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_111")
				(number "AH10")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_111")
				(number "AH9")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_111")
				(number "AG12")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_111")
				(number "AG11")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_111")
				(number "AF10")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_111")
				(number "AF9")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_111")
				(number "AE12")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_111")
				(number "AE11")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_111")
				(number "AC8")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_111")
				(number "AC7")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_111")
				(number "AE8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_111")
				(number "AE7")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_112")
				(number "AK6")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_112")
				(number "AK5")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_112")
				(number "AJ4")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_112")
				(number "AJ3")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_112")
				(number "AK2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_112")
				(number "AK1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_112")
				(number "AH2")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_112")
				(number "AH1")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_112")
				(number "AH6")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_112")
				(number "AH5")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_112")
				(number "AG4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_112")
				(number "AG3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_112")
				(number "AE4")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_112")
				(number "AE3")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_112")
				(number "AC4")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_112")
				(number "AC3")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_112")
				(number "AD6")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_112")
				(number "AD5")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_112")
				(number "AF6")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_112")
				(number "AF5")
			)
		)
		(symbol "XC7K420T-FFG901_6_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_113")
				(number "AF2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_113")
				(number "AF1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_113")
				(number "AD2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_113")
				(number "AD1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_113")
				(number "AB2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_113")
				(number "AB1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_113")
				(number "Y2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_113")
				(number "Y1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_113")
				(number "AB6")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_113")
				(number "AB5")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_113")
				(number "AA4")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_113")
				(number "AA3")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_113")
				(number "Y6")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_113")
				(number "Y5")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_113")
				(number "W4")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_113")
				(number "W3")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_113")
				(number "U8")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_113")
				(number "U7")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_113")
				(number "W8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_113")
				(number "W7")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_114")
				(number "V2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_114")
				(number "V1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_114")
				(number "T2")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_114")
				(number "T1")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_114")
				(number "P2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_114")
				(number "P1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_114")
				(number "N4")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_114")
				(number "N3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_114")
				(number "V6")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_114")
				(number "V5")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_114")
				(number "U4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_114")
				(number "U3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_114")
				(number "R4")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_114")
				(number "R3")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_114")
				(number "P6")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_114")
				(number "P5")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_114")
				(number "R8")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_114")
				(number "R7")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_114")
				(number "T6")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_114")
				(number "T5")
			)
		)
		(symbol "XC7K420T-FFG901_7_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_115")
				(number "M2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_115")
				(number "M1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_115")
				(number "K2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_115")
				(number "K1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_115")
				(number "H2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_115")
				(number "H1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_115")
				(number "F2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_115")
				(number "F1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_115")
				(number "M6")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_115")
				(number "M5")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_115")
				(number "L4")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_115")
				(number "L3")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_115")
				(number "K6")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_115")
				(number "K5")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_115")
				(number "J4")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_115")
				(number "J3")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_115")
				(number "J8")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_115")
				(number "J7")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_115")
				(number "L8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_115")
				(number "L7")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_116")
				(number "D2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_116")
				(number "D1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_116")
				(number "B2")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_116")
				(number "B1")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_116")
				(number "A4")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_116")
				(number "A3")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_116")
				(number "B6")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_116")
				(number "B5")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_116")
				(number "G4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_116")
				(number "G3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_116")
				(number "E4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_116")
				(number "E3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_116")
				(number "D6")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_116")
				(number "D5")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_116")
				(number "C4")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_116")
				(number "C3")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_116")
				(number "F6")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_116")
				(number "F5")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_116")
				(number "H6")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_116")
				(number "H5")
			)
		)
		(symbol "XC7K420T-FFG901_8_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_117")
				(number "C8")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_117")
				(number "C7")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_117")
				(number "A8")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_117")
				(number "A7")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_117")
				(number "B10")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_117")
				(number "B9")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_117")
				(number "A12")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_117")
				(number "A11")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_117")
				(number "F10")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_117")
				(number "F9")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_117")
				(number "D10")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_117")
				(number "D9")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_117")
				(number "E12")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_117")
				(number "E11")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_117")
				(number "C12")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_117")
				(number "C11")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_117")
				(number "E8")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_117")
				(number "E7")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_117")
				(number "G8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_117")
				(number "G7")
			)
		)
		(symbol "XC7K420T-FFG901_9_1"
			(pin power_in line
				(at -38.1 33.02 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AA6")
			)
			(pin power_in line
				(at -38.1 30.48 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AC6")
			)
			(pin power_in line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AE6")
			)
			(pin power_in line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AG6")
			)
			(pin power_in line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AH7")
			)
			(pin power_in line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AH11")
			)
			(pin power_in line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AK11")
			)
			(pin power_in line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "N6")
			)
			(pin power_in line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "R6")
			)
			(pin power_in line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "U6")
			)
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "W6")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTVCCAUX_G10")
				(number "AA8")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTVCCAUX_G10")
				(number "Y7")
			)
			(pin power_in line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "B11")
			)
			(pin power_in line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "D7")
			)
			(pin power_in line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "D11")
			)
			(pin power_in line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "E6")
			)
			(pin power_in line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "G6")
			)
			(pin power_in line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "J6")
			)
			(pin power_in line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "L6")
			)
			(pin power_in line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTVCCAUX_G11")
				(number "K8")
			)
			(pin power_in line
				(at 38.1 33.02 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AB3")
			)
			(pin power_in line
				(at 38.1 30.48 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AC2")
			)
			(pin power_in line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AF3")
			)
			(pin power_in line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AG2")
			)
			(pin power_in line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AG9")
			)
			(pin power_in line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AJ6")
			)
			(pin power_in line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AJ9")
			)
			(pin power_in line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AK3")
			)
			(pin power_in line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AK7")
			)
			(pin power_in line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "P3")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "R2")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "V3")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "W2")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "B3")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "B7")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "C2")
			)
			(pin power_in line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "C6")
			)
			(pin power_in line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "C9")
			)
			(pin power_in line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "E9")
			)
			(pin power_in line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "F3")
			)
			(pin power_in line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "G2")
			)
			(pin power_in line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "K3")
			)
			(pin power_in line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "L2")
			)
			(pin power_in line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "MGTAVTTRCAL_115")
				(number "N8")
			)
			(pin power_in line
				(at 38.1 -33.02 180)
				(length 6.35)
				(name "MGTRREF_115")
				(number "N7")
			)
		)
		(symbol "XC7K420T-FFG901_10_1"
			(pin power_in line
				(at 25.4 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "J10")
			)
			(pin power_in line
				(at 27.94 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "K11")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "TDI_0")
				(number "H11")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "TDO_0")
				(number "J13")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "TMS_0")
				(number "J11")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TCK_0")
				(number "H12")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "CCLK_0")
				(number "H13")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "M0_0")
				(number "AC13")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "M1_0")
				(number "AC12")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "M2_0")
				(number "AB12")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "DONE_0")
				(number "AC10")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "INIT_B_0")
				(number "H10")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "PROGRAM_B_0")
				(number "AB11")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "CFGBVS_0")
				(number "AC11")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "VP_0")
				(number "R13")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "VN_0")
				(number "T12")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 6.35)
				(name "VREFP_0")
				(number "T13")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "VREFN_0")
				(number "R12")
			)
			(pin bidirectional line
				(at 38.1 -35.56 180)
				(length 6.35)
				(name "DXP_0")
				(number "U13")
			)
			(pin bidirectional line
				(at 38.1 -38.1 180)
				(length 6.35)
				(name "DXN_0")
				(number "U12")
			)
		)
		(symbol "XC7K420T-FFG901_11_1"
			(pin power_in line
				(at -25.4 99.06 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M16")
			)
			(pin power_in line
				(at -25.4 96.52 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P16")
			)
			(pin power_in line
				(at -25.4 93.98 0)
				(length 6.35)
				(name "VCCAUX")
				(number "T16")
			)
			(pin power_in line
				(at -25.4 91.44 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V16")
			)
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "VCCAUX")
				(number "Y16")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "GNDADC_0")
				(number "P12")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "VCCADC_0")
				(number "P13")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "VCCBATT_0")
				(number "G13")
			)
			(pin power_in line
				(at -25.4 76.2 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "AA15")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "R15")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "U15")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "W15")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "A2")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "A5")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "A6")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "A10")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A13")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A24")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "B4")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B8")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B12")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B21")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C1")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "C5")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "C10")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "C13")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "C18")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "C28")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "D3")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "D8")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "D12")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "D13")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "D15")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "D25")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "E1")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "E10")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "E13")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "E22")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "F8")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "F12")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "F13")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "F19")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "F29")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "G1")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "G9")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "G10")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "G11")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 -91.44 0)
				(length 6.35)
				(name "GND")
				(number "G16")
			)
			(pin power_in line
				(at -25.4 -93.98 0)
				(length 6.35)
				(name "GND")
				(number "G26")
			)
			(pin power_in line
				(at -25.4 -96.52 0)
				(length 6.35)
				(name "GND")
				(number "H3")
			)
			(pin power_in line
				(at -25.4 -99.06 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at 25.4 99.06 180)
				(length 6.35)
				(name "VCCINT")
				(number "K12")
			)
			(pin power_in line
				(at 25.4 96.52 180)
				(length 6.35)
				(name "VCCINT")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 93.98 180)
				(length 6.35)
				(name "VCCINT")
				(number "K16")
			)
			(pin power_in line
				(at 25.4 91.44 180)
				(length 6.35)
				(name "VCCINT")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "L13")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "L15")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "R11")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "T10")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "T14")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "U11")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "V10")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "V12")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "W11")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "W13")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y10")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y12")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y14")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "AA11")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "H9")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "H23")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "J1")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "J5")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "J20")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "J30")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "K4")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "K7")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "K15")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "K17")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "K27")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "L1")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "L16")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "L24")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "M3")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "M4")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "M7")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "M8")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "M21")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "N1")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "N5")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "N16")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "N18")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "N28")
			)
			(pin power_in line
				(at 25.4 -91.44 180)
				(length 6.35)
				(name "GND")
				(number "P4")
			)
			(pin power_in line
				(at 25.4 -93.98 180)
				(length 6.35)
				(name "GND")
				(number "P7")
			)
			(pin power_in line
				(at 25.4 -96.52 180)
				(length 6.35)
				(name "GND")
				(number "P8")
			)
			(pin power_in line
				(at 25.4 -99.06 180)
				(length 6.35)
				(name "GND")
				(number "P9")
			)
		)
		(symbol "XC7K420T-FFG901_12_1"
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "GND")
				(number "P11")
			)
			(pin power_in line
				(at -25.4 76.2 0)
				(length 6.35)
				(name "GND")
				(number "P15")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "GND")
				(number "P25")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "GND")
				(number "R9")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "GND")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "GND")
				(number "R14")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "GND")
				(number "R16")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "GND")
				(number "R22")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "GND")
				(number "T3")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "GND")
				(number "T4")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "GND")
				(number "T7")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "GND")
				(number "T8")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "GND")
				(number "T9")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "GND")
				(number "T11")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "GND")
				(number "T15")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "T19")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "T29")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "U1")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "U5")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "U9")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "U10")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "U14")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "U16")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "U26")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "V7")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "V8")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "V9")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "V11")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "V13")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "V15")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "V23")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "W1")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "W5")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "W9")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "W10")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "W12")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "W14")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "W16")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "W20")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "W30")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "Y3")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "Y4")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "Y8")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "Y9")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "Y11")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "Y13")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "Y15")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "Y17")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "Y27")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "AA1")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "AA2")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "AA7")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "AA10")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "AA12")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "AA14")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "AA16")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "AA24")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "GND")
				(number "AB4")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "GND")
				(number "AB7")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "GND")
				(number "AB8")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "GND")
				(number "AB9")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "GND")
				(number "AB10")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "GND")
				(number "AB13")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "GND")
				(number "AB21")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "GND")
				(number "AC1")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "GND")
				(number "AC5")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "GND")
				(number "AC9")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "GND")
				(number "AC18")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "GND")
				(number "AC28")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "GND")
				(number "AD3")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "GND")
				(number "AD4")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "GND")
				(number "AD7")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "GND")
				(number "AD8")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "GND")
				(number "AD9")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "AD10")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "AD11")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "AD12")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "AD13")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "AD15")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "AD25")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "AE1")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "AE2")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "AE5")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "AE9")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "AE10")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "AE13")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "AE22")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "AF4")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "AF7")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "AF8")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "AF11")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "AF12")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "AF13")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "AF19")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "AF29")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "AG1")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "AG5")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "AG10")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "AG13")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "AG16")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "AG26")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "AH3")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "AH4")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "AH8")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "AH12")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "AH13")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "AH23")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "AJ1")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AJ2")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AJ5")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AJ10")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AJ13")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AJ20")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AJ30")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AK4")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AK8")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AK12")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AK13")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "AK17")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "AK27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC7K480T-FFG1156"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC7K480T-FFG1156"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Kintex 7 T 480 XC7K480T-FFG1156"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC7K480T-FFG1156_1_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_11")
				(number "AG18")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_11")
				(number "AK23")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_11")
				(number "AL23")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_11")
				(number "AM22")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_11")
				(number "AN22")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_11")
				(number "AP21")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_11")
				(number "AP22")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_11")
				(number "AN20")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_11")
				(number "AP20")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_11")
				(number "AN19")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_11")
				(number "AP19")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_11")
				(number "AL21")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_11")
				(number "AM21")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_11")
				(number "AN17")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_11")
				(number "AN18")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_11")
				(number "AP16")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_11")
				(number "AP17")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_11")
				(number "AM17")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_11")
				(number "AM18")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_11")
				(number "AL16")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_11")
				(number "AM16")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_11")
				(number "AL20")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_11")
				(number "AM20")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_11")
				(number "AL18")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_11")
				(number "AL19")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_11")
				(number "AK18")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_11")
				(number "AK19")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_11")
				(number "AH19")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_11")
				(number "AJ19")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_11")
				(number "AK16")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_11")
				(number "AK17")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_11")
				(number "AJ16")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_11")
				(number "AJ17")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_11")
				(number "AH17")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_11")
				(number "AH18")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_11")
				(number "AG16")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_11")
				(number "AG17")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_11")
				(number "AJ22")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_11")
				(number "AK22")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_11")
				(number "AJ21")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_11")
				(number "AK21")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_11")
				(number "AH20")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_11")
				(number "AJ20")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_11")
				(number "AG20")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_11")
				(number "AG21")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_11")
				(number "AG22")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_11")
				(number "AH22")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_11")
				(number "AG23")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_11")
				(number "AH23")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_11")
				(number "AG15")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AH21")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AJ18")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AK15")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AL22")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AM19")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AN16")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AF27")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AG24")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AJ28")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AK25")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AN26")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AP23")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_12")
				(number "AD25")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_12")
				(number "AM23")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_12")
				(number "AN23")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_12")
				(number "AN24")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_12")
				(number "AP24")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_12")
				(number "AN25")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_12")
				(number "AP25")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_12")
				(number "AP26")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_12")
				(number "AP27")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_12")
				(number "AN27")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_12")
				(number "AN28")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_12")
				(number "AM27")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_12")
				(number "AM28")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_12")
				(number "AM25")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_12")
				(number "AM26")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_12")
				(number "AJ29")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_12")
				(number "AK29")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_12")
				(number "AK24")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_12")
				(number "AL24")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_12")
				(number "AK28")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_12")
				(number "AL28")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_12")
				(number "AL25")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_12")
				(number "AL26")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_12")
				(number "AK26")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_12")
				(number "AK27")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_12")
				(number "AJ26")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_12")
				(number "AJ27")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_12")
				(number "AH27")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_12")
				(number "AH28")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_12")
				(number "AH25")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_12")
				(number "AJ25")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_12")
				(number "AH24")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_12")
				(number "AJ24")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_12")
				(number "AG26")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_12")
				(number "AG27")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_12")
				(number "AG28")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_12")
				(number "AH29")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_12")
				(number "AD29")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_12")
				(number "AE29")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_12")
				(number "AF28")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_12")
				(number "AF29")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_12")
				(number "AE27")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_12")
				(number "AE28")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_12")
				(number "AE26")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_12")
				(number "AF26")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_12")
				(number "AE24")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_12")
				(number "AF24")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_12")
				(number "AF25")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_12")
				(number "AG25")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_12")
				(number "AD24")
			)
		)
		(symbol "XC7K480T-FFG1156_2_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_13")
				(number "AC30")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_13")
				(number "AC32")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_13")
				(number "AC33")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_13")
				(number "AC34")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_13")
				(number "AD34")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_13")
				(number "AE34")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_13")
				(number "AF34")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_13")
				(number "AE33")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_13")
				(number "AF33")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_13")
				(number "AE31")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_13")
				(number "AE32")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_13")
				(number "AD31")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_13")
				(number "AD32")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_13")
				(number "AH34")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_13")
				(number "AJ34")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_13")
				(number "AF30")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_13")
				(number "AG30")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_13")
				(number "AG33")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_13")
				(number "AH33")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_13")
				(number "AH30")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_13")
				(number "AJ30")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_13")
				(number "AG32")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_13")
				(number "AH32")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_13")
				(number "AF31")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_13")
				(number "AG31")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_13")
				(number "AJ31")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_13")
				(number "AK31")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_13")
				(number "AJ32")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_13")
				(number "AK32")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_13")
				(number "AK33")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_13")
				(number "AL33")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_13")
				(number "AK34")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_13")
				(number "AL34")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_13")
				(number "AL30")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_13")
				(number "AL31")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_13")
				(number "AL29")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_13")
				(number "AM30")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_13")
				(number "AM31")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_13")
				(number "AM32")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_13")
				(number "AM33")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_13")
				(number "AN34")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_13")
				(number "AN32")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_13")
				(number "AP33")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_13")
				(number "AP31")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_13")
				(number "AP32")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_13")
				(number "AP29")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_13")
				(number "AP30")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_13")
				(number "AN29")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_13")
				(number "AN30")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_13")
				(number "AD30")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AD33")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AE30")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AG34")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AH31")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AL32")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AM29")
			)
			(pin power_in line
				(at -25.4 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AN33")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "AA32")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "AB29")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "AC26")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "V31")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "W28")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "Y25")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_14")
				(number "AA24")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_D00_MOSI_14")
				(number "AA33")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_D01_DIN_14")
				(number "AA34")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_D02_14")
				(number "Y33")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_D03_14")
				(number "Y34")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_PUDC_B_14")
				(number "V34")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_EMCCLK_14")
				(number "W34")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_D04_14")
				(number "V32")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_D05_14")
				(number "V33")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_D06_14")
				(number "W31")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_D07_14")
				(number "W32")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_FCS_B_14")
				(number "V30")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_D08_VREF_14")
				(number "W30")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_D09_14")
				(number "V25")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_D10_14")
				(number "W25")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_D11_14")
				(number "V29")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_D12_14")
				(number "W29")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_14")
				(number "V27")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_D13_14")
				(number "V28")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_D14_14")
				(number "W24")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_D15_14")
				(number "Y24")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_14")
				(number "W26")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_14")
				(number "W27")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_14")
				(number "Y26")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_14")
				(number "Y27")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_14")
				(number "AA28")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_14")
				(number "AA29")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_14")
				(number "Y28")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_14")
				(number "Y29")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_RDWR_B_14")
				(number "AB30")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_DOUT_CSO_B_14")
				(number "AB31")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_CSI_B_14")
				(number "Y31")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_A15_D31_14")
				(number "Y32")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_A14_D30_14")
				(number "AB32")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_A13_D29_14")
				(number "AB33")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_A12_D28_14")
				(number "AA30")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_A11_D27_14")
				(number "AA31")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_A10_D26_14")
				(number "AA26")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_A09_D25_VREF_14")
				(number "AB26")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_A08_D24_14")
				(number "AB27")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_A07_D23_14")
				(number "AB28")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_14")
				(number "AA25")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A06_D22_14")
				(number "AB25")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_A05_D21_14")
				(number "AC27")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_A04_D20_14")
				(number "AD27")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_A03_D19_14")
				(number "AC28")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_A02_D18_14")
				(number "AC29")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_A01_D17_14")
				(number "AC25")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_A00_D16_14")
				(number "AD26")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_14")
				(number "AC24")
			)
		)
		(symbol "XC7K480T-FFG1156_3_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_15")
				(number "T24")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_AD0P_15")
				(number "N28")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_AD0N_15")
				(number "M28")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_AD8P_15")
				(number "P29")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_AD8N_15")
				(number "N29")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_AD1P_15")
				(number "P27")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_AD1N_15")
				(number "N27")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_AD9P_15")
				(number "N24")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_AD9N_15")
				(number "N25")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_AD2P_15")
				(number "P25")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_AD2N_15")
				(number "P26")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_15")
				(number "R24")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_15")
				(number "P24")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_AD10P_15")
				(number "R26")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_AD10N_15")
				(number "R27")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_AD3P_15")
				(number "T25")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_AD3N_15")
				(number "T26")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_AD11P_15")
				(number "U25")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_AD11N_15")
				(number "U26")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_AD4P_15")
				(number "U27")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_AD4N_15")
				(number "U28")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_AD12P_15")
				(number "T28")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_AD12N_15")
				(number "T29")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_AD5P_15")
				(number "R28")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_AD5N_15")
				(number "R29")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_15")
				(number "R31")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_15")
				(number "P31")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_15")
				(number "P30")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_15")
				(number "N30")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_15")
				(number "M30")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_ADV_B_15")
				(number "M31")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_A28_15")
				(number "N32")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_A27_15")
				(number "M32")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_A26_15")
				(number "N33")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_A25_15")
				(number "M33")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_A24_15")
				(number "P34")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_A23_15")
				(number "N34")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_A22_15")
				(number "U30")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_A21_VREF_15")
				(number "U31")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_A20_15")
				(number "T30")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_A19_15")
				(number "T31")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_15")
				(number "U32")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A18_15")
				(number "U33")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_A17_15")
				(number "R32")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_A16_15")
				(number "P32")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_FOE_B_15")
				(number "T33")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_FWE_B_15")
				(number "T34")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_RS1_15")
				(number "R33")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_RS0_15")
				(number "R34")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_15")
				(number "V24")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "N26")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "P33")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "R30")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "T27")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "U24")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "U34")
			)
			(pin power_in line
				(at 25.4 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "A32")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "B29")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "D33")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "E30")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "G34")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "H31")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "L32")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_16")
				(number "J29")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_16")
				(number "A29")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_16")
				(number "A30")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_16")
				(number "B30")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_16")
				(number "A31")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_16")
				(number "B31")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_16")
				(number "B32")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_16")
				(number "B33")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_16")
				(number "A33")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_16")
				(number "C32")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_16")
				(number "C33")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_16")
				(number "C29")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_16")
				(number "C30")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_16")
				(number "D29")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_16")
				(number "D30")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_16")
				(number "F34")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_16")
				(number "E34")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_16")
				(number "D34")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_16")
				(number "C34")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_16")
				(number "F33")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_16")
				(number "E33")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_16")
				(number "E31")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_16")
				(number "D31")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_16")
				(number "E32")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_16")
				(number "D32")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_16")
				(number "G30")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_16")
				(number "F30")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_16")
				(number "G31")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_16")
				(number "F31")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_16")
				(number "H29")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_16")
				(number "H30")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_16")
				(number "F29")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_16")
				(number "E29")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_16")
				(number "H32")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_16")
				(number "G32")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_16")
				(number "H33")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_16")
				(number "G33")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_16")
				(number "J30")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_16")
				(number "J31")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_16")
				(number "L31")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_16")
				(number "K31")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_16")
				(number "K32")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_16")
				(number "J32")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_16")
				(number "L33")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_16")
				(number "K33")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_16")
				(number "L34")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_16")
				(number "K34")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_16")
				(number "J34")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_16")
				(number "H34")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_16")
				(number "L30")
			)
		)
		(symbol "XC7K480T-FFG1156_4_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_17")
				(number "H23")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_17")
				(number "C24")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_17")
				(number "C25")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_17")
				(number "A24")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_17")
				(number "A25")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_17")
				(number "B25")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_17")
				(number "A26")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_17")
				(number "B26")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_17")
				(number "B27")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_17")
				(number "B28")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_17")
				(number "A28")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_17")
				(number "C27")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_17")
				(number "C28")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_17")
				(number "F24")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_17")
				(number "E24")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_17")
				(number "D26")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_17")
				(number "D27")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_17")
				(number "D24")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_17")
				(number "D25")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_17")
				(number "F28")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_17")
				(number "E28")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_17")
				(number "F25")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_17")
				(number "F26")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_17")
				(number "E26")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_17")
				(number "E27")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_17")
				(number "H27")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_17")
				(number "G27")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_17")
				(number "G25")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_17")
				(number "G26")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_17")
				(number "J24")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_17")
				(number "J25")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_17")
				(number "H24")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_17")
				(number "H25")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_17")
				(number "H28")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_17")
				(number "G28")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_17")
				(number "J26")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_17")
				(number "J27")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_17")
				(number "L25")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_17")
				(number "L26")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_17")
				(number "L24")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_17")
				(number "K24")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_17")
				(number "K28")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_17")
				(number "K29")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_17")
				(number "K26")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_17")
				(number "K27")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_17")
				(number "M26")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_17")
				(number "M27")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_17")
				(number "L28")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_17")
				(number "L29")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_17")
				(number "M25")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "C26")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "F27")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "G24")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "J28")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "K25")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "M29")
			)
			(pin power_in line
				(at 25.4 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "A22")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "B19")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "C16")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "D23")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "E20")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "F17")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_18")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_18")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_18")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_18")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_18")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_18")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_18")
				(number "G18")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_18")
				(number "F16")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_18")
				(number "E16")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_18")
				(number "E17")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_18")
				(number "E18")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_18")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_18")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_18")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_18")
				(number "G21")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_18")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_18")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_18")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_18")
				(number "G23")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_18")
				(number "F23")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_18")
				(number "E23")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_18")
				(number "D20")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_18")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_18")
				(number "E21")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_18")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_18")
				(number "E19")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_18")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_18")
				(number "C18")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_18")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_18")
				(number "D16")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_18")
				(number "D17")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_18")
				(number "C17")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_18")
				(number "B17")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_18")
				(number "B16")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_18")
				(number "A16")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_18")
				(number "B18")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_18")
				(number "A18")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_18")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_18")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_18")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_18")
				(number "B20")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_18")
				(number "A19")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_18")
				(number "A20")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_18")
				(number "B21")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_18")
				(number "A21")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_18")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_18")
				(number "A23")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_18")
				(number "C23")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_18")
				(number "B23")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_18")
				(number "H22")
			)
		)
		(symbol "XC7K480T-FFG1156_5_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_111")
				(number "AN12")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_111")
				(number "AN11")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_111")
				(number "AP10")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_111")
				(number "AP9")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_111")
				(number "AN8")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_111")
				(number "AN7")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_111")
				(number "AL8")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_111")
				(number "AL7")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_111")
				(number "AM10")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_111")
				(number "AM9")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_111")
				(number "AL12")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_111")
				(number "AL11")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_111")
				(number "AJ12")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_111")
				(number "AJ11")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_111")
				(number "AK10")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_111")
				(number "AK9")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_111")
				(number "AH10")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_111")
				(number "AH9")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_111")
				(number "AJ8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_111")
				(number "AJ7")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_112")
				(number "AP6")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_112")
				(number "AP5")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_112")
				(number "AN4")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_112")
				(number "AN3")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_112")
				(number "AP2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_112")
				(number "AP1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_112")
				(number "AM2")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_112")
				(number "AM1")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_112")
				(number "AM6")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_112")
				(number "AM5")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_112")
				(number "AL4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_112")
				(number "AL3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_112")
				(number "AK6")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_112")
				(number "AK5")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_112")
				(number "AJ4")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_112")
				(number "AJ3")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_112")
				(number "AG8")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_112")
				(number "AG7")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_112")
				(number "AH6")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_112")
				(number "AH5")
			)
		)
		(symbol "XC7K480T-FFG1156_6_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_113")
				(number "AK2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_113")
				(number "AK1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_113")
				(number "AH2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_113")
				(number "AH1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_113")
				(number "AF2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_113")
				(number "AF1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_113")
				(number "AD2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_113")
				(number "AD1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_113")
				(number "AG4")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_113")
				(number "AG3")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_113")
				(number "AF6")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_113")
				(number "AF5")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_113")
				(number "AE4")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_113")
				(number "AE3")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_113")
				(number "AC4")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_113")
				(number "AC3")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_113")
				(number "AC8")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_113")
				(number "AC7")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_113")
				(number "AD6")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_113")
				(number "AD5")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_114")
				(number "AB2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_114")
				(number "AB1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_114")
				(number "Y2")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_114")
				(number "Y1")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_114")
				(number "W4")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_114")
				(number "W3")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_114")
				(number "V2")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_114")
				(number "V1")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_114")
				(number "AB6")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_114")
				(number "AB5")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_114")
				(number "AA4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_114")
				(number "AA3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_114")
				(number "Y6")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_114")
				(number "Y5")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_114")
				(number "V6")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_114")
				(number "V5")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_114")
				(number "W8")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_114")
				(number "W7")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_114")
				(number "AA8")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_114")
				(number "AA7")
			)
		)
		(symbol "XC7K480T-FFG1156_7_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_115")
				(number "U4")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_115")
				(number "U3")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_115")
				(number "T2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_115")
				(number "T1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_115")
				(number "P2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_115")
				(number "P1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_115")
				(number "N4")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_115")
				(number "N3")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_115")
				(number "T6")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_115")
				(number "T5")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_115")
				(number "R4")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_115")
				(number "R3")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_115")
				(number "P6")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_115")
				(number "P5")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_115")
				(number "M6")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_115")
				(number "M5")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_115")
				(number "R8")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_115")
				(number "R7")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_115")
				(number "U8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_115")
				(number "U7")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_116")
				(number "M2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_116")
				(number "M1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_116")
				(number "K2")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_116")
				(number "K1")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_116")
				(number "H2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_116")
				(number "H1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_116")
				(number "F2")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_116")
				(number "F1")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_116")
				(number "L4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_116")
				(number "L3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_116")
				(number "K6")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_116")
				(number "K5")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_116")
				(number "J4")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_116")
				(number "J3")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_116")
				(number "H6")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_116")
				(number "H5")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_116")
				(number "J8")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_116")
				(number "J7")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_116")
				(number "L8")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_116")
				(number "L7")
			)
		)
		(symbol "XC7K480T-FFG1156_8_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_117")
				(number "D2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_117")
				(number "D1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_117")
				(number "B2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_117")
				(number "B1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_117")
				(number "A4")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_117")
				(number "A3")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_117")
				(number "B6")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_117")
				(number "B5")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_117")
				(number "G4")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_117")
				(number "G3")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_117")
				(number "E4")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_117")
				(number "E3")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_117")
				(number "D6")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_117")
				(number "D5")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_117")
				(number "C4")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_117")
				(number "C3")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_117")
				(number "F6")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_117")
				(number "F5")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_117")
				(number "G8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_117")
				(number "G7")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_118")
				(number "C8")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_118")
				(number "C7")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_118")
				(number "A8")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_118")
				(number "A7")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_118")
				(number "B10")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_118")
				(number "B9")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_118")
				(number "A12")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_118")
				(number "A11")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_118")
				(number "F10")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_118")
				(number "F9")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_118")
				(number "E12")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_118")
				(number "E11")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_118")
				(number "D10")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_118")
				(number "D9")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_118")
				(number "C12")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_118")
				(number "C11")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_118")
				(number "E8")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_118")
				(number "E7")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_118")
				(number "H10")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_118")
				(number "H9")
			)
		)
		(symbol "XC7K480T-FFG1156_9_1"
			(pin power_in line
				(at -38.1 35.56 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AA6")
			)
			(pin power_in line
				(at -38.1 33.02 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AC6")
			)
			(pin power_in line
				(at -38.1 30.48 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AE6")
			)
			(pin power_in line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AG6")
			)
			(pin power_in line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AJ6")
			)
			(pin power_in line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AJ9")
			)
			(pin power_in line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AK12")
			)
			(pin power_in line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AM12")
			)
			(pin power_in line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AP12")
			)
			(pin power_in line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "W6")
			)
			(pin power_in line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTVCCAUX_G10")
				(number "AD9")
			)
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTVCCAUX_G10")
				(number "AE8")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "B12")
			)
			(pin power_in line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "D12")
			)
			(pin power_in line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "F12")
			)
			(pin power_in line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "G6")
			)
			(pin power_in line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "G9")
			)
			(pin power_in line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "J6")
			)
			(pin power_in line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "L6")
			)
			(pin power_in line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "N6")
			)
			(pin power_in line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "R6")
			)
			(pin power_in line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "U6")
			)
			(pin power_in line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTVCCAUX_G11")
				(number "M9")
			)
			(pin power_in line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTVCCAUX_G11")
				(number "N8")
			)
			(pin power_in line
				(at 38.1 35.56 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AC2")
			)
			(pin power_in line
				(at 38.1 33.02 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AD3")
			)
			(pin power_in line
				(at 38.1 30.48 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AG2")
			)
			(pin power_in line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AH3")
			)
			(pin power_in line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AL2")
			)
			(pin power_in line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AL6")
			)
			(pin power_in line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AL9")
			)
			(pin power_in line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AM3")
			)
			(pin power_in line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AN6")
			)
			(pin power_in line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AN9")
			)
			(pin power_in line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "W2")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "Y3")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "C2")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "C6")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "C9")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "D3")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "E6")
			)
			(pin power_in line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "E9")
			)
			(pin power_in line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "G2")
			)
			(pin power_in line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "H3")
			)
			(pin power_in line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "L2")
			)
			(pin power_in line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "M3")
			)
			(pin power_in line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "R2")
			)
			(pin power_in line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "T3")
			)
			(pin power_in line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "MGTAVTTRCAL_115")
				(number "T10")
			)
			(pin power_in line
				(at 38.1 -33.02 180)
				(length 6.35)
				(name "MGTRREF_115")
				(number "T9")
			)
		)
		(symbol "XC7K480T-FFG1156_10_1"
			(pin power_in line
				(at 25.4 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G14")
			)
			(pin power_in line
				(at 27.94 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H13")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "TDI_0")
				(number "G15")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "TDO_0")
				(number "F14")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "TMS_0")
				(number "H15")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TCK_0")
				(number "F15")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "CCLK_0")
				(number "D15")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "M0_0")
				(number "AJ15")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "M1_0")
				(number "AH15")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "M2_0")
				(number "AJ14")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "DONE_0")
				(number "AH14")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "INIT_B_0")
				(number "AG14")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "PROGRAM_B_0")
				(number "AM15")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "CFGBVS_0")
				(number "AL15")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "VP_0")
				(number "U17")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "VN_0")
				(number "V16")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 6.35)
				(name "VREFP_0")
				(number "V17")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "VREFN_0")
				(number "U16")
			)
			(pin bidirectional line
				(at 38.1 -35.56 180)
				(length 6.35)
				(name "DXP_0")
				(number "W17")
			)
			(pin bidirectional line
				(at 38.1 -38.1 180)
				(length 6.35)
				(name "DXN_0")
				(number "W16")
			)
		)
		(symbol "XC7K480T-FFG1156_11_1"
			(pin power_in line
				(at -25.4 175.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "Y15")
			)
			(pin power_in line
				(at -25.4 172.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "Y17")
			)
			(pin power_in line
				(at -25.4 170.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA16")
			)
			(pin power_in line
				(at -25.4 167.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA18")
			)
			(pin power_in line
				(at -25.4 165.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AB15")
			)
			(pin power_in line
				(at -25.4 162.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AB17")
			)
			(pin power_in line
				(at -25.4 160.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AC16")
			)
			(pin power_in line
				(at -25.4 157.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AC18")
			)
			(pin power_in line
				(at -25.4 154.94 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AD15")
			)
			(pin power_in line
				(at -25.4 152.4 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AD17")
			)
			(pin power_in line
				(at -25.4 149.86 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AE16")
			)
			(pin power_in line
				(at -25.4 147.32 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AE18")
			)
			(pin power_in line
				(at -25.4 144.78 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AF15")
			)
			(pin power_in line
				(at -25.4 142.24 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AF17")
			)
			(pin power_in line
				(at -25.4 137.16 0)
				(length 6.35)
				(name "GNDADC_0")
				(number "T16")
			)
			(pin power_in line
				(at -25.4 134.62 0)
				(length 6.35)
				(name "VCCADC_0")
				(number "T17")
			)
			(pin power_in line
				(at -25.4 132.08 0)
				(length 6.35)
				(name "VCCBATT_0")
				(number "C15")
			)
			(pin power_in line
				(at -25.4 129.54 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "AA20")
			)
			(pin power_in line
				(at -25.4 127 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "AB19")
			)
			(pin power_in line
				(at -25.4 124.46 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "AC20")
			)
			(pin power_in line
				(at -25.4 121.92 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "AD19")
			)
			(pin power_in line
				(at -25.4 119.38 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "AE20")
			)
			(pin power_in line
				(at -25.4 116.84 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "AF19")
			)
			(pin power_in line
				(at -25.4 114.3 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "R20")
			)
			(pin power_in line
				(at -25.4 111.76 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "T19")
			)
			(pin power_in line
				(at -25.4 109.22 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "U20")
			)
			(pin power_in line
				(at -25.4 106.68 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "V19")
			)
			(pin power_in line
				(at -25.4 104.14 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "W20")
			)
			(pin power_in line
				(at -25.4 101.6 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "Y19")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "A2")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "A5")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "A6")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "A10")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "A13")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "A14")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "A15")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "A17")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "A27")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "A34")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "B3")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "B4")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "B8")
			)
			(pin power_in line
				(at -25.4 -91.44 0)
				(length 6.35)
				(name "GND")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 -93.98 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 -96.52 0)
				(length 6.35)
				(name "GND")
				(number "B14")
			)
			(pin power_in line
				(at -25.4 -99.06 0)
				(length 6.35)
				(name "GND")
				(number "B15")
			)
			(pin power_in line
				(at -25.4 -101.6 0)
				(length 6.35)
				(name "GND")
				(number "B24")
			)
			(pin power_in line
				(at -25.4 -104.14 0)
				(length 6.35)
				(name "GND")
				(number "B34")
			)
			(pin power_in line
				(at -25.4 -106.68 0)
				(length 6.35)
				(name "GND")
				(number "C1")
			)
			(pin power_in line
				(at -25.4 -109.22 0)
				(length 6.35)
				(name "GND")
				(number "C5")
			)
			(pin power_in line
				(at -25.4 -111.76 0)
				(length 6.35)
				(name "GND")
				(number "C10")
			)
			(pin power_in line
				(at -25.4 -114.3 0)
				(length 6.35)
				(name "GND")
				(number "C13")
			)
			(pin power_in line
				(at -25.4 -116.84 0)
				(length 6.35)
				(name "GND")
				(number "C14")
			)
			(pin power_in line
				(at -25.4 -119.38 0)
				(length 6.35)
				(name "GND")
				(number "C21")
			)
			(pin power_in line
				(at -25.4 -121.92 0)
				(length 6.35)
				(name "GND")
				(number "C31")
			)
			(pin power_in line
				(at -25.4 -124.46 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -127 0)
				(length 6.35)
				(name "GND")
				(number "D7")
			)
			(pin power_in line
				(at -25.4 -129.54 0)
				(length 6.35)
				(name "GND")
				(number "D8")
			)
			(pin power_in line
				(at -25.4 -132.08 0)
				(length 6.35)
				(name "GND")
				(number "D11")
			)
			(pin power_in line
				(at -25.4 -134.62 0)
				(length 6.35)
				(name "GND")
				(number "D13")
			)
			(pin power_in line
				(at -25.4 -137.16 0)
				(length 6.35)
				(name "GND")
				(number "D14")
			)
			(pin power_in line
				(at -25.4 -139.7 0)
				(length 6.35)
				(name "GND")
				(number "D18")
			)
			(pin power_in line
				(at -25.4 -142.24 0)
				(length 6.35)
				(name "GND")
				(number "D28")
			)
			(pin power_in line
				(at -25.4 -144.78 0)
				(length 6.35)
				(name "GND")
				(number "E1")
			)
			(pin power_in line
				(at -25.4 -147.32 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -149.86 0)
				(length 6.35)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 -152.4 0)
				(length 6.35)
				(name "GND")
				(number "E10")
			)
			(pin power_in line
				(at -25.4 -154.94 0)
				(length 6.35)
				(name "GND")
				(number "E13")
			)
			(pin power_in line
				(at -25.4 -157.48 0)
				(length 6.35)
				(name "GND")
				(number "E14")
			)
			(pin power_in line
				(at -25.4 -160.02 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -162.56 0)
				(length 6.35)
				(name "GND")
				(number "E25")
			)
			(pin power_in line
				(at -25.4 -165.1 0)
				(length 6.35)
				(name "GND")
				(number "F3")
			)
			(pin power_in line
				(at -25.4 -167.64 0)
				(length 6.35)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at -25.4 -170.18 0)
				(length 6.35)
				(name "GND")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 -172.72 0)
				(length 6.35)
				(name "GND")
				(number "F8")
			)
			(pin power_in line
				(at -25.4 -175.26 0)
				(length 6.35)
				(name "GND")
				(number "F11")
			)
			(pin power_in line
				(at 25.4 175.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 172.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "J14")
			)
			(pin power_in line
				(at 25.4 170.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "J16")
			)
			(pin power_in line
				(at 25.4 167.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "J18")
			)
			(pin power_in line
				(at 25.4 165.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "J20")
			)
			(pin power_in line
				(at 25.4 162.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "J22")
			)
			(pin power_in line
				(at 25.4 160.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 157.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 154.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "K15")
			)
			(pin power_in line
				(at 25.4 152.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "K17")
			)
			(pin power_in line
				(at 25.4 149.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "K19")
			)
			(pin power_in line
				(at 25.4 147.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "K21")
			)
			(pin power_in line
				(at 25.4 144.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "K23")
			)
			(pin power_in line
				(at 25.4 142.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 139.7 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 137.16 180)
				(length 6.35)
				(name "VCCINT")
				(number "L16")
			)
			(pin power_in line
				(at 25.4 134.62 180)
				(length 6.35)
				(name "VCCINT")
				(number "L18")
			)
			(pin power_in line
				(at 25.4 132.08 180)
				(length 6.35)
				(name "VCCINT")
				(number "L20")
			)
			(pin power_in line
				(at 25.4 129.54 180)
				(length 6.35)
				(name "VCCINT")
				(number "L22")
			)
			(pin power_in line
				(at 25.4 127 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 124.46 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 121.92 180)
				(length 6.35)
				(name "VCCINT")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 119.38 180)
				(length 6.35)
				(name "VCCINT")
				(number "M17")
			)
			(pin power_in line
				(at 25.4 116.84 180)
				(length 6.35)
				(name "VCCINT")
				(number "M19")
			)
			(pin power_in line
				(at 25.4 114.3 180)
				(length 6.35)
				(name "VCCINT")
				(number "M21")
			)
			(pin power_in line
				(at 25.4 111.76 180)
				(length 6.35)
				(name "VCCINT")
				(number "M23")
			)
			(pin power_in line
				(at 25.4 109.22 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 106.68 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 104.14 180)
				(length 6.35)
				(name "VCCINT")
				(number "N16")
			)
			(pin power_in line
				(at 25.4 101.6 180)
				(length 6.35)
				(name "VCCINT")
				(number "N18")
			)
			(pin power_in line
				(at 25.4 99.06 180)
				(length 6.35)
				(name "VCCINT")
				(number "N20")
			)
			(pin power_in line
				(at 25.4 96.52 180)
				(length 6.35)
				(name "VCCINT")
				(number "N22")
			)
			(pin power_in line
				(at 25.4 93.98 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 91.44 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "P15")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "P17")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "P19")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "P21")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "P23")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "R12")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "R16")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "R22")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "T13")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "T15")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "T21")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "T23")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "U14")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "U18")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "U22")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "V11")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "V13")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "V15")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "V21")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "V23")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "W10")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "W12")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "W14")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "W18")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "W22")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y11")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y13")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y21")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y23")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "VCCINT")
				(number "AA10")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "VCCINT")
				(number "AA12")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "VCCINT")
				(number "AA14")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "VCCINT")
				(number "AA22")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "VCCINT")
				(number "AB11")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "VCCINT")
				(number "AB13")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "VCCINT")
				(number "AB21")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "VCCINT")
				(number "AB23")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "VCCINT")
				(number "AC12")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "AC14")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "AC22")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "AD11")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "AD13")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "AD21")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "AD23")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "AE12")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "AE14")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "AE22")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "AF11")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "AF13")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "AF21")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "AF23")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "F13")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "F22")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "F32")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "G1")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "G10")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "G11")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "G12")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "G13")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "G19")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "G29")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "H11")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "H12")
			)
			(pin power_in line
				(at 25.4 -91.44 180)
				(length 6.35)
				(name "GND")
				(number "H14")
			)
			(pin power_in line
				(at 25.4 -93.98 180)
				(length 6.35)
				(name "GND")
				(number "H16")
			)
			(pin power_in line
				(at 25.4 -96.52 180)
				(length 6.35)
				(name "GND")
				(number "H26")
			)
			(pin power_in line
				(at 25.4 -99.06 180)
				(length 6.35)
				(name "GND")
				(number "J1")
			)
			(pin power_in line
				(at 25.4 -101.6 180)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at 25.4 -104.14 180)
				(length 6.35)
				(name "GND")
				(number "J5")
			)
			(pin power_in line
				(at 25.4 -106.68 180)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 -109.22 180)
				(length 6.35)
				(name "GND")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 -111.76 180)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at 25.4 -114.3 180)
				(length 6.35)
				(name "GND")
				(number "J13")
			)
			(pin power_in line
				(at 25.4 -116.84 180)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at 25.4 -119.38 180)
				(length 6.35)
				(name "GND")
				(number "J17")
			)
			(pin power_in line
				(at 25.4 -121.92 180)
				(length 6.35)
				(name "GND")
				(number "J19")
			)
			(pin power_in line
				(at 25.4 -124.46 180)
				(length 6.35)
				(name "GND")
				(number "J21")
			)
			(pin power_in line
				(at 25.4 -127 180)
				(length 6.35)
				(name "GND")
				(number "J23")
			)
			(pin power_in line
				(at 25.4 -129.54 180)
				(length 6.35)
				(name "GND")
				(number "J33")
			)
			(pin power_in line
				(at 25.4 -132.08 180)
				(length 6.35)
				(name "GND")
				(number "K3")
			)
			(pin power_in line
				(at 25.4 -134.62 180)
				(length 6.35)
				(name "GND")
				(number "K4")
			)
			(pin power_in line
				(at 25.4 -137.16 180)
				(length 6.35)
				(name "GND")
				(number "K7")
			)
			(pin power_in line
				(at 25.4 -139.7 180)
				(length 6.35)
				(name "GND")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 -142.24 180)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 -144.78 180)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 -147.32 180)
				(length 6.35)
				(name "GND")
				(number "K12")
			)
			(pin power_in line
				(at 25.4 -149.86 180)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 -152.4 180)
				(length 6.35)
				(name "GND")
				(number "K16")
			)
			(pin power_in line
				(at 25.4 -154.94 180)
				(length 6.35)
				(name "GND")
				(number "K18")
			)
			(pin power_in line
				(at 25.4 -157.48 180)
				(length 6.35)
				(name "GND")
				(number "K20")
			)
			(pin power_in line
				(at 25.4 -160.02 180)
				(length 6.35)
				(name "GND")
				(number "K22")
			)
			(pin power_in line
				(at 25.4 -162.56 180)
				(length 6.35)
				(name "GND")
				(number "K30")
			)
			(pin power_in line
				(at 25.4 -165.1 180)
				(length 6.35)
				(name "GND")
				(number "L1")
			)
			(pin power_in line
				(at 25.4 -167.64 180)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at 25.4 -170.18 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 -172.72 180)
				(length 6.35)
				(name "GND")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 -175.26 180)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
		)
		(symbol "XC7K480T-FFG1156_12_1"
			(pin power_in line
				(at -25.4 162.56 0)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at -25.4 160.02 0)
				(length 6.35)
				(name "GND")
				(number "L15")
			)
			(pin power_in line
				(at -25.4 157.48 0)
				(length 6.35)
				(name "GND")
				(number "L17")
			)
			(pin power_in line
				(at -25.4 154.94 0)
				(length 6.35)
				(name "GND")
				(number "L19")
			)
			(pin power_in line
				(at -25.4 152.4 0)
				(length 6.35)
				(name "GND")
				(number "L21")
			)
			(pin power_in line
				(at -25.4 149.86 0)
				(length 6.35)
				(name "GND")
				(number "L23")
			)
			(pin power_in line
				(at -25.4 147.32 0)
				(length 6.35)
				(name "GND")
				(number "L27")
			)
			(pin power_in line
				(at -25.4 144.78 0)
				(length 6.35)
				(name "GND")
				(number "M4")
			)
			(pin power_in line
				(at -25.4 142.24 0)
				(length 6.35)
				(name "GND")
				(number "M7")
			)
			(pin power_in line
				(at -25.4 139.7 0)
				(length 6.35)
				(name "GND")
				(number "M8")
			)
			(pin power_in line
				(at -25.4 137.16 0)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at -25.4 134.62 0)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at -25.4 132.08 0)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at -25.4 129.54 0)
				(length 6.35)
				(name "GND")
				(number "M16")
			)
			(pin power_in line
				(at -25.4 127 0)
				(length 6.35)
				(name "GND")
				(number "M18")
			)
			(pin power_in line
				(at -25.4 124.46 0)
				(length 6.35)
				(name "GND")
				(number "M20")
			)
			(pin power_in line
				(at -25.4 121.92 0)
				(length 6.35)
				(name "GND")
				(number "M22")
			)
			(pin power_in line
				(at -25.4 119.38 0)
				(length 6.35)
				(name "GND")
				(number "M24")
			)
			(pin power_in line
				(at -25.4 116.84 0)
				(length 6.35)
				(name "GND")
				(number "M34")
			)
			(pin power_in line
				(at -25.4 114.3 0)
				(length 6.35)
				(name "GND")
				(number "N1")
			)
			(pin power_in line
				(at -25.4 111.76 0)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at -25.4 109.22 0)
				(length 6.35)
				(name "GND")
				(number "N5")
			)
			(pin power_in line
				(at -25.4 106.68 0)
				(length 6.35)
				(name "GND")
				(number "N7")
			)
			(pin power_in line
				(at -25.4 104.14 0)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at -25.4 101.6 0)
				(length 6.35)
				(name "GND")
				(number "N10")
			)
			(pin power_in line
				(at -25.4 99.06 0)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at -25.4 96.52 0)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at -25.4 93.98 0)
				(length 6.35)
				(name "GND")
				(number "N15")
			)
			(pin power_in line
				(at -25.4 91.44 0)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "GND")
				(number "N19")
			)
			(pin power_in line
				(at -25.4 86.36 0)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "GND")
				(number "N23")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "GND")
				(number "N31")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "GND")
				(number "P3")
			)
			(pin power_in line
				(at -25.4 76.2 0)
				(length 6.35)
				(name "GND")
				(number "P4")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "GND")
				(number "P7")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "GND")
				(number "P8")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "GND")
				(number "P9")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "GND")
				(number "P16")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "GND")
				(number "P18")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "GND")
				(number "P20")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "GND")
				(number "P22")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "GND")
				(number "P28")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "GND")
				(number "R9")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "GND")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "R11")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "R13")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "R15")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "R17")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "R19")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "R21")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "R23")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "R25")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "T4")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "T7")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "T8")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "T11")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "T12")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "T14")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "T18")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "T20")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "T22")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "T32")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "U1")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "U5")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "U9")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "U10")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "U13")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "U15")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "U19")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "U23")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "U29")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "V3")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "V7")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "V8")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "V9")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "V12")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "V18")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "V20")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "V22")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "V26")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "W1")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "W5")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "W9")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "W11")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "W13")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "W15")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "W21")
			)
			(pin power_in line
				(at -25.4 -91.44 0)
				(length 6.35)
				(name "GND")
				(number "W23")
			)
			(pin power_in line
				(at -25.4 -93.98 0)
				(length 6.35)
				(name "GND")
				(number "W33")
			)
			(pin power_in line
				(at -25.4 -96.52 0)
				(length 6.35)
				(name "GND")
				(number "Y4")
			)
			(pin power_in line
				(at -25.4 -99.06 0)
				(length 6.35)
				(name "GND")
				(number "Y7")
			)
			(pin power_in line
				(at -25.4 -101.6 0)
				(length 6.35)
				(name "GND")
				(number "Y8")
			)
			(pin power_in line
				(at -25.4 -104.14 0)
				(length 6.35)
				(name "GND")
				(number "Y9")
			)
			(pin power_in line
				(at -25.4 -106.68 0)
				(length 6.35)
				(name "GND")
				(number "Y10")
			)
			(pin power_in line
				(at -25.4 -109.22 0)
				(length 6.35)
				(name "GND")
				(number "Y12")
			)
			(pin power_in line
				(at -25.4 -111.76 0)
				(length 6.35)
				(name "GND")
				(number "Y14")
			)
			(pin power_in line
				(at -25.4 -114.3 0)
				(length 6.35)
				(name "GND")
				(number "Y16")
			)
			(pin power_in line
				(at -25.4 -116.84 0)
				(length 6.35)
				(name "GND")
				(number "Y18")
			)
			(pin power_in line
				(at -25.4 -119.38 0)
				(length 6.35)
				(name "GND")
				(number "Y20")
			)
			(pin power_in line
				(at -25.4 -121.92 0)
				(length 6.35)
				(name "GND")
				(number "Y22")
			)
			(pin power_in line
				(at -25.4 -124.46 0)
				(length 6.35)
				(name "GND")
				(number "Y30")
			)
			(pin power_in line
				(at -25.4 -127 0)
				(length 6.35)
				(name "GND")
				(number "AA1")
			)
			(pin power_in line
				(at -25.4 -129.54 0)
				(length 6.35)
				(name "GND")
				(number "AA2")
			)
			(pin power_in line
				(at -25.4 -132.08 0)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at -25.4 -134.62 0)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at -25.4 -137.16 0)
				(length 6.35)
				(name "GND")
				(number "AA11")
			)
			(pin power_in line
				(at -25.4 -139.7 0)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at -25.4 -142.24 0)
				(length 6.35)
				(name "GND")
				(number "AA15")
			)
			(pin power_in line
				(at -25.4 -144.78 0)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at -25.4 -147.32 0)
				(length 6.35)
				(name "GND")
				(number "AA19")
			)
			(pin power_in line
				(at -25.4 -149.86 0)
				(length 6.35)
				(name "GND")
				(number "AA21")
			)
			(pin power_in line
				(at -25.4 -152.4 0)
				(length 6.35)
				(name "GND")
				(number "AA23")
			)
			(pin power_in line
				(at -25.4 -154.94 0)
				(length 6.35)
				(name "GND")
				(number "AA27")
			)
			(pin power_in line
				(at -25.4 -157.48 0)
				(length 6.35)
				(name "GND")
				(number "AB3")
			)
			(pin power_in line
				(at -25.4 -160.02 0)
				(length 6.35)
				(name "GND")
				(number "AB4")
			)
			(pin power_in line
				(at -25.4 -162.56 0)
				(length 6.35)
				(name "GND")
				(number "AB7")
			)
			(pin power_in line
				(at 25.4 162.56 180)
				(length 6.35)
				(name "GND")
				(number "AB8")
			)
			(pin power_in line
				(at 25.4 160.02 180)
				(length 6.35)
				(name "GND")
				(number "AB9")
			)
			(pin power_in line
				(at 25.4 157.48 180)
				(length 6.35)
				(name "GND")
				(number "AB10")
			)
			(pin power_in line
				(at 25.4 154.94 180)
				(length 6.35)
				(name "GND")
				(number "AB12")
			)
			(pin power_in line
				(at 25.4 152.4 180)
				(length 6.35)
				(name "GND")
				(number "AB14")
			)
			(pin power_in line
				(at 25.4 149.86 180)
				(length 6.35)
				(name "GND")
				(number "AB16")
			)
			(pin power_in line
				(at 25.4 147.32 180)
				(length 6.35)
				(name "GND")
				(number "AB18")
			)
			(pin power_in line
				(at 25.4 144.78 180)
				(length 6.35)
				(name "GND")
				(number "AB20")
			)
			(pin power_in line
				(at 25.4 142.24 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
			(pin power_in line
				(at 25.4 139.7 180)
				(length 6.35)
				(name "GND")
				(number "AB24")
			)
			(pin power_in line
				(at 25.4 137.16 180)
				(length 6.35)
				(name "GND")
				(number "AB34")
			)
			(pin power_in line
				(at 25.4 134.62 180)
				(length 6.35)
				(name "GND")
				(number "AC1")
			)
			(pin power_in line
				(at 25.4 132.08 180)
				(length 6.35)
				(name "GND")
				(number "AC5")
			)
			(pin power_in line
				(at 25.4 129.54 180)
				(length 6.35)
				(name "GND")
				(number "AC9")
			)
			(pin power_in line
				(at 25.4 127 180)
				(length 6.35)
				(name "GND")
				(number "AC10")
			)
			(pin power_in line
				(at 25.4 124.46 180)
				(length 6.35)
				(name "GND")
				(number "AC11")
			)
			(pin power_in line
				(at 25.4 121.92 180)
				(length 6.35)
				(name "GND")
				(number "AC13")
			)
			(pin power_in line
				(at 25.4 119.38 180)
				(length 6.35)
				(name "GND")
				(number "AC15")
			)
			(pin power_in line
				(at 25.4 116.84 180)
				(length 6.35)
				(name "GND")
				(number "AC17")
			)
			(pin power_in line
				(at 25.4 114.3 180)
				(length 6.35)
				(name "GND")
				(number "AC19")
			)
			(pin power_in line
				(at 25.4 111.76 180)
				(length 6.35)
				(name "GND")
				(number "AC21")
			)
			(pin power_in line
				(at 25.4 109.22 180)
				(length 6.35)
				(name "GND")
				(number "AC23")
			)
			(pin power_in line
				(at 25.4 106.68 180)
				(length 6.35)
				(name "GND")
				(number "AC31")
			)
			(pin power_in line
				(at 25.4 104.14 180)
				(length 6.35)
				(name "GND")
				(number "AD4")
			)
			(pin power_in line
				(at 25.4 101.6 180)
				(length 6.35)
				(name "GND")
				(number "AD7")
			)
			(pin power_in line
				(at 25.4 99.06 180)
				(length 6.35)
				(name "GND")
				(number "AD8")
			)
			(pin power_in line
				(at 25.4 96.52 180)
				(length 6.35)
				(name "GND")
				(number "AD10")
			)
			(pin power_in line
				(at 25.4 93.98 180)
				(length 6.35)
				(name "GND")
				(number "AD12")
			)
			(pin power_in line
				(at 25.4 91.44 180)
				(length 6.35)
				(name "GND")
				(number "AD14")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "GND")
				(number "AD16")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "GND")
				(number "AD18")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "GND")
				(number "AD20")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "GND")
				(number "AD22")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "GND")
				(number "AD28")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "GND")
				(number "AE1")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "GND")
				(number "AE2")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "GND")
				(number "AE5")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "GND")
				(number "AE7")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "GND")
				(number "AE9")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "GND")
				(number "AE10")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "GND")
				(number "AE11")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "GND")
				(number "AE13")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "GND")
				(number "AE15")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "GND")
				(number "AE17")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "GND")
				(number "AE19")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "GND")
				(number "AE21")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "GND")
				(number "AE23")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "GND")
				(number "AE25")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "GND")
				(number "AF3")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "GND")
				(number "AF4")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "AF7")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "AF8")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "AF9")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "AF10")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "AF12")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "AF14")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "AF16")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "AF18")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "AF20")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "AF22")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "AF32")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "AG1")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "AG5")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "AG9")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "AG10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "AG11")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "AG12")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "AG13")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "AG19")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "AG29")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "AH4")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "AH7")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "AH8")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "AH11")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "AH12")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "AH13")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "AH16")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "AH26")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "AJ1")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "AJ2")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "AJ5")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "AJ10")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "AJ13")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "AJ23")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AJ33")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AK3")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AK4")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AK7")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AK8")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AK11")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AK13")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AK14")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AK20")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AK30")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "AL1")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "AL5")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "AL10")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "AL13")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "AL14")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "AL17")
			)
			(pin power_in line
				(at 25.4 -91.44 180)
				(length 6.35)
				(name "GND")
				(number "AL27")
			)
			(pin power_in line
				(at 25.4 -93.98 180)
				(length 6.35)
				(name "GND")
				(number "AM4")
			)
			(pin power_in line
				(at 25.4 -96.52 180)
				(length 6.35)
				(name "GND")
				(number "AM7")
			)
			(pin power_in line
				(at 25.4 -99.06 180)
				(length 6.35)
				(name "GND")
				(number "AM8")
			)
			(pin power_in line
				(at 25.4 -101.6 180)
				(length 6.35)
				(name "GND")
				(number "AM11")
			)
			(pin power_in line
				(at 25.4 -104.14 180)
				(length 6.35)
				(name "GND")
				(number "AM13")
			)
			(pin power_in line
				(at 25.4 -106.68 180)
				(length 6.35)
				(name "GND")
				(number "AM14")
			)
			(pin power_in line
				(at 25.4 -109.22 180)
				(length 6.35)
				(name "GND")
				(number "AM24")
			)
			(pin power_in line
				(at 25.4 -111.76 180)
				(length 6.35)
				(name "GND")
				(number "AM34")
			)
			(pin power_in line
				(at 25.4 -114.3 180)
				(length 6.35)
				(name "GND")
				(number "AN1")
			)
			(pin power_in line
				(at 25.4 -116.84 180)
				(length 6.35)
				(name "GND")
				(number "AN2")
			)
			(pin power_in line
				(at 25.4 -119.38 180)
				(length 6.35)
				(name "GND")
				(number "AN5")
			)
			(pin power_in line
				(at 25.4 -121.92 180)
				(length 6.35)
				(name "GND")
				(number "AN10")
			)
			(pin power_in line
				(at 25.4 -124.46 180)
				(length 6.35)
				(name "GND")
				(number "AN13")
			)
			(pin power_in line
				(at 25.4 -127 180)
				(length 6.35)
				(name "GND")
				(number "AN14")
			)
			(pin power_in line
				(at 25.4 -129.54 180)
				(length 6.35)
				(name "GND")
				(number "AN15")
			)
			(pin power_in line
				(at 25.4 -132.08 180)
				(length 6.35)
				(name "GND")
				(number "AN21")
			)
			(pin power_in line
				(at 25.4 -134.62 180)
				(length 6.35)
				(name "GND")
				(number "AN31")
			)
			(pin power_in line
				(at 25.4 -137.16 180)
				(length 6.35)
				(name "GND")
				(number "AP3")
			)
			(pin power_in line
				(at 25.4 -139.7 180)
				(length 6.35)
				(name "GND")
				(number "AP4")
			)
			(pin power_in line
				(at 25.4 -142.24 180)
				(length 6.35)
				(name "GND")
				(number "AP7")
			)
			(pin power_in line
				(at 25.4 -144.78 180)
				(length 6.35)
				(name "GND")
				(number "AP8")
			)
			(pin power_in line
				(at 25.4 -147.32 180)
				(length 6.35)
				(name "GND")
				(number "AP11")
			)
			(pin power_in line
				(at 25.4 -149.86 180)
				(length 6.35)
				(name "GND")
				(number "AP13")
			)
			(pin power_in line
				(at 25.4 -152.4 180)
				(length 6.35)
				(name "GND")
				(number "AP14")
			)
			(pin power_in line
				(at 25.4 -154.94 180)
				(length 6.35)
				(name "GND")
				(number "AP15")
			)
			(pin power_in line
				(at 25.4 -157.48 180)
				(length 6.35)
				(name "GND")
				(number "AP18")
			)
			(pin power_in line
				(at 25.4 -160.02 180)
				(length 6.35)
				(name "GND")
				(number "AP28")
			)
			(pin power_in line
				(at 25.4 -162.56 180)
				(length 6.35)
				(name "GND")
				(number "AP34")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC7K480T-FFG901"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC7K480T-FFG901"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Kintex 7 T 480 XC7K480T-FFG901"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC7K480T-FFG901_1_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_11")
				(number "AC19")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_11")
				(number "AG19")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_11")
				(number "AH20")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_11")
				(number "AH19")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_11")
				(number "AJ19")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_11")
				(number "AK19")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_11")
				(number "AK20")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_11")
				(number "AJ18")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_11")
				(number "AK18")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_11")
				(number "AJ16")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_11")
				(number "AJ17")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_11")
				(number "AF18")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_11")
				(number "AG18")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_11")
				(number "AK15")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_11")
				(number "AK16")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_11")
				(number "AH14")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_11")
				(number "AH15")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_11")
				(number "AG14")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_11")
				(number "AG15")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_11")
				(number "AJ14")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_11")
				(number "AK14")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_11")
				(number "AH16")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_11")
				(number "AH17")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_11")
				(number "AF17")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_11")
				(number "AG17")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_11")
				(number "AF15")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_11")
				(number "AF16")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_11")
				(number "AE15")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_11")
				(number "AE16")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_11")
				(number "AC16")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_11")
				(number "AD16")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_11")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_11")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_11")
				(number "AC14")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_11")
				(number "AC15")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_11")
				(number "AD14")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_11")
				(number "AE14")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_11")
				(number "AE18")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_11")
				(number "AE19")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_11")
				(number "AD18")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_11")
				(number "AD19")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_11")
				(number "AC17")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_11")
				(number "AD17")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_11")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_11")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_11")
				(number "AA17")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_11")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_11")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_11")
				(number "Y19")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_11")
				(number "AB19")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AA19")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AB16")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AE17")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AF14")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AH18")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_11")
				(number "AJ15")
			)
			(pin power_in line
				(at 25.4 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AC23")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AD20")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AF24")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AG21")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AJ25")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AK22")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_12")
				(number "Y23")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_12")
				(number "Y20")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_12")
				(number "Y21")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_12")
				(number "AA20")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_12")
				(number "AA21")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_12")
				(number "AA22")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_12")
				(number "AA23")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_12")
				(number "AB20")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_12")
				(number "AC20")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_12")
				(number "AB22")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_12")
				(number "AB23")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_12")
				(number "AC21")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_12")
				(number "AC22")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_12")
				(number "AD26")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_12")
				(number "AE26")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_12")
				(number "AH25")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_12")
				(number "AH26")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_12")
				(number "AE25")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_12")
				(number "AF26")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_12")
				(number "AD24")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_12")
				(number "AE24")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_12")
				(number "AF25")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_12")
				(number "AG25")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_12")
				(number "AG24")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_12")
				(number "AH24")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_12")
				(number "AG22")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_12")
				(number "AG23")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_12")
				(number "AF22")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_12")
				(number "AF23")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_12")
				(number "AD23")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_12")
				(number "AE23")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_12")
				(number "AD21")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_12")
				(number "AD22")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_12")
				(number "AE21")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_12")
				(number "AF21")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_12")
				(number "AF20")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_12")
				(number "AG20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_12")
				(number "AH21")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_12")
				(number "AH22")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_12")
				(number "AJ21")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_12")
				(number "AK21")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_12")
				(number "AJ22")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_12")
				(number "AK23")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_12")
				(number "AJ23")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_12")
				(number "AJ24")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_12")
				(number "AK24")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_12")
				(number "AK25")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_12")
				(number "AJ26")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_12")
				(number "AK26")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_12")
				(number "AE20")
			)
		)
		(symbol "XC7K480T-FFG901_2_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_13")
				(number "W24")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_13")
				(number "AA28")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_13")
				(number "AB28")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_13")
				(number "AB29")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_13")
				(number "AB30")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_13")
				(number "Y30")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_13")
				(number "AA30")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_13")
				(number "Y28")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_13")
				(number "Y29")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_13")
				(number "W28")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_13")
				(number "W29")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_13")
				(number "W26")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_13")
				(number "W27")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_13")
				(number "AC26")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_13")
				(number "AD27")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_13")
				(number "Y25")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_13")
				(number "AA25")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_13")
				(number "AB25")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_13")
				(number "AC25")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_13")
				(number "AB24")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_13")
				(number "AC24")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_13")
				(number "Y26")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_13")
				(number "AA26")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_13")
				(number "AA27")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_13")
				(number "AB27")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_13")
				(number "AC27")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_13")
				(number "AD28")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_13")
				(number "AE28")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_13")
				(number "AF28")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_13")
				(number "AC29")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_13")
				(number "AC30")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_13")
				(number "AD29")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_13")
				(number "AE29")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_13")
				(number "AE30")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_13")
				(number "AF30")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_13")
				(number "AF27")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_13")
				(number "AG28")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_13")
				(number "AG27")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_13")
				(number "AH27")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_13")
				(number "AG29")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_13")
				(number "AH29")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_13")
				(number "AJ27")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_13")
				(number "AJ28")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_13")
				(number "AG30")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_13")
				(number "AH30")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_13")
				(number "AJ29")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_13")
				(number "AK30")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_13")
				(number "AK28")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_13")
				(number "AK29")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_13")
				(number "Y24")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AA29")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AB26")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AD30")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AE27")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AH28")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "W25")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "R17")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "R27")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "T24")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "U21")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "V18")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "V28")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_14")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_D00_MOSI_14")
				(number "R30")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_D01_DIN_14")
				(number "T30")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_D02_14")
				(number "R28")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_D03_14")
				(number "T28")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_PUDC_B_14")
				(number "V29")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_EMCCLK_14")
				(number "V30")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_D04_14")
				(number "U29")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_D05_14")
				(number "U30")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_D06_14")
				(number "U27")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_D07_14")
				(number "U28")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_FCS_B_14")
				(number "V26")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_D08_VREF_14")
				(number "V27")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_D09_14")
				(number "R24")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_D10_14")
				(number "R25")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_D11_14")
				(number "R23")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_D12_14")
				(number "T23")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_14")
				(number "V24")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_D13_14")
				(number "V25")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_D14_14")
				(number "R26")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_D15_14")
				(number "T27")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_14")
				(number "T25")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_14")
				(number "T26")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_14")
				(number "U24")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_14")
				(number "U25")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_14")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_14")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_14")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_14")
				(number "U23")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_RDWR_B_14")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_DOUT_CSO_B_14")
				(number "R21")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_CSI_B_14")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_A15_D31_14")
				(number "T21")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_A14_D30_14")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_A13_D29_14")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_A12_D28_14")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_A11_D27_14")
				(number "W23")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_A10_D26_14")
				(number "R18")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_A09_D25_VREF_14")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_A08_D24_14")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_A07_D23_14")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_14")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A06_D22_14")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_A05_D21_14")
				(number "U17")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_A04_D20_14")
				(number "U18")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_A03_D19_14")
				(number "V17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_A02_D18_14")
				(number "W17")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_A01_D17_14")
				(number "W18")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_A00_D16_14")
				(number "W19")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_14")
				(number "W21")
			)
		)
		(symbol "XC7K480T-FFG901_3_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_15")
				(number "L22")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_AD0P_15")
				(number "K28")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_AD0N_15")
				(number "K29")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_AD8P_15")
				(number "L30")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_AD8N_15")
				(number "K30")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_AD1P_15")
				(number "N30")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_AD1N_15")
				(number "M30")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_AD9P_15")
				(number "N29")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_AD9N_15")
				(number "M29")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_AD2P_15")
				(number "R29")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_AD2N_15")
				(number "P29")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_15")
				(number "M28")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_15")
				(number "L28")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_AD10P_15")
				(number "K25")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_AD10N_15")
				(number "K26")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_AD3P_15")
				(number "P26")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_AD3N_15")
				(number "N26")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_AD11P_15")
				(number "N27")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_AD11N_15")
				(number "M27")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_AD4P_15")
				(number "P27")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_AD4N_15")
				(number "P28")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_AD12P_15")
				(number "M25")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_AD12N_15")
				(number "L25")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_AD5P_15")
				(number "L26")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_AD5N_15")
				(number "L27")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_15")
				(number "M23")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_15")
				(number "M24")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_15")
				(number "N24")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_15")
				(number "N25")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_15")
				(number "L23")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_ADV_B_15")
				(number "K24")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_A28_15")
				(number "N22")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_A27_15")
				(number "M22")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_A26_15")
				(number "P23")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_A25_15")
				(number "P24")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_A24_15")
				(number "L20")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_A23_15")
				(number "L21")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_A22_15")
				(number "N20")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_A21_VREF_15")
				(number "M20")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_A20_15")
				(number "P21")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_A19_15")
				(number "N21")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_15")
				(number "M18")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A18_15")
				(number "M19")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_A17_15")
				(number "P19")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_A16_15")
				(number "N19")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_FOE_B_15")
				(number "N17")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_FWE_B_15")
				(number "M17")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_RS1_15")
				(number "P17")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_RS0_15")
				(number "P18")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_15")
				(number "P22")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "L19")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "L29")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "M26")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "N23")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "P20")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "P30")
			)
			(pin power_in line
				(at 25.4 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "A29")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "B26")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "D30")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "E27")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "F24")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "H28")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "J25")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_16")
				(number "E24")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_16")
				(number "D24")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_16")
				(number "C24")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_16")
				(number "B24")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_16")
				(number "B25")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_16")
				(number "C25")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_16")
				(number "C26")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_16")
				(number "A25")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_16")
				(number "A26")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_16")
				(number "C27")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_16")
				(number "B27")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_16")
				(number "D26")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_16")
				(number "D27")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_16")
				(number "H24")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_16")
				(number "G24")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_16")
				(number "H25")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_16")
				(number "G25")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_16")
				(number "J26")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_16")
				(number "J27")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_16")
				(number "H26")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_16")
				(number "H27")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_16")
				(number "F25")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_16")
				(number "F26")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_16")
				(number "E25")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_16")
				(number "E26")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_16")
				(number "G27")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_16")
				(number "F27")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_16")
				(number "G28")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_16")
				(number "F28")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_16")
				(number "H29")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_16")
				(number "G29")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_16")
				(number "F30")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_16")
				(number "E30")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_16")
				(number "H30")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_16")
				(number "G30")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_16")
				(number "J28")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_16")
				(number "J29")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_16")
				(number "E28")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_16")
				(number "D28")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_16")
				(number "E29")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_16")
				(number "D29")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_16")
				(number "C29")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_16")
				(number "C30")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_16")
				(number "B28")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_16")
				(number "B29")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_16")
				(number "B30")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_16")
				(number "A30")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_16")
				(number "A27")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_16")
				(number "A28")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_16")
				(number "J24")
			)
		)
		(symbol "XC7K480T-FFG901_4_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_17")
				(number "H21")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_17")
				(number "K23")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_17")
				(number "J23")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_17")
				(number "J22")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_17")
				(number "H22")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_17")
				(number "K21")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_17")
				(number "J21")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_17")
				(number "K19")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_17")
				(number "K20")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_17")
				(number "J18")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_17")
				(number "J19")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_17")
				(number "L18")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_17")
				(number "K18")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_17")
				(number "G23")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_17")
				(number "F23")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_17")
				(number "H20")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_17")
				(number "G20")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_17")
				(number "H19")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_17")
				(number "G19")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_17")
				(number "G18")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_17")
				(number "F18")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_17")
				(number "G22")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_17")
				(number "F22")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_17")
				(number "F20")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_17")
				(number "F21")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_17")
				(number "E20")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_17")
				(number "E21")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_17")
				(number "D21")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_17")
				(number "D22")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_17")
				(number "E23")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_17")
				(number "D23")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_17")
				(number "C21")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_17")
				(number "C22")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_17")
				(number "E18")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_17")
				(number "E19")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_17")
				(number "D18")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_17")
				(number "D19")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_17")
				(number "C19")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_17")
				(number "C20")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_17")
				(number "B19")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_17")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_17")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_17")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_17")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_17")
				(number "A21")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_17")
				(number "B22")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_17")
				(number "B23")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_17")
				(number "A22")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_17")
				(number "A23")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_17")
				(number "L17")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "A19")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "C23")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "D20")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "G21")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "H18")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_17")
				(number "K22")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "B16")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "E17")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "F14")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_18")
				(number "J15")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L6P_T0_18")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_18")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L7P_T1_18")
				(number "J14")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L7N_T1_18")
				(number "H15")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L8P_T1_18")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L8N_T1_18")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_18")
				(number "H14")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_18")
				(number "G14")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L10P_T1_18")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L10N_T1_18")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_18")
				(number "F16")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_18")
				(number "E16")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_18")
				(number "G15")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_18")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_18")
				(number "C15")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_18")
				(number "C16")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_18")
				(number "E15")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_18")
				(number "D16")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_18")
				(number "E14")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_18")
				(number "D14")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L16P_T2_18")
				(number "C14")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L16N_T2_18")
				(number "B15")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L17P_T2_18")
				(number "B14")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L17N_T2_18")
				(number "A14")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L18P_T2_18")
				(number "A15")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L18N_T2_18")
				(number "A16")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L19P_T3_18")
				(number "D17")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_18")
				(number "C17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L20P_T3_18")
				(number "B17")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L20N_T3_18")
				(number "A17")
			)
		)
		(symbol "XC7K480T-FFG901_5_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_111")
				(number "AJ12")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_111")
				(number "AJ11")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_111")
				(number "AK10")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_111")
				(number "AK9")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_111")
				(number "AJ8")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_111")
				(number "AJ7")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_111")
				(number "AG8")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_111")
				(number "AG7")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_111")
				(number "AH10")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_111")
				(number "AH9")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_111")
				(number "AG12")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_111")
				(number "AG11")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_111")
				(number "AF10")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_111")
				(number "AF9")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_111")
				(number "AE12")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_111")
				(number "AE11")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_111")
				(number "AC8")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_111")
				(number "AC7")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_111")
				(number "AE8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_111")
				(number "AE7")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_112")
				(number "AK6")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_112")
				(number "AK5")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_112")
				(number "AJ4")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_112")
				(number "AJ3")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_112")
				(number "AK2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_112")
				(number "AK1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_112")
				(number "AH2")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_112")
				(number "AH1")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_112")
				(number "AH6")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_112")
				(number "AH5")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_112")
				(number "AG4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_112")
				(number "AG3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_112")
				(number "AE4")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_112")
				(number "AE3")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_112")
				(number "AC4")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_112")
				(number "AC3")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_112")
				(number "AD6")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_112")
				(number "AD5")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_112")
				(number "AF6")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_112")
				(number "AF5")
			)
		)
		(symbol "XC7K480T-FFG901_6_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_113")
				(number "AF2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_113")
				(number "AF1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_113")
				(number "AD2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_113")
				(number "AD1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_113")
				(number "AB2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_113")
				(number "AB1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_113")
				(number "Y2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_113")
				(number "Y1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_113")
				(number "AB6")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_113")
				(number "AB5")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_113")
				(number "AA4")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_113")
				(number "AA3")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_113")
				(number "Y6")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_113")
				(number "Y5")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_113")
				(number "W4")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_113")
				(number "W3")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_113")
				(number "U8")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_113")
				(number "U7")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_113")
				(number "W8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_113")
				(number "W7")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_114")
				(number "V2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_114")
				(number "V1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_114")
				(number "T2")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_114")
				(number "T1")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_114")
				(number "P2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_114")
				(number "P1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_114")
				(number "N4")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_114")
				(number "N3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_114")
				(number "V6")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_114")
				(number "V5")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_114")
				(number "U4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_114")
				(number "U3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_114")
				(number "R4")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_114")
				(number "R3")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_114")
				(number "P6")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_114")
				(number "P5")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_114")
				(number "R8")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_114")
				(number "R7")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_114")
				(number "T6")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_114")
				(number "T5")
			)
		)
		(symbol "XC7K480T-FFG901_7_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_115")
				(number "M2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_115")
				(number "M1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_115")
				(number "K2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_115")
				(number "K1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_115")
				(number "H2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_115")
				(number "H1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_115")
				(number "F2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_115")
				(number "F1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_115")
				(number "M6")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_115")
				(number "M5")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_115")
				(number "L4")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_115")
				(number "L3")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_115")
				(number "K6")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_115")
				(number "K5")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_115")
				(number "J4")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_115")
				(number "J3")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_115")
				(number "J8")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_115")
				(number "J7")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_115")
				(number "L8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_115")
				(number "L7")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_116")
				(number "D2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_116")
				(number "D1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_116")
				(number "B2")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_116")
				(number "B1")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_116")
				(number "A4")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_116")
				(number "A3")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_116")
				(number "B6")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_116")
				(number "B5")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_116")
				(number "G4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_116")
				(number "G3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_116")
				(number "E4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_116")
				(number "E3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_116")
				(number "D6")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_116")
				(number "D5")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_116")
				(number "C4")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_116")
				(number "C3")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_116")
				(number "F6")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_116")
				(number "F5")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_116")
				(number "H6")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_116")
				(number "H5")
			)
		)
		(symbol "XC7K480T-FFG901_8_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_117")
				(number "C8")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_117")
				(number "C7")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_117")
				(number "A8")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_117")
				(number "A7")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_117")
				(number "B10")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_117")
				(number "B9")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_117")
				(number "A12")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_117")
				(number "A11")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_117")
				(number "F10")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_117")
				(number "F9")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_117")
				(number "D10")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_117")
				(number "D9")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_117")
				(number "E12")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_117")
				(number "E11")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_117")
				(number "C12")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_117")
				(number "C11")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_117")
				(number "E8")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_117")
				(number "E7")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_117")
				(number "G8")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_117")
				(number "G7")
			)
		)
		(symbol "XC7K480T-FFG901_9_1"
			(pin power_in line
				(at -38.1 33.02 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AA6")
			)
			(pin power_in line
				(at -38.1 30.48 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AC6")
			)
			(pin power_in line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AE6")
			)
			(pin power_in line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AG6")
			)
			(pin power_in line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AH7")
			)
			(pin power_in line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AH11")
			)
			(pin power_in line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "AK11")
			)
			(pin power_in line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "N6")
			)
			(pin power_in line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "R6")
			)
			(pin power_in line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "U6")
			)
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCC_G10")
				(number "W6")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTVCCAUX_G10")
				(number "AA8")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTVCCAUX_G10")
				(number "Y7")
			)
			(pin power_in line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "B11")
			)
			(pin power_in line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "D7")
			)
			(pin power_in line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "D11")
			)
			(pin power_in line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "E6")
			)
			(pin power_in line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "G6")
			)
			(pin power_in line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "J6")
			)
			(pin power_in line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTAVCC_G11")
				(number "L6")
			)
			(pin power_in line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTVCCAUX_G11")
				(number "K8")
			)
			(pin power_in line
				(at 38.1 33.02 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AB3")
			)
			(pin power_in line
				(at 38.1 30.48 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AC2")
			)
			(pin power_in line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AF3")
			)
			(pin power_in line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AG2")
			)
			(pin power_in line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AG9")
			)
			(pin power_in line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AJ6")
			)
			(pin power_in line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AJ9")
			)
			(pin power_in line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AK3")
			)
			(pin power_in line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "AK7")
			)
			(pin power_in line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "P3")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "R2")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "V3")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTT_G10")
				(number "W2")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "B3")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "B7")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "C2")
			)
			(pin power_in line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "C6")
			)
			(pin power_in line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "C9")
			)
			(pin power_in line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "E9")
			)
			(pin power_in line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "F3")
			)
			(pin power_in line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "G2")
			)
			(pin power_in line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "K3")
			)
			(pin power_in line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTAVTT_G11")
				(number "L2")
			)
			(pin power_in line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "MGTAVTTRCAL_115")
				(number "N8")
			)
			(pin power_in line
				(at 38.1 -33.02 180)
				(length 6.35)
				(name "MGTRREF_115")
				(number "N7")
			)
		)
		(symbol "XC7K480T-FFG901_10_1"
			(pin power_in line
				(at 25.4 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "J10")
			)
			(pin power_in line
				(at 27.94 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "K11")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "TDI_0")
				(number "H11")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "TDO_0")
				(number "J13")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "TMS_0")
				(number "J11")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TCK_0")
				(number "H12")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "CCLK_0")
				(number "H13")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "M0_0")
				(number "AC13")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "M1_0")
				(number "AC12")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "M2_0")
				(number "AB12")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "DONE_0")
				(number "AC10")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "INIT_B_0")
				(number "H10")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "PROGRAM_B_0")
				(number "AB11")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "CFGBVS_0")
				(number "AC11")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "VP_0")
				(number "R13")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "VN_0")
				(number "T12")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 6.35)
				(name "VREFP_0")
				(number "T13")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "VREFN_0")
				(number "R12")
			)
			(pin bidirectional line
				(at 38.1 -35.56 180)
				(length 6.35)
				(name "DXP_0")
				(number "U13")
			)
			(pin bidirectional line
				(at 38.1 -38.1 180)
				(length 6.35)
				(name "DXN_0")
				(number "U12")
			)
		)
		(symbol "XC7K480T-FFG901_11_1"
			(pin power_in line
				(at -25.4 99.06 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M16")
			)
			(pin power_in line
				(at -25.4 96.52 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P16")
			)
			(pin power_in line
				(at -25.4 93.98 0)
				(length 6.35)
				(name "VCCAUX")
				(number "T16")
			)
			(pin power_in line
				(at -25.4 91.44 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V16")
			)
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "VCCAUX")
				(number "Y16")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "GNDADC_0")
				(number "P12")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "VCCADC_0")
				(number "P13")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "VCCBATT_0")
				(number "G13")
			)
			(pin power_in line
				(at -25.4 76.2 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "AA15")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "R15")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "U15")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "W15")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "A2")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "A5")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "A6")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "A10")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A13")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A24")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "B4")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B8")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B12")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B21")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C1")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "C5")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "C10")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "C13")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "C18")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "C28")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "D3")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "D8")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "D12")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "D13")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "D15")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "D25")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "E1")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "E10")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "E13")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "E22")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "F8")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "F12")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "F13")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "F19")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "F29")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "G1")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "G9")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "G10")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "G11")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 -91.44 0)
				(length 6.35)
				(name "GND")
				(number "G16")
			)
			(pin power_in line
				(at -25.4 -93.98 0)
				(length 6.35)
				(name "GND")
				(number "G26")
			)
			(pin power_in line
				(at -25.4 -96.52 0)
				(length 6.35)
				(name "GND")
				(number "H3")
			)
			(pin power_in line
				(at -25.4 -99.06 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at 25.4 99.06 180)
				(length 6.35)
				(name "VCCINT")
				(number "K12")
			)
			(pin power_in line
				(at 25.4 96.52 180)
				(length 6.35)
				(name "VCCINT")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 93.98 180)
				(length 6.35)
				(name "VCCINT")
				(number "K16")
			)
			(pin power_in line
				(at 25.4 91.44 180)
				(length 6.35)
				(name "VCCINT")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "L13")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "L15")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "R11")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "T10")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "T14")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "U11")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "V10")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "V12")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "W11")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "W13")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y10")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y12")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y14")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "AA11")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "H9")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "H23")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "J1")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "J5")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "J20")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "J30")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "K4")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "K7")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "K15")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "K17")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "K27")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "L1")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "L16")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "L24")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "M3")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "M4")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "M7")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "M8")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "M21")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "N1")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "N5")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "N16")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "N18")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "N28")
			)
			(pin power_in line
				(at 25.4 -91.44 180)
				(length 6.35)
				(name "GND")
				(number "P4")
			)
			(pin power_in line
				(at 25.4 -93.98 180)
				(length 6.35)
				(name "GND")
				(number "P7")
			)
			(pin power_in line
				(at 25.4 -96.52 180)
				(length 6.35)
				(name "GND")
				(number "P8")
			)
			(pin power_in line
				(at 25.4 -99.06 180)
				(length 6.35)
				(name "GND")
				(number "P9")
			)
		)
		(symbol "XC7K480T-FFG901_12_1"
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "GND")
				(number "P11")
			)
			(pin power_in line
				(at -25.4 76.2 0)
				(length 6.35)
				(name "GND")
				(number "P15")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "GND")
				(number "P25")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "GND")
				(number "R9")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "GND")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "GND")
				(number "R14")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "GND")
				(number "R16")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "GND")
				(number "R22")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "GND")
				(number "T3")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "GND")
				(number "T4")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "GND")
				(number "T7")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "GND")
				(number "T8")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "GND")
				(number "T9")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "GND")
				(number "T11")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "GND")
				(number "T15")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "T19")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "T29")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "U1")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "U5")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "U9")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "U10")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "U14")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "U16")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "U26")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "V7")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "V8")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "V9")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "V11")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "V13")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "V15")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "V23")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "W1")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "W5")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "W9")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "W10")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "W12")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "W14")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "W16")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "W20")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "W30")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "Y3")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "Y4")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "Y8")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "Y9")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "Y11")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "Y13")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "Y15")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "Y17")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "Y27")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "AA1")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "AA2")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "AA7")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "AA10")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "AA12")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "AA14")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "AA16")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "AA24")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "GND")
				(number "AB4")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "GND")
				(number "AB7")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "GND")
				(number "AB8")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "GND")
				(number "AB9")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "GND")
				(number "AB10")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "GND")
				(number "AB13")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "GND")
				(number "AB21")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "GND")
				(number "AC1")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "GND")
				(number "AC5")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "GND")
				(number "AC9")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "GND")
				(number "AC18")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "GND")
				(number "AC28")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "GND")
				(number "AD3")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "GND")
				(number "AD4")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "GND")
				(number "AD7")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "GND")
				(number "AD8")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "GND")
				(number "AD9")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "AD10")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "AD11")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "AD12")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "AD13")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "AD15")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "AD25")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "AE1")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "AE2")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "AE5")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "AE9")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "AE10")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "AE13")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "AE22")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "AF4")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "AF7")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "AF8")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "AF11")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "AF12")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "AF13")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "AF19")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "AF29")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "AG1")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "AG5")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "AG10")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "AG13")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "AG16")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "AG26")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "AH3")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "AH4")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "AH8")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "AH12")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "AH13")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "AH23")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "AJ1")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AJ2")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AJ5")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AJ10")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AJ13")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AJ20")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AJ30")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AK4")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AK8")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AK12")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AK13")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "AK17")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "AK27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC7K70T-FBG484"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC7K70T-FBG484"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Kintex 7 T 70 XC7K70T-FBG484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC7K70T-FBG484_1_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_13")
				(number "T19")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_13")
				(number "T21")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_13")
				(number "U21")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_13")
				(number "U22")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_13")
				(number "V22")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_13")
				(number "T18")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_13")
				(number "U18")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_13")
				(number "W21")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_13")
				(number "W22")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_13")
				(number "U17")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_13")
				(number "V18")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_13")
				(number "T20")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_13")
				(number "U20")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_13")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_13")
				(number "Y22")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_13")
				(number "AA20")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_13")
				(number "AB21")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_13")
				(number "AA21")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_13")
				(number "AB22")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_13")
				(number "AA19")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_13")
				(number "AB20")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_13")
				(number "V20")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_13")
				(number "W20")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_13")
				(number "V19")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_13")
				(number "W19")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_13")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_13")
				(number "Y19")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_13")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_13")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_13")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_13")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_13")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_13")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_13")
				(number "AA16")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_13")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_13")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_13")
				(number "AA15")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_13")
				(number "U16")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_13")
				(number "V17")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_13")
				(number "R16")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_13")
				(number "T16")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_13")
				(number "W16")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_13")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_13")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_13")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_13")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_13")
				(number "W15")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_13")
				(number "T15")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_13")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_13")
				(number "V14")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AA17")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "AB14")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "T22")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "U19")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "V16")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "Y20")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "F22")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "G19")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "K20")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "L17")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "N21")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_14")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_D00_MOSI_14")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_D01_DIN_14")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_D02_14")
				(number "G18")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_D03_14")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_PUDC_B_14")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_EMCCLK_14")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_D04_14")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_D05_14")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_D06_14")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_D07_14")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_FCS_B_14")
				(number "L16")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_D08_VREF_14")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_D09_14")
				(number "E21")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_D10_14")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_D11_14")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_D12_14")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_14")
				(number "G21")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_D13_14")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_D14_14")
				(number "J21")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_D15_14")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_14")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_14")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_14")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_14")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_14")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_14")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_14")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_14")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_RDWR_B_14")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_DOUT_CSO_B_14")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_CSI_B_14")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_A15_D31_14")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_A14_D30_14")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_A13_D29_14")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_A12_D28_14")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_A11_D27_14")
				(number "L21")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_A10_D26_14")
				(number "R18")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_A09_D25_VREF_14")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_A08_D24_14")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_A07_D23_14")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_14")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A06_D22_14")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_A05_D21_14")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_A04_D20_14")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_A03_D19_14")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_A02_D18_14")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_A01_D17_14")
				(number "R21")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_A00_D16_14")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_14")
				(number "M16")
			)
		)
		(symbol "XC7K70T-FBG484_2_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_15")
				(number "D12")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_AD0P_15")
				(number "G15")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_AD0N_15")
				(number "G16")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_AD8P_15")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_AD8N_15")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_AD1P_15")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_AD1N_15")
				(number "F16")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_AD9P_15")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_AD9N_15")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_AD2P_15")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_AD2N_15")
				(number "B13")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_15")
				(number "E14")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_15")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_AD10P_15")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_AD10N_15")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_AD3P_15")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_AD3N_15")
				(number "A16")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_AD11P_15")
				(number "B15")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_AD11N_15")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_AD4P_15")
				(number "B17")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_AD4N_15")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_AD12P_15")
				(number "D15")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_AD12N_15")
				(number "D16")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_AD5P_15")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_AD5N_15")
				(number "C18")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_15")
				(number "E17")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_15")
				(number "E18")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_15")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_15")
				(number "D17")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_15")
				(number "H17")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_ADV_B_15")
				(number "G17")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_A28_15")
				(number "J16")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_A27_15")
				(number "J17")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_A26_15")
				(number "F18")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_A25_15")
				(number "E19")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_A24_15")
				(number "D19")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_A23_15")
				(number "D20")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_A22_15")
				(number "C19")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_A21_VREF_15")
				(number "C20")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_A20_15")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_A19_15")
				(number "A19")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_15")
				(number "C22")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A18_15")
				(number "B22")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_A17_15")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_A16_15")
				(number "A21")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_FOE_B_15")
				(number "D21")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_FWE_B_15")
				(number "D22")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_RS1_15")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_RS0_15")
				(number "B21")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_15")
				(number "H15")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "A17")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "B14")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "C21")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "D18")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "E15")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "H16")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "C11")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "D8")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "F12")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "G9")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_6_T0_VREF_16")
				(number "F14")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L7P_T1_16")
				(number "D10")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L7N_T1_16")
				(number "C10")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L8P_T1_16")
				(number "G13")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L8N_T1_16")
				(number "F13")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_16")
				(number "H14")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_16")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L10P_T1_16")
				(number "E13")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L10N_T1_16")
				(number "E12")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_16")
				(number "F11")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_16")
				(number "F10")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_16")
				(number "E11")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_16")
				(number "D11")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_16")
				(number "G11")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_16")
				(number "G10")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_16")
				(number "H12")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_16")
				(number "G12")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_16")
				(number "F9")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_16")
				(number "E9")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L16P_T2_16")
				(number "H9")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L16N_T2_16")
				(number "H8")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L17P_T2_16")
				(number "G8")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L17N_T2_16")
				(number "F8")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_18_T2_16")
				(number "H10")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L19P_T3_16")
				(number "D9")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_16")
				(number "C9")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L20P_T3_16")
				(number "B11")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L20N_T3_16")
				(number "B10")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_16")
				(number "A9")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_16")
				(number "A8")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L22P_T3_16")
				(number "C8")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L22N_T3_16")
				(number "B8")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L23P_T3_16")
				(number "A11")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L23N_T3_16")
				(number "A10")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_24_T3_16")
				(number "E8")
			)
		)
		(symbol "XC7K70T-FBG484_3_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_VRN_33")
				(number "T6")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_33")
				(number "AA5")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_33")
				(number "AB5")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_33")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_33")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_33")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_33")
				(number "AB6")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_33")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_33")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_33")
				(number "AA9")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_33")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_33")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_33")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_33")
				(number "W6")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_33")
				(number "Y6")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_33")
				(number "R7")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_33")
				(number "R6")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_33")
				(number "U8")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_33")
				(number "V8")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_33")
				(number "U7")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_33")
				(number "U6")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_33")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_33")
				(number "W7")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_33")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_33")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_33")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_33")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_33")
				(number "U10")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_33")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_33")
				(number "V10")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_33")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_33")
				(number "T11")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_33")
				(number "T10")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_33")
				(number "U12")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_33")
				(number "U11")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_33")
				(number "T9")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_33")
				(number "T8")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_33")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_33")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_33")
				(number "AA11")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_33")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_33")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_33")
				(number "AA13")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_33")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_33")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_33")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_33")
				(number "V12")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_33")
				(number "T13")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_33")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_VRP_33")
				(number "T14")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AA7")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "T12")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "U9")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "V6")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "W13")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "Y10")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AB4")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "M4")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "N1")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "R5")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "T2")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_34")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_34")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_34")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_34")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_34")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_34")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_34")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_34")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_34")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_34")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_34")
				(number "N2")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_34")
				(number "L5")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_34")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_34")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_34")
				(number "R2")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_34")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_34")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_34")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_34")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_34")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_34")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_34")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_34")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_34")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_34")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_34")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_34")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_34")
				(number "V4")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_34")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_34")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_34")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_34")
				(number "T5")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_34")
				(number "U5")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_34")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_34")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_34")
				(number "N5")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_34")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_34")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_34")
				(number "Y4")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_34")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_34")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_34")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_34")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_34")
				(number "AA1")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_34")
				(number "AB1")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_34")
				(number "AA3")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_34")
				(number "AB2")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_34")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_34")
				(number "AB3")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_34")
				(number "V5")
			)
		)
		(symbol "XC7K70T-FBG484_4_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_115")
				(number "F2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_115")
				(number "F1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_115")
				(number "D2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_115")
				(number "D1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_115")
				(number "B2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_115")
				(number "B1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_115")
				(number "A4")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_115")
				(number "A3")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_115")
				(number "G4")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_115")
				(number "G3")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_115")
				(number "E4")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_115")
				(number "E3")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_115")
				(number "C4")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_115")
				(number "C3")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_115")
				(number "B6")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_115")
				(number "B5")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_115")
				(number "D6")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_115")
				(number "D5")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_115")
				(number "F6")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_115")
				(number "F5")
			)
		)
		(symbol "XC7K70T-FBG484_5_1"
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "A6")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "C6")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "E6")
			)
			(pin power_in line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "G6")
			)
			(pin power_in line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTVCCAUX")
				(number "J4")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "A2")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "C2")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "E2")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "G2")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTTRCAL_115")
				(number "H1")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTRREF_115")
				(number "H2")
			)
		)
		(symbol "XC7K70T-FBG484_6_1"
			(pin power_in line
				(at 25.4 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "J7")
			)
			(pin power_in line
				(at 27.94 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "N7")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "TDI_0")
				(number "K6")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "TDO_0")
				(number "J6")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "TMS_0")
				(number "L6")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TCK_0")
				(number "K7")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "CCLK_0")
				(number "G7")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "M0_0")
				(number "H7")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "M1_0")
				(number "H6")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "M2_0")
				(number "J5")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "DONE_0")
				(number "P6")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "INIT_B_0")
				(number "L7")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "PROGRAM_B_0")
				(number "M6")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "CFGBVS_0")
				(number "M7")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "VP_0")
				(number "L12")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "VN_0")
				(number "M11")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 6.35)
				(name "VREFP_0")
				(number "M12")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "VREFN_0")
				(number "L11")
			)
			(pin bidirectional line
				(at 38.1 -35.56 180)
				(length 6.35)
				(name "DXP_0")
				(number "N12")
			)
			(pin bidirectional line
				(at 38.1 -38.1 180)
				(length 6.35)
				(name "DXN_0")
				(number "N11")
			)
		)
		(symbol "XC7K70T-FBG484_7_1"
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M10")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P8")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P10")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P12")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R9")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R11")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "GNDADC_0")
				(number "K11")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCADC_0")
				(number "K12")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCBATT_0")
				(number "P7")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "L13")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "N13")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "R13")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "A5")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "A7")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "A12")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "B3")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "B4")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "B19")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "C1")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "C5")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "C7")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "C16")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "D3")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "D7")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "D13")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E1")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "E10")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "E20")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "F3")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "F17")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "G1")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "G14")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "H3")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "H5")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "H11")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "H21")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "J1")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "J3")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "J8")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "J10")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "J12")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "J14")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "J18")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "K5")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "J11")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "J13")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "J15")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "L15")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "M8")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "R15")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "K15")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "L2")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "L8")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "L22")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "M19")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "N6")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "N8")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "N16")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "P3")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "P15")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "R8")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "R10")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "R12")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "R20")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "T7")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "T17")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "U4")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "U14")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "V1")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "V11")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "V21")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "W8")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "W18")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "Y5")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "Y15")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AA2")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AA12")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AA22")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AB9")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AB19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC7K70T-FBG676"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC7K70T-FBG676"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Kintex 7 T 70 XC7K70T-FBG676"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC7K70T-FBG676_1_1"
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AA21")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AC25")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AD22")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "AF26")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "U23")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "V20")
			)
			(pin power_in line
				(at -25.4 73.66 270)
				(length 6.35)
				(name "VCCO_12")
				(number "Y24")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "K24")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "N25")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "P22")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "R19")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "T16")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_13")
				(number "T26")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_13")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_13")
				(number "K25")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_13")
				(number "K26")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_13")
				(number "R26")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_13")
				(number "P26")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_13")
				(number "M25")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_13")
				(number "L25")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_13")
				(number "P24")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_13")
				(number "N24")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_13")
				(number "N26")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_13")
				(number "M26")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_13")
				(number "R25")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_13")
				(number "P25")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_13")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_13")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_13")
				(number "M24")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_13")
				(number "L24")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_13")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_13")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_13")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_13")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_13")
				(number "P23")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_13")
				(number "N23")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_13")
				(number "N21")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_13")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_13")
				(number "R21")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_13")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_13")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_13")
				(number "R23")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_13")
				(number "T24")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_13")
				(number "T25")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_13")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_13")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_13")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_13")
				(number "T23")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_13")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_13")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_13")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_13")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_13")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_13")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_13")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_13")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_13")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_13")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_13")
				(number "U17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_13")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_13")
				(number "R18")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_13")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_13")
				(number "U16")
			)
		)
		(symbol "XC7K70T-FBG676_2_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_14")
				(number "K21")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_D00_MOSI_14")
				(number "B24")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_D01_DIN_14")
				(number "A25")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_D02_14")
				(number "B22")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_D03_14")
				(number "A22")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_PUDC_B_14")
				(number "B25")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_EMCCLK_14")
				(number "B26")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_D04_14")
				(number "A23")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_D05_14")
				(number "A24")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_D06_14")
				(number "D26")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_D07_14")
				(number "C26")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_FCS_B_14")
				(number "C23")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_D08_VREF_14")
				(number "C24")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_D09_14")
				(number "D21")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_D10_14")
				(number "C22")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_D11_14")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_D12_14")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_14")
				(number "E21")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_D13_14")
				(number "E22")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_D14_14")
				(number "C21")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_D15_14")
				(number "B21")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_14")
				(number "D23")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_14")
				(number "D24")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_14")
				(number "F22")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_14")
				(number "E23")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_14")
				(number "G22")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_14")
				(number "F23")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_14")
				(number "G24")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_14")
				(number "F24")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_RDWR_B_14")
				(number "E25")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_DOUT_CSO_B_14")
				(number "D25")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_CSI_B_14")
				(number "G25")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_A15_D31_14")
				(number "G26")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_A14_D30_14")
				(number "F25")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_A13_D29_14")
				(number "E26")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_A12_D28_14")
				(number "J26")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_A11_D27_14")
				(number "H26")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_A10_D26_14")
				(number "H21")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_A09_D25_VREF_14")
				(number "G21")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_A08_D24_14")
				(number "H23")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_A07_D23_14")
				(number "H24")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_14")
				(number "J21")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A06_D22_14")
				(number "H22")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_A05_D21_14")
				(number "J24")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_A04_D20_14")
				(number "J25")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_A03_D19_14")
				(number "L22")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_A02_D18_14")
				(number "K22")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_A01_D17_14")
				(number "K23")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_A00_D16_14")
				(number "J23")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_14")
				(number "L23")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "A21")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "C25")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "D22")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "F26")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "G23")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_14")
				(number "L21")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "B18")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "E19")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "F16")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "H20")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "J17")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_15")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_15")
				(number "K15")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_AD0P_15")
				(number "C16")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_AD0N_15")
				(number "B16")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_AD8P_15")
				(number "A18")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_AD8N_15")
				(number "A19")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_AD1P_15")
				(number "B17")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_AD1N_15")
				(number "A17")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_AD9P_15")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_AD9N_15")
				(number "B19")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_AD2P_15")
				(number "C17")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_AD2N_15")
				(number "C18")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_15")
				(number "D15")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_15")
				(number "D16")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_AD10P_15")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_AD10N_15")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_AD3P_15")
				(number "G15")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_AD3N_15")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_AD11P_15")
				(number "J15")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_AD11N_15")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_AD4P_15")
				(number "E15")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_AD4N_15")
				(number "E16")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_AD12P_15")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_AD12N_15")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_AD5P_15")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_AD5N_15")
				(number "E17")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_15")
				(number "E18")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_15")
				(number "D18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_15")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_15")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_15")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_ADV_B_15")
				(number "D20")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_A28_15")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_A27_15")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_A26_15")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_A25_15")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_A24_15")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_A23_15")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_A22_15")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_A21_VREF_15")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_A20_15")
				(number "J18")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_A19_15")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_15")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_A18_15")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_A17_15")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_A16_15")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_FOE_B_15")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_FWE_B_15")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_RS1_15")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_RS0_15")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_15")
				(number "M16")
			)
		)
		(symbol "XC7K70T-FBG676_3_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_16")
				(number "J8")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_16")
				(number "H9")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_16")
				(number "H8")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_16")
				(number "G10")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_16")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_16")
				(number "J13")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_16")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_16")
				(number "J11")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_16")
				(number "J10")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_16")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_16")
				(number "G14")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_16")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_16")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_16")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_16")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_16")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_16")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_16")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_16")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_16")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_16")
				(number "B9")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_16")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_16")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_16")
				(number "E10")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_16")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_16")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_16")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_16")
				(number "E11")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_16")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_16")
				(number "F14")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_16")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_16")
				(number "G12")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_16")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_16")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_16")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_16")
				(number "E13")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_16")
				(number "E12")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_16")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_16")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_16")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_16")
				(number "B11")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_16")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_16")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_16")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_16")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_16")
				(number "B15")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_16")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_16")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_16")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_16")
				(number "J14")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "A11")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "B8")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "C15")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "D12")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "E9")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "G13")
			)
			(pin power_in line
				(at -25.4 73.66 270)
				(length 6.35)
				(name "VCCO_16")
				(number "H10")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AB18")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AC15")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AE19")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "AF16")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "W17")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_32")
				(number "Y14")
			)
		)
		(symbol "XC7K70T-FBG676_4_1"
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_0_VRN_33")
				(number "U9")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L1P_T0_33")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L1N_T0_33")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L2P_T0_33")
				(number "V8")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L2N_T0_33")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L3P_T0_DQS_33")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L3N_T0_DQS_33")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L4P_T0_33")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L4N_T0_33")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L5P_T0_33")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L5N_T0_33")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L6P_T0_33")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L6N_T0_VREF_33")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L7P_T1_33")
				(number "AE7")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L7N_T1_33")
				(number "AF7")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L8P_T1_33")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L8N_T1_33")
				(number "AA7")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L9P_T1_DQS_33")
				(number "AC8")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L9N_T1_DQS_33")
				(number "AD8")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L10P_T1_33")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L10N_T1_33")
				(number "AC7")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_33")
				(number "AA9")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_33")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_33")
				(number "AC9")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_33")
				(number "AD9")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_33")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_33")
				(number "AC11")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_33")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_33")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L15P_T2_DQS_33")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L15N_T2_DQS_33")
				(number "AC12")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L16P_T2_33")
				(number "AA13")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L16N_T2_33")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L17P_T2_33")
				(number "AC13")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L17N_T2_33")
				(number "AD13")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L18P_T2_33")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L18N_T2_33")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L19P_T3_33")
				(number "AD11")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L19N_T3_VREF_33")
				(number "AE11")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L20P_T3_33")
				(number "AD10")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L20N_T3_33")
				(number "AE10")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L21P_T3_DQS_33")
				(number "AE12")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L21N_T3_DQS_33")
				(number "AF12")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L22P_T3_33")
				(number "AE8")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L22N_T3_33")
				(number "AF8")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L23P_T3_33")
				(number "AE13")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L23N_T3_33")
				(number "AF13")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L24P_T3_33")
				(number "AF10")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L24N_T3_33")
				(number "AF9")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_25_VRP_33")
				(number "V12")
			)
			(pin power_in line
				(at -40.64 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AA11")
			)
			(pin power_in line
				(at -38.1 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AB8")
			)
			(pin power_in line
				(at -35.56 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AD12")
			)
			(pin power_in line
				(at -33.02 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "AE9")
			)
			(pin power_in line
				(at -30.48 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "V10")
			)
			(pin power_in line
				(at -27.94 73.66 270)
				(length 6.35)
				(name "VCCO_33")
				(number "W7")
			)
			(pin power_in line
				(at 27.94 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AA1")
			)
			(pin power_in line
				(at 30.48 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AC5")
			)
			(pin power_in line
				(at 33.02 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AD2")
			)
			(pin power_in line
				(at 35.56 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "AF6")
			)
			(pin power_in line
				(at 38.1 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "U3")
			)
			(pin power_in line
				(at 40.64 73.66 270)
				(length 6.35)
				(name "VCCO_34")
				(number "Y4")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_0_VRN_34")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L1P_T0_34")
				(number "U6")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L1N_T0_34")
				(number "U5")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L2P_T0_34")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L2N_T0_34")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L3P_T0_DQS_34")
				(number "W6")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L3N_T0_DQS_34")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L4P_T0_34")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L4N_T0_34")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L5P_T0_34")
				(number "U7")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L5N_T0_34")
				(number "V6")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L6P_T0_34")
				(number "V4")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L6N_T0_VREF_34")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L7P_T1_34")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L7N_T1_34")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L8P_T1_34")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L8N_T1_34")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L9P_T1_DQS_34")
				(number "AB1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L9N_T1_DQS_34")
				(number "AC1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L10P_T1_34")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L10N_T1_34")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L11P_T1_SRCC_34")
				(number "AB2")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L11N_T1_SRCC_34")
				(number "AC2")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L12P_T1_MRCC_34")
				(number "AA3")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L12N_T1_MRCC_34")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L13P_T2_MRCC_34")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L13N_T2_MRCC_34")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L14P_T2_SRCC_34")
				(number "AC4")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L14N_T2_SRCC_34")
				(number "AC3")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L15P_T2_DQS_34")
				(number "AA5")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L15N_T2_DQS_34")
				(number "AB5")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L16P_T2_34")
				(number "AB6")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L16N_T2_34")
				(number "AC6")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L17P_T2_34")
				(number "Y6")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L17N_T2_34")
				(number "Y5")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L18P_T2_34")
				(number "AD6")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L18N_T2_34")
				(number "AD5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L19P_T3_34")
				(number "AD4")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L19N_T3_VREF_34")
				(number "AD3")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L20P_T3_34")
				(number "AD1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L20N_T3_34")
				(number "AE1")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L21P_T3_DQS_34")
				(number "AF5")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L21N_T3_DQS_34")
				(number "AF4")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L22P_T3_34")
				(number "AE3")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L22N_T3_34")
				(number "AE2")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L23P_T3_34")
				(number "AE6")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L23N_T3_34")
				(number "AE5")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L24P_T3_34")
				(number "AF3")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L24N_T3_34")
				(number "AF2")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_25_VRP_34")
				(number "T7")
			)
		)
		(symbol "XC7K70T-FBG676_5_1"
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 6.35)
				(name "MGTXTXP0_115")
				(number "P2")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 6.35)
				(name "MGTXTXN0_115")
				(number "P1")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 6.35)
				(name "MGTXTXP1_115")
				(number "M2")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 6.35)
				(name "MGTXTXN1_115")
				(number "M1")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTXTXP2_115")
				(number "K2")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTXTXN2_115")
				(number "K1")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTXTXP3_115")
				(number "H2")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTXTXN3_115")
				(number "H1")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTXRXP0_115")
				(number "R4")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTXRXN0_115")
				(number "R3")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTXRXP1_115")
				(number "N4")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTXRXN1_115")
				(number "N3")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTXRXP2_115")
				(number "L4")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTXRXN2_115")
				(number "L3")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTXRXP3_115")
				(number "J4")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTXRXN3_115")
				(number "J3")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTREFCLK0P_115")
				(number "H6")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 6.35)
				(name "MGTREFCLK0N_115")
				(number "H5")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 6.35)
				(name "MGTREFCLK1P_115")
				(number "K6")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 6.35)
				(name "MGTREFCLK1N_115")
				(number "K5")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 6.35)
				(name "MGTXTXP0_116")
				(number "F2")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 6.35)
				(name "MGTXTXN0_116")
				(number "F1")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 6.35)
				(name "MGTXTXP1_116")
				(number "D2")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "MGTXTXN1_116")
				(number "D1")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTXTXP2_116")
				(number "B2")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTXTXN2_116")
				(number "B1")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTXTXP3_116")
				(number "A4")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTXTXN3_116")
				(number "A3")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTXRXP0_116")
				(number "G4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTXRXN0_116")
				(number "G3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTXRXP1_116")
				(number "E4")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTXRXN1_116")
				(number "E3")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTXRXP2_116")
				(number "C4")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTXRXN2_116")
				(number "C3")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTXRXP3_116")
				(number "B6")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTXRXN3_116")
				(number "B5")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTREFCLK0P_116")
				(number "D6")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "MGTREFCLK0N_116")
				(number "D5")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "MGTREFCLK1P_116")
				(number "F6")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 6.35)
				(name "MGTREFCLK1N_116")
				(number "F5")
			)
		)
		(symbol "XC7K70T-FBG676_6_1"
			(pin power_in line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "C6")
			)
			(pin power_in line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "E6")
			)
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "G6")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "J6")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC")
				(number "L6")
			)
			(pin power_in line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTVCCAUX")
				(number "N6")
			)
			(pin power_in line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "B3")
			)
			(pin power_in line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "C2")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "D3")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "G2")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "H3")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "L2")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTAVTT")
				(number "M3")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTTRCAL_115")
				(number "M5")
			)
			(pin power_in line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTRREF_115")
				(number "M6")
			)
		)
		(symbol "XC7K70T-FBG676_7_1"
			(pin power_in line
				(at 25.4 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "L7")
			)
			(pin power_in line
				(at 27.94 40.64 270)
				(length 6.35)
				(name "VCCO_0")
				(number "T6")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 6.35)
				(name "TDI_0")
				(number "R6")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "TDO_0")
				(number "R7")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "TMS_0")
				(number "N8")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TCK_0")
				(number "L8")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "CCLK_0")
				(number "C8")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "M0_0")
				(number "T5")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "M1_0")
				(number "T2")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "M2_0")
				(number "P5")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "DONE_0")
				(number "J7")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "INIT_B_0")
				(number "G7")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "PROGRAM_B_0")
				(number "P6")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "CFGBVS_0")
				(number "P7")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 6.35)
				(name "VP_0")
				(number "N12")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 6.35)
				(name "VN_0")
				(number "P11")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 6.35)
				(name "VREFP_0")
				(number "P12")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 6.35)
				(name "VREFN_0")
				(number "N11")
			)
			(pin bidirectional line
				(at 38.1 -35.56 180)
				(length 6.35)
				(name "DXP_0")
				(number "R12")
			)
			(pin bidirectional line
				(at 38.1 -38.1 180)
				(length 6.35)
				(name "DXN_0")
				(number "R11")
			)
		)
		(symbol "XC7K70T-FBG676_8_1"
			(pin power_in line
				(at -25.4 99.06 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 96.52 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M10")
			)
			(pin power_in line
				(at -25.4 93.98 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P10")
			)
			(pin power_in line
				(at -25.4 91.44 0)
				(length 6.35)
				(name "VCCAUX")
				(number "T10")
			)
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "T8")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "R9")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "VCCAUX_IO_G0")
				(number "P8")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "GNDADC_0")
				(number "M11")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCADC_0")
				(number "M12")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCBATT_0")
				(number "E8")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "N13")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "R13")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "T12")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCBRAM")
				(number "U13")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "GND")
				(number "A2")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "GND")
				(number "A5")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "GND")
				(number "A6")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "GND")
				(number "A7")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "GND")
				(number "A16")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "A26")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "B4")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "B23")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "C1")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "C5")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "C7")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "C10")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "C20")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "D7")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "D17")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "E1")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "E14")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E24")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "F3")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "F4")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "F21")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G1")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "H25")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "J1")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "J5")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "J12")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "J22")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "K3")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "K4")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "K7")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "K11")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "K13")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "K19")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "L1")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "L10")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "L12")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "L14")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "L16")
			)
			(pin power_in line
				(at -25.4 -91.44 0)
				(length 6.35)
				(name "GND")
				(number "L26")
			)
			(pin power_in line
				(at -25.4 -93.98 0)
				(length 6.35)
				(name "GND")
				(number "M4")
			)
			(pin power_in line
				(at -25.4 -96.52 0)
				(length 6.35)
				(name "GND")
				(number "M7")
			)
			(pin power_in line
				(at -25.4 -99.06 0)
				(length 6.35)
				(name "GND")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 99.06 180)
				(length 6.35)
				(name "VCCINT")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 96.52 180)
				(length 6.35)
				(name "VCCINT")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 93.98 180)
				(length 6.35)
				(name "VCCINT")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 91.44 180)
				(length 6.35)
				(name "VCCINT")
				(number "K12")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "L13")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "L15")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "M8")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "R15")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "T14")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "U15")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "GND")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "GND")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "GND")
				(number "M23")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "GND")
				(number "N1")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "GND")
				(number "N5")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "N7")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "N20")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "P3")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "P4")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "P15")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "P17")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "R2")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "R8")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "R10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "R24")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "T1")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "T3")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "T4")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "T9")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "T11")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "T13")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "T15")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "T21")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "U8")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "U10")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U14")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "U18")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V5")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "V15")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "V25")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "W2")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "W12")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "W22")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "Y9")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "Y19")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AA6")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AA16")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AA26")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AB3")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AB13")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AB23")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "AC10")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "AC20")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "AD7")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "AD17")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "AE4")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "AE14")
			)
			(pin power_in line
				(at 25.4 -91.44 180)
				(length 6.35)
				(name "GND")
				(number "AE24")
			)
			(pin power_in line
				(at 25.4 -93.98 180)
				(length 6.35)
				(name "GND")
				(number "AF1")
			)
			(pin power_in line
				(at 25.4 -96.52 180)
				(length 6.35)
				(name "GND")
				(number "AF11")
			)
			(pin power_in line
				(at 25.4 -99.06 180)
				(length 6.35)
				(name "GND")
				(number "AF21")
			)
		)
		(embedded_fonts no)
	)
)
